<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<packages>
<package name="SOT131-2H">
</package>
<package name="SOT157-2">
</package>
<package name="SOT243-1">
</package>
<package name="PENTAWATT-V">
</package>
<package name="SOT141-6">
</package>
<package name="SIP11">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
11 lead, National Semiconductor</description>
</package>
<package name="CB360">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt; 5 lead</description>
</package>
<package name="CE82">
<description>&lt;b&gt;Package DIL 16 (CE83)&lt;/b&gt;</description>
</package>
<package name="HSIP17-P-2.00">
<description>&lt;b&gt;HSIP17-P-2.00&lt;/b&gt;&lt;p&gt;
Source: http://www.semicon.toshiba.co.jp/td/en/ASSP/Audio_ICs/en_20050517_TA8210ALQ_datasheet.pdf</description>
</package>
<package name="HZIP17-P-2.00">
<description>&lt;b&gt;HZIP17-P-2.00&lt;/b&gt;&lt;p&gt;
Source: http://www.semicon.toshiba.co.jp/td/en/ASSP/Audio_ICs/en_20050517_TA8210ALQ_datasheet.pdf</description>
</package>
<package name="MULTIWAT-SIL13">
<description>&lt;b&gt;DBS13P&lt;/b&gt; plastic DIL-bent-SIL power package&lt;p&gt;
13 leads (lead length 12 mm) SOT141-6&lt;br&gt;
Source: TDA1516BQ_1.pdf</description>
</package>
<package name="MULTIWAT-SIL17">
<description>&lt;b&gt;DBS17P&lt;/b&gt; plastic DIL-bent-SIL power package&lt;p&gt;
17 leads (lead length 12 mm) SOT243-1</description>
</package>
<package name="14-DIPH-300">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SIP8">
</package>
<package name="MULTIWATT15H">
<description>Multiwatt 15-pin horizontal package</description>
</package>
<package name="MULTIWATT15V">
<description>Multiwatt 15-pin vertical package</description>
</package>
<package name="MULTIWATT-15H">
<description>Multiwatt 15  horizontal</description>
</package>
<package name="MULTIWATT-15V">
<description>Multiwatt 15 vertical</description>
</package>
<package name="FLEXIWATT25">
</package>
<package name="MULTIWATT-11">
<description>&lt;b&gt;Muliwatt 11 lead&lt;/b&gt;</description>
</package>
<package name="SO8">
</package>
<package name="SIP13">
</package>
<package name="FINDIP12">
</package>
<package name="CE-50/TO3">
<description>&lt;b&gt;TO-3&lt;/b&gt;&lt;p&gt;
National Semiconductor K08A</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT38-1">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="12-DIPH-300">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="HEPTAWATT">
<description>&lt;b&gt;HEPTAWATT 7&lt;/b&gt;</description>
</package>
<package name="HEPTAW.H">
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="CLIPWATT11">
</package>
<package name="STK4241/2">
</package>
<package name="ZIP12/CPP-12">
<description>&lt;b&gt;Single In Line Socket&lt;/b&gt;</description>
</package>
<package name="SOT527-1">
</package>
<package name="SOT97-1">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT96-1">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="SOT162-1">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO20_SOT163-1-R">
<description>&lt;b&gt;SO20 / SOT163-1 Reflow soldering&lt;/b&gt; Philips SC01_Mounting_1996.pdf</description>
</package>
<package name="SO20_SOT163-1-W">
<description>&lt;b&gt;SO20 / SOT163-1 Wave soldering&lt;/b&gt; Philips SC01_Mounting_1996.pdf</description>
</package>
<package name="SOT266-1">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT109-1">
</package>
<package name="SOT577-2">
</package>
<package name="SOT163-1">
</package>
<package name="SOP16">
</package>
<package name="SSOP-A16">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT566-3">
</package>
<package name="SOT767-1">
</package>
<package name="SOT521-1">
</package>
<package name="SOT725-1">
</package>
<package name="SOT418-3">
</package>
<package name="SOT523-1">
</package>
<package name="SOT110-1">
</package>
<package name="HSOP28">
</package>
<package name="HSIP15-P-2.00A">
</package>
<package name="SOP018-P-0300">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="HSIP15">
</package>
<package name="HSOP056-P-0300A">
</package>
<package name="TA11B">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
11 lead, National Semiconductor</description>
</package>
<package name="TF11B">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
11 lead, National Semiconductor</description>
</package>
<package name="SOT354-1">
</package>
<package name="DKD">
</package>
<package name="SOT411-1">
</package>
<package name="SOT397-1">
</package>
<package name="SO36-POWER_SLUG_UP">
</package>
<package name="SOP08">
</package>
<package name="SIL08">
<description>7 &lt;B&gt;DIODES&lt;/B&gt;&lt;p&gt;
single in line 7 diodes with common anode</description>
</package>
<package name="SSIP-32">
<description>&lt;b&gt; 32-pin SSIP&lt;/b&gt;&lt;p&gt;
Source: http://www.tripath.com/audio.htm</description>
</package>
<package name="SIP12">
</package>
<package name="HZIP12-P-1,78B">
</package>
<package name="CLIPWATT15">
</package>
</packages>
<symbols>
<symbol name="TDA1521Q">
<pin name="-INV1" direction="in"/>
<pin name="INV1" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT1" direction="in"/>
<pin name="+VP" direction="in"/>
<pin name="INV2" direction="in"/>
<pin name="-INV2" direction="in"/>
<pin name="OUT2" direction="in"/>
<pin name="-VP" direction="in"/>
</symbol>
<symbol name="TDA1554">
<pin name="NINV1" direction="in"/>
<pin name="NIV1" direction="in"/>
<pin name="RR" direction="pas"/>
<pin name="NINV2" direction="in"/>
<pin name="INV2" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="M/SS" direction="pas"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="VP1" direction="pwr"/>
<pin name="VP2" direction="pwr"/>
</symbol>
<symbol name="TDA1558Q">
<pin name="INPUT1" direction="in"/>
<pin name="INPUT2" direction="in"/>
<pin name="GNDSIG" direction="pwr"/>
<pin name="RR" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="N/C" direction="nc"/>
<pin name="OUT4" direction="out"/>
<pin name="GND2" direction="pwr"/>
<pin name="OUT3" direction="out"/>
<pin name="VCC1" direction="pwr"/>
<pin name="MUTE" direction="in"/>
<pin name="IRV"/>
<pin name="INPUT4" direction="in"/>
<pin name="IN3" direction="in"/>
</symbol>
<symbol name="TDA200X">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TDA8560Q">
<pin name="OUT2A"/>
<pin name="MODE"/>
<pin name="OUT1A"/>
<pin name="IN1"/>
<pin name="GND(S)"/>
<pin name="IN2"/>
<pin name="OUT1B"/>
<pin name="VDIAG"/>
<pin name="OUT2B"/>
<pin name="VP1"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="VP2"/>
</symbol>
<symbol name="2005">
<pin name="BTSP" direction="pas"/>
<pin name="SVRR" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="2005A">
<pin name="BTSP" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OPAMP+-">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP+GN">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="UL1440">
<pin name="GND" direction="pwr"/>
<pin name="GND@" direction="pwr"/>
<pin name="TW" direction="pas"/>
<pin name="F_BACK" direction="pas"/>
<pin name="FCORE" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="BOSTRAP" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="IN" direction="pas"/>
</symbol>
<symbol name="2GND">
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
</symbol>
<symbol name="TA8210">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="NF1" direction="in"/>
<pin name="NF2" direction="in"/>
<pin name="MUTE_SW" direction="in"/>
<pin name="RIPPLE" direction="in"/>
<pin name="PRE-VCC" direction="pwr"/>
<pin name="PRE-GND" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="STAND-BY_SW" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="TDA1516">
<pin name="VREF" direction="pas"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="STDBY" direction="in"/>
<pin name="INT_VP1/2" direction="pas"/>
<pin name="VP1" direction="pwr"/>
<pin name="VP2" direction="pwr"/>
<pin name="GNDS" direction="pwr"/>
<pin name="GNDP" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="VP" direction="in"/>
</symbol>
<symbol name="TDA1560Q">
<pin name="VP" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="S1" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="SIG-GND" direction="in"/>
<pin name="INPP" direction="in"/>
<pin name="INPN" direction="in"/>
<pin name="OUT2P" direction="out"/>
<pin name="OUT1N" direction="out"/>
<pin name="VDIAG" direction="out"/>
<pin name="CDEC" direction="pas"/>
<pin name="MODE" direction="in"/>
</symbol>
<symbol name="TDA1562">
<pin name="VP1" direction="pwr"/>
<pin name="VP2" direction="pwr"/>
<pin name="PGND1" direction="pwr"/>
<pin name="PGND2" direction="pwr"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="STATUS_IO" direction="in"/>
<pin name="M-SEL" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="SIG-GND" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="DIAGNOSTIC" direction="out"/>
</symbol>
<symbol name="UPC1237HA">
<pin name="2"/>
<pin name="1"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
</symbol>
<symbol name="TDA7294">
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="STBY" direction="in"/>
<pin name="STBY-GND" direction="pwr"/>
<pin name="VS-" direction="pwr"/>
<pin name="IN+MUTE" direction="pwr"/>
<pin name="PWVS-" direction="pwr"/>
<pin name="VS+" direction="pwr"/>
<pin name="PWVS+" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="BOOTSTRAP" direction="pas"/>
</symbol>
<symbol name="TDA7293">
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="SGND" direction="pwr"/>
<pin name="MUTE" direction="in"/>
<pin name="STBY" direction="in"/>
<pin name="STBY-GND" direction="pwr"/>
<pin name="VS-" direction="pwr"/>
<pin name="PWVS-" direction="pwr"/>
<pin name="VS+" direction="pwr"/>
<pin name="BUFFER" direction="pas"/>
<pin name="PWVS+" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="BOOTLOADER" direction="pas"/>
<pin name="BOOSTRAP" direction="pas"/>
<pin name="CLIP" direction="oc"/>
</symbol>
<symbol name="TDA7375">
<pin name="IN1" direction="in"/>
<pin name="OUT4" direction="out"/>
<pin name="VCC3-4" direction="pwr"/>
<pin name="PWRGND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="SGNG" direction="pwr"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="DIAG" direction="pas"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="STD-BY" direction="in"/>
<pin name="VCC1-2" direction="pwr"/>
<pin name="OUT3" direction="out"/>
<pin name="SVR" direction="pas"/>
</symbol>
<symbol name="TDA7386">
<pin name="ST-BY"/>
<pin name="MUTE"/>
<pin name="IN4"/>
<pin name="IN3"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="AC-GND"/>
<pin name="SVR"/>
<pin name="S-GND"/>
<pin name="TAB"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="PW-GND$4"/>
<pin name="OUT4-"/>
<pin name="OUT4+"/>
<pin name="PW-GND$3"/>
<pin name="OUT3-"/>
<pin name="OUT3+"/>
<pin name="PW-GND$2"/>
<pin name="OUT2-"/>
<pin name="OUT2+"/>
<pin name="PW-GND$1"/>
<pin name="OUT1-"/>
<pin name="OUT1+"/>
<pin name="N.C."/>
</symbol>
<symbol name="TDA8571J">
<pin name="VP1" direction="pwr"/>
<pin name="OUT1+" direction="out"/>
<pin name="PGND1" direction="pwr"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="PGND2" direction="pwr"/>
<pin name="OUT2+" direction="out"/>
<pin name="VP2" direction="pwr"/>
<pin name="VDIAG"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="SGND" direction="pwr"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="MODE"/>
<pin name="VP3" direction="pwr"/>
<pin name="OUT3+" direction="out"/>
<pin name="PGND3" direction="pwr"/>
<pin name="OUT3-" direction="out"/>
<pin name="OUT4-" direction="out"/>
<pin name="PGND4" direction="pwr"/>
<pin name="OUT4+" direction="out"/>
<pin name="VP4" direction="pwr"/>
</symbol>
<symbol name="TDA7050">
<pin name="1_INA+"/>
<pin name="2_INA-"/>
<pin name="3_INB-"/>
<pin name="4_INB+"/>
<pin name="5_GND"/>
<pin name="6_OUTB"/>
<pin name="7_OUTA"/>
<pin name="8_VDD"/>
</symbol>
<symbol name="TDA1557">
<pin name="1_IN1"/>
<pin name="2_GNDIN"/>
<pin name="3_VP1"/>
<pin name="4_OUT1A"/>
<pin name="5_GNDPWR"/>
<pin name="6_OUT1B"/>
<pin name="7_OUT2A"/>
<pin name="8_GNDPWR"/>
<pin name="9_OUT2B"/>
<pin name="10_VP2"/>
<pin name="11_MUTE"/>
<pin name="12_NC"/>
<pin name="13_IN2"/>
</symbol>
<symbol name="TDA1308">
<pin name="1_OUTA"/>
<pin name="2_INA-"/>
<pin name="3_INA+"/>
<pin name="4_GND"/>
<pin name="5_INB+"/>
<pin name="6_INB-"/>
<pin name="7_OUTB"/>
<pin name="8_+VDD"/>
</symbol>
<symbol name="TBA800">
<pin name="12" direction="out"/>
<pin name="8" direction="in"/>
<pin name="9" direction="in"/>
<pin name="VCC/1" direction="pwr"/>
<pin name="7"/>
<pin name="5"/>
<pin name="3"/>
<pin name="4"/>
<pin name="10/GND" direction="pwr"/>
<pin name="6"/>
<pin name="2" direction="nc"/>
<pin name="11" direction="nc"/>
<pin name="P$1" direction="pwr"/>
<pin name="P$2" direction="pwr"/>
<pin name="P$3" direction="pwr"/>
<pin name="P$4" direction="pwr"/>
</symbol>
<symbol name="UL140*">
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+V" direction="pwr"/>
<pin name="NC"/>
<pin name="IO3"/>
<pin name="IO2"/>
<pin name="IN" direction="in"/>
<pin name="IO1"/>
<pin name="IO"/>
<pin name="R1" direction="pwr"/>
<pin name="R" direction="pwr"/>
</symbol>
<symbol name="KA2102A">
<pin name="D"/>
<pin name="D1"/>
<pin name="SIF"/>
<pin name="OUD" direction="out"/>
<pin name="+VC" direction="pwr"/>
<pin name="FED"/>
<pin name="IN1"/>
<pin name="OUT" direction="out"/>
<pin name="BO"/>
<pin name="+VP" direction="pwr"/>
<pin name="F1"/>
<pin name="INA"/>
<pin name="INB"/>
<pin name="VOL"/>
<pin name="TAB1"/>
<pin name="TAB2"/>
<pin name="TAB3"/>
<pin name="TAB4"/>
</symbol>
<symbol name="TDA1904">
<pin name="OUT" direction="out"/>
<pin name="+VSS" direction="pwr"/>
<pin name="BOST"/>
<pin name="NC" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="INV" direction="in"/>
<pin name="SVR" direction="in"/>
<pin name="NINV" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND6" direction="pwr"/>
<pin name="GND7" direction="pwr"/>
</symbol>
<symbol name="KA2206BN">
<pin name="BTLOUT" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="BS2"/>
<pin name="FGND" direction="pwr"/>
<pin name="FGND1" direction="pwr"/>
<pin name="NF2"/>
<pin name="IN2" direction="in"/>
<pin name="RR"/>
<pin name="PREGND" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="NF1"/>
<pin name="FGND2" direction="pwr"/>
<pin name="FGND3" direction="pwr"/>
<pin name="BS1"/>
<pin name="OUT1" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TDA2052">
<pin name="OUT" direction="out"/>
<pin name="+V" direction="pwr"/>
<pin name="ST/MUT"/>
<pin name="-V" direction="pwr"/>
<pin name="-INV(MUTE)" direction="in"/>
<pin name="-INP" direction="in"/>
<pin name="+INP" direction="in"/>
</symbol>
<symbol name="TDA7052">
<pin name="VP" direction="sup"/>
<pin name="GND" direction="sup"/>
<pin name="GND@" direction="sup"/>
<pin name="IN" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="TDA7393">
<pin name="IN1" direction="in"/>
<pin name="OUT2+" direction="out"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="IN-MUTE" direction="in"/>
<pin name="MONO" direction="in"/>
<pin name="MUTE2-MO" direction="in"/>
<pin name="MUTE1-ST" direction="in"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="STD-BY" direction="in"/>
<pin name="VCC1" direction="pwr"/>
<pin name="OUT2-" direction="out"/>
<pin name="SVR" direction="pas"/>
</symbol>
<symbol name="TDA7372B">
<pin name="IN1" direction="in"/>
<pin name="OUT4" direction="out"/>
<pin name="VCC2" direction="pwr"/>
<pin name="PW-GND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="S-GND" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="STD-BY" direction="in"/>
<pin name="VCC1" direction="pwr"/>
<pin name="OUT3" direction="out"/>
<pin name="SVR" direction="pas"/>
</symbol>
<symbol name="TDA7523">
<pin name="NC" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="SMUTE"/>
<pin name="INV/IN" direction="in"/>
<pin name="NINV/IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="NC2" direction="nc"/>
<pin name="OUT" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="TDA7253">
<pin name="NC" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="S/MUTE"/>
<pin name="INV/IN" direction="in"/>
<pin name="NINV/IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="NC2" direction="nc"/>
<pin name="OUT" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="STK4241/2">
<pin name="1"/>
<pin name="2"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="pwr"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11" direction="pwr"/>
<pin name="12" direction="out"/>
<pin name="13" direction="pwr"/>
<pin name="14" direction="pwr"/>
<pin name="15" direction="out"/>
<pin name="16" direction="pwr"/>
<pin name="17"/>
<pin name="18" direction="pwr"/>
<pin name="19" direction="in"/>
<pin name="20" direction="in"/>
<pin name="21"/>
<pin name="22"/>
</symbol>
<symbol name="TDA1517ATW">
<pin name="NC" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="IN1" direction="in"/>
<pin name="SGND" direction="pwr"/>
<pin name="SVRR"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="OUT1A" direction="out"/>
<pin name="OUT1B" direction="out"/>
<pin name="PGND1" direction="pwr"/>
<pin name="PGND2" direction="pwr"/>
<pin name="OUT2A" direction="out"/>
<pin name="OUT2B" direction="out"/>
<pin name="NC4" direction="nc"/>
<pin name="VP1" direction="pwr"/>
<pin name="VP2" direction="pwr"/>
<pin name="MODE"/>
<pin name="IN2-" direction="in"/>
<pin name="NC5" direction="nc"/>
<pin name="NC6" direction="nc"/>
<pin name="HEATHSINK_SIDE" direction="pwr"/>
</symbol>
<symbol name="TDA8543">
<pin name="NC" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="MO"/>
<pin name="SVR"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC5" direction="nc"/>
<pin name="OUT-" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT+" direction="out"/>
<pin name="NC6" direction="nc"/>
<pin name="NC7" direction="nc"/>
</symbol>
<symbol name="TDA8552T/S">
<pin name="GND1" direction="pwr"/>
<pin name="OUT2+" direction="out"/>
<pin name="VDD1" direction="pwr"/>
<pin name="HPS"/>
<pin name="MOD"/>
<pin name="UP/DO1"/>
<pin name="UP/DO2"/>
<pin name="VDD2" direction="pwr"/>
<pin name="OUT2-" direction="out"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="OUT1+" direction="out"/>
<pin name="VDD3" direction="pwr"/>
<pin name="GAINS"/>
<pin name="IN2" direction="in"/>
<pin name="SVR"/>
<pin name="IN1" direction="in"/>
<pin name="VDD4" direction="pwr"/>
<pin name="OUT1-" direction="out"/>
<pin name="GND4" direction="pwr"/>
</symbol>
<symbol name="TDA8551">
<pin name="U/D"/>
<pin name="MOD"/>
<pin name="SVR"/>
<pin name="IN" direction="in"/>
<pin name="OUT-" direction="out"/>
<pin name="VP" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT+" direction="out"/>
</symbol>
<symbol name="TDA8542TS">
<pin name="LGND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="OUTL+" direction="out"/>
<pin name="MOD"/>
<pin name="SVR"/>
<pin name="BT/SE"/>
<pin name="NC1" direction="nc"/>
<pin name="OUTR+" direction="out"/>
<pin name="NC2" direction="nc"/>
<pin name="RGND" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="NC3" direction="nc"/>
<pin name="OUTR-" direction="out"/>
<pin name="INR-" direction="in"/>
<pin name="INR+" direction="in"/>
<pin name="INL+" direction="in"/>
<pin name="INL-" direction="in"/>
<pin name="OUTL-" direction="out"/>
<pin name="NC4" direction="nc"/>
<pin name="VCCL" direction="pwr"/>
</symbol>
<symbol name="TDA8542">
<pin name="LGND" direction="pwr"/>
<pin name="OUTL+" direction="out"/>
<pin name="MOD"/>
<pin name="SVR"/>
<pin name="BTL/SE"/>
<pin name="NC" direction="nc"/>
<pin name="OUTR+" direction="out"/>
<pin name="RGND" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="OUTR-" direction="out"/>
<pin name="INR-" direction="in"/>
<pin name="INR+" direction="in"/>
<pin name="INL+" direction="in"/>
<pin name="INL-" direction="in"/>
<pin name="OUTL-" direction="out"/>
<pin name="VCCL" direction="pwr"/>
</symbol>
<symbol name="BA5204F">
<pin name="B/ST1"/>
<pin name="OUT1" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="B/ST2"/>
<pin name="SUB2"/>
<pin name="IN2" direction="in"/>
<pin name="NFB2"/>
<pin name="NC1" direction="nc"/>
<pin name="FILTER"/>
<pin name="NFB1"/>
<pin name="IN1" direction="in"/>
<pin name="SUB1"/>
</symbol>
<symbol name="BA5208AF">
<pin name="GND" direction="pwr"/>
<pin name="MOUT2" direction="out"/>
<pin name="BIAS2"/>
<pin name="INOUT" direction="out"/>
<pin name="IN2" direction="in"/>
<pin name="NFB2"/>
<pin name="OUT2" direction="out"/>
<pin name="PGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="NFB1"/>
<pin name="IN1" direction="in"/>
<pin name="BIAS1"/>
<pin name="FILTER"/>
<pin name="MUTE/IN" direction="in"/>
<pin name="MOUT1" direction="out"/>
</symbol>
<symbol name="BA5210FS">
<pin name="PWRGND" direction="pwr"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="ST/BTL"/>
<pin name="F"/>
<pin name="BIASIN" direction="in"/>
<pin name="STBY"/>
<pin name="MUTE"/>
<pin name="B/OUT" direction="out"/>
<pin name="PREGND" direction="pwr"/>
<pin name="INL" direction="in"/>
<pin name="NFL"/>
<pin name="INR" direction="in"/>
<pin name="NFR"/>
<pin name="OUTC" direction="out"/>
</symbol>
<symbol name="TDA8593J">
<pin name="1/ADSEL"/>
<pin name="2/SDA"/>
<pin name="3/PGND2" direction="pwr"/>
<pin name="4/OUTRR-" direction="out"/>
<pin name="5/SCL"/>
<pin name="6/OUTRR+" direction="out"/>
<pin name="7/VP2" direction="pwr"/>
<pin name="8/OUTRF-" direction="out"/>
<pin name="9/PGND1" direction="pwr"/>
<pin name="10/OUTRF+" direction="out"/>
<pin name="11/SVR"/>
<pin name="12/INRF" direction="in"/>
<pin name="13/INRR" direction="in"/>
<pin name="14/SGND" direction="pwr"/>
<pin name="15/INLR" direction="in"/>
<pin name="16/INLF" direction="in"/>
<pin name="17/ACGND" direction="pwr"/>
<pin name="18/OUTLF+" direction="out"/>
<pin name="19/PGND3" direction="pwr"/>
<pin name="20/OUTLF-" direction="out"/>
<pin name="21/VP1" direction="pwr"/>
<pin name="22/OUTLR+" direction="out"/>
<pin name="23/STMB"/>
<pin name="24/OUTLR-" direction="out"/>
<pin name="25/PGND4" direction="pwr"/>
<pin name="26/DIAG"/>
<pin name="27/TAB"/>
</symbol>
<symbol name="TDA8589XJ">
<pin name="1/PGND2_TAB" direction="pwr"/>
<pin name="2/SDA"/>
<pin name="3/OUT3-" direction="out"/>
<pin name="4/SCL"/>
<pin name="5/OUT3+" direction="out"/>
<pin name="6/VP2" direction="pwr"/>
<pin name="7/OUT1-" direction="out"/>
<pin name="8/PGND1" direction="pwr"/>
<pin name="9/OUT1+" direction="out"/>
<pin name="10/SVR"/>
<pin name="11/IN1" direction="in"/>
<pin name="12/IN3" direction="in"/>
<pin name="13/SGND" direction="pwr"/>
<pin name="14/IN4" direction="in"/>
<pin name="15/IN2" direction="in"/>
<pin name="16/ACGND" direction="pwr"/>
<pin name="17/OUT2+" direction="out"/>
<pin name="18/PGND3" direction="pwr"/>
<pin name="19/OUT2-" direction="out"/>
<pin name="20/VP1" direction="pwr"/>
<pin name="21/OUT4+" direction="out"/>
<pin name="22/STB"/>
<pin name="23/OUT4-" direction="out"/>
<pin name="24/PGND4" direction="pwr"/>
<pin name="25/DIAG"/>
<pin name="26/RST"/>
<pin name="27/SW2"/>
<pin name="28/RESCAP"/>
<pin name="29/SW1"/>
<pin name="30/REG1"/>
<pin name="31/REG3"/>
<pin name="32/GND" direction="pwr"/>
<pin name="33/REG4"/>
<pin name="34/REG5"/>
<pin name="35/VP" direction="pwr"/>
<pin name="36/BUCAP"/>
<pin name="37/REG2"/>
</symbol>
<symbol name="TFA9843J">
<pin name="IN2+" direction="in"/>
<pin name="OUT2-" direction="out"/>
<pin name="CIV"/>
<pin name="IN1+" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SVR"/>
<pin name="MODE"/>
<pin name="OUT1+" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TDA8943SF">
<pin name="1/OUT-" direction="out"/>
<pin name="2/VCC" direction="pwr"/>
<pin name="3/OUT+" direction="out"/>
<pin name="4/IN+" direction="in"/>
<pin name="5/IN-" direction="in"/>
<pin name="6/SVR"/>
<pin name="7/MODE"/>
<pin name="8/GND" direction="pwr"/>
<pin name="9/NC" direction="nc"/>
</symbol>
<symbol name="BA3528/9AFP">
<pin name="1/P_MUT_SW"/>
<pin name="2/P_OUT2" direction="out"/>
<pin name="3/COM"/>
<pin name="4/MOT+" direction="out"/>
<pin name="5/MOT-" direction="out"/>
<pin name="6/VOC1" direction="pwr"/>
<pin name="7/VOC2" direction="pwr"/>
<pin name="8/PGND1" direction="pwr"/>
<pin name="9/MTER"/>
<pin name="10/PHASE"/>
<pin name="11/VREF"/>
<pin name="12/P_OUT1" direction="out"/>
<pin name="13/NC" direction="nc"/>
<pin name="14/NC" direction="nc"/>
<pin name="15/P_IN1" direction="in"/>
<pin name="16/PREOUT1" direction="out"/>
<pin name="17/PREQ1"/>
<pin name="18/PRENF1"/>
<pin name="19/PREIN1" direction="in"/>
<pin name="20/NC" direction="nc"/>
<pin name="21/PREGND" direction="pwr"/>
<pin name="22/BIAS"/>
<pin name="23/PREIN2" direction="in"/>
<pin name="24PRENF2"/>
<pin name="25/PREQ2"/>
<pin name="26/PREOUT2" direction="out"/>
<pin name="27/P_IN2" direction="in"/>
<pin name="28/FILTER"/>
<pin name="29/PGND2" direction="pwr"/>
<pin name="30/PGND" direction="pwr"/>
</symbol>
<symbol name="TA8238K">
<pin name="B.S.1" direction="pas"/>
<pin name="B.S.2" direction="pas"/>
<pin name="ST-BY" direction="pas"/>
<pin name="SMOOTHING" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="PRE-GND" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="NF2" direction="in"/>
<pin name="RIP." direction="pas"/>
<pin name="IN1" direction="in"/>
<pin name="NF1" direction="in"/>
<pin name="TJ-DET" direction="pas"/>
<pin name="PW-GND" direction="pas"/>
<pin name="IN2" direction="in"/>
</symbol>
<symbol name="AN7118S">
<pin name="1" direction="pwr"/>
<pin name="2" direction="out"/>
<pin name="3" direction="oc"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8" direction="in"/>
<pin name="9" direction="pwr"/>
<pin name="10"/>
<pin name="11" direction="out"/>
<pin name="12" direction="nc"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17" direction="in"/>
<pin name="18" direction="pwr"/>
</symbol>
<symbol name="CXA1622M/P">
<pin name="1/IN2" direction="in"/>
<pin name="2/SW"/>
<pin name="3/NC" direction="nc"/>
<pin name="4/NF2"/>
<pin name="5/GND" direction="pwr"/>
<pin name="6/PG2" direction="pwr"/>
<pin name="7/OUT2" direction="out"/>
<pin name="8/RIP"/>
<pin name="9/VCC" direction="pwr"/>
<pin name="10/OUT1" direction="out"/>
<pin name="11/PGN1" direction="pwr"/>
<pin name="12GND1" direction="pwr"/>
<pin name="13/NF1"/>
<pin name="14/VOL"/>
<pin name="15/REG"/>
<pin name="16/IN1" direction="in"/>
</symbol>
<symbol name="BA5417">
<pin name="1/NC" direction="nc"/>
<pin name="2/BS2"/>
<pin name="3/OUT2" direction="out"/>
<pin name="4/VCC" direction="pwr"/>
<pin name="5/OUT1" direction="out"/>
<pin name="6/BS1"/>
<pin name="7/PGND" direction="pwr"/>
<pin name="8/STBY"/>
<pin name="9/FILTER"/>
<pin name="10/NF1"/>
<pin name="11/IN1" direction="in"/>
<pin name="12/IN2" direction="in"/>
<pin name="13/NF2"/>
<pin name="14/PREGND1" direction="pwr"/>
<pin name="15/PREGND2" direction="pwr"/>
</symbol>
<symbol name="AN12941A">
<pin name="P$1" direction="pwr"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4" direction="in"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15" direction="pwr"/>
<pin name="P$16" direction="in"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20" direction="pwr"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23" direction="pwr"/>
<pin name="P$24" direction="out"/>
<pin name="P$25" direction="out"/>
<pin name="P$26" direction="out"/>
<pin name="P$27" direction="out"/>
<pin name="P$28" direction="pwr"/>
<pin name="P$29" direction="pwr"/>
<pin name="P$30" direction="out"/>
<pin name="P$31" direction="out"/>
<pin name="P$32" direction="out"/>
<pin name="P$33" direction="out"/>
<pin name="P$34" direction="pwr"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37" direction="pwr"/>
<pin name="P$38"/>
<pin name="P$39" direction="out"/>
<pin name="P$40"/>
<pin name="P$41" direction="in"/>
<pin name="P$42" direction="pwr"/>
<pin name="P$43" direction="out"/>
<pin name="P$44" direction="out"/>
<pin name="P$45"/>
<pin name="P$46" direction="out"/>
<pin name="P$47" direction="in"/>
<pin name="P$48" direction="out"/>
<pin name="P$49" direction="out"/>
<pin name="P$50" direction="in"/>
<pin name="P$51" direction="out"/>
<pin name="P$52" direction="in"/>
<pin name="P$53"/>
<pin name="P$54" direction="in"/>
<pin name="P$55" direction="pwr"/>
<pin name="P$56" direction="in"/>
</symbol>
<symbol name="LM3876">
<pin name="1" direction="pwr"/>
<pin name="2" direction="nc"/>
<pin name="3" direction="out"/>
<pin name="4" direction="pwr"/>
<pin name="5" direction="nc"/>
<pin name="6" direction="nc"/>
<pin name="7" direction="pwr"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10" direction="in"/>
<pin name="11" direction="nc"/>
</symbol>
<symbol name="LM3886">
<pin name="1" direction="pwr"/>
<pin name="2" direction="pwr"/>
<pin name="3" direction="out"/>
<pin name="4" direction="pwr"/>
<pin name="5" direction="pwr"/>
<pin name="6" direction="nc"/>
<pin name="7" direction="pwr"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10" direction="in"/>
<pin name="11" direction="nc"/>
</symbol>
<symbol name="TDA1519CTD">
<pin name="1/RR"/>
<pin name="2/NC" direction="nc"/>
<pin name="3/OUT" direction="out"/>
<pin name="4/NC" direction="nc"/>
<pin name="5/GND" direction="pwr"/>
<pin name="6/NC" direction="nc"/>
<pin name="7/NC" direction="nc"/>
<pin name="8/OUT2" direction="out"/>
<pin name="9/NC" direction="nc"/>
<pin name="10/VP" direction="pwr"/>
<pin name="11/M_SS"/>
<pin name="12/INV"/>
<pin name="13/NC" direction="nc"/>
<pin name="14/NC" direction="nc"/>
<pin name="15/NC" direction="nc"/>
<pin name="16/NC" direction="nc"/>
<pin name="17/NC" direction="nc"/>
<pin name="18/NC" direction="nc"/>
<pin name="19/NINV"/>
<pin name="20/GND1" direction="pwr"/>
</symbol>
<symbol name="44-PIN">
<pin name="PSU_REF"/>
<pin name="VDD"/>
<pin name="OC_ADJ"/>
<pin name="RESET"/>
<pin name="C_STARTUP"/>
<pin name="INPUT_A"/>
<pin name="INPUT_B"/>
<pin name="VI_CM"/>
<pin name="GND"/>
<pin name="AGND"/>
<pin name="VREG"/>
<pin name="INPUT_C"/>
<pin name="INPUT_D"/>
<pin name="FREQ_ADJ"/>
<pin name="OSC_IO+"/>
<pin name="OSC_IO-"/>
<pin name="SD"/>
<pin name="OTW"/>
<pin name="READY"/>
<pin name="M1"/>
<pin name="M2"/>
<pin name="M3"/>
<pin name="GVDD_CD"/>
<pin name="BST_D"/>
<pin name="PVDD_D1"/>
<pin name="PVDD_D2"/>
<pin name="OUT_D1"/>
<pin name="OUT_D2"/>
<pin name="GND_D"/>
<pin name="GND_C"/>
<pin name="OUT_C"/>
<pin name="PVDD_C"/>
<pin name="BST_C"/>
<pin name="BST_B"/>
<pin name="PVDD_B"/>
<pin name="OUT_B"/>
<pin name="GND_B"/>
<pin name="GND_A"/>
<pin name="OUT_A1"/>
<pin name="OUT_A2"/>
<pin name="PVDD_A1"/>
<pin name="PVDD_A2"/>
<pin name="BST_A"/>
<pin name="GVDD_AB"/>
</symbol>
<symbol name="TDA8568Q">
<pin name="1/VP1" direction="pwr"/>
<pin name="2/OUT1+" direction="out"/>
<pin name="3/PGND1" direction="pwr"/>
<pin name="4/OUT1-" direction="out"/>
<pin name="5/OUT2-" direction="out"/>
<pin name="6/PGND2" direction="pwr"/>
<pin name="7/OUT2+" direction="out"/>
<pin name="8/VP2" direction="pwr"/>
<pin name="9/VDIAG"/>
<pin name="10/IN1" direction="in"/>
<pin name="11/IN2" direction="in"/>
<pin name="12/SGND" direction="pwr"/>
<pin name="13/IN3" direction="in"/>
<pin name="14/IN4" direction="in"/>
<pin name="15/MODE"/>
<pin name="16/VP3" direction="pwr"/>
<pin name="17/OUT3+" direction="out"/>
<pin name="18/PGND3" direction="pwr"/>
<pin name="19/OUT3-" direction="out"/>
<pin name="20/OUT4-" direction="out"/>
<pin name="21/PGND4" direction="pwr"/>
<pin name="22/OUT4+" direction="out"/>
<pin name="23/VP4" direction="pwr"/>
</symbol>
<symbol name="TDA1519CSP">
<pin name="1/NINV"/>
<pin name="2/GND1" direction="pwr"/>
<pin name="3/RR"/>
<pin name="4/OUT1" direction="out"/>
<pin name="5/GND2" direction="pwr"/>
<pin name="6/OUT2" direction="out"/>
<pin name="7/VP" direction="pwr"/>
<pin name="8/M_SS"/>
<pin name="9/INV"/>
</symbol>
<symbol name="TDA8586TH">
<pin name="1" direction="nc"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11" direction="out"/>
<pin name="12"/>
<pin name="13" direction="pwr"/>
<pin name="14" direction="out"/>
<pin name="15" direction="pwr"/>
<pin name="16" direction="pwr"/>
<pin name="17" direction="out"/>
<pin name="18" direction="pwr"/>
<pin name="19"/>
<pin name="20" direction="out"/>
</symbol>
<symbol name="TDA8586Q">
<pin name="1" direction="out"/>
<pin name="2" direction="pwr"/>
<pin name="3"/>
<pin name="4" direction="out"/>
<pin name="5" direction="in"/>
<pin name="6" direction="in"/>
<pin name="7" direction="in"/>
<pin name="8" direction="in"/>
<pin name="9" direction="pwr"/>
<pin name="10" direction="pwr"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14" direction="out"/>
<pin name="15"/>
<pin name="16" direction="pwr"/>
<pin name="17" direction="out"/>
</symbol>
<symbol name="TDA7376PD">
<pin name="1"/>
<pin name="2" direction="pwr"/>
<pin name="3" direction="pwr"/>
<pin name="4" direction="nc"/>
<pin name="5" direction="out"/>
<pin name="6" direction="out"/>
<pin name="7" direction="nc"/>
<pin name="8" direction="out"/>
<pin name="9" direction="out"/>
<pin name="10" direction="pwr"/>
<pin name="11" direction="pwr"/>
<pin name="12" direction="in"/>
<pin name="13" direction="in"/>
<pin name="14" direction="nc"/>
<pin name="15" direction="nc"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18" direction="pwr"/>
<pin name="19" direction="nc"/>
<pin name="20"/>
<pin name="21" direction="out"/>
<pin name="22" direction="nc"/>
<pin name="23" direction="nc"/>
<pin name="24" direction="in"/>
<pin name="25" direction="in"/>
<pin name="26" direction="pwr"/>
<pin name="27" direction="pwr"/>
<pin name="28" direction="out"/>
<pin name="29" direction="out"/>
<pin name="30" direction="nc"/>
<pin name="31" direction="out"/>
<pin name="32" direction="out"/>
<pin name="33" direction="out"/>
<pin name="34" direction="pwr"/>
<pin name="35" direction="pwr"/>
<pin name="36" direction="nc"/>
</symbol>
<symbol name="M5218AL/P/FP">
<pin name="1/OUT1" direction="out"/>
<pin name="2/-IN1" direction="in"/>
<pin name="3/+IN1" direction="in"/>
<pin name="4/GND" direction="pwr"/>
<pin name="5/+IN2" direction="in"/>
<pin name="6/-IN" direction="in"/>
<pin name="7/OUT2" direction="out"/>
<pin name="8/VCC" direction="pwr"/>
</symbol>
<symbol name="TA2022">
<pin name="OAOUT1" direction="out"/>
<pin name="INV1" direction="in"/>
<pin name="BIASCAP" direction="pas"/>
<pin name="MUTE" direction="in"/>
<pin name="OAOUT2" direction="out"/>
<pin name="INV2" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="V5@1" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="V5@2" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="VNNSENSE" direction="in"/>
<pin name="VPPSENSE" direction="in"/>
<pin name="VPP2" direction="pwr"/>
<pin name="VNN2" direction="pwr"/>
<pin name="VPP1" direction="pwr"/>
<pin name="VNN1" direction="pwr"/>
<pin name="VN10FBK" direction="out"/>
<pin name="VN10SW" direction="out"/>
<pin name="VN10GND" direction="pwr"/>
<pin name="VN10" direction="in"/>
<pin name="FBKGND2" direction="out"/>
<pin name="FBKOUT2" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="VBOOT2" direction="in"/>
<pin name="HMUTE" direction="out"/>
<pin name="FBKGND1"/>
<pin name="FBKOUT1" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="VBOOT1" direction="in"/>
</symbol>
<symbol name="NTE1898">
<pin name="1/IN1" direction="in"/>
<pin name="2/NF1"/>
<pin name="3/PGND" direction="pwr"/>
<pin name="4/NF2"/>
<pin name="5/IN2" direction="in"/>
<pin name="6/RIP"/>
<pin name="7/OUT2" direction="out"/>
<pin name="8/BST2"/>
<pin name="GND" direction="pwr"/>
<pin name="10/VCC" direction="pwr"/>
<pin name="11/BST1"/>
<pin name="12/OUT1" direction="out"/>
</symbol>
<symbol name="TA7251BP">
<pin name="1/OUT1" direction="out"/>
<pin name="2/BS1"/>
<pin name="3/VCC" direction="pwr"/>
<pin name="4/GND" direction="pwr"/>
<pin name="5/BS2"/>
<pin name="6/OUT2" direction="out"/>
<pin name="7/CRIP"/>
<pin name="8/NF2"/>
<pin name="9/IN-" direction="in"/>
<pin name="10/PGND" direction="pwr"/>
<pin name="11/IN+" direction="in"/>
<pin name="12/NF1"/>
</symbol>
<symbol name="TDA7266SA">
<pin name="1/OUT1+" direction="out"/>
<pin name="2/OUT1-" direction="out"/>
<pin name="3/VCC" direction="pwr"/>
<pin name="4/IN1" direction="in"/>
<pin name="5/NC" direction="nc"/>
<pin name="6/MUTE"/>
<pin name="7/ST-BY"/>
<pin name="8/PWGND" direction="pwr"/>
<pin name="9/SGND" direction="pwr"/>
<pin name="10/NC" direction="nc"/>
<pin name="11/NC" direction="nc"/>
<pin name="12/IN2" direction="in"/>
<pin name="13/VCC" direction="pwr"/>
<pin name="14/OUT2-" direction="out"/>
<pin name="15/OUT2+" direction="out"/>
</symbol>
<symbol name="TBA810AS">
<pin name="12" direction="out"/>
<pin name="8" direction="in"/>
<pin name="9" direction="in"/>
<pin name="VCC/1" direction="pwr"/>
<pin name="7"/>
<pin name="5"/>
<pin name="3"/>
<pin name="4"/>
<pin name="10/GND" direction="pwr"/>
<pin name="6"/>
<pin name="2" direction="nc"/>
<pin name="11" direction="nc"/>
<pin name="P$1" direction="pwr"/>
<pin name="P$2" direction="pwr"/>
<pin name="P$3" direction="pwr"/>
<pin name="P$4" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TDA1521Q" prefix="US" uservalue="yes">
<description>&lt;b&gt;2 x 12 W hi-fi audio power amplifier&lt;/b&gt;&lt;br&gt;
&lt;a href&gt;http://www.datasheetcatalog.org/datasheet/philips/TDA1521Q.pdf&lt;/a&gt;</description>
<gates>
<gate name="TDA1521Q" symbol="TDA1521Q"/>
</gates>
<devices>
<device name="PION" package="SOT131-2H">
<connects>
<connect gate="TDA1521Q" pin="+VP" pad="7"/>
<connect gate="TDA1521Q" pin="-INV1" pad="1"/>
<connect gate="TDA1521Q" pin="-INV2" pad="9"/>
<connect gate="TDA1521Q" pin="-VP" pad="5"/>
<connect gate="TDA1521Q" pin="GND" pad="3"/>
<connect gate="TDA1521Q" pin="INV1" pad="2"/>
<connect gate="TDA1521Q" pin="INV2" pad="8"/>
<connect gate="TDA1521Q" pin="OUT1" pad="4"/>
<connect gate="TDA1521Q" pin="OUT2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT157-2" package="SOT157-2">
<connects>
<connect gate="TDA1521Q" pin="+VP" pad="7"/>
<connect gate="TDA1521Q" pin="-INV1" pad="1"/>
<connect gate="TDA1521Q" pin="-INV2" pad="9"/>
<connect gate="TDA1521Q" pin="-VP" pad="5"/>
<connect gate="TDA1521Q" pin="GND" pad="3"/>
<connect gate="TDA1521Q" pin="INV1" pad="2"/>
<connect gate="TDA1521Q" pin="INV2" pad="8"/>
<connect gate="TDA1521Q" pin="OUT1" pad="4"/>
<connect gate="TDA1521Q" pin="OUT2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1554" prefix="US">
<description>The TDA1554Q is an integrated class-B output amplifier in a 17-lead single-in-line (SIL) plastic power package.
The circuit contains 4 x 11 W single-ended or 2 x 22 W bridge amplifiers. The device is primarily developed for car radio
applications.</description>
<gates>
<gate name="G$1" symbol="TDA1554"/>
</gates>
<devices>
<device name="Q" package="SOT243-1">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="INV2" pad="16"/>
<connect gate="G$1" pin="M/SS" pad="14"/>
<connect gate="G$1" pin="NINV1" pad="1"/>
<connect gate="G$1" pin="NINV2" pad="17"/>
<connect gate="G$1" pin="NIV1" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="OUT3" pad="10"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="RR" pad="4"/>
<connect gate="G$1" pin="VP1" pad="5"/>
<connect gate="G$1" pin="VP2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1558Q" prefix="IC" uservalue="yes">
<description>http://www.datasheetcatalog.com/datasheets_pdf/T/D/A/1/TDA1558.shtml</description>
<gates>
<gate name="G$1" symbol="TDA1558Q"/>
</gates>
<devices>
<device name="" package="SOT243-1">
<connects>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="GNDSIG" pad="3"/>
<connect gate="G$1" pin="IN3" pad="17"/>
<connect gate="G$1" pin="INPUT1" pad="1"/>
<connect gate="G$1" pin="INPUT2" pad="2"/>
<connect gate="G$1" pin="INPUT4" pad="16"/>
<connect gate="G$1" pin="IRV" pad="15"/>
<connect gate="G$1" pin="MUTE" pad="14"/>
<connect gate="G$1" pin="N/C" pad="9"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="OUT3" pad="12"/>
<connect gate="G$1" pin="OUT4" pad="10"/>
<connect gate="G$1" pin="RR" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2003" prefix="IC">
<description>Car Radio Audio Amplifier</description>
<gates>
<gate name="IC" symbol="TDA200X"/>
</gates>
<devices>
<device name="" package="PENTAWATT-V">
<connects>
<connect gate="IC" pin="+IN" pad="1"/>
<connect gate="IC" pin="-IN" pad="2"/>
<connect gate="IC" pin="GND" pad="3"/>
<connect gate="IC" pin="OUT" pad="4"/>
<connect gate="IC" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8560Q" prefix="IC" uservalue="yes">
<description>2x40W Stereo BTL Amplifier</description>
<gates>
<gate name="G$1" symbol="TDA8560Q"/>
</gates>
<devices>
<device name="" package="SOT141-6">
<connects>
<connect gate="G$1" pin="GND(S)" pad="P$2"/>
<connect gate="G$1" pin="GND1" pad="P$5"/>
<connect gate="G$1" pin="GND2" pad="P$8"/>
<connect gate="G$1" pin="IN1" pad="P$1"/>
<connect gate="G$1" pin="IN2" pad="P$13"/>
<connect gate="G$1" pin="MODE" pad="P$11"/>
<connect gate="G$1" pin="OUT1A" pad="P$4"/>
<connect gate="G$1" pin="OUT1B" pad="P$6"/>
<connect gate="G$1" pin="OUT2A" pad="P$7"/>
<connect gate="G$1" pin="OUT2B" pad="P$9"/>
<connect gate="G$1" pin="VDIAG" pad="P$12"/>
<connect gate="G$1" pin="VP1" pad="P$3"/>
<connect gate="G$1" pin="VP2" pad="P$10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2004" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2005"/>
<gate name="B" symbol="2005A"/>
</gates>
<devices>
<device name="T" package="SIP11">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BTSP" pad="11"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="SVRR" pad="3"/>
<connect gate="A" pin="V+" pad="9"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="BTSP" pad="7"/>
<connect gate="B" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2005" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2005"/>
<gate name="B" symbol="2005A"/>
</gates>
<devices>
<device name="T" package="SIP11">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BTSP" pad="11"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="SVRR" pad="3"/>
<connect gate="A" pin="V+" pad="9"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="BTSP" pad="7"/>
<connect gate="B" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2006" prefix="IC">
<description>&lt;b&gt;AUDIO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2008" prefix="IC">
<description>&lt;b&gt;AUDIO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+GN"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2009" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2005"/>
<gate name="B" symbol="2005A"/>
</gates>
<devices>
<device name="T" package="SIP11">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BTSP" pad="11"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="SVRR" pad="3"/>
<connect gate="A" pin="V+" pad="9"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="BTSP" pad="7"/>
<connect gate="B" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2030" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+GN"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2040" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UL1440" prefix="IC">
<gates>
<gate name="1" symbol="UL1440"/>
<gate name="P" symbol="2GND"/>
</gates>
<devices>
<device name="T" package="CE82">
<connects>
<connect gate="1" pin="BOSTRAP" pad="4"/>
<connect gate="1" pin="FCORE" pad="5"/>
<connect gate="1" pin="F_BACK" pad="6"/>
<connect gate="1" pin="GND" pad="9"/>
<connect gate="1" pin="GND@" pad="10"/>
<connect gate="1" pin="IN" pad="8"/>
<connect gate="1" pin="OUT" pad="12"/>
<connect gate="1" pin="TW" pad="7"/>
<connect gate="1" pin="VCC" pad="1"/>
<connect gate="P" pin="GND@8" pad="GND"/>
<connect gate="P" pin="GND@9" pad="@GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TA8210A?*" prefix="IC">
<description>&lt;b&gt;20W BTL × 2ch Audio Power Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.semicon.toshiba.co.jp/td/en/ASSP/Audio_ICs/en_20050517_TA8210ALQ_datasheet.pdf</description>
<gates>
<gate name="G$1" symbol="TA8210"/>
</gates>
<devices>
<device name="L" package="HSIP17-P-2.00">
<connects>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="13"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="MUTE_SW" pad="1"/>
<connect gate="G$1" pin="NF1" pad="3"/>
<connect gate="G$1" pin="NF2" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="16"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="PRE-GND" pad="5"/>
<connect gate="G$1" pin="PRE-VCC" pad="9"/>
<connect gate="G$1" pin="RIPPLE" pad="8"/>
<connect gate="G$1" pin="STAND-BY_SW" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
<technology name="Q"/>
</technologies>
</device>
<device name="H" package="HZIP17-P-2.00">
<connects>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="13"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="MUTE_SW" pad="1"/>
<connect gate="G$1" pin="NF1" pad="3"/>
<connect gate="G$1" pin="NF2" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="16"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="PRE-GND" pad="5"/>
<connect gate="G$1" pin="PRE-VCC" pad="9"/>
<connect gate="G$1" pin="RIPPLE" pad="8"/>
<connect gate="G$1" pin="STAND-BY_SW" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
<technology name="Q"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1516BQ" prefix="IC">
<description>&lt;b&gt;radio power amplifier&lt;/b&gt;&lt;p&gt;
24 W BTL or 2 x 12 watt stereo car&lt;br&gt;
Source: TDA1516BQ_1.pdf</description>
<gates>
<gate name="G$1" symbol="TDA1516"/>
</gates>
<devices>
<device name="" package="MULTIWAT-SIL13">
<connects>
<connect gate="G$1" pin="GNDP" pad="7"/>
<connect gate="G$1" pin="GNDS" pad="3"/>
<connect gate="G$1" pin="IN1+" pad="1"/>
<connect gate="G$1" pin="IN1-" pad="2"/>
<connect gate="G$1" pin="IN2+" pad="13"/>
<connect gate="G$1" pin="INT_VP1/2" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="STDBY" pad="11"/>
<connect gate="G$1" pin="VP" pad="10"/>
<connect gate="G$1" pin="VP1" pad="6"/>
<connect gate="G$1" pin="VP2" pad="8"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1560Q" prefix="IC">
<description>&lt;b&gt;40 W car radio high power amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TDA1560Q"/>
</gates>
<devices>
<device name="" package="MULTIWAT-SIL17">
<connects>
<connect gate="G$1" pin="C1+" pad="10"/>
<connect gate="G$1" pin="C1-" pad="13"/>
<connect gate="G$1" pin="C2+" pad="8"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="CDEC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="INPN" pad="2"/>
<connect gate="G$1" pin="INPP" pad="1"/>
<connect gate="G$1" pin="MODE" pad="16"/>
<connect gate="G$1" pin="OUT1N" pad="7"/>
<connect gate="G$1" pin="OUT2P" pad="11"/>
<connect gate="G$1" pin="S1" pad="17"/>
<connect gate="G$1" pin="SIG-GND" pad="3"/>
<connect gate="G$1" pin="VDIAG" pad="14"/>
<connect gate="G$1" pin="VP" pad="9"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1562" prefix="IC">
<description>&lt;b&gt;70 W High Efficiency Power Amplifier&lt;/b&gt;&lt;p&gt;
with diagnostic facility</description>
<gates>
<gate name="G$1" symbol="TDA1562"/>
</gates>
<devices>
<device name="Q" package="MULTIWAT-SIL17">
<connects>
<connect gate="G$1" pin="C1+" pad="5"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="13"/>
<connect gate="G$1" pin="C2-" pad="15"/>
<connect gate="G$1" pin="DIAGNOSTIC" pad="8"/>
<connect gate="G$1" pin="IN+" pad="1"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="M-SEL" pad="4"/>
<connect gate="G$1" pin="OUT+" pad="7"/>
<connect gate="G$1" pin="OUT-" pad="11"/>
<connect gate="G$1" pin="PGND1" pad="6"/>
<connect gate="G$1" pin="PGND2" pad="12"/>
<connect gate="G$1" pin="SIG-GND" pad="17"/>
<connect gate="G$1" pin="STATUS_IO" pad="16"/>
<connect gate="G$1" pin="VP1" pad="9"/>
<connect gate="G$1" pin="VP2" pad="10"/>
<connect gate="G$1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UPC1237HA" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="UPC1237HA"/>
</gates>
<devices>
<device name="" package="SIP8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7294*" prefix="IC">
<description>100V - 100W DMOS Audio Amplifier with Mute/Standby</description>
<gates>
<gate name="G$1" symbol="TDA7294"/>
</gates>
<devices>
<device name="HS" package="MULTIWATT15H">
<connects>
<connect gate="G$1" pin="BOOTSTRAP" pad="6"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN+MUTE" pad="4"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="MUTE" pad="10"/>
<connect gate="G$1" pin="OUT" pad="14"/>
<connect gate="G$1" pin="PWVS+" pad="13"/>
<connect gate="G$1" pin="PWVS-" pad="15"/>
<connect gate="G$1" pin="STBY" pad="9"/>
<connect gate="G$1" pin="STBY-GND" pad="1"/>
<connect gate="G$1" pin="VS+" pad="7"/>
<connect gate="G$1" pin="VS-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="MULTIWATT15V">
<connects>
<connect gate="G$1" pin="BOOTSTRAP" pad="6"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN+MUTE" pad="4"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="MUTE" pad="10"/>
<connect gate="G$1" pin="OUT" pad="14"/>
<connect gate="G$1" pin="PWVS+" pad="13"/>
<connect gate="G$1" pin="PWVS-" pad="15"/>
<connect gate="G$1" pin="STBY" pad="9"/>
<connect gate="G$1" pin="STBY-GND" pad="1"/>
<connect gate="G$1" pin="VS+" pad="7"/>
<connect gate="G$1" pin="VS-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7293*" prefix="IC">
<description>120V - 100W DMOS Audio Amplifier with Mute/Standby</description>
<gates>
<gate name="G$1" symbol="TDA7293"/>
</gates>
<devices>
<device name="HS" package="MULTIWATT15H">
<connects>
<connect gate="G$1" pin="BOOSTRAP" pad="6"/>
<connect gate="G$1" pin="BOOTLOADER" pad="12"/>
<connect gate="G$1" pin="BUFFER" pad="11"/>
<connect gate="G$1" pin="CLIP" pad="5"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="MUTE" pad="10"/>
<connect gate="G$1" pin="OUT" pad="14"/>
<connect gate="G$1" pin="PWVS+" pad="13"/>
<connect gate="G$1" pin="PWVS-" pad="15"/>
<connect gate="G$1" pin="SGND" pad="4"/>
<connect gate="G$1" pin="STBY" pad="9"/>
<connect gate="G$1" pin="STBY-GND" pad="1"/>
<connect gate="G$1" pin="VS+" pad="7"/>
<connect gate="G$1" pin="VS-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="MULTIWATT15V">
<connects>
<connect gate="G$1" pin="BOOSTRAP" pad="6"/>
<connect gate="G$1" pin="BOOTLOADER" pad="12"/>
<connect gate="G$1" pin="BUFFER" pad="11"/>
<connect gate="G$1" pin="CLIP" pad="5"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="MUTE" pad="10"/>
<connect gate="G$1" pin="OUT" pad="14"/>
<connect gate="G$1" pin="PWVS+" pad="13"/>
<connect gate="G$1" pin="PWVS-" pad="15"/>
<connect gate="G$1" pin="SGND" pad="4"/>
<connect gate="G$1" pin="STBY" pad="9"/>
<connect gate="G$1" pin="STBY-GND" pad="1"/>
<connect gate="G$1" pin="VS+" pad="7"/>
<connect gate="G$1" pin="VS-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7375" prefix="IC">
<gates>
<gate name="G$1" symbol="TDA7375"/>
</gates>
<devices>
<device name="H" package="MULTIWATT-15H">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="PWRGND" pad="8"/>
<connect gate="G$1" pin="SGNG" pad="9"/>
<connect gate="G$1" pin="STD-BY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1-2" pad="3"/>
<connect gate="G$1" pin="VCC3-4" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="MULTIWATT-15V">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="PWRGND" pad="8"/>
<connect gate="G$1" pin="SGNG" pad="9"/>
<connect gate="G$1" pin="STD-BY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1-2" pad="3"/>
<connect gate="G$1" pin="VCC3-4" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7386">
<gates>
<gate name="G$1" symbol="TDA7386"/>
</gates>
<devices>
<device name="" package="FLEXIWATT25">
<connects>
<connect gate="G$1" pin="AC-GND" pad="P$16"/>
<connect gate="G$1" pin="IN1" pad="P$11"/>
<connect gate="G$1" pin="IN2" pad="P$12"/>
<connect gate="G$1" pin="IN3" pad="P$15"/>
<connect gate="G$1" pin="IN4" pad="P$14"/>
<connect gate="G$1" pin="MUTE" pad="P$22"/>
<connect gate="G$1" pin="N.C." pad="P$25"/>
<connect gate="G$1" pin="OUT1+" pad="P$9"/>
<connect gate="G$1" pin="OUT1-" pad="P$7"/>
<connect gate="G$1" pin="OUT2+" pad="P$5"/>
<connect gate="G$1" pin="OUT2-" pad="P$3"/>
<connect gate="G$1" pin="OUT3+" pad="P$17"/>
<connect gate="G$1" pin="OUT3-" pad="P$19"/>
<connect gate="G$1" pin="OUT4+" pad="P$21"/>
<connect gate="G$1" pin="OUT4-" pad="P$23"/>
<connect gate="G$1" pin="PW-GND$1" pad="P$8"/>
<connect gate="G$1" pin="PW-GND$2" pad="P$2"/>
<connect gate="G$1" pin="PW-GND$3" pad="P$18"/>
<connect gate="G$1" pin="PW-GND$4" pad="P$24"/>
<connect gate="G$1" pin="S-GND" pad="P$13"/>
<connect gate="G$1" pin="ST-BY" pad="P$4"/>
<connect gate="G$1" pin="SVR" pad="P$10"/>
<connect gate="G$1" pin="TAB" pad="P$1"/>
<connect gate="G$1" pin="VCC1" pad="P$6"/>
<connect gate="G$1" pin="VCC2" pad="P$20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8571J" prefix="IC" uservalue="yes">
<description>2x40W Stereo BTL Amplifier</description>
<gates>
<gate name="G$1" symbol="TDA8571J"/>
</gates>
<devices>
<device name="" package="SOT411-1">
<connects>
<connect gate="G$1" pin="IN1" pad="P$10"/>
<connect gate="G$1" pin="IN2" pad="P$11"/>
<connect gate="G$1" pin="IN3" pad="P$13"/>
<connect gate="G$1" pin="IN4" pad="P$14"/>
<connect gate="G$1" pin="MODE" pad="P$15"/>
<connect gate="G$1" pin="OUT1+" pad="P$2"/>
<connect gate="G$1" pin="OUT1-" pad="P$4"/>
<connect gate="G$1" pin="OUT2+" pad="P$7"/>
<connect gate="G$1" pin="OUT2-" pad="P$5"/>
<connect gate="G$1" pin="OUT3+" pad="P$17"/>
<connect gate="G$1" pin="OUT3-" pad="P$19"/>
<connect gate="G$1" pin="OUT4+" pad="P$22"/>
<connect gate="G$1" pin="OUT4-" pad="P$20"/>
<connect gate="G$1" pin="PGND1" pad="P$3"/>
<connect gate="G$1" pin="PGND2" pad="P$6"/>
<connect gate="G$1" pin="PGND3" pad="P$18"/>
<connect gate="G$1" pin="PGND4" pad="P$21"/>
<connect gate="G$1" pin="SGND" pad="P$12"/>
<connect gate="G$1" pin="VDIAG" pad="P$9"/>
<connect gate="G$1" pin="VP1" pad="P$1"/>
<connect gate="G$1" pin="VP2" pad="P$8"/>
<connect gate="G$1" pin="VP3" pad="P$16"/>
<connect gate="G$1" pin="VP4" pad="P$23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7050">
<gates>
<gate name="G$1" symbol="TDA7050"/>
</gates>
<devices>
<device name="SO8" package="SO8">
<connects>
<connect gate="G$1" pin="1_INA+" pad="1"/>
<connect gate="G$1" pin="2_INA-" pad="2"/>
<connect gate="G$1" pin="3_INB-" pad="3"/>
<connect gate="G$1" pin="4_INB+" pad="4"/>
<connect gate="G$1" pin="5_GND" pad="5"/>
<connect gate="G$1" pin="6_OUTB" pad="6"/>
<connect gate="G$1" pin="7_OUTA" pad="7"/>
<connect gate="G$1" pin="8_VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1557Q">
<gates>
<gate name="G$1" symbol="TDA1557"/>
</gates>
<devices>
<device name="SIP13" package="SIP13">
<connects>
<connect gate="G$1" pin="10_VP2" pad="10"/>
<connect gate="G$1" pin="11_MUTE" pad="11"/>
<connect gate="G$1" pin="12_NC" pad="12"/>
<connect gate="G$1" pin="13_IN2" pad="13"/>
<connect gate="G$1" pin="1_IN1" pad="1"/>
<connect gate="G$1" pin="2_GNDIN" pad="2"/>
<connect gate="G$1" pin="3_VP1" pad="3"/>
<connect gate="G$1" pin="4_OUT1A" pad="4"/>
<connect gate="G$1" pin="5_GNDPWR" pad="5"/>
<connect gate="G$1" pin="6_OUT1B" pad="6"/>
<connect gate="G$1" pin="7_OUT2A" pad="7"/>
<connect gate="G$1" pin="8_GNDPWR" pad="8"/>
<connect gate="G$1" pin="9_OUT2B" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1308">
<gates>
<gate name="G$1" symbol="TDA1308"/>
</gates>
<devices>
<device name="SO8" package="SO8">
<connects>
<connect gate="G$1" pin="1_OUTA" pad="1"/>
<connect gate="G$1" pin="2_INA-" pad="2"/>
<connect gate="G$1" pin="3_INA+" pad="3"/>
<connect gate="G$1" pin="4_GND" pad="4"/>
<connect gate="G$1" pin="5_INB+" pad="5"/>
<connect gate="G$1" pin="6_INB-" pad="6"/>
<connect gate="G$1" pin="7_OUTB" pad="7"/>
<connect gate="G$1" pin="8_+VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TBA800" prefix="IC" uservalue="yes">
<description>http://www.datasheetcatalog.org/datasheets/480/499897_DS.pdf</description>
<gates>
<gate name="G$1" symbol="TBA800"/>
</gates>
<devices>
<device name="CB-155" package="CE82">
<connects>
<connect gate="G$1" pin="10/GND" pad="10 @GND GND"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="VCC/1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="FINDIP12">
<connects>
<connect gate="G$1" pin="10/GND" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="VCC/1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UL1401*2/3/5" prefix="IC" uservalue="yes">
<description>Polish CEMI UL1401,UL1402,UL1403,UL1405</description>
<gates>
<gate name="G$1" symbol="UL140*"/>
</gates>
<devices>
<device name="" package="CE-50/TO3">
<connects>
<connect gate="G$1" pin="+V" pad="P$3"/>
<connect gate="G$1" pin="GND" pad="P$1"/>
<connect gate="G$1" pin="IN" pad="P$7"/>
<connect gate="G$1" pin="IO" pad="P$9"/>
<connect gate="G$1" pin="IO1" pad="P$8"/>
<connect gate="G$1" pin="IO2" pad="P$6"/>
<connect gate="G$1" pin="IO3" pad="P$5"/>
<connect gate="G$1" pin="NC" pad="P$4"/>
<connect gate="G$1" pin="OUT" pad="P$2"/>
<connect gate="G$1" pin="R" pad="C"/>
<connect gate="G$1" pin="R1" pad="C/"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KA2102A" prefix="IC" uservalue="yes">
<description>http://www.datasheetcatalog.org/datasheet/SamsungElectronic/mXuztvq.pdf</description>
<gates>
<gate name="G$1" symbol="KA2102A"/>
</gates>
<devices>
<device name="" package="14-DIPH-300">
<connects>
<connect gate="G$1" pin="+VC" pad="5"/>
<connect gate="G$1" pin="+VP" pad="10"/>
<connect gate="G$1" pin="BO" pad="9"/>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="F1" pad="11"/>
<connect gate="G$1" pin="FED" pad="6"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="INA" pad="12"/>
<connect gate="G$1" pin="INB" pad="13"/>
<connect gate="G$1" pin="OUD" pad="4"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="SIF" pad="3"/>
<connect gate="G$1" pin="TAB1" pad="P$1"/>
<connect gate="G$1" pin="TAB2" pad="P$2"/>
<connect gate="G$1" pin="TAB3" pad="P$3"/>
<connect gate="G$1" pin="TAB4" pad="P$4"/>
<connect gate="G$1" pin="VOL" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1904" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="TDA1904"/>
</gates>
<devices>
<device name="" package="SOT38-1">
<connects>
<connect gate="G$1" pin="+VSS" pad="2"/>
<connect gate="G$1" pin="BOST" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND1" pad="10"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="GND3" pad="12"/>
<connect gate="G$1" pin="GND4" pad="13"/>
<connect gate="G$1" pin="GND5" pad="14"/>
<connect gate="G$1" pin="GND6" pad="15"/>
<connect gate="G$1" pin="GND7" pad="16"/>
<connect gate="G$1" pin="INV" pad="6"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NC1" pad="5"/>
<connect gate="G$1" pin="NINV" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SVR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KA2206BN" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="KA2206BN"/>
</gates>
<devices>
<device name="" package="12-DIPH-300">
<connects>
<connect gate="G$1" pin="BS1" pad="14"/>
<connect gate="G$1" pin="BS2" pad="3"/>
<connect gate="G$1" pin="BTLOUT" pad="1"/>
<connect gate="G$1" pin="FGND" pad="P$1"/>
<connect gate="G$1" pin="FGND1" pad="P$2"/>
<connect gate="G$1" pin="FGND2" pad="P$3"/>
<connect gate="G$1" pin="FGND3" pad="P$4"/>
<connect gate="G$1" pin="IN1" pad="10"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="NF1" pad="11"/>
<connect gate="G$1" pin="NF2" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="PREGND" pad="9"/>
<connect gate="G$1" pin="RR" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2052">
<description>TDA2052   60W Hi-Fi AUDIO POWER AMPLIFIER
                          WITH MUTE / STAND-BY</description>
<gates>
<gate name="G$1" symbol="TDA2052"/>
</gates>
<devices>
<device name="TDA2052V" package="HEPTAWATT">
<connects>
<connect gate="G$1" pin="+INP" pad="7"/>
<connect gate="G$1" pin="+V" pad="2"/>
<connect gate="G$1" pin="-INP" pad="6"/>
<connect gate="G$1" pin="-INV(MUTE)" pad="5"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="ST/MUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TDA2052H" package="HEPTAW.H">
<connects>
<connect gate="G$1" pin="+INP" pad="7"/>
<connect gate="G$1" pin="+V" pad="2"/>
<connect gate="G$1" pin="-INP" pad="6"/>
<connect gate="G$1" pin="-INV(MUTE)" pad="5"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="ST/MUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7052" prefix="IC">
<description>&lt;b&gt;1 W BTL mono audio amplifier&lt;/b&gt;&lt;p&gt;
Source : www.datasheetcatalog.org/datasheet/philips/TDA7052_CNV_2.pdf</description>
<gates>
<gate name="G$1" symbol="TDA7052"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@" pad="6"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="VP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7393" prefix="IC">
<description>2 x 35W Dual Bridge Car Radio Amplifier</description>
<gates>
<gate name="G$1" symbol="TDA7393"/>
</gates>
<devices>
<device name="H" package="MULTIWATT-15H">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN-MUTE" pad="9"/>
<connect gate="G$1" pin="IN1" pad="6"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="MONO" pad="7"/>
<connect gate="G$1" pin="MUTE1-ST" pad="4"/>
<connect gate="G$1" pin="MUTE2-MO" pad="5"/>
<connect gate="G$1" pin="OUT1+" pad="1"/>
<connect gate="G$1" pin="OUT1-" pad="2"/>
<connect gate="G$1" pin="OUT2+" pad="15"/>
<connect gate="G$1" pin="OUT2-" pad="14"/>
<connect gate="G$1" pin="STD-BY" pad="12"/>
<connect gate="G$1" pin="SVR" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="MULTIWATT-15V">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN-MUTE" pad="9"/>
<connect gate="G$1" pin="IN1" pad="6"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="MONO" pad="7"/>
<connect gate="G$1" pin="MUTE1-ST" pad="4"/>
<connect gate="G$1" pin="MUTE2-MO" pad="5"/>
<connect gate="G$1" pin="OUT1+" pad="1"/>
<connect gate="G$1" pin="OUT1-" pad="2"/>
<connect gate="G$1" pin="OUT2+" pad="15"/>
<connect gate="G$1" pin="OUT2-" pad="14"/>
<connect gate="G$1" pin="STD-BY" pad="12"/>
<connect gate="G$1" pin="SVR" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7372B" uservalue="yes">
<gates>
<gate name="G$1" symbol="TDA7372B"/>
</gates>
<devices>
<device name="" package="MULTIWATT-15V">
<connects>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="MUTE" pad="10"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="PW-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STD-BY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7253" prefix="IC" uservalue="yes">
<description>8W AMPLIFIER WITH MUTING</description>
<gates>
<gate name="G$1" symbol="TDA7253"/>
</gates>
<devices>
<device name="" package="CLIPWATT11">
<connects>
<connect gate="G$1" pin="+VS" pad="P$9"/>
<connect gate="G$1" pin="GND" pad="P$6"/>
<connect gate="G$1" pin="INV/IN" pad="P$4"/>
<connect gate="G$1" pin="NC" pad="P$1"/>
<connect gate="G$1" pin="NC1" pad="P$2"/>
<connect gate="G$1" pin="NC2" pad="P$7"/>
<connect gate="G$1" pin="NC3" pad="P$10"/>
<connect gate="G$1" pin="NC4" pad="P$11"/>
<connect gate="G$1" pin="NINV/IN" pad="P$5"/>
<connect gate="G$1" pin="OUT" pad="P$8"/>
<connect gate="G$1" pin="S/MUTE" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STK4241/2" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="STK4241/2"/>
</gates>
<devices>
<device name="" package="STK4241/2">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="13" pad="P$13"/>
<connect gate="G$1" pin="14" pad="P$14"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="19" pad="P$19"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="20" pad="P$20"/>
<connect gate="G$1" pin="21" pad="P$21"/>
<connect gate="G$1" pin="22" pad="P$22"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1517ATW" prefix="IC" uservalue="yes">
<description>8 W BTL or 2 ´ 4 W SE power amplifier</description>
<gates>
<gate name="G$1" symbol="TDA1517ATW"/>
</gates>
<devices>
<device name="" package="SOT527-1">
<connects>
<connect gate="G$1" pin="HEATHSINK_SIDE" pad="P$21"/>
<connect gate="G$1" pin="IN1" pad="P$3"/>
<connect gate="G$1" pin="IN2-" pad="P$18"/>
<connect gate="G$1" pin="MODE" pad="P$17"/>
<connect gate="G$1" pin="NC" pad="P$1"/>
<connect gate="G$1" pin="NC1" pad="P$2"/>
<connect gate="G$1" pin="NC2" pad="P$6"/>
<connect gate="G$1" pin="NC3" pad="P$7"/>
<connect gate="G$1" pin="NC4" pad="P$14"/>
<connect gate="G$1" pin="NC5" pad="P$19"/>
<connect gate="G$1" pin="NC6" pad="P$20"/>
<connect gate="G$1" pin="OUT1A" pad="P$8"/>
<connect gate="G$1" pin="OUT1B" pad="P$9"/>
<connect gate="G$1" pin="OUT2A" pad="P$12"/>
<connect gate="G$1" pin="OUT2B" pad="P$13"/>
<connect gate="G$1" pin="PGND1" pad="P$10"/>
<connect gate="G$1" pin="PGND2" pad="P$11"/>
<connect gate="G$1" pin="SGND" pad="P$4"/>
<connect gate="G$1" pin="SVRR" pad="P$5"/>
<connect gate="G$1" pin="VP1" pad="P$15"/>
<connect gate="G$1" pin="VP2" pad="P$16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8543" prefix="IC" uservalue="yes">
<description>2 W BTL audio amplifier</description>
<gates>
<gate name="G$1" symbol="TDA8543"/>
</gates>
<devices>
<device name="" package="SOT38-1">
<connects>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="IN+" pad="5"/>
<connect gate="G$1" pin="IN-" pad="6"/>
<connect gate="G$1" pin="MO" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC1" pad="2"/>
<connect gate="G$1" pin="NC2" pad="7"/>
<connect gate="G$1" pin="NC3" pad="8"/>
<connect gate="G$1" pin="NC4" pad="9"/>
<connect gate="G$1" pin="NC5" pad="10"/>
<connect gate="G$1" pin="NC6" pad="15"/>
<connect gate="G$1" pin="NC7" pad="16"/>
<connect gate="G$1" pin="OUT+" pad="14"/>
<connect gate="G$1" pin="OUT-" pad="11"/>
<connect gate="G$1" pin="SVR" pad="4"/>
<connect gate="G$1" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT109-1" package="SOT109-1">
<connects>
<connect gate="G$1" pin="GND" pad="P$13"/>
<connect gate="G$1" pin="IN+" pad="P$5"/>
<connect gate="G$1" pin="IN-" pad="P$6"/>
<connect gate="G$1" pin="MO" pad="P$3"/>
<connect gate="G$1" pin="NC" pad="P$1"/>
<connect gate="G$1" pin="NC1" pad="P$2"/>
<connect gate="G$1" pin="NC2" pad="P$7"/>
<connect gate="G$1" pin="NC3" pad="P$8"/>
<connect gate="G$1" pin="NC4" pad="P$9"/>
<connect gate="G$1" pin="NC5" pad="P$10"/>
<connect gate="G$1" pin="NC6" pad="P$15"/>
<connect gate="G$1" pin="NC7" pad="P$16"/>
<connect gate="G$1" pin="OUT+" pad="P$14"/>
<connect gate="G$1" pin="OUT-" pad="P$11"/>
<connect gate="G$1" pin="SVR" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8552T/S" prefix="IC" uservalue="yes">
<description>2 ´ 1.4 W BTL audio amplifiers with
digital volume control and
headphone sensing</description>
<gates>
<gate name="G$1" symbol="TDA8552T/S"/>
</gates>
<devices>
<device name="" package="SOT163-1">
<connects>
<connect gate="G$1" pin="GAINS" pad="P$14"/>
<connect gate="G$1" pin="GND1" pad="P$1"/>
<connect gate="G$1" pin="GND2" pad="P$10"/>
<connect gate="G$1" pin="GND3" pad="P$11"/>
<connect gate="G$1" pin="GND4" pad="P$20"/>
<connect gate="G$1" pin="HPS" pad="P$4"/>
<connect gate="G$1" pin="IN1" pad="P$17"/>
<connect gate="G$1" pin="IN2" pad="P$15"/>
<connect gate="G$1" pin="MOD" pad="P$5"/>
<connect gate="G$1" pin="OUT1+" pad="P$12"/>
<connect gate="G$1" pin="OUT1-" pad="P$19"/>
<connect gate="G$1" pin="OUT2+" pad="P$2"/>
<connect gate="G$1" pin="OUT2-" pad="P$9"/>
<connect gate="G$1" pin="SVR" pad="P$16"/>
<connect gate="G$1" pin="UP/DO1" pad="P$6"/>
<connect gate="G$1" pin="UP/DO2" pad="P$7"/>
<connect gate="G$1" pin="VDD1" pad="P$3"/>
<connect gate="G$1" pin="VDD2" pad="P$8"/>
<connect gate="G$1" pin="VDD3" pad="P$13"/>
<connect gate="G$1" pin="VDD4" pad="P$18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT266-1" package="SOT266-1">
<connects>
<connect gate="G$1" pin="GAINS" pad="14"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GND3" pad="11"/>
<connect gate="G$1" pin="GND4" pad="20"/>
<connect gate="G$1" pin="HPS" pad="4"/>
<connect gate="G$1" pin="IN1" pad="17"/>
<connect gate="G$1" pin="IN2" pad="15"/>
<connect gate="G$1" pin="MOD" pad="5"/>
<connect gate="G$1" pin="OUT1+" pad="12"/>
<connect gate="G$1" pin="OUT1-" pad="19"/>
<connect gate="G$1" pin="OUT2+" pad="2"/>
<connect gate="G$1" pin="OUT2-" pad="9"/>
<connect gate="G$1" pin="SVR" pad="16"/>
<connect gate="G$1" pin="UP/DO1" pad="6"/>
<connect gate="G$1" pin="UP/DO2" pad="7"/>
<connect gate="G$1" pin="VDD1" pad="3"/>
<connect gate="G$1" pin="VDD2" pad="8"/>
<connect gate="G$1" pin="VDD3" pad="13"/>
<connect gate="G$1" pin="VDD4" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8551" prefix="IC" uservalue="yes">
<description>1 W BTL audio amplifier with digital
volume control</description>
<gates>
<gate name="G$1" symbol="TDA8551"/>
</gates>
<devices>
<device name="" package="SOT96-1">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="MOD" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="8"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
<connect gate="G$1" pin="SVR" pad="3"/>
<connect gate="G$1" pin="U/D" pad="1"/>
<connect gate="G$1" pin="VP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT97-1" package="SOT97-1">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="MOD" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="8"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
<connect gate="G$1" pin="SVR" pad="3"/>
<connect gate="G$1" pin="U/D" pad="1"/>
<connect gate="G$1" pin="VP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8542TS" prefix="IC" uservalue="yes">
<description>2 ´ 0.7 W BTL audio amplifier</description>
<gates>
<gate name="G$1" symbol="TDA8542TS"/>
</gates>
<devices>
<device name="" package="SOT266-1">
<connects>
<connect gate="G$1" pin="BT/SE" pad="6"/>
<connect gate="G$1" pin="INL+" pad="16"/>
<connect gate="G$1" pin="INL-" pad="17"/>
<connect gate="G$1" pin="INR+" pad="15"/>
<connect gate="G$1" pin="INR-" pad="14"/>
<connect gate="G$1" pin="LGND" pad="1"/>
<connect gate="G$1" pin="MOD" pad="4"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC1" pad="7"/>
<connect gate="G$1" pin="NC2" pad="9"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="19"/>
<connect gate="G$1" pin="OUTL+" pad="3"/>
<connect gate="G$1" pin="OUTL-" pad="18"/>
<connect gate="G$1" pin="OUTR+" pad="8"/>
<connect gate="G$1" pin="OUTR-" pad="13"/>
<connect gate="G$1" pin="RGND" pad="10"/>
<connect gate="G$1" pin="SVR" pad="5"/>
<connect gate="G$1" pin="VCCL" pad="20"/>
<connect gate="G$1" pin="VCCR" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8542" prefix="IC" uservalue="yes">
<description>2 ´ 1 W BTL audio amplifier</description>
<gates>
<gate name="G$1" symbol="TDA8542"/>
</gates>
<devices>
<device name="" package="SOT162-1">
<connects>
<connect gate="G$1" pin="BTL/SE" pad="5"/>
<connect gate="G$1" pin="INL+" pad="13"/>
<connect gate="G$1" pin="INL-" pad="14"/>
<connect gate="G$1" pin="INR+" pad="12"/>
<connect gate="G$1" pin="INR-" pad="11"/>
<connect gate="G$1" pin="LGND" pad="1"/>
<connect gate="G$1" pin="MOD" pad="3"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUTL+" pad="2"/>
<connect gate="G$1" pin="OUTL-" pad="15"/>
<connect gate="G$1" pin="OUTR+" pad="7"/>
<connect gate="G$1" pin="OUTR-" pad="10"/>
<connect gate="G$1" pin="RGND" pad="8"/>
<connect gate="G$1" pin="SVR" pad="4"/>
<connect gate="G$1" pin="VCCL" pad="16"/>
<connect gate="G$1" pin="VCCR" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT38-1" package="SOT38-1">
<connects>
<connect gate="G$1" pin="BTL/SE" pad="5"/>
<connect gate="G$1" pin="INL+" pad="13"/>
<connect gate="G$1" pin="INL-" pad="14"/>
<connect gate="G$1" pin="INR+" pad="12"/>
<connect gate="G$1" pin="INR-" pad="11"/>
<connect gate="G$1" pin="LGND" pad="1"/>
<connect gate="G$1" pin="MOD" pad="3"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUTL+" pad="2"/>
<connect gate="G$1" pin="OUTL-" pad="15"/>
<connect gate="G$1" pin="OUTR+" pad="7"/>
<connect gate="G$1" pin="OUTR-" pad="10"/>
<connect gate="G$1" pin="RGND" pad="8"/>
<connect gate="G$1" pin="SVR" pad="4"/>
<connect gate="G$1" pin="VCCL" pad="16"/>
<connect gate="G$1" pin="VCCR" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA5204F" prefix="IC" uservalue="yes">
<description>3V / 35mW dual power amplifier</description>
<gates>
<gate name="G$1" symbol="BA5204F"/>
</gates>
<devices>
<device name="" package="SOP16">
<connects>
<connect gate="G$1" pin="B/ST1" pad="1"/>
<connect gate="G$1" pin="B/ST2" pad="8"/>
<connect gate="G$1" pin="FILTER" pad="13"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="15"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC1" pad="12"/>
<connect gate="G$1" pin="NFB1" pad="14"/>
<connect gate="G$1" pin="NFB2" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="PGND" pad="5"/>
<connect gate="G$1" pin="SUB1" pad="16"/>
<connect gate="G$1" pin="SUB2" pad="9"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA5208AF" prefix="IC" uservalue="yes">
<description>3V-400mW BTL Power Audio Amplifier</description>
<gates>
<gate name="G$1" symbol="BA5208AF"/>
</gates>
<devices>
<device name="" package="SOP16">
<connects>
<connect gate="G$1" pin="BIAS1" pad="13"/>
<connect gate="G$1" pin="BIAS2" pad="3"/>
<connect gate="G$1" pin="FILTER" pad="14"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN1" pad="12"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="INOUT" pad="4"/>
<connect gate="G$1" pin="MOUT1" pad="16"/>
<connect gate="G$1" pin="MOUT2" pad="2"/>
<connect gate="G$1" pin="MUTE/IN" pad="15"/>
<connect gate="G$1" pin="NFB1" pad="11"/>
<connect gate="G$1" pin="NFB2" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="10"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA5210FS" prefix="IC" uservalue="yes">
<description>Speaker / headphone switch power
amplifier</description>
<gates>
<gate name="G$1" symbol="BA5210FS"/>
</gates>
<devices>
<device name="" package="SSOP-A16">
<connects>
<connect gate="G$1" pin="B/OUT" pad="10"/>
<connect gate="G$1" pin="BIASIN" pad="7"/>
<connect gate="G$1" pin="F" pad="6"/>
<connect gate="G$1" pin="INL" pad="12"/>
<connect gate="G$1" pin="INR" pad="14"/>
<connect gate="G$1" pin="MUTE" pad="9"/>
<connect gate="G$1" pin="NFL" pad="13"/>
<connect gate="G$1" pin="NFR" pad="15"/>
<connect gate="G$1" pin="OUTC" pad="16"/>
<connect gate="G$1" pin="OUTL" pad="3"/>
<connect gate="G$1" pin="OUTR" pad="2"/>
<connect gate="G$1" pin="PREGND" pad="11"/>
<connect gate="G$1" pin="PWRGND" pad="1"/>
<connect gate="G$1" pin="ST/BTL" pad="5"/>
<connect gate="G$1" pin="STBY" pad="8"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8593J" prefix="IC" uservalue="yes">
<description>I2C-bus controlled 4 ´ 45 W power amplifier</description>
<gates>
<gate name="G$1" symbol="TDA8593J"/>
</gates>
<devices>
<device name="" package="SOT767-1">
<connects>
<connect gate="G$1" pin="1/ADSEL" pad="P$1"/>
<connect gate="G$1" pin="10/OUTRF+" pad="P$10"/>
<connect gate="G$1" pin="11/SVR" pad="P$11"/>
<connect gate="G$1" pin="12/INRF" pad="P$12"/>
<connect gate="G$1" pin="13/INRR" pad="P$13"/>
<connect gate="G$1" pin="14/SGND" pad="P$14"/>
<connect gate="G$1" pin="15/INLR" pad="P$15"/>
<connect gate="G$1" pin="16/INLF" pad="P$16"/>
<connect gate="G$1" pin="17/ACGND" pad="P$17"/>
<connect gate="G$1" pin="18/OUTLF+" pad="P$18"/>
<connect gate="G$1" pin="19/PGND3" pad="P$19"/>
<connect gate="G$1" pin="2/SDA" pad="P$2"/>
<connect gate="G$1" pin="20/OUTLF-" pad="P$20"/>
<connect gate="G$1" pin="21/VP1" pad="P$21"/>
<connect gate="G$1" pin="22/OUTLR+" pad="P$22"/>
<connect gate="G$1" pin="23/STMB" pad="P$23"/>
<connect gate="G$1" pin="24/OUTLR-" pad="P$24"/>
<connect gate="G$1" pin="25/PGND4" pad="P$25"/>
<connect gate="G$1" pin="26/DIAG" pad="P$26"/>
<connect gate="G$1" pin="27/TAB" pad="P$27"/>
<connect gate="G$1" pin="3/PGND2" pad="P$3"/>
<connect gate="G$1" pin="4/OUTRR-" pad="P$4"/>
<connect gate="G$1" pin="5/SCL" pad="P$5"/>
<connect gate="G$1" pin="6/OUTRR+" pad="P$6"/>
<connect gate="G$1" pin="7/VP2" pad="P$7"/>
<connect gate="G$1" pin="8/OUTRF-" pad="P$8"/>
<connect gate="G$1" pin="9/PGND1" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8589XJ" prefix="IC" uservalue="yes">
<description>I2C-bus controlled 4 ´ 45 Watt
power amplifier and multiple
voltage regulator</description>
<gates>
<gate name="G$1" symbol="TDA8589XJ"/>
</gates>
<devices>
<device name="" package="SOT725-1">
<connects>
<connect gate="G$1" pin="1/PGND2_TAB" pad="P$1"/>
<connect gate="G$1" pin="10/SVR" pad="P$10"/>
<connect gate="G$1" pin="11/IN1" pad="P$11"/>
<connect gate="G$1" pin="12/IN3" pad="P$12"/>
<connect gate="G$1" pin="13/SGND" pad="P$13"/>
<connect gate="G$1" pin="14/IN4" pad="P$14"/>
<connect gate="G$1" pin="15/IN2" pad="P$15"/>
<connect gate="G$1" pin="16/ACGND" pad="P$16"/>
<connect gate="G$1" pin="17/OUT2+" pad="P$17"/>
<connect gate="G$1" pin="18/PGND3" pad="P$18"/>
<connect gate="G$1" pin="19/OUT2-" pad="P$19"/>
<connect gate="G$1" pin="2/SDA" pad="P$2"/>
<connect gate="G$1" pin="20/VP1" pad="P$20"/>
<connect gate="G$1" pin="21/OUT4+" pad="P$21"/>
<connect gate="G$1" pin="22/STB" pad="P$22"/>
<connect gate="G$1" pin="23/OUT4-" pad="P$23"/>
<connect gate="G$1" pin="24/PGND4" pad="P$24"/>
<connect gate="G$1" pin="25/DIAG" pad="P$25"/>
<connect gate="G$1" pin="26/RST" pad="P$26"/>
<connect gate="G$1" pin="27/SW2" pad="P$27"/>
<connect gate="G$1" pin="28/RESCAP" pad="P$28"/>
<connect gate="G$1" pin="29/SW1" pad="P$29"/>
<connect gate="G$1" pin="3/OUT3-" pad="P$3"/>
<connect gate="G$1" pin="30/REG1" pad="P$30"/>
<connect gate="G$1" pin="31/REG3" pad="P$31"/>
<connect gate="G$1" pin="32/GND" pad="P$32"/>
<connect gate="G$1" pin="33/REG4" pad="P$33"/>
<connect gate="G$1" pin="34/REG5" pad="P$34"/>
<connect gate="G$1" pin="35/VP" pad="P$35"/>
<connect gate="G$1" pin="36/BUCAP" pad="P$36"/>
<connect gate="G$1" pin="37/REG2" pad="P$37"/>
<connect gate="G$1" pin="4/SCL" pad="P$4"/>
<connect gate="G$1" pin="5/OUT3+" pad="P$5"/>
<connect gate="G$1" pin="6/VP2" pad="P$6"/>
<connect gate="G$1" pin="7/OUT1-" pad="P$7"/>
<connect gate="G$1" pin="8/PGND1" pad="P$8"/>
<connect gate="G$1" pin="9/OUT1+" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TFA9843J" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="TFA9843J"/>
</gates>
<devices>
<device name="" package="SOT523-1">
<connects>
<connect gate="G$1" pin="CIV" pad="P$3"/>
<connect gate="G$1" pin="GND" pad="P$5"/>
<connect gate="G$1" pin="IN1+" pad="P$4"/>
<connect gate="G$1" pin="IN2+" pad="P$1"/>
<connect gate="G$1" pin="MODE" pad="P$7"/>
<connect gate="G$1" pin="OUT1+" pad="P$8"/>
<connect gate="G$1" pin="OUT2-" pad="P$2"/>
<connect gate="G$1" pin="SVR" pad="P$6"/>
<connect gate="G$1" pin="VCC" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8943SF" prefix="IC" uservalue="yes">
<description>6 W mono Bridge Tied Load (BTL) audio amplifier</description>
<gates>
<gate name="G$1" symbol="TDA8943SF"/>
</gates>
<devices>
<device name="" package="SOT110-1">
<connects>
<connect gate="G$1" pin="1/OUT-" pad="P$1"/>
<connect gate="G$1" pin="2/VCC" pad="P$2"/>
<connect gate="G$1" pin="3/OUT+" pad="P$3"/>
<connect gate="G$1" pin="4/IN+" pad="P$4"/>
<connect gate="G$1" pin="5/IN-" pad="P$5"/>
<connect gate="G$1" pin="6/SVR" pad="P$6"/>
<connect gate="G$1" pin="7/MODE" pad="P$7"/>
<connect gate="G$1" pin="8/GND" pad="P$8"/>
<connect gate="G$1" pin="9/NC" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA3528/9AFP" prefix="IC" uservalue="yes">
<description>Pre / power amplifier and motor
governor for 3V headphone stereos</description>
<gates>
<gate name="G$1" symbol="BA3528/9AFP"/>
</gates>
<devices>
<device name="" package="HSOP28">
<connects>
<connect gate="G$1" pin="1/P_MUT_SW" pad="P$1"/>
<connect gate="G$1" pin="10/PHASE" pad="P$10"/>
<connect gate="G$1" pin="11/VREF" pad="P$11"/>
<connect gate="G$1" pin="12/P_OUT1" pad="P$12"/>
<connect gate="G$1" pin="13/NC" pad="P$13"/>
<connect gate="G$1" pin="14/NC" pad="P$14"/>
<connect gate="G$1" pin="15/P_IN1" pad="P$15"/>
<connect gate="G$1" pin="16/PREOUT1" pad="P$16"/>
<connect gate="G$1" pin="17/PREQ1" pad="P$17"/>
<connect gate="G$1" pin="18/PRENF1" pad="P$18"/>
<connect gate="G$1" pin="19/PREIN1" pad="P$19"/>
<connect gate="G$1" pin="2/P_OUT2" pad="P$2"/>
<connect gate="G$1" pin="20/NC" pad="P$20"/>
<connect gate="G$1" pin="21/PREGND" pad="P$21"/>
<connect gate="G$1" pin="22/BIAS" pad="P$22"/>
<connect gate="G$1" pin="23/PREIN2" pad="P$23"/>
<connect gate="G$1" pin="24PRENF2" pad="P$24"/>
<connect gate="G$1" pin="25/PREQ2" pad="P$25"/>
<connect gate="G$1" pin="26/PREOUT2" pad="P$26"/>
<connect gate="G$1" pin="27/P_IN2" pad="P$27"/>
<connect gate="G$1" pin="28/FILTER" pad="P$28"/>
<connect gate="G$1" pin="29/PGND2" pad="P$29"/>
<connect gate="G$1" pin="3/COM" pad="P$3"/>
<connect gate="G$1" pin="30/PGND" pad="P$30"/>
<connect gate="G$1" pin="4/MOT+" pad="P$4"/>
<connect gate="G$1" pin="5/MOT-" pad="P$5"/>
<connect gate="G$1" pin="6/VOC1" pad="P$6"/>
<connect gate="G$1" pin="7/VOC2" pad="P$7"/>
<connect gate="G$1" pin="8/PGND1" pad="P$8"/>
<connect gate="G$1" pin="9/MTER" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TA8238K" prefix="IC" uservalue="yes">
<description>http://www.datasheetcatalog.org/datasheet/toshiba/1383.pdf</description>
<gates>
<gate name="G$1" symbol="TA8238K"/>
</gates>
<devices>
<device name="" package="HSIP15-P-2.00A">
<connects>
<connect gate="G$1" pin="B.S.1" pad="14"/>
<connect gate="G$1" pin="B.S.2" pad="11"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="NF1" pad="2"/>
<connect gate="G$1" pin="NF2" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="PRE-GND" pad="4"/>
<connect gate="G$1" pin="PW-GND" pad="13"/>
<connect gate="G$1" pin="RIP." pad="7"/>
<connect gate="G$1" pin="SMOOTHING" pad="8"/>
<connect gate="G$1" pin="ST-BY" pad="9"/>
<connect gate="G$1" pin="TJ-DET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AN7118S" prefix="IC" uservalue="yes">
<description>Low Voltage Dual 35mW Audio Power Amplifier Circuits (BTL 300mW)</description>
<gates>
<gate name="G$1" symbol="AN7118S"/>
</gates>
<devices>
<device name="" package="SOP018-P-0300">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CXA1622M/P" prefix="IC" uservalue="yes">
<description>SONY Stereo Power Amplifier/Monaural BTL Power Amplifier</description>
<gates>
<gate name="G$1" symbol="CXA1622M/P"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="1/IN2" pad="1"/>
<connect gate="G$1" pin="10/OUT1" pad="10"/>
<connect gate="G$1" pin="11/PGN1" pad="11"/>
<connect gate="G$1" pin="12GND1" pad="12"/>
<connect gate="G$1" pin="13/NF1" pad="13"/>
<connect gate="G$1" pin="14/VOL" pad="14"/>
<connect gate="G$1" pin="15/REG" pad="15"/>
<connect gate="G$1" pin="16/IN1" pad="16"/>
<connect gate="G$1" pin="2/SW" pad="2"/>
<connect gate="G$1" pin="3/NC" pad="3"/>
<connect gate="G$1" pin="4/NF2" pad="4"/>
<connect gate="G$1" pin="5/GND" pad="5"/>
<connect gate="G$1" pin="6/PG2" pad="6"/>
<connect gate="G$1" pin="7/OUT2" pad="7"/>
<connect gate="G$1" pin="8/RIP" pad="8"/>
<connect gate="G$1" pin="9/VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIP16" value="IC"/>
</technology>
</technologies>
</device>
<device name="SOP16" package="SOP16">
<connects>
<connect gate="G$1" pin="1/IN2" pad="1"/>
<connect gate="G$1" pin="10/OUT1" pad="10"/>
<connect gate="G$1" pin="11/PGN1" pad="11"/>
<connect gate="G$1" pin="12GND1" pad="12"/>
<connect gate="G$1" pin="13/NF1" pad="13"/>
<connect gate="G$1" pin="14/VOL" pad="14"/>
<connect gate="G$1" pin="15/REG" pad="15"/>
<connect gate="G$1" pin="16/IN1" pad="16"/>
<connect gate="G$1" pin="2/SW" pad="2"/>
<connect gate="G$1" pin="3/NC" pad="3"/>
<connect gate="G$1" pin="4/NF2" pad="4"/>
<connect gate="G$1" pin="5/GND" pad="5"/>
<connect gate="G$1" pin="6/PG2" pad="6"/>
<connect gate="G$1" pin="7/OUT2" pad="7"/>
<connect gate="G$1" pin="8/RIP" pad="8"/>
<connect gate="G$1" pin="9/VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA5417" prefix="IC" uservalue="yes">
<description>High-output dual power amplifier</description>
<gates>
<gate name="G$1" symbol="BA5417"/>
</gates>
<devices>
<device name="" package="HSIP15">
<connects>
<connect gate="G$1" pin="1/NC" pad="1"/>
<connect gate="G$1" pin="10/NF1" pad="10"/>
<connect gate="G$1" pin="11/IN1" pad="11"/>
<connect gate="G$1" pin="12/IN2" pad="12"/>
<connect gate="G$1" pin="13/NF2" pad="13"/>
<connect gate="G$1" pin="14/PREGND1" pad="14"/>
<connect gate="G$1" pin="15/PREGND2" pad="15"/>
<connect gate="G$1" pin="2/BS2" pad="2"/>
<connect gate="G$1" pin="3/OUT2" pad="3"/>
<connect gate="G$1" pin="4/VCC" pad="4"/>
<connect gate="G$1" pin="5/OUT1" pad="5"/>
<connect gate="G$1" pin="6/BS1" pad="6"/>
<connect gate="G$1" pin="7/PGND" pad="7"/>
<connect gate="G$1" pin="8/STBY" pad="8"/>
<connect gate="G$1" pin="9/FILTER" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AN12941A" prefix="IC" uservalue="yes">
<description>Audio power IC for notebook PC</description>
<gates>
<gate name="G$1" symbol="AN12941A"/>
</gates>
<devices>
<device name="" package="HSOP056-P-0300A">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$16" pad="P$16"/>
<connect gate="G$1" pin="P$17" pad="P$17"/>
<connect gate="G$1" pin="P$18" pad="P$18"/>
<connect gate="G$1" pin="P$19" pad="P$19"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$20" pad="P$20"/>
<connect gate="G$1" pin="P$21" pad="P$21"/>
<connect gate="G$1" pin="P$22" pad="P$22"/>
<connect gate="G$1" pin="P$23" pad="P$23"/>
<connect gate="G$1" pin="P$24" pad="P$24"/>
<connect gate="G$1" pin="P$25" pad="P$25"/>
<connect gate="G$1" pin="P$26" pad="P$26"/>
<connect gate="G$1" pin="P$27" pad="P$27"/>
<connect gate="G$1" pin="P$28" pad="P$28"/>
<connect gate="G$1" pin="P$29" pad="P$29"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$30" pad="P$30"/>
<connect gate="G$1" pin="P$31" pad="P$31"/>
<connect gate="G$1" pin="P$32" pad="P$32"/>
<connect gate="G$1" pin="P$33" pad="P$33"/>
<connect gate="G$1" pin="P$34" pad="P$34"/>
<connect gate="G$1" pin="P$35" pad="P$35"/>
<connect gate="G$1" pin="P$36" pad="P$36"/>
<connect gate="G$1" pin="P$37" pad="P$37"/>
<connect gate="G$1" pin="P$38" pad="P$38"/>
<connect gate="G$1" pin="P$39" pad="P$39"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$40" pad="P$40"/>
<connect gate="G$1" pin="P$41" pad="P$41"/>
<connect gate="G$1" pin="P$42" pad="P$42"/>
<connect gate="G$1" pin="P$43" pad="P$43"/>
<connect gate="G$1" pin="P$44" pad="P$44"/>
<connect gate="G$1" pin="P$45" pad="P$45"/>
<connect gate="G$1" pin="P$46" pad="P$46"/>
<connect gate="G$1" pin="P$47" pad="P$47"/>
<connect gate="G$1" pin="P$48" pad="P$48"/>
<connect gate="G$1" pin="P$49" pad="P$49"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$50" pad="P$50"/>
<connect gate="G$1" pin="P$51" pad="P$51"/>
<connect gate="G$1" pin="P$52" pad="P$52"/>
<connect gate="G$1" pin="P$53" pad="P$53"/>
<connect gate="G$1" pin="P$54" pad="P$54"/>
<connect gate="G$1" pin="P$55" pad="P$55"/>
<connect gate="G$1" pin="P$56" pad="P$56"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3876" prefix="IC" uservalue="yes">
<description>Audio Power Amplifier Series
High-Performance 56W Audio Power Amplifier w/Mute</description>
<gates>
<gate name="G$1" symbol="LM3876"/>
</gates>
<devices>
<device name="" package="TA11B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TF11B" package="TF11B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3886" prefix="IC" uservalue="yes">
<description>LM3886 Overture™ Audio Power Amplifier Series
High-Performance 68W Audio Power Amplifier w/Mute</description>
<gates>
<gate name="G$1" symbol="LM3886"/>
</gates>
<devices>
<device name="" package="TA11B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TF11B" package="TF11B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1519*" prefix="IC" uservalue="yes">
<description>22WBTL or 2 ´ 11Wstereo power
amplifier</description>
<gates>
<gate name="G$1" symbol="TDA1519CSP"/>
</gates>
<devices>
<device name="" package="SOT354-1">
<connects>
<connect gate="G$1" pin="1/NINV" pad="1"/>
<connect gate="G$1" pin="2/GND1" pad="2"/>
<connect gate="G$1" pin="3/RR" pad="3"/>
<connect gate="G$1" pin="4/OUT1" pad="4"/>
<connect gate="G$1" pin="5/GND2" pad="5"/>
<connect gate="G$1" pin="6/OUT2" pad="6"/>
<connect gate="G$1" pin="7/VP" pad="7"/>
<connect gate="G$1" pin="8/M_SS" pad="8"/>
<connect gate="G$1" pin="9/INV" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT131-2H" package="SOT131-2H">
<connects>
<connect gate="G$1" pin="1/NINV" pad="1"/>
<connect gate="G$1" pin="2/GND1" pad="2"/>
<connect gate="G$1" pin="3/RR" pad="3"/>
<connect gate="G$1" pin="4/OUT1" pad="4"/>
<connect gate="G$1" pin="5/GND2" pad="5"/>
<connect gate="G$1" pin="6/OUT2" pad="6"/>
<connect gate="G$1" pin="7/VP" pad="7"/>
<connect gate="G$1" pin="8/M_SS" pad="8"/>
<connect gate="G$1" pin="9/INV" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT110-1" package="SOT110-1">
<connects>
<connect gate="G$1" pin="1/NINV" pad="P$1"/>
<connect gate="G$1" pin="2/GND1" pad="P$2"/>
<connect gate="G$1" pin="3/RR" pad="P$3"/>
<connect gate="G$1" pin="4/OUT1" pad="P$4"/>
<connect gate="G$1" pin="5/GND2" pad="P$5"/>
<connect gate="G$1" pin="6/OUT2" pad="P$6"/>
<connect gate="G$1" pin="7/VP" pad="P$7"/>
<connect gate="G$1" pin="8/M_SS" pad="P$8"/>
<connect gate="G$1" pin="9/INV" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT157-2" package="SOT157-2">
<connects>
<connect gate="G$1" pin="1/NINV" pad="1"/>
<connect gate="G$1" pin="2/GND1" pad="2"/>
<connect gate="G$1" pin="3/RR" pad="3"/>
<connect gate="G$1" pin="4/OUT1" pad="4"/>
<connect gate="G$1" pin="5/GND2" pad="5"/>
<connect gate="G$1" pin="6/OUT2" pad="6"/>
<connect gate="G$1" pin="7/VP" pad="7"/>
<connect gate="G$1" pin="8/M_SS" pad="8"/>
<connect gate="G$1" pin="9/INV" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAS5630" prefix="IC">
<description>300W STEREO / 600W MONO PurePath ? HD ANALOG-INPUT POWER STAGE CW07/2009</description>
<gates>
<gate name="G$1" symbol="44-PIN"/>
</gates>
<devices>
<device name="" package="DKD">
<connects>
<connect gate="G$1" pin="AGND" pad="P$10"/>
<connect gate="G$1" pin="BST_A" pad="P$43"/>
<connect gate="G$1" pin="BST_B" pad="P$34"/>
<connect gate="G$1" pin="BST_C" pad="P$33"/>
<connect gate="G$1" pin="BST_D" pad="P$24"/>
<connect gate="G$1" pin="C_STARTUP" pad="P$5"/>
<connect gate="G$1" pin="FREQ_ADJ" pad="P$14"/>
<connect gate="G$1" pin="GND" pad="P$9"/>
<connect gate="G$1" pin="GND_A" pad="P$38"/>
<connect gate="G$1" pin="GND_B" pad="P$37"/>
<connect gate="G$1" pin="GND_C" pad="P$30"/>
<connect gate="G$1" pin="GND_D" pad="P$29"/>
<connect gate="G$1" pin="GVDD_AB" pad="P$44"/>
<connect gate="G$1" pin="GVDD_CD" pad="P$23"/>
<connect gate="G$1" pin="INPUT_A" pad="P$6"/>
<connect gate="G$1" pin="INPUT_B" pad="P$7"/>
<connect gate="G$1" pin="INPUT_C" pad="P$12"/>
<connect gate="G$1" pin="INPUT_D" pad="P$13"/>
<connect gate="G$1" pin="M1" pad="P$20"/>
<connect gate="G$1" pin="M2" pad="P$21"/>
<connect gate="G$1" pin="M3" pad="P$22"/>
<connect gate="G$1" pin="OC_ADJ" pad="P$3"/>
<connect gate="G$1" pin="OSC_IO+" pad="P$15"/>
<connect gate="G$1" pin="OSC_IO-" pad="P$16"/>
<connect gate="G$1" pin="OTW" pad="P$18"/>
<connect gate="G$1" pin="OUT_A1" pad="P$39"/>
<connect gate="G$1" pin="OUT_A2" pad="P$40"/>
<connect gate="G$1" pin="OUT_B" pad="P$36"/>
<connect gate="G$1" pin="OUT_C" pad="P$31"/>
<connect gate="G$1" pin="OUT_D1" pad="P$27"/>
<connect gate="G$1" pin="OUT_D2" pad="P$28"/>
<connect gate="G$1" pin="PSU_REF" pad="P$1"/>
<connect gate="G$1" pin="PVDD_A1" pad="P$41"/>
<connect gate="G$1" pin="PVDD_A2" pad="P$42"/>
<connect gate="G$1" pin="PVDD_B" pad="P$35"/>
<connect gate="G$1" pin="PVDD_C" pad="P$32"/>
<connect gate="G$1" pin="PVDD_D1" pad="P$25"/>
<connect gate="G$1" pin="PVDD_D2" pad="P$26"/>
<connect gate="G$1" pin="READY" pad="P$19"/>
<connect gate="G$1" pin="RESET" pad="P$4"/>
<connect gate="G$1" pin="SD" pad="P$17"/>
<connect gate="G$1" pin="VDD" pad="P$2"/>
<connect gate="G$1" pin="VI_CM" pad="P$8"/>
<connect gate="G$1" pin="VREG" pad="P$11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8568Q" prefix="IC" uservalue="yes">
<description>Philips	4 x 25 W BTL quad car radio power amplifier

http://www.datasheetcatalog.com/datasheets_pdf/T/D/A/8/TDA8568Q.shtml</description>
<gates>
<gate name="G$1" symbol="TDA8568Q"/>
</gates>
<devices>
<device name="" package="SOT411-1">
<connects>
<connect gate="G$1" pin="1/VP1" pad="P$1"/>
<connect gate="G$1" pin="10/IN1" pad="P$10"/>
<connect gate="G$1" pin="11/IN2" pad="P$11"/>
<connect gate="G$1" pin="12/SGND" pad="P$12"/>
<connect gate="G$1" pin="13/IN3" pad="P$13"/>
<connect gate="G$1" pin="14/IN4" pad="P$14"/>
<connect gate="G$1" pin="15/MODE" pad="P$15"/>
<connect gate="G$1" pin="16/VP3" pad="P$16"/>
<connect gate="G$1" pin="17/OUT3+" pad="P$17"/>
<connect gate="G$1" pin="18/PGND3" pad="P$18"/>
<connect gate="G$1" pin="19/OUT3-" pad="P$19"/>
<connect gate="G$1" pin="2/OUT1+" pad="P$2"/>
<connect gate="G$1" pin="20/OUT4-" pad="P$20"/>
<connect gate="G$1" pin="21/PGND4" pad="P$21"/>
<connect gate="G$1" pin="22/OUT4+" pad="P$22"/>
<connect gate="G$1" pin="23/VP4" pad="P$23"/>
<connect gate="G$1" pin="3/PGND1" pad="P$3"/>
<connect gate="G$1" pin="4/OUT1-" pad="P$4"/>
<connect gate="G$1" pin="5/OUT2-" pad="P$5"/>
<connect gate="G$1" pin="6/PGND2" pad="P$6"/>
<connect gate="G$1" pin="7/OUT2+" pad="P$7"/>
<connect gate="G$1" pin="8/VP2" pad="P$8"/>
<connect gate="G$1" pin="9/VDIAG" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1519CTXX" prefix="IC" uservalue="yes">
<description>22WBTL or 2 ´ 11Wstereo power
amplifier</description>
<gates>
<gate name="G$1" symbol="TDA1519CTD"/>
</gates>
<devices>
<device name="" package="SOT418-3">
<connects>
<connect gate="G$1" pin="1/RR" pad="1"/>
<connect gate="G$1" pin="10/VP" pad="10"/>
<connect gate="G$1" pin="11/M_SS" pad="11"/>
<connect gate="G$1" pin="12/INV" pad="12"/>
<connect gate="G$1" pin="13/NC" pad="13"/>
<connect gate="G$1" pin="14/NC" pad="14"/>
<connect gate="G$1" pin="15/NC" pad="15"/>
<connect gate="G$1" pin="16/NC" pad="16"/>
<connect gate="G$1" pin="17/NC" pad="17"/>
<connect gate="G$1" pin="18/NC" pad="18"/>
<connect gate="G$1" pin="19/NINV" pad="19"/>
<connect gate="G$1" pin="2/NC" pad="2"/>
<connect gate="G$1" pin="20/GND1" pad="20"/>
<connect gate="G$1" pin="3/OUT" pad="3"/>
<connect gate="G$1" pin="4/NC" pad="4"/>
<connect gate="G$1" pin="5/GND" pad="5"/>
<connect gate="G$1" pin="6/NC" pad="6"/>
<connect gate="G$1" pin="7/NC" pad="7"/>
<connect gate="G$1" pin="8/OUT2" pad="8"/>
<connect gate="G$1" pin="9/NC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT397-1" package="SOT397-1">
<connects>
<connect gate="G$1" pin="1/RR" pad="1"/>
<connect gate="G$1" pin="10/VP" pad="10"/>
<connect gate="G$1" pin="11/M_SS" pad="11"/>
<connect gate="G$1" pin="12/INV" pad="12"/>
<connect gate="G$1" pin="13/NC" pad="13"/>
<connect gate="G$1" pin="14/NC" pad="14"/>
<connect gate="G$1" pin="15/NC" pad="15"/>
<connect gate="G$1" pin="16/NC" pad="16"/>
<connect gate="G$1" pin="17/NC" pad="17"/>
<connect gate="G$1" pin="18/NC" pad="18"/>
<connect gate="G$1" pin="19/NINV" pad="19"/>
<connect gate="G$1" pin="2/NC" pad="2"/>
<connect gate="G$1" pin="20/GND1" pad="20"/>
<connect gate="G$1" pin="3/OUT" pad="3"/>
<connect gate="G$1" pin="4/NC" pad="4"/>
<connect gate="G$1" pin="5/GND" pad="5"/>
<connect gate="G$1" pin="6/NC" pad="6"/>
<connect gate="G$1" pin="7/NC" pad="7"/>
<connect gate="G$1" pin="8/OUT2" pad="8"/>
<connect gate="G$1" pin="9/NC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8586TH" prefix="IC" uservalue="yes">
<description>Power amplifier with load detection
and auto BTL/SE selection</description>
<gates>
<gate name="G$1" symbol="TDA8586TH"/>
</gates>
<devices>
<device name="" package="SOT418-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8586Q" prefix="IC" uservalue="yes">
<description>Power amplifier with load detection
and auto BTL/SE selection</description>
<gates>
<gate name="G$1" symbol="TDA8586Q"/>
</gates>
<devices>
<device name="" package="SOT243-1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7376PD" prefix="IC" uservalue="yes">
<description>2 X 35W POWER AMPLIFIER FOR CAR RADIO</description>
<gates>
<gate name="G$1" symbol="TDA7376PD"/>
</gates>
<devices>
<device name="" package="SO36-POWER_SLUG_UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M5218AL/P/FP" prefix="IC" uservalue="yes">
<description>Dual power ampliefier</description>
<gates>
<gate name="G$1" symbol="M5218AL/P/FP"/>
</gates>
<devices>
<device name="" package="SOP08">
<connects>
<connect gate="G$1" pin="1/OUT1" pad="1"/>
<connect gate="G$1" pin="2/-IN1" pad="2"/>
<connect gate="G$1" pin="3/+IN1" pad="3"/>
<connect gate="G$1" pin="4/GND" pad="4"/>
<connect gate="G$1" pin="5/+IN2" pad="5"/>
<connect gate="G$1" pin="6/-IN" pad="6"/>
<connect gate="G$1" pin="7/OUT2" pad="7"/>
<connect gate="G$1" pin="8/VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIL08" package="SIL08">
<connects>
<connect gate="G$1" pin="1/OUT1" pad="1"/>
<connect gate="G$1" pin="2/-IN1" pad="2"/>
<connect gate="G$1" pin="3/+IN1" pad="3"/>
<connect gate="G$1" pin="4/GND" pad="4"/>
<connect gate="G$1" pin="5/+IN2" pad="5"/>
<connect gate="G$1" pin="6/-IN" pad="6"/>
<connect gate="G$1" pin="7/OUT2" pad="7"/>
<connect gate="G$1" pin="8/VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TA2022" prefix="IC">
<description>&lt;b&gt;STEREO 90W (4.) CLASS-TM DIGITAL AUDIO AMPLIFIER DRIVER&lt;/b&gt;&lt;p&gt;
USING DIGITAL POWER PROCESSING  (DPP TM) TECHNOLOGY&lt;br&gt;
Source: http://www.tripath.com/audio.htm .. TA2022.pdf</description>
<gates>
<gate name="G$1" symbol="TA2022"/>
</gates>
<devices>
<device name="" package="SSIP-32">
<connects>
<connect gate="G$1" pin="AGND@1" pad="15"/>
<connect gate="G$1" pin="AGND@2" pad="20"/>
<connect gate="G$1" pin="BIASCAP" pad="27"/>
<connect gate="G$1" pin="FBKGND1" pad="30"/>
<connect gate="G$1" pin="FBKGND2" pad="28"/>
<connect gate="G$1" pin="FBKOUT1" pad="31"/>
<connect gate="G$1" pin="FBKOUT2" pad="29"/>
<connect gate="G$1" pin="HMUTE" pad="32"/>
<connect gate="G$1" pin="INV1" pad="23"/>
<connect gate="G$1" pin="INV2" pad="26"/>
<connect gate="G$1" pin="MUTE" pad="24"/>
<connect gate="G$1" pin="OAOUT1" pad="22"/>
<connect gate="G$1" pin="OAOUT2" pad="25"/>
<connect gate="G$1" pin="OUT1" pad="10"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="REF" pad="17"/>
<connect gate="G$1" pin="V5@1" pad="16"/>
<connect gate="G$1" pin="V5@2" pad="21"/>
<connect gate="G$1" pin="VBOOT1" pad="13"/>
<connect gate="G$1" pin="VBOOT2" pad="1"/>
<connect gate="G$1" pin="VN10" pad="2"/>
<connect gate="G$1" pin="VN10FBK" pad="14"/>
<connect gate="G$1" pin="VN10GND" pad="3"/>
<connect gate="G$1" pin="VN10SW" pad="5"/>
<connect gate="G$1" pin="VNN1" pad="9"/>
<connect gate="G$1" pin="VNN2" pad="8"/>
<connect gate="G$1" pin="VNNSENSE" pad="18"/>
<connect gate="G$1" pin="VPP1" pad="12"/>
<connect gate="G$1" pin="VPP2" pad="4"/>
<connect gate="G$1" pin="VPPSENSE" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NTE1898" prefix="IC" uservalue="yes">
<description>Dual Audio Power Amp, 5.8W (22W BTL)</description>
<gates>
<gate name="G$1" symbol="NTE1898"/>
</gates>
<devices>
<device name="" package="SIP12">
<connects>
<connect gate="G$1" pin="1/IN1" pad="1"/>
<connect gate="G$1" pin="10/VCC" pad="9"/>
<connect gate="G$1" pin="11/BST1" pad="10"/>
<connect gate="G$1" pin="12/OUT1" pad="11"/>
<connect gate="G$1" pin="2/NF1" pad="2"/>
<connect gate="G$1" pin="3/PGND" pad="3"/>
<connect gate="G$1" pin="4/NF2" pad="4"/>
<connect gate="G$1" pin="5/IN2" pad="5"/>
<connect gate="G$1" pin="6/RIP" pad="6"/>
<connect gate="G$1" pin="7/OUT2" pad="7"/>
<connect gate="G$1" pin="8/BST2" pad="8"/>
<connect gate="G$1" pin="GND" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TA7251BP" prefix="IC" uservalue="yes">
<description>30W BTL Audio Power Amplifier of Toshiba Bipolar Linear.</description>
<gates>
<gate name="G$1" symbol="TA7251BP"/>
</gates>
<devices>
<device name="" package="HZIP12-P-1,78B">
<connects>
<connect gate="G$1" pin="1/OUT1" pad="P$1"/>
<connect gate="G$1" pin="10/PGND" pad="P$10"/>
<connect gate="G$1" pin="11/IN+" pad="P$11"/>
<connect gate="G$1" pin="12/NF1" pad="P$12"/>
<connect gate="G$1" pin="2/BS1" pad="P$2"/>
<connect gate="G$1" pin="3/VCC" pad="P$3"/>
<connect gate="G$1" pin="4/GND" pad="P$4"/>
<connect gate="G$1" pin="5/BS2" pad="P$5"/>
<connect gate="G$1" pin="6/OUT2" pad="P$6"/>
<connect gate="G$1" pin="7/CRIP" pad="P$7"/>
<connect gate="G$1" pin="8/NF2" pad="P$8"/>
<connect gate="G$1" pin="9/IN-" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7266SA" prefix="IC" uservalue="yes">
<description>7W+7W DUAL BRIDGE AMPLIFIER</description>
<gates>
<gate name="G$1" symbol="TDA7266SA"/>
</gates>
<devices>
<device name="" package="CLIPWATT15">
<connects>
<connect gate="G$1" pin="1/OUT1+" pad="1"/>
<connect gate="G$1" pin="10/NC" pad="10"/>
<connect gate="G$1" pin="11/NC" pad="11"/>
<connect gate="G$1" pin="12/IN2" pad="12"/>
<connect gate="G$1" pin="13/VCC" pad="13"/>
<connect gate="G$1" pin="14/OUT2-" pad="14"/>
<connect gate="G$1" pin="15/OUT2+" pad="15"/>
<connect gate="G$1" pin="2/OUT1-" pad="2"/>
<connect gate="G$1" pin="3/VCC" pad="3"/>
<connect gate="G$1" pin="4/IN1" pad="4"/>
<connect gate="G$1" pin="5/NC" pad="5"/>
<connect gate="G$1" pin="6/MUTE" pad="6"/>
<connect gate="G$1" pin="7/ST-BY" pad="7"/>
<connect gate="G$1" pin="8/PWGND" pad="8"/>
<connect gate="G$1" pin="9/SGND" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TBA810AS" prefix="IC" uservalue="yes">
<description>http://www.datasheetcatalog.com/datasheets_pdf/T/B/A/8/TBA810AS.shtml</description>
<gates>
<gate name="G$1" symbol="TBA810AS"/>
</gates>
<devices>
<device name="CB-155" package="CE82">
<connects>
<connect gate="G$1" pin="10/GND" pad="10 @GND GND"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="VCC/1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="FINDIP12">
<connects>
<connect gate="G$1" pin="10/GND" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="VCC/1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
