<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;I2C Bus Devices&lt;/b&gt;
&lt;p&gt;
See &lt;a href="http://www.philipslogic.com/products/i2c/"&gt;http://www.philipslogic.com/products/i2c/&lt;/a&gt; for more devices.
&lt;p&gt;
Version history:&lt;br&gt;
02 Jun 2004 v1.00 Created by Eelco Huininga (&lt;a href="mailto:eelcapone@beer.com"&gt;eelcapone@NOSPAMbeer.com&lt;/a&gt;)&lt;br&gt;
30 Aug 2004 v1.01 Updated by P. Klaja (added PCF8583)&lt;br&gt;
04 Dec 2004 v1.02 Updated by Eelco Huininga (added 82B715)&lt;br&gt;
19 Dec 2004 v1.03 Bugfix: 82B715 package SO08 had pin 6 and 7 swapped&lt;br&gt;</description>
<packages>
<package name="DIL20">
</package>
<package name="SO20W">
</package>
<package name="DIL16">
</package>
<package name="SO16">
</package>
<package name="DIL08">
</package>
<package name="SO08">
</package>
<package name="SO16W">
</package>
</packages>
<symbols>
<symbol name="PCF8584">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="/CS" direction="in" function="dot"/>
<pin name="/RST" function="dot"/>
<pin name="/IACK" direction="in" function="dot"/>
<pin name="/INT" direction="out" function="dot"/>
<pin name="/WR" direction="in" function="dot"/>
<pin name="/RD" function="dot"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PCF8574">
<pin name="/INT" direction="out" function="dot"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
</symbol>
<symbol name="PCF8570">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="TEST"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF8582">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="PTC"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF8594">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="PTC"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="PCF8598">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="PTC"/>
<pin name="A2" direction="in"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="PCF85102">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF85103">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF85116">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="PCF8591">
<pin name="AOUT" direction="out"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OSC"/>
<pin name="EXT" direction="in"/>
<pin name="AGND"/>
</symbol>
<symbol name="PCA9564">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="A0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="/CE" direction="in" function="dot"/>
<pin name="/RST" direction="in" function="dot"/>
<pin name="/INT" direction="out" function="dot"/>
<pin name="/WR" direction="in" function="dot"/>
<pin name="/RD" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
</symbol>
<symbol name="PCA24S08">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="WP" direction="in"/>
<pin name="/PROT" direction="in" function="dot"/>
</symbol>
<symbol name="PCA8581">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="TEST"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="LM75A">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="OS" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF8583">
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="INT" direction="out" function="dot"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
</symbol>
<symbol name="82B715">
<pin name="SX"/>
<pin name="SY"/>
<pin name="LX"/>
<pin name="LY"/>
</symbol>
<symbol name="DS3231">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VBAT"/>
<pin name="GND"/>
<pin name="INT" function="dot"/>
<pin name="RST" function="dot"/>
<pin name="32KHZ" direction="out"/>
<pin name="VCC" direction="in"/>
<pin name="P$1" direction="nc"/>
<pin name="P$2" direction="nc"/>
<pin name="P$3" direction="nc"/>
<pin name="P$4" direction="nc"/>
<pin name="P$5" direction="nc"/>
<pin name="P$6" direction="nc"/>
<pin name="P$7" direction="nc"/>
<pin name="P$8" direction="nc"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PCF8584">
<description>I2C Bus Controller</description>
<gates>
<gate name="IC$1" symbol="PCF8584"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="IC$1" pin="/CS" pad="17"/>
<connect gate="IC$1" pin="/IACK" pad="4"/>
<connect gate="IC$1" pin="/INT" pad="5"/>
<connect gate="IC$1" pin="/RD" pad="16"/>
<connect gate="IC$1" pin="/RST" pad="19"/>
<connect gate="IC$1" pin="/WR" pad="18"/>
<connect gate="IC$1" pin="A0" pad="6"/>
<connect gate="IC$1" pin="CLK" pad="1"/>
<connect gate="IC$1" pin="D0" pad="7"/>
<connect gate="IC$1" pin="D1" pad="8"/>
<connect gate="IC$1" pin="D2" pad="9"/>
<connect gate="IC$1" pin="D3" pad="11"/>
<connect gate="IC$1" pin="D4" pad="12"/>
<connect gate="IC$1" pin="D5" pad="13"/>
<connect gate="IC$1" pin="D6" pad="14"/>
<connect gate="IC$1" pin="D7" pad="15"/>
<connect gate="IC$1" pin="SCL" pad="3"/>
<connect gate="IC$1" pin="SDA" pad="2"/>
<connect gate="PWR" pin="GND" pad="10"/>
<connect gate="PWR" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO20W">
<connects>
<connect gate="IC$1" pin="/CS" pad="17"/>
<connect gate="IC$1" pin="/IACK" pad="4"/>
<connect gate="IC$1" pin="/INT" pad="5"/>
<connect gate="IC$1" pin="/RD" pad="16"/>
<connect gate="IC$1" pin="/RST" pad="19"/>
<connect gate="IC$1" pin="/WR" pad="18"/>
<connect gate="IC$1" pin="A0" pad="6"/>
<connect gate="IC$1" pin="CLK" pad="1"/>
<connect gate="IC$1" pin="D0" pad="7"/>
<connect gate="IC$1" pin="D1" pad="8"/>
<connect gate="IC$1" pin="D2" pad="9"/>
<connect gate="IC$1" pin="D3" pad="11"/>
<connect gate="IC$1" pin="D4" pad="12"/>
<connect gate="IC$1" pin="D5" pad="13"/>
<connect gate="IC$1" pin="D6" pad="14"/>
<connect gate="IC$1" pin="D7" pad="15"/>
<connect gate="IC$1" pin="SCL" pad="3"/>
<connect gate="IC$1" pin="SDA" pad="2"/>
<connect gate="PWR" pin="GND" pad="10"/>
<connect gate="PWR" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8574">
<description>Remote 8-Bit I/O Expander for I2C Bus</description>
<gates>
<gate name="IC$1" symbol="PCF8574"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="IC$1" pin="/INT" pad="13"/>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="P0" pad="4"/>
<connect gate="IC$1" pin="P1" pad="5"/>
<connect gate="IC$1" pin="P2" pad="6"/>
<connect gate="IC$1" pin="P3" pad="7"/>
<connect gate="IC$1" pin="P4" pad="9"/>
<connect gate="IC$1" pin="P5" pad="10"/>
<connect gate="IC$1" pin="P6" pad="11"/>
<connect gate="IC$1" pin="P7" pad="12"/>
<connect gate="IC$1" pin="SCL" pad="14"/>
<connect gate="IC$1" pin="SDA" pad="15"/>
<connect gate="PWR" pin="GND" pad="8"/>
<connect gate="PWR" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AP" package="DIL16">
<connects>
<connect gate="IC$1" pin="/INT" pad="13"/>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="P0" pad="4"/>
<connect gate="IC$1" pin="P1" pad="5"/>
<connect gate="IC$1" pin="P2" pad="6"/>
<connect gate="IC$1" pin="P3" pad="7"/>
<connect gate="IC$1" pin="P4" pad="9"/>
<connect gate="IC$1" pin="P5" pad="10"/>
<connect gate="IC$1" pin="P6" pad="11"/>
<connect gate="IC$1" pin="P7" pad="12"/>
<connect gate="IC$1" pin="SCL" pad="14"/>
<connect gate="IC$1" pin="SDA" pad="15"/>
<connect gate="PWR" pin="GND" pad="8"/>
<connect gate="PWR" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO16">
<connects>
<connect gate="IC$1" pin="/INT" pad="13"/>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="P0" pad="4"/>
<connect gate="IC$1" pin="P1" pad="5"/>
<connect gate="IC$1" pin="P2" pad="6"/>
<connect gate="IC$1" pin="P3" pad="7"/>
<connect gate="IC$1" pin="P4" pad="9"/>
<connect gate="IC$1" pin="P5" pad="10"/>
<connect gate="IC$1" pin="P6" pad="11"/>
<connect gate="IC$1" pin="P7" pad="12"/>
<connect gate="IC$1" pin="SCL" pad="14"/>
<connect gate="IC$1" pin="SDA" pad="15"/>
<connect gate="PWR" pin="GND" pad="8"/>
<connect gate="PWR" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AT" package="SO16">
<connects>
<connect gate="IC$1" pin="/INT" pad="13"/>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="P0" pad="4"/>
<connect gate="IC$1" pin="P1" pad="5"/>
<connect gate="IC$1" pin="P2" pad="6"/>
<connect gate="IC$1" pin="P3" pad="7"/>
<connect gate="IC$1" pin="P4" pad="9"/>
<connect gate="IC$1" pin="P5" pad="10"/>
<connect gate="IC$1" pin="P6" pad="11"/>
<connect gate="IC$1" pin="P7" pad="12"/>
<connect gate="IC$1" pin="SCL" pad="14"/>
<connect gate="IC$1" pin="SDA" pad="15"/>
<connect gate="PWR" pin="GND" pad="8"/>
<connect gate="PWR" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SO16">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8570">
<description>256 x 8-Bit Static Low-Voltage RAM with I2C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF8570"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8582C-2">
<description>256 x 8-Bit CMOS EEPROM with I2C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF8582"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/03" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/03" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8594C-2">
<description>512 x 8-Bit CMOS EEPROM with I2C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF8594"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/02" package="DIL08">
<connects>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/02" package="SO08">
<connects>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8598C-2">
<description>1024 x 8-Bit CMOS EEPROM with I2C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF8598"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/02" package="DIL08">
<connects>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/02" package="SO08">
<connects>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF85102C-2">
<description>256 x 8-Bit CMOS EEPROM with I2C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF85102"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/03" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/03" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF85103C-2">
<description>256 x 8-Bit CMOS EEPROM with I2C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF85103"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/00" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/00" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF85116C-3">
<gates>
<gate name="IC$1" symbol="PCF85116"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="SO08">
<connects>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8591">
<description>8-Bit A/D and D/A Converter</description>
<gates>
<gate name="PWR" symbol="PWRN"/>
<gate name="G$1" symbol="PCF8591"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AIN0" pad="1"/>
<connect gate="G$1" pin="AIN1" pad="2"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3" pad="4"/>
<connect gate="G$1" pin="AOUT" pad="15"/>
<connect gate="G$1" pin="EXT" pad="12"/>
<connect gate="G$1" pin="OSC" pad="11"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VREF" pad="14"/>
<connect gate="PWR" pin="GND" pad="8"/>
<connect gate="PWR" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO16">
<connects>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AIN0" pad="1"/>
<connect gate="G$1" pin="AIN1" pad="2"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3" pad="4"/>
<connect gate="G$1" pin="AOUT" pad="15"/>
<connect gate="G$1" pin="EXT" pad="12"/>
<connect gate="G$1" pin="OSC" pad="11"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VREF" pad="14"/>
<connect gate="PWR" pin="GND" pad="8"/>
<connect gate="PWR" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9564">
<description>Parallel Bus to I2C Bus Controller</description>
<gates>
<gate name="PWR" symbol="PWRN"/>
<gate name="IC$1" symbol="PCA9564"/>
</gates>
<devices>
<device name="D" package="SO20W">
<connects>
<connect gate="IC$1" pin="/CE" pad="13"/>
<connect gate="IC$1" pin="/INT" pad="16"/>
<connect gate="IC$1" pin="/RD" pad="12"/>
<connect gate="IC$1" pin="/RST" pad="17"/>
<connect gate="IC$1" pin="/WR" pad="11"/>
<connect gate="IC$1" pin="A0" pad="14"/>
<connect gate="IC$1" pin="A1" pad="15"/>
<connect gate="IC$1" pin="D0" pad="1"/>
<connect gate="IC$1" pin="D1" pad="2"/>
<connect gate="IC$1" pin="D2" pad="3"/>
<connect gate="IC$1" pin="D3" pad="4"/>
<connect gate="IC$1" pin="D4" pad="5"/>
<connect gate="IC$1" pin="D5" pad="6"/>
<connect gate="IC$1" pin="D6" pad="7"/>
<connect gate="IC$1" pin="D7" pad="8"/>
<connect gate="IC$1" pin="SCL" pad="18"/>
<connect gate="IC$1" pin="SDA" pad="19"/>
<connect gate="PWR" pin="GND" pad="10"/>
<connect gate="PWR" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA24S08">
<description>1024 x 8-Bit CMOS EEPROM with Access Protection</description>
<gates>
<gate name="IC$1" symbol="PCA24S08"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="IC$1" pin="/PROT" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA8581">
<description>128 x 8-Bit EEPROM with I2C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCA8581"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM75AD">
<description>Digital Temperature Sensor and Thermal Watchdog</description>
<gates>
<gate name="IC$1" symbol="LM75A"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="7"/>
<connect gate="IC$1" pin="A1" pad="6"/>
<connect gate="IC$1" pin="A2" pad="5"/>
<connect gate="IC$1" pin="OS" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="2"/>
<connect gate="IC$1" pin="SDA" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8583">
<description>Clock/calendar with 240 x 8-bit RAM</description>
<gates>
<gate name="G$1" symbol="PCF8583"/>
<gate name="G$2" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="INT" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$2" pin="GND" pad="4"/>
<connect gate="G$2" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO08">
<connects>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="INT" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$2" pin="GND" pad="4"/>
<connect gate="G$2" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82B715">
<description>I2C Bus Extender</description>
<gates>
<gate name="IC$1" symbol="82B715"/>
<gate name="G$2" symbol="PWRN"/>
</gates>
<devices>
<device name="PN" package="DIL08">
<connects>
<connect gate="G$2" pin="GND" pad="4"/>
<connect gate="G$2" pin="VCC" pad="8"/>
<connect gate="IC$1" pin="LX" pad="2"/>
<connect gate="IC$1" pin="LY" pad="7"/>
<connect gate="IC$1" pin="SX" pad="3"/>
<connect gate="IC$1" pin="SY" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TD" package="SO08">
<connects>
<connect gate="G$2" pin="GND" pad="4"/>
<connect gate="G$2" pin="VCC" pad="8"/>
<connect gate="IC$1" pin="LX" pad="2"/>
<connect gate="IC$1" pin="LY" pad="7"/>
<connect gate="IC$1" pin="SX" pad="3"/>
<connect gate="IC$1" pin="SY" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3231">
<gates>
<gate name="G$1" symbol="DS3231"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="32KHZ" pad="1"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="INT" pad="3"/>
<connect gate="G$1" pin="P$1" pad="5"/>
<connect gate="G$1" pin="P$2" pad="6"/>
<connect gate="G$1" pin="P$3" pad="7"/>
<connect gate="G$1" pin="P$4" pad="8"/>
<connect gate="G$1" pin="P$5" pad="9"/>
<connect gate="G$1" pin="P$6" pad="10"/>
<connect gate="G$1" pin="P$7" pad="11"/>
<connect gate="G$1" pin="P$8" pad="12"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="SCL" pad="16"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VBAT" pad="14"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SO16W">
<connects>
<connect gate="G$1" pin="32KHZ" pad="1"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="INT" pad="3"/>
<connect gate="G$1" pin="P$1" pad="5"/>
<connect gate="G$1" pin="P$2" pad="6"/>
<connect gate="G$1" pin="P$3" pad="7"/>
<connect gate="G$1" pin="P$4" pad="8"/>
<connect gate="G$1" pin="P$5" pad="9"/>
<connect gate="G$1" pin="P$6" pad="10"/>
<connect gate="G$1" pin="P$7" pad="11"/>
<connect gate="G$1" pin="P$8" pad="12"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="SCL" pad="16"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VBAT" pad="14"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>