<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<packages>
<package name="QFP12-80">
</package>
<package name="PLCC68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="QFP100R">
</package>
<package name="QFP80R">
</package>
<package name="SOT505-1">
</package>
<package name="DIL8">
</package>
<package name="SOT136-1">
</package>
<package name="DIL08">
</package>
<package name="SO16">
</package>
<package name="DIL16">
</package>
<package name="SO16W">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; 7.6 x 10.6 mm</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="DIP28">
</package>
<package name="DIP8">
</package>
<package name="SIP13">
</package>
<package name="SO08">
</package>
<package name="LQFP32-7X7MM">
<description>&lt;b&gt;LQFP32&lt;/b&gt; plastic low profile quad flat package, 32 leads, body 7 x 7 x 1.4 mm&lt;p&gt;
Source: TDA8029.pdf</description>
</package>
<package name="TEA5767">
</package>
<package name="SOT96-1">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="SOT97-1">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="PLCC44S">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="QFP44_SOT307-2">
<description>&lt;b&gt;Plastic Quad Flat Package SOT307-2&lt;/b&gt;&lt;p&gt;
44 leads (lead length 1.3 mm); body 10 x 10 x 1.75 mm SOT307-2&lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP80">
<description>&lt;b&gt;Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PLCC-S68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt; Socked</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="SO8">
</package>
<package name="DIP24SKI">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO28">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; 7.6 x 18.3 mm</description>
</package>
<package name="DIL28">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="PLCC28S">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="HVQFN28">
<description>&lt;b&gt;plastic thermal enhanced very thin quad flat package&lt;/b&gt; SOT993-1&lt;p&gt;
no leads; 24 terminals; body 4 x 4 x 0.85 mm&lt;br&gt;
Source: SOT993-1.pdf</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line 24 leads (600 mil) &lt;P&gt; SOT101-1</description>
</package>
<package name="SO24">
<description>&lt;b&gt;Small Outline Package SOT137-1&lt;/b&gt; 7.5 x 15.74 mm</description>
</package>
<package name="SSOP24">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;&lt;p&gt;
SOT340-1 / JEDEC MO-150AG</description>
</package>
<package name="HVQFN24">
<description>&lt;b&gt;plastic thermal enhanced very thin quad flat package&lt;/b&gt; SOT616-1&lt;p&gt;
no leads; 24 terminals; body 4 x 4 x 0.85 mm&lt;br&gt;
Source: PCA9555_5.pdf</description>
</package>
<package name="TSSOP24">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 24&lt;/b&gt;&lt;p&gt;
Source: MAX3223-MAX3243.pdf</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;plastic shrink small outline package&lt;/b&gt; 20 leads; body width 4.4 mm SOT266-1&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/PCF8574_4.pdf</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO20W">
</package>
<package name="SO8-7_5">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="HVQFN40">
<description>&lt;b&gt;HVQFN40&lt;/b&gt; plastic thermal enhanced very thin quad flat package SOT618-1&lt;p&gt;
no leads; 40 terminals; body 6 x 6 x 0.85 mm&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/packages/SOT618-1.pdf</description>
</package>
<package name="SSOP16">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT545-2">
</package>
<package name="PLCC-S28">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt; Socked</description>
</package>
<package name="TQFP64-10X10">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="TQFP144">
<description>&lt;b&gt;THIN QUAD FLAT PACK&lt;/b&gt;</description>
</package>
<package name="ICP_CON">
</package>
<package name="ISP_CON">
</package>
<package name="SQFP-S-10X10-64">
<description>&lt;b&gt;QFP64&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;Small Outline Package 28&lt;/b&gt; wide</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="SOT270-1">
</package>
<package name="HTQFP48">
</package>
<package name="TDA8708A">
</package>
<package name="HVQFN20_6X5X0,85">
<description>HVQFN20: plastic thermal enhanced very thin quad flat package; no leads;
20 terminals; body 6 x 5 x 0.85 mm
SOT910-1</description>
</package>
<package name="SOT662">
<description>&lt;li&gt;&lt;b&gt;SOT662&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN20: plastic thermal enhanced very thin quad flat package; no leads; 20 terminals; body 5 x 5 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
</packages>
<symbols>
<symbol name="P90CL301">
<pin name="HALT"/>
<pin name="RESET"/>
<pin name="RESETIN" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="SP0/INT0/"/>
<pin name="SP1/INT1/"/>
<pin name="SP2/INT2/"/>
<pin name="SP3/INT3/"/>
<pin name="SP4/INT4"/>
<pin name="SP5/INT5"/>
<pin name="SP6/INT6"/>
<pin name="SP7/NMIN"/>
<pin name="P8/PWM0"/>
<pin name="P9/PWM1"/>
<pin name="P10/SCL"/>
<pin name="P11/SDA"/>
<pin name="P12/ADC0"/>
<pin name="P13/ADC1"/>
<pin name="P14/ADC2"/>
<pin name="P15/ADC3"/>
<pin name="UDS/A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="PCS0/A19" direction="out"/>
<pin name="PCS1/A20" direction="out"/>
<pin name="PCS2/A21" direction="out"/>
<pin name="PCS3/A22" direction="out"/>
<pin name="CS6/A23" direction="out"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8/P0"/>
<pin name="D9/P1"/>
<pin name="D10/P2"/>
<pin name="D11/P3"/>
<pin name="D12/P4"/>
<pin name="D13/P5"/>
<pin name="D14/P6"/>
<pin name="D15/P7"/>
<pin name="AS" direction="out"/>
<pin name="TROM_R/W"/>
<pin name="CS5/WR" direction="out"/>
<pin name="DTACK" direction="out"/>
<pin name="BSIZE" direction="out"/>
<pin name="VREF" direction="pas"/>
<pin name="LDS/DS" direction="out"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="CS0/FC0"/>
<pin name="CS1/FC1"/>
<pin name="CS2/FC2"/>
<pin name="CS3/ALE" direction="out"/>
<pin name="CS4/RD" direction="out"/>
<pin name="CSBT/ONCE"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="80C552">
<pin name="AD0-P0.0"/>
<pin name="AD1-P0.1"/>
<pin name="AD2-P0.2"/>
<pin name="AD3-P0.3"/>
<pin name="AD4-P0.4"/>
<pin name="AD5-P0.5"/>
<pin name="AD6-P0.6"/>
<pin name="AD7-P0.7"/>
<pin name="CT0I-P1.0"/>
<pin name="CT1I-P1.1"/>
<pin name="CT2I-P1.2"/>
<pin name="CT3I-P1.3"/>
<pin name="T2-P1.4"/>
<pin name="RT2-P1.5"/>
<pin name="CSL-P1.6"/>
<pin name="SDA-P1.7"/>
<pin name="A08-P2.0"/>
<pin name="A09-P2.1"/>
<pin name="A10-P2.2"/>
<pin name="A11-P2.3"/>
<pin name="A12-P2.4"/>
<pin name="A13-P2.5"/>
<pin name="A14-P2.6"/>
<pin name="A15-P2.7"/>
<pin name="P3.0-RXD"/>
<pin name="P3.1-TXD"/>
<pin name="P3.2-INT0/"/>
<pin name="P3.3-INT1/"/>
<pin name="P3.4-T0"/>
<pin name="P3.5-T1"/>
<pin name="P3.6-WR/"/>
<pin name="P3.7-RD/"/>
<pin name="P4.0-CMSR0"/>
<pin name="P4.1-CMSR1"/>
<pin name="P4.2-CMSR2"/>
<pin name="P4.3-CMSR3"/>
<pin name="P4.4-CMSR4"/>
<pin name="P4.5-CMSR5"/>
<pin name="P4.6-CMT0"/>
<pin name="P4.7-CMT1"/>
<pin name="P5.0-ADC0"/>
<pin name="P5.1-ADC1"/>
<pin name="P5.2-ADC2"/>
<pin name="P5.3-ADC3"/>
<pin name="P5.4-ADC4"/>
<pin name="P5.5-ADC5"/>
<pin name="P5.6-ADC6"/>
<pin name="P5.7-ADC7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="EA/VPP" direction="in"/>
<pin name="ALE-PROG/" direction="out"/>
<pin name="PSEN/" direction="out"/>
<pin name="RST"/>
<pin name="EW/" direction="in"/>
<pin name="STADC" direction="in"/>
<pin name="AVREF-" direction="in"/>
<pin name="AVREF+" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="AVSS" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="PWM0/" direction="out"/>
<pin name="PWM1/" direction="out"/>
<pin name="NC3" direction="nc"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="VSS">
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="NU">
<pin name="IC-NU" direction="nc"/>
</symbol>
<symbol name="OP+-DIF">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="P$1" direction="out"/>
<pin name="P$2" direction="out"/>
</symbol>
<symbol name="82C250">
<pin name="VCC" direction="sup"/>
<pin name="GND" direction="sup"/>
<pin name="TXD" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="RXD" direction="out"/>
<pin name="VREFOUT" direction="out"/>
<pin name="CANH"/>
<pin name="CANL"/>
</symbol>
<symbol name="NE567">
<pin name="P$1" direction="in"/>
<pin name="P$2" direction="out"/>
</symbol>
<symbol name="SJA1000">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="ALE/AS" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="RD/E" direction="in" function="dot"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CLK_OUT" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="INT" direction="in" function="dot"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VDD3" direction="pwr"/>
<pin name="VSS3" direction="pwr"/>
<pin name="TX0" direction="out"/>
<pin name="TX1" direction="out"/>
<pin name="RX0" direction="in"/>
<pin name="RX1" direction="in"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
</symbol>
<symbol name="82C150">
<pin name="RX0" direction="in"/>
<pin name="RX1" direction="in"/>
<pin name="REF" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="TX0" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="XMOD" direction="in"/>
<pin name="P8_AIN_SW"/>
<pin name="P7_AIN_SW"/>
<pin name="P6_AIN_SW"/>
<pin name="P5_AIN_SW"/>
<pin name="P4_DPM2OUT"/>
<pin name="P3_IDENT"/>
<pin name="P2_IDENT"/>
<pin name="P9_AIN_SW"/>
<pin name="P10_AIN_M1"/>
<pin name="P11_AIN"/>
<pin name="P12_AIN"/>
<pin name="P14_MPX_AD"/>
<pin name="P15_ADCOMP"/>
<pin name="P1_IDENT"/>
<pin name="P0/CLK"/>
<pin name="P16_ADFEED" direction="out"/>
<pin name="P13_AIN"/>
</symbol>
<symbol name="DAC08">
<pin name="B2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="B8" direction="in"/>
<pin name="VREF+" direction="pas"/>
<pin name="VREF-" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="IOUT" direction="oc"/>
<pin name="*IOUT" direction="oc" function="dot"/>
<pin name="VLC" direction="oc"/>
</symbol>
<symbol name="VCCVSS">
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="TJA1020">
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="NSLP" direction="in"/>
<pin name="NWAKE" direction="in"/>
<pin name="LIN"/>
<pin name="INH" direction="out"/>
<pin name="BAT" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TDA5051">
<pin name="DATAIN" direction="in"/>
<pin name="DATAOUT" direction="out"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="CLKOUT" direction="out"/>
<pin name="TEST1"/>
<pin name="SCANTEST"/>
<pin name="TXOUT" direction="out"/>
<pin name="RXIN" direction="in"/>
<pin name="VDDAP" direction="sup"/>
<pin name="VDDA" direction="sup"/>
<pin name="VDDD" direction="sup"/>
<pin name="AGND" direction="sup"/>
<pin name="DGND" direction="sup"/>
<pin name="PD" direction="in"/>
<pin name="APGND"/>
</symbol>
<symbol name="HTRC110">
<pin name="VSS" direction="pwr"/>
<pin name="TX2"/>
<pin name="VDD" direction="pwr"/>
<pin name="TX1"/>
<pin name="MOD"/>
<pin name="XT1"/>
<pin name="XT2"/>
<pin name="SCL"/>
<pin name="DIN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="CEXT"/>
<pin name="QGND" direction="pwr"/>
<pin name="RX" direction="in"/>
</symbol>
<symbol name="TDA1308">
<pin name="1_OUTA"/>
<pin name="2_INA-"/>
<pin name="3_INA+"/>
<pin name="4_GND"/>
<pin name="5_INB+"/>
<pin name="6_INB-"/>
<pin name="7_OUTB"/>
<pin name="8_+VDD"/>
</symbol>
<symbol name="TDA1541">
<pin name="P$1_WS"/>
<pin name="P$2_BCK"/>
<pin name="P$3_DATA"/>
<pin name="P$4_SCK"/>
<pin name="P$5_GNDA"/>
<pin name="P$6_AOR"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14_GNDD"/>
<pin name="P$15_VDD2"/>
<pin name="P$16_NC"/>
<pin name="P$17_NC"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25_AOL"/>
<pin name="P$26_VDD1"/>
<pin name="P$27_TWC"/>
<pin name="P$28_VDD"/>
</symbol>
<symbol name="TDA1543">
<pin name="1_BCK"/>
<pin name="2_WS"/>
<pin name="3_DATA"/>
<pin name="4_GND"/>
<pin name="5_VDD"/>
<pin name="6_AOL"/>
<pin name="7_VRF"/>
<pin name="8_AOR"/>
</symbol>
<symbol name="TDA1545">
<pin name="1_BCK"/>
<pin name="2_WS"/>
<pin name="3_DATA"/>
<pin name="4_GND"/>
<pin name="5_VDD"/>
<pin name="6_IOL"/>
<pin name="7_IREF"/>
<pin name="8_IOR"/>
</symbol>
<symbol name="TDA1557">
<pin name="1_IN1"/>
<pin name="2_GNDIN"/>
<pin name="3_VP1"/>
<pin name="4_OUT1A"/>
<pin name="5_GNDPWR"/>
<pin name="6_OUT1B"/>
<pin name="7_OUT2A"/>
<pin name="8_GNDPWR"/>
<pin name="9_OUT2B"/>
<pin name="10_VP2"/>
<pin name="11_MUTE"/>
<pin name="12_NC"/>
<pin name="13_IN2"/>
</symbol>
<symbol name="TDA7021">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
</symbol>
<symbol name="TDA7050">
<pin name="1_INA+"/>
<pin name="2_INA-"/>
<pin name="3_INB-"/>
<pin name="4_INB+"/>
<pin name="5_GND"/>
<pin name="6_OUTB"/>
<pin name="7_OUTA"/>
<pin name="8_VDD"/>
</symbol>
<symbol name="SAB6456">
<pin name="C1" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="MC" direction="in"/>
<pin name="QH" direction="out"/>
<pin name="VEE" direction="pwr"/>
<pin name="QL" direction="out"/>
<pin name="C2" direction="in"/>
</symbol>
<symbol name="TDA8029">
<pin name="RESET" direction="in"/>
<pin name="!SDWN" direction="in"/>
<pin name="P33/!INT1"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P27"/>
<pin name="P26"/>
<pin name="P30/RX"/>
<pin name="P31/TX"/>
<pin name="!EA" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="!PSEN" direction="out"/>
<pin name="P32/!INT0" direction="out"/>
<pin name="TEST" direction="pas"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="PRES" direction="in"/>
<pin name="I/O"/>
<pin name="CLK" direction="out"/>
<pin name="RST" direction="out"/>
<pin name="GNDC" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="DCIN" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="VUP" direction="pas"/>
<pin name="SBP" direction="pas"/>
<pin name="SBM" direction="pas"/>
<pin name="SAP" direction="pas"/>
<pin name="SAM" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="CDEL" direction="pas"/>
</symbol>
<symbol name="TEA5767">
<pin name="GND"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="VCC"/>
<pin name="DAT"/>
<pin name="CLK"/>
<pin name="NC"/>
<pin name="LOUT"/>
<pin name="ROUT"/>
<pin name="ANT"/>
</symbol>
<symbol name="80C52DIL40">
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="RESET"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="P32"/>
<pin name="P33"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="P36"/>
<pin name="P37"/>
<pin name="X2" direction="out"/>
<pin name="X1" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="P07"/>
<pin name="P06"/>
<pin name="P05"/>
<pin name="P04"/>
<pin name="P03"/>
<pin name="P02"/>
<pin name="P01"/>
<pin name="P00"/>
<pin name="VDD" direction="pwr"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
</symbol>
<symbol name="80C52">
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="RESET"/>
<pin name="P30"/>
<pin name="VSS@3"/>
<pin name="P31"/>
<pin name="P32"/>
<pin name="P33"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="P36"/>
<pin name="P37"/>
<pin name="X2" direction="out"/>
<pin name="X1" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="NC"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="VSS@2"/>
<pin name="!EA" direction="in"/>
<pin name="P07"/>
<pin name="P06"/>
<pin name="P05"/>
<pin name="P04"/>
<pin name="P03"/>
<pin name="P02"/>
<pin name="P01"/>
<pin name="P00"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
</symbol>
<symbol name="8XC598">
<pin name="EA" direction="in" function="dot"/>
<pin name="P0.0/D0"/>
<pin name="P0.1/D1"/>
<pin name="P0.2/D2"/>
<pin name="P0.3/D3"/>
<pin name="P0.4/D4"/>
<pin name="P0.5/D5"/>
<pin name="P0.6/D6"/>
<pin name="P0.7/D7"/>
<pin name="P5.0/AN0"/>
<pin name="P5.1/AN1"/>
<pin name="P5.2/AN2"/>
<pin name="P5.3/AN3"/>
<pin name="P5.4/AN4"/>
<pin name="P5.5/AN5"/>
<pin name="P5.6/AN6"/>
<pin name="P5.7/AN7"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out" function="dot"/>
<pin name="VAREF"/>
<pin name="VAGND"/>
<pin name="P4.3"/>
<pin name="P2.0/A8"/>
<pin name="P4.2"/>
<pin name="P4.1"/>
<pin name="P4.0"/>
<pin name="P2.1/A9"/>
<pin name="P2.2/A10"/>
<pin name="P2.3/A11"/>
<pin name="P2.4/A12"/>
<pin name="P2.5/A13"/>
<pin name="P2.6/A14"/>
<pin name="P2.7/A15"/>
<pin name="INT2"/>
<pin name="INT3"/>
<pin name="INT4"/>
<pin name="INT5"/>
<pin name="T2"/>
<pin name="RT2"/>
<pin name="CTX0"/>
<pin name="CTX1"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2" function="dot"/>
<pin name="P3.3" function="dot"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR" function="dot"/>
<pin name="P3.7/RD" function="dot"/>
<pin name="REF"/>
<pin name="CRX0"/>
<pin name="CRX1"/>
<pin name="STADC"/>
<pin name="PWM0"/>
<pin name="PWM1"/>
<pin name="/EW" function="dot"/>
</symbol>
<symbol name="PWR5">
<pin name="VCC@0" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="PWRC">
<pin name="CVCC" direction="pwr"/>
<pin name="CGND" direction="pwr"/>
</symbol>
<symbol name="NC5">
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
</symbol>
<symbol name="PWR2">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PWRA">
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="8XC576">
<pin name="EA" direction="in" function="dot"/>
<pin name="P0.0/D0"/>
<pin name="P0.1/D1"/>
<pin name="P0.2/D2"/>
<pin name="P0.3/D3"/>
<pin name="P0.4/D4"/>
<pin name="P0.5/D5"/>
<pin name="P0.6/D6"/>
<pin name="P0.7/D7"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out" function="dot"/>
<pin name="P2.0/A8"/>
<pin name="P2.1/A9"/>
<pin name="P2.2/A10"/>
<pin name="P2.3/A11"/>
<pin name="P2.4/A12"/>
<pin name="P2.5/A13"/>
<pin name="P2.6/A14"/>
<pin name="P2.7/A15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2" function="dot"/>
<pin name="P3.3" function="dot"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR" function="dot"/>
<pin name="P3.7/RD" function="dot"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
</symbol>
<symbol name="82B715">
<pin name="LX"/>
<pin name="LY"/>
<pin name="SX"/>
<pin name="SY"/>
</symbol>
<symbol name="NC2">
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="8XC748">
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="X1" direction="in" function="clk"/>
<pin name="X2" direction="in" function="clk"/>
<pin name="VPP" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="ASEL" direction="out"/>
<pin name="OE-PGM" direction="in"/>
</symbol>
<symbol name="8XC751">
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VPP" direction="pwr"/>
</symbol>
<symbol name="P82C150">
<pin name="TX1" direction="out"/>
<pin name="TX0" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="XMOD" direction="in"/>
<pin name="RX0" direction="in"/>
<pin name="RX1" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="AVSS" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CLK/P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
</symbol>
<symbol name="P98LPC935">
<pin name="AD03/DAC0/P2.0"/>
<pin name="AD02/P2.1"/>
<pin name="AD01/P2.0"/>
<pin name="AD00/P1.7"/>
<pin name="OCB/P1.6"/>
<pin name="VSS"/>
<pin name="XTAL1/P3.1"/>
<pin name="CLKOUT/XTAL2/P3.0"/>
<pin name="!INT1/P1.4"/>
<pin name="SDA/!INT0/P1.2"/>
<pin name="SCL/T0/P1.2"/>
<pin name="MOSI/P2.2"/>
<pin name="MISO/P2.3"/>
<pin name="P2.4/!SS"/>
<pin name="P2.5/SPICLK"/>
<pin name="P1.1/RXD"/>
<pin name="P1.0/TXD"/>
<pin name="P0.7/T1"/>
<pin name="P0.6/CMP1"/>
<pin name="VDD"/>
<pin name="P0.5/CMPREF"/>
<pin name="P0.4/CIN1A/DAC1/AD13"/>
<pin name="P0.3/CIN1B/AD12"/>
<pin name="P0.2/CIN2A/AD11"/>
<pin name="P0.1/CIN2B/AD10"/>
<pin name="P2.6/OCA"/>
<pin name="P2.7/ICA"/>
<pin name="!RST/P1.5"/>
</symbol>
<symbol name="P82C250">
<pin name="TXD" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="VREF" direction="out"/>
<pin name="RXD" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PCA9555">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="I/O0.0"/>
<pin name="I/O0.1"/>
<pin name="I/O0.2"/>
<pin name="I/O0.3"/>
<pin name="I/O0.4"/>
<pin name="I/O0.5"/>
<pin name="I/O0.6"/>
<pin name="I/O0.7"/>
<pin name="I/O1.0"/>
<pin name="I/O1.1"/>
<pin name="I/O1.2"/>
<pin name="I/O1.3"/>
<pin name="I/O1.4"/>
<pin name="I/O1.5"/>
<pin name="I/O1.6"/>
<pin name="I/O1.7"/>
</symbol>
<symbol name="PCF8573">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="COMP" direction="out"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="EXTPF" direction="in"/>
<pin name="PFIN" direction="in"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="MIN" direction="out"/>
<pin name="SEC" direction="out"/>
<pin name="FSET" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PCF8574">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
</symbol>
<symbol name="PCF8584">
<pin name="A0" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="!IACK" direction="in"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
</symbol>
<symbol name="PCF8591">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EXT" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AOUT" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PFC8583">
<pin name="A0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PN531">
<pin name="DVDD" direction="in"/>
<pin name="DVSS" direction="pwr"/>
<pin name="P32_INT0"/>
<pin name="P33_INT1"/>
<pin name="!RSTOUT"/>
<pin name="IRQ" direction="out"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="NSS"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="OSC2IN" direction="in"/>
<pin name="VBUS" direction="in"/>
<pin name="DELATT" direction="out"/>
<pin name="TESTEN" direction="in"/>
<pin name="OSC2OUT" direction="out"/>
<pin name="PVDD" direction="pwr"/>
<pin name="SVDD" direction="pwr"/>
<pin name="!RSTPD" direction="in"/>
<pin name="OSCOUT" direction="out"/>
<pin name="OSCIN" direction="in"/>
<pin name="TVDD" direction="pwr"/>
<pin name="TVSS1" direction="pwr"/>
<pin name="TX1" direction="out"/>
<pin name="TX2" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RX" direction="in"/>
<pin name="VMID" direction="pwr"/>
<pin name="AUX1" direction="out"/>
<pin name="AUX2" direction="out"/>
<pin name="SIGOUT" direction="out"/>
<pin name="SIGIN" direction="in"/>
<pin name="LOADMOD" direction="out"/>
<pin name="TVSS2" direction="pwr"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="SAA1064">
<pin name="SCL" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="CEXT" direction="in"/>
<pin name="ADR" direction="in"/>
<pin name="MX1" direction="out"/>
<pin name="MX2" direction="out"/>
<pin name="P1" direction="out"/>
<pin name="P2" direction="out"/>
<pin name="P3" direction="out"/>
<pin name="P4" direction="out"/>
<pin name="P5" direction="out"/>
<pin name="P6" direction="out"/>
<pin name="P7" direction="out"/>
<pin name="P8" direction="out"/>
<pin name="P9" direction="out"/>
<pin name="P10" direction="out"/>
<pin name="P11" direction="out"/>
<pin name="P12" direction="out"/>
<pin name="P13" direction="out"/>
<pin name="P14" direction="out"/>
<pin name="P15" direction="out"/>
<pin name="P16" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="TEA5764HN">
<pin name="LOOPSW" direction="in"/>
<pin name="CPOUT" direction="in"/>
<pin name="LO1" direction="in"/>
<pin name="LO2" direction="in"/>
<pin name="CD1" direction="in"/>
<pin name="PILLP" direction="in"/>
<pin name="SWPORT" direction="out"/>
<pin name="BUSENBABLE" direction="in"/>
<pin name="VREFDIG" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="GNDD" direction="pwr"/>
<pin name="GNDD@1" direction="pwr"/>
<pin name="VCCD" direction="pwr"/>
<pin name="CD2/INTCON3" direction="in"/>
<pin name="INTCON2" direction="in"/>
<pin name="GNDD@2" direction="pwr"/>
<pin name="INTX" direction="out"/>
<pin name="INTCON1" direction="in"/>
<pin name="TMUTE" direction="in"/>
<pin name="VAFR" direction="out"/>
<pin name="VAFL" direction="out"/>
<pin name="MPXOUT" direction="out"/>
<pin name="GNDD@3" direction="pwr"/>
<pin name="GNDA" direction="in"/>
<pin name="FREQIN" direction="in"/>
<pin name="XTAL" direction="in"/>
<pin name="VCCA" direction="in"/>
<pin name="CD3" direction="in"/>
<pin name="RFIN1" direction="in"/>
<pin name="RFIN2" direction="in"/>
<pin name="GNDRF" direction="in"/>
<pin name="CAGC" direction="in"/>
<pin name="MPXIN" direction="in"/>
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="UAA3220TS">
<pin name="MGND" direction="pas"/>
<pin name="MIXIN" direction="pas"/>
<pin name="FA" direction="pas"/>
<pin name="VCCI" direction="pwr"/>
<pin name="LIN" direction="pas"/>
<pin name="LFB" direction="pas"/>
<pin name="RSSI" direction="pas"/>
<pin name="CPC" direction="pas"/>
<pin name="CPB" direction="pas"/>
<pin name="CPA" direction="pas"/>
<pin name="DATA" direction="pas"/>
<pin name="CGND" direction="pwr"/>
<pin name="OGND" direction="pwr"/>
<pin name="OSE" direction="pas"/>
<pin name="OSB" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="OSC" direction="oc"/>
<pin name="TEM" direction="pas"/>
<pin name="TN" direction="oc"/>
<pin name="TP" direction="oc"/>
<pin name="PWD" direction="pas"/>
<pin name="DEMO1" direction="pas"/>
<pin name="DEMO2" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="UDA1320">
<pin name="BCK" direction="in"/>
<pin name="WS" direction="in"/>
<pin name="DATAI" direction="in"/>
<pin name="SYSCLK" direction="in"/>
<pin name="VOUTL" direction="out"/>
<pin name="VOUTR" direction="out"/>
<pin name="VREFDAC" direction="in"/>
<pin name="APPSEL" direction="in"/>
<pin name="APPL0" direction="in"/>
<pin name="APPL1" direction="in"/>
<pin name="APPL2" direction="in"/>
<pin name="APPL3" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSSD" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
</symbol>
<symbol name="UDA1360T">
<pin name="BCK" direction="in"/>
<pin name="WS" direction="in"/>
<pin name="DATAO" direction="in"/>
<pin name="SYSCLK" direction="in"/>
<pin name="VINL" direction="in"/>
<pin name="VINR" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="SFOR" direction="in"/>
<pin name="FSEL" direction="in"/>
<pin name="PWON" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSSD" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VREFP" direction="in"/>
<pin name="VREFN" direction="in"/>
</symbol>
<symbol name="LPC904">
<pin name="VDD"/>
<pin name="AD11/PO.2/CIN2A/KBI2"/>
<pin name="P1.1/RXD"/>
<pin name="RST/P1.5"/>
<pin name="P1.0/TXD"/>
<pin name="P0.5/CMPREF/CLKIN"/>
<pin name="P0.4/CIN1A/AD13/DAC1"/>
<pin name="VSS"/>
</symbol>
<symbol name="LPC938">
<pin name="P2.0/ICB/AD07"/>
<pin name="P2.1/OCD/AD06"/>
<pin name="P0.0/CMP2/KBI0/AD05"/>
<pin name="P1.7/OCC/AD04"/>
<pin name="P1.6/OCB"/>
<pin name="P1.5/RST"/>
<pin name="VSS"/>
<pin name="XTAL1/P3.1"/>
<pin name="CLKOUT/XTAL2/P3.0"/>
<pin name="P1.4/INT1"/>
<pin name="P1.3/INT0/SDA"/>
<pin name="P1.2/T0/SCL"/>
<pin name="P2.2/MOSI"/>
<pin name="P2.3/MISO"/>
<pin name="P2.4/SS"/>
<pin name="P2.5/SPICLK"/>
<pin name="P1.1/RXD"/>
<pin name="P1.0/TXD"/>
<pin name="P0.7/T1/KBI7"/>
<pin name="P0.6/CMP1/KBI6"/>
<pin name="VDD"/>
<pin name="P0.5/CMPREF/KBI5"/>
<pin name="P0.4/CIN1A/KBI4/AD03"/>
<pin name="P0.3/CIN1B/KBI3/AD02"/>
<pin name="P0.2/CIN2A/KBI2/AD01"/>
<pin name="P0.1/CIN2B/KBI1/AD00"/>
<pin name="P2.6/OCA"/>
<pin name="P2.7/ICA"/>
</symbol>
<symbol name="LPC2114">
<pin name="P0.21/PWM5/RD3/CAP1.3"/>
<pin name="P0.22/TD3/CAP0.0/MAT0.0"/>
<pin name="P0.23/RD2"/>
<pin name="P1.19/TRACEPKT3"/>
<pin name="P0.24/TD2"/>
<pin name="VSS-1"/>
<pin name="V3A"/>
<pin name="P1.18/TRACEPKT2"/>
<pin name="P0.25/RD1"/>
<pin name="TD1"/>
<pin name="P0.27/AIN0/CAP0.1/MAT0.1"/>
<pin name="P1.17/TRACEPKT1"/>
<pin name="P0.28/AIN1/CAP0.2/MAT0.2"/>
<pin name="P0.29/AIN2/CAP0.3/MAT0.3"/>
<pin name="P0.30/AIN3/EINT3/CAP0.0"/>
<pin name="P1.16/TRACEPKT0"/>
<pin name="V18-1"/>
<pin name="VSS-2"/>
<pin name="P0.0/TXD0/PWM1"/>
<pin name="P1.31/TRST"/>
<pin name="P0.1/RXD0/PWM3/EINT0"/>
<pin name="P0.2/SCL/CAP0.0"/>
<pin name="V3-1"/>
<pin name="P1.26/RTCK"/>
<pin name="VSS-3"/>
<pin name="P0.3/SDA/MAT0.0/EINT1"/>
<pin name="P0.4/SCK0/CAP0.1"/>
<pin name="P1.25/EXTIN0"/>
<pin name="P0.5/MISO0/MAT0.1"/>
<pin name="P0.6/MOSI0/CAP0.2"/>
<pin name="P0.7/SSEL0/PWM2/EINT2"/>
<pin name="P1.24/TRACECLK"/>
<pin name="P0.8/TXD1/PWM4"/>
<pin name="P0.9/RXD1/PWM6/EINT3"/>
<pin name="P0.10/RTS1/CAP1.0/RD5"/>
<pin name="P1.23/PIPESTAT2"/>
<pin name="P0.11/CTS1/CAP1.1/TD5"/>
<pin name="P0.12/DSR1/MAT1.0/RD4"/>
<pin name="P0.13/DTR1/MAT1.1/TD4"/>
<pin name="P1.22/PIPESTAT1"/>
<pin name="P0.14/DCD1/EINT1"/>
<pin name="VSS-4"/>
<pin name="V3-2"/>
<pin name="P1.21/PIPESTAT0"/>
<pin name="P0.15/RI1/EINT2"/>
<pin name="P0.16/EINT0/MAT0.2/CAP0.2"/>
<pin name="P0.17/CAP1.2/SCK1/MAT1.2"/>
<pin name="P1.20/TRACESYNC"/>
<pin name="V18-2"/>
<pin name="VSS-5"/>
<pin name="V3-3"/>
<pin name="P1.3/TMS"/>
<pin name="P0.18/CAP1.3/MISO1/MAT1.3"/>
<pin name="P0.19/MAT1.2/MOSI1/MAT1.3"/>
<pin name="P0.20/MAT1.3/SSEL1/EINT3"/>
<pin name="P1.29/TCK"/>
<pin name="RST"/>
<pin name="VSSA_PLL"/>
<pin name="VSSA"/>
<pin name="P1.28/TDI"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="V18A"/>
<pin name="P1.27TDO"/>
</symbol>
<symbol name="LPC2214">
<pin name="P2.22/D22"/>
<pin name="VDD3-1(I/O)"/>
<pin name="VSS1"/>
<pin name="P0.21/PWM5/CAP1.3"/>
<pin name="P0.22/CAP0.0/MAT0.0"/>
<pin name="P0.23"/>
<pin name="P1.19/TRACEPKT3"/>
<pin name="P0.24"/>
<pin name="VSS2"/>
<pin name="P2.23/D23"/>
<pin name="P2.24/D24"/>
<pin name="P2.25/D25"/>
<pin name="P2.26/D26/BOOT0"/>
<pin name="VDD3-1(A)"/>
<pin name="P1.18/TRACEPKT2"/>
<pin name="P2.27/D27/BOOT1"/>
<pin name="P2.28/D28"/>
<pin name="P2.29/D29"/>
<pin name="P2.30/D30/AIN4"/>
<pin name="P2.31/D31/AIN5"/>
<pin name="P0.25"/>
<pin name="TD1"/>
<pin name="P0.27/AIN0/CAP0.1/MAT0.1"/>
<pin name="P1.17/TRACEPKT1"/>
<pin name="P0.28/AIN1/CAP0.2/MAT0.2"/>
<pin name="VSS3"/>
<pin name="P3.29/BLS2/AIN6"/>
<pin name="P3.28/BLS3/AIN7"/>
<pin name="P3.27/WE"/>
<pin name="P3.26/CS1"/>
<pin name="VDD3-2(I/O)"/>
<pin name="P0.29/AIN2/CAP0.3/MAT0.3"/>
<pin name="P0.30/AIN3/EINT3/CAP0.0"/>
<pin name="P1.16/TRACEPKT0"/>
<pin name="P3.25/CS2"/>
<pin name="P3.24/CS3"/>
<pin name="VDD1.8-1(CORE)"/>
<pin name="VSS4"/>
<pin name="VDD3-3(I/O)"/>
<pin name="P3.23/A23/XCLK"/>
<pin name="P3.22/A21"/>
<pin name="P0.0/TXD0/PWM1"/>
<pin name="P1.31/TRST"/>
<pin name="P3.21/A21"/>
<pin name="P3.20/A20"/>
<pin name="P3.19/A19"/>
<pin name="P3.18/A18"/>
<pin name="P3.17/A17"/>
<pin name="P0.1/RXD0/PWM3/EINT0"/>
<pin name="P0.2/SCL/CAP0.0"/>
<pin name="VDD3-4(I/O)"/>
<pin name="P1.26/RTCK"/>
<pin name="P3.16/A16"/>
<pin name="VSS5"/>
<pin name="P3.15/A15"/>
<pin name="P3.14/14"/>
<pin name="VDD3-5(I/O)"/>
<pin name="P0.3/SDA/MAT0.0/EINT1"/>
<pin name="P0.4/SCK0/CAP0.1"/>
<pin name="P1.25/EXTIN0"/>
<pin name="P0.5/MISO0/MAT0.1"/>
<pin name="P3.13/A13"/>
<pin name="P3.12/A12"/>
<pin name="P3.11/A11"/>
<pin name="P3.10/A10"/>
<pin name="P3.9/A9"/>
<pin name="VSS6"/>
<pin name="P0.6/MOSI0/CAP0.2"/>
<pin name="P0.7/SSEL0/PWM2/EINT2"/>
<pin name="P1.24/TRACECLK"/>
<pin name="P3.8/A8"/>
<pin name="P3.7/A7"/>
<pin name="P3.6/A6"/>
<pin name="P3.5/A5"/>
<pin name="P0.8/TXD1/PWM4"/>
<pin name="P0.9/RXD1/PWM6/EINT3"/>
<pin name="VDD3-6(I/O)"/>
<pin name="P0.10/RTS1/CAP1.0"/>
<pin name="VSS7"/>
<pin name="P3.4/A4"/>
<pin name="P3.3/A3"/>
<pin name="P1.23/PIPESTAT2"/>
<pin name="P0.11/CTS1/CAP1.1"/>
<pin name="P.012/DSR1/MAT1.0"/>
<pin name="P0.13/DTR1/MAT1.1"/>
<pin name="P1.22/PIPESTAT1"/>
<pin name="P3.2/A2"/>
<pin name="P3.1/A1"/>
<pin name="P3.0//A0"/>
<pin name="P1.1/OE"/>
<pin name="P1.0/CS0"/>
<pin name="P0.14/DCD1/EINT1"/>
<pin name="VSS8"/>
<pin name="VDD3-7(I/O)"/>
<pin name="P1.21/PIPESTAT0"/>
<pin name="P3.31/BLS0"/>
<pin name="P3.30/BLS1"/>
<pin name="P2.0/D0"/>
<pin name="P0.15/RI1/EINT2"/>
<pin name="P0.16/EINT0/MAT0.2/CAP0.2"/>
<pin name="P0.17/CAP1.2/SCK1/MAT1.2"/>
<pin name="P1.20/TRACESYNC"/>
<pin name="VSS9"/>
<pin name="VDD3-8(I/O)"/>
<pin name="P2.1/D1"/>
<pin name="P2.2/D2"/>
<pin name="VSS10"/>
<pin name="P2.3/D3"/>
<pin name="P2.4/D4"/>
<pin name="VDD1.8-2(CORE)"/>
<pin name="VSS11"/>
<pin name="VDD3-9(I/O)"/>
<pin name="P1.30/TMS"/>
<pin name="P2.5/D5"/>
<pin name="P2.6/D6"/>
<pin name="P2.7/D7"/>
<pin name="P2.8/D8"/>
<pin name="P2.9/D9"/>
<pin name="VDD3-10(I/O)"/>
<pin name="P2.10/D10"/>
<pin name="P0.18/CAP1.3/MISO1/MAT1.3"/>
<pin name="P0.19/MAT1.2/MOSI1/CAP1.2"/>
<pin name="P0.20/MAT1.3/SSEL1/EINT3"/>
<pin name="P2.11/D11"/>
<pin name="P2.12/D12"/>
<pin name="P1.29/TCK"/>
<pin name="P2.13/D13"/>
<pin name="VSS12"/>
<pin name="P2.14/D14"/>
<pin name="P2.15/D15"/>
<pin name="P2.16/D16"/>
<pin name="P2.17/D17"/>
<pin name="P2.18/D18"/>
<pin name="P2.19/D19"/>
<pin name="RST" function="dot"/>
<pin name="P2.20/D20"/>
<pin name="P2.21/D21"/>
<pin name="VSSA_PLL"/>
<pin name="VSSA"/>
<pin name="P1.28/TDI"/>
<pin name="X2"/>
<pin name="X1"/>
<pin name="VDD1.8(A)"/>
<pin name="P1.27/TDO"/>
</symbol>
<symbol name="ICP_CON">
<pin name="3.3V" direction="pas"/>
<pin name="/RST" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="P0.4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="P0.5" direction="pas"/>
</symbol>
<symbol name="ISP_CON">
<pin name="3.3V" direction="pas"/>
<pin name="/RST" direction="pas"/>
<pin name="/ISP" direction="pas"/>
<pin name="RXD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TXD" direction="pas"/>
</symbol>
<symbol name="LM75A">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="OS"/>
<pin name="GND"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VCC"/>
</symbol>
<symbol name="LPC213X">
<pin name="P1.16(TRACEPKT0)"/>
<pin name="P1.17(TRACEPKT1)"/>
<pin name="P1.18(TRACEPKT2)"/>
<pin name="P1.19(TRACEPKT3)"/>
<pin name="P1.20(TRACESYNC)"/>
<pin name="P1.21(PIPESTAT0)"/>
<pin name="P1.22(PIPESTAT1)"/>
<pin name="P1.23(PIPESTAT2)"/>
<pin name="(MISO0/MAT0.1/A0.7)P0.5"/>
<pin name="(SSEL0/PWM2/EINT2)P0.7"/>
<pin name="(TXD1/PWM4/A1.1)P0.8"/>
<pin name="(RXD1/PWM6/EINT3)P0.9"/>
<pin name="(RTS1/CAP1.0/AD1.2)P0.10"/>
<pin name="(CTS1/CAP1.1/SCL1)P0.11"/>
<pin name="P1.24(TRACECLK)"/>
<pin name="P1.25(EXTIN0)"/>
<pin name="P1.26(RTCK)"/>
<pin name="P1.27(TDO)"/>
<pin name="P1.28(TDI)"/>
<pin name="P1.29(TCK)"/>
<pin name="P1.30(TMS)"/>
<pin name="P1.31(/TRST)"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="(DSR1/MAT1.0/AD1.3)P0.12"/>
<pin name="(DTR1/MAT1.1/AD1.4)P0.13"/>
<pin name="(DCD1/EINT1/SDA1)P0.14"/>
<pin name="(RI1/EINT2/AD1.5)P0.15"/>
<pin name="(EINT0/MAT0.2/CAP0.2)P0.16"/>
<pin name="(CAP1.2/SCK1/MAT1.2)P0.17"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA3" direction="pwr"/>
<pin name="VDD3-1" direction="pwr"/>
<pin name="VDD3-2" direction="pwr"/>
<pin name="VDD3-3" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="(TXD0/PWM1)P0.0"/>
<pin name="(RXD0/PWM3/EINT0)P0.1"/>
<pin name="(SCL0/CAP0.0)P0.2"/>
<pin name="(SDA0/MAT0.0/EINT1)P0.3"/>
<pin name="(SCK0/CAP0.1/AD0.6)P0.4"/>
<pin name="(MOSI0/CAP0.2/AD1.0)P0.6"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="RTXC1" direction="in"/>
<pin name="RTXC2" direction="out"/>
<pin name="(CAP1.3/MISO1/MAT1.3)P0.18"/>
<pin name="(MAT1.2/MOSI1/CAP1.2)P0.19"/>
<pin name="(MAT1.3/SSEL1/EINT3)P0.20"/>
<pin name="(PWM5/AD1.6/CAP1.3)P0.21"/>
<pin name="(AD1.7/CAP0.0/MAT0.0)P0.22"/>
<pin name="P0.23"/>
<pin name="(AD0.4/AOUT)P0.25"/>
<pin name="(AD0.5)P0.26"/>
<pin name="(AD0.0/CAP0.1/MAT0.1)P0.27"/>
<pin name="(AD0.1/CAP0.2/MAT0.2)P0.28"/>
<pin name="(AD0.2/CAP0.3/MAT0.3)P0.29"/>
<pin name="(AD0.3/EINT3/CAP0.0)P0.30"/>
<pin name="P0.31" direction="out"/>
</symbol>
<symbol name="LPC9107">
<pin name="P0.2/KBI2/AD11"/>
<pin name="N.C." direction="nc"/>
<pin name="P1.5/RST"/>
<pin name="VSS"/>
<pin name="P0.1/KBI1/AD10"/>
<pin name="P1.0/TXD"/>
<pin name="P1.2/T0"/>
<pin name="P0.7/T1/CLKOUT"/>
<pin name="P1.1/RXD"/>
<pin name="VDD"/>
<pin name="P0.5/CMPREF/CLKIN"/>
<pin name="P0.4/CIN1A/AD13/DAC1"/>
<pin name="NC" direction="nc"/>
<pin name="P0.3/CIN1B/AD12"/>
</symbol>
<symbol name="PCF8563">
<pin name="OSCI"/>
<pin name="OSCO"/>
<pin name="/INT"/>
<pin name="VSS"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="CLKOUT"/>
<pin name="VDD"/>
</symbol>
<symbol name="PCA24S08">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="WP" direction="in"/>
<pin name="/PROT" direction="in" function="dot"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PCA8581">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="TEST"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCA9538">
<pin name="A0"/>
<pin name="A1"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="/RST"/>
<pin name="/INT"/>
<pin name="IO0"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
</symbol>
<symbol name="PCA9557">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="/RST"/>
<pin name="IO0"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
</symbol>
<symbol name="PCF8570">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="TEST"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF8582">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="PTC"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF8583">
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="INT" direction="out" function="dot"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
</symbol>
<symbol name="PCF8594">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="PTC"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="PCF8598">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="PTC"/>
<pin name="A2" direction="in"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="PCF85102">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF85103">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="PCF85116">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="SAA3010">
<pin name="1/X7"/>
<pin name="2/SSM"/>
<pin name="3/Z0"/>
<pin name="4/Z1"/>
<pin name="5/Z2"/>
<pin name="6/Z3"/>
<pin name="7/MDATA"/>
<pin name="8/DATA"/>
<pin name="9/DR7"/>
<pin name="10/DR6"/>
<pin name="11/DR5"/>
<pin name="12/DR4"/>
<pin name="13/DR3"/>
<pin name="14/VSS" direction="pwr"/>
<pin name="15/DR2"/>
<pin name="16/DR1"/>
<pin name="17/DR0"/>
<pin name="18/OSC"/>
<pin name="19/TP2"/>
<pin name="20/TP1"/>
<pin name="21/X0"/>
<pin name="22/X1"/>
<pin name="23/X2"/>
<pin name="24/X3"/>
<pin name="25/X4"/>
<pin name="26/X5"/>
<pin name="27/X6"/>
<pin name="28/VDD" direction="pwr"/>
</symbol>
<symbol name="SAA1101">
<pin name="FSI" direction="in"/>
<pin name="FSO" direction="out"/>
<pin name="CS1" direction="in"/>
<pin name="CS0" direction="in"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="VLE" direction="in"/>
<pin name="PH" direction="hiz"/>
<pin name="LM1" direction="in"/>
<pin name="LM0" direction="in"/>
<pin name="ECS" direction="in"/>
<pin name="RR" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="ID" direction="out"/>
<pin name="BK" direction="out"/>
<pin name="CB" direction="out"/>
<pin name="CS" direction="out"/>
<pin name="CLP" direction="out"/>
<pin name="WMP" direction="pas"/>
<pin name="VD" direction="out"/>
<pin name="HD" direction="out"/>
<pin name="NORM" direction="in"/>
<pin name="CLO" direction="out"/>
<pin name="X" direction="in"/>
<pin name="Y" direction="in"/>
<pin name="Z" direction="in"/>
</symbol>
<symbol name="VDDVSS">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PCA84CX40/84CX43">
<pin name="1/DP0.0/TDAC"/>
<pin name="2/DP0.1/PWM1"/>
<pin name="3/DP0.2/PWM2"/>
<pin name="4/DP0.3/PWM3"/>
<pin name="5/DP0.4/PWM4"/>
<pin name="6/DP0.5/PWM5"/>
<pin name="7/P1.0"/>
<pin name="8/P1.1"/>
<pin name="9/DP1.7/AFC"/>
<pin name="10/P1.2"/>
<pin name="11/P1.3"/>
<pin name="12/1.4"/>
<pin name="13/P0.0"/>
<pin name="14/P0.1"/>
<pin name="15/P0.2"/>
<pin name="16/P0.3"/>
<pin name="17/P0.4"/>
<pin name="18/P0.5"/>
<pin name="19/P0.6"/>
<pin name="20/P0.7"/>
<pin name="21/VSS" direction="pwr"/>
<pin name="22/VOW1/DP1.6"/>
<pin name="23/VOW2/DP1.5"/>
<pin name="24/VOW3"/>
<pin name="25/VOB"/>
<pin name="26/HSYNCN"/>
<pin name="27/VSYNCN"/>
<pin name="28/DOSC1"/>
<pin name="29/T1"/>
<pin name="30/TEST/EMU"/>
<pin name="31/XTAL1"/>
<pin name="32/XTAL2"/>
<pin name="33/RESET"/>
<pin name="34/DP1.4"/>
<pin name="35/INT/T0"/>
<pin name="36/DP1.3"/>
<pin name="37/DP1.2"/>
<pin name="38/DP1.1"/>
<pin name="39/DP0.7/SCL"/>
<pin name="40/DP0.6/SDA"/>
<pin name="41/DP1.0"/>
<pin name="42/VDD" direction="pwr"/>
</symbol>
<symbol name="PCA84CX41/84CX44">
<pin name="1/DP0.0/TDAC"/>
<pin name="2/DP0.1/PWM1"/>
<pin name="3/DP0.2/PWM2"/>
<pin name="4/DP0.3/PWM3"/>
<pin name="5/DP0.4/PWM4"/>
<pin name="6/DP0.5/PWM5"/>
<pin name="7/P1.0"/>
<pin name="8/P1.1"/>
<pin name="9/DP1.7/AFC"/>
<pin name="10/P1.2"/>
<pin name="11/P1.3"/>
<pin name="12/1.4"/>
<pin name="13/P0.0"/>
<pin name="14/P0.1"/>
<pin name="15/P0.2"/>
<pin name="16/P0.3"/>
<pin name="17/P0.4"/>
<pin name="18/P0.5"/>
<pin name="19/P0.6"/>
<pin name="20/P0.7"/>
<pin name="21/VSS" direction="pwr"/>
<pin name="22/VOW1/DP1.6"/>
<pin name="23/VOW2/DP1.5"/>
<pin name="24/VOW3"/>
<pin name="25/VOB"/>
<pin name="26/HSYNCN"/>
<pin name="27/VSYNCN"/>
<pin name="28/DOSC1"/>
<pin name="29/DOSC2"/>
<pin name="30/TEST/EMU"/>
<pin name="31/XTAL1"/>
<pin name="32/XTAL2"/>
<pin name="33/RESET"/>
<pin name="34/T1"/>
<pin name="35/INT/T0"/>
<pin name="36/DP1.3"/>
<pin name="37/DP1.2"/>
<pin name="38/DP1.1"/>
<pin name="39/DP0.7/SCL"/>
<pin name="40/DP0.6/SDA"/>
<pin name="41/DP1.0"/>
<pin name="42/VDD" direction="pwr"/>
</symbol>
<symbol name="PCA9564">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="A0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="/CE" direction="in" function="dot"/>
<pin name="/RST" direction="in" function="dot"/>
<pin name="/INT" direction="out" function="dot"/>
<pin name="/WR" direction="in" function="dot"/>
<pin name="/RD" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
</symbol>
<symbol name="PWR5+2">
<pin name="VDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VREF" direction="pwr"/>
<pin name="AVREF-" direction="pwr"/>
</symbol>
<symbol name="8XC562">
<pin name="EA" direction="in" function="dot"/>
<pin name="P0.0/D0"/>
<pin name="P0.1/D1"/>
<pin name="P0.2/D2"/>
<pin name="P0.3/D3"/>
<pin name="P0.4/D4"/>
<pin name="P0.5/D5"/>
<pin name="P0.6/D6"/>
<pin name="P0.7/D7"/>
<pin name="P5.0/ADC0"/>
<pin name="P5.1/ADC1"/>
<pin name="P5.2/ADC2"/>
<pin name="P5.3/ADC3"/>
<pin name="P5.4/ADC4"/>
<pin name="P5.5/ADC5"/>
<pin name="P5.6/ADC6"/>
<pin name="P5.7/ADC7"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out" function="dot"/>
<pin name="P4.0/CMSR0"/>
<pin name="P2.0/A8" direction="out"/>
<pin name="P4.1/CMSR1"/>
<pin name="P4.2/CMSR2"/>
<pin name="P4.3/CMSR3"/>
<pin name="P2.1/A9" direction="out"/>
<pin name="P2.2/A10" direction="out"/>
<pin name="P2.3/A11" direction="out"/>
<pin name="P2.4/A12" direction="out"/>
<pin name="P2.5/A13" direction="out"/>
<pin name="P2.6/A14" direction="out"/>
<pin name="P2.7/A15" direction="out"/>
<pin name="P1.0/CT0I"/>
<pin name="P1.1/CT1I"/>
<pin name="P1.2/CT2I"/>
<pin name="P1.3/CT3I"/>
<pin name="P1.4/T2"/>
<pin name="P1.5/RT2"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P4.4/CMSR4"/>
<pin name="P4.5/CMSR5"/>
<pin name="P4.6/CMT0"/>
<pin name="P4.7/CMT1"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2" function="dot"/>
<pin name="P3.3" function="dot"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR" function="dot"/>
<pin name="P3.7/RD" function="dot"/>
<pin name="STADC"/>
<pin name="PWM0"/>
<pin name="PWM1"/>
<pin name="/EW" function="dot"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
</symbol>
<symbol name="LOGO10">
</symbol>
<symbol name="LOGO20">
</symbol>
<symbol name="PCF9543">
<pin name="A0" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="!RST" direction="in"/>
<pin name="!INT0" direction="in"/>
<pin name="SD0"/>
<pin name="SC0"/>
<pin name="VSS" direction="pwr"/>
<pin name="!INT1" direction="in"/>
<pin name="SD1"/>
<pin name="SC1"/>
<pin name="!INT" direction="out"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="TDA8708A">
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="VCCA" direction="sup"/>
<pin name="VCCD" direction="sup"/>
<pin name="VCCO" direction="sup"/>
<pin name="AGND" direction="sup"/>
<pin name="DGND" direction="sup"/>
<pin name="I0" direction="sup"/>
<pin name="I1" direction="sup"/>
<pin name="VIN0" direction="sup"/>
<pin name="VIN1" direction="sup"/>
<pin name="VIN2" direction="sup"/>
<pin name="RPEAK" direction="in"/>
<pin name="AGC" direction="in"/>
<pin name="DEC" direction="in"/>
<pin name="CLAMP" direction="in"/>
<pin name="ADCIN" direction="in"/>
<pin name="ANOUT" direction="out"/>
<pin name="OF" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="GATEA" direction="in"/>
<pin name="GATEB" direction="in"/>
</symbol>
<symbol name="74LVC4245A">
<pin name="VCCA" direction="pwr"/>
<pin name="VCCB@" direction="pwr"/>
<pin name="VCCB" direction="pwr"/>
<pin name="GND@" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="DIR" direction="in"/>
<pin name="!OE" direction="out"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="A7"/>
<pin name="B6"/>
<pin name="B7"/>
</symbol>
<symbol name="TDA8703">
<pin name="1/D1" direction="out"/>
<pin name="2/D0" direction="out"/>
<pin name="3/AGND" direction="pwr"/>
<pin name="4/VRB"/>
<pin name="5/DEC" direction="in"/>
<pin name="6/NC" direction="nc"/>
<pin name="7/VCCA" direction="pwr"/>
<pin name="8/VI" direction="in"/>
<pin name="9/VRT"/>
<pin name="10/NC" direction="nc"/>
<pin name="11/O/UF" direction="out"/>
<pin name="12/D7" direction="out"/>
<pin name="13/D6" direction="out"/>
<pin name="14/D5" direction="out"/>
<pin name="15/D4" direction="out"/>
<pin name="16/CLK" direction="in"/>
<pin name="17/CLK" direction="in"/>
<pin name="18/VCCD" direction="pwr"/>
<pin name="19/VCCO" direction="pwr"/>
<pin name="20/DGND" direction="pwr"/>
<pin name="21/TC" direction="in"/>
<pin name="22/CE" direction="in"/>
<pin name="23/D3" direction="out"/>
<pin name="24/D2" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="P90CL301" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="P90CL301"/>
</gates>
<devices>
<device name="" package="QFP12-80">
<connects>
<connect gate="G$1" pin="A1" pad="14"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="24"/>
<connect gate="G$1" pin="A12" pad="25"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="28"/>
<connect gate="G$1" pin="A16" pad="29"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="16"/>
<connect gate="G$1" pin="A4" pad="17"/>
<connect gate="G$1" pin="A5" pad="18"/>
<connect gate="G$1" pin="A6" pad="19"/>
<connect gate="G$1" pin="A7" pad="20"/>
<connect gate="G$1" pin="A8" pad="21"/>
<connect gate="G$1" pin="A9" pad="22"/>
<connect gate="G$1" pin="AS" pad="1"/>
<connect gate="G$1" pin="BSIZE" pad="58"/>
<connect gate="G$1" pin="CS0/FC0" pad="44"/>
<connect gate="G$1" pin="CS1/FC1" pad="43"/>
<connect gate="G$1" pin="CS2/FC2" pad="42"/>
<connect gate="G$1" pin="CS3/ALE" pad="41"/>
<connect gate="G$1" pin="CS4/RD" pad="40"/>
<connect gate="G$1" pin="CS5/WR" pad="39"/>
<connect gate="G$1" pin="CS6/A23" pad="37"/>
<connect gate="G$1" pin="CSBT/ONCE" pad="38"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="D10/P2" pad="75"/>
<connect gate="G$1" pin="D11/P3" pad="74"/>
<connect gate="G$1" pin="D12/P4" pad="73"/>
<connect gate="G$1" pin="D13/P5" pad="72"/>
<connect gate="G$1" pin="D14/P6" pad="71"/>
<connect gate="G$1" pin="D15/P7" pad="70"/>
<connect gate="G$1" pin="D2" pad="7"/>
<connect gate="G$1" pin="D3" pad="6"/>
<connect gate="G$1" pin="D4" pad="5"/>
<connect gate="G$1" pin="D5" pad="4"/>
<connect gate="G$1" pin="D6" pad="3"/>
<connect gate="G$1" pin="D7" pad="2"/>
<connect gate="G$1" pin="D8/P0" pad="77"/>
<connect gate="G$1" pin="D9/P1" pad="76"/>
<connect gate="G$1" pin="DTACK" pad="78"/>
<connect gate="G$1" pin="HALT" pad="68"/>
<connect gate="G$1" pin="LDS/DS" pad="80"/>
<connect gate="G$1" pin="P10/SCL" pad="56"/>
<connect gate="G$1" pin="P11/SDA" pad="57"/>
<connect gate="G$1" pin="P12/ADC0" pad="64"/>
<connect gate="G$1" pin="P13/ADC1" pad="63"/>
<connect gate="G$1" pin="P14/ADC2" pad="62"/>
<connect gate="G$1" pin="P15/ADC3" pad="60"/>
<connect gate="G$1" pin="P8/PWM0" pad="54"/>
<connect gate="G$1" pin="P9/PWM1" pad="55"/>
<connect gate="G$1" pin="PCS0/A19" pad="33"/>
<connect gate="G$1" pin="PCS1/A20" pad="34"/>
<connect gate="G$1" pin="PCS2/A21" pad="35"/>
<connect gate="G$1" pin="PCS3/A22" pad="36"/>
<connect gate="G$1" pin="RESET" pad="67"/>
<connect gate="G$1" pin="RESETIN" pad="66"/>
<connect gate="G$1" pin="SP0/INT0/" pad="53"/>
<connect gate="G$1" pin="SP1/INT1/" pad="52"/>
<connect gate="G$1" pin="SP2/INT2/" pad="50"/>
<connect gate="G$1" pin="SP3/INT3/" pad="49"/>
<connect gate="G$1" pin="SP4/INT4" pad="48"/>
<connect gate="G$1" pin="SP5/INT5" pad="47"/>
<connect gate="G$1" pin="SP6/INT6" pad="46"/>
<connect gate="G$1" pin="SP7/NMIN" pad="45"/>
<connect gate="G$1" pin="TROM_R/W" pad="79"/>
<connect gate="G$1" pin="UDS/A0" pad="13"/>
<connect gate="G$1" pin="VDD" pad="69"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VDD@2" pad="10"/>
<connect gate="G$1" pin="VDDA" pad="59"/>
<connect gate="G$1" pin="VREF" pad="61"/>
<connect gate="G$1" pin="VSS" pad="51"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
<connect gate="G$1" pin="VSSA" pad="65"/>
<connect gate="G$1" pin="XTAL1" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C552" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="80C552"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="A08-P2.0" pad="39"/>
<connect gate="G$1" pin="A09-P2.1" pad="40"/>
<connect gate="G$1" pin="A10-P2.2" pad="41"/>
<connect gate="G$1" pin="A11-P2.3" pad="42"/>
<connect gate="G$1" pin="A12-P2.4" pad="43"/>
<connect gate="G$1" pin="A13-P2.5" pad="44"/>
<connect gate="G$1" pin="A14-P2.6" pad="45"/>
<connect gate="G$1" pin="A15-P2.7" pad="46"/>
<connect gate="G$1" pin="AD0-P0.0" pad="57"/>
<connect gate="G$1" pin="AD1-P0.1" pad="56"/>
<connect gate="G$1" pin="AD2-P0.2" pad="55"/>
<connect gate="G$1" pin="AD3-P0.3" pad="54"/>
<connect gate="G$1" pin="AD4-P0.4" pad="53"/>
<connect gate="G$1" pin="AD5-P0.5" pad="52"/>
<connect gate="G$1" pin="AD6-P0.6" pad="51"/>
<connect gate="G$1" pin="AD7-P0.7" pad="50"/>
<connect gate="G$1" pin="ALE-PROG/" pad="48"/>
<connect gate="G$1" pin="AVDD" pad="61"/>
<connect gate="G$1" pin="AVREF+" pad="59"/>
<connect gate="G$1" pin="AVREF-" pad="58"/>
<connect gate="G$1" pin="AVSS" pad="60"/>
<connect gate="G$1" pin="CSL-P1.6" pad="22"/>
<connect gate="G$1" pin="CT0I-P1.0" pad="16"/>
<connect gate="G$1" pin="CT1I-P1.1" pad="17"/>
<connect gate="G$1" pin="CT2I-P1.2" pad="18"/>
<connect gate="G$1" pin="CT3I-P1.3" pad="19"/>
<connect gate="G$1" pin="EA/VPP" pad="49"/>
<connect gate="G$1" pin="EW/" pad="6"/>
<connect gate="G$1" pin="NC1" pad="32"/>
<connect gate="G$1" pin="NC2" pad="33"/>
<connect gate="G$1" pin="NC3" pad="38"/>
<connect gate="G$1" pin="P3.0-RXD" pad="24"/>
<connect gate="G$1" pin="P3.1-TXD" pad="25"/>
<connect gate="G$1" pin="P3.2-INT0/" pad="26"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="27"/>
<connect gate="G$1" pin="P3.4-T0" pad="28"/>
<connect gate="G$1" pin="P3.5-T1" pad="29"/>
<connect gate="G$1" pin="P3.6-WR/" pad="30"/>
<connect gate="G$1" pin="P3.7-RD/" pad="31"/>
<connect gate="G$1" pin="P4.0-CMSR0" pad="7"/>
<connect gate="G$1" pin="P4.1-CMSR1" pad="8"/>
<connect gate="G$1" pin="P4.2-CMSR2" pad="9"/>
<connect gate="G$1" pin="P4.3-CMSR3" pad="10"/>
<connect gate="G$1" pin="P4.4-CMSR4" pad="11"/>
<connect gate="G$1" pin="P4.5-CMSR5" pad="12"/>
<connect gate="G$1" pin="P4.6-CMT0" pad="13"/>
<connect gate="G$1" pin="P4.7-CMT1" pad="14"/>
<connect gate="G$1" pin="P5.0-ADC0" pad="1"/>
<connect gate="G$1" pin="P5.1-ADC1" pad="68"/>
<connect gate="G$1" pin="P5.2-ADC2" pad="67"/>
<connect gate="G$1" pin="P5.3-ADC3" pad="66"/>
<connect gate="G$1" pin="P5.4-ADC4" pad="65"/>
<connect gate="G$1" pin="P5.5-ADC5" pad="64"/>
<connect gate="G$1" pin="P5.6-ADC6" pad="63"/>
<connect gate="G$1" pin="P5.7-ADC7" pad="62"/>
<connect gate="G$1" pin="PSEN/" pad="47"/>
<connect gate="G$1" pin="PWM0/" pad="4"/>
<connect gate="G$1" pin="PWM1/" pad="5"/>
<connect gate="G$1" pin="RST" pad="15"/>
<connect gate="G$1" pin="RT2-P1.5" pad="21"/>
<connect gate="G$1" pin="SDA-P1.7" pad="23"/>
<connect gate="G$1" pin="STADC" pad="3"/>
<connect gate="G$1" pin="T2-P1.4" pad="20"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="36"/>
<connect gate="G$1" pin="VSS@1" pad="37"/>
<connect gate="G$1" pin="XTAL1" pad="35"/>
<connect gate="G$1" pin="XTAL2" pad="34"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C552Q80" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="80C552"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="P" symbol="VSS"/>
<gate name="NU33" symbol="NU"/>
<gate name="NU73" symbol="NU"/>
</gates>
<devices>
<device name="" package="QFP80R">
<connects>
<connect gate="G$1" pin="A08-P2.0" pad="38"/>
<connect gate="G$1" pin="A09-P2.1" pad="39"/>
<connect gate="G$1" pin="A10-P2.2" pad="40"/>
<connect gate="G$1" pin="A11-P2.3" pad="41"/>
<connect gate="G$1" pin="A12-P2.4" pad="42"/>
<connect gate="G$1" pin="A13-P2.5" pad="45"/>
<connect gate="G$1" pin="A14-P2.6" pad="46"/>
<connect gate="G$1" pin="A15-P2.7" pad="47"/>
<connect gate="G$1" pin="AD0-P0.0" pad="58"/>
<connect gate="G$1" pin="AD1-P0.1" pad="57"/>
<connect gate="G$1" pin="AD2-P0.2" pad="56"/>
<connect gate="G$1" pin="AD3-P0.3" pad="55"/>
<connect gate="G$1" pin="AD4-P0.4" pad="54"/>
<connect gate="G$1" pin="AD5-P0.5" pad="53"/>
<connect gate="G$1" pin="AD6-P0.6" pad="52"/>
<connect gate="G$1" pin="AD7-P0.7" pad="51"/>
<connect gate="G$1" pin="ALE-PROG/" pad="49"/>
<connect gate="G$1" pin="AVDD" pad="63"/>
<connect gate="G$1" pin="AVREF+" pad="60"/>
<connect gate="G$1" pin="AVREF-" pad="59"/>
<connect gate="G$1" pin="AVSS" pad="61"/>
<connect gate="G$1" pin="CSL-P1.6" pad="16"/>
<connect gate="G$1" pin="CT0I-P1.0" pad="10"/>
<connect gate="G$1" pin="CT1I-P1.1" pad="11"/>
<connect gate="G$1" pin="CT2I-P1.2" pad="12"/>
<connect gate="G$1" pin="CT3I-P1.3" pad="13"/>
<connect gate="G$1" pin="EA/VPP" pad="50"/>
<connect gate="G$1" pin="EW/" pad="77"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="21"/>
<connect gate="G$1" pin="NC3" pad="22"/>
<connect gate="G$1" pin="P3.0-RXD" pad="18"/>
<connect gate="G$1" pin="P3.1-TXD" pad="19"/>
<connect gate="G$1" pin="P3.2-INT0/" pad="20"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="23"/>
<connect gate="G$1" pin="P3.4-T0" pad="24"/>
<connect gate="G$1" pin="P3.5-T1" pad="25"/>
<connect gate="G$1" pin="P3.6-WR/" pad="26"/>
<connect gate="G$1" pin="P3.7-RD/" pad="27"/>
<connect gate="G$1" pin="P4.0-CMSR0" pad="80"/>
<connect gate="G$1" pin="P4.1-CMSR1" pad="1"/>
<connect gate="G$1" pin="P4.2-CMSR2" pad="2"/>
<connect gate="G$1" pin="P4.3-CMSR3" pad="4"/>
<connect gate="G$1" pin="P4.4-CMSR4" pad="5"/>
<connect gate="G$1" pin="P4.5-CMSR5" pad="6"/>
<connect gate="G$1" pin="P4.6-CMT0" pad="7"/>
<connect gate="G$1" pin="P4.7-CMT1" pad="8"/>
<connect gate="G$1" pin="P5.0-ADC0" pad="71"/>
<connect gate="G$1" pin="P5.1-ADC1" pad="70"/>
<connect gate="G$1" pin="P5.2-ADC2" pad="69"/>
<connect gate="G$1" pin="P5.3-ADC3" pad="68"/>
<connect gate="G$1" pin="P5.4-ADC4" pad="67"/>
<connect gate="G$1" pin="P5.5-ADC5" pad="66"/>
<connect gate="G$1" pin="P5.6-ADC6" pad="65"/>
<connect gate="G$1" pin="P5.7-ADC7" pad="64"/>
<connect gate="G$1" pin="PSEN/" pad="48"/>
<connect gate="G$1" pin="PWM0/" pad="75"/>
<connect gate="G$1" pin="PWM1/" pad="76"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="RT2-P1.5" pad="15"/>
<connect gate="G$1" pin="SDA-P1.7" pad="17"/>
<connect gate="G$1" pin="STADC" pad="74"/>
<connect gate="G$1" pin="T2-P1.4" pad="14"/>
<connect gate="G$1" pin="VDD" pad="72"/>
<connect gate="G$1" pin="VSS" pad="34"/>
<connect gate="G$1" pin="VSS@1" pad="35"/>
<connect gate="G$1" pin="XTAL1" pad="32"/>
<connect gate="G$1" pin="XTAL2" pad="31"/>
<connect gate="NC1" pin="NC" pad="28"/>
<connect gate="NC2" pin="NC" pad="29"/>
<connect gate="NC3" pin="NC" pad="30"/>
<connect gate="NC4" pin="NC" pad="37"/>
<connect gate="NC5" pin="NC" pad="43"/>
<connect gate="NC6" pin="NC" pad="44"/>
<connect gate="NC7" pin="NC" pad="62"/>
<connect gate="NC8" pin="NC" pad="78"/>
<connect gate="NC9" pin="NC" pad="79"/>
<connect gate="NU33" pin="IC-NU" pad="33"/>
<connect gate="NU73" pin="IC-NU" pad="73"/>
<connect gate="P" pin="VSS" pad="36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7052SMD" prefix="IC">
<gates>
<gate name="G$1" symbol="OP+-DIF"/>
</gates>
<devices>
<device name="" package="SOT505-1">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="P$1" pad="5"/>
<connect gate="G$1" pin="P$2" pad="8"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7052DIL" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="OP+-DIF"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="P$1" pad="5"/>
<connect gate="G$1" pin="P$2" pad="8"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82C250SMD" prefix="IC">
<gates>
<gate name="82C250" symbol="82C250"/>
</gates>
<devices>
<device name="SMD" package="SOT505-1">
<connects>
<connect gate="82C250" pin="CANH" pad="7"/>
<connect gate="82C250" pin="CANL" pad="6"/>
<connect gate="82C250" pin="GND" pad="2"/>
<connect gate="82C250" pin="RS" pad="8"/>
<connect gate="82C250" pin="RXD" pad="4"/>
<connect gate="82C250" pin="TXD" pad="1"/>
<connect gate="82C250" pin="VCC" pad="3"/>
<connect gate="82C250" pin="VREFOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIL" package="DIL08">
<connects>
<connect gate="82C250" pin="CANH" pad="7"/>
<connect gate="82C250" pin="CANL" pad="6"/>
<connect gate="82C250" pin="GND" pad="2"/>
<connect gate="82C250" pin="RS" pad="8"/>
<connect gate="82C250" pin="RXD" pad="4"/>
<connect gate="82C250" pin="TXD" pad="1"/>
<connect gate="82C250" pin="VCC" pad="3"/>
<connect gate="82C250" pin="VREFOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SJA1000" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="SJA1000"/>
</gates>
<devices>
<device name="" package="SOT136-1">
<connects>
<connect gate="G$1" pin="AD0" pad="23"/>
<connect gate="G$1" pin="AD1" pad="24"/>
<connect gate="G$1" pin="AD2" pad="25"/>
<connect gate="G$1" pin="AD3" pad="26"/>
<connect gate="G$1" pin="AD4" pad="27"/>
<connect gate="G$1" pin="AD5" pad="28"/>
<connect gate="G$1" pin="AD6" pad="1"/>
<connect gate="G$1" pin="AD7" pad="2"/>
<connect gate="G$1" pin="ALE/AS" pad="3"/>
<connect gate="G$1" pin="CLK_OUT" pad="7"/>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="INT" pad="16"/>
<connect gate="G$1" pin="MODE" pad="11"/>
<connect gate="G$1" pin="RD/E" pad="5"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="RX0" pad="19"/>
<connect gate="G$1" pin="RX1" pad="20"/>
<connect gate="G$1" pin="TX0" pad="13"/>
<connect gate="G$1" pin="TX1" pad="14"/>
<connect gate="G$1" pin="VDD1" pad="22"/>
<connect gate="G$1" pin="VDD2" pad="18"/>
<connect gate="G$1" pin="VDD3" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="21"/>
<connect gate="G$1" pin="VSS3" pad="15"/>
<connect gate="G$1" pin="WR" pad="6"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82C150" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="82C150"/>
</gates>
<devices>
<device name="" package="SOT136-1">
<connects>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="P0/CLK" pad="27"/>
<connect gate="G$1" pin="P10_AIN_M1" pad="11"/>
<connect gate="G$1" pin="P11_AIN" pad="12"/>
<connect gate="G$1" pin="P12_AIN" pad="13"/>
<connect gate="G$1" pin="P13_AIN" pad="14"/>
<connect gate="G$1" pin="P14_MPX_AD" pad="15"/>
<connect gate="G$1" pin="P15_ADCOMP" pad="16"/>
<connect gate="G$1" pin="P16_ADFEED" pad="17"/>
<connect gate="G$1" pin="P1_IDENT" pad="28"/>
<connect gate="G$1" pin="P2_IDENT" pad="1"/>
<connect gate="G$1" pin="P3_IDENT" pad="2"/>
<connect gate="G$1" pin="P4_DPM2OUT" pad="3"/>
<connect gate="G$1" pin="P5_AIN_SW" pad="5"/>
<connect gate="G$1" pin="P6_AIN_SW" pad="6"/>
<connect gate="G$1" pin="P7_AIN_SW" pad="7"/>
<connect gate="G$1" pin="P8_AIN_SW" pad="9"/>
<connect gate="G$1" pin="P9_AIN_SW" pad="10"/>
<connect gate="G$1" pin="REF" pad="19"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="RX0" pad="21"/>
<connect gate="G$1" pin="RX1" pad="22"/>
<connect gate="G$1" pin="TX0" pad="25"/>
<connect gate="G$1" pin="TX1" pad="26"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="XMOD" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC08" prefix="IC">
<description>8bit DAC parallel in, without buslogic 70nssettling time, power supply  +- 4,5..18V</description>
<gates>
<gate name="G$1" symbol="DAC08"/>
<gate name="G$2" symbol="VCCVSS"/>
</gates>
<devices>
<device name="SOT16W" package="SO16W">
<connects>
<connect gate="G$1" pin="*IOUT" pad="2"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="B3" pad="7"/>
<connect gate="G$1" pin="B4" pad="8"/>
<connect gate="G$1" pin="B5" pad="9"/>
<connect gate="G$1" pin="B6" pad="10"/>
<connect gate="G$1" pin="B7" pad="11"/>
<connect gate="G$1" pin="B8" pad="12"/>
<connect gate="G$1" pin="COMP" pad="16"/>
<connect gate="G$1" pin="IOUT" pad="4"/>
<connect gate="G$1" pin="VLC" pad="1"/>
<connect gate="G$1" pin="VREF+" pad="14"/>
<connect gate="G$1" pin="VREF-" pad="15"/>
<connect gate="G$2" pin="VCC" pad="3"/>
<connect gate="G$2" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TJA1020">
<description>Lin Transiver  
Vbat 5...27Volt
3,3Volt support no extra supply needed
-&gt;www.lin-subbus.org
-&gt;www.semiconductor.philips.com/pip/tja1020t</description>
<gates>
<gate name="G$1" symbol="TJA1020"/>
</gates>
<devices>
<device name="SO8" package="SOT505-1">
<connects>
<connect gate="G$1" pin="BAT" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="INH" pad="8"/>
<connect gate="G$1" pin="LIN" pad="6"/>
<connect gate="G$1" pin="NSLP" pad="2"/>
<connect gate="G$1" pin="NWAKE" pad="3"/>
<connect gate="G$1" pin="RXD" pad="1"/>
<connect gate="G$1" pin="TXD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA5051">
<gates>
<gate name="TDA5051" symbol="TDA5051"/>
</gates>
<devices>
<device name="" package="SO16W">
<connects>
<connect gate="TDA5051" pin="AGND" pad="12"/>
<connect gate="TDA5051" pin="APGND" pad="9"/>
<connect gate="TDA5051" pin="CLKOUT" pad="4"/>
<connect gate="TDA5051" pin="DATAIN" pad="1"/>
<connect gate="TDA5051" pin="DATAOUT" pad="2"/>
<connect gate="TDA5051" pin="DGND" pad="5"/>
<connect gate="TDA5051" pin="OSC1" pad="7"/>
<connect gate="TDA5051" pin="OSC2" pad="8"/>
<connect gate="TDA5051" pin="PD" pad="15"/>
<connect gate="TDA5051" pin="RXIN" pad="14"/>
<connect gate="TDA5051" pin="SCANTEST" pad="6"/>
<connect gate="TDA5051" pin="TEST1" pad="16"/>
<connect gate="TDA5051" pin="TXOUT" pad="10"/>
<connect gate="TDA5051" pin="VDDA" pad="13"/>
<connect gate="TDA5051" pin="VDDAP" pad="11"/>
<connect gate="TDA5051" pin="VDDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HTRC110" prefix="IC" uservalue="yes">
<description>http://www.nxp.com/documents/data_sheet/ht037030.pdf</description>
<gates>
<gate name="G$1" symbol="HTRC110"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="CEXT" pad="12"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="MOD" pad="5"/>
<connect gate="G$1" pin="NC" pad="11"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="QGND" pad="13"/>
<connect gate="G$1" pin="RX" pad="14"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="TX1" pad="4"/>
<connect gate="G$1" pin="TX2" pad="2"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="XT1" pad="6"/>
<connect gate="G$1" pin="XT2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1308" prefix="IC" uservalue="yes">
<description>Class AB stereo headphone driver</description>
<gates>
<gate name="G$1" symbol="TDA1308"/>
</gates>
<devices>
<device name="" package="SOT505-1">
<connects>
<connect gate="G$1" pin="1_OUTA" pad="1"/>
<connect gate="G$1" pin="2_INA-" pad="2"/>
<connect gate="G$1" pin="3_INA+" pad="3"/>
<connect gate="G$1" pin="4_GND" pad="4"/>
<connect gate="G$1" pin="5_INB+" pad="5"/>
<connect gate="G$1" pin="6_INB-" pad="6"/>
<connect gate="G$1" pin="7_OUTB" pad="7"/>
<connect gate="G$1" pin="8_+VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT96-1" package="SOT96-1">
<connects>
<connect gate="G$1" pin="1_OUTA" pad="1"/>
<connect gate="G$1" pin="2_INA-" pad="2"/>
<connect gate="G$1" pin="3_INA+" pad="3"/>
<connect gate="G$1" pin="4_GND" pad="4"/>
<connect gate="G$1" pin="5_INB+" pad="5"/>
<connect gate="G$1" pin="6_INB-" pad="6"/>
<connect gate="G$1" pin="7_OUTB" pad="7"/>
<connect gate="G$1" pin="8_+VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT97-1" package="SOT97-1">
<connects>
<connect gate="G$1" pin="1_OUTA" pad="1"/>
<connect gate="G$1" pin="2_INA-" pad="2"/>
<connect gate="G$1" pin="3_INA+" pad="3"/>
<connect gate="G$1" pin="4_GND" pad="4"/>
<connect gate="G$1" pin="5_INB+" pad="5"/>
<connect gate="G$1" pin="6_INB-" pad="6"/>
<connect gate="G$1" pin="7_OUTB" pad="7"/>
<connect gate="G$1" pin="8_+VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1541">
<gates>
<gate name="G$1" symbol="TDA1541"/>
</gates>
<devices>
<device name="DIP28" package="DIP28">
<connects>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14_GNDD" pad="14"/>
<connect gate="G$1" pin="P$15_VDD2" pad="15"/>
<connect gate="G$1" pin="P$16_NC" pad="16"/>
<connect gate="G$1" pin="P$17_NC" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$1_WS" pad="1"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25_AOL" pad="25"/>
<connect gate="G$1" pin="P$26_VDD1" pad="26"/>
<connect gate="G$1" pin="P$27_TWC" pad="27"/>
<connect gate="G$1" pin="P$28_VDD" pad="28"/>
<connect gate="G$1" pin="P$2_BCK" pad="2"/>
<connect gate="G$1" pin="P$3_DATA" pad="3"/>
<connect gate="G$1" pin="P$4_SCK" pad="4"/>
<connect gate="G$1" pin="P$5_GNDA" pad="5"/>
<connect gate="G$1" pin="P$6_AOR" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1543">
<gates>
<gate name="G$1" symbol="TDA1543"/>
</gates>
<devices>
<device name="DIP8" package="DIP8">
<connects>
<connect gate="G$1" pin="1_BCK" pad="1"/>
<connect gate="G$1" pin="2_WS" pad="2"/>
<connect gate="G$1" pin="3_DATA" pad="3"/>
<connect gate="G$1" pin="4_GND" pad="4"/>
<connect gate="G$1" pin="5_VDD" pad="5"/>
<connect gate="G$1" pin="6_AOL" pad="6"/>
<connect gate="G$1" pin="7_VRF" pad="7"/>
<connect gate="G$1" pin="8_AOR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1545">
<gates>
<gate name="G$1" symbol="TDA1545"/>
</gates>
<devices>
<device name="SO8" package="SOT505-1">
<connects>
<connect gate="G$1" pin="1_BCK" pad="1"/>
<connect gate="G$1" pin="2_WS" pad="2"/>
<connect gate="G$1" pin="3_DATA" pad="3"/>
<connect gate="G$1" pin="4_GND" pad="4"/>
<connect gate="G$1" pin="5_VDD" pad="5"/>
<connect gate="G$1" pin="6_IOL" pad="6"/>
<connect gate="G$1" pin="7_IREF" pad="7"/>
<connect gate="G$1" pin="8_IOR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1557Q">
<gates>
<gate name="G$1" symbol="TDA1557"/>
</gates>
<devices>
<device name="SIP13" package="SIP13">
<connects>
<connect gate="G$1" pin="10_VP2" pad="10"/>
<connect gate="G$1" pin="11_MUTE" pad="11"/>
<connect gate="G$1" pin="12_NC" pad="12"/>
<connect gate="G$1" pin="13_IN2" pad="13"/>
<connect gate="G$1" pin="1_IN1" pad="1"/>
<connect gate="G$1" pin="2_GNDIN" pad="2"/>
<connect gate="G$1" pin="3_VP1" pad="3"/>
<connect gate="G$1" pin="4_OUT1A" pad="4"/>
<connect gate="G$1" pin="5_GNDPWR" pad="5"/>
<connect gate="G$1" pin="6_OUT1B" pad="6"/>
<connect gate="G$1" pin="7_OUT2A" pad="7"/>
<connect gate="G$1" pin="8_GNDPWR" pad="8"/>
<connect gate="G$1" pin="9_OUT2B" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7021">
<gates>
<gate name="G$1" symbol="TDA7021"/>
</gates>
<devices>
<device name="SO16" package="SO16">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7050">
<gates>
<gate name="G$1" symbol="TDA7050"/>
</gates>
<devices>
<device name="SO8" package="SOT505-1">
<connects>
<connect gate="G$1" pin="1_INA+" pad="1"/>
<connect gate="G$1" pin="2_INA-" pad="2"/>
<connect gate="G$1" pin="3_INB-" pad="3"/>
<connect gate="G$1" pin="4_INB+" pad="4"/>
<connect gate="G$1" pin="5_GND" pad="5"/>
<connect gate="G$1" pin="6_OUTB" pad="6"/>
<connect gate="G$1" pin="7_OUTA" pad="7"/>
<connect gate="G$1" pin="8_VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAB6456" prefix="IC">
<description>&lt;b&gt;Sensitive 1 GHz divide-by-64/divide-by-256 switchable prescaler&lt;/b&gt;&lt;p&gt;
Source: PHILIPS .. SAB6456.pdf</description>
<gates>
<gate name="G$1" symbol="SAB6456"/>
</gates>
<devices>
<device name="T" package="SO08">
<connects>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="3"/>
<connect gate="G$1" pin="MC" pad="5"/>
<connect gate="G$1" pin="QH" pad="6"/>
<connect gate="G$1" pin="QL" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="3"/>
<connect gate="G$1" pin="MC" pad="5"/>
<connect gate="G$1" pin="QH" pad="6"/>
<connect gate="G$1" pin="QL" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8029" prefix="IC">
<description>&lt;b&gt;Low power single card reader&lt;/b&gt;&lt;p&gt;
Source: TDA8029.pdf</description>
<gates>
<gate name="G$1" symbol="TDA8029"/>
</gates>
<devices>
<device name="" package="LQFP32-7X7MM">
<connects>
<connect gate="G$1" pin="!EA" pad="21"/>
<connect gate="G$1" pin="!PSEN" pad="23"/>
<connect gate="G$1" pin="!SDWN" pad="5"/>
<connect gate="G$1" pin="ALE" pad="22"/>
<connect gate="G$1" pin="CDEL" pad="6"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="DCIN" pad="16"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GNDC" pad="9"/>
<connect gate="G$1" pin="I/O" pad="7"/>
<connect gate="G$1" pin="P16" pad="2"/>
<connect gate="G$1" pin="P17" pad="1"/>
<connect gate="G$1" pin="P26" pad="25"/>
<connect gate="G$1" pin="P27" pad="24"/>
<connect gate="G$1" pin="P30/RX" pad="32"/>
<connect gate="G$1" pin="P31/TX" pad="31"/>
<connect gate="G$1" pin="P32/!INT0" pad="29"/>
<connect gate="G$1" pin="P33/!INT1" pad="30"/>
<connect gate="G$1" pin="PGND" pad="18"/>
<connect gate="G$1" pin="PRES" pad="8"/>
<connect gate="G$1" pin="RESET" pad="28"/>
<connect gate="G$1" pin="RST" pad="12"/>
<connect gate="G$1" pin="SAM" pad="19"/>
<connect gate="G$1" pin="SAP" pad="14"/>
<connect gate="G$1" pin="SBM" pad="17"/>
<connect gate="G$1" pin="SBP" pad="15"/>
<connect gate="G$1" pin="TEST" pad="20"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VUP" pad="13"/>
<connect gate="G$1" pin="XTAL1" pad="26"/>
<connect gate="G$1" pin="XTAL2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TDA8029HL/C207,118"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R9255"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA5767/68" prefix="IC" uservalue="yes">
<description>Philips Semiconductors’ digitally tuned TEA5767/68 FM stereo
receiver IC is based on an innovative architecture concept that
simplifies radio design, significantly reducing the number of external
components. Delivering the highest performance levels, this one-chip
radio solution occupies minimal PCB area (9x9 mm) making it ideal
for all space-critical and low voltage applications such as mobile
phones and MP3 players.</description>
<gates>
<gate name="G$1" symbol="TEA5767"/>
</gates>
<devices>
<device name="" package="TEA5767">
<connects>
<connect gate="G$1" pin="ANT" pad="10"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="DAT" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND2" pad="6"/>
<connect gate="G$1" pin="GND3" pad="9"/>
<connect gate="G$1" pin="LOUT" pad="7"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="ROUT" pad="8"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8*" prefix="IC">
<description>&lt;b&gt;CMOS single-chip 8-bit Microcontroller&lt;/b&gt;&lt;p&gt;
80C31/32 pin compatible</description>
<gates>
<gate name="G$1" symbol="80C52DIL40"/>
</gates>
<devices>
<device name="PN" package="DIL40">
<connects>
<connect gate="G$1" pin="!EA" pad="31"/>
<connect gate="G$1" pin="!PSEN" pad="29"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="P00" pad="39"/>
<connect gate="G$1" pin="P01" pad="38"/>
<connect gate="G$1" pin="P02" pad="37"/>
<connect gate="G$1" pin="P03" pad="36"/>
<connect gate="G$1" pin="P04" pad="35"/>
<connect gate="G$1" pin="P05" pad="34"/>
<connect gate="G$1" pin="P06" pad="33"/>
<connect gate="G$1" pin="P07" pad="32"/>
<connect gate="G$1" pin="P10" pad="1"/>
<connect gate="G$1" pin="P11" pad="2"/>
<connect gate="G$1" pin="P12" pad="3"/>
<connect gate="G$1" pin="P13" pad="4"/>
<connect gate="G$1" pin="P14" pad="5"/>
<connect gate="G$1" pin="P15" pad="6"/>
<connect gate="G$1" pin="P16" pad="7"/>
<connect gate="G$1" pin="P17" pad="8"/>
<connect gate="G$1" pin="P20" pad="21"/>
<connect gate="G$1" pin="P21" pad="22"/>
<connect gate="G$1" pin="P22" pad="23"/>
<connect gate="G$1" pin="P23" pad="24"/>
<connect gate="G$1" pin="P24" pad="25"/>
<connect gate="G$1" pin="P25" pad="26"/>
<connect gate="G$1" pin="P26" pad="27"/>
<connect gate="G$1" pin="P27" pad="28"/>
<connect gate="G$1" pin="P30" pad="10"/>
<connect gate="G$1" pin="P31" pad="11"/>
<connect gate="G$1" pin="P32" pad="12"/>
<connect gate="G$1" pin="P33" pad="13"/>
<connect gate="G$1" pin="P34" pad="14"/>
<connect gate="G$1" pin="P35" pad="15"/>
<connect gate="G$1" pin="P36" pad="16"/>
<connect gate="G$1" pin="P37" pad="17"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VDD" pad="40"/>
<connect gate="G$1" pin="VSS" pad="20"/>
<connect gate="G$1" pin="X1" pad="19"/>
<connect gate="G$1" pin="X2" pad="18"/>
</connects>
<technologies>
<technology name="0C31SB"/>
<technology name="0C31SF"/>
<technology name="0C32SB"/>
<technology name="0C32SF"/>
<technology name="0C32UB"/>
<technology name="0C32UF"/>
<technology name="0C652"/>
<technology name="3C652"/>
</technologies>
</device>
<device name="AA" package="PLCC44S">
<connects>
<connect gate="G$1" pin="!EA" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="32"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="P00" pad="43"/>
<connect gate="G$1" pin="P01" pad="42"/>
<connect gate="G$1" pin="P02" pad="41"/>
<connect gate="G$1" pin="P03" pad="40"/>
<connect gate="G$1" pin="P04" pad="39"/>
<connect gate="G$1" pin="P05" pad="38"/>
<connect gate="G$1" pin="P06" pad="37"/>
<connect gate="G$1" pin="P07" pad="36"/>
<connect gate="G$1" pin="P10" pad="2"/>
<connect gate="G$1" pin="P11" pad="3"/>
<connect gate="G$1" pin="P12" pad="4"/>
<connect gate="G$1" pin="P13" pad="5"/>
<connect gate="G$1" pin="P14" pad="6"/>
<connect gate="G$1" pin="P15" pad="7"/>
<connect gate="G$1" pin="P16" pad="8"/>
<connect gate="G$1" pin="P17" pad="9"/>
<connect gate="G$1" pin="P20" pad="24"/>
<connect gate="G$1" pin="P21" pad="25"/>
<connect gate="G$1" pin="P22" pad="26"/>
<connect gate="G$1" pin="P23" pad="27"/>
<connect gate="G$1" pin="P24" pad="28"/>
<connect gate="G$1" pin="P25" pad="29"/>
<connect gate="G$1" pin="P26" pad="30"/>
<connect gate="G$1" pin="P27" pad="31"/>
<connect gate="G$1" pin="P30" pad="11"/>
<connect gate="G$1" pin="P31" pad="13"/>
<connect gate="G$1" pin="P32" pad="14"/>
<connect gate="G$1" pin="P33" pad="15"/>
<connect gate="G$1" pin="P34" pad="16"/>
<connect gate="G$1" pin="P35" pad="17"/>
<connect gate="G$1" pin="P36" pad="18"/>
<connect gate="G$1" pin="P37" pad="19"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VDD" pad="44"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="X1" pad="21"/>
<connect gate="G$1" pin="X2" pad="20"/>
</connects>
<technologies>
<technology name="0C31SB"/>
<technology name="0C31SF"/>
<technology name="0C32SB"/>
<technology name="0C32SF"/>
<technology name="0C32UB"/>
<technology name="0C32UF"/>
</technologies>
</device>
<device name="BB" package="QFP44_SOT307-2">
<connects>
<connect gate="G$1" pin="!EA" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="P00" pad="37"/>
<connect gate="G$1" pin="P01" pad="36"/>
<connect gate="G$1" pin="P02" pad="35"/>
<connect gate="G$1" pin="P03" pad="34"/>
<connect gate="G$1" pin="P04" pad="33"/>
<connect gate="G$1" pin="P05" pad="32"/>
<connect gate="G$1" pin="P06" pad="31"/>
<connect gate="G$1" pin="P07" pad="30"/>
<connect gate="G$1" pin="P10" pad="40"/>
<connect gate="G$1" pin="P11" pad="41"/>
<connect gate="G$1" pin="P12" pad="42"/>
<connect gate="G$1" pin="P13" pad="43"/>
<connect gate="G$1" pin="P14" pad="44"/>
<connect gate="G$1" pin="P15" pad="1"/>
<connect gate="G$1" pin="P16" pad="2"/>
<connect gate="G$1" pin="P17" pad="3"/>
<connect gate="G$1" pin="P20" pad="18"/>
<connect gate="G$1" pin="P21" pad="19"/>
<connect gate="G$1" pin="P22" pad="20"/>
<connect gate="G$1" pin="P23" pad="21"/>
<connect gate="G$1" pin="P24" pad="22"/>
<connect gate="G$1" pin="P25" pad="23"/>
<connect gate="G$1" pin="P26" pad="24"/>
<connect gate="G$1" pin="P27" pad="25"/>
<connect gate="G$1" pin="P30" pad="5"/>
<connect gate="G$1" pin="P31" pad="7"/>
<connect gate="G$1" pin="P32" pad="8"/>
<connect gate="G$1" pin="P33" pad="9"/>
<connect gate="G$1" pin="P34" pad="10"/>
<connect gate="G$1" pin="P35" pad="11"/>
<connect gate="G$1" pin="P36" pad="12"/>
<connect gate="G$1" pin="P37" pad="13"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VDD" pad="38"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="X1" pad="15"/>
<connect gate="G$1" pin="X2" pad="14"/>
</connects>
<technologies>
<technology name="0C31SB"/>
<technology name="0C31SF"/>
<technology name="0C32SB"/>
<technology name="0C32SF"/>
<technology name="0C32UB"/>
<technology name="0C32UF"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8*C652-QFP44" prefix="IC">
<description>&lt;b&gt;CMOS single-chip 8-bit Microcontroller&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C52"/>
</gates>
<devices>
<device name="" package="QFP44_SOT307-2">
<connects>
<connect gate="G$1" pin="!EA" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="NC" pad="17"/>
<connect gate="G$1" pin="P00" pad="37"/>
<connect gate="G$1" pin="P01" pad="36"/>
<connect gate="G$1" pin="P02" pad="35"/>
<connect gate="G$1" pin="P03" pad="34"/>
<connect gate="G$1" pin="P04" pad="33"/>
<connect gate="G$1" pin="P05" pad="32"/>
<connect gate="G$1" pin="P06" pad="31"/>
<connect gate="G$1" pin="P07" pad="30"/>
<connect gate="G$1" pin="P10" pad="40"/>
<connect gate="G$1" pin="P11" pad="41"/>
<connect gate="G$1" pin="P12" pad="42"/>
<connect gate="G$1" pin="P13" pad="43"/>
<connect gate="G$1" pin="P14" pad="44"/>
<connect gate="G$1" pin="P15" pad="1"/>
<connect gate="G$1" pin="P16" pad="2"/>
<connect gate="G$1" pin="P17" pad="3"/>
<connect gate="G$1" pin="P20" pad="18"/>
<connect gate="G$1" pin="P21" pad="19"/>
<connect gate="G$1" pin="P22" pad="20"/>
<connect gate="G$1" pin="P23" pad="21"/>
<connect gate="G$1" pin="P24" pad="22"/>
<connect gate="G$1" pin="P25" pad="23"/>
<connect gate="G$1" pin="P26" pad="24"/>
<connect gate="G$1" pin="P27" pad="25"/>
<connect gate="G$1" pin="P30" pad="5"/>
<connect gate="G$1" pin="P31" pad="7"/>
<connect gate="G$1" pin="P32" pad="8"/>
<connect gate="G$1" pin="P33" pad="9"/>
<connect gate="G$1" pin="P34" pad="10"/>
<connect gate="G$1" pin="P35" pad="11"/>
<connect gate="G$1" pin="P36" pad="12"/>
<connect gate="G$1" pin="P37" pad="13"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VDD" pad="38"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="VSS@1" pad="39"/>
<connect gate="G$1" pin="VSS@2" pad="28"/>
<connect gate="G$1" pin="VSS@3" pad="6"/>
<connect gate="G$1" pin="X1" pad="15"/>
<connect gate="G$1" pin="X2" pad="14"/>
</connects>
<technologies>
<technology name="0"/>
<technology name="3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8*CE598" prefix="IC" uservalue="yes">
<description>&lt;b&gt;8bit 8051 Microcontroller, CAN 2.0A&lt;/b&gt;&lt;p&gt;
 Without ROM P80CE598FFB/P80CE598FHB&lt;p&gt;
 With ROM P83CE598FFB/P83CE598FHB</description>
<gates>
<gate name="G" symbol="8XC598"/>
<gate name="P" symbol="PWR5"/>
<gate name="C" symbol="PWRC"/>
<gate name="N" symbol="NC5"/>
</gates>
<devices>
<device name="FP" package="QFP80">
<connects>
<connect gate="C" pin="CGND" pad="37"/>
<connect gate="C" pin="CVCC" pad="40"/>
<connect gate="G" pin="/EW" pad="18"/>
<connect gate="G" pin="ALE" pad="64"/>
<connect gate="G" pin="CRX0" pad="80"/>
<connect gate="G" pin="CRX1" pad="79"/>
<connect gate="G" pin="CTX0" pad="38"/>
<connect gate="G" pin="CTX1" pad="39"/>
<connect gate="G" pin="EA" pad="65"/>
<connect gate="G" pin="INT2" pad="31"/>
<connect gate="G" pin="INT3" pad="32"/>
<connect gate="G" pin="INT4" pad="33"/>
<connect gate="G" pin="INT5" pad="34"/>
<connect gate="G" pin="P0.0/D0" pad="75"/>
<connect gate="G" pin="P0.1/D1" pad="74"/>
<connect gate="G" pin="P0.2/D2" pad="73"/>
<connect gate="G" pin="P0.3/D3" pad="72"/>
<connect gate="G" pin="P0.4/D4" pad="71"/>
<connect gate="G" pin="P0.5/D5" pad="70"/>
<connect gate="G" pin="P0.6/D6" pad="69"/>
<connect gate="G" pin="P0.7/D7" pad="68"/>
<connect gate="G" pin="P2.0/A8" pad="55"/>
<connect gate="G" pin="P2.1/A9" pad="56"/>
<connect gate="G" pin="P2.2/A10" pad="57"/>
<connect gate="G" pin="P2.3/A11" pad="58"/>
<connect gate="G" pin="P2.4/A12" pad="59"/>
<connect gate="G" pin="P2.5/A13" pad="60"/>
<connect gate="G" pin="P2.6/A14" pad="61"/>
<connect gate="G" pin="P2.7/A15" pad="62"/>
<connect gate="G" pin="P3.0" pad="41"/>
<connect gate="G" pin="P3.1" pad="42"/>
<connect gate="G" pin="P3.2" pad="43"/>
<connect gate="G" pin="P3.3" pad="44"/>
<connect gate="G" pin="P3.4/T0" pad="45"/>
<connect gate="G" pin="P3.5/T1" pad="46"/>
<connect gate="G" pin="P3.6/WR" pad="47"/>
<connect gate="G" pin="P3.7/RD" pad="48"/>
<connect gate="G" pin="P4.0" pad="19"/>
<connect gate="G" pin="P4.1" pad="20"/>
<connect gate="G" pin="P4.2" pad="21"/>
<connect gate="G" pin="P4.3" pad="22"/>
<connect gate="G" pin="P4.4" pad="24"/>
<connect gate="G" pin="P4.5" pad="25"/>
<connect gate="G" pin="P4.6" pad="26"/>
<connect gate="G" pin="P4.7" pad="27"/>
<connect gate="G" pin="P5.0/AN0" pad="12"/>
<connect gate="G" pin="P5.1/AN1" pad="11"/>
<connect gate="G" pin="P5.2/AN2" pad="10"/>
<connect gate="G" pin="P5.3/AN3" pad="9"/>
<connect gate="G" pin="P5.4/AN4" pad="8"/>
<connect gate="G" pin="P5.5/AN5" pad="7"/>
<connect gate="G" pin="P5.6/AN6" pad="6"/>
<connect gate="G" pin="P5.7/AN7" pad="5"/>
<connect gate="G" pin="PSEN" pad="63"/>
<connect gate="G" pin="PWM0" pad="16"/>
<connect gate="G" pin="PWM1" pad="17"/>
<connect gate="G" pin="REF" pad="78"/>
<connect gate="G" pin="RST" pad="30"/>
<connect gate="G" pin="RT2" pad="36"/>
<connect gate="G" pin="STADC" pad="15"/>
<connect gate="G" pin="T2" pad="35"/>
<connect gate="G" pin="VAGND" pad="1"/>
<connect gate="G" pin="VAREF" pad="2"/>
<connect gate="G" pin="XTAL1" pad="52"/>
<connect gate="G" pin="XTAL2" pad="51"/>
<connect gate="N" pin="NC@0" pad="23"/>
<connect gate="N" pin="NC@1" pad="49"/>
<connect gate="N" pin="NC@2" pad="50"/>
<connect gate="N" pin="NC@3" pad="66"/>
<connect gate="N" pin="NC@4" pad="67"/>
<connect gate="P" pin="GND@0" pad="13"/>
<connect gate="P" pin="GND@1" pad="29"/>
<connect gate="P" pin="GND@2" pad="54"/>
<connect gate="P" pin="GND@3" pad="77"/>
<connect gate="P" pin="GND@4" pad="3"/>
<connect gate="P" pin="VCC@0" pad="14"/>
<connect gate="P" pin="VCC@1" pad="28"/>
<connect gate="P" pin="VCC@2" pad="53"/>
<connect gate="P" pin="VCC@3" pad="76"/>
<connect gate="P" pin="VCC@4" pad="4"/>
</connects>
<technologies>
<technology name="0"/>
<technology name="3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C576" prefix="IC" uservalue="yes">
<description>&lt;b&gt;8051 -compatible 8-bit Microcontroller&lt;p&gt;</description>
<gates>
<gate name="P" symbol="PWR2"/>
<gate name="A" symbol="PWRA"/>
<gate name="G" symbol="8XC576"/>
</gates>
<devices>
<device name="SMD" package="PLCC44">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="AVCC" pad="2"/>
<connect gate="G" pin="ALE" pad="33"/>
<connect gate="G" pin="EA" pad="35"/>
<connect gate="G" pin="NC@0" pad="1"/>
<connect gate="G" pin="NC@1" pad="12"/>
<connect gate="G" pin="NC@2" pad="23"/>
<connect gate="G" pin="NC@3" pad="34"/>
<connect gate="G" pin="P0.0/D0" pad="43"/>
<connect gate="G" pin="P0.1/D1" pad="42"/>
<connect gate="G" pin="P0.2/D2" pad="41"/>
<connect gate="G" pin="P0.3/D3" pad="40"/>
<connect gate="G" pin="P0.4/D4" pad="39"/>
<connect gate="G" pin="P0.5/D5" pad="38"/>
<connect gate="G" pin="P0.6/D6" pad="37"/>
<connect gate="G" pin="P0.7/D7" pad="36"/>
<connect gate="G" pin="P1.0" pad="4"/>
<connect gate="G" pin="P1.1" pad="5"/>
<connect gate="G" pin="P1.2" pad="6"/>
<connect gate="G" pin="P1.3" pad="7"/>
<connect gate="G" pin="P1.4" pad="8"/>
<connect gate="G" pin="P1.5" pad="9"/>
<connect gate="G" pin="P2.0/A8" pad="24"/>
<connect gate="G" pin="P2.1/A9" pad="25"/>
<connect gate="G" pin="P2.2/A10" pad="26"/>
<connect gate="G" pin="P2.3/A11" pad="27"/>
<connect gate="G" pin="P2.4/A12" pad="28"/>
<connect gate="G" pin="P2.5/A13" pad="29"/>
<connect gate="G" pin="P2.6/A14" pad="30"/>
<connect gate="G" pin="P2.7/A15" pad="31"/>
<connect gate="G" pin="P3.0" pad="11"/>
<connect gate="G" pin="P3.1" pad="13"/>
<connect gate="G" pin="P3.2" pad="14"/>
<connect gate="G" pin="P3.3" pad="15"/>
<connect gate="G" pin="P3.4/T0" pad="16"/>
<connect gate="G" pin="P3.5/T1" pad="17"/>
<connect gate="G" pin="P3.6/WR" pad="18"/>
<connect gate="G" pin="P3.7/RD" pad="19"/>
<connect gate="G" pin="PSEN" pad="32"/>
<connect gate="G" pin="RST" pad="10"/>
<connect gate="G" pin="XTAL1" pad="21"/>
<connect gate="G" pin="XTAL2" pad="20"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="VCC" pad="44"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="PLCC44S">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="AVCC" pad="2"/>
<connect gate="G" pin="ALE" pad="33"/>
<connect gate="G" pin="EA" pad="35"/>
<connect gate="G" pin="NC@0" pad="1"/>
<connect gate="G" pin="NC@1" pad="12"/>
<connect gate="G" pin="NC@2" pad="23"/>
<connect gate="G" pin="NC@3" pad="34"/>
<connect gate="G" pin="P0.0/D0" pad="43"/>
<connect gate="G" pin="P0.1/D1" pad="42"/>
<connect gate="G" pin="P0.2/D2" pad="41"/>
<connect gate="G" pin="P0.3/D3" pad="40"/>
<connect gate="G" pin="P0.4/D4" pad="39"/>
<connect gate="G" pin="P0.5/D5" pad="38"/>
<connect gate="G" pin="P0.6/D6" pad="37"/>
<connect gate="G" pin="P0.7/D7" pad="36"/>
<connect gate="G" pin="P1.0" pad="4"/>
<connect gate="G" pin="P1.1" pad="5"/>
<connect gate="G" pin="P1.2" pad="6"/>
<connect gate="G" pin="P1.3" pad="7"/>
<connect gate="G" pin="P1.4" pad="8"/>
<connect gate="G" pin="P1.5" pad="9"/>
<connect gate="G" pin="P2.0/A8" pad="24"/>
<connect gate="G" pin="P2.1/A9" pad="25"/>
<connect gate="G" pin="P2.2/A10" pad="26"/>
<connect gate="G" pin="P2.3/A11" pad="27"/>
<connect gate="G" pin="P2.4/A12" pad="28"/>
<connect gate="G" pin="P2.5/A13" pad="29"/>
<connect gate="G" pin="P2.6/A14" pad="30"/>
<connect gate="G" pin="P2.7/A15" pad="31"/>
<connect gate="G" pin="P3.0" pad="11"/>
<connect gate="G" pin="P3.1" pad="13"/>
<connect gate="G" pin="P3.2" pad="14"/>
<connect gate="G" pin="P3.3" pad="15"/>
<connect gate="G" pin="P3.4/T0" pad="16"/>
<connect gate="G" pin="P3.5/T1" pad="17"/>
<connect gate="G" pin="P3.6/WR" pad="18"/>
<connect gate="G" pin="P3.7/RD" pad="19"/>
<connect gate="G" pin="PSEN" pad="32"/>
<connect gate="G" pin="RST" pad="10"/>
<connect gate="G" pin="XTAL1" pad="21"/>
<connect gate="G" pin="XTAL2" pad="20"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="VCC" pad="44"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82B715" prefix="IC" uservalue="yes">
<description>&lt;b&gt;I2C bus extender&lt;/b&gt;</description>
<gates>
<gate name="G" symbol="82B715"/>
<gate name="P" symbol="PWR2"/>
<gate name="NC" symbol="NC2"/>
</gates>
<devices>
<device name="TD" package="SO8">
<connects>
<connect gate="G" pin="LX" pad="2"/>
<connect gate="G" pin="LY" pad="7"/>
<connect gate="G" pin="SX" pad="3"/>
<connect gate="G" pin="SY" pad="6"/>
<connect gate="NC" pin="NC@0" pad="5"/>
<connect gate="NC" pin="NC@1" pad="1"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="87C748" prefix="IC" uservalue="yes">
<description>&lt;b&gt;8051 -comabtible 8bit Microcontroller&lt;/b&gt;</description>
<gates>
<gate name="G" symbol="8XC748"/>
<gate name="P" symbol="PWR2"/>
</gates>
<devices>
<device name="" package="DIP24SKI">
<connects>
<connect gate="G" pin="A0" pad="5"/>
<connect gate="G" pin="A1" pad="4"/>
<connect gate="G" pin="A2" pad="3"/>
<connect gate="G" pin="A3" pad="2"/>
<connect gate="G" pin="A4" pad="1"/>
<connect gate="G" pin="A5" pad="23"/>
<connect gate="G" pin="A6" pad="22"/>
<connect gate="G" pin="A7" pad="21"/>
<connect gate="G" pin="ASEL" pad="8"/>
<connect gate="G" pin="D0" pad="13"/>
<connect gate="G" pin="D1" pad="14"/>
<connect gate="G" pin="D2" pad="15"/>
<connect gate="G" pin="D3" pad="16"/>
<connect gate="G" pin="D4" pad="17"/>
<connect gate="G" pin="D5" pad="18"/>
<connect gate="G" pin="D6" pad="19"/>
<connect gate="G" pin="D7" pad="20"/>
<connect gate="G" pin="OE-PGM" pad="7"/>
<connect gate="G" pin="RESET" pad="9"/>
<connect gate="G" pin="VPP" pad="6"/>
<connect gate="G" pin="X1" pad="11"/>
<connect gate="G" pin="X2" pad="10"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="87C751" prefix="IC" uservalue="yes">
<description>&lt;b&gt;83C751/87C751 80C51 with  I2C bus, 8-bit Microcontroller&lt;/b&gt;&lt;p&gt;
2K/64 OTP/ROM</description>
<gates>
<gate name="G" symbol="8XC751"/>
<gate name="P" symbol="PWR2"/>
</gates>
<devices>
<device name="" package="DIP24SKI">
<connects>
<connect gate="G" pin="A0" pad="5"/>
<connect gate="G" pin="A1" pad="4"/>
<connect gate="G" pin="A2" pad="3"/>
<connect gate="G" pin="A3" pad="2"/>
<connect gate="G" pin="A4" pad="1"/>
<connect gate="G" pin="A5" pad="23"/>
<connect gate="G" pin="A6" pad="22"/>
<connect gate="G" pin="A7" pad="21"/>
<connect gate="G" pin="D0" pad="13"/>
<connect gate="G" pin="D1" pad="14"/>
<connect gate="G" pin="D2" pad="15"/>
<connect gate="G" pin="D3" pad="16"/>
<connect gate="G" pin="D4" pad="17"/>
<connect gate="G" pin="D5" pad="18"/>
<connect gate="G" pin="D6" pad="19"/>
<connect gate="G" pin="D7" pad="20"/>
<connect gate="G" pin="RST" pad="9"/>
<connect gate="G" pin="SCL" pad="8"/>
<connect gate="G" pin="SDA" pad="7"/>
<connect gate="G" pin="VPP" pad="6"/>
<connect gate="G" pin="XTAL1" pad="11"/>
<connect gate="G" pin="XTAL2" pad="10"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P82C150" prefix="IC">
<description>CAN BUS &lt;b&gt;I/O DEVICE&lt;/b&gt;, SLIO&lt;p&gt;
with digital and analog port functions</description>
<gates>
<gate name="G$1" symbol="P82C150"/>
</gates>
<devices>
<device name="" package="SO28">
<connects>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="CLK/P0" pad="27"/>
<connect gate="G$1" pin="P1" pad="28"/>
<connect gate="G$1" pin="P10" pad="11"/>
<connect gate="G$1" pin="P11" pad="12"/>
<connect gate="G$1" pin="P12" pad="13"/>
<connect gate="G$1" pin="P13" pad="14"/>
<connect gate="G$1" pin="P14" pad="15"/>
<connect gate="G$1" pin="P15" pad="16"/>
<connect gate="G$1" pin="P16" pad="17"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="P3" pad="2"/>
<connect gate="G$1" pin="P4" pad="3"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
<connect gate="G$1" pin="P7" pad="7"/>
<connect gate="G$1" pin="P8" pad="9"/>
<connect gate="G$1" pin="P9" pad="10"/>
<connect gate="G$1" pin="REF" pad="19"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="RX0" pad="21"/>
<connect gate="G$1" pin="RX1" pad="22"/>
<connect gate="G$1" pin="TX0" pad="25"/>
<connect gate="G$1" pin="TX1" pad="26"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="XMOD" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P98LPC935" prefix="IC">
<description>&lt;b&gt;8-bit microcontroller with accelerated two-clock core&lt;/b&gt;&lt;p&gt;
4 KB/ 8 KB/ 8 KB 3 V byte-erasable Flash with 8-bit A/D converter&lt;br&gt;
Source: http://www.nxp.com .. UM_P89LPC933_934_935_1.pdf</description>
<gates>
<gate name="G$1" symbol="P98LPC935"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!INT1/P1.4" pad="10"/>
<connect gate="G$1" pin="!RST/P1.5" pad="6"/>
<connect gate="G$1" pin="AD00/P1.7" pad="4"/>
<connect gate="G$1" pin="AD01/P2.0" pad="3"/>
<connect gate="G$1" pin="AD02/P2.1" pad="2"/>
<connect gate="G$1" pin="AD03/DAC0/P2.0" pad="1"/>
<connect gate="G$1" pin="CLKOUT/XTAL2/P3.0" pad="9"/>
<connect gate="G$1" pin="MISO/P2.3" pad="14"/>
<connect gate="G$1" pin="MOSI/P2.2" pad="13"/>
<connect gate="G$1" pin="OCB/P1.6" pad="5"/>
<connect gate="G$1" pin="P0.1/CIN2B/AD10" pad="26"/>
<connect gate="G$1" pin="P0.2/CIN2A/AD11" pad="25"/>
<connect gate="G$1" pin="P0.3/CIN1B/AD12" pad="24"/>
<connect gate="G$1" pin="P0.4/CIN1A/DAC1/AD13" pad="23"/>
<connect gate="G$1" pin="P0.5/CMPREF" pad="22"/>
<connect gate="G$1" pin="P0.6/CMP1" pad="20"/>
<connect gate="G$1" pin="P0.7/T1" pad="19"/>
<connect gate="G$1" pin="P1.0/TXD" pad="18"/>
<connect gate="G$1" pin="P1.1/RXD" pad="17"/>
<connect gate="G$1" pin="P2.4/!SS" pad="15"/>
<connect gate="G$1" pin="P2.5/SPICLK" pad="16"/>
<connect gate="G$1" pin="P2.6/OCA" pad="27"/>
<connect gate="G$1" pin="P2.7/ICA" pad="28"/>
<connect gate="G$1" pin="SCL/T0/P1.2" pad="12"/>
<connect gate="G$1" pin="SDA/!INT0/P1.2" pad="11"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="XTAL1/P3.1" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="PLCC28S">
<connects>
<connect gate="G$1" pin="!INT1/P1.4" pad="10"/>
<connect gate="G$1" pin="!RST/P1.5" pad="6"/>
<connect gate="G$1" pin="AD00/P1.7" pad="4"/>
<connect gate="G$1" pin="AD01/P2.0" pad="3"/>
<connect gate="G$1" pin="AD02/P2.1" pad="2"/>
<connect gate="G$1" pin="AD03/DAC0/P2.0" pad="1"/>
<connect gate="G$1" pin="CLKOUT/XTAL2/P3.0" pad="9"/>
<connect gate="G$1" pin="MISO/P2.3" pad="14"/>
<connect gate="G$1" pin="MOSI/P2.2" pad="13"/>
<connect gate="G$1" pin="OCB/P1.6" pad="5"/>
<connect gate="G$1" pin="P0.1/CIN2B/AD10" pad="26"/>
<connect gate="G$1" pin="P0.2/CIN2A/AD11" pad="25"/>
<connect gate="G$1" pin="P0.3/CIN1B/AD12" pad="24"/>
<connect gate="G$1" pin="P0.4/CIN1A/DAC1/AD13" pad="23"/>
<connect gate="G$1" pin="P0.5/CMPREF" pad="22"/>
<connect gate="G$1" pin="P0.6/CMP1" pad="20"/>
<connect gate="G$1" pin="P0.7/T1" pad="19"/>
<connect gate="G$1" pin="P1.0/TXD" pad="18"/>
<connect gate="G$1" pin="P1.1/RXD" pad="17"/>
<connect gate="G$1" pin="P2.4/!SS" pad="15"/>
<connect gate="G$1" pin="P2.5/SPICLK" pad="16"/>
<connect gate="G$1" pin="P2.6/OCA" pad="27"/>
<connect gate="G$1" pin="P2.7/ICA" pad="28"/>
<connect gate="G$1" pin="SCL/T0/P1.2" pad="12"/>
<connect gate="G$1" pin="SDA/!INT0/P1.2" pad="11"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="XTAL1/P3.1" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="HVQFN28">
<connects>
<connect gate="G$1" pin="!INT1/P1.4" pad="6"/>
<connect gate="G$1" pin="!RST/P1.5" pad="2"/>
<connect gate="G$1" pin="AD00/P1.7" pad="28"/>
<connect gate="G$1" pin="AD01/P2.0" pad="27"/>
<connect gate="G$1" pin="AD02/P2.1" pad="26"/>
<connect gate="G$1" pin="AD03/DAC0/P2.0" pad="25"/>
<connect gate="G$1" pin="CLKOUT/XTAL2/P3.0" pad="5"/>
<connect gate="G$1" pin="MISO/P2.3" pad="10"/>
<connect gate="G$1" pin="MOSI/P2.2" pad="9"/>
<connect gate="G$1" pin="OCB/P1.6" pad="1"/>
<connect gate="G$1" pin="P0.1/CIN2B/AD10" pad="22"/>
<connect gate="G$1" pin="P0.2/CIN2A/AD11" pad="21"/>
<connect gate="G$1" pin="P0.3/CIN1B/AD12" pad="20"/>
<connect gate="G$1" pin="P0.4/CIN1A/DAC1/AD13" pad="19"/>
<connect gate="G$1" pin="P0.5/CMPREF" pad="18"/>
<connect gate="G$1" pin="P0.6/CMP1" pad="16"/>
<connect gate="G$1" pin="P0.7/T1" pad="15"/>
<connect gate="G$1" pin="P1.0/TXD" pad="14"/>
<connect gate="G$1" pin="P1.1/RXD" pad="13"/>
<connect gate="G$1" pin="P2.4/!SS" pad="11"/>
<connect gate="G$1" pin="P2.5/SPICLK" pad="12"/>
<connect gate="G$1" pin="P2.6/OCA" pad="23"/>
<connect gate="G$1" pin="P2.7/ICA" pad="24"/>
<connect gate="G$1" pin="SCL/T0/P1.2" pad="8"/>
<connect gate="G$1" pin="SDA/!INT0/P1.2" pad="7"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VSS" pad="3"/>
<connect gate="G$1" pin="XTAL1/P3.1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA82C250" prefix="IC">
<description>&lt;b&gt;CAN CONTROLLER INTERFACE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="P82C250"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9555" prefix="IC">
<description>&lt;b&gt;16-bit I2C and SMBus I/O port with interrupt&lt;/b&gt;&lt;p&gt;
Source: PCA9555_5.pdf</description>
<gates>
<gate name="G$1" symbol="PCA9555"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="I/O0.0" pad="4"/>
<connect gate="G$1" pin="I/O0.1" pad="5"/>
<connect gate="G$1" pin="I/O0.2" pad="6"/>
<connect gate="G$1" pin="I/O0.3" pad="7"/>
<connect gate="G$1" pin="I/O0.4" pad="8"/>
<connect gate="G$1" pin="I/O0.5" pad="9"/>
<connect gate="G$1" pin="I/O0.6" pad="10"/>
<connect gate="G$1" pin="I/O0.7" pad="11"/>
<connect gate="G$1" pin="I/O1.0" pad="13"/>
<connect gate="G$1" pin="I/O1.1" pad="14"/>
<connect gate="G$1" pin="I/O1.2" pad="15"/>
<connect gate="G$1" pin="I/O1.3" pad="16"/>
<connect gate="G$1" pin="I/O1.4" pad="17"/>
<connect gate="G$1" pin="I/O1.5" pad="18"/>
<connect gate="G$1" pin="I/O1.6" pad="19"/>
<connect gate="G$1" pin="I/O1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="I/O0.0" pad="4"/>
<connect gate="G$1" pin="I/O0.1" pad="5"/>
<connect gate="G$1" pin="I/O0.2" pad="6"/>
<connect gate="G$1" pin="I/O0.3" pad="7"/>
<connect gate="G$1" pin="I/O0.4" pad="8"/>
<connect gate="G$1" pin="I/O0.5" pad="9"/>
<connect gate="G$1" pin="I/O0.6" pad="10"/>
<connect gate="G$1" pin="I/O0.7" pad="11"/>
<connect gate="G$1" pin="I/O1.0" pad="13"/>
<connect gate="G$1" pin="I/O1.1" pad="14"/>
<connect gate="G$1" pin="I/O1.2" pad="15"/>
<connect gate="G$1" pin="I/O1.3" pad="16"/>
<connect gate="G$1" pin="I/O1.4" pad="17"/>
<connect gate="G$1" pin="I/O1.5" pad="18"/>
<connect gate="G$1" pin="I/O1.6" pad="19"/>
<connect gate="G$1" pin="I/O1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DB" package="SSOP24">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="I/O0.0" pad="4"/>
<connect gate="G$1" pin="I/O0.1" pad="5"/>
<connect gate="G$1" pin="I/O0.2" pad="6"/>
<connect gate="G$1" pin="I/O0.3" pad="7"/>
<connect gate="G$1" pin="I/O0.4" pad="8"/>
<connect gate="G$1" pin="I/O0.5" pad="9"/>
<connect gate="G$1" pin="I/O0.6" pad="10"/>
<connect gate="G$1" pin="I/O0.7" pad="11"/>
<connect gate="G$1" pin="I/O1.0" pad="13"/>
<connect gate="G$1" pin="I/O1.1" pad="14"/>
<connect gate="G$1" pin="I/O1.2" pad="15"/>
<connect gate="G$1" pin="I/O1.3" pad="16"/>
<connect gate="G$1" pin="I/O1.4" pad="17"/>
<connect gate="G$1" pin="I/O1.5" pad="18"/>
<connect gate="G$1" pin="I/O1.6" pad="19"/>
<connect gate="G$1" pin="I/O1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BS" package="HVQFN24">
<connects>
<connect gate="G$1" pin="!INT" pad="22"/>
<connect gate="G$1" pin="A0" pad="18"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A2" pad="24"/>
<connect gate="G$1" pin="I/O0.0" pad="1"/>
<connect gate="G$1" pin="I/O0.1" pad="2"/>
<connect gate="G$1" pin="I/O0.2" pad="3"/>
<connect gate="G$1" pin="I/O0.3" pad="4"/>
<connect gate="G$1" pin="I/O0.4" pad="5"/>
<connect gate="G$1" pin="I/O0.5" pad="6"/>
<connect gate="G$1" pin="I/O0.6" pad="7"/>
<connect gate="G$1" pin="I/O0.7" pad="8"/>
<connect gate="G$1" pin="I/O1.0" pad="10"/>
<connect gate="G$1" pin="I/O1.1" pad="11"/>
<connect gate="G$1" pin="I/O1.2" pad="12"/>
<connect gate="G$1" pin="I/O1.3" pad="13"/>
<connect gate="G$1" pin="I/O1.4" pad="14"/>
<connect gate="G$1" pin="I/O1.5" pad="15"/>
<connect gate="G$1" pin="I/O1.6" pad="16"/>
<connect gate="G$1" pin="I/O1.7" pad="17"/>
<connect gate="G$1" pin="SCL" pad="19"/>
<connect gate="G$1" pin="SDA" pad="20"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PW" package="TSSOP24">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="I/O0.0" pad="4"/>
<connect gate="G$1" pin="I/O0.1" pad="5"/>
<connect gate="G$1" pin="I/O0.2" pad="6"/>
<connect gate="G$1" pin="I/O0.3" pad="7"/>
<connect gate="G$1" pin="I/O0.4" pad="8"/>
<connect gate="G$1" pin="I/O0.5" pad="9"/>
<connect gate="G$1" pin="I/O0.6" pad="10"/>
<connect gate="G$1" pin="I/O0.7" pad="11"/>
<connect gate="G$1" pin="I/O1.0" pad="13"/>
<connect gate="G$1" pin="I/O1.1" pad="14"/>
<connect gate="G$1" pin="I/O1.2" pad="15"/>
<connect gate="G$1" pin="I/O1.3" pad="16"/>
<connect gate="G$1" pin="I/O1.4" pad="17"/>
<connect gate="G$1" pin="I/O1.5" pad="18"/>
<connect gate="G$1" pin="I/O1.6" pad="19"/>
<connect gate="G$1" pin="I/O1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8573" prefix="IC">
<description>I2C-Bus &lt;b&gt;CLOCK/CALENDAR&lt;/b&gt;&lt;p&gt;
with power fail detector</description>
<gates>
<gate name="G$1" symbol="PCF8573"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="EXTPF" pad="6"/>
<connect gate="G$1" pin="FSET" pad="11"/>
<connect gate="G$1" pin="MIN" pad="9"/>
<connect gate="G$1" pin="OSCI" pad="13"/>
<connect gate="G$1" pin="OSCO" pad="14"/>
<connect gate="G$1" pin="PFIN" pad="7"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SEC" pad="10"/>
<connect gate="G$1" pin="TEST" pad="12"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS@1" pad="15"/>
<connect gate="G$1" pin="VSS@2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO16W">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="EXTPF" pad="6"/>
<connect gate="G$1" pin="FSET" pad="11"/>
<connect gate="G$1" pin="MIN" pad="9"/>
<connect gate="G$1" pin="OSCI" pad="13"/>
<connect gate="G$1" pin="OSCO" pad="14"/>
<connect gate="G$1" pin="PFIN" pad="7"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SEC" pad="10"/>
<connect gate="G$1" pin="TEST" pad="12"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS@1" pad="15"/>
<connect gate="G$1" pin="VSS@2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8574" prefix="IC">
<description>I2C-Bus &lt;b&gt;Remote 8-bit I/O expander&lt;/b&gt;&lt;p&gt;
http://www.semiconductors.philips.com/acrobat_download/datasheets/PCF8574_4.pdf</description>
<gates>
<gate name="G$1" symbol="PCF8574"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!INT" pad="13"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="P0" pad="4"/>
<connect gate="G$1" pin="P1" pad="5"/>
<connect gate="G$1" pin="P2" pad="6"/>
<connect gate="G$1" pin="P3" pad="7"/>
<connect gate="G$1" pin="P4" pad="9"/>
<connect gate="G$1" pin="P5" pad="10"/>
<connect gate="G$1" pin="P6" pad="11"/>
<connect gate="G$1" pin="P7" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO16W">
<connects>
<connect gate="G$1" pin="!INT" pad="13"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="P0" pad="4"/>
<connect gate="G$1" pin="P1" pad="5"/>
<connect gate="G$1" pin="P2" pad="6"/>
<connect gate="G$1" pin="P3" pad="7"/>
<connect gate="G$1" pin="P4" pad="9"/>
<connect gate="G$1" pin="P5" pad="10"/>
<connect gate="G$1" pin="P6" pad="11"/>
<connect gate="G$1" pin="P7" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TS" package="SSOP20">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="P0" pad="10"/>
<connect gate="G$1" pin="P1" pad="11"/>
<connect gate="G$1" pin="P2" pad="12"/>
<connect gate="G$1" pin="P3" pad="14"/>
<connect gate="G$1" pin="P4" pad="16"/>
<connect gate="G$1" pin="P5" pad="17"/>
<connect gate="G$1" pin="P6" pad="19"/>
<connect gate="G$1" pin="P7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8584" prefix="IC">
<description>I2C-Bus &lt;b&gt;CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8584"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="!CS" pad="17"/>
<connect gate="G$1" pin="!IACK" pad="4"/>
<connect gate="G$1" pin="!INT" pad="5"/>
<connect gate="G$1" pin="!RD" pad="16"/>
<connect gate="G$1" pin="!RESET" pad="19"/>
<connect gate="G$1" pin="!WR" pad="18"/>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="11"/>
<connect gate="G$1" pin="DB4" pad="12"/>
<connect gate="G$1" pin="DB5" pad="13"/>
<connect gate="G$1" pin="DB6" pad="14"/>
<connect gate="G$1" pin="DB7" pad="15"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO20W">
<connects>
<connect gate="G$1" pin="!CS" pad="17"/>
<connect gate="G$1" pin="!IACK" pad="4"/>
<connect gate="G$1" pin="!INT" pad="5"/>
<connect gate="G$1" pin="!RD" pad="16"/>
<connect gate="G$1" pin="!RESET" pad="19"/>
<connect gate="G$1" pin="!WR" pad="18"/>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="11"/>
<connect gate="G$1" pin="DB4" pad="12"/>
<connect gate="G$1" pin="DB5" pad="13"/>
<connect gate="G$1" pin="DB6" pad="14"/>
<connect gate="G$1" pin="DB7" pad="15"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8591" prefix="IC">
<description>I2C-Bus &lt;b&gt;D/A CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8591"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AIN0" pad="1"/>
<connect gate="G$1" pin="AIN1" pad="2"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3" pad="4"/>
<connect gate="G$1" pin="AOUT" pad="15"/>
<connect gate="G$1" pin="EXT" pad="12"/>
<connect gate="G$1" pin="OSC" pad="11"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="14"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO16W">
<connects>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AIN0" pad="1"/>
<connect gate="G$1" pin="AIN1" pad="2"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3" pad="4"/>
<connect gate="G$1" pin="AOUT" pad="15"/>
<connect gate="G$1" pin="EXT" pad="12"/>
<connect gate="G$1" pin="OSC" pad="11"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="14"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PFC8583" prefix="IC">
<description>I2C-Bus &lt;b&gt;CLOCK/CALENDAR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PFC8583"/>
</gates>
<devices>
<device name="T" package="SO8-7_5">
<connects>
<connect gate="G$1" pin="!INT" pad="7"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="!INT" pad="7"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PN531" prefix="IC">
<description>&lt;b&gt;Near Field Communication Transmission module&lt;/b&gt;&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/other/identification/sfs_pn531_rev2.0.pdf</description>
<gates>
<gate name="G$1" symbol="PN531"/>
</gates>
<devices>
<device name="" package="HVQFN40">
<connects>
<connect gate="G$1" pin="!RSTOUT" pad="29"/>
<connect gate="G$1" pin="!RSTPD" pad="38"/>
<connect gate="G$1" pin="AUX1" pad="12"/>
<connect gate="G$1" pin="AUX2" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="8"/>
<connect gate="G$1" pin="AVSS" pad="11"/>
<connect gate="G$1" pin="DELATT" pad="30"/>
<connect gate="G$1" pin="DVDD" pad="39"/>
<connect gate="G$1" pin="DVSS" pad="1"/>
<connect gate="G$1" pin="I0" pad="16"/>
<connect gate="G$1" pin="I1" pad="17"/>
<connect gate="G$1" pin="IRQ" pad="28"/>
<connect gate="G$1" pin="LOADMOD" pad="2"/>
<connect gate="G$1" pin="MISO" pad="33"/>
<connect gate="G$1" pin="MOSI" pad="32"/>
<connect gate="G$1" pin="NSS" pad="31"/>
<connect gate="G$1" pin="OSC2IN" pad="20"/>
<connect gate="G$1" pin="OSC2OUT" pad="19"/>
<connect gate="G$1" pin="OSCIN" pad="14"/>
<connect gate="G$1" pin="OSCOUT" pad="15"/>
<connect gate="G$1" pin="P30" pad="27"/>
<connect gate="G$1" pin="P31" pad="26"/>
<connect gate="G$1" pin="P32_INT0" pad="37"/>
<connect gate="G$1" pin="P33_INT1" pad="36"/>
<connect gate="G$1" pin="P34" pad="22"/>
<connect gate="G$1" pin="P35" pad="21"/>
<connect gate="G$1" pin="PVDD" pad="35"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="SCK" pad="34"/>
<connect gate="G$1" pin="SIGIN" pad="24"/>
<connect gate="G$1" pin="SIGOUT" pad="23"/>
<connect gate="G$1" pin="SVDD" pad="25"/>
<connect gate="G$1" pin="TESTEN" pad="18"/>
<connect gate="G$1" pin="TH" pad="TH"/>
<connect gate="G$1" pin="TVDD" pad="5"/>
<connect gate="G$1" pin="TVSS1" pad="3"/>
<connect gate="G$1" pin="TVSS2" pad="7"/>
<connect gate="G$1" pin="TX1" pad="4"/>
<connect gate="G$1" pin="TX2" pad="6"/>
<connect gate="G$1" pin="VBUS" pad="40"/>
<connect gate="G$1" pin="VMID" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAA1064" prefix="IC">
<description>I2C-Bus 4-digit &lt;b&gt;LED-DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SAA1064"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="ADR" pad="1"/>
<connect gate="G$1" pin="CEXT" pad="2"/>
<connect gate="G$1" pin="MX1" pad="11"/>
<connect gate="G$1" pin="MX2" pad="14"/>
<connect gate="G$1" pin="P1" pad="10"/>
<connect gate="G$1" pin="P10" pad="16"/>
<connect gate="G$1" pin="P11" pad="17"/>
<connect gate="G$1" pin="P12" pad="18"/>
<connect gate="G$1" pin="P13" pad="19"/>
<connect gate="G$1" pin="P14" pad="20"/>
<connect gate="G$1" pin="P15" pad="21"/>
<connect gate="G$1" pin="P16" pad="22"/>
<connect gate="G$1" pin="P2" pad="9"/>
<connect gate="G$1" pin="P3" pad="8"/>
<connect gate="G$1" pin="P4" pad="7"/>
<connect gate="G$1" pin="P5" pad="6"/>
<connect gate="G$1" pin="P6" pad="5"/>
<connect gate="G$1" pin="P7" pad="4"/>
<connect gate="G$1" pin="P8" pad="3"/>
<connect gate="G$1" pin="P9" pad="15"/>
<connect gate="G$1" pin="SCL" pad="24"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VEE" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO24">
<connects>
<connect gate="G$1" pin="ADR" pad="1"/>
<connect gate="G$1" pin="CEXT" pad="2"/>
<connect gate="G$1" pin="MX1" pad="11"/>
<connect gate="G$1" pin="MX2" pad="14"/>
<connect gate="G$1" pin="P1" pad="10"/>
<connect gate="G$1" pin="P10" pad="16"/>
<connect gate="G$1" pin="P11" pad="17"/>
<connect gate="G$1" pin="P12" pad="18"/>
<connect gate="G$1" pin="P13" pad="19"/>
<connect gate="G$1" pin="P14" pad="20"/>
<connect gate="G$1" pin="P15" pad="21"/>
<connect gate="G$1" pin="P16" pad="22"/>
<connect gate="G$1" pin="P2" pad="9"/>
<connect gate="G$1" pin="P3" pad="8"/>
<connect gate="G$1" pin="P4" pad="7"/>
<connect gate="G$1" pin="P5" pad="6"/>
<connect gate="G$1" pin="P6" pad="5"/>
<connect gate="G$1" pin="P7" pad="4"/>
<connect gate="G$1" pin="P8" pad="3"/>
<connect gate="G$1" pin="P9" pad="15"/>
<connect gate="G$1" pin="SCL" pad="24"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VEE" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA5764HN" prefix="IC">
<description>&lt;b&gt;FM radio + RDS&lt;/b&gt;&lt;p&gt;
single chip electronically tuned FM stereo radio with Radio Data System (RDS)&lt;br&gt;
and Radio Broadcast Data System (RBDS) demodulator and RDS/RBDS decoder&lt;br&gt;
for portable application with fully integrated IF selectivity and demodulation.&lt;br&gt;
Source: http://www.nxp.com .. TEA5764HN_2.pdf</description>
<gates>
<gate name="G$1" symbol="TEA5764HN"/>
</gates>
<devices>
<device name="" package="HVQFN40">
<connects>
<connect gate="G$1" pin="BUSENBABLE" pad="8"/>
<connect gate="G$1" pin="CAGC" pad="39"/>
<connect gate="G$1" pin="CD1" pad="5"/>
<connect gate="G$1" pin="CD2/INTCON3" pad="16"/>
<connect gate="G$1" pin="CD3" pad="35"/>
<connect gate="G$1" pin="CPOUT" pad="2"/>
<connect gate="G$1" pin="FREQIN" pad="32"/>
<connect gate="G$1" pin="GNDA" pad="30"/>
<connect gate="G$1" pin="GNDD" pad="13"/>
<connect gate="G$1" pin="GNDD@1" pad="14"/>
<connect gate="G$1" pin="GNDD@2" pad="19"/>
<connect gate="G$1" pin="GNDD@3" pad="28"/>
<connect gate="G$1" pin="GNDRF" pad="38"/>
<connect gate="G$1" pin="INTCON1" pad="22"/>
<connect gate="G$1" pin="INTCON2" pad="18"/>
<connect gate="G$1" pin="INTX" pad="20"/>
<connect gate="G$1" pin="LO1" pad="3"/>
<connect gate="G$1" pin="LO2" pad="4"/>
<connect gate="G$1" pin="LOOPSW" pad="1"/>
<connect gate="G$1" pin="MPXIN" pad="27"/>
<connect gate="G$1" pin="MPXOUT" pad="26"/>
<connect gate="G$1" pin="PILLP" pad="6"/>
<connect gate="G$1" pin="RFIN1" pad="36"/>
<connect gate="G$1" pin="RFIN2" pad="37"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="SWPORT" pad="7"/>
<connect gate="G$1" pin="TH" pad="TH"/>
<connect gate="G$1" pin="TMUTE" pad="23"/>
<connect gate="G$1" pin="VAFL" pad="25"/>
<connect gate="G$1" pin="VAFR" pad="24"/>
<connect gate="G$1" pin="VCCA" pad="34"/>
<connect gate="G$1" pin="VCCD" pad="15"/>
<connect gate="G$1" pin="VREFDIG" pad="9"/>
<connect gate="G$1" pin="XTAL" pad="33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UAA3220TS" prefix="IC">
<description>&lt;b&gt;FSK / ASK  Receiver&lt;/b&gt; Frequency Shift Keying / Amplitude Shift Keying</description>
<gates>
<gate name="G$1" symbol="UAA3220TS"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="CGND" pad="13"/>
<connect gate="G$1" pin="CPA" pad="15"/>
<connect gate="G$1" pin="CPB" pad="16"/>
<connect gate="G$1" pin="CPC" pad="17"/>
<connect gate="G$1" pin="DATA" pad="14"/>
<connect gate="G$1" pin="DEMO1" pad="10"/>
<connect gate="G$1" pin="DEMO2" pad="11"/>
<connect gate="G$1" pin="FA" pad="22"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="LFB" pad="19"/>
<connect gate="G$1" pin="LIN" pad="20"/>
<connect gate="G$1" pin="MGND" pad="24"/>
<connect gate="G$1" pin="MIXIN" pad="23"/>
<connect gate="G$1" pin="OGND" pad="1"/>
<connect gate="G$1" pin="OSB" pad="3"/>
<connect gate="G$1" pin="OSC" pad="5"/>
<connect gate="G$1" pin="OSE" pad="2"/>
<connect gate="G$1" pin="PWD" pad="9"/>
<connect gate="G$1" pin="RSSI" pad="18"/>
<connect gate="G$1" pin="TEM" pad="6"/>
<connect gate="G$1" pin="TN" pad="7"/>
<connect gate="G$1" pin="TP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VCCI" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UDA1320ATS" prefix="IC">
<description>Stereo filter &lt;b&gt;D/A CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UDA1320"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="G$1" pin="APPL0" pad="11"/>
<connect gate="G$1" pin="APPL1" pad="10"/>
<connect gate="G$1" pin="APPL2" pad="9"/>
<connect gate="G$1" pin="APPL3" pad="8"/>
<connect gate="G$1" pin="APPSEL" pad="7"/>
<connect gate="G$1" pin="BCK" pad="1"/>
<connect gate="G$1" pin="DATAI" pad="3"/>
<connect gate="G$1" pin="SYSCLK" pad="6"/>
<connect gate="G$1" pin="VDDA" pad="13"/>
<connect gate="G$1" pin="VDDD" pad="4"/>
<connect gate="G$1" pin="VOUTL" pad="14"/>
<connect gate="G$1" pin="VOUTR" pad="16"/>
<connect gate="G$1" pin="VREFDAC" pad="12"/>
<connect gate="G$1" pin="VSSA" pad="15"/>
<connect gate="G$1" pin="VSSD" pad="5"/>
<connect gate="G$1" pin="WS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UDA1360TS" prefix="IC">
<description>Stereo audio &lt;b&gt;A/D CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UDA1360T"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="G$1" pin="BCK" pad="11"/>
<connect gate="G$1" pin="DATAO" pad="13"/>
<connect gate="G$1" pin="FSEL" pad="14"/>
<connect gate="G$1" pin="PWON" pad="7"/>
<connect gate="G$1" pin="SFOR" pad="6"/>
<connect gate="G$1" pin="SYSCLK" pad="8"/>
<connect gate="G$1" pin="VDDA" pad="16"/>
<connect gate="G$1" pin="VDDD" pad="9"/>
<connect gate="G$1" pin="VINL" pad="1"/>
<connect gate="G$1" pin="VINR" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
<connect gate="G$1" pin="VREFN" pad="4"/>
<connect gate="G$1" pin="VREFP" pad="5"/>
<connect gate="G$1" pin="VSSA" pad="15"/>
<connect gate="G$1" pin="VSSD" pad="10"/>
<connect gate="G$1" pin="WS" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC904" prefix="IC">
<gates>
<gate name="G$1" symbol="LPC904"/>
</gates>
<devices>
<device name="FD" package="SO8">
<connects>
<connect gate="G$1" pin="AD11/PO.2/CIN2A/KBI2" pad="2"/>
<connect gate="G$1" pin="P0.4/CIN1A/AD13/DAC1" pad="7"/>
<connect gate="G$1" pin="P0.5/CMPREF/CLKIN" pad="6"/>
<connect gate="G$1" pin="P1.0/TXD" pad="5"/>
<connect gate="G$1" pin="P1.1/RXD" pad="3"/>
<connect gate="G$1" pin="RST/P1.5" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FN" package="DIL08">
<connects>
<connect gate="G$1" pin="AD11/PO.2/CIN2A/KBI2" pad="2"/>
<connect gate="G$1" pin="P0.4/CIN1A/AD13/DAC1" pad="7"/>
<connect gate="G$1" pin="P0.5/CMPREF/CLKIN" pad="6"/>
<connect gate="G$1" pin="P1.0/TXD" pad="5"/>
<connect gate="G$1" pin="P1.1/RXD" pad="3"/>
<connect gate="G$1" pin="RST/P1.5" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC938" prefix="IC">
<gates>
<gate name="IC" symbol="LPC938"/>
</gates>
<devices>
<device name="" package="PLCC-S28">
<connects>
<connect gate="IC" pin="CLKOUT/XTAL2/P3.0" pad="9"/>
<connect gate="IC" pin="P0.0/CMP2/KBI0/AD05" pad="3"/>
<connect gate="IC" pin="P0.1/CIN2B/KBI1/AD00" pad="26"/>
<connect gate="IC" pin="P0.2/CIN2A/KBI2/AD01" pad="25"/>
<connect gate="IC" pin="P0.3/CIN1B/KBI3/AD02" pad="24"/>
<connect gate="IC" pin="P0.4/CIN1A/KBI4/AD03" pad="23"/>
<connect gate="IC" pin="P0.5/CMPREF/KBI5" pad="22"/>
<connect gate="IC" pin="P0.6/CMP1/KBI6" pad="20"/>
<connect gate="IC" pin="P0.7/T1/KBI7" pad="19"/>
<connect gate="IC" pin="P1.0/TXD" pad="18"/>
<connect gate="IC" pin="P1.1/RXD" pad="17"/>
<connect gate="IC" pin="P1.2/T0/SCL" pad="12"/>
<connect gate="IC" pin="P1.3/INT0/SDA" pad="11"/>
<connect gate="IC" pin="P1.4/INT1" pad="10"/>
<connect gate="IC" pin="P1.5/RST" pad="6"/>
<connect gate="IC" pin="P1.6/OCB" pad="5"/>
<connect gate="IC" pin="P1.7/OCC/AD04" pad="4"/>
<connect gate="IC" pin="P2.0/ICB/AD07" pad="1"/>
<connect gate="IC" pin="P2.1/OCD/AD06" pad="2"/>
<connect gate="IC" pin="P2.2/MOSI" pad="13"/>
<connect gate="IC" pin="P2.3/MISO" pad="14"/>
<connect gate="IC" pin="P2.4/SS" pad="15"/>
<connect gate="IC" pin="P2.5/SPICLK" pad="16"/>
<connect gate="IC" pin="P2.6/OCA" pad="27"/>
<connect gate="IC" pin="P2.7/ICA" pad="28"/>
<connect gate="IC" pin="VDD" pad="21"/>
<connect gate="IC" pin="VSS" pad="7"/>
<connect gate="IC" pin="XTAL1/P3.1" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC2114">
<gates>
<gate name="G$1" symbol="LPC2114"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="P0.0/TXD0/PWM1" pad="19"/>
<connect gate="G$1" pin="P0.1/RXD0/PWM3/EINT0" pad="21"/>
<connect gate="G$1" pin="P0.10/RTS1/CAP1.0/RD5" pad="35"/>
<connect gate="G$1" pin="P0.11/CTS1/CAP1.1/TD5" pad="37"/>
<connect gate="G$1" pin="P0.12/DSR1/MAT1.0/RD4" pad="38"/>
<connect gate="G$1" pin="P0.13/DTR1/MAT1.1/TD4" pad="39"/>
<connect gate="G$1" pin="P0.14/DCD1/EINT1" pad="41"/>
<connect gate="G$1" pin="P0.15/RI1/EINT2" pad="45"/>
<connect gate="G$1" pin="P0.16/EINT0/MAT0.2/CAP0.2" pad="46"/>
<connect gate="G$1" pin="P0.17/CAP1.2/SCK1/MAT1.2" pad="47"/>
<connect gate="G$1" pin="P0.18/CAP1.3/MISO1/MAT1.3" pad="53"/>
<connect gate="G$1" pin="P0.19/MAT1.2/MOSI1/MAT1.3" pad="54"/>
<connect gate="G$1" pin="P0.2/SCL/CAP0.0" pad="22"/>
<connect gate="G$1" pin="P0.20/MAT1.3/SSEL1/EINT3" pad="55"/>
<connect gate="G$1" pin="P0.21/PWM5/RD3/CAP1.3" pad="1"/>
<connect gate="G$1" pin="P0.22/TD3/CAP0.0/MAT0.0" pad="2"/>
<connect gate="G$1" pin="P0.23/RD2" pad="3"/>
<connect gate="G$1" pin="P0.24/TD2" pad="5"/>
<connect gate="G$1" pin="P0.25/RD1" pad="9"/>
<connect gate="G$1" pin="P0.27/AIN0/CAP0.1/MAT0.1" pad="11"/>
<connect gate="G$1" pin="P0.28/AIN1/CAP0.2/MAT0.2" pad="13"/>
<connect gate="G$1" pin="P0.29/AIN2/CAP0.3/MAT0.3" pad="14"/>
<connect gate="G$1" pin="P0.3/SDA/MAT0.0/EINT1" pad="26"/>
<connect gate="G$1" pin="P0.30/AIN3/EINT3/CAP0.0" pad="15"/>
<connect gate="G$1" pin="P0.4/SCK0/CAP0.1" pad="27"/>
<connect gate="G$1" pin="P0.5/MISO0/MAT0.1" pad="29"/>
<connect gate="G$1" pin="P0.6/MOSI0/CAP0.2" pad="30"/>
<connect gate="G$1" pin="P0.7/SSEL0/PWM2/EINT2" pad="31"/>
<connect gate="G$1" pin="P0.8/TXD1/PWM4" pad="33"/>
<connect gate="G$1" pin="P0.9/RXD1/PWM6/EINT3" pad="34"/>
<connect gate="G$1" pin="P1.16/TRACEPKT0" pad="16"/>
<connect gate="G$1" pin="P1.17/TRACEPKT1" pad="12"/>
<connect gate="G$1" pin="P1.18/TRACEPKT2" pad="8"/>
<connect gate="G$1" pin="P1.19/TRACEPKT3" pad="4"/>
<connect gate="G$1" pin="P1.20/TRACESYNC" pad="48"/>
<connect gate="G$1" pin="P1.21/PIPESTAT0" pad="44"/>
<connect gate="G$1" pin="P1.22/PIPESTAT1" pad="40"/>
<connect gate="G$1" pin="P1.23/PIPESTAT2" pad="36"/>
<connect gate="G$1" pin="P1.24/TRACECLK" pad="32"/>
<connect gate="G$1" pin="P1.25/EXTIN0" pad="28"/>
<connect gate="G$1" pin="P1.26/RTCK" pad="24"/>
<connect gate="G$1" pin="P1.27TDO" pad="64"/>
<connect gate="G$1" pin="P1.28/TDI" pad="60"/>
<connect gate="G$1" pin="P1.29/TCK" pad="56"/>
<connect gate="G$1" pin="P1.3/TMS" pad="52"/>
<connect gate="G$1" pin="P1.31/TRST" pad="20"/>
<connect gate="G$1" pin="RST" pad="57"/>
<connect gate="G$1" pin="TD1" pad="10"/>
<connect gate="G$1" pin="V18-1" pad="17"/>
<connect gate="G$1" pin="V18-2" pad="49"/>
<connect gate="G$1" pin="V18A" pad="63"/>
<connect gate="G$1" pin="V3-1" pad="23"/>
<connect gate="G$1" pin="V3-2" pad="43"/>
<connect gate="G$1" pin="V3-3" pad="51"/>
<connect gate="G$1" pin="V3A" pad="7"/>
<connect gate="G$1" pin="VSS-1" pad="6"/>
<connect gate="G$1" pin="VSS-2" pad="18"/>
<connect gate="G$1" pin="VSS-3" pad="25"/>
<connect gate="G$1" pin="VSS-4" pad="42"/>
<connect gate="G$1" pin="VSS-5" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="59"/>
<connect gate="G$1" pin="VSSA_PLL" pad="58"/>
<connect gate="G$1" pin="X1" pad="61"/>
<connect gate="G$1" pin="X2" pad="62"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC2214">
<gates>
<gate name="G$1" symbol="LPC2214"/>
</gates>
<devices>
<device name="" package="TQFP144">
<connects>
<connect gate="G$1" pin="P.012/DSR1/MAT1.0" pad="84"/>
<connect gate="G$1" pin="P0.0/TXD0/PWM1" pad="42"/>
<connect gate="G$1" pin="P0.1/RXD0/PWM3/EINT0" pad="49"/>
<connect gate="G$1" pin="P0.10/RTS1/CAP1.0" pad="78"/>
<connect gate="G$1" pin="P0.11/CTS1/CAP1.1" pad="83"/>
<connect gate="G$1" pin="P0.13/DTR1/MAT1.1" pad="85"/>
<connect gate="G$1" pin="P0.14/DCD1/EINT1" pad="92"/>
<connect gate="G$1" pin="P0.15/RI1/EINT2" pad="99"/>
<connect gate="G$1" pin="P0.16/EINT0/MAT0.2/CAP0.2" pad="100"/>
<connect gate="G$1" pin="P0.17/CAP1.2/SCK1/MAT1.2" pad="101"/>
<connect gate="G$1" pin="P0.18/CAP1.3/MISO1/MAT1.3" pad="121"/>
<connect gate="G$1" pin="P0.19/MAT1.2/MOSI1/CAP1.2" pad="122"/>
<connect gate="G$1" pin="P0.2/SCL/CAP0.0" pad="50"/>
<connect gate="G$1" pin="P0.20/MAT1.3/SSEL1/EINT3" pad="123"/>
<connect gate="G$1" pin="P0.21/PWM5/CAP1.3" pad="4"/>
<connect gate="G$1" pin="P0.22/CAP0.0/MAT0.0" pad="5"/>
<connect gate="G$1" pin="P0.23" pad="6"/>
<connect gate="G$1" pin="P0.24" pad="8"/>
<connect gate="G$1" pin="P0.25" pad="21"/>
<connect gate="G$1" pin="P0.27/AIN0/CAP0.1/MAT0.1" pad="23"/>
<connect gate="G$1" pin="P0.28/AIN1/CAP0.2/MAT0.2" pad="25"/>
<connect gate="G$1" pin="P0.29/AIN2/CAP0.3/MAT0.3" pad="32"/>
<connect gate="G$1" pin="P0.3/SDA/MAT0.0/EINT1" pad="58"/>
<connect gate="G$1" pin="P0.30/AIN3/EINT3/CAP0.0" pad="33"/>
<connect gate="G$1" pin="P0.4/SCK0/CAP0.1" pad="59"/>
<connect gate="G$1" pin="P0.5/MISO0/MAT0.1" pad="61"/>
<connect gate="G$1" pin="P0.6/MOSI0/CAP0.2" pad="68"/>
<connect gate="G$1" pin="P0.7/SSEL0/PWM2/EINT2" pad="69"/>
<connect gate="G$1" pin="P0.8/TXD1/PWM4" pad="75"/>
<connect gate="G$1" pin="P0.9/RXD1/PWM6/EINT3" pad="76"/>
<connect gate="G$1" pin="P1.0/CS0" pad="91"/>
<connect gate="G$1" pin="P1.1/OE" pad="90"/>
<connect gate="G$1" pin="P1.16/TRACEPKT0" pad="34"/>
<connect gate="G$1" pin="P1.17/TRACEPKT1" pad="24"/>
<connect gate="G$1" pin="P1.18/TRACEPKT2" pad="15"/>
<connect gate="G$1" pin="P1.19/TRACEPKT3" pad="7"/>
<connect gate="G$1" pin="P1.20/TRACESYNC" pad="102"/>
<connect gate="G$1" pin="P1.21/PIPESTAT0" pad="95"/>
<connect gate="G$1" pin="P1.22/PIPESTAT1" pad="86"/>
<connect gate="G$1" pin="P1.23/PIPESTAT2" pad="82"/>
<connect gate="G$1" pin="P1.24/TRACECLK" pad="70"/>
<connect gate="G$1" pin="P1.25/EXTIN0" pad="60"/>
<connect gate="G$1" pin="P1.26/RTCK" pad="52"/>
<connect gate="G$1" pin="P1.27/TDO" pad="144"/>
<connect gate="G$1" pin="P1.28/TDI" pad="140"/>
<connect gate="G$1" pin="P1.29/TCK" pad="126"/>
<connect gate="G$1" pin="P1.30/TMS" pad="113"/>
<connect gate="G$1" pin="P1.31/TRST" pad="43"/>
<connect gate="G$1" pin="P2.0/D0" pad="98"/>
<connect gate="G$1" pin="P2.1/D1" pad="105"/>
<connect gate="G$1" pin="P2.10/D10" pad="120"/>
<connect gate="G$1" pin="P2.11/D11" pad="124"/>
<connect gate="G$1" pin="P2.12/D12" pad="125"/>
<connect gate="G$1" pin="P2.13/D13" pad="127"/>
<connect gate="G$1" pin="P2.14/D14" pad="129"/>
<connect gate="G$1" pin="P2.15/D15" pad="130"/>
<connect gate="G$1" pin="P2.16/D16" pad="131"/>
<connect gate="G$1" pin="P2.17/D17" pad="132"/>
<connect gate="G$1" pin="P2.18/D18" pad="133"/>
<connect gate="G$1" pin="P2.19/D19" pad="134"/>
<connect gate="G$1" pin="P2.2/D2" pad="106"/>
<connect gate="G$1" pin="P2.20/D20" pad="136"/>
<connect gate="G$1" pin="P2.21/D21" pad="137"/>
<connect gate="G$1" pin="P2.22/D22" pad="1"/>
<connect gate="G$1" pin="P2.23/D23" pad="10"/>
<connect gate="G$1" pin="P2.24/D24" pad="11"/>
<connect gate="G$1" pin="P2.25/D25" pad="12"/>
<connect gate="G$1" pin="P2.26/D26/BOOT0" pad="13"/>
<connect gate="G$1" pin="P2.27/D27/BOOT1" pad="16"/>
<connect gate="G$1" pin="P2.28/D28" pad="17"/>
<connect gate="G$1" pin="P2.29/D29" pad="18"/>
<connect gate="G$1" pin="P2.3/D3" pad="108"/>
<connect gate="G$1" pin="P2.30/D30/AIN4" pad="19"/>
<connect gate="G$1" pin="P2.31/D31/AIN5" pad="20"/>
<connect gate="G$1" pin="P2.4/D4" pad="109"/>
<connect gate="G$1" pin="P2.5/D5" pad="114"/>
<connect gate="G$1" pin="P2.6/D6" pad="115"/>
<connect gate="G$1" pin="P2.7/D7" pad="116"/>
<connect gate="G$1" pin="P2.8/D8" pad="117"/>
<connect gate="G$1" pin="P2.9/D9" pad="118"/>
<connect gate="G$1" pin="P3.0//A0" pad="89"/>
<connect gate="G$1" pin="P3.1/A1" pad="88"/>
<connect gate="G$1" pin="P3.10/A10" pad="65"/>
<connect gate="G$1" pin="P3.11/A11" pad="64"/>
<connect gate="G$1" pin="P3.12/A12" pad="63"/>
<connect gate="G$1" pin="P3.13/A13" pad="62"/>
<connect gate="G$1" pin="P3.14/14" pad="56"/>
<connect gate="G$1" pin="P3.15/A15" pad="55"/>
<connect gate="G$1" pin="P3.16/A16" pad="53"/>
<connect gate="G$1" pin="P3.17/A17" pad="48"/>
<connect gate="G$1" pin="P3.18/A18" pad="47"/>
<connect gate="G$1" pin="P3.19/A19" pad="46"/>
<connect gate="G$1" pin="P3.2/A2" pad="87"/>
<connect gate="G$1" pin="P3.20/A20" pad="45"/>
<connect gate="G$1" pin="P3.21/A21" pad="44"/>
<connect gate="G$1" pin="P3.22/A21" pad="41"/>
<connect gate="G$1" pin="P3.23/A23/XCLK" pad="40"/>
<connect gate="G$1" pin="P3.24/CS3" pad="36"/>
<connect gate="G$1" pin="P3.25/CS2" pad="35"/>
<connect gate="G$1" pin="P3.26/CS1" pad="30"/>
<connect gate="G$1" pin="P3.27/WE" pad="29"/>
<connect gate="G$1" pin="P3.28/BLS3/AIN7" pad="28"/>
<connect gate="G$1" pin="P3.29/BLS2/AIN6" pad="27"/>
<connect gate="G$1" pin="P3.3/A3" pad="81"/>
<connect gate="G$1" pin="P3.30/BLS1" pad="97"/>
<connect gate="G$1" pin="P3.31/BLS0" pad="96"/>
<connect gate="G$1" pin="P3.4/A4" pad="80"/>
<connect gate="G$1" pin="P3.5/A5" pad="74"/>
<connect gate="G$1" pin="P3.6/A6" pad="73"/>
<connect gate="G$1" pin="P3.7/A7" pad="72"/>
<connect gate="G$1" pin="P3.8/A8" pad="71"/>
<connect gate="G$1" pin="P3.9/A9" pad="66"/>
<connect gate="G$1" pin="RST" pad="135"/>
<connect gate="G$1" pin="TD1" pad="22"/>
<connect gate="G$1" pin="VDD1.8(A)" pad="143"/>
<connect gate="G$1" pin="VDD1.8-1(CORE)" pad="37"/>
<connect gate="G$1" pin="VDD1.8-2(CORE)" pad="110"/>
<connect gate="G$1" pin="VDD3-1(A)" pad="14"/>
<connect gate="G$1" pin="VDD3-1(I/O)" pad="2"/>
<connect gate="G$1" pin="VDD3-10(I/O)" pad="119"/>
<connect gate="G$1" pin="VDD3-2(I/O)" pad="31"/>
<connect gate="G$1" pin="VDD3-3(I/O)" pad="39"/>
<connect gate="G$1" pin="VDD3-4(I/O)" pad="51"/>
<connect gate="G$1" pin="VDD3-5(I/O)" pad="57"/>
<connect gate="G$1" pin="VDD3-6(I/O)" pad="77"/>
<connect gate="G$1" pin="VDD3-7(I/O)" pad="94"/>
<connect gate="G$1" pin="VDD3-8(I/O)" pad="104"/>
<connect gate="G$1" pin="VDD3-9(I/O)" pad="112"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS10" pad="107"/>
<connect gate="G$1" pin="VSS11" pad="111"/>
<connect gate="G$1" pin="VSS12" pad="128"/>
<connect gate="G$1" pin="VSS2" pad="9"/>
<connect gate="G$1" pin="VSS3" pad="26"/>
<connect gate="G$1" pin="VSS4" pad="38"/>
<connect gate="G$1" pin="VSS5" pad="54"/>
<connect gate="G$1" pin="VSS6" pad="67"/>
<connect gate="G$1" pin="VSS7" pad="79"/>
<connect gate="G$1" pin="VSS8" pad="93"/>
<connect gate="G$1" pin="VSS9" pad="103"/>
<connect gate="G$1" pin="VSSA" pad="139"/>
<connect gate="G$1" pin="VSSA_PLL" pad="138"/>
<connect gate="G$1" pin="X1" pad="142"/>
<connect gate="G$1" pin="X2" pad="141"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICP_CON">
<gates>
<gate name="G$1" symbol="ICP_CON"/>
</gates>
<devices>
<device name="" package="ICP_CON">
<connects>
<connect gate="G$1" pin="/RST" pad="/RST"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="P0.4" pad="P0.4"/>
<connect gate="G$1" pin="P0.5" pad="P0.5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISP_CON">
<gates>
<gate name="G$1" symbol="ISP_CON"/>
</gates>
<devices>
<device name="" package="ISP_CON">
<connects>
<connect gate="G$1" pin="/ISP" pad="/ISP"/>
<connect gate="G$1" pin="/RST" pad="/RST"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RXD" pad="RXD"/>
<connect gate="G$1" pin="TXD" pad="TXD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM75A" prefix="IC">
<gates>
<gate name="G$1" symbol="LM75A"/>
</gates>
<devices>
<device name="" package="SO8">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OS" pad="3"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC213X" prefix="IC">
<gates>
<gate name="G$1" symbol="LPC213X"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="(AD0.0/CAP0.1/MAT0.1)P0.27" pad="11"/>
<connect gate="G$1" pin="(AD0.1/CAP0.2/MAT0.2)P0.28" pad="13"/>
<connect gate="G$1" pin="(AD0.2/CAP0.3/MAT0.3)P0.29" pad="14"/>
<connect gate="G$1" pin="(AD0.3/EINT3/CAP0.0)P0.30" pad="15"/>
<connect gate="G$1" pin="(AD0.4/AOUT)P0.25" pad="9"/>
<connect gate="G$1" pin="(AD0.5)P0.26" pad="10"/>
<connect gate="G$1" pin="(AD1.7/CAP0.0/MAT0.0)P0.22" pad="2"/>
<connect gate="G$1" pin="(CAP1.2/SCK1/MAT1.2)P0.17" pad="47"/>
<connect gate="G$1" pin="(CAP1.3/MISO1/MAT1.3)P0.18" pad="53"/>
<connect gate="G$1" pin="(CTS1/CAP1.1/SCL1)P0.11" pad="37"/>
<connect gate="G$1" pin="(DCD1/EINT1/SDA1)P0.14" pad="41"/>
<connect gate="G$1" pin="(DSR1/MAT1.0/AD1.3)P0.12" pad="38"/>
<connect gate="G$1" pin="(DTR1/MAT1.1/AD1.4)P0.13" pad="39"/>
<connect gate="G$1" pin="(EINT0/MAT0.2/CAP0.2)P0.16" pad="46"/>
<connect gate="G$1" pin="(MAT1.2/MOSI1/CAP1.2)P0.19" pad="54"/>
<connect gate="G$1" pin="(MAT1.3/SSEL1/EINT3)P0.20" pad="55"/>
<connect gate="G$1" pin="(MISO0/MAT0.1/A0.7)P0.5" pad="29"/>
<connect gate="G$1" pin="(MOSI0/CAP0.2/AD1.0)P0.6" pad="30"/>
<connect gate="G$1" pin="(PWM5/AD1.6/CAP1.3)P0.21" pad="1"/>
<connect gate="G$1" pin="(RI1/EINT2/AD1.5)P0.15" pad="45"/>
<connect gate="G$1" pin="(RTS1/CAP1.0/AD1.2)P0.10" pad="35"/>
<connect gate="G$1" pin="(RXD0/PWM3/EINT0)P0.1" pad="21"/>
<connect gate="G$1" pin="(RXD1/PWM6/EINT3)P0.9" pad="34"/>
<connect gate="G$1" pin="(SCK0/CAP0.1/AD0.6)P0.4" pad="27"/>
<connect gate="G$1" pin="(SCL0/CAP0.0)P0.2" pad="22"/>
<connect gate="G$1" pin="(SDA0/MAT0.0/EINT1)P0.3" pad="26"/>
<connect gate="G$1" pin="(SSEL0/PWM2/EINT2)P0.7" pad="31"/>
<connect gate="G$1" pin="(TXD0/PWM1)P0.0" pad="19"/>
<connect gate="G$1" pin="(TXD1/PWM4/A1.1)P0.8" pad="33"/>
<connect gate="G$1" pin="P0.23" pad="58"/>
<connect gate="G$1" pin="P0.31" pad="17"/>
<connect gate="G$1" pin="P1.16(TRACEPKT0)" pad="16"/>
<connect gate="G$1" pin="P1.17(TRACEPKT1)" pad="12"/>
<connect gate="G$1" pin="P1.18(TRACEPKT2)" pad="8"/>
<connect gate="G$1" pin="P1.19(TRACEPKT3)" pad="4"/>
<connect gate="G$1" pin="P1.20(TRACESYNC)" pad="48"/>
<connect gate="G$1" pin="P1.21(PIPESTAT0)" pad="44"/>
<connect gate="G$1" pin="P1.22(PIPESTAT1)" pad="40"/>
<connect gate="G$1" pin="P1.23(PIPESTAT2)" pad="36"/>
<connect gate="G$1" pin="P1.24(TRACECLK)" pad="32"/>
<connect gate="G$1" pin="P1.25(EXTIN0)" pad="28"/>
<connect gate="G$1" pin="P1.26(RTCK)" pad="24"/>
<connect gate="G$1" pin="P1.27(TDO)" pad="64"/>
<connect gate="G$1" pin="P1.28(TDI)" pad="60"/>
<connect gate="G$1" pin="P1.29(TCK)" pad="56"/>
<connect gate="G$1" pin="P1.30(TMS)" pad="52"/>
<connect gate="G$1" pin="P1.31(/TRST)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="57"/>
<connect gate="G$1" pin="RTXC1" pad="3"/>
<connect gate="G$1" pin="RTXC2" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="49"/>
<connect gate="G$1" pin="VDD3-1" pad="23"/>
<connect gate="G$1" pin="VDD3-2" pad="43"/>
<connect gate="G$1" pin="VDD3-3" pad="51"/>
<connect gate="G$1" pin="VDDA3" pad="7"/>
<connect gate="G$1" pin="VREF" pad="63"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="18"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="42"/>
<connect gate="G$1" pin="VSS@4" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="59"/>
<connect gate="G$1" pin="XTAL1" pad="62"/>
<connect gate="G$1" pin="XTAL2" pad="61"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC9107" prefix="IC">
<gates>
<gate name="G$1" symbol="LPC9107"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="N.C." pad="2"/>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="P0.1/KBI1/AD10" pad="5"/>
<connect gate="G$1" pin="P0.2/KBI2/AD11" pad="1"/>
<connect gate="G$1" pin="P0.3/CIN1B/AD12" pad="14"/>
<connect gate="G$1" pin="P0.4/CIN1A/AD13/DAC1" pad="12"/>
<connect gate="G$1" pin="P0.5/CMPREF/CLKIN" pad="11"/>
<connect gate="G$1" pin="P0.7/T1/CLKOUT" pad="8"/>
<connect gate="G$1" pin="P1.0/TXD" pad="6"/>
<connect gate="G$1" pin="P1.1/RXD" pad="9"/>
<connect gate="G$1" pin="P1.2/T0" pad="7"/>
<connect gate="G$1" pin="P1.5/RST" pad="3"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8563" prefix="IC">
<gates>
<gate name="G$1" symbol="PCF8563"/>
</gates>
<devices>
<device name="T" package="SO8">
<connects>
<connect gate="G$1" pin="/INT" pad="3"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA24S08">
<description>1024 x 8-Bit CMOS EEPROM with Access Protection</description>
<gates>
<gate name="IC$1" symbol="PCA24S08"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="IC$1" pin="/PROT" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA8581">
<description>128 x 8-Bit EEPROM with I²C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCA8581"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9538">
<description>8bit I2C-Bus-Expander with Interrupt and Reset</description>
<gates>
<gate name="G$1" symbol="PCA9538"/>
<gate name="G$2" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="/INT" pad="13"/>
<connect gate="G$1" pin="/RST" pad="3"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="IO0" pad="4"/>
<connect gate="G$1" pin="IO1" pad="5"/>
<connect gate="G$1" pin="IO2" pad="6"/>
<connect gate="G$1" pin="IO3" pad="7"/>
<connect gate="G$1" pin="IO4" pad="9"/>
<connect gate="G$1" pin="IO5" pad="10"/>
<connect gate="G$1" pin="IO6" pad="11"/>
<connect gate="G$1" pin="IO7" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$2" pin="GND" pad="8"/>
<connect gate="G$2" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9557">
<description>8bit I2C-Bus-Expander with Reset</description>
<gates>
<gate name="G$1" symbol="PCA9557"/>
<gate name="G$2" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="/RST" pad="15"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="IO0" pad="6"/>
<connect gate="G$1" pin="IO1" pad="7"/>
<connect gate="G$1" pin="IO2" pad="9"/>
<connect gate="G$1" pin="IO3" pad="10"/>
<connect gate="G$1" pin="IO4" pad="11"/>
<connect gate="G$1" pin="IO5" pad="12"/>
<connect gate="G$1" pin="IO6" pad="13"/>
<connect gate="G$1" pin="IO7" pad="14"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$2" pin="GND" pad="8"/>
<connect gate="G$2" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8570">
<description>256 x 8-Bit Static Low-Voltage RAM with I²C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF8570"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="TEST" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8582C-2">
<description>256 x 8-Bit CMOS EEPROM with I²C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF8582"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/03" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/03" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8583" prefix="IC" uservalue="yes">
<description>Clock/calendar with 240 x 8-bit RAM</description>
<gates>
<gate name="G$1" symbol="PCF8583"/>
<gate name="G$2" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="INT" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$2" pin="GND" pad="4"/>
<connect gate="G$2" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SO08">
<connects>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="INT" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$2" pin="GND" pad="4"/>
<connect gate="G$2" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PCF8583BS" package="SOT662">
<connects>
<connect gate="G$1" pin="A0" pad="4"/>
<connect gate="G$1" pin="INT" pad="14"/>
<connect gate="G$1" pin="OSCI" pad="2"/>
<connect gate="G$1" pin="OSCO" pad="3"/>
<connect gate="G$1" pin="SCL" pad="13"/>
<connect gate="G$1" pin="SDA" pad="12"/>
<connect gate="G$2" pin="GND" pad="15"/>
<connect gate="G$2" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8594C-2">
<description>512 x 8-Bit CMOS EEPROM with I²C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF8594"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/02" package="DIL08">
<connects>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/02" package="SO08">
<connects>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8598C-2">
<description>1024 x 8-Bit CMOS EEPROM with I²C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF8598"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/02" package="DIL08">
<connects>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/02" package="SO08">
<connects>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="PTC" pad="7"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="1"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF85102C-2">
<description>256 x 8-Bit CMOS EEPROM with I²C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF85102"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/03" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/03" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF85103C-2">
<description>256 x 8-Bit CMOS EEPROM with I²C Bus Interface</description>
<gates>
<gate name="IC$1" symbol="PCF85103"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="P/00" package="DIL08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T/00" package="SO08">
<connects>
<connect gate="IC$1" pin="A0" pad="1"/>
<connect gate="IC$1" pin="A1" pad="2"/>
<connect gate="IC$1" pin="A2" pad="3"/>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF85116C-3">
<gates>
<gate name="IC$1" symbol="PCF85116"/>
<gate name="PWR" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="SO08">
<connects>
<connect gate="IC$1" pin="SCL" pad="6"/>
<connect gate="IC$1" pin="SDA" pad="5"/>
<connect gate="IC$1" pin="WP" pad="7"/>
<connect gate="PWR" pin="GND" pad="4"/>
<connect gate="PWR" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAA3010" prefix="IC" uservalue="yes">
<description>GENERAL DESCRIPTION
The SAA3010 is intended as a general purpose (RC-5)
infrared remote control system for use where a low voltage
supply and a large debounce time are expected.
The device can generate 2048 different commands and
utilizes a keyboard with a single pole switch for each key.
The commands are arranged so that 32 systems can be
addressed, each system containing 64 different
commands. The keyboard interconnection is illustrated by
Fig.3.
The circuit response to legal (one key pressed at a time)
and illegal (more than one key pressed at a time) keyboard
operation is specified in the section “Keyboard operation</description>
<gates>
<gate name="SAA3010" symbol="SAA3010"/>
</gates>
<devices>
<device name="" package="DIP28">
<connects>
<connect gate="SAA3010" pin="1/X7" pad="1"/>
<connect gate="SAA3010" pin="10/DR6" pad="10"/>
<connect gate="SAA3010" pin="11/DR5" pad="11"/>
<connect gate="SAA3010" pin="12/DR4" pad="12"/>
<connect gate="SAA3010" pin="13/DR3" pad="13"/>
<connect gate="SAA3010" pin="14/VSS" pad="14"/>
<connect gate="SAA3010" pin="15/DR2" pad="15"/>
<connect gate="SAA3010" pin="16/DR1" pad="16"/>
<connect gate="SAA3010" pin="17/DR0" pad="17"/>
<connect gate="SAA3010" pin="18/OSC" pad="18"/>
<connect gate="SAA3010" pin="19/TP2" pad="19"/>
<connect gate="SAA3010" pin="2/SSM" pad="2"/>
<connect gate="SAA3010" pin="20/TP1" pad="20"/>
<connect gate="SAA3010" pin="21/X0" pad="21"/>
<connect gate="SAA3010" pin="22/X1" pad="22"/>
<connect gate="SAA3010" pin="23/X2" pad="23"/>
<connect gate="SAA3010" pin="24/X3" pad="24"/>
<connect gate="SAA3010" pin="25/X4" pad="25"/>
<connect gate="SAA3010" pin="26/X5" pad="26"/>
<connect gate="SAA3010" pin="27/X6" pad="27"/>
<connect gate="SAA3010" pin="28/VDD" pad="28"/>
<connect gate="SAA3010" pin="3/Z0" pad="3"/>
<connect gate="SAA3010" pin="4/Z1" pad="4"/>
<connect gate="SAA3010" pin="5/Z2" pad="5"/>
<connect gate="SAA3010" pin="6/Z3" pad="6"/>
<connect gate="SAA3010" pin="7/MDATA" pad="7"/>
<connect gate="SAA3010" pin="8/DATA" pad="8"/>
<connect gate="SAA3010" pin="9/DR7" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO28" package="SO28">
<connects>
<connect gate="SAA3010" pin="1/X7" pad="1"/>
<connect gate="SAA3010" pin="10/DR6" pad="10"/>
<connect gate="SAA3010" pin="11/DR5" pad="11"/>
<connect gate="SAA3010" pin="12/DR4" pad="12"/>
<connect gate="SAA3010" pin="13/DR3" pad="13"/>
<connect gate="SAA3010" pin="14/VSS" pad="14"/>
<connect gate="SAA3010" pin="15/DR2" pad="15"/>
<connect gate="SAA3010" pin="16/DR1" pad="16"/>
<connect gate="SAA3010" pin="17/DR0" pad="17"/>
<connect gate="SAA3010" pin="18/OSC" pad="18"/>
<connect gate="SAA3010" pin="19/TP2" pad="19"/>
<connect gate="SAA3010" pin="2/SSM" pad="2"/>
<connect gate="SAA3010" pin="20/TP1" pad="20"/>
<connect gate="SAA3010" pin="21/X0" pad="21"/>
<connect gate="SAA3010" pin="22/X1" pad="22"/>
<connect gate="SAA3010" pin="23/X2" pad="23"/>
<connect gate="SAA3010" pin="24/X3" pad="24"/>
<connect gate="SAA3010" pin="25/X4" pad="25"/>
<connect gate="SAA3010" pin="26/X5" pad="26"/>
<connect gate="SAA3010" pin="27/X6" pad="27"/>
<connect gate="SAA3010" pin="28/VDD" pad="28"/>
<connect gate="SAA3010" pin="3/Z0" pad="3"/>
<connect gate="SAA3010" pin="4/Z1" pad="4"/>
<connect gate="SAA3010" pin="5/Z2" pad="5"/>
<connect gate="SAA3010" pin="6/Z3" pad="6"/>
<connect gate="SAA3010" pin="7/MDATA" pad="7"/>
<connect gate="SAA3010" pin="8/DATA" pad="8"/>
<connect gate="SAA3010" pin="9/DR7" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAA1101" prefix="IC" uservalue="yes">
<description>The SAA1101 is a Universal Sync Generator (USG) and is designed for application in video sources such as cameras,
film scanners, video generators and associated apparatus. The circuit can be considered as a successor to the SAA1043
sync generator and the SAA1044 subcarrier coupling IC.</description>
<gates>
<gate name="G$1" symbol="SAA1101"/>
<gate name="P" symbol="VDDVSS"/>
</gates>
<devices>
<device name="T" package="SO28W">
<connects>
<connect gate="G$1" pin="BK" pad="16"/>
<connect gate="G$1" pin="CB" pad="17"/>
<connect gate="G$1" pin="CLO" pad="24"/>
<connect gate="G$1" pin="CLP" pad="19"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="CS0" pad="4"/>
<connect gate="G$1" pin="CS1" pad="3"/>
<connect gate="G$1" pin="ECS" pad="11"/>
<connect gate="G$1" pin="FSI" pad="1"/>
<connect gate="G$1" pin="FSO" pad="2"/>
<connect gate="G$1" pin="HD" pad="22"/>
<connect gate="G$1" pin="ID" pad="15"/>
<connect gate="G$1" pin="LM0" pad="10"/>
<connect gate="G$1" pin="LM1" pad="9"/>
<connect gate="G$1" pin="NORM" pad="23"/>
<connect gate="G$1" pin="OSCI" pad="5"/>
<connect gate="G$1" pin="OSCO" pad="6"/>
<connect gate="G$1" pin="PH" pad="8"/>
<connect gate="G$1" pin="RR" pad="12"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="VD" pad="21"/>
<connect gate="G$1" pin="VLE" pad="7"/>
<connect gate="G$1" pin="WMP" pad="20"/>
<connect gate="G$1" pin="X" pad="25"/>
<connect gate="G$1" pin="Y" pad="26"/>
<connect gate="G$1" pin="Z" pad="27"/>
<connect gate="P" pin="VDD" pad="28"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="BK" pad="16"/>
<connect gate="G$1" pin="CB" pad="17"/>
<connect gate="G$1" pin="CLO" pad="24"/>
<connect gate="G$1" pin="CLP" pad="19"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="CS0" pad="4"/>
<connect gate="G$1" pin="CS1" pad="3"/>
<connect gate="G$1" pin="ECS" pad="11"/>
<connect gate="G$1" pin="FSI" pad="1"/>
<connect gate="G$1" pin="FSO" pad="2"/>
<connect gate="G$1" pin="HD" pad="22"/>
<connect gate="G$1" pin="ID" pad="15"/>
<connect gate="G$1" pin="LM0" pad="10"/>
<connect gate="G$1" pin="LM1" pad="9"/>
<connect gate="G$1" pin="NORM" pad="23"/>
<connect gate="G$1" pin="OSCI" pad="5"/>
<connect gate="G$1" pin="OSCO" pad="6"/>
<connect gate="G$1" pin="PH" pad="8"/>
<connect gate="G$1" pin="RR" pad="12"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="VD" pad="21"/>
<connect gate="G$1" pin="VLE" pad="7"/>
<connect gate="G$1" pin="WMP" pad="20"/>
<connect gate="G$1" pin="X" pad="25"/>
<connect gate="G$1" pin="Y" pad="26"/>
<connect gate="G$1" pin="Z" pad="27"/>
<connect gate="P" pin="VDD" pad="28"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA84CX40/84CX43" prefix="IC" uservalue="yes">
<description>The 84C44X; 84C64X; 84C84X denotes the types:
· PCA84C440; 84C441; 84C443; 84C444
· PCA84C640; 84C641; 84C643; 84C644
· PCA84C840; 84C841; 84C843; 84C844.
which are 8-bit microcontrollers with On Screen Display
(OSD) and Voltage Synthesized Tuning (VST) functions.
All are members of the 84CXXX microcontroller family.
There are two oscillator types for the OSD function in the
various types, i.e.,
· RC oscillator: PCA84C440; 84C443; 84C640; 84C643;
84C840; 84C843
· LC oscillator: PCA84C441; 84C444; 84C641; 84C644;
84C841; 84C844.</description>
<gates>
<gate name="G$1" symbol="PCA84CX40/84CX43"/>
</gates>
<devices>
<device name="" package="SOT270-1">
<connects>
<connect gate="G$1" pin="1/DP0.0/TDAC" pad="P$1"/>
<connect gate="G$1" pin="10/P1.2" pad="P$10"/>
<connect gate="G$1" pin="11/P1.3" pad="P$11"/>
<connect gate="G$1" pin="12/1.4" pad="P$12"/>
<connect gate="G$1" pin="13/P0.0" pad="P$13"/>
<connect gate="G$1" pin="14/P0.1" pad="P$14"/>
<connect gate="G$1" pin="15/P0.2" pad="P$15"/>
<connect gate="G$1" pin="16/P0.3" pad="P$16"/>
<connect gate="G$1" pin="17/P0.4" pad="P$17"/>
<connect gate="G$1" pin="18/P0.5" pad="P$18"/>
<connect gate="G$1" pin="19/P0.6" pad="P$19"/>
<connect gate="G$1" pin="2/DP0.1/PWM1" pad="P$2"/>
<connect gate="G$1" pin="20/P0.7" pad="P$20"/>
<connect gate="G$1" pin="21/VSS" pad="P$21"/>
<connect gate="G$1" pin="22/VOW1/DP1.6" pad="P$22"/>
<connect gate="G$1" pin="23/VOW2/DP1.5" pad="P$23"/>
<connect gate="G$1" pin="24/VOW3" pad="P$24"/>
<connect gate="G$1" pin="25/VOB" pad="P$25"/>
<connect gate="G$1" pin="26/HSYNCN" pad="P$26"/>
<connect gate="G$1" pin="27/VSYNCN" pad="P$27"/>
<connect gate="G$1" pin="28/DOSC1" pad="P$28"/>
<connect gate="G$1" pin="29/T1" pad="P$29"/>
<connect gate="G$1" pin="3/DP0.2/PWM2" pad="P$3"/>
<connect gate="G$1" pin="30/TEST/EMU" pad="P$30"/>
<connect gate="G$1" pin="31/XTAL1" pad="P$31"/>
<connect gate="G$1" pin="32/XTAL2" pad="P$32"/>
<connect gate="G$1" pin="33/RESET" pad="P$33"/>
<connect gate="G$1" pin="34/DP1.4" pad="P$34"/>
<connect gate="G$1" pin="35/INT/T0" pad="P$35"/>
<connect gate="G$1" pin="36/DP1.3" pad="P$36"/>
<connect gate="G$1" pin="37/DP1.2" pad="P$37"/>
<connect gate="G$1" pin="38/DP1.1" pad="P$38"/>
<connect gate="G$1" pin="39/DP0.7/SCL" pad="P$39"/>
<connect gate="G$1" pin="4/DP0.3/PWM3" pad="P$4"/>
<connect gate="G$1" pin="40/DP0.6/SDA" pad="P$40"/>
<connect gate="G$1" pin="41/DP1.0" pad="P$41"/>
<connect gate="G$1" pin="42/VDD" pad="P$42"/>
<connect gate="G$1" pin="5/DP0.4/PWM4" pad="P$5"/>
<connect gate="G$1" pin="6/DP0.5/PWM5" pad="P$6"/>
<connect gate="G$1" pin="7/P1.0" pad="P$7"/>
<connect gate="G$1" pin="8/P1.1" pad="P$8"/>
<connect gate="G$1" pin="9/DP1.7/AFC" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA84CX41/84CX44" prefix="IC" uservalue="yes">
<description>The 84C44X; 84C64X; 84C84X denotes the types:
· PCA84C440; 84C441; 84C443; 84C444
· PCA84C640; 84C641; 84C643; 84C644
· PCA84C840; 84C841; 84C843; 84C844.
which are 8-bit microcontrollers with On Screen Display
(OSD) and Voltage Synthesized Tuning (VST) functions.
All are members of the 84CXXX microcontroller family.
There are two oscillator types for the OSD function in the
various types, i.e.,
· RC oscillator: PCA84C440; 84C443; 84C640; 84C643;
84C840; 84C843
· LC oscillator: PCA84C441; 84C444; 84C641; 84C644;
84C841; 84C844.</description>
<gates>
<gate name="G$1" symbol="PCA84CX41/84CX44"/>
</gates>
<devices>
<device name="" package="SOT270-1">
<connects>
<connect gate="G$1" pin="1/DP0.0/TDAC" pad="P$1"/>
<connect gate="G$1" pin="10/P1.2" pad="P$10"/>
<connect gate="G$1" pin="11/P1.3" pad="P$11"/>
<connect gate="G$1" pin="12/1.4" pad="P$12"/>
<connect gate="G$1" pin="13/P0.0" pad="P$13"/>
<connect gate="G$1" pin="14/P0.1" pad="P$14"/>
<connect gate="G$1" pin="15/P0.2" pad="P$15"/>
<connect gate="G$1" pin="16/P0.3" pad="P$16"/>
<connect gate="G$1" pin="17/P0.4" pad="P$17"/>
<connect gate="G$1" pin="18/P0.5" pad="P$18"/>
<connect gate="G$1" pin="19/P0.6" pad="P$19"/>
<connect gate="G$1" pin="2/DP0.1/PWM1" pad="P$2"/>
<connect gate="G$1" pin="20/P0.7" pad="P$20"/>
<connect gate="G$1" pin="21/VSS" pad="P$21"/>
<connect gate="G$1" pin="22/VOW1/DP1.6" pad="P$22"/>
<connect gate="G$1" pin="23/VOW2/DP1.5" pad="P$23"/>
<connect gate="G$1" pin="24/VOW3" pad="P$24"/>
<connect gate="G$1" pin="25/VOB" pad="P$25"/>
<connect gate="G$1" pin="26/HSYNCN" pad="P$26"/>
<connect gate="G$1" pin="27/VSYNCN" pad="P$27"/>
<connect gate="G$1" pin="28/DOSC1" pad="P$28"/>
<connect gate="G$1" pin="29/DOSC2" pad="P$29"/>
<connect gate="G$1" pin="3/DP0.2/PWM2" pad="P$3"/>
<connect gate="G$1" pin="30/TEST/EMU" pad="P$30"/>
<connect gate="G$1" pin="31/XTAL1" pad="P$31"/>
<connect gate="G$1" pin="32/XTAL2" pad="P$32"/>
<connect gate="G$1" pin="33/RESET" pad="P$33"/>
<connect gate="G$1" pin="34/T1" pad="P$34"/>
<connect gate="G$1" pin="35/INT/T0" pad="P$35"/>
<connect gate="G$1" pin="36/DP1.3" pad="P$36"/>
<connect gate="G$1" pin="37/DP1.2" pad="P$37"/>
<connect gate="G$1" pin="38/DP1.1" pad="P$38"/>
<connect gate="G$1" pin="39/DP0.7/SCL" pad="P$39"/>
<connect gate="G$1" pin="4/DP0.3/PWM3" pad="P$4"/>
<connect gate="G$1" pin="40/DP0.6/SDA" pad="P$40"/>
<connect gate="G$1" pin="41/DP1.0" pad="P$41"/>
<connect gate="G$1" pin="42/VDD" pad="P$42"/>
<connect gate="G$1" pin="5/DP0.4/PWM4" pad="P$5"/>
<connect gate="G$1" pin="6/DP0.5/PWM5" pad="P$6"/>
<connect gate="G$1" pin="7/P1.0" pad="P$7"/>
<connect gate="G$1" pin="8/P1.1" pad="P$8"/>
<connect gate="G$1" pin="9/DP1.7/AFC" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9564">
<description>Parallel Bus to I²C Bus Controller</description>
<gates>
<gate name="PWR" symbol="PWRN"/>
<gate name="IC$1" symbol="PCA9564"/>
</gates>
<devices>
<device name="D" package="SO20W">
<connects>
<connect gate="IC$1" pin="/CE" pad="13"/>
<connect gate="IC$1" pin="/INT" pad="16"/>
<connect gate="IC$1" pin="/RD" pad="12"/>
<connect gate="IC$1" pin="/RST" pad="17"/>
<connect gate="IC$1" pin="/WR" pad="11"/>
<connect gate="IC$1" pin="A0" pad="14"/>
<connect gate="IC$1" pin="A1" pad="15"/>
<connect gate="IC$1" pin="D0" pad="1"/>
<connect gate="IC$1" pin="D1" pad="2"/>
<connect gate="IC$1" pin="D2" pad="3"/>
<connect gate="IC$1" pin="D3" pad="4"/>
<connect gate="IC$1" pin="D4" pad="5"/>
<connect gate="IC$1" pin="D5" pad="6"/>
<connect gate="IC$1" pin="D6" pad="7"/>
<connect gate="IC$1" pin="D7" pad="8"/>
<connect gate="IC$1" pin="SCL" pad="18"/>
<connect gate="IC$1" pin="SDA" pad="19"/>
<connect gate="PWR" pin="GND" pad="10"/>
<connect gate="PWR" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C562" prefix="IC">
<description>&lt;b&gt;8051-compatible 8bit Microcontroller&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="PWR5+2"/>
<gate name="G" symbol="8XC562"/>
</gates>
<devices>
<device name="" package="PLCC-S68">
<connects>
<connect gate="G" pin="/EW" pad="6"/>
<connect gate="G" pin="ALE" pad="48"/>
<connect gate="G" pin="EA" pad="49"/>
<connect gate="G" pin="NC@0" pad="32"/>
<connect gate="G" pin="NC@1" pad="33"/>
<connect gate="G" pin="NC@2" pad="38"/>
<connect gate="G" pin="P0.0/D0" pad="57"/>
<connect gate="G" pin="P0.1/D1" pad="56"/>
<connect gate="G" pin="P0.2/D2" pad="55"/>
<connect gate="G" pin="P0.3/D3" pad="54"/>
<connect gate="G" pin="P0.4/D4" pad="53"/>
<connect gate="G" pin="P0.5/D5" pad="52"/>
<connect gate="G" pin="P0.6/D6" pad="51"/>
<connect gate="G" pin="P0.7/D7" pad="50"/>
<connect gate="G" pin="P1.0/CT0I" pad="16"/>
<connect gate="G" pin="P1.1/CT1I" pad="17"/>
<connect gate="G" pin="P1.2/CT2I" pad="18"/>
<connect gate="G" pin="P1.3/CT3I" pad="19"/>
<connect gate="G" pin="P1.4/T2" pad="20"/>
<connect gate="G" pin="P1.5/RT2" pad="21"/>
<connect gate="G" pin="P1.6" pad="22"/>
<connect gate="G" pin="P1.7" pad="23"/>
<connect gate="G" pin="P2.0/A8" pad="39"/>
<connect gate="G" pin="P2.1/A9" pad="40"/>
<connect gate="G" pin="P2.2/A10" pad="41"/>
<connect gate="G" pin="P2.3/A11" pad="42"/>
<connect gate="G" pin="P2.4/A12" pad="43"/>
<connect gate="G" pin="P2.5/A13" pad="44"/>
<connect gate="G" pin="P2.6/A14" pad="45"/>
<connect gate="G" pin="P2.7/A15" pad="46"/>
<connect gate="G" pin="P3.0" pad="24"/>
<connect gate="G" pin="P3.1" pad="25"/>
<connect gate="G" pin="P3.2" pad="26"/>
<connect gate="G" pin="P3.3" pad="27"/>
<connect gate="G" pin="P3.4/T0" pad="28"/>
<connect gate="G" pin="P3.5/T1" pad="29"/>
<connect gate="G" pin="P3.6/WR" pad="30"/>
<connect gate="G" pin="P3.7/RD" pad="31"/>
<connect gate="G" pin="P4.0/CMSR0" pad="7"/>
<connect gate="G" pin="P4.1/CMSR1" pad="8"/>
<connect gate="G" pin="P4.2/CMSR2" pad="9"/>
<connect gate="G" pin="P4.3/CMSR3" pad="10"/>
<connect gate="G" pin="P4.4/CMSR4" pad="11"/>
<connect gate="G" pin="P4.5/CMSR5" pad="12"/>
<connect gate="G" pin="P4.6/CMT0" pad="13"/>
<connect gate="G" pin="P4.7/CMT1" pad="14"/>
<connect gate="G" pin="P5.0/ADC0" pad="1"/>
<connect gate="G" pin="P5.1/ADC1" pad="68"/>
<connect gate="G" pin="P5.2/ADC2" pad="67"/>
<connect gate="G" pin="P5.3/ADC3" pad="66"/>
<connect gate="G" pin="P5.4/ADC4" pad="65"/>
<connect gate="G" pin="P5.5/ADC5" pad="64"/>
<connect gate="G" pin="P5.6/ADC6" pad="63"/>
<connect gate="G" pin="P5.7/ADC7" pad="62"/>
<connect gate="G" pin="PSEN" pad="47"/>
<connect gate="G" pin="PWM0" pad="4"/>
<connect gate="G" pin="PWM1" pad="5"/>
<connect gate="G" pin="RST" pad="15"/>
<connect gate="G" pin="STADC" pad="3"/>
<connect gate="G" pin="XTAL1" pad="35"/>
<connect gate="G" pin="XTAL2" pad="34"/>
<connect gate="P" pin="AVDD" pad="61"/>
<connect gate="P" pin="AVREF-" pad="58"/>
<connect gate="P" pin="AVSS" pad="60"/>
<connect gate="P" pin="VDD" pad="2"/>
<connect gate="P" pin="VREF" pad="59"/>
<connect gate="P" pin="VSS@0" pad="36"/>
<connect gate="P" pin="VSS@1" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="PLCC68">
<connects>
<connect gate="G" pin="/EW" pad="6"/>
<connect gate="G" pin="ALE" pad="48"/>
<connect gate="G" pin="EA" pad="49"/>
<connect gate="G" pin="NC@0" pad="32"/>
<connect gate="G" pin="NC@1" pad="33"/>
<connect gate="G" pin="NC@2" pad="38"/>
<connect gate="G" pin="P0.0/D0" pad="57"/>
<connect gate="G" pin="P0.1/D1" pad="56"/>
<connect gate="G" pin="P0.2/D2" pad="55"/>
<connect gate="G" pin="P0.3/D3" pad="54"/>
<connect gate="G" pin="P0.4/D4" pad="53"/>
<connect gate="G" pin="P0.5/D5" pad="52"/>
<connect gate="G" pin="P0.6/D6" pad="51"/>
<connect gate="G" pin="P0.7/D7" pad="50"/>
<connect gate="G" pin="P1.0/CT0I" pad="16"/>
<connect gate="G" pin="P1.1/CT1I" pad="17"/>
<connect gate="G" pin="P1.2/CT2I" pad="18"/>
<connect gate="G" pin="P1.3/CT3I" pad="19"/>
<connect gate="G" pin="P1.4/T2" pad="20"/>
<connect gate="G" pin="P1.5/RT2" pad="21"/>
<connect gate="G" pin="P1.6" pad="22"/>
<connect gate="G" pin="P1.7" pad="23"/>
<connect gate="G" pin="P2.0/A8" pad="39"/>
<connect gate="G" pin="P2.1/A9" pad="40"/>
<connect gate="G" pin="P2.2/A10" pad="41"/>
<connect gate="G" pin="P2.3/A11" pad="42"/>
<connect gate="G" pin="P2.4/A12" pad="43"/>
<connect gate="G" pin="P2.5/A13" pad="44"/>
<connect gate="G" pin="P2.6/A14" pad="45"/>
<connect gate="G" pin="P2.7/A15" pad="46"/>
<connect gate="G" pin="P3.0" pad="24"/>
<connect gate="G" pin="P3.1" pad="25"/>
<connect gate="G" pin="P3.2" pad="26"/>
<connect gate="G" pin="P3.3" pad="27"/>
<connect gate="G" pin="P3.4/T0" pad="28"/>
<connect gate="G" pin="P3.5/T1" pad="29"/>
<connect gate="G" pin="P3.6/WR" pad="30"/>
<connect gate="G" pin="P3.7/RD" pad="31"/>
<connect gate="G" pin="P4.0/CMSR0" pad="7"/>
<connect gate="G" pin="P4.1/CMSR1" pad="8"/>
<connect gate="G" pin="P4.2/CMSR2" pad="9"/>
<connect gate="G" pin="P4.3/CMSR3" pad="10"/>
<connect gate="G" pin="P4.4/CMSR4" pad="11"/>
<connect gate="G" pin="P4.5/CMSR5" pad="12"/>
<connect gate="G" pin="P4.6/CMT0" pad="13"/>
<connect gate="G" pin="P4.7/CMT1" pad="14"/>
<connect gate="G" pin="P5.0/ADC0" pad="1"/>
<connect gate="G" pin="P5.1/ADC1" pad="68"/>
<connect gate="G" pin="P5.2/ADC2" pad="67"/>
<connect gate="G" pin="P5.3/ADC3" pad="66"/>
<connect gate="G" pin="P5.4/ADC4" pad="65"/>
<connect gate="G" pin="P5.5/ADC5" pad="64"/>
<connect gate="G" pin="P5.6/ADC6" pad="63"/>
<connect gate="G" pin="P5.7/ADC7" pad="62"/>
<connect gate="G" pin="PSEN" pad="47"/>
<connect gate="G" pin="PWM0" pad="4"/>
<connect gate="G" pin="PWM1" pad="5"/>
<connect gate="G" pin="RST" pad="15"/>
<connect gate="G" pin="STADC" pad="3"/>
<connect gate="G" pin="XTAL1" pad="35"/>
<connect gate="G" pin="XTAL2" pad="34"/>
<connect gate="P" pin="AVDD" pad="61"/>
<connect gate="P" pin="AVREF-" pad="58"/>
<connect gate="P" pin="AVSS" pad="60"/>
<connect gate="P" pin="VDD" pad="2"/>
<connect gate="P" pin="VREF" pad="59"/>
<connect gate="P" pin="VSS@0" pad="36"/>
<connect gate="P" pin="VSS@1" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO10" prefix="_">
<description>&lt;b&gt;LOGO&lt;/b&gt; 10 mm</description>
<gates>
<gate name="-1" symbol="LOGO10"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO20" prefix="_">
<description>&lt;b&gt;LOGO&lt;/b&gt; 20 mm</description>
<gates>
<gate name="-1" symbol="LOGO20"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9543" prefix="IC" uservalue="yes">
<description>&lt;b&gt;2-channel I2C switch with interrupt logic
and reset&lt;/b&gt;&lt;p&gt;
Source : http://www.datasheetcatalog.org/datasheet/philips/PCA9543_1.pdf</description>
<gates>
<gate name="G$1" symbol="PCF9543"/>
</gates>
<devices>
<device name="D" package="SO14">
<connects>
<connect gate="G$1" pin="!INT" pad="11"/>
<connect gate="G$1" pin="!INT0" pad="4"/>
<connect gate="G$1" pin="!INT1" pad="8"/>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="SC0" pad="6"/>
<connect gate="G$1" pin="SC1" pad="10"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SD0" pad="5"/>
<connect gate="G$1" pin="SD1" pad="9"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PW" package="TSSOP14">
<connects>
<connect gate="G$1" pin="!INT" pad="11"/>
<connect gate="G$1" pin="!INT0" pad="4"/>
<connect gate="G$1" pin="!INT1" pad="8"/>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="SC0" pad="6"/>
<connect gate="G$1" pin="SC1" pad="10"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SD0" pad="5"/>
<connect gate="G$1" pin="SD1" pad="9"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8708A" prefix="IC" uservalue="yes">
<description>The TDA8708A is an analog input interface for video signal
processing. It includes a video amplifier with clamp and
gain control, an 8-bit analog-to-digital converter (ADC)
with a sampling rate of 32 MHz and an input selector.</description>
<gates>
<gate name="TDA8708A" symbol="TDA8708A"/>
</gates>
<devices>
<device name="" package="TDA8708A">
<connects>
<connect gate="TDA8708A" pin="ADCIN" pad="20"/>
<connect gate="TDA8708A" pin="AGC" pad="25"/>
<connect gate="TDA8708A" pin="AGND" pad="23"/>
<connect gate="TDA8708A" pin="ANOUT" pad="19"/>
<connect gate="TDA8708A" pin="CLAMP" pad="24"/>
<connect gate="TDA8708A" pin="CLK" pad="5"/>
<connect gate="TDA8708A" pin="D0" pad="13"/>
<connect gate="TDA8708A" pin="D1" pad="12"/>
<connect gate="TDA8708A" pin="D2" pad="11"/>
<connect gate="TDA8708A" pin="D3" pad="10"/>
<connect gate="TDA8708A" pin="D4" pad="4"/>
<connect gate="TDA8708A" pin="D5" pad="3"/>
<connect gate="TDA8708A" pin="D6" pad="2"/>
<connect gate="TDA8708A" pin="D7" pad="1"/>
<connect gate="TDA8708A" pin="DEC" pad="21"/>
<connect gate="TDA8708A" pin="DGND" pad="8"/>
<connect gate="TDA8708A" pin="GATEA" pad="27"/>
<connect gate="TDA8708A" pin="GATEB" pad="26"/>
<connect gate="TDA8708A" pin="I0" pad="14"/>
<connect gate="TDA8708A" pin="I1" pad="15"/>
<connect gate="TDA8708A" pin="OF" pad="9"/>
<connect gate="TDA8708A" pin="RPEAK" pad="28"/>
<connect gate="TDA8708A" pin="VCCA" pad="22"/>
<connect gate="TDA8708A" pin="VCCD" pad="6"/>
<connect gate="TDA8708A" pin="VCCO" pad="7"/>
<connect gate="TDA8708A" pin="VIN0" pad="16"/>
<connect gate="TDA8708A" pin="VIN1" pad="17"/>
<connect gate="TDA8708A" pin="VIN2" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LSV4245A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Octal dual supply translating
transceiver&lt;/b&gt;&lt;p&gt;
http://pdf.datasheetcatalog.com/datasheet/philips/74lvc4245a.pdf</description>
<gates>
<gate name="G$1" symbol="74LVC4245A"/>
</gates>
<devices>
<device name="74LVC4245AD" package="SO24">
<connects>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="8"/>
<connect gate="G$1" pin="A6" pad="9"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="B0" pad="21"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="19"/>
<connect gate="G$1" pin="B3" pad="18"/>
<connect gate="G$1" pin="B4" pad="17"/>
<connect gate="G$1" pin="B5" pad="16"/>
<connect gate="G$1" pin="B6" pad="15"/>
<connect gate="G$1" pin="B7" pad="14"/>
<connect gate="G$1" pin="DIR" pad="2"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="23"/>
<connect gate="G$1" pin="VCCB@" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="74LVC4245ADB" package="SSOP24">
<connects>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="8"/>
<connect gate="G$1" pin="A6" pad="9"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="B0" pad="21"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="19"/>
<connect gate="G$1" pin="B3" pad="18"/>
<connect gate="G$1" pin="B4" pad="17"/>
<connect gate="G$1" pin="B5" pad="16"/>
<connect gate="G$1" pin="B6" pad="15"/>
<connect gate="G$1" pin="B7" pad="14"/>
<connect gate="G$1" pin="DIR" pad="2"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="23"/>
<connect gate="G$1" pin="VCCB@" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="74LVC4245ADH" package="TSSOP24">
<connects>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="8"/>
<connect gate="G$1" pin="A6" pad="9"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="B0" pad="21"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="19"/>
<connect gate="G$1" pin="B3" pad="18"/>
<connect gate="G$1" pin="B4" pad="17"/>
<connect gate="G$1" pin="B5" pad="16"/>
<connect gate="G$1" pin="B6" pad="15"/>
<connect gate="G$1" pin="B7" pad="14"/>
<connect gate="G$1" pin="DIR" pad="2"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="23"/>
<connect gate="G$1" pin="VCCB@" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8703" prefix="IC" uservalue="yes">
<description>The TDA8703 is an 8-bit high-speed Analog-to-Digital
Converter (ADC) for video and other applications.
It converts the analog input signal into 8-bit binary-coded
digital words at a maximum sampling rate of 40 MHz.
All digital inputs and outputs are TTL compatible, although
a low-level AC clock input signal is allowed</description>
<gates>
<gate name="TDA8703" symbol="TDA8703"/>
</gates>
<devices>
<device name="TDA8703" package="DIL24-6">
<connects>
<connect gate="TDA8703" pin="1/D1" pad="1"/>
<connect gate="TDA8703" pin="10/NC" pad="10"/>
<connect gate="TDA8703" pin="11/O/UF" pad="11"/>
<connect gate="TDA8703" pin="12/D7" pad="12"/>
<connect gate="TDA8703" pin="13/D6" pad="13"/>
<connect gate="TDA8703" pin="14/D5" pad="14"/>
<connect gate="TDA8703" pin="15/D4" pad="15"/>
<connect gate="TDA8703" pin="16/CLK" pad="16"/>
<connect gate="TDA8703" pin="17/CLK" pad="17"/>
<connect gate="TDA8703" pin="18/VCCD" pad="18"/>
<connect gate="TDA8703" pin="19/VCCO" pad="19"/>
<connect gate="TDA8703" pin="2/D0" pad="2"/>
<connect gate="TDA8703" pin="20/DGND" pad="20"/>
<connect gate="TDA8703" pin="21/TC" pad="21"/>
<connect gate="TDA8703" pin="22/CE" pad="22"/>
<connect gate="TDA8703" pin="23/D3" pad="23"/>
<connect gate="TDA8703" pin="24/D2" pad="24"/>
<connect gate="TDA8703" pin="3/AGND" pad="3"/>
<connect gate="TDA8703" pin="4/VRB" pad="4"/>
<connect gate="TDA8703" pin="5/DEC" pad="5"/>
<connect gate="TDA8703" pin="6/NC" pad="6"/>
<connect gate="TDA8703" pin="7/VCCA" pad="7"/>
<connect gate="TDA8703" pin="8/VI" pad="8"/>
<connect gate="TDA8703" pin="9/VRT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TDA8703T" package="SO24">
<connects>
<connect gate="TDA8703" pin="1/D1" pad="1"/>
<connect gate="TDA8703" pin="10/NC" pad="10"/>
<connect gate="TDA8703" pin="11/O/UF" pad="11"/>
<connect gate="TDA8703" pin="12/D7" pad="12"/>
<connect gate="TDA8703" pin="13/D6" pad="13"/>
<connect gate="TDA8703" pin="14/D5" pad="14"/>
<connect gate="TDA8703" pin="15/D4" pad="15"/>
<connect gate="TDA8703" pin="16/CLK" pad="16"/>
<connect gate="TDA8703" pin="17/CLK" pad="17"/>
<connect gate="TDA8703" pin="18/VCCD" pad="18"/>
<connect gate="TDA8703" pin="19/VCCO" pad="19"/>
<connect gate="TDA8703" pin="2/D0" pad="2"/>
<connect gate="TDA8703" pin="20/DGND" pad="20"/>
<connect gate="TDA8703" pin="21/TC" pad="21"/>
<connect gate="TDA8703" pin="22/CE" pad="22"/>
<connect gate="TDA8703" pin="23/D3" pad="23"/>
<connect gate="TDA8703" pin="24/D2" pad="24"/>
<connect gate="TDA8703" pin="3/AGND" pad="3"/>
<connect gate="TDA8703" pin="4/VRB" pad="4"/>
<connect gate="TDA8703" pin="5/DEC" pad="5"/>
<connect gate="TDA8703" pin="6/NC" pad="6"/>
<connect gate="TDA8703" pin="7/VCCA" pad="7"/>
<connect gate="TDA8703" pin="8/VI" pad="8"/>
<connect gate="TDA8703" pin="9/VRT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
