<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SSOP48">
</package>
<package name="TQFP44">
</package>
<package name="0603">
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="1206">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
<package name="HC49U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SMB-DIODE">
<description>&lt;b&gt;Diode&lt;/b&gt;&lt;p&gt;
Basic small signal diode good up to 200mA. SMB footprint. Common part #: BAS16</description>
</package>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="MIRF">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="EIA3216">
</package>
<package name="MLP28">
<description>&lt;b&gt;MLP 28&lt;/b&gt;&lt;p&gt;
Source: www.silabs.com .. CP2101.pdf</description>
</package>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-H">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="SWITCH-SPDT">
</package>
<package name="LASSEN_IQ_GPS">
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="SQFP-S-10X10-64">
<description>&lt;b&gt;QFP64&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="ZIF_18POS">
</package>
<package name="SO08-GW">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, gull wing</description>
</package>
<package name="SO08WIDE">
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DIPSWITCH-02">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
<package name="DIPSWITCH-08">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
<package name="DB9">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
<package name="BLUERADIO_BR-C40A">
</package>
<package name="1X08">
</package>
<package name="SO016">
</package>
<package name="SOD323-W">
<description>&lt;b&gt;SOD323 Wave soldering&lt;/b&gt; Philips SC01_Mounting_1996.pdf</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="NOKIA6100_LCD">
</package>
<package name="MMA7260">
</package>
<package name="GND_CONNECT">
</package>
<package name="BATTCON_12MM">
</package>
<package name="LCD-G12864">
</package>
<package name="ALPS_POT">
</package>
<package name="TRIM_POT">
</package>
<package name="SO014">
</package>
<package name="LCD_CFAX">
</package>
<package name="CFAX_CONNECTOR">
</package>
<package name="CFAX_COMBO_CON">
</package>
<package name="LCD_BACKLIGHT_PADS">
</package>
<package name="INDUCTOR-1206">
</package>
<package name="INDUCTOR-0603">
<description>Iductor</description>
</package>
<package name="PAD.02X.02">
</package>
<package name="PAD.03X.03">
</package>
<package name="POWER_JACK_SMD">
</package>
<package name="CAMERA_CMOS_CON">
</package>
<package name="CAMERA_CMOS_PLUG">
</package>
<package name="WLANMODULE">
</package>
<package name="16LPCC">
</package>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
<package name="EMB001">
</package>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
<package name="SD-MMC_SOCKET-PP">
</package>
<package name="ET-301">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED-1206">
</package>
<package name="LED-0603">
</package>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="04P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="05P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="06P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="07P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="08P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="1X07">
</package>
<package name="1X06">
</package>
<package name="1X05">
</package>
<package name="1X04">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
<package name="1X01_LONGPAD">
</package>
<package name="COPERNICUS">
</package>
<package name="1X14">
</package>
<package name="COPERNICUS-DIP">
</package>
<package name="SJ-NC">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJW">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_2W">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="POWER_JACK_SLOT">
</package>
<package name="SCP1000">
</package>
<package name="SO-18W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="SOIC-14">
</package>
<package name="BATTERY-AAA">
</package>
<package name="BATTERY">
<description>&lt;B&gt;BATTERY&lt;/B&gt;&lt;p&gt;
22 mm</description>
</package>
<package name="CR54">
</package>
<package name="EIA3528">
</package>
<package name="BUTTONPAD-2X2">
</package>
<package name="BUZZER-12MM">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
<package name="PIC-ICSP-MINI">
</package>
<package name="BATTERY-AA">
</package>
<package name="1X10">
</package>
<package name="SFE-LOGO">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO018">
</package>
<package name="SO18W">
</package>
<package name="SO18L">
</package>
<package name="MOLEX-1X6">
</package>
<package name="LED-TRICOLOR-SMD">
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="LCC24">
</package>
<package name="MOLEX-1X2">
</package>
<package name="MOLEX-1X4">
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="AXIAL-0.3">
</package>
<package name="TO220-ADJ">
</package>
<package name="TO220-IGO">
</package>
<package name="DIODE-1N4001">
</package>
<package name="B82462G">
</package>
<package name="1X11">
</package>
<package name="1X12">
</package>
<package name="COPERNICUS-TRIMBLE">
</package>
<package name="Q5-DD">
<description>&lt;b&gt;Q5-DD&lt;/b&gt;</description>
</package>
<package name="EIA7343">
</package>
<package name="LQFP-32">
<description>&lt;b&gt;Quad Flat Package&lt;/b&gt; 32 LD LQFP&lt;p&gt;
Source: ds232b12.pdf&lt;br&gt;
http://www.ftdichip.com</description>
</package>
<package name="1X09">
</package>
<package name="CRYSTAL-32KHZ-SMD">
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="SOD-323">
</package>
<package name="SOT23-6">
</package>
<package name="RESONATOR-SMD">
</package>
<package name="LFCSP-16">
</package>
<package name="CAMERA_SFV24R-2ST">
</package>
<package name="CAMERA_SFV24R-2ST_2">
</package>
<package name="USD-SOCKET-PP">
<description>OLD Production Socket. DO NOT USE for production boards.</description>
</package>
<package name="QFN-24">
</package>
<package name="MOLEX-1X3">
</package>
<package name="LQFP32">
<description>&lt;b&gt;LQFP-32 package&lt;/b&gt;&lt;p&gt;
7x7 mm case, 0.8 mm lead pitch</description>
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="POWER_JACK_COMBO">
</package>
<package name="BGB203_ORIGINAL">
</package>
<package name="NAV_SWITCH">
</package>
<package name="Q5-DD_SPX29300">
</package>
<package name="BLUERADIO_BR-C40N">
</package>
<package name="SJ-NO">
</package>
<package name="SHT1X">
<description>&lt;b&gt;SHT1x&lt;/b&gt;
Sensirion Humdity Sensor</description>
</package>
<package name="IDG300">
</package>
<package name="IPOD_FEMALE_CONNECTOR">
</package>
<package name="IPOD_MALE_CONNECTOR">
</package>
<package name="1X15">
</package>
<package name="GE863">
</package>
<package name="SO-24W">
</package>
<package name="SO-28W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="RESONATOR-PTH">
</package>
<package name="SIMHOLDER">
</package>
<package name="BGB203">
</package>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="SCREWTERMINAL-3.5MM-4">
</package>
<package name="1X20">
</package>
<package name="HMC6042">
</package>
<package name="HMC1041Z">
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="TSSOP8">
<description>&lt;b&gt;Plastic Small Outline&lt;/b&gt;</description>
</package>
<package name="AVR_MINI_PROG">
</package>
<package name="EB-85A">
</package>
<package name="ET312">
</package>
<package name="BATTCON_12MM_PTH">
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="CDRH125">
</package>
<package name="1X10-2MM">
</package>
<package name="ANTENNA-CHIP">
</package>
<package name="ANTENNA-CHIP2">
</package>
<package name="ANTENNA-CHIP3">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="BLUETOOTH-SMD-FP">
</package>
<package name="V18ZA2P">
</package>
<package name="MOLEX-1X6-RA">
</package>
<package name="MLX90609">
</package>
<package name="0805">
</package>
<package name="3.3V-DEVICE">
</package>
<package name="BUTTONPAD-1X1">
</package>
<package name="BUTTONPAD-4X4">
</package>
<package name="TEMT6000-SEN">
</package>
<package name="2X5-RA">
</package>
<package name="2X5-RAF">
</package>
<package name="FIDUCIAL">
</package>
<package name="FIDUCIAL-1X2">
</package>
<package name="FIDUCIAL-1X2.5">
</package>
<package name="FIDUCIAL-1.5X3">
</package>
<package name="GR-10">
</package>
<package name="ANTENNA-CHIP4">
</package>
<package name="SOT23-3">
</package>
<package name="BUTTONPAD-2X2SINGLE">
</package>
<package name="BUZZER-CMT1603">
</package>
<package name="SFE-NEW-WEBLOGO">
</package>
<package name="G3VM-61E1">
</package>
<package name="RJ11-6">
</package>
<package name="GM862">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="VIBE-MOTOR-10MM">
</package>
<package name="EM408_CON">
</package>
<package name="ARDUINO-OUTLINE">
</package>
<package name="1X16">
</package>
<package name="BREADBOARD-MINI">
</package>
<package name="NS73M">
</package>
<package name="AUDIO-JACK">
</package>
<package name="MINI-DIN6">
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="LUXEON">
</package>
<package name="LUXEON-PAD">
</package>
<package name="SWITCHE-DPDT">
</package>
<package name="MLP-24">
</package>
<package name="PTC-1206">
</package>
<package name="2X3">
</package>
<package name="BLUETOOTH-INTERNAL-FP">
</package>
<package name="PAD.03X.05">
</package>
<package name="2X5-NS">
</package>
<package name="2X3-NS">
</package>
<package name="BUZZER-CMT1102">
</package>
<package name="SCP1000-LG">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="S4B-PH">
</package>
<package name="KSA_SEALED_TAC_SWITCH">
</package>
<package name="SMTSO-256-ET">
</package>
<package name="B82464-A4">
</package>
<package name="1X02_BIG">
</package>
<package name="JST-2-SMD-VERT">
</package>
<package name="SFE-LOGO-FLAME">
</package>
<package name="SFE-LOGO-FLAME-COPPER">
</package>
<package name="TVSOP-16">
</package>
<package name="ALM-1412">
</package>
<package name="SJ_3">
</package>
<package name="CR75">
</package>
<package name="SI4700/01-GM">
</package>
<package name="2X26">
</package>
<package name="QFN20">
</package>
<package name="BATTCOM_20MM_PTH">
</package>
<package name="BUTTON-CONDUCTIVE">
</package>
<package name="ADJD-S371">
</package>
<package name="HMC1051Z">
</package>
<package name="3362U">
</package>
<package name="FIDUCIAL-1.5X3_BOTTOM">
</package>
<package name="3362U-2">
</package>
<package name="SMTRA-256-8-6">
</package>
<package name="SCA1000">
</package>
<package name="DIODE-1N4148">
</package>
<package name="PQ208">
</package>
<package name="F25D">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25VP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25VB">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25VP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25VB">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="BLUETOOTH-INTERNAL-FP2">
</package>
<package name="LQFP-48">
</package>
<package name="ANTENNA-CHIP5">
</package>
<package name="TSSOP5">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="PQFP208">
</package>
<package name="USB-A-PCB">
</package>
<package name="QFN-28">
</package>
<package name="RMCM01">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="LGA14">
</package>
<package name="MIC-9.7MM">
</package>
<package name="1210">
</package>
<package name="SPM0204UD5">
</package>
<package name="WT32">
</package>
<package name="TSSOP30">
</package>
<package name="EM408_OUTLINE">
</package>
<package name="XBEE-1">
</package>
<package name="1X25">
</package>
<package name="ZUNE_CONNECTOR_MALE">
</package>
<package name="2X12">
</package>
<package name="HMC1051Z_2">
</package>
<package name="HMC1051Z3">
</package>
<package name="R_SW_TH">
</package>
<package name="CNZ1120">
</package>
<package name="LED-0402">
</package>
<package name="NEW">
</package>
<package name="LIGHTPIPE-7511">
</package>
<package name="LIPO-1100">
</package>
<package name="SWITCH-SPST-VERTICAL">
</package>
<package name="LIPO-2000">
</package>
<package name="RCA">
</package>
<package name="SOT-23-6">
</package>
<package name="SIMHOLDER2">
</package>
<package name="LCC36">
</package>
<package name="ADXLXXX_E8">
</package>
<package name="SOT666">
</package>
<package name="BATT_245MM_TABS">
</package>
<package name="TOUCH-SCREEN">
</package>
<package name="NRF24Z1">
</package>
<package name="QFN-36">
</package>
<package name="TSSOP16">
<description>&lt;b&gt;TSOP16&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
<package name="TOUCH1">
</package>
<package name="TOUCH2">
</package>
<package name="SWITCH-SPDT-SMD">
</package>
<package name="BUTTON-10MM">
</package>
<package name="BUTTON-18MM">
</package>
<package name="LIPO-100">
</package>
<package name="BATTCON_245MM">
</package>
<package name="TSOP48">
</package>
<package name="DIL28-3">
</package>
<package name="BUZZER-12MM-NS">
</package>
<package name="SCA3000">
</package>
<package name="1X06-SMD">
</package>
<package name="TFM-511">
</package>
<package name="BUTTON-CONDUCTIVE-0.1">
</package>
<package name="1X12-2MM">
</package>
<package name="XPORT_DIRECT_MODULE">
</package>
<package name="XPORT">
</package>
<package name="BUTTON-CONDUCTIVE-MINI">
</package>
<package name="LED-TRICOLOR-THROUGHHOLE">
</package>
<package name="MSOP-8">
</package>
<package name="DIL40">
<description>Dual In Line Package: 40-pin PDIP</description>
</package>
<package name="EM406_OUTLINE">
</package>
<package name="ID-12">
<description>ID12 Footprint (works with ID2, ID12, and ID20)</description>
</package>
<package name="RF24G-2X5">
<description>test</description>
</package>
<package name="MN5010HS">
<description>MN5010HS GPS Module</description>
</package>
<package name="SPARKFUN_MOLEX-1X6">
</package>
<package name="SFE-LOGO-FLAME-LARGE">
</package>
<package name="1X01NS">
</package>
<package name="MQ-3">
<description>MQ-3 in Configuration B</description>
</package>
<package name="RJ45-8">
</package>
<package name="QRD1114">
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO-24DW">
<description>300-mil body, package type SO</description>
</package>
<package name="CREATIVE_COMMONS">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="BATTCON_245MM_PTH">
</package>
<package name="XBEE-SILK">
</package>
<package name="LGA28">
<description>Untested fp for LGA28 package</description>
</package>
<package name="RELAY-G5V">
<description>G5Q SPDT Relay (SparkFun SKU: COM-00100). Footprint should also work with SPST-NO relay.</description>
</package>
<package name="RJ9">
<description>Footprint for RJ9 simple connector. Common with telephone handsets. SparkFun SKU: PRT-08694</description>
</package>
<package name="LCD-16X2">
</package>
<package name="RELAY-G5Q">
</package>
<package name="RELAY-T9A">
<description>Big relay. 220V/30A. SparkFun SKU: COM-00101</description>
</package>
<package name="LGA16">
<description>LGA16 for LY530AL</description>
</package>
<package name="1X10-2MM-SMD">
</package>
<package name="XBEE-SMD">
</package>
<package name="USB-B-PTH-VERTICAL">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="DIN7">
</package>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X06_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X01">
</package>
<package name="1X20_LOCK_LONGPADS">
</package>
<package name="LED10MM">
</package>
<package name="MOLEX-1X6_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X11-1.27MM">
<description>Header for the OS4000-T</description>
</package>
<package name="1X05-1.27MM">
<description>Header for OS4000-T</description>
</package>
<package name="1X04-1.27MM">
</package>
<package name="1X02_LOCK">
</package>
<package name="MOLEX-1X2_LOCK">
</package>
<package name="MOLEX-1X3_LOCK">
</package>
<package name="1X07_LOCK">
</package>
<package name="1X03_LOCK">
</package>
<package name="1X04_LOCK">
</package>
<package name="1X05_LOCK">
</package>
<package name="1X08_LOCK">
</package>
<package name="1X09_LOCK">
</package>
<package name="1X10_LOCK">
</package>
<package name="1X11_LOCK">
</package>
<package name="1X12_LOCK">
</package>
<package name="1X14_LOCK">
</package>
<package name="1X15_LOCK">
</package>
<package name="1X16_LOCK">
</package>
<package name="1X05_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X04_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X03_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X02_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X07_LOCK_LONGPADS">
</package>
<package name="1X16_LOCK_LONGPADS">
</package>
<package name="1X15_LOCK_LONGPADS">
</package>
<package name="1X14_LOCK_LONGPADS">
</package>
<package name="1X12_LOCK_LONGPADS">
</package>
<package name="1X11_LOCK_LONGPADS">
</package>
<package name="1X10_LOCK_LONGPADS">
</package>
<package name="1X09_LOCK_LONGPADS">
</package>
<package name="1X08_LOCK_LONGPADS">
</package>
<package name="1X20_LOCK">
</package>
<package name="1X25_LOCK">
</package>
<package name="1X25_LOCK_LONGPADS">
</package>
<package name="MOLEX-1X4_LOCK">
</package>
<package name="MOLEX-1X6-RA_LOCK">
</package>
<package name="TRF-24G-SOCKET">
</package>
<package name="RELAY-T9A-2">
</package>
<package name="ADXL180">
</package>
<package name="1X12_MACHINE-PIN-HEADER_LOCK.004">
</package>
<package name="1X16_MACHINE-PIN-HEADER_LOCK.004">
</package>
<package name="OS4000-T">
<description>Footprint for the OS4000-T</description>
</package>
<package name="2X5-SHROUDED_LOCK">
</package>
<package name="SSOP24">
</package>
<package name="2X10_LOCK">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10_LOCK_SPECIAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X20_LOCK_SPECIAL">
</package>
<package name="JOYSTICK">
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
</package>
<package name="POWER_JACK_PTH_LOCK">
</package>
<package name="MOTOR_MOUNT">
</package>
<package name="1X04-SMD">
</package>
<package name="SOIC18-W">
</package>
<package name="TRIM_POT_PTH">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="TQFP32-5MM">
</package>
<package name="1X06-SIP_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="SWITCH-SPDT_LOCK.007S">
</package>
<package name="1X06_FEMALE_LOCK.010">
</package>
<package name="SCREWTERMINAL-3.5MM-3_LOCK.007S">
</package>
<package name="MICRO-SD-SOCKET-PP">
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="IDG500">
</package>
<package name="LGA44">
<description>LGA44 - Used for Venus GPS</description>
</package>
<package name="MMA7260_REV">
<description>Disregard this package...I hate having to modify footprints in use directly...but I guess there's no other way.
-abe</description>
</package>
<package name="UBW32_TQFP100">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="OPENSERVO_VIA">
</package>
<package name="BC-32">
<description>ADXRS6xx and ADXRS150, 300, and 401</description>
</package>
<package name="7-SEGMENT-DISPLAY">
</package>
<package name="7-SEGMENT-4DIGIT">
</package>
<package name="PHOTOCELL">
</package>
<package name="MAGNET-18MM">
</package>
<package name="TSSOP28">
</package>
<package name="CRYSTAL-SMD-7X5">
</package>
<package name="FRACTUS">
</package>
<package name="PSP_TOUCH_CONNECTOR">
<description>4-Pin connector for PSP touch screen</description>
</package>
<package name="DS_TOUCH_CONNECTOR">
<description>4-pin DS touch screen connector</description>
</package>
<package name="POWERSO20">
</package>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="ANTENNA-CHIP6">
<description>Footprint for Part#1575AT43A40</description>
</package>
<package name="GE864">
</package>
<package name="2X10_NOSILK">
</package>
<package name="DIODE-ZENER">
</package>
<package name="TRANSFORMER">
</package>
<package name="GEIGER_TUBE">
</package>
<package name="ID-12_LOCK">
<description>ID12 Footprint (works with ID2, ID12, and ID20)</description>
</package>
<package name="TRIMPOT_PTH_S3_LOCK">
</package>
<package name="XBEE-1_LOCK">
</package>
<package name="TSOP8523">
</package>
<package name="RN41">
</package>
<package name="ADXL193">
</package>
<package name="GE865">
</package>
<package name="1X13">
</package>
<package name="ATARI_CONNECTOR">
</package>
<package name="QFN-24_ALT1.PAC">
</package>
<package name="GM862_CONNECTOR">
</package>
<package name="1X25_LONGPAD">
</package>
<package name="TRANSFORMER_SMD">
<description>TTC-5023</description>
</package>
<package name="GRM43D">
</package>
<package name="1X01_2MM">
</package>
<package name="SD-MMC-CARD">
</package>
<package name="RCA_LOCK">
</package>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="NIPPON_F80">
</package>
<package name="7-SEGMENT-1&quot;PTH">
<description>7 Segment display Storefront SKU#: COM-08546</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="DUEMILANOVE_SHIELD">
</package>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X5-SHROUDED">
</package>
<package name="U.FL">
</package>
<package name="1X27">
</package>
<package name="SIMHOLDER3">
</package>
<package name="1X17">
</package>
<package name="1X19">
</package>
<package name="LPCC20">
</package>
<package name="TSSOP20">
</package>
<package name="1X02_LONGPADS">
</package>
<package name="BNC">
<description>Fits Mouser Part#5227161</description>
</package>
<package name="1X01_TURRET">
<description>0.08" Drill, 0.13" tDoc</description>
</package>
<package name="FRIST_LOGO">
</package>
<package name="DIL28-3-SIMON">
</package>
<package name="DC-DC_CONVERTER">
</package>
<package name="GP1A57HR">
</package>
<package name="XPORT_DIRECT_MODULE-SMD">
</package>
<package name="RN-131G">
</package>
<package name="HTCUSB">
</package>
<package name="1X14-LONGPADS">
</package>
<package name="1X13-LONGPADS">
</package>
<package name="MSS12">
</package>
<package name="MSS22">
<description>MSS22 DPDT Switch</description>
</package>
<package name="DIODE-HV">
</package>
<package name="SO20W">
<description>20 pin soic package that should fit both wide and narrow, UNPROOVEN</description>
</package>
<package name="CMA3000-A01">
</package>
<package name="CMA3000">
</package>
<package name="ODFN6">
</package>
<package name="SO28-EIAJ">
<description>SOIC 28 pin EIAJ (5.3mm wide) packages</description>
</package>
<package name="TRACKBALL">
</package>
<package name="SC70">
</package>
<package name="WIFLY_GSX">
</package>
<package name="CRYSTAL-SMD-7.5X5.2-6PIN">
<description>FXO-HC73 Series Oscillator. 7.5x5.2mm 6-pin package</description>
</package>
<package name="SM5100B">
</package>
<package name="SSOP16">
</package>
<package name="SPARKFUN_TACTILE_SWITCH_SMD-2">
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="TACTILE_SWITCH_SMD-2">
</package>
<package name="SPARKFUN_IDG500">
</package>
<package name="QFN-24_ALT1">
</package>
<package name="QFN-28_6X8">
<description>QFN package with a 6x8 pin configuration.</description>
</package>
<package name="MICRO-SDCARD">
</package>
<package name="BANANA_CONN">
</package>
<package name="MEMS-MIC">
</package>
<package name="LED-TRICOLOR-PTH_SPECIAL">
</package>
<package name="BUTTONPAD-4X4-SPECIAL">
</package>
<package name="SMARTCARD">
<description>&lt;b&gt;Description:&lt;/b&gt; S..m..r..t. I am so smrt!</description>
</package>
<package name="LIPO-1100MAH">
</package>
<package name="BUTTONPAD-2X2-SPECIAL">
</package>
<package name="SQFP-S-10X10-64-XS1">
</package>
<package name="PLASTIC_SMALL_OUTLINE">
</package>
<package name="SOT563">
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="USB-A-S-NOSILK">
</package>
<package name="1X01_OFFSET">
</package>
<package name="1X05_LONGPADS">
</package>
<package name="ST-GYRO">
</package>
<package name="CRYSTAL-32KHZ-SMD_EPSON_MC146">
</package>
<package name="2X3_OFFSET">
</package>
<package name="1X08_LONGPADS">
</package>
<package name="DIL28-3-ZIF_SOCKET">
</package>
<package name="SOT363">
</package>
<package name="DPAK">
</package>
<package name="JOYSTICK-PSP1000">
</package>
<package name="SOT89">
</package>
<package name="PAD-1.5X4.5">
</package>
<package name="TCM8240MD">
</package>
<package name="2X4">
</package>
<package name="ID-12_SMD">
<description>ID12 Footprint (works with ID2, ID12, and ID20)</description>
</package>
<package name="1007">
<description>1007 (2518 metric) package</description>
</package>
<package name="PANASONIC_D">
</package>
<package name="BATTERY-AA-PANEL">
</package>
<package name="NUBBIN_LOCKER">
</package>
<package name="SC70-6">
</package>
<package name="2X8">
</package>
<package name="SIT8002">
</package>
<package name="1X11_SMD_PTHCOMBO">
</package>
<package name="GS406SMD">
<description>50 Channel GS406 Helical GPS Receiver - SMD Connector

sku: GPS-09079</description>
</package>
<package name="RESONATOR-WIDE-SMD">
</package>
<package name="QRE1113">
</package>
<package name="CRYSTAL-SMD-10.5X4.8-2PIN">
</package>
<package name="1X06_LONGPADS">
</package>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="1X24">
</package>
<package name="1X24_LONGPADS">
</package>
<package name="XTEND-DIGI-MODEM">
<description>Package for the Xtend Digi Modem 40 mile range</description>
</package>
<package name="7-SEGMENT-4DIGIT-YOUNGSUN">
<description>This is a package for the 4-digit 7-segment RED LED from Young Sun.</description>
</package>
<package name="2_LEAD_RESONATOR">
</package>
<package name="RESONATOR_NOCAP">
</package>
<package name="1X07_LONGPADS">
</package>
<package name="TO-220-11LEAD">
<description>TO-220 11 Pin Package</description>
</package>
<package name="1X18">
</package>
<package name="MULTIWATT15V">
<description>Multiwatt15V package for the L298 dual full bridge driver</description>
</package>
<package name="MULTIWATT15">
<description>Multiwatt15V package for the L298 dual full bridge driver</description>
</package>
<package name="TQFP-100-14X14MM">
</package>
<package name="1X01_POGOPIN_HOLE_LARGE">
</package>
<package name="DIN_5_FEMALE">
</package>
<package name="CPOL-RADIAL-1000UF-63V">
</package>
<package name="MS">
<description>Series S Slide Switch</description>
</package>
<package name="ES">
<description>Right Angle Slide Switch. Works with part#ES21MABE</description>
</package>
<package name="OS">
</package>
<package name="SSOP20-LONG">
<description>SSOP-20PIN Do Not Use as this is for the silkscreen of the breakout board for 20pin-SSOP ICs</description>
</package>
<package name="HIH-4030">
<description>HIH-4030 Humidity Sensor</description>
</package>
<package name="OVERTONE_LOGO">
</package>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
<package name="TQFP64">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 10x10x1mm Body, 2mmFP</description>
</package>
<package name="DIL40-6-ZIF_SOCKET">
</package>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
<package name="FFC_16">
</package>
<package name="SLIDER">
</package>
<package name="DUEMILANOVE_VIAS">
</package>
<package name="1X16_LONGPADS">
</package>
<package name="1X04_LONGPADS">
</package>
<package name="1X09_LONGPADS">
</package>
<package name="1X06-SMD_EDGE">
</package>
<package name="SM5100B-SPECIAL_FOR_TESTING">
</package>
<package name="DIN_5_FEMALE_SUPPORT">
</package>
<package name="8-SMD">
</package>
<package name="6400BG_HEATSINK">
</package>
<package name="MULTIWATT15_6400BGHEATSINK">
</package>
<package name="YB324G_HEATSINK">
</package>
<package name="MULTIWATT15_YB324GHEATSINK">
</package>
<package name="SOIC-28">
</package>
<package name="VISHAY_C">
</package>
<package name="SCREWTERMINAL-3.5MM-6">
</package>
<package name="SCREWTERMINAL-3.5MM-8">
</package>
<package name="CRYSTAL-OSC-SMD-5X3">
</package>
<package name="LED-TRICOLOR-PTH-SQUARE">
<description>RGB LED used in 3x3x3 LED Cube Kit</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="SPARKFUN_1X02_NO_SILK">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="1X04_NO_SILK">
</package>
<package name="EG2211">
</package>
<package name="TACTILE-PTH-12MM">
</package>
<package name="LITTLEBITS">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="FUSE_5MM">
</package>
<package name="LITTLE_BITS_MALE">
</package>
<package name="LITTLE_BITS_FEMALE">
</package>
<package name="MULTIWATT15_6400BGHEATSINK_2">
</package>
<package name="DUEMILANOVE_SHIELD_NOHOLES">
</package>
<package name="LUXEON-REBEL">
</package>
<package name="QFN-24-USB">
</package>
<package name="1X06-SMD-FEMALE">
</package>
<package name="QFN-20-0.4MM">
<description>** 20-pin QFN ** 
initially designed for MPR121 | 
0.4mm pitch | 
3x3x0.65mm |
** VERY UNPROVEN **</description>
</package>
<package name="USB-MINIB-NOSTOP">
</package>
<package name="SCREENKEYMATINGCONNECTOR">
</package>
<package name="1X11_LONGPADS">
</package>
<package name="FUNNEL_LOGO_BOTTOM">
</package>
<package name="FUNNEL_LOGO_BOTTOM_V2">
</package>
<package name="BMP085">
</package>
<package name="DIL14">
</package>
<package name="POT_ALPHA_RV16AF-20">
<description>Package for Alpha RV16AF-20 potentiometer</description>
</package>
<package name="TQFP64_14X14MM">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 14x14x1mm Body</description>
</package>
<package name="MPL115A">
</package>
<package name="LGA28L">
</package>
<package name="BATTERY_20MM_PTH_COMPACT">
</package>
<package name="MICRO-B-RA-SMT">
<description>Package for an SMT Micro-B connector.  Digikey part #H11613-ND
*** Unproven***</description>
</package>
<package name="LGA12">
</package>
<package name="DUEMILANOVE_SHIELD_LONGPADS">
</package>
<package name="2X5-SHROUDED_SMD">
</package>
<package name="TO-PMOD-7">
<description>7-Lead package for National voltage switchers (LMZ14203)</description>
</package>
<package name="7-SEGMENT-4DIGIT_LONGPADS_FOR_POGOBED">
</package>
<package name="M25D">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="LGA28-5X5">
</package>
<package name="SFE-NEW-WEB">
</package>
<package name="QFN-64">
<description>QFN package with a 6x8 pin configuration.</description>
</package>
<package name="BALUN">
</package>
<package name="SWITCH-4PDT-CNK">
</package>
<package name="R2512">
</package>
<package name="DUEMILANOVE_SHIELD_NOLABELS">
</package>
<package name="ADMP401">
</package>
<package name="USB-A-S-SILK-FEMALE">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
<package name="TO-39">
</package>
<package name="COOPER_UP4B">
</package>
<package name="DOIDE-DO-214">
</package>
<package name="PANASONIC_H13">
</package>
<package name="AXIAL-5MM">
</package>
<package name="SOIC-18">
</package>
<package name="TQFP-100-12X12MM">
</package>
<package name="7-SEGMENT-4DIGIT-YOUNGSUN-LONGPADS">
</package>
<package name="ZG2100M">
</package>
<package name="DIL06">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="OBDII">
<description>OBDII Connector footprint, for your late model automotive needs</description>
</package>
<package name="LIS331">
</package>
<package name="2X3_LOCK">
</package>
<package name="PSP_CONNECTOR">
</package>
<package name="1X12_LONGPADS">
</package>
<package name="MSOP-10-GNDPAD">
<description>10-lead MSOP w/ center GND pad</description>
</package>
<package name="CDRH3D28">
</package>
<package name="SOLARBIT-12X1">
</package>
<package name="SCREENKEY-TFT128">
</package>
<package name="1X03_LONGPADS">
</package>
<package name="LCD-16X2_NOSILK">
</package>
<package name="LGA8">
<description>&lt;h4&gt;LGA8 Package&lt;/h4&gt; &lt;B&gt;**UNPROVEN**&lt;/b&gt;
&lt;ul&gt;&lt;li&gt; 5.0x3.0x1.2mm&lt;/li&gt;
&lt;li&gt;8-pad&lt;/li&gt;&lt;br&gt;&lt;/ul&gt;
Used in MPL115A1 -</description>
</package>
<package name="ADNS2610">
</package>
<package name="DUEMILANOVE_SHIELD_NOHOLES_NOLABELS">
</package>
<package name="SUP500F">
</package>
<package name="MICRO-B-RA-TH">
<description>&lt;h3&gt;Micro B Right Angle through-hole PCB plug connector&lt;/h3&gt;
&lt;b&gt;**Unproven**&lt;/b&gt;&lt;br&gt;
See digikey part #H11673TR-ND</description>
</package>
<package name="MICRO-B-TH">
<description>&lt;h3&gt;Micro B USB Plug Assembly - Straight Through-hole&lt;/h3&gt;
&lt;b&gt;**UNPROVEN**&lt;/b&gt;&lt;Br&gt;
See Digikey part #H11497-ND</description>
</package>
<package name="ADMP421">
</package>
<package name="JST-3-PTH">
</package>
<package name="JST-4-PTH">
</package>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
<package name="SJ_3_PASTE1&amp;2">
</package>
<package name="SJ_3_PASTE2&amp;3">
</package>
<package name="SJ_2S-NOTRACE">
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="1X40">
</package>
<package name="1X40_OFFSET">
</package>
<package name="CTZ3">
<description>CTZ3 Series land pattern for variable capacitor - CTZ3E-50C-W1-PF</description>
</package>
<package name="GS406-MATING_SMD_***SPECIAL">
</package>
<package name="EIA6032">
</package>
<package name="ARDUINO_MINI">
</package>
<package name="RELAY-JZC">
</package>
<package name="1X01_POGOPIN_HOLE_0.58">
</package>
<package name="MICRO-B-SMT">
<description>&lt;h3&gt;USB Micro-B Plug Connector&lt;/h3&gt;
Manufacturer part #: ZX80-B-5SA&lt;br&gt;
Manufacturer: Hirose&lt;br&gt;&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt; (Passed 1:1 printout test though!)</description>
</package>
<package name="STEREOJACK2.5MM_STEREOJACK2.5MM">
</package>
<package name="LCD-16X2_NOHOLES">
</package>
<package name="BTM182">
<description>BTM-182 Class2 Bluetooth Module from Rayson</description>
</package>
<package name="50-PIN-CENTRONICS-F">
</package>
<package name="50-PIN-CENTRONICS-M">
</package>
<package name="QRB1114">
</package>
<package name="QRB1114-SIDE">
</package>
<package name="1X05-1MM">
</package>
<package name="RF-LINK_TX">
<description>RF-LINK transmitters WRL-8945, 8946</description>
</package>
<package name="RF-LINK_RX">
<description>RF-LINK receivers WRL-8947, 8948, 8949, 8950</description>
</package>
<package name="3386U">
<description>&lt;h3&gt;TSR-3386U Trimpot&lt;/h3&gt;
Trimpot with a knob&lt;br&gt;
For COM-09806 in the SparkFun catalog&lt;br&gt;</description>
</package>
<package name="FTDI_BASIC">
</package>
<package name="VNH2SP30">
</package>
<package name="1X02_XTRA_BIG">
</package>
<package name="DB9_MALE">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="1X11_SMD_NO_HOLES">
</package>
<package name="CR75_V2">
</package>
<package name="ALPHANUMERIC">
</package>
<package name="SFE-NEW-WEB-SOLDERMASK">
</package>
<package name="STARBOARD_GROUND_SMALL">
</package>
<package name="STARBOARD_GROUND_WIDE">
</package>
<package name="STARBOARD_PWR_WIDE">
</package>
<package name="STARBOARD_GROUND_SMALL2">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="1X02_PP_HOLES_ONLY">
</package>
<package name="1X03_PP_HOLES_ONLY">
</package>
<package name="1X07_HOLES_ONLY">
</package>
<package name="1X06_HOLES_ONLY">
</package>
<package name="1X11_HOLES_ONLY">
</package>
<package name="1X12_HOLES_ONLY">
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.8">
<description>2W Resistor, 0.8" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="LS20126">
<description>&lt;h3&gt;LS20126 GPS Receiver&lt;/h3&gt;
Package for LOCOSYS LS20126 GPS smart antenna module.&lt;br&gt;
SparkFun Sku# GPS-09838&lt;br&gt;&lt;br&gt;
Note: PCB cannot extend past top tPlace border @ 25mm&lt;br&gt;
&lt;b&gt;Unproven!&lt;/b&gt;&lt;br&gt;</description>
</package>
<package name="SC-70">
</package>
<package name="SCREWTERMINAL-5MM-3">
</package>
<package name="1X03_LOCK_NO_SILK">
</package>
<package name="SCREWTERMINAL-3.5MM-4_LOCK">
</package>
<package name="TRIMPOT_TC33">
</package>
<package name="DRC-10">
<description>&lt;h3&gt;10-pin QFN/SON package&lt;/h3&gt;
Package Type: SON&lt;br&gt;
Package Drawing: DRC&lt;Br&gt;
Pitch: 0.5mm&lt;br&gt;
Overall Dimensions: 3.15x3.15mm&lt;br&gt;
Pins: 10 (+1 exposed heatsink pin)&lt;br&gt;
&lt;br&gt;Related ICs:&lt;ul&gt;&lt;li&gt; TI's BQ2402x - http://focus.ti.com/lit/ds/symlink/bq24023.pdf&lt;br&gt;
&lt;/ul&gt;

Last modified: 8/16/10&lt;br&gt;
&lt;B&gt;Unproven!!!&lt;/B&gt;&lt;br&gt;</description>
</package>
<package name="MSOP-10">
</package>
<package name="STEREOJACK2.5MM_SPECIA_POGOPINS">
</package>
<package name="STEREOJACK2.5MM_SPECIAL_HOLES-ONLY">
</package>
<package name="_STN_SCANTOOL_QFN-28-S">
<description>&lt;H1&gt;Quad Flat No Leads package, 28 pin&lt;/H1&gt;
  &lt;tr
&lt;table align=left&gt;
  &lt;tr&gt;&lt;td&gt;&lt;h2&gt;Change Log&lt;/h2&gt;&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;
    &lt;th&gt;Date&lt;/th&gt;&lt;th&gt;Author&lt;/th&gt;&lt;th&gt;Change&lt;/th&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 23, 2010&lt;/td&gt;&lt;td&gt;joe@scantool.net&lt;/td&gt;&lt;td&gt;Added t-keepout layer.&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 22, 2010&lt;/td&gt;&lt;td&gt;engineering@scantool.net&lt;/td&gt;&lt;td&gt;Resized per PIC24HJ64GPx02 (QFN-S) datasheet. Fixed tStop and tCream layers. Redesigned silkscreen.&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 17, 2010&lt;/td&gt;&lt;td&gt;vitaliy@scantool.net&lt;/td&gt;&lt;td&gt;Verified package.&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 17, 2010&lt;/td&gt;&lt;td&gt;jason@scantool.net&lt;/td&gt;&lt;td&gt;Increased silkscreen ratio.&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 02, 2010&lt;/td&gt;&lt;td&gt;jason@scantool.net&lt;/td&gt;&lt;td&gt;Copied from Microchip Library.&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;</description>
</package>
<package name="SO08-EPAD">
</package>
<package name="V-REG_DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 369C-01&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM317M-D.PDF</description>
</package>
<package name="ODFN">
<description>ODFN: 1.5mm x 1.5mm. Used on the Si1120</description>
</package>
<package name="TSSOP-24">
<description>&lt;h3&gt;24-pin TSSOP with Exposed Thermal Pad&lt;/h3&gt;
Used on: &lt;ul&gt;
&lt;li&gt;Allegro A6282 16-bit LED driver&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/21/10&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;&lt;br&gt;</description>
</package>
<package name="QFN-24_ALT2">
<description>&lt;h3&gt;24-pin QFN with Exposed Thermal pad&lt;/h3&gt;
Parts that use this package:
&lt;ul&gt;
&lt;li&gt;A6282&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/20/10&lt;br&gt;
&lt;br&gt;
&lt;b&gt;***UNPROVEN***&lt;/b&gt;&lt;BR&gt;</description>
</package>
<package name="QFN-28-S">
<description>&lt;h1&gt;Quad Flat No Leads package, 28 pin&lt;/h1&gt;</description>
</package>
<package name="SPARKFUN_JOYSTICK_MINI">
</package>
<package name="JOYSTICK_MINI">
</package>
<package name="QFN-10_PAD">
</package>
<package name="SM130">
<description>30-pin DIL with 100mil spacing between headers</description>
</package>
<package name="STEREOJACK2.5MM_SMD">
</package>
<package name="FKIT-RIBBON_CONNECTOR_03_2MM_L">
</package>
<package name="FKIT-RIBBON_CONNECTOR_03_2MM_R">
</package>
<package name="FKIT-LOGO_MEDIUM">
</package>
<package name="FKIT-LOGO_SMALL">
</package>
<package name="FKIT-LOGO_VERY_SMALL">
</package>
<package name="JST-2-PTH">
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS">
</package>
<package name="JST-2-PTH-NS">
</package>
<package name="LED_PIRANHA_5MM">
</package>
<package name="FKIT-LED-1206">
</package>
<package name="FKIT-LOGOTYPE_SMALL">
</package>
<package name="FKIT-LOGOTYPE_VERY_SMALL">
</package>
<package name="FKIT-LOGOTYPE_MEDIUM">
</package>
<package name="LED3MM-NS">
<description>&lt;h3&gt;LED 3MM - No Silk&lt;/h3&gt;
3 mm, round</description>
</package>
<package name="CDRH2D09">
<description>1.3x1.3mm 1.7mm between. Fits Sumida CDRH2D09, CDRH2D18 inductor</description>
</package>
<package name="BATTCON_20MM">
</package>
<package name="DS3234">
</package>
<package name="REED_SWITCH_PTH">
</package>
<package name="PIC24FXXX_TQFP64">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 10x10x1mm Body, 2mmFP</description>
</package>
<package name="SSOP-4">
</package>
<package name="STARBOARD_GROUND">
</package>
<package name="STARBOARD_PWR">
</package>
<package name="SOIC8">
</package>
<package name="STARBOARD_LOGO">
</package>
<package name="STARBOARD_LOGO_TEXT">
</package>
<package name="WIZ811MJ">
<description>&lt;h3&gt;WIZnet W5100 Network Module with MagJack - WIZ811MJ&lt;/h3&gt;
WIZnet's WIZ811MJ is a breakout board for the W5100 embedded TCP/IP chip. Also included on the board is a RJ-45 MagJack Connector (RJ45 with X'FMR).&lt;br&gt;&lt;br&gt;

See http://www.sparkfun.com/commerce/product_info.php?products_id=9473 for more documentation and info.&lt;br&gt;
&lt;B&gt;**UNPROVEN&lt;/b&gt;</description>
</package>
<package name="XLR3_NC3FAH2">
</package>
<package name="FKIT-SNAP_FEMALE">
</package>
<package name="FKIT-SNAP_MALE">
</package>
<package name="FKIT-LIR2450-H">
</package>
<package name="1X06-SMD-FEMALE-V2">
<description>Package for 4UCONN part #19686 *UNPROVEN*</description>
</package>
<package name="PSOP-8">
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="1X06_SMD_STRAIGHT">
</package>
<package name="1X06_SMD_STRAIGHT_ALT">
</package>
<package name="1X08_SMD_ALT">
</package>
<package name="1X08_SMD">
</package>
<package name="LGA16-3MM">
<description>LGA16 (3x3x1mm)</description>
</package>
<package name="QFN-28-5MM">
</package>
<package name="CSP-9">
</package>
<package name="DPAK-5">
<description>DPAK 5, center lead crop, case 175AA</description>
</package>
<package name="EN_J2">
<description>Type J2 package for SMD supercap PRT-10317 (p# EEC-EN0F204J2)</description>
</package>
<package name="ADH8066">
<description>FP for ADH8066 cell modules. Uses 50-pin connector with 0.5mm pitch Hirose part# DF12(3.0)-50DP-0.5V</description>
</package>
<package name="FFC26">
<description>&lt;b&gt;26-pin FFC connector&lt;/b&gt;
&lt;br&gt;See 4UCONN part #08630</description>
</package>
<package name="DCM01">
</package>
<package name="1X06_SMD_STRAIGHT_COMBO">
</package>
<package name="SOP-14">
<description>&lt;h3&gt;14-pin SOP-14 package&lt;/h3&gt;
Used on WS2801 RGB controller</description>
</package>
<package name="LED-TRICOLOR-5050">
<description>&lt;H3&gt;5050 SMD RGB LED&lt;/h3&gt;
5.0mm x 5.0mm, 2.6mm thickness</description>
</package>
<package name="1X08_SMD_COMBINED">
</package>
<package name="LQFP-80">
<description>&lt;h3&gt;LQFP-80&lt;/h3&gt;
80-pin, 10x10mm, 0.4mm pitch, SMD package&lt;br&gt;
Used for WIZnet W5100 (COM-09471)&lt;br&gt;
http://www.sparkfun.com/products/9471
&lt;br&gt;&lt;br&gt;
&lt;b&gt;***UNPROVEN***&lt;/b&gt;</description>
</package>
<package name="TO-220-ALT">
</package>
<package name="MAGJACK">
</package>
<package name="1X04-1MM-RA">
</package>
<package name="1X05-1MM-RA">
</package>
<package name="SI470X">
</package>
<package name="OSHW-LOGO-S">
</package>
<package name="ATX24_RIGHT_ANGLE">
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
<package name="NPI75C">
</package>
<package name="CAPSENSE_PAD">
</package>
<package name="AUDIO-JACK-3.5MM-SMD">
</package>
<package name="LGA16-4X4">
<description>&lt;h3&gt;16-pin LGA Package&lt;/h3&gt;
4x4x1.1mm&lt;br&gt;
0.65mm pitch&lt;br&gt;
4pins-by-4pins&lt;br&gt;
&lt;br&gt;
Package used by L3G4200D 3-axis gyro&lt;br&gt;
&lt;br&gt;
&lt;B&gt;***UNPROVEN***&lt;/b&gt;</description>
</package>
<package name="MAGJACK-19938">
</package>
<package name="GS1011MXX">
<description>SMD GS1011Mxx</description>
</package>
<package name="CAP-PTH-SMALL-KIT">
</package>
<package name="AXIAL-0.3-KIT">
</package>
<package name="SWITCH-SPDT_KIT">
</package>
<package name="DIL28-3-SIMON-KIT">
</package>
<package name="D2PACK/A">
<description>&lt;h3&gt;D&lt;sup&gt;2&lt;/sup&gt;PAK/A V-reg Package&lt;/h3&gt;
3-pins w/ tab&lt;br&gt;&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;b&gt;Used on:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;LD1085xx Adjustable 3A Regulator
&lt;/ul&gt;</description>
</package>
<package name="QFN-32">
<description>&lt;h3&gt;QFN 32-Pin package w/ Thermal Pad&lt;/h3&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
&lt;B&gt;Applicable Parts:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;TLC5940&lt;/ul&gt;</description>
</package>
<package name="TSSOP28-GROUNDPAD">
</package>
<package name="DFN-10">
<description>10-pin DFN, 2mm x 2mm x 0.85mm</description>
</package>
<package name="TDFN-8">
<description>TDFN - 8pin, 2mmx3mm</description>
</package>
<package name="TRIMPOT-3MM">
</package>
<package name="SRU5028">
</package>
<package name="QFN16-4X4">
<description>&lt;b&gt;16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9mm Body [QFN]&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41203E.pdf</description>
</package>
<package name="MIC_ELECTRET_SMD">
</package>
<package name="LED5MM-KIT">
</package>
<package name="TO-92-KIT">
</package>
<package name="PTC">
</package>
<package name="JST-3-SMD">
</package>
<package name="TACTILE_SWITCH_TALL">
</package>
<package name="TQFP100">
<description>&lt;b&gt;100-lead Thin Quad Flat Pack Package Outline&lt;/b&gt;</description>
</package>
<package name="BM08B-SRSS-TB">
<description>JST crimp connector: 1mm pitch, top entry</description>
</package>
<package name="FIDUCIALTAB">
<description>This is half of a tab, with fiducial reference mark, used to connect individual boards in a panel of PCBs.
Two of these half tabs, rotated in opposite directions, can be connected together to form a full tab, with two fiducial markings. Place along the edge of a panel of PCBs, this will allow for panels with boards not connected by v-scores, which allows for easier depanelization where there are overhanging components. It can also be used for designs too small to accomodate fiducial marks on individual boards.</description>
</package>
<package name="RELAY-S108T02">
</package>
<package name="OSHW-LOGO-M">
</package>
<package name="OSHW-LOGO-L">
</package>
<package name="1X03-1MM-RA">
</package>
<package name="TSSOP-16">
</package>
<package name="LED_RING">
<description>&lt;h3&gt;LED Ring&lt;/h3&gt;
http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Components/LED/Top-Up%20LED%20Ring%20LED-CCL-A.pdf&lt;br&gt;</description>
</package>
<package name="LCD-8X2">
<description>&lt;h3&gt;8x2 Character LCD w/ Backlight&lt;/h3&gt;
Outer Dimensions: 40.0 x 35.4mm&lt;br&gt;
Viewing Area: 26.4 x 13.9mm&lt;br&gt;
Character Size: 2.95 x 4.75mm&lt;br&gt;
&lt;br&gt;
For Reference, see Amotec Display part ADM0802A (http://amotec-display.com/pdf/ADM0802A.pdf).
&lt;br&gt;
&lt;br&gt;
&lt;B&gt;***Footprint Unproven***&lt;/b&gt;</description>
</package>
<package name="LCD-8X2-KIT">
</package>
<package name="PHOTOCELL-KIT">
</package>
<package name="BUZZER-12MM-NS-KIT">
</package>
<package name="SJ_2S-NO-NS">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="JST-2-PTH-KIT">
</package>
<package name="1X06-KIT">
</package>
<package name="EM406">
</package>
<package name="REED_SWITCH_PLASTIC">
</package>
<package name="LGA28-4X5">
</package>
<package name="ENCODER_LED_2">
<description>&lt;h3&gt;2-color Illuminated Rotary Encoder&lt;/h3&gt;</description>
</package>
<package name="TO-92-AMMO">
</package>
<package name="ARDUINO_MEGA">
<description>Full Arduino MEGA footprint</description>
</package>
<package name="ARDUINO_MEGA-PRO-3.3V">
<description>Arduino Mega Pro footprint</description>
</package>
<package name="GPI-152-3013">
<description>Switch with part number: GPI-152-3013</description>
</package>
<package name="RS9110-N-11-22-SHORT">
<description>Redpine WiFi module: short FP (doesn't include the NC pads around the antenna)</description>
</package>
<package name="CAP-PTH-LARGE">
</package>
<package name="SWITCH-SPST-SMD-A">
</package>
<package name="BATTCON_20MM_4LEGS">
</package>
<package name="DIL24">
</package>
<package name="QFN-16">
</package>
<package name="RPACK-SIP-PTH-5">
</package>
<package name="LED_BARGAPH_10">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT143">
<description>&lt;h3&gt;SOT143&lt;/h3&gt;
Package is used for the STM811 (also APX811)&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Proven&lt;/b&gt;</description>
</package>
<package name="MAGJACK-POE">
<description>&lt;h3&gt;PoE Compatible MagJack&lt;/h3&gt;
This RJ-45 jack with magnetics has 10 pins, gives you access to the unused twisted pair (10BASE-T, and 100BASE-T) which usually carries power in a power-over-ethernet system.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Footprint is Proven&lt;/b&gt;</description>
</package>
<package name="SNAP-FEMALE">
</package>
<package name="SNAP-MALE">
</package>
<package name="VCNL4000">
<description>&lt;h3&gt;VCNL4000 Footprint&lt;/h3&gt;
For Vishay VNCL4000 proximity and ambient light sensor.&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Unproven&lt;/b&gt;</description>
</package>
<package name="BATTERY-AA-KIT">
</package>
<package name="BUTTONPAD-2X2SINGLE-KIT">
</package>
<package name="MICRO-FIDUCIAL">
</package>
<package name="DIL-08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="VENUS638FLPX">
</package>
<package name="MSOP-8-EP">
</package>
<package name="SRU1038">
</package>
<package name="CR54-KIT">
</package>
<package name="SMA-DIODE_ALT">
</package>
<package name="SMA-DIODE-KIT">
</package>
<package name="EIA3528-KIT">
</package>
<package name="EIA3216-KIT">
</package>
<package name="BUZZER-CCV">
</package>
<package name="BUZZER-CCV-KIT">
</package>
<package name="QFN-16_0.5MM">
<description>&lt;h3&gt;QFN-16 0.5mm Pitch&lt;/h3&gt;
3 x 3mm Outline&lt;br&gt;
16-pin&lt;br&gt;
Used on the MMA8452Q accelerometer&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Unproven&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Layout in accordance with App note AN4077&lt;br&gt;
http://cache.freescale.com/files/sensors/doc/app_note/AN4077.pdf</description>
</package>
<package name="TRIMPOT-3MM-2">
</package>
<package name="SO08-MAX6675">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="POT_MAMMOTH">
</package>
<package name="QFN-16-(ROUNDED0THERMAL-PAD)">
</package>
<package name="RFM22-XXX-S2">
<description>Package for Hope RF s RFM22-xxx-S2 SMD wireless transciever, xxx is module s frequency band.
*Unproven*''</description>
</package>
<package name="QFN-44">
</package>
<package name="QFN-44-NOPAD">
</package>
<package name="ANDROID-ELECTRIC_SHEEP_LOGO">
</package>
<package name="ANDROID-ELECTRIC_SHEEP_LOGO_SMALL">
</package>
<package name="GP-2106">
</package>
<package name="POT_PTH">
</package>
<package name="SPRINGTERMINAL-2.54MM-2">
</package>
<package name="SWITCH-SP3T-SMD">
</package>
<package name="SOT353">
<description>&lt;h3&gt;SOT353 aka SC70-5&lt;/h3&gt;
Used on single circuit logic gates</description>
</package>
<package name="ENCODER_LED_RGB">
</package>
<package name="P8X32A-Q44">
</package>
<package name="4X0402ARV341">
<description>&lt;b&gt;Array chip resistor&lt;/b&gt; size 4 × 0402&lt;p&gt;
Source: http://docs-europe.electrocomponents.com/webdocs/0114/0900766b80114d99.pdf</description>
</package>
<package name="0603-ARC">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
concave termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
<package name="0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
<package name="CAT16">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
<package name="CAY16">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
<package name="EXB18V">
<description>&lt;b&gt;Chip Resistor Array 0201x4&lt;/b&gt; 4 resistors in 1.4 mm x 0.6 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXB28V">
<description>&lt;b&gt;Chip Resistor Array 0402x4&lt;/b&gt; 4 resistors in 2.0 mm x 1.0 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXB38V">
<description>&lt;b&gt;Chip Resistor Array 0603x4&lt;/b&gt; 4 resistors in 3.2 mm x 1.6 mm size (EXB38V, V8V)&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXBN8V">
<description>&lt;b&gt;Chip Resistor Array 0402x4&lt;/b&gt; 4 resistors in 2.0 mm x 1.0 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXBS8V">
<description>&lt;b&gt;Chip Resistor Array 0805x4&lt;/b&gt; 4 resistors in 5.08 mm x 2.20 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXBV8V">
<description>&lt;b&gt;Chip Resistor Array 0603x4&lt;/b&gt; 4 resistors in 3.20 mm x 1.60 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="YC124">
<description>&lt;b&gt;ARRAY CHIP RESISTOR&lt;/b&gt; Size 4 x 0402&lt;p&gt;
Source: www.yageo.com .. Pu-YC124_51_PbFree_L_1.pdf</description>
</package>
<package name="ENCODER_LED_3">
</package>
</packages>
<symbols>
<symbol name="SSOP48">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
<pin name="P$41"/>
<pin name="P$42"/>
<pin name="P$43"/>
<pin name="P$44"/>
<pin name="P$45"/>
<pin name="P$46"/>
<pin name="P$47"/>
<pin name="P$48"/>
</symbol>
<symbol name="TQFP44">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
<pin name="P$41"/>
<pin name="P$42"/>
<pin name="P$43"/>
<pin name="P$44"/>
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="23-I/O-2">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="VCC@1"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="DIODE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="TPS76433DBVT">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="in"/>
</symbol>
<symbol name="MIRF">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="78ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
</symbol>
<symbol name="AVR_SPI_PROGRAMMER">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="CP2103">
<pin name="REGIN" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VBUS" direction="in"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="!RST"/>
<pin name="SUSPEND" direction="out"/>
<pin name="!SUSPEND" direction="out"/>
<pin name="RI" direction="in"/>
<pin name="DCD" direction="in"/>
<pin name="DTR" direction="out"/>
<pin name="DSR" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="GND@EXP" direction="pwr"/>
<pin name="GND@M" direction="pwr"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
<pin name="GPIO_3"/>
<pin name="VIO" direction="pwr"/>
</symbol>
<symbol name="CP2101">
<pin name="REGIN" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VBUS" direction="in"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="!RST"/>
<pin name="SUSPEND" direction="out"/>
<pin name="!SUSPEND" direction="out"/>
<pin name="RI" direction="in"/>
<pin name="DCD" direction="in"/>
<pin name="DTR" direction="out"/>
<pin name="DSR" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="GND@EXP" direction="pwr"/>
<pin name="GND@M" direction="pwr"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="TOGGLE">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LM4871">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="BYPASS"/>
<pin name="SHUTDWN"/>
<pin name="V02"/>
<pin name="V01"/>
</symbol>
<symbol name="X9015_DIGI_POT">
<pin name="VSS" direction="pwr"/>
<pin name="RW/VW"/>
<pin name="VCC" direction="pwr"/>
<pin name="CS'"/>
<pin name="INC'"/>
<pin name="U/D'"/>
<pin name="RH/VH"/>
<pin name="RL/VL"/>
</symbol>
<symbol name="LASSEN_IQ_GPS">
<pin name="RXA" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="TXA" direction="out"/>
<pin name="PPS" direction="out"/>
<pin name="RXB" direction="in"/>
<pin name="BATT" direction="pwr"/>
<pin name="TXB" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="HV826MG_BACKLIGHT">
<pin name="RSW"/>
<pin name="VA"/>
<pin name="VCC"/>
<pin name="VB"/>
<pin name="CS"/>
<pin name="LX"/>
<pin name="REL" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LPC213X">
<pin name="P1.16(TRACEPKT0)"/>
<pin name="P1.17(TRACEPKT1)"/>
<pin name="P1.18(TRACEPKT2)"/>
<pin name="P1.19(TRACEPKT3)"/>
<pin name="P1.20(TRACESYNC)"/>
<pin name="P1.21(PIPESTAT0)"/>
<pin name="P1.22(PIPESTAT1)"/>
<pin name="P1.23(PIPESTAT2)"/>
<pin name="(MISO0/MAT0.1/A0.7)P0.5"/>
<pin name="(SSEL0/PWM2/EINT2)P0.7"/>
<pin name="(TXD1/PWM4/A1.1)P0.8"/>
<pin name="(RXD1/PWM6/EINT3)P0.9"/>
<pin name="(RTS1/CAP1.0/AD1.2)P0.10"/>
<pin name="(CTS1/CAP1.1/SCL1)P0.11"/>
<pin name="P1.24(TRACECLK)"/>
<pin name="P1.25(EXTIN0)"/>
<pin name="P1.26(RTCK)"/>
<pin name="P1.27(TDO)"/>
<pin name="P1.28(TDI)"/>
<pin name="P1.29(TCK)"/>
<pin name="P1.30(TMS)"/>
<pin name="P1.31(/TRST)"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="(DSR1/MAT1.0/AD1.3)P0.12"/>
<pin name="(DTR1/MAT1.1/AD1.4)P0.13"/>
<pin name="(DCD1/EINT1/SDA1)P0.14"/>
<pin name="(RI1/EINT2/AD1.5)P0.15"/>
<pin name="(EINT0/MAT0.2/CAP0.2)P0.16"/>
<pin name="(CAP1.2/SCK1/MAT1.2)P0.17"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA3" direction="pwr"/>
<pin name="VDD3-1" direction="pwr"/>
<pin name="VDD3-2" direction="pwr"/>
<pin name="VDD3-3" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="(TXD0/PWM1)P0.0"/>
<pin name="(RXD0/PWM3/EINT0)P0.1"/>
<pin name="(SCL0/CAP0.0)P0.2"/>
<pin name="(SDA0/MAT0.0/EINT1)P0.3"/>
<pin name="(SCK0/CAP0.1/AD0.6)P0.4"/>
<pin name="(MOSI0/CAP0.2/AD1.0)P0.6"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="RTXC1" direction="in"/>
<pin name="RTXC2" direction="out"/>
<pin name="(CAP1.3/MISO1/MAT1.3)P0.18"/>
<pin name="(MAT1.2/MOSI1/CAP1.2)P0.19"/>
<pin name="(MAT1.3/SSEL1/EINT3)P0.20"/>
<pin name="(PWM5/AD1.6/CAP1.3)P0.21"/>
<pin name="(AD1.7/CAP0.0/MAT0.0)P0.22"/>
<pin name="P0.23"/>
<pin name="(AD0.4/AOUT)P0.25"/>
<pin name="(AD0.5)P0.26"/>
<pin name="(AD0.0/CAP0.1/MAT0.1)P0.27"/>
<pin name="(AD0.1/CAP0.2/MAT0.2)P0.28"/>
<pin name="(AD0.2/CAP0.3/MAT0.3)P0.29"/>
<pin name="(AD0.3/EINT3/CAP0.0)P0.30"/>
<pin name="P0.31" direction="out"/>
</symbol>
<symbol name="74VHC4052_ANALOG_MUX">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="X3"/>
<pin name="IN/OUT_X"/>
<pin name="X2"/>
<pin name="X1"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="X0"/>
<pin name="Y0"/>
<pin name="Y3"/>
<pin name="IN/OUT_Y"/>
<pin name="A"/>
<pin name="B"/>
<pin name="VEE"/>
<pin name="INH"/>
</symbol>
<symbol name="ATMEL_DATA_FLASH">
<pin name="SCK" direction="in" function="clk"/>
<pin name="SO" direction="out"/>
<pin name="SI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="WP"/>
<pin name="RESET"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="PINH2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="SW_DIP-2">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SW_DIP-8">
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="F09G">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="VCC-GND">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX232">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="BLUERADIO_BR-C40A">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCC"/>
<pin name="SPI_CSB"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="PIO_2/CONNECT" direction="out"/>
<pin name="PIO_3/INT" direction="in"/>
<pin name="PIO_4/FACRST"/>
<pin name="PIO_5/STATUS" direction="out"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="PCM_CLK"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_IN"/>
<pin name="PCM_OUT"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="UART_RTS" direction="out" function="dot"/>
<pin name="UART_CTS" direction="in" function="dot"/>
<pin name="RESET"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="MMA_CON">
<pin name="VCC" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="X" direction="pas" function="dot"/>
<pin name="Y" direction="pas" function="dot"/>
<pin name="Z" direction="pas" function="dot"/>
<pin name="GS1" direction="pas" function="dot"/>
<pin name="GS2" direction="pas" function="dot"/>
<pin name="SLP" direction="pas" function="dot"/>
</symbol>
<symbol name="POWERJACK">
<pin name="GNDBREAK"/>
<pin name="GND"/>
<pin name="PWR"/>
</symbol>
<symbol name="SDCARD">
<pin name="CS"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="GND1"/>
<pin name="DO"/>
<pin name="IRQ"/>
<pin name="WP"/>
<pin name="CD"/>
<pin name="SW"/>
<pin name="SHIELD"/>
<pin name="P9"/>
</symbol>
<symbol name="NOKIA6100_LCD">
<pin name="VDISPLAY"/>
<pin name="VDIGITAL"/>
<pin name="SCK"/>
<pin name="DIO"/>
<pin name="CS"/>
<pin name="GND"/>
<pin name="LEDGND"/>
<pin name="RESET"/>
<pin name="VLED"/>
</symbol>
<symbol name="MMA7260">
<pin name="VCC"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
<pin name="GS1"/>
<pin name="GS2"/>
<pin name="SLP"/>
<pin name="GND"/>
<pin name="PAD"/>
</symbol>
<symbol name="GND_CONNECT">
<pin name="IN"/>
<pin name="AGND"/>
<pin name="DGND"/>
</symbol>
<symbol name="BATTCON_12MM">
<pin name="+"/>
<pin name="+@1"/>
<pin name="-"/>
</symbol>
<symbol name="LM34">
<pin name="V+"/>
<pin name="VOUT"/>
<pin name="GND"/>
</symbol>
<symbol name="AD725">
<pin name="STND"/>
<pin name="AGND"/>
<pin name="4FSC"/>
<pin name="APOS"/>
<pin name="CE"/>
<pin name="RIN"/>
<pin name="GIN"/>
<pin name="BIN"/>
<pin name="HSYNC"/>
<pin name="VSYNC"/>
<pin name="DPOS"/>
<pin name="DGND"/>
<pin name="YTRAP"/>
<pin name="LUMA"/>
<pin name="COMP"/>
<pin name="CRMA"/>
</symbol>
<symbol name="LCD-G12864">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VO"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="R/W" direction="in"/>
<pin name="D/I" direction="in"/>
<pin name="E" direction="in"/>
<pin name="VEE"/>
<pin name="A" direction="pwr"/>
<pin name="K" direction="pwr"/>
</symbol>
<symbol name="POT">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MCP42XXX">
<pin name="A0"/>
<pin name="W0"/>
<pin name="B0"/>
<pin name="A1"/>
<pin name="W1"/>
<pin name="B1"/>
<pin name="SCK"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="SHTDWN"/>
<pin name="RST"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="CS"/>
</symbol>
<symbol name="MCP41XXX">
<pin name="VCC"/>
<pin name="CS"/>
<pin name="SCK"/>
<pin name="DI"/>
<pin name="A"/>
<pin name="W"/>
<pin name="B"/>
<pin name="GND"/>
</symbol>
<symbol name="HV857_BACKLIGHT">
<pin name="VDD"/>
<pin name="RSW"/>
<pin name="REL"/>
<pin name="GND"/>
<pin name="VB"/>
<pin name="VA"/>
<pin name="CS"/>
<pin name="LX"/>
</symbol>
<symbol name="NDS8434">
<pin name="S@1"/>
<pin name="S@2"/>
<pin name="S@3"/>
<pin name="G"/>
<pin name="D@1"/>
<pin name="D@2"/>
<pin name="D@3"/>
<pin name="D@4"/>
</symbol>
<symbol name="MCP73842">
<pin name="SENSE"/>
<pin name="VDD"/>
<pin name="STAT1"/>
<pin name="EN"/>
<pin name="TIMER"/>
<pin name="VSS"/>
<pin name="VBAT"/>
<pin name="DRV"/>
</symbol>
<symbol name="LCD_CFAX">
<pin name="VCC"/>
<pin name="RESET"/>
<pin name="GND"/>
<pin name="CS1B"/>
<pin name="CS2"/>
<pin name="RS"/>
<pin name="RW"/>
<pin name="ERD"/>
<pin name="MI"/>
<pin name="P/S"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
</symbol>
<symbol name="MAX1555">
<pin name="USB"/>
<pin name="GND"/>
<pin name="CHG"/>
<pin name="BATT"/>
<pin name="DC"/>
</symbol>
<symbol name="LCD_BACKLIGHT_PADS">
<pin name="A"/>
<pin name="K"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="FERRITE_BEAD">
<pin name="H1"/>
<pin name="H2"/>
</symbol>
<symbol name="PAD">
</symbol>
<symbol name="MCP130">
<pin name="RESET"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="CAMERA_CMOS_CON">
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
<pin name="Y4"/>
<pin name="Y5"/>
<pin name="Y6"/>
<pin name="Y7"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="ENB"/>
<pin name="RST"/>
<pin name="GND@1"/>
<pin name="VCC@1"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="FVL"/>
<pin name="LVL"/>
<pin name="PCK"/>
<pin name="MCK"/>
</symbol>
<symbol name="WLANMODULE">
<pin name="VSS@0"/>
<pin name="TSI"/>
<pin name="DVDD@0"/>
<pin name="DVDD@2"/>
<pin name="V2.5"/>
<pin name="RFU"/>
<pin name="/RST"/>
<pin name="/TSS"/>
<pin name="G6"/>
<pin name="TSO"/>
<pin name="G3"/>
<pin name="F5"/>
<pin name="G5"/>
<pin name="G4"/>
<pin name="VSS@1"/>
<pin name="VSS@2"/>
<pin name="G2"/>
<pin name="F4"/>
<pin name="G1"/>
<pin name="TSCK"/>
<pin name="G7"/>
<pin name="G0"/>
<pin name="F6"/>
<pin name="F7"/>
<pin name="F0"/>
<pin name="F3"/>
<pin name="F2"/>
<pin name="F1"/>
<pin name="E6"/>
<pin name="E5"/>
<pin name="E7"/>
<pin name="E4"/>
<pin name="DVDD@1"/>
<pin name="DVDD@3"/>
<pin name="/RF_LED"/>
<pin name="VSS@3"/>
</symbol>
<symbol name="HMC1052L">
<pin name="GND2A"/>
<pin name="OFF+"/>
<pin name="OUT+A"/>
<pin name="VB"/>
<pin name="NC"/>
<pin name="OFF-"/>
<pin name="GND2B"/>
<pin name="S/R+"/>
<pin name="NC2"/>
<pin name="OUT-B"/>
<pin name="S/R-"/>
<pin name="NC3"/>
<pin name="GND1A"/>
<pin name="OUT-A"/>
<pin name="GND1B"/>
<pin name="OUT+B"/>
</symbol>
<symbol name="AYZ0202">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="LOGO1">
</symbol>
<symbol name="EMB001">
<pin name="ANT"/>
<pin name="GND@0"/>
<pin name="PIO2"/>
<pin name="PIO3"/>
<pin name="PIO4"/>
<pin name="PIO5"/>
<pin name="PIO6"/>
<pin name="PIO7"/>
<pin name="PIO8"/>
<pin name="PIO9"/>
<pin name="PIO10"/>
<pin name="PIO11"/>
<pin name="USB_DN"/>
<pin name="USB_DP"/>
<pin name="PCM_CLK"/>
<pin name="PCM_IN"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_OUT"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="VSUP"/>
<pin name="1V8"/>
<pin name="RX"/>
<pin name="RTS"/>
<pin name="TX"/>
<pin name="CTS"/>
<pin name="MOSI"/>
<pin name="SPI_CLK"/>
<pin name="SPI_CSB"/>
<pin name="MISO"/>
<pin name="RST"/>
<pin name="AIO1"/>
<pin name="AIO0"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="PIO1"/>
<pin name="PIO0"/>
<pin name="GND@9"/>
</symbol>
<symbol name="SMA_EDGE">
<pin name="GND@0"/>
<pin name="SIGNAL"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
</symbol>
<symbol name="FT245R">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="RXF" function="dot"/>
<pin name="TXE" function="dot"/>
<pin name="RD" function="dot"/>
<pin name="WR"/>
<pin name="PWEN"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PINHD8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="M02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="M04">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="M05">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="M06">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="M07">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="M08">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="COPERNICUS">
<pin name="BOOT"/>
<pin name="SHORT"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="RFIN"/>
<pin name="GND@3"/>
<pin name="LNA"/>
<pin name="GND@6"/>
<pin name="XSTANDBY"/>
<pin name="RESERVED3"/>
<pin name="RESERVED4"/>
<pin name="PPS"/>
<pin name="RXD-A"/>
<pin name="RESERVED5"/>
<pin name="TXD-A"/>
<pin name="TXD-B"/>
<pin name="RESERVED6"/>
<pin name="RESERVED7"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="RESERVED1"/>
<pin name="OPEN"/>
<pin name="RESERVED2"/>
<pin name="XRESET"/>
<pin name="RXD-B"/>
<pin name="VCC"/>
</symbol>
<symbol name="M14">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="JUMPER-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SJ">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SJ_2">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SCP1000_D01">
<pin name="TRIG"/>
<pin name="AVSS"/>
<pin name="ATST"/>
<pin name="AVDD"/>
<pin name="CSB"/>
<pin name="MISO"/>
<pin name="DRDY"/>
<pin name="CLK"/>
<pin name="DVDD"/>
<pin name="DVSS"/>
<pin name="DVDDS"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="PD"/>
</symbol>
<symbol name="PIC16F88-SSOP">
<pin name="RA5/MCLR" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/AN4"/>
<pin name="RB0/INT"/>
<pin name="RB1/SDA"/>
<pin name="RB2/RX"/>
<pin name="RB3"/>
<pin name="RB4/SCL"/>
<pin name="RB5/TX"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RA6/OSC2"/>
<pin name="RA7/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
</symbol>
<symbol name="PIC16F688">
<pin name="RA3/MCLR"/>
<pin name="RA5/OSC1"/>
<pin name="RA0/PGD"/>
<pin name="RC2/AN6"/>
<pin name="RC1/AN5"/>
<pin name="RC0/AN4"/>
<pin name="RA2/AN2"/>
<pin name="RA1/PGC"/>
<pin name="RC3/AN7"/>
<pin name="RC4/TX"/>
<pin name="RC5/RX"/>
<pin name="RA4/OSC2"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="NCP1400">
<pin name="LX" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="in"/>
</symbol>
<symbol name="BATTERY">
<pin name="-" direction="pwr"/>
<pin name="+" direction="pwr"/>
</symbol>
<symbol name="BUTTONPAD_SINGLE">
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="GND"/>
<pin name="RED"/>
<pin name="SIG2"/>
<pin name="SIG1"/>
</symbol>
<symbol name="BUZZER">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PIC-ISCP-MINI">
<pin name="VPP" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGD" direction="pas"/>
<pin name="PGC" direction="pas"/>
</symbol>
<symbol name="M10">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="XTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="ULN2803">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
</symbol>
<symbol name="HMC6352">
<pin name="CA1"/>
<pin name="CA2"/>
<pin name="CB1"/>
<pin name="CB2"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC"/>
</symbol>
<symbol name="VCC2">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="LETTER_L">
</symbol>
<symbol name="DOCFIELD">
</symbol>
<symbol name="78ADJ-2">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="M01">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="M11">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="M12">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="COPERNICUS-DIP">
<pin name="BOOT"/>
<pin name="SHORT"/>
<pin name="GND"/>
<pin name="LNA"/>
<pin name="XSTANDBY"/>
<pin name="RESERVED3"/>
<pin name="RESERVED4"/>
<pin name="PPS"/>
<pin name="RXD-A"/>
<pin name="RESERVED5"/>
<pin name="TXD-A"/>
<pin name="TXD-B"/>
<pin name="RESERVED6"/>
<pin name="RESERVED7"/>
<pin name="RESERVED1"/>
<pin name="OPEN"/>
<pin name="RESERVED2"/>
<pin name="XRESET"/>
<pin name="RXD-B"/>
<pin name="VCC"/>
</symbol>
<symbol name="LT1528">
<pin name="OUT"/>
<pin name="SENSE"/>
<pin name="GND"/>
<pin name="SHDN"/>
<pin name="IN"/>
</symbol>
<symbol name="DOSONCHIP-IC">
<pin name="UART_TX" direction="out"/>
<pin name="CARD_SCLK" direction="out"/>
<pin name="SPI_CS" direction="in" function="dot"/>
<pin name="CARD_DIN"/>
<pin name="CARD_WP" direction="in"/>
<pin name="CARD_CD" direction="in" function="dot"/>
<pin name="XTAL_OUT" direction="out"/>
<pin name="XTAL_IN" direction="in"/>
<pin name="SPI_MOSI" direction="in"/>
<pin name="UART_RX" direction="in"/>
<pin name="SPI_MISO" direction="out"/>
<pin name="SPI_SCLK" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="MODE0" direction="in"/>
<pin name="CARD_DOUT" direction="out"/>
<pin name="CARD_CS" direction="in" function="dot"/>
<pin name="MODE1" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="UART_CTS" direction="in"/>
<pin name="UART_RTS/BUSY" direction="out"/>
<pin name="I2C_SCL"/>
<pin name="I2C_SDA"/>
</symbol>
<symbol name="M09">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="XN04312">
<pin name="E2"/>
<pin name="B2"/>
<pin name="C1"/>
<pin name="E1"/>
<pin name="B1"/>
<pin name="C2"/>
</symbol>
<symbol name="RESONATOR">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="V-REG-LDO">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="BP" direction="in"/>
</symbol>
<symbol name="ADXL330">
<pin name="ST"/>
<pin name="COM@3"/>
<pin name="COM@2"/>
<pin name="COM@1"/>
<pin name="COM"/>
<pin name="ZOUT"/>
<pin name="YOUT"/>
<pin name="XOUT"/>
<pin name="VS@1"/>
<pin name="VS"/>
</symbol>
<symbol name="CAMERA_SFV24R-2ST">
<pin name="SCLK"/>
<pin name="AGND"/>
<pin name="AVDD28"/>
<pin name="RESET_N"/>
<pin name="CLK_IN"/>
<pin name="DGND"/>
<pin name="DOUT_0"/>
<pin name="DOUT_1"/>
<pin name="DOUT_2"/>
<pin name="DOUT_3"/>
<pin name="DOUT_4"/>
<pin name="DOUT_5"/>
<pin name="DOUT_6"/>
<pin name="DOUT_7"/>
<pin name="DOUT_8"/>
<pin name="VCLK_OUT"/>
<pin name="VALIDH"/>
<pin name="VALIDV"/>
<pin name="DVDD28"/>
<pin name="SDIN"/>
<pin name="PS1"/>
<pin name="PS2"/>
<pin name="SHIELD"/>
<pin name="LED_CTRL"/>
</symbol>
<symbol name="TC7SU04F">
<pin name="NC"/>
<pin name="GND"/>
<pin name="IN"/>
<pin name="OUT"/>
<pin name="+V"/>
</symbol>
<symbol name="SN74LVC1G08">
<pin name="A"/>
<pin name="B"/>
<pin name="GND"/>
<pin name="Y"/>
<pin name="+V"/>
</symbol>
<symbol name="USDCARD">
<pin name="CS"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="RSV"/>
<pin name="DO"/>
<pin name="NC"/>
<pin name="SHIELD@3"/>
<pin name="SHIELD@1"/>
<pin name="SHIELD@2"/>
<pin name="SHIELD@4"/>
</symbol>
<symbol name="2VCC2GND">
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="FT232R">
<pin name="RESET" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="DSR" direction="in" function="dot"/>
<pin name="DCD" direction="in" function="dot"/>
<pin name="RI" direction="in" function="dot"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND7" direction="pwr"/>
<pin name="GND18" direction="pwr"/>
<pin name="GND21" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="TXLED" direction="in" function="dot"/>
<pin name="RXLED" direction="in" function="dot"/>
<pin name="RTS" direction="out" function="dot"/>
<pin name="CTS" direction="in" function="dot"/>
<pin name="DTR" direction="out" function="dot"/>
<pin name="PWREN" direction="in" function="dot"/>
<pin name="TXDEN" direction="in"/>
<pin name="SLEEP" direction="in" function="dot"/>
</symbol>
<symbol name="FT232R-BASIC">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="TXLED" function="dot"/>
<pin name="RXLED" function="dot"/>
<pin name="RTS" function="dot"/>
<pin name="CTS" function="dot"/>
<pin name="DTR" function="dot"/>
</symbol>
<symbol name="BGB203_BLUETOOTH">
<pin name="GND@1"/>
<pin name="ANT"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
<pin name="GND@10"/>
<pin name="GPIO[14]"/>
<pin name="GPIO[12]"/>
<pin name="VDDRF"/>
<pin name="BTACT/GPIO[17]"/>
<pin name="VANLO"/>
<pin name="I2C_SDA/GPIO[1]"/>
<pin name="I2C_SCL/GPIO[0]"/>
<pin name="VDDA/VDDO"/>
<pin name="XTAL2_SYS"/>
<pin name="XTAL1_SYS"/>
<pin name="GPIO[13]"/>
<pin name="GPIO[11]"/>
<pin name="GPIO[10]"/>
<pin name="VDDC/VDDIO1"/>
<pin name="GPIO[16]"/>
<pin name="VDDIO1"/>
<pin name="XTAL1_LP"/>
<pin name="XTAL2_LP"/>
<pin name="VBUS_USB"/>
<pin name="GPIO[15]"/>
<pin name="GPIO[7]"/>
<pin name="GPIO[9]"/>
<pin name="GPIO[6]"/>
<pin name="GPIO[8]"/>
<pin name="VDDC"/>
<pin name="VDDIO2"/>
<pin name="DN_USB"/>
<pin name="DP_USB"/>
<pin name="RTS/GPIO[3]"/>
<pin name="RX/GPIO[5]"/>
<pin name="TX/GPIO[4]"/>
<pin name="CTS/GPIO[2]"/>
<pin name="RESET_N"/>
<pin name="VDDIORF"/>
<pin name="TMS_JTAG"/>
<pin name="TDO_JTAG"/>
<pin name="TDI_JTAG"/>
<pin name="TCK_JTAG"/>
<pin name="GND@49"/>
</symbol>
<symbol name="NAV_SWITCH">
<pin name="1" direction="in"/>
<pin name="T" direction="in"/>
<pin name="2" direction="in"/>
<pin name="C" direction="pwr"/>
</symbol>
<symbol name="SPX29300">
<pin name="ENABLE"/>
<pin name="VIN"/>
<pin name="GND@1"/>
<pin name="VOUT"/>
<pin name="ADJUST"/>
<pin name="GND@0"/>
</symbol>
<symbol name="BLUERADIO_BR-C40N">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCC"/>
<pin name="SPI_CSB"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="PIO_2/CONNECT" direction="out"/>
<pin name="PIO_3/INT" direction="in"/>
<pin name="PIO_4/FACRST"/>
<pin name="PIO_5/STATUS" direction="out"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="PCM_CLK"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_IN"/>
<pin name="PCM_OUT"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="UART_RTS" direction="out" function="dot"/>
<pin name="UART_CTS" direction="in" function="dot"/>
<pin name="RESET"/>
<pin name="GND@4" direction="pwr"/>
<pin name="ANT"/>
</symbol>
<symbol name="SHT1X">
<pin name="DATA"/>
<pin name="GND" direction="pwr"/>
<pin name="SCK" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="IDG300">
<pin name="GND@0"/>
<pin name="X_RO"/>
<pin name="XAGC"/>
<pin name="VDD@0"/>
<pin name="CPOUT"/>
<pin name="GND@1"/>
<pin name="YAGC"/>
<pin name="GND@2"/>
<pin name="Y_RO"/>
<pin name="VDD@1"/>
<pin name="VREF"/>
<pin name="VDD@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
</symbol>
<symbol name="LMV324">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-V" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+V" direction="pwr"/>
</symbol>
<symbol name="LMV324_2">
<pin name="-IN" direction="pwr"/>
<pin name="+IN" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
</symbol>
<symbol name="OPA344">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+V" direction="pwr"/>
</symbol>
<symbol name="IPOD_CONNECTOR_FEMALE">
<pin name="LEFT_IN"/>
<pin name="VIDEO_OUT"/>
<pin name="RIGHT_IN"/>
<pin name="SCHROME_OUT"/>
<pin name="GND@1"/>
<pin name="SLUM_OUT"/>
<pin name="GND@2"/>
<pin name="GND@11"/>
<pin name="LEFT_OUT"/>
<pin name="GND@16"/>
<pin name="RIGHT_OUT"/>
<pin name="FW_12V@20"/>
<pin name="ACC_INDICATOR"/>
<pin name="FW_TPA-"/>
<pin name="USB_5V"/>
<pin name="17"/>
<pin name="3.3V"/>
<pin name="FW_12V@19"/>
<pin name="GND@15"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="FW_TPA+"/>
<pin name="USB_D-"/>
<pin name="FW_TPB-"/>
<pin name="USB_D+"/>
<pin name="FW_TPB+"/>
<pin name="GND@29"/>
<pin name="GND@30"/>
<pin name="14"/>
<pin name="7"/>
</symbol>
<symbol name="M15">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="PIC18F2550">
<pin name="RX/RC7" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/AN4"/>
<pin name="TX/RC6"/>
<pin name="RC5/D+"/>
<pin name="RB0/INT0"/>
<pin name="RC4/D-"/>
<pin name="RB4/AN11"/>
<pin name="RB5/PGM"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2/INT2/AN8"/>
<pin name="RB1/INT1/AN10"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3/AN9"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="V-USB"/>
<pin name="RC0"/>
</symbol>
<symbol name="GE863">
<pin name="GPIO13"/>
<pin name="GPIO12"/>
<pin name="GPIO11"/>
<pin name="GPIO10"/>
<pin name="GPIO9/CAM_RST"/>
<pin name="GPIO8/CAM_ON"/>
<pin name="CAM_CLK"/>
<pin name="GND@0"/>
<pin name="EAR_MT-"/>
<pin name="EAR_MT+"/>
<pin name="EAR_HF+"/>
<pin name="EAR_HF-"/>
<pin name="MIC_MT+"/>
<pin name="MIN_MT-"/>
<pin name="MIC_HF+"/>
<pin name="MIC_HF-"/>
<pin name="GND@1"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="ADC_IN1"/>
<pin name="VRTC"/>
<pin name="TX_TRACE"/>
<pin name="RX_TRACE"/>
<pin name="VBATT"/>
<pin name="GND@2"/>
<pin name="STAT_LED"/>
<pin name="AXE"/>
<pin name="VAUX1"/>
<pin name="GPIO4/CAM_SDA"/>
<pin name="GPIO2/JDR"/>
<pin name="GPIO1"/>
<pin name="CHARGE"/>
<pin name="GND@3"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="GND@4"/>
<pin name="ON/OFF"/>
<pin name="RESET"/>
<pin name="GND@5"/>
<pin name="ANT"/>
<pin name="GND@6"/>
<pin name="GPIO7/BUZZER"/>
<pin name="PWRMON"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO3/CAM_SCL"/>
<pin name="GND@7"/>
<pin name="GPIO17"/>
<pin name="GPIO14"/>
<pin name="DAC_OUT"/>
<pin name="GPIO16"/>
<pin name="GND@8"/>
<pin name="TX_GPS"/>
<pin name="GND@9"/>
<pin name="GPIO15"/>
<pin name="GND@10"/>
<pin name="RX_GPS"/>
<pin name="PPS"/>
<pin name="GPIO18"/>
<pin name="GND@11"/>
<pin name="RX_GPS_BIN"/>
<pin name="GND@12"/>
<pin name="TX_GPS_BIN"/>
<pin name="GND@13"/>
<pin name="GPS_ANT"/>
<pin name="GND_GPS"/>
</symbol>
<symbol name="SIMHOLDER">
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="C7"/>
<pin name="C6"/>
<pin name="C5"/>
</symbol>
<symbol name="PIC16F883">
<pin name="RX/RC7" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4"/>
<pin name="TX/RC6"/>
<pin name="RC5/SDO"/>
<pin name="RB0/INT0"/>
<pin name="RC4/SDI"/>
<pin name="RB4/AN11"/>
<pin name="RB5/PGM"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2/INT2/AN8"/>
<pin name="RB1/INT1/AN10"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3/AN9"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3/SCK"/>
<pin name="RC0"/>
</symbol>
<symbol name="TRIMPOT">
<pin name="WIPER" direction="pas"/>
<pin name="CCW" direction="pas"/>
<pin name="CW" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="HMC6042">
<pin name="C1"/>
<pin name="S/R-IN" direction="in"/>
<pin name="INZ+" direction="in"/>
<pin name="INZ-" direction="in"/>
<pin name="VDD1"/>
<pin name="S/R+"/>
<pin name="S/R-"/>
<pin name="S/R-C"/>
<pin name="FBY"/>
<pin name="OUTY" direction="out"/>
<pin name="FBX"/>
<pin name="OUTX" direction="out"/>
<pin name="OUTZ" direction="out"/>
<pin name="FBZ"/>
<pin name="VDD2"/>
<pin name="GND"/>
</symbol>
<symbol name="HMC1041Z">
<pin name="S/R+"/>
<pin name="S/R-"/>
<pin name="GND"/>
<pin name="OUT-"/>
<pin name="OUT+"/>
<pin name="OFFSET+"/>
<pin name="VBRIDGE"/>
<pin name="OFFSET-"/>
</symbol>
<symbol name="PIC16F88-DIP">
<pin name="RA5/MCLR" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/AN4"/>
<pin name="RB0/INT"/>
<pin name="RB1/SDA"/>
<pin name="RB2/RX"/>
<pin name="RB3"/>
<pin name="RB4/SCL"/>
<pin name="RB5/TX"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA6/OSC2"/>
<pin name="RA7/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
</symbol>
<symbol name="ATMEGA168">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="A3L-LOC">
</symbol>
<symbol name="CON_2X10">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
</symbol>
<symbol name="SN74LV4052APWR">
<pin name="2Y0"/>
<pin name="2Y2"/>
<pin name="2-COM"/>
<pin name="2Y3"/>
<pin name="2Y1"/>
<pin name="INH"/>
<pin name="GNG@7"/>
<pin name="GND@8"/>
<pin name="B"/>
<pin name="A"/>
<pin name="1Y3"/>
<pin name="1Y0"/>
<pin name="1-COM"/>
<pin name="1Y1"/>
<pin name="1Y2"/>
<pin name="VCC"/>
</symbol>
<symbol name="AVR_MINI_PROGRAMMER">
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="RST" direction="pas"/>
<pin name="MOSI" direction="pas"/>
<pin name="SCK" direction="pas"/>
<pin name="MISO" direction="pas"/>
</symbol>
<symbol name="MOSFET-PCHANNEL">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="EM406">
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="1PPS"/>
<pin name="VCC"/>
</symbol>
<symbol name="ET312">
<pin name="GND6" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="GND7" direction="pwr"/>
<pin name="RF"/>
<pin name="GPIO1"/>
<pin name="VCC" direction="pwr"/>
<pin name="BATT" direction="pwr"/>
</symbol>
<symbol name="EB-85A">
<pin name="GND" direction="pwr"/>
<pin name="TX2" direction="out"/>
<pin name="RX1" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="RX2" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="PPS" direction="out"/>
<pin name="BATT" direction="pwr"/>
</symbol>
<symbol name="IRF9410">
<pin name="S@1"/>
<pin name="S@2"/>
<pin name="S@3"/>
<pin name="G"/>
<pin name="D@1"/>
<pin name="D@2"/>
<pin name="D@3"/>
<pin name="D@4"/>
</symbol>
<symbol name="NJM2670">
<pin name="NC@1" direction="in"/>
<pin name="SENSEA"/>
<pin name="INA1"/>
<pin name="ENABLEA"/>
<pin name="GND@2"/>
<pin name="INB1"/>
<pin name="ENABLEB"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="TSDARM"/>
<pin name="INB2"/>
<pin name="GND@3"/>
<pin name="GND@1" direction="pwr"/>
<pin name="OUTA1" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="OUTA2" direction="pwr"/>
<pin name="NC@4"/>
<pin name="INA2"/>
<pin name="VCC"/>
<pin name="VSA"/>
<pin name="OUTB1"/>
<pin name="SENSEB"/>
<pin name="OUTB2"/>
<pin name="VSB"/>
</symbol>
<symbol name="MC34063">
<pin name="DVR"/>
<pin name="COMP"/>
<pin name="TC"/>
<pin name="SWC"/>
<pin name="GND"/>
<pin name="SWE"/>
<pin name="VCC"/>
<pin name="SEN"/>
</symbol>
<symbol name="ANTENNA">
<pin name="GND"/>
<pin name="SIGNAL"/>
</symbol>
<symbol name="ANTENNA2">
<pin name="SIGNAL"/>
</symbol>
<symbol name="BLUESMIRF-V2">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCC"/>
<pin name="SPI_CSB"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="PIO_2/CONNECT" direction="out"/>
<pin name="PIO_3/INT" direction="in"/>
<pin name="PIO_4/FACRST"/>
<pin name="PIO_5/STATUS" direction="out"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="PCM_CLK"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_IN"/>
<pin name="PCM_OUT"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="UART_RTS" direction="out" function="dot"/>
<pin name="UART_CTS" direction="in" function="dot"/>
<pin name="RESET"/>
<pin name="GND@4" direction="pwr"/>
<pin name="ANT"/>
</symbol>
<symbol name="LTC6244">
<pin name="-IN"/>
<pin name="+IN"/>
<pin name="-V"/>
<pin name="+V"/>
<pin name="OUT"/>
</symbol>
<symbol name="LTC6244_2">
<pin name="-IN"/>
<pin name="+IN"/>
<pin name="OUT"/>
</symbol>
<symbol name="V18ZA2P">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="74595">
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QH*" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PTC">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="MLX90609">
<pin name="TOPCAP@1"/>
<pin name="GND"/>
<pin name="VDD"/>
<pin name="SCLK"/>
<pin name="SS"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="TEST"/>
<pin name="ERROR"/>
<pin name="SELFTEST"/>
<pin name="HVIN"/>
<pin name="OUTTEMP"/>
<pin name="FLT"/>
<pin name="OUTAR"/>
<pin name="VREF"/>
<pin name="VSSA"/>
<pin name="VDDA"/>
<pin name="CASE"/>
<pin name="TESTIN"/>
<pin name="TESTOUT"/>
<pin name="TOPCAP@2"/>
</symbol>
<symbol name="LT1014">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-V" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+V" direction="pwr"/>
</symbol>
<symbol name="LT1014_2">
<pin name="-IN" direction="pwr"/>
<pin name="+IN" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
</symbol>
<symbol name="SEWTAP">
<pin name="1"/>
</symbol>
<symbol name="LED-TRICOLORSMD">
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="A"/>
<pin name="RED"/>
</symbol>
<symbol name="SEWTAP-SMALL">
<pin name="1"/>
</symbol>
<symbol name="SEWTAP-SMALL-2">
<pin name="1"/>
</symbol>
<symbol name="TEMT6000">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E1" direction="pas"/>
<pin name="C1" direction="pas"/>
</symbol>
<symbol name="TEMT6000-SEN">
<pin name="E1" direction="pas"/>
<pin name="C1" direction="pas"/>
</symbol>
<symbol name="M05X2">
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="FIDUCIAL">
</symbol>
<symbol name="GR-10">
<pin name="FREF"/>
<pin name="GND@2" direction="pwr"/>
<pin name="1.8V@3" direction="pwr"/>
<pin name="SB" direction="in"/>
<pin name="RX1" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="RX0" direction="in"/>
<pin name="TX0" direction="out"/>
<pin name="1PPS" direction="out"/>
<pin name="1.8V@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GPIO_A11"/>
<pin name="GPIO_A5"/>
<pin name="GPIO_A6"/>
<pin name="GPIO_A9"/>
<pin name="APIO_A4"/>
<pin name="RTC_XIN"/>
<pin name="RTC_XOUT"/>
<pin name="GPIO_B19"/>
<pin name="VALID_FIX" direction="out"/>
<pin name="1.8V@21" direction="pwr"/>
<pin name="GPIO_B16"/>
<pin name="RESET" direction="in"/>
<pin name="GND@24" direction="pwr"/>
<pin name="1.8VVCO" direction="pwr"/>
<pin name="1.8VIF" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="1.8VLNA" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="ANT" direction="in"/>
<pin name="GND@31" direction="pwr"/>
<pin name="RFEN" direction="out"/>
<pin name="3V" direction="pwr"/>
<pin name="1.8VRF" direction="pwr"/>
<pin name="TPI" direction="in"/>
<pin name="TPQ" direction="in"/>
</symbol>
<symbol name="3.3V">
<pin name="3.3V" direction="sup"/>
</symbol>
<symbol name="5V">
<pin name="5V" direction="sup"/>
</symbol>
<symbol name="BUTTONPAD_1LED">
<pin name="A"/>
<pin name="K"/>
<pin name="SIG2"/>
<pin name="SIG1"/>
</symbol>
<symbol name="BUZZER-CMT1603">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="MOSFET-NCHANNEL">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="DOIDE-1N4148">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MCP2551">
<pin name="TXD"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="RXD"/>
<pin name="VREF"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="RS"/>
</symbol>
<symbol name="MAX323">
<pin name="NO1"/>
<pin name="COM1"/>
<pin name="IN2"/>
<pin name="V-"/>
<pin name="NO2"/>
<pin name="COM2"/>
<pin name="IN1"/>
<pin name="V+"/>
</symbol>
<symbol name="G3VM-61E1">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
<symbol name="DB9_MALE">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
</symbol>
<symbol name="RJ11-6">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="GM862">
<pin name="VBATT@0" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="VBATT@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VBATT@2" direction="pwr"/>
<pin name="GND/ADC" direction="pwr"/>
<pin name="VBATT@3" direction="pwr"/>
<pin name="CHARGE" direction="in"/>
<pin name="EAR_HF+" direction="out"/>
<pin name="EAR_MT-" direction="out"/>
<pin name="EAR_HF-" direction="out"/>
<pin name="EAR_MT+" direction="out"/>
<pin name="MIC_HF-" direction="in"/>
<pin name="MIC_MT+" direction="in"/>
<pin name="MIC_HF+" direction="in"/>
<pin name="MIC_MT-" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="AXE" direction="in"/>
<pin name="SIMIO"/>
<pin name="C103/TXD" direction="in"/>
<pin name="PWRMON" direction="out"/>
<pin name="SIMVCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="SIMRST" direction="out"/>
<pin name="RES@25"/>
<pin name="SIMCLK" direction="out"/>
<pin name="CCIN/SIMIN"/>
<pin name="GPO2/JDR" direction="out"/>
<pin name="C106/CTS"/>
<pin name="C125/RING" direction="out"/>
<pin name="GPI1" direction="in"/>
<pin name="GPIO8/PD[0]/CAM_ON"/>
<pin name="C107/DSR" direction="out"/>
<pin name="GPIO9/PD[1]/CAM_RST"/>
<pin name="EMMI_TX/TX_GPS" direction="out"/>
<pin name="C109/DCD" direction="out"/>
<pin name="C104/RXD" direction="out"/>
<pin name="GPIO10/PD[2]"/>
<pin name="STAT_LED" direction="out"/>
<pin name="GPIO11/PD[3]"/>
<pin name="EMMI_RX/RX_GPS" direction="in"/>
<pin name="GPIO12/PD[4]"/>
<pin name="C108/DTR" direction="in"/>
<pin name="GPIO13/PD[5]"/>
<pin name="C105/RTS" direction="in"/>
<pin name="GPIO3/PD[6]/CAM_SCL"/>
<pin name="GPIO4/IICSDA/CAM_SDA"/>
<pin name="GPIO5/CAM_RDY/RFTXMON"/>
<pin name="GPIO6/ALARM/PD[7]"/>
<pin name="GPIO7/BUZZER/CAM_PWR_ON"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
</symbol>
<symbol name="SEWTAP-NOHOLE">
</symbol>
<symbol name="STAND-OFF">
</symbol>
<symbol name="MOTOR">
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="EM408_CON">
<pin name="EN"/>
<pin name="GND"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="VCC"/>
</symbol>
<symbol name="M16">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="BREADBOARD">
</symbol>
<symbol name="NS73M">
<pin name="RFO"/>
<pin name="GND@14"/>
<pin name="RIN"/>
<pin name="LIN"/>
<pin name="GND@11"/>
<pin name="X1"/>
<pin name="VCC"/>
<pin name="GND@1"/>
<pin name="VDRF"/>
<pin name="TEB"/>
<pin name="PWE"/>
<pin name="CK"/>
<pin name="DA"/>
<pin name="LA"/>
<pin name="IIC"/>
</symbol>
<symbol name="AUDIO-JACK">
<pin name="RIGHT"/>
<pin name="LEFT"/>
<pin name="SLEEVE"/>
</symbol>
<symbol name="EEPROM-I2C">
<pin name="VSS" direction="pwr"/>
<pin name="WP"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A2"/>
<pin name="A0"/>
<pin name="A1"/>
</symbol>
<symbol name="OPAMP-DUAL">
<pin name="OUT" direction="out"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="VCC+" direction="pwr"/>
<pin name="VCC-" direction="pwr"/>
</symbol>
<symbol name="OP-AMP+-">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OP-AMP">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MINI-DIN6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="LUXEON">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="S"/>
</symbol>
<symbol name="NRF24AP1">
<pin name="BR2"/>
<pin name="BR1" direction="in"/>
<pin name="EXT32K" direction="in"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="SLEEP" direction="in"/>
<pin name="SUSPEND" direction="in" function="dot"/>
<pin name="RTS" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="XC2" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="out"/>
<pin name="ANT2" direction="out"/>
<pin name="VSS_PA" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="IREF" direction="in"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="PORTSEL" direction="in"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VSS@0" direction="out"/>
</symbol>
<symbol name="AVR_SPI_PROGRAMMER_6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="TEST-POINT">
<pin name="1"/>
</symbol>
<symbol name="TRIAC">
<pin name="M2"/>
<pin name="M1"/>
<pin name="G"/>
</symbol>
<symbol name="ALM-1412">
<pin name="RF_IN"/>
<pin name="GND"/>
<pin name="SD"/>
<pin name="RF_OUT"/>
<pin name="VDD"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
</symbol>
<symbol name="SI4700/01-GM">
<pin name="GND"/>
<pin name="VA" direction="pwr"/>
<pin name="FMIP" direction="in"/>
<pin name="RFGND"/>
<pin name="FMIN" direction="in"/>
<pin name="RST" function="dot"/>
<pin name="SEN" function="dot"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="RCLK"/>
<pin name="VIO" direction="pwr"/>
<pin name="LOUT"/>
<pin name="ROUT"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="VD" direction="pwr"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="GND@0"/>
</symbol>
<symbol name="PINH2X26">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="41" direction="pas" function="dot"/>
<pin name="43" direction="pas" function="dot"/>
<pin name="45" direction="pas" function="dot"/>
<pin name="47" direction="pas" function="dot"/>
<pin name="49" direction="pas" function="dot"/>
<pin name="51" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
<pin name="42" direction="pas" function="dot"/>
<pin name="44" direction="pas" function="dot"/>
<pin name="46" direction="pas" function="dot"/>
<pin name="48" direction="pas" function="dot"/>
<pin name="50" direction="pas" function="dot"/>
<pin name="52" direction="pas" function="dot"/>
</symbol>
<symbol name="NRF24L01">
<pin name="VDD@7"/>
<pin name="VSS@8" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="SUSPEND" direction="in" function="dot"/>
<pin name="IRQ" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="XC2" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="out"/>
<pin name="ANT2" direction="out"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="IREF" direction="in"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="CSN" direction="in"/>
<pin name="VDD@24" direction="pwr"/>
</symbol>
<symbol name="NRF24L01-1">
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="IRQ" direction="out" function="dot"/>
<pin name="DVDD" direction="pwr"/>
<pin name="XC2" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="out"/>
<pin name="ANT2" direction="out"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="IREF" direction="in"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="CSN" direction="in"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
</symbol>
<symbol name="NRF2401A">
<pin name="DATA"/>
<pin name="DVDD" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="DR1" direction="out"/>
<pin name="CLK2"/>
<pin name="DOUT2" direction="out"/>
<pin name="CLK1"/>
<pin name="PWR_UP" direction="pwr"/>
<pin name="XC2" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="out"/>
<pin name="ANT2" direction="out"/>
<pin name="VSS_PA" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="IREF" direction="in"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="DR2" direction="out"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
</symbol>
<symbol name="ATTINY24">
<pin name="VCC"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3/RESET"/>
<pin name="PA7/ADC7"/>
<pin name="PA6/MOSI"/>
<pin name="PA5/MISO"/>
<pin name="PA4/SCL"/>
<pin name="PA3/ADC3"/>
<pin name="PA2/ADC2"/>
<pin name="PA1/ADC1"/>
<pin name="PA0/ADC0"/>
<pin name="GND"/>
<pin name="GND@0"/>
</symbol>
<symbol name="BUTTON-CONDUCTIVE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="ADJD">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SLEEP"/>
<pin name="-VE"/>
<pin name="+VE"/>
<pin name="NC"/>
<pin name="DVDD"/>
<pin name="AVDD"/>
<pin name="AGND"/>
<pin name="XRST"/>
<pin name="DGND"/>
<pin name="XCLK"/>
</symbol>
<symbol name="HMC1051Z">
<pin name="GND@1"/>
<pin name="V0+"/>
<pin name="VCC"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="S/R+"/>
<pin name="S/R-"/>
<pin name="VO-"/>
</symbol>
<symbol name="IRF7507">
<pin name="S1"/>
<pin name="G1"/>
<pin name="S2"/>
<pin name="G2"/>
<pin name="D2@5"/>
<pin name="D2@6"/>
<pin name="D1@7"/>
<pin name="D1@8"/>
</symbol>
<symbol name="OPAMP_2">
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="+V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="OPAMP_2_1">
<pin name="OUT2" direction="out"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
</symbol>
<symbol name="DIODE-SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SCA1000">
<pin name="SCK"/>
<pin name="N/C@2"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="OUTY"/>
<pin name="GND"/>
<pin name="CSB"/>
<pin name="N/C@8"/>
<pin name="ST2"/>
<pin name="ST1"/>
<pin name="OUTX"/>
<pin name="VDD"/>
</symbol>
<symbol name="XC3S250/500E-PQ208">
<pin name="GND"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="GND@12"/>
<pin name="GND@13"/>
<pin name="GND@14"/>
<pin name="GND@15"/>
<pin name="GND@16"/>
<pin name="GND@17"/>
<pin name="GND@18"/>
<pin name="GND@19"/>
<pin name="GND@20"/>
<pin name="VCCAUX"/>
<pin name="VCCAUX@2"/>
<pin name="VCCAUX@3"/>
<pin name="VCCAUX@4"/>
<pin name="VCCAUX@5"/>
<pin name="VCCAUX@6"/>
<pin name="VCCAUX@7"/>
<pin name="VCCAUX@8"/>
<pin name="VCCINT"/>
<pin name="VCCINT@2"/>
<pin name="VCCINT@3"/>
<pin name="VCCINT@4"/>
<pin name="DONE"/>
<pin name="PROG_B"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="IO"/>
<pin name="IO/VREF_0"/>
<pin name="IO_L01N_0"/>
<pin name="IO_L01P_0"/>
<pin name="IO_L02N_0/VREF_0"/>
<pin name="IO_L02P_0"/>
<pin name="IO_L03N_0"/>
<pin name="IO_L03P_0"/>
<pin name="IO_L04N_0/VREF_0"/>
<pin name="IO_L04P_0"/>
<pin name="IO_L05N_0"/>
<pin name="IO_L05P_0"/>
<pin name="IO_L07N_0/GCLK5"/>
<pin name="IO_LO7P_0/GCLK4"/>
<pin name="IO_L08N_0/GCLK7"/>
<pin name="IO_L08P_0/GCLK6"/>
<pin name="IO_L10N_0/GCLK11"/>
<pin name="IO_L10P_0/GCLK10"/>
<pin name="IO_L11N_0"/>
<pin name="IO_L11P_0"/>
<pin name="IO_L12N_0/VREF_0"/>
<pin name="IO_L12P_0"/>
<pin name="IO_L13N_0"/>
<pin name="IO_L13P_0"/>
<pin name="IO_L14N_0/VREF_0"/>
<pin name="IO_L15N_0"/>
<pin name="IO_L14P_0"/>
<pin name="IO_L15P_0"/>
<pin name="IO_L16N_0/HSWAP"/>
<pin name="IO_L16P_0"/>
<pin name="IP"/>
<pin name="IP@2"/>
<pin name="IP@3"/>
<pin name="IP@4"/>
<pin name="IP_L06N_0"/>
<pin name="IP_L06P_0"/>
<pin name="IP_LO9N_0/GCLK9"/>
<pin name="IP_L09P_0/GCLK8"/>
<pin name="VCCO_0"/>
<pin name="VCCO_0@2"/>
<pin name="VCCO_0@3"/>
<pin name="IO_L01N_1/A15"/>
<pin name="IO_L01P_1/A16"/>
<pin name="IO_L02N_1/A13"/>
<pin name="IO_L02P_1/A14"/>
<pin name="IO_L03N_1/VREF_1"/>
<pin name="IO_L03P_1"/>
<pin name="IO_L04N_1"/>
<pin name="IO_L04P_1"/>
<pin name="IO_L05N_1/A11"/>
<pin name="IO_L05P_1/A12"/>
<pin name="IO_L06N_1/VREF_1"/>
<pin name="IO_L06P_1"/>
<pin name="IO_L07N_1/A7/RHCLK1"/>
<pin name="IO_L07P_1/A10/RHCLK0"/>
<pin name="IO_L08N_1/A7/RHCLK3"/>
<pin name="IO_L08P_1/A8/RHCLK2"/>
<pin name="IO_L09N_1/A5/RHCLK5"/>
<pin name="IO_L09P_1/A6/RHCLK4"/>
<pin name="IO_L10N_1/A3/RHCLK7"/>
<pin name="IO_L10P_1/A4/RHCLK6"/>
<pin name="IO_L11N_1/A1"/>
<pin name="IO_L11P_1/A2"/>
<pin name="IO_L12N_1/A0"/>
<pin name="IO_L12P_1"/>
<pin name="IO_L13N_1"/>
<pin name="IO_L13P_1"/>
<pin name="IO_L14N_1"/>
<pin name="IO_L14P_1"/>
<pin name="IO_L15_1/LDC0"/>
<pin name="IO_L15P_1/HDC"/>
<pin name="IO_L16N_1/LDC2"/>
<pin name="IO_16P_1/LDC1"/>
<pin name="IP@5"/>
<pin name="IP@6"/>
<pin name="IP@7"/>
<pin name="IP@8"/>
<pin name="IP@9"/>
<pin name="IP@10"/>
<pin name="IP@11"/>
<pin name="IP/VREF_1"/>
<pin name="VCC0_1"/>
<pin name="VCC0_1@2"/>
<pin name="VCC0_1@3"/>
<pin name="IO/D5"/>
<pin name="IO/M1"/>
<pin name="IO/VREF_2"/>
<pin name="IO/L01N_2/INIT_B"/>
<pin name="IO_L01P_2/CSO_B"/>
<pin name="IO_L03N_2/MOSI/CSI_B"/>
<pin name="IO_L03P_2/DOUT/BUSY"/>
<pin name="IO_L04N_2"/>
<pin name="IO_L04P_2"/>
<pin name="IO_L05N_2"/>
<pin name="IO_L05P_2"/>
<pin name="IO_L06N_2"/>
<pin name="IO_L06P_2"/>
<pin name="IO_L08N_2/D6/GCLK13"/>
<pin name="10_L08P_2/D7/GCLK12"/>
<pin name="IO_L09N_2/D3/GCLK15"/>
<pin name="IO_L09P_2/D4/GCLK14"/>
<pin name="IO_L11N_2/D1/GCLK3"/>
<pin name="IO_L11P_2/D2/GCLK2"/>
<pin name="IO_L12N_2/DIN/D0"/>
<pin name="IO_L12P_2/M0"/>
<pin name="IO_L13N_2"/>
<pin name="IO_L13P_2"/>
<pin name="IO_L14N_2/A22"/>
<pin name="IO_L14P_2/A23"/>
<pin name="IO_L15N_2/A20"/>
<pin name="IO_L15P_2/A21"/>
<pin name="IO_L16N_2/VS1/A18"/>
<pin name="IO_L16P_2/VS2/A19"/>
<pin name="IO_L17N_2/CCLK"/>
<pin name="IO_L17P_2/VS0/A17"/>
<pin name="IP@12"/>
<pin name="IP@13"/>
<pin name="IP@14"/>
<pin name="IP_L02N_2"/>
<pin name="IP_L02P_2"/>
<pin name="IP_L07N_2/VREF_2"/>
<pin name="IP_L07P_2"/>
<pin name="IP_L10N_2/M2/GCLK1"/>
<pin name="IP_L10P_2/RDWR_B/GCLK0"/>
<pin name="VCCO_2"/>
<pin name="VCCO_2@2"/>
<pin name="VCCO_2@3"/>
<pin name="IO/VREF_3"/>
<pin name="IO_L01N_3"/>
<pin name="IO_L01P_3"/>
<pin name="IO_L02N_3/VREF_3"/>
<pin name="IO_L02P_3"/>
<pin name="IO_L03N_3"/>
<pin name="IO_L03P_3"/>
<pin name="IO_L04N_3"/>
<pin name="IO_L04P_3"/>
<pin name="IO_L05N_3"/>
<pin name="IO_L05P_3"/>
<pin name="IO_L06N_3"/>
<pin name="IO_L06P_3"/>
<pin name="IO_L07N_3/LHCLK1"/>
<pin name="IO_L07P_3/LHCLK0"/>
<pin name="IO_L08N_3/LHCLK3"/>
<pin name="IO_L08P_3/LHCLK2"/>
<pin name="IO_L09N_3/LHCLK5"/>
<pin name="IO_L09P_3/LHCLK4"/>
<pin name="IO_L10N_3/LHCLK7"/>
<pin name="IO_L10P_3/LHCLK6"/>
<pin name="IO_L11N_3"/>
<pin name="IO_L11P_3"/>
<pin name="IO_L12N_3"/>
<pin name="IO_L12P_3"/>
<pin name="IO_L13N_3"/>
<pin name="IO_L13P_3"/>
<pin name="IO_L14N_3"/>
<pin name="IO_L14P_3"/>
<pin name="IO_L15N_3"/>
<pin name="IO_L15P_3"/>
<pin name="IO_L16N_3"/>
<pin name="IO_L16P_3"/>
<pin name="IP@15"/>
<pin name="IP@16"/>
<pin name="IP@17"/>
<pin name="IP@18"/>
<pin name="IP@19"/>
<pin name="IP@20"/>
<pin name="IP/VREF_3"/>
<pin name="VCCO_3"/>
<pin name="VCCO_3@2"/>
<pin name="VCCO_3@3"/>
</symbol>
<symbol name="F25">
<pin name="1" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="DB25">
<pin name="1" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="VS1002">
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="XRESET"/>
<pin name="D_REQ"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="XDCS/BSYNC"/>
<pin name="XTAL0"/>
<pin name="XTAL1"/>
<pin name="XCS"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SCLK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="TEST"/>
<pin name="SPIBOOT/GPIO0"/>
<pin name="GPIO1"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="LEFT"/>
<pin name="AVDD1" direction="pwr"/>
<pin name="AVDD2" direction="pwr"/>
<pin name="AVDD3" direction="pwr"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DVDD1" direction="pwr"/>
<pin name="DVDD2" direction="pwr"/>
<pin name="DVDD3" direction="pwr"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="DGND1" direction="pwr"/>
</symbol>
<symbol name="INVERTING_SCHMITT_TRIGGER">
<pin name="NC"/>
<pin name="A"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="Y"/>
</symbol>
<symbol name="INVERTER">
<pin name="NC"/>
<pin name="A"/>
<pin name="GND"/>
<pin name="Y"/>
<pin name="VCC"/>
</symbol>
<symbol name="TS3A5017">
<pin name="IN2"/>
<pin name="1S4"/>
<pin name="1S3"/>
<pin name="1S2"/>
<pin name="1S1"/>
<pin name="1D"/>
<pin name="GND"/>
<pin name="2D"/>
<pin name="2S1"/>
<pin name="2S2"/>
<pin name="2S3"/>
<pin name="2S4"/>
<pin name="IN1"/>
<pin name="VCC"/>
<pin name="1EN" function="dot"/>
<pin name="2EN" function="dot"/>
</symbol>
<symbol name="74ACT125D">
<pin name="VCC"/>
<pin name="A0"/>
<pin name="B0"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="A2"/>
<pin name="B2"/>
<pin name="GND"/>
<pin name="B3"/>
<pin name="A3"/>
<pin name="O3"/>
<pin name="O2"/>
<pin name="O1"/>
<pin name="O0"/>
</symbol>
<symbol name="EP2C20_PQ208_PLL">
<pin name="GND_PLL1" direction="pwr"/>
<pin name="GND_PLL1@1" direction="pwr"/>
<pin name="GND_PLL2" direction="pwr"/>
<pin name="GND_PLL2@1" direction="pwr"/>
<pin name="GNDA_PLL1" direction="pwr"/>
<pin name="GNDA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
</symbol>
<symbol name="EP2C20_PQ208_B3">
<pin name="IO_LVDS56N"/>
<pin name="IO_LVDS56P"/>
<pin name="VCCIO3@1"/>
<pin name="IO_LVDS53N"/>
<pin name="IO_LVDS53P"/>
<pin name="IO_LVDS52N"/>
<pin name="IO_LVDS52P"/>
<pin name="IO_LVDS51N"/>
<pin name="IO_LVDS51P"/>
<pin name="IO_VREFB3N1"/>
<pin name="VCCIO3@2"/>
<pin name="IO_LVDS48N"/>
<pin name="IO_LVDS48P"/>
<pin name="CLK7_LVDSCLK3N"/>
<pin name="CLK6_LVDSCLK3P"/>
<pin name="CLK5_LVDSCLK2N"/>
<pin name="CLK4_LVDSCLK2P"/>
<pin name="IO_LVDS47N"/>
<pin name="IO_LVDS47P"/>
<pin name="IO_LVDS46N"/>
<pin name="VCCIO3@3"/>
<pin name="IO_LVDS46P"/>
<pin name="IO_LVDS45N"/>
<pin name="IO_LVDS45P"/>
<pin name="IO_LVDS44N"/>
<pin name="IO_LVDS44P"/>
<pin name="IO_LVDS42N"/>
<pin name="IO_LVDS42P"/>
<pin name="IO_VREFB3N0"/>
<pin name="IO_LVDS39N"/>
<pin name="IO_LVDS39P"/>
<pin name="VCCIO3@4"/>
<pin name="IO_LVDS38N"/>
<pin name="IO_LVDS38P"/>
<pin name="IO_PLL2_OUTP"/>
<pin name="IO_PLL2_OUTN"/>
<pin name="IO@1"/>
</symbol>
<symbol name="EP2C20_PQ208_B1">
<pin name="IO_LVDS14P"/>
<pin name="IO_LVDS14N"/>
<pin name="VCCIO1@1"/>
<pin name="IO_LVDS13P"/>
<pin name="IO_LVDS13N"/>
<pin name="IO_LVDS12P"/>
<pin name="IO_LVDS12N"/>
<pin name="IO_VREFB1N0"/>
<pin name="IO_LVDS8P"/>
<pin name="IO_LVDS8N"/>
<pin name="CLK0_LVDSCLK0P"/>
<pin name="CLK1_LVDSCLK0N"/>
<pin name="CLK2_LVDSCLK1P"/>
<pin name="CLK3_LVDSCLK1N"/>
<pin name="VCCIO1@4"/>
<pin name="IO_LVDS7P"/>
<pin name="IO_LVDS7N"/>
<pin name="IO_LVDS6N"/>
<pin name="IO@2"/>
<pin name="IO_LVDS5P"/>
<pin name="IO_VREFB1N1"/>
<pin name="IO_LVDS3N"/>
<pin name="IO_LVDS2P"/>
<pin name="IO_LVDS2N"/>
<pin name="VCCIO1@6"/>
<pin name="IO@3"/>
<pin name="IO_LVDS0P"/>
<pin name="IO_LVDS0N"/>
<pin name="IO@4"/>
<pin name="IO_PLL1_OUTP"/>
<pin name="IO_PLL1_OUTN"/>
</symbol>
<symbol name="EP2C20_PQ208_B4">
<pin name="IO_LVDS77P"/>
<pin name="IO_LVDS76P"/>
<pin name="IO_LVDS76N"/>
<pin name="IO_LVDS75P"/>
<pin name="IO_LVDS75N"/>
<pin name="VCCIO4@1"/>
<pin name="IO_LVDS74P"/>
<pin name="IO_LVDS74N"/>
<pin name="IO_VREFB4N1"/>
<pin name="IO_LVDS70P"/>
<pin name="IO_LVDS70N"/>
<pin name="IO_LVDS68P"/>
<pin name="IO_LVDS68N"/>
<pin name="VCCIO4@2"/>
<pin name="IO_LVDS67P"/>
<pin name="IO_LVDS67N"/>
<pin name="IO_LVDS66P"/>
<pin name="IO_LVDS66N"/>
<pin name="IO_LVDS64P"/>
<pin name="IO_LVDS64N"/>
<pin name="VCCIO4@3"/>
<pin name="IO_LVDS63P"/>
<pin name="IO_LVDS63N"/>
<pin name="IO_LVDS62P"/>
<pin name="IO_LVDS62N"/>
<pin name="IO_VREFB4N0"/>
<pin name="IO_LVDS61P"/>
<pin name="VCCIO4@4"/>
<pin name="IO_LVDS61N"/>
<pin name="IO_LVDS60P"/>
<pin name="IO_LVDS60N"/>
<pin name="IO@2"/>
<pin name="IO_LVDS59P"/>
<pin name="VCCIO4@5"/>
<pin name="IO_LVDS59N"/>
<pin name="IO_LVDS58P"/>
<pin name="IO_LVDS58N"/>
<pin name="IO_LVDS57P"/>
<pin name="IO_LVDS57N"/>
<pin name="IO@1"/>
</symbol>
<symbol name="EP2C20_PQ208_POWER">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="VCCINT@1" direction="pwr"/>
<pin name="VCCINT@2" direction="pwr"/>
<pin name="VCCINT@3" direction="pwr"/>
<pin name="VCCINT@4" direction="pwr"/>
<pin name="VCCINT@5" direction="pwr"/>
<pin name="VCCINT@6" direction="pwr"/>
<pin name="GND@15"/>
<pin name="GND@16"/>
<pin name="GND@17"/>
<pin name="GND@18"/>
<pin name="GND@19"/>
<pin name="GND@20"/>
<pin name="GND@21"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
<pin name="GND@25"/>
</symbol>
<symbol name="EP2C20_PQ208_B2">
<pin name="IO_LVDS37N"/>
<pin name="IO_LVDS37P"/>
<pin name="IO_LVDS36N"/>
<pin name="IO_LVDS36P"/>
<pin name="IO_LVDS35N"/>
<pin name="IO_LVDS35P"/>
<pin name="VCCIO2@1"/>
<pin name="IO_LVDS34N"/>
<pin name="IO_LVDS34P"/>
<pin name="IO_VREFB2N0"/>
<pin name="IO_LVDS33N"/>
<pin name="VCCIO2@2"/>
<pin name="IO_LVDS33P"/>
<pin name="IO_LVDS31N"/>
<pin name="IO_LVDS31P"/>
<pin name="IO_LVDS29N"/>
<pin name="IO_LVDS29P"/>
<pin name="IO_LVDS28N"/>
<pin name="IO_LVDS28P"/>
<pin name="VCCIO2@3"/>
<pin name="IO_LVDS26P"/>
<pin name="IO_LVDS25N"/>
<pin name="IO_LVDS25P"/>
<pin name="IO_LVDS24N"/>
<pin name="IO_LVDS24P"/>
<pin name="IO_VREFB2N1"/>
<pin name="IO_LVDS23N"/>
<pin name="VCCIO2@4"/>
<pin name="IO_LVDS23P"/>
<pin name="IO_LVDS21N"/>
<pin name="IO_LVDS21P"/>
<pin name="IO_LVDS19N"/>
<pin name="IO_LVDS19P"/>
<pin name="IO_LVDS18N"/>
<pin name="VCCIO2@5"/>
<pin name="IO_LVDS18P"/>
<pin name="IO_LVDS17P"/>
<pin name="IO_LVDS16N"/>
<pin name="IO_LVDS16P"/>
<pin name="IO_LVDS17N"/>
</symbol>
<symbol name="EP2C20_PQ208_CONFIG">
<pin name="ASDO"/>
<pin name="CRC_ERROR"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="DATA0"/>
<pin name="NCSO"/>
<pin name="CLKUSR"/>
<pin name="TMS"/>
<pin name="TDI"/>
<pin name="NCE"/>
<pin name="NCONFIG"/>
<pin name="DEV_OE"/>
<pin name="INIT_DONE"/>
<pin name="NCEO"/>
<pin name="NSTATUS"/>
<pin name="CONF_DONE"/>
<pin name="MSEL1"/>
<pin name="MSEL0"/>
<pin name="DCLK"/>
</symbol>
<symbol name="LIS3LV02DQ">
<pin name="INT" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="SDA/SDI"/>
<pin name="SCL/SPC" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="CK" direction="in"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD_IO" direction="pwr"/>
</symbol>
<symbol name="RMCM01">
<pin name="FPLS"/>
<pin name="HR"/>
<pin name="OSC"/>
<pin name="F32KIN"/>
<pin name="OSC_ON"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="LX1"/>
<pin name="LX2"/>
<pin name="WIDB_DET"/>
<pin name="RESET"/>
</symbol>
<symbol name="PIC16F913">
<pin name="RX/RC7/SDA" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4"/>
<pin name="TX/RC6/SCL"/>
<pin name="RC5"/>
<pin name="RB0/INT0"/>
<pin name="RC4/SD0"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RA6/OSC2"/>
<pin name="RA7/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC0"/>
</symbol>
<symbol name="LIS302DL">
<pin name="VDD_IO" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="INT1" direction="out"/>
<pin name="INT2" direction="out"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="SDA/SDI" direction="in"/>
<pin name="SCL/SPC" direction="in"/>
</symbol>
<symbol name="TPS61040">
<pin name="EN"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="SW"/>
<pin name="FB"/>
</symbol>
<symbol name="ICSP-OLIMEX-MINI">
<pin name="VPP"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="PGD"/>
<pin name="PGC"/>
</symbol>
<symbol name="SPM0204UD5">
<pin name="VS"/>
<pin name="OUT"/>
<pin name="GND"/>
<pin name="GND#"/>
</symbol>
<symbol name="WT32">
<pin name="VDDIO@17"/>
<pin name="VDD_BAT@37"/>
<pin name="VDD_CHG@38"/>
<pin name="AIO0@5"/>
<pin name="AIO1@6"/>
<pin name="VREG_ENA@1"/>
<pin name="PIO0@7"/>
<pin name="PIO1@8"/>
<pin name="PIO2@9"/>
<pin name="PIO3@10"/>
<pin name="PIO4@26"/>
<pin name="PIO5@25"/>
<pin name="PIO6@24"/>
<pin name="PIO7@23"/>
<pin name="PIO8@22"/>
<pin name="PIO9@13"/>
<pin name="PIO10@14"/>
<pin name="USB_DN@11"/>
<pin name="USB_DP@12"/>
<pin name="RXD@15"/>
<pin name="TXD@16"/>
<pin name="PCM_IN@27"/>
<pin name="PCM_OUT@28"/>
<pin name="PCM_SYNC@29"/>
<pin name="PCM_CLK@30"/>
<pin name="RESET@19"/>
<pin name="RTS@20"/>
<pin name="CTS@21"/>
<pin name="SPI_CS@32"/>
<pin name="SPI_MISO@34"/>
<pin name="SPI_CLK@33"/>
<pin name="SPI_MOSI@35"/>
<pin name="LED0@36"/>
<pin name="MIC_BIAS@40"/>
<pin name="AUDIO_IN_P_RIGHT@41"/>
<pin name="AUDIO_IN_N_RIGHT@42"/>
<pin name="AUDIO_IN_P_LEFT@44"/>
<pin name="AUDIO_IN_N_LEFT@45"/>
<pin name="AUDIO_OUT_N_RIGHT@46"/>
<pin name="AUDIO_OUT_P_RIGHT@47"/>
<pin name="AUDIO_OUT_N_LEFT@49"/>
<pin name="AUDIO_OUT_P_LEFT@50"/>
<pin name="DGND@2"/>
<pin name="DGND@3"/>
<pin name="DGND@4"/>
<pin name="DGND@18"/>
<pin name="DGND@31"/>
<pin name="AGND@39"/>
<pin name="AGND@43"/>
<pin name="AGND@48"/>
</symbol>
<symbol name="STW5093">
<pin name="VCC"/>
<pin name="REMOUT"/>
<pin name="REMIN"/>
<pin name="MIC3+"/>
<pin name="MIC3-"/>
<pin name="MBIAS"/>
<pin name="VCCA"/>
<pin name="MIC1+"/>
<pin name="MIC1-"/>
<pin name="GNDA"/>
<pin name="MIC2+"/>
<pin name="MIC2-"/>
<pin name="VCCP"/>
<pin name="VLR-"/>
<pin name="VLR+"/>
<pin name="GNDP"/>
<pin name="VFR"/>
<pin name="LO"/>
<pin name="BZ"/>
<pin name="CCLK"/>
<pin name="CS-"/>
<pin name="CI"/>
<pin name="AUXCLK"/>
<pin name="VCCIO"/>
<pin name="CO"/>
<pin name="GND"/>
<pin name="DX"/>
<pin name="DR"/>
<pin name="FS"/>
<pin name="MCLK"/>
</symbol>
<symbol name="EM408_OUTLINE">
</symbol>
<symbol name="XBEE-1">
<pin name="VDD" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="DIO12"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="RSSI"/>
<pin name="DIO11"/>
<pin name="RES@8"/>
<pin name="DTR" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="DIO4"/>
<pin name="CTS" direction="out" function="dot"/>
<pin name="DIO9"/>
<pin name="RES@14"/>
<pin name="DIO5"/>
<pin name="RTS" direction="in" function="dot"/>
<pin name="DIO3"/>
<pin name="DIO2"/>
<pin name="DIO1"/>
<pin name="DIO0"/>
</symbol>
<symbol name="M25">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="2.8V">
<pin name="2.8V" direction="sup"/>
</symbol>
<symbol name="ZUNE_CONNECTOR_MALE">
<pin name="USB_5V@1"/>
<pin name="USB_5V@2"/>
<pin name="USB_5V@3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="VIDEO+"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="AUDIO_L"/>
<pin name="AUDIO_R"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="GND@19"/>
<pin name="USB_DATA-"/>
<pin name="USB_DATA+"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
</symbol>
<symbol name="PINH2X12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
</symbol>
<symbol name="DS1307">
<pin name="X1"/>
<pin name="X2"/>
<pin name="VBATT"/>
<pin name="GND"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SQW"/>
<pin name="VCC"/>
</symbol>
<symbol name="CNZ1120">
<pin name="2"/>
<pin name="1"/>
<pin name="4"/>
<pin name="3"/>
</symbol>
<symbol name="NDS8434-1">
<pin name="D@1"/>
<pin name="D@2"/>
<pin name="D@3"/>
<pin name="D@4"/>
<pin name="G"/>
<pin name="S@1"/>
<pin name="S@2"/>
<pin name="S@3"/>
</symbol>
<symbol name="RN41">
<pin name="GND"/>
<pin name="SPIMOSI"/>
<pin name="PIO6"/>
<pin name="PIO7"/>
<pin name="RESET"/>
<pin name="SPICLK"/>
<pin name="PCMCLK"/>
<pin name="PCMSYNC"/>
<pin name="PCMIN"/>
<pin name="PCMOUT"/>
<pin name="VDD"/>
<pin name="GND1"/>
<pin name="UARTRX"/>
<pin name="UARTTX"/>
<pin name="UARTRTS"/>
<pin name="UARTCTS"/>
<pin name="USBD+"/>
<pin name="USBD-"/>
<pin name="PIO2"/>
<pin name="PIO3"/>
<pin name="PIO5"/>
<pin name="PIO4"/>
<pin name="SPICSB"/>
<pin name="SPIMISO"/>
<pin name="GND2"/>
<pin name="NC"/>
<pin name="GND3"/>
<pin name="PIO9"/>
<pin name="GND4"/>
<pin name="PIO8"/>
<pin name="PIO10"/>
<pin name="PIO11"/>
<pin name="AIO1"/>
<pin name="AIO2"/>
<pin name="GND5"/>
</symbol>
<symbol name="SPST">
<pin name="P" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="LIGHTPIPE-7511">
</symbol>
<symbol name="LIPO-1100">
</symbol>
<symbol name="AT45DB041B">
<pin name="SI"/>
<pin name="SCK"/>
<pin name="RST" function="dot"/>
<pin name="CS" function="dot"/>
<pin name="WP" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="MCP4725">
<pin name="VOUT"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="AO"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="SIMHOLDER2">
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="SW1"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
<pin name="SW2"/>
</symbol>
<symbol name="HMC6343">
<pin name="VDD@3"/>
<pin name="VDD@21"/>
<pin name="VDD@11"/>
<pin name="GND@25"/>
<pin name="GND@29"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="CS"/>
<pin name="CSC"/>
</symbol>
<symbol name="BATTERY-2">
<pin name="-1" direction="pwr"/>
<pin name="+2" direction="pwr"/>
<pin name="+1" direction="pwr"/>
<pin name="-2" direction="pwr"/>
</symbol>
<symbol name="AUDIO-JACK2">
<pin name="RING"/>
<pin name="TIP"/>
<pin name="SLEEVE"/>
<pin name="RSH"/>
<pin name="TSH"/>
</symbol>
<symbol name="ADXLXXX_E8">
<pin name="ST"/>
<pin name="T2"/>
<pin name="COM"/>
<pin name="YOUT"/>
<pin name="XOUT"/>
<pin name="YFILT"/>
<pin name="XFILT"/>
<pin name="VDD"/>
</symbol>
<symbol name="SMA661AS">
<pin name="IN"/>
<pin name="GND@2"/>
<pin name="PD"/>
<pin name="OUT"/>
<pin name="GND@5"/>
<pin name="VCC"/>
</symbol>
<symbol name="TOUCH-SCREEN">
<pin name="TS4"/>
<pin name="TS3"/>
<pin name="TS2"/>
<pin name="TS1"/>
</symbol>
<symbol name="NRF24Z1">
<pin name="SSEL"/>
<pin name="SMISO"/>
<pin name="SSCK"/>
<pin name="SCSN"/>
<pin name="VDD"/>
<pin name="SMOSI"/>
<pin name="DD1"/>
<pin name="DD0"/>
<pin name="REQ"/>
<pin name="CLK"/>
<pin name="WS"/>
<pin name="DATA"/>
<pin name="SPDIO"/>
<pin name="MCLK"/>
<pin name="DVDD"/>
<pin name="VSS"/>
<pin name="XC2"/>
<pin name="XC1"/>
<pin name="VDD1"/>
<pin name="VDD_PA"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="VSS_PA"/>
<pin name="IREF"/>
<pin name="VSS1"/>
<pin name="MODE"/>
<pin name="MSDA"/>
<pin name="MSCL"/>
<pin name="MCSN"/>
<pin name="MMISO"/>
<pin name="MMOSI"/>
<pin name="VSS2"/>
<pin name="VDD2"/>
<pin name="VSS3"/>
<pin name="MSCK"/>
<pin name="IRQ"/>
</symbol>
<symbol name="AD7745">
<pin name="/RDY"/>
<pin name="CIN1+"/>
<pin name="CIN1-"/>
<pin name="CIN2+"/>
<pin name="CIN2-"/>
<pin name="EXCA"/>
<pin name="EXCB"/>
<pin name="GND"/>
<pin name="NC"/>
<pin name="REFIN+"/>
<pin name="REFIN-"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
<pin name="VIN+"/>
<pin name="VIN-"/>
</symbol>
<symbol name="TOUCH">
<pin name="T1"/>
<pin name="T2"/>
</symbol>
<symbol name="JUMPER-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="VS1033D">
<pin name="S0"/>
<pin name="SI"/>
<pin name="SCLK"/>
<pin name="XCS"/>
<pin name="XDCS/BSYNC"/>
<pin name="DREQ"/>
<pin name="XRESET"/>
<pin name="TEST"/>
<pin name="XTAL1/MCLK"/>
<pin name="XTAL2"/>
<pin name="VCO"/>
<pin name="GPIO0/I2S_SCLK"/>
<pin name="GPIO1/I2S_SDATA"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="GPIO4/I2S_LROUT"/>
<pin name="GPIO5/I2C_MCLK"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="IOVDD1"/>
<pin name="IOVDD2"/>
<pin name="IOVDD3"/>
<pin name="CVDD1"/>
<pin name="CVDD2"/>
<pin name="CVDD3"/>
<pin name="AVDD1"/>
<pin name="AVDD2"/>
<pin name="AVDD3"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="LINEIN"/>
<pin name="RCAP"/>
<pin name="DGND6"/>
<pin name="DGND1"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="AGND4"/>
<pin name="CVDD4"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
</symbol>
<symbol name="VS1000">
<pin name="XRESET"/>
<pin name="TEST"/>
<pin name="XTAL1"/>
<pin name="XTAL0"/>
<pin name="NFDIO0/IO0_0"/>
<pin name="NFDIO1/IO0_1"/>
<pin name="NFDIO2/IO0_2"/>
<pin name="NFDIO3/IO0_3"/>
<pin name="NFDIO4/IO0_4"/>
<pin name="NFDIO5/IO0_5"/>
<pin name="NFDIO6/IO0_6"/>
<pin name="NFDIO7/IO0_7"/>
<pin name="NFRDY/GPIO0_8"/>
<pin name="NFRD/GPIO0_9"/>
<pin name="CS1/GPIO0_10"/>
<pin name="NFCLE/GPIO0_12"/>
<pin name="NFALE/GPIO0_13"/>
<pin name="NFWR/GPIO0_11"/>
<pin name="CS2/GPIO0_14"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DGND1"/>
<pin name="VHIGH"/>
<pin name="POWBTN"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="XCS/GPIO1_0"/>
<pin name="SCLK/GPIO1_1"/>
<pin name="SI/GPIO1_2"/>
<pin name="SO/GPIO1_3"/>
<pin name="RX/GPIO1_4"/>
<pin name="TX/GPIO1_5"/>
<pin name="USBN"/>
<pin name="USBP"/>
<pin name="CVDD"/>
<pin name="IOVDD2"/>
<pin name="AVDD1"/>
<pin name="AVDD2"/>
<pin name="AVDD3"/>
<pin name="AVDD4"/>
<pin name="IOVDD3"/>
<pin name="IOVDD1"/>
</symbol>
<symbol name="NAND256">
<pin name="RXB"/>
<pin name="XR"/>
<pin name="XE"/>
<pin name="CL"/>
<pin name="AL"/>
<pin name="XW"/>
<pin name="XWP"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VSS1"/>
<pin name="IO7"/>
<pin name="IO6"/>
<pin name="IO5"/>
<pin name="IO4"/>
<pin name="IO3"/>
<pin name="IO2"/>
<pin name="IO1"/>
<pin name="IO0"/>
<pin name="VSS2"/>
</symbol>
<symbol name="MCP9700">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="VO"/>
</symbol>
<symbol name="PIC24HJ32GP202">
<pin name="AN0/VREF+/CN2/RA0"/>
<pin name="AN1/VREF-/CN2/RA1"/>
<pin name="AN4/RP2/CN6/RB2"/>
<pin name="AN5/RP3/CN7/RB3"/>
<pin name="AN9/RP15/CN11/RB15"/>
<pin name="AN10/RP14/CN12/RB14"/>
<pin name="AN11/RP13/CN13/RB13"/>
<pin name="AN12/RP12/CN14/RB12"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="INT0/RP7/CN23/RB7"/>
<pin name="MCLR" direction="in"/>
<pin name="OSCO/CLKO/CN29/RA3" direction="out"/>
<pin name="OSCI/CLKI/CN30/RA2" direction="in"/>
<pin name="PGEC1/AN3/C2IN+/RP1/CN5/RB1"/>
<pin name="PGEC2/TMS/RP11/CN15/RB11"/>
<pin name="PGEC3/ASCL1/RP6/CN24/RB6"/>
<pin name="PGED1/AN2/C2IN-/RP0/CN4/RB0"/>
<pin name="PGED2/TDI/RP10/CN16/RB10"/>
<pin name="PGED3/ASDA1/RP5/CN27/RB5"/>
<pin name="SOSCI/RP4/CN1/RB4"/>
<pin name="SOSCO/T1CK/CN0/RA4"/>
<pin name="TCK/SCL/RP8/CN22/RB8"/>
<pin name="TDO/SDA1/RP9/CN12/RB9"/>
<pin name="VCAP/VDDCORE" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="PL-2303XA">
<pin name="TXD"/>
<pin name="DTR_N"/>
<pin name="RTS_N"/>
<pin name="VDD_325"/>
<pin name="RXD"/>
<pin name="RI_N"/>
<pin name="GND@7"/>
<pin name="VDD_33"/>
<pin name="DSR_N"/>
<pin name="DCD_N"/>
<pin name="CTS_N"/>
<pin name="SHTD_N"/>
<pin name="EE_CLK"/>
<pin name="EE_DATA"/>
<pin name="DP"/>
<pin name="DM"/>
<pin name="VO_33"/>
<pin name="GND@18"/>
<pin name="RESET_N"/>
<pin name="VDD_5"/>
<pin name="GND@21"/>
<pin name="GP0"/>
<pin name="GP1"/>
<pin name="VDD_33A"/>
<pin name="GND_A"/>
<pin name="PLL_TEST"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
</symbol>
<symbol name="SCA3000">
<pin name="RST"/>
<pin name="INT"/>
<pin name="CLK"/>
<pin name="DVSS"/>
<pin name="DVDD"/>
<pin name="DVIO"/>
<pin name="CSB"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="AVDD"/>
<pin name="AVSS@15"/>
<pin name="AVSS@16"/>
</symbol>
<symbol name="TFM-511">
<pin name="ANT"/>
<pin name="NC"/>
<pin name="ROUT"/>
<pin name="LOUT"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="BUSEN"/>
<pin name="BUSMOD"/>
<pin name="CLK"/>
<pin name="DAT"/>
</symbol>
<symbol name="ARDUINO_SERIAL_PROGRAM">
<pin name="DTR" direction="pas"/>
<pin name="RXI" direction="pas"/>
<pin name="TXO" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="CTS" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER">
<pin name="1"/>
<pin name="4"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="THERMALCUTOFF">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="XPORT_DIRECT">
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="3.3V"/>
<pin name="RST"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="RTS"/>
<pin name="DTR"/>
<pin name="CTS"/>
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="GND@24"/>
</symbol>
<symbol name="XPORT">
<pin name="GND"/>
<pin name="3.3V"/>
<pin name="RST" function="dot"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="RTS"/>
<pin name="DTR"/>
<pin name="CTS"/>
</symbol>
<symbol name="LED-TRICOLOR-THROUGHHOLE">
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="C"/>
<pin name="RED"/>
</symbol>
<symbol name="LM2621">
<pin name="PGND"/>
<pin name="EN"/>
<pin name="FREQ"/>
<pin name="FB"/>
<pin name="SGND"/>
<pin name="VDD"/>
<pin name="BOOT"/>
<pin name="SW"/>
</symbol>
<symbol name="DSPIC30F4011">
<pin name="MCLR"/>
<pin name="RB0/AREF+"/>
<pin name="RB1/AREF-"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4/IC7"/>
<pin name="RB5/IC8"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RB8"/>
<pin name="VDD0"/>
<pin name="VSS0"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="RC13/TX1"/>
<pin name="RC14/RX1"/>
<pin name="INT0/RE8"/>
<pin name="OC2/RD1"/>
<pin name="RD3"/>
<pin name="VSS1"/>
<pin name="VDD1"/>
<pin name="RD2"/>
<pin name="OC1/RD0"/>
<pin name="RF6/SCK1"/>
<pin name="PGD/SCL"/>
<pin name="PGC/SDA"/>
<pin name="RF5/TX2"/>
<pin name="RF4/RX2"/>
<pin name="RF1"/>
<pin name="RF0"/>
<pin name="VSS2"/>
<pin name="VDD2"/>
<pin name="RE5"/>
<pin name="RE4"/>
<pin name="RE3"/>
<pin name="RE2"/>
<pin name="RE1"/>
<pin name="RE0"/>
<pin name="AVSS"/>
<pin name="AVDD"/>
</symbol>
<symbol name="EM406_OUTLINE">
</symbol>
<symbol name="ID-12">
<pin name="GNDT"/>
<pin name="RES"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="CP"/>
<pin name="FUTURE"/>
<pin name="+/-"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="LED"/>
<pin name="5V"/>
</symbol>
<symbol name="RF24G">
<pin name="GND"/>
<pin name="CE"/>
<pin name="CLK2"/>
<pin name="CS"/>
<pin name="CLK1"/>
<pin name="VCC"/>
<pin name="DR2"/>
<pin name="DOUT2"/>
<pin name="DR1"/>
<pin name="DATA"/>
</symbol>
<symbol name="TCM8230MD">
</symbol>
<symbol name="1.8V">
<pin name="1.8V" direction="sup"/>
</symbol>
<symbol name="ICSP-PIC">
<pin name="GND"/>
<pin name="PGC"/>
<pin name="PGD"/>
<pin name="PGM"/>
<pin name="VCC"/>
<pin name="VPP"/>
</symbol>
<symbol name="MN5010HS">
<pin name="1PPS"/>
<pin name="ANT"/>
<pin name="BATT"/>
<pin name="GND2"/>
<pin name="GND11"/>
<pin name="GND24"/>
<pin name="GND27"/>
<pin name="GND29"/>
<pin name="GND31"/>
<pin name="NAV"/>
<pin name="NMR"/>
<pin name="ONOFF"/>
<pin name="OPT1"/>
<pin name="OPT2"/>
<pin name="RX-I"/>
<pin name="TX-O"/>
<pin name="VIO"/>
<pin name="GND4"/>
</symbol>
<symbol name="MQ-3">
<pin name="A1"/>
<pin name="H1"/>
<pin name="B1"/>
<pin name="H2"/>
</symbol>
<symbol name="M02NG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="M20">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="M10X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="ACS712">
<pin name="IP+@1"/>
<pin name="IP+@2"/>
<pin name="IP-@3"/>
<pin name="IP-@4"/>
<pin name="GND"/>
<pin name="FILT"/>
<pin name="VOUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="RJ45-8">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
</symbol>
<symbol name="NRF24LU1">
<pin name="VDD3"/>
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="VSS2"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="/RESET"/>
<pin name="PROG"/>
<pin name="VSS1"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="VDD2"/>
<pin name="VBUS"/>
<pin name="VDD1"/>
<pin name="XC1"/>
<pin name="XC2"/>
<pin name="VSS7"/>
<pin name="DEC2"/>
<pin name="DEC1"/>
<pin name="VDD6"/>
<pin name="VSS6"/>
<pin name="IREF"/>
<pin name="VDD5"/>
<pin name="VSS5"/>
<pin name="ANT2"/>
<pin name="ANT1"/>
<pin name="VDD_PA"/>
<pin name="VDD4"/>
<pin name="VSS4"/>
<pin name="VSS3"/>
</symbol>
<symbol name="ATTINY13">
<pin name="VCC"/>
<pin name="PB1(MISO)"/>
<pin name="PB5(NRES)"/>
<pin name="GND"/>
<pin name="PB0(MOSI)"/>
<pin name="PB2(SCK/ADC1)"/>
<pin name="PB3(ADC3)"/>
<pin name="PB4(ADC2)"/>
</symbol>
<symbol name="QRD1114">
<pin name="C"/>
<pin name="E"/>
<pin name="K"/>
<pin name="A"/>
</symbol>
<symbol name="PCF8575C">
<pin name="INT"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="PO0"/>
<pin name="PO1"/>
<pin name="PO2"/>
<pin name="PO3"/>
<pin name="PO4"/>
<pin name="PO5"/>
<pin name="PO6"/>
<pin name="PO7"/>
<pin name="GND"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="A0"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC"/>
</symbol>
<symbol name="NRF24LE1">
<pin name="P0.1"/>
<pin name="VDD1"/>
<pin name="DEC1"/>
<pin name="DEC2"/>
<pin name="P0.2"/>
<pin name="PROG"/>
<pin name="P0.3"/>
<pin name="VSS1"/>
<pin name="VDD2"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="RESET"/>
<pin name="VDD_PA"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="VSS2"/>
<pin name="VDD3"/>
<pin name="IREF"/>
<pin name="VSS3"/>
<pin name="VDD4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="XC2"/>
<pin name="XC1"/>
<pin name="P0.0"/>
</symbol>
<symbol name="CREATIVE_COMMONS">
</symbol>
<symbol name="FC30">
<pin name="VDD_IO" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="RES@7" direction="nc"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="RES@4" direction="pwr"/>
<pin name="RES@10" direction="pwr"/>
<pin name="RES@13" direction="nc"/>
<pin name="RES@14" direction="nc"/>
<pin name="PD" direction="in"/>
<pin name="SIGN" direction="out"/>
<pin name="LC" direction="out"/>
<pin name="PC" direction="out"/>
</symbol>
<symbol name="LISY300AL">
<pin name="CACT"/>
<pin name="VDD"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="GND1"/>
<pin name="GND"/>
<pin name="AOUT"/>
<pin name="PD"/>
<pin name="ST"/>
<pin name="VCONT"/>
<pin name="FVDD"/>
</symbol>
<symbol name="RELAY-SPDT">
<pin name="COIL2"/>
<pin name="MAIN"/>
<pin name="NO"/>
<pin name="NC"/>
<pin name="COIL1"/>
</symbol>
<symbol name="M04-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="LCD-16X2">
<pin name="A" direction="pwr"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="E" direction="in"/>
<pin name="K" direction="pwr"/>
<pin name="R/W" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VO"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="RELAY-SPDT-2">
<pin name="9"/>
<pin name="6"/>
<pin name="10"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
</symbol>
<symbol name="LY530AL">
<pin name="VDDD"/>
<pin name="VDDA"/>
<pin name="RES"/>
<pin name="PD"/>
<pin name="AOUT"/>
<pin name="ST"/>
<pin name="PLL2"/>
<pin name="PLL1"/>
<pin name="DIS"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="SDO"/>
<pin name="CS"/>
<pin name="DR"/>
<pin name="CACT"/>
<pin name="GND"/>
</symbol>
<symbol name="ICL3232">
<pin name="C1+"/>
<pin name="V+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="V-"/>
<pin name="T2OUT"/>
<pin name="R2IN"/>
<pin name="R2OUT"/>
<pin name="T2IN"/>
<pin name="T1IN"/>
<pin name="R1OUT"/>
<pin name="R1IN"/>
<pin name="T1OUT"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="DIN7">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
</symbol>
<symbol name="VS1103">
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="XRESET"/>
<pin name="D_REQ"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="XDCS/BSYNC"/>
<pin name="XTAL0"/>
<pin name="XTAL1"/>
<pin name="XCS"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SCLK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="TEST"/>
<pin name="SPIBOOT/GPIO0"/>
<pin name="GPIO1"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="LEFT"/>
<pin name="AVDD1" direction="pwr"/>
<pin name="AVDD2" direction="pwr"/>
<pin name="AVDD3" direction="pwr"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DVDD1" direction="pwr"/>
<pin name="DVDD2" direction="pwr"/>
<pin name="DVDD3" direction="pwr"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="DGND1" direction="pwr"/>
<pin name="CVDD1"/>
<pin name="CVDD2"/>
<pin name="CVDD3"/>
<pin name="CVDD4"/>
</symbol>
<symbol name="TRF-24G">
<pin name="VCC"/>
<pin name="DR2"/>
<pin name="DOUT2"/>
<pin name="DR1"/>
<pin name="DATA"/>
<pin name="CLK1"/>
<pin name="CS"/>
<pin name="CLK2"/>
<pin name="CE"/>
<pin name="GND"/>
</symbol>
<symbol name="ADXL180">
<pin name="VBN@3"/>
<pin name="VDD"/>
<pin name="VBN@8"/>
<pin name="VBC"/>
<pin name="VBN@10"/>
<pin name="VBP"/>
<pin name="VSCI"/>
<pin name="VBN@18"/>
</symbol>
<symbol name="OS4000-T">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="20"/>
<pin name="19"/>
<pin name="18"/>
<pin name="17"/>
<pin name="16"/>
<pin name="14"/>
<pin name="13"/>
<pin name="12"/>
<pin name="15"/>
</symbol>
<symbol name="SSOP28">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
</symbol>
<symbol name="CD74HC4067">
<pin name="COM"/>
<pin name="CHAN7"/>
<pin name="CHAN6"/>
<pin name="CHAN5"/>
<pin name="CHAN4"/>
<pin name="CHAN3"/>
<pin name="CHAN2"/>
<pin name="CHAN1"/>
<pin name="CHAN0"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="GND"/>
<pin name="S3" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="EN" direction="in" function="dot"/>
<pin name="CHAN15"/>
<pin name="CHAN14"/>
<pin name="CHAN13"/>
<pin name="CHAN12"/>
<pin name="CHAN11"/>
<pin name="CHAN10"/>
<pin name="CHAN9"/>
<pin name="CHAN8"/>
<pin name="VCC"/>
</symbol>
<symbol name="TVP5150-NTSC_DECODER">
<pin name="AGND"/>
<pin name="CH_AGND"/>
<pin name="PLL_AGND"/>
<pin name="DGND"/>
<pin name="REFM"/>
<pin name="CH_AVDD"/>
<pin name="PLL_AVDD"/>
<pin name="DVDD"/>
<pin name="IO_DVDD"/>
<pin name="PDN"/>
<pin name="RESET/"/>
<pin name="REFP"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
</symbol>
<symbol name="JOYSTICK">
<pin name="V+"/>
<pin name="V"/>
<pin name="V-"/>
<pin name="H+"/>
<pin name="H"/>
<pin name="H-"/>
<pin name="SEL+"/>
<pin name="SEL-"/>
</symbol>
<symbol name="UM-FPU_V3_1">
<pin name="CS" direction="in"/>
<pin name="!MCLR" direction="in" function="dot"/>
<pin name="AN0" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="in"/>
<pin name="SEROUT" direction="out"/>
<pin name="SERIN" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="SOUT/SCL" direction="out"/>
<pin name="SIN/SDA" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="EXTIN" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT0" direction="out"/>
<pin name="SCLK" direction="in"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
</symbol>
<symbol name="TVP5150-NTSC_DECODER-1">
<pin name="AGND"/>
<pin name="AIP1A"/>
<pin name="AIP1B"/>
<pin name="AVID"/>
<pin name="CH_AGND"/>
<pin name="CH_AVDD"/>
<pin name="DGND"/>
<pin name="DVDD"/>
<pin name="FID/GLCO"/>
<pin name="HSYNC"/>
<pin name="INT_REQ"/>
<pin name="IO_DVDD"/>
<pin name="PCLK/SCLK"/>
<pin name="PDN"/>
<pin name="PLL_AGND"/>
<pin name="PLL_AVDD"/>
<pin name="REFM"/>
<pin name="REFP"/>
<pin name="RESET/"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VSYNC"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="YOUT_0"/>
<pin name="YOUT_1"/>
<pin name="YOUT_2"/>
<pin name="YOUT_3"/>
<pin name="YOUT_4"/>
<pin name="YOUT_5"/>
<pin name="YOUT_6"/>
<pin name="YOUT_7"/>
</symbol>
<symbol name="ADXL345">
<pin name="VDD"/>
<pin name="NC@11"/>
<pin name="NC@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="VSS"/>
<pin name="CS"/>
<pin name="INT1"/>
<pin name="INT2"/>
<pin name="GND@2"/>
<pin name="NC@10"/>
<pin name="SDO"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="IDG500">
<pin name="GND@2"/>
<pin name="GND@8"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="CPOUT"/>
<pin name="YAGC"/>
<pin name="XAGC"/>
<pin name="VDD@19"/>
<pin name="VDD@9"/>
<pin name="X4.5IN"/>
<pin name="XOUT"/>
<pin name="X4.5OUT"/>
<pin name="Y4.5IN"/>
<pin name="YOUT"/>
<pin name="Y4.5OUT"/>
<pin name="PTATS"/>
<pin name="AZ"/>
<pin name="VREF"/>
</symbol>
<symbol name="IDG1215">
<pin name="GND@2"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="CPOUT"/>
<pin name="YAGC"/>
<pin name="XAGC"/>
<pin name="VDD@19"/>
<pin name="VDD@9"/>
<pin name="XHP1"/>
<pin name="XOUT"/>
<pin name="XHP2"/>
<pin name="YHP1"/>
<pin name="YOUT"/>
<pin name="YHP2"/>
<pin name="PTATS"/>
<pin name="AZ"/>
<pin name="VREF"/>
</symbol>
<symbol name="VENUS634FLPX">
<pin name="LED"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="PPS"/>
<pin name="CLK"/>
<pin name="CSN"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="GND@19"/>
<pin name="GND@15"/>
<pin name="GNDRF@21"/>
<pin name="GNDRF@22"/>
<pin name="GNDRF@24"/>
<pin name="GNDRF@25"/>
<pin name="GNDRF@27"/>
<pin name="GNDRF@28"/>
<pin name="GNDRF@29"/>
<pin name="GNDRF@31"/>
<pin name="GNDRF@33"/>
<pin name="RTC"/>
<pin name="BTSEL"/>
<pin name="RSTN"/>
<pin name="RFIN"/>
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="GPIO1"/>
<pin name="REGEN"/>
<pin name="GPIO2"/>
<pin name="GPIO20"/>
<pin name="PIO12"/>
<pin name="PIO14"/>
<pin name="GPIO24"/>
</symbol>
<symbol name="DS1077">
<pin name="OUT1"/>
<pin name="OUT0"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="CTRL0"/>
<pin name="CTRL1"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="UBW32_PIC32MX4XXL">
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="C1IN-/AN4/CN6/RB4"/>
<pin name="C1OUT/AN8/RB8"/>
<pin name="C2IN+/AN3/CN5/RB3"/>
<pin name="C2IN-/AN2/CN4/RB2"/>
<pin name="C2OUT/AN9/RB9"/>
<pin name="CN20/U1CTS/RD14"/>
<pin name="CVREFOUT/PMA13/AN10/RB10"/>
<pin name="D+/RG2"/>
<pin name="D-/RG3"/>
<pin name="ENVREG"/>
<pin name="IC1/RTCC/RD8"/>
<pin name="IC2/SS1/RD9"/>
<pin name="IC3/SCKI/PMCS2/PMA15/RD10"/>
<pin name="IC4/PMCS1/PMA14/RD11"/>
<pin name="INT1/RE8"/>
<pin name="INT2/RE9"/>
<pin name="MCLR"/>
<pin name="OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="OSC1/CLKI/RC12"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="PGC1/EMUC1/AN1/CN3/RB1"/>
<pin name="PGC2/EMUC2/AN6/OCFA/RB6"/>
<pin name="PGD1/EMUD1/AN0/CN2/RB0"/>
<pin name="PGD2/EMUD2/AN7/RB7"/>
<pin name="PMA2/SS2/CN11/RG9"/>
<pin name="PMA3/SDO2/CN10/RG8"/>
<pin name="PMA4/SDI2/CN9/RG7"/>
<pin name="PMA5/SCK2/CN8/RG6"/>
<pin name="PMA6/VREF+/CVREF+/RA10"/>
<pin name="PMA7/VREF-/CVREF-/RA9"/>
<pin name="PMA8/U2TX/CN18/RF5"/>
<pin name="PMA9/U2RX/CN17/RF4"/>
<pin name="PMA10/AN13/RB13"/>
<pin name="PMA11/AN12/RB12"/>
<pin name="PMA12/AN11/RB11"/>
<pin name="PMALH/PMA1/AN14/RB14"/>
<pin name="PMALL/PMA0/AN15/OCFB/CN12/RB15"/>
<pin name="PMD0/RE0"/>
<pin name="PMD1/RE1"/>
<pin name="PMD2/RE2"/>
<pin name="PMD3/RE3"/>
<pin name="PMD4/RE4"/>
<pin name="PMD5/RE5"/>
<pin name="PMD6/RE6"/>
<pin name="PMD7/RE7"/>
<pin name="PMD8/RG0"/>
<pin name="PMD9/RG1"/>
<pin name="PMD10/RF1"/>
<pin name="PMD11/RF0"/>
<pin name="PMD12/IC5/RD12"/>
<pin name="PMD13/CN19/RD13"/>
<pin name="PMD14/CN15/RD6"/>
<pin name="PMD15/CN16/RD7"/>
<pin name="PMRD/CN14/RD5"/>
<pin name="PMWR/OC5/CN13/RD4"/>
<pin name="RG15"/>
<pin name="SCL1/INT3/RA14"/>
<pin name="SCL2/RA2"/>
<pin name="SDA1/INT4/RA15"/>
<pin name="SDA2/RA3"/>
<pin name="SDI1/T5CK/RC4"/>
<pin name="SDO1/OC1/INT0/RD0"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="T2CK/RC1"/>
<pin name="T3CK/RC2"/>
<pin name="T4CK/RC3"/>
<pin name="TCK/RA1"/>
<pin name="TDI/RA4"/>
<pin name="TDO/RA5"/>
<pin name="TMS/RA0"/>
<pin name="TRCLK/RA6"/>
<pin name="TRD0/RG13"/>
<pin name="TRD1/RG12"/>
<pin name="TRD2/RG14"/>
<pin name="TRD3/RA7"/>
<pin name="U1RTS/BCLK1/CN21/RD15"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF8"/>
<pin name="U2CTS/RF12"/>
<pin name="U2RTS/BCLK2/RF13"/>
<pin name="USBID/RF3"/>
<pin name="VBUS"/>
<pin name="VBUSON/C1IN+/AN5/CN7/RB5"/>
<pin name="VCAP/VDDCORE"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VDD3"/>
<pin name="VDD4"/>
<pin name="VDD5"/>
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSS4"/>
<pin name="VSS6"/>
<pin name="VUSB"/>
</symbol>
<symbol name="TEMPERATURE-SENSOR">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="ADJ"/>
</symbol>
<symbol name="ADXRS">
<pin name="AVCC"/>
<pin name="VDD"/>
<pin name="AGND"/>
<pin name="PGND"/>
<pin name="VRATIO"/>
<pin name="RATEOUT"/>
<pin name="SUMJ"/>
<pin name="NC"/>
<pin name="ST1"/>
<pin name="ST2"/>
<pin name="TEMP"/>
<pin name="CP5"/>
<pin name="CP4"/>
<pin name="CP3"/>
<pin name="CP2"/>
<pin name="CP1"/>
</symbol>
<symbol name="7-SEGMENT-DISPLAY">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="DP"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="G1"/>
<pin name="G2"/>
</symbol>
<symbol name="HEF4543">
<pin name="A"/>
<pin name="B"/>
<pin name="BL"/>
<pin name="C"/>
<pin name="D"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="GND"/>
<pin name="LD"/>
<pin name="PH"/>
<pin name="VCC"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="7-SEGMENT-4DIGIT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="11"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="PHOTOCELL">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="MAGNET">
</symbol>
<symbol name="MAX7456">
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="CLKIN"/>
<pin name="XFB"/>
<pin name="CLKOUT"/>
<pin name="~CS"/>
<pin name="DIN"/>
<pin name="SCK"/>
<pin name="DOUT"/>
<pin name="LOS"/>
<pin name="~VSYNC"/>
<pin name="~HSYNC"/>
<pin name="~RESET"/>
<pin name="AGND"/>
<pin name="AVDD"/>
<pin name="VIN"/>
<pin name="PGND"/>
<pin name="PVDD"/>
<pin name="SAG"/>
<pin name="VOUT"/>
</symbol>
<symbol name="SPI_FLASH">
<pin name="CS"/>
<pin name="MISO"/>
<pin name="WP"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="HOLD"/>
<pin name="SCK"/>
<pin name="MOSI"/>
</symbol>
<symbol name="AD9835">
<pin name="FS_ADJ"/>
<pin name="REFIN"/>
<pin name="REFOUT"/>
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="MCLK"/>
<pin name="SCLK"/>
<pin name="SDATA"/>
<pin name="FSYNC"/>
<pin name="FSEL"/>
<pin name="PSEL1"/>
<pin name="PSEL0"/>
<pin name="AGND"/>
<pin name="IOUT"/>
<pin name="AVDD"/>
<pin name="COMP"/>
</symbol>
<symbol name="OSCILLATOR">
<pin name="EN"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="PSP_TOUCH_CONNECTOR">
<pin name="X1"/>
<pin name="Y2"/>
<pin name="X2"/>
<pin name="Y1"/>
</symbol>
<symbol name="DS_TOUCH_CONNECTOR">
<pin name="X1"/>
<pin name="Y2"/>
<pin name="X2"/>
<pin name="Y1"/>
</symbol>
<symbol name="L298_BRIDGE_DRIVER">
<pin name="GND@1"/>
<pin name="SENSE_A"/>
<pin name="NC@3"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="VS"/>
<pin name="IN1"/>
<pin name="ENA"/>
<pin name="IN2"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="VSS"/>
<pin name="IN3"/>
<pin name="ENB"/>
<pin name="IN4"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="NC@18"/>
<pin name="SENSE_B"/>
<pin name="GND@20"/>
</symbol>
<symbol name="GE864">
<pin name="EAR_MT-"/>
<pin name="EAR_MT+"/>
<pin name="EAR_HF+"/>
<pin name="EAR_HF-"/>
<pin name="MIC_MT+"/>
<pin name="MIC_MT-"/>
<pin name="MIC_HF+"/>
<pin name="MIC_HF-"/>
<pin name="AXE"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="TX_TRACE"/>
<pin name="RX_TRACE"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="DAC_OUT"/>
<pin name="ACD_IN1"/>
<pin name="ADC_IN2"/>
<pin name="ADC_IN3"/>
<pin name="RESET"/>
<pin name="VRTC"/>
<pin name="STAT_LED"/>
<pin name="CHARGE@G1"/>
<pin name="CHARGE@G2"/>
<pin name="ON_OFF"/>
<pin name="VAUX1"/>
<pin name="PWRMON"/>
<pin name="ANTENNA"/>
<pin name="DV12_CLK"/>
<pin name="TGPIO_12"/>
<pin name="TGPIO_03"/>
<pin name="TGPIO_04"/>
<pin name="TGPIO_20"/>
<pin name="TGPIO_14"/>
<pin name="TGPIO_11"/>
<pin name="TGPIO_19"/>
<pin name="TGPIO_01"/>
<pin name="TGPIO_18"/>
<pin name="TGPIO_17"/>
<pin name="TGPIO_15"/>
<pin name="TGPIO_08"/>
<pin name="TGPIO_06/ALARM"/>
<pin name="TGPIO_09"/>
<pin name="TGPIO_02/JDR"/>
<pin name="TGPIO_07/BUZZER"/>
<pin name="TGPIO_16"/>
<pin name="TGPIO_13"/>
<pin name="TGPIO_05/RFTXMON"/>
<pin name="TGPIO_21"/>
<pin name="TGPIO_22"/>
<pin name="TGPIO_10"/>
<pin name="VBATT@J1"/>
<pin name="VBATT@K1"/>
<pin name="VBATT@J2"/>
<pin name="VBATT@K2"/>
<pin name="GND@A1"/>
<pin name="GND@F1"/>
<pin name="GND@H1"/>
<pin name="GND@L1"/>
<pin name="GND@H2"/>
<pin name="GND@L2"/>
<pin name="GND@J3"/>
<pin name="GND@K3"/>
<pin name="GND@L3"/>
<pin name="GND@K4"/>
<pin name="GND@K5"/>
<pin name="GND@D6"/>
<pin name="GND@K6"/>
<pin name="GND@L6"/>
<pin name="GND@A11"/>
<pin name="GND@F11"/>
<pin name="GND@L11"/>
</symbol>
<symbol name="DIODE-ZENER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="GEIGER_TUBE">
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="TSOP8523">
<pin name="GND"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="OUT"/>
<pin name="VS"/>
</symbol>
<symbol name="RN41-1">
<pin name="AIO1"/>
<pin name="AIO2"/>
<pin name="GND"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="NC"/>
<pin name="PCMCLK"/>
<pin name="PCMIN"/>
<pin name="PCMOUT"/>
<pin name="PCMSYNC"/>
<pin name="PIO2"/>
<pin name="PIO3"/>
<pin name="PIO4"/>
<pin name="PIO5"/>
<pin name="PIO6"/>
<pin name="PIO7"/>
<pin name="PIO8"/>
<pin name="PIO9"/>
<pin name="PIO10"/>
<pin name="PIO11"/>
<pin name="RESET"/>
<pin name="SPICLK"/>
<pin name="SPICSB"/>
<pin name="SPIMISO"/>
<pin name="SPIMOSI"/>
<pin name="UARTCTS"/>
<pin name="UARTRTS"/>
<pin name="UARTRX"/>
<pin name="UARTTX"/>
<pin name="USBD+"/>
<pin name="USBD-"/>
<pin name="VDD"/>
</symbol>
<symbol name="ADXL193">
<pin name="VDD"/>
<pin name="VDD2"/>
<pin name="ST"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="GE865">
<pin name="EAR-"/>
<pin name="EAR+"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="TXD_AUX"/>
<pin name="RXD_AUX"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="DAC_OUT"/>
<pin name="ACD_IN1"/>
<pin name="ADC_IN2"/>
<pin name="RESET"/>
<pin name="VRTC"/>
<pin name="STAT_LED"/>
<pin name="ON_OFF"/>
<pin name="PWRMON"/>
<pin name="ANTENNA"/>
<pin name="GPIO_03"/>
<pin name="GPIO_04/TX_DISAB"/>
<pin name="GPIO_01"/>
<pin name="GPIO_08"/>
<pin name="GPIO_06/ALARM"/>
<pin name="GPIO_09"/>
<pin name="GPIO_02/JDR"/>
<pin name="GPIO_07/BUZZER"/>
<pin name="GPIO_05/RFTXMON"/>
<pin name="GPIO_10"/>
<pin name="VBATT@F1"/>
<pin name="VBATT@F2"/>
<pin name="VBATT@F3"/>
<pin name="GND@G1"/>
<pin name="GND@C2"/>
<pin name="GND@C7"/>
<pin name="GND@E5"/>
<pin name="GND@E7"/>
<pin name="GND@G5"/>
<pin name="GND@G4"/>
<pin name="GND@G3"/>
<pin name="GND@H3"/>
<pin name="GND@H6"/>
</symbol>
<symbol name="M13">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="ATARI_CONNECTOR">
<pin name="UP"/>
<pin name="DOWN"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="NC1"/>
<pin name="BUTTON"/>
<pin name="NC2"/>
<pin name="GND"/>
<pin name="NC3"/>
</symbol>
<symbol name="74LVC138AD">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="/E1"/>
<pin name="/E2"/>
<pin name="E3"/>
<pin name="/Y7"/>
<pin name="GND"/>
<pin name="/Y6"/>
<pin name="/Y5"/>
<pin name="/Y4"/>
<pin name="/Y3"/>
<pin name="/Y2"/>
<pin name="/Y1"/>
<pin name="/Y0"/>
<pin name="VCC"/>
</symbol>
<symbol name="GE865_2">
<pin name="EAR-"/>
<pin name="EAR+"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="TXD_AUX"/>
<pin name="RXD_AUX"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="DAC_OUT"/>
<pin name="ACD_IN1"/>
<pin name="ADC_IN2"/>
<pin name="RESET"/>
<pin name="VRTC"/>
<pin name="STAT_LED"/>
<pin name="ON_OFF"/>
<pin name="PWRMON"/>
<pin name="ANTENNA"/>
<pin name="GPIO_03"/>
<pin name="GPIO_04/TX_DISAB"/>
<pin name="GPIO_01"/>
<pin name="GPIO_08"/>
<pin name="GPIO_06/ALARM"/>
<pin name="GPIO_09"/>
<pin name="GPIO_02/JDR"/>
<pin name="GPIO_07/BUZZER"/>
<pin name="GPIO_05/RFTXMON"/>
<pin name="GPIO_10"/>
<pin name="VBATT@F1"/>
<pin name="VBATT@F2"/>
<pin name="VBATT@F3"/>
<pin name="GND@G1"/>
<pin name="GND@C2"/>
<pin name="GND@C7"/>
<pin name="GND@E5"/>
<pin name="GND@E7"/>
<pin name="GND@G5"/>
<pin name="GND@G4"/>
<pin name="GND@G3"/>
<pin name="GND@H3"/>
<pin name="GND@H6"/>
<pin name="SERVICE"/>
</symbol>
<symbol name="SD-MMC-CARD">
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VSS1"/>
<pin name="VDD"/>
<pin name="DAT1"/>
<pin name="DAT0"/>
<pin name="VSS2"/>
<pin name="CLK"/>
</symbol>
<symbol name="DPDT">
</symbol>
<symbol name="7-SEGMENT-1&quot;">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="G1"/>
<pin name="G2"/>
</symbol>
<symbol name="LM3480IM4">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="ZCT1009FTA">
<pin name="LOAD"/>
<pin name="VIN"/>
<pin name="IOUT"/>
</symbol>
<symbol name="ARDUINO_SHIELD">
<pin name="RX"/>
<pin name="TX"/>
<pin name="D2"/>
<pin name="*D3"/>
<pin name="D4"/>
<pin name="*D5"/>
<pin name="*D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="*D9"/>
<pin name="*D10"/>
<pin name="*D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VIN"/>
<pin name="RES"/>
<pin name="5V"/>
<pin name="AREF"/>
<pin name="GND@2"/>
<pin name="GND@1"/>
<pin name="GND@0"/>
<pin name="3.3V"/>
</symbol>
<symbol name="AVR_SPI_PROGRAMMER-1">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="U.FL">
<pin name="GND@0"/>
<pin name="SIGNAL"/>
<pin name="GND@1"/>
</symbol>
<symbol name="SIMHOLDER3">
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
</symbol>
<symbol name="M27">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
</symbol>
<symbol name="M17">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
</symbol>
<symbol name="M19">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
</symbol>
<symbol name="HMC5843">
<pin name="AVDD"/>
<pin name="DRDY"/>
<pin name="SDA"/>
<pin name="AGND"/>
<pin name="VREN"/>
<pin name="SCLP"/>
<pin name="SDAP"/>
<pin name="SCL"/>
<pin name="C1"/>
<pin name="SETC"/>
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="SVDD"/>
<pin name="SETN"/>
<pin name="SETP"/>
<pin name="OFFN"/>
<pin name="OFFP"/>
</symbol>
<symbol name="AD7302">
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="CS"/>
<pin name="WR"/>
<pin name="DGND"/>
<pin name="VOUTA"/>
<pin name="VOUTB"/>
<pin name="AGND"/>
<pin name="REFIN"/>
<pin name="VDD"/>
<pin name="CLR"/>
<pin name="LDAC"/>
<pin name="PD"/>
<pin name="AB"/>
</symbol>
<symbol name="BNC">
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="TURRET">
<pin name="1"/>
</symbol>
<symbol name="ADXL335">
<pin name="ST"/>
<pin name="COM@6"/>
<pin name="ZOUT"/>
<pin name="YOUT"/>
<pin name="XOUT"/>
<pin name="VS@14"/>
<pin name="VS@15"/>
<pin name="COM@5"/>
<pin name="COM@3"/>
<pin name="COM@7"/>
</symbol>
<symbol name="FIRST">
</symbol>
<symbol name="DC-DC_CONVERTER">
<pin name="VIN"/>
<pin name="GND1"/>
<pin name="ON/OFF"/>
<pin name="PGOOD"/>
<pin name="SEQ"/>
<pin name="VOUT"/>
<pin name="SENSE"/>
<pin name="TRIM"/>
<pin name="GND2"/>
</symbol>
<symbol name="GP1A57HR">
<pin name="2"/>
<pin name="1"/>
<pin name="5"/>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="RN-131G">
<pin name="SEN6"/>
<pin name="SEN4"/>
<pin name="SEN5"/>
<pin name="SEN7"/>
<pin name="RESET"/>
<pin name="EPC-A"/>
<pin name="EPC-B"/>
<pin name="S_CAP"/>
<pin name="F_AWAKE"/>
<pin name="GPIO-13"/>
<pin name="GPIO-12"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="MOSI"/>
<pin name="CLK"/>
<pin name="MISO"/>
<pin name="3.3V-ROUT"/>
<pin name="3.3V-RIN"/>
<pin name="GND@19"/>
<pin name="VDD-BATT"/>
<pin name="VDD-IN"/>
<pin name="DMA-TX"/>
<pin name="DMA-RX"/>
<pin name="GPIO-9"/>
<pin name="GPIO-8"/>
<pin name="GPIO-7"/>
<pin name="GPIO-6"/>
<pin name="GPIO-5"/>
<pin name="GPIO-4"/>
<pin name="SEN1"/>
<pin name="SEN2"/>
<pin name="SEN3"/>
<pin name="SENSE-PWR"/>
<pin name="SEN0"/>
<pin name="GND@36"/>
<pin name="GND@37"/>
<pin name="GND@38"/>
<pin name="GND@39"/>
<pin name="GND@40"/>
<pin name="GND@41"/>
<pin name="GND@42"/>
<pin name="GND@43"/>
<pin name="GND@44"/>
</symbol>
<symbol name="HTCUSB">
<pin name="USBVCC"/>
<pin name="USBDATA-"/>
<pin name="USBDATA+"/>
<pin name="N/C"/>
<pin name="USBGND"/>
<pin name="LEFTAUDIO"/>
<pin name="AG"/>
<pin name="AUDIOGRND"/>
<pin name="OT"/>
<pin name="RIGHTAUDIO"/>
<pin name="MIC"/>
</symbol>
<symbol name="SOIC_20W">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
</symbol>
<symbol name="CMA3000-A01">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="VDD1"/>
<pin name="Z"/>
<pin name="PD"/>
<pin name="RANGE"/>
<pin name="X"/>
<pin name="Y"/>
</symbol>
<symbol name="CMA3000-D01">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="DVIO"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="CS"/>
<pin name="INT"/>
</symbol>
<symbol name="ISL29102">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="NC"/>
<pin name="REXT"/>
<pin name="NC1"/>
<pin name="VOUT"/>
</symbol>
<symbol name="PCM1803A">
<pin name="VINL"/>
<pin name="VINR"/>
<pin name="VREF1"/>
<pin name="VREF2"/>
<pin name="VCCA"/>
<pin name="GNDA"/>
<pin name="PDWN"/>
<pin name="BPAS"/>
<pin name="TEST"/>
<pin name="LRCK"/>
<pin name="BCK"/>
<pin name="DOUT"/>
<pin name="GNDD"/>
<pin name="VDD"/>
<pin name="SCK"/>
<pin name="OSR"/>
<pin name="FMT0"/>
<pin name="FMT1"/>
<pin name="MD0"/>
<pin name="MD1"/>
</symbol>
<symbol name="TRACKBALL">
</symbol>
<symbol name="HALL-EFFECT">
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="WIFLY_GSX">
<pin name="EPCB"/>
<pin name="EPCA"/>
<pin name="FORCE_WAKE"/>
<pin name="RESET_L"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MISO"/>
<pin name="GPIO9"/>
<pin name="GPIO8"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="GPIO_13"/>
<pin name="GPIO_12"/>
<pin name="URX"/>
<pin name="UTX"/>
<pin name="VD_BAT"/>
<pin name="VD_3V_IN"/>
<pin name="SENS0"/>
<pin name="SENS1"/>
<pin name="SENS2"/>
<pin name="SENS3"/>
<pin name="SENS4"/>
<pin name="SENS5"/>
<pin name="SENS6"/>
<pin name="SENS7"/>
<pin name="SENSPWR"/>
<pin name="DMA_RX"/>
<pin name="DMA_TX"/>
<pin name="SUPCAP"/>
<pin name="3V3_OUT"/>
<pin name="3V3_IN"/>
<pin name="G9"/>
<pin name="G8"/>
<pin name="G7"/>
<pin name="G6"/>
<pin name="G5"/>
<pin name="G4"/>
<pin name="G3"/>
<pin name="G2"/>
<pin name="G1"/>
<pin name="G10"/>
<pin name="NC"/>
</symbol>
<symbol name="XMEGAA1">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
<pin name="P$41"/>
<pin name="P$42"/>
<pin name="P$43"/>
<pin name="P$44"/>
<pin name="P$45"/>
<pin name="P$46"/>
<pin name="P$47"/>
<pin name="P$48"/>
<pin name="P$49"/>
<pin name="P$50"/>
</symbol>
<symbol name="SM5100B">
<pin name="VBAT@0"/>
<pin name="VCHG@0"/>
<pin name="VBAT@1"/>
<pin name="VCHG@1"/>
<pin name="VBAT@2"/>
<pin name="ADIN1"/>
<pin name="VBAT@3"/>
<pin name="ADIN2"/>
<pin name="GND@0"/>
<pin name="GPIO_19"/>
<pin name="GND@1"/>
<pin name="EAR_MICN"/>
<pin name="GND@2"/>
<pin name="EAR_MICP"/>
<pin name="GND@3"/>
<pin name="EAR_SPKN"/>
<pin name="GND@4"/>
<pin name="EAR_SPKP"/>
<pin name="TXD0"/>
<pin name="RXD0"/>
<pin name="SIM_RST"/>
<pin name="GPIO_17"/>
<pin name="KEY_DRV3"/>
<pin name="KEY_DRV0"/>
<pin name="KEY_DRV4"/>
<pin name="KEY_DRV2"/>
<pin name="SIM_CLK"/>
<pin name="KEY_DRV1"/>
<pin name="SIM_DA"/>
<pin name="KEY_DRV5"/>
<pin name="KEY_SEN2"/>
<pin name="KEY_SEN1"/>
<pin name="GPO42/NBOOT"/>
<pin name="RESET"/>
<pin name="GPIO_4"/>
<pin name="KEY_SEN0"/>
<pin name="GPIO_10"/>
<pin name="GPIO_6"/>
<pin name="GPIO_1"/>
<pin name="KEY_SEN3"/>
<pin name="GPIO_9"/>
<pin name="AUX_MICP"/>
<pin name="RXD1"/>
<pin name="AUX_SPKP"/>
<pin name="GPIO_18"/>
<pin name="TXD1"/>
<pin name="VCC@0"/>
<pin name="RTC_BATT"/>
<pin name="GPIO_26"/>
<pin name="AUX_MICN"/>
<pin name="SIM_VCC"/>
<pin name="GPIO_16"/>
<pin name="GPO_11"/>
<pin name="GPIO_8"/>
<pin name="GPIO_3"/>
<pin name="GPIO_20"/>
<pin name="GPIO_46"/>
<pin name="AUX_SPKN"/>
<pin name="POWER_ON"/>
<pin name="VCC@1"/>
</symbol>
<symbol name="SSOP16">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
</symbol>
<symbol name="IXZ500">
<pin name="GND@2"/>
<pin name="GND@8"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="CPOUT"/>
<pin name="ZAGC"/>
<pin name="XAGC"/>
<pin name="VDD@19"/>
<pin name="VDD@9"/>
<pin name="X4.5IN"/>
<pin name="XOUT"/>
<pin name="X4.5OUT"/>
<pin name="Z4.5IN"/>
<pin name="ZOUT"/>
<pin name="Z4.5OUT"/>
<pin name="PTATS"/>
<pin name="AZ"/>
<pin name="VREF"/>
</symbol>
<symbol name="MICRO-SDCARD">
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="GND"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
</symbol>
<symbol name="CY7C64215">
<pin name="VSS@1"/>
<pin name="P07"/>
<pin name="P05"/>
<pin name="P03"/>
<pin name="P01"/>
<pin name="P25"/>
<pin name="P23"/>
<pin name="P21"/>
<pin name="P17"/>
<pin name="P15"/>
<pin name="P13"/>
<pin name="P11"/>
<pin name="VSS@13"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VDD@16"/>
<pin name="P10"/>
<pin name="P12"/>
<pin name="P14"/>
<pin name="P16"/>
<pin name="P20"/>
<pin name="P22"/>
<pin name="P24"/>
<pin name="P00"/>
<pin name="P02"/>
<pin name="P04"/>
<pin name="P06"/>
<pin name="VDD@28"/>
</symbol>
<symbol name="MEMS-MIC">
<pin name="VIN"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="OUT"/>
</symbol>
<symbol name="SMARTCARD">
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="I/O"/>
<pin name="VPP"/>
<pin name="GND"/>
<pin name="C4"/>
<pin name="C8"/>
</symbol>
<symbol name="XS1-L1-64LQFP">
<pin name="VDDIO_6"/>
<pin name="VDDIO_18"/>
<pin name="VDDIO_32"/>
<pin name="VDDIO_40"/>
<pin name="VDDIO_53"/>
<pin name="VDDIO_60"/>
<pin name="VDD_4"/>
<pin name="VDD_13"/>
<pin name="VDD_21"/>
<pin name="VDD_28"/>
<pin name="VDD_37"/>
<pin name="VDD_43"/>
<pin name="VDD_52"/>
<pin name="VDD_61"/>
<pin name="PLL_AVDD"/>
<pin name="PLL_AGND"/>
<pin name="MODE0"/>
<pin name="MODE1"/>
<pin name="MODE2"/>
<pin name="MODE3"/>
<pin name="DEBUG"/>
<pin name="RST_N"/>
<pin name="CLK"/>
<pin name="TDO"/>
<pin name="TDI"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="TRST_N"/>
<pin name="GND"/>
<pin name="X0D0"/>
<pin name="X0D1"/>
<pin name="X0D2"/>
<pin name="X0D3"/>
<pin name="X0D4"/>
<pin name="X0D5"/>
<pin name="X0D6"/>
<pin name="X0D7"/>
<pin name="X0D8"/>
<pin name="X0D9"/>
<pin name="X0D10"/>
<pin name="X0D11"/>
<pin name="X0D12"/>
<pin name="X0D13"/>
<pin name="X0D14"/>
<pin name="X0D15"/>
<pin name="X0D16"/>
<pin name="X0D17"/>
<pin name="X0D18"/>
<pin name="X0D19"/>
<pin name="X0D20"/>
<pin name="X0D21"/>
<pin name="X0D22"/>
<pin name="X0D23"/>
<pin name="X0D24"/>
<pin name="X0D25"/>
<pin name="X0D26"/>
<pin name="X0D32"/>
<pin name="X0D33"/>
<pin name="X0D34"/>
<pin name="X0D35"/>
<pin name="X0D36"/>
<pin name="X0D37"/>
<pin name="X0D38"/>
<pin name="X0D27"/>
<pin name="X0D39"/>
</symbol>
<symbol name="PIC32MX440F512H">
<pin name="RE5/PMD5"/>
<pin name="RE6/PMD6"/>
<pin name="RE7/PMD7"/>
<pin name="RG6/PMA5/SCK2/CN8"/>
<pin name="RG7/PMA4/SDI2/CN9"/>
<pin name="RG8/PMA3/SDO2/CN10"/>
<pin name="~MCLR"/>
<pin name="RG9/PMA2/~SS2/CN11"/>
<pin name="VSS@9"/>
<pin name="VDD@10"/>
<pin name="RB5/AN5/VBUSON/C1IN+/CN7"/>
<pin name="RB4/AN4/C1IN-/CN6"/>
<pin name="RB3/AN3/C2IN+/CN5"/>
<pin name="RB2/AN2/C2IN-/CN4"/>
<pin name="RB1/AN1/PGEC1/VREF-/CVREF-/CN3"/>
<pin name="RB0/AN0/PGED1/EMUD1/PMA6/VREF+/CVREF+/CN2"/>
<pin name="RB6/AN6/PGEC2/OCFA"/>
<pin name="RB7/AN7/PGED2"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="RB8/AN8/~U2CTS/C1OUT"/>
<pin name="RB9/AN9/PMA7/C2OUT"/>
<pin name="RB10/AN10/TMS/CVREFOUT/PMA13"/>
<pin name="RB11/AN11/TDO/PMA12"/>
<pin name="VSS@25"/>
<pin name="VDD@26"/>
<pin name="RB12/AN12/TCK/PMA11"/>
<pin name="RB13/AN13/TDI/PMA10"/>
<pin name="RB14/AN14/PMALH/PMA1/~U2RTS/BCLK2"/>
<pin name="RB15/AN15/PMALL/PMA0/OCFB/CN12"/>
<pin name="RF4/PMA9/U2RX/SDA2/CN17"/>
<pin name="RF5/PMA8/U2TX/SCL2/CN18"/>
<pin name="RF3/USBID"/>
<pin name="VBUS"/>
<pin name="VUSB"/>
<pin name="D-/RG3"/>
<pin name="D+/RG2"/>
<pin name="VDD@38"/>
<pin name="RC12/OSC1/CLKI"/>
<pin name="RC15/OSC2/CLKO"/>
<pin name="VSS@41"/>
<pin name="RD8/IC1/RTCC/INT1"/>
<pin name="RD9/IC2/~U1CTS//INT2/SDA1"/>
<pin name="RD10/IC3/PMCS2/PMA15/INT3/SCL1"/>
<pin name="RD11/IC4/PMCS1/PMA14/INT4"/>
<pin name="RD0/OC1/INT0"/>
<pin name="RC13/SOSCI/CN1"/>
<pin name="RC14/SOSCO/T1CK/CN0"/>
<pin name="RD1/OC2/~U1RTS/BCLK1"/>
<pin name="RD2/OC3/U1RX"/>
<pin name="RD3/OC4/U1TX"/>
<pin name="RD4/PMWR/OC5/IC5/CN13"/>
<pin name="RD5/PMRD/CN14"/>
<pin name="RD6/CN15"/>
<pin name="RD7/CN16"/>
<pin name="VCAP/VDDCORE"/>
<pin name="ENVREG"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RE0/PMD0"/>
<pin name="RE1/PMD1"/>
<pin name="RE2/PMD2"/>
<pin name="RE3/PMD3"/>
<pin name="RE4/PMD4"/>
</symbol>
<symbol name="TMP102">
<pin name="SCL"/>
<pin name="GND"/>
<pin name="ALERT"/>
<pin name="ADD0"/>
<pin name="VCC"/>
<pin name="SDA"/>
</symbol>
<symbol name="NCP303LSN09">
<pin name="RST"/>
<pin name="IN"/>
<pin name="GND"/>
<pin name="CD"/>
<pin name="NC"/>
</symbol>
<symbol name="BD10KA5WF-E2">
<pin name="OUT"/>
<pin name="VCC"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="CTL"/>
</symbol>
<symbol name="1.0V">
<pin name="1.0V" direction="sup"/>
</symbol>
<symbol name="LM4128-2.5VREF">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="ST-GYRO-PR">
<pin name="4XINX"/>
<pin name="4XINY"/>
<pin name="4XOUTX"/>
<pin name="4XOUTY"/>
<pin name="FILTVDD"/>
<pin name="GND"/>
<pin name="HP"/>
<pin name="OUTX"/>
<pin name="OUTY"/>
<pin name="PD"/>
<pin name="RES@14"/>
<pin name="RES@15"/>
<pin name="ST"/>
<pin name="VCONT"/>
<pin name="VDD"/>
<pin name="VREF"/>
</symbol>
<symbol name="ST-GYRO-PY">
<pin name="4XINZ"/>
<pin name="4XINX"/>
<pin name="4XOUTZ"/>
<pin name="4XOUTX"/>
<pin name="FILTVDD"/>
<pin name="GND"/>
<pin name="HP"/>
<pin name="OUTZ"/>
<pin name="OUTX"/>
<pin name="PD"/>
<pin name="RES@14"/>
<pin name="RES@15"/>
<pin name="ST"/>
<pin name="VCONT"/>
<pin name="VDD"/>
<pin name="VREF"/>
</symbol>
<symbol name="TVS">
<pin name="A1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="LM2931">
<pin name="OUT"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="ADJ"/>
<pin name="INH"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="IN"/>
</symbol>
<symbol name="MC9S12XS64">
<pin name="PWM3/KWP3/PP3"/>
<pin name="TXD1/IOC2/PWM2/KWP2/PP2"/>
<pin name="IOC1/PWM1/KWP1/PP1"/>
<pin name="RXD1/IOC0/PWM0/KWP0/PP0"/>
<pin name="IOC0/PT0"/>
<pin name="IOC1/PT1"/>
<pin name="IOC2/PT2"/>
<pin name="IOC3/PT3"/>
<pin name="VDDF"/>
<pin name="VSS1"/>
<pin name="PWM4/IOC4/PT4"/>
<pin name="VREG_API/PWM5/IOC5/PT"/>
<pin name="PWM6/IOC6/PT6"/>
<pin name="PWM7/IOC7/PT7"/>
<pin name="MODC/BKGD"/>
<pin name="PB0"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="XCLKS/ECLKX2/PE7"/>
<pin name="ECLK/PE4"/>
<pin name="VSSX2"/>
<pin name="VDDX2"/>
<pin name="RESET"/>
<pin name="VDDR"/>
<pin name="VSS3"/>
<pin name="VSSPLL"/>
<pin name="EXTAL"/>
<pin name="XTAL"/>
<pin name="VDDPLL"/>
<pin name="IRQ/PE1"/>
<pin name="XIRQ/PE0"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="VDD"/>
<pin name="VSS2"/>
<pin name="PAD00/AN00"/>
<pin name="PAD01/AN01"/>
<pin name="PAD02/AN02"/>
<pin name="PAD03/AN03"/>
<pin name="PAD04/AN04"/>
<pin name="PAD05/AN05"/>
<pin name="PAD06/AN06"/>
<pin name="PAD07/AN07"/>
<pin name="VDDA"/>
<pin name="VRH"/>
<pin name="VSSA/VRL"/>
<pin name="PS0/RXD0"/>
<pin name="PS1/TXD0"/>
<pin name="PS2/RXD1"/>
<pin name="PS3/TXD1"/>
<pin name="TEST"/>
<pin name="PM5/SCK0"/>
<pin name="PM4/MOSI0"/>
<pin name="PM3/SS0"/>
<pin name="PM2/MISO0"/>
<pin name="PM1/TXCAN0/TXD1"/>
<pin name="PM0/RXCAN0/RXD1"/>
<pin name="VSSX1"/>
<pin name="VDDX1"/>
<pin name="PP7/KWP7/PWM7"/>
<pin name="PP5/KPW5/PWM5"/>
</symbol>
<symbol name="TJA1040TD-T">
<pin name="TXD"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="RXD"/>
<pin name="SPLIT"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="STB"/>
</symbol>
<symbol name="LM2931_FIXED">
<pin name="VIN"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="JOYSTICK-PSP1000">
<pin name="X"/>
<pin name="Y"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="SCHOTTKY_BRIDGE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SC16IS750">
<pin name="RESET"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VDD"/>
<pin name="I2C-/SPI"/>
<pin name="A0-/CS"/>
<pin name="A1-SI"/>
<pin name="NC-SO"/>
<pin name="SCL-SCLK"/>
<pin name="SDA-VSS"/>
<pin name="/IRQ"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="VSS"/>
<pin name="GPIO4-/DSR"/>
<pin name="GPIO5-/DTR"/>
<pin name="GPIO6-/CD"/>
<pin name="GPIO7-/RI"/>
<pin name="/RTS"/>
<pin name="/CTS"/>
<pin name="TX"/>
<pin name="RX"/>
</symbol>
<symbol name="LPC2103">
<pin name="P0.19/MAT1.2/MISO1"/>
<pin name="P0.20/MAT1.3/MOSI1"/>
<pin name="P0.21/SSEL1/MAT3.0"/>
<pin name="VBAT"/>
<pin name="VDD(1V8)"/>
<pin name="RST"/>
<pin name="VSS@7"/>
<pin name="P0.27/TRST/CAP2.0"/>
<pin name="P0.28/TMS/CAP2.1"/>
<pin name="P0.29/TCK/CAP2.2"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="P0.0/TXD0/MAT3.1"/>
<pin name="P0.1/RXD0/MAT3.2"/>
<pin name="P0.30/TDI/MAT3.3"/>
<pin name="P0.31/TDO"/>
<pin name="VDD(3V3)@17"/>
<pin name="P0.2/SCL0/CAP0.0"/>
<pin name="VSS@19"/>
<pin name="RTCX1"/>
<pin name="P0.3/SDA0/MAT0.0"/>
<pin name="P0.4/SCK0/CAP0.1"/>
<pin name="P0.5/MISO0/MAT0.1"/>
<pin name="P0.6/MOSI0/CAP0.2"/>
<pin name="RTCX2"/>
<pin name="RTCK"/>
<pin name="DBGSEL"/>
<pin name="P0.7/SSEL0/MAT2.0"/>
<pin name="P0.8/TXD1/MAT2.1"/>
<pin name="P0.9/RXD1/MAT2.2"/>
<pin name="VSSA"/>
<pin name="P0.22/AD0.0"/>
<pin name="P0.23/AD0.1"/>
<pin name="P0.24/AD0.2"/>
<pin name="P0.10/RTS1/CAP1.0/AD0.3"/>
<pin name="P0.11/CTS1/CAP1.1/AD0.4"/>
<pin name="P0.12/DSR1/MAT1.0/AD0.5"/>
<pin name="P0.25/AD0.6"/>
<pin name="P0.26/AD0.7"/>
<pin name="VDD(3V3)@40"/>
<pin name="P0.13/DTR1/MAT1.1"/>
<pin name="VDDA"/>
<pin name="VSS@43"/>
<pin name="P0.14/DCD1/SCK1/EINT1"/>
<pin name="P0.15/RI1/EINT2"/>
<pin name="P0.16/EINT0/MAT0.2"/>
<pin name="P0.17/CAP1.2/SCL1"/>
<pin name="P0.18/CAP1.3/SDA1"/>
</symbol>
<symbol name="TCM8240MD">
<pin name="DOUT3"/>
<pin name="DOUT2"/>
<pin name="DOUT1"/>
<pin name="DOUT0"/>
<pin name="GND@5"/>
<pin name="PVDD(2.8V)"/>
<pin name="RESET"/>
<pin name="SCL"/>
<pin name="GND@9"/>
<pin name="SDA"/>
<pin name="GND@11"/>
<pin name="DVDD(1.6V)"/>
<pin name="EXTCLK"/>
<pin name="STROBE"/>
<pin name="HBLK"/>
<pin name="VBLK"/>
<pin name="GND@17"/>
<pin name="IOVDD"/>
<pin name="DCLK"/>
<pin name="GND@20"/>
<pin name="DOUT7"/>
<pin name="DOUT6"/>
<pin name="DOUT5"/>
<pin name="DOUT4"/>
</symbol>
<symbol name="M04X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="MIC2571-1">
<pin name="IN"/>
<pin name="GND"/>
<pin name="SW"/>
<pin name="2.85V"/>
<pin name="3.3V"/>
<pin name="5V"/>
<pin name="SYNC"/>
</symbol>
<symbol name="BUFFER-DUAL">
<pin name="A2"/>
<pin name="A1"/>
<pin name="GND"/>
<pin name="Y1"/>
<pin name="VCC"/>
<pin name="Y2"/>
</symbol>
<symbol name="M2X8">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="SIT8002">
<pin name="/ST-OE"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VDD"/>
</symbol>
<symbol name="AT25FS010">
<pin name="SI"/>
<pin name="SCK"/>
<pin name="HOLD" function="dot"/>
<pin name="CS" function="dot"/>
<pin name="WP" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="GS406SMD">
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
</symbol>
<symbol name="FT2232D">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="BDBUS0" direction="out"/>
<pin name="BDBUS1" direction="in"/>
<pin name="BDBUS2" direction="out"/>
<pin name="BDBUS3" direction="in"/>
<pin name="BDBUS4" direction="out"/>
<pin name="BDBUS5" direction="in"/>
<pin name="BDBUS6" direction="in"/>
<pin name="BDBUS7" direction="in"/>
<pin name="PWEN#"/>
<pin name="VCCIOA" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC2" direction="pwr"/>
<pin name="RSTOUT#"/>
<pin name="RESET#"/>
<pin name="XTIN"/>
<pin name="XTOUT"/>
<pin name="EECS"/>
<pin name="EESK"/>
<pin name="EEDATA"/>
<pin name="GND4"/>
<pin name="SI/WUB"/>
<pin name="BCBUS3"/>
<pin name="BCBUS2"/>
<pin name="BCBUS1"/>
<pin name="BCBUS0"/>
<pin name="ACBUS2"/>
<pin name="ACBUS1"/>
<pin name="ACBUS0"/>
<pin name="ADBUS7"/>
<pin name="ADBUS6"/>
<pin name="ADBUS5"/>
<pin name="SI/WUA"/>
<pin name="ACBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS3"/>
<pin name="ADBUS2"/>
<pin name="ADBUS1"/>
<pin name="ADBUS0"/>
<pin name="VCC1" direction="pwr"/>
<pin name="AVCC"/>
<pin name="VCCIOB"/>
</symbol>
<symbol name="M93C46">
<pin name="CS"/>
<pin name="SK"/>
<pin name="DIN"/>
<pin name="DOUT"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="QRE1113">
<pin name="A"/>
<pin name="E"/>
<pin name="C"/>
<pin name="K"/>
</symbol>
<symbol name="RS485">
<pin name="RO"/>
<pin name="/RE"/>
<pin name="DE"/>
<pin name="DI"/>
<pin name="VCC"/>
<pin name="B"/>
<pin name="A"/>
<pin name="GND"/>
</symbol>
<symbol name="TB6612FNG">
<pin name="A01@1"/>
<pin name="A01@2"/>
<pin name="PGND1@3"/>
<pin name="PGND1@4"/>
<pin name="A02@5"/>
<pin name="A02@6"/>
<pin name="B02@7"/>
<pin name="B02@8"/>
<pin name="PGND2@9"/>
<pin name="PGND2@10"/>
<pin name="B01@11"/>
<pin name="B01@12"/>
<pin name="VM2"/>
<pin name="VM3"/>
<pin name="PWMB"/>
<pin name="BIN2"/>
<pin name="BIN1"/>
<pin name="GND"/>
<pin name="STBY"/>
<pin name="VCC"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="PWMA"/>
<pin name="VM1"/>
</symbol>
<symbol name="M24">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="XTEND-DIGI-MODEM">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="GPO2"/>
<pin name="TX_PWR"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="SHDN"/>
<pin name="SLEEP"/>
<pin name="CTS"/>
<pin name="RTS"/>
<pin name="CONFIG"/>
</symbol>
<symbol name="7-SEGMENT-4DIGIT-YOUNGSUN">
<pin name="DIG2"/>
<pin name="DIG3"/>
<pin name="DIG4"/>
<pin name="COL-A"/>
<pin name="APOS-A"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="COL-C"/>
<pin name="APOS-C"/>
<pin name="DIG1"/>
</symbol>
<symbol name="RESONATOR_NOCAP">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="LMD1820X">
<pin name="BS1"/>
<pin name="OUT1"/>
<pin name="DIR"/>
<pin name="BRK"/>
<pin name="PWM"/>
<pin name="PWR"/>
<pin name="PGND"/>
<pin name="SGND"/>
<pin name="TF"/>
<pin name="OUT2"/>
<pin name="BS2"/>
</symbol>
<symbol name="M18">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="STA540">
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="IN3"/>
<pin name="SVR"/>
<pin name="IN4"/>
<pin name="P-GND"/>
<pin name="S-GND"/>
<pin name="DIAG"/>
<pin name="OUT4"/>
<pin name="OUT3"/>
<pin name="OUT2"/>
<pin name="OUT1"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="STBY"/>
</symbol>
<symbol name="L298">
<pin name="OUT1"/>
<pin name="VS"/>
<pin name="ENA"/>
<pin name="GND"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="OUT4"/>
<pin name="CSA"/>
<pin name="OUT2"/>
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="VLS"/>
<pin name="ENB"/>
<pin name="OUT3"/>
<pin name="CSB"/>
</symbol>
<symbol name="XMEGA">
<pin name="GND@84"/>
<pin name="GND@93"/>
<pin name="AVCC@4"/>
<pin name="AVCC@94"/>
<pin name="GND@3"/>
<pin name="GND@13"/>
<pin name="GND@23"/>
<pin name="GND@33"/>
<pin name="GND@43"/>
<pin name="GND@53"/>
<pin name="GND@63"/>
<pin name="GND@73"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PDI/PDI_DATA"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PH0"/>
<pin name="PH1"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PJ0"/>
<pin name="PJ1"/>
<pin name="PJ2"/>
<pin name="PJ3"/>
<pin name="PJ4"/>
<pin name="PJ5"/>
<pin name="PJ6"/>
<pin name="PJ7"/>
<pin name="PK0"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="PK3"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PK6"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="RESET/PDI_CLOCK"/>
<pin name="VCC@14"/>
<pin name="VCC@24"/>
<pin name="VCC@34"/>
<pin name="VCC@44"/>
<pin name="VCC@54"/>
<pin name="VCC@64"/>
<pin name="VCC@74"/>
<pin name="VCC@83"/>
</symbol>
<symbol name="ILD213T">
<pin name="C2"/>
<pin name="A2"/>
<pin name="C1"/>
<pin name="A1"/>
<pin name="ET2"/>
<pin name="CT2"/>
<pin name="ET1"/>
<pin name="CT1"/>
</symbol>
<symbol name="MIDI_CONN_FEMALE">
<pin name="NC3"/>
<pin name="NC2"/>
<pin name="NC1"/>
<pin name="MIDI_OUT"/>
<pin name="MIDI_IN"/>
</symbol>
<symbol name="HIH-4030">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="OVERTONE_LOGO">
</symbol>
<symbol name="ISZ-500">
<pin name="GND@28"/>
<pin name="GND@27"/>
<pin name="GND@26"/>
<pin name="GND@8"/>
<pin name="GND@2"/>
<pin name="VDD@9"/>
<pin name="VDD@19"/>
<pin name="CPOUT"/>
<pin name="Z4.5OUT"/>
<pin name="ZAGC"/>
<pin name="Z4.5IN"/>
<pin name="Z-OUT"/>
<pin name="VREF"/>
<pin name="PTATS"/>
<pin name="AZ"/>
</symbol>
<symbol name="DSPIC30F6015">
<pin name="VDD@10"/>
<pin name="VDD@26"/>
<pin name="VDD@38"/>
<pin name="VDD@57"/>
<pin name="AVDD@19"/>
<pin name="MCLR@7"/>
<pin name="PGC@17"/>
<pin name="PGD@18"/>
<pin name="OSC1@39"/>
<pin name="OSC2@40"/>
<pin name="RX1@34"/>
<pin name="TX1@33"/>
<pin name="VREF+/RB0@16"/>
<pin name="VREF-/RB1@15"/>
<pin name="RB2@14"/>
<pin name="RB3@13"/>
<pin name="RB4@12"/>
<pin name="RB5@11"/>
<pin name="RB8@21"/>
<pin name="RB9@22"/>
<pin name="RB10@23"/>
<pin name="RB11@24"/>
<pin name="RB12@27"/>
<pin name="RB13@28"/>
<pin name="RB14@29"/>
<pin name="RB15@30"/>
<pin name="GND@56"/>
<pin name="GND@41"/>
<pin name="GND@25"/>
<pin name="GND@9"/>
<pin name="AGND@20"/>
<pin name="RC13@47"/>
<pin name="RC14@48"/>
<pin name="RD0@46"/>
<pin name="RD1@49"/>
<pin name="RD2@50"/>
<pin name="RD3@51"/>
<pin name="RD4@52"/>
<pin name="RD5@53"/>
<pin name="RD6@54"/>
<pin name="RD7@55"/>
<pin name="RG8@6"/>
<pin name="RG9@8"/>
<pin name="RG2@37"/>
<pin name="RD8@42"/>
<pin name="RF6@35"/>
<pin name="RG3@36"/>
<pin name="RD9@43"/>
<pin name="RD10@44"/>
<pin name="RD11@45"/>
<pin name="RF0@58"/>
<pin name="RF1@59"/>
<pin name="RE0@60"/>
<pin name="RE1@61"/>
<pin name="RE2@62"/>
<pin name="RE3@63"/>
<pin name="RG7@5"/>
<pin name="RG6@4"/>
<pin name="RE7@3"/>
<pin name="RE6@2"/>
<pin name="RE5@1"/>
<pin name="RE4@64"/>
<pin name="TX2@31"/>
<pin name="RX2@32"/>
</symbol>
<symbol name="MIC5216">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="VOUT"/>
<pin name="FLAG"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
</symbol>
<symbol name="DIL-28-3">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
</symbol>
<symbol name="DIL-40-6">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
</symbol>
<symbol name="SSOP20">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
</symbol>
<symbol name="ATX24">
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="3.3V@0"/>
<pin name="3.3V@1"/>
<pin name="3.3V@2"/>
<pin name="3.3V@3"/>
<pin name="5V@0"/>
<pin name="5V@1"/>
<pin name="5V@2"/>
<pin name="5V@3"/>
<pin name="5V@4"/>
<pin name="12V@0"/>
<pin name="12V@1"/>
<pin name="-12V"/>
<pin name="PS_ON"/>
<pin name="PWR_OK"/>
<pin name="5V_STDBY"/>
<pin name="NC"/>
</symbol>
<symbol name="KENT_LCD_CONN">
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSS4"/>
<pin name="VCC"/>
<pin name="VPWR1"/>
<pin name="VPWR2"/>
<pin name="VPWR3"/>
<pin name="/RESET"/>
<pin name="BUSY"/>
<pin name="SCK"/>
<pin name="SO"/>
<pin name="SI"/>
<pin name="CS"/>
<pin name="NC1"/>
<pin name="NC2"/>
</symbol>
<symbol name="OPTO_DARLINGTON_6N138-39">
<pin name="C"/>
<pin name="A"/>
<pin name="VCC"/>
<pin name="VOUT"/>
<pin name="GND"/>
</symbol>
<symbol name="6400GB_HEATSINK">
</symbol>
<symbol name="ISD1932">
<pin name="_REC"/>
<pin name="_PLAYE/FMC2"/>
<pin name="_PLAYL/FMC1"/>
<pin name="S3/_M4"/>
<pin name="S2/_M3"/>
<pin name="S1/_M2"/>
<pin name="S0/_M1"/>
<pin name="E3/_M8"/>
<pin name="E2/_M7"/>
<pin name="E1/_M6"/>
<pin name="E0/_M5"/>
<pin name="_FT"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="AGC"/>
<pin name="ROSC"/>
<pin name="SP-"/>
<pin name="SP+"/>
<pin name="VSSP2"/>
<pin name="VSSP1"/>
<pin name="VCCP"/>
<pin name="VSSA"/>
<pin name="VCCA"/>
<pin name="VSSD"/>
<pin name="VCCD"/>
<pin name="XCLK/FMC3"/>
<pin name="_LED"/>
<pin name="ADDR/_DRCT"/>
</symbol>
<symbol name="M74HC238">
<pin name="VCC"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="G1"/>
<pin name="~G2B"/>
<pin name="~G2A"/>
<pin name="GND"/>
<pin name="Y7"/>
<pin name="Y6"/>
<pin name="Y5"/>
<pin name="Y4"/>
<pin name="Y3"/>
<pin name="Y2"/>
<pin name="Y1"/>
<pin name="Y0"/>
</symbol>
<symbol name="ENC28J60">
<pin name="VCAP"/>
<pin name="VSS"/>
<pin name="CLKOUT"/>
<pin name="/INT"/>
<pin name="NC"/>
<pin name="SO"/>
<pin name="SI"/>
<pin name="SCK"/>
<pin name="CS"/>
<pin name="RESET"/>
<pin name="VSSRX"/>
<pin name="TPIN-"/>
<pin name="TPIN+"/>
<pin name="RBIAS"/>
<pin name="VDDTX"/>
<pin name="TPOUT-"/>
<pin name="TPOUT+"/>
<pin name="VSSTX"/>
<pin name="VDDRX"/>
<pin name="VDDPLL"/>
<pin name="VSSPLL"/>
<pin name="VSSOSC"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="VDDOSC"/>
<pin name="LEDB"/>
<pin name="LEDA"/>
<pin name="VDD"/>
</symbol>
<symbol name="MAX3421E">
<pin name="VCC"/>
<pin name="VL"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBCOMP"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="INT"/>
<pin name="RES"/>
<pin name="GPX"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="SS"/>
<pin name="GND@3"/>
<pin name="GND@19"/>
<pin name="GOUT7"/>
<pin name="GOUT6"/>
<pin name="GOUT5"/>
<pin name="GOUT4"/>
<pin name="GOUT3"/>
<pin name="GOUT2"/>
<pin name="GOUT1"/>
<pin name="GOUT0"/>
<pin name="GPIN7"/>
<pin name="GPIN6"/>
<pin name="GPIN5"/>
<pin name="GPIN4"/>
<pin name="GPIN3"/>
<pin name="GPIN2"/>
<pin name="GPIN1"/>
<pin name="GPIN0"/>
</symbol>
<symbol name="LITTLEBITS">
<pin name="GND"/>
<pin name="SIG"/>
<pin name="VCC"/>
</symbol>
<symbol name="FUSE">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="SPEAKJET">
<pin name="E0"/>
<pin name="E1"/>
<pin name="E2"/>
<pin name="E3"/>
<pin name="E4"/>
<pin name="E5"/>
<pin name="E6/RC0"/>
<pin name="E7/RC1"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="RX"/>
<pin name="RST"/>
<pin name="M0"/>
<pin name="M1"/>
<pin name="D0/RDY"/>
<pin name="D1/SPK"/>
<pin name="D2/BHF"/>
<pin name="VOICE"/>
</symbol>
<symbol name="LITTLEBITS_MALE">
<pin name="GND"/>
<pin name="SIG"/>
<pin name="VCC"/>
</symbol>
<symbol name="LITTLEBITS_FEMALE">
<pin name="VCC"/>
<pin name="SIG"/>
<pin name="GND"/>
</symbol>
<symbol name="SN74HC251">
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="Y"/>
<pin name="W"/>
<pin name="OE"/>
<pin name="GND"/>
<pin name="C"/>
<pin name="B"/>
<pin name="A"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="VCC"/>
</symbol>
<symbol name="USB3318">
<pin name="DATA7"/>
<pin name="DATA6"/>
<pin name="DATA5"/>
<pin name="DATA4"/>
<pin name="DATA3"/>
<pin name="DATA2"/>
<pin name="DATA1"/>
<pin name="DATA0"/>
<pin name="STP"/>
<pin name="NXT"/>
<pin name="DIR"/>
<pin name="CLKOUT"/>
<pin name="RESETB"/>
<pin name="REFCLK"/>
<pin name="RBIAS"/>
<pin name="VBUS"/>
<pin name="VBAT"/>
<pin name="VDD33"/>
<pin name="VDDIO"/>
<pin name="VDD18"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="ID"/>
<pin name="CPEN"/>
<pin name="GND1"/>
<pin name="GND2"/>
</symbol>
<symbol name="MPR121">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="VREG"/>
<pin name="~IRQ"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="ADDR"/>
<pin name="REXT"/>
<pin name="ELE11/LED7"/>
<pin name="ELE10/LED6"/>
<pin name="ELE9/LED5"/>
<pin name="ELE8/LED4"/>
<pin name="ELE7/LED3"/>
<pin name="ELE6/LED2"/>
<pin name="ELE5/LED1"/>
<pin name="ELE4/LED0"/>
<pin name="ELE3"/>
<pin name="ELE2"/>
<pin name="ELE1"/>
<pin name="ELE0"/>
</symbol>
<symbol name="MMA7361">
<pin name="XOUT"/>
<pin name="YOUT"/>
<pin name="ZOUT"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="SLEEP"/>
<pin name="0GD"/>
<pin name="GSELECT"/>
<pin name="ST"/>
</symbol>
<symbol name="ATMEGA128">
<pin name="VCC@21"/>
<pin name="VCC@52"/>
<pin name="AVCC"/>
<pin name="AREF"/>
<pin name="RESET"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AGND"/>
<pin name="GND@53"/>
<pin name="GND@22"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PE0(RXD)"/>
<pin name="PE1(TXD)"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1(SDA)"/>
<pin name="PD0(SCL)"/>
<pin name="PC7"/>
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="PB7"/>
<pin name="PB6"/>
<pin name="PB5"/>
<pin name="PB4"/>
<pin name="PB3(MISO)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB1(SCK)"/>
<pin name="PB0(SS)"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
</symbol>
<symbol name="SCREENKEYMATINGCONNECTOR">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
</symbol>
<symbol name="FIO_LOGO">
</symbol>
<symbol name="BMP085">
<pin name="XCLR" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="NC"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="EOC" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="XR2206">
<pin name="AMSI" direction="in"/>
<pin name="STO" direction="out"/>
<pin name="MO" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="TC1" direction="in"/>
<pin name="TC2" direction="in"/>
<pin name="TR1" direction="out"/>
<pin name="TR2" direction="out"/>
<pin name="FSKI" direction="in"/>
<pin name="BIAS" direction="out"/>
<pin name="SYNCO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="WAVEA1" direction="in"/>
<pin name="WAVEA2" direction="in"/>
<pin name="SYMA1" direction="in"/>
<pin name="SYMA2" direction="in"/>
</symbol>
<symbol name="74HC04_HEX_INVERTER">
<pin name="VCC" direction="pwr"/>
<pin name="2A" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="5A" direction="in"/>
<pin name="6A" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="6Y" direction="out"/>
<pin name="5Y" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="1A" direction="in"/>
<pin name="1Y" direction="out"/>
</symbol>
<symbol name="M74HC4050">
<pin name="VCC"/>
<pin name="1A"/>
<pin name="2A"/>
<pin name="3A"/>
<pin name="4A"/>
<pin name="5A"/>
<pin name="6A"/>
<pin name="1Y"/>
<pin name="2Y"/>
<pin name="3Y"/>
<pin name="4Y"/>
<pin name="5Y"/>
<pin name="6Y"/>
<pin name="GND"/>
</symbol>
<symbol name="MPL115A">
<pin name="VDD"/>
<pin name="CAP"/>
<pin name="GND"/>
<pin name="SHDN"/>
<pin name="RST/CS"/>
<pin name="NC/DOUT"/>
<pin name="SDA/DIN"/>
<pin name="SCLK"/>
</symbol>
<symbol name="MICROB-PLUG">
<pin name="VCC"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="ID"/>
<pin name="GND"/>
</symbol>
<symbol name="BMA180">
<pin name="NC"/>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="INT"/>
<pin name="CSB"/>
<pin name="NC1"/>
<pin name="SCK"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="VDDIO"/>
<pin name="NC2"/>
<pin name="NC3"/>
</symbol>
<symbol name="LYPR540AH">
<pin name="RESGND1"/>
<pin name="ST"/>
<pin name="GND"/>
<pin name="VCONT_1G"/>
<pin name="VCONT_2G"/>
<pin name="FILTVDD_2G"/>
<pin name="4XZ"/>
<pin name="4XY"/>
<pin name="4XX"/>
<pin name="Z"/>
<pin name="Y"/>
<pin name="X"/>
<pin name="RESGND2"/>
<pin name="RESVDD1"/>
<pin name="RESVDD2"/>
<pin name="RESVDD3"/>
<pin name="RESVDD4"/>
<pin name="VDD"/>
</symbol>
<symbol name="LMZ14203">
<pin name="VIN"/>
<pin name="RON"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="SS"/>
<pin name="FB"/>
<pin name="VOUT"/>
<pin name="EP"/>
</symbol>
<symbol name="AD5330">
<pin name="VDD"/>
<pin name="VREF"/>
<pin name="CS"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="WR"/>
<pin name="CLR"/>
<pin name="PD"/>
<pin name="GND"/>
<pin name="VOUT"/>
<pin name="LDAC"/>
<pin name="GAIN"/>
<pin name="BUF"/>
</symbol>
<symbol name="LSM303DLH">
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="SA0_A"/>
<pin name="VDD_I2C"/>
<pin name="VDD"/>
<pin name="VDD@7"/>
<pin name="SET2"/>
<pin name="C1"/>
<pin name="SET1"/>
<pin name="GND@17"/>
<pin name="DRDY_M"/>
<pin name="SDA_M"/>
<pin name="SCL_M"/>
<pin name="VDD_M"/>
<pin name="VDD_IO@22"/>
<pin name="VDD_IO@23"/>
<pin name="SCL_A"/>
<pin name="SDA_A"/>
<pin name="INT1"/>
<pin name="INT2"/>
<pin name="GND@28"/>
</symbol>
<symbol name="ATMEGA128RFA1">
<pin name="EVDD"/>
<pin name="DEVDD@23"/>
<pin name="AVDD"/>
<pin name="DVDD@21"/>
<pin name="AVSS@58"/>
<pin name="DVSS@20"/>
<pin name="PB0"/>
<pin name="PB1/SCK"/>
<pin name="PB2/PDI"/>
<pin name="PB3/PDO"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="PF6"/>
<pin name="PF5"/>
<pin name="PF4"/>
<pin name="PF3"/>
<pin name="PF2"/>
<pin name="PF1"/>
<pin name="PF0"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="AVSS_RFN"/>
<pin name="AVSS_RFP"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="RSTN"/>
<pin name="RSTON"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AREF"/>
<pin name="TST"/>
<pin name="CLKI"/>
<pin name="DVDD@22"/>
<pin name="DVSS@24"/>
<pin name="DVSS@35"/>
<pin name="DVSS@45"/>
<pin name="DVSS@55"/>
<pin name="DEVDD@34"/>
<pin name="DEVDD@44"/>
<pin name="DEVDD@54"/>
<pin name="AVSS@61"/>
</symbol>
<symbol name="BALUN">
<pin name="IN"/>
<pin name="OUT1"/>
<pin name="GND@5"/>
<pin name="OUT2"/>
<pin name="GND@2"/>
</symbol>
<symbol name="SWITCH-4PDT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
</symbol>
<symbol name="ADMP401">
<pin name="VDD"/>
<pin name="OUT"/>
<pin name="GND@6"/>
<pin name="GND@2"/>
<pin name="GND@4"/>
</symbol>
<symbol name="MLX90614">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="SCL/VZ"/>
<pin name="PWM/SDA"/>
</symbol>
<symbol name="D2523T">
<pin name="RX"/>
<pin name="TX"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="VBAT"/>
<pin name="LED"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_CONTROL">
<pin name="RB0/AN0"/>
<pin name="RB1/AN1"/>
<pin name="RB3/AN3"/>
<pin name="RB4/AN4"/>
<pin name="RB5/AN5"/>
<pin name="RB6/AN6"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RG2/SCL1"/>
<pin name="RG3/SDA1"/>
<pin name="RD8/IC1"/>
<pin name="RD9/IC2"/>
<pin name="RD14/U1CTS/IC7"/>
<pin name="RD15/U1RTS/IC8"/>
<pin name="RD10/IC3"/>
<pin name="RD11/IC4"/>
<pin name="RD0/OC1"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5"/>
<pin name="RD12/IC5"/>
<pin name="RD13/IC6"/>
<pin name="RD5/OC6"/>
<pin name="RD6/OC7"/>
<pin name="RD7/OC8"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RF2/U1RX"/>
<pin name="RF3/U1TX"/>
<pin name="RB14/AN14"/>
<pin name="RC4/AN19"/>
<pin name="RA6/AN22"/>
<pin name="RE4"/>
<pin name="RE3"/>
<pin name="RE2"/>
<pin name="RE1/AN25"/>
</symbol>
<symbol name="PQ1CY1032Z">
<pin name="VIN"/>
<pin name="VOUT"/>
<pin name="GND"/>
<pin name="ADJ"/>
<pin name="VS"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_POWER">
<pin name="VSS@75"/>
<pin name="VDD@2"/>
<pin name="VDD@86"/>
<pin name="VCAP"/>
<pin name="VDD@46"/>
<pin name="VSS@45"/>
<pin name="VDD@37"/>
<pin name="VSS@36"/>
<pin name="RA9/VREF-"/>
<pin name="RA10/VREF+"/>
<pin name="VDD@16"/>
<pin name="VSS@15"/>
<pin name="VSS@65"/>
<pin name="VDD@62"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_EXTERNAL">
<pin name="RB15/AN15"/>
<pin name="RC1/AN16"/>
<pin name="RC2/AN17"/>
<pin name="RC3/AN18"/>
<pin name="RA12/INT1"/>
<pin name="RA13/INT2"/>
<pin name="RA7/AN23"/>
<pin name="RG6/SCK2"/>
<pin name="RG7/SDI2"/>
<pin name="RG8/SDO2"/>
<pin name="RG9/SS2"/>
<pin name="RF4/U2RX"/>
<pin name="RF5/U2TX"/>
<pin name="RF13/U2RTS"/>
<pin name="RF12/U2CTS"/>
<pin name="RC14/PGEC2"/>
<pin name="RC13/PGED2"/>
<pin name="MCLR"/>
<pin name="RF1/C1TX1"/>
<pin name="RF0/C1RX1"/>
<pin name="RF6/SCK1"/>
<pin name="RF7/SDI1"/>
<pin name="RF8/SDO1"/>
<pin name="RA2/SCL2"/>
<pin name="RA3/SDA2"/>
<pin name="RB2/SS1"/>
<pin name="RE0/AN24"/>
<pin name="RA1"/>
<pin name="RA5/TDO"/>
<pin name="RA4/TDI"/>
<pin name="RA14"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_EXTRA">
<pin name="RE5/AN29"/>
<pin name="RE6/AN30"/>
<pin name="RE7/AN31"/>
<pin name="RG0/C2RX"/>
<pin name="RG1/C2TX"/>
<pin name="RG13/CSDO"/>
<pin name="RG12/CSDI"/>
<pin name="RG14/CSCK"/>
<pin name="RA0/TMS"/>
<pin name="RA15"/>
<pin name="RC15/OSC2"/>
<pin name="RC12/OSC1"/>
<pin name="RG15/COFS"/>
</symbol>
<symbol name="ZG2100M">
<pin name="GND1"/>
<pin name="VDD_1.8_1"/>
<pin name="JTAG_TDO"/>
<pin name="JTAG_TCK"/>
<pin name="JTAG_TMS"/>
<pin name="JTAG_TDI"/>
<pin name="RST_N"/>
<pin name="NC6"/>
<pin name="JTAG_RST_N"/>
<pin name="GND2"/>
<pin name="VDD_1.8_2"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="RES"/>
<pin name="VDD_3.3_1"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="CE_N"/>
<pin name="JTAG_EN"/>
<pin name="NC5"/>
<pin name="SCS_N"/>
<pin name="VDD_1.8_3"/>
<pin name="GND5"/>
<pin name="UART_RX"/>
<pin name="UART_TX"/>
<pin name="GND6"/>
<pin name="VDD_3.3_2"/>
<pin name="GND7"/>
<pin name="VDD_1.8_4"/>
<pin name="SDO"/>
<pin name="INT_NX"/>
<pin name="SCK"/>
<pin name="SDI"/>
<pin name="GND8"/>
</symbol>
<symbol name="MOC3031-M">
<pin name="1"/>
<pin name="2"/>
<pin name="6"/>
<pin name="4"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="OBDII">
<pin name="1"/>
<pin name="J1850BUS+"/>
<pin name="3"/>
<pin name="CHASGND"/>
<pin name="SIGGND"/>
<pin name="CANHIGH"/>
<pin name="ISOK-LINE"/>
<pin name="8"/>
<pin name="9"/>
<pin name="J1850BUS"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="CANLOW"/>
<pin name="ISOL-LINE"/>
<pin name="BATTPOWER"/>
</symbol>
<symbol name="LIS331">
<pin name="VDD"/>
<pin name="NC"/>
<pin name="NC2"/>
<pin name="SCL"/>
<pin name="GND"/>
<pin name="GND3"/>
<pin name="GND2"/>
<pin name="INT1"/>
<pin name="RSV"/>
<pin name="INT2"/>
<pin name="VDD2"/>
<pin name="RSV2"/>
<pin name="GND4"/>
<pin name="CS"/>
<pin name="SA0"/>
<pin name="SDA"/>
</symbol>
<symbol name="PSP_CONNECTOR">
<pin name="G7"/>
<pin name="G6"/>
<pin name="G5"/>
<pin name="G4"/>
<pin name="G3"/>
<pin name="G2"/>
<pin name="G1"/>
<pin name="G0"/>
<pin name="R7"/>
<pin name="R6"/>
<pin name="R5"/>
<pin name="R4"/>
<pin name="R3"/>
<pin name="R2"/>
<pin name="R1"/>
<pin name="R0"/>
<pin name="VCC2"/>
<pin name="VCC"/>
<pin name="GND2"/>
<pin name="GND"/>
<pin name="TEST3"/>
<pin name="TEST2"/>
<pin name="TEST1"/>
<pin name="NC2"/>
<pin name="AVDD2"/>
<pin name="AVDD"/>
<pin name="NC"/>
<pin name="VSYNC"/>
<pin name="HSYNC"/>
<pin name="DISP"/>
<pin name="CK"/>
<pin name="GND3"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="B0"/>
</symbol>
<symbol name="LTC3588">
<pin name="PZ1"/>
<pin name="PZ2"/>
<pin name="CAP"/>
<pin name="VIN"/>
<pin name="SW"/>
<pin name="VOUT"/>
<pin name="VIN2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="PGOOD"/>
<pin name="GND"/>
</symbol>
<symbol name="SOLARCELL_SINGLE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="ITG-3200">
<pin name="CLKIN"/>
<pin name="VLOGIC"/>
<pin name="AD0"/>
<pin name="REGOUT"/>
<pin name="RESV-G"/>
<pin name="INT"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="CPOUT"/>
<pin name="GND"/>
<pin name="VDD"/>
</symbol>
<symbol name="SCREENKEY-TFT128">
</symbol>
<symbol name="XMEGA-A3B">
<pin name="/RESET_PDI_CLK"/>
<pin name="PDI_DATA"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="VCC3"/>
<pin name="VCC4"/>
<pin name="VCC5"/>
<pin name="PF5"/>
<pin name="PR0(XTAL2)"/>
<pin name="PR1(XTAL1)"/>
<pin name="PA0(ADC0/AC0/AREF)"/>
<pin name="PA1(ADC1/AC1)"/>
<pin name="PA2(ADC2/AC2)"/>
<pin name="PA3(ADC3/AC3)"/>
<pin name="PA4(ADC4/AC4)"/>
<pin name="PA5(ADC5/AC5)"/>
<pin name="PA6(ADC6/AC6)"/>
<pin name="PA7(ADC7/AC7/AC0OUT)"/>
<pin name="PB0(ADC0/AC0/AREF)"/>
<pin name="PB1(ADC1/AC1)"/>
<pin name="PB2(ADC2/AC2/DAC0)"/>
<pin name="PB3(ADC3/AC3/DAC1)"/>
<pin name="PB4(ADC4/AC4/TMS)"/>
<pin name="PB5(ADC5/AC5/TDI)"/>
<pin name="PB6(ADC6/AC6/TCK)"/>
<pin name="PB7(ADC7/AC7/AC0OUT/TDO)"/>
<pin name="PC1(OC0B/AC0AH/XCK0/SCL)"/>
<pin name="PC0(OC0A/OC0AL/SDA)"/>
<pin name="PC2(OC0C/OC0BL/RXD0)"/>
<pin name="PC3(OC0D/OX0BH/TXD0)"/>
<pin name="PC4(AC1A/OC0CL/SS)"/>
<pin name="PC5(OC1B/OC0CH/XCK1/MOSI)"/>
<pin name="PC6(OC0DL/RXD1/MISO)"/>
<pin name="PC7(OC0DH/CKOUT/EVO/TXD1/SCK)"/>
<pin name="PD0(OC0A)"/>
<pin name="PD1(OC0B/XCK0)"/>
<pin name="PD2(OC0C/RXD0)"/>
<pin name="PD3(OX0D/TXD0)"/>
<pin name="PD4(OC1A/SS)"/>
<pin name="PD5(OC1B/XCK1/MOSI)"/>
<pin name="PD6(RXD1/MISO)"/>
<pin name="PD7(CKOUT/EVO/TXD1/SCK)"/>
<pin name="PE0(OC0A/SDA)"/>
<pin name="PE1(OC0B/XCK0/SCL)"/>
<pin name="PE2(OC0C/RXD0)"/>
<pin name="PE3(OC0D/TXD0)"/>
<pin name="PE4(OC1A/SS)"/>
<pin name="PE5(OC1B/XCK1/MOSI)"/>
<pin name="PE6(TOSC2/RXD1/MISO)"/>
<pin name="PE7(TOSC1/CKOUT/EVO/TXD1/SCK)"/>
<pin name="PF0(OC0A)"/>
<pin name="PF1(OC0B/XCK0)"/>
<pin name="PF2(OC0C/RXD0)"/>
<pin name="PF3(OC0D/TXD0)"/>
<pin name="PF4"/>
<pin name="PF6"/>
<pin name="PF7"/>
</symbol>
<symbol name="ZXLD1360">
<pin name="LX"/>
<pin name="GND"/>
<pin name="ADJ"/>
<pin name="SENSE"/>
<pin name="VIN"/>
</symbol>
<symbol name="ADNS2610">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="OSC_OUT"/>
<pin name="OSC_IN"/>
<pin name="SCK"/>
<pin name="SDIO"/>
<pin name="LED_CNTL"/>
<pin name="REFA"/>
</symbol>
<symbol name="SUP500F">
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="PSEL"/>
<pin name="GND"/>
<pin name="PPS"/>
<pin name="TX-O"/>
<pin name="RX-I"/>
</symbol>
<symbol name="ADMP421">
<pin name="VDD"/>
<pin name="DATA"/>
<pin name="GND@2"/>
<pin name="CLK"/>
<pin name="L/R"/>
<pin name="GND@1"/>
<pin name="GND@3"/>
</symbol>
<symbol name="SPARKFUN-EAGLE-RULES">
</symbol>
<symbol name="74157">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
<pin name="3A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3Y" direction="out"/>
<pin name="4A" direction="in"/>
<pin name="4B" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="MLX90121">
<pin name="VDD1"/>
<pin name="TX"/>
<pin name="MOD"/>
<pin name="VSS1"/>
<pin name="XOUT"/>
<pin name="XIN"/>
<pin name="VSS2"/>
<pin name="XBUF"/>
<pin name="RES1"/>
<pin name="RTB"/>
<pin name="DOUT"/>
<pin name="VDD2"/>
<pin name="DIN"/>
<pin name="MODE"/>
<pin name="CK"/>
<pin name="DSYC"/>
<pin name="VDD3"/>
<pin name="RES2(DNC)"/>
<pin name="VSS3"/>
<pin name="RX"/>
</symbol>
<symbol name="FT232RQ">
<pin name="RESET" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="DSR" direction="in" function="dot"/>
<pin name="DCD" direction="in" function="dot"/>
<pin name="RI" direction="in" function="dot"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="TXLED" direction="in" function="dot"/>
<pin name="RXLED" direction="in" function="dot"/>
<pin name="RTS" direction="out" function="dot"/>
<pin name="CTS" direction="in" function="dot"/>
<pin name="DTR" direction="out" function="dot"/>
<pin name="PWREN" direction="in" function="dot"/>
<pin name="TXDEN" direction="in"/>
<pin name="SLEEP" direction="in" function="dot"/>
</symbol>
<symbol name="FB">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="M40">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="74HC4052">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="X"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="Y"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
</symbol>
<symbol name="CAP_ADJ">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="AT45DB161D">
<pin name="CS" function="dot"/>
<pin name="RST" function="dot"/>
<pin name="SCK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="WP" function="dot"/>
</symbol>
<symbol name="ARDUINO_MINI">
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="GND"/>
<pin name="GND2"/>
<pin name="RAW"/>
<pin name="RST"/>
<pin name="RST2"/>
<pin name="RX1"/>
<pin name="TX0"/>
<pin name="VCC"/>
</symbol>
<symbol name="USB-5PIN">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="ID"/>
<pin name="MTN1"/>
<pin name="MTN2"/>
<pin name="MTN3"/>
<pin name="MTN4"/>
</symbol>
<symbol name="BTM182">
<pin name="VDD"/>
<pin name="VDD_USB"/>
<pin name="USB_DP"/>
<pin name="USB_DN"/>
<pin name="PCM_OUT"/>
<pin name="PCM_CLK"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_IN"/>
<pin name="UART_CTS"/>
<pin name="UART_TX"/>
<pin name="UART_RX"/>
<pin name="UART_RTS"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_CSB"/>
<pin name="SPI_MISO"/>
<pin name="SPI_CLK"/>
<pin name="GND"/>
<pin name="RESET"/>
<pin name="AIO1"/>
<pin name="AIO0"/>
<pin name="PIO11"/>
<pin name="PIO10"/>
<pin name="PIO9"/>
<pin name="PIO8"/>
<pin name="PIO7"/>
<pin name="PIO6"/>
<pin name="PIO5"/>
<pin name="PIO4"/>
<pin name="PIO3"/>
<pin name="PIO2"/>
<pin name="PIO1"/>
<pin name="PIO0"/>
</symbol>
<symbol name="50-PIN-CENTRONICS">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
<pin name="P$41"/>
<pin name="P$42"/>
<pin name="P$43"/>
<pin name="P$44"/>
<pin name="P$45"/>
<pin name="P$46"/>
<pin name="P$47"/>
<pin name="P$48"/>
<pin name="P$49"/>
<pin name="P$50"/>
</symbol>
<symbol name="RF-LINK_TX">
<pin name="GND" direction="pwr"/>
<pin name="DATA" direction="in"/>
<pin name="ANT" direction="pas"/>
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="RF-LINK_RX">
<pin name="GND" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="+5V" direction="pwr"/>
<pin name="DATA" direction="in"/>
</symbol>
<symbol name="VNH2SP30">
<pin name="OUTB@15"/>
<pin name="INB"/>
<pin name="VCC@13"/>
<pin name="EN/DIAB"/>
<pin name="CS"/>
<pin name="PWM"/>
<pin name="EN/DIAA"/>
<pin name="INA"/>
<pin name="VCC@3"/>
<pin name="OUTA@1"/>
<pin name="OUTA@30"/>
<pin name="GNDA@28"/>
<pin name="GNDA@27"/>
<pin name="GNDA@26"/>
<pin name="OUTA@25"/>
<pin name="VCC@23"/>
<pin name="OUTB@21"/>
<pin name="GNDB@20"/>
<pin name="GNDB@19"/>
<pin name="GNDB@18"/>
<pin name="OUTB@16"/>
<pin name="VCC@SLUG1"/>
<pin name="OUTA@SLUG3"/>
<pin name="OUTB@SLUG2"/>
</symbol>
<symbol name="ALPHANUMERIC">
<pin name="A1"/>
<pin name="A2"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G1"/>
<pin name="G2"/>
<pin name="H"/>
<pin name="J"/>
<pin name="K"/>
<pin name="L"/>
<pin name="M"/>
<pin name="N"/>
<pin name="NC@1"/>
<pin name="NC@13"/>
<pin name="VCC@6"/>
<pin name="VCC@18"/>
</symbol>
<symbol name="ADH8066">
<pin name="SIMCLK"/>
<pin name="SIMVDD"/>
<pin name="SIMIO"/>
<pin name="SIMRST"/>
<pin name="GPIO10"/>
<pin name="GND@6"/>
<pin name="PCMDI"/>
<pin name="PCMFSO"/>
<pin name="PCMCLK"/>
<pin name="PCMDO"/>
<pin name="ADC1"/>
<pin name="BATTTEMP"/>
<pin name="GPIO3"/>
<pin name="TXD1"/>
<pin name="TXD0"/>
<pin name="RXD1"/>
<pin name="RXD0"/>
<pin name="VCHAR@18"/>
<pin name="VCHAR@19"/>
<pin name="CHV_DRV"/>
<pin name="GND@21"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
<pin name="GND@25"/>
<pin name="VBAT@26"/>
<pin name="VBAT@27"/>
<pin name="VBAT@28"/>
<pin name="VBAT@29"/>
<pin name="VBAT@30"/>
<pin name="RI0"/>
<pin name="1.8V"/>
<pin name="DTR0"/>
<pin name="CTS0"/>
<pin name="DSR0"/>
<pin name="SCL(NC)"/>
<pin name="RTS0"/>
<pin name="SDA(NC)"/>
<pin name="DCD0"/>
<pin name="CHV_MAX"/>
<pin name="ON_KEY"/>
<pin name="GND@42"/>
<pin name="MIC1_P"/>
<pin name="MIC1_N"/>
<pin name="MIC2_P"/>
<pin name="MIC2_N"/>
<pin name="AUXOUTP"/>
<pin name="AUXOUTN"/>
<pin name="EARP"/>
<pin name="EARN"/>
</symbol>
<symbol name="STP16CP05/A6282">
<pin name="GND"/>
<pin name="SDI"/>
<pin name="CLK"/>
<pin name="LE"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="VDD"/>
<pin name="REXT"/>
<pin name="SDO"/>
<pin name="~OE"/>
<pin name="OUT15"/>
<pin name="OUT14"/>
<pin name="OUT13"/>
<pin name="OUT12"/>
<pin name="OUT11"/>
<pin name="OUT10"/>
<pin name="OUT8"/>
<pin name="OUT9"/>
</symbol>
<symbol name="LS20126">
<pin name="GND@1"/>
<pin name="VSTBY"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="GPIO"/>
<pin name="BOOTSL"/>
<pin name="EN"/>
<pin name="VCC"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
</symbol>
<symbol name="ADM1087">
<pin name="ENIN"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="ENOUT"/>
<pin name="CEXT"/>
<pin name="VCC"/>
</symbol>
<symbol name="STARBOARD_LOGO">
</symbol>
<symbol name="WIZ811MJ">
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="SCLK"/>
<pin name="/SCS"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="A14"/>
<pin name="A13"/>
<pin name="A12"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A7"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="/RD"/>
<pin name="/CS"/>
<pin name="/WR"/>
<pin name="/INT"/>
<pin name="D0"/>
<pin name="/RESET"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
</symbol>
<symbol name="WATN001001">
<pin name="V0@1"/>
<pin name="V1@1"/>
<pin name="V2@1"/>
<pin name="VSSE@1"/>
<pin name="VSS@1"/>
<pin name="EIO1"/>
<pin name="XCK"/>
<pin name="VDD"/>
<pin name="LATCH"/>
<pin name="RESERVED@1"/>
<pin name="SHL"/>
<pin name="SLEEPB"/>
<pin name="DLY0"/>
<pin name="DLY1"/>
<pin name="RESERVED@2"/>
<pin name="DI0"/>
<pin name="DI1"/>
<pin name="DI2"/>
<pin name="RESERVED@3"/>
<pin name="EIO2"/>
<pin name="VSS@2"/>
<pin name="VSSE@2"/>
<pin name="V0@2"/>
<pin name="V1@2"/>
<pin name="V2@2"/>
<pin name="RESERVED@4"/>
</symbol>
<symbol name="BQ24022">
<pin name="AC"/>
<pin name="USB"/>
<pin name="STAT1"/>
<pin name="STAT2"/>
<pin name="GND"/>
<pin name="ISET1"/>
<pin name="ISET2"/>
<pin name="~PG"/>
<pin name="~CE"/>
<pin name="OUT"/>
<pin name="ETP"/>
</symbol>
<symbol name="MCP73833">
<pin name="VDD@1"/>
<pin name="VDD@2"/>
<pin name="STAT1"/>
<pin name="STAT2"/>
<pin name="VSS"/>
<pin name="PROG"/>
<pin name="~PG"/>
<pin name="THERM"/>
<pin name="VBAT@1"/>
<pin name="VBAT@2"/>
</symbol>
<symbol name="OP-AMP+--1">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="EPAD"/>
</symbol>
<symbol name="OP-AMP-1">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MCP73831">
<pin name="VIN" direction="pwr"/>
<pin name="STAT" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PROG" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="SI1120">
<pin name="VDD"/>
<pin name="TXGD"/>
<pin name="TXO"/>
<pin name="VSS"/>
<pin name="PRX"/>
<pin name="MD"/>
<pin name="SC"/>
<pin name="STX"/>
</symbol>
<symbol name="A6282">
<pin name="GND@1"/>
<pin name="SDI"/>
<pin name="CLK"/>
<pin name="LE"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="VDD"/>
<pin name="REXT"/>
<pin name="SDO"/>
<pin name="~OE"/>
<pin name="OUT15"/>
<pin name="OUT14"/>
<pin name="OUT13"/>
<pin name="OUT12"/>
<pin name="OUT11"/>
<pin name="OUT10"/>
<pin name="OUT8"/>
<pin name="OUT9"/>
<pin name="GND@2"/>
</symbol>
<symbol name="STN1110-QFN">
<pin name="!VPW_RX" direction="in"/>
<pin name="PWM_RX" direction="in"/>
<pin name="J1850_BUS+_TX" direction="out"/>
<pin name="!J1850_BUS-_TX" direction="out"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="!ISO_RX" direction="in"/>
<pin name="!SLEEP" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="CAN_RX" direction="in"/>
<pin name="CAN_TX" direction="out"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="PWR_CTRL" direction="out"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="!OBD_TX_LED!/!RST_NVM"/>
<pin name="!OBD_RX_LED!/!INT" direction="out"/>
<pin name="!UART_TX_LED" direction="out"/>
<pin name="!UART_RX_LED" direction="out"/>
<pin name="!ISO_K_TX" direction="out"/>
<pin name="!ISO_L_TX" direction="out"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="ANALOG_IN" direction="in"/>
<pin name="PWM/!VPW" direction="out"/>
<pin name="PAD" direction="pas"/>
</symbol>
<symbol name="SM130">
<pin name="VCC"/>
<pin name="RFVCC"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="OK"/>
<pin name="ERROR"/>
<pin name="RESET"/>
<pin name="I1"/>
<pin name="I2"/>
<pin name="GND"/>
<pin name="RFGND@23"/>
<pin name="RFGND@25"/>
<pin name="RFGND@27"/>
<pin name="ANT2"/>
<pin name="ANT1"/>
<pin name="O2"/>
<pin name="O1"/>
<pin name="RX-I"/>
<pin name="TX-O"/>
</symbol>
<symbol name="JOYSTICK_MINI">
<pin name="CENT"/>
<pin name="DOWN"/>
<pin name="GND"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="UP"/>
</symbol>
<symbol name="AT42QT1012">
<pin name="VDD"/>
<pin name="SNSK"/>
<pin name="GND"/>
<pin name="SNS"/>
<pin name="OUT"/>
<pin name="TIME"/>
</symbol>
<symbol name="TPS61200">
<pin name="EN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="sup"/>
<pin name="L" direction="pas"/>
<pin name="PAD@1" direction="sup"/>
<pin name="PAD@2" direction="sup"/>
<pin name="PAD@3" direction="sup"/>
<pin name="PAD@4" direction="sup"/>
<pin name="PAD@5" direction="sup"/>
<pin name="PGND" direction="sup"/>
<pin name="PS" direction="in"/>
<pin name="UVLO" direction="pas"/>
<pin name="VAUX" direction="pas"/>
<pin name="VIN" direction="sup"/>
<pin name="VOUT" direction="pas"/>
</symbol>
<symbol name="IMU3000">
<pin name="VDD"/>
<pin name="GND@18"/>
<pin name="INT"/>
<pin name="CPOUT"/>
<pin name="VLOG"/>
<pin name="CLKOUT"/>
<pin name="REGOUT"/>
<pin name="GND@11"/>
<pin name="SDA"/>
<pin name="AD0"/>
<pin name="CLKIN"/>
<pin name="AUX_DA"/>
<pin name="AUX_CL"/>
<pin name="SCL"/>
</symbol>
<symbol name="FKIT-CONNECTOR_COND_03">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
<symbol name="FKIT-BATTERY">
<pin name="NEG"/>
<pin name="POS"/>
</symbol>
<symbol name="FKIT-LOGO">
</symbol>
<symbol name="FKIT-LOGOTYPE">
</symbol>
<symbol name="USB-MICROB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="ID"/>
<pin name="MTN2"/>
<pin name="MTN4"/>
</symbol>
<symbol name="DS3234">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SCLK@20"/>
<pin name="DOUT"/>
<pin name="DIN"/>
<pin name="CS"/>
<pin name="INT/SQW"/>
<pin name="RST"/>
<pin name="32KHZ"/>
<pin name="GND@2"/>
<pin name="VBAT"/>
<pin name="SCLK@18"/>
<pin name="GND@14"/>
<pin name="GND@9"/>
<pin name="GND@13"/>
<pin name="GND@12"/>
<pin name="GND@11"/>
<pin name="GND@10"/>
<pin name="GND@8"/>
<pin name="GND@7"/>
</symbol>
<symbol name="PIC24FJXXXDAX06">
<pin name="!MCLR" direction="in"/>
<pin name="AN2/C2INB/VMIO/RP13/CN4/RB2"/>
<pin name="AN3/C2INA/VPIO/CN5/RB3"/>
<pin name="AN8/RP8/CN26/RB8"/>
<pin name="AN9/RP9/CN27/RB9"/>
<pin name="AN14/CTPLS/RP14/CN32/RB14"/>
<pin name="AN15/RP29/REFO/CN12/RB15"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="C1INC/RP26/CN9/RG7"/>
<pin name="C1IND/RP21/CN8/RG6"/>
<pin name="C2INC/RP27/GD15/CN11/RG9"/>
<pin name="C2IND/RP19/GD14/CN10/RG8"/>
<pin name="C3INA/SESSEND/CN16/RD7"/>
<pin name="C3INB/CN15/RD6"/>
<pin name="D+/CN83/RG2"/>
<pin name="D-/CN84/RG3"/>
<pin name="DMH/RP11/INT0/CN49/RD0"/>
<pin name="DPH/RP23/CN51/RD2"/>
<pin name="DPLN/SDA1/RP4/GD8/CN54/RD9"/>
<pin name="ENVREG" direction="in"/>
<pin name="GD0/CN58/RE0"/>
<pin name="GD1/CN59/RE1"/>
<pin name="GD2/CN60/RE2"/>
<pin name="GD3/CN61/RE3"/>
<pin name="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0"/>
<pin name="GD11/VCMPST2/SESSVLD/CN69/RF1"/>
<pin name="GD12/SCL3/CN64/RE6"/>
<pin name="GD13/SDA3/CN65/RE7"/>
<pin name="HSYNC/CN62/RE4"/>
<pin name="OSCI/CLKI/CN23/RC12"/>
<pin name="OSCO/CLKO/CN22/RC15"/>
<pin name="PGEC1/AN1/VREF-/RP1/CN3/RB1"/>
<pin name="PGEC2/AN6/RP6/CN24/RB6"/>
<pin name="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5"/>
<pin name="PGED1/AN0/VREF+/RP0/CN2/RB0"/>
<pin name="PGED2/AN7/RP7/RCV/CN25/RB7"/>
<pin name="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4"/>
<pin name="RP12/GD7/CN56/RD11"/>
<pin name="RP16/USBID/CN71/RF3"/>
<pin name="RP20/GPWR/CN14/RD5"/>
<pin name="RP22/GEN/CN52/RD3"/>
<pin name="RP25/GCLK/CN13/RD4"/>
<pin name="RTCC/DMLN/RP2/CN53/RD8"/>
<pin name="SCL1/RP3/GD6/CN55/RD10"/>
<pin name="SCL2/RP17/GD5/CN18/RF5"/>
<pin name="SDA2/RP10/GD4/CN17/RF4"/>
<pin name="SOSCI/C3IND/CN1/RC13"/>
<pin name="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14"/>
<pin name="TCK/AN12/CTEDG2/CN30/RB12"/>
<pin name="TDI/AN13/CTEDG1/CN31/RB13"/>
<pin name="TDO/AN11/CN29/RB11"/>
<pin name="TMS/CVREF/AN10/CN28/RB10"/>
<pin name="VBUS/RF7" direction="in"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSYNC/CN63/RE5"/>
<pin name="VUSB" direction="pwr"/>
</symbol>
<symbol name="RS485_SP491">
<pin name="A"/>
<pin name="B"/>
<pin name="Z"/>
<pin name="Y"/>
<pin name="R"/>
<pin name="/RE"/>
<pin name="DE"/>
<pin name="D"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="VCC"/>
<pin name="NC2"/>
<pin name="NC1"/>
<pin name="NC3"/>
</symbol>
<symbol name="74HC4051_MUX">
<pin name="VSS"/>
<pin name="VEE"/>
<pin name="INH"/>
<pin name="IO7"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO"/>
<pin name="IO4"/>
<pin name="VDD"/>
<pin name="IO2"/>
<pin name="IO1"/>
<pin name="IO0"/>
<pin name="IO3"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
</symbol>
<symbol name="TCMT1103">
<pin name="C"/>
<pin name="E"/>
<pin name="K"/>
<pin name="A"/>
</symbol>
<symbol name="MSGEQ7">
<pin name="DCOUT"/>
<pin name="CG"/>
<pin name="CKIN"/>
<pin name="GND"/>
<pin name="RESET" direction="in"/>
<pin name="STROBE" direction="in"/>
<pin name="AUDIO_IN" direction="in"/>
<pin name="VDD" direction="in"/>
</symbol>
<symbol name="STARBOARD_PAD">
<pin name="MOUNT" direction="pas"/>
</symbol>
<symbol name="STARBOARD_PAD+">
<pin name="MOUNT" direction="pas"/>
</symbol>
<symbol name="BANANA_CONN">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="XLR3_NCFAH2">
<pin name="3"/>
<pin name="2"/>
<pin name="1"/>
<pin name="G"/>
</symbol>
<symbol name="FKIT-SNAP_CONNECTOR">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="PCA9306">
<pin name="SDA1"/>
<pin name="SCL1"/>
<pin name="EN"/>
<pin name="VREF1"/>
<pin name="VREF2"/>
<pin name="SCL2"/>
<pin name="SDA2"/>
<pin name="GND"/>
</symbol>
<symbol name="ATMEGA8U2">
<pin name="AVCC"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="PB0"/>
<pin name="PB1(SCK)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB3(MISO)"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2(RX)"/>
<pin name="PD3(TX)"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6(RTS)"/>
<pin name="PD7(CTS)"/>
<pin name="RESET/PC1"/>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="UVCC"/>
<pin name="VCC"/>
<pin name="XTAL1"/>
<pin name="XTAL2/PC0"/>
</symbol>
<symbol name="VARISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="USB+SHIELD">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="LIS331-1">
<pin name="VDD"/>
<pin name="SCL/SPC"/>
<pin name="GND@5"/>
<pin name="GND@13"/>
<pin name="GND@12"/>
<pin name="INT1"/>
<pin name="GNDR"/>
<pin name="INT2"/>
<pin name="VDDIO"/>
<pin name="VDDR"/>
<pin name="GND@16"/>
<pin name="CS"/>
<pin name="SA0/SDO"/>
<pin name="SDA/SDI"/>
</symbol>
<symbol name="A4983">
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="DIR" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND_PAD" direction="pwr"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="MS3" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="OUT1A"/>
<pin name="OUT1B"/>
<pin name="OUT2A"/>
<pin name="OUT2B"/>
<pin name="REF"/>
<pin name="RESET" direction="in"/>
<pin name="ROSC"/>
<pin name="SENSE1"/>
<pin name="SENSE2"/>
<pin name="SLEEP" direction="in"/>
<pin name="STEP" direction="in"/>
<pin name="VBB1"/>
<pin name="VBB2"/>
<pin name="VCP"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREG"/>
</symbol>
<symbol name="ADJD-S311-CR999">
<pin name="DVDD"/>
<pin name="AVDD"/>
<pin name="DGND"/>
<pin name="AGND"/>
<pin name="SCKSLV"/>
<pin name="CLKIO"/>
<pin name="SDASLV"/>
<pin name="SLEEP"/>
<pin name="RESET"/>
</symbol>
<symbol name="78ADJ-3">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND"/>
<pin name="EN"/>
</symbol>
<symbol name="DCM01">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WS2801">
<pin name="CKI"/>
<pin name="SDI"/>
<pin name="VCC"/>
<pin name="POL"/>
<pin name="CKO"/>
<pin name="SDO"/>
<pin name="BOUT"/>
<pin name="GOUT"/>
<pin name="ROUT"/>
<pin name="BFB"/>
<pin name="GFB"/>
<pin name="RFB"/>
<pin name="GND"/>
</symbol>
<symbol name="LED-TRICOLOR-INDV">
<pin name="GRN-A"/>
<pin name="BLU-A"/>
<pin name="RED-C"/>
<pin name="RED-A"/>
<pin name="BLU-C"/>
<pin name="GRN-C"/>
</symbol>
<symbol name="W5100">
<pin name="RSET_BG"/>
<pin name="3V3A"/>
<pin name="NC@0"/>
<pin name="GNDA@0"/>
<pin name="RXIP"/>
<pin name="RXIN"/>
<pin name="1V8A@0"/>
<pin name="TXOP"/>
<pin name="TXON"/>
<pin name="GNDA@1"/>
<pin name="1V8OUT"/>
<pin name="3V3D@0"/>
<pin name="GNDD@0"/>
<pin name="GNDD@1"/>
<pin name="1V8D@0"/>
<pin name="1V8D@1"/>
<pin name="GNDD@2"/>
<pin name="3V3D@1"/>
<pin name="DATA7"/>
<pin name="DATA6"/>
<pin name="DATA5"/>
<pin name="DATA4"/>
<pin name="DATA3"/>
<pin name="DATA2"/>
<pin name="DATA1"/>
<pin name="DATA0"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="*SCS"/>
<pin name="SCLK"/>
<pin name="SEN"/>
<pin name="GNDD@3"/>
<pin name="1V8D@2"/>
<pin name="TEST3"/>
<pin name="TEST2"/>
<pin name="TEST1"/>
<pin name="TEST0"/>
<pin name="ADDR14"/>
<pin name="ADDR13"/>
<pin name="ADDR12"/>
<pin name="ADDR11"/>
<pin name="ADDR10"/>
<pin name="GNDD@4"/>
<pin name="3V3D@2"/>
<pin name="ADDR9"/>
<pin name="ADDR8"/>
<pin name="ADDR7"/>
<pin name="ADDR6"/>
<pin name="ADDR5"/>
<pin name="ADDR4"/>
<pin name="ADDR3"/>
<pin name="ADDR2"/>
<pin name="ADDR1"/>
<pin name="ADDR0"/>
<pin name="*CS"/>
<pin name="*INT"/>
<pin name="*WR"/>
<pin name="*RD"/>
<pin name="*RESET"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="OPMODE0"/>
<pin name="OPMODE1"/>
<pin name="OPMODE2"/>
<pin name="LINKLED"/>
<pin name="SPDLED"/>
<pin name="GNDD@5"/>
<pin name="1V8D@3"/>
<pin name="FDXLED"/>
<pin name="COLLED"/>
<pin name="RXLED"/>
<pin name="TXLED"/>
<pin name="1V8A@1"/>
<pin name="XTLN"/>
<pin name="XTLP"/>
<pin name="GNDA@2"/>
<pin name="NC@4"/>
<pin name="NC@5"/>
<pin name="NC@6"/>
</symbol>
<symbol name="MAGJACK">
<pin name="YLED-"/>
<pin name="YLED+"/>
<pin name="GLED-"/>
<pin name="GLED+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TD+"/>
<pin name="SHIELD@0"/>
<pin name="SHIELD@1"/>
</symbol>
<symbol name="SI470X">
<pin name="!RST"/>
<pin name="!SEN"/>
<pin name="DOUT"/>
<pin name="FMIP"/>
<pin name="GND@12"/>
<pin name="GND@PAD"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="LOUT"/>
<pin name="LPI"/>
<pin name="RCLK"/>
<pin name="RFGND"/>
<pin name="ROUT"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="VA"/>
<pin name="VD"/>
<pin name="VIO"/>
</symbol>
<symbol name="OSHW-LOGO">
</symbol>
<symbol name="ATX24-1">
<pin name="-12V"/>
<pin name="3.3V@0"/>
<pin name="3.3V@1"/>
<pin name="3.3V@2"/>
<pin name="3.3V@3"/>
<pin name="5V@0"/>
<pin name="5V@1"/>
<pin name="5V@2"/>
<pin name="5V@3"/>
<pin name="5V@4"/>
<pin name="5V_STDBY"/>
<pin name="12V@0"/>
<pin name="12V@1"/>
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="NC"/>
<pin name="PS_ON"/>
<pin name="PWR_OK"/>
</symbol>
<symbol name="GS1011">
<pin name="GND@1"/>
<pin name="JTAG_TCK"/>
<pin name="JTAG_TDO"/>
<pin name="JTAG_TDI"/>
<pin name="JTAG_TMS"/>
<pin name="JTAG_RST"/>
<pin name="ALARM1"/>
<pin name="RTC_OUT1"/>
<pin name="VBAT"/>
<pin name="DC_CNTL"/>
<pin name="ADC1"/>
<pin name="ADC2"/>
<pin name="ALARM2"/>
<pin name="MSPI_DIN"/>
<pin name="MSPI_DOUT"/>
<pin name="VOUT_1.8V"/>
<pin name="GND@17"/>
<pin name="MSPI_CLK"/>
<pin name="MSPI_CS0"/>
<pin name="MSPI_CS1"/>
<pin name="GPIO21_11MHZ"/>
<pin name="GPIO20_22MHZ"/>
<pin name="GPIO19_44MHZ"/>
<pin name="PWM0/GPIO10"/>
<pin name="I2C_CLK"/>
<pin name="I2C_DATA"/>
<pin name="SSPI_DOUT"/>
<pin name="SSPI_CLK"/>
<pin name="SSPI_CS"/>
<pin name="SSPI_DIN"/>
<pin name="VIN_3V3"/>
<pin name="GND@32"/>
<pin name="EN_1.8V"/>
<pin name="VDDIO"/>
<pin name="UART1_CTS/GPIO26"/>
<pin name="UART1_RTS/GPIO27"/>
<pin name="UART1_RX/GPIO3"/>
<pin name="UART1_TX/GPIO2"/>
<pin name="UART0_TX/GPIO1"/>
<pin name="UART0_RTS/GPIO25"/>
<pin name="UART0_RX/GPIO0"/>
<pin name="UART0_CTS/GPIO24"/>
<pin name="GPIO31_LED2"/>
<pin name="GPIO30_LED1"/>
<pin name="GPIO29"/>
<pin name="GPIO28"/>
<pin name="EXT_RESET"/>
<pin name="GND@48"/>
</symbol>
<symbol name="CAPSENSE_PAD">
<pin name="RES"/>
<pin name="RECEIVE"/>
</symbol>
<symbol name="HMC5883L">
<pin name="SCL"/>
<pin name="VDD"/>
<pin name="NC@1"/>
<pin name="S1"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
<pin name="SETP"/>
<pin name="GND@1"/>
<pin name="C1"/>
<pin name="GND@2"/>
<pin name="SETC"/>
<pin name="VDDIO"/>
<pin name="NC@5"/>
<pin name="DRDY"/>
<pin name="SDA"/>
</symbol>
<symbol name="L3G4200D">
<pin name="VDDIO"/>
<pin name="SCL"/>
<pin name="SDA/SDI"/>
<pin name="SDO"/>
<pin name="CS"/>
<pin name="INT2"/>
<pin name="INT1"/>
<pin name="RSVDG@0"/>
<pin name="VDD"/>
<pin name="RSVDV@0"/>
<pin name="PLL"/>
<pin name="GND"/>
<pin name="RSVDG@4"/>
<pin name="RSDVG@3"/>
<pin name="RSVDG@2"/>
<pin name="RSVDG@1"/>
</symbol>
<symbol name="MAGJACK-2">
<pin name="YLED-"/>
<pin name="YLED+"/>
<pin name="GLED-"/>
<pin name="GLED+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TD+"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="MAX1704X">
<pin name="CTG"/>
<pin name="CELL"/>
<pin name="VDD"/>
<pin name="GND@4"/>
<pin name="ALT"/>
<pin name="QST"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND@EP"/>
</symbol>
<symbol name="TLC5940">
<pin name="GND"/>
<pin name="BLANK"/>
<pin name="SCLK"/>
<pin name="SIN"/>
<pin name="VPRG"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="OUT8"/>
<pin name="XLAT"/>
<pin name="OUT9"/>
<pin name="OUT10"/>
<pin name="OUT11"/>
<pin name="OUT12"/>
<pin name="OUT13"/>
<pin name="OUT14"/>
<pin name="OUT15"/>
<pin name="XERR"/>
<pin name="SOUT"/>
<pin name="GSCLK"/>
<pin name="DCPRG"/>
<pin name="IREF"/>
<pin name="VCC"/>
</symbol>
<symbol name="TMP36">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="MAG3110">
<pin name="CAP-A"/>
<pin name="CAP-R"/>
<pin name="GND@5"/>
<pin name="GND@10"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="INT1"/>
<pin name="VDDIO"/>
<pin name="VDD"/>
</symbol>
<symbol name="TPS6211*">
<pin name="AGND" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="LBI" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="PG" direction="out"/>
<pin name="PGND@1" direction="pwr"/>
<pin name="PGND@2" direction="pwr"/>
<pin name="PWPD" direction="pwr"/>
<pin name="SW@1" direction="out"/>
<pin name="SW@2" direction="out"/>
<pin name="SYNC" direction="in"/>
<pin name="VIN@1" direction="pwr"/>
<pin name="VIN@2" direction="pwr"/>
<pin name="VINA" direction="pwr"/>
</symbol>
<symbol name="ATMEGA2560">
<pin name="(A8)PC0"/>
<pin name="(A9)PC1"/>
<pin name="(A10)PC2"/>
<pin name="(A11)PC3"/>
<pin name="(A12)PC4"/>
<pin name="(A13)PC5"/>
<pin name="(A14)PC6"/>
<pin name="(A15)PC7"/>
<pin name="(AD0)PA0"/>
<pin name="(AD1)PA1"/>
<pin name="(AD2)PA2"/>
<pin name="(AD3)PA3"/>
<pin name="(AD4)PA4"/>
<pin name="(AD5)PA5"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(ADC0)PF0"/>
<pin name="(ADC1)PF1"/>
<pin name="(ADC2)PF2"/>
<pin name="(ADC3)PF3"/>
<pin name="(ADC4/TCK)PF4"/>
<pin name="(ADC5/TMS)PF5"/>
<pin name="(ADC6/TDO)PF6"/>
<pin name="(ADC7/TDI)PF7"/>
<pin name="(ALE)PG2"/>
<pin name="(CLKO/ICP3/INT7)PE7"/>
<pin name="(ICP1)PD4"/>
<pin name="(MISO/PCINT3)PB3"/>
<pin name="(MOSI/PCINT2)PB2"/>
<pin name="(OC0A/OC1C/PCINT7)PB7"/>
<pin name="(OC0B)PG5"/>
<pin name="(OC1A/PCINT5)PB5"/>
<pin name="(OC1B/PCINT6)PB6"/>
<pin name="(OC2A/PCINT4)PB4"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(RD)PG1"/>
<pin name="(RXD0/PCIN8)PE0"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SCK/PCINT1)PB1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SS/PCINT0)PB0"/>
<pin name="(T0)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(TOSC1)PG4"/>
<pin name="(TOSC2)PG3"/>
<pin name="(TXD0)PE1"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(WR)PG0"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(XCK1)PD5"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="PH0(RXD2)"/>
<pin name="PH1(TXD2)"/>
<pin name="PH2(XCK2)"/>
<pin name="PH3(OC4A)"/>
<pin name="PH4(OC4B)"/>
<pin name="PH5(OC4C)"/>
<pin name="PH6(OC2B)"/>
<pin name="PH7(T4)"/>
<pin name="PJ0(RXD3/PCINT9)"/>
<pin name="PJ1(TXD3/PCINT10)"/>
<pin name="PJ2(XCK3/PCINT11)"/>
<pin name="PJ3(PCINT12)"/>
<pin name="PJ4(PCINT13)"/>
<pin name="PJ5(PCINT14)"/>
<pin name="PJ6(PCINT15)"/>
<pin name="PJ7"/>
<pin name="PK0(ADC8/PCINT16)"/>
<pin name="PK1(ADC9/PCINT17)"/>
<pin name="PK2(ADC10/PCINT18)"/>
<pin name="PK3(ADC11/PCINT19)"/>
<pin name="PK4(ADC12/PCINT20)"/>
<pin name="PK5(ADC13/PCINT21)"/>
<pin name="PK6(ADC14/PCINT22)"/>
<pin name="PK7(ADC15/PCINT23)"/>
<pin name="PL0(ICP4)"/>
<pin name="PL1(ICP5)"/>
<pin name="PL2(T5)"/>
<pin name="PL3(OC5A)"/>
<pin name="PL4(OC5B)"/>
<pin name="PL5(OC5C)"/>
<pin name="PL6"/>
<pin name="PL7"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
</symbol>
<symbol name="FIDUCIALTAB">
</symbol>
<symbol name="74AHC1G08">
<pin name="B"/>
<pin name="A"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="Y"/>
</symbol>
<symbol name="RELAY-SOLIDSTATE">
<pin name="T1"/>
<pin name="T2"/>
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="LOAD_CELL">
<pin name="B" direction="pas"/>
<pin name="R" direction="pas"/>
<pin name="W" direction="pas"/>
</symbol>
<symbol name="AD7781">
<pin name="SCLK"/>
<pin name="DOUT"/>
<pin name="GAIN"/>
<pin name="AIN+"/>
<pin name="AIN-"/>
<pin name="REFIN+"/>
<pin name="REFIN-"/>
<pin name="BPDSW"/>
<pin name="GND"/>
<pin name="AVDD"/>
<pin name="DVDD"/>
<pin name="*PDRST"/>
<pin name="FILTER"/>
</symbol>
<symbol name="ENCODER_LED_2">
<pin name="-" direction="pas"/>
<pin name="+R" direction="pas"/>
<pin name="A"/>
<pin name="C"/>
<pin name="B"/>
<pin name="+G" direction="pas"/>
</symbol>
<symbol name="LED_RING">
<pin name="COM1" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="COM0" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="ENCODER_LED_2-1">
<pin name="-" direction="pas"/>
<pin name="+R" direction="pas"/>
<pin name="A"/>
<pin name="C"/>
<pin name="B"/>
<pin name="+G" direction="pas"/>
<pin name="SW" direction="pas"/>
</symbol>
<symbol name="ARDUINO-MEGA">
<pin name="5V@0"/>
<pin name="RESET"/>
<pin name="5V@1"/>
<pin name="A0(RX0)"/>
<pin name="A1(TX0)"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="1(TX0)"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="GND@4"/>
<pin name="16(TX2)"/>
<pin name="17(RX2)"/>
<pin name="18(TX1)"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="40"/>
<pin name="39"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="15(RX3)"/>
<pin name="14(TX3)"/>
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="53"/>
<pin name="52"/>
<pin name="51"/>
<pin name="50"/>
<pin name="49"/>
<pin name="5V@2"/>
<pin name="3.3V"/>
<pin name="AREF"/>
<pin name="21(SCL)"/>
<pin name="20(SDA)"/>
<pin name="19(RX1)"/>
<pin name="VIN"/>
<pin name="0(RX0)"/>
</symbol>
<symbol name="MAX3421E-1">
<pin name="VCC"/>
<pin name="VL"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBCOMP"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="INT"/>
<pin name="RES"/>
<pin name="GPX"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="SS"/>
<pin name="GND@3"/>
<pin name="GND@19"/>
<pin name="GOUT7"/>
<pin name="GOUT6"/>
<pin name="GOUT5"/>
<pin name="GOUT4"/>
<pin name="GOUT3"/>
<pin name="GOUT2"/>
<pin name="GOUT1"/>
<pin name="GOUT0"/>
<pin name="GPIN7"/>
<pin name="GPIN6"/>
<pin name="GPIN5"/>
<pin name="GPIN4"/>
<pin name="GPIN3"/>
<pin name="GPIN2"/>
<pin name="GPIN1"/>
<pin name="GPIN0"/>
</symbol>
<symbol name="IDG500-1">
<pin name="GND@2"/>
<pin name="GND@8"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="CPOUT"/>
<pin name="YAGC"/>
<pin name="XAGC"/>
<pin name="VDD@19"/>
<pin name="VDD@9"/>
<pin name="X4.5IN"/>
<pin name="XOUT"/>
<pin name="X4.5OUT"/>
<pin name="Y4.5IN"/>
<pin name="YOUT"/>
<pin name="Y4.5OUT"/>
<pin name="PTATS"/>
<pin name="AZ"/>
<pin name="VREF"/>
</symbol>
<symbol name="RS9110-N-11-22">
<pin name="VIN@46"/>
<pin name="VIN@47"/>
<pin name="JPD0"/>
<pin name="JPD1"/>
<pin name="JPD2"/>
<pin name="INTR"/>
<pin name="RST"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="SD3"/>
<pin name="CLK"/>
<pin name="CS"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="MODE"/>
<pin name="GND@10"/>
<pin name="GND@16"/>
<pin name="GND@20"/>
<pin name="GND@21"/>
<pin name="GND@48"/>
<pin name="GND@PAD"/>
</symbol>
<symbol name="MAX7219">
<pin name="DIN"/>
<pin name="DIG0"/>
<pin name="DIG4"/>
<pin name="GND"/>
<pin name="DIG6"/>
<pin name="DIG2"/>
<pin name="DIG3"/>
<pin name="DIG7"/>
<pin name="GND2"/>
<pin name="DIG5"/>
<pin name="DIG1"/>
<pin name="LOAD"/>
<pin name="CLK"/>
<pin name="SEGA"/>
<pin name="SEGF"/>
<pin name="SEGB"/>
<pin name="SEGG"/>
<pin name="ISET"/>
<pin name="VCC"/>
<pin name="SEGC"/>
<pin name="SEGE"/>
<pin name="SEGDP"/>
<pin name="SEGD"/>
<pin name="DOUT"/>
</symbol>
<symbol name="MAX485">
<pin name="RO"/>
<pin name="RE" function="dot"/>
<pin name="DE"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="A"/>
<pin name="B"/>
<pin name="VCC"/>
</symbol>
<symbol name="HDJD-S822-QR999">
<pin name="VROUT"/>
<pin name="VGOUT"/>
<pin name="VBOUT"/>
<pin name="GSBLUE1"/>
<pin name="GSGRN0"/>
<pin name="VDD3"/>
<pin name="GND"/>
<pin name="TEST_EN"/>
<pin name="VDD5"/>
<pin name="GSRED1"/>
<pin name="GSGRN1"/>
<pin name="GSBLUE0"/>
<pin name="GSRED0"/>
</symbol>
<symbol name="RPACK-BUSSED-5">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="LED_BARGRAPH_10">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="STM811">
<pin name="VCC"/>
<pin name="VSS"/>
<pin name="~RST"/>
<pin name="~MR"/>
</symbol>
<symbol name="MAGJACK-POE">
<pin name="YLED-"/>
<pin name="YLED+"/>
<pin name="GLED-"/>
<pin name="GLED+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TD+"/>
<pin name="SHIELD@0"/>
<pin name="SHIELD@1"/>
<pin name="V+"/>
<pin name="V-"/>
</symbol>
<symbol name="VCNL4000">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="IR-@1"/>
<pin name="IR-@0"/>
<pin name="IR+"/>
<pin name="VDD"/>
<pin name="GND@1"/>
<pin name="GND@0"/>
</symbol>
<symbol name="NE555">
<pin name="TRE" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="DIS" direction="in"/>
<pin name="TRI" direction="in"/>
<pin name="VCC+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CON" direction="in"/>
<pin name="/RES" direction="in"/>
</symbol>
<symbol name="VENUS638FLPX-L">
<pin name="LED/GPIO0"/>
<pin name="TXD0"/>
<pin name="RXD0"/>
<pin name="PPS"/>
<pin name="CLK"/>
<pin name="CSN"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="GND@19"/>
<pin name="GND@15"/>
<pin name="GNDRF@21"/>
<pin name="GNDRF@22"/>
<pin name="GNDRF@24"/>
<pin name="GNDRF@25"/>
<pin name="GNDRF@27"/>
<pin name="GNDRF@28"/>
<pin name="GNDRF@29"/>
<pin name="GNDRF@31"/>
<pin name="GNDRF@33"/>
<pin name="RTC"/>
<pin name="BTSEL"/>
<pin name="RSTN"/>
<pin name="RFIN"/>
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="GPIO1"/>
<pin name="REGEN"/>
<pin name="GPIO2"/>
<pin name="GPIO20"/>
<pin name="PIO12"/>
<pin name="PIO14"/>
<pin name="GPIO24"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GPIO4"/>
<pin name="GPIO3"/>
<pin name="GND@49"/>
<pin name="PIO5"/>
<pin name="PIO11"/>
<pin name="RXD1"/>
<pin name="GPIO25"/>
<pin name="GPIO30"/>
<pin name="PIO15"/>
<pin name="TXD1"/>
<pin name="VCC@58"/>
<pin name="GPIO28"/>
<pin name="GND@60"/>
<pin name="GNDRF@61"/>
<pin name="GNDRF@62"/>
<pin name="GPIO6"/>
<pin name="GND@64"/>
<pin name="GNDRF@65"/>
<pin name="GNDRF@69"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO29"/>
</symbol>
<symbol name="LM5007">
<pin name="SW"/>
<pin name="BST"/>
<pin name="RCL"/>
<pin name="RTN"/>
<pin name="FB"/>
<pin name="RON"/>
<pin name="VCC"/>
<pin name="VIN"/>
<pin name="EP"/>
</symbol>
<symbol name="LM5574">
<pin name="VCC"/>
<pin name="SD"/>
<pin name="VIN"/>
<pin name="SYNC"/>
<pin name="COMP"/>
<pin name="FB"/>
<pin name="RT"/>
<pin name="RAMP"/>
<pin name="AGND"/>
<pin name="SS"/>
<pin name="OUT"/>
<pin name="PGND"/>
<pin name="IS"/>
<pin name="SW"/>
<pin name="PRE"/>
<pin name="BST"/>
</symbol>
<symbol name="MMA8452Q">
<pin name="VDDIO"/>
<pin name="BYP"/>
<pin name="SCL"/>
<pin name="GND@0"/>
<pin name="SDA"/>
<pin name="SA0"/>
<pin name="INT2"/>
<pin name="GND@1"/>
<pin name="INT1"/>
<pin name="GND@2"/>
<pin name="VDD"/>
</symbol>
<symbol name="MAX6675">
<pin name="VSS"/>
<pin name="T-"/>
<pin name="T+"/>
<pin name="VDD"/>
<pin name="MISO"/>
<pin name="CS"/>
<pin name="SCK"/>
</symbol>
<symbol name="556_TIMER_DUAL">
<pin name="GND"/>
<pin name="TRIG"/>
<pin name="OUT"/>
<pin name="CV"/>
<pin name="RST"/>
<pin name="THR"/>
<pin name="DIS"/>
<pin name="TRIG2"/>
<pin name="OUT2"/>
<pin name="RST2"/>
<pin name="CV2"/>
<pin name="THR2"/>
<pin name="DIS2"/>
<pin name="VCC"/>
</symbol>
<symbol name="RFM22">
<pin name="ANT"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="NIRQ" direction="out"/>
<pin name="NSEL" direction="in"/>
<pin name="RXANT" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDN" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="TXANT" direction="in"/>
<pin name="VCC"/>
</symbol>
<symbol name="ATMEGA32U4">
<pin name="!RESET"/>
<pin name="AREF"/>
<pin name="AVCC@24"/>
<pin name="AVCC@44"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND@15"/>
<pin name="GND@23"/>
<pin name="GND@35"/>
<pin name="GND@43"/>
<pin name="PB0(SS)"/>
<pin name="PB1(SCK)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB3(MISO)"/>
<pin name="PB4(ADC11)"/>
<pin name="PB5(ADC12)"/>
<pin name="PB6(ADC13)"/>
<pin name="PB7"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0(SCL)"/>
<pin name="PD1(SDA)"/>
<pin name="PD2(RX)"/>
<pin name="PD3(TX)"/>
<pin name="PD4(ADC8)"/>
<pin name="PD5"/>
<pin name="PD6(ADC9)"/>
<pin name="PD7(ADC10)"/>
<pin name="PE2/!HWB"/>
<pin name="PE6"/>
<pin name="PF0(ADC0)"/>
<pin name="PF1(ADC1)"/>
<pin name="PF4(ADC4)"/>
<pin name="PF5(ADC5)"/>
<pin name="PF6(ADC6)"/>
<pin name="PF7(ADC7)"/>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="UVCC"/>
<pin name="VBUS"/>
<pin name="VCC@14"/>
<pin name="VCC@34"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
</symbol>
<symbol name="ANDROID-ELECTRIC_SHEEP_LOGO">
</symbol>
<symbol name="GP-2106">
<pin name="VCC"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="ONOFF"/>
<pin name="1PPS"/>
<pin name="GND"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="V-REG-LDO-ADJ">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="ADJ" direction="in"/>
</symbol>
<symbol name="SWITCH-SP3T">
<pin name="1"/>
<pin name="3"/>
<pin name="2"/>
<pin name="4"/>
</symbol>
<symbol name="OR-SINGLE">
<pin name="B"/>
<pin name="A"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="Y"/>
</symbol>
<symbol name="ENCODER_LED_RGB">
<pin name="K" direction="pas"/>
<pin name="R" direction="pas"/>
<pin name="A"/>
<pin name="C"/>
<pin name="B"/>
<pin name="G" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="BL" direction="pas"/>
</symbol>
<symbol name="HT8950">
<pin name="SW0"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="VSS"/>
<pin name="AO"/>
<pin name="AIN"/>
<pin name="VDD"/>
<pin name="LAMP"/>
<pin name="AUDIO"/>
<pin name="VREF"/>
<pin name="TS"/>
<pin name="FVIB"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="VIB"/>
<pin name="TGU"/>
<pin name="TGD"/>
<pin name="ROB"/>
</symbol>
<symbol name="4VDD4VSS">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
</symbol>
<symbol name="P8X32A">
<pin name="BOE/" direction="in"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="RES/"/>
<pin name="XI" direction="in"/>
<pin name="XO" direction="out"/>
</symbol>
<symbol name="RESISTOR-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="ENCODER_LED_3_CA">
<pin name="+" direction="pas"/>
<pin name="-G" direction="pas"/>
<pin name="A"/>
<pin name="C"/>
<pin name="B"/>
<pin name="-R" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="-B" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SSOP48">
<gates>
<gate name="G$1" symbol="SSOP48"/>
</gates>
<devices>
<device name="" package="SSOP48">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$41" pad="41"/>
<connect gate="G$1" pin="P$42" pad="42"/>
<connect gate="G$1" pin="P$43" pad="43"/>
<connect gate="G$1" pin="P$44" pad="44"/>
<connect gate="G$1" pin="P$45" pad="45"/>
<connect gate="G$1" pin="P$46" pad="46"/>
<connect gate="G$1" pin="P$47" pad="47"/>
<connect gate="G$1" pin="P$48" pad="48"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TQFP44">
<gates>
<gate name="G$1" symbol="TQFP44"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$41" pad="41"/>
<connect gate="G$1" pin="P$42" pad="42"/>
<connect gate="G$1" pin="P$43" pad="43"/>
<connect gate="G$1" pin="P$44" pad="44"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor&lt;/b&gt;
Basic schematic elements and footprints for 0603, 1206, and PTH resistors.</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AXIAL-0.3" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805-RES" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-RES" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-RES" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/6W" package="1/6W-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/4W" package="AXIAL-0.4">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/2W" package="AXIAL-0.5">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1W" package="AXIAL-0.6">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-2W" package="AXIAL-0.8">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="AXIAL-0.3-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-MEGA8" prefix="U$">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
6-channel 10 bit ADC&lt;p&gt;
2-channel 8 bit ADC</description>
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="-MI" package="MLF32">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AI" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-MEGA8-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
2-channel 8 bit ADC</description>
<gates>
<gate name="G$1" symbol="23-I/O-2"/>
</gates>
<devices>
<device name="PTH" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIM" package="DIL28-3-SIMON">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ZIF_SOCKET" package="DIL28-3-ZIF_SOCKET">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="DIL28-3-SIMON-KIT">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LEDs&lt;/b&gt;
Standard schematic elements and footprints for 5mm, 3mm, 1206, and 0603 sized LEDs. 5mm - Spark Fun Electronics SKU : COM-00529 (and others)</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FKIT-1206" package="FKIT-LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3MM-NO_SILK" package="LED3MM-NS">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM-KIT" package="LED5MM-KIT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL" prefix="Y" uservalue="yes">
<description>&lt;b&gt;Crystals&lt;/b&gt;
Various standard crystals. Proven footprints. Spark Fun Electronics SKU : COM-00534</description>
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="HC49UV" package="HC49U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC38H" package="TC38H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC26H" package="TC26H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49US" package="HC49US">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="32-SMD" package="CRYSTAL-32KHZ-SMD">
<connects>
<connect gate="G$1" pin="1" pad="X1"/>
<connect gate="G$1" pin="2" pad="X2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5X3" package="CRYSTAL-SMD-5X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EPSONMC146" package="CRYSTAL-32KHZ-SMD_EPSON_MC146">
<connects>
<connect gate="G$1" pin="1" pad="P$2"/>
<connect gate="G$1" pin="2" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10.5X4.8" package="CRYSTAL-SMD-10.5X4.8-2PIN">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_78XX" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator&lt;/b&gt;
Standard 7805 5V regulator. IGO (Input Ground Output). Spark Fun Electronics SKU : COM-00107</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="SIDE" package="78XXL">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SINK" package="TO220-IGO">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO-92" package="TO-92">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-220" package="TO-220-ALT">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_TPS76433" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator&lt;/b&gt;
Older TI part. LDO 150mA regulator. No output by-pass cap option. See V_REG_LDO for a better part.</description>
<gates>
<gate name="G$1" symbol="TPS76433DBVT"/>
</gates>
<devices>
<device name="SOT23-5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIRF" prefix="MIRF" uservalue="yes">
<description>&lt;b&gt;MiRF Layout&lt;/b&gt;
This layout mates with the Spark Fun Electronics SKU : WRL-00153 transceiver.</description>
<gates>
<gate name="A" symbol="MIRF"/>
</gates>
<devices>
<device name="" package="MIRF">
<connects>
<connect gate="A" pin="1" pad="7"/>
<connect gate="A" pin="2" pad="6"/>
<connect gate="A" pin="3" pad="5"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="3"/>
<connect gate="A" pin="6" pad="2"/>
<connect gate="A" pin="7" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_NPN" prefix="Q" uservalue="yes">
<description>&lt;b&gt;Transistor NPN&lt;/b&gt;
BJT configuration in SOT23 package. MMBT2222 is the common NPN we use. Double check BCE configuration again layout.</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23-3" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="&quot;" package="SOT223">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT89" package="SOT89">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO-92-AMMO" package="TO-92-AMMO">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="VCC2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LM1117" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator LM1117&lt;/b&gt;
Standard adjustable voltage regulator but in SMD form. Spark Fun Electronics SKU : COM-00595</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_SPI_PROG">
<description>&lt;b&gt;AVR ICSP Header&lt;/b&gt; 
This is the standard AVR In Circuit Serial Programming header. Minimal, but includes pin one indicator. Works with standard Olimex programmers. Also look for the 6-pin reduced version. Spark Fun Electronics SKU: PRT-00778</description>
<gates>
<gate name="A" symbol="AVR_SPI_PROGRAMMER"/>
</gates>
<devices>
<device name="" package="AVR_ICSP">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP2103_USB_UART" prefix="IC">
<description>&lt;b&gt;Single-Chip USB to UART Bridge&lt;/b&gt;
Source: www.silabs.com .. CP2103.pdf. Spark Fun Electronics SKU : COM-00309</description>
<gates>
<gate name="G$1" symbol="CP2103"/>
</gates>
<devices>
<device name="" package="MLP28">
<connects>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="!SUSPEND" pad="11"/>
<connect gate="G$1" pin="CTS" pad="22"/>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="4"/>
<connect gate="G$1" pin="DCD" pad="28"/>
<connect gate="G$1" pin="DSR" pad="26"/>
<connect gate="G$1" pin="DTR" pad="27"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@M" pad="M"/>
<connect gate="G$1" pin="GPIO_0" pad="19"/>
<connect gate="G$1" pin="GPIO_1" pad="18"/>
<connect gate="G$1" pin="GPIO_2" pad="17"/>
<connect gate="G$1" pin="GPIO_3" pad="16"/>
<connect gate="G$1" pin="REGIN" pad="7"/>
<connect gate="G$1" pin="RI" pad="1"/>
<connect gate="G$1" pin="RTS" pad="23"/>
<connect gate="G$1" pin="RXD" pad="24"/>
<connect gate="G$1" pin="SUSPEND" pad="12"/>
<connect gate="G$1" pin="TXD" pad="25"/>
<connect gate="G$1" pin="VBUS" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VIO" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP210X_USB_UART" prefix="IC">
<description>&lt;b&gt;Single-Chip USB to UART Bridge&lt;/b&gt;&lt;p&gt;
Source: www.silabs.com .. CP2101.pdf / cp2102.pdf. Spark Fun Electronics SKU : COM-00310</description>
<gates>
<gate name="G$1" symbol="CP2101"/>
</gates>
<devices>
<device name="" package="MLP28">
<connects>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="!SUSPEND" pad="11"/>
<connect gate="G$1" pin="CTS" pad="23"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="5"/>
<connect gate="G$1" pin="DCD" pad="1"/>
<connect gate="G$1" pin="DSR" pad="27"/>
<connect gate="G$1" pin="DTR" pad="28"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@M" pad="M"/>
<connect gate="G$1" pin="REGIN" pad="7"/>
<connect gate="G$1" pin="RI" pad="2"/>
<connect gate="G$1" pin="RTS" pad="24"/>
<connect gate="G$1" pin="RXD" pad="25"/>
<connect gate="G$1" pin="SUSPEND" pad="12"/>
<connect gate="G$1" pin="TXD" pad="26"/>
<connect gate="G$1" pin="VBUS" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="X">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;
&lt;p&gt;USB-B-PTH is fully proven SKU : PRT-00139
&lt;p&gt;USB-miniB is fully proven SKU : PRT-00587
&lt;p&gt;USB-A-PCB is untested.
&lt;p&gt;USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437
&lt;p&gt;USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.
&lt;p&gt;USB-A-S has not been used/tested
&lt;p&gt;USB-MB-H has not been used/tested</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D-"/>
<connect gate="G$1" pin="D-" pad="D+"/>
<connect gate="G$1" pin="GND" pad="VBUS"/>
<connect gate="G$1" pin="VBUS" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OLD" package="USB-MINIB-OLD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S4B-PH">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VBUS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PCB" package="USB-A-PCB">
<connects>
<connect gate="G$1" pin="D+" pad="USB_P"/>
<connect gate="G$1" pin="D-" pad="USB_M"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="5V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-VERTICAL" package="USB-B-PTH-VERTICAL">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-A-S-NOSILK" package="USB-A-S-NOSILK">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-SMD" package="USB-A-S-NOSILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-NS" package="USB-MINIB-NOSTOP">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="USB-A-S-SILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAC_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;Momentary Switch&lt;/b&gt;
Button commonly used for reset or general input. Spark Fun Electronics SKU : COM-00097</description>
<gates>
<gate name="S" symbol="SWITCH-MOMENTARY"/>
</gates>
<devices>
<device name="SMD" package="TACTILE_SWITCH_SMD">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KSA_SEALED" package="KSA_SEALED_TAC_SWITCH">
<connects>
<connect gate="S" pin="1" pad="P$1"/>
<connect gate="S" pin="2" pad="P$2"/>
<connect gate="S" pin="3" pad="P$3"/>
<connect gate="S" pin="4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4871">
<gates>
<gate name="G$1" symbol="LM4871"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="BYPASS" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="SHUTDWN" pad="1"/>
<connect gate="G$1" pin="V01" pad="5"/>
<connect gate="G$1" pin="V02" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="X9015_DIGI_POT">
<gates>
<gate name="G$1" symbol="X9015_DIGI_POT"/>
</gates>
<devices>
<device name="S" package="SO08">
<connects>
<connect gate="G$1" pin="CS'" pad="7"/>
<connect gate="G$1" pin="INC'" pad="1"/>
<connect gate="G$1" pin="RH/VH" pad="3"/>
<connect gate="G$1" pin="RL/VL" pad="6"/>
<connect gate="G$1" pin="RW/VW" pad="5"/>
<connect gate="G$1" pin="U/D'" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LASSEN_IQ_GPS">
<description>&lt;b&gt;Lassen iq&lt;/b&gt;
12-Channel GPS receiver. Schematic and footprint production proven. Spark Fun Electronics SKU : GPS-00163. Surface mount mating connector : GPS-00170</description>
<gates>
<gate name="G$1" symbol="LASSEN_IQ_GPS"/>
</gates>
<devices>
<device name="LASSEN" package="LASSEN_IQ_GPS">
<connects>
<connect gate="G$1" pin="BATT" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PPS" pad="4"/>
<connect gate="G$1" pin="RXA" pad="3"/>
<connect gate="G$1" pin="RXB" pad="6"/>
<connect gate="G$1" pin="TXA" pad="1"/>
<connect gate="G$1" pin="TXB" pad="5"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HV826MG_BACKLIGHT">
<description>&lt;b&gt;HV826MG&lt;/b&gt;
Small EL backlight driver for the CFAX 128x64 graphical display.</description>
<gates>
<gate name="G$1" symbol="HV826MG_BACKLIGHT"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="REL" pad="3"/>
<connect gate="G$1" pin="RSW" pad="2"/>
<connect gate="G$1" pin="VA" pad="8"/>
<connect gate="G$1" pin="VB" pad="7"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC213X" prefix="IC">
<description>&lt;b&gt;LPC213x&lt;/b&gt;
Schematic element and footprint for NXP LPC213x. Spark Fun Electronics SKU : COM-00520</description>
<gates>
<gate name="G$1" symbol="LPC213X"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="(AD0.0/CAP0.1/MAT0.1)P0.27" pad="11"/>
<connect gate="G$1" pin="(AD0.1/CAP0.2/MAT0.2)P0.28" pad="13"/>
<connect gate="G$1" pin="(AD0.2/CAP0.3/MAT0.3)P0.29" pad="14"/>
<connect gate="G$1" pin="(AD0.3/EINT3/CAP0.0)P0.30" pad="15"/>
<connect gate="G$1" pin="(AD0.4/AOUT)P0.25" pad="9"/>
<connect gate="G$1" pin="(AD0.5)P0.26" pad="10"/>
<connect gate="G$1" pin="(AD1.7/CAP0.0/MAT0.0)P0.22" pad="2"/>
<connect gate="G$1" pin="(CAP1.2/SCK1/MAT1.2)P0.17" pad="47"/>
<connect gate="G$1" pin="(CAP1.3/MISO1/MAT1.3)P0.18" pad="53"/>
<connect gate="G$1" pin="(CTS1/CAP1.1/SCL1)P0.11" pad="37"/>
<connect gate="G$1" pin="(DCD1/EINT1/SDA1)P0.14" pad="41"/>
<connect gate="G$1" pin="(DSR1/MAT1.0/AD1.3)P0.12" pad="38"/>
<connect gate="G$1" pin="(DTR1/MAT1.1/AD1.4)P0.13" pad="39"/>
<connect gate="G$1" pin="(EINT0/MAT0.2/CAP0.2)P0.16" pad="46"/>
<connect gate="G$1" pin="(MAT1.2/MOSI1/CAP1.2)P0.19" pad="54"/>
<connect gate="G$1" pin="(MAT1.3/SSEL1/EINT3)P0.20" pad="55"/>
<connect gate="G$1" pin="(MISO0/MAT0.1/A0.7)P0.5" pad="29"/>
<connect gate="G$1" pin="(MOSI0/CAP0.2/AD1.0)P0.6" pad="30"/>
<connect gate="G$1" pin="(PWM5/AD1.6/CAP1.3)P0.21" pad="1"/>
<connect gate="G$1" pin="(RI1/EINT2/AD1.5)P0.15" pad="45"/>
<connect gate="G$1" pin="(RTS1/CAP1.0/AD1.2)P0.10" pad="35"/>
<connect gate="G$1" pin="(RXD0/PWM3/EINT0)P0.1" pad="21"/>
<connect gate="G$1" pin="(RXD1/PWM6/EINT3)P0.9" pad="34"/>
<connect gate="G$1" pin="(SCK0/CAP0.1/AD0.6)P0.4" pad="27"/>
<connect gate="G$1" pin="(SCL0/CAP0.0)P0.2" pad="22"/>
<connect gate="G$1" pin="(SDA0/MAT0.0/EINT1)P0.3" pad="26"/>
<connect gate="G$1" pin="(SSEL0/PWM2/EINT2)P0.7" pad="31"/>
<connect gate="G$1" pin="(TXD0/PWM1)P0.0" pad="19"/>
<connect gate="G$1" pin="(TXD1/PWM4/A1.1)P0.8" pad="33"/>
<connect gate="G$1" pin="P0.23" pad="58"/>
<connect gate="G$1" pin="P0.31" pad="17"/>
<connect gate="G$1" pin="P1.16(TRACEPKT0)" pad="16"/>
<connect gate="G$1" pin="P1.17(TRACEPKT1)" pad="12"/>
<connect gate="G$1" pin="P1.18(TRACEPKT2)" pad="8"/>
<connect gate="G$1" pin="P1.19(TRACEPKT3)" pad="4"/>
<connect gate="G$1" pin="P1.20(TRACESYNC)" pad="48"/>
<connect gate="G$1" pin="P1.21(PIPESTAT0)" pad="44"/>
<connect gate="G$1" pin="P1.22(PIPESTAT1)" pad="40"/>
<connect gate="G$1" pin="P1.23(PIPESTAT2)" pad="36"/>
<connect gate="G$1" pin="P1.24(TRACECLK)" pad="32"/>
<connect gate="G$1" pin="P1.25(EXTIN0)" pad="28"/>
<connect gate="G$1" pin="P1.26(RTCK)" pad="24"/>
<connect gate="G$1" pin="P1.27(TDO)" pad="64"/>
<connect gate="G$1" pin="P1.28(TDI)" pad="60"/>
<connect gate="G$1" pin="P1.29(TCK)" pad="56"/>
<connect gate="G$1" pin="P1.30(TMS)" pad="52"/>
<connect gate="G$1" pin="P1.31(/TRST)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="57"/>
<connect gate="G$1" pin="RTXC1" pad="3"/>
<connect gate="G$1" pin="RTXC2" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="49"/>
<connect gate="G$1" pin="VDD3-1" pad="23"/>
<connect gate="G$1" pin="VDD3-2" pad="43"/>
<connect gate="G$1" pin="VDD3-3" pad="51"/>
<connect gate="G$1" pin="VDDA3" pad="7"/>
<connect gate="G$1" pin="VREF" pad="63"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="18"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="42"/>
<connect gate="G$1" pin="VSS@4" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="59"/>
<connect gate="G$1" pin="XTAL1" pad="62"/>
<connect gate="G$1" pin="XTAL2" pad="61"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74VHC4052_ANALOG_MUX">
<gates>
<gate name="G$1" symbol="74VHC4052_ANALOG_MUX"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN/OUT_X" pad="13"/>
<connect gate="G$1" pin="IN/OUT_Y" pad="3"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="X0" pad="12"/>
<connect gate="G$1" pin="X1" pad="14"/>
<connect gate="G$1" pin="X2" pad="15"/>
<connect gate="G$1" pin="X3" pad="11"/>
<connect gate="G$1" pin="Y0" pad="1"/>
<connect gate="G$1" pin="Y1" pad="5"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEL_DATA_FLASH">
<description>&lt;b&gt;16Mbit EEPROM DataFlash&lt;/b&gt;
Footprint needs touching up. Spark Fun Electronics SKU : COM-00301</description>
<gates>
<gate name="G$1" symbol="ATMEL_DATA_FLASH"/>
</gates>
<devices>
<device name="" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RESET" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X10"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_DIP-2" prefix="SW" uservalue="yes">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SW_DIP-2"/>
</gates>
<devices>
<device name="" package="DIPSWITCH-02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_DIP-8" prefix="SW" uservalue="yes">
<description>&lt;b&gt;DIP Switch 8 Position&lt;/b&gt;
Spark Fun Electronics SKU : COM-08034</description>
<gates>
<gate name="A" symbol="SW_DIP-8"/>
</gates>
<devices>
<device name="" package="DIPSWITCH-08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB9" prefix="X" uservalue="yes">
<description>&lt;b&gt;DB9 Connector&lt;/b&gt;
Standard DB9 (D-Sub 9) serial connector. Can be used for CAN bus as well as RS485 and RS232. Footprint production proven. Spark Fun Electronics SKU : PRT-00429</description>
<gates>
<gate name="G$1" symbol="F09G"/>
</gates>
<devices>
<device name="FEMALE" package="DB9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MALE" package="DB9_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX232" prefix="U">
<description>&lt;b&gt;RS232 Transceiver&lt;/b&gt;
Very common IC. This is generically called 'MAX232', but works with the 3V equivalent MAX3232 generic ICs. Field tested and mother approved. Spark Fun Electronics SKU : COM-00316 (DIP) and COM-00589 (SMD)</description>
<gates>
<gate name="G$1" symbol="MAX232"/>
</gates>
<devices>
<device name="SOIC16" package="SO016">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUERADIO_BR-C40A">
<description>&lt;b&gt;Bluetooth SMD Module&lt;/b&gt;
Footprint fully proven. Spark Fun Electronics SKU : WRL-00149</description>
<gates>
<gate name="G$1" symbol="BLUERADIO_BR-C40A"/>
</gates>
<devices>
<device name="BAS" package="BLUERADIO_BR-C40A">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA_ACCEL_CONNECTOR">
<gates>
<gate name="G$1" symbol="MMA_CON"/>
</gates>
<devices>
<device name="" package="1X08">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GS1" pad="6"/>
<connect gate="G$1" pin="GS2" pad="7"/>
<connect gate="G$1" pin="SLP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="X" pad="3"/>
<connect gate="G$1" pin="Y" pad="4"/>
<connect gate="G$1" pin="Z" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD_CARD_SOCKET">
<description>&lt;b&gt;SD/MMC Socket&lt;/b&gt;
Media socket for SD and MMC cards. Push-push type. Schematic element and footprint production proven. Spark Fun Electronics SKU : PRT-00136</description>
<gates>
<gate name="G$1" symbol="SDCARD"/>
</gates>
<devices>
<device name="SD" package="SD-MMC_SOCKET-PP">
<connects>
<connect gate="G$1" pin="CD" pad="WP"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="2"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="IRQ" pad="8"/>
<connect gate="G$1" pin="P9" pad="9"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD" pad="14"/>
<connect gate="G$1" pin="SW" pad="SW"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="WP" pad="CD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NOKIA6100_LCD">
<description>&lt;b&gt;Nokia 6100 Color LCD&lt;/b&gt;
Schematic element and footprint production proven but could use some touching up. Spark Fun Electronics SKU : LCD-00569. Mating SMD connector : LCD-00570</description>
<gates>
<gate name="G$1" symbol="NOKIA6100_LCD"/>
</gates>
<devices>
<device name="" package="NOKIA6100_LCD">
<connects>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DIO" pad="3"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LEDGND" pad="9"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="VDIGITAL" pad="1"/>
<connect gate="G$1" pin="VDISPLAY" pad="6"/>
<connect gate="G$1" pin="VLED" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA7260" prefix="U">
<description>&lt;b&gt;MMA7260Q&lt;/b&gt;
Triple axis accelerometer from Freescale. Schematic element and footprint production proven. Center pad has reduced paste layer for solder short reduction. Spark Fun Electronics SKU : COM-00308</description>
<gates>
<gate name="G$1" symbol="MMA7260"/>
</gates>
<devices>
<device name="" package="MMA7260">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GS1" pad="1"/>
<connect gate="G$1" pin="GS2" pad="2"/>
<connect gate="G$1" pin="PAD" pad="PAD"/>
<connect gate="G$1" pin="SLP" pad="12"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="X" pad="15"/>
<connect gate="G$1" pin="Y" pad="14"/>
<connect gate="G$1" pin="Z" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND_CONNECT">
<gates>
<gate name="G$1" symbol="GND_CONNECT"/>
</gates>
<devices>
<device name="" package="GND_CONNECT">
<connects>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM34">
<gates>
<gate name="G$1" symbol="LM34"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD725">
<gates>
<gate name="G$1" symbol="AD725"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G$1" pin="4FSC" pad="3"/>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="APOS" pad="4"/>
<connect gate="G$1" pin="BIN" pad="8"/>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="COMP" pad="10"/>
<connect gate="G$1" pin="CRMA" pad="9"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="DPOS" pad="14"/>
<connect gate="G$1" pin="GIN" pad="7"/>
<connect gate="G$1" pin="HSYNC" pad="16"/>
<connect gate="G$1" pin="LUMA" pad="11"/>
<connect gate="G$1" pin="RIN" pad="6"/>
<connect gate="G$1" pin="STND" pad="1"/>
<connect gate="G$1" pin="VSYNC" pad="15"/>
<connect gate="G$1" pin="YTRAP" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-G12864">
<description>&lt;b&gt;Graphical LCD 128x64&lt;/b&gt; 
Footprint is not yet proven. Double check it. Spark Fun Electronics SKU : LCD-00710</description>
<gates>
<gate name="G$1" symbol="LCD-G12864"/>
</gates>
<devices>
<device name="FULL" package="LCD-G12864">
<connects>
<connect gate="G$1" pin="A" pad="19"/>
<connect gate="G$1" pin="CS1" pad="13"/>
<connect gate="G$1" pin="CS2" pad="12"/>
<connect gate="G$1" pin="D/I" pad="16"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="E" pad="17"/>
<connect gate="G$1" pin="K" pad="20"/>
<connect gate="G$1" pin="R/W" pad="15"/>
<connect gate="G$1" pin="RST" pad="14"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="18"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BARE" package="1X20">
<connects>
<connect gate="G$1" pin="A" pad="19"/>
<connect gate="G$1" pin="CS1" pad="13"/>
<connect gate="G$1" pin="CS2" pad="12"/>
<connect gate="G$1" pin="D/I" pad="16"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="E" pad="17"/>
<connect gate="G$1" pin="K" pad="20"/>
<connect gate="G$1" pin="R/W" pad="15"/>
<connect gate="G$1" pin="RST" pad="14"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="18"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT" uservalue="yes">
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="" package="ALPS_POT">
<connects>
<connect gate="G$1" pin="A" pad="P$3"/>
<connect gate="G$1" pin="E" pad="P$1"/>
<connect gate="G$1" pin="S" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRIM" package="TRIM_POT">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="100K_3362U" package="3362U">
<connects>
<connect gate="G$1" pin="A" pad="P$3"/>
<connect gate="G$1" pin="E" pad="P$1"/>
<connect gate="G$1" pin="S" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RV16AF-20" package="POT_ALPHA_RV16AF-20">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MAM" package="POT_MAMMOTH">
<connects>
<connect gate="G$1" pin="A" pad="P$2"/>
<connect gate="G$1" pin="E" pad="P$3"/>
<connect gate="G$1" pin="S" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP41XXX" prefix="U">
<gates>
<gate name="G$1" symbol="MCP41XXX"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="5"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="W" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP42XXX" prefix="U">
<gates>
<gate name="G$1" symbol="MCP42XXX"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="B0" pad="10"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="13"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SHTDWN" pad="12"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="W0" pad="9"/>
<connect gate="G$1" pin="W1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NDS8434">
<gates>
<gate name="G$1" symbol="NDS8434"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="D@1" pad="7"/>
<connect gate="G$1" pin="D@2" pad="8"/>
<connect gate="G$1" pin="D@3" pad="6"/>
<connect gate="G$1" pin="D@4" pad="5"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S@1" pad="1"/>
<connect gate="G$1" pin="S@2" pad="2"/>
<connect gate="G$1" pin="S@3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP7384XX" prefix="U">
<gates>
<gate name="G$1" symbol="MCP73842"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="DRV" pad="8"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="TIMER" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="7"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD_CFAX">
<gates>
<gate name="LCD" symbol="LCD_CFAX"/>
</gates>
<devices>
<device name="" package="LCD_CFAX">
<connects>
<connect gate="LCD" pin="CS1B" pad="P$3"/>
<connect gate="LCD" pin="CS2" pad="P$4"/>
<connect gate="LCD" pin="D0" pad="P$9"/>
<connect gate="LCD" pin="D1" pad="P$10"/>
<connect gate="LCD" pin="D2" pad="P$11"/>
<connect gate="LCD" pin="D3" pad="P$12"/>
<connect gate="LCD" pin="D4" pad="P$13"/>
<connect gate="LCD" pin="D5" pad="P$14"/>
<connect gate="LCD" pin="D6" pad="P$15"/>
<connect gate="LCD" pin="D7" pad="P$16"/>
<connect gate="LCD" pin="ERD" pad="P$8"/>
<connect gate="LCD" pin="GND" pad="P$2"/>
<connect gate="LCD" pin="MI" pad="P$17"/>
<connect gate="LCD" pin="P/S" pad="P$18"/>
<connect gate="LCD" pin="RESET" pad="P$5"/>
<connect gate="LCD" pin="RS" pad="P$6"/>
<connect gate="LCD" pin="RW" pad="P$7"/>
<connect gate="LCD" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1555" prefix="U">
<description>&lt;b&gt;MAX1555 Lithium Charger IC&lt;/b&gt;
SOT-23 Lithium Polymer charging IC. Schematic element and footprint proven. Spark Fun Electronics SKU : COM-00674</description>
<gates>
<gate name="G$1" symbol="MAX1555"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BATT" pad="5"/>
<connect gate="G$1" pin="CHG" pad="3"/>
<connect gate="G$1" pin="DC" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="USB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD_BACKLIGHT_PADS">
<gates>
<gate name="G$1" symbol="LCD_BACKLIGHT_PADS"/>
</gates>
<devices>
<device name="" package="LCD_BACKLIGHT_PADS">
<connects>
<connect gate="G$1" pin="A" pad="P$1"/>
<connect gate="G$1" pin="K" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PAD">
<gates>
<gate name="G$1" symbol="PAD"/>
</gates>
<devices>
<device name=".02" package="PAD.02X.02">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".03" package="PAD.03X.03">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP130" prefix="U">
<gates>
<gate name="G$1" symbol="MCP130"/>
</gates>
<devices>
<device name="SOT" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAMERA_CMOS_CON">
<description>&lt;b&gt;640x480 CMOS Color Camera&lt;/b&gt;
Footprint proven. Spark Fun Electronics Camera SKU : SEN-00637, Mating Connector SKU : SEN-00638</description>
<gates>
<gate name="G$1" symbol="CAMERA_CMOS_CON"/>
</gates>
<devices>
<device name="SMD" package="CAMERA_CMOS_CON">
<connects>
<connect gate="G$1" pin="ENB" pad="ENB"/>
<connect gate="G$1" pin="FVL" pad="FVLD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="LVL" pad="LVLD"/>
<connect gate="G$1" pin="MCK" pad="MCLK"/>
<connect gate="G$1" pin="PCK" pad="PCLK"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC@1" pad="VCC@1"/>
<connect gate="G$1" pin="Y0" pad="Y0"/>
<connect gate="G$1" pin="Y1" pad="Y1"/>
<connect gate="G$1" pin="Y2" pad="Y2"/>
<connect gate="G$1" pin="Y3" pad="Y3"/>
<connect gate="G$1" pin="Y4" pad="Y4"/>
<connect gate="G$1" pin="Y5" pad="Y5"/>
<connect gate="G$1" pin="Y6" pad="Y6"/>
<connect gate="G$1" pin="Y7" pad="Y7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PLUG" package="CAMERA_CMOS_PLUG">
<connects>
<connect gate="G$1" pin="ENB" pad="11"/>
<connect gate="G$1" pin="FVL" pad="17"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="LVL" pad="18"/>
<connect gate="G$1" pin="MCK" pad="20"/>
<connect gate="G$1" pin="PCK" pad="19"/>
<connect gate="G$1" pin="RST" pad="12"/>
<connect gate="G$1" pin="SCL" pad="15"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC@1" pad="14"/>
<connect gate="G$1" pin="Y0" pad="1"/>
<connect gate="G$1" pin="Y1" pad="2"/>
<connect gate="G$1" pin="Y2" pad="3"/>
<connect gate="G$1" pin="Y3" pad="4"/>
<connect gate="G$1" pin="Y4" pad="5"/>
<connect gate="G$1" pin="Y5" pad="6"/>
<connect gate="G$1" pin="Y6" pad="7"/>
<connect gate="G$1" pin="Y7" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WLANMODULE">
<description>&lt;b&gt;DPAC WiFi Module&lt;/b&gt;
Footprint for DPAC wireless module. Not fully tested so double check it. Spark Fun Electronics SKU : (Module) WRL-00665, (Connector) WRL-00673</description>
<gates>
<gate name="G$1" symbol="WLANMODULE"/>
</gates>
<devices>
<device name="" package="WLANMODULE">
<connects>
<connect gate="G$1" pin="/RF_LED" pad="P35"/>
<connect gate="G$1" pin="/RST" pad="P7"/>
<connect gate="G$1" pin="/TSS" pad="P8"/>
<connect gate="G$1" pin="DVDD@0" pad="P3"/>
<connect gate="G$1" pin="DVDD@1" pad="P33"/>
<connect gate="G$1" pin="DVDD@2" pad="P4"/>
<connect gate="G$1" pin="DVDD@3" pad="P34"/>
<connect gate="G$1" pin="E4" pad="P32"/>
<connect gate="G$1" pin="E5" pad="P30"/>
<connect gate="G$1" pin="E6" pad="P29"/>
<connect gate="G$1" pin="E7" pad="P31"/>
<connect gate="G$1" pin="F0" pad="P25"/>
<connect gate="G$1" pin="F1" pad="P28"/>
<connect gate="G$1" pin="F2" pad="P27"/>
<connect gate="G$1" pin="F3" pad="P26"/>
<connect gate="G$1" pin="F4" pad="P18"/>
<connect gate="G$1" pin="F5" pad="P12"/>
<connect gate="G$1" pin="F6" pad="P23"/>
<connect gate="G$1" pin="F7" pad="P24"/>
<connect gate="G$1" pin="G0" pad="P22"/>
<connect gate="G$1" pin="G1" pad="P19"/>
<connect gate="G$1" pin="G2" pad="P17"/>
<connect gate="G$1" pin="G3" pad="P11"/>
<connect gate="G$1" pin="G4" pad="P14"/>
<connect gate="G$1" pin="G5" pad="P13"/>
<connect gate="G$1" pin="G6" pad="P9"/>
<connect gate="G$1" pin="G7" pad="P21"/>
<connect gate="G$1" pin="RFU" pad="P6"/>
<connect gate="G$1" pin="TSCK" pad="P20"/>
<connect gate="G$1" pin="TSI" pad="P2"/>
<connect gate="G$1" pin="TSO" pad="P10"/>
<connect gate="G$1" pin="V2.5" pad="P5"/>
<connect gate="G$1" pin="VSS@0" pad="P1"/>
<connect gate="G$1" pin="VSS@1" pad="P15"/>
<connect gate="G$1" pin="VSS@2" pad="P16"/>
<connect gate="G$1" pin="VSS@3" pad="P36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC1052L">
<description>&lt;b&gt;HMC1052L&lt;/b&gt;
Dual axis magnetic sensor. Used for compass and magnetometer applications. Schematic and footprint are not tested and probably need fixing. Spark Fun Electronics SKU : COM-00708</description>
<gates>
<gate name="G$1" symbol="HMC1052L"/>
</gates>
<devices>
<device name="" package="16LPCC">
<connects>
<connect gate="G$1" pin="GND1A" pad="13"/>
<connect gate="G$1" pin="GND1B" pad="15"/>
<connect gate="G$1" pin="GND2A" pad="1"/>
<connect gate="G$1" pin="GND2B" pad="7"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="NC2" pad="9"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="OFF+" pad="2"/>
<connect gate="G$1" pin="OFF-" pad="6"/>
<connect gate="G$1" pin="OUT+A" pad="3"/>
<connect gate="G$1" pin="OUT+B" pad="16"/>
<connect gate="G$1" pin="OUT-A" pad="14"/>
<connect gate="G$1" pin="OUT-B" pad="10"/>
<connect gate="G$1" pin="S/R+" pad="8"/>
<connect gate="G$1" pin="S/R-" pad="11"/>
<connect gate="G$1" pin="VB" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AYZ0202">
<description>&lt;b&gt;SPDT Slide Switch&lt;/b&gt;
Simple SMD single-pull double-throw slide switch. Good for  less than 350mA power switch, switching UARTs between devices, etc. Spark Fun Electronics SKU : COM-00597</description>
<gates>
<gate name="G$1" symbol="AYZ0202"/>
</gates>
<devices>
<device name="" package="AYZ0202">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-SFE" prefix="JP">
<description>&lt;b&gt;Spark Fun Electronics PCB Logo&lt;/b&gt;
This is the standard Spark Fun Electronics PCB logo.</description>
<gates>
<gate name="G$1" symbol="LOGO1"/>
</gates>
<devices>
<device name="M" package="SFE-LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEW" package="SFE-NEW-WEBLOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP" package="SFE-LOGO-FLAME-COPPER">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SK" package="SFE-LOGO-FLAME">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NW2" package="SFE-NEW-WEB">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM" package="SFE-NEW-WEB-SOLDERMASK">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EBM001">
<gates>
<gate name="G$1" symbol="EMB001"/>
</gates>
<devices>
<device name="" package="EMB001">
<connects>
<connect gate="G$1" pin="1V8" pad="23"/>
<connect gate="G$1" pin="AIO0" pad="34"/>
<connect gate="G$1" pin="AIO1" pad="33"/>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="CTS" pad="27"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="19"/>
<connect gate="G$1" pin="GND@2" pad="20"/>
<connect gate="G$1" pin="GND@3" pad="21"/>
<connect gate="G$1" pin="GND@4" pad="35"/>
<connect gate="G$1" pin="GND@5" pad="36"/>
<connect gate="G$1" pin="GND@6" pad="37"/>
<connect gate="G$1" pin="GND@7" pad="38"/>
<connect gate="G$1" pin="GND@8" pad="39"/>
<connect gate="G$1" pin="GND@9" pad="42"/>
<connect gate="G$1" pin="MISO" pad="31"/>
<connect gate="G$1" pin="MOSI" pad="28"/>
<connect gate="G$1" pin="PCM_CLK" pad="15"/>
<connect gate="G$1" pin="PCM_IN" pad="16"/>
<connect gate="G$1" pin="PCM_OUT" pad="18"/>
<connect gate="G$1" pin="PCM_SYNC" pad="17"/>
<connect gate="G$1" pin="PIO0" pad="41"/>
<connect gate="G$1" pin="PIO1" pad="40"/>
<connect gate="G$1" pin="PIO10" pad="11"/>
<connect gate="G$1" pin="PIO11" pad="12"/>
<connect gate="G$1" pin="PIO2" pad="3"/>
<connect gate="G$1" pin="PIO3" pad="4"/>
<connect gate="G$1" pin="PIO4" pad="5"/>
<connect gate="G$1" pin="PIO5" pad="6"/>
<connect gate="G$1" pin="PIO6" pad="7"/>
<connect gate="G$1" pin="PIO7" pad="8"/>
<connect gate="G$1" pin="PIO8" pad="9"/>
<connect gate="G$1" pin="PIO9" pad="10"/>
<connect gate="G$1" pin="RST" pad="32"/>
<connect gate="G$1" pin="RTS" pad="25"/>
<connect gate="G$1" pin="RX" pad="24"/>
<connect gate="G$1" pin="SPI_CLK" pad="29"/>
<connect gate="G$1" pin="SPI_CSB" pad="30"/>
<connect gate="G$1" pin="TX" pad="26"/>
<connect gate="G$1" pin="USB_DN" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="14"/>
<connect gate="G$1" pin="VSUP" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA_EDGE" prefix="J$">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;
End launch SMA connector. The paste layer has been removed so that the connector can be hand soldered onto the board after reflow.</description>
<gates>
<gate name="1" symbol="SMA_EDGE"/>
</gates>
<devices>
<device name="" package="SMA-EDGE">
<connects>
<connect gate="1" pin="GND@0" pad="GND@0"/>
<connect gate="1" pin="GND@1" pad="GND@1"/>
<connect gate="1" pin="GND@2" pad="GND@2"/>
<connect gate="1" pin="GND@3" pad="GND@3"/>
<connect gate="1" pin="SIGNAL" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3.3V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="3.3V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT245RL">
<description>&lt;b&gt;USB FIFO Controller&lt;/b&gt;
4&lt;sup&gt;th&lt;/sup&gt; Generation USB Controller (USB &amp;lt;-&amp;gt; Parallel) - FIFO. Spark Fun Electronics SKU : COM-00787</description>
<gates>
<gate name="G$1" symbol="FT245R"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="D0" pad="1"/>
<connect gate="G$1" pin="D1" pad="5"/>
<connect gate="G$1" pin="D2" pad="3"/>
<connect gate="G$1" pin="D3" pad="11"/>
<connect gate="G$1" pin="D4" pad="2"/>
<connect gate="G$1" pin="D5" pad="9"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="6"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWEN" pad="12"/>
<connect gate="G$1" pin="RD" pad="13"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="RXF" pad="23"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXE" pad="22"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
<connect gate="G$1" pin="WR" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 3&lt;/b&gt;
Standard 3-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08232 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X03_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X03_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X3_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-3_LOCK.007S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X03_NO_SILK" package="1X03_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X03_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH" package="JST-3-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X03_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SCREW-5MM" package="SCREWTERMINAL-5MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X03_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="JST-3-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X03-1MM-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 4&lt;/b&gt;
Standard 4-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208</description>
<gates>
<gate name="G$1" symbol="M04"/>
</gates>
<devices>
<device name="PTH" package="1X04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X04-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X04_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X04_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X4_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X04-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X04_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X04_NO_SILK" package="1X04_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH" package="JST-4-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-4_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="1X04-1MM-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M05" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 5&lt;/b&gt;
Standard 5-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08230 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M05"/>
</gates>
<devices>
<device name="PTH" package="1X05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X05-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X05_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X05_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LONGPADS" package="1X05_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X05-1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="1X05-1MM-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M07" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 7&lt;/b&gt;
Standard 7-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).  NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS... This footprint was designed to help hold the alignment of a through-hole component (i.e. 7-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is usually a perfectly straight line). This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes. Because they are alternating, it causes a "brace" to hold the header in place. 0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice. Also, if you push a header all the way into place, it is covered up entirely on the bottom side. This idea of altering the position of holes to aid alignment will be further integrated into the Sparkfun Library for other footprints. It can help hold any component with 3 or more connection pins.</description>
<gates>
<gate name="G$1" symbol="M07"/>
</gates>
<devices>
<device name="" package="1X07">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X07_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X07_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X07_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPINS_HOLES_ONLY" package="1X07_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COPERNICUS" prefix="IC">
<description>&lt;b&gt;Copernicus&lt;/b&gt;
Massively edited and tweaked footprint to meet the Trimble recommended layout and paste layer. Footprint production proven. Spark Fun Electronics SKU : GPS-07951</description>
<gates>
<gate name="G$2" symbol="COPERNICUS"/>
</gates>
<devices>
<device name="SMD" package="COPERNICUS">
<connects>
<connect gate="G$2" pin="BOOT" pad="10"/>
<connect gate="G$2" pin="GND@1" pad="1"/>
<connect gate="G$2" pin="GND@2" pad="2"/>
<connect gate="G$2" pin="GND@3" pad="4"/>
<connect gate="G$2" pin="GND@4" pad="13"/>
<connect gate="G$2" pin="GND@5" pad="14"/>
<connect gate="G$2" pin="GND@6" pad="15"/>
<connect gate="G$2" pin="GND@7" pad="27"/>
<connect gate="G$2" pin="GND@8" pad="28"/>
<connect gate="G$2" pin="LNA" pad="5"/>
<connect gate="G$2" pin="OPEN" pad="7"/>
<connect gate="G$2" pin="PPS" pad="19"/>
<connect gate="G$2" pin="RESERVED1" pad="6"/>
<connect gate="G$2" pin="RESERVED2" pad="9"/>
<connect gate="G$2" pin="RESERVED3" pad="17"/>
<connect gate="G$2" pin="RESERVED4" pad="18"/>
<connect gate="G$2" pin="RESERVED5" pad="22"/>
<connect gate="G$2" pin="RESERVED6" pad="25"/>
<connect gate="G$2" pin="RESERVED7" pad="26"/>
<connect gate="G$2" pin="RFIN" pad="3"/>
<connect gate="G$2" pin="RXD-A" pad="21"/>
<connect gate="G$2" pin="RXD-B" pad="20"/>
<connect gate="G$2" pin="SHORT" pad="8"/>
<connect gate="G$2" pin="TXD-A" pad="23"/>
<connect gate="G$2" pin="TXD-B" pad="24"/>
<connect gate="G$2" pin="VCC" pad="12"/>
<connect gate="G$2" pin="XRESET" pad="11"/>
<connect gate="G$2" pin="XSTANDBY" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M14" prefix="JP">
<description>&lt;b&gt;Header 14&lt;/b&gt;
Standard 14-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M14"/>
</gates>
<devices>
<device name="" package="1X14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X14_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X14_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X14-LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-2-OLD" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Jumper&lt;/b&gt;
Basic 0.1" spaced jumper. Use with breakaway headers.</description>
<gates>
<gate name="A" symbol="JUMPER-2"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NC" package="SJ_2S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="1X02_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO" package="SJ_2S-NO">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER-OLD" prefix="SJ">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
Standard SMD solder jumper. Used to automate production. Two varients : Normally Open and Normally Closed are the same, but have different paste layers. NC will have a large amount of paste and should jumper during reflow.</description>
<gates>
<gate name="1" symbol="SJ"/>
</gates>
<devices>
<device name="NC" package="SJ_2S">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE" package="SJ_2S-TRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NC2" package="SJ_2S-NOTRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO" package="SJ_2S-NO">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_2WAY-OLD" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
2 way solder jumper</description>
<gates>
<gate name="G$1" symbol="SJ_2"/>
</gates>
<devices>
<device name="W" package="SJ_2W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SJ_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE2&amp;3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER_JACK" prefix="J">
<description>&lt;b&gt;Power Jack&lt;/b&gt;
This is the standard 5.5mm barrel jack for power. The PTH is the most common, proven, reliable, footprint. All others are experimental. The Slot footprint only works if the mill layer is transmitted to the PCB fab house so be warned. Spark Fun Electronics SKU : PRT-00119. Mating wall wart : TOL-00298 (and others)</description>
<gates>
<gate name="G$1" symbol="POWERJACK"/>
</gates>
<devices>
<device name="SMD" package="POWER_JACK_SMD">
<connects>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="VIN0"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SLT" package="POWER_JACK_SLOT">
<connects>
<connect gate="G$1" pin="GND" pad="GND@2"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND@1"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="POWER_JACK_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="COMBO" package="POWER_JACK_COMBO">
<connects>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="POWER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RCA" package="RCA">
<connects>
<connect gate="G$1" pin="GND" pad="BARREL"/>
<connect gate="G$1" pin="GNDBREAK" pad="SPRING"/>
<connect gate="G$1" pin="PWR" pad="BREAK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="POWER_JACK_PTH_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RCA_LOCK" package="RCA_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="BARREL"/>
<connect gate="G$1" pin="GNDBREAK" pad="SPRING"/>
<connect gate="G$1" pin="PWR" pad="BREAK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCP1000_D01" prefix="U">
<description>&lt;b&gt;SCP1000&lt;/b&gt;
Barometric pressure sensor. Schematic elements and footprint production proven. Spark Fun Electronics SKU : COM-08128</description>
<gates>
<gate name="G$1" symbol="SCP1000_D01"/>
</gates>
<devices>
<device name="SMD" package="SCP1000">
<connects>
<connect gate="G$1" pin="ATST" pad="ATST"/>
<connect gate="G$1" pin="AVDD" pad="AVDD"/>
<connect gate="G$1" pin="AVSS" pad="AVSS"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CSB" pad="CSB"/>
<connect gate="G$1" pin="DRDY" pad="DRDY"/>
<connect gate="G$1" pin="DVDD" pad="DVDD"/>
<connect gate="G$1" pin="DVDDS" pad="DVDDS"/>
<connect gate="G$1" pin="DVSS" pad="DVSS"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI/SDA"/>
<connect gate="G$1" pin="PD" pad="PD"/>
<connect gate="G$1" pin="SCK" pad="SCK/SCL"/>
<connect gate="G$1" pin="TRIG" pad="TRIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="SCP1000-LG">
<connects>
<connect gate="G$1" pin="ATST" pad="ATST"/>
<connect gate="G$1" pin="AVDD" pad="AVDD"/>
<connect gate="G$1" pin="AVSS" pad="AVSS"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CSB" pad="CSB"/>
<connect gate="G$1" pin="DRDY" pad="DRDY"/>
<connect gate="G$1" pin="DVDD" pad="DVDD"/>
<connect gate="G$1" pin="DVDDS" pad="DVDDS"/>
<connect gate="G$1" pin="DVSS" pad="DVSS"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI/SDA"/>
<connect gate="G$1" pin="PD" pad="PD"/>
<connect gate="G$1" pin="SCK" pad="SCK/SCL"/>
<connect gate="G$1" pin="TRIG" pad="TRIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F88-SSOP" prefix="IC">
<description>&lt;b&gt;PIC 16F8x&lt;/b&gt;
8-Bit PIC16F8X Family

&lt;p&gt;Pin Compatible : PIC16F83, PIC16CR83, PIC16F84A, PIC16CR84</description>
<gates>
<gate name="G$1" symbol="PIC16F88-SSOP"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="1"/>
<connect gate="G$1" pin="RA3/AN3" pad="2"/>
<connect gate="G$1" pin="RA4/AN4" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2" pad="17"/>
<connect gate="G$1" pin="RA7/OSC1" pad="18"/>
<connect gate="G$1" pin="RB0/INT" pad="7"/>
<connect gate="G$1" pin="RB1/SDA" pad="8"/>
<connect gate="G$1" pin="RB2/RX" pad="9"/>
<connect gate="G$1" pin="RB3" pad="10"/>
<connect gate="G$1" pin="RB4/SCL" pad="11"/>
<connect gate="G$1" pin="RB5/TX" pad="12"/>
<connect gate="G$1" pin="RB6/PGC" pad="13"/>
<connect gate="G$1" pin="RB7/PGD" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F688">
<description>&lt;b&gt;PIC 16F688&lt;/b&gt;
8-Bit PIC16F88</description>
<gates>
<gate name="G$1" symbol="PIC16F688"/>
</gates>
<devices>
<device name="SMD" package="SOIC-14">
<connects>
<connect gate="G$1" pin="RA0/PGD" pad="13"/>
<connect gate="G$1" pin="RA1/PGC" pad="12"/>
<connect gate="G$1" pin="RA2/AN2" pad="11"/>
<connect gate="G$1" pin="RA3/MCLR" pad="4"/>
<connect gate="G$1" pin="RA4/OSC2" pad="3"/>
<connect gate="G$1" pin="RA5/OSC1" pad="2"/>
<connect gate="G$1" pin="RC0/AN4" pad="10"/>
<connect gate="G$1" pin="RC1/AN5" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4/TX" pad="6"/>
<connect gate="G$1" pin="RC5/RX" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_NCP1400" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Switching step-up voltage regulator&lt;/b&gt;
NCP1400 switiching regulator takes single cell AA and outputs 100mA at 3.3V or 5V with minimal number of external components.</description>
<gates>
<gate name="G$1" symbol="NCP1400"/>
</gates>
<devices>
<device name="SOT23-5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY" prefix="BAT" uservalue="yes">
<description>&lt;b&gt;Battery Holders&lt;/b&gt;
Various common sizes : AA, AAA, 20mm coin cell and 12mm coin cell.</description>
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="AAA" package="BATTERY-AAA">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20PTH2" package="BATTERY">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AA" package="BATTERY-AA">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="12PTH" package="BATTCON_12MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="VCC@1"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20SMD" package="BATTCON_20MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="245MM" package="BATTCON_245MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20PTH" package="BATTCOM_20MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="245PTH" package="BATTCON_245MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1100" package="LIPO-1100MAH">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AA-PANEL" package="BATTERY-AA-PANEL">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FOB" package="BATTERY_20MM_PTH_COMPACT">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="12MM" package="BATTCON_12MM">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20MM_4LEGS" package="BATTCON_20MM_4LEGS">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AA-KIT" package="BATTERY-AA-KIT">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-2X2">
<description>&lt;b&gt;5mm Button Pad&lt;/b&gt;
Proven layout and schematic for 2x2 button pad. Panelize this device/fp to a 4x4 pad if needed. Spark Fun Electronics SKU : COM-07835. Compatible common cathode tri-color LED SKU : COM-00105</description>
<gates>
<gate name="-C1" symbol="BUTTONPAD_SINGLE"/>
<gate name="-C2" symbol="BUTTONPAD_SINGLE"/>
<gate name="-C3" symbol="BUTTONPAD_SINGLE"/>
<gate name="-C4" symbol="BUTTONPAD_SINGLE"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-2X2">
<connects>
<connect gate="-C1" pin="BLU" pad="BLU1"/>
<connect gate="-C1" pin="GND" pad="GND1"/>
<connect gate="-C1" pin="GRN" pad="GRN1"/>
<connect gate="-C1" pin="RED" pad="RED1"/>
<connect gate="-C1" pin="SIG1" pad="SIG1"/>
<connect gate="-C1" pin="SIG2" pad="SIG2"/>
<connect gate="-C2" pin="BLU" pad="BLU2"/>
<connect gate="-C2" pin="GND" pad="GND2"/>
<connect gate="-C2" pin="GRN" pad="GRN2"/>
<connect gate="-C2" pin="RED" pad="RED2"/>
<connect gate="-C2" pin="SIG1" pad="SIG3"/>
<connect gate="-C2" pin="SIG2" pad="SIG4"/>
<connect gate="-C3" pin="BLU" pad="BLU3"/>
<connect gate="-C3" pin="GND" pad="GND3"/>
<connect gate="-C3" pin="GRN" pad="GRN3"/>
<connect gate="-C3" pin="RED" pad="RED3"/>
<connect gate="-C3" pin="SIG1" pad="SIG5"/>
<connect gate="-C3" pin="SIG2" pad="SIG6"/>
<connect gate="-C4" pin="BLU" pad="BLU4"/>
<connect gate="-C4" pin="GND" pad="GND4"/>
<connect gate="-C4" pin="GRN" pad="GRN4"/>
<connect gate="-C4" pin="RED" pad="RED4"/>
<connect gate="-C4" pin="SIG1" pad="SIG7"/>
<connect gate="-C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SPECIAL" package="BUTTONPAD-2X2-SPECIAL">
<connects>
<connect gate="-C1" pin="BLU" pad="BLU1"/>
<connect gate="-C1" pin="GND" pad="GND1"/>
<connect gate="-C1" pin="GRN" pad="GRN1"/>
<connect gate="-C1" pin="RED" pad="RED1"/>
<connect gate="-C1" pin="SIG1" pad="SIG1"/>
<connect gate="-C1" pin="SIG2" pad="SIG2"/>
<connect gate="-C2" pin="BLU" pad="BLU2"/>
<connect gate="-C2" pin="GND" pad="GND2"/>
<connect gate="-C2" pin="GRN" pad="GRN2"/>
<connect gate="-C2" pin="RED" pad="RED2"/>
<connect gate="-C2" pin="SIG1" pad="SIG3"/>
<connect gate="-C2" pin="SIG2" pad="SIG4"/>
<connect gate="-C3" pin="BLU" pad="BLU3"/>
<connect gate="-C3" pin="GND" pad="GND3"/>
<connect gate="-C3" pin="GRN" pad="GRN3"/>
<connect gate="-C3" pin="RED" pad="RED3"/>
<connect gate="-C3" pin="SIG1" pad="SIG5"/>
<connect gate="-C3" pin="SIG2" pad="SIG6"/>
<connect gate="-C4" pin="BLU" pad="BLU4"/>
<connect gate="-C4" pin="GND" pad="GND4"/>
<connect gate="-C4" pin="GRN" pad="GRN4"/>
<connect gate="-C4" pin="RED" pad="RED4"/>
<connect gate="-C4" pin="SIG1" pad="SIG7"/>
<connect gate="-C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC-ICSP-MINI">
<description>&lt;b&gt;PIC-ICSP-Mini&lt;/b&gt;
Miniature 5-pin connection for temporary programming of PICs. Use this device in your design to save space. Program the PIC with this adapter Spark Fun Electronics SKU : BOB-00194</description>
<gates>
<gate name="G$1" symbol="PIC-ISCP-MINI"/>
</gates>
<devices>
<device name="" package="PIC-ICSP-MINI">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PGC" pad="5"/>
<connect gate="G$1" pin="PGD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M10" prefix="JP">
<description>&lt;b&gt;Header 10&lt;/b&gt;
Standard 10-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M10"/>
</gates>
<devices>
<device name="&quot;" package="1X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="1X10-2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MMSMD" package="1X10-2MM-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X10_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X10_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULN2803" prefix="ULN2803" uservalue="yes">
<description>&lt;b&gt;Darlington Driver&lt;/b&gt;
ULN2803 Darlington array. 500mA max per channel, 8-channel package. Spark Fun Electronics SKU : COM-00312</description>
<gates>
<gate name="G$1" symbol="ULN2803"/>
</gates>
<devices>
<device name="DIP" package="DIL18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SO018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOICW" package="SO18L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC6352">
<description>&lt;b&gt;HMC6352&lt;/b&gt;
This is the compass module from Honeywell. Works very well. Schematic and footprint are production proven. Spark Fun Electronics SKU : COM-07892</description>
<gates>
<gate name="G$1" symbol="HMC6352"/>
</gates>
<devices>
<device name="" package="LCC24">
<connects>
<connect gate="G$1" pin="CA1" pad="23"/>
<connect gate="G$1" pin="CA2" pad="22"/>
<connect gate="G$1" pin="CB1" pad="20"/>
<connect gate="G$1" pin="CB2" pad="19"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME-LETTER" prefix="FRAME">
<description>&lt;b&gt;Schematic Frame&lt;/b&gt;&lt;p&gt;
Standard 8.5x11 US Letter frame</description>
<gates>
<gate name="G$1" symbol="LETTER_L"/>
<gate name="G$2" symbol="DOCFIELD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_317" prefix="U">
<description>&lt;b&gt;Voltage Regulator&lt;/b&gt;
Standard LM317 adjustable voltage regulator. AOI (Adjust Output Input). Google 'LM317 Calculator' for easy to use app to get the two resistor values needed. 240/720 for 5V output. 240/390 for 3.3V output. Spark Fun Electronics SKU : COM-00527</description>
<gates>
<gate name="G$1" symbol="78ADJ-2"/>
</gates>
<devices>
<device name="SINK" package="TO220-ADJ">
<connects>
<connect gate="G$1" pin="ADJ" pad="ADJ"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DPACK" package="V-REG_DPACK">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M01" prefix="JP">
<description>&lt;b&gt;Header 1&lt;/b&gt;
Standard 1-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M01"/>
</gates>
<devices>
<device name="PTH_LONGPAD" package="1X01_LONGPAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="LUXEON-PAD">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMTSO-256-ET" package="SMTSO-256-ET">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMTRA-256-8-6" package="SMTRA-256-8-6">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMDNS" package="1X01NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_2MM" package="1X01_2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OFFSET" package="1X01_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-4.5X1.5" package="PAD-1.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLE_LARGE" package="1X01_POGOPIN_HOLE_LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLE_0.58" package="1X01_POGOPIN_HOLE_0.58">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SNAP-FEMALE" package="SNAP-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SNAP-MALE" package="SNAP-MALE">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M11" prefix="JP">
<description>&lt;b&gt;Header 11&lt;/b&gt;
Standard 11-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M11"/>
</gates>
<devices>
<device name="PTH" package="1X11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X11-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X11_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X11_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X11_SMD_PTHCOMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X11_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_NO_HOLES" package="1X11_SMD_NO_HOLES">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X11_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M12" prefix="JP">
<description>&lt;b&gt;Header 12&lt;/b&gt;
Standard 12-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M12"/>
</gates>
<devices>
<device name="PTH" package="1X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X12_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X12_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MACHINE-PIN_LOCK" package="1X12_MACHINE-PIN-HEADER_LOCK.004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X12_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X12_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COPERNICUS-DIP">
<gates>
<gate name="G$1" symbol="COPERNICUS-DIP"/>
</gates>
<devices>
<device name="PTH" package="COPERNICUS-DIP">
<connects>
<connect gate="G$1" pin="BOOT" pad="6"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="LNA" pad="1"/>
<connect gate="G$1" pin="OPEN" pad="3"/>
<connect gate="G$1" pin="PPS" pad="13"/>
<connect gate="G$1" pin="RESERVED1" pad="2"/>
<connect gate="G$1" pin="RESERVED2" pad="5"/>
<connect gate="G$1" pin="RESERVED3" pad="11"/>
<connect gate="G$1" pin="RESERVED4" pad="12"/>
<connect gate="G$1" pin="RESERVED5" pad="16"/>
<connect gate="G$1" pin="RESERVED6" pad="19"/>
<connect gate="G$1" pin="RESERVED7" pad="20"/>
<connect gate="G$1" pin="RXD-A" pad="15"/>
<connect gate="G$1" pin="RXD-B" pad="14"/>
<connect gate="G$1" pin="SHORT" pad="4"/>
<connect gate="G$1" pin="TXD-A" pad="17"/>
<connect gate="G$1" pin="TXD-B" pad="18"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="XRESET" pad="7"/>
<connect gate="G$1" pin="XSTANDBY" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1528">
<description>&lt;b&gt;LT1528&lt;/b&gt;
High current voltage regulator commonly used with GM862 cellular module. Spark Fun Electronics SKU : COM-00311. Footprint may need to have the large paste aperature reduced.</description>
<gates>
<gate name="G$1" symbol="LT1528"/>
</gates>
<devices>
<device name="" package="Q5-DD">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DOSONCHIP-IC">
<description>&lt;b&gt;DOSonCHIP IC&lt;/b&gt;
This is the tested schematic and footprint for the DOSonCHIP FAT16 FAT32 IC. Spark Fun Electronics SKU : COM-07956. QFN package also tested/proven.</description>
<gates>
<gate name="G$1" symbol="DOSONCHIP-IC"/>
</gates>
<devices>
<device name="LQFP" package="LQFP-32">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="13"/>
<connect gate="G$1" pin="CARD_CS" pad="18"/>
<connect gate="G$1" pin="CARD_DIN" pad="15"/>
<connect gate="G$1" pin="CARD_DOUT" pad="17"/>
<connect gate="G$1" pin="CARD_SCLK" pad="16"/>
<connect gate="G$1" pin="CARD_WP" pad="14"/>
<connect gate="G$1" pin="DIR" pad="22"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="25"/>
<connect gate="G$1" pin="I2C_SDA" pad="26"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="21"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="27"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="28"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="23"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="24"/>
<connect gate="G$1" pin="UART_RX" pad="29"/>
<connect gate="G$1" pin="UART_TX" pad="30"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="32"/>
<connect gate="G$1" pin="XTAL_OUT" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN" package="QFN-24">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="7"/>
<connect gate="G$1" pin="CARD_CS" pad="12"/>
<connect gate="G$1" pin="CARD_DIN" pad="9"/>
<connect gate="G$1" pin="CARD_DOUT" pad="11"/>
<connect gate="G$1" pin="CARD_SCLK" pad="10"/>
<connect gate="G$1" pin="CARD_WP" pad="8"/>
<connect gate="G$1" pin="DIR" pad="14"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="17"/>
<connect gate="G$1" pin="I2C_SDA" pad="18"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="13"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="19"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="20"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="15"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="16"/>
<connect gate="G$1" pin="UART_RX" pad="21"/>
<connect gate="G$1" pin="UART_TX" pad="22"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="24"/>
<connect gate="G$1" pin="XTAL_OUT" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN_ALT1" package="QFN-24_ALT1.PAC">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="7"/>
<connect gate="G$1" pin="CARD_CS" pad="12"/>
<connect gate="G$1" pin="CARD_DIN" pad="9"/>
<connect gate="G$1" pin="CARD_DOUT" pad="11"/>
<connect gate="G$1" pin="CARD_SCLK" pad="10"/>
<connect gate="G$1" pin="CARD_WP" pad="8"/>
<connect gate="G$1" pin="DIR" pad="14"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="17"/>
<connect gate="G$1" pin="I2C_SDA" pad="18"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="13"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="19"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="20"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="15"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="16"/>
<connect gate="G$1" pin="UART_RX" pad="21"/>
<connect gate="G$1" pin="UART_TX" pad="22"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="24"/>
<connect gate="G$1" pin="XTAL_OUT" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M09" prefix="JP">
<description>&lt;b&gt;Header 9&lt;/b&gt;
Standard 9-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M09"/>
</gates>
<devices>
<device name="" package="1X09">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X09_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK-LONGPADS" package="1X09_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X09_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XN04312">
<description>&lt;b&gt;NPN/PNP Transistor Array&lt;/b&gt;
Handy dandy transistor array for level shifting and inverting signals. Spark Fun Electronics SKU : COM-00588</description>
<gates>
<gate name="G$1" symbol="XN04312"/>
</gates>
<devices>
<device name="SOT" package="SOT23-6">
<connects>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="2"/>
<connect gate="G$1" pin="C1" pad="1"/>
<connect gate="G$1" pin="C2" pad="4"/>
<connect gate="G$1" pin="E1" pad="6"/>
<connect gate="G$1" pin="E2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR" prefix="Y">
<description>&lt;b&gt;Resonator&lt;/b&gt;
Small SMD resonator. This is the itty bitty 10/20MHz resonators with built in caps. CSTCE10M0G55 and CSTCE20M0V53. Footprint has been reviewed closely but hasn't been tested yet.</description>
<gates>
<gate name="G$1" symbol="RESONATOR"/>
</gates>
<devices>
<device name="SMD" package="RESONATOR-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="RESONATOR-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LDO" prefix="U">
<description>&lt;b&gt;Voltage Regulator LDO&lt;/b&gt;
Standard 150mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5205. BP (by-pass) pin is used to lower output noise with 470pF cap.</description>
<gates>
<gate name="G$1" symbol="V-REG-LDO"/>
</gates>
<devices>
<device name="SMD" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="SC70">
<connects>
<connect gate="G$1" pin="BP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL330">
<description>&lt;b&gt;Triple Axis Accelerometer&lt;/b&gt;
Analog Devices ADXL330 +/-3g 2.4V-5.25V Analog output. Spark Fun Electronics SKU : COM-00730. Center pad paste layer has been reduced to avoid shorting.</description>
<gates>
<gate name="G$1" symbol="ADXL330"/>
</gates>
<devices>
<device name="SMD" package="LFCSP-16">
<connects>
<connect gate="G$1" pin="COM" pad="3"/>
<connect gate="G$1" pin="COM@1" pad="5"/>
<connect gate="G$1" pin="COM@2" pad="6"/>
<connect gate="G$1" pin="COM@3" pad="7"/>
<connect gate="G$1" pin="ST" pad="2"/>
<connect gate="G$1" pin="VS" pad="14"/>
<connect gate="G$1" pin="VS@1" pad="15"/>
<connect gate="G$1" pin="XOUT" pad="12"/>
<connect gate="G$1" pin="YOUT" pad="10"/>
<connect gate="G$1" pin="ZOUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSCHIPTC5747">
<gates>
<gate name="G$1" symbol="CAMERA_SFV24R-2ST"/>
</gates>
<devices>
<device name="" package="CAMERA_SFV24R-2ST_2">
<connects>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="AVDD28" pad="3"/>
<connect gate="G$1" pin="CLK_IN" pad="5"/>
<connect gate="G$1" pin="DGND" pad="6"/>
<connect gate="G$1" pin="DOUT_0" pad="7"/>
<connect gate="G$1" pin="DOUT_1" pad="8"/>
<connect gate="G$1" pin="DOUT_2" pad="9"/>
<connect gate="G$1" pin="DOUT_3" pad="10"/>
<connect gate="G$1" pin="DOUT_4" pad="11"/>
<connect gate="G$1" pin="DOUT_5" pad="12"/>
<connect gate="G$1" pin="DOUT_6" pad="13"/>
<connect gate="G$1" pin="DOUT_7" pad="14"/>
<connect gate="G$1" pin="DOUT_8" pad="15"/>
<connect gate="G$1" pin="DVDD28" pad="19"/>
<connect gate="G$1" pin="LED_CTRL" pad="24"/>
<connect gate="G$1" pin="PS1" pad="21"/>
<connect gate="G$1" pin="PS2" pad="22"/>
<connect gate="G$1" pin="RESET_N" pad="4"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="SDIN" pad="20"/>
<connect gate="G$1" pin="SHIELD" pad="23"/>
<connect gate="G$1" pin="VALIDH" pad="17"/>
<connect gate="G$1" pin="VALIDV" pad="18"/>
<connect gate="G$1" pin="VCLK_OUT" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC7SU04F">
<gates>
<gate name="G$1" symbol="TC7SU04F"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+V" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC1G08">
<gates>
<gate name="G$1" symbol="SN74LVC1G08"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+V" pad="5"/>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USD-SOCKET" prefix="U">
<description>&lt;b&gt;microSD Socket&lt;/b&gt;
Push-push type uSD socket. Schematic element and footprint production proven. Spark Fun Electronics SKU : PRT-00127. tDoc lines correctly indicate media card edge positions when inserting (unlocked, locked, depressed).</description>
<gates>
<gate name="G$1" symbol="USDCARD"/>
</gates>
<devices>
<device name="USD" package="USD-SOCKET-PP">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RSV" pad="8"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD@1" pad="CD1"/>
<connect gate="G$1" pin="SHIELD@2" pad="CD2"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="SHIELD@4" pad="GND2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEW" package="MICRO-SD-SOCKET-PP">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RSV" pad="8"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND3"/>
<connect gate="G$1" pin="SHIELD@2" pad="CD1"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="SHIELD@4" pad="CD2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RL" prefix="IC">
<description>&lt;b&gt;USB UART&lt;/b&gt;
FT232RL 4&lt;sup&gt;th&lt;/sup&gt; Generation USB UART (USB &amp;lt;-&amp;gt; Serial) Controller. Spark Fun Electronics SKU : COM-00650</description>
<gates>
<gate name="G$1" symbol="FT232R"/>
</gates>
<devices>
<device name="SSOP" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="DCD" pad="10"/>
<connect gate="G$1" pin="DSR" pad="9"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND18" pad="18"/>
<connect gate="G$1" pin="GND21" pad="21"/>
<connect gate="G$1" pin="GND7" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWREN" pad="14"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="RI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="RXLED" pad="22"/>
<connect gate="G$1" pin="SLEEP" pad="12"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="TXDEN" pad="13"/>
<connect gate="G$1" pin="TXLED" pad="23"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RL-BASIC" prefix="U">
<description>&lt;b&gt;USB UART&lt;/b&gt;
This is the simplified version of the FT232RL unit. Only what you need, nothing you don't. Spark Fun Electronics SKU : COM-00650</description>
<gates>
<gate name="G$1" symbol="FT232R-BASIC"/>
</gates>
<devices>
<device name="SSOP" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="RTS" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="RXLED" pad="22"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="TXLED" pad="23"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BGB203_BLUETOOTH">
<gates>
<gate name="G$1" symbol="BGB203_BLUETOOTH"/>
</gates>
<devices>
<device name="OLD" package="BGB203_ORIGINAL">
<connects>
<connect gate="G$1" pin="ANT" pad="2"/>
<connect gate="G$1" pin="BTACT/GPIO[17]" pad="14"/>
<connect gate="G$1" pin="CTS/GPIO[2]" pad="42"/>
<connect gate="G$1" pin="DN_USB" pad="37"/>
<connect gate="G$1" pin="DP_USB" pad="38"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@49" pad="49"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="GPIO[10]" pad="23"/>
<connect gate="G$1" pin="GPIO[11]" pad="22"/>
<connect gate="G$1" pin="GPIO[12]" pad="12"/>
<connect gate="G$1" pin="GPIO[13]" pad="21"/>
<connect gate="G$1" pin="GPIO[14]" pad="11"/>
<connect gate="G$1" pin="GPIO[15]" pad="30"/>
<connect gate="G$1" pin="GPIO[16]" pad="25"/>
<connect gate="G$1" pin="GPIO[6]" pad="33"/>
<connect gate="G$1" pin="GPIO[7]" pad="31"/>
<connect gate="G$1" pin="GPIO[8]" pad="34"/>
<connect gate="G$1" pin="GPIO[9]" pad="32"/>
<connect gate="G$1" pin="I2C_SCL/GPIO[0]" pad="17"/>
<connect gate="G$1" pin="I2C_SDA/GPIO[1]" pad="16"/>
<connect gate="G$1" pin="RESET_N" pad="43"/>
<connect gate="G$1" pin="RTS/GPIO[3]" pad="39"/>
<connect gate="G$1" pin="RX/GPIO[5]" pad="40"/>
<connect gate="G$1" pin="TCK_JTAG" pad="48"/>
<connect gate="G$1" pin="TDI_JTAG" pad="47"/>
<connect gate="G$1" pin="TDO_JTAG" pad="46"/>
<connect gate="G$1" pin="TMS_JTAG" pad="45"/>
<connect gate="G$1" pin="TX/GPIO[4]" pad="41"/>
<connect gate="G$1" pin="VANLO" pad="15"/>
<connect gate="G$1" pin="VBUS_USB" pad="29"/>
<connect gate="G$1" pin="VDDA/VDDO" pad="18"/>
<connect gate="G$1" pin="VDDC" pad="35"/>
<connect gate="G$1" pin="VDDC/VDDIO1" pad="24"/>
<connect gate="G$1" pin="VDDIO1" pad="26"/>
<connect gate="G$1" pin="VDDIO2" pad="36"/>
<connect gate="G$1" pin="VDDIORF" pad="44"/>
<connect gate="G$1" pin="VDDRF" pad="13"/>
<connect gate="G$1" pin="XTAL1_LP" pad="27"/>
<connect gate="G$1" pin="XTAL1_SYS" pad="20"/>
<connect gate="G$1" pin="XTAL2_LP" pad="28"/>
<connect gate="G$1" pin="XTAL2_SYS" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="BGB203">
<connects>
<connect gate="G$1" pin="ANT" pad="2"/>
<connect gate="G$1" pin="BTACT/GPIO[17]" pad="14"/>
<connect gate="G$1" pin="CTS/GPIO[2]" pad="42"/>
<connect gate="G$1" pin="DN_USB" pad="37"/>
<connect gate="G$1" pin="DP_USB" pad="38"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@49" pad="49"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="GPIO[10]" pad="23"/>
<connect gate="G$1" pin="GPIO[11]" pad="22"/>
<connect gate="G$1" pin="GPIO[12]" pad="12"/>
<connect gate="G$1" pin="GPIO[13]" pad="21"/>
<connect gate="G$1" pin="GPIO[14]" pad="11"/>
<connect gate="G$1" pin="GPIO[15]" pad="30"/>
<connect gate="G$1" pin="GPIO[16]" pad="25"/>
<connect gate="G$1" pin="GPIO[6]" pad="33"/>
<connect gate="G$1" pin="GPIO[7]" pad="31"/>
<connect gate="G$1" pin="GPIO[8]" pad="34"/>
<connect gate="G$1" pin="GPIO[9]" pad="32"/>
<connect gate="G$1" pin="I2C_SCL/GPIO[0]" pad="17"/>
<connect gate="G$1" pin="I2C_SDA/GPIO[1]" pad="16"/>
<connect gate="G$1" pin="RESET_N" pad="43"/>
<connect gate="G$1" pin="RTS/GPIO[3]" pad="39"/>
<connect gate="G$1" pin="RX/GPIO[5]" pad="40"/>
<connect gate="G$1" pin="TCK_JTAG" pad="48"/>
<connect gate="G$1" pin="TDI_JTAG" pad="47"/>
<connect gate="G$1" pin="TDO_JTAG" pad="46"/>
<connect gate="G$1" pin="TMS_JTAG" pad="45"/>
<connect gate="G$1" pin="TX/GPIO[4]" pad="41"/>
<connect gate="G$1" pin="VANLO" pad="15"/>
<connect gate="G$1" pin="VBUS_USB" pad="29"/>
<connect gate="G$1" pin="VDDA/VDDO" pad="18"/>
<connect gate="G$1" pin="VDDC" pad="35"/>
<connect gate="G$1" pin="VDDC/VDDIO1" pad="24"/>
<connect gate="G$1" pin="VDDIO1" pad="26"/>
<connect gate="G$1" pin="VDDIO2" pad="36"/>
<connect gate="G$1" pin="VDDIORF" pad="44"/>
<connect gate="G$1" pin="VDDRF" pad="13"/>
<connect gate="G$1" pin="XTAL1_LP" pad="27"/>
<connect gate="G$1" pin="XTAL1_SYS" pad="20"/>
<connect gate="G$1" pin="XTAL2_LP" pad="28"/>
<connect gate="G$1" pin="XTAL2_SYS" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NAV_SWITCH">
<description>&lt;b&gt;Navigation Switch&lt;/b&gt;
Three way navigation switch. Commonly used as up/down/select on MP3 players. Schematic element and footprint production proven. Spark Fun Electronics SKU : COM-08184</description>
<gates>
<gate name="G$1" symbol="NAV_SWITCH"/>
</gates>
<devices>
<device name="SMD" package="NAV_SWITCH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="T" pad="T"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPX29302">
<gates>
<gate name="G$1" symbol="SPX29300"/>
</gates>
<devices>
<device name="" package="Q5-DD_SPX29300">
<connects>
<connect gate="G$1" pin="ADJUST" pad="5"/>
<connect gate="G$1" pin="ENABLE" pad="1"/>
<connect gate="G$1" pin="GND@0" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUERADIO_BR-C40N">
<description>&lt;b&gt;Bluetooth SMD Module&lt;/b&gt;
BR-C40A with antenna cut off. 50 Ohm antenna trace and connector required. Footprint fully proven. Spark Fun Electronics SKU : WRL-00149</description>
<gates>
<gate name="G$1" symbol="BLUERADIO_BR-C40N"/>
</gates>
<devices>
<device name="BAS" package="BLUERADIO_BR-C40N">
<connects>
<connect gate="G$1" pin="ANT" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFE" package="BLUETOOTH-SMD-FP">
<connects>
<connect gate="G$1" pin="ANT" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="INTERNAL" package="BLUETOOTH-INTERNAL-FP">
<connects>
<connect gate="G$1" pin="ANT" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="INT2" package="BLUETOOTH-INTERNAL-FP2">
<connects>
<connect gate="G$1" pin="ANT" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SHT1X">
<description>&lt;b&gt;SHT1x Humdity Sensor&lt;/b&gt;
Sensirion humdity sensor. Schematic element and footprint proven. Spark Fun Electronics SKU : COM-08227</description>
<gates>
<gate name="G$1" symbol="SHT1X"/>
</gates>
<devices>
<device name="SMD" package="SHT1X">
<connects>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDG300">
<description>&lt;b&gt;IDG300&lt;/b&gt;
This is a dual axis MEMs based gyroscope sensor from Invensense. The only gyro in currently available with two axis on one chip. Works very well. Schematic and footprint are not yet production proven. Spark Fun Electronics SKU : COM-00700</description>
<gates>
<gate name="G$1" symbol="IDG300"/>
</gates>
<devices>
<device name="SMD" package="IDG300">
<connects>
<connect gate="G$1" pin="CPOUT" pad="17"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="38"/>
<connect gate="G$1" pin="GND@4" pad="39"/>
<connect gate="G$1" pin="GND@5" pad="40"/>
<connect gate="G$1" pin="GND@6" pad="GND"/>
<connect gate="G$1" pin="VDD@0" pad="14"/>
<connect gate="G$1" pin="VDD@1" pad="29"/>
<connect gate="G$1" pin="VDD@2" pad="34"/>
<connect gate="G$1" pin="VREF" pad="32"/>
<connect gate="G$1" pin="XAGC" pad="8"/>
<connect gate="G$1" pin="X_RO" pad="3"/>
<connect gate="G$1" pin="YAGC" pad="23"/>
<connect gate="G$1" pin="Y_RO" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV324">
<gates>
<gate name="G$1" symbol="LMV324"/>
<gate name="G$2" symbol="LMV324_2"/>
<gate name="G$3" symbol="LMV324_2"/>
<gate name="G$4" symbol="LMV324_2"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="+V" pad="4"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-V" pad="11"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$2" pin="+IN" pad="5"/>
<connect gate="G$2" pin="-IN" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="+IN" pad="10"/>
<connect gate="G$3" pin="-IN" pad="9"/>
<connect gate="G$3" pin="OUT" pad="8"/>
<connect gate="G$4" pin="+IN" pad="12"/>
<connect gate="G$4" pin="-IN" pad="13"/>
<connect gate="G$4" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA344">
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IPOD_CONNECTOR_FEMALE">
<description>&lt;b&gt;iPod Female Connector&lt;/b&gt;
This is the connector found inside current iPods. Use this connector to attach to iPod accessories like Nike+iPods, etc. Schematic and footprint are not yet production proven. Spark Fun Electronics SKU : DEV-08035</description>
<gates>
<gate name="G$1" symbol="IPOD_CONNECTOR_FEMALE"/>
</gates>
<devices>
<device name="" package="IPOD_FEMALE_CONNECTOR">
<connects>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="3.3V" pad="18"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="ACC_INDICATOR" pad="21"/>
<connect gate="G$1" pin="FW_12V@19" pad="19"/>
<connect gate="G$1" pin="FW_12V@20" pad="20"/>
<connect gate="G$1" pin="FW_TPA+" pad="24"/>
<connect gate="G$1" pin="FW_TPA-" pad="22"/>
<connect gate="G$1" pin="FW_TPB+" pad="28"/>
<connect gate="G$1" pin="FW_TPB-" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@30" pad="30"/>
<connect gate="G$1" pin="LEFT_IN" pad="6"/>
<connect gate="G$1" pin="LEFT_OUT" pad="4"/>
<connect gate="G$1" pin="RIGHT_IN" pad="5"/>
<connect gate="G$1" pin="RIGHT_OUT" pad="3"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCHROME_OUT" pad="9"/>
<connect gate="G$1" pin="SLUM_OUT" pad="10"/>
<connect gate="G$1" pin="TX" pad="12"/>
<connect gate="G$1" pin="USB_5V" pad="23"/>
<connect gate="G$1" pin="USB_D+" pad="27"/>
<connect gate="G$1" pin="USB_D-" pad="25"/>
<connect gate="G$1" pin="VIDEO_OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IPOD_CONNECTOR_MALE">
<description>&lt;b&gt;iPod Male Connector&lt;/b&gt;
This is the connector that will insert into an iPods. Use this connector to gain access to the various iPod pins. Schematic and footprint are not yet production proven. The PCB thickness must be more thin than the standard 0.062" FR4. Spark Fun Electronics SKU : DEV-00633</description>
<gates>
<gate name="G$1" symbol="IPOD_CONNECTOR_FEMALE"/>
</gates>
<devices>
<device name="" package="IPOD_MALE_CONNECTOR">
<connects>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="3.3V" pad="18"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="ACC_INDICATOR" pad="21"/>
<connect gate="G$1" pin="FW_12V@19" pad="19"/>
<connect gate="G$1" pin="FW_12V@20" pad="20"/>
<connect gate="G$1" pin="FW_TPA+" pad="24"/>
<connect gate="G$1" pin="FW_TPA-" pad="22"/>
<connect gate="G$1" pin="FW_TPB+" pad="28"/>
<connect gate="G$1" pin="FW_TPB-" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@30" pad="30"/>
<connect gate="G$1" pin="LEFT_IN" pad="6"/>
<connect gate="G$1" pin="LEFT_OUT" pad="4"/>
<connect gate="G$1" pin="RIGHT_IN" pad="5"/>
<connect gate="G$1" pin="RIGHT_OUT" pad="3"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCHROME_OUT" pad="9"/>
<connect gate="G$1" pin="SLUM_OUT" pad="10"/>
<connect gate="G$1" pin="TX" pad="12"/>
<connect gate="G$1" pin="USB_5V" pad="23"/>
<connect gate="G$1" pin="USB_D+" pad="27"/>
<connect gate="G$1" pin="USB_D-" pad="25"/>
<connect gate="G$1" pin="VIDEO_OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M15" prefix="JP">
<description>&lt;b&gt;Header 15&lt;/b&gt;
Standard 15-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M15"/>
</gates>
<devices>
<device name="" package="1X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X15_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X15_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2550">
<gates>
<gate name="G$1" symbol="PIC18F2550"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/AN4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC4/D-" pad="15"/>
<connect gate="G$1" pin="RC5/D+" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="V-USB" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GE863_GPS">
<description>&lt;b&gt;GE863 Cellular Module with GPS&lt;/b&gt;
Proto layout and schematic for GE863 cellular module with SiRF III GPS. Spark Fun Electronics SKU : CEL-08246</description>
<gates>
<gate name="G$1" symbol="GE863"/>
</gates>
<devices>
<device name="" package="GE863">
<connects>
<connect gate="G$1" pin="ADC_IN1" pad="23"/>
<connect gate="G$1" pin="ANT" pad="49"/>
<connect gate="G$1" pin="AXE" pad="30"/>
<connect gate="G$1" pin="C103/TXD" pad="37"/>
<connect gate="G$1" pin="C104/RXD" pad="38"/>
<connect gate="G$1" pin="C105/RTS" pad="40"/>
<connect gate="G$1" pin="C106/CTS" pad="41"/>
<connect gate="G$1" pin="C107/DSR" pad="43"/>
<connect gate="G$1" pin="C108/DTR" pad="39"/>
<connect gate="G$1" pin="C109/DCD" pad="42"/>
<connect gate="G$1" pin="C125/RING" pad="44"/>
<connect gate="G$1" pin="CAM_CLK" pad="7"/>
<connect gate="G$1" pin="CHARGE" pad="35"/>
<connect gate="G$1" pin="DAC_OUT" pad="63"/>
<connect gate="G$1" pin="EAR_HF+" pad="11"/>
<connect gate="G$1" pin="EAR_HF-" pad="12"/>
<connect gate="G$1" pin="EAR_MT+" pad="10"/>
<connect gate="G$1" pin="EAR_MT-" pad="9"/>
<connect gate="G$1" pin="GND@0" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="17"/>
<connect gate="G$1" pin="GND@10" pad="72"/>
<connect gate="G$1" pin="GND@11" pad="77"/>
<connect gate="G$1" pin="GND@12" pad="79"/>
<connect gate="G$1" pin="GND@13" pad="82"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="36"/>
<connect gate="G$1" pin="GND@4" pad="45"/>
<connect gate="G$1" pin="GND@5" pad="48"/>
<connect gate="G$1" pin="GND@6" pad="50"/>
<connect gate="G$1" pin="GND@7" pad="56"/>
<connect gate="G$1" pin="GND@8" pad="67"/>
<connect gate="G$1" pin="GND@9" pad="69"/>
<connect gate="G$1" pin="GND_GPS" pad="84"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO10" pad="4"/>
<connect gate="G$1" pin="GPIO11" pad="3"/>
<connect gate="G$1" pin="GPIO12" pad="2"/>
<connect gate="G$1" pin="GPIO13" pad="1"/>
<connect gate="G$1" pin="GPIO14" pad="60"/>
<connect gate="G$1" pin="GPIO15" pad="71"/>
<connect gate="G$1" pin="GPIO16" pad="64"/>
<connect gate="G$1" pin="GPIO17" pad="59"/>
<connect gate="G$1" pin="GPIO18" pad="76"/>
<connect gate="G$1" pin="GPIO2/JDR" pad="33"/>
<connect gate="G$1" pin="GPIO3/CAM_SCL" pad="55"/>
<connect gate="G$1" pin="GPIO4/CAM_SDA" pad="32"/>
<connect gate="G$1" pin="GPIO5" pad="53"/>
<connect gate="G$1" pin="GPIO6" pad="54"/>
<connect gate="G$1" pin="GPIO7/BUZZER" pad="51"/>
<connect gate="G$1" pin="GPIO8/CAM_ON" pad="6"/>
<connect gate="G$1" pin="GPIO9/CAM_RST" pad="5"/>
<connect gate="G$1" pin="GPS_ANT" pad="83"/>
<connect gate="G$1" pin="MIC_HF+" pad="15"/>
<connect gate="G$1" pin="MIC_HF-" pad="16"/>
<connect gate="G$1" pin="MIC_MT+" pad="13"/>
<connect gate="G$1" pin="MIN_MT-" pad="14"/>
<connect gate="G$1" pin="ON/OFF" pad="46"/>
<connect gate="G$1" pin="PPS" pad="75"/>
<connect gate="G$1" pin="PWRMON" pad="52"/>
<connect gate="G$1" pin="RESET" pad="47"/>
<connect gate="G$1" pin="RX_GPS" pad="73"/>
<connect gate="G$1" pin="RX_GPS_BIN" pad="78"/>
<connect gate="G$1" pin="RX_TRACE" pad="26"/>
<connect gate="G$1" pin="SIMCLK" pad="18"/>
<connect gate="G$1" pin="SIMIN" pad="21"/>
<connect gate="G$1" pin="SIMIO" pad="20"/>
<connect gate="G$1" pin="SIMRST" pad="19"/>
<connect gate="G$1" pin="SIMVCC" pad="22"/>
<connect gate="G$1" pin="STAT_LED" pad="29"/>
<connect gate="G$1" pin="TX_GPS" pad="68"/>
<connect gate="G$1" pin="TX_GPS_BIN" pad="80"/>
<connect gate="G$1" pin="TX_TRACE" pad="25"/>
<connect gate="G$1" pin="VAUX1" pad="31"/>
<connect gate="G$1" pin="VBATT" pad="27"/>
<connect gate="G$1" pin="VRTC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIMHOLDER">
<description>&lt;b&gt;SIM Socket&lt;/b&gt;
Socket for SIM cellular cards. Schematic element and footprint production proven. Spark Fun Electronics SKU : PRT-00548</description>
<gates>
<gate name="G$1" symbol="SIMHOLDER"/>
</gates>
<devices>
<device name="" package="SIMHOLDER">
<connects>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="C3" pad="C3"/>
<connect gate="G$1" pin="C5" pad="C5"/>
<connect gate="G$1" pin="C6" pad="C6"/>
<connect gate="G$1" pin="C7" pad="C7"/>
<connect gate="G$1" pin="SW1" pad="SW1"/>
<connect gate="G$1" pin="SW2" pad="SW2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F883">
<gates>
<gate name="G$1" symbol="PIC16F883"/>
</gates>
<devices>
<device name="" package="SO-28W">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC4/SDI" pad="15"/>
<connect gate="G$1" pin="RC5/SDO" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_PNP" prefix="Q">
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOT89">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC1041Z">
<gates>
<gate name="G$1" symbol="HMC1041Z"/>
</gates>
<devices>
<device name="" package="HMC1041Z">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="OFFSET+" pad="3"/>
<connect gate="G$1" pin="OFFSET-" pad="1"/>
<connect gate="G$1" pin="OUT+" pad="4"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
<connect gate="G$1" pin="S/R+" pad="8"/>
<connect gate="G$1" pin="S/R-" pad="7"/>
<connect gate="G$1" pin="VBRIDGE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC6042">
<gates>
<gate name="G$1" symbol="HMC6042"/>
</gates>
<devices>
<device name="" package="HMC6042">
<connects>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="FBX" pad="15"/>
<connect gate="G$1" pin="FBY" pad="13"/>
<connect gate="G$1" pin="FBZ" pad="11"/>
<connect gate="G$1" pin="GND" pad="17"/>
<connect gate="G$1" pin="INZ+" pad="6"/>
<connect gate="G$1" pin="INZ-" pad="7"/>
<connect gate="G$1" pin="OUTX" pad="16"/>
<connect gate="G$1" pin="OUTY" pad="14"/>
<connect gate="G$1" pin="OUTZ" pad="12"/>
<connect gate="G$1" pin="S/R+" pad="4"/>
<connect gate="G$1" pin="S/R-" pad="5"/>
<connect gate="G$1" pin="S/R-C" pad="9"/>
<connect gate="G$1" pin="S/R-IN" pad="10"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F88-DIP">
<gates>
<gate name="G$1" symbol="PIC16F88-DIP"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="17"/>
<connect gate="G$1" pin="RA1/AN1" pad="18"/>
<connect gate="G$1" pin="RA2/AN2" pad="1"/>
<connect gate="G$1" pin="RA3/AN3" pad="2"/>
<connect gate="G$1" pin="RA4/AN4" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2" pad="15"/>
<connect gate="G$1" pin="RA7/OSC1" pad="16"/>
<connect gate="G$1" pin="RB0/INT" pad="6"/>
<connect gate="G$1" pin="RB1/SDA" pad="7"/>
<connect gate="G$1" pin="RB2/RX" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4/SCL" pad="10"/>
<connect gate="G$1" pin="RB5/TX" pad="11"/>
<connect gate="G$1" pin="RB6/PGC" pad="12"/>
<connect gate="G$1" pin="RB7/PGD" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA168" prefix="U">
<gates>
<gate name="G$1" symbol="ATMEGA168"/>
</gates>
<devices>
<device name="MLF" package="MLF32">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="21"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GM862">
<description>&lt;b&gt;GM862 Cellular Module with GPS&lt;/b&gt;
Proven layout and schematic for GM862 cellular module with SiRF III GPS. Spark Fun Electronics SKU : CEL-07917</description>
<gates>
<gate name="G$1" symbol="GM862"/>
</gates>
<devices>
<device name="GND" package="GM862">
<connects>
<connect gate="G$1" pin="AXE" pad="18"/>
<connect gate="G$1" pin="C103/TXD" pad="20"/>
<connect gate="G$1" pin="C104/RXD" pad="37"/>
<connect gate="G$1" pin="C105/RTS" pad="45"/>
<connect gate="G$1" pin="C106/CTS" pad="29"/>
<connect gate="G$1" pin="C107/DSR" pad="33"/>
<connect gate="G$1" pin="C108/DTR" pad="43"/>
<connect gate="G$1" pin="C109/DCD" pad="36"/>
<connect gate="G$1" pin="C125/RING" pad="30"/>
<connect gate="G$1" pin="CCIN/SIMIN" pad="27"/>
<connect gate="G$1" pin="CHARGE" pad="8"/>
<connect gate="G$1" pin="EAR_HF+" pad="9"/>
<connect gate="G$1" pin="EAR_HF-" pad="11"/>
<connect gate="G$1" pin="EAR_MT+" pad="12"/>
<connect gate="G$1" pin="EAR_MT-" pad="10"/>
<connect gate="G$1" pin="EMMI_RX/RX_GPS" pad="41"/>
<connect gate="G$1" pin="EMMI_TX/TX_GPS" pad="35"/>
<connect gate="G$1" pin="GND/ADC" pad="6"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="G1"/>
<connect gate="G$1" pin="GND@3" pad="G2"/>
<connect gate="G$1" pin="GND@4" pad="G3"/>
<connect gate="G$1" pin="GND@5" pad="G8"/>
<connect gate="G$1" pin="GND@6" pad="G4"/>
<connect gate="G$1" pin="GND@7" pad="G5"/>
<connect gate="G$1" pin="GND@8" pad="G6"/>
<connect gate="G$1" pin="GND@9" pad="G7"/>
<connect gate="G$1" pin="GPI1" pad="31"/>
<connect gate="G$1" pin="GPIO10/PD[2]" pad="38"/>
<connect gate="G$1" pin="GPIO11/PD[3]" pad="40"/>
<connect gate="G$1" pin="GPIO12/PD[4]" pad="42"/>
<connect gate="G$1" pin="GPIO13/PD[5]" pad="44"/>
<connect gate="G$1" pin="GPIO3/PD[6]/CAM_SCL" pad="46"/>
<connect gate="G$1" pin="GPIO4/IICSDA/CAM_SDA" pad="47"/>
<connect gate="G$1" pin="GPIO5/CAM_RDY/RFTXMON" pad="48"/>
<connect gate="G$1" pin="GPIO6/ALARM/PD[7]" pad="49"/>
<connect gate="G$1" pin="GPIO7/BUZZER/CAM_PWR_ON" pad="50"/>
<connect gate="G$1" pin="GPIO8/PD[0]/CAM_ON" pad="32"/>
<connect gate="G$1" pin="GPIO9/PD[1]/CAM_RST" pad="34"/>
<connect gate="G$1" pin="GPO2/JDR" pad="28"/>
<connect gate="G$1" pin="MIC_HF+" pad="15"/>
<connect gate="G$1" pin="MIC_HF-" pad="13"/>
<connect gate="G$1" pin="MIC_MT+" pad="14"/>
<connect gate="G$1" pin="MIC_MT-" pad="16"/>
<connect gate="G$1" pin="ON/OFF" pad="17"/>
<connect gate="G$1" pin="PWRMON" pad="21"/>
<connect gate="G$1" pin="RES@25" pad="25"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="SIMCLK" pad="26"/>
<connect gate="G$1" pin="SIMIO" pad="19"/>
<connect gate="G$1" pin="SIMRST" pad="24"/>
<connect gate="G$1" pin="SIMVCC" pad="22"/>
<connect gate="G$1" pin="STAT_LED" pad="39"/>
<connect gate="G$1" pin="VBATT@0" pad="1"/>
<connect gate="G$1" pin="VBATT@1" pad="3"/>
<connect gate="G$1" pin="VBATT@2" pad="5"/>
<connect gate="G$1" pin="VBATT@3" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM862_CONNECTOR" package="GM862_CONNECTOR">
<connects>
<connect gate="G$1" pin="AXE" pad="18"/>
<connect gate="G$1" pin="C103/TXD" pad="20"/>
<connect gate="G$1" pin="C104/RXD" pad="37"/>
<connect gate="G$1" pin="C105/RTS" pad="45"/>
<connect gate="G$1" pin="C106/CTS" pad="29"/>
<connect gate="G$1" pin="C107/DSR" pad="33"/>
<connect gate="G$1" pin="C108/DTR" pad="43"/>
<connect gate="G$1" pin="C109/DCD" pad="36"/>
<connect gate="G$1" pin="C125/RING" pad="30"/>
<connect gate="G$1" pin="CCIN/SIMIN" pad="27"/>
<connect gate="G$1" pin="CHARGE" pad="8"/>
<connect gate="G$1" pin="EAR_HF+" pad="9"/>
<connect gate="G$1" pin="EAR_HF-" pad="11"/>
<connect gate="G$1" pin="EAR_MT+" pad="12"/>
<connect gate="G$1" pin="EAR_MT-" pad="10"/>
<connect gate="G$1" pin="EMMI_RX/RX_GPS" pad="41"/>
<connect gate="G$1" pin="EMMI_TX/TX_GPS" pad="35"/>
<connect gate="G$1" pin="GND/ADC" pad="6"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="G1"/>
<connect gate="G$1" pin="GND@3" pad="G2"/>
<connect gate="G$1" pin="GND@4" pad="G3"/>
<connect gate="G$1" pin="GND@5" pad="G8"/>
<connect gate="G$1" pin="GND@6" pad="G4"/>
<connect gate="G$1" pin="GND@7" pad="G5"/>
<connect gate="G$1" pin="GND@8" pad="G6"/>
<connect gate="G$1" pin="GND@9" pad="G7"/>
<connect gate="G$1" pin="GPI1" pad="31"/>
<connect gate="G$1" pin="GPIO10/PD[2]" pad="38"/>
<connect gate="G$1" pin="GPIO11/PD[3]" pad="40"/>
<connect gate="G$1" pin="GPIO12/PD[4]" pad="42"/>
<connect gate="G$1" pin="GPIO13/PD[5]" pad="44"/>
<connect gate="G$1" pin="GPIO3/PD[6]/CAM_SCL" pad="46"/>
<connect gate="G$1" pin="GPIO4/IICSDA/CAM_SDA" pad="47"/>
<connect gate="G$1" pin="GPIO5/CAM_RDY/RFTXMON" pad="48"/>
<connect gate="G$1" pin="GPIO6/ALARM/PD[7]" pad="49"/>
<connect gate="G$1" pin="GPIO7/BUZZER/CAM_PWR_ON" pad="50"/>
<connect gate="G$1" pin="GPIO8/PD[0]/CAM_ON" pad="32"/>
<connect gate="G$1" pin="GPIO9/PD[1]/CAM_RST" pad="34"/>
<connect gate="G$1" pin="GPO2/JDR" pad="28"/>
<connect gate="G$1" pin="MIC_HF+" pad="15"/>
<connect gate="G$1" pin="MIC_HF-" pad="13"/>
<connect gate="G$1" pin="MIC_MT+" pad="14"/>
<connect gate="G$1" pin="MIC_MT-" pad="16"/>
<connect gate="G$1" pin="ON/OFF" pad="17"/>
<connect gate="G$1" pin="PWRMON" pad="21"/>
<connect gate="G$1" pin="RES@25" pad="25"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="SIMCLK" pad="26"/>
<connect gate="G$1" pin="SIMIO" pad="19"/>
<connect gate="G$1" pin="SIMRST" pad="24"/>
<connect gate="G$1" pin="SIMVCC" pad="22"/>
<connect gate="G$1" pin="STAT_LED" pad="39"/>
<connect gate="G$1" pin="VBATT@0" pad="1"/>
<connect gate="G$1" pin="VBATT@1" pad="3"/>
<connect gate="G$1" pin="VBATT@2" pad="5"/>
<connect gate="G$1" pin="VBATT@3" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME-A3" prefix="FRAME">
<description>&lt;b&gt;Schematic Frame&lt;/b&gt;&lt;p&gt;
A3 Larger Frame</description>
<gates>
<gate name="G$1" symbol="A3L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_MINI_PROG">
<gates>
<gate name="G$1" symbol="AVR_MINI_PROGRAMMER"/>
</gates>
<devices>
<device name="SMD" package="AVR_MINI_PROG">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="MISO" pad="6"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SV74LV4052APWR">
<gates>
<gate name="G$1" symbol="SN74LV4052APWR"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="1-COM" pad="13"/>
<connect gate="G$1" pin="1Y0" pad="12"/>
<connect gate="G$1" pin="1Y1" pad="14"/>
<connect gate="G$1" pin="1Y2" pad="15"/>
<connect gate="G$1" pin="1Y3" pad="11"/>
<connect gate="G$1" pin="2-COM" pad="3"/>
<connect gate="G$1" pin="2Y0" pad="1"/>
<connect gate="G$1" pin="2Y1" pad="5"/>
<connect gate="G$1" pin="2Y2" pad="2"/>
<connect gate="G$1" pin="2Y3" pad="4"/>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GNG@7" pad="7"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="TVSOP-16">
<connects>
<connect gate="G$1" pin="1-COM" pad="P$13"/>
<connect gate="G$1" pin="1Y0" pad="P$12"/>
<connect gate="G$1" pin="1Y1" pad="P$14"/>
<connect gate="G$1" pin="1Y2" pad="P$15"/>
<connect gate="G$1" pin="1Y3" pad="P$11"/>
<connect gate="G$1" pin="2-COM" pad="P$3"/>
<connect gate="G$1" pin="2Y0" pad="P$1"/>
<connect gate="G$1" pin="2Y1" pad="P$5"/>
<connect gate="G$1" pin="2Y2" pad="P$2"/>
<connect gate="G$1" pin="2Y3" pad="P$4"/>
<connect gate="G$1" pin="A" pad="P$10"/>
<connect gate="G$1" pin="B" pad="P$9"/>
<connect gate="G$1" pin="GND@8" pad="P$8"/>
<connect gate="G$1" pin="GNG@7" pad="P$7"/>
<connect gate="G$1" pin="INH" pad="P$6"/>
<connect gate="G$1" pin="VCC" pad="P$16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM406" prefix="U">
<description>&lt;b&gt;EM406 Connector&lt;/b&gt;
Proven layout and schematic for EM406 connector. Spark Fun Electronics SKU : GPS-00579</description>
<gates>
<gate name="G$1" symbol="EM406"/>
</gates>
<devices>
<device name="" package="EM406">
<connects>
<connect gate="G$1" pin="1PPS" pad="6"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ET312">
<description>&lt;b&gt;ET312 GPS Receiver&lt;/b&gt;
Proven layout and schematic for SiRF III ET312 GPS receiver. This footprint has been tweaked significantly to work with the ET312. This footprint has been fully qualified. Spark Fun Electronics SKU : GPS-08268.</description>
<gates>
<gate name="G$1" symbol="ET312"/>
</gates>
<devices>
<device name="SMD" package="ET312">
<connects>
<connect gate="G$1" pin="BATT" pad="6"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="2"/>
<connect gate="G$1" pin="GND3" pad="8"/>
<connect gate="G$1" pin="GND4" pad="9"/>
<connect gate="G$1" pin="GND5" pad="10"/>
<connect gate="G$1" pin="GND6" pad="11"/>
<connect gate="G$1" pin="GND7" pad="13"/>
<connect gate="G$1" pin="GPIO1" pad="5"/>
<connect gate="G$1" pin="RF" pad="12"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EB-85A">
<description>&lt;b&gt;EB-85A Connector&lt;/b&gt;
Proven layout and schematic for ETek 5Hz GPS receiver connector. Spark Fun Electronics SKU : GPS-08297</description>
<gates>
<gate name="G$1" symbol="EB-85A"/>
</gates>
<devices>
<device name="SMD" package="EB-85A">
<connects>
<connect gate="G$1" pin="BATT" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PPS" pad="7"/>
<connect gate="G$1" pin="RX1" pad="4"/>
<connect gate="G$1" pin="RX2" pad="6"/>
<connect gate="G$1" pin="TX1" pad="3"/>
<connect gate="G$1" pin="TX2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-NCHANNEL-SOIC8">
<description>&lt;b&gt;N-Channel MOSFET&lt;/b&gt;
IRF9410 and NDS8434 are common, SOIC-8 parts.</description>
<gates>
<gate name="G$1" symbol="IRF9410"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="D@1" pad="8"/>
<connect gate="G$1" pin="D@2" pad="7"/>
<connect gate="G$1" pin="D@3" pad="6"/>
<connect gate="G$1" pin="D@4" pad="5"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S@1" pad="1"/>
<connect gate="G$1" pin="S@2" pad="2"/>
<connect gate="G$1" pin="S@3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NJM2670">
<gates>
<gate name="G$1" symbol="NJM2670"/>
</gates>
<devices>
<device name="SMD" package="SO-24W">
<connects>
<connect gate="G$1" pin="ENABLEA" pad="3"/>
<connect gate="G$1" pin="ENABLEB" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="GND@3" pad="18"/>
<connect gate="G$1" pin="GND@4" pad="19"/>
<connect gate="G$1" pin="INA1" pad="2"/>
<connect gate="G$1" pin="INA2" pad="22"/>
<connect gate="G$1" pin="INB1" pad="8"/>
<connect gate="G$1" pin="INB2" pad="17"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="10"/>
<connect gate="G$1" pin="NC@3" pad="15"/>
<connect gate="G$1" pin="NC@4" pad="21"/>
<connect gate="G$1" pin="OUTA1" pad="5"/>
<connect gate="G$1" pin="OUTA2" pad="20"/>
<connect gate="G$1" pin="OUTB1" pad="11"/>
<connect gate="G$1" pin="OUTB2" pad="14"/>
<connect gate="G$1" pin="SENSEA" pad="1"/>
<connect gate="G$1" pin="SENSEB" pad="12"/>
<connect gate="G$1" pin="TSDARM" pad="16"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VSA" pad="24"/>
<connect gate="G$1" pin="VSB" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34063" prefix="U">
<gates>
<gate name="G$1" symbol="MC34063"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="COMP" pad="5"/>
<connect gate="G$1" pin="DVR" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SEN" pad="7"/>
<connect gate="G$1" pin="SWC" pad="1"/>
<connect gate="G$1" pin="SWE" pad="2"/>
<connect gate="G$1" pin="TC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA">
<description>&lt;b&gt;Antenna&lt;/b&gt;&lt;p&gt;
Antenna with ground or secondary connection. Common with larger metal RF connectors.</description>
<gates>
<gate name="G$1" symbol="ANTENNA"/>
</gates>
<devices>
<device name="SMD1" package="ANTENNA-CHIP">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA2">
<description>&lt;b&gt;Antenna&lt;/b&gt;&lt;p&gt;
Single endded antenna. Common with smaller chip antennas. CHIP4 package is the GPS Chip Antenna &lt;b&gt;SKU:&lt;/b&gt; GPS-08418. CHIP5 package is 2.4GHz chip antenna &lt;b&gt;SKU:&lt;/b&gt; WRL-00144.</description>
<gates>
<gate name="G$1" symbol="ANTENNA2"/>
</gates>
<devices>
<device name="SMD" package="ANTENNA-CHIP2">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="ANTENNA-CHIP3">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD3" package="ANTENNA-CHIP4">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD5" package="ANTENNA-CHIP5">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD6" package="ANTENNA-CHIP6">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC6244">
<gates>
<gate name="G$1" symbol="LTC6244"/>
<gate name="G$2" symbol="LTC6244_2"/>
</gates>
<devices>
<device name="" package="MSOP8">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V18ZA2P">
<gates>
<gate name="G$1" symbol="V18ZA2P"/>
</gates>
<devices>
<device name="" package="V18ZA2P">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*595" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch</description>
<gates>
<gate name="A" symbol="74595"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="G" pad="17"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="3"/>
<connect gate="A" pin="QD" pad="4"/>
<connect gate="A" pin="QE" pad="5"/>
<connect gate="A" pin="QF" pad="7"/>
<connect gate="A" pin="QG" pad="8"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="QH*" pad="12"/>
<connect gate="A" pin="RCK" pad="15"/>
<connect gate="A" pin="SCK" pad="14"/>
<connect gate="A" pin="SCL" pad="13"/>
<connect gate="A" pin="SER" pad="18"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="" package="TSSOP16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTC" prefix="F">
<description>&lt;b&gt;Resettable Fuse PTC&lt;/b&gt;
Resettable Fuse. Spark Fun Electronics SKU : COM-08357</description>
<gates>
<gate name="G$1" symbol="PTC"/>
</gates>
<devices>
<device name="PTH" package="PTC">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="PTC-1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MLX90609">
<description>&lt;b&gt;Melexis Gyroscope MLX90609&lt;/b&gt;
Proven footprint and schematic for single axis MEMs gyroscope. Spark Fun Electronics SKU: COM-08336 and others</description>
<gates>
<gate name="G$1" symbol="MLX90609"/>
</gates>
<devices>
<device name="SMD" package="MLX90609">
<connects>
<connect gate="G$1" pin="CASE" pad="28"/>
<connect gate="G$1" pin="ERROR" pad="11"/>
<connect gate="G$1" pin="FLT" pad="23"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="HVIN" pad="21"/>
<connect gate="G$1" pin="MISO" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="9"/>
<connect gate="G$1" pin="OUTAR" pad="24"/>
<connect gate="G$1" pin="OUTTEMP" pad="22"/>
<connect gate="G$1" pin="SCLK" pad="6"/>
<connect gate="G$1" pin="SELFTEST" pad="12"/>
<connect gate="G$1" pin="SS" pad="7"/>
<connect gate="G$1" pin="TEST" pad="10"/>
<connect gate="G$1" pin="TESTIN" pad="29"/>
<connect gate="G$1" pin="TESTOUT" pad="30"/>
<connect gate="G$1" pin="TOPCAP@1" pad="1"/>
<connect gate="G$1" pin="TOPCAP@2" pad="32"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VDDA" pad="27"/>
<connect gate="G$1" pin="VREF" pad="25"/>
<connect gate="G$1" pin="VSSA" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1014">
<gates>
<gate name="G$1" symbol="LT1014"/>
<gate name="G$2" symbol="LT1014_2"/>
<gate name="G$3" symbol="LT1014_2"/>
<gate name="G$4" symbol="LT1014_2"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="+V" pad="4"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-V" pad="13"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$2" pin="+IN" pad="5"/>
<connect gate="G$2" pin="-IN" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="+IN" pad="12"/>
<connect gate="G$3" pin="-IN" pad="11"/>
<connect gate="G$3" pin="OUT" pad="10"/>
<connect gate="G$4" pin="+IN" pad="14"/>
<connect gate="G$4" pin="-IN" pad="15"/>
<connect gate="G$4" pin="OUT" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-TRICOLOR">
<description>&lt;b&gt;Tri-Color LED SMD&lt;/b&gt;
Proven layout and schematic for triple color LED in SMD package - common anode. Spark Fun Electronics SKU : COM-07844</description>
<gates>
<gate name="G$1" symbol="LED-TRICOLORSMD"/>
</gates>
<devices>
<device name="" package="LED-TRICOLOR-SMD">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="BLU" pad="B"/>
<connect gate="G$1" pin="GRN" pad="G"/>
<connect gate="G$1" pin="RED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMT6000">
<description>&lt;b&gt;Ambient Light Sensor&lt;/b&gt;
Simple light detection sensor. Output varies with light intensity input. Spark Fun Electronics SKU : COM-08348</description>
<gates>
<gate name="G$1" symbol="TEMT6000-SEN"/>
</gates>
<devices>
<device name="" package="TEMT6000-SEN">
<connects>
<connect gate="G$1" pin="C1" pad="COLLECTOR"/>
<connect gate="G$1" pin="E1" pad="EMITTER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-4X4">
<description>&lt;b&gt;5mm Button Pad&lt;/b&gt;
Proto layout and schematic for 4x4 button pad. Spark Fun Electronics SKU : COM-07835. Compatible common cathode tri-color LED SKU : COM-00105</description>
<gates>
<gate name="G$0" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$1" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$2" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$3" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$4" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$5" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$6" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$7" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$8" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$9" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$10" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$11" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$12" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$13" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$14" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$15" symbol="BUTTONPAD_SINGLE"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-4X4">
<connects>
<connect gate="G$0" pin="BLU" pad="BLU0"/>
<connect gate="G$0" pin="GND" pad="GND0"/>
<connect gate="G$0" pin="GRN" pad="GRN0"/>
<connect gate="G$0" pin="RED" pad="RED0"/>
<connect gate="G$0" pin="SIG1" pad="SIG0"/>
<connect gate="G$0" pin="SIG2" pad="SIG1"/>
<connect gate="G$1" pin="BLU" pad="BLU1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="GRN" pad="GRN1"/>
<connect gate="G$1" pin="RED" pad="RED1"/>
<connect gate="G$1" pin="SIG1" pad="SIG2"/>
<connect gate="G$1" pin="SIG2" pad="SIG3"/>
<connect gate="G$10" pin="BLU" pad="BLU10"/>
<connect gate="G$10" pin="GND" pad="GND10"/>
<connect gate="G$10" pin="GRN" pad="GRN10"/>
<connect gate="G$10" pin="RED" pad="RED10"/>
<connect gate="G$10" pin="SIG1" pad="SIG20"/>
<connect gate="G$10" pin="SIG2" pad="SIG21"/>
<connect gate="G$11" pin="BLU" pad="BLU11"/>
<connect gate="G$11" pin="GND" pad="GND11"/>
<connect gate="G$11" pin="GRN" pad="GRN11"/>
<connect gate="G$11" pin="RED" pad="RED11"/>
<connect gate="G$11" pin="SIG1" pad="SIG22"/>
<connect gate="G$11" pin="SIG2" pad="SIG23"/>
<connect gate="G$12" pin="BLU" pad="BLU12"/>
<connect gate="G$12" pin="GND" pad="GND12"/>
<connect gate="G$12" pin="GRN" pad="GRN12"/>
<connect gate="G$12" pin="RED" pad="RED12"/>
<connect gate="G$12" pin="SIG1" pad="SIG24"/>
<connect gate="G$12" pin="SIG2" pad="SIG25"/>
<connect gate="G$13" pin="BLU" pad="BLU13"/>
<connect gate="G$13" pin="GND" pad="GND13"/>
<connect gate="G$13" pin="GRN" pad="GRN13"/>
<connect gate="G$13" pin="RED" pad="RED13"/>
<connect gate="G$13" pin="SIG1" pad="SIG26"/>
<connect gate="G$13" pin="SIG2" pad="SIG27"/>
<connect gate="G$14" pin="BLU" pad="BLU14"/>
<connect gate="G$14" pin="GND" pad="GND14"/>
<connect gate="G$14" pin="GRN" pad="GRN14"/>
<connect gate="G$14" pin="RED" pad="RED14"/>
<connect gate="G$14" pin="SIG1" pad="SIG28"/>
<connect gate="G$14" pin="SIG2" pad="SIG29"/>
<connect gate="G$15" pin="BLU" pad="BLU15"/>
<connect gate="G$15" pin="GND" pad="GND15"/>
<connect gate="G$15" pin="GRN" pad="GRN15"/>
<connect gate="G$15" pin="RED" pad="RED15"/>
<connect gate="G$15" pin="SIG1" pad="SIG30"/>
<connect gate="G$15" pin="SIG2" pad="SIG31"/>
<connect gate="G$2" pin="BLU" pad="BLU2"/>
<connect gate="G$2" pin="GND" pad="GND2"/>
<connect gate="G$2" pin="GRN" pad="GRN2"/>
<connect gate="G$2" pin="RED" pad="RED2"/>
<connect gate="G$2" pin="SIG1" pad="SIG4"/>
<connect gate="G$2" pin="SIG2" pad="SIG5"/>
<connect gate="G$3" pin="BLU" pad="BLU3"/>
<connect gate="G$3" pin="GND" pad="GND3"/>
<connect gate="G$3" pin="GRN" pad="GRN3"/>
<connect gate="G$3" pin="RED" pad="RED3"/>
<connect gate="G$3" pin="SIG1" pad="SIG6"/>
<connect gate="G$3" pin="SIG2" pad="SIG7"/>
<connect gate="G$4" pin="BLU" pad="BLU4"/>
<connect gate="G$4" pin="GND" pad="GND4"/>
<connect gate="G$4" pin="GRN" pad="GRN4"/>
<connect gate="G$4" pin="RED" pad="RED4"/>
<connect gate="G$4" pin="SIG1" pad="SIG8"/>
<connect gate="G$4" pin="SIG2" pad="SIG9"/>
<connect gate="G$5" pin="BLU" pad="BLU5"/>
<connect gate="G$5" pin="GND" pad="GND5"/>
<connect gate="G$5" pin="GRN" pad="GRN6"/>
<connect gate="G$5" pin="RED" pad="RED5"/>
<connect gate="G$5" pin="SIG1" pad="SIG10"/>
<connect gate="G$5" pin="SIG2" pad="SIG11"/>
<connect gate="G$6" pin="BLU" pad="BLU6"/>
<connect gate="G$6" pin="GND" pad="GND6"/>
<connect gate="G$6" pin="GRN" pad="GRN5"/>
<connect gate="G$6" pin="RED" pad="RED6"/>
<connect gate="G$6" pin="SIG1" pad="SIG12"/>
<connect gate="G$6" pin="SIG2" pad="SIG13"/>
<connect gate="G$7" pin="BLU" pad="BLU7"/>
<connect gate="G$7" pin="GND" pad="GND7"/>
<connect gate="G$7" pin="GRN" pad="GRN7"/>
<connect gate="G$7" pin="RED" pad="RED7"/>
<connect gate="G$7" pin="SIG1" pad="SIG14"/>
<connect gate="G$7" pin="SIG2" pad="SIG15"/>
<connect gate="G$8" pin="BLU" pad="BLU8"/>
<connect gate="G$8" pin="GND" pad="GND8"/>
<connect gate="G$8" pin="GRN" pad="GRN8"/>
<connect gate="G$8" pin="RED" pad="RED8"/>
<connect gate="G$8" pin="SIG1" pad="SIG16"/>
<connect gate="G$8" pin="SIG2" pad="SIG17"/>
<connect gate="G$9" pin="BLU" pad="BLU9"/>
<connect gate="G$9" pin="GND" pad="GND9"/>
<connect gate="G$9" pin="GRN" pad="GRN9"/>
<connect gate="G$9" pin="RED" pad="RED9"/>
<connect gate="G$9" pin="SIG1" pad="SIG18"/>
<connect gate="G$9" pin="SIG2" pad="SIG19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="BUTTONPAD-4X4-SPECIAL">
<connects>
<connect gate="G$0" pin="BLU" pad="BLU0"/>
<connect gate="G$0" pin="GND" pad="GND0"/>
<connect gate="G$0" pin="GRN" pad="GRN0"/>
<connect gate="G$0" pin="RED" pad="RED0"/>
<connect gate="G$0" pin="SIG1" pad="SIG0"/>
<connect gate="G$0" pin="SIG2" pad="SIG1"/>
<connect gate="G$1" pin="BLU" pad="BLU1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="GRN" pad="GRN1"/>
<connect gate="G$1" pin="RED" pad="RED1"/>
<connect gate="G$1" pin="SIG1" pad="SIG2"/>
<connect gate="G$1" pin="SIG2" pad="SIG3"/>
<connect gate="G$10" pin="BLU" pad="BLU10"/>
<connect gate="G$10" pin="GND" pad="GND10"/>
<connect gate="G$10" pin="GRN" pad="GRN10"/>
<connect gate="G$10" pin="RED" pad="RED10"/>
<connect gate="G$10" pin="SIG1" pad="SIG20"/>
<connect gate="G$10" pin="SIG2" pad="SIG21"/>
<connect gate="G$11" pin="BLU" pad="BLU11"/>
<connect gate="G$11" pin="GND" pad="GND11"/>
<connect gate="G$11" pin="GRN" pad="GRN11"/>
<connect gate="G$11" pin="RED" pad="RED11"/>
<connect gate="G$11" pin="SIG1" pad="SIG22"/>
<connect gate="G$11" pin="SIG2" pad="SIG23"/>
<connect gate="G$12" pin="BLU" pad="BLU12"/>
<connect gate="G$12" pin="GND" pad="GND12"/>
<connect gate="G$12" pin="GRN" pad="GRN12"/>
<connect gate="G$12" pin="RED" pad="RED12"/>
<connect gate="G$12" pin="SIG1" pad="SIG24"/>
<connect gate="G$12" pin="SIG2" pad="SIG25"/>
<connect gate="G$13" pin="BLU" pad="BLU13"/>
<connect gate="G$13" pin="GND" pad="GND13"/>
<connect gate="G$13" pin="GRN" pad="GRN13"/>
<connect gate="G$13" pin="RED" pad="RED13"/>
<connect gate="G$13" pin="SIG1" pad="SIG26"/>
<connect gate="G$13" pin="SIG2" pad="SIG27"/>
<connect gate="G$14" pin="BLU" pad="BLU14"/>
<connect gate="G$14" pin="GND" pad="GND14"/>
<connect gate="G$14" pin="GRN" pad="GRN14"/>
<connect gate="G$14" pin="RED" pad="RED14"/>
<connect gate="G$14" pin="SIG1" pad="SIG28"/>
<connect gate="G$14" pin="SIG2" pad="SIG29"/>
<connect gate="G$15" pin="BLU" pad="BLU15"/>
<connect gate="G$15" pin="GND" pad="GND15"/>
<connect gate="G$15" pin="GRN" pad="GRN15"/>
<connect gate="G$15" pin="RED" pad="RED15"/>
<connect gate="G$15" pin="SIG1" pad="SIG30"/>
<connect gate="G$15" pin="SIG2" pad="SIG31"/>
<connect gate="G$2" pin="BLU" pad="BLU2"/>
<connect gate="G$2" pin="GND" pad="GND2"/>
<connect gate="G$2" pin="GRN" pad="GRN2"/>
<connect gate="G$2" pin="RED" pad="RED2"/>
<connect gate="G$2" pin="SIG1" pad="SIG4"/>
<connect gate="G$2" pin="SIG2" pad="SIG5"/>
<connect gate="G$3" pin="BLU" pad="BLU3"/>
<connect gate="G$3" pin="GND" pad="GND3"/>
<connect gate="G$3" pin="GRN" pad="GRN3"/>
<connect gate="G$3" pin="RED" pad="RED3"/>
<connect gate="G$3" pin="SIG1" pad="SIG6"/>
<connect gate="G$3" pin="SIG2" pad="SIG7"/>
<connect gate="G$4" pin="BLU" pad="BLU4"/>
<connect gate="G$4" pin="GND" pad="GND4"/>
<connect gate="G$4" pin="GRN" pad="GRN4"/>
<connect gate="G$4" pin="RED" pad="RED4"/>
<connect gate="G$4" pin="SIG1" pad="SIG8"/>
<connect gate="G$4" pin="SIG2" pad="SIG9"/>
<connect gate="G$5" pin="BLU" pad="BLU5"/>
<connect gate="G$5" pin="GND" pad="GND5"/>
<connect gate="G$5" pin="GRN" pad="GRN6"/>
<connect gate="G$5" pin="RED" pad="RED5"/>
<connect gate="G$5" pin="SIG1" pad="SIG10"/>
<connect gate="G$5" pin="SIG2" pad="SIG11"/>
<connect gate="G$6" pin="BLU" pad="BLU6"/>
<connect gate="G$6" pin="GND" pad="GND6"/>
<connect gate="G$6" pin="GRN" pad="GRN5"/>
<connect gate="G$6" pin="RED" pad="RED6"/>
<connect gate="G$6" pin="SIG1" pad="SIG12"/>
<connect gate="G$6" pin="SIG2" pad="SIG13"/>
<connect gate="G$7" pin="BLU" pad="BLU7"/>
<connect gate="G$7" pin="GND" pad="GND7"/>
<connect gate="G$7" pin="GRN" pad="GRN7"/>
<connect gate="G$7" pin="RED" pad="RED7"/>
<connect gate="G$7" pin="SIG1" pad="SIG14"/>
<connect gate="G$7" pin="SIG2" pad="SIG15"/>
<connect gate="G$8" pin="BLU" pad="BLU8"/>
<connect gate="G$8" pin="GND" pad="GND8"/>
<connect gate="G$8" pin="GRN" pad="GRN8"/>
<connect gate="G$8" pin="RED" pad="RED8"/>
<connect gate="G$8" pin="SIG1" pad="SIG16"/>
<connect gate="G$8" pin="SIG2" pad="SIG17"/>
<connect gate="G$9" pin="BLU" pad="BLU9"/>
<connect gate="G$9" pin="GND" pad="GND9"/>
<connect gate="G$9" pin="GRN" pad="GRN9"/>
<connect gate="G$9" pin="RED" pad="RED9"/>
<connect gate="G$9" pin="SIG1" pad="SIG18"/>
<connect gate="G$9" pin="SIG2" pad="SIG19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M05X2" prefix="JP">
<description>&lt;b&gt;Header 5x2&lt;/b&gt;
Standard 10-pin dual row 0.1" header. Commonly used with AVR-ISP. Use with Spark Fun Electronics SKU: PRT-00778</description>
<gates>
<gate name="G$1" symbol="M05X2"/>
</gates>
<devices>
<device name="PTH" package="AVR_ICSP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="2X5-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAF" package="2X5-RAF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD" package="2X5-SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD_LOCK" package="2X5-SHROUDED_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD_SMD" package="2X5-SHROUDED_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL" prefix="JP">
<description>&lt;b&gt;Fiducial Alignment Points&lt;/b&gt;
Various fiducial points for machine vision alignment.</description>
<gates>
<gate name="G$1" symbol="FIDUCIAL"/>
</gates>
<devices>
<device name="1.5X3" package="FIDUCIAL-1.5X3">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X2" package="FIDUCIAL-1X2">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X2.5" package="FIDUCIAL-1X2.5">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UFIDUCIAL" package="MICRO-FIDUCIAL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GR-10">
<description>&lt;b&gt;GR-10 GPS Receiver Module&lt;/b&gt;
Proto layout and schematic for GR-10 GPS receiver. Spark Fun Electronics SKU : GPS-08291</description>
<gates>
<gate name="G$1" symbol="GR-10"/>
</gates>
<devices>
<device name="SMD" package="GR-10">
<connects>
<connect gate="G$1" pin="1.8V@10" pad="10"/>
<connect gate="G$1" pin="1.8V@21" pad="21"/>
<connect gate="G$1" pin="1.8V@3" pad="3"/>
<connect gate="G$1" pin="1.8VIF" pad="26"/>
<connect gate="G$1" pin="1.8VLNA" pad="28"/>
<connect gate="G$1" pin="1.8VRF" pad="34"/>
<connect gate="G$1" pin="1.8VVCO" pad="25"/>
<connect gate="G$1" pin="1PPS" pad="9"/>
<connect gate="G$1" pin="3V" pad="33"/>
<connect gate="G$1" pin="ANT" pad="30"/>
<connect gate="G$1" pin="APIO_A4" pad="16"/>
<connect gate="G$1" pin="FREF" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@31" pad="31"/>
<connect gate="G$1" pin="GPIO_A11" pad="12"/>
<connect gate="G$1" pin="GPIO_A5" pad="13"/>
<connect gate="G$1" pin="GPIO_A6" pad="14"/>
<connect gate="G$1" pin="GPIO_A9" pad="15"/>
<connect gate="G$1" pin="GPIO_B16" pad="22"/>
<connect gate="G$1" pin="GPIO_B19" pad="19"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="RFEN" pad="32"/>
<connect gate="G$1" pin="RTC_XIN" pad="17"/>
<connect gate="G$1" pin="RTC_XOUT" pad="18"/>
<connect gate="G$1" pin="RX0" pad="7"/>
<connect gate="G$1" pin="RX1" pad="5"/>
<connect gate="G$1" pin="SB" pad="4"/>
<connect gate="G$1" pin="TPI" pad="35"/>
<connect gate="G$1" pin="TPQ" pad="36"/>
<connect gate="G$1" pin="TX0" pad="8"/>
<connect gate="G$1" pin="TX1" pad="6"/>
<connect gate="G$1" pin="VALID_FIX" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5V">
<gates>
<gate name="G$1" symbol="5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-2X2SINGLE">
<description>&lt;b&gt;5mm Button Pad&lt;/b&gt;
Proto layout and schematic for 2x2 button pad with single color LEDs (used on Simon board). Panelize this device/fp to a 4x4 pad if needed. Any single-color 5mm LED should be compatible. Spark Fun Electronics SKU : COM-07835.</description>
<gates>
<gate name="C1" symbol="BUTTONPAD_1LED"/>
<gate name="C2" symbol="BUTTONPAD_1LED"/>
<gate name="C3" symbol="BUTTONPAD_1LED"/>
<gate name="C4" symbol="BUTTONPAD_1LED"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-2X2SINGLE">
<connects>
<connect gate="C1" pin="A" pad="A1"/>
<connect gate="C1" pin="K" pad="K1"/>
<connect gate="C1" pin="SIG1" pad="SIG1"/>
<connect gate="C1" pin="SIG2" pad="SIG2"/>
<connect gate="C2" pin="A" pad="A2"/>
<connect gate="C2" pin="K" pad="K2"/>
<connect gate="C2" pin="SIG1" pad="SIG3"/>
<connect gate="C2" pin="SIG2" pad="SIG4"/>
<connect gate="C3" pin="A" pad="A3"/>
<connect gate="C3" pin="K" pad="K3"/>
<connect gate="C3" pin="SIG1" pad="SIG5"/>
<connect gate="C3" pin="SIG2" pad="SIG6"/>
<connect gate="C4" pin="A" pad="A4"/>
<connect gate="C4" pin="K" pad="K4"/>
<connect gate="C4" pin="SIG1" pad="SIG7"/>
<connect gate="C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="BUTTONPAD-2X2SINGLE-KIT">
<connects>
<connect gate="C1" pin="A" pad="A1"/>
<connect gate="C1" pin="K" pad="K1"/>
<connect gate="C1" pin="SIG1" pad="SIG1"/>
<connect gate="C1" pin="SIG2" pad="SIG2"/>
<connect gate="C2" pin="A" pad="A2"/>
<connect gate="C2" pin="K" pad="K2"/>
<connect gate="C2" pin="SIG1" pad="SIG3"/>
<connect gate="C2" pin="SIG2" pad="SIG4"/>
<connect gate="C3" pin="A" pad="A3"/>
<connect gate="C3" pin="K" pad="K3"/>
<connect gate="C3" pin="SIG1" pad="SIG5"/>
<connect gate="C3" pin="SIG2" pad="SIG6"/>
<connect gate="C4" pin="A" pad="A4"/>
<connect gate="C4" pin="K" pad="K4"/>
<connect gate="C4" pin="SIG1" pad="SIG7"/>
<connect gate="C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-NCHANNEL" prefix="Q">
<gates>
<gate name="G$1" symbol="MOSFET-NCHANNEL"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FDD8580" package="DPAK">
<connects>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="TO220V">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP2551" prefix="U">
<gates>
<gate name="G$1" symbol="MCP2551"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX323" prefix="U">
<gates>
<gate name="G$1" symbol="MAX323"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="3"/>
<connect gate="G$1" pin="NO1" pad="1"/>
<connect gate="G$1" pin="NO2" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G3VM-61E1">
<gates>
<gate name="G$1" symbol="G3VM-61E1"/>
</gates>
<devices>
<device name="" package="G3VM-61E1">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ11-6" prefix="J">
<description>&lt;b&gt;RJ11 Jack&lt;/b&gt;
Simple 6 pin RJ11 jack. Commonly found on CAT3 devices and Microchip programmers. SKU: PRT-00132</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="PTH" package="RJ11-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STAND-OFF" prefix="JP">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
<gates>
<gate name="G$1" symbol="STAND-OFF"/>
</gates>
<devices>
<device name="" package="STAND-OFF">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TIGHT" package="STAND-OFF-TIGHT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOTOR">
<description>&lt;b&gt;Vibration Motor&lt;/b&gt;
Physical dimension and wire connections for this powerful vibration motor. Motor has a self adhesive backing. Spark Fun Electronics SKU : ROB-08449</description>
<gates>
<gate name="G$1" symbol="MOTOR"/>
</gates>
<devices>
<device name="10MM" package="VIBE-MOTOR-10MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM408_CON" prefix="U">
<description>This is the mating connector for the EM408 GPS receiver.  The EM408 connects to the board via a cable, 
this connector footprint does not include the outline of the receiver.

You should include the "EM408_Outline" device in your schematic if you are to use the EM408 in your design.</description>
<gates>
<gate name="G$1" symbol="EM408_CON"/>
</gates>
<devices>
<device name="" package="EM408_CON">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M16" prefix="JP">
<gates>
<gate name="G$1" symbol="M16"/>
</gates>
<devices>
<device name="PTH" package="1X16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X16_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X16_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MACHIINE-PIN_LOCK" package="1X16_MACHINE-PIN-HEADER_LOCK.004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X16_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREADBOARD">
<description>&lt;b&gt;Breadboard Mini Self Adhesive&lt;/b&gt;&lt;p&gt;
This is the mechnical outline for the very small self adhesive breadboard from SparkFun Electronics. Good for very small proto areas. SKU : PRT-07916</description>
<gates>
<gate name="G$1" symbol="BREADBOARD"/>
</gates>
<devices>
<device name="MINI" package="BREADBOARD-MINI">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NS73M" prefix="U">
<description>&lt;b&gt;FM Transmitter&lt;/b&gt;
2mW transmitter NS73M. Easy SPI interface. Digital tuning. SKU: WRL-08452</description>
<gates>
<gate name="G$1" symbol="NS73M"/>
</gates>
<devices>
<device name="SMD" package="NS73M">
<connects>
<connect gate="G$1" pin="CK" pad="5"/>
<connect gate="G$1" pin="DA" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="IIC" pad="8"/>
<connect gate="G$1" pin="LA" pad="7"/>
<connect gate="G$1" pin="LIN" pad="12"/>
<connect gate="G$1" pin="PWE" pad="4"/>
<connect gate="G$1" pin="RFO" pad="15"/>
<connect gate="G$1" pin="RIN" pad="13"/>
<connect gate="G$1" pin="TEB" pad="3"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VDRF" pad="2"/>
<connect gate="G$1" pin="X1" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO-JACK" prefix="U" uservalue="yes">
<description>&lt;b&gt;3.5mm Audio Jack&lt;/b&gt;
Simple 3.5mm common PCB mount audio jack. SKU: PRT-08032</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK"/>
</gates>
<devices>
<device name="PTH" package="AUDIO-JACK">
<connects>
<connect gate="G$1" pin="LEFT" pad="TIP"/>
<connect gate="G$1" pin="RIGHT" pad="RING"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.5MM" package="STEREOJACK2.5MM_STEREOJACK2.5MM">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL_POGO_PINS" package="STEREOJACK2.5MM_SPECIA_POGOPINS">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HOLESONLY" package="STEREOJACK2.5MM_SPECIAL_HOLES-ONLY">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="STEREOJACK2.5MM_SMD">
<connects>
<connect gate="G$1" pin="LEFT" pad="1"/>
<connect gate="G$1" pin="RIGHT" pad="4"/>
<connect gate="G$1" pin="SLEEVE" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="AUDIO-JACK-3.5MM-SMD">
<connects>
<connect gate="G$1" pin="LEFT" pad="TIP"/>
<connect gate="G$1" pin="RIGHT" pad="RING"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM-I2C">
<gates>
<gate name="G$1" symbol="EEPROM-I2C"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MINI-DIN6">
<description>&lt;b&gt;mini DIN 6 Connector&lt;/b&gt;
Commonly found on the back of a computer for PS2 keyboard and mice. Schematic and footprint are proven. Spark Fun Electronics SKU : PRT-08509</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="PTH" package="MINI-DIN6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPAMP-DUAL" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="DIP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="DIP"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON">
<description>&lt;b&gt;Luxeon LED&lt;/b&gt;
This footprint works with the current 1 Watt, 3 Watt, and 5 Watt LEDs. These blindingly bright LEDs generate a lot of heat so the footprint has a large pad under the LED for thermal transfer. Schematic and footprint are proven. Spark Fun Electronics SKU : COM-00603</description>
<gates>
<gate name="G$1" symbol="LUXEON"/>
</gates>
<devices>
<device name="SMD" package="LUXEON">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24AP1" prefix="U">
<description>&lt;b&gt;2.4GHz ANT IC&lt;/b&gt;
Nordic Semiconductor 2.4GHz transceiver that implements the ANT protocol.</description>
<gates>
<gate name="G$1" symbol="NRF24AP1"/>
</gates>
<devices>
<device name="SMD" package="MLP-24">
<connects>
<connect gate="G$1" pin="ANT1" pad="14"/>
<connect gate="G$1" pin="ANT2" pad="15"/>
<connect gate="G$1" pin="BR1" pad="2"/>
<connect gate="G$1" pin="BR2" pad="1"/>
<connect gate="G$1" pin="DVDD" pad="9"/>
<connect gate="G$1" pin="EXT32K" pad="3"/>
<connect gate="G$1" pin="IREF" pad="19"/>
<connect gate="G$1" pin="PORTSEL" pad="23"/>
<connect gate="G$1" pin="RTS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SLEEP" pad="6"/>
<connect gate="G$1" pin="SUSPEND" pad="7"/>
<connect gate="G$1" pin="TXD" pad="5"/>
<connect gate="G$1" pin="VDD@17" pad="17"/>
<connect gate="G$1" pin="VDD@21" pad="21"/>
<connect gate="G$1" pin="VDD@24" pad="24"/>
<connect gate="G$1" pin="VDD_PA" pad="13"/>
<connect gate="G$1" pin="VSS@0" pad="0"/>
<connect gate="G$1" pin="VSS@10" pad="10"/>
<connect gate="G$1" pin="VSS@18" pad="18"/>
<connect gate="G$1" pin="VSS@20" pad="20"/>
<connect gate="G$1" pin="VSS@22" pad="22"/>
<connect gate="G$1" pin="VSS_PA" pad="16"/>
<connect gate="G$1" pin="XC1" pad="12"/>
<connect gate="G$1" pin="XC2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_SPI_PRG_6" prefix="J">
<description>&lt;b&gt;AVR ISP 6 Pin&lt;/b&gt;
This is the reduced ISP connector for AVR programming. Common on Arduino. This footprint will take up less PCB space and can be used with a 10-pin to 6-pin adapter such as SKU: BOB-08508</description>
<gates>
<gate name="G$1" symbol="AVR_SPI_PROGRAMMER_6"/>
</gates>
<devices>
<device name="PTH" package="2X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NS" package="2X3-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OFFSET_PADS" package="2X3_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X3_LOCK" package="2X3_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEST-POINT" prefix="TP">
<gates>
<gate name="G$1" symbol="TEST-POINT"/>
</gates>
<devices>
<device name="2" package="PAD.02X.02">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3" package="PAD.03X.03">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3X5" package="PAD.03X.05">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIAC">
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="M1" pad="1"/>
<connect gate="G$1" pin="M2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOT223">
<connects>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="M1" pad="1"/>
<connect gate="G$1" pin="M2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ALM-1412">
<description>&lt;b&gt;GPS Antenna Amp&lt;/b&gt;
Filter and Amp built into one. Very small package.</description>
<gates>
<gate name="G$1" symbol="ALM-1412"/>
</gates>
<devices>
<device name="SMD" package="ALM-1412">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="5"/>
<connect gate="G$1" pin="RF_OUT" pad="3"/>
<connect gate="G$1" pin="SD" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI4700">
<description>&lt;b&gt;Silicon Labs FM Receiver&lt;/b&gt;&lt;p&gt;
76-108 MHz FM band support with integrated VCO, automatic gain control, automatic frequency control and seek tuning.</description>
<gates>
<gate name="G$1" symbol="SI4700/01-GM"/>
</gates>
<devices>
<device name="SMD" package="SI4700/01-GM">
<connects>
<connect gate="G$1" pin="FMIN" pad="4"/>
<connect gate="G$1" pin="FMIP" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="6"/>
<connect gate="G$1" pin="GND3" pad="14"/>
<connect gate="G$1" pin="GND4" pad="17"/>
<connect gate="G$1" pin="GND5" pad="24"/>
<connect gate="G$1" pin="GND@0" pad="0"/>
<connect gate="G$1" pin="GPIO1" pad="21"/>
<connect gate="G$1" pin="GPIO2" pad="20"/>
<connect gate="G$1" pin="GPIO3" pad="19"/>
<connect gate="G$1" pin="LOUT" pad="16"/>
<connect gate="G$1" pin="RCLK" pad="11"/>
<connect gate="G$1" pin="RFGND" pad="3"/>
<connect gate="G$1" pin="ROUT" pad="15"/>
<connect gate="G$1" pin="RST" pad="7"/>
<connect gate="G$1" pin="SCLK" pad="9"/>
<connect gate="G$1" pin="SDIO" pad="10"/>
<connect gate="G$1" pin="SEN" pad="8"/>
<connect gate="G$1" pin="VA" pad="18"/>
<connect gate="G$1" pin="VD" pad="13"/>
<connect gate="G$1" pin="VIO" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X26">
<gates>
<gate name="G$1" symbol="PINH2X26"/>
</gates>
<devices>
<device name="" package="2X26">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24L01">
<description>&lt;b&gt;2.4GHz Low Power Transceiver&lt;/b&gt;
This is the very popular, low cost, very low power RF transceiver from Nordic Semiconductor. Simple SPI interface. SKU: COM-00690</description>
<gates>
<gate name="G$1" symbol="NRF24L01-1"/>
</gates>
<devices>
<device name="SMD" package="QFN20">
<connects>
<connect gate="G$1" pin="ANT1" pad="12"/>
<connect gate="G$1" pin="ANT2" pad="13"/>
<connect gate="G$1" pin="CE" pad="1"/>
<connect gate="G$1" pin="CSN" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="19"/>
<connect gate="G$1" pin="IREF" pad="16"/>
<connect gate="G$1" pin="IRQ" pad="6"/>
<connect gate="G$1" pin="MISO" pad="5"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VDD@15" pad="15"/>
<connect gate="G$1" pin="VDD@18" pad="18"/>
<connect gate="G$1" pin="VDD@7" pad="7"/>
<connect gate="G$1" pin="VDD_PA" pad="11"/>
<connect gate="G$1" pin="VSS@0" pad="0"/>
<connect gate="G$1" pin="VSS@14" pad="14"/>
<connect gate="G$1" pin="VSS@17" pad="17"/>
<connect gate="G$1" pin="VSS@20" pad="20"/>
<connect gate="G$1" pin="VSS@8" pad="8"/>
<connect gate="G$1" pin="XC1" pad="10"/>
<connect gate="G$1" pin="XC2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF2401A">
<description>&lt;b&gt;2.4GHz Transceiver&lt;/b&gt;
This is the very popular, low power RF transceiver from Nordic Semiconductor. Used in the Nike+iPod product. SKU: COM-00300</description>
<gates>
<gate name="G$1" symbol="NRF2401A"/>
</gates>
<devices>
<device name="SMD" package="MLP-24">
<connects>
<connect gate="G$1" pin="ANT1" pad="14"/>
<connect gate="G$1" pin="ANT2" pad="15"/>
<connect gate="G$1" pin="CE" pad="1"/>
<connect gate="G$1" pin="CLK1" pad="7"/>
<connect gate="G$1" pin="CLK2" pad="3"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DATA" pad="8"/>
<connect gate="G$1" pin="DOUT2" pad="4"/>
<connect gate="G$1" pin="DR1" pad="6"/>
<connect gate="G$1" pin="DR2" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="9"/>
<connect gate="G$1" pin="IREF" pad="19"/>
<connect gate="G$1" pin="PWR_UP" pad="23"/>
<connect gate="G$1" pin="VDD@17" pad="17"/>
<connect gate="G$1" pin="VDD@21" pad="21"/>
<connect gate="G$1" pin="VDD@24" pad="24"/>
<connect gate="G$1" pin="VDD_PA" pad="13"/>
<connect gate="G$1" pin="VSS@0" pad="0"/>
<connect gate="G$1" pin="VSS@10" pad="10"/>
<connect gate="G$1" pin="VSS@18" pad="18"/>
<connect gate="G$1" pin="VSS@20" pad="20"/>
<connect gate="G$1" pin="VSS@22" pad="22"/>
<connect gate="G$1" pin="VSS_PA" pad="16"/>
<connect gate="G$1" pin="XC1" pad="12"/>
<connect gate="G$1" pin="XC2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY24">
<gates>
<gate name="G$1" symbol="ATTINY24"/>
</gates>
<devices>
<device name="QFN" package="QFN20">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@0" pad="0"/>
<connect gate="G$1" pin="PA0/ADC0" pad="5"/>
<connect gate="G$1" pin="PA1/ADC1" pad="4"/>
<connect gate="G$1" pin="PA2/ADC2" pad="3"/>
<connect gate="G$1" pin="PA3/ADC3" pad="2"/>
<connect gate="G$1" pin="PA4/SCL" pad="1"/>
<connect gate="G$1" pin="PA5/MISO" pad="20"/>
<connect gate="G$1" pin="PA6/MOSI" pad="16"/>
<connect gate="G$1" pin="PA7/ADC7" pad="15"/>
<connect gate="G$1" pin="PB0" pad="11"/>
<connect gate="G$1" pin="PB1" pad="12"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3/RESET" pad="13"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTON-CONDUCTIVE">
<description>&lt;b&gt;Conductive Button&lt;/b&gt;
Used with rubber key pads. This one was designed and proven to work with the PolyCase Key FOB enclosures.</description>
<gates>
<gate name="G$1" symbol="BUTTON-CONDUCTIVE"/>
</gates>
<devices>
<device name="SMD" package="BUTTON-CONDUCTIVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-0.1&quot;" package="BUTTON-CONDUCTIVE-0.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="BUTTON-CONDUCTIVE-MINI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADJD_COLOR_SENSOR" uservalue="yes">
<description>&lt;b&gt;Color Light Sensor&lt;/b&gt;
ADJD-S371 from Avago. Digital RGB light sensor (I2C) with on-board white LED. Not quite proven footprint or schematic component. SKU: COM-08618</description>
<gates>
<gate name="G$1" symbol="ADJD"/>
</gates>
<devices>
<device name="_SMD" package="ADJD-S371">
<connects>
<connect gate="G$1" pin="+VE" pad="3"/>
<connect gate="G$1" pin="-VE" pad="1"/>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="7"/>
<connect gate="G$1" pin="DGND" pad="11"/>
<connect gate="G$1" pin="DVDD" pad="5"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SLEEP" pad="8"/>
<connect gate="G$1" pin="XCLK" pad="12"/>
<connect gate="G$1" pin="XRST" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC1051Z">
<gates>
<gate name="G$1" symbol="HMC1051Z"/>
</gates>
<devices>
<device name="2" package="HMC1051Z_2">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="S/R+" pad="6"/>
<connect gate="G$1" pin="S/R-" pad="7"/>
<connect gate="G$1" pin="V0+" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VO-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="HMC1051Z3">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="S/R+" pad="6"/>
<connect gate="G$1" pin="S/R-" pad="7"/>
<connect gate="G$1" pin="V0+" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VO-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF7507">
<gates>
<gate name="G$1" symbol="IRF7507"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="D1@7" pad="7"/>
<connect gate="G$1" pin="D1@8" pad="8"/>
<connect gate="G$1" pin="D2@5" pad="5"/>
<connect gate="G$1" pin="D2@6" pad="6"/>
<connect gate="G$1" pin="G1" pad="2"/>
<connect gate="G$1" pin="G2" pad="4"/>
<connect gate="G$1" pin="S1" pad="1"/>
<connect gate="G$1" pin="S2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV358">
<gates>
<gate name="G$1" symbol="OPAMP_2"/>
<gate name="G$2" symbol="OPAMP_2_1"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+IN1" pad="3"/>
<connect gate="G$1" pin="+V" pad="8"/>
<connect gate="G$1" pin="-IN1" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$2" pin="+IN2" pad="5"/>
<connect gate="G$2" pin="-IN2" pad="6"/>
<connect gate="G$2" pin="OUT2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V-REFERENCE">
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCA1000">
<gates>
<gate name="G$1" symbol="SCA1000"/>
</gates>
<devices>
<device name="" package="SCA1000">
<connects>
<connect gate="G$1" pin="CSB" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="3"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="N/C@2" pad="2"/>
<connect gate="G$1" pin="N/C@8" pad="8"/>
<connect gate="G$1" pin="OUTX" pad="11"/>
<connect gate="G$1" pin="OUTY" pad="5"/>
<connect gate="G$1" pin="SCK" pad="1"/>
<connect gate="G$1" pin="ST1" pad="10"/>
<connect gate="G$1" pin="ST2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XC3S250/500E-PQ208">
<gates>
<gate name="G$1" symbol="XC3S250/500E-PQ208"/>
</gates>
<devices>
<device name="" package="PQ208">
<connects>
<connect gate="G$1" pin="10_L08P_2/D7/GCLK12" pad="74"/>
<connect gate="G$1" pin="DONE" pad="104"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="GND@10" pad="95"/>
<connect gate="G$1" pin="GND@11" pad="105"/>
<connect gate="G$1" pin="GND@12" pad="121"/>
<connect gate="G$1" pin="GND@13" pad="131"/>
<connect gate="G$1" pin="GND@14" pad="141"/>
<connect gate="G$1" pin="GND@15" pad="156"/>
<connect gate="G$1" pin="GND@16" pad="173"/>
<connect gate="G$1" pin="GND@17" pad="182"/>
<connect gate="G$1" pin="GND@18" pad="188"/>
<connect gate="G$1" pin="GND@19" pad="198"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@20" pad="208"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="37"/>
<connect gate="G$1" pin="GND@5" pad="52"/>
<connect gate="G$1" pin="GND@6" pad="53"/>
<connect gate="G$1" pin="GND@7" pad="70"/>
<connect gate="G$1" pin="GND@8" pad="79"/>
<connect gate="G$1" pin="GND@9" pad="85"/>
<connect gate="G$1" pin="IO" pad="187"/>
<connect gate="G$1" pin="IO/D5" pad="76"/>
<connect gate="G$1" pin="IO/L01N_2/INIT_B" pad="56"/>
<connect gate="G$1" pin="IO/M1" pad="84"/>
<connect gate="G$1" pin="IO/VREF_0" pad="179"/>
<connect gate="G$1" pin="IO/VREF_2" pad="98"/>
<connect gate="G$1" pin="IO/VREF_3" pad="45"/>
<connect gate="G$1" pin="IO_16P_1/LDC1" pad="152"/>
<connect gate="G$1" pin="IO_L01N_0" pad="161"/>
<connect gate="G$1" pin="IO_L01N_1/A15" pad="107"/>
<connect gate="G$1" pin="IO_L01N_3" pad="3"/>
<connect gate="G$1" pin="IO_L01P_0" pad="160"/>
<connect gate="G$1" pin="IO_L01P_1/A16" pad="106"/>
<connect gate="G$1" pin="IO_L01P_2/CSO_B" pad="55"/>
<connect gate="G$1" pin="IO_L01P_3" pad="2"/>
<connect gate="G$1" pin="IO_L02N_0/VREF_0" pad="163"/>
<connect gate="G$1" pin="IO_L02N_1/A13" pad="109"/>
<connect gate="G$1" pin="IO_L02N_3/VREF_3" pad="5"/>
<connect gate="G$1" pin="IO_L02P_0" pad="162"/>
<connect gate="G$1" pin="IO_L02P_1/A14" pad="108"/>
<connect gate="G$1" pin="IO_L02P_3" pad="4"/>
<connect gate="G$1" pin="IO_L03N_0" pad="165"/>
<connect gate="G$1" pin="IO_L03N_1/VREF_1" pad="113"/>
<connect gate="G$1" pin="IO_L03N_2/MOSI/CSI_B" pad="61"/>
<connect gate="G$1" pin="IO_L03N_3" pad="9"/>
<connect gate="G$1" pin="IO_L03P_0" pad="164"/>
<connect gate="G$1" pin="IO_L03P_1" pad="112"/>
<connect gate="G$1" pin="IO_L03P_2/DOUT/BUSY" pad="60"/>
<connect gate="G$1" pin="IO_L03P_3" pad="8"/>
<connect gate="G$1" pin="IO_L04N_0/VREF_0" pad="168"/>
<connect gate="G$1" pin="IO_L04N_1" pad="116"/>
<connect gate="G$1" pin="IO_L04N_2" pad="63"/>
<connect gate="G$1" pin="IO_L04N_3" pad="12"/>
<connect gate="G$1" pin="IO_L04P_0" pad="167"/>
<connect gate="G$1" pin="IO_L04P_1" pad="115"/>
<connect gate="G$1" pin="IO_L04P_2" pad="62"/>
<connect gate="G$1" pin="IO_L04P_3" pad="11"/>
<connect gate="G$1" pin="IO_L05N_0" pad="172"/>
<connect gate="G$1" pin="IO_L05N_1/A11" pad="120"/>
<connect gate="G$1" pin="IO_L05N_2" pad="65"/>
<connect gate="G$1" pin="IO_L05N_3" pad="16"/>
<connect gate="G$1" pin="IO_L05P_0" pad="171"/>
<connect gate="G$1" pin="IO_L05P_1/A12" pad="119"/>
<connect gate="G$1" pin="IO_L05P_2" pad="64"/>
<connect gate="G$1" pin="IO_L05P_3" pad="15"/>
<connect gate="G$1" pin="IO_L06N_1/VREF_1" pad="123"/>
<connect gate="G$1" pin="IO_L06N_2" pad="69"/>
<connect gate="G$1" pin="IO_L06N_3" pad="19"/>
<connect gate="G$1" pin="IO_L06P_1" pad="122"/>
<connect gate="G$1" pin="IO_L06P_2" pad="68"/>
<connect gate="G$1" pin="IO_L06P_3" pad="18"/>
<connect gate="G$1" pin="IO_L07N_0/GCLK5" pad="178"/>
<connect gate="G$1" pin="IO_L07N_1/A7/RHCLK1" pad="127"/>
<connect gate="G$1" pin="IO_L07N_3/LHCLK1" pad="23"/>
<connect gate="G$1" pin="IO_L07P_1/A10/RHCLK0" pad="126"/>
<connect gate="G$1" pin="IO_L07P_3/LHCLK0" pad="22"/>
<connect gate="G$1" pin="IO_L08N_0/GCLK7" pad="181"/>
<connect gate="G$1" pin="IO_L08N_1/A7/RHCLK3" pad="129"/>
<connect gate="G$1" pin="IO_L08N_2/D6/GCLK13" pad="75"/>
<connect gate="G$1" pin="IO_L08N_3/LHCLK3" pad="25"/>
<connect gate="G$1" pin="IO_L08P_0/GCLK6" pad="180"/>
<connect gate="G$1" pin="IO_L08P_1/A8/RHCLK2" pad="128"/>
<connect gate="G$1" pin="IO_L08P_3/LHCLK2" pad="24"/>
<connect gate="G$1" pin="IO_L09N_1/A5/RHCLK5" pad="133"/>
<connect gate="G$1" pin="IO_L09N_2/D3/GCLK15" pad="78"/>
<connect gate="G$1" pin="IO_L09N_3/LHCLK5" pad="29"/>
<connect gate="G$1" pin="IO_L09P_1/A6/RHCLK4" pad="132"/>
<connect gate="G$1" pin="IO_L09P_2/D4/GCLK14" pad="77"/>
<connect gate="G$1" pin="IO_L09P_3/LHCLK4" pad="28"/>
<connect gate="G$1" pin="IO_L10N_0/GCLK11" pad="186"/>
<connect gate="G$1" pin="IO_L10N_1/A3/RHCLK7" pad="135"/>
<connect gate="G$1" pin="IO_L10N_3/LHCLK7" pad="31"/>
<connect gate="G$1" pin="IO_L10P_0/GCLK10" pad="185"/>
<connect gate="G$1" pin="IO_L10P_1/A4/RHCLK6" pad="134"/>
<connect gate="G$1" pin="IO_L10P_3/LHCLK6" pad="30"/>
<connect gate="G$1" pin="IO_L11N_0" pad="190"/>
<connect gate="G$1" pin="IO_L11N_1/A1" pad="138"/>
<connect gate="G$1" pin="IO_L11N_2/D1/GCLK3" pad="83"/>
<connect gate="G$1" pin="IO_L11N_3" pad="34"/>
<connect gate="G$1" pin="IO_L11P_0" pad="189"/>
<connect gate="G$1" pin="IO_L11P_1/A2" pad="137"/>
<connect gate="G$1" pin="IO_L11P_2/D2/GCLK2" pad="82"/>
<connect gate="G$1" pin="IO_L11P_3" pad="33"/>
<connect gate="G$1" pin="IO_L12N_0/VREF_0" pad="193"/>
<connect gate="G$1" pin="IO_L12N_1/A0" pad="140"/>
<connect gate="G$1" pin="IO_L12N_2/DIN/D0" pad="87"/>
<connect gate="G$1" pin="IO_L12N_3" pad="36"/>
<connect gate="G$1" pin="IO_L12P_0" pad="192"/>
<connect gate="G$1" pin="IO_L12P_1" pad="139"/>
<connect gate="G$1" pin="IO_L12P_2/M0" pad="86"/>
<connect gate="G$1" pin="IO_L12P_3" pad="35"/>
<connect gate="G$1" pin="IO_L13N_0" pad="197"/>
<connect gate="G$1" pin="IO_L13N_1" pad="145"/>
<connect gate="G$1" pin="IO_L13N_2" pad="90"/>
<connect gate="G$1" pin="IO_L13N_3" pad="40"/>
<connect gate="G$1" pin="IO_L13P_0" pad="196"/>
<connect gate="G$1" pin="IO_L13P_1" pad="144"/>
<connect gate="G$1" pin="IO_L13P_2" pad="89"/>
<connect gate="G$1" pin="IO_L13P_3" pad="39"/>
<connect gate="G$1" pin="IO_L14N_0/VREF_0" pad="200"/>
<connect gate="G$1" pin="IO_L14N_1" pad="147"/>
<connect gate="G$1" pin="IO_L14N_2/A22" pad="94"/>
<connect gate="G$1" pin="IO_L14N_3" pad="42"/>
<connect gate="G$1" pin="IO_L14P_0" pad="199"/>
<connect gate="G$1" pin="IO_L14P_1" pad="146"/>
<connect gate="G$1" pin="IO_L14P_2/A23" pad="93"/>
<connect gate="G$1" pin="IO_L14P_3" pad="41"/>
<connect gate="G$1" pin="IO_L15N_0" pad="203"/>
<connect gate="G$1" pin="IO_L15N_2/A20" pad="97"/>
<connect gate="G$1" pin="IO_L15N_3" pad="48"/>
<connect gate="G$1" pin="IO_L15P_0" pad="202"/>
<connect gate="G$1" pin="IO_L15P_1/HDC" pad="150"/>
<connect gate="G$1" pin="IO_L15P_2/A21" pad="96"/>
<connect gate="G$1" pin="IO_L15P_3" pad="47"/>
<connect gate="G$1" pin="IO_L15_1/LDC0" pad="151"/>
<connect gate="G$1" pin="IO_L16N_0/HSWAP" pad="206"/>
<connect gate="G$1" pin="IO_L16N_1/LDC2" pad="153"/>
<connect gate="G$1" pin="IO_L16N_2/VS1/A18" pad="100"/>
<connect gate="G$1" pin="IO_L16N_3" pad="50"/>
<connect gate="G$1" pin="IO_L16P_0" pad="205"/>
<connect gate="G$1" pin="IO_L16P_2/VS2/A19" pad="99"/>
<connect gate="G$1" pin="IO_L16P_3" pad="49"/>
<connect gate="G$1" pin="IO_L17N_2/CCLK" pad="103"/>
<connect gate="G$1" pin="IO_L17P_2/VS0/A17" pad="102"/>
<connect gate="G$1" pin="IO_LO7P_0/GCLK4" pad="177"/>
<connect gate="G$1" pin="IP" pad="159"/>
<connect gate="G$1" pin="IP/VREF_1" pad="136"/>
<connect gate="G$1" pin="IP/VREF_3" pad="20"/>
<connect gate="G$1" pin="IP@10" pad="148"/>
<connect gate="G$1" pin="IP@11" pad="154"/>
<connect gate="G$1" pin="IP@12" pad="54"/>
<connect gate="G$1" pin="IP@13" pad="91"/>
<connect gate="G$1" pin="IP@14" pad="101"/>
<connect gate="G$1" pin="IP@15" pad="6"/>
<connect gate="G$1" pin="IP@16" pad="14"/>
<connect gate="G$1" pin="IP@17" pad="26"/>
<connect gate="G$1" pin="IP@18" pad="32"/>
<connect gate="G$1" pin="IP@19" pad="43"/>
<connect gate="G$1" pin="IP@2" pad="169"/>
<connect gate="G$1" pin="IP@20" pad="51"/>
<connect gate="G$1" pin="IP@3" pad="194"/>
<connect gate="G$1" pin="IP@4" pad="204"/>
<connect gate="G$1" pin="IP@5" pad="110"/>
<connect gate="G$1" pin="IP@6" pad="118"/>
<connect gate="G$1" pin="IP@7" pad="124"/>
<connect gate="G$1" pin="IP@8" pad="130"/>
<connect gate="G$1" pin="IP@9" pad="142"/>
<connect gate="G$1" pin="IP_L02N_2" pad="58"/>
<connect gate="G$1" pin="IP_L02P_2" pad="57"/>
<connect gate="G$1" pin="IP_L06N_0" pad="175"/>
<connect gate="G$1" pin="IP_L06P_0" pad="174"/>
<connect gate="G$1" pin="IP_L07N_2/VREF_2" pad="72"/>
<connect gate="G$1" pin="IP_L07P_2" pad="71"/>
<connect gate="G$1" pin="IP_L09P_0/GCLK8" pad="183"/>
<connect gate="G$1" pin="IP_L10N_2/M2/GCLK1" pad="81"/>
<connect gate="G$1" pin="IP_L10P_2/RDWR_B/GCLK0" pad="80"/>
<connect gate="G$1" pin="IP_LO9N_0/GCLK9" pad="184"/>
<connect gate="G$1" pin="PROG_B" pad="1"/>
<connect gate="G$1" pin="TCK" pad="158"/>
<connect gate="G$1" pin="TDI" pad="207"/>
<connect gate="G$1" pin="TDO" pad="157"/>
<connect gate="G$1" pin="TMS" pad="155"/>
<connect gate="G$1" pin="VCC0_1" pad="114"/>
<connect gate="G$1" pin="VCC0_1@2" pad="125"/>
<connect gate="G$1" pin="VCC0_1@3" pad="143"/>
<connect gate="G$1" pin="VCCAUX" pad="7"/>
<connect gate="G$1" pin="VCCAUX@2" pad="44"/>
<connect gate="G$1" pin="VCCAUX@3" pad="66"/>
<connect gate="G$1" pin="VCCAUX@4" pad="92"/>
<connect gate="G$1" pin="VCCAUX@5" pad="111"/>
<connect gate="G$1" pin="VCCAUX@6" pad="149"/>
<connect gate="G$1" pin="VCCAUX@7" pad="166"/>
<connect gate="G$1" pin="VCCAUX@8" pad="195"/>
<connect gate="G$1" pin="VCCINT" pad="13"/>
<connect gate="G$1" pin="VCCINT@2" pad="67"/>
<connect gate="G$1" pin="VCCINT@3" pad="117"/>
<connect gate="G$1" pin="VCCINT@4" pad="170"/>
<connect gate="G$1" pin="VCCO_0" pad="176"/>
<connect gate="G$1" pin="VCCO_0@2" pad="191"/>
<connect gate="G$1" pin="VCCO_0@3" pad="201"/>
<connect gate="G$1" pin="VCCO_2" pad="59"/>
<connect gate="G$1" pin="VCCO_2@2" pad="73"/>
<connect gate="G$1" pin="VCCO_2@3" pad="88"/>
<connect gate="G$1" pin="VCCO_3" pad="21"/>
<connect gate="G$1" pin="VCCO_3@2" pad="38"/>
<connect gate="G$1" pin="VCCO_3@3" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="F25" prefix="X" uservalue="yes">
<description>&lt;b&gt;D-SUB 25&lt;/b&gt;
25 Pin male connector. PCB edge mount for regular PCB thicknesses. This connector will connect directly to the back of a PC parallel port or through a normal DB25 extension cable (M/F). SKU: PRT-08287</description>
<gates>
<gate name="-1" symbol="F25"/>
</gates>
<devices>
<device name="D" package="F25D">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="F25H">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HP" package="F25HP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="F25V">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VP" package="F25VP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VB" package="F25VB">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB25" prefix="X" uservalue="yes">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
<gates>
<gate name="-1" symbol="DB25"/>
</gates>
<devices>
<device name="D" package="M25D">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="M25H">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HP" package="M25HP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="M25V">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VP" package="M25VP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VB" package="M25VB">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1002">
<gates>
<gate name="G$1" symbol="VS1002"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DVDD1" pad="6"/>
<connect gate="G$1" pin="DVDD2" pad="14"/>
<connect gate="G$1" pin="DVDD3" pad="19"/>
<connect gate="G$1" pin="D_REQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="SO" pad="30"/>
<connect gate="G$1" pin="SPIBOOT/GPIO0" pad="33"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL0" pad="17"/>
<connect gate="G$1" pin="XTAL1" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INVERTING_SCHMITT_TRIGGER">
<description>FAIRCHILD Inverting Schmitt Trigger

UNTESTED FOOTPRINT!!
Used in External Clock Sources.
Digikey P/N NC7SZ14M5XCT-ND</description>
<gates>
<gate name="G$1" symbol="INVERTING_SCHMITT_TRIGGER"/>
</gates>
<devices>
<device name="" package="TSSOP5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UNBUFFERED_INVERTER">
<description>FAIRCHILD Unbuffered Inverter.
Used for external clock sources
Digikey P/N NC7SPU04P5XCT-ND</description>
<gates>
<gate name="G$1" symbol="INVERTER"/>
</gates>
<devices>
<device name="" package="SC70">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MUX-TS3A5017">
<gates>
<gate name="G$1" symbol="TS3A5017"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="1D" pad="7"/>
<connect gate="G$1" pin="1EN" pad="1"/>
<connect gate="G$1" pin="1S1" pad="6"/>
<connect gate="G$1" pin="1S2" pad="5"/>
<connect gate="G$1" pin="1S3" pad="4"/>
<connect gate="G$1" pin="1S4" pad="3"/>
<connect gate="G$1" pin="2D" pad="9"/>
<connect gate="G$1" pin="2EN" pad="15"/>
<connect gate="G$1" pin="2S1" pad="10"/>
<connect gate="G$1" pin="2S2" pad="11"/>
<connect gate="G$1" pin="2S3" pad="12"/>
<connect gate="G$1" pin="2S4" pad="13"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="14"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74ACT125D">
<description>Quad Buffer with 3-State Outputs-
ON Semi Conductor:

Digikey P/N MC74ACT125DR2GOSTR-ND</description>
<gates>
<gate name="G$1" symbol="74ACT125D"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="B0" pad="2"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="9"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="O0" pad="3"/>
<connect gate="G$1" pin="O1" pad="6"/>
<connect gate="G$1" pin="O2" pad="11"/>
<connect gate="G$1" pin="O3" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C8_PQ208">
<gates>
<gate name="G$2" symbol="EP2C20_PQ208_PLL"/>
<gate name="G$6" symbol="EP2C20_PQ208_B3"/>
<gate name="G$4" symbol="EP2C20_PQ208_B1"/>
<gate name="G$3" symbol="EP2C20_PQ208_B4"/>
<gate name="G$7" symbol="EP2C20_PQ208_POWER"/>
<gate name="G$5" symbol="EP2C20_PQ208_B2"/>
<gate name="G$1" symbol="EP2C20_PQ208_CONFIG"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="G$1" pin="ASDO" pad="1"/>
<connect gate="G$1" pin="CLKUSR" pad="4"/>
<connect gate="G$1" pin="CONF_DONE" pad="123"/>
<connect gate="G$1" pin="CRC_ERROR" pad="3"/>
<connect gate="G$1" pin="DATA0" pad="20"/>
<connect gate="G$1" pin="DCLK" pad="21"/>
<connect gate="G$1" pin="DEV_OE" pad="56"/>
<connect gate="G$1" pin="INIT_DONE" pad="107"/>
<connect gate="G$1" pin="MSEL0" pad="126"/>
<connect gate="G$1" pin="MSEL1" pad="125"/>
<connect gate="G$1" pin="NCE" pad="22"/>
<connect gate="G$1" pin="NCEO" pad="108"/>
<connect gate="G$1" pin="NCONFIG" pad="26"/>
<connect gate="G$1" pin="NCSO" pad="2"/>
<connect gate="G$1" pin="NSTATUS" pad="121"/>
<connect gate="G$1" pin="TCK" pad="18"/>
<connect gate="G$1" pin="TDI" pad="19"/>
<connect gate="G$1" pin="TDO" pad="16"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$2" pin="GNDA_PLL1" pad="54"/>
<connect gate="G$2" pin="GNDA_PLL2" pad="158"/>
<connect gate="G$2" pin="GND_PLL1" pad="50"/>
<connect gate="G$2" pin="GND_PLL1@1" pad="52"/>
<connect gate="G$2" pin="GND_PLL2" pad="154"/>
<connect gate="G$2" pin="GND_PLL2@1" pad="156"/>
<connect gate="G$2" pin="VCCA_PLL1" pad="53"/>
<connect gate="G$2" pin="VCCA_PLL2" pad="157"/>
<connect gate="G$2" pin="VCCD_PLL1" pad="51"/>
<connect gate="G$2" pin="VCCD_PLL2" pad="155"/>
<connect gate="G$3" pin="IO@1" pad="80"/>
<connect gate="G$3" pin="IO@2" pad="96"/>
<connect gate="G$3" pin="IO_LVDS57N" pad="104"/>
<connect gate="G$3" pin="IO_LVDS57P" pad="103"/>
<connect gate="G$3" pin="IO_LVDS58N" pad="102"/>
<connect gate="G$3" pin="IO_LVDS58P" pad="101"/>
<connect gate="G$3" pin="IO_LVDS59N" pad="99"/>
<connect gate="G$3" pin="IO_LVDS59P" pad="97"/>
<connect gate="G$3" pin="IO_LVDS60N" pad="95"/>
<connect gate="G$3" pin="IO_LVDS60P" pad="94"/>
<connect gate="G$3" pin="IO_LVDS61N" pad="92"/>
<connect gate="G$3" pin="IO_LVDS61P" pad="90"/>
<connect gate="G$3" pin="IO_LVDS62N" pad="88"/>
<connect gate="G$3" pin="IO_LVDS62P" pad="87"/>
<connect gate="G$3" pin="IO_LVDS63N" pad="86"/>
<connect gate="G$3" pin="IO_LVDS63P" pad="84"/>
<connect gate="G$3" pin="IO_LVDS64N" pad="82"/>
<connect gate="G$3" pin="IO_LVDS64P" pad="81"/>
<connect gate="G$3" pin="IO_LVDS66N" pad="77"/>
<connect gate="G$3" pin="IO_LVDS66P" pad="76"/>
<connect gate="G$3" pin="IO_LVDS67N" pad="75"/>
<connect gate="G$3" pin="IO_LVDS67P" pad="74"/>
<connect gate="G$3" pin="IO_LVDS68N" pad="72"/>
<connect gate="G$3" pin="IO_LVDS68P" pad="70"/>
<connect gate="G$3" pin="IO_LVDS70N" pad="69"/>
<connect gate="G$3" pin="IO_LVDS70P" pad="68"/>
<connect gate="G$3" pin="IO_LVDS74N" pad="64"/>
<connect gate="G$3" pin="IO_LVDS74P" pad="63"/>
<connect gate="G$3" pin="IO_LVDS75N" pad="61"/>
<connect gate="G$3" pin="IO_LVDS75P" pad="60"/>
<connect gate="G$3" pin="IO_LVDS76N" pad="59"/>
<connect gate="G$3" pin="IO_LVDS76P" pad="58"/>
<connect gate="G$3" pin="IO_LVDS77P" pad="57"/>
<connect gate="G$3" pin="IO_VREFB4N0" pad="89"/>
<connect gate="G$3" pin="IO_VREFB4N1" pad="67"/>
<connect gate="G$3" pin="VCCIO4@1" pad="62"/>
<connect gate="G$3" pin="VCCIO4@2" pad="71"/>
<connect gate="G$3" pin="VCCIO4@3" pad="83"/>
<connect gate="G$3" pin="VCCIO4@4" pad="91"/>
<connect gate="G$3" pin="VCCIO4@5" pad="98"/>
<connect gate="G$4" pin="CLK0_LVDSCLK0P" pad="23"/>
<connect gate="G$4" pin="CLK1_LVDSCLK0N" pad="24"/>
<connect gate="G$4" pin="CLK2_LVDSCLK1P" pad="27"/>
<connect gate="G$4" pin="CLK3_LVDSCLK1N" pad="28"/>
<connect gate="G$4" pin="IO@2" pad="34"/>
<connect gate="G$4" pin="IO@3" pad="43"/>
<connect gate="G$4" pin="IO@4" pad="46"/>
<connect gate="G$4" pin="IO_LVDS0N" pad="45"/>
<connect gate="G$4" pin="IO_LVDS0P" pad="44"/>
<connect gate="G$4" pin="IO_LVDS12N" pad="12"/>
<connect gate="G$4" pin="IO_LVDS12P" pad="11"/>
<connect gate="G$4" pin="IO_LVDS13N" pad="10"/>
<connect gate="G$4" pin="IO_LVDS13P" pad="8"/>
<connect gate="G$4" pin="IO_LVDS14N" pad="6"/>
<connect gate="G$4" pin="IO_LVDS14P" pad="5"/>
<connect gate="G$4" pin="IO_LVDS2N" pad="41"/>
<connect gate="G$4" pin="IO_LVDS2P" pad="40"/>
<connect gate="G$4" pin="IO_LVDS3N" pad="39"/>
<connect gate="G$4" pin="IO_LVDS5P" pad="35"/>
<connect gate="G$4" pin="IO_LVDS6N" pad="33"/>
<connect gate="G$4" pin="IO_LVDS7N" pad="31"/>
<connect gate="G$4" pin="IO_LVDS7P" pad="30"/>
<connect gate="G$4" pin="IO_LVDS8N" pad="15"/>
<connect gate="G$4" pin="IO_LVDS8P" pad="14"/>
<connect gate="G$4" pin="IO_PLL1_OUTN" pad="48"/>
<connect gate="G$4" pin="IO_PLL1_OUTP" pad="47"/>
<connect gate="G$4" pin="IO_VREFB1N0" pad="13"/>
<connect gate="G$4" pin="IO_VREFB1N1" pad="37"/>
<connect gate="G$4" pin="VCCIO1@1" pad="7"/>
<connect gate="G$4" pin="VCCIO1@4" pad="29"/>
<connect gate="G$4" pin="VCCIO1@6" pad="42"/>
<connect gate="G$5" pin="IO_LVDS16N" pad="208"/>
<connect gate="G$5" pin="IO_LVDS16P" pad="207"/>
<connect gate="G$5" pin="IO_LVDS17N" pad="206"/>
<connect gate="G$5" pin="IO_LVDS17P" pad="205"/>
<connect gate="G$5" pin="IO_LVDS18N" pad="201"/>
<connect gate="G$5" pin="IO_LVDS18P" pad="203"/>
<connect gate="G$5" pin="IO_LVDS19N" pad="199"/>
<connect gate="G$5" pin="IO_LVDS19P" pad="200"/>
<connect gate="G$5" pin="IO_LVDS21N" pad="197"/>
<connect gate="G$5" pin="IO_LVDS21P" pad="198"/>
<connect gate="G$5" pin="IO_LVDS23N" pad="193"/>
<connect gate="G$5" pin="IO_LVDS23P" pad="195"/>
<connect gate="G$5" pin="IO_LVDS24N" pad="189"/>
<connect gate="G$5" pin="IO_LVDS24P" pad="191"/>
<connect gate="G$5" pin="IO_LVDS25N" pad="187"/>
<connect gate="G$5" pin="IO_LVDS25P" pad="188"/>
<connect gate="G$5" pin="IO_LVDS26P" pad="185"/>
<connect gate="G$5" pin="IO_LVDS28N" pad="181"/>
<connect gate="G$5" pin="IO_LVDS28P" pad="182"/>
<connect gate="G$5" pin="IO_LVDS29N" pad="179"/>
<connect gate="G$5" pin="IO_LVDS29P" pad="180"/>
<connect gate="G$5" pin="IO_LVDS31N" pad="175"/>
<connect gate="G$5" pin="IO_LVDS31P" pad="176"/>
<connect gate="G$5" pin="IO_LVDS33N" pad="171"/>
<connect gate="G$5" pin="IO_LVDS33P" pad="173"/>
<connect gate="G$5" pin="IO_LVDS34N" pad="168"/>
<connect gate="G$5" pin="IO_LVDS34P" pad="169"/>
<connect gate="G$5" pin="IO_LVDS35N" pad="164"/>
<connect gate="G$5" pin="IO_LVDS35P" pad="165"/>
<connect gate="G$5" pin="IO_LVDS36N" pad="162"/>
<connect gate="G$5" pin="IO_LVDS36P" pad="163"/>
<connect gate="G$5" pin="IO_LVDS37N" pad="160"/>
<connect gate="G$5" pin="IO_LVDS37P" pad="161"/>
<connect gate="G$5" pin="IO_VREFB2N0" pad="170"/>
<connect gate="G$5" pin="IO_VREFB2N1" pad="192"/>
<connect gate="G$5" pin="VCCIO2@1" pad="166"/>
<connect gate="G$5" pin="VCCIO2@2" pad="172"/>
<connect gate="G$5" pin="VCCIO2@3" pad="183"/>
<connect gate="G$5" pin="VCCIO2@4" pad="194"/>
<connect gate="G$5" pin="VCCIO2@5" pad="202"/>
<connect gate="G$6" pin="CLK4_LVDSCLK2P" pad="132"/>
<connect gate="G$6" pin="CLK5_LVDSCLK2N" pad="131"/>
<connect gate="G$6" pin="CLK6_LVDSCLK3P" pad="130"/>
<connect gate="G$6" pin="CLK7_LVDSCLK3N" pad="129"/>
<connect gate="G$6" pin="IO@1" pad="118"/>
<connect gate="G$6" pin="IO_LVDS38N" pad="149"/>
<connect gate="G$6" pin="IO_LVDS38P" pad="150"/>
<connect gate="G$6" pin="IO_LVDS39N" pad="146"/>
<connect gate="G$6" pin="IO_LVDS39P" pad="147"/>
<connect gate="G$6" pin="IO_LVDS42N" pad="143"/>
<connect gate="G$6" pin="IO_LVDS42P" pad="144"/>
<connect gate="G$6" pin="IO_LVDS44N" pad="141"/>
<connect gate="G$6" pin="IO_LVDS44P" pad="142"/>
<connect gate="G$6" pin="IO_LVDS45N" pad="138"/>
<connect gate="G$6" pin="IO_LVDS45P" pad="139"/>
<connect gate="G$6" pin="IO_LVDS46N" pad="135"/>
<connect gate="G$6" pin="IO_LVDS46P" pad="137"/>
<connect gate="G$6" pin="IO_LVDS47N" pad="133"/>
<connect gate="G$6" pin="IO_LVDS47P" pad="134"/>
<connect gate="G$6" pin="IO_LVDS48N" pad="127"/>
<connect gate="G$6" pin="IO_LVDS48P" pad="128"/>
<connect gate="G$6" pin="IO_LVDS51N" pad="115"/>
<connect gate="G$6" pin="IO_LVDS51P" pad="116"/>
<connect gate="G$6" pin="IO_LVDS52N" pad="113"/>
<connect gate="G$6" pin="IO_LVDS52P" pad="114"/>
<connect gate="G$6" pin="IO_LVDS53N" pad="110"/>
<connect gate="G$6" pin="IO_LVDS53P" pad="112"/>
<connect gate="G$6" pin="IO_LVDS56N" pad="105"/>
<connect gate="G$6" pin="IO_LVDS56P" pad="106"/>
<connect gate="G$6" pin="IO_PLL2_OUTN" pad="152"/>
<connect gate="G$6" pin="IO_PLL2_OUTP" pad="151"/>
<connect gate="G$6" pin="IO_VREFB3N0" pad="145"/>
<connect gate="G$6" pin="IO_VREFB3N1" pad="117"/>
<connect gate="G$6" pin="VCCIO3@1" pad="109"/>
<connect gate="G$6" pin="VCCIO3@2" pad="122"/>
<connect gate="G$6" pin="VCCIO3@3" pad="136"/>
<connect gate="G$6" pin="VCCIO3@4" pad="148"/>
<connect gate="G$7" pin="GND@1" pad="9"/>
<connect gate="G$7" pin="GND@10" pad="85"/>
<connect gate="G$7" pin="GND@11" pad="93"/>
<connect gate="G$7" pin="GND@12" pad="100"/>
<connect gate="G$7" pin="GND@13" pad="111"/>
<connect gate="G$7" pin="GND@14" pad="119"/>
<connect gate="G$7" pin="GND@15" pad="124"/>
<connect gate="G$7" pin="GND@16" pad="140"/>
<connect gate="G$7" pin="GND@17" pad="153"/>
<connect gate="G$7" pin="GND@18" pad="159"/>
<connect gate="G$7" pin="GND@19" pad="167"/>
<connect gate="G$7" pin="GND@2" pad="25"/>
<connect gate="G$7" pin="GND@20" pad="174"/>
<connect gate="G$7" pin="GND@21" pad="177"/>
<connect gate="G$7" pin="GND@22" pad="184"/>
<connect gate="G$7" pin="GND@23" pad="186"/>
<connect gate="G$7" pin="GND@24" pad="196"/>
<connect gate="G$7" pin="GND@25" pad="204"/>
<connect gate="G$7" pin="GND@3" pad="36"/>
<connect gate="G$7" pin="GND@4" pad="38"/>
<connect gate="G$7" pin="GND@5" pad="49"/>
<connect gate="G$7" pin="GND@6" pad="55"/>
<connect gate="G$7" pin="GND@7" pad="65"/>
<connect gate="G$7" pin="GND@8" pad="73"/>
<connect gate="G$7" pin="GND@9" pad="78"/>
<connect gate="G$7" pin="VCCINT@1" pad="32"/>
<connect gate="G$7" pin="VCCINT@2" pad="66"/>
<connect gate="G$7" pin="VCCINT@3" pad="79"/>
<connect gate="G$7" pin="VCCINT@4" pad="120"/>
<connect gate="G$7" pin="VCCINT@5" pad="178"/>
<connect gate="G$7" pin="VCCINT@6" pad="190"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2455">
<gates>
<gate name="G$1" symbol="PIC18F2550"/>
</gates>
<devices>
<device name="SMD" package="SO-28W">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/AN4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC4/D-" pad="15"/>
<connect gate="G$1" pin="RC5/D+" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="V-USB" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS3LV02DQ">
<gates>
<gate name="G$1" symbol="LIS3LV02DQ"/>
</gates>
<devices>
<device name="SMD" package="QFN-28">
<connects>
<connect gate="G$1" pin="CK" pad="16"/>
<connect gate="G$1" pin="CS" pad="13"/>
<connect gate="G$1" pin="GND@0" pad="0"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="INT" pad="6"/>
<connect gate="G$1" pin="SCL/SPC" pad="12"/>
<connect gate="G$1" pin="SDA/SDI" pad="10"/>
<connect gate="G$1" pin="SDO" pad="9"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@20" pad="20"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
<connect gate="G$1" pin="VDD_IO" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RMCM01">
<gates>
<gate name="G$1" symbol="RMCM01"/>
</gates>
<devices>
<device name="SMD" package="RMCM01">
<connects>
<connect gate="G$1" pin="F32KIN" pad="3"/>
<connect gate="G$1" pin="FPLS" pad="6"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="HR" pad="5"/>
<connect gate="G$1" pin="LX1" pad="10"/>
<connect gate="G$1" pin="LX2" pad="9"/>
<connect gate="G$1" pin="OSC" pad="4"/>
<connect gate="G$1" pin="OSC_ON" pad="2"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="WIDB_DET" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F913">
<gates>
<gate name="G$1" symbol="PIC16F913"/>
</gates>
<devices>
<device name="SOIC28" package="SO-28W">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2" pad="10"/>
<connect gate="G$1" pin="RA7/OSC1" pad="9"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4/SD0" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RX/RC7/SDA" pad="18"/>
<connect gate="G$1" pin="TX/RC6/SCL" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS302DL">
<gates>
<gate name="G$1" symbol="LIS302DL"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="INT1" pad="8"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="SCL/SPC" pad="14"/>
<connect gate="G$1" pin="SDA/SDI" pad="13"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
<connect gate="G$1" pin="VDD@6" pad="6"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_TPS61040">
<gates>
<gate name="G$1" symbol="TPS61040"/>
</gates>
<devices>
<device name="SMD" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC">
<description>&lt;b&gt;Microphone&lt;/b&gt;
Omni-directional electret microphone. 9.7mm standard diameter.</description>
<gates>
<gate name="G$1" symbol="BUZZER"/>
</gates>
<devices>
<device name="9.7MM" package="MIC-9.7MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ELECTRET_SMD" package="MIC_ELECTRET_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPM0204UD5">
<gates>
<gate name="G$1" symbol="SPM0204UD5"/>
</gates>
<devices>
<device name="SMD" package="SPM0204UD5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND#" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WT32">
<description>Blue Giga Audio Bluetooth Module

Footprint is not confirmed yet.</description>
<gates>
<gate name="G$1" symbol="WT32"/>
</gates>
<devices>
<device name="" package="WT32">
<connects>
<connect gate="G$1" pin="AGND@39" pad="39"/>
<connect gate="G$1" pin="AGND@43" pad="43"/>
<connect gate="G$1" pin="AGND@48" pad="48"/>
<connect gate="G$1" pin="AIO0@5" pad="5"/>
<connect gate="G$1" pin="AIO1@6" pad="6"/>
<connect gate="G$1" pin="AUDIO_IN_N_LEFT@45" pad="45"/>
<connect gate="G$1" pin="AUDIO_IN_N_RIGHT@42" pad="42"/>
<connect gate="G$1" pin="AUDIO_IN_P_LEFT@44" pad="44"/>
<connect gate="G$1" pin="AUDIO_IN_P_RIGHT@41" pad="41"/>
<connect gate="G$1" pin="AUDIO_OUT_N_LEFT@49" pad="49"/>
<connect gate="G$1" pin="AUDIO_OUT_N_RIGHT@46" pad="46"/>
<connect gate="G$1" pin="AUDIO_OUT_P_LEFT@50" pad="50"/>
<connect gate="G$1" pin="AUDIO_OUT_P_RIGHT@47" pad="47"/>
<connect gate="G$1" pin="CTS@21" pad="21"/>
<connect gate="G$1" pin="DGND@18" pad="18"/>
<connect gate="G$1" pin="DGND@2" pad="2"/>
<connect gate="G$1" pin="DGND@3" pad="3"/>
<connect gate="G$1" pin="DGND@31" pad="31"/>
<connect gate="G$1" pin="DGND@4" pad="4"/>
<connect gate="G$1" pin="LED0@36" pad="36"/>
<connect gate="G$1" pin="MIC_BIAS@40" pad="40"/>
<connect gate="G$1" pin="PCM_CLK@30" pad="30"/>
<connect gate="G$1" pin="PCM_IN@27" pad="27"/>
<connect gate="G$1" pin="PCM_OUT@28" pad="28"/>
<connect gate="G$1" pin="PCM_SYNC@29" pad="29"/>
<connect gate="G$1" pin="PIO0@7" pad="7"/>
<connect gate="G$1" pin="PIO10@14" pad="14"/>
<connect gate="G$1" pin="PIO1@8" pad="8"/>
<connect gate="G$1" pin="PIO2@9" pad="9"/>
<connect gate="G$1" pin="PIO3@10" pad="10"/>
<connect gate="G$1" pin="PIO4@26" pad="26"/>
<connect gate="G$1" pin="PIO5@25" pad="25"/>
<connect gate="G$1" pin="PIO6@24" pad="24"/>
<connect gate="G$1" pin="PIO7@23" pad="23"/>
<connect gate="G$1" pin="PIO8@22" pad="22"/>
<connect gate="G$1" pin="PIO9@13" pad="13"/>
<connect gate="G$1" pin="RESET@19" pad="19"/>
<connect gate="G$1" pin="RTS@20" pad="20"/>
<connect gate="G$1" pin="RXD@15" pad="15"/>
<connect gate="G$1" pin="SPI_CLK@33" pad="33"/>
<connect gate="G$1" pin="SPI_CS@32" pad="32"/>
<connect gate="G$1" pin="SPI_MISO@34" pad="34"/>
<connect gate="G$1" pin="SPI_MOSI@35" pad="35"/>
<connect gate="G$1" pin="TXD@16" pad="16"/>
<connect gate="G$1" pin="USB_DN@11" pad="11"/>
<connect gate="G$1" pin="USB_DP@12" pad="12"/>
<connect gate="G$1" pin="VDDIO@17" pad="17"/>
<connect gate="G$1" pin="VDD_BAT@37" pad="37"/>
<connect gate="G$1" pin="VDD_CHG@38" pad="38"/>
<connect gate="G$1" pin="VREG_ENA@1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STW5093">
<description>STW5093 - PCM Audio Codec</description>
<gates>
<gate name="G$1" symbol="STW5093"/>
</gates>
<devices>
<device name="" package="TSSOP30">
<connects>
<connect gate="G$1" pin="AUXCLK" pad="P$23"/>
<connect gate="G$1" pin="BZ" pad="P$19"/>
<connect gate="G$1" pin="CCLK" pad="P$20"/>
<connect gate="G$1" pin="CI" pad="P$22"/>
<connect gate="G$1" pin="CO" pad="P$25"/>
<connect gate="G$1" pin="CS-" pad="P$21"/>
<connect gate="G$1" pin="DR" pad="P$28"/>
<connect gate="G$1" pin="DX" pad="P$27"/>
<connect gate="G$1" pin="FS" pad="P$29"/>
<connect gate="G$1" pin="GND" pad="P$26"/>
<connect gate="G$1" pin="GNDA" pad="P$10"/>
<connect gate="G$1" pin="GNDP" pad="P$16"/>
<connect gate="G$1" pin="LO" pad="P$18"/>
<connect gate="G$1" pin="MBIAS" pad="P$6"/>
<connect gate="G$1" pin="MCLK" pad="P$30"/>
<connect gate="G$1" pin="MIC1+" pad="P$8"/>
<connect gate="G$1" pin="MIC1-" pad="P$9"/>
<connect gate="G$1" pin="MIC2+" pad="P$11"/>
<connect gate="G$1" pin="MIC2-" pad="P$12"/>
<connect gate="G$1" pin="MIC3+" pad="P$4"/>
<connect gate="G$1" pin="MIC3-" pad="P$5"/>
<connect gate="G$1" pin="REMIN" pad="P$3"/>
<connect gate="G$1" pin="REMOUT" pad="P$2"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
<connect gate="G$1" pin="VCCA" pad="P$7"/>
<connect gate="G$1" pin="VCCIO" pad="P$24"/>
<connect gate="G$1" pin="VCCP" pad="P$13"/>
<connect gate="G$1" pin="VFR" pad="P$17"/>
<connect gate="G$1" pin="VLR+" pad="P$15"/>
<connect gate="G$1" pin="VLR-" pad="P$14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM408_OUTLINE">
<description>This device is only the outline of the EM408 GPS receiver.  The device is intended to give the
designer an idea of what how the receiver will fit on the board.  THIS DEVICE DOES NOT PROVIDE ANY ELECTRICAL CONNECTION TO THE BOARD!  Include the "EM408_CON" device in order to connect the EM408 to your design.</description>
<gates>
<gate name="G$1" symbol="EM408_OUTLINE"/>
</gates>
<devices>
<device name="" package="EM408_OUTLINE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XBEE-1">
<gates>
<gate name="G$1" symbol="XBEE-1"/>
</gates>
<devices>
<device name="B1" package="XBEE-1">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B2" package="XBEE-SILK">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B3" package="XBEE-SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="XBEE-1_LOCK" package="XBEE-1_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M25" prefix="JP">
<gates>
<gate name="G$1" symbol="M25"/>
</gates>
<devices>
<device name="PTH" package="1X25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X25_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X25_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LONGPADS" package="1X25_LONGPAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.8V">
<gates>
<gate name="G$1" symbol="2.8V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZUNE_CONNECTOR_MALE">
<description>Male connector for the Zune media player.  UNPROVEN FOOTPRINT!  This connector must be used only with a 1.2mm PCB thickness.</description>
<gates>
<gate name="G$1" symbol="ZUNE_CONNECTOR_MALE"/>
</gates>
<devices>
<device name="" package="ZUNE_CONNECTOR_MALE">
<connects>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="AUDIO_L" pad="P$13"/>
<connect gate="G$1" pin="AUDIO_R" pad="P$14"/>
<connect gate="G$1" pin="GND@19" pad="P$19"/>
<connect gate="G$1" pin="GND@22" pad="P$22"/>
<connect gate="G$1" pin="GND@23" pad="P$23"/>
<connect gate="G$1" pin="GND@24" pad="P$24"/>
<connect gate="G$1" pin="USB_5V@1" pad="P$1"/>
<connect gate="G$1" pin="USB_5V@2" pad="P$2"/>
<connect gate="G$1" pin="USB_5V@3" pad="P$3"/>
<connect gate="G$1" pin="USB_DATA+" pad="P$21"/>
<connect gate="G$1" pin="USB_DATA-" pad="P$20"/>
<connect gate="G$1" pin="VIDEO+" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINH2X12">
<gates>
<gate name="G$1" symbol="PINH2X12"/>
</gates>
<devices>
<device name="" package="2X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1307">
<gates>
<gate name="G$1" symbol="DS1307"/>
</gates>
<devices>
<device name="SO8" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW" pad="7"/>
<connect gate="G$1" pin="VBATT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CNZ1120">
<gates>
<gate name="G$1" symbol="CNZ1120"/>
</gates>
<devices>
<device name="PTH" package="CNZ1120">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-PCHANNEL-SOIC8">
<gates>
<gate name="G$1" symbol="NDS8434-1"/>
</gates>
<devices>
<device name="SOIC8" package="SO08">
<connects>
<connect gate="G$1" pin="D@1" pad="5"/>
<connect gate="G$1" pin="D@2" pad="6"/>
<connect gate="G$1" pin="D@3" pad="7"/>
<connect gate="G$1" pin="D@4" pad="8"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S@1" pad="1"/>
<connect gate="G$1" pin="S@2" pad="2"/>
<connect gate="G$1" pin="S@3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUETOOTH-RN41">
<gates>
<gate name="G$1" symbol="RN41"/>
</gates>
<devices>
<device name="&quot;" package="RN41">
<connects>
<connect gate="G$1" pin="AIO1" pad="35"/>
<connect gate="G$1" pin="AIO2" pad="30"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="GND3" pad="27"/>
<connect gate="G$1" pin="GND4" pad="28"/>
<connect gate="G$1" pin="GND5" pad="29"/>
<connect gate="G$1" pin="NC" pad="26"/>
<connect gate="G$1" pin="PCMCLK" pad="7"/>
<connect gate="G$1" pin="PCMIN" pad="9"/>
<connect gate="G$1" pin="PCMOUT" pad="10"/>
<connect gate="G$1" pin="PCMSYNC" pad="8"/>
<connect gate="G$1" pin="PIO10" pad="33"/>
<connect gate="G$1" pin="PIO11" pad="34"/>
<connect gate="G$1" pin="PIO2" pad="19"/>
<connect gate="G$1" pin="PIO3" pad="20"/>
<connect gate="G$1" pin="PIO4" pad="22"/>
<connect gate="G$1" pin="PIO5" pad="21"/>
<connect gate="G$1" pin="PIO6" pad="3"/>
<connect gate="G$1" pin="PIO7" pad="4"/>
<connect gate="G$1" pin="PIO8" pad="31"/>
<connect gate="G$1" pin="PIO9" pad="32"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPICLK" pad="6"/>
<connect gate="G$1" pin="SPICSB" pad="23"/>
<connect gate="G$1" pin="SPIMISO" pad="24"/>
<connect gate="G$1" pin="SPIMOSI" pad="2"/>
<connect gate="G$1" pin="UARTCTS" pad="16"/>
<connect gate="G$1" pin="UARTRTS" pad="15"/>
<connect gate="G$1" pin="UARTRX" pad="13"/>
<connect gate="G$1" pin="UARTTX" pad="14"/>
<connect gate="G$1" pin="USBD+" pad="17"/>
<connect gate="G$1" pin="USBD-" pad="18"/>
<connect gate="G$1" pin="VDD" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SPST-2">
<gates>
<gate name="G$1" symbol="SPST"/>
</gates>
<devices>
<device name="RA" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="O" pad="P$3"/>
<connect gate="G$1" pin="P" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TV" package="SWITCH-SPST-VERTICAL">
<connects>
<connect gate="G$1" pin="O" pad="1"/>
<connect gate="G$1" pin="P" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHTPIPE-7511">
<gates>
<gate name="G$1" symbol="LIGHTPIPE-7511"/>
</gates>
<devices>
<device name="" package="LIGHTPIPE-7511">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIPO-OUTLINE">
<gates>
<gate name="G$1" symbol="LIPO-1100"/>
</gates>
<devices>
<device name="1100" package="LIPO-1100">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2000" package="LIPO-2000">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="100" package="LIPO-100">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB041B">
<gates>
<gate name="G$1" symbol="AT45DB041B"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_NPN_2">
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC_MCP4725">
<gates>
<gate name="G$1" symbol="MCP4725"/>
</gates>
<devices>
<device name="SOT" package="SOT23-6">
<connects>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIMHOLDER2">
<gates>
<gate name="G$1" symbol="SIMHOLDER2"/>
</gates>
<devices>
<device name="" package="SIMHOLDER2">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="I/O" pad="6"/>
<connect gate="G$1" pin="RST" pad="2"/>
<connect gate="G$1" pin="SW1" pad="4"/>
<connect gate="G$1" pin="SW2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VPP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC6343">
<gates>
<gate name="G$1" symbol="HMC6343"/>
</gates>
<devices>
<device name="A" package="LCC36">
<connects>
<connect gate="G$1" pin="CS" pad="22"/>
<connect gate="G$1" pin="CSC" pad="35"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="SCL" pad="32"/>
<connect gate="G$1" pin="SDA" pad="36"/>
<connect gate="G$1" pin="VDD@11" pad="11"/>
<connect gate="G$1" pin="VDD@21" pad="21"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-2">
<gates>
<gate name="G$1" symbol="BATTERY-2"/>
</gates>
<devices>
<device name="AA" package="BATTERY-AA">
<connects>
<connect gate="G$1" pin="+1" pad="PWR@1"/>
<connect gate="G$1" pin="+2" pad="PWR@2"/>
<connect gate="G$1" pin="-1" pad="GND@1"/>
<connect gate="G$1" pin="-2" pad="GND@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AAA" package="BATTERY-AAA">
<connects>
<connect gate="G$1" pin="+1" pad="PWR@1"/>
<connect gate="G$1" pin="+2" pad="PWR@2"/>
<connect gate="G$1" pin="-1" pad="GND@1"/>
<connect gate="G$1" pin="-2" pad="GND@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO-JACK2">
<gates>
<gate name="G$1" symbol="AUDIO-JACK2"/>
</gates>
<devices>
<device name="PTH" package="AUDIO-JACK">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="AUDIO-JACK-3.5MM-SMD">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXLXXX_E8">
<gates>
<gate name="G$1" symbol="ADXLXXX_E8"/>
</gates>
<devices>
<device name="" package="ADXLXXX_E8">
<connects>
<connect gate="G$1" pin="COM" pad="P$3"/>
<connect gate="G$1" pin="ST" pad="P$1"/>
<connect gate="G$1" pin="T2" pad="P$2"/>
<connect gate="G$1" pin="VDD" pad="P$8"/>
<connect gate="G$1" pin="XFILT" pad="P$7"/>
<connect gate="G$1" pin="XOUT" pad="P$5"/>
<connect gate="G$1" pin="YFILT" pad="P$6"/>
<connect gate="G$1" pin="YOUT" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA661AS">
<description>GPS LNA, 18dB gain, low external parts count</description>
<gates>
<gate name="G$1" symbol="SMA661AS"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="PD" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH-SCREEN">
<gates>
<gate name="G$1" symbol="TOUCH-SCREEN"/>
</gates>
<devices>
<device name="" package="TOUCH-SCREEN">
<connects>
<connect gate="G$1" pin="TS1" pad="P$4"/>
<connect gate="G$1" pin="TS2" pad="P$3"/>
<connect gate="G$1" pin="TS3" pad="P$2"/>
<connect gate="G$1" pin="TS4" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24Z1">
<gates>
<gate name="G$1" symbol="NRF24Z1"/>
</gates>
<devices>
<device name="" package="QFN-36">
<connects>
<connect gate="G$1" pin="ANT1" pad="21"/>
<connect gate="G$1" pin="ANT2" pad="22"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="DATA" pad="12"/>
<connect gate="G$1" pin="DD0" pad="8"/>
<connect gate="G$1" pin="DD1" pad="7"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="IREF" pad="24"/>
<connect gate="G$1" pin="IRQ" pad="36"/>
<connect gate="G$1" pin="MCLK" pad="14"/>
<connect gate="G$1" pin="MCSN" pad="29"/>
<connect gate="G$1" pin="MMISO" pad="30"/>
<connect gate="G$1" pin="MMOSI" pad="31"/>
<connect gate="G$1" pin="MODE" pad="26"/>
<connect gate="G$1" pin="MSCK" pad="35"/>
<connect gate="G$1" pin="MSCL" pad="28"/>
<connect gate="G$1" pin="MSDA" pad="27"/>
<connect gate="G$1" pin="REQ" pad="9"/>
<connect gate="G$1" pin="SCSN" pad="4"/>
<connect gate="G$1" pin="SMISO" pad="2"/>
<connect gate="G$1" pin="SMOSI" pad="6"/>
<connect gate="G$1" pin="SPDIO" pad="13"/>
<connect gate="G$1" pin="SSCK" pad="3"/>
<connect gate="G$1" pin="SSEL" pad="1"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VDD1" pad="19"/>
<connect gate="G$1" pin="VDD2" pad="33"/>
<connect gate="G$1" pin="VDD_PA" pad="20"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="VSS1" pad="25"/>
<connect gate="G$1" pin="VSS2" pad="32"/>
<connect gate="G$1" pin="VSS3" pad="34"/>
<connect gate="G$1" pin="VSS_PA" pad="23"/>
<connect gate="G$1" pin="WS" pad="11"/>
<connect gate="G$1" pin="XC1" pad="18"/>
<connect gate="G$1" pin="XC2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7745">
<gates>
<gate name="G$1" symbol="AD7745"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="/RDY" pad="2"/>
<connect gate="G$1" pin="CIN1+" pad="8"/>
<connect gate="G$1" pin="CIN1-" pad="7"/>
<connect gate="G$1" pin="CIN2+" pad="9"/>
<connect gate="G$1" pin="CIN2-" pad="10"/>
<connect gate="G$1" pin="EXCA" pad="3"/>
<connect gate="G$1" pin="EXCB" pad="4"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="NC" pad="15"/>
<connect gate="G$1" pin="REFIN+" pad="5"/>
<connect gate="G$1" pin="REFIN-" pad="6"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VIN+" pad="11"/>
<connect gate="G$1" pin="VIN-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH">
<gates>
<gate name="G$1" symbol="TOUCH"/>
</gates>
<devices>
<device name="" package="TOUCH1">
<connects>
<connect gate="G$1" pin="T1" pad="P$1"/>
<connect gate="G$1" pin="T2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="TOUCH2">
<connects>
<connect gate="G$1" pin="T1" pad="P$1"/>
<connect gate="G$1" pin="T2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTON-MAGNETIC">
<gates>
<gate name="G$1" symbol="SEWTAP"/>
</gates>
<devices>
<device name="10MM" package="BUTTON-10MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="18MM" package="BUTTON-18MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-3-OLD" prefix="JP">
<gates>
<gate name="G$1" symbol="JUMPER-3"/>
</gates>
<devices>
<device name="SMD" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1-2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2-3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1033" prefix="U">
<gates>
<gate name="G$1" symbol="VS1033D"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="CVDD1" pad="5"/>
<connect gate="G$1" pin="CVDD2" pad="7"/>
<connect gate="G$1" pin="CVDD3" pad="24"/>
<connect gate="G$1" pin="CVDD4" pad="31"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DGND6" pad="35"/>
<connect gate="G$1" pin="DREQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO0/I2S_SCLK" pad="33"/>
<connect gate="G$1" pin="GPIO1/I2S_SDATA" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="GPIO4/I2S_LROUT" pad="36"/>
<connect gate="G$1" pin="GPIO5/I2C_MCLK" pad="25"/>
<connect gate="G$1" pin="GPIO6" pad="11"/>
<connect gate="G$1" pin="GPIO7" pad="12"/>
<connect gate="G$1" pin="IOVDD1" pad="6"/>
<connect gate="G$1" pin="IOVDD2" pad="14"/>
<connect gate="G$1" pin="IOVDD3" pad="19"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="LINEIN" pad="48"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="S0" pad="30"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="VCO" pad="15"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL1/MCLK" pad="18"/>
<connect gate="G$1" pin="XTAL2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1000">
<gates>
<gate name="G$1" symbol="VS1000"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="38"/>
<connect gate="G$1" pin="AGND2" pad="41"/>
<connect gate="G$1" pin="AGND3" pad="42"/>
<connect gate="G$1" pin="AGND4" pad="48"/>
<connect gate="G$1" pin="AVDD1" pad="34"/>
<connect gate="G$1" pin="AVDD2" pad="39"/>
<connect gate="G$1" pin="AVDD3" pad="44"/>
<connect gate="G$1" pin="AVDD4" pad="46"/>
<connect gate="G$1" pin="CS1/GPIO0_10" pad="15"/>
<connect gate="G$1" pin="CS2/GPIO0_14" pad="21"/>
<connect gate="G$1" pin="CVDD" pad="32"/>
<connect gate="G$1" pin="DGND1" pad="6"/>
<connect gate="G$1" pin="DGND2" pad="18"/>
<connect gate="G$1" pin="DGND3" pad="31"/>
<connect gate="G$1" pin="GBUF" pad="43"/>
<connect gate="G$1" pin="IOVDD1" pad="30"/>
<connect gate="G$1" pin="IOVDD2" pad="19"/>
<connect gate="G$1" pin="IOVDD3" pad="7"/>
<connect gate="G$1" pin="LEFT" pad="47"/>
<connect gate="G$1" pin="NFALE/GPIO0_13" pad="17"/>
<connect gate="G$1" pin="NFCLE/GPIO0_12" pad="16"/>
<connect gate="G$1" pin="NFDIO0/IO0_0" pad="2"/>
<connect gate="G$1" pin="NFDIO1/IO0_1" pad="3"/>
<connect gate="G$1" pin="NFDIO2/IO0_2" pad="4"/>
<connect gate="G$1" pin="NFDIO3/IO0_3" pad="5"/>
<connect gate="G$1" pin="NFDIO4/IO0_4" pad="9"/>
<connect gate="G$1" pin="NFDIO5/IO0_5" pad="10"/>
<connect gate="G$1" pin="NFDIO6/IO0_6" pad="11"/>
<connect gate="G$1" pin="NFDIO7/IO0_7" pad="12"/>
<connect gate="G$1" pin="NFRD/GPIO0_9" pad="14"/>
<connect gate="G$1" pin="NFRDY/GPIO0_8" pad="13"/>
<connect gate="G$1" pin="NFWR/GPIO0_11" pad="20"/>
<connect gate="G$1" pin="POWBTN" pad="37"/>
<connect gate="G$1" pin="RCAP" pad="45"/>
<connect gate="G$1" pin="RIGHT" pad="40"/>
<connect gate="G$1" pin="RX/GPIO1_4" pad="27"/>
<connect gate="G$1" pin="SCLK/GPIO1_1" pad="23"/>
<connect gate="G$1" pin="SI/GPIO1_2" pad="24"/>
<connect gate="G$1" pin="SO/GPIO1_3" pad="25"/>
<connect gate="G$1" pin="TEST" pad="8"/>
<connect gate="G$1" pin="TX/GPIO1_5" pad="26"/>
<connect gate="G$1" pin="USBN" pad="36"/>
<connect gate="G$1" pin="USBP" pad="35"/>
<connect gate="G$1" pin="VHIGH" pad="33"/>
<connect gate="G$1" pin="XCS/GPIO1_0" pad="22"/>
<connect gate="G$1" pin="XRESET" pad="1"/>
<connect gate="G$1" pin="XTAL0" pad="29"/>
<connect gate="G$1" pin="XTAL1" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NAND256">
<gates>
<gate name="G$1" symbol="NAND256"/>
</gates>
<devices>
<device name="" package="TSOP48">
<connects>
<connect gate="G$1" pin="AL" pad="17"/>
<connect gate="G$1" pin="CL" pad="16"/>
<connect gate="G$1" pin="IO0" pad="29"/>
<connect gate="G$1" pin="IO1" pad="30"/>
<connect gate="G$1" pin="IO2" pad="31"/>
<connect gate="G$1" pin="IO3" pad="32"/>
<connect gate="G$1" pin="IO4" pad="41"/>
<connect gate="G$1" pin="IO5" pad="42"/>
<connect gate="G$1" pin="IO6" pad="43"/>
<connect gate="G$1" pin="IO7" pad="44"/>
<connect gate="G$1" pin="RXB" pad="7"/>
<connect gate="G$1" pin="VDD1" pad="12"/>
<connect gate="G$1" pin="VDD2" pad="37"/>
<connect gate="G$1" pin="VSS1" pad="13"/>
<connect gate="G$1" pin="VSS2" pad="36"/>
<connect gate="G$1" pin="XE" pad="9"/>
<connect gate="G$1" pin="XR" pad="8"/>
<connect gate="G$1" pin="XW" pad="18"/>
<connect gate="G$1" pin="XWP" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP9700">
<gates>
<gate name="G$1" symbol="MCP9700"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ32GP202">
<gates>
<gate name="G$1" symbol="PIC24HJ32GP202"/>
</gates>
<devices>
<device name="DIP" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AN0/VREF+/CN2/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/VREF-/CN2/RA1" pad="3"/>
<connect gate="G$1" pin="AN10/RP14/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/RP13/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/RP12/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN4/RP2/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/RP3/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/RP15/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="28"/>
<connect gate="G$1" pin="AVSS" pad="27"/>
<connect gate="G$1" pin="INT0/RP7/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OSCI/CLKI/CN30/RA2" pad="9"/>
<connect gate="G$1" pin="OSCO/CLKO/CN29/RA3" pad="10"/>
<connect gate="G$1" pin="PGEC1/AN3/C2IN+/RP1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/TMS/RP11/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/RP6/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/AN2/C2IN-/RP0/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/TDI/RP10/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/RP5/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="SOSCI/RP4/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RA4" pad="12"/>
<connect gate="G$1" pin="TCK/SCL/RP8/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="TDO/SDA1/RP9/CN12/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SO-28W">
<connects>
<connect gate="G$1" pin="AN0/VREF+/CN2/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/VREF-/CN2/RA1" pad="3"/>
<connect gate="G$1" pin="AN10/RP14/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/RP13/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/RP12/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN4/RP2/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/RP3/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/RP15/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="28"/>
<connect gate="G$1" pin="AVSS" pad="27"/>
<connect gate="G$1" pin="INT0/RP7/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OSCI/CLKI/CN30/RA2" pad="9"/>
<connect gate="G$1" pin="OSCO/CLKO/CN29/RA3" pad="10"/>
<connect gate="G$1" pin="PGEC1/AN3/C2IN+/RP1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/TMS/RP11/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/RP6/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/AN2/C2IN-/RP0/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/TDI/RP10/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/RP5/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="SOSCI/RP4/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RA4" pad="12"/>
<connect gate="G$1" pin="TCK/SCL/RP8/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="TDO/SDA1/RP9/CN12/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PL-2303XA">
<description>Prolific USB chip, requires 12MHz xtal</description>
<gates>
<gate name="G$1" symbol="PL-2303XA"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="CTS_N" pad="11"/>
<connect gate="G$1" pin="DCD_N" pad="10"/>
<connect gate="G$1" pin="DM" pad="16"/>
<connect gate="G$1" pin="DP" pad="15"/>
<connect gate="G$1" pin="DSR_N" pad="9"/>
<connect gate="G$1" pin="DTR_N" pad="2"/>
<connect gate="G$1" pin="EE_CLK" pad="13"/>
<connect gate="G$1" pin="EE_DATA" pad="14"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND_A" pad="25"/>
<connect gate="G$1" pin="GP0" pad="22"/>
<connect gate="G$1" pin="GP1" pad="23"/>
<connect gate="G$1" pin="OSC1" pad="27"/>
<connect gate="G$1" pin="OSC2" pad="28"/>
<connect gate="G$1" pin="PLL_TEST" pad="26"/>
<connect gate="G$1" pin="RESET_N" pad="19"/>
<connect gate="G$1" pin="RI_N" pad="6"/>
<connect gate="G$1" pin="RTS_N" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="SHTD_N" pad="12"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VDD_325" pad="4"/>
<connect gate="G$1" pin="VDD_33" pad="8"/>
<connect gate="G$1" pin="VDD_33A" pad="24"/>
<connect gate="G$1" pin="VDD_5" pad="20"/>
<connect gate="G$1" pin="VO_33" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCA3000">
<description>2g SPI accelerometer with interrrupt</description>
<gates>
<gate name="G$1" symbol="SCA3000"/>
</gates>
<devices>
<device name="" package="SCA3000">
<connects>
<connect gate="G$1" pin="AVDD" pad="P$14"/>
<connect gate="G$1" pin="AVSS@15" pad="P$15"/>
<connect gate="G$1" pin="AVSS@16" pad="P$16"/>
<connect gate="G$1" pin="CLK" pad="P$4"/>
<connect gate="G$1" pin="CSB" pad="P$8"/>
<connect gate="G$1" pin="DVDD" pad="P$6"/>
<connect gate="G$1" pin="DVIO" pad="P$7"/>
<connect gate="G$1" pin="DVSS" pad="P$5"/>
<connect gate="G$1" pin="INT" pad="P$3"/>
<connect gate="G$1" pin="MISO" pad="P$12"/>
<connect gate="G$1" pin="MOSI" pad="P$13"/>
<connect gate="G$1" pin="RST" pad="P$2"/>
<connect gate="G$1" pin="SCK" pad="P$11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TFM-511P">
<gates>
<gate name="G$1" symbol="TFM-511"/>
</gates>
<devices>
<device name="" package="TFM-511">
<connects>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="BUSEN" pad="7"/>
<connect gate="G$1" pin="BUSMOD" pad="8"/>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="DAT" pad="10"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LOUT" pad="4"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="ROUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XPORT-DIRECT">
<gates>
<gate name="G$1" symbol="XPORT_DIRECT"/>
</gates>
<devices>
<device name="" package="XPORT_DIRECT_MODULE">
<connects>
<connect gate="G$1" pin="3.3V" pad="P3"/>
<connect gate="G$1" pin="CP1" pad="P23"/>
<connect gate="G$1" pin="CP2" pad="P21"/>
<connect gate="G$1" pin="CTS" pad="P15"/>
<connect gate="G$1" pin="DTR" pad="P13"/>
<connect gate="G$1" pin="GND@1" pad="P1"/>
<connect gate="G$1" pin="GND@2" pad="P2"/>
<connect gate="G$1" pin="GND@24" pad="P24"/>
<connect gate="G$1" pin="RST" pad="P5"/>
<connect gate="G$1" pin="RTS" pad="P11"/>
<connect gate="G$1" pin="RX" pad="P9"/>
<connect gate="G$1" pin="TX" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="XPORT_DIRECT_MODULE-SMD">
<connects>
<connect gate="G$1" pin="3.3V" pad="P3"/>
<connect gate="G$1" pin="CP1" pad="P23"/>
<connect gate="G$1" pin="CP2" pad="P21"/>
<connect gate="G$1" pin="CTS" pad="P15"/>
<connect gate="G$1" pin="DTR" pad="P13"/>
<connect gate="G$1" pin="GND@1" pad="P1"/>
<connect gate="G$1" pin="GND@2" pad="P2"/>
<connect gate="G$1" pin="GND@24" pad="P24"/>
<connect gate="G$1" pin="RST" pad="P5"/>
<connect gate="G$1" pin="RTS" pad="P11"/>
<connect gate="G$1" pin="RX" pad="P9"/>
<connect gate="G$1" pin="TX" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XPORT">
<gates>
<gate name="G$1" symbol="XPORT"/>
</gates>
<devices>
<device name="" package="XPORT">
<connects>
<connect gate="G$1" pin="3.3V" pad="P2"/>
<connect gate="G$1" pin="CTS" pad="P8"/>
<connect gate="G$1" pin="DTR" pad="P7"/>
<connect gate="G$1" pin="GND" pad="P1"/>
<connect gate="G$1" pin="RST" pad="P3"/>
<connect gate="G$1" pin="RTS" pad="P6"/>
<connect gate="G$1" pin="RX" pad="P5"/>
<connect gate="G$1" pin="TX" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-TRICOLOR-THROUGHHOLE">
<gates>
<gate name="G$1" symbol="LED-TRICOLOR-THROUGHHOLE"/>
</gates>
<devices>
<device name="" package="LED-TRICOLOR-THROUGHHOLE">
<connects>
<connect gate="G$1" pin="BLU" pad="BLU"/>
<connect gate="G$1" pin="C" pad="GND"/>
<connect gate="G$1" pin="GRN" pad="GRN"/>
<connect gate="G$1" pin="RED" pad="RED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="LED-TRICOLOR-PTH_SPECIAL">
<connects>
<connect gate="G$1" pin="BLU" pad="BLU"/>
<connect gate="G$1" pin="C" pad="GND"/>
<connect gate="G$1" pin="GRN" pad="GRN"/>
<connect gate="G$1" pin="RED" pad="RED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQUARE" package="LED-TRICOLOR-PTH-SQUARE">
<connects>
<connect gate="G$1" pin="BLU" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="GRN" pad="G"/>
<connect gate="G$1" pin="RED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2621">
<gates>
<gate name="G$1" symbol="LM2621"/>
</gates>
<devices>
<device name="SMD" package="MSOP-8">
<connects>
<connect gate="G$1" pin="BOOT" pad="7"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="FREQ" pad="3"/>
<connect gate="G$1" pin="PGND" pad="1"/>
<connect gate="G$1" pin="SGND" pad="5"/>
<connect gate="G$1" pin="SW" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F4011">
<description>dsPIC30F4012 Footprint for UAVv2x, not tested</description>
<gates>
<gate name="G$1" symbol="DSPIC30F4011"/>
</gates>
<devices>
<device name="DIL" package="DIL40">
<connects>
<connect gate="G$1" pin="AVDD" pad="40"/>
<connect gate="G$1" pin="AVSS" pad="39"/>
<connect gate="G$1" pin="INT0/RE8" pad="17"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OC1/RD0" pad="23"/>
<connect gate="G$1" pin="OC2/RD1" pad="18"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="PGC/SDA" pad="26"/>
<connect gate="G$1" pin="PGD/SCL" pad="25"/>
<connect gate="G$1" pin="RB0/AREF+" pad="2"/>
<connect gate="G$1" pin="RB1/AREF-" pad="3"/>
<connect gate="G$1" pin="RB2" pad="4"/>
<connect gate="G$1" pin="RB3" pad="5"/>
<connect gate="G$1" pin="RB4/IC7" pad="6"/>
<connect gate="G$1" pin="RB5/IC8" pad="7"/>
<connect gate="G$1" pin="RB6" pad="8"/>
<connect gate="G$1" pin="RB7" pad="9"/>
<connect gate="G$1" pin="RB8" pad="10"/>
<connect gate="G$1" pin="RC13/TX1" pad="15"/>
<connect gate="G$1" pin="RC14/RX1" pad="16"/>
<connect gate="G$1" pin="RD2" pad="22"/>
<connect gate="G$1" pin="RD3" pad="19"/>
<connect gate="G$1" pin="RE0" pad="38"/>
<connect gate="G$1" pin="RE1" pad="37"/>
<connect gate="G$1" pin="RE2" pad="36"/>
<connect gate="G$1" pin="RE3" pad="35"/>
<connect gate="G$1" pin="RE4" pad="34"/>
<connect gate="G$1" pin="RE5" pad="33"/>
<connect gate="G$1" pin="RF0" pad="30"/>
<connect gate="G$1" pin="RF1" pad="29"/>
<connect gate="G$1" pin="RF4/RX2" pad="28"/>
<connect gate="G$1" pin="RF5/TX2" pad="27"/>
<connect gate="G$1" pin="RF6/SCK1" pad="24"/>
<connect gate="G$1" pin="VDD0" pad="11"/>
<connect gate="G$1" pin="VDD1" pad="21"/>
<connect gate="G$1" pin="VDD2" pad="32"/>
<connect gate="G$1" pin="VSS0" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="20"/>
<connect gate="G$1" pin="VSS2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="16"/>
<connect gate="G$1" pin="INT0/RE8" pad="36"/>
<connect gate="G$1" pin="MCLR" pad="18"/>
<connect gate="G$1" pin="OC1/RD0" pad="42"/>
<connect gate="G$1" pin="OC2/RD1" pad="37"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="PGC/SDA" pad="1"/>
<connect gate="G$1" pin="PGD/SCL" pad="44"/>
<connect gate="G$1" pin="RB0/AREF+" pad="19"/>
<connect gate="G$1" pin="RB1/AREF-" pad="20"/>
<connect gate="G$1" pin="RB2" pad="21"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4/IC7" pad="23"/>
<connect gate="G$1" pin="RB5/IC8" pad="24"/>
<connect gate="G$1" pin="RB6" pad="25"/>
<connect gate="G$1" pin="RB7" pad="26"/>
<connect gate="G$1" pin="RB8" pad="27"/>
<connect gate="G$1" pin="RC13/TX1" pad="32"/>
<connect gate="G$1" pin="RC14/RX1" pad="35"/>
<connect gate="G$1" pin="RD2" pad="41"/>
<connect gate="G$1" pin="RD3" pad="38"/>
<connect gate="G$1" pin="RE0" pad="15"/>
<connect gate="G$1" pin="RE1" pad="14"/>
<connect gate="G$1" pin="RE2" pad="11"/>
<connect gate="G$1" pin="RE3" pad="10"/>
<connect gate="G$1" pin="RE4" pad="9"/>
<connect gate="G$1" pin="RE5" pad="8"/>
<connect gate="G$1" pin="RF0" pad="5"/>
<connect gate="G$1" pin="RF1" pad="4"/>
<connect gate="G$1" pin="RF4/RX2" pad="3"/>
<connect gate="G$1" pin="RF5/TX2" pad="2"/>
<connect gate="G$1" pin="RF6/SCK1" pad="43"/>
<connect gate="G$1" pin="VDD0" pad="7"/>
<connect gate="G$1" pin="VDD1" pad="28"/>
<connect gate="G$1" pin="VDD2" pad="40"/>
<connect gate="G$1" pin="VSS0" pad="6"/>
<connect gate="G$1" pin="VSS1" pad="29"/>
<connect gate="G$1" pin="VSS2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM406_OUTLINE">
<gates>
<gate name="G$1" symbol="EM406_OUTLINE"/>
</gates>
<devices>
<device name="" package="EM406_OUTLINE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ID-12/20">
<description>ID2, ID12, and ID20 Package</description>
<gates>
<gate name="G$1" symbol="ID-12"/>
</gates>
<devices>
<device name="" package="ID-12">
<connects>
<connect gate="G$1" pin="+/-" pad="7"/>
<connect gate="G$1" pin="5V" pad="11"/>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="FUTURE" pad="6"/>
<connect gate="G$1" pin="GNDT" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ID-12_LOCK" package="ID-12_LOCK">
<connects>
<connect gate="G$1" pin="+/-" pad="7"/>
<connect gate="G$1" pin="5V" pad="11"/>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="FUTURE" pad="6"/>
<connect gate="G$1" pin="GNDT" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="ID-12_SMD">
<connects>
<connect gate="G$1" pin="+/-" pad="7"/>
<connect gate="G$1" pin="5V" pad="11"/>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="FUTURE" pad="6"/>
<connect gate="G$1" pin="GNDT" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF24G">
<description>&lt;b&gt;RF24G Header&lt;/b&gt; This is the header for connections to the RF24G Transceiver (SparkFun Electronics SKU: WRL-00151), used in the Breakout Board for RF24G Transceiver (SparkFun Electronics SKU: BOB-00196). This footprint has not yet been proven in production.</description>
<gates>
<gate name="G$1" symbol="RF24G"/>
</gates>
<devices>
<device name="" package="RF24G-2X5">
<connects>
<connect gate="G$1" pin="CE" pad="2"/>
<connect gate="G$1" pin="CLK1" pad="5"/>
<connect gate="G$1" pin="CLK2" pad="3"/>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="DATA" pad="6"/>
<connect gate="G$1" pin="DOUT2" pad="8"/>
<connect gate="G$1" pin="DR1" pad="7"/>
<connect gate="G$1" pin="DR2" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.8V">
<gates>
<gate name="G$1" symbol="1.8V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC-ICSP">
<description>ISCP Programming connector for UAV, UBW Kit, etc.</description>
<gates>
<gate name="G$1" symbol="ICSP-PIC"/>
</gates>
<devices>
<device name="PTH" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PGC" pad="2"/>
<connect gate="G$1" pin="PGD" pad="3"/>
<connect gate="G$1" pin="PGM" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VPP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PGC" pad="2"/>
<connect gate="G$1" pin="PGD" pad="3"/>
<connect gate="G$1" pin="PGM" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VPP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MN5010HS">
<description>MN5010HS GPS Receiver Module. Packagse GR-10 and MN5010HS are NOT tested with this device.</description>
<gates>
<gate name="G$1" symbol="MN5010HS"/>
</gates>
<devices>
<device name="SMD" package="MN5010HS">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="GR-10">
<connects>
<connect gate="G$1" pin="1PPS" pad="9"/>
<connect gate="G$1" pin="ANT" pad="30"/>
<connect gate="G$1" pin="BATT" pad="33"/>
<connect gate="G$1" pin="GND11" pad="11"/>
<connect gate="G$1" pin="GND2" pad="2"/>
<connect gate="G$1" pin="GND24" pad="24"/>
<connect gate="G$1" pin="GND27" pad="27"/>
<connect gate="G$1" pin="GND29" pad="29"/>
<connect gate="G$1" pin="GND31" pad="31"/>
<connect gate="G$1" pin="GND4" pad="4"/>
<connect gate="G$1" pin="NAV" pad="20"/>
<connect gate="G$1" pin="NMR" pad="23"/>
<connect gate="G$1" pin="ONOFF" pad="22"/>
<connect gate="G$1" pin="OPT1" pad="13"/>
<connect gate="G$1" pin="OPT2" pad="14"/>
<connect gate="G$1" pin="RX-I" pad="7"/>
<connect gate="G$1" pin="TX-O" pad="8"/>
<connect gate="G$1" pin="VIO" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GAS_SENSOR" prefix="U">
<description>MQ-3 Gas Sensor. FP not tested. Part#</description>
<gates>
<gate name="G$1" symbol="MQ-3"/>
</gates>
<devices>
<device name="" package="MQ-3">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="H1" pad="HA"/>
<connect gate="G$1" pin="H2" pad="HB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M02NG">
<gates>
<gate name="G$1" symbol="M02NG"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M20" prefix="JP">
<description>This is just like the LOCK variant in that the holes are staggared by 5 mil, but except for the last two holes.  They are not altered from the "standard" footprint layout.  This is used for a special purpose on the layout of our Graphic LCD Backpack.  Make sure you want to use this device before selecting it for you project!</description>
<gates>
<gate name="G$1" symbol="M20"/>
</gates>
<devices>
<device name="" package="1X20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X20_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X20_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="1X20_LOCK_SPECIAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M10X2">
<description>This was SPECIALLY designed to be used with our Graphic LCD Backpack.  Be sure you want to use this!  It is not only staggered on each line of header holes, but IT IS ALSO offset of the center point of the top and bottom lines by 5 mil.  This causes the headers to lock into place on the "standard" footprint on the LCD screen.  The extra squares on the tdocu layer are there simply to reference other pins (if you were to actually populate a longer header than ten long - this is what we do with the backpacks).</description>
<gates>
<gate name="G$1" symbol="M10X2"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X10_LOCK" package="2X10_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="2X10_LOCK_SPECIAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOSILK" package="2X10_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACS712">
<gates>
<gate name="G$1" symbol="ACS712"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="FILT" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IP+@1" pad="1"/>
<connect gate="G$1" pin="IP+@2" pad="2"/>
<connect gate="G$1" pin="IP-@3" pad="3"/>
<connect gate="G$1" pin="IP-@4" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45-8">
<description>&lt;b&gt;RJ45 Jack&lt;/b&gt;
Simple RJ45, 8-pin connection - connector for common Cat5, Cat5e, and Cat6 Ethernet cables. Footprint not yet proven in production. Connector sku is PRT-00643; Breakout PCB sku is BOB-00716.</description>
<gates>
<gate name="G$1" symbol="RJ45-8"/>
</gates>
<devices>
<device name="PTH" package="RJ45-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24LU1">
<gates>
<gate name="G$1" symbol="NRF24LU1"/>
</gates>
<devices>
<device name="" package="QFN-32">
<connects>
<connect gate="G$1" pin="/RESET" pad="8"/>
<connect gate="G$1" pin="ANT1" pad="21"/>
<connect gate="G$1" pin="ANT2" pad="22"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="5"/>
<connect gate="G$1" pin="DEC1" pad="28"/>
<connect gate="G$1" pin="DEC2" pad="29"/>
<connect gate="G$1" pin="IREF" pad="25"/>
<connect gate="G$1" pin="P0.0" pad="10"/>
<connect gate="G$1" pin="P0.1" pad="11"/>
<connect gate="G$1" pin="P0.2" pad="13"/>
<connect gate="G$1" pin="P0.3" pad="14"/>
<connect gate="G$1" pin="P0.4" pad="15"/>
<connect gate="G$1" pin="P0.5" pad="16"/>
<connect gate="G$1" pin="PROG" pad="7"/>
<connect gate="G$1" pin="VBUS" pad="2"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="3"/>
<connect gate="G$1" pin="VDD3" pad="9"/>
<connect gate="G$1" pin="VDD4" pad="19"/>
<connect gate="G$1" pin="VDD5" pad="24"/>
<connect gate="G$1" pin="VDD6" pad="27"/>
<connect gate="G$1" pin="VDD_PA" pad="20"/>
<connect gate="G$1" pin="VSS1" pad="6"/>
<connect gate="G$1" pin="VSS2" pad="12"/>
<connect gate="G$1" pin="VSS3" pad="17"/>
<connect gate="G$1" pin="VSS4" pad="18"/>
<connect gate="G$1" pin="VSS5" pad="23"/>
<connect gate="G$1" pin="VSS6" pad="26"/>
<connect gate="G$1" pin="VSS7" pad="30"/>
<connect gate="G$1" pin="XC1" pad="32"/>
<connect gate="G$1" pin="XC2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13">
<gates>
<gate name="G$1" symbol="ATTINY13"/>
</gates>
<devices>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP" package="DIP08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QRD1114">
<gates>
<gate name="G$1" symbol="QRD1114"/>
</gates>
<devices>
<device name="" package="QRD1114">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8575C">
<description>PCF8575C I/O Expander.</description>
<gates>
<gate name="G$1" symbol="PCF8575C"/>
</gates>
<devices>
<device name="" package="SO-24DW">
<connects>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INT" pad="1"/>
<connect gate="G$1" pin="P10" pad="13"/>
<connect gate="G$1" pin="P11" pad="14"/>
<connect gate="G$1" pin="P12" pad="15"/>
<connect gate="G$1" pin="P13" pad="16"/>
<connect gate="G$1" pin="P14" pad="17"/>
<connect gate="G$1" pin="P15" pad="18"/>
<connect gate="G$1" pin="P16" pad="19"/>
<connect gate="G$1" pin="P17" pad="20"/>
<connect gate="G$1" pin="PO0" pad="4"/>
<connect gate="G$1" pin="PO1" pad="5"/>
<connect gate="G$1" pin="PO2" pad="6"/>
<connect gate="G$1" pin="PO3" pad="7"/>
<connect gate="G$1" pin="PO4" pad="8"/>
<connect gate="G$1" pin="PO5" pad="9"/>
<connect gate="G$1" pin="PO6" pad="10"/>
<connect gate="G$1" pin="PO7" pad="11"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24LE1">
<gates>
<gate name="G$1" symbol="NRF24LE1"/>
</gates>
<devices>
<device name="" package="QFN-32">
<connects>
<connect gate="G$1" pin="ANT1" pad="21"/>
<connect gate="G$1" pin="ANT2" pad="22"/>
<connect gate="G$1" pin="DEC1" pad="3"/>
<connect gate="G$1" pin="DEC2" pad="4"/>
<connect gate="G$1" pin="IREF" pad="25"/>
<connect gate="G$1" pin="P0.0" pad="32"/>
<connect gate="G$1" pin="P0.1" pad="1"/>
<connect gate="G$1" pin="P0.2" pad="5"/>
<connect gate="G$1" pin="P0.3" pad="7"/>
<connect gate="G$1" pin="P0.4" pad="10"/>
<connect gate="G$1" pin="P0.5" pad="11"/>
<connect gate="G$1" pin="P0.6" pad="12"/>
<connect gate="G$1" pin="P0.7" pad="13"/>
<connect gate="G$1" pin="P1.0" pad="14"/>
<connect gate="G$1" pin="P1.1" pad="15"/>
<connect gate="G$1" pin="P1.2" pad="16"/>
<connect gate="G$1" pin="P1.3" pad="17"/>
<connect gate="G$1" pin="P1.4" pad="18"/>
<connect gate="G$1" pin="P1.5" pad="28"/>
<connect gate="G$1" pin="P1.6" pad="29"/>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="9"/>
<connect gate="G$1" pin="VDD3" pad="24"/>
<connect gate="G$1" pin="VDD4" pad="27"/>
<connect gate="G$1" pin="VDD_PA" pad="20"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="23"/>
<connect gate="G$1" pin="VSS3" pad="26"/>
<connect gate="G$1" pin="XC1" pad="31"/>
<connect gate="G$1" pin="XC2" pad="30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CREATIVE_COMMONS">
<gates>
<gate name="G$1" symbol="CREATIVE_COMMONS"/>
</gates>
<devices>
<device name="" package="CREATIVE_COMMONS">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FC30">
<description>Simple directional accelerometer. Outputs 1 of 6 positions in space.</description>
<gates>
<gate name="G$1" symbol="FC30"/>
</gates>
<devices>
<device name="SMD" package="LGA14">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="LC" pad="9"/>
<connect gate="G$1" pin="PC" pad="8"/>
<connect gate="G$1" pin="PD" pad="11"/>
<connect gate="G$1" pin="RES@10" pad="10"/>
<connect gate="G$1" pin="RES@13" pad="13"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@4" pad="4"/>
<connect gate="G$1" pin="RES@7" pad="7"/>
<connect gate="G$1" pin="SIGN" pad="12"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
<connect gate="G$1" pin="VDD@6" pad="6"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LISY300AL">
<description>Untested part for LIS300AL.</description>
<gates>
<gate name="G$1" symbol="LISY300AL"/>
</gates>
<devices>
<device name="SMD" package="LGA28">
<connects>
<connect gate="G$1" pin="AOUT" pad="6"/>
<connect gate="G$1" pin="CACT" pad="5"/>
<connect gate="G$1" pin="FVDD" pad="24"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="PD" pad="10"/>
<connect gate="G$1" pin="ST" pad="11"/>
<connect gate="G$1" pin="VCONT" pad="23"/>
<connect gate="G$1" pin="VDD" pad="25"/>
<connect gate="G$1" pin="VDD1" pad="26"/>
<connect gate="G$1" pin="VDD2" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY">
<gates>
<gate name="G$1" symbol="RELAY-SPDT"/>
</gates>
<devices>
<device name="PTH" package="RELAY-G5Q">
<connects>
<connect gate="G$1" pin="COIL1" pad="5"/>
<connect gate="G$1" pin="COIL2" pad="1"/>
<connect gate="G$1" pin="MAIN" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="RELAY-T9A">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="MAIN"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="RELAY-T9A-2">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="MAIN"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="RELAY-JZC">
<connects>
<connect gate="G$1" pin="COIL1" pad="5"/>
<connect gate="G$1" pin="COIL2" pad="1"/>
<connect gate="G$1" pin="MAIN" pad="4"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ9">
<gates>
<gate name="G$1" symbol="M04-1"/>
</gates>
<devices>
<device name="PTH" package="RJ9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-2">
<gates>
<gate name="G$1" symbol="RELAY-SPDT-2"/>
</gates>
<devices>
<device name="G5Q" package="RELAY-G5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL3232">
<gates>
<gate name="G$1" symbol="ICL3232"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIN7">
<gates>
<gate name="G$1" symbol="DIN7"/>
</gates>
<devices>
<device name="" package="DIN7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1103">
<gates>
<gate name="G$1" symbol="VS1103"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="CVDD1" pad="5"/>
<connect gate="G$1" pin="CVDD2" pad="7"/>
<connect gate="G$1" pin="CVDD3" pad="24"/>
<connect gate="G$1" pin="CVDD4" pad="31"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DVDD1" pad="6"/>
<connect gate="G$1" pin="DVDD2" pad="14"/>
<connect gate="G$1" pin="DVDD3" pad="19"/>
<connect gate="G$1" pin="D_REQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="SO" pad="30"/>
<connect gate="G$1" pin="SPIBOOT/GPIO0" pad="33"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL0" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRF-24G">
<gates>
<gate name="G$1" symbol="TRF-24G"/>
</gates>
<devices>
<device name="" package="TRF-24G-SOCKET">
<connects>
<connect gate="G$1" pin="CE" pad="P$9"/>
<connect gate="G$1" pin="CLK1" pad="P$6"/>
<connect gate="G$1" pin="CLK2" pad="P$8"/>
<connect gate="G$1" pin="CS" pad="P$7"/>
<connect gate="G$1" pin="DATA" pad="P$5"/>
<connect gate="G$1" pin="DOUT2" pad="P$3"/>
<connect gate="G$1" pin="DR1" pad="P$4"/>
<connect gate="G$1" pin="DR2" pad="P$2"/>
<connect gate="G$1" pin="GND" pad="P$10"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL180">
<gates>
<gate name="G$1" symbol="ADXL180"/>
</gates>
<devices>
<device name="" package="ADXL180">
<connects>
<connect gate="G$1" pin="VBC" pad="9"/>
<connect gate="G$1" pin="VBN@10" pad="10"/>
<connect gate="G$1" pin="VBN@18" pad="18"/>
<connect gate="G$1" pin="VBN@3" pad="3"/>
<connect gate="G$1" pin="VBN@8" pad="8"/>
<connect gate="G$1" pin="VBP" pad="12"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSCI" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OS4000-T">
<description>OS4000-T Device</description>
<gates>
<gate name="G$1" symbol="OS4000-T"/>
</gates>
<devices>
<device name="" package="OS4000-T">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSOP28">
<gates>
<gate name="G$1" symbol="SSOP28"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MUX-74HC4067">
<gates>
<gate name="G$1" symbol="CD74HC4067"/>
</gates>
<devices>
<device name="SMD" package="SSOP24">
<connects>
<connect gate="G$1" pin="CHAN0" pad="9"/>
<connect gate="G$1" pin="CHAN1" pad="8"/>
<connect gate="G$1" pin="CHAN10" pad="21"/>
<connect gate="G$1" pin="CHAN11" pad="20"/>
<connect gate="G$1" pin="CHAN12" pad="19"/>
<connect gate="G$1" pin="CHAN13" pad="18"/>
<connect gate="G$1" pin="CHAN14" pad="17"/>
<connect gate="G$1" pin="CHAN15" pad="16"/>
<connect gate="G$1" pin="CHAN2" pad="7"/>
<connect gate="G$1" pin="CHAN3" pad="6"/>
<connect gate="G$1" pin="CHAN4" pad="5"/>
<connect gate="G$1" pin="CHAN5" pad="4"/>
<connect gate="G$1" pin="CHAN6" pad="3"/>
<connect gate="G$1" pin="CHAN7" pad="2"/>
<connect gate="G$1" pin="CHAN8" pad="23"/>
<connect gate="G$1" pin="CHAN9" pad="22"/>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="EN" pad="15"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="S0" pad="10"/>
<connect gate="G$1" pin="S1" pad="11"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="13"/>
<connect gate="G$1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK" prefix="U">
<description>&lt;b&gt;Thumb Joystick&lt;/b&gt;
Joystick commonly found in PS2 controllers. Two pots and a select switch. Footprint proven. Spark Fun Electronics SKU : COM-09032</description>
<gates>
<gate name="G$1" symbol="JOYSTICK"/>
</gates>
<devices>
<device name="PTH" package="JOYSTICK">
<connects>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="H+" pad="H1"/>
<connect gate="G$1" pin="H-" pad="H3"/>
<connect gate="G$1" pin="SEL+" pad="B1A"/>
<connect gate="G$1" pin="SEL-" pad="B2A"/>
<connect gate="G$1" pin="V" pad="V2"/>
<connect gate="G$1" pin="V+" pad="V1"/>
<connect gate="G$1" pin="V-" pad="V3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UM-FPU_V3_1">
<gates>
<gate name="G$1" symbol="UM-FPU_V3_1"/>
</gates>
<devices>
<device name="DIL" package="DIL18">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="AN0" pad="2"/>
<connect gate="G$1" pin="AN1" pad="3"/>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="AVSS" pad="17"/>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="EXTIN" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="6"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="OUT0" pad="15"/>
<connect gate="G$1" pin="OUT1" pad="10"/>
<connect gate="G$1" pin="SCLK" pad="16"/>
<connect gate="G$1" pin="SERIN" pad="9"/>
<connect gate="G$1" pin="SEROUT" pad="8"/>
<connect gate="G$1" pin="SIN/SDA" pad="12"/>
<connect gate="G$1" pin="SOUT/SCL" pad="11"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO" package="SOIC18-W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="AN0" pad="2"/>
<connect gate="G$1" pin="AN1" pad="3"/>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="AVSS" pad="17"/>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="EXTIN" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="6"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="OUT0" pad="15"/>
<connect gate="G$1" pin="OUT1" pad="10"/>
<connect gate="G$1" pin="SCLK" pad="16"/>
<connect gate="G$1" pin="SERIN" pad="9"/>
<connect gate="G$1" pin="SEROUT" pad="8"/>
<connect gate="G$1" pin="SIN/SDA" pad="12"/>
<connect gate="G$1" pin="SOUT/SCL" pad="11"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVP5150-NTSC_DECODER">
<description>*** UNPROVEN FOOTPRINT ***
Texas Instrument NTSC/PAL Decoder
TI Part #TVP5150AM1
Digikey Part #

Decodes NTSC video signal to YCbCr 4:2:2 signal</description>
<gates>
<gate name="G$1" symbol="TVP5150-NTSC_DECODER-1"/>
</gates>
<devices>
<device name="" package="TQFP32-5MM">
<connects>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="AIP1A" pad="1"/>
<connect gate="G$1" pin="AIP1B" pad="2"/>
<connect gate="G$1" pin="AVID" pad="26"/>
<connect gate="G$1" pin="CH_AGND" pad="31"/>
<connect gate="G$1" pin="CH_AVDD" pad="32"/>
<connect gate="G$1" pin="DGND" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="FID/GLCO" pad="23"/>
<connect gate="G$1" pin="HSYNC" pad="25"/>
<connect gate="G$1" pin="INT_REQ" pad="27"/>
<connect gate="G$1" pin="IO_DVDD" pad="10"/>
<connect gate="G$1" pin="PCLK/SCLK" pad="9"/>
<connect gate="G$1" pin="PDN" pad="28"/>
<connect gate="G$1" pin="PLL_AGND" pad="3"/>
<connect gate="G$1" pin="PLL_AVDD" pad="4"/>
<connect gate="G$1" pin="REFM" pad="30"/>
<connect gate="G$1" pin="REFP" pad="29"/>
<connect gate="G$1" pin="RESET/" pad="8"/>
<connect gate="G$1" pin="SCL" pad="21"/>
<connect gate="G$1" pin="SDA" pad="22"/>
<connect gate="G$1" pin="VSYNC" pad="24"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="6"/>
<connect gate="G$1" pin="YOUT_0" pad="18"/>
<connect gate="G$1" pin="YOUT_1" pad="17"/>
<connect gate="G$1" pin="YOUT_2" pad="16"/>
<connect gate="G$1" pin="YOUT_3" pad="15"/>
<connect gate="G$1" pin="YOUT_4" pad="14"/>
<connect gate="G$1" pin="YOUT_5" pad="13"/>
<connect gate="G$1" pin="YOUT_6" pad="12"/>
<connect gate="G$1" pin="YOUT_7" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL345" prefix="U">
<gates>
<gate name="G$1" symbol="ADXL345"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="INT1" pad="8"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC@10" pad="10"/>
<connect gate="G$1" pin="NC@11" pad="11"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDG1215">
<gates>
<gate name="G$1" symbol="IDG1215"/>
</gates>
<devices>
<device name="-1215" package="IDG500">
<connects>
<connect gate="G$1" pin="AZ" pad="24"/>
<connect gate="G$1" pin="CPOUT" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="PTATS" pad="23"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
<connect gate="G$1" pin="XAGC" pad="6"/>
<connect gate="G$1" pin="XHP1" pad="1"/>
<connect gate="G$1" pin="XHP2" pad="5"/>
<connect gate="G$1" pin="XOUT" pad="7"/>
<connect gate="G$1" pin="YAGC" pad="15"/>
<connect gate="G$1" pin="YHP1" pad="20"/>
<connect gate="G$1" pin="YHP2" pad="16"/>
<connect gate="G$1" pin="YOUT" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LY530AL">
<description>LY530AL</description>
<gates>
<gate name="G$1" symbol="LY530AL"/>
</gates>
<devices>
<device name="SMD" package="LGA16">
<connects>
<connect gate="G$1" pin="AOUT" pad="4"/>
<connect gate="G$1" pin="CACT" pad="3"/>
<connect gate="G$1" pin="CS" pad="10"/>
<connect gate="G$1" pin="DIS" pad="5"/>
<connect gate="G$1" pin="DR" pad="11"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="PD" pad="8"/>
<connect gate="G$1" pin="PLL1" pad="2"/>
<connect gate="G$1" pin="PLL2" pad="1"/>
<connect gate="G$1" pin="RES" pad="14"/>
<connect gate="G$1" pin="SCL" pad="9"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="ST" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="16"/>
<connect gate="G$1" pin="VDDD" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VENUS634">
<description>Venus634 from SkyTraq</description>
<gates>
<gate name="G$1" symbol="VENUS634FLPX"/>
</gates>
<devices>
<device name="SMD" package="LGA44">
<connects>
<connect gate="G$1" pin="BTSEL" pad="9"/>
<connect gate="G$1" pin="CLK" pad="41"/>
<connect gate="G$1" pin="CSN" pad="43"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GNDRF@21" pad="21"/>
<connect gate="G$1" pin="GNDRF@22" pad="22"/>
<connect gate="G$1" pin="GNDRF@24" pad="24"/>
<connect gate="G$1" pin="GNDRF@25" pad="25"/>
<connect gate="G$1" pin="GNDRF@27" pad="27"/>
<connect gate="G$1" pin="GNDRF@28" pad="28"/>
<connect gate="G$1" pin="GNDRF@29" pad="29"/>
<connect gate="G$1" pin="GNDRF@31" pad="31"/>
<connect gate="G$1" pin="GNDRF@33" pad="33"/>
<connect gate="G$1" pin="GPIO1" pad="6"/>
<connect gate="G$1" pin="GPIO2" pad="5"/>
<connect gate="G$1" pin="GPIO20" pad="14"/>
<connect gate="G$1" pin="GPIO24" pad="8"/>
<connect gate="G$1" pin="LED" pad="7"/>
<connect gate="G$1" pin="MISO" pad="39"/>
<connect gate="G$1" pin="MOSI" pad="38"/>
<connect gate="G$1" pin="PIO12" pad="4"/>
<connect gate="G$1" pin="PIO14" pad="37"/>
<connect gate="G$1" pin="PPS" pad="40"/>
<connect gate="G$1" pin="REGEN" pad="36"/>
<connect gate="G$1" pin="RFIN" pad="32"/>
<connect gate="G$1" pin="RSTN" pad="1"/>
<connect gate="G$1" pin="RTC" pad="17"/>
<connect gate="G$1" pin="RX" pad="42"/>
<connect gate="G$1" pin="TX" pad="44"/>
<connect gate="G$1" pin="VBAT" pad="18"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1077">
<gates>
<gate name="G$1" symbol="DS1077"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CTRL0" pad="5"/>
<connect gate="G$1" pin="CTRL1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT0" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UBW32_PIC32MX4XXL">
<gates>
<gate name="G$1" symbol="UBW32_PIC32MX4XXL"/>
</gates>
<devices>
<device name="TQFP100" package="UBW32_TQFP100">
<connects>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="C1IN-/AN4/CN6/RB4" pad="21"/>
<connect gate="G$1" pin="C1OUT/AN8/RB8" pad="32"/>
<connect gate="G$1" pin="C2IN+/AN3/CN5/RB3" pad="22"/>
<connect gate="G$1" pin="C2IN-/AN2/CN4/RB2" pad="23"/>
<connect gate="G$1" pin="C2OUT/AN9/RB9" pad="33"/>
<connect gate="G$1" pin="CN20/U1CTS/RD14" pad="47"/>
<connect gate="G$1" pin="CVREFOUT/PMA13/AN10/RB10" pad="34"/>
<connect gate="G$1" pin="D+/RG2" pad="57"/>
<connect gate="G$1" pin="D-/RG3" pad="56"/>
<connect gate="G$1" pin="ENVREG" pad="86"/>
<connect gate="G$1" pin="IC1/RTCC/RD8" pad="68"/>
<connect gate="G$1" pin="IC2/SS1/RD9" pad="69"/>
<connect gate="G$1" pin="IC3/SCKI/PMCS2/PMA15/RD10" pad="70"/>
<connect gate="G$1" pin="IC4/PMCS1/PMA14/RD11" pad="71"/>
<connect gate="G$1" pin="INT1/RE8" pad="18"/>
<connect gate="G$1" pin="INT2/RE9" pad="19"/>
<connect gate="G$1" pin="MCLR" pad="13"/>
<connect gate="G$1" pin="OC2/RD1" pad="76"/>
<connect gate="G$1" pin="OC3/RD2" pad="77"/>
<connect gate="G$1" pin="OC4/RD3" pad="78"/>
<connect gate="G$1" pin="OSC1/CLKI/RC12" pad="63"/>
<connect gate="G$1" pin="OSC2/CLKO/RC15" pad="64"/>
<connect gate="G$1" pin="PGC1/EMUC1/AN1/CN3/RB1" pad="24"/>
<connect gate="G$1" pin="PGC2/EMUC2/AN6/OCFA/RB6" pad="26"/>
<connect gate="G$1" pin="PGD1/EMUD1/AN0/CN2/RB0" pad="25"/>
<connect gate="G$1" pin="PGD2/EMUD2/AN7/RB7" pad="27"/>
<connect gate="G$1" pin="PMA10/AN13/RB13" pad="42"/>
<connect gate="G$1" pin="PMA11/AN12/RB12" pad="41"/>
<connect gate="G$1" pin="PMA12/AN11/RB11" pad="35"/>
<connect gate="G$1" pin="PMA2/SS2/CN11/RG9" pad="14"/>
<connect gate="G$1" pin="PMA3/SDO2/CN10/RG8" pad="12"/>
<connect gate="G$1" pin="PMA4/SDI2/CN9/RG7" pad="11"/>
<connect gate="G$1" pin="PMA5/SCK2/CN8/RG6" pad="10"/>
<connect gate="G$1" pin="PMA6/VREF+/CVREF+/RA10" pad="29"/>
<connect gate="G$1" pin="PMA7/VREF-/CVREF-/RA9" pad="28"/>
<connect gate="G$1" pin="PMA8/U2TX/CN18/RF5" pad="50"/>
<connect gate="G$1" pin="PMA9/U2RX/CN17/RF4" pad="49"/>
<connect gate="G$1" pin="PMALH/PMA1/AN14/RB14" pad="43"/>
<connect gate="G$1" pin="PMALL/PMA0/AN15/OCFB/CN12/RB15" pad="44"/>
<connect gate="G$1" pin="PMD0/RE0" pad="93"/>
<connect gate="G$1" pin="PMD1/RE1" pad="94"/>
<connect gate="G$1" pin="PMD10/RF1" pad="88"/>
<connect gate="G$1" pin="PMD11/RF0" pad="87"/>
<connect gate="G$1" pin="PMD12/IC5/RD12" pad="79"/>
<connect gate="G$1" pin="PMD13/CN19/RD13" pad="80"/>
<connect gate="G$1" pin="PMD14/CN15/RD6" pad="83"/>
<connect gate="G$1" pin="PMD15/CN16/RD7" pad="84"/>
<connect gate="G$1" pin="PMD2/RE2" pad="98"/>
<connect gate="G$1" pin="PMD3/RE3" pad="99"/>
<connect gate="G$1" pin="PMD4/RE4" pad="100"/>
<connect gate="G$1" pin="PMD5/RE5" pad="3"/>
<connect gate="G$1" pin="PMD6/RE6" pad="4"/>
<connect gate="G$1" pin="PMD7/RE7" pad="5"/>
<connect gate="G$1" pin="PMD8/RG0" pad="90"/>
<connect gate="G$1" pin="PMD9/RG1" pad="89"/>
<connect gate="G$1" pin="PMRD/CN14/RD5" pad="82"/>
<connect gate="G$1" pin="PMWR/OC5/CN13/RD4" pad="81"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="SCL1/INT3/RA14" pad="66"/>
<connect gate="G$1" pin="SCL2/RA2" pad="58"/>
<connect gate="G$1" pin="SDA1/INT4/RA15" pad="67"/>
<connect gate="G$1" pin="SDA2/RA3" pad="59"/>
<connect gate="G$1" pin="SDI1/T5CK/RC4" pad="9"/>
<connect gate="G$1" pin="SDO1/OC1/INT0/RD0" pad="72"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="73"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="74"/>
<connect gate="G$1" pin="T2CK/RC1" pad="6"/>
<connect gate="G$1" pin="T3CK/RC2" pad="7"/>
<connect gate="G$1" pin="T4CK/RC3" pad="8"/>
<connect gate="G$1" pin="TCK/RA1" pad="38"/>
<connect gate="G$1" pin="TDI/RA4" pad="60"/>
<connect gate="G$1" pin="TDO/RA5" pad="61"/>
<connect gate="G$1" pin="TMS/RA0" pad="17"/>
<connect gate="G$1" pin="TRCLK/RA6" pad="91"/>
<connect gate="G$1" pin="TRD0/RG13" pad="97"/>
<connect gate="G$1" pin="TRD1/RG12" pad="96"/>
<connect gate="G$1" pin="TRD2/RG14" pad="95"/>
<connect gate="G$1" pin="TRD3/RA7" pad="92"/>
<connect gate="G$1" pin="U1RTS/BCLK1/CN21/RD15" pad="48"/>
<connect gate="G$1" pin="U1RX/RF2" pad="52"/>
<connect gate="G$1" pin="U1TX/RF8" pad="53"/>
<connect gate="G$1" pin="U2CTS/RF12" pad="40"/>
<connect gate="G$1" pin="U2RTS/BCLK2/RF13" pad="39"/>
<connect gate="G$1" pin="USBID/RF3" pad="51"/>
<connect gate="G$1" pin="VBUS" pad="54"/>
<connect gate="G$1" pin="VBUSON/C1IN+/AN5/CN7/RB5" pad="20"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="85"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VDD3" pad="37"/>
<connect gate="G$1" pin="VDD4" pad="46"/>
<connect gate="G$1" pin="VDD5" pad="62"/>
<connect gate="G$1" pin="VSS1" pad="15"/>
<connect gate="G$1" pin="VSS2" pad="36"/>
<connect gate="G$1" pin="VSS3" pad="45"/>
<connect gate="G$1" pin="VSS4" pad="65"/>
<connect gate="G$1" pin="VSS6" pad="75"/>
<connect gate="G$1" pin="VUSB" pad="55"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPENSERVO_VIA">
<gates>
<gate name="G$1" symbol="M01"/>
</gates>
<devices>
<device name="" package="OPENSERVO_VIA">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMPERATURE-SENSOR">
<gates>
<gate name="G$1" symbol="TEMPERATURE-SENSOR"/>
</gates>
<devices>
<device name="" package="TO-92">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXRSXXX">
<description>ADXRS6xx, ADXRS150, 300, and 401</description>
<gates>
<gate name="G$1" symbol="ADXRS"/>
</gates>
<devices>
<device name="SMD" package="BC-32">
<connects>
<connect gate="G$1" pin="AGND" pad="AGND"/>
<connect gate="G$1" pin="AVCC" pad="AVCC"/>
<connect gate="G$1" pin="CP1" pad="CP1"/>
<connect gate="G$1" pin="CP2" pad="CP2"/>
<connect gate="G$1" pin="CP3" pad="CP3"/>
<connect gate="G$1" pin="CP4" pad="CP4"/>
<connect gate="G$1" pin="CP5" pad="CP5"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="PGND" pad="PGND"/>
<connect gate="G$1" pin="RATEOUT" pad="RATEOUT"/>
<connect gate="G$1" pin="ST1" pad="ST1"/>
<connect gate="G$1" pin="ST2" pad="ST2"/>
<connect gate="G$1" pin="SUMJ" pad="SUMJ"/>
<connect gate="G$1" pin="TEMP" pad="TEMP"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
<connect gate="G$1" pin="VRATIO" pad="VRATIO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-DISPLAY">
<gates>
<gate name="G$1" symbol="7-SEGMENT-DISPLAY"/>
</gates>
<devices>
<device name="PTH" package="7-SEGMENT-DISPLAY">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEF4543">
<gates>
<gate name="G$1" symbol="HEF4543"/>
</gates>
<devices>
<device name="PTH" package="DIL16">
<connects>
<connect gate="G$1" pin="A" pad="9"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="BL" pad="7"/>
<connect gate="G$1" pin="C" pad="11"/>
<connect gate="G$1" pin="D" pad="12"/>
<connect gate="G$1" pin="D0" pad="5"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="4"/>
<connect gate="G$1" pin="E" pad="13"/>
<connect gate="G$1" pin="F" pad="15"/>
<connect gate="G$1" pin="G" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LD" pad="1"/>
<connect gate="G$1" pin="PH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-MOMENTARY-2" prefix="S">
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-2"/>
</gates>
<devices>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TACTILE_SWITCH_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-2" package="TACTILE_SWITCH_SMD-2">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="12MM" package="TACTILE-PTH-12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-1101NE" package="TACTILE-SWITCH-1101NE">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_REED" package="REED_SWITCH_PTH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TACTILE_SWITCH_TALL">
<connects>
<connect gate="G$1" pin="1" pad="A2"/>
<connect gate="G$1" pin="2" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_REED2" package="REED_SWITCH_PLASTIC">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-4DIGIT">
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT"/>
</gates>
<devices>
<device name="PTH" package="7-SEGMENT-4DIGIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FOR_POGOBED_ONLY" package="7-SEGMENT-4DIGIT_LONGPADS_FOR_POGOBED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGNET">
<gates>
<gate name="G$1" symbol="MAGNET"/>
</gates>
<devices>
<device name="18MM" package="MAGNET-18MM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7456">
<gates>
<gate name="G$1" symbol="MAX7456"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AVDD" pad="21"/>
<connect gate="G$1" pin="CLKIN" pad="5"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="DGND" pad="4"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="11"/>
<connect gate="G$1" pin="DVDD" pad="3"/>
<connect gate="G$1" pin="LOS" pad="12"/>
<connect gate="G$1" pin="PGND" pad="23"/>
<connect gate="G$1" pin="PVDD" pad="24"/>
<connect gate="G$1" pin="SAG" pad="25"/>
<connect gate="G$1" pin="SCK" pad="10"/>
<connect gate="G$1" pin="VIN" pad="22"/>
<connect gate="G$1" pin="VOUT" pad="26"/>
<connect gate="G$1" pin="XFB" pad="6"/>
<connect gate="G$1" pin="~CS" pad="8"/>
<connect gate="G$1" pin="~HSYNC" pad="18"/>
<connect gate="G$1" pin="~RESET" pad="19"/>
<connect gate="G$1" pin="~VSYNC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GROUNDPAD" package="TSSOP28-GROUNDPAD">
<connects>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AVDD" pad="21"/>
<connect gate="G$1" pin="CLKIN" pad="5"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="DGND" pad="4"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="11"/>
<connect gate="G$1" pin="DVDD" pad="3"/>
<connect gate="G$1" pin="LOS" pad="12"/>
<connect gate="G$1" pin="PGND" pad="23"/>
<connect gate="G$1" pin="PVDD" pad="24"/>
<connect gate="G$1" pin="SAG" pad="25"/>
<connect gate="G$1" pin="SCK" pad="10"/>
<connect gate="G$1" pin="VIN" pad="22"/>
<connect gate="G$1" pin="VOUT" pad="26"/>
<connect gate="G$1" pin="XFB" pad="6"/>
<connect gate="G$1" pin="~CS" pad="8"/>
<connect gate="G$1" pin="~HSYNC" pad="18"/>
<connect gate="G$1" pin="~RESET" pad="19"/>
<connect gate="G$1" pin="~VSYNC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPI_FLASH-X25XX">
<description>8pin SPI Flash series x25xx. Works with devices like W25X32 and BR25L32</description>
<gates>
<gate name="G$1" symbol="SPI_FLASH"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD1" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9835">
<gates>
<gate name="G$1" symbol="AD9835"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="15"/>
<connect gate="G$1" pin="COMP" pad="16"/>
<connect gate="G$1" pin="DGND" pad="5"/>
<connect gate="G$1" pin="DVDD" pad="4"/>
<connect gate="G$1" pin="FSEL" pad="10"/>
<connect gate="G$1" pin="FSYNC" pad="9"/>
<connect gate="G$1" pin="FS_ADJ" pad="1"/>
<connect gate="G$1" pin="IOUT" pad="14"/>
<connect gate="G$1" pin="MCLK" pad="6"/>
<connect gate="G$1" pin="PSEL0" pad="12"/>
<connect gate="G$1" pin="PSEL1" pad="11"/>
<connect gate="G$1" pin="REFIN" pad="2"/>
<connect gate="G$1" pin="REFOUT" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="SDATA" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSCILLATOR" prefix="U">
<gates>
<gate name="G$1" symbol="OSCILLATOR"/>
</gates>
<devices>
<device name="SMD" package="CRYSTAL-SMD-7X5">
<connects>
<connect gate="G$1" pin="EN" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="OUT" pad="P$3"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD6" package="CRYSTAL-SMD-7.5X5.2-6PIN">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5X3" package="CRYSTAL-SMD-5X3">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5X3-PIN1-INDICATED" package="CRYSTAL-OSC-SMD-5X3">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PSP_TOUCH_CONNECTOR">
<description>4-Pin Connector for PSP Touch Screen</description>
<gates>
<gate name="G$1" symbol="PSP_TOUCH_CONNECTOR"/>
</gates>
<devices>
<device name="" package="PSP_TOUCH_CONNECTOR">
<connects>
<connect gate="G$1" pin="X1" pad="X1"/>
<connect gate="G$1" pin="X2" pad="X2"/>
<connect gate="G$1" pin="Y1" pad="Y1"/>
<connect gate="G$1" pin="Y2" pad="Y2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS_TOUCH_CONNECTOR" prefix="JP">
<description>4-pin DS touch screen connector</description>
<gates>
<gate name="G$1" symbol="DS_TOUCH_CONNECTOR"/>
</gates>
<devices>
<device name="" package="DS_TOUCH_CONNECTOR">
<connects>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="3"/>
<connect gate="G$1" pin="Y1" pad="4"/>
<connect gate="G$1" pin="Y2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INVERTER">
<description>Single inverter, SOT23-5</description>
<gates>
<gate name="G$1" symbol="INVERTER"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="&quot;&quot;" package="SC70">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L298_BRIDGE_DRIVER">
<gates>
<gate name="G$1" symbol="L298_BRIDGE_DRIVER"/>
</gates>
<devices>
<device name="" package="POWERSO20">
<connects>
<connect gate="G$1" pin="ENA" pad="8"/>
<connect gate="G$1" pin="ENB" pad="14"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="13"/>
<connect gate="G$1" pin="IN4" pad="15"/>
<connect gate="G$1" pin="NC@18" pad="18"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="OUT3" pad="16"/>
<connect gate="G$1" pin="OUT4" pad="17"/>
<connect gate="G$1" pin="SENSE_A" pad="2"/>
<connect gate="G$1" pin="SENSE_B" pad="19"/>
<connect gate="G$1" pin="VS" pad="6"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GE864">
<gates>
<gate name="G$1" symbol="GE864"/>
</gates>
<devices>
<device name="" package="GE864">
<connects>
<connect gate="G$1" pin="ACD_IN1" pad="J11"/>
<connect gate="G$1" pin="ADC_IN2" pad="H11"/>
<connect gate="G$1" pin="ADC_IN3" pad="G11"/>
<connect gate="G$1" pin="ANTENNA" pad="L4"/>
<connect gate="G$1" pin="AXE" pad="F9"/>
<connect gate="G$1" pin="C103/TXD" pad="E7"/>
<connect gate="G$1" pin="C104/RXD" pad="H8"/>
<connect gate="G$1" pin="C105/RTS" pad="F7"/>
<connect gate="G$1" pin="C106/CTS" pad="F6"/>
<connect gate="G$1" pin="C107/DSR" pad="E11"/>
<connect gate="G$1" pin="C108/DTR" pad="B7"/>
<connect gate="G$1" pin="C109/DCD" pad="D9"/>
<connect gate="G$1" pin="C125/RING" pad="B6"/>
<connect gate="G$1" pin="CHARGE@G1" pad="G1"/>
<connect gate="G$1" pin="CHARGE@G2" pad="G2"/>
<connect gate="G$1" pin="DAC_OUT" pad="C7"/>
<connect gate="G$1" pin="DV12_CLK" pad="D7"/>
<connect gate="G$1" pin="EAR_HF+" pad="H10"/>
<connect gate="G$1" pin="EAR_HF-" pad="J10"/>
<connect gate="G$1" pin="EAR_MT+" pad="G10"/>
<connect gate="G$1" pin="EAR_MT-" pad="H9"/>
<connect gate="G$1" pin="GND@A1" pad="A1"/>
<connect gate="G$1" pin="GND@A11" pad="A11"/>
<connect gate="G$1" pin="GND@D6" pad="D6"/>
<connect gate="G$1" pin="GND@F1" pad="F1"/>
<connect gate="G$1" pin="GND@F11" pad="F11"/>
<connect gate="G$1" pin="GND@H1" pad="H1"/>
<connect gate="G$1" pin="GND@H2" pad="H2"/>
<connect gate="G$1" pin="GND@J3" pad="J3"/>
<connect gate="G$1" pin="GND@K3" pad="K3"/>
<connect gate="G$1" pin="GND@K4" pad="K4"/>
<connect gate="G$1" pin="GND@K5" pad="K5"/>
<connect gate="G$1" pin="GND@K6" pad="K6"/>
<connect gate="G$1" pin="GND@L1" pad="L1"/>
<connect gate="G$1" pin="GND@L11" pad="L11"/>
<connect gate="G$1" pin="GND@L2" pad="L2"/>
<connect gate="G$1" pin="GND@L3" pad="L3"/>
<connect gate="G$1" pin="GND@L6" pad="L6"/>
<connect gate="G$1" pin="MIC_HF+" pad="G8"/>
<connect gate="G$1" pin="MIC_HF-" pad="J9"/>
<connect gate="G$1" pin="MIC_MT+" pad="J8"/>
<connect gate="G$1" pin="MIC_MT-" pad="G9"/>
<connect gate="G$1" pin="ON_OFF" pad="J5"/>
<connect gate="G$1" pin="PWRMON" pad="L8"/>
<connect gate="G$1" pin="RESET" pad="A2"/>
<connect gate="G$1" pin="RX_TRACE" pad="F10"/>
<connect gate="G$1" pin="SIMCLK" pad="C10"/>
<connect gate="G$1" pin="SIMIN" pad="C11"/>
<connect gate="G$1" pin="SIMIO" pad="D10"/>
<connect gate="G$1" pin="SIMRST" pad="E9"/>
<connect gate="G$1" pin="SIMVCC" pad="D4"/>
<connect gate="G$1" pin="STAT_LED" pad="D8"/>
<connect gate="G$1" pin="TGPIO_01" pad="C1"/>
<connect gate="G$1" pin="TGPIO_02/JDR" pad="E6"/>
<connect gate="G$1" pin="TGPIO_03" pad="C2"/>
<connect gate="G$1" pin="TGPIO_04" pad="B3"/>
<connect gate="G$1" pin="TGPIO_05/RFTXMON" pad="K8"/>
<connect gate="G$1" pin="TGPIO_06/ALARM" pad="B5"/>
<connect gate="G$1" pin="TGPIO_07/BUZZER" pad="L9"/>
<connect gate="G$1" pin="TGPIO_08" pad="K11"/>
<connect gate="G$1" pin="TGPIO_09" pad="C9"/>
<connect gate="G$1" pin="TGPIO_10" pad="H3"/>
<connect gate="G$1" pin="TGPIO_11" pad="D1"/>
<connect gate="G$1" pin="TGPIO_12" pad="G4"/>
<connect gate="G$1" pin="TGPIO_13" pad="K10"/>
<connect gate="G$1" pin="TGPIO_14" pad="B4"/>
<connect gate="G$1" pin="TGPIO_15" pad="F5"/>
<connect gate="G$1" pin="TGPIO_16" pad="H6"/>
<connect gate="G$1" pin="TGPIO_17" pad="H5"/>
<connect gate="G$1" pin="TGPIO_18" pad="K7"/>
<connect gate="G$1" pin="TGPIO_19" pad="B1"/>
<connect gate="G$1" pin="TGPIO_20" pad="C3"/>
<connect gate="G$1" pin="TGPIO_21" pad="L10"/>
<connect gate="G$1" pin="TGPIO_22" pad="E8"/>
<connect gate="G$1" pin="TX_TRACE" pad="D11"/>
<connect gate="G$1" pin="VAUX1" pad="D5"/>
<connect gate="G$1" pin="VBATT@J1" pad="J1"/>
<connect gate="G$1" pin="VBATT@J2" pad="J2"/>
<connect gate="G$1" pin="VBATT@K1" pad="K1"/>
<connect gate="G$1" pin="VBATT@K2" pad="K2"/>
<connect gate="G$1" pin="VRTC" pad="E2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-ZENER">
<description>Zener Diode
Production Part - 8199
3.4V Zener Voltage</description>
<gates>
<gate name="G$1" symbol="DIODE-ZENER"/>
</gates>
<devices>
<device name="PTH" package="DIODE-ZENER">
<connects>
<connect gate="G$1" pin="A" pad="P$2"/>
<connect gate="G$1" pin="C" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMB" package="SMB-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BZT52" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSFORMER">
<gates>
<gate name="G$1" symbol="TRANSFORMER"/>
</gates>
<devices>
<device name="PTH" package="TRANSFORMER">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TRANSFORMER_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GEIGER_TUBE">
<description>LND712 Geiger Tube</description>
<gates>
<gate name="G$1" symbol="GEIGER_TUBE"/>
</gates>
<devices>
<device name="LND712" package="GEIGER_TUBE">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45">
<description>Atmel ATTiny45</description>
<gates>
<gate name="G$1" symbol="ATTINY13"/>
</gates>
<devices>
<device name="" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP8" package="DIP08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRRECEIVER">
<description>&lt;b&gt;Description:&lt;/b&gt; IR receiver with built in demodulation and filtering. SparkFun SKU: SEN-08545</description>
<gates>
<gate name="G$1" symbol="TSOP8523"/>
</gates>
<devices>
<device name="SMD" package="TSOP8523">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="4"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL193">
<description>250g accelerometer analog out</description>
<gates>
<gate name="G$1" symbol="ADXL193"/>
</gates>
<devices>
<device name="" package="ADXL193">
<connects>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="OUT" pad="P$6"/>
<connect gate="G$1" pin="ST" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$7"/>
<connect gate="G$1" pin="VDD2" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GE865">
<gates>
<gate name="G$1" symbol="GE865"/>
</gates>
<devices>
<device name="" package="GE865">
<connects>
<connect gate="G$1" pin="ACD_IN1" pad="F5"/>
<connect gate="G$1" pin="ADC_IN2" pad="F6"/>
<connect gate="G$1" pin="ANTENNA" pad="H5"/>
<connect gate="G$1" pin="C103/TXD" pad="A3"/>
<connect gate="G$1" pin="C104/RXD" pad="A4"/>
<connect gate="G$1" pin="C105/RTS" pad="A1"/>
<connect gate="G$1" pin="C106/CTS" pad="A2"/>
<connect gate="G$1" pin="C107/DSR" pad="B2"/>
<connect gate="G$1" pin="C108/DTR" pad="B3"/>
<connect gate="G$1" pin="C109/DCD" pad="B5"/>
<connect gate="G$1" pin="C125/RING" pad="B4"/>
<connect gate="G$1" pin="DAC_OUT" pad="G7"/>
<connect gate="G$1" pin="EAR+" pad="D8"/>
<connect gate="G$1" pin="EAR-" pad="E8"/>
<connect gate="G$1" pin="GND@C2" pad="C2"/>
<connect gate="G$1" pin="GND@C7" pad="C7"/>
<connect gate="G$1" pin="GND@E5" pad="E5"/>
<connect gate="G$1" pin="GND@E7" pad="E7"/>
<connect gate="G$1" pin="GND@G1" pad="G1"/>
<connect gate="G$1" pin="GND@G3" pad="G3"/>
<connect gate="G$1" pin="GND@G4" pad="G4"/>
<connect gate="G$1" pin="GND@G5" pad="G5"/>
<connect gate="G$1" pin="GND@H3" pad="H3"/>
<connect gate="G$1" pin="GND@H6" pad="H6"/>
<connect gate="G$1" pin="GPIO_01" pad="D3"/>
<connect gate="G$1" pin="GPIO_02/JDR" pad="D2"/>
<connect gate="G$1" pin="GPIO_03" pad="E4"/>
<connect gate="G$1" pin="GPIO_04/TX_DISAB" pad="H7"/>
<connect gate="G$1" pin="GPIO_05/RFTXMON" pad="G2"/>
<connect gate="G$1" pin="GPIO_06/ALARM" pad="H8"/>
<connect gate="G$1" pin="GPIO_07/BUZZER" pad="G6"/>
<connect gate="G$1" pin="GPIO_08" pad="D4"/>
<connect gate="G$1" pin="GPIO_09" pad="F4"/>
<connect gate="G$1" pin="GPIO_10" pad="E3"/>
<connect gate="G$1" pin="MIC+" pad="B8"/>
<connect gate="G$1" pin="MIC-" pad="C8"/>
<connect gate="G$1" pin="ON_OFF" pad="B1"/>
<connect gate="G$1" pin="PWRMON" pad="E2"/>
<connect gate="G$1" pin="RESET" pad="C1"/>
<connect gate="G$1" pin="RXD_AUX" pad="E1"/>
<connect gate="G$1" pin="SIMCLK" pad="A5"/>
<connect gate="G$1" pin="SIMIN" pad="B7"/>
<connect gate="G$1" pin="SIMIO" pad="A6"/>
<connect gate="G$1" pin="SIMRST" pad="A8"/>
<connect gate="G$1" pin="SIMVCC" pad="A7"/>
<connect gate="G$1" pin="STAT_LED" pad="G8"/>
<connect gate="G$1" pin="TXD_AUX" pad="D1"/>
<connect gate="G$1" pin="VBATT@F1" pad="F1"/>
<connect gate="G$1" pin="VBATT@F2" pad="F2"/>
<connect gate="G$1" pin="VBATT@F3" pad="F3"/>
<connect gate="G$1" pin="VRTC" pad="H2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M13" prefix="JP">
<gates>
<gate name="G$1" symbol="M13"/>
</gates>
<devices>
<device name="" package="1X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X13-LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATARI_CONNECTOR">
<gates>
<gate name="G$1" symbol="ATARI_CONNECTOR"/>
</gates>
<devices>
<device name="" package="ATARI_CONNECTOR">
<connects>
<connect gate="G$1" pin="BUTTON" pad="P$1"/>
<connect gate="G$1" pin="DOWN" pad="P$6"/>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="LEFT" pad="P$7"/>
<connect gate="G$1" pin="NC1" pad="P$9"/>
<connect gate="G$1" pin="NC2" pad="P$2"/>
<connect gate="G$1" pin="NC3" pad="P$4"/>
<connect gate="G$1" pin="RIGHT" pad="P$8"/>
<connect gate="G$1" pin="UP" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC138AD">
<gates>
<gate name="G$1" symbol="74LVC138AD"/>
</gates>
<devices>
<device name="" package="SO016">
<connects>
<connect gate="G$1" pin="/E1" pad="4"/>
<connect gate="G$1" pin="/E2" pad="5"/>
<connect gate="G$1" pin="/Y0" pad="15"/>
<connect gate="G$1" pin="/Y1" pad="14"/>
<connect gate="G$1" pin="/Y2" pad="13"/>
<connect gate="G$1" pin="/Y3" pad="12"/>
<connect gate="G$1" pin="/Y4" pad="11"/>
<connect gate="G$1" pin="/Y5" pad="10"/>
<connect gate="G$1" pin="/Y6" pad="9"/>
<connect gate="G$1" pin="/Y7" pad="7"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="E3" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GE865_2">
<gates>
<gate name="G$1" symbol="GE865_2"/>
</gates>
<devices>
<device name="" package="GE865">
<connects>
<connect gate="G$1" pin="ACD_IN1" pad="F5"/>
<connect gate="G$1" pin="ADC_IN2" pad="F6"/>
<connect gate="G$1" pin="ANTENNA" pad="H5"/>
<connect gate="G$1" pin="C103/TXD" pad="A3"/>
<connect gate="G$1" pin="C104/RXD" pad="A4"/>
<connect gate="G$1" pin="C105/RTS" pad="A1"/>
<connect gate="G$1" pin="C106/CTS" pad="A2"/>
<connect gate="G$1" pin="C107/DSR" pad="B2"/>
<connect gate="G$1" pin="C108/DTR" pad="B3"/>
<connect gate="G$1" pin="C109/DCD" pad="B5"/>
<connect gate="G$1" pin="C125/RING" pad="B4"/>
<connect gate="G$1" pin="DAC_OUT" pad="G7"/>
<connect gate="G$1" pin="EAR+" pad="D8"/>
<connect gate="G$1" pin="EAR-" pad="E8"/>
<connect gate="G$1" pin="GND@C2" pad="C2"/>
<connect gate="G$1" pin="GND@C7" pad="C7"/>
<connect gate="G$1" pin="GND@E5" pad="E5"/>
<connect gate="G$1" pin="GND@E7" pad="E7"/>
<connect gate="G$1" pin="GND@G1" pad="G1"/>
<connect gate="G$1" pin="GND@G3" pad="G3"/>
<connect gate="G$1" pin="GND@G4" pad="G4"/>
<connect gate="G$1" pin="GND@G5" pad="G5"/>
<connect gate="G$1" pin="GND@H3" pad="H3"/>
<connect gate="G$1" pin="GND@H6" pad="H6"/>
<connect gate="G$1" pin="GPIO_01" pad="D3"/>
<connect gate="G$1" pin="GPIO_02/JDR" pad="D2"/>
<connect gate="G$1" pin="GPIO_03" pad="E4"/>
<connect gate="G$1" pin="GPIO_04/TX_DISAB" pad="H7"/>
<connect gate="G$1" pin="GPIO_05/RFTXMON" pad="G2"/>
<connect gate="G$1" pin="GPIO_06/ALARM" pad="H8"/>
<connect gate="G$1" pin="GPIO_07/BUZZER" pad="G6"/>
<connect gate="G$1" pin="GPIO_08" pad="D4"/>
<connect gate="G$1" pin="GPIO_09" pad="F4"/>
<connect gate="G$1" pin="GPIO_10" pad="E3"/>
<connect gate="G$1" pin="MIC+" pad="B8"/>
<connect gate="G$1" pin="MIC-" pad="C8"/>
<connect gate="G$1" pin="ON_OFF" pad="B1"/>
<connect gate="G$1" pin="PWRMON" pad="E2"/>
<connect gate="G$1" pin="RESET" pad="C1"/>
<connect gate="G$1" pin="RXD_AUX" pad="E1"/>
<connect gate="G$1" pin="SERVICE" pad="H1"/>
<connect gate="G$1" pin="SIMCLK" pad="A5"/>
<connect gate="G$1" pin="SIMIN" pad="B7"/>
<connect gate="G$1" pin="SIMIO" pad="A6"/>
<connect gate="G$1" pin="SIMRST" pad="A8"/>
<connect gate="G$1" pin="SIMVCC" pad="A7"/>
<connect gate="G$1" pin="STAT_LED" pad="G8"/>
<connect gate="G$1" pin="TXD_AUX" pad="D1"/>
<connect gate="G$1" pin="VBATT@F1" pad="F1"/>
<connect gate="G$1" pin="VBATT@F2" pad="F2"/>
<connect gate="G$1" pin="VBATT@F3" pad="F3"/>
<connect gate="G$1" pin="VRTC" pad="H2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD_MMC_CARD">
<gates>
<gate name="G$1" symbol="SD-MMC-CARD"/>
</gates>
<devices>
<device name="SD_PCB" package="SD-MMC-CARD">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-DISPLAY-1&quot;-RED">
<description>7-Segment Display 1" Red (COM-08546)</description>
<gates>
<gate name="G$1" symbol="7-SEGMENT-1&quot;"/>
</gates>
<devices>
<device name="" package="7-SEGMENT-1&quot;PTH">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3480IM4">
<gates>
<gate name="G$1" symbol="LM3480IM4"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZCT1009FTA">
<gates>
<gate name="G$1" symbol="ZCT1009FTA"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="IOUT" pad="3"/>
<connect gate="G$1" pin="LOAD" pad="1"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_SHIELD" prefix="U">
<gates>
<gate name="G$1" symbol="ARDUINO_SHIELD"/>
</gates>
<devices>
<device name="LABEL" package="DUEMILANOVE_SHIELD">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="DUEMILANOVE_VIAS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLES" package="DUEMILANOVE_SHIELD_NOHOLES">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="DUEMILANOVE_SHIELD_LONGPADS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOLABELS" package="DUEMILANOVE_SHIELD_NOLABELS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLESORLABELS" package="DUEMILANOVE_SHIELD_NOHOLES_NOLABELS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_SPI_PROG2">
<description>&lt;b&gt;AVR ICSP Header&lt;/b&gt; 
This is the standard AVR In Circuit Serial Programming header. Minimal, but includes pin one indicator. Works with standard Olimex programmers. Also look for the 6-pin reduced version. Spark Fun Electronics SKU: PRT-00778</description>
<gates>
<gate name="A" symbol="AVR_SPI_PROGRAMMER-1"/>
</gates>
<devices>
<device name="PTH" package="AVR_ICSP">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="2X5-SHROUDED">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="2X5-SHROUDED_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="2X5-SHROUDED_SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U.FL">
<gates>
<gate name="G$1" symbol="U.FL"/>
</gates>
<devices>
<device name="" package="U.FL">
<connects>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="SIGNAL" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIMHOLDER3">
<gates>
<gate name="G$1" symbol="SIMHOLDER3"/>
</gates>
<devices>
<device name="" package="SIMHOLDER3">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="I/O" pad="4"/>
<connect gate="G$1" pin="RST" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VPP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M27">
<gates>
<gate name="G$1" symbol="M27"/>
</gates>
<devices>
<device name="" package="1X27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M17">
<gates>
<gate name="G$1" symbol="M17"/>
</gates>
<devices>
<device name="" package="1X17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M19">
<gates>
<gate name="G$1" symbol="M19"/>
</gates>
<devices>
<device name="" package="1X19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7302">
<description>AD7302</description>
<gates>
<gate name="G$1" symbol="AD7302"/>
</gates>
<devices>
<device name="SMD" package="TSSOP20">
<connects>
<connect gate="G$1" pin="AB" pad="11"/>
<connect gate="G$1" pin="AGND" pad="17"/>
<connect gate="G$1" pin="CLR" pad="14"/>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="DB0" pad="8"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="5"/>
<connect gate="G$1" pin="DB4" pad="4"/>
<connect gate="G$1" pin="DB5" pad="3"/>
<connect gate="G$1" pin="DB6" pad="2"/>
<connect gate="G$1" pin="DB7" pad="1"/>
<connect gate="G$1" pin="DGND" pad="20"/>
<connect gate="G$1" pin="LDAC" pad="13"/>
<connect gate="G$1" pin="PD" pad="12"/>
<connect gate="G$1" pin="REFIN" pad="16"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VOUTA" pad="19"/>
<connect gate="G$1" pin="VOUTB" pad="18"/>
<connect gate="G$1" pin="WR" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC5843" prefix="U">
<gates>
<gate name="G$1" symbol="HMC5843"/>
</gates>
<devices>
<device name="SMD" package="LPCC20">
<connects>
<connect gate="G$1" pin="AGND" pad="17"/>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="C1" pad="13"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DRDY" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="OFFN" pad="7"/>
<connect gate="G$1" pin="OFFP" pad="6"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SCLP" pad="3"/>
<connect gate="G$1" pin="SDA" pad="20"/>
<connect gate="G$1" pin="SDAP" pad="2"/>
<connect gate="G$1" pin="SETC" pad="14"/>
<connect gate="G$1" pin="SETN" pad="10"/>
<connect gate="G$1" pin="SETP" pad="9"/>
<connect gate="G$1" pin="SVDD" pad="11"/>
<connect gate="G$1" pin="VREN" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BNC">
<description>BNC Connector, Mouser Part# 5227161</description>
<gates>
<gate name="G$1" symbol="BNC"/>
</gates>
<devices>
<device name="PTH" package="BNC">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="OUT" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TURRET-1520">
<description>Turret FP for Keystone Electronics Part#1520</description>
<gates>
<gate name="G$1" symbol="TURRET"/>
</gates>
<devices>
<device name="PTH" package="1X01_TURRET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL335" prefix="U">
<gates>
<gate name="G$1" symbol="ADXL335"/>
</gates>
<devices>
<device name="" package="LFCSP-16">
<connects>
<connect gate="G$1" pin="COM@3" pad="3"/>
<connect gate="G$1" pin="COM@5" pad="5"/>
<connect gate="G$1" pin="COM@6" pad="6"/>
<connect gate="G$1" pin="COM@7" pad="7"/>
<connect gate="G$1" pin="ST" pad="2"/>
<connect gate="G$1" pin="VS@14" pad="14"/>
<connect gate="G$1" pin="VS@15" pad="15"/>
<connect gate="G$1" pin="XOUT" pad="12"/>
<connect gate="G$1" pin="YOUT" pad="10"/>
<connect gate="G$1" pin="ZOUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-FIRST">
<gates>
<gate name="G$1" symbol="FIRST"/>
</gates>
<devices>
<device name="" package="FRIST_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC_CONVERTER">
<gates>
<gate name="G$1" symbol="DC-DC_CONVERTER"/>
</gates>
<devices>
<device name="" package="DC-DC_CONVERTER">
<connects>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="ON/OFF" pad="1"/>
<connect gate="G$1" pin="PGOOD" pad="10"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="SEQ" pad="9"/>
<connect gate="G$1" pin="TRIM" pad="6"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GP1A57HR">
<gates>
<gate name="G$1" symbol="GP1A57HR"/>
</gates>
<devices>
<device name="" package="GP1A57HR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN-131G">
<description>Roving Netowrks WiFLy GSX Module</description>
<gates>
<gate name="G$1" symbol="RN-131G"/>
</gates>
<devices>
<device name="" package="RN-131G">
<connects>
<connect gate="G$1" pin="3.3V-RIN" pad="P$18"/>
<connect gate="G$1" pin="3.3V-ROUT" pad="P$17"/>
<connect gate="G$1" pin="CLK" pad="P$15"/>
<connect gate="G$1" pin="DMA-RX" pad="P$23"/>
<connect gate="G$1" pin="DMA-TX" pad="P$22"/>
<connect gate="G$1" pin="EPC-A" pad="P$6"/>
<connect gate="G$1" pin="EPC-B" pad="P$7"/>
<connect gate="G$1" pin="F_AWAKE" pad="P$9"/>
<connect gate="G$1" pin="GND@19" pad="P$19"/>
<connect gate="G$1" pin="GND@36" pad="P$36"/>
<connect gate="G$1" pin="GND@37" pad="P$37"/>
<connect gate="G$1" pin="GND@38" pad="P$38"/>
<connect gate="G$1" pin="GND@39" pad="P$39"/>
<connect gate="G$1" pin="GND@40" pad="P$40"/>
<connect gate="G$1" pin="GND@41" pad="P$41"/>
<connect gate="G$1" pin="GND@42" pad="P$42"/>
<connect gate="G$1" pin="GND@43" pad="P$43"/>
<connect gate="G$1" pin="GND@44" pad="P$44"/>
<connect gate="G$1" pin="GPIO-12" pad="P$11"/>
<connect gate="G$1" pin="GPIO-13" pad="P$10"/>
<connect gate="G$1" pin="GPIO-4" pad="P$29"/>
<connect gate="G$1" pin="GPIO-5" pad="P$28"/>
<connect gate="G$1" pin="GPIO-6" pad="P$27"/>
<connect gate="G$1" pin="GPIO-7" pad="P$26"/>
<connect gate="G$1" pin="GPIO-8" pad="P$25"/>
<connect gate="G$1" pin="GPIO-9" pad="P$24"/>
<connect gate="G$1" pin="MISO" pad="P$16"/>
<connect gate="G$1" pin="MOSI" pad="P$14"/>
<connect gate="G$1" pin="RESET" pad="P$5"/>
<connect gate="G$1" pin="RX" pad="P$12"/>
<connect gate="G$1" pin="SEN0" pad="P$34"/>
<connect gate="G$1" pin="SEN1" pad="P$30"/>
<connect gate="G$1" pin="SEN2" pad="P$31"/>
<connect gate="G$1" pin="SEN3" pad="P$32"/>
<connect gate="G$1" pin="SEN4" pad="P$2"/>
<connect gate="G$1" pin="SEN5" pad="P$3"/>
<connect gate="G$1" pin="SEN6" pad="P$1"/>
<connect gate="G$1" pin="SEN7" pad="P$4"/>
<connect gate="G$1" pin="SENSE-PWR" pad="P$33"/>
<connect gate="G$1" pin="S_CAP" pad="P$8"/>
<connect gate="G$1" pin="TX" pad="P$13"/>
<connect gate="G$1" pin="VDD-BATT" pad="P$20"/>
<connect gate="G$1" pin="VDD-IN" pad="P$21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOIC_20">
<gates>
<gate name="G$1" symbol="SOIC_20W"/>
</gates>
<devices>
<device name="" package="SO20W">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$16" pad="P$16"/>
<connect gate="G$1" pin="P$17" pad="P$17"/>
<connect gate="G$1" pin="P$18" pad="P$18"/>
<connect gate="G$1" pin="P$19" pad="P$19"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$20" pad="P$20"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CMA3000-A01">
<gates>
<gate name="G$1" symbol="CMA3000-A01"/>
</gates>
<devices>
<device name="" package="CMA3000">
<connects>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="PD" pad="P$5"/>
<connect gate="G$1" pin="RANGE" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
<connect gate="G$1" pin="VDD1" pad="P$3"/>
<connect gate="G$1" pin="X" pad="P$7"/>
<connect gate="G$1" pin="Y" pad="P$8"/>
<connect gate="G$1" pin="Z" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CMA3000-D01">
<gates>
<gate name="G$1" symbol="CMA3000-D01"/>
</gates>
<devices>
<device name="" package="CMA3000">
<connects>
<connect gate="G$1" pin="CS" pad="P$7"/>
<connect gate="G$1" pin="DVIO" pad="P$3"/>
<connect gate="G$1" pin="INT" pad="P$8"/>
<connect gate="G$1" pin="MISO" pad="P$4"/>
<connect gate="G$1" pin="MOSI" pad="P$6"/>
<connect gate="G$1" pin="SCK" pad="P$5"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
<connect gate="G$1" pin="VSS" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISL29102">
<gates>
<gate name="G$1" symbol="ISL29102"/>
</gates>
<devices>
<device name="" package="ODFN6">
<connects>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="NC" pad="P$3"/>
<connect gate="G$1" pin="NC1" pad="P$5"/>
<connect gate="G$1" pin="REXT" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
<connect gate="G$1" pin="VOUT" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1803" prefix="U">
<description>24-bit ADC</description>
<gates>
<gate name="G$1" symbol="PCM1803A"/>
</gates>
<devices>
<device name="SMD" package="SSOP20">
<connects>
<connect gate="G$1" pin="BCK" pad="11"/>
<connect gate="G$1" pin="BPAS" pad="8"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="FMT0" pad="17"/>
<connect gate="G$1" pin="FMT1" pad="18"/>
<connect gate="G$1" pin="GNDA" pad="6"/>
<connect gate="G$1" pin="GNDD" pad="13"/>
<connect gate="G$1" pin="LRCK" pad="10"/>
<connect gate="G$1" pin="MD0" pad="19"/>
<connect gate="G$1" pin="MD1" pad="20"/>
<connect gate="G$1" pin="OSR" pad="16"/>
<connect gate="G$1" pin="PDWN" pad="7"/>
<connect gate="G$1" pin="SCK" pad="15"/>
<connect gate="G$1" pin="TEST" pad="9"/>
<connect gate="G$1" pin="VCCA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VINL" pad="1"/>
<connect gate="G$1" pin="VINR" pad="2"/>
<connect gate="G$1" pin="VREF1" pad="3"/>
<connect gate="G$1" pin="VREF2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRACKBALL">
<gates>
<gate name="G$1" symbol="TRACKBALL"/>
</gates>
<devices>
<device name="MECH" package="TRACKBALL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HALL-EFFECT">
<gates>
<gate name="G$1" symbol="HALL-EFFECT"/>
</gates>
<devices>
<device name="SMD" package="SC70">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIFLY_GSX">
<gates>
<gate name="G$1" symbol="WIFLY_GSX"/>
</gates>
<devices>
<device name="" package="WIFLY_GSX">
<connects>
<connect gate="G$1" pin="3V3_IN" pad="18"/>
<connect gate="G$1" pin="3V3_OUT" pad="17"/>
<connect gate="G$1" pin="DMA_RX" pad="23"/>
<connect gate="G$1" pin="DMA_TX" pad="22"/>
<connect gate="G$1" pin="EPCA" pad="6"/>
<connect gate="G$1" pin="EPCB" pad="7"/>
<connect gate="G$1" pin="FORCE_WAKE" pad="9"/>
<connect gate="G$1" pin="G1" pad="19"/>
<connect gate="G$1" pin="G10" pad="44"/>
<connect gate="G$1" pin="G2" pad="36"/>
<connect gate="G$1" pin="G3" pad="37"/>
<connect gate="G$1" pin="G4" pad="38"/>
<connect gate="G$1" pin="G5" pad="39"/>
<connect gate="G$1" pin="G6" pad="40"/>
<connect gate="G$1" pin="G7" pad="41"/>
<connect gate="G$1" pin="G8" pad="42"/>
<connect gate="G$1" pin="G9" pad="43"/>
<connect gate="G$1" pin="GPIO4" pad="29"/>
<connect gate="G$1" pin="GPIO5" pad="28"/>
<connect gate="G$1" pin="GPIO6" pad="27"/>
<connect gate="G$1" pin="GPIO7" pad="26"/>
<connect gate="G$1" pin="GPIO8" pad="25"/>
<connect gate="G$1" pin="GPIO9" pad="24"/>
<connect gate="G$1" pin="GPIO_12" pad="11"/>
<connect gate="G$1" pin="GPIO_13" pad="10"/>
<connect gate="G$1" pin="NC" pad="35"/>
<connect gate="G$1" pin="RESET_L" pad="5"/>
<connect gate="G$1" pin="SENS0" pad="34"/>
<connect gate="G$1" pin="SENS1" pad="30"/>
<connect gate="G$1" pin="SENS2" pad="31"/>
<connect gate="G$1" pin="SENS3" pad="32"/>
<connect gate="G$1" pin="SENS4" pad="2"/>
<connect gate="G$1" pin="SENS5" pad="3"/>
<connect gate="G$1" pin="SENS6" pad="1"/>
<connect gate="G$1" pin="SENS7" pad="4"/>
<connect gate="G$1" pin="SENSPWR" pad="33"/>
<connect gate="G$1" pin="SPI_CLK" pad="15"/>
<connect gate="G$1" pin="SPI_MISO" pad="16"/>
<connect gate="G$1" pin="SPI_MOSI" pad="14"/>
<connect gate="G$1" pin="SUPCAP" pad="8"/>
<connect gate="G$1" pin="URX" pad="12"/>
<connect gate="G$1" pin="UTX" pad="13"/>
<connect gate="G$1" pin="VD_3V_IN" pad="21"/>
<connect gate="G$1" pin="VD_BAT" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SM5100B">
<gates>
<gate name="G$1" symbol="SM5100B"/>
</gates>
<devices>
<device name="" package="SM5100B">
<connects>
<connect gate="G$1" pin="ADIN1" pad="6"/>
<connect gate="G$1" pin="ADIN2" pad="8"/>
<connect gate="G$1" pin="AUX_MICN" pad="50"/>
<connect gate="G$1" pin="AUX_MICP" pad="42"/>
<connect gate="G$1" pin="AUX_SPKN" pad="58"/>
<connect gate="G$1" pin="AUX_SPKP" pad="44"/>
<connect gate="G$1" pin="EAR_MICN" pad="12"/>
<connect gate="G$1" pin="EAR_MICP" pad="14"/>
<connect gate="G$1" pin="EAR_SPKN" pad="16"/>
<connect gate="G$1" pin="EAR_SPKP" pad="18"/>
<connect gate="G$1" pin="GND@0" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GPIO_1" pad="39"/>
<connect gate="G$1" pin="GPIO_10" pad="37"/>
<connect gate="G$1" pin="GPIO_16" pad="52"/>
<connect gate="G$1" pin="GPIO_17" pad="22"/>
<connect gate="G$1" pin="GPIO_18" pad="45"/>
<connect gate="G$1" pin="GPIO_19" pad="10"/>
<connect gate="G$1" pin="GPIO_20" pad="56"/>
<connect gate="G$1" pin="GPIO_26" pad="49"/>
<connect gate="G$1" pin="GPIO_3" pad="55"/>
<connect gate="G$1" pin="GPIO_4" pad="35"/>
<connect gate="G$1" pin="GPIO_46" pad="57"/>
<connect gate="G$1" pin="GPIO_6" pad="38"/>
<connect gate="G$1" pin="GPIO_8" pad="54"/>
<connect gate="G$1" pin="GPIO_9" pad="41"/>
<connect gate="G$1" pin="GPO42/NBOOT" pad="33"/>
<connect gate="G$1" pin="GPO_11" pad="53"/>
<connect gate="G$1" pin="KEY_DRV0" pad="24"/>
<connect gate="G$1" pin="KEY_DRV1" pad="28"/>
<connect gate="G$1" pin="KEY_DRV2" pad="26"/>
<connect gate="G$1" pin="KEY_DRV3" pad="23"/>
<connect gate="G$1" pin="KEY_DRV4" pad="25"/>
<connect gate="G$1" pin="KEY_DRV5" pad="30"/>
<connect gate="G$1" pin="KEY_SEN0" pad="36"/>
<connect gate="G$1" pin="KEY_SEN1" pad="32"/>
<connect gate="G$1" pin="KEY_SEN2" pad="31"/>
<connect gate="G$1" pin="KEY_SEN3" pad="40"/>
<connect gate="G$1" pin="POWER_ON" pad="59"/>
<connect gate="G$1" pin="RESET" pad="34"/>
<connect gate="G$1" pin="RTC_BATT" pad="48"/>
<connect gate="G$1" pin="RXD0" pad="20"/>
<connect gate="G$1" pin="RXD1" pad="43"/>
<connect gate="G$1" pin="SIM_CLK" pad="27"/>
<connect gate="G$1" pin="SIM_DA" pad="29"/>
<connect gate="G$1" pin="SIM_RST" pad="21"/>
<connect gate="G$1" pin="SIM_VCC" pad="51"/>
<connect gate="G$1" pin="TXD0" pad="19"/>
<connect gate="G$1" pin="TXD1" pad="46"/>
<connect gate="G$1" pin="VBAT@0" pad="7"/>
<connect gate="G$1" pin="VBAT@1" pad="1"/>
<connect gate="G$1" pin="VBAT@2" pad="3"/>
<connect gate="G$1" pin="VBAT@3" pad="5"/>
<connect gate="G$1" pin="VCC@0" pad="47"/>
<connect gate="G$1" pin="VCC@1" pad="60"/>
<connect gate="G$1" pin="VCHG@0" pad="2"/>
<connect gate="G$1" pin="VCHG@1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL_FOR_TESTING!!" package="SM5100B-SPECIAL_FOR_TESTING">
<connects>
<connect gate="G$1" pin="ADIN1" pad="6"/>
<connect gate="G$1" pin="ADIN2" pad="8"/>
<connect gate="G$1" pin="AUX_MICN" pad="50"/>
<connect gate="G$1" pin="AUX_MICP" pad="42"/>
<connect gate="G$1" pin="AUX_SPKN" pad="58"/>
<connect gate="G$1" pin="AUX_SPKP" pad="44"/>
<connect gate="G$1" pin="EAR_MICN" pad="12"/>
<connect gate="G$1" pin="EAR_MICP" pad="14"/>
<connect gate="G$1" pin="EAR_SPKN" pad="16"/>
<connect gate="G$1" pin="EAR_SPKP" pad="18"/>
<connect gate="G$1" pin="GND@0" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GPIO_1" pad="39"/>
<connect gate="G$1" pin="GPIO_10" pad="37"/>
<connect gate="G$1" pin="GPIO_16" pad="52"/>
<connect gate="G$1" pin="GPIO_17" pad="22"/>
<connect gate="G$1" pin="GPIO_18" pad="45"/>
<connect gate="G$1" pin="GPIO_19" pad="10"/>
<connect gate="G$1" pin="GPIO_20" pad="56"/>
<connect gate="G$1" pin="GPIO_26" pad="49"/>
<connect gate="G$1" pin="GPIO_3" pad="55"/>
<connect gate="G$1" pin="GPIO_4" pad="35"/>
<connect gate="G$1" pin="GPIO_46" pad="57"/>
<connect gate="G$1" pin="GPIO_6" pad="38"/>
<connect gate="G$1" pin="GPIO_8" pad="54"/>
<connect gate="G$1" pin="GPIO_9" pad="41"/>
<connect gate="G$1" pin="GPO42/NBOOT" pad="33"/>
<connect gate="G$1" pin="GPO_11" pad="53"/>
<connect gate="G$1" pin="KEY_DRV0" pad="24"/>
<connect gate="G$1" pin="KEY_DRV1" pad="28"/>
<connect gate="G$1" pin="KEY_DRV2" pad="26"/>
<connect gate="G$1" pin="KEY_DRV3" pad="23"/>
<connect gate="G$1" pin="KEY_DRV4" pad="25"/>
<connect gate="G$1" pin="KEY_DRV5" pad="30"/>
<connect gate="G$1" pin="KEY_SEN0" pad="36"/>
<connect gate="G$1" pin="KEY_SEN1" pad="32"/>
<connect gate="G$1" pin="KEY_SEN2" pad="31"/>
<connect gate="G$1" pin="KEY_SEN3" pad="40"/>
<connect gate="G$1" pin="POWER_ON" pad="59"/>
<connect gate="G$1" pin="RESET" pad="34"/>
<connect gate="G$1" pin="RTC_BATT" pad="48"/>
<connect gate="G$1" pin="RXD0" pad="20"/>
<connect gate="G$1" pin="RXD1" pad="43"/>
<connect gate="G$1" pin="SIM_CLK" pad="27"/>
<connect gate="G$1" pin="SIM_DA" pad="29"/>
<connect gate="G$1" pin="SIM_RST" pad="21"/>
<connect gate="G$1" pin="SIM_VCC" pad="51"/>
<connect gate="G$1" pin="TXD0" pad="19"/>
<connect gate="G$1" pin="TXD1" pad="46"/>
<connect gate="G$1" pin="VBAT@0" pad="7"/>
<connect gate="G$1" pin="VBAT@1" pad="1"/>
<connect gate="G$1" pin="VBAT@2" pad="3"/>
<connect gate="G$1" pin="VBAT@3" pad="5"/>
<connect gate="G$1" pin="VCC@0" pad="47"/>
<connect gate="G$1" pin="VCC@1" pad="60"/>
<connect gate="G$1" pin="VCHG@0" pad="2"/>
<connect gate="G$1" pin="VCHG@1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSOP16">
<gates>
<gate name="G$1" symbol="SSOP16"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$16" pad="P$16"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IXZ500" prefix="U">
<description>IXZ-500 Dual Axis (X/Z) Gyro</description>
<gates>
<gate name="G$1" symbol="IXZ500"/>
</gates>
<devices>
<device name="SMD" package="QFN-28_6X8">
<connects>
<connect gate="G$1" pin="AZ" pad="24"/>
<connect gate="G$1" pin="CPOUT" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="PTATS" pad="23"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
<connect gate="G$1" pin="X4.5IN" pad="5"/>
<connect gate="G$1" pin="X4.5OUT" pad="7"/>
<connect gate="G$1" pin="XAGC" pad="6"/>
<connect gate="G$1" pin="XOUT" pad="1"/>
<connect gate="G$1" pin="Z4.5IN" pad="16"/>
<connect gate="G$1" pin="Z4.5OUT" pad="14"/>
<connect gate="G$1" pin="ZAGC" pad="15"/>
<connect gate="G$1" pin="ZOUT" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO-SDCARD">
<gates>
<gate name="G$1" symbol="MICRO-SDCARD"/>
</gates>
<devices>
<device name="" package="MICRO-SDCARD">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="CD/DAT3"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CMD" pad="CMD"/>
<connect gate="G$1" pin="DAT0" pad="DAT0"/>
<connect gate="G$1" pin="DAT1" pad="DAT1"/>
<connect gate="G$1" pin="DAT2" pad="DAT2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VDD" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C64215">
<gates>
<gate name="G$1" symbol="CY7C64215"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="D+" pad="14"/>
<connect gate="G$1" pin="D-" pad="15"/>
<connect gate="G$1" pin="P00" pad="24"/>
<connect gate="G$1" pin="P01" pad="5"/>
<connect gate="G$1" pin="P02" pad="25"/>
<connect gate="G$1" pin="P03" pad="4"/>
<connect gate="G$1" pin="P04" pad="26"/>
<connect gate="G$1" pin="P05" pad="3"/>
<connect gate="G$1" pin="P06" pad="27"/>
<connect gate="G$1" pin="P07" pad="2"/>
<connect gate="G$1" pin="P10" pad="17"/>
<connect gate="G$1" pin="P11" pad="12"/>
<connect gate="G$1" pin="P12" pad="18"/>
<connect gate="G$1" pin="P13" pad="11"/>
<connect gate="G$1" pin="P14" pad="19"/>
<connect gate="G$1" pin="P15" pad="10"/>
<connect gate="G$1" pin="P16" pad="20"/>
<connect gate="G$1" pin="P17" pad="9"/>
<connect gate="G$1" pin="P20" pad="21"/>
<connect gate="G$1" pin="P21" pad="8"/>
<connect gate="G$1" pin="P22" pad="22"/>
<connect gate="G$1" pin="P23" pad="7"/>
<connect gate="G$1" pin="P24" pad="23"/>
<connect gate="G$1" pin="P25" pad="6"/>
<connect gate="G$1" pin="VDD@16" pad="16"/>
<connect gate="G$1" pin="VDD@28" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="1"/>
<connect gate="G$1" pin="VSS@13" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEMS-MIC">
<gates>
<gate name="G$1" symbol="MEMS-MIC"/>
</gates>
<devices>
<device name="" package="MEMS-MIC">
<connects>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VIN" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMARTCARD" prefix="JP">
<gates>
<gate name="G$1" symbol="SMARTCARD"/>
</gates>
<devices>
<device name="SMD" package="SMARTCARD">
<connects>
<connect gate="G$1" pin="C4" pad="C4"/>
<connect gate="G$1" pin="C8" pad="C8"/>
<connect gate="G$1" pin="CLK" pad="C3"/>
<connect gate="G$1" pin="GND" pad="C5"/>
<connect gate="G$1" pin="I/O" pad="C7"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="SW1" pad="P1"/>
<connect gate="G$1" pin="SW2" pad="P2"/>
<connect gate="G$1" pin="VCC" pad="C1"/>
<connect gate="G$1" pin="VPP" pad="C6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XS1_L1_64LQFP">
<gates>
<gate name="G$1" symbol="XS1-L1-64LQFP"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64-XS1">
<connects>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="DEBUG" pad="17"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="MODE0" pad="22"/>
<connect gate="G$1" pin="MODE1" pad="23"/>
<connect gate="G$1" pin="MODE2" pad="24"/>
<connect gate="G$1" pin="MODE3" pad="25"/>
<connect gate="G$1" pin="PLL_AGND" pad="19"/>
<connect gate="G$1" pin="PLL_AVDD" pad="20"/>
<connect gate="G$1" pin="RST_N" pad="8"/>
<connect gate="G$1" pin="TCK" pad="29"/>
<connect gate="G$1" pin="TDI" pad="30"/>
<connect gate="G$1" pin="TDO" pad="31"/>
<connect gate="G$1" pin="TMS" pad="27"/>
<connect gate="G$1" pin="TRST_N" pad="26"/>
<connect gate="G$1" pin="VDDIO_18" pad="18"/>
<connect gate="G$1" pin="VDDIO_32" pad="32"/>
<connect gate="G$1" pin="VDDIO_40" pad="40"/>
<connect gate="G$1" pin="VDDIO_53" pad="53"/>
<connect gate="G$1" pin="VDDIO_6" pad="6"/>
<connect gate="G$1" pin="VDDIO_60" pad="60"/>
<connect gate="G$1" pin="VDD_13" pad="13"/>
<connect gate="G$1" pin="VDD_21" pad="21"/>
<connect gate="G$1" pin="VDD_28" pad="28"/>
<connect gate="G$1" pin="VDD_37" pad="37"/>
<connect gate="G$1" pin="VDD_4" pad="4"/>
<connect gate="G$1" pin="VDD_43" pad="43"/>
<connect gate="G$1" pin="VDD_52" pad="52"/>
<connect gate="G$1" pin="VDD_61" pad="61"/>
<connect gate="G$1" pin="X0D0" pad="16"/>
<connect gate="G$1" pin="X0D1" pad="15"/>
<connect gate="G$1" pin="X0D10" pad="1"/>
<connect gate="G$1" pin="X0D11" pad="64"/>
<connect gate="G$1" pin="X0D12" pad="63"/>
<connect gate="G$1" pin="X0D13" pad="62"/>
<connect gate="G$1" pin="X0D14" pad="59"/>
<connect gate="G$1" pin="X0D15" pad="58"/>
<connect gate="G$1" pin="X0D16" pad="57"/>
<connect gate="G$1" pin="X0D17" pad="56"/>
<connect gate="G$1" pin="X0D18" pad="55"/>
<connect gate="G$1" pin="X0D19" pad="54"/>
<connect gate="G$1" pin="X0D2" pad="14"/>
<connect gate="G$1" pin="X0D20" pad="51"/>
<connect gate="G$1" pin="X0D21" pad="50"/>
<connect gate="G$1" pin="X0D22" pad="49"/>
<connect gate="G$1" pin="X0D23" pad="48"/>
<connect gate="G$1" pin="X0D24" pad="47"/>
<connect gate="G$1" pin="X0D25" pad="46"/>
<connect gate="G$1" pin="X0D26" pad="45"/>
<connect gate="G$1" pin="X0D27" pad="44"/>
<connect gate="G$1" pin="X0D3" pad="12"/>
<connect gate="G$1" pin="X0D32" pad="36"/>
<connect gate="G$1" pin="X0D33" pad="35"/>
<connect gate="G$1" pin="X0D34" pad="34"/>
<connect gate="G$1" pin="X0D35" pad="33"/>
<connect gate="G$1" pin="X0D36" pad="42"/>
<connect gate="G$1" pin="X0D37" pad="41"/>
<connect gate="G$1" pin="X0D38" pad="39"/>
<connect gate="G$1" pin="X0D39" pad="38"/>
<connect gate="G$1" pin="X0D4" pad="11"/>
<connect gate="G$1" pin="X0D5" pad="10"/>
<connect gate="G$1" pin="X0D6" pad="7"/>
<connect gate="G$1" pin="X0D7" pad="5"/>
<connect gate="G$1" pin="X0D8" pad="3"/>
<connect gate="G$1" pin="X0D9" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX440F512H">
<gates>
<gate name="G$1" symbol="PIC32MX440F512H"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="D+/RG2" pad="37"/>
<connect gate="G$1" pin="D-/RG3" pad="36"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="RB0/AN0/PGED1/EMUD1/PMA6/VREF+/CVREF+/CN2" pad="16"/>
<connect gate="G$1" pin="RB1/AN1/PGEC1/VREF-/CVREF-/CN3" pad="15"/>
<connect gate="G$1" pin="RB10/AN10/TMS/CVREFOUT/PMA13" pad="23"/>
<connect gate="G$1" pin="RB11/AN11/TDO/PMA12" pad="24"/>
<connect gate="G$1" pin="RB12/AN12/TCK/PMA11" pad="27"/>
<connect gate="G$1" pin="RB13/AN13/TDI/PMA10" pad="28"/>
<connect gate="G$1" pin="RB14/AN14/PMALH/PMA1/~U2RTS/BCLK2" pad="29"/>
<connect gate="G$1" pin="RB15/AN15/PMALL/PMA0/OCFB/CN12" pad="30"/>
<connect gate="G$1" pin="RB2/AN2/C2IN-/CN4" pad="14"/>
<connect gate="G$1" pin="RB3/AN3/C2IN+/CN5" pad="13"/>
<connect gate="G$1" pin="RB4/AN4/C1IN-/CN6" pad="12"/>
<connect gate="G$1" pin="RB5/AN5/VBUSON/C1IN+/CN7" pad="11"/>
<connect gate="G$1" pin="RB6/AN6/PGEC2/OCFA" pad="17"/>
<connect gate="G$1" pin="RB7/AN7/PGED2" pad="18"/>
<connect gate="G$1" pin="RB8/AN8/~U2CTS/C1OUT" pad="21"/>
<connect gate="G$1" pin="RB9/AN9/PMA7/C2OUT" pad="22"/>
<connect gate="G$1" pin="RC12/OSC1/CLKI" pad="39"/>
<connect gate="G$1" pin="RC13/SOSCI/CN1" pad="47"/>
<connect gate="G$1" pin="RC14/SOSCO/T1CK/CN0" pad="48"/>
<connect gate="G$1" pin="RC15/OSC2/CLKO" pad="40"/>
<connect gate="G$1" pin="RD0/OC1/INT0" pad="46"/>
<connect gate="G$1" pin="RD1/OC2/~U1RTS/BCLK1" pad="49"/>
<connect gate="G$1" pin="RD10/IC3/PMCS2/PMA15/INT3/SCL1" pad="44"/>
<connect gate="G$1" pin="RD11/IC4/PMCS1/PMA14/INT4" pad="45"/>
<connect gate="G$1" pin="RD2/OC3/U1RX" pad="50"/>
<connect gate="G$1" pin="RD3/OC4/U1TX" pad="51"/>
<connect gate="G$1" pin="RD4/PMWR/OC5/IC5/CN13" pad="52"/>
<connect gate="G$1" pin="RD5/PMRD/CN14" pad="53"/>
<connect gate="G$1" pin="RD6/CN15" pad="54"/>
<connect gate="G$1" pin="RD7/CN16" pad="55"/>
<connect gate="G$1" pin="RD8/IC1/RTCC/INT1" pad="42"/>
<connect gate="G$1" pin="RD9/IC2/~U1CTS//INT2/SDA1" pad="43"/>
<connect gate="G$1" pin="RE0/PMD0" pad="60"/>
<connect gate="G$1" pin="RE1/PMD1" pad="61"/>
<connect gate="G$1" pin="RE2/PMD2" pad="62"/>
<connect gate="G$1" pin="RE3/PMD3" pad="63"/>
<connect gate="G$1" pin="RE4/PMD4" pad="64"/>
<connect gate="G$1" pin="RE5/PMD5" pad="1"/>
<connect gate="G$1" pin="RE6/PMD6" pad="2"/>
<connect gate="G$1" pin="RE7/PMD7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF3/USBID" pad="33"/>
<connect gate="G$1" pin="RF4/PMA9/U2RX/SDA2/CN17" pad="31"/>
<connect gate="G$1" pin="RF5/PMA8/U2TX/SCL2/CN18" pad="32"/>
<connect gate="G$1" pin="RG6/PMA5/SCK2/CN8" pad="4"/>
<connect gate="G$1" pin="RG7/PMA4/SDI2/CN9" pad="5"/>
<connect gate="G$1" pin="RG8/PMA3/SDO2/CN10" pad="6"/>
<connect gate="G$1" pin="RG9/PMA2/~SS2/CN11" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="56"/>
<connect gate="G$1" pin="VDD@10" pad="10"/>
<connect gate="G$1" pin="VDD@26" pad="26"/>
<connect gate="G$1" pin="VDD@38" pad="38"/>
<connect gate="G$1" pin="VSS@25" pad="25"/>
<connect gate="G$1" pin="VSS@41" pad="41"/>
<connect gate="G$1" pin="VSS@9" pad="9"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
<connect gate="G$1" pin="~MCLR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMP102" prefix="U">
<gates>
<gate name="G$1" symbol="TMP102"/>
</gates>
<devices>
<device name="" package="SOT563">
<connects>
<connect gate="G$1" pin="ADD0" pad="4"/>
<connect gate="G$1" pin="ALERT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP303LSN09">
<gates>
<gate name="G$1" symbol="NCP303LSN09"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CD" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD10KA5WF-E2">
<gates>
<gate name="G$1" symbol="BD10KA5WF-E2"/>
</gates>
<devices>
<device name="" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CTL" pad="5"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.0V">
<gates>
<gate name="G$1" symbol="1.0V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4128-2.5VREF">
<gates>
<gate name="G$1" symbol="LM4128-2.5VREF"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST-GYRO-PR">
<gates>
<gate name="G$1" symbol="ST-GYRO-PR"/>
</gates>
<devices>
<device name="LGA" package="ST-GYRO">
<connects>
<connect gate="G$1" pin="4XINX" pad="9"/>
<connect gate="G$1" pin="4XINY" pad="5"/>
<connect gate="G$1" pin="4XOUTX" pad="8"/>
<connect gate="G$1" pin="4XOUTY" pad="6"/>
<connect gate="G$1" pin="FILTVDD" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HP" pad="13"/>
<connect gate="G$1" pin="OUTX" pad="10"/>
<connect gate="G$1" pin="OUTY" pad="4"/>
<connect gate="G$1" pin="PD" pad="12"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@15" pad="15"/>
<connect gate="G$1" pin="ST" pad="11"/>
<connect gate="G$1" pin="VCONT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LGA28" package="LGA28-4X5">
<connects>
<connect gate="G$1" pin="4XINX" pad="5"/>
<connect gate="G$1" pin="4XINY" pad="16"/>
<connect gate="G$1" pin="4XOUTX" pad="7"/>
<connect gate="G$1" pin="4XOUTY" pad="14"/>
<connect gate="G$1" pin="FILTVDD" pad="18"/>
<connect gate="G$1" pin="GND" pad="26"/>
<connect gate="G$1" pin="HP" pad="24"/>
<connect gate="G$1" pin="OUTX" pad="1"/>
<connect gate="G$1" pin="OUTY" pad="20"/>
<connect gate="G$1" pin="PD" pad="28"/>
<connect gate="G$1" pin="RES@14" pad="19"/>
<connect gate="G$1" pin="RES@15" pad="25"/>
<connect gate="G$1" pin="ST" pad="27"/>
<connect gate="G$1" pin="VCONT" pad="17"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST-GYRO-PY">
<gates>
<gate name="G$1" symbol="ST-GYRO-PY"/>
</gates>
<devices>
<device name="SMD" package="ST-GYRO">
<connects>
<connect gate="G$1" pin="4XINX" pad="5"/>
<connect gate="G$1" pin="4XINZ" pad="9"/>
<connect gate="G$1" pin="4XOUTX" pad="6"/>
<connect gate="G$1" pin="4XOUTZ" pad="8"/>
<connect gate="G$1" pin="FILTVDD" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HP" pad="13"/>
<connect gate="G$1" pin="OUTX" pad="4"/>
<connect gate="G$1" pin="OUTZ" pad="10"/>
<connect gate="G$1" pin="PD" pad="12"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@15" pad="15"/>
<connect gate="G$1" pin="ST" pad="11"/>
<connect gate="G$1" pin="VCONT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC847PN">
<gates>
<gate name="G1" symbol="PNP"/>
<gate name="G2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G1" pin="B" pad="2"/>
<connect gate="G1" pin="C" pad="6"/>
<connect gate="G1" pin="E" pad="1"/>
<connect gate="G2" pin="B" pad="5"/>
<connect gate="G2" pin="C" pad="3"/>
<connect gate="G2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMBZ27VCLT1">
<gates>
<gate name="G$1" symbol="TVS"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMDT3904">
<gates>
<gate name="G$1" symbol="NPN"/>
<gate name="G$2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G$1" pin="B" pad="5"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$2" pin="B" pad="2"/>
<connect gate="G$2" pin="C" pad="6"/>
<connect gate="G$2" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931">
<gates>
<gate name="G$1" symbol="LM2931"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="INH" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S12XS64">
<gates>
<gate name="G$1" symbol="MC9S12XS64"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="ECLK/PE4" pad="21"/>
<connect gate="G$1" pin="EXTAL" pad="28"/>
<connect gate="G$1" pin="IOC0/PT0" pad="5"/>
<connect gate="G$1" pin="IOC1/PT1" pad="6"/>
<connect gate="G$1" pin="IOC1/PWM1/KWP1/PP1" pad="3"/>
<connect gate="G$1" pin="IOC2/PT2" pad="7"/>
<connect gate="G$1" pin="IOC3/PT3" pad="8"/>
<connect gate="G$1" pin="IRQ/PE1" pad="31"/>
<connect gate="G$1" pin="MODC/BKGD" pad="15"/>
<connect gate="G$1" pin="PA0" pad="33"/>
<connect gate="G$1" pin="PA1" pad="34"/>
<connect gate="G$1" pin="PA2" pad="35"/>
<connect gate="G$1" pin="PA3" pad="36"/>
<connect gate="G$1" pin="PAD00/AN00" pad="39"/>
<connect gate="G$1" pin="PAD01/AN01" pad="40"/>
<connect gate="G$1" pin="PAD02/AN02" pad="41"/>
<connect gate="G$1" pin="PAD03/AN03" pad="42"/>
<connect gate="G$1" pin="PAD04/AN04" pad="43"/>
<connect gate="G$1" pin="PAD05/AN05" pad="44"/>
<connect gate="G$1" pin="PAD06/AN06" pad="45"/>
<connect gate="G$1" pin="PAD07/AN07" pad="46"/>
<connect gate="G$1" pin="PB0" pad="16"/>
<connect gate="G$1" pin="PB5" pad="17"/>
<connect gate="G$1" pin="PB6" pad="18"/>
<connect gate="G$1" pin="PB7" pad="19"/>
<connect gate="G$1" pin="PM0/RXCAN0/RXD1" pad="60"/>
<connect gate="G$1" pin="PM1/TXCAN0/TXD1" pad="59"/>
<connect gate="G$1" pin="PM2/MISO0" pad="58"/>
<connect gate="G$1" pin="PM3/SS0" pad="57"/>
<connect gate="G$1" pin="PM4/MOSI0" pad="56"/>
<connect gate="G$1" pin="PM5/SCK0" pad="55"/>
<connect gate="G$1" pin="PP5/KPW5/PWM5" pad="64"/>
<connect gate="G$1" pin="PP7/KWP7/PWM7" pad="63"/>
<connect gate="G$1" pin="PS0/RXD0" pad="50"/>
<connect gate="G$1" pin="PS1/TXD0" pad="51"/>
<connect gate="G$1" pin="PS2/RXD1" pad="52"/>
<connect gate="G$1" pin="PS3/TXD1" pad="53"/>
<connect gate="G$1" pin="PWM3/KWP3/PP3" pad="1"/>
<connect gate="G$1" pin="PWM4/IOC4/PT4" pad="11"/>
<connect gate="G$1" pin="PWM6/IOC6/PT6" pad="13"/>
<connect gate="G$1" pin="PWM7/IOC7/PT7" pad="14"/>
<connect gate="G$1" pin="RESET" pad="24"/>
<connect gate="G$1" pin="RXD1/IOC0/PWM0/KWP0/PP0" pad="4"/>
<connect gate="G$1" pin="TEST" pad="54"/>
<connect gate="G$1" pin="TXD1/IOC2/PWM2/KWP2/PP2" pad="2"/>
<connect gate="G$1" pin="VDD" pad="37"/>
<connect gate="G$1" pin="VDDA" pad="47"/>
<connect gate="G$1" pin="VDDF" pad="9"/>
<connect gate="G$1" pin="VDDPLL" pad="30"/>
<connect gate="G$1" pin="VDDR" pad="25"/>
<connect gate="G$1" pin="VDDX1" pad="62"/>
<connect gate="G$1" pin="VDDX2" pad="23"/>
<connect gate="G$1" pin="VREG_API/PWM5/IOC5/PT" pad="12"/>
<connect gate="G$1" pin="VRH" pad="48"/>
<connect gate="G$1" pin="VSS1" pad="10"/>
<connect gate="G$1" pin="VSS2" pad="38"/>
<connect gate="G$1" pin="VSS3" pad="26"/>
<connect gate="G$1" pin="VSSA/VRL" pad="49"/>
<connect gate="G$1" pin="VSSPLL" pad="27"/>
<connect gate="G$1" pin="VSSX1" pad="61"/>
<connect gate="G$1" pin="VSSX2" pad="22"/>
<connect gate="G$1" pin="XCLKS/ECLKX2/PE7" pad="20"/>
<connect gate="G$1" pin="XIRQ/PE0" pad="32"/>
<connect gate="G$1" pin="XTAL" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393">
<gates>
<gate name="G1" symbol="OP-AMP+-"/>
<gate name="G2" symbol="OP-AMP"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G1" pin="V+" pad="8"/>
<connect gate="G1" pin="V-" pad="4"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TJA1040">
<description>CAN Tranceiver</description>
<gates>
<gate name="G$1" symbol="TJA1040TD-T"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SPLIT" pad="5"/>
<connect gate="G$1" pin="STB" pad="8"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931_FIXED">
<gates>
<gate name="G$1" symbol="LM2931_FIXED"/>
</gates>
<devices>
<device name="" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK-PSP1000">
<description>This is a footprint for the PSP-1000 Joystick.  4-pins: X, Y, Vcc and GND</description>
<gates>
<gate name="G$1" symbol="JOYSTICK-PSP1000"/>
</gates>
<devices>
<device name="" package="JOYSTICK-PSP1000">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="X" pad="X"/>
<connect gate="G$1" pin="Y" pad="Y"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVS">
<gates>
<gate name="G$1" symbol="SCHOTTKY_BRIDGE"/>
</gates>
<devices>
<device name="" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SC16IS750" prefix="IC">
<gates>
<gate name="G$1" symbol="SC16IS750"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="/CTS" pad="22"/>
<connect gate="G$1" pin="/IRQ" pad="11"/>
<connect gate="G$1" pin="/RTS" pad="21"/>
<connect gate="G$1" pin="A0-/CS" pad="6"/>
<connect gate="G$1" pin="A1-SI" pad="7"/>
<connect gate="G$1" pin="GPIO0" pad="12"/>
<connect gate="G$1" pin="GPIO1" pad="13"/>
<connect gate="G$1" pin="GPIO2" pad="14"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4-/DSR" pad="17"/>
<connect gate="G$1" pin="GPIO5-/DTR" pad="18"/>
<connect gate="G$1" pin="GPIO6-/CD" pad="19"/>
<connect gate="G$1" pin="GPIO7-/RI" pad="20"/>
<connect gate="G$1" pin="I2C-/SPI" pad="5"/>
<connect gate="G$1" pin="NC-SO" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="RX" pad="24"/>
<connect gate="G$1" pin="SCL-SCLK" pad="9"/>
<connect gate="G$1" pin="SDA-VSS" pad="10"/>
<connect gate="G$1" pin="TX" pad="23"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC2103">
<gates>
<gate name="G$1" symbol="LPC2103"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="DBGSEL" pad="27"/>
<connect gate="G$1" pin="P0.0/TXD0/MAT3.1" pad="13"/>
<connect gate="G$1" pin="P0.1/RXD0/MAT3.2" pad="14"/>
<connect gate="G$1" pin="P0.10/RTS1/CAP1.0/AD0.3" pad="35"/>
<connect gate="G$1" pin="P0.11/CTS1/CAP1.1/AD0.4" pad="36"/>
<connect gate="G$1" pin="P0.12/DSR1/MAT1.0/AD0.5" pad="37"/>
<connect gate="G$1" pin="P0.13/DTR1/MAT1.1" pad="41"/>
<connect gate="G$1" pin="P0.14/DCD1/SCK1/EINT1" pad="44"/>
<connect gate="G$1" pin="P0.15/RI1/EINT2" pad="45"/>
<connect gate="G$1" pin="P0.16/EINT0/MAT0.2" pad="46"/>
<connect gate="G$1" pin="P0.17/CAP1.2/SCL1" pad="47"/>
<connect gate="G$1" pin="P0.18/CAP1.3/SDA1" pad="48"/>
<connect gate="G$1" pin="P0.19/MAT1.2/MISO1" pad="1"/>
<connect gate="G$1" pin="P0.2/SCL0/CAP0.0" pad="18"/>
<connect gate="G$1" pin="P0.20/MAT1.3/MOSI1" pad="2"/>
<connect gate="G$1" pin="P0.21/SSEL1/MAT3.0" pad="3"/>
<connect gate="G$1" pin="P0.22/AD0.0" pad="32"/>
<connect gate="G$1" pin="P0.23/AD0.1" pad="33"/>
<connect gate="G$1" pin="P0.24/AD0.2" pad="34"/>
<connect gate="G$1" pin="P0.25/AD0.6" pad="38"/>
<connect gate="G$1" pin="P0.26/AD0.7" pad="39"/>
<connect gate="G$1" pin="P0.27/TRST/CAP2.0" pad="8"/>
<connect gate="G$1" pin="P0.28/TMS/CAP2.1" pad="9"/>
<connect gate="G$1" pin="P0.29/TCK/CAP2.2" pad="10"/>
<connect gate="G$1" pin="P0.3/SDA0/MAT0.0" pad="21"/>
<connect gate="G$1" pin="P0.30/TDI/MAT3.3" pad="15"/>
<connect gate="G$1" pin="P0.31/TDO" pad="16"/>
<connect gate="G$1" pin="P0.4/SCK0/CAP0.1" pad="22"/>
<connect gate="G$1" pin="P0.5/MISO0/MAT0.1" pad="23"/>
<connect gate="G$1" pin="P0.6/MOSI0/CAP0.2" pad="24"/>
<connect gate="G$1" pin="P0.7/SSEL0/MAT2.0" pad="28"/>
<connect gate="G$1" pin="P0.8/TXD1/MAT2.1" pad="29"/>
<connect gate="G$1" pin="P0.9/RXD1/MAT2.2" pad="30"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="RTCK" pad="26"/>
<connect gate="G$1" pin="RTCX1" pad="20"/>
<connect gate="G$1" pin="RTCX2" pad="25"/>
<connect gate="G$1" pin="VBAT" pad="4"/>
<connect gate="G$1" pin="VDD(1V8)" pad="5"/>
<connect gate="G$1" pin="VDD(3V3)@17" pad="17"/>
<connect gate="G$1" pin="VDD(3V3)@40" pad="40"/>
<connect gate="G$1" pin="VDDA" pad="42"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
<connect gate="G$1" pin="VSS@43" pad="43"/>
<connect gate="G$1" pin="VSS@7" pad="7"/>
<connect gate="G$1" pin="VSSA" pad="31"/>
<connect gate="G$1" pin="XTAL1" pad="11"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCM8240MD">
<gates>
<gate name="G$1" symbol="TCM8240MD"/>
</gates>
<devices>
<device name="" package="TCM8240MD">
<connects>
<connect gate="G$1" pin="DCLK" pad="P$19"/>
<connect gate="G$1" pin="DOUT0" pad="P$4"/>
<connect gate="G$1" pin="DOUT1" pad="P$3"/>
<connect gate="G$1" pin="DOUT2" pad="P$2"/>
<connect gate="G$1" pin="DOUT3" pad="P$1"/>
<connect gate="G$1" pin="DOUT4" pad="P$24"/>
<connect gate="G$1" pin="DOUT5" pad="P$23"/>
<connect gate="G$1" pin="DOUT6" pad="P$22"/>
<connect gate="G$1" pin="DOUT7" pad="P$21"/>
<connect gate="G$1" pin="DVDD(1.6V)" pad="P$12"/>
<connect gate="G$1" pin="EXTCLK" pad="P$13"/>
<connect gate="G$1" pin="GND@11" pad="P$11"/>
<connect gate="G$1" pin="GND@17" pad="P$17"/>
<connect gate="G$1" pin="GND@20" pad="P$20"/>
<connect gate="G$1" pin="GND@5" pad="P$5"/>
<connect gate="G$1" pin="GND@9" pad="P$9"/>
<connect gate="G$1" pin="HBLK" pad="P$15"/>
<connect gate="G$1" pin="IOVDD" pad="P$18"/>
<connect gate="G$1" pin="PVDD(2.8V)" pad="P$6"/>
<connect gate="G$1" pin="RESET" pad="P$7"/>
<connect gate="G$1" pin="SCL" pad="P$8"/>
<connect gate="G$1" pin="SDA" pad="P$10"/>
<connect gate="G$1" pin="STROBE" pad="P$14"/>
<connect gate="G$1" pin="VBLK" pad="P$16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04X2">
<gates>
<gate name="G$1" symbol="M04X2"/>
</gates>
<devices>
<device name="" package="2X4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC2571" prefix="U">
<description>Single Cell Switching Regulator - MIC2571</description>
<gates>
<gate name="G$1" symbol="MIC2571-1"/>
</gates>
<devices>
<device name="SMD" package="MSOP-8">
<connects>
<connect gate="G$1" pin="2.85V" pad="6"/>
<connect gate="G$1" pin="3.3V" pad="5"/>
<connect gate="G$1" pin="5V" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="SYNC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC7WZ07">
<gates>
<gate name="G$1" symbol="BUFFER-DUAL"/>
</gates>
<devices>
<device name="" package="SC70-6">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y1" pad="6"/>
<connect gate="G$1" pin="Y2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M08X2">
<gates>
<gate name="G$1" symbol="M2X8"/>
</gates>
<devices>
<device name="" package="2X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIT8002">
<gates>
<gate name="G$1" symbol="SIT8002"/>
</gates>
<devices>
<device name="" package="SIT8002">
<connects>
<connect gate="G$1" pin="/ST-OE" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT25FS010">
<gates>
<gate name="G$1" symbol="AT25FS010"/>
</gates>
<devices>
<device name="" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GS406SMD" prefix="U">
<description>50 Channel GS406 Helical GPS Receiver - SMD Connector.  The Mating SMD SPECIAL is called SPECIAL for a reason. This package was only made in order to make a dummy gs407 PCB with mating connector (used for testing).

sku: GPS-09079</description>
<gates>
<gate name="CONNECTOR" symbol="GS406SMD"/>
</gates>
<devices>
<device name="SOCKET" package="GS406SMD">
<connects>
<connect gate="CONNECTOR" pin="P1" pad="1"/>
<connect gate="CONNECTOR" pin="P10" pad="10"/>
<connect gate="CONNECTOR" pin="P2" pad="2"/>
<connect gate="CONNECTOR" pin="P3" pad="3"/>
<connect gate="CONNECTOR" pin="P4" pad="4"/>
<connect gate="CONNECTOR" pin="P5" pad="5"/>
<connect gate="CONNECTOR" pin="P6" pad="6"/>
<connect gate="CONNECTOR" pin="P7" pad="7"/>
<connect gate="CONNECTOR" pin="P8" pad="8"/>
<connect gate="CONNECTOR" pin="P9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MATING_SMD_***SPECIAL" package="GS406-MATING_SMD_***SPECIAL">
<connects>
<connect gate="CONNECTOR" pin="P1" pad="1"/>
<connect gate="CONNECTOR" pin="P10" pad="10"/>
<connect gate="CONNECTOR" pin="P2" pad="2"/>
<connect gate="CONNECTOR" pin="P3" pad="3"/>
<connect gate="CONNECTOR" pin="P4" pad="4"/>
<connect gate="CONNECTOR" pin="P5" pad="5"/>
<connect gate="CONNECTOR" pin="P6" pad="6"/>
<connect gate="CONNECTOR" pin="P7" pad="7"/>
<connect gate="CONNECTOR" pin="P8" pad="8"/>
<connect gate="CONNECTOR" pin="P9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT2232D">
<gates>
<gate name="G$1" symbol="FT2232D"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="6"/>
<connect gate="G$1" pin="ACBUS0" pad="15"/>
<connect gate="G$1" pin="ACBUS1" pad="13"/>
<connect gate="G$1" pin="ACBUS2" pad="12"/>
<connect gate="G$1" pin="ACBUS3" pad="11"/>
<connect gate="G$1" pin="ADBUS0" pad="24"/>
<connect gate="G$1" pin="ADBUS1" pad="23"/>
<connect gate="G$1" pin="ADBUS2" pad="22"/>
<connect gate="G$1" pin="ADBUS3" pad="21"/>
<connect gate="G$1" pin="ADBUS4" pad="20"/>
<connect gate="G$1" pin="ADBUS5" pad="19"/>
<connect gate="G$1" pin="ADBUS6" pad="17"/>
<connect gate="G$1" pin="ADBUS7" pad="16"/>
<connect gate="G$1" pin="AGND" pad="45"/>
<connect gate="G$1" pin="AVCC" pad="46"/>
<connect gate="G$1" pin="BCBUS0" pad="30"/>
<connect gate="G$1" pin="BCBUS1" pad="29"/>
<connect gate="G$1" pin="BCBUS2" pad="28"/>
<connect gate="G$1" pin="BCBUS3" pad="27"/>
<connect gate="G$1" pin="BDBUS0" pad="40"/>
<connect gate="G$1" pin="BDBUS1" pad="39"/>
<connect gate="G$1" pin="BDBUS2" pad="38"/>
<connect gate="G$1" pin="BDBUS3" pad="37"/>
<connect gate="G$1" pin="BDBUS4" pad="36"/>
<connect gate="G$1" pin="BDBUS5" pad="35"/>
<connect gate="G$1" pin="BDBUS6" pad="33"/>
<connect gate="G$1" pin="BDBUS7" pad="32"/>
<connect gate="G$1" pin="EECS" pad="48"/>
<connect gate="G$1" pin="EEDATA" pad="2"/>
<connect gate="G$1" pin="EESK" pad="1"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="GND3" pad="34"/>
<connect gate="G$1" pin="GND4" pad="9"/>
<connect gate="G$1" pin="PWEN#" pad="41"/>
<connect gate="G$1" pin="RESET#" pad="4"/>
<connect gate="G$1" pin="RSTOUT#" pad="5"/>
<connect gate="G$1" pin="SI/WUA" pad="10"/>
<connect gate="G$1" pin="SI/WUB" pad="26"/>
<connect gate="G$1" pin="TEST" pad="47"/>
<connect gate="G$1" pin="USBDM" pad="8"/>
<connect gate="G$1" pin="USBDP" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="42"/>
<connect gate="G$1" pin="VCCIOA" pad="14"/>
<connect gate="G$1" pin="VCCIOB" pad="31"/>
<connect gate="G$1" pin="XTIN" pad="43"/>
<connect gate="G$1" pin="XTOUT" pad="44"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M93C46">
<gates>
<gate name="G$1" symbol="M93C46"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR-WIDE">
<gates>
<gate name="G$1" symbol="RESONATOR"/>
</gates>
<devices>
<device name="" package="RESONATOR-WIDE-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QRE1113">
<gates>
<gate name="G$1" symbol="QRE1113"/>
</gates>
<devices>
<device name="" package="QRE1113">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS485">
<gates>
<gate name="G$1" symbol="RS485"/>
</gates>
<devices>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G$1" pin="/RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TB6621FNG">
<description>Toshiba 1A motor driver</description>
<gates>
<gate name="G$1" symbol="TB6612FNG"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="A01@1" pad="1"/>
<connect gate="G$1" pin="A01@2" pad="2"/>
<connect gate="G$1" pin="A02@5" pad="5"/>
<connect gate="G$1" pin="A02@6" pad="6"/>
<connect gate="G$1" pin="AIN1" pad="21"/>
<connect gate="G$1" pin="AIN2" pad="22"/>
<connect gate="G$1" pin="B01@11" pad="11"/>
<connect gate="G$1" pin="B01@12" pad="12"/>
<connect gate="G$1" pin="B02@7" pad="7"/>
<connect gate="G$1" pin="B02@8" pad="8"/>
<connect gate="G$1" pin="BIN1" pad="17"/>
<connect gate="G$1" pin="BIN2" pad="16"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="PGND1@3" pad="3"/>
<connect gate="G$1" pin="PGND1@4" pad="4"/>
<connect gate="G$1" pin="PGND2@10" pad="10"/>
<connect gate="G$1" pin="PGND2@9" pad="9"/>
<connect gate="G$1" pin="PWMA" pad="23"/>
<connect gate="G$1" pin="PWMB" pad="15"/>
<connect gate="G$1" pin="STBY" pad="19"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VM1" pad="24"/>
<connect gate="G$1" pin="VM2" pad="13"/>
<connect gate="G$1" pin="VM3" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTEND-DIGI-MODEM">
<description>Xtend Digi Modem WRL-09411</description>
<gates>
<gate name="G$1" symbol="XTEND-DIGI-MODEM"/>
</gates>
<devices>
<device name="" package="XTEND-DIGI-MODEM">
<connects>
<connect gate="G$1" pin="CONFIG" pad="11"/>
<connect gate="G$1" pin="CTS" pad="9"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="DO" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GPO2" pad="3"/>
<connect gate="G$1" pin="RTS" pad="10"/>
<connect gate="G$1" pin="SHDN" pad="7"/>
<connect gate="G$1" pin="SLEEP" pad="8"/>
<connect gate="G$1" pin="TX_PWR" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M24">
<gates>
<gate name="G$1" symbol="M24"/>
</gates>
<devices>
<device name="" package="1X24">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X24_LONGPADS">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-4DIGIT-YOUNGSUN" prefix="LED">
<description>This is a part for the 4-Digit 7-segment LEDs from Young Sun.  Different from the Digikey LEDs, all 16 pins are used.
The LONGPADS Variant is used for a test jig, but you may like it because there is more pad to solder to. If you are concerned about routing space, the standard works just fine though.</description>
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT-YOUNGSUN"/>
</gates>
<devices>
<device name="" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="7-SEGMENT-4DIGIT-YOUNGSUN-LONGPADS">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR_NOCAP">
<gates>
<gate name="G$1" symbol="RESONATOR_NOCAP"/>
</gates>
<devices>
<device name="" package="RESONATOR_NOCAP">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="3" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LD1117VXX">
<description>LD1117VXX voltage regulator. We carry the 3.3V version (COM-00526) in TO-220 package.</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="78XXL">
<connects>
<connect gate="G$1" pin="GND" pad="IN"/>
<connect gate="G$1" pin="IN" pad="OUT"/>
<connect gate="G$1" pin="OUT" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMD1820X">
<description>LMD1820X H-Bridge - BOB-00747</description>
<gates>
<gate name="G$1" symbol="LMD1820X"/>
</gates>
<devices>
<device name="" package="TO-220-11LEAD">
<connects>
<connect gate="G$1" pin="BRK" pad="4"/>
<connect gate="G$1" pin="BS1" pad="1"/>
<connect gate="G$1" pin="BS2" pad="11"/>
<connect gate="G$1" pin="DIR" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="PGND" pad="7"/>
<connect gate="G$1" pin="PWM" pad="5"/>
<connect gate="G$1" pin="PWR" pad="6"/>
<connect gate="G$1" pin="SGND" pad="8"/>
<connect gate="G$1" pin="TF" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M18">
<gates>
<gate name="G$1" symbol="M18"/>
</gates>
<devices>
<device name="_" package="1X18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STA540">
<gates>
<gate name="G$1" symbol="STA540"/>
</gates>
<devices>
<device name="" package="MULTIWATT15">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W/6400BG_HEATSINK" package="MULTIWATT15_6400BGHEATSINK">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W/YB324G_HEATSINK" package="MULTIWATT15_YB324GHEATSINK">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6400BG_W/SOLDERPOSTS" package="MULTIWATT15_6400BGHEATSINK_2">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358">
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
<gate name="G$2" symbol="OP-AMP"/>
</gates>
<devices>
<device name="" package="DIP08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$2" pin="+IN" pad="5"/>
<connect gate="G$2" pin="-IN" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA-100">
<gates>
<gate name="G$1" symbol="XMEGA"/>
</gates>
<devices>
<device name="SMD" package="TQFP-100-14X14MM">
<connects>
<connect gate="G$1" pin="AVCC@4" pad="4"/>
<connect gate="G$1" pin="AVCC@94" pad="94"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@33" pad="33"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="GND@53" pad="53"/>
<connect gate="G$1" pin="GND@63" pad="63"/>
<connect gate="G$1" pin="GND@73" pad="73"/>
<connect gate="G$1" pin="GND@84" pad="84"/>
<connect gate="G$1" pin="GND@93" pad="93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI/PDI_DATA" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="RESET/PDI_CLOCK" pad="90"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@24" pad="24"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="VCC@44" pad="44"/>
<connect gate="G$1" pin="VCC@54" pad="54"/>
<connect gate="G$1" pin="VCC@64" pad="64"/>
<connect gate="G$1" pin="VCC@74" pad="74"/>
<connect gate="G$1" pin="VCC@83" pad="83"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L298" prefix="U">
<description>L298 Dual Full Bridge Driver</description>
<gates>
<gate name="G$1" symbol="L298"/>
</gates>
<devices>
<device name="" package="MULTIWATT15">
<connects>
<connect gate="G$1" pin="CSA" pad="1"/>
<connect gate="G$1" pin="CSB" pad="15"/>
<connect gate="G$1" pin="ENA" pad="6"/>
<connect gate="G$1" pin="ENB" pad="11"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="OUT3" pad="13"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="VLS" pad="9"/>
<connect gate="G$1" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HEATSINK" package="MULTIWATT15_6400BGHEATSINK">
<connects>
<connect gate="G$1" pin="CSA" pad="1"/>
<connect gate="G$1" pin="CSB" pad="15"/>
<connect gate="G$1" pin="ENA" pad="6"/>
<connect gate="G$1" pin="ENB" pad="11"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="OUT3" pad="13"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="VLS" pad="9"/>
<connect gate="G$1" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ILD213T" prefix="IC">
<gates>
<gate name="G$1" symbol="ILD213T"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="4"/>
<connect gate="G$1" pin="CT1" pad="6"/>
<connect gate="G$1" pin="CT2" pad="8"/>
<connect gate="G$1" pin="ET1" pad="5"/>
<connect gate="G$1" pin="ET2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIN_5_FEMALE">
<gates>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIDI_CONN_FEMALE">
<gates>
<gate name="G$1" symbol="MIDI_CONN_FEMALE"/>
</gates>
<devices>
<device name="" package="DIN_5_FEMALE">
<connects>
<connect gate="G$1" pin="MIDI_IN" pad="4"/>
<connect gate="G$1" pin="MIDI_OUT" pad="5"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
<connect gate="G$1" pin="NC3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSOP20">
<gates>
<gate name="G$1" symbol="SSOP20"/>
</gates>
<devices>
<device name="" package="SSOP20-LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HIH-4030" prefix="U">
<description>Humidity Sensor</description>
<gates>
<gate name="G$1" symbol="HIH-4030"/>
</gates>
<devices>
<device name="SMD" package="HIH-4030">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-OTL">
<gates>
<gate name="G$1" symbol="OVERTONE_LOGO"/>
</gates>
<devices>
<device name="" package="OVERTONE_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISZ500" prefix="U">
<description>ISZ500 Single axis gyro</description>
<gates>
<gate name="G$1" symbol="ISZ-500"/>
</gates>
<devices>
<device name="SMD" package="QFN-28_6X8">
<connects>
<connect gate="G$1" pin="AZ" pad="24"/>
<connect gate="G$1" pin="CPOUT" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="PTATS" pad="23"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
<connect gate="G$1" pin="Z-OUT" pad="20"/>
<connect gate="G$1" pin="Z4.5IN" pad="16"/>
<connect gate="G$1" pin="Z4.5OUT" pad="14"/>
<connect gate="G$1" pin="ZAGC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F6015" prefix="U">
<gates>
<gate name="G$1" symbol="DSPIC30F6015"/>
</gates>
<devices>
<device name="SMD" package="TQFP64">
<connects>
<connect gate="G$1" pin="AGND@20" pad="20"/>
<connect gate="G$1" pin="AVDD@19" pad="19"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@41" pad="41"/>
<connect gate="G$1" pin="GND@56" pad="56"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="MCLR@7" pad="7"/>
<connect gate="G$1" pin="OSC1@39" pad="39"/>
<connect gate="G$1" pin="OSC2@40" pad="40"/>
<connect gate="G$1" pin="PGC@17" pad="17"/>
<connect gate="G$1" pin="PGD@18" pad="18"/>
<connect gate="G$1" pin="RB10@23" pad="23"/>
<connect gate="G$1" pin="RB11@24" pad="24"/>
<connect gate="G$1" pin="RB12@27" pad="27"/>
<connect gate="G$1" pin="RB13@28" pad="28"/>
<connect gate="G$1" pin="RB14@29" pad="29"/>
<connect gate="G$1" pin="RB15@30" pad="30"/>
<connect gate="G$1" pin="RB2@14" pad="14"/>
<connect gate="G$1" pin="RB3@13" pad="13"/>
<connect gate="G$1" pin="RB4@12" pad="12"/>
<connect gate="G$1" pin="RB5@11" pad="11"/>
<connect gate="G$1" pin="RB8@21" pad="21"/>
<connect gate="G$1" pin="RB9@22" pad="22"/>
<connect gate="G$1" pin="RC13@47" pad="47"/>
<connect gate="G$1" pin="RC14@48" pad="48"/>
<connect gate="G$1" pin="RD0@46" pad="46"/>
<connect gate="G$1" pin="RD10@44" pad="44"/>
<connect gate="G$1" pin="RD11@45" pad="45"/>
<connect gate="G$1" pin="RD1@49" pad="49"/>
<connect gate="G$1" pin="RD2@50" pad="50"/>
<connect gate="G$1" pin="RD3@51" pad="51"/>
<connect gate="G$1" pin="RD4@52" pad="52"/>
<connect gate="G$1" pin="RD5@53" pad="53"/>
<connect gate="G$1" pin="RD6@54" pad="54"/>
<connect gate="G$1" pin="RD7@55" pad="55"/>
<connect gate="G$1" pin="RD8@42" pad="42"/>
<connect gate="G$1" pin="RD9@43" pad="43"/>
<connect gate="G$1" pin="RE0@60" pad="60"/>
<connect gate="G$1" pin="RE1@61" pad="61"/>
<connect gate="G$1" pin="RE2@62" pad="62"/>
<connect gate="G$1" pin="RE3@63" pad="63"/>
<connect gate="G$1" pin="RE4@64" pad="64"/>
<connect gate="G$1" pin="RE5@1" pad="1"/>
<connect gate="G$1" pin="RE6@2" pad="2"/>
<connect gate="G$1" pin="RE7@3" pad="3"/>
<connect gate="G$1" pin="RF0@58" pad="58"/>
<connect gate="G$1" pin="RF1@59" pad="59"/>
<connect gate="G$1" pin="RF6@35" pad="35"/>
<connect gate="G$1" pin="RG2@37" pad="37"/>
<connect gate="G$1" pin="RG3@36" pad="36"/>
<connect gate="G$1" pin="RG6@4" pad="4"/>
<connect gate="G$1" pin="RG7@5" pad="5"/>
<connect gate="G$1" pin="RG8@6" pad="6"/>
<connect gate="G$1" pin="RG9@8" pad="8"/>
<connect gate="G$1" pin="RX1@34" pad="34"/>
<connect gate="G$1" pin="RX2@32" pad="32"/>
<connect gate="G$1" pin="TX1@33" pad="33"/>
<connect gate="G$1" pin="TX2@31" pad="31"/>
<connect gate="G$1" pin="VDD@10" pad="10"/>
<connect gate="G$1" pin="VDD@26" pad="26"/>
<connect gate="G$1" pin="VDD@38" pad="38"/>
<connect gate="G$1" pin="VDD@57" pad="57"/>
<connect gate="G$1" pin="VREF+/RB0@16" pad="16"/>
<connect gate="G$1" pin="VREF-/RB1@15" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_MIC5216">
<description>500mA LDO, MSOP8 for better dissipation</description>
<gates>
<gate name="G$1" symbol="MIC5216"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="FLAG" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZIFSOCKET-28-3">
<gates>
<gate name="G$1" symbol="DIL-28-3"/>
</gates>
<devices>
<device name="ZIFFSOCKET-28-3" package="DIL28-3-ZIF_SOCKET">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZIFSOCKET-40-6">
<gates>
<gate name="G$1" symbol="DIL-40-6"/>
</gates>
<devices>
<device name="DIL40-6-ZIF_SOCKET" package="DIL40-6-ZIF_SOCKET">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KENT_LCD_CONN">
<gates>
<gate name="G$1" symbol="KENT_LCD_CONN"/>
</gates>
<devices>
<device name="" package="FFC_16">
<connects>
<connect gate="G$1" pin="/RESET" pad="1"/>
<connect gate="G$1" pin="BUSY" pad="2"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="NC1" pad="15"/>
<connect gate="G$1" pin="NC2" pad="16"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SI" pad="6"/>
<connect gate="G$1" pin="SO" pad="5"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VPWR1" pad="10"/>
<connect gate="G$1" pin="VPWR2" pad="11"/>
<connect gate="G$1" pin="VPWR3" pad="13"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="8"/>
<connect gate="G$1" pin="VSS3" pad="12"/>
<connect gate="G$1" pin="VSS4" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDER">
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="" package="SLIDER">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="S" pad="2A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIDI_CONN_FEMALE_SUPPORT">
<gates>
<gate name="G$1" symbol="MIDI_CONN_FEMALE"/>
</gates>
<devices>
<device name="" package="DIN_5_FEMALE_SUPPORT">
<connects>
<connect gate="G$1" pin="MIDI_IN" pad="4"/>
<connect gate="G$1" pin="MIDI_OUT" pad="5"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
<connect gate="G$1" pin="NC3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPTO_DARL_6N138S">
<gates>
<gate name="G$1" symbol="OPTO_DARLINGTON_6N138-39"/>
</gates>
<devices>
<device name="" package="8-SMD">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6400BG_HEATSINK">
<gates>
<gate name="G$1" symbol="6400GB_HEATSINK"/>
</gates>
<devices>
<device name="" package="6400BG_HEATSINK">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISD1900" prefix="U">
<gates>
<gate name="G$1" symbol="ISD1932"/>
</gates>
<devices>
<device name="ISD1932" package="SO-28W">
<connects>
<connect gate="G$1" pin="ADDR/_DRCT" pad="27"/>
<connect gate="G$1" pin="AGC" pad="17"/>
<connect gate="G$1" pin="E0/_M5" pad="7"/>
<connect gate="G$1" pin="E1/_M6" pad="9"/>
<connect gate="G$1" pin="E2/_M7" pad="10"/>
<connect gate="G$1" pin="E3/_M8" pad="11"/>
<connect gate="G$1" pin="MIC+" pad="18"/>
<connect gate="G$1" pin="MIC-" pad="19"/>
<connect gate="G$1" pin="ROSC" pad="20"/>
<connect gate="G$1" pin="S0/_M1" pad="2"/>
<connect gate="G$1" pin="S1/_M2" pad="3"/>
<connect gate="G$1" pin="S2/_M3" pad="4"/>
<connect gate="G$1" pin="S3/_M4" pad="5"/>
<connect gate="G$1" pin="SP+" pad="15"/>
<connect gate="G$1" pin="SP-" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="21"/>
<connect gate="G$1" pin="VCCD" pad="28"/>
<connect gate="G$1" pin="VCCP" pad="14"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="VSSD" pad="1"/>
<connect gate="G$1" pin="VSSP1" pad="16"/>
<connect gate="G$1" pin="VSSP2" pad="12"/>
<connect gate="G$1" pin="XCLK/FMC3" pad="25"/>
<connect gate="G$1" pin="_FT" pad="26"/>
<connect gate="G$1" pin="_LED" pad="22"/>
<connect gate="G$1" pin="_PLAYE/FMC2" pad="23"/>
<connect gate="G$1" pin="_PLAYL/FMC1" pad="6"/>
<connect gate="G$1" pin="_REC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74HC238">
<description>M74HC238 - CMOS 3 TO 8 LINE DECODER</description>
<gates>
<gate name="G$1" symbol="M74HC238"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="G1" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y0" pad="15"/>
<connect gate="G$1" pin="Y1" pad="14"/>
<connect gate="G$1" pin="Y2" pad="13"/>
<connect gate="G$1" pin="Y3" pad="12"/>
<connect gate="G$1" pin="Y4" pad="11"/>
<connect gate="G$1" pin="Y5" pad="10"/>
<connect gate="G$1" pin="Y6" pad="9"/>
<connect gate="G$1" pin="Y7" pad="7"/>
<connect gate="G$1" pin="~G2A" pad="4"/>
<connect gate="G$1" pin="~G2B" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENC28J60" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="ENC28J60"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="/INT" pad="4"/>
<connect gate="G$1" pin="CLKOUT" pad="3"/>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="LEDA" pad="27"/>
<connect gate="G$1" pin="LEDB" pad="26"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="23"/>
<connect gate="G$1" pin="OSC2" pad="24"/>
<connect gate="G$1" pin="RBIAS" pad="14"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SCK" pad="8"/>
<connect gate="G$1" pin="SI" pad="7"/>
<connect gate="G$1" pin="SO" pad="6"/>
<connect gate="G$1" pin="TPIN+" pad="13"/>
<connect gate="G$1" pin="TPIN-" pad="12"/>
<connect gate="G$1" pin="TPOUT+" pad="17"/>
<connect gate="G$1" pin="TPOUT-" pad="16"/>
<connect gate="G$1" pin="VCAP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VDDOSC" pad="25"/>
<connect gate="G$1" pin="VDDPLL" pad="20"/>
<connect gate="G$1" pin="VDDRX" pad="19"/>
<connect gate="G$1" pin="VDDTX" pad="15"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="VSSOSC" pad="22"/>
<connect gate="G$1" pin="VSSPLL" pad="21"/>
<connect gate="G$1" pin="VSSRX" pad="11"/>
<connect gate="G$1" pin="VSSTX" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLE_BITS_CONN">
<gates>
<gate name="G$1" symbol="LITTLEBITS"/>
</gates>
<devices>
<device name="" package="LITTLEBITS">
<connects>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="SIG" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FUSE" prefix="F">
<gates>
<gate name="G$1" symbol="FUSE"/>
</gates>
<devices>
<device name="X20MM" package="FUSE_5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPEAKJET" prefix="U">
<gates>
<gate name="G$1" symbol="SPEAKJET"/>
</gates>
<devices>
<device name="DIP" package="DIL18">
<connects>
<connect gate="G$1" pin="D0/RDY" pad="17"/>
<connect gate="G$1" pin="D1/SPK" pad="16"/>
<connect gate="G$1" pin="D2/BHF" pad="15"/>
<connect gate="G$1" pin="E0" pad="9"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="7"/>
<connect gate="G$1" pin="E3" pad="6"/>
<connect gate="G$1" pin="E4" pad="4"/>
<connect gate="G$1" pin="E5" pad="3"/>
<connect gate="G$1" pin="E6/RC0" pad="2"/>
<connect gate="G$1" pin="E7/RC1" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="M0" pad="13"/>
<connect gate="G$1" pin="M1" pad="12"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VOICE" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOIC-18">
<connects>
<connect gate="G$1" pin="D0/RDY" pad="17"/>
<connect gate="G$1" pin="D1/SPK" pad="16"/>
<connect gate="G$1" pin="D2/BHF" pad="15"/>
<connect gate="G$1" pin="E0" pad="9"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="7"/>
<connect gate="G$1" pin="E3" pad="6"/>
<connect gate="G$1" pin="E4" pad="4"/>
<connect gate="G$1" pin="E5" pad="3"/>
<connect gate="G$1" pin="E6/RC0" pad="2"/>
<connect gate="G$1" pin="E7/RC1" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="M0" pad="13"/>
<connect gate="G$1" pin="M1" pad="12"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VOICE" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLEBITS_MALE">
<gates>
<gate name="G$1" symbol="LITTLEBITS_MALE"/>
</gates>
<devices>
<device name="" package="LITTLE_BITS_MALE">
<connects>
<connect gate="G$1" pin="GND" pad="V-"/>
<connect gate="G$1" pin="SIG" pad="SIG"/>
<connect gate="G$1" pin="VCC" pad="V+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLEBITS_FEMALE" prefix="JP">
<gates>
<gate name="G$1" symbol="LITTLEBITS_FEMALE"/>
</gates>
<devices>
<device name="" package="LITTLE_BITS_FEMALE">
<connects>
<connect gate="G$1" pin="GND" pad="V-"/>
<connect gate="G$1" pin="SIG" pad="SIG"/>
<connect gate="G$1" pin="VCC" pad="V+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74HC251" prefix="U">
<description>SN54HC251 Data Selector/Multiplexer</description>
<gates>
<gate name="G$1" symbol="SN74HC251"/>
</gates>
<devices>
<device name="_SMD" package="SO016">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="9"/>
<connect gate="G$1" pin="D0" pad="4"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="1"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="12"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="OE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="W" pad="6"/>
<connect gate="G$1" pin="Y" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON-REBEL">
<gates>
<gate name="G$1" symbol="LUXEON"/>
</gates>
<devices>
<device name="" package="LUXEON-REBEL">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
<connect gate="G$1" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB3318">
<gates>
<gate name="G$1" symbol="USB3318"/>
</gates>
<devices>
<device name="" package="QFN-24-USB">
<connects>
<connect gate="G$1" pin="CLKOUT" pad="12"/>
<connect gate="G$1" pin="CPEN" pad="7"/>
<connect gate="G$1" pin="DATA0" pad="16"/>
<connect gate="G$1" pin="DATA1" pad="15"/>
<connect gate="G$1" pin="DATA2" pad="14"/>
<connect gate="G$1" pin="DATA3" pad="13"/>
<connect gate="G$1" pin="DATA4" pad="11"/>
<connect gate="G$1" pin="DATA5" pad="10"/>
<connect gate="G$1" pin="DATA6" pad="9"/>
<connect gate="G$1" pin="DATA7" pad="8"/>
<connect gate="G$1" pin="DIR" pad="19"/>
<connect gate="G$1" pin="DM" pad="5"/>
<connect gate="G$1" pin="DP" pad="6"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="ID" pad="1"/>
<connect gate="G$1" pin="NXT" pad="18"/>
<connect gate="G$1" pin="RBIAS" pad="24"/>
<connect gate="G$1" pin="REFCLK" pad="23"/>
<connect gate="G$1" pin="RESETB" pad="22"/>
<connect gate="G$1" pin="STP" pad="20"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VBUS" pad="2"/>
<connect gate="G$1" pin="VDD18" pad="21"/>
<connect gate="G$1" pin="VDD33" pad="4"/>
<connect gate="G$1" pin="VDDIO" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPR121">
<description>MPR121 Capacitive Touch Sensor Controller</description>
<gates>
<gate name="G$1" symbol="MPR121"/>
</gates>
<devices>
<device name="QFN20" package="QFN-20-0.4MM">
<connects>
<connect gate="G$1" pin="ADDR" pad="4"/>
<connect gate="G$1" pin="ELE0" pad="8"/>
<connect gate="G$1" pin="ELE1" pad="9"/>
<connect gate="G$1" pin="ELE10/LED6" pad="18"/>
<connect gate="G$1" pin="ELE11/LED7" pad="19"/>
<connect gate="G$1" pin="ELE2" pad="10"/>
<connect gate="G$1" pin="ELE3" pad="11"/>
<connect gate="G$1" pin="ELE4/LED0" pad="12"/>
<connect gate="G$1" pin="ELE5/LED1" pad="13"/>
<connect gate="G$1" pin="ELE6/LED2" pad="14"/>
<connect gate="G$1" pin="ELE7/LED3" pad="15"/>
<connect gate="G$1" pin="ELE8/LED4" pad="16"/>
<connect gate="G$1" pin="ELE9/LED5" pad="17"/>
<connect gate="G$1" pin="REXT" pad="7"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VREG" pad="5"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="~IRQ" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA7361" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="MMA7361"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="0GD" pad="9"/>
<connect gate="G$1" pin="GSELECT" pad="10"/>
<connect gate="G$1" pin="SLEEP" pad="7"/>
<connect gate="G$1" pin="ST" pad="13"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="XOUT" pad="2"/>
<connect gate="G$1" pin="YOUT" pad="3"/>
<connect gate="G$1" pin="ZOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA128" prefix="U">
<description>ATmega128/128L/1281/2561. Note: The ATmega128 pin 1 is PEN and the ATmega256/1281 pin 1 is PG5.</description>
<gates>
<gate name="G$1" symbol="ATMEGA128"/>
</gates>
<devices>
<device name="_SMD" package="TQFP64">
<connects>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@53" pad="53"/>
<connect gate="G$1" pin="PA0" pad="51"/>
<connect gate="G$1" pin="PA1" pad="50"/>
<connect gate="G$1" pin="PA2" pad="49"/>
<connect gate="G$1" pin="PA3" pad="48"/>
<connect gate="G$1" pin="PA4" pad="47"/>
<connect gate="G$1" pin="PA5" pad="46"/>
<connect gate="G$1" pin="PA6" pad="45"/>
<connect gate="G$1" pin="PA7" pad="44"/>
<connect gate="G$1" pin="PB0(SS)" pad="10"/>
<connect gate="G$1" pin="PB1(SCK)" pad="11"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="12"/>
<connect gate="G$1" pin="PB3(MISO)" pad="13"/>
<connect gate="G$1" pin="PB4" pad="14"/>
<connect gate="G$1" pin="PB5" pad="15"/>
<connect gate="G$1" pin="PB6" pad="16"/>
<connect gate="G$1" pin="PB7" pad="17"/>
<connect gate="G$1" pin="PC0" pad="35"/>
<connect gate="G$1" pin="PC1" pad="36"/>
<connect gate="G$1" pin="PC2" pad="37"/>
<connect gate="G$1" pin="PC3" pad="38"/>
<connect gate="G$1" pin="PC4" pad="39"/>
<connect gate="G$1" pin="PC5" pad="40"/>
<connect gate="G$1" pin="PC6" pad="41"/>
<connect gate="G$1" pin="PC7" pad="42"/>
<connect gate="G$1" pin="PD0(SCL)" pad="25"/>
<connect gate="G$1" pin="PD1(SDA)" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PE0(RXD)" pad="2"/>
<connect gate="G$1" pin="PE1(TXD)" pad="3"/>
<connect gate="G$1" pin="PE2" pad="4"/>
<connect gate="G$1" pin="PE3" pad="5"/>
<connect gate="G$1" pin="PE4" pad="6"/>
<connect gate="G$1" pin="PE5" pad="7"/>
<connect gate="G$1" pin="PE6" pad="8"/>
<connect gate="G$1" pin="PE7" pad="9"/>
<connect gate="G$1" pin="PF0" pad="61"/>
<connect gate="G$1" pin="PF1" pad="60"/>
<connect gate="G$1" pin="PF2" pad="59"/>
<connect gate="G$1" pin="PF3" pad="58"/>
<connect gate="G$1" pin="PF4" pad="57"/>
<connect gate="G$1" pin="PF5" pad="56"/>
<connect gate="G$1" pin="PF6" pad="55"/>
<connect gate="G$1" pin="PF7" pad="54"/>
<connect gate="G$1" pin="PG0" pad="33"/>
<connect gate="G$1" pin="PG1" pad="34"/>
<connect gate="G$1" pin="PG2" pad="43"/>
<connect gate="G$1" pin="PG3" pad="18"/>
<connect gate="G$1" pin="PG4" pad="19"/>
<connect gate="G$1" pin="PG5" pad="1"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@21" pad="21"/>
<connect gate="G$1" pin="VCC@52" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="TQFP64_14X14MM">
<connects>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@53" pad="53"/>
<connect gate="G$1" pin="PA0" pad="51"/>
<connect gate="G$1" pin="PA1" pad="50"/>
<connect gate="G$1" pin="PA2" pad="49"/>
<connect gate="G$1" pin="PA3" pad="48"/>
<connect gate="G$1" pin="PA4" pad="47"/>
<connect gate="G$1" pin="PA5" pad="46"/>
<connect gate="G$1" pin="PA6" pad="45"/>
<connect gate="G$1" pin="PA7" pad="44"/>
<connect gate="G$1" pin="PB0(SS)" pad="10"/>
<connect gate="G$1" pin="PB1(SCK)" pad="11"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="12"/>
<connect gate="G$1" pin="PB3(MISO)" pad="13"/>
<connect gate="G$1" pin="PB4" pad="14"/>
<connect gate="G$1" pin="PB5" pad="15"/>
<connect gate="G$1" pin="PB6" pad="16"/>
<connect gate="G$1" pin="PB7" pad="17"/>
<connect gate="G$1" pin="PC0" pad="35"/>
<connect gate="G$1" pin="PC1" pad="36"/>
<connect gate="G$1" pin="PC2" pad="37"/>
<connect gate="G$1" pin="PC3" pad="38"/>
<connect gate="G$1" pin="PC4" pad="39"/>
<connect gate="G$1" pin="PC5" pad="40"/>
<connect gate="G$1" pin="PC6" pad="41"/>
<connect gate="G$1" pin="PC7" pad="42"/>
<connect gate="G$1" pin="PD0(SCL)" pad="25"/>
<connect gate="G$1" pin="PD1(SDA)" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PE0(RXD)" pad="2"/>
<connect gate="G$1" pin="PE1(TXD)" pad="3"/>
<connect gate="G$1" pin="PE2" pad="4"/>
<connect gate="G$1" pin="PE3" pad="5"/>
<connect gate="G$1" pin="PE4" pad="6"/>
<connect gate="G$1" pin="PE5" pad="7"/>
<connect gate="G$1" pin="PE6" pad="8"/>
<connect gate="G$1" pin="PE7" pad="9"/>
<connect gate="G$1" pin="PF0" pad="61"/>
<connect gate="G$1" pin="PF1" pad="60"/>
<connect gate="G$1" pin="PF2" pad="59"/>
<connect gate="G$1" pin="PF3" pad="58"/>
<connect gate="G$1" pin="PF4" pad="57"/>
<connect gate="G$1" pin="PF5" pad="56"/>
<connect gate="G$1" pin="PF6" pad="55"/>
<connect gate="G$1" pin="PF7" pad="54"/>
<connect gate="G$1" pin="PG0" pad="33"/>
<connect gate="G$1" pin="PG1" pad="34"/>
<connect gate="G$1" pin="PG2" pad="43"/>
<connect gate="G$1" pin="PG3" pad="18"/>
<connect gate="G$1" pin="PG4" pad="19"/>
<connect gate="G$1" pin="PG5" pad="1"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@21" pad="21"/>
<connect gate="G$1" pin="VCC@52" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREENKEYMATINGCONNECTOR">
<gates>
<gate name="G$1" symbol="SCREENKEYMATINGCONNECTOR"/>
</gates>
<devices>
<device name="" package="SCREENKEYMATINGCONNECTOR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIO_LOGO">
<gates>
<gate name="G$1" symbol="FIO_LOGO"/>
</gates>
<devices>
<device name="V2" package="FUNNEL_LOGO_BOTTOM_V2">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMP085">
<description>&lt;b&gt;BMP085 Pressure Sensor&lt;/b&gt; Great little MEMS pressure sensor. SKU: COM-09603</description>
<gates>
<gate name="G$1" symbol="BMP085"/>
</gates>
<devices>
<device name="" package="BMP085">
<connects>
<connect gate="G$1" pin="EOC" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="3"/>
<connect gate="G$1" pin="VDDD" pad="4"/>
<connect gate="G$1" pin="XCLR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XR2206" prefix="U">
<description>XR2206 Monolithic Function Generator</description>
<gates>
<gate name="G$1" symbol="XR2206"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="AMSI" pad="1"/>
<connect gate="G$1" pin="BIAS" pad="10"/>
<connect gate="G$1" pin="FSKI" pad="9"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="MO" pad="3"/>
<connect gate="G$1" pin="STO" pad="2"/>
<connect gate="G$1" pin="SYMA1" pad="15"/>
<connect gate="G$1" pin="SYMA2" pad="16"/>
<connect gate="G$1" pin="SYNCO" pad="11"/>
<connect gate="G$1" pin="TC1" pad="5"/>
<connect gate="G$1" pin="TC2" pad="6"/>
<connect gate="G$1" pin="TR1" pad="7"/>
<connect gate="G$1" pin="TR2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="WAVEA1" pad="13"/>
<connect gate="G$1" pin="WAVEA2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC04_HEX_INVERTER" prefix="U">
<description>74HC04 Hex Inverter</description>
<gates>
<gate name="G$1" symbol="74HC04_HEX_INVERTER"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1Y" pad="2"/>
<connect gate="G$1" pin="2A" pad="3"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="3A" pad="5"/>
<connect gate="G$1" pin="3Y" pad="6"/>
<connect gate="G$1" pin="4A" pad="9"/>
<connect gate="G$1" pin="4Y" pad="8"/>
<connect gate="G$1" pin="5A" pad="11"/>
<connect gate="G$1" pin="5Y" pad="10"/>
<connect gate="G$1" pin="6A" pad="13"/>
<connect gate="G$1" pin="6Y" pad="12"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEX_CONVERTER" prefix="U">
<gates>
<gate name="G$1" symbol="M74HC4050"/>
</gates>
<devices>
<device name="" package="SO016">
<connects>
<connect gate="G$1" pin="1A" pad="3"/>
<connect gate="G$1" pin="1Y" pad="2"/>
<connect gate="G$1" pin="2A" pad="5"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="3A" pad="7"/>
<connect gate="G$1" pin="3Y" pad="6"/>
<connect gate="G$1" pin="4A" pad="9"/>
<connect gate="G$1" pin="4Y" pad="10"/>
<connect gate="G$1" pin="5A" pad="11"/>
<connect gate="G$1" pin="5Y" pad="12"/>
<connect gate="G$1" pin="6A" pad="14"/>
<connect gate="G$1" pin="6Y" pad="15"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPL115A" prefix="U">
<description>&lt;b&gt;&lt;h3&gt;MPL115A1 (SPI) and MPL115A2 (I2C)&lt;/h3&gt;&lt;/b&gt;&lt;br&gt;
Miniature Digital Barometer&lt;br&gt;&lt;br&gt;
5.0x3.0x1.2mm LGA Package</description>
<gates>
<gate name="G$1" symbol="MPL115A"/>
</gates>
<devices>
<device name="" package="LGA8">
<connects>
<connect gate="G$1" pin="CAP" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC/DOUT" pad="6"/>
<connect gate="G$1" pin="RST/CS" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="8"/>
<connect gate="G$1" pin="SDA/DIN" pad="7"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_MICROB_PLUG" prefix="JP">
<description>&lt;h3&gt;USB Micro-B Plug&lt;/h3&gt;
Comes in a variety of packages.  Check out Hirose's ZX-x0 line: http://www.hirose.co.jp/cataloge_hp/e24200011.pdf</description>
<gates>
<gate name="G$1" symbol="MICROB-PLUG"/>
</gates>
<devices>
<device name="" package="MICRO-B-RA-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH" package="MICRO-B-RA-TH">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH2" package="MICRO-B-TH">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT" package="MICRO-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMA180">
<gates>
<gate name="G$1" symbol="BMA180"/>
</gates>
<devices>
<device name="" package="LGA12">
<connects>
<connect gate="G$1" pin="CSB" pad="5"/>
<connect gate="G$1" pin="INT" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="11"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="SDI" pad="9"/>
<connect gate="G$1" pin="SDO" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="10"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LYPR540AH">
<gates>
<gate name="G$1" symbol="LYPR540AH"/>
</gates>
<devices>
<device name="" package="LGA28L">
<connects>
<connect gate="G$1" pin="4XX" pad="17"/>
<connect gate="G$1" pin="4XY" pad="16"/>
<connect gate="G$1" pin="4XZ" pad="15"/>
<connect gate="G$1" pin="FILTVDD_2G" pad="14"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESGND1" pad="8"/>
<connect gate="G$1" pin="RESGND2" pad="23"/>
<connect gate="G$1" pin="RESVDD1" pad="24"/>
<connect gate="G$1" pin="RESVDD2" pad="25"/>
<connect gate="G$1" pin="RESVDD3" pad="26"/>
<connect gate="G$1" pin="RESVDD4" pad="27"/>
<connect gate="G$1" pin="ST" pad="9"/>
<connect gate="G$1" pin="VCONT_1G" pad="12"/>
<connect gate="G$1" pin="VCONT_2G" pad="13"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="X" pad="22"/>
<connect gate="G$1" pin="Y" pad="21"/>
<connect gate="G$1" pin="Z" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMZ14203" prefix="U">
<description>LMZ14203 3A, Simple Switcher Power Module with 42V Maximum Input</description>
<gates>
<gate name="G$1" symbol="LMZ14203"/>
</gates>
<devices>
<device name="" package="TO-PMOD-7">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="EP" pad="EP"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD5330" prefix="U">
<gates>
<gate name="G$1" symbol="AD5330"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="BUF" pad="1"/>
<connect gate="G$1" pin="CLR" pad="9"/>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="DB0" pad="13"/>
<connect gate="G$1" pin="DB1" pad="14"/>
<connect gate="G$1" pin="DB2" pad="15"/>
<connect gate="G$1" pin="DB3" pad="16"/>
<connect gate="G$1" pin="DB4" pad="17"/>
<connect gate="G$1" pin="DB5" pad="18"/>
<connect gate="G$1" pin="DB6" pad="19"/>
<connect gate="G$1" pin="DB7" pad="20"/>
<connect gate="G$1" pin="GAIN" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LDAC" pad="10"/>
<connect gate="G$1" pin="PD" pad="11"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
<connect gate="G$1" pin="VREF" pad="3"/>
<connect gate="G$1" pin="WR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LSM303DLH" prefix="U">
<gates>
<gate name="G$1" symbol="LSM303DLH"/>
</gates>
<devices>
<device name="SMD" package="LGA28-5X5">
<connects>
<connect gate="G$1" pin="C1" pad="15"/>
<connect gate="G$1" pin="DRDY_M" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="INT1" pad="26"/>
<connect gate="G$1" pin="INT2" pad="27"/>
<connect gate="G$1" pin="SA0_A" pad="4"/>
<connect gate="G$1" pin="SCL_A" pad="24"/>
<connect gate="G$1" pin="SCL_M" pad="20"/>
<connect gate="G$1" pin="SDA_A" pad="25"/>
<connect gate="G$1" pin="SDA_M" pad="19"/>
<connect gate="G$1" pin="SET1" pad="16"/>
<connect gate="G$1" pin="SET2" pad="12"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VDD@7" pad="7"/>
<connect gate="G$1" pin="VDD_I2C" pad="5"/>
<connect gate="G$1" pin="VDD_IO@22" pad="22"/>
<connect gate="G$1" pin="VDD_IO@23" pad="23"/>
<connect gate="G$1" pin="VDD_M" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA128RFA1" prefix="U">
<gates>
<gate name="G$1" symbol="ATMEGA128RFA1"/>
</gates>
<devices>
<device name="" package="QFN-64">
<connects>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVDD" pad="60"/>
<connect gate="G$1" pin="AVSS@58" pad="58"/>
<connect gate="G$1" pin="AVSS@61" pad="61"/>
<connect gate="G$1" pin="AVSS_RFN" pad="10"/>
<connect gate="G$1" pin="AVSS_RFP" pad="7"/>
<connect gate="G$1" pin="CLKI" pad="33"/>
<connect gate="G$1" pin="DEVDD@23" pad="23"/>
<connect gate="G$1" pin="DEVDD@34" pad="34"/>
<connect gate="G$1" pin="DEVDD@44" pad="44"/>
<connect gate="G$1" pin="DEVDD@54" pad="54"/>
<connect gate="G$1" pin="DVDD@21" pad="21"/>
<connect gate="G$1" pin="DVDD@22" pad="22"/>
<connect gate="G$1" pin="DVSS@20" pad="20"/>
<connect gate="G$1" pin="DVSS@24" pad="24"/>
<connect gate="G$1" pin="DVSS@35" pad="35"/>
<connect gate="G$1" pin="DVSS@45" pad="45"/>
<connect gate="G$1" pin="DVSS@55" pad="55"/>
<connect gate="G$1" pin="EVDD" pad="59"/>
<connect gate="G$1" pin="PB0" pad="36"/>
<connect gate="G$1" pin="PB1/SCK" pad="37"/>
<connect gate="G$1" pin="PB2/PDI" pad="38"/>
<connect gate="G$1" pin="PB3/PDO" pad="39"/>
<connect gate="G$1" pin="PB4" pad="40"/>
<connect gate="G$1" pin="PB5" pad="41"/>
<connect gate="G$1" pin="PB6" pad="42"/>
<connect gate="G$1" pin="PB7" pad="43"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PE0" pad="46"/>
<connect gate="G$1" pin="PE1" pad="47"/>
<connect gate="G$1" pin="PE2" pad="48"/>
<connect gate="G$1" pin="PE3" pad="49"/>
<connect gate="G$1" pin="PE4" pad="50"/>
<connect gate="G$1" pin="PE5" pad="51"/>
<connect gate="G$1" pin="PE6" pad="52"/>
<connect gate="G$1" pin="PE7" pad="53"/>
<connect gate="G$1" pin="PF0" pad="63"/>
<connect gate="G$1" pin="PF1" pad="64"/>
<connect gate="G$1" pin="PF2" pad="1"/>
<connect gate="G$1" pin="PF3" pad="2"/>
<connect gate="G$1" pin="PF4" pad="3"/>
<connect gate="G$1" pin="PF5" pad="4"/>
<connect gate="G$1" pin="PF6" pad="5"/>
<connect gate="G$1" pin="PF7" pad="6"/>
<connect gate="G$1" pin="PG0" pad="14"/>
<connect gate="G$1" pin="PG1" pad="15"/>
<connect gate="G$1" pin="PG2" pad="16"/>
<connect gate="G$1" pin="PG3" pad="17"/>
<connect gate="G$1" pin="PG4" pad="18"/>
<connect gate="G$1" pin="PG5" pad="19"/>
<connect gate="G$1" pin="RFN" pad="9"/>
<connect gate="G$1" pin="RFP" pad="8"/>
<connect gate="G$1" pin="RSTN" pad="12"/>
<connect gate="G$1" pin="RSTON" pad="13"/>
<connect gate="G$1" pin="TST" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="57"/>
<connect gate="G$1" pin="XTAL2" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BALUN" prefix="B">
<gates>
<gate name="G$1" symbol="BALUN"/>
</gates>
<devices>
<device name="0805" package="BALUN">
<connects>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-4PDT">
<description>For use with a push-button switch made by CnK components. The Part # is</description>
<gates>
<gate name="G$1" symbol="SWITCH-4PDT"/>
</gates>
<devices>
<device name="CNK_LOCK" package="SWITCH-4PDT-CNK">
<connects>
<connect gate="G$1" pin="1" pad="PP$1"/>
<connect gate="G$1" pin="10" pad="PP$10"/>
<connect gate="G$1" pin="11" pad="PP$11"/>
<connect gate="G$1" pin="12" pad="PP$12"/>
<connect gate="G$1" pin="2" pad="PP$2"/>
<connect gate="G$1" pin="3" pad="PP$3"/>
<connect gate="G$1" pin="4" pad="PP$4"/>
<connect gate="G$1" pin="5" pad="PP$5"/>
<connect gate="G$1" pin="6" pad="PP$6"/>
<connect gate="G$1" pin="7" pad="PP$7"/>
<connect gate="G$1" pin="8" pad="PP$8"/>
<connect gate="G$1" pin="9" pad="PP$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADMP401">
<gates>
<gate name="G$1" symbol="ADMP401"/>
</gates>
<devices>
<device name="" package="ADMP401">
<connects>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MLX90614" prefix="U">
<description>Melexis IR Thermometer</description>
<gates>
<gate name="G$1" symbol="MLX90614"/>
</gates>
<devices>
<device name="_" package="TO-39">
<connects>
<connect gate="G$1" pin="PWM/SDA" pad="2"/>
<connect gate="G$1" pin="SCL/VZ" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PQ1CY1032Z">
<description>3.5A Switching Regulator</description>
<gates>
<gate name="G$1" symbol="PQ1CY1032Z"/>
</gates>
<devices>
<device name="" package="Q5-DD_SPX29300">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
<connect gate="G$1" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ256GP710" prefix="U">
<gates>
<gate name="G1" symbol="DSPIC33FJ256GP710_POWER"/>
<gate name="G2" symbol="DSPIC33FJ256GP710_CONTROL"/>
<gate name="G3" symbol="DSPIC33FJ256GP710_EXTERNAL"/>
<gate name="G4" symbol="DSPIC33FJ256GP710_EXTRA"/>
</gates>
<devices>
<device name="_" package="TQFP-100-12X12MM">
<connects>
<connect gate="G1" pin="AVDD" pad="30"/>
<connect gate="G1" pin="AVSS" pad="31"/>
<connect gate="G1" pin="RA10/VREF+" pad="29"/>
<connect gate="G1" pin="RA9/VREF-" pad="28"/>
<connect gate="G1" pin="VCAP" pad="85"/>
<connect gate="G1" pin="VDD@16" pad="16"/>
<connect gate="G1" pin="VDD@2" pad="2"/>
<connect gate="G1" pin="VDD@37" pad="37"/>
<connect gate="G1" pin="VDD@46" pad="46"/>
<connect gate="G1" pin="VDD@62" pad="62"/>
<connect gate="G1" pin="VDD@86" pad="86"/>
<connect gate="G1" pin="VSS@15" pad="15"/>
<connect gate="G1" pin="VSS@36" pad="36"/>
<connect gate="G1" pin="VSS@45" pad="45"/>
<connect gate="G1" pin="VSS@65" pad="65"/>
<connect gate="G1" pin="VSS@75" pad="75"/>
<connect gate="G2" pin="RA6/AN22" pad="91"/>
<connect gate="G2" pin="RB0/AN0" pad="25"/>
<connect gate="G2" pin="RB1/AN1" pad="24"/>
<connect gate="G2" pin="RB10/AN10" pad="34"/>
<connect gate="G2" pin="RB11/AN11" pad="35"/>
<connect gate="G2" pin="RB12/AN12" pad="41"/>
<connect gate="G2" pin="RB13/AN13" pad="42"/>
<connect gate="G2" pin="RB14/AN14" pad="43"/>
<connect gate="G2" pin="RB3/AN3" pad="22"/>
<connect gate="G2" pin="RB4/AN4" pad="21"/>
<connect gate="G2" pin="RB5/AN5" pad="20"/>
<connect gate="G2" pin="RB6/AN6" pad="26"/>
<connect gate="G2" pin="RB7/AN7" pad="27"/>
<connect gate="G2" pin="RB8/AN8" pad="32"/>
<connect gate="G2" pin="RB9/AN9" pad="33"/>
<connect gate="G2" pin="RC4/AN19" pad="9"/>
<connect gate="G2" pin="RD0/OC1" pad="72"/>
<connect gate="G2" pin="RD1/OC2" pad="76"/>
<connect gate="G2" pin="RD10/IC3" pad="70"/>
<connect gate="G2" pin="RD11/IC4" pad="71"/>
<connect gate="G2" pin="RD12/IC5" pad="79"/>
<connect gate="G2" pin="RD13/IC6" pad="80"/>
<connect gate="G2" pin="RD14/U1CTS/IC7" pad="47"/>
<connect gate="G2" pin="RD15/U1RTS/IC8" pad="48"/>
<connect gate="G2" pin="RD2/OC3" pad="77"/>
<connect gate="G2" pin="RD3/OC4" pad="78"/>
<connect gate="G2" pin="RD4/OC5" pad="81"/>
<connect gate="G2" pin="RD5/OC6" pad="82"/>
<connect gate="G2" pin="RD6/OC7" pad="83"/>
<connect gate="G2" pin="RD7/OC8" pad="84"/>
<connect gate="G2" pin="RD8/IC1" pad="68"/>
<connect gate="G2" pin="RD9/IC2" pad="69"/>
<connect gate="G2" pin="RE1/AN25" pad="94"/>
<connect gate="G2" pin="RE2" pad="98"/>
<connect gate="G2" pin="RE3" pad="99"/>
<connect gate="G2" pin="RE4" pad="100"/>
<connect gate="G2" pin="RF2/U1RX" pad="52"/>
<connect gate="G2" pin="RF3/U1TX" pad="51"/>
<connect gate="G2" pin="RG2/SCL1" pad="57"/>
<connect gate="G2" pin="RG3/SDA1" pad="56"/>
<connect gate="G3" pin="MCLR" pad="13"/>
<connect gate="G3" pin="RA1" pad="38"/>
<connect gate="G3" pin="RA12/INT1" pad="18"/>
<connect gate="G3" pin="RA13/INT2" pad="19"/>
<connect gate="G3" pin="RA14" pad="66"/>
<connect gate="G3" pin="RA2/SCL2" pad="58"/>
<connect gate="G3" pin="RA3/SDA2" pad="59"/>
<connect gate="G3" pin="RA4/TDI" pad="60"/>
<connect gate="G3" pin="RA5/TDO" pad="61"/>
<connect gate="G3" pin="RA7/AN23" pad="92"/>
<connect gate="G3" pin="RB15/AN15" pad="44"/>
<connect gate="G3" pin="RB2/SS1" pad="23"/>
<connect gate="G3" pin="RC1/AN16" pad="6"/>
<connect gate="G3" pin="RC13/PGED2" pad="73"/>
<connect gate="G3" pin="RC14/PGEC2" pad="74"/>
<connect gate="G3" pin="RC2/AN17" pad="7"/>
<connect gate="G3" pin="RC3/AN18" pad="8"/>
<connect gate="G3" pin="RE0/AN24" pad="93"/>
<connect gate="G3" pin="RF0/C1RX1" pad="87"/>
<connect gate="G3" pin="RF1/C1TX1" pad="88"/>
<connect gate="G3" pin="RF12/U2CTS" pad="40"/>
<connect gate="G3" pin="RF13/U2RTS" pad="39"/>
<connect gate="G3" pin="RF4/U2RX" pad="49"/>
<connect gate="G3" pin="RF5/U2TX" pad="50"/>
<connect gate="G3" pin="RF6/SCK1" pad="55"/>
<connect gate="G3" pin="RF7/SDI1" pad="54"/>
<connect gate="G3" pin="RF8/SDO1" pad="53"/>
<connect gate="G3" pin="RG6/SCK2" pad="10"/>
<connect gate="G3" pin="RG7/SDI2" pad="11"/>
<connect gate="G3" pin="RG8/SDO2" pad="12"/>
<connect gate="G3" pin="RG9/SS2" pad="14"/>
<connect gate="G4" pin="RA0/TMS" pad="17"/>
<connect gate="G4" pin="RA15" pad="67"/>
<connect gate="G4" pin="RC12/OSC1" pad="63"/>
<connect gate="G4" pin="RC15/OSC2" pad="64"/>
<connect gate="G4" pin="RE5/AN29" pad="3"/>
<connect gate="G4" pin="RE6/AN30" pad="4"/>
<connect gate="G4" pin="RE7/AN31" pad="5"/>
<connect gate="G4" pin="RG0/C2RX" pad="90"/>
<connect gate="G4" pin="RG1/C2TX" pad="89"/>
<connect gate="G4" pin="RG12/CSDI" pad="96"/>
<connect gate="G4" pin="RG13/CSDO" pad="97"/>
<connect gate="G4" pin="RG14/CSCK" pad="95"/>
<connect gate="G4" pin="RG15/COFS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZG2100M">
<gates>
<gate name="G$1" symbol="ZG2100M"/>
</gates>
<devices>
<device name="" package="ZG2100M">
<connects>
<connect gate="G$1" pin="CE_N" pad="20"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GND3" pad="18"/>
<connect gate="G$1" pin="GND4" pad="19"/>
<connect gate="G$1" pin="GND5" pad="36"/>
<connect gate="G$1" pin="GND6" pad="25"/>
<connect gate="G$1" pin="GND7" pad="28"/>
<connect gate="G$1" pin="GND8" pad="30"/>
<connect gate="G$1" pin="INT_NX" pad="33"/>
<connect gate="G$1" pin="JTAG_EN" pad="21"/>
<connect gate="G$1" pin="JTAG_RST_N" pad="9"/>
<connect gate="G$1" pin="JTAG_TCK" pad="4"/>
<connect gate="G$1" pin="JTAG_TDI" pad="6"/>
<connect gate="G$1" pin="JTAG_TDO" pad="3"/>
<connect gate="G$1" pin="JTAG_TMS" pad="5"/>
<connect gate="G$1" pin="NC1" pad="8"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="13"/>
<connect gate="G$1" pin="NC4" pad="14"/>
<connect gate="G$1" pin="NC5" pad="15"/>
<connect gate="G$1" pin="NC6" pad="22"/>
<connect gate="G$1" pin="RES" pad="16"/>
<connect gate="G$1" pin="RST_N" pad="7"/>
<connect gate="G$1" pin="SCK" pad="34"/>
<connect gate="G$1" pin="SCS_N" pad="23"/>
<connect gate="G$1" pin="SDI" pad="35"/>
<connect gate="G$1" pin="SDO" pad="32"/>
<connect gate="G$1" pin="UART_RX" pad="26"/>
<connect gate="G$1" pin="UART_TX" pad="27"/>
<connect gate="G$1" pin="VDD_1.8_1" pad="2"/>
<connect gate="G$1" pin="VDD_1.8_2" pad="11"/>
<connect gate="G$1" pin="VDD_1.8_3" pad="24"/>
<connect gate="G$1" pin="VDD_1.8_4" pad="31"/>
<connect gate="G$1" pin="VDD_3.3_1" pad="17"/>
<connect gate="G$1" pin="VDD_3.3_2" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOC3031-M">
<gates>
<gate name="G$1" symbol="MOC3031-M"/>
</gates>
<devices>
<device name="" package="DIL06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OBDII">
<gates>
<gate name="G$1" symbol="OBDII"/>
</gates>
<devices>
<device name="" package="OBDII">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="BATTPOWER" pad="16"/>
<connect gate="G$1" pin="CANHIGH" pad="6"/>
<connect gate="G$1" pin="CANLOW" pad="14"/>
<connect gate="G$1" pin="CHASGND" pad="4"/>
<connect gate="G$1" pin="ISOK-LINE" pad="7"/>
<connect gate="G$1" pin="ISOL-LINE" pad="15"/>
<connect gate="G$1" pin="J1850BUS" pad="10"/>
<connect gate="G$1" pin="J1850BUS+" pad="2"/>
<connect gate="G$1" pin="SIGGND" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PSP_CONNECTOR">
<gates>
<gate name="G$1" symbol="PSP_CONNECTOR"/>
</gates>
<devices>
<device name="" package="PSP_CONNECTOR">
<connects>
<connect gate="G$1" pin="AVDD" pad="AVDD"/>
<connect gate="G$1" pin="AVDD2" pad="AVDD2"/>
<connect gate="G$1" pin="B0" pad="B0"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="CK" pad="CK"/>
<connect gate="G$1" pin="DISP" pad="DISP"/>
<connect gate="G$1" pin="G0" pad="G0"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="G3" pad="G3"/>
<connect gate="G$1" pin="G4" pad="G4"/>
<connect gate="G$1" pin="G5" pad="G5"/>
<connect gate="G$1" pin="G6" pad="G6"/>
<connect gate="G$1" pin="G7" pad="G7"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="HSYNC" pad="HSYNC"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="R0" pad="R0"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="R3" pad="R3"/>
<connect gate="G$1" pin="R4" pad="R4"/>
<connect gate="G$1" pin="R5" pad="R5"/>
<connect gate="G$1" pin="R6" pad="R6"/>
<connect gate="G$1" pin="R7" pad="R7"/>
<connect gate="G$1" pin="TEST1" pad="TEST1"/>
<connect gate="G$1" pin="TEST2" pad="TEST2"/>
<connect gate="G$1" pin="TEST3" pad="TEST3"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC2" pad="VCC2"/>
<connect gate="G$1" pin="VSYNC" pad="VSYNC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3588" prefix="U">
<description>LTC3588 Energy Harvesting Power Supply</description>
<gates>
<gate name="G$1" symbol="LTC3588"/>
</gates>
<devices>
<device name="_" package="MSOP-10-GNDPAD">
<connects>
<connect gate="G$1" pin="CAP" pad="3"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PGOOD" pad="10"/>
<connect gate="G$1" pin="PZ1" pad="1"/>
<connect gate="G$1" pin="PZ2" pad="2"/>
<connect gate="G$1" pin="SW" pad="5"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VIN2" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLAR-IXYS" prefix="D">
<gates>
<gate name="G$1" symbol="SOLARCELL_SINGLE"/>
</gates>
<devices>
<device name="_" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="C" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-" package="SOLARBIT-12X1">
<connects>
<connect gate="G$1" pin="A" pad="+"/>
<connect gate="G$1" pin="C" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-SCHOTTKY" prefix="D">
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="_" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITG-3200" prefix="U">
<description>ITG-3200 3-axis gyro, digital output, qfn24 package</description>
<gates>
<gate name="G$1" symbol="ITG-3200"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="RESV-G" pad="11"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VLOGIC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREENKEY-TFT128">
<gates>
<gate name="G$1" symbol="SCREENKEY-TFT128"/>
</gates>
<devices>
<device name="DEMENSIONANDHOLES" package="SCREENKEY-TFT128">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA-A3">
<description>Atmel's 8/16-bit AVR XMEGA A3 Microcontroller - ATxmega256A3, etc.</description>
<gates>
<gate name="G$1" symbol="XMEGA-A3B"/>
</gates>
<devices>
<device name="-AU" package="TQFP64_14X14MM">
<connects>
<connect gate="G$1" pin="/RESET_PDI_CLK" pad="57"/>
<connect gate="G$1" pin="AGND" pad="60"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND1" pad="14"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="GND3" pad="34"/>
<connect gate="G$1" pin="GND4" pad="44"/>
<connect gate="G$1" pin="GND5" pad="52"/>
<connect gate="G$1" pin="PA0(ADC0/AC0/AREF)" pad="62"/>
<connect gate="G$1" pin="PA1(ADC1/AC1)" pad="63"/>
<connect gate="G$1" pin="PA2(ADC2/AC2)" pad="64"/>
<connect gate="G$1" pin="PA3(ADC3/AC3)" pad="1"/>
<connect gate="G$1" pin="PA4(ADC4/AC4)" pad="2"/>
<connect gate="G$1" pin="PA5(ADC5/AC5)" pad="3"/>
<connect gate="G$1" pin="PA6(ADC6/AC6)" pad="4"/>
<connect gate="G$1" pin="PA7(ADC7/AC7/AC0OUT)" pad="5"/>
<connect gate="G$1" pin="PB0(ADC0/AC0/AREF)" pad="6"/>
<connect gate="G$1" pin="PB1(ADC1/AC1)" pad="7"/>
<connect gate="G$1" pin="PB2(ADC2/AC2/DAC0)" pad="8"/>
<connect gate="G$1" pin="PB3(ADC3/AC3/DAC1)" pad="9"/>
<connect gate="G$1" pin="PB4(ADC4/AC4/TMS)" pad="10"/>
<connect gate="G$1" pin="PB5(ADC5/AC5/TDI)" pad="11"/>
<connect gate="G$1" pin="PB6(ADC6/AC6/TCK)" pad="12"/>
<connect gate="G$1" pin="PB7(ADC7/AC7/AC0OUT/TDO)" pad="13"/>
<connect gate="G$1" pin="PC0(OC0A/OC0AL/SDA)" pad="16"/>
<connect gate="G$1" pin="PC1(OC0B/AC0AH/XCK0/SCL)" pad="17"/>
<connect gate="G$1" pin="PC2(OC0C/OC0BL/RXD0)" pad="18"/>
<connect gate="G$1" pin="PC3(OC0D/OX0BH/TXD0)" pad="19"/>
<connect gate="G$1" pin="PC4(AC1A/OC0CL/SS)" pad="20"/>
<connect gate="G$1" pin="PC5(OC1B/OC0CH/XCK1/MOSI)" pad="21"/>
<connect gate="G$1" pin="PC6(OC0DL/RXD1/MISO)" pad="22"/>
<connect gate="G$1" pin="PC7(OC0DH/CKOUT/EVO/TXD1/SCK)" pad="23"/>
<connect gate="G$1" pin="PD0(OC0A)" pad="26"/>
<connect gate="G$1" pin="PD1(OC0B/XCK0)" pad="27"/>
<connect gate="G$1" pin="PD2(OC0C/RXD0)" pad="28"/>
<connect gate="G$1" pin="PD3(OX0D/TXD0)" pad="29"/>
<connect gate="G$1" pin="PD4(OC1A/SS)" pad="30"/>
<connect gate="G$1" pin="PD5(OC1B/XCK1/MOSI)" pad="31"/>
<connect gate="G$1" pin="PD6(RXD1/MISO)" pad="32"/>
<connect gate="G$1" pin="PD7(CKOUT/EVO/TXD1/SCK)" pad="33"/>
<connect gate="G$1" pin="PDI_DATA" pad="56"/>
<connect gate="G$1" pin="PE0(OC0A/SDA)" pad="36"/>
<connect gate="G$1" pin="PE1(OC0B/XCK0/SCL)" pad="37"/>
<connect gate="G$1" pin="PE2(OC0C/RXD0)" pad="38"/>
<connect gate="G$1" pin="PE3(OC0D/TXD0)" pad="39"/>
<connect gate="G$1" pin="PE4(OC1A/SS)" pad="40"/>
<connect gate="G$1" pin="PE5(OC1B/XCK1/MOSI)" pad="41"/>
<connect gate="G$1" pin="PE6(TOSC2/RXD1/MISO)" pad="42"/>
<connect gate="G$1" pin="PE7(TOSC1/CKOUT/EVO/TXD1/SCK)" pad="43"/>
<connect gate="G$1" pin="PF0(OC0A)" pad="46"/>
<connect gate="G$1" pin="PF1(OC0B/XCK0)" pad="47"/>
<connect gate="G$1" pin="PF2(OC0C/RXD0)" pad="48"/>
<connect gate="G$1" pin="PF3(OC0D/TXD0)" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0(XTAL2)" pad="58"/>
<connect gate="G$1" pin="PR1(XTAL1)" pad="59"/>
<connect gate="G$1" pin="VCC1" pad="15"/>
<connect gate="G$1" pin="VCC2" pad="25"/>
<connect gate="G$1" pin="VCC3" pad="35"/>
<connect gate="G$1" pin="VCC4" pad="45"/>
<connect gate="G$1" pin="VCC5" pad="53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_MIC2920">
<description>MIC2920A (http://www.micrel.com/_PDF/mic2920.pdf) - 400mA output LDO Regulator</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZXLD1360">
<description>Adjustable constant current switching driver for high-power LEDs</description>
<gates>
<gate name="G$1" symbol="ZXLD1360"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="LX" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="4"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADNS2610" prefix="U">
<gates>
<gate name="G$1" symbol="ADNS2610"/>
</gates>
<devices>
<device name="PTH" package="ADNS2610">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LED_CNTL" pad="5"/>
<connect gate="G$1" pin="OSC_IN" pad="1"/>
<connect gate="G$1" pin="OSC_OUT" pad="2"/>
<connect gate="G$1" pin="REFA" pad="8"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SDIO" pad="3"/>
<connect gate="G$1" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUP500F" prefix="U">
<description>SUP500F Venus GPS</description>
<gates>
<gate name="G$1" symbol="SUP500F"/>
</gates>
<devices>
<device name="" package="SUP500F">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PPS" pad="6"/>
<connect gate="G$1" pin="PSEL" pad="7"/>
<connect gate="G$1" pin="RX-I" pad="1"/>
<connect gate="G$1" pin="TX-O" pad="2"/>
<connect gate="G$1" pin="VBAT" pad="5"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADMP421">
<gates>
<gate name="G$1" symbol="ADMP421"/>
</gates>
<devices>
<device name="" package="ADMP421">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DATA" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="L/R" pad="2"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-EAGLE-RULES">
<description>&lt;b&gt;Description:&lt;/b&gt; These are the default rules that SparkFun engineers must follow. We highly recommend following these rules as well.</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-EAGLE-RULES"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-3" prefix="JP">
<gates>
<gate name="G$1" symbol="JUMPER-3"/>
</gates>
<devices>
<device name="SMD" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1-2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2-3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER" prefix="SJ">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
Standard SMD solder jumper. Used to automate production. Two varients : Normally Open and Normally Closed are the same, but have different paste layers. NC will have a large amount of paste and should jumper during reflow.</description>
<gates>
<gate name="1" symbol="SJ"/>
</gates>
<devices>
<device name="NC" package="SJ_2S">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE" package="SJ_2S-TRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NC2" package="SJ_2S-NOTRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO" package="SJ_2S-NO">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_2WAY" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
2 way solder jumper</description>
<gates>
<gate name="G$1" symbol="SJ_2"/>
</gates>
<devices>
<device name="W" package="SJ_2W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SJ_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE2&amp;3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*157" prefix="IC">
<description>Quadruple 2-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74157"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!A!/B" pad="2"/>
<connect gate="A" pin="1A" pad="3"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1Y" pad="5"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="4A" pad="18"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4Y" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="SO" package="SO016">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MLX90121" prefix="U">
<description>MLX90121 13.56MHz RFID Transceiver</description>
<gates>
<gate name="G$1" symbol="MLX90121"/>
</gates>
<devices>
<device name="_" package="SSOP20">
<connects>
<connect gate="G$1" pin="CK" pad="15"/>
<connect gate="G$1" pin="DIN" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="11"/>
<connect gate="G$1" pin="DSYC" pad="16"/>
<connect gate="G$1" pin="MOD" pad="3"/>
<connect gate="G$1" pin="MODE" pad="14"/>
<connect gate="G$1" pin="RES1" pad="9"/>
<connect gate="G$1" pin="RES2(DNC)" pad="18"/>
<connect gate="G$1" pin="RTB" pad="10"/>
<connect gate="G$1" pin="RX" pad="20"/>
<connect gate="G$1" pin="TX" pad="2"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="12"/>
<connect gate="G$1" pin="VDD3" pad="17"/>
<connect gate="G$1" pin="VSS1" pad="4"/>
<connect gate="G$1" pin="VSS2" pad="7"/>
<connect gate="G$1" pin="VSS3" pad="19"/>
<connect gate="G$1" pin="XBUF" pad="8"/>
<connect gate="G$1" pin="XIN" pad="6"/>
<connect gate="G$1" pin="XOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RQ">
<description>Non-stock item, unproven FP for this part.</description>
<gates>
<gate name="G$1" symbol="FT232RQ"/>
</gates>
<devices>
<device name="" package="QFN-32">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="16"/>
<connect gate="G$1" pin="AGND" pad="24"/>
<connect gate="G$1" pin="CTS" pad="8"/>
<connect gate="G$1" pin="DCD" pad="7"/>
<connect gate="G$1" pin="DSR" pad="6"/>
<connect gate="G$1" pin="DTR" pad="31"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWREN" pad="11"/>
<connect gate="G$1" pin="RESET" pad="18"/>
<connect gate="G$1" pin="RI" pad="3"/>
<connect gate="G$1" pin="RTS" pad="32"/>
<connect gate="G$1" pin="RXD" pad="2"/>
<connect gate="G$1" pin="RXLED" pad="21"/>
<connect gate="G$1" pin="SLEEP" pad="9"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="30"/>
<connect gate="G$1" pin="TXDEN" pad="10"/>
<connect gate="G$1" pin="TXLED" pad="22"/>
<connect gate="G$1" pin="USBDM" pad="15"/>
<connect gate="G$1" pin="USBDP" pad="14"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VCCIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FB">
<gates>
<gate name="G$1" symbol="FB"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M40">
<gates>
<gate name="G$1" symbol="M40"/>
</gates>
<devices>
<device name="OFFSET" package="1X40_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC4052">
<gates>
<gate name="G$1" symbol="74HC4052"/>
</gates>
<devices>
<device name="SO" package="SO16">
<connects>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="X" pad="13"/>
<connect gate="G$1" pin="X0" pad="12"/>
<connect gate="G$1" pin="X1" pad="14"/>
<connect gate="G$1" pin="X2" pad="15"/>
<connect gate="G$1" pin="X3" pad="11"/>
<connect gate="G$1" pin="Y" pad="3"/>
<connect gate="G$1" pin="Y0" pad="1"/>
<connect gate="G$1" pin="Y1" pad="5"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP" package="DIL16">
<connects>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="X" pad="13"/>
<connect gate="G$1" pin="X0" pad="12"/>
<connect gate="G$1" pin="X1" pad="14"/>
<connect gate="G$1" pin="X2" pad="15"/>
<connect gate="G$1" pin="X3" pad="11"/>
<connect gate="G$1" pin="Y" pad="3"/>
<connect gate="G$1" pin="Y0" pad="1"/>
<connect gate="G$1" pin="Y1" pad="5"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_ADJ" prefix="C">
<description>Variable, non-polarized capacitor</description>
<gates>
<gate name="G$1" symbol="CAP_ADJ"/>
</gates>
<devices>
<device name="SMD" package="CTZ3">
<connects>
<connect gate="G$1" pin="3" pad="+"/>
<connect gate="G$1" pin="4" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD45DB161D">
<gates>
<gate name="G$1" symbol="AT45DB161D"/>
</gates>
<devices>
<device name="" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB161D">
<gates>
<gate name="G$1" symbol="AT45DB161D"/>
</gates>
<devices>
<device name="" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MINI">
<gates>
<gate name="G$1" symbol="ARDUINO_MINI"/>
</gates>
<devices>
<device name="" package="ARDUINO_MINI">
<connects>
<connect gate="G$1" pin="10" pad="13"/>
<connect gate="G$1" pin="11" pad="14"/>
<connect gate="G$1" pin="12" pad="15"/>
<connect gate="G$1" pin="13" pad="16"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="12"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="A2" pad="19"/>
<connect gate="G$1" pin="A3" pad="20"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND2" pad="23"/>
<connect gate="G$1" pin="RAW" pad="24"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="RST2" pad="22"/>
<connect gate="G$1" pin="RX1" pad="2"/>
<connect gate="G$1" pin="TX0" pad="1"/>
<connect gate="G$1" pin="VCC" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-MINIB">
<description>&lt;b&gt;Mini-USB "B" connector with 5th pin broken out.&lt;/b&gt;&lt;p&gt;
Created new symbol breaking out 5th "ID" pin in mini/micro USB connector spec.  See: http://en.wikipedia.org/wiki/Mini_usb#Cables.  Uses same footprint as 4-pin symbol.&lt;p&gt;
 

Also added pins to connect to mounting / shield pads if required (probably not generally needed as signals aren't shielded once they leave the connector).</description>
<gates>
<gate name="G$1" symbol="USB-5PIN"/>
</gates>
<devices>
<device name="-5PIN" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="MTN1" pad="MTN3"/>
<connect gate="G$1" pin="MTN2" pad="MTN1"/>
<connect gate="G$1" pin="MTN3" pad="MTN2"/>
<connect gate="G$1" pin="MTN4" pad="MTN4"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTM182" prefix="U">
<description>BTM-182 Bluetooth Module from Rayson</description>
<gates>
<gate name="G$1" symbol="BTM182"/>
</gates>
<devices>
<device name="_" package="BTM182">
<connects>
<connect gate="G$1" pin="AIO0" pad="2"/>
<connect gate="G$1" pin="AIO1" pad="3"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="PCM_CLK" pad="5"/>
<connect gate="G$1" pin="PCM_IN" pad="7"/>
<connect gate="G$1" pin="PCM_OUT" pad="4"/>
<connect gate="G$1" pin="PCM_SYNC" pad="6"/>
<connect gate="G$1" pin="PIO0" pad="31"/>
<connect gate="G$1" pin="PIO1" pad="32"/>
<connect gate="G$1" pin="PIO10" pad="30"/>
<connect gate="G$1" pin="PIO11" pad="1"/>
<connect gate="G$1" pin="PIO2" pad="27"/>
<connect gate="G$1" pin="PIO3" pad="26"/>
<connect gate="G$1" pin="PIO4" pad="25"/>
<connect gate="G$1" pin="PIO5" pad="24"/>
<connect gate="G$1" pin="PIO6" pad="23"/>
<connect gate="G$1" pin="PIO7" pad="22"/>
<connect gate="G$1" pin="PIO8" pad="28"/>
<connect gate="G$1" pin="PIO9" pad="29"/>
<connect gate="G$1" pin="RESET" pad="21"/>
<connect gate="G$1" pin="SPI_CLK" pad="20"/>
<connect gate="G$1" pin="SPI_CSB" pad="18"/>
<connect gate="G$1" pin="SPI_MISO" pad="19"/>
<connect gate="G$1" pin="SPI_MOSI" pad="17"/>
<connect gate="G$1" pin="UART_CTS" pad="8"/>
<connect gate="G$1" pin="UART_RTS" pad="11"/>
<connect gate="G$1" pin="UART_RX" pad="10"/>
<connect gate="G$1" pin="UART_TX" pad="9"/>
<connect gate="G$1" pin="USB_DN" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="12"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDD_USB" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-PIN-CENTRONICS-F">
<gates>
<gate name="G$1" symbol="50-PIN-CENTRONICS"/>
</gates>
<devices>
<device name="FEMALE" package="50-PIN-CENTRONICS-F">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$16" pad="P$16"/>
<connect gate="G$1" pin="P$17" pad="P$17"/>
<connect gate="G$1" pin="P$18" pad="P$18"/>
<connect gate="G$1" pin="P$19" pad="P$19"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$20" pad="P$20"/>
<connect gate="G$1" pin="P$21" pad="P$21"/>
<connect gate="G$1" pin="P$22" pad="P$22"/>
<connect gate="G$1" pin="P$23" pad="P$23"/>
<connect gate="G$1" pin="P$24" pad="P$24"/>
<connect gate="G$1" pin="P$25" pad="P$25"/>
<connect gate="G$1" pin="P$26" pad="P$26"/>
<connect gate="G$1" pin="P$27" pad="P$27"/>
<connect gate="G$1" pin="P$28" pad="P$28"/>
<connect gate="G$1" pin="P$29" pad="P$29"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$30" pad="P$30"/>
<connect gate="G$1" pin="P$31" pad="P$31"/>
<connect gate="G$1" pin="P$32" pad="P$32"/>
<connect gate="G$1" pin="P$33" pad="P$33"/>
<connect gate="G$1" pin="P$34" pad="P$34"/>
<connect gate="G$1" pin="P$35" pad="P$35"/>
<connect gate="G$1" pin="P$36" pad="P$36"/>
<connect gate="G$1" pin="P$37" pad="P$37"/>
<connect gate="G$1" pin="P$38" pad="P$38"/>
<connect gate="G$1" pin="P$39" pad="P$39"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$40" pad="P$40"/>
<connect gate="G$1" pin="P$41" pad="P$41"/>
<connect gate="G$1" pin="P$42" pad="P$42"/>
<connect gate="G$1" pin="P$43" pad="P$43"/>
<connect gate="G$1" pin="P$44" pad="P$44"/>
<connect gate="G$1" pin="P$45" pad="P$45"/>
<connect gate="G$1" pin="P$46" pad="P$46"/>
<connect gate="G$1" pin="P$47" pad="P$47"/>
<connect gate="G$1" pin="P$48" pad="P$48"/>
<connect gate="G$1" pin="P$49" pad="P$49"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$50" pad="P$50"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-PIN-CENTRONICS-M">
<gates>
<gate name="G$1" symbol="50-PIN-CENTRONICS"/>
</gates>
<devices>
<device name="MALE" package="50-PIN-CENTRONICS-M">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$16" pad="P$16"/>
<connect gate="G$1" pin="P$17" pad="P$17"/>
<connect gate="G$1" pin="P$18" pad="P$18"/>
<connect gate="G$1" pin="P$19" pad="P$19"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$20" pad="P$20"/>
<connect gate="G$1" pin="P$21" pad="P$21"/>
<connect gate="G$1" pin="P$22" pad="P$22"/>
<connect gate="G$1" pin="P$23" pad="P$23"/>
<connect gate="G$1" pin="P$24" pad="P$24"/>
<connect gate="G$1" pin="P$25" pad="P$25"/>
<connect gate="G$1" pin="P$26" pad="P$26"/>
<connect gate="G$1" pin="P$27" pad="P$27"/>
<connect gate="G$1" pin="P$28" pad="P$28"/>
<connect gate="G$1" pin="P$29" pad="P$29"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$30" pad="P$30"/>
<connect gate="G$1" pin="P$31" pad="P$31"/>
<connect gate="G$1" pin="P$32" pad="P$32"/>
<connect gate="G$1" pin="P$33" pad="P$33"/>
<connect gate="G$1" pin="P$34" pad="P$34"/>
<connect gate="G$1" pin="P$35" pad="P$35"/>
<connect gate="G$1" pin="P$36" pad="P$36"/>
<connect gate="G$1" pin="P$37" pad="P$37"/>
<connect gate="G$1" pin="P$38" pad="P$38"/>
<connect gate="G$1" pin="P$39" pad="P$39"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$40" pad="P$40"/>
<connect gate="G$1" pin="P$41" pad="P$41"/>
<connect gate="G$1" pin="P$42" pad="P$42"/>
<connect gate="G$1" pin="P$43" pad="P$43"/>
<connect gate="G$1" pin="P$44" pad="P$44"/>
<connect gate="G$1" pin="P$45" pad="P$45"/>
<connect gate="G$1" pin="P$46" pad="P$46"/>
<connect gate="G$1" pin="P$47" pad="P$47"/>
<connect gate="G$1" pin="P$48" pad="P$48"/>
<connect gate="G$1" pin="P$49" pad="P$49"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$50" pad="P$50"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QRB1114" prefix="Q">
<description>&lt;b&gt;PHOTOTRANSISTOR REFLECTIVE OBJECT SENSOR&lt;/b&gt;
&lt;p&gt;
The QRB1113/1114 consists of an infrared emitting diode and an NPN silicon phototransistor mounted side by side on a converging
optical axis in a black plastic housing. The phototransistor responds to radiation from the emitting diode only when a reflective
object passes within its field of view. The area of the optimum response approximates a circle .200" in diameter.
&lt;p&gt;Datasheet: http://www.sparkfun.com/datasheets/Sensors/QRB1114.pdf
&lt;p&gt;MAX RATINGS:
&lt;p&gt;EMITTER
&lt;br&gt;Continuous Forward Current (IF) 50 mA
&lt;br&gt;Reverse Voltage (VR) 5 V
&lt;br&gt;Power Dissipation (PD) 100 mW
&lt;p&gt;SENSOR
&lt;br&gt;Collector-Emitter Voltage (VCEO) 30 V
&lt;br&gt;Emitter-Collector Voltage (VECO) 4.5 V
&lt;br&gt;Collector Current 20 mA
&lt;br&gt;Power Dissipation (PD) 100 mW</description>
<gates>
<gate name="G$1" symbol="QRE1113"/>
</gates>
<devices>
<device name="" package="QRB1114-SIDE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="K" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF-LINK_TX">
<gates>
<gate name="G$1" symbol="RF-LINK_TX"/>
</gates>
<devices>
<device name="" package="RF-LINK_TX">
<connects>
<connect gate="G$1" pin="+5V" pad="VCC"/>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF-LINK_RX">
<gates>
<gate name="G$1" symbol="RF-LINK_RX"/>
</gates>
<devices>
<device name="" package="RF-LINK_RX">
<connects>
<connect gate="G$1" pin="+5V" pad="+5V@1"/>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA" pad="DATA@1"/>
<connect gate="G$1" pin="GND" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI_BASIC" prefix="JP">
<description>FTDI Basic: 3.3V and 5V</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="PTH" package="FTDI_BASIC">
<connects>
<connect gate="G$1" pin="1" pad="DTR"/>
<connect gate="G$1" pin="2" pad="RXI"/>
<connect gate="G$1" pin="3" pad="TXO"/>
<connect gate="G$1" pin="4" pad="VCC"/>
<connect gate="G$1" pin="5" pad="CTS"/>
<connect gate="G$1" pin="6" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNH2SP30">
<gates>
<gate name="G$1" symbol="VNH2SP30"/>
</gates>
<devices>
<device name="" package="VNH2SP30">
<connects>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="EN/DIAA" pad="6"/>
<connect gate="G$1" pin="EN/DIAB" pad="10"/>
<connect gate="G$1" pin="GNDA@26" pad="26"/>
<connect gate="G$1" pin="GNDA@27" pad="27"/>
<connect gate="G$1" pin="GNDA@28" pad="28"/>
<connect gate="G$1" pin="GNDB@18" pad="18"/>
<connect gate="G$1" pin="GNDB@19" pad="19"/>
<connect gate="G$1" pin="GNDB@20" pad="20"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="11"/>
<connect gate="G$1" pin="OUTA@1" pad="1"/>
<connect gate="G$1" pin="OUTA@25" pad="25"/>
<connect gate="G$1" pin="OUTA@30" pad="30"/>
<connect gate="G$1" pin="OUTA@SLUG3" pad="SLUG3"/>
<connect gate="G$1" pin="OUTB@15" pad="15"/>
<connect gate="G$1" pin="OUTB@16" pad="16"/>
<connect gate="G$1" pin="OUTB@21" pad="21"/>
<connect gate="G$1" pin="OUTB@SLUG2" pad="SLUG2"/>
<connect gate="G$1" pin="PWM" pad="8"/>
<connect gate="G$1" pin="VCC@13" pad="13"/>
<connect gate="G$1" pin="VCC@23" pad="23"/>
<connect gate="G$1" pin="VCC@3" pad="3"/>
<connect gate="G$1" pin="VCC@SLUG1" pad="SLUG1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ALPHANUMERIC" prefix="U">
<description>&lt;b&gt;Alphanumeric LED Display&lt;/b&gt; Common anode. Multiple LEDs on some segments. Multiple LED colors available. Works great with A6282 driver IC. Decimal points are unfornately not connected. SKU: COM-09933.</description>
<gates>
<gate name="G$1" symbol="ALPHANUMERIC"/>
</gates>
<devices>
<device name="PTH" package="ALPHANUMERIC">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="22"/>
<connect gate="G$1" pin="B" pad="21"/>
<connect gate="G$1" pin="C" pad="16"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="14"/>
<connect gate="G$1" pin="E" pad="9"/>
<connect gate="G$1" pin="F" pad="4"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="19"/>
<connect gate="G$1" pin="H" pad="3"/>
<connect gate="G$1" pin="J" pad="24"/>
<connect gate="G$1" pin="K" pad="23"/>
<connect gate="G$1" pin="L" pad="15"/>
<connect gate="G$1" pin="M" pad="12"/>
<connect gate="G$1" pin="N" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@13" pad="13"/>
<connect gate="G$1" pin="VCC@18" pad="18"/>
<connect gate="G$1" pin="VCC@6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STP16CP05">
<gates>
<gate name="G$1" symbol="STP16CP05/A6282"/>
</gates>
<devices>
<device name="" package="SO-24DW">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LE" pad="4"/>
<connect gate="G$1" pin="OUT0" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT10" pad="15"/>
<connect gate="G$1" pin="OUT11" pad="16"/>
<connect gate="G$1" pin="OUT12" pad="17"/>
<connect gate="G$1" pin="OUT13" pad="18"/>
<connect gate="G$1" pin="OUT14" pad="19"/>
<connect gate="G$1" pin="OUT15" pad="20"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="9"/>
<connect gate="G$1" pin="OUT5" pad="10"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="12"/>
<connect gate="G$1" pin="OUT8" pad="13"/>
<connect gate="G$1" pin="OUT9" pad="14"/>
<connect gate="G$1" pin="REXT" pad="23"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="22"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="~OE" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LS20126" prefix="U">
<description>&lt;h3&gt; LS20126 20-Channel GPS Module&lt;/h3&gt;&lt;br&gt;
SparkFun SKU# &lt;b&gt;GPS-09838&lt;/b&gt;&lt;br&gt;
The LOCOSYS LS20126 GPS smart antenna module is a high sensitivity, low power, SMD type, 20 channels with built-in magnetic sensor, 3-axial acceleration sensor L1 GPS receiver and 10mm patch antenna designed for portable applications.</description>
<gates>
<gate name="G$1" symbol="LS20126"/>
</gates>
<devices>
<device name="" package="LS20126">
<connects>
<connect gate="G$1" pin="BOOTSL" pad="6"/>
<connect gate="G$1" pin="EN" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="10"/>
<connect gate="G$1" pin="GPIO" pad="5"/>
<connect gate="G$1" pin="RX" pad="4"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSTBY" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADM1087">
<gates>
<gate name="G$1" symbol="ADM1087"/>
</gates>
<devices>
<device name="SC-70" package="SC-70">
<connects>
<connect gate="G$1" pin="CEXT" pad="5"/>
<connect gate="G$1" pin="ENIN" pad="1"/>
<connect gate="G$1" pin="ENOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24022" prefix="U">
<description>&lt;h3&gt;TI BQ24022&lt;/h3&gt;
 Single-chip, Li-ion and Li-pol charger IC with autonomous USB-port and AC-adapter supply management.&lt;br&gt;
Datasheet: http://focus.ti.com/lit/ds/symlink/bq24022.pdf&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Unproven&lt;/b&gt;&lt;br&gt;
Last modified: 8/16/10&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="BQ24022"/>
</gates>
<devices>
<device name="" package="DRC-10">
<connects>
<connect gate="G$1" pin="AC" pad="1"/>
<connect gate="G$1" pin="ETP" pad="EP"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISET1" pad="6"/>
<connect gate="G$1" pin="ISET2" pad="7"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="STAT2" pad="4"/>
<connect gate="G$1" pin="USB" pad="2"/>
<connect gate="G$1" pin="~CE" pad="9"/>
<connect gate="G$1" pin="~PG" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73833" prefix="U">
<description>&lt;h3&gt;Microchip MCP73833&lt;/h3&gt;
Stand-alone Linear Li-ion/Li-polymer Charge Management Controller&lt;br&gt;
Packages: DFN-10, MSOP-10&lt;br&gt;
&lt;br&gt;
Last modified: 8/17/10&lt;br&gt;
&lt;b&gt;Unproven!&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MCP73833"/>
</gates>
<devices>
<device name="" package="MSOP-10">
<connects>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="STAT2" pad="4"/>
<connect gate="G$1" pin="THERM" pad="8"/>
<connect gate="G$1" pin="VBAT@1" pad="9"/>
<connect gate="G$1" pin="VBAT@2" pad="10"/>
<connect gate="G$1" pin="VDD@1" pad="1"/>
<connect gate="G$1" pin="VDD@2" pad="2"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="~PG" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8397-EPAD" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+--1"/>
<gate name="B" symbol="OP-AMP-1"/>
</gates>
<devices>
<device name="EPAD" package="SO08-EPAD">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="EPAD" pad="EPAD"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI1120">
<description>Si1120: Proximity/Ambient Light Sensor</description>
<gates>
<gate name="G$1" symbol="SI1120"/>
</gates>
<devices>
<device name="" package="ODFN">
<connects>
<connect gate="G$1" pin="MD" pad="7"/>
<connect gate="G$1" pin="PRX" pad="1"/>
<connect gate="G$1" pin="SC" pad="6"/>
<connect gate="G$1" pin="STX" pad="4"/>
<connect gate="G$1" pin="TXGD" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A6282" prefix="U">
<description>&lt;h3&gt;Allegro A6282&lt;/h3&gt;
16-Channel Constant-Current LED Driver&lt;br&gt;
Packages: TSSOP-24, 24-pin QFN&lt;br&gt;
&lt;br&gt;
Last modified: 8/20/10&lt;br&gt;
&lt;B&gt;Unproven!&lt;/b&gt;&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="A6282"/>
</gates>
<devices>
<device name="-LP" package="TSSOP-24">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="EP"/>
<connect gate="G$1" pin="LE" pad="4"/>
<connect gate="G$1" pin="OUT0" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT10" pad="15"/>
<connect gate="G$1" pin="OUT11" pad="16"/>
<connect gate="G$1" pin="OUT12" pad="17"/>
<connect gate="G$1" pin="OUT13" pad="18"/>
<connect gate="G$1" pin="OUT14" pad="19"/>
<connect gate="G$1" pin="OUT15" pad="20"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="9"/>
<connect gate="G$1" pin="OUT5" pad="10"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="12"/>
<connect gate="G$1" pin="OUT8" pad="13"/>
<connect gate="G$1" pin="OUT9" pad="14"/>
<connect gate="G$1" pin="REXT" pad="23"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="22"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="~OE" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ES" package="QFN-24_ALT2">
<connects>
<connect gate="G$1" pin="CLK" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="EP"/>
<connect gate="G$1" pin="LE" pad="7"/>
<connect gate="G$1" pin="OUT0" pad="8"/>
<connect gate="G$1" pin="OUT1" pad="9"/>
<connect gate="G$1" pin="OUT10" pad="18"/>
<connect gate="G$1" pin="OUT11" pad="19"/>
<connect gate="G$1" pin="OUT12" pad="20"/>
<connect gate="G$1" pin="OUT13" pad="21"/>
<connect gate="G$1" pin="OUT14" pad="22"/>
<connect gate="G$1" pin="OUT15" pad="23"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="OUT5" pad="13"/>
<connect gate="G$1" pin="OUT6" pad="14"/>
<connect gate="G$1" pin="OUT7" pad="15"/>
<connect gate="G$1" pin="OUT8" pad="16"/>
<connect gate="G$1" pin="OUT9" pad="17"/>
<connect gate="G$1" pin="REXT" pad="2"/>
<connect gate="G$1" pin="SDI" pad="5"/>
<connect gate="G$1" pin="SDO" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="~OE" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCANTOOL" prefix="U">
<description>&lt;h1&gt;STN1110 - Multiprotocol OBD II to UART Interpreter, QFN Package&lt;/h1&gt;

&lt;p&gt;
&lt;table&gt;
  &lt;tr&gt;&lt;td&gt;&lt;h2&gt;Change Log&lt;/h2&gt;&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;
    &lt;th&gt;Date&lt;/th&gt;&lt;th&gt;Author&lt;/th&gt;&lt;th&gt;Change&lt;/th&gt;
  &lt;tr&gt;
    &lt;td&gt;Aug 23, 2010&lt;/td&gt;&lt;td&gt;vit@scantool.net&lt;/td&gt;&lt;td&gt;Created device&lt;/td&gt;
  &lt;/tr&gt;
 &lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;

&lt;br /&gt;</description>
<gates>
<gate name="G$1" symbol="STN1110-QFN"/>
</gates>
<devices>
<device name="" package="_STN_SCANTOOL_QFN-28-S">
<connects>
<connect gate="G$1" pin="!ISO_K_TX" pad="22"/>
<connect gate="G$1" pin="!ISO_L_TX" pad="23"/>
<connect gate="G$1" pin="!ISO_RX" pad="8"/>
<connect gate="G$1" pin="!J1850_BUS-_TX" pad="4"/>
<connect gate="G$1" pin="!OBD_RX_LED!/!INT" pad="19"/>
<connect gate="G$1" pin="!OBD_TX_LED!/!RST_NVM" pad="18"/>
<connect gate="G$1" pin="!RESET" pad="26"/>
<connect gate="G$1" pin="!SLEEP" pad="9"/>
<connect gate="G$1" pin="!UART_RX_LED" pad="21"/>
<connect gate="G$1" pin="!UART_TX_LED" pad="20"/>
<connect gate="G$1" pin="!VPW_RX" pad="1"/>
<connect gate="G$1" pin="ANALOG_IN" pad="27"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="24"/>
<connect gate="G$1" pin="CAN_RX" pad="11"/>
<connect gate="G$1" pin="CAN_TX" pad="12"/>
<connect gate="G$1" pin="J1850_BUS+_TX" pad="3"/>
<connect gate="G$1" pin="OSC1" pad="6"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="PAD" pad="EXP"/>
<connect gate="G$1" pin="PWM/!VPW" pad="28"/>
<connect gate="G$1" pin="PWM_RX" pad="2"/>
<connect gate="G$1" pin="PWR_CTRL" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCAP" pad="17"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VSS@16" pad="16"/>
<connect gate="G$1" pin="VSS@5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK_MINI" prefix="JP">
<gates>
<gate name="G$1" symbol="JOYSTICK_MINI"/>
</gates>
<devices>
<device name="4UCON" package="JOYSTICK_MINI">
<connects>
<connect gate="G$1" pin="CENT" pad="CTR"/>
<connect gate="G$1" pin="DOWN" pad="D"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="LEFT" pad="B"/>
<connect gate="G$1" pin="RIGHT" pad="C"/>
<connect gate="G$1" pin="UP" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT42QT1012" prefix="U">
<description>One channel touch sensor IC</description>
<gates>
<gate name="G$1" symbol="AT42QT1012"/>
</gates>
<devices>
<device name="" package="SOT-23-6">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SNS" pad="4"/>
<connect gate="G$1" pin="SNSK" pad="3"/>
<connect gate="G$1" pin="TIME" pad="6"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS61200" prefix="U">
<description>DC to DC Booster</description>
<gates>
<gate name="G$1" symbol="TPS61200"/>
</gates>
<devices>
<device name="" package="QFN-10_PAD">
<connects>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="FB" pad="10"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="L" pad="3"/>
<connect gate="G$1" pin="PAD@1" pad="15"/>
<connect gate="G$1" pin="PAD@2" pad="11"/>
<connect gate="G$1" pin="PAD@3" pad="12"/>
<connect gate="G$1" pin="PAD@4" pad="13"/>
<connect gate="G$1" pin="PAD@5" pad="14"/>
<connect gate="G$1" pin="PGND" pad="4"/>
<connect gate="G$1" pin="PS" pad="8"/>
<connect gate="G$1" pin="UVLO" pad="7"/>
<connect gate="G$1" pin="VAUX" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SM130" prefix="U">
<description>13.56MHz RFID Mifare Read/Write Module</description>
<gates>
<gate name="G$1" symbol="SM130"/>
</gates>
<devices>
<device name="" package="SM130">
<connects>
<connect gate="G$1" pin="ANT1" pad="24"/>
<connect gate="G$1" pin="ANT2" pad="26"/>
<connect gate="G$1" pin="ERROR" pad="17"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="I1" pad="19"/>
<connect gate="G$1" pin="I2" pad="20"/>
<connect gate="G$1" pin="O1" pad="21"/>
<connect gate="G$1" pin="O2" pad="22"/>
<connect gate="G$1" pin="OK" pad="16"/>
<connect gate="G$1" pin="RESET" pad="18"/>
<connect gate="G$1" pin="RFGND@23" pad="23"/>
<connect gate="G$1" pin="RFGND@25" pad="25"/>
<connect gate="G$1" pin="RFGND@27" pad="27"/>
<connect gate="G$1" pin="RFVCC" pad="1"/>
<connect gate="G$1" pin="RX-I" pad="11"/>
<connect gate="G$1" pin="SCL" pad="9"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="TX-O" pad="12"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IMU3000" prefix="U">
<gates>
<gate name="G$1" symbol="IMU3000"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="AUX_CL" pad="7"/>
<connect gate="G$1" pin="AUX_DA" pad="6"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CLKOUT" pad="22"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VLOG" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73831" prefix="U">
<description>&lt;h3&gt; Microchip's MCP73831&lt;/h3&gt;
Miniature single cell, fully integrated Li-Ion, Li-polymer charge management controller&lt;br&gt;
http://ww1.microchip.com/downloads/en/DeviceDoc/21984a.pdf</description>
<gates>
<gate name="G$1" symbol="MCP73831"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="STAT" pad="1"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-RIBBON_CONNECTOR" prefix="J">
<description>&lt;h3&gt;fabrick.it Conductive Ribbon Connector&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="FKIT-CONNECTOR_COND_03"/>
</gates>
<devices>
<device name="-2MM_L_REV2" package="FKIT-RIBBON_CONNECTOR_03_2MM_L">
<connects>
<connect gate="G$1" pin="P$1" pad="P1A"/>
<connect gate="G$1" pin="P$2" pad="P2A"/>
<connect gate="G$1" pin="P$3" pad="P3A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2MM_R_REV2" package="FKIT-RIBBON_CONNECTOR_03_2MM_R">
<connects>
<connect gate="G$1" pin="P$1" pad="P1A"/>
<connect gate="G$1" pin="P$2" pad="P2A"/>
<connect gate="G$1" pin="P$3" pad="P3A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-COIN_CELL" prefix="BATT">
<description>&lt;h3&gt;Fabrick.it Coin Cell Holder&lt;/h3&gt;
Coin cell holder for 24.5mm rechargable coin cell</description>
<gates>
<gate name="G$1" symbol="FKIT-BATTERY"/>
</gates>
<devices>
<device name="LIR2450-H" package="FKIT-LIR2450-H">
<connects>
<connect gate="G$1" pin="NEG" pad="NEG"/>
<connect gate="G$1" pin="POS" pad="POS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-LOGO" prefix="LOGO">
<description>&lt;h3&gt;Fabrick.it Logos&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="FKIT-LOGO"/>
</gates>
<devices>
<device name="-MEDIUM" package="FKIT-LOGO_MEDIUM">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMALL" package="FKIT-LOGO_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-VERY_SMALL" package="FKIT-LOGO_VERY_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-VERY_SMALL_VECTOR" package="FKIT-LOGO_VERY_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_PIRANHA_5MM">
<gates>
<gate name="G$1" symbol="LED-TRICOLOR-THROUGHHOLE"/>
</gates>
<devices>
<device name="" package="LED_PIRANHA_5MM">
<connects>
<connect gate="G$1" pin="BLU" pad="B"/>
<connect gate="G$1" pin="C" pad="-"/>
<connect gate="G$1" pin="GRN" pad="G"/>
<connect gate="G$1" pin="RED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-LOGOTYPE" prefix="LOGO">
<description>&lt;h3&gt;Fabrick.it Logotype&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="FKIT-LOGOTYPE"/>
</gates>
<devices>
<device name="-SMALL" package="FKIT-LOGOTYPE_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-VERY_SMALL" package="FKIT-LOGOTYPE_VERY_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MEDIUM" package="FKIT-LOGOTYPE_MEDIUM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3234">
<description>DS3234 Real Time Clock</description>
<gates>
<gate name="G$1" symbol="DS3234"/>
</gates>
<devices>
<device name="" package="DS3234">
<connects>
<connect gate="G$1" pin="32KHZ" pad="3"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DIN" pad="17"/>
<connect gate="G$1" pin="DOUT" pad="19"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="INT/SQW" pad="5"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="SCLK@18" pad="18"/>
<connect gate="G$1" pin="SCLK@20" pad="20"/>
<connect gate="G$1" pin="VBAT" pad="16"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXXDAX06" prefix="U">
<description>&lt;b&gt;PIC24FXXXDAX06&lt;/b&gt;
PIC24FXXXDA106 / PIC24FXXXDA206</description>
<gates>
<gate name="G$1" symbol="PIC24FJXXXDAX06"/>
</gates>
<devices>
<device name="" package="PIC24FXXX_TQFP64">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AN14/CTPLS/RP14/CN32/RB14" pad="29"/>
<connect gate="G$1" pin="AN15/RP29/REFO/CN12/RB15" pad="30"/>
<connect gate="G$1" pin="AN2/C2INB/VMIO/RP13/CN4/RB2" pad="14"/>
<connect gate="G$1" pin="AN3/C2INA/VPIO/CN5/RB3" pad="13"/>
<connect gate="G$1" pin="AN8/RP8/CN26/RB8" pad="21"/>
<connect gate="G$1" pin="AN9/RP9/CN27/RB9" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="C1INC/RP26/CN9/RG7" pad="5"/>
<connect gate="G$1" pin="C1IND/RP21/CN8/RG6" pad="4"/>
<connect gate="G$1" pin="C2INC/RP27/GD15/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="C2IND/RP19/GD14/CN10/RG8" pad="6"/>
<connect gate="G$1" pin="C3INA/SESSEND/CN16/RD7" pad="55"/>
<connect gate="G$1" pin="C3INB/CN15/RD6" pad="54"/>
<connect gate="G$1" pin="D+/CN83/RG2" pad="37"/>
<connect gate="G$1" pin="D-/CN84/RG3" pad="36"/>
<connect gate="G$1" pin="DMH/RP11/INT0/CN49/RD0" pad="46"/>
<connect gate="G$1" pin="DPH/RP23/CN51/RD2" pad="50"/>
<connect gate="G$1" pin="DPLN/SDA1/RP4/GD8/CN54/RD9" pad="43"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="GD0/CN58/RE0" pad="60"/>
<connect gate="G$1" pin="GD1/CN59/RE1" pad="61"/>
<connect gate="G$1" pin="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0" pad="58"/>
<connect gate="G$1" pin="GD11/VCMPST2/SESSVLD/CN69/RF1" pad="59"/>
<connect gate="G$1" pin="GD12/SCL3/CN64/RE6" pad="2"/>
<connect gate="G$1" pin="GD13/SDA3/CN65/RE7" pad="3"/>
<connect gate="G$1" pin="GD2/CN60/RE2" pad="62"/>
<connect gate="G$1" pin="GD3/CN61/RE3" pad="63"/>
<connect gate="G$1" pin="HSYNC/CN62/RE4" pad="64"/>
<connect gate="G$1" pin="OSCI/CLKI/CN23/RC12" pad="39"/>
<connect gate="G$1" pin="OSCO/CLKO/CN22/RC15" pad="40"/>
<connect gate="G$1" pin="PGEC1/AN1/VREF-/RP1/CN3/RB1" pad="15"/>
<connect gate="G$1" pin="PGEC2/AN6/RP6/CN24/RB6" pad="17"/>
<connect gate="G$1" pin="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5" pad="11"/>
<connect gate="G$1" pin="PGED1/AN0/VREF+/RP0/CN2/RB0" pad="16"/>
<connect gate="G$1" pin="PGED2/AN7/RP7/RCV/CN25/RB7" pad="18"/>
<connect gate="G$1" pin="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4" pad="12"/>
<connect gate="G$1" pin="RP12/GD7/CN56/RD11" pad="45"/>
<connect gate="G$1" pin="RP16/USBID/CN71/RF3" pad="33"/>
<connect gate="G$1" pin="RP20/GPWR/CN14/RD5" pad="53"/>
<connect gate="G$1" pin="RP22/GEN/CN52/RD3" pad="51"/>
<connect gate="G$1" pin="RP25/GCLK/CN13/RD4" pad="52"/>
<connect gate="G$1" pin="RTCC/DMLN/RP2/CN53/RD8" pad="42"/>
<connect gate="G$1" pin="SCL1/RP3/GD6/CN55/RD10" pad="44"/>
<connect gate="G$1" pin="SCL2/RP17/GD5/CN18/RF5" pad="32"/>
<connect gate="G$1" pin="SDA2/RP10/GD4/CN17/RF4" pad="31"/>
<connect gate="G$1" pin="SOSCI/C3IND/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="TCK/AN12/CTEDG2/CN30/RB12" pad="27"/>
<connect gate="G$1" pin="TDI/AN13/CTEDG1/CN31/RB13" pad="28"/>
<connect gate="G$1" pin="TDO/AN11/CN29/RB11" pad="24"/>
<connect gate="G$1" pin="TMS/CVREF/AN10/CN28/RB10" pad="23"/>
<connect gate="G$1" pin="VBUS/RF7" pad="34"/>
<connect gate="G$1" pin="VCAP" pad="56"/>
<connect gate="G$1" pin="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1" pad="49"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSYNC/CN63/RE5" pad="1"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS485_SP491">
<gates>
<gate name="G$1" symbol="RS485_SP491"/>
</gates>
<devices>
<device name="" package="SOIC-14">
<connects>
<connect gate="G$1" pin="/RE" pad="3"/>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="D" pad="5"/>
<connect gate="G$1" pin="DE" pad="4"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="8"/>
<connect gate="G$1" pin="NC3" pad="13"/>
<connect gate="G$1" pin="R" pad="2"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="Y" pad="9"/>
<connect gate="G$1" pin="Z" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC4051_MUX">
<gates>
<gate name="G$1" symbol="74HC4051_MUX"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="9"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="IO" pad="3"/>
<connect gate="G$1" pin="IO0" pad="13"/>
<connect gate="G$1" pin="IO1" pad="14"/>
<connect gate="G$1" pin="IO2" pad="15"/>
<connect gate="G$1" pin="IO3" pad="12"/>
<connect gate="G$1" pin="IO4" pad="1"/>
<connect gate="G$1" pin="IO5" pad="5"/>
<connect gate="G$1" pin="IO6" pad="2"/>
<connect gate="G$1" pin="IO7" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCMT1103-OPTO">
<gates>
<gate name="G$1" symbol="TCMT1103"/>
</gates>
<devices>
<device name="" package="SSOP-4">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSGEQ7" prefix="IC">
<gates>
<gate name="G$1" symbol="MSGEQ7"/>
</gates>
<devices>
<device name="SOIC" package="SOIC8">
<connects>
<connect gate="G$1" pin="AUDIO_IN" pad="5"/>
<connect gate="G$1" pin="CG" pad="6"/>
<connect gate="G$1" pin="CKIN" pad="8"/>
<connect gate="G$1" pin="DCOUT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="STROBE" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STARBOARD_GND" prefix="J" uservalue="yes">
<description>&lt;h3&gt;StarBoard ground Pad&lt;/h3&gt;
Starboard pads sans the star cutout in top layer</description>
<gates>
<gate name="G$1" symbol="STARBOARD_PAD"/>
</gates>
<devices>
<device name="" package="STARBOARD_GROUND">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMALL" package="STARBOARD_GROUND_SMALL">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-WIDE" package="STARBOARD_GROUND_WIDE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMALL2" package="STARBOARD_GROUND_SMALL2">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STARBOARD_PWR" prefix="J" uservalue="yes">
<description>&lt;h3&gt;StarbBoard Power pad&lt;/h3&gt;
Power pads are designated by the star cutout in the top layer.</description>
<gates>
<gate name="G$1" symbol="STARBOARD_PAD+"/>
</gates>
<devices>
<device name="-WIDE" package="STARBOARD_PWR_WIDE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TALL" package="STARBOARD_PWR">
<connects>
<connect gate="G$1" pin="MOUNT" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BANANA_CONN" prefix="J" uservalue="yes">
<gates>
<gate name="G$1" symbol="BANANA_CONN"/>
</gates>
<devices>
<device name="" package="BANANA_CONN">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STARBOARD_LOGO">
<gates>
<gate name="G$1" symbol="STARBOARD_LOGO"/>
</gates>
<devices>
<device name="" package="STARBOARD_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TEXT" package="STARBOARD_LOGO_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIZ811MJ" prefix="U">
<description>&lt;h3&gt;WIZnet W5100 Network Module with MagJack - WIZ811MJ&lt;/h3&gt;
WIZnet's WIZ811MJ is a breakout board for the W5100 embedded TCP/IP chip. Also included on the board is a RJ-45 MagJack Connector (RJ45 with X'FMR).&lt;br&gt;&lt;br&gt;

See http://www.sparkfun.com/commerce/product_info.php?products_id=9473 for more documentation and info.&lt;br&gt;
&lt;B&gt;**UNPROVEN&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="WIZ811MJ"/>
</gates>
<devices>
<device name="" package="WIZ811MJ">
<connects>
<connect gate="G$1" pin="/CS" pad="27"/>
<connect gate="G$1" pin="/INT" pad="28"/>
<connect gate="G$1" pin="/RD" pad="26"/>
<connect gate="G$1" pin="/RESET" pad="22"/>
<connect gate="G$1" pin="/SCS" pad="24"/>
<connect gate="G$1" pin="/WR" pad="25"/>
<connect gate="G$1" pin="A0" pad="31"/>
<connect gate="G$1" pin="A1" pad="32"/>
<connect gate="G$1" pin="A10" pad="15"/>
<connect gate="G$1" pin="A11" pad="16"/>
<connect gate="G$1" pin="A12" pad="17"/>
<connect gate="G$1" pin="A13" pad="18"/>
<connect gate="G$1" pin="A14" pad="19"/>
<connect gate="G$1" pin="A2" pad="33"/>
<connect gate="G$1" pin="A3" pad="34"/>
<connect gate="G$1" pin="A4" pad="35"/>
<connect gate="G$1" pin="A5" pad="36"/>
<connect gate="G$1" pin="A6" pad="37"/>
<connect gate="G$1" pin="A7" pad="38"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="A9" pad="14"/>
<connect gate="G$1" pin="D0" pad="4"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="6"/>
<connect gate="G$1" pin="D3" pad="5"/>
<connect gate="G$1" pin="D4" pad="8"/>
<connect gate="G$1" pin="D5" pad="7"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="29"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="GND@4" pad="40"/>
<connect gate="G$1" pin="GND@5" pad="30"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="SCLK" pad="23"/>
<connect gate="G$1" pin="VCC@1" pad="12"/>
<connect gate="G$1" pin="VCC@2" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XLR3_NCFAH2" prefix="XLR">
<gates>
<gate name="G$1" symbol="XLR3_NCFAH2"/>
</gates>
<devices>
<device name="" package="XLR3_NC3FAH2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="G" pad="G"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-SNAP_CONNECTOR">
<gates>
<gate name="G$1" symbol="FKIT-SNAP_CONNECTOR"/>
</gates>
<devices>
<device name="-FEMALE" package="FKIT-SNAP_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MALE" package="FKIT-SNAP_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9306">
<gates>
<gate name="G$1" symbol="PCA9306"/>
</gates>
<devices>
<device name="" package="PSOP-8">
<connects>
<connect gate="G$1" pin="EN" pad="8"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCL1" pad="3"/>
<connect gate="G$1" pin="SCL2" pad="6"/>
<connect gate="G$1" pin="SDA1" pad="4"/>
<connect gate="G$1" pin="SDA2" pad="5"/>
<connect gate="G$1" pin="VREF1" pad="2"/>
<connect gate="G$1" pin="VREF2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_MC33269" prefix="U">
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="DT" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8U2" prefix="U">
<description>Atmel 8-bit Microcontroller with 8/16/32K Bystes of ISP Flash and USB Controller. ATmega8U2, ATmega16U2, and ATmega32U2</description>
<gates>
<gate name="G$1" symbol="ATMEGA8U2"/>
</gates>
<devices>
<device name="AU" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="D+" pad="29"/>
<connect gate="G$1" pin="D-" pad="30"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PB0" pad="14"/>
<connect gate="G$1" pin="PB1(SCK)" pad="15"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="16"/>
<connect gate="G$1" pin="PB3(MISO)" pad="17"/>
<connect gate="G$1" pin="PB4" pad="18"/>
<connect gate="G$1" pin="PB5" pad="19"/>
<connect gate="G$1" pin="PB6" pad="20"/>
<connect gate="G$1" pin="PB7" pad="21"/>
<connect gate="G$1" pin="PC2" pad="5"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="25"/>
<connect gate="G$1" pin="PC6" pad="23"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="6"/>
<connect gate="G$1" pin="PD1" pad="7"/>
<connect gate="G$1" pin="PD2(RX)" pad="8"/>
<connect gate="G$1" pin="PD3(TX)" pad="9"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="PD5" pad="11"/>
<connect gate="G$1" pin="PD6(RTS)" pad="12"/>
<connect gate="G$1" pin="PD7(CTS)" pad="13"/>
<connect gate="G$1" pin="RESET/PC1" pad="24"/>
<connect gate="G$1" pin="UCAP" pad="27"/>
<connect gate="G$1" pin="UGND" pad="28"/>
<connect gate="G$1" pin="UVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="1"/>
<connect gate="G$1" pin="XTAL2/PC0" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VARISTOR" prefix="Z" uservalue="yes">
<description>&lt;h3&gt;Varistor&lt;/h3&gt;
Varistor (Variable resistor) is a nonlinear resistive element of the
voltage dependence that resistance changes with applied voltage.
Varistor is equivalent with Zener diode of two series connection.</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="-0603" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB+SHIELD">
<description>&lt;h3&gt;USB+Shield&lt;/h3&gt;
USB connector with shield pins connectable</description>
<gates>
<gate name="G$1" symbol="USB+SHIELD"/>
</gates>
<devices>
<device name="" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="P$1" pad="S1"/>
<connect gate="G$1" pin="P$2" pad="S2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-PCHANNEL" prefix="Q">
<gates>
<gate name="G$1" symbol="MOSFET-PCHANNEL"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS331" prefix="U">
<description>LIS331HH 3-axis accelerometer</description>
<gates>
<gate name="G$1" symbol="LIS331-1"/>
</gates>
<devices>
<device name="" package="LGA16-3MM">
<connects>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GNDR" pad="10"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="SA0/SDO" pad="7"/>
<connect gate="G$1" pin="SCL/SPC" pad="4"/>
<connect gate="G$1" pin="SDA/SDI" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
<connect gate="G$1" pin="VDDR" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4983" prefix="U">
<description>DMOS Microstepping Driver with Translator</description>
<gates>
<gate name="G$1" symbol="A4983"/>
</gates>
<devices>
<device name="" package="QFN-28-5MM">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADJD-S311-CR999">
<gates>
<gate name="G$1" symbol="ADJD-S311-CR999"/>
</gates>
<devices>
<device name="" package="CSP-9">
<connects>
<connect gate="G$1" pin="AGND" pad="C3"/>
<connect gate="G$1" pin="AVDD" pad="A3"/>
<connect gate="G$1" pin="CLKIO" pad="B1"/>
<connect gate="G$1" pin="DGND" pad="C1"/>
<connect gate="G$1" pin="DVDD" pad="A1"/>
<connect gate="G$1" pin="RESET" pad="C2"/>
<connect gate="G$1" pin="SCKSLV" pad="A2"/>
<connect gate="G$1" pin="SDASLV" pad="B2"/>
<connect gate="G$1" pin="SLEEP" pad="B3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_NCP50X" prefix="U">
<description>NCP550x 500mA LDO Voltage Regulator</description>
<gates>
<gate name="G$1" symbol="78ADJ-3"/>
</gates>
<devices>
<device name="" package="DPAK-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="ADJ"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="VIN"/>
<connect gate="G$1" pin="OUT" pad="VOUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="D2523T" prefix="U">
<description>D2523T GPS Module</description>
<gates>
<gate name="G$1" symbol="D2523T"/>
</gates>
<devices>
<device name="_" package="EM406">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LED" pad="1"/>
<connect gate="G$1" pin="RX" pad="6"/>
<connect gate="G$1" pin="TX" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="2"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADH8066" prefix="U">
<description>8066-GSM-GPRS module from ADH-Tech</description>
<gates>
<gate name="G$1" symbol="ADH8066"/>
</gates>
<devices>
<device name="_SMD" package="ADH8066">
<connects>
<connect gate="G$1" pin="1.8V" pad="31"/>
<connect gate="G$1" pin="ADC1" pad="11"/>
<connect gate="G$1" pin="AUXOUTN" pad="48"/>
<connect gate="G$1" pin="AUXOUTP" pad="47"/>
<connect gate="G$1" pin="BATTTEMP" pad="12"/>
<connect gate="G$1" pin="CHV_DRV" pad="20"/>
<connect gate="G$1" pin="CHV_MAX" pad="40"/>
<connect gate="G$1" pin="CTS0" pad="34"/>
<connect gate="G$1" pin="DCD0" pad="39"/>
<connect gate="G$1" pin="DSR0" pad="35"/>
<connect gate="G$1" pin="DTR0" pad="33"/>
<connect gate="G$1" pin="EARN" pad="50"/>
<connect gate="G$1" pin="EARP" pad="49"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@42" pad="42"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GPIO10" pad="5"/>
<connect gate="G$1" pin="GPIO3" pad="13"/>
<connect gate="G$1" pin="MIC1_N" pad="44"/>
<connect gate="G$1" pin="MIC1_P" pad="43"/>
<connect gate="G$1" pin="MIC2_N" pad="46"/>
<connect gate="G$1" pin="MIC2_P" pad="45"/>
<connect gate="G$1" pin="ON_KEY" pad="41"/>
<connect gate="G$1" pin="PCMCLK" pad="9"/>
<connect gate="G$1" pin="PCMDI" pad="7"/>
<connect gate="G$1" pin="PCMDO" pad="10"/>
<connect gate="G$1" pin="PCMFSO" pad="8"/>
<connect gate="G$1" pin="RI0" pad="32"/>
<connect gate="G$1" pin="RTS0" pad="37"/>
<connect gate="G$1" pin="RXD0" pad="17"/>
<connect gate="G$1" pin="RXD1" pad="16"/>
<connect gate="G$1" pin="SCL(NC)" pad="36"/>
<connect gate="G$1" pin="SDA(NC)" pad="38"/>
<connect gate="G$1" pin="SIMCLK" pad="1"/>
<connect gate="G$1" pin="SIMIO" pad="3"/>
<connect gate="G$1" pin="SIMRST" pad="4"/>
<connect gate="G$1" pin="SIMVDD" pad="2"/>
<connect gate="G$1" pin="TXD0" pad="15"/>
<connect gate="G$1" pin="TXD1" pad="14"/>
<connect gate="G$1" pin="VBAT@26" pad="26"/>
<connect gate="G$1" pin="VBAT@27" pad="27"/>
<connect gate="G$1" pin="VBAT@28" pad="28"/>
<connect gate="G$1" pin="VBAT@29" pad="29"/>
<connect gate="G$1" pin="VBAT@30" pad="30"/>
<connect gate="G$1" pin="VCHAR@18" pad="18"/>
<connect gate="G$1" pin="VCHAR@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WATN001002BF" prefix="U">
<description>10x1 and 10x2 16-segment E-paper Display&lt;br&gt;
&lt;b&gt;***Unproven!!!***&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="WATN001001"/>
</gates>
<devices>
<device name="" package="FFC26">
<connects>
<connect gate="G$1" pin="DI0" pad="16"/>
<connect gate="G$1" pin="DI1" pad="17"/>
<connect gate="G$1" pin="DI2" pad="18"/>
<connect gate="G$1" pin="DLY0" pad="13"/>
<connect gate="G$1" pin="DLY1" pad="14"/>
<connect gate="G$1" pin="EIO1" pad="6"/>
<connect gate="G$1" pin="EIO2" pad="20"/>
<connect gate="G$1" pin="LATCH" pad="9"/>
<connect gate="G$1" pin="RESERVED@1" pad="10"/>
<connect gate="G$1" pin="RESERVED@2" pad="15"/>
<connect gate="G$1" pin="RESERVED@3" pad="19"/>
<connect gate="G$1" pin="RESERVED@4" pad="26"/>
<connect gate="G$1" pin="SHL" pad="11"/>
<connect gate="G$1" pin="SLEEPB" pad="12"/>
<connect gate="G$1" pin="V0@1" pad="1"/>
<connect gate="G$1" pin="V0@2" pad="25"/>
<connect gate="G$1" pin="V1@1" pad="2"/>
<connect gate="G$1" pin="V1@2" pad="24"/>
<connect gate="G$1" pin="V2@1" pad="3"/>
<connect gate="G$1" pin="V2@2" pad="23"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="21"/>
<connect gate="G$1" pin="VSSE@1" pad="4"/>
<connect gate="G$1" pin="VSSE@2" pad="22"/>
<connect gate="G$1" pin="XCK" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCM01" prefix="U">
<description>&lt;b&gt;DCM01 Reflective Blood Sensor&lt;/b&gt;&lt;br&gt;
UNPROVEN&lt;br&gt;
Sensor head for Pulse Oximeter.  Contains IR and visible red LEDs, and PIN photodiode.&lt;br&gt;
&lt;href="http://www.apmkr.com/bio-device/DCM01_datasheet.pdf"&gt;http://www.apmkr.com/bio-device/DCM01_datasheet.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="DCM01"/>
</gates>
<devices>
<device name="" package="DCM01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2801" prefix="U">
<description>&lt;h3&gt;WS2801&lt;/h3&gt;
3 Channel Constant Current LED Driver with programmable PWM outputs.
&lt;br&gt;
&lt;br&gt;
Datasheet:  http://www.sparkfun.com/datasheets/Components/LED/WS2801.pdf</description>
<gates>
<gate name="G$1" symbol="WS2801"/>
</gates>
<devices>
<device name="" package="SOP-14">
<connects>
<connect gate="G$1" pin="BFB" pad="6"/>
<connect gate="G$1" pin="BOUT" pad="8"/>
<connect gate="G$1" pin="CKI" pad="1"/>
<connect gate="G$1" pin="CKO" pad="13"/>
<connect gate="G$1" pin="GFB" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GOUT" pad="9"/>
<connect gate="G$1" pin="POL" pad="3"/>
<connect gate="G$1" pin="RFB" pad="4"/>
<connect gate="G$1" pin="ROUT" pad="10"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-TRICOLOR-5050" prefix="LED">
<gates>
<gate name="G$1" symbol="LED-TRICOLOR-INDV"/>
</gates>
<devices>
<device name="" package="LED-TRICOLOR-5050">
<connects>
<connect gate="G$1" pin="BLU-A" pad="3"/>
<connect gate="G$1" pin="BLU-C" pad="4"/>
<connect gate="G$1" pin="GRN-A" pad="1"/>
<connect gate="G$1" pin="GRN-C" pad="6"/>
<connect gate="G$1" pin="RED-A" pad="2"/>
<connect gate="G$1" pin="RED-C" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W5100" prefix="U" uservalue="yes">
<description>&lt;h3&gt;WIZnet W5100&lt;/h3&gt;
TCP/IP PHY Embedded Chip&lt;br&gt;
See SparkFun catalog # COM-09471&lt;br&gt;
&lt;br&gt;
Package: &lt;b&gt;LQFP-80&lt;/b&gt;,10x10mm,  0.4mm pitch</description>
<gates>
<gate name="G$1" symbol="W5100"/>
</gates>
<devices>
<device name="" package="LQFP-80">
<connects>
<connect gate="G$1" pin="*CS" pad="55"/>
<connect gate="G$1" pin="*INT" pad="56"/>
<connect gate="G$1" pin="*RD" pad="58"/>
<connect gate="G$1" pin="*RESET" pad="59"/>
<connect gate="G$1" pin="*SCS" pad="29"/>
<connect gate="G$1" pin="*WR" pad="57"/>
<connect gate="G$1" pin="1V8A@0" pad="7"/>
<connect gate="G$1" pin="1V8A@1" pad="74"/>
<connect gate="G$1" pin="1V8D@0" pad="15"/>
<connect gate="G$1" pin="1V8D@1" pad="16"/>
<connect gate="G$1" pin="1V8D@2" pad="33"/>
<connect gate="G$1" pin="1V8D@3" pad="69"/>
<connect gate="G$1" pin="1V8OUT" pad="11"/>
<connect gate="G$1" pin="3V3A" pad="2"/>
<connect gate="G$1" pin="3V3D@0" pad="12"/>
<connect gate="G$1" pin="3V3D@1" pad="18"/>
<connect gate="G$1" pin="3V3D@2" pad="44"/>
<connect gate="G$1" pin="ADDR0" pad="54"/>
<connect gate="G$1" pin="ADDR1" pad="53"/>
<connect gate="G$1" pin="ADDR10" pad="42"/>
<connect gate="G$1" pin="ADDR11" pad="41"/>
<connect gate="G$1" pin="ADDR12" pad="40"/>
<connect gate="G$1" pin="ADDR13" pad="39"/>
<connect gate="G$1" pin="ADDR14" pad="38"/>
<connect gate="G$1" pin="ADDR2" pad="52"/>
<connect gate="G$1" pin="ADDR3" pad="51"/>
<connect gate="G$1" pin="ADDR4" pad="50"/>
<connect gate="G$1" pin="ADDR5" pad="49"/>
<connect gate="G$1" pin="ADDR6" pad="48"/>
<connect gate="G$1" pin="ADDR7" pad="47"/>
<connect gate="G$1" pin="ADDR8" pad="46"/>
<connect gate="G$1" pin="ADDR9" pad="45"/>
<connect gate="G$1" pin="COLLED" pad="71"/>
<connect gate="G$1" pin="DATA0" pad="26"/>
<connect gate="G$1" pin="DATA1" pad="25"/>
<connect gate="G$1" pin="DATA2" pad="24"/>
<connect gate="G$1" pin="DATA3" pad="23"/>
<connect gate="G$1" pin="DATA4" pad="22"/>
<connect gate="G$1" pin="DATA5" pad="21"/>
<connect gate="G$1" pin="DATA6" pad="20"/>
<connect gate="G$1" pin="DATA7" pad="19"/>
<connect gate="G$1" pin="FDXLED" pad="70"/>
<connect gate="G$1" pin="GNDA@0" pad="4"/>
<connect gate="G$1" pin="GNDA@1" pad="10"/>
<connect gate="G$1" pin="GNDA@2" pad="77"/>
<connect gate="G$1" pin="GNDD@0" pad="13"/>
<connect gate="G$1" pin="GNDD@1" pad="14"/>
<connect gate="G$1" pin="GNDD@2" pad="17"/>
<connect gate="G$1" pin="GNDD@3" pad="32"/>
<connect gate="G$1" pin="GNDD@4" pad="43"/>
<connect gate="G$1" pin="GNDD@5" pad="68"/>
<connect gate="G$1" pin="LINKLED" pad="66"/>
<connect gate="G$1" pin="MISO" pad="27"/>
<connect gate="G$1" pin="MOSI" pad="28"/>
<connect gate="G$1" pin="NC@0" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="60"/>
<connect gate="G$1" pin="NC@2" pad="61"/>
<connect gate="G$1" pin="NC@3" pad="62"/>
<connect gate="G$1" pin="NC@4" pad="78"/>
<connect gate="G$1" pin="NC@5" pad="79"/>
<connect gate="G$1" pin="NC@6" pad="80"/>
<connect gate="G$1" pin="OPMODE0" pad="63"/>
<connect gate="G$1" pin="OPMODE1" pad="64"/>
<connect gate="G$1" pin="OPMODE2" pad="65"/>
<connect gate="G$1" pin="RSET_BG" pad="1"/>
<connect gate="G$1" pin="RXIN" pad="6"/>
<connect gate="G$1" pin="RXIP" pad="5"/>
<connect gate="G$1" pin="RXLED" pad="72"/>
<connect gate="G$1" pin="SCLK" pad="30"/>
<connect gate="G$1" pin="SEN" pad="31"/>
<connect gate="G$1" pin="SPDLED" pad="67"/>
<connect gate="G$1" pin="TEST0" pad="37"/>
<connect gate="G$1" pin="TEST1" pad="36"/>
<connect gate="G$1" pin="TEST2" pad="35"/>
<connect gate="G$1" pin="TEST3" pad="34"/>
<connect gate="G$1" pin="TXLED" pad="73"/>
<connect gate="G$1" pin="TXON" pad="9"/>
<connect gate="G$1" pin="TXOP" pad="8"/>
<connect gate="G$1" pin="XTLN" pad="75"/>
<connect gate="G$1" pin="XTLP" pad="76"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGJACK" prefix="J">
<gates>
<gate name="G$1" symbol="MAGJACK"/>
</gates>
<devices>
<device name="" package="MAGJACK">
<connects>
<connect gate="G$1" pin="GLED+" pad="11"/>
<connect gate="G$1" pin="GLED-" pad="12"/>
<connect gate="G$1" pin="RCT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD@0" pad="M1"/>
<connect gate="G$1" pin="SHIELD@1" pad="M2"/>
<connect gate="G$1" pin="TCT" pad="6"/>
<connect gate="G$1" pin="TD+" pad="7"/>
<connect gate="G$1" pin="TD-" pad="8"/>
<connect gate="G$1" pin="YLED+" pad="9"/>
<connect gate="G$1" pin="YLED-" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI470X" prefix="U">
<description>&lt;b&gt;Description:&lt;/b&gt; This is a powerful FM receiver IC. Tested with Si4703. You really only need SEN, RST, SCLK, and SDIO to get a full FM radio working. Antenna comes from headphone jack. See breakout board on SparkFun website for more information.</description>
<gates>
<gate name="G$1" symbol="SI470X"/>
</gates>
<devices>
<device name="" package="SI470X">
<connects>
<connect gate="G$1" pin="!RST" pad="5"/>
<connect gate="G$1" pin="!SEN" pad="6"/>
<connect gate="G$1" pin="DOUT" pad="15"/>
<connect gate="G$1" pin="FMIP" pad="2"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@PAD" pad="21"/>
<connect gate="G$1" pin="GPIO1" pad="19"/>
<connect gate="G$1" pin="GPIO2" pad="18"/>
<connect gate="G$1" pin="GPIO3" pad="17"/>
<connect gate="G$1" pin="LOUT" pad="14"/>
<connect gate="G$1" pin="LPI" pad="4"/>
<connect gate="G$1" pin="RCLK" pad="9"/>
<connect gate="G$1" pin="RFGND" pad="3"/>
<connect gate="G$1" pin="ROUT" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="SDIO" pad="8"/>
<connect gate="G$1" pin="VA" pad="16"/>
<connect gate="G$1" pin="VD" pad="11"/>
<connect gate="G$1" pin="VIO" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSHW-LOGO">
<description>&lt;b&gt;Open Source Hardware Logo&lt;/b&gt; This logo indicates the piece of hardware it is found on incorporates a OSHW license and/or adheres to the definition of open source hardware found here: http://freedomdefined.org/OSHW</description>
<gates>
<gate name="G$1" symbol="OSHW-LOGO"/>
</gates>
<devices>
<device name="S" package="OSHW-LOGO-S">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="OSHW-LOGO-M">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="OSHW-LOGO-L">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATX24" prefix="J">
<description>&lt;b&gt;ATX24 Pin Power Supply Connector&lt;/b&gt; This is a good connector for connecting a computer power supply to a PCB. It's massive, but provides many amps of power at 5V and 12V. SKU: PRT-09498</description>
<gates>
<gate name="G$1" symbol="ATX24-1"/>
</gates>
<devices>
<device name="RH" package="ATX24_RIGHT_ANGLE">
<connects>
<connect gate="G$1" pin="-12V" pad="14"/>
<connect gate="G$1" pin="12V@0" pad="10"/>
<connect gate="G$1" pin="12V@1" pad="11"/>
<connect gate="G$1" pin="3.3V@0" pad="1"/>
<connect gate="G$1" pin="3.3V@1" pad="2"/>
<connect gate="G$1" pin="3.3V@2" pad="12"/>
<connect gate="G$1" pin="3.3V@3" pad="13"/>
<connect gate="G$1" pin="5V@0" pad="4"/>
<connect gate="G$1" pin="5V@1" pad="6"/>
<connect gate="G$1" pin="5V@2" pad="21"/>
<connect gate="G$1" pin="5V@3" pad="22"/>
<connect gate="G$1" pin="5V@4" pad="23"/>
<connect gate="G$1" pin="5V_STDBY" pad="9"/>
<connect gate="G$1" pin="GND@0" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="GND@3" pad="15"/>
<connect gate="G$1" pin="GND@4" pad="17"/>
<connect gate="G$1" pin="GND@5" pad="18"/>
<connect gate="G$1" pin="GND@6" pad="19"/>
<connect gate="G$1" pin="GND@7" pad="24"/>
<connect gate="G$1" pin="NC" pad="20"/>
<connect gate="G$1" pin="PS_ON" pad="16"/>
<connect gate="G$1" pin="PWR_OK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPSENSE_PAD">
<gates>
<gate name="G$1" symbol="CAPSENSE_PAD"/>
</gates>
<devices>
<device name="" package="CAPSENSE_PAD">
<connects>
<connect gate="G$1" pin="RECEIVE" pad="P$1"/>
<connect gate="G$1" pin="RES" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC5883L">
<description>3 Axis Digital Compass IC</description>
<gates>
<gate name="G$1" symbol="HMC5883L"/>
</gates>
<devices>
<device name="SMD" package="16LPCC">
<connects>
<connect gate="G$1" pin="C1" pad="10"/>
<connect gate="G$1" pin="DRDY" pad="15"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="5"/>
<connect gate="G$1" pin="NC@3" pad="6"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
<connect gate="G$1" pin="NC@5" pad="14"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="SETC" pad="12"/>
<connect gate="G$1" pin="SETP" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L3G4200D" prefix="U">
<description>&lt;h3&gt;L3G4200D Three-axis, digital output gyroscope&lt;/h3&gt;
The L3G4200D is a low-power three-axis angular rate sensor, has a full scale of ±250/±500/±2000 dps and is capable of measuring rates with a user-selectable bandwidth.&lt;br&gt;&lt;br&gt;
It includes a sensing element and an IC interface capable of providing the measured angular rate to the external world through a digital interface (I2C/SPI).
&lt;hr&gt;
&lt;b&gt;Package:&lt;/b&gt; 4x4x1.1 LGA-16 (LGA16-4x4.PAC)&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L3G4200D"/>
</gates>
<devices>
<device name="" package="LGA16-4X4">
<connects>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="INT2" pad="6"/>
<connect gate="G$1" pin="PLL" pad="14"/>
<connect gate="G$1" pin="RSDVG@3" pad="11"/>
<connect gate="G$1" pin="RSVDG@0" pad="8"/>
<connect gate="G$1" pin="RSVDG@1" pad="9"/>
<connect gate="G$1" pin="RSVDG@2" pad="10"/>
<connect gate="G$1" pin="RSVDG@4" pad="12"/>
<connect gate="G$1" pin="RSVDV@0" pad="15"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA/SDI" pad="3"/>
<connect gate="G$1" pin="SDO" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGJACK-2" prefix="J">
<gates>
<gate name="G$1" symbol="MAGJACK-2"/>
</gates>
<devices>
<device name="" package="MAGJACK-19938">
<connects>
<connect gate="G$1" pin="GLED+" pad="10"/>
<connect gate="G$1" pin="GLED-" pad="9"/>
<connect gate="G$1" pin="RCT" pad="2"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="3"/>
<connect gate="G$1" pin="SHIELD" pad="8"/>
<connect gate="G$1" pin="TCT" pad="5"/>
<connect gate="G$1" pin="TD+" pad="4"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="YLED+" pad="12"/>
<connect gate="G$1" pin="YLED-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GS1011" prefix="U">
<description>GainSpan GS1011M Low-Power Wireless SOC Wi-Fi Module</description>
<gates>
<gate name="G$1" symbol="GS1011"/>
</gates>
<devices>
<device name="GS1011MXX" package="GS1011MXX">
<connects>
<connect gate="G$1" pin="ADC1" pad="11"/>
<connect gate="G$1" pin="ADC2" pad="12"/>
<connect gate="G$1" pin="ALARM1" pad="7"/>
<connect gate="G$1" pin="ALARM2" pad="13"/>
<connect gate="G$1" pin="DC_CNTL" pad="10"/>
<connect gate="G$1" pin="EN_1.8V" pad="33"/>
<connect gate="G$1" pin="EXT_RESET" pad="47"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@32" pad="32"/>
<connect gate="G$1" pin="GND@48" pad="48"/>
<connect gate="G$1" pin="GPIO19_44MHZ" pad="23"/>
<connect gate="G$1" pin="GPIO20_22MHZ" pad="22"/>
<connect gate="G$1" pin="GPIO21_11MHZ" pad="21"/>
<connect gate="G$1" pin="GPIO28" pad="46"/>
<connect gate="G$1" pin="GPIO29" pad="45"/>
<connect gate="G$1" pin="GPIO30_LED1" pad="44"/>
<connect gate="G$1" pin="GPIO31_LED2" pad="43"/>
<connect gate="G$1" pin="I2C_CLK" pad="25"/>
<connect gate="G$1" pin="I2C_DATA" pad="26"/>
<connect gate="G$1" pin="JTAG_RST" pad="6"/>
<connect gate="G$1" pin="JTAG_TCK" pad="2"/>
<connect gate="G$1" pin="JTAG_TDI" pad="4"/>
<connect gate="G$1" pin="JTAG_TDO" pad="3"/>
<connect gate="G$1" pin="JTAG_TMS" pad="5"/>
<connect gate="G$1" pin="MSPI_CLK" pad="18"/>
<connect gate="G$1" pin="MSPI_CS0" pad="19"/>
<connect gate="G$1" pin="MSPI_CS1" pad="20"/>
<connect gate="G$1" pin="MSPI_DIN" pad="14"/>
<connect gate="G$1" pin="MSPI_DOUT" pad="15"/>
<connect gate="G$1" pin="PWM0/GPIO10" pad="24"/>
<connect gate="G$1" pin="RTC_OUT1" pad="8"/>
<connect gate="G$1" pin="SSPI_CLK" pad="28"/>
<connect gate="G$1" pin="SSPI_CS" pad="29"/>
<connect gate="G$1" pin="SSPI_DIN" pad="30"/>
<connect gate="G$1" pin="SSPI_DOUT" pad="27"/>
<connect gate="G$1" pin="UART0_CTS/GPIO24" pad="42"/>
<connect gate="G$1" pin="UART0_RTS/GPIO25" pad="40"/>
<connect gate="G$1" pin="UART0_RX/GPIO0" pad="41"/>
<connect gate="G$1" pin="UART0_TX/GPIO1" pad="39"/>
<connect gate="G$1" pin="UART1_CTS/GPIO26" pad="35"/>
<connect gate="G$1" pin="UART1_RTS/GPIO27" pad="36"/>
<connect gate="G$1" pin="UART1_RX/GPIO3" pad="37"/>
<connect gate="G$1" pin="UART1_TX/GPIO2" pad="38"/>
<connect gate="G$1" pin="VBAT" pad="9"/>
<connect gate="G$1" pin="VDDIO" pad="34"/>
<connect gate="G$1" pin="VIN_3V3" pad="31"/>
<connect gate="G$1" pin="VOUT_1.8V" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LD1085" prefix="U">
<description>&lt;h3&gt;LD1085 3A low-drop positive voltage regulator, adjustable&lt;/h3&gt;

The LD1085xx is a low drop voltage regulator able to provide up to 3 A of output current. Dropout is guaranteed at a maximum of 1.2 V at the maximum output current, decreasing at lower loads. The LD1085xx is pin to pin compatible with the older 3-terminal adjustable regulators, but has better performances in term of drop and output tolerance.&lt;br&gt;
&lt;br&gt;
&lt;B&gt;Available Packages&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;D&lt;sup&gt;2&lt;/sup&gt;PAK/A - 3-pin w/ tabs, SMD</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="D2" package="D2PACK/A">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="TAB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC5940" prefix="U">
<description>&lt;h3&gt;TI TLC5940&lt;/h3&gt;
16-channel LED Driver with Dot Correction and Grayscale PWM Control
&lt;hr&gt;
&lt;p&gt;The TLC5940 is a 16-channel, constant-current sink LED driver. Each channel has an individually adjustable 4096-step grayscale PWM brightness control and a 64-step, constant-current sink (dot correction). The dot correction adjusts the brightness variations between LED channels and other LED drivers. The dot correction data is stored in an integrated EEPROM. Both grayscale control and dot correction are accessible via a serial interface. A single external resistor sets the maximum current value of all 16 channels.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;28-pin HTSSOP
&lt;li&gt;32-pin 5x5mm QFN
&lt;li&gt;28-pin DIP&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TLC5940"/>
</gates>
<devices>
<device name="-NT" package="DIL28-3">
<connects>
<connect gate="G$1" pin="BLANK" pad="23"/>
<connect gate="G$1" pin="DCPRG" pad="19"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GSCLK" pad="18"/>
<connect gate="G$1" pin="IREF" pad="20"/>
<connect gate="G$1" pin="OUT0" pad="28"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT10" pad="10"/>
<connect gate="G$1" pin="OUT11" pad="11"/>
<connect gate="G$1" pin="OUT12" pad="12"/>
<connect gate="G$1" pin="OUT13" pad="13"/>
<connect gate="G$1" pin="OUT14" pad="14"/>
<connect gate="G$1" pin="OUT15" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="3"/>
<connect gate="G$1" pin="OUT4" pad="4"/>
<connect gate="G$1" pin="OUT5" pad="5"/>
<connect gate="G$1" pin="OUT6" pad="6"/>
<connect gate="G$1" pin="OUT7" pad="7"/>
<connect gate="G$1" pin="OUT8" pad="8"/>
<connect gate="G$1" pin="OUT9" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="25"/>
<connect gate="G$1" pin="SIN" pad="26"/>
<connect gate="G$1" pin="SOUT" pad="17"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VPRG" pad="27"/>
<connect gate="G$1" pin="XERR" pad="16"/>
<connect gate="G$1" pin="XLAT" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RHB" package="QFN-32">
<connects>
<connect gate="G$1" pin="BLANK" pad="31"/>
<connect gate="G$1" pin="DCPRG" pad="25"/>
<connect gate="G$1" pin="GND" pad="30"/>
<connect gate="G$1" pin="GSCLK" pad="24"/>
<connect gate="G$1" pin="IREF" pad="26"/>
<connect gate="G$1" pin="OUT0" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT10" pad="16"/>
<connect gate="G$1" pin="OUT11" pad="17"/>
<connect gate="G$1" pin="OUT12" pad="18"/>
<connect gate="G$1" pin="OUT13" pad="19"/>
<connect gate="G$1" pin="OUT14" pad="20"/>
<connect gate="G$1" pin="OUT15" pad="21"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="OUT3" pad="7"/>
<connect gate="G$1" pin="OUT4" pad="8"/>
<connect gate="G$1" pin="OUT5" pad="9"/>
<connect gate="G$1" pin="OUT6" pad="10"/>
<connect gate="G$1" pin="OUT7" pad="11"/>
<connect gate="G$1" pin="OUT8" pad="14"/>
<connect gate="G$1" pin="OUT9" pad="15"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="SIN" pad="2"/>
<connect gate="G$1" pin="SOUT" pad="23"/>
<connect gate="G$1" pin="VCC" pad="27"/>
<connect gate="G$1" pin="VPRG" pad="3"/>
<connect gate="G$1" pin="XERR" pad="22"/>
<connect gate="G$1" pin="XLAT" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PWP" package="TSSOP28-GROUNDPAD">
<connects>
<connect gate="G$1" pin="BLANK" pad="2"/>
<connect gate="G$1" pin="DCPRG" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GSCLK" pad="25"/>
<connect gate="G$1" pin="IREF" pad="27"/>
<connect gate="G$1" pin="OUT0" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="8"/>
<connect gate="G$1" pin="OUT10" pad="17"/>
<connect gate="G$1" pin="OUT11" pad="18"/>
<connect gate="G$1" pin="OUT12" pad="19"/>
<connect gate="G$1" pin="OUT13" pad="20"/>
<connect gate="G$1" pin="OUT14" pad="21"/>
<connect gate="G$1" pin="OUT15" pad="22"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="OUT3" pad="10"/>
<connect gate="G$1" pin="OUT4" pad="11"/>
<connect gate="G$1" pin="OUT5" pad="12"/>
<connect gate="G$1" pin="OUT6" pad="13"/>
<connect gate="G$1" pin="OUT7" pad="14"/>
<connect gate="G$1" pin="OUT8" pad="15"/>
<connect gate="G$1" pin="OUT9" pad="16"/>
<connect gate="G$1" pin="SCLK" pad="4"/>
<connect gate="G$1" pin="SIN" pad="5"/>
<connect gate="G$1" pin="SOUT" pad="24"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPRG" pad="6"/>
<connect gate="G$1" pin="XERR" pad="23"/>
<connect gate="G$1" pin="XLAT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAG3110" prefix="U">
<description>3-axis digital (I2C) magnetometer</description>
<gates>
<gate name="G$1" symbol="MAG3110"/>
</gates>
<devices>
<device name="" package="DFN-10">
<connects>
<connect gate="G$1" pin="CAP-A" pad="1"/>
<connect gate="G$1" pin="CAP-R" pad="4"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="INT1" pad="9"/>
<connect gate="G$1" pin="SCL" pad="7"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1704X" prefix="U">
<description>MAX17043/MAX17044: Battery Fuel Guage (43 is 1cell, 44 is 2cell)</description>
<gates>
<gate name="G$1" symbol="MAX1704X"/>
</gates>
<devices>
<device name="" package="TDFN-8">
<connects>
<connect gate="G$1" pin="ALT" pad="5"/>
<connect gate="G$1" pin="CELL" pad="2"/>
<connect gate="G$1" pin="CTG" pad="1"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@EP" pad="EP"/>
<connect gate="G$1" pin="QST" pad="6"/>
<connect gate="G$1" pin="SCL" pad="7"/>
<connect gate="G$1" pin="SDA" pad="8"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMPOT" prefix="R">
<gates>
<gate name="R?" symbol="TRIMPOT"/>
</gates>
<devices>
<device name="SMD" package="TRIMPOT-3MM">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="3362U-2">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="TRIM_POT_PTH">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRIMPOT_PTH_S3_LOCK" package="TRIMPOT_PTH_S3_LOCK">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH-KNOB" package="3386U">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2" package="TRIMPOT_TC33">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM-2" package="TRIMPOT-3MM-2">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA2560" prefix="U">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64/128/256 Kbytes FLASH&lt;p&gt;
4 Kbytes EEPROM&lt;p&gt;
8 Kbytes SRAM&lt;p&gt;
86 General Purpose I/O pins&lt;p&gt;
12-channels16-bit PWM&lt;p&gt;
4 x Serial USARTs&lt;p&gt;
16-channels 10-bit A/D&lt;p&gt;</description>
<gates>
<gate name="1" symbol="ATMEGA2560"/>
</gates>
<devices>
<device name="AU" package="TQFP100">
<connects>
<connect gate="1" pin="(A10)PC2" pad="55"/>
<connect gate="1" pin="(A11)PC3" pad="56"/>
<connect gate="1" pin="(A12)PC4" pad="57"/>
<connect gate="1" pin="(A13)PC5" pad="58"/>
<connect gate="1" pin="(A14)PC6" pad="59"/>
<connect gate="1" pin="(A15)PC7" pad="60"/>
<connect gate="1" pin="(A8)PC0" pad="53"/>
<connect gate="1" pin="(A9)PC1" pad="54"/>
<connect gate="1" pin="(AD0)PA0" pad="78"/>
<connect gate="1" pin="(AD1)PA1" pad="77"/>
<connect gate="1" pin="(AD2)PA2" pad="76"/>
<connect gate="1" pin="(AD3)PA3" pad="75"/>
<connect gate="1" pin="(AD4)PA4" pad="74"/>
<connect gate="1" pin="(AD5)PA5" pad="73"/>
<connect gate="1" pin="(AD6)PA6" pad="72"/>
<connect gate="1" pin="(AD7)PA7" pad="71"/>
<connect gate="1" pin="(ADC0)PF0" pad="97"/>
<connect gate="1" pin="(ADC1)PF1" pad="96"/>
<connect gate="1" pin="(ADC2)PF2" pad="95"/>
<connect gate="1" pin="(ADC3)PF3" pad="94"/>
<connect gate="1" pin="(ADC4/TCK)PF4" pad="93"/>
<connect gate="1" pin="(ADC5/TMS)PF5" pad="92"/>
<connect gate="1" pin="(ADC6/TDO)PF6" pad="91"/>
<connect gate="1" pin="(ADC7/TDI)PF7" pad="90"/>
<connect gate="1" pin="(ALE)PG2" pad="70"/>
<connect gate="1" pin="(CLKO/ICP3/INT7)PE7" pad="9"/>
<connect gate="1" pin="(ICP1)PD4" pad="47"/>
<connect gate="1" pin="(MISO/PCINT3)PB3" pad="22"/>
<connect gate="1" pin="(MOSI/PCINT2)PB2" pad="21"/>
<connect gate="1" pin="(OC0A/OC1C/PCINT7)PB7" pad="26"/>
<connect gate="1" pin="(OC0B)PG5" pad="1"/>
<connect gate="1" pin="(OC1A/PCINT5)PB5" pad="24"/>
<connect gate="1" pin="(OC1B/PCINT6)PB6" pad="25"/>
<connect gate="1" pin="(OC2A/PCINT4)PB4" pad="23"/>
<connect gate="1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="1" pin="(RD)PG1" pad="52"/>
<connect gate="1" pin="(RXD0/PCIN8)PE0" pad="2"/>
<connect gate="1" pin="(RXD1/INT2)PD2" pad="45"/>
<connect gate="1" pin="(SCK/PCINT1)PB1" pad="20"/>
<connect gate="1" pin="(SCL/INT0)PD0" pad="43"/>
<connect gate="1" pin="(SDA/INT1)PD1" pad="44"/>
<connect gate="1" pin="(SS/PCINT0)PB0" pad="19"/>
<connect gate="1" pin="(T0)PD7" pad="50"/>
<connect gate="1" pin="(T1)PD6" pad="49"/>
<connect gate="1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="1" pin="(TOSC1)PG4" pad="29"/>
<connect gate="1" pin="(TOSC2)PG3" pad="28"/>
<connect gate="1" pin="(TXD0)PE1" pad="3"/>
<connect gate="1" pin="(TXD1/INT3)PD3" pad="46"/>
<connect gate="1" pin="(WR)PG0" pad="51"/>
<connect gate="1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="1" pin="(XCK1)PD5" pad="48"/>
<connect gate="1" pin="AGND" pad="99"/>
<connect gate="1" pin="AREF" pad="98"/>
<connect gate="1" pin="AVCC" pad="100"/>
<connect gate="1" pin="GND" pad="11"/>
<connect gate="1" pin="GND1" pad="32"/>
<connect gate="1" pin="GND2" pad="62"/>
<connect gate="1" pin="GND3" pad="81"/>
<connect gate="1" pin="PH0(RXD2)" pad="12"/>
<connect gate="1" pin="PH1(TXD2)" pad="13"/>
<connect gate="1" pin="PH2(XCK2)" pad="14"/>
<connect gate="1" pin="PH3(OC4A)" pad="15"/>
<connect gate="1" pin="PH4(OC4B)" pad="16"/>
<connect gate="1" pin="PH5(OC4C)" pad="17"/>
<connect gate="1" pin="PH6(OC2B)" pad="18"/>
<connect gate="1" pin="PH7(T4)" pad="27"/>
<connect gate="1" pin="PJ0(RXD3/PCINT9)" pad="63"/>
<connect gate="1" pin="PJ1(TXD3/PCINT10)" pad="64"/>
<connect gate="1" pin="PJ2(XCK3/PCINT11)" pad="65"/>
<connect gate="1" pin="PJ3(PCINT12)" pad="66"/>
<connect gate="1" pin="PJ4(PCINT13)" pad="67"/>
<connect gate="1" pin="PJ5(PCINT14)" pad="68"/>
<connect gate="1" pin="PJ6(PCINT15)" pad="69"/>
<connect gate="1" pin="PJ7" pad="79"/>
<connect gate="1" pin="PK0(ADC8/PCINT16)" pad="89"/>
<connect gate="1" pin="PK1(ADC9/PCINT17)" pad="88"/>
<connect gate="1" pin="PK2(ADC10/PCINT18)" pad="87"/>
<connect gate="1" pin="PK3(ADC11/PCINT19)" pad="86"/>
<connect gate="1" pin="PK4(ADC12/PCINT20)" pad="85"/>
<connect gate="1" pin="PK5(ADC13/PCINT21)" pad="84"/>
<connect gate="1" pin="PK6(ADC14/PCINT22)" pad="83"/>
<connect gate="1" pin="PK7(ADC15/PCINT23)" pad="82"/>
<connect gate="1" pin="PL0(ICP4)" pad="35"/>
<connect gate="1" pin="PL1(ICP5)" pad="36"/>
<connect gate="1" pin="PL2(T5)" pad="37"/>
<connect gate="1" pin="PL3(OC5A)" pad="38"/>
<connect gate="1" pin="PL4(OC5B)" pad="39"/>
<connect gate="1" pin="PL5(OC5C)" pad="40"/>
<connect gate="1" pin="PL6" pad="41"/>
<connect gate="1" pin="PL7" pad="42"/>
<connect gate="1" pin="RESET" pad="30"/>
<connect gate="1" pin="VCC" pad="10"/>
<connect gate="1" pin="VCC1" pad="31"/>
<connect gate="1" pin="VCC2" pad="61"/>
<connect gate="1" pin="VCC3" pad="80"/>
<connect gate="1" pin="XTAL1" pad="34"/>
<connect gate="1" pin="XTAL2" pad="33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M08" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 8&lt;/b&gt;
Standard 8-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M08"/>
</gates>
<devices>
<device name="1X08" package="1X08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X08_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X08_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X08_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-8" package="SCREWTERMINAL-3.5MM-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT" package="1X08_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT-ALT" package="1X08_SMD_ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-COMBO" package="1X08_SMD_COMBINED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BM08B-SRSS-TB" package="BM08B-SRSS-TB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIALTAB">
<gates>
<gate name="G$1" symbol="FIDUCIALTAB"/>
</gates>
<devices>
<device name="" package="FIDUCIALTAB">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AHC1G08">
<gates>
<gate name="G$1" symbol="74AHC1G08"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-SOLIDSTATE" prefix="U">
<gates>
<gate name="G$1" symbol="RELAY-SOLIDSTATE"/>
</gates>
<devices>
<device name="PTH" package="RELAY-S108T02">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="4"/>
<connect gate="G$1" pin="T1" pad="1"/>
<connect gate="G$1" pin="T2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOAD_CELL" prefix="J">
<description>&lt;h3&gt;Half-wheatstone bridge Load Cell&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="LOAD_CELL"/>
</gates>
<devices>
<device name="1X03-PTH" package="1X03">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="R" pad="3"/>
<connect gate="G$1" pin="W" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7781" prefix="U">
<description>&lt;h3&gt;AD7781 
20-Bit, Pin-Programmable, Ultralow Power Sigma-Delta ADC &lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="AD7781"/>
</gates>
<devices>
<device name="CRZ" package="SOIC-14">
<connects>
<connect gate="G$1" pin="*PDRST" pad="13"/>
<connect gate="G$1" pin="AIN+" pad="5"/>
<connect gate="G$1" pin="AIN-" pad="6"/>
<connect gate="G$1" pin="AVDD" pad="11"/>
<connect gate="G$1" pin="BPDSW" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="12"/>
<connect gate="G$1" pin="FILTER" pad="14"/>
<connect gate="G$1" pin="GAIN" pad="4"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="REFIN+" pad="7"/>
<connect gate="G$1" pin="REFIN-" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CRUZ" package="TSSOP-16">
<connects>
<connect gate="G$1" pin="*PDRST" pad="14"/>
<connect gate="G$1" pin="AIN+" pad="6"/>
<connect gate="G$1" pin="AIN-" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="12"/>
<connect gate="G$1" pin="BPDSW" pad="10"/>
<connect gate="G$1" pin="DOUT" pad="3"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="FILTER" pad="15"/>
<connect gate="G$1" pin="GAIN" pad="5"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="REFIN+" pad="8"/>
<connect gate="G$1" pin="REFIN-" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RING" prefix="LED">
<description>&lt;h3&gt;16 LED Ring&lt;/h3&gt;

http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Components/LED/Top-Up%20LED%20Ring%20LED-CCL-A.pdf</description>
<gates>
<gate name="G$1" symbol="LED_RING"/>
</gates>
<devices>
<device name="" package="LED_RING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="COM0" pad="COM0"/>
<connect gate="G$1" pin="COM1" pad="COM1"/>
<connect gate="G$1" pin="COM2" pad="COM2"/>
<connect gate="G$1" pin="COM3" pad="COM3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMP36" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="TMP36"/>
</gates>
<devices>
<device name="GT9" package="TO-92">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO-92-KIT" package="TO-92-KIT">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-16X2" prefix="U">
<gates>
<gate name="G$1" symbol="LCD-16X2"/>
</gates>
<devices>
<device name="SILK" package="LCD-16X2">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOSILK" package="LCD-16X2_NOSILK">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLES" package="LCD-16X2_NOHOLES">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8X2" package="LCD-8X2">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8X2-KIT" package="LCD-8X2-KIT">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PHOTOCELL" prefix="R">
<description>&lt;b&gt;Photocell&lt;/b&gt; Also known as a CdS photoresistor. This is a low cost way to detect light levels. Resistance decreases with more incoming light. SparkFun SKU: SEN-09088</description>
<gates>
<gate name="G$1" symbol="PHOTOCELL"/>
</gates>
<devices>
<device name="PTH" package="PHOTOCELL">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-KIT" package="PHOTOCELL-KIT">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Jumper&lt;/b&gt;
Basic 0.1" spaced jumper. Use with breakaway headers.</description>
<gates>
<gate name="A" symbol="JUMPER-2"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NC" package="SJ_2S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="1X02_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO" package="SJ_2S-NO">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO-NS" package="SJ_2S-NO-NS">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M02" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 2&lt;/b&gt;
Standard 2-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08233 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M02"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROCKER" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="1" pad="P$3"/>
<connect gate="G$1" pin="2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-2.54-RA" package="SPRINGTERMINAL-2.54MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_SERIAL_PROGRAM" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="ARDUINO_SERIAL_PROGRAM"/>
</gates>
<devices>
<device name="SMD" package="1X06-SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X06">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX-1X6-RA_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="DTR" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RXI" pad="5"/>
<connect gate="G$1" pin="TXO" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-KIT" package="1X06-KIT">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M06" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 6&lt;/b&gt;
Standard 6-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08094 with associated crimp pins and housings.

NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="SIP" package="1X06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-1X6-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X06-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X06_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX-1X6-RA_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIP_LOCK" package="1X06-SIP_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_LOCK" package="1X06_FEMALE_LOCK.010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X06-SMD_EDGE_FEMALE" package="1X06-SMD_EDGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-6" package="SCREWTERMINAL-3.5MM-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMDF" package="1X06-SMD-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-FEMALE-V2" package="1X06-SMD-FEMALE-V2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X06_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT" package="1X06_SMD_STRAIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT-ALT" package="1X06_SMD_STRAIGHT_ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT-COMBO" package="1X06_SMD_STRAIGHT_COMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EM406" package="EM406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER_2LED" prefix="U">
<description>&lt;H3&gt;Illuminated Rotary Encoder w/ 2 LEDs&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="ENCODER_LED_2-1"/>
</gates>
<devices>
<device name="" package="ENCODER_LED_2">
<connects>
<connect gate="G$1" pin="+G" pad="+G"/>
<connect gate="G$1" pin="+R" pad="+R"/>
<connect gate="G$1" pin="-" pad="GND"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW" pad="SW"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-MEGA" prefix="U">
<description>Arduino Mega footprint connections</description>
<gates>
<gate name="G$1" symbol="ARDUINO-MEGA"/>
</gates>
<devices>
<device name="FULL" package="ARDUINO_MEGA">
<connects>
<connect gate="G$1" pin="0(RX0)" pad="0"/>
<connect gate="G$1" pin="1(TX0)" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14(TX3)" pad="14"/>
<connect gate="G$1" pin="15(RX3)" pad="15"/>
<connect gate="G$1" pin="16(TX2)" pad="16"/>
<connect gate="G$1" pin="17(RX2)" pad="17"/>
<connect gate="G$1" pin="18(TX1)" pad="18"/>
<connect gate="G$1" pin="19(RX1)" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20(SDA)" pad="20"/>
<connect gate="G$1" pin="21(SCL)" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="5V@0" pad="5V@0"/>
<connect gate="G$1" pin="5V@1" pad="5V@1"/>
<connect gate="G$1" pin="5V@2" pad="5V@2"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A0(RX0)" pad="A0"/>
<connect gate="G$1" pin="A1(TX0)" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="GND@4" pad="GND@4"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PRO" package="ARDUINO_MEGA-PRO-3.3V">
<connects>
<connect gate="G$1" pin="0(RX0)" pad="0"/>
<connect gate="G$1" pin="1(TX0)" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14(TX3)" pad="14"/>
<connect gate="G$1" pin="15(RX3)" pad="15"/>
<connect gate="G$1" pin="16(TX2)" pad="16"/>
<connect gate="G$1" pin="17(RX2)" pad="17"/>
<connect gate="G$1" pin="18(TX1)" pad="18"/>
<connect gate="G$1" pin="19(RX1)" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20(SDA)" pad="20"/>
<connect gate="G$1" pin="21(SCL)" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="5V@0" pad="5V@0"/>
<connect gate="G$1" pin="5V@1" pad="5V@1"/>
<connect gate="G$1" pin="5V@2" pad="5V@2"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A0(RX0)" pad="A0"/>
<connect gate="G$1" pin="A1(TX0)" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="GND@4" pad="GND@4"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-DPDT" prefix="S">
<description>DPDT Version of the COM-00597</description>
<gates>
<gate name="G$1" symbol="AYZ0202"/>
</gates>
<devices>
<device name="SMD" package="AYZ0202">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="MSS22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="MS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ES" package="ES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OS" package="OS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EG2211" package="EG2211">
<connects>
<connect gate="G$1" pin="1" pad="P1-TA"/>
<connect gate="G$1" pin="2" pad="P1"/>
<connect gate="G$1" pin="3" pad="P1-TB"/>
<connect gate="G$1" pin="4" pad="P2-TA"/>
<connect gate="G$1" pin="5" pad="P2"/>
<connect gate="G$1" pin="6" pad="P2-TB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GPI" package="GPI-152-3013">
<connects>
<connect gate="G$1" pin="1" pad="10"/>
<connect gate="G$1" pin="2" pad="C@1"/>
<connect gate="G$1" pin="3" pad="20"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="C@2"/>
<connect gate="G$1" pin="6" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDG500" prefix="U">
<gates>
<gate name="G$1" symbol="IDG500-1"/>
</gates>
<devices>
<device name="" package="SPARKFUN_IDG500">
<connects>
<connect gate="G$1" pin="AZ" pad="24"/>
<connect gate="G$1" pin="CPOUT" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="PTATS" pad="23"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
<connect gate="G$1" pin="X4.5IN" pad="5"/>
<connect gate="G$1" pin="X4.5OUT" pad="7"/>
<connect gate="G$1" pin="XAGC" pad="6"/>
<connect gate="G$1" pin="XOUT" pad="1"/>
<connect gate="G$1" pin="Y4.5IN" pad="16"/>
<connect gate="G$1" pin="Y4.5OUT" pad="14"/>
<connect gate="G$1" pin="YAGC" pad="15"/>
<connect gate="G$1" pin="YOUT" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3421E" prefix="U">
<description>USB Peripheral/Host Controller w/ SPI</description>
<gates>
<gate name="G$1" symbol="MAX3421E-1"/>
</gates>
<devices>
<device name="SMD" package="TQFP32-5MM">
<connects>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="20"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GOUT0" pad="4"/>
<connect gate="G$1" pin="GOUT1" pad="5"/>
<connect gate="G$1" pin="GOUT2" pad="6"/>
<connect gate="G$1" pin="GOUT3" pad="7"/>
<connect gate="G$1" pin="GOUT4" pad="8"/>
<connect gate="G$1" pin="GOUT5" pad="9"/>
<connect gate="G$1" pin="GOUT6" pad="10"/>
<connect gate="G$1" pin="GOUT7" pad="11"/>
<connect gate="G$1" pin="GPIN0" pad="26"/>
<connect gate="G$1" pin="GPIN1" pad="27"/>
<connect gate="G$1" pin="GPIN2" pad="28"/>
<connect gate="G$1" pin="GPIN3" pad="29"/>
<connect gate="G$1" pin="GPIN4" pad="30"/>
<connect gate="G$1" pin="GPIN5" pad="31"/>
<connect gate="G$1" pin="GPIN6" pad="32"/>
<connect gate="G$1" pin="GPIN7" pad="1"/>
<connect gate="G$1" pin="GPX" pad="17"/>
<connect gate="G$1" pin="INT" pad="18"/>
<connect gate="G$1" pin="MISO" pad="15"/>
<connect gate="G$1" pin="MOSI" pad="16"/>
<connect gate="G$1" pin="RES" pad="12"/>
<connect gate="G$1" pin="SCK" pad="13"/>
<connect gate="G$1" pin="SS" pad="14"/>
<connect gate="G$1" pin="VBCOMP" pad="22"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VL" pad="2"/>
<connect gate="G$1" pin="X0" pad="25"/>
<connect gate="G$1" pin="X1" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6211*" prefix="U">
<description>TPS62112: 1.5A Step-Down Converter</description>
<gates>
<gate name="G$1" symbol="TPS6211*"/>
</gates>
<devices>
<device name="" package="QFN16-4X4">
<connects>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="FB" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="LBI" pad="7"/>
<connect gate="G$1" pin="LBO" pad="6"/>
<connect gate="G$1" pin="PG" pad="13"/>
<connect gate="G$1" pin="PGND@1" pad="1"/>
<connect gate="G$1" pin="PGND@2" pad="16"/>
<connect gate="G$1" pin="PWPD" pad="EXP"/>
<connect gate="G$1" pin="SW@1" pad="14"/>
<connect gate="G$1" pin="SW@2" pad="15"/>
<connect gate="G$1" pin="SYNC" pad="5"/>
<connect gate="G$1" pin="VIN@1" pad="2"/>
<connect gate="G$1" pin="VIN@2" pad="3"/>
<connect gate="G$1" pin="VINA" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS9110" prefix="U">
<gates>
<gate name="G$1" symbol="RS9110-N-11-22"/>
</gates>
<devices>
<device name="" package="RS9110-N-11-22-SHORT">
<connects>
<connect gate="G$1" pin="CLK" pad="51"/>
<connect gate="G$1" pin="CS" pad="52"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@48" pad="48"/>
<connect gate="G$1" pin="GND@PAD" pad="GND"/>
<connect gate="G$1" pin="INTR" pad="3"/>
<connect gate="G$1" pin="JPD0" pad="42"/>
<connect gate="G$1" pin="JPD1" pad="43"/>
<connect gate="G$1" pin="JPD2" pad="44"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MODE" pad="22"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RX" pad="7"/>
<connect gate="G$1" pin="SD3" pad="6"/>
<connect gate="G$1" pin="TX" pad="5"/>
<connect gate="G$1" pin="VIN@46" pad="46"/>
<connect gate="G$1" pin="VIN@47" pad="47"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor&lt;/b&gt;
Standard 0603 ceramic capacitor, and 0.1" leaded capacitor.</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="PTH" package="CAP-PTH-SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CAP-PTH-SMALL2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CAP-PTH-LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="GRM43D">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-CAP" package="0603-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-CAP" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CAP-PTH-5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="AXIAL-5MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ASMD" package="CTZ3">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="CAP-PTH-SMALL-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SPST" prefix="S" uservalue="yes">
<description>&lt;b&gt;SPST Switch&lt;/b&gt;
Simple slide switch. Spark Fun Electronics SKU : COM-00102</description>
<gates>
<gate name="1" symbol="TOGGLE"/>
</gates>
<devices>
<device name="PTH" package="SWITCH-SPDT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="AYZ0202">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="SWITCHE-DPDT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="R_SW_TH">
<connects>
<connect gate="1" pin="O" pad="P$1"/>
<connect gate="1" pin="P" pad="P$2"/>
<connect gate="1" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="SWITCH-SPDT-SMD">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="SWITCH-SPDT_LOCK.007S">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="SWITCH-SPDT_KIT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-A" package="SWITCH-SPST-SMD-A">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7219">
<gates>
<gate name="G$1" symbol="MAX7219"/>
</gates>
<devices>
<device name="DIP" package="DIL24">
<connects>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="DIG0" pad="2"/>
<connect gate="G$1" pin="DIG1" pad="11"/>
<connect gate="G$1" pin="DIG2" pad="6"/>
<connect gate="G$1" pin="DIG3" pad="7"/>
<connect gate="G$1" pin="DIG4" pad="3"/>
<connect gate="G$1" pin="DIG5" pad="10"/>
<connect gate="G$1" pin="DIG6" pad="5"/>
<connect gate="G$1" pin="DIG7" pad="8"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="24"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND2" pad="9"/>
<connect gate="G$1" pin="ISET" pad="18"/>
<connect gate="G$1" pin="LOAD" pad="12"/>
<connect gate="G$1" pin="SEGA" pad="14"/>
<connect gate="G$1" pin="SEGB" pad="16"/>
<connect gate="G$1" pin="SEGC" pad="20"/>
<connect gate="G$1" pin="SEGD" pad="23"/>
<connect gate="G$1" pin="SEGDP" pad="22"/>
<connect gate="G$1" pin="SEGE" pad="21"/>
<connect gate="G$1" pin="SEGF" pad="15"/>
<connect gate="G$1" pin="SEGG" pad="17"/>
<connect gate="G$1" pin="VCC" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX485">
<gates>
<gate name="G$1" symbol="MAX485"/>
</gates>
<devices>
<device name="DIL" package="DIL08">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RE" pad="2"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HDJD-S822-QR999">
<gates>
<gate name="G$1" symbol="HDJD-S822-QR999"/>
</gates>
<devices>
<device name="" package="QFN-16">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GSBLUE0" pad="11"/>
<connect gate="G$1" pin="GSBLUE1" pad="13"/>
<connect gate="G$1" pin="GSGRN0" pad="3"/>
<connect gate="G$1" pin="GSGRN1" pad="8"/>
<connect gate="G$1" pin="GSRED0" pad="16"/>
<connect gate="G$1" pin="GSRED1" pad="6"/>
<connect gate="G$1" pin="TEST_EN" pad="5"/>
<connect gate="G$1" pin="VBOUT" pad="12"/>
<connect gate="G$1" pin="VDD3" pad="4"/>
<connect gate="G$1" pin="VDD5" pad="1"/>
<connect gate="G$1" pin="VGOUT" pad="10"/>
<connect gate="G$1" pin="VROUT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHPIC" package="QFN-16-(ROUNDED0THERMAL-PAD)">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GSBLUE0" pad="11"/>
<connect gate="G$1" pin="GSBLUE1" pad="13"/>
<connect gate="G$1" pin="GSGRN0" pad="3"/>
<connect gate="G$1" pin="GSGRN1" pad="8"/>
<connect gate="G$1" pin="GSRED0" pad="16"/>
<connect gate="G$1" pin="GSRED1" pad="6"/>
<connect gate="G$1" pin="TEST_EN" pad="5"/>
<connect gate="G$1" pin="VBOUT" pad="12"/>
<connect gate="G$1" pin="VDD3" pad="4"/>
<connect gate="G$1" pin="VDD5" pad="1"/>
<connect gate="G$1" pin="VGOUT" pad="10"/>
<connect gate="G$1" pin="VROUT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RPACK*" prefix="R" uservalue="yes">
<description>BOURNS 4600X series thick-film SIP resistor packs&lt;br&gt;
&lt;br&gt;
Five resistors bussed to a single pin (denoted by dot).&lt;br&gt;
0.2W / resistor&lt;br&gt;
&lt;a href="http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Components/General/4600x.pdf"&gt;datasheet&lt;/a&gt;&lt;br&gt;
&lt;br&gt;
SFE parts COM-10855 (330), COM-10856 (10K)&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="RPACK-BUSSED-5"/>
</gates>
<devices>
<device name="-BUSSED-SIP-PTH-5" package="RPACK-SIP-PTH-5">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_BARGRAPH_10" prefix="D" uservalue="yes">
<description>10-Segment LED Bar Graph&lt;p&gt;
&lt;p&gt;
SFE part numbers:&lt;p&gt;
COM-09935 (red, Vf = 2.1V, Ifmax = 20mA)&lt;br&gt;
COM-09936 (yellow, Vf = 2.1V, Ifmax = 20mA)&lt;br&gt;
COM-09937 (blue, Vf = 3.4V, Ifmax = 20mA)&lt;br&gt;
COM-09938 (green, Vf = 3.4V, Ifmax = 20mA)&lt;br&gt;</description>
<gates>
<gate name="A" symbol="LED_BARGRAPH_10"/>
<gate name="B" symbol="LED_BARGRAPH_10"/>
<gate name="C" symbol="LED_BARGRAPH_10"/>
<gate name="D" symbol="LED_BARGRAPH_10"/>
<gate name="E" symbol="LED_BARGRAPH_10"/>
<gate name="F" symbol="LED_BARGRAPH_10"/>
<gate name="G" symbol="LED_BARGRAPH_10"/>
<gate name="H" symbol="LED_BARGRAPH_10"/>
<gate name="I" symbol="LED_BARGRAPH_10"/>
<gate name="J" symbol="LED_BARGRAPH_10"/>
</gates>
<devices>
<device name="" package="LED_BARGAPH_10">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="C" pad="20"/>
<connect gate="B" pin="A" pad="2"/>
<connect gate="B" pin="C" pad="19"/>
<connect gate="C" pin="A" pad="3"/>
<connect gate="C" pin="C" pad="18"/>
<connect gate="D" pin="A" pad="4"/>
<connect gate="D" pin="C" pad="17"/>
<connect gate="E" pin="A" pad="5"/>
<connect gate="E" pin="C" pad="16"/>
<connect gate="F" pin="A" pad="6"/>
<connect gate="F" pin="C" pad="15"/>
<connect gate="G" pin="A" pad="7"/>
<connect gate="G" pin="C" pad="14"/>
<connect gate="H" pin="A" pad="8"/>
<connect gate="H" pin="C" pad="13"/>
<connect gate="I" pin="A" pad="9"/>
<connect gate="I" pin="C" pad="12"/>
<connect gate="J" pin="A" pad="10"/>
<connect gate="J" pin="C" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM811" prefix="U">
<description>&lt;h3&gt;STM811 Reset Circuit&lt;/h3&gt;
Used in the Ethernet Shield</description>
<gates>
<gate name="G$1" symbol="STM811"/>
</gates>
<devices>
<device name="" package="SOT143">
<connects>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="~MR" pad="3"/>
<connect gate="G$1" pin="~RST" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGJACK-POE" prefix="U">
<description>&lt;h3&gt;PoE compatible MagJack&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="MAGJACK-POE"/>
</gates>
<devices>
<device name="" package="MAGJACK-POE">
<connects>
<connect gate="G$1" pin="GLED+" pad="13"/>
<connect gate="G$1" pin="GLED-" pad="14"/>
<connect gate="G$1" pin="RCT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD@0" pad="GND0"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND1"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="5"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
<connect gate="G$1" pin="YLED+" pad="11"/>
<connect gate="G$1" pin="YLED-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCNL4000" prefix="U">
<description>&lt;h3&gt;VNCL4000&lt;/h3&gt;
Fully integrated proximity and ambient light sensor with infrared emitter and I2C interface&lt;br&gt;
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="VCNL4000"/>
</gates>
<devices>
<device name="" package="VCNL4000">
<connects>
<connect gate="G$1" pin="GND@0" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="IR+" pad="1"/>
<connect gate="G$1" pin="IR-@0" pad="2"/>
<connect gate="G$1" pin="IR-@1" pad="3"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE555" prefix="IC">
<description>&lt;b&gt;General purpose bipolar Timer&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="NE555"/>
</gates>
<devices>
<device name="P" package="DIL-08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="NE555N"/>
<attribute name="OC_FARNELL" value="1467742"/>
<attribute name="OC_NEWARK" value="89K1486"/>
</technology>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VENUS638FLPX-L" prefix="U">
<description>&lt;b&gt;Venus638FLPX-L GPS Receiver&lt;/b&gt;&lt;p&gt;

Venus638FLPx is a high performance, low cost, single
chip GPS receiver targeting mobile consumer and cellular
handset applications. It offers very low power
consumption, high sensitivity, and best in class signal
acquisition and time-to-first-fix performance.&lt;p&gt;
Venus638FLPx contains all the necessary components of
a complete GPS receiver, includes 1.2dB cascaded
system NF RF front-end, GPS baseband signal processor,
0.5ppm TCXO, 32.768kHz RTC crystal, RTC LDO
regulator, and passive components. It requires very low
external component count and takes up only 100mm2
PCB footprint.&lt;p&gt;
Dedicated massive-correlator signal parameter search
engine within the baseband enables rapid search of all the
available satellites and acquisition of very weak signal. An
advanced track engine allows weak signal tracking and
positioning in harsh environments such as urban canyons
and under deep foliage. The self-contained architecture keeps GPS processing off
the host and allows integration into applications with very
little resource.&lt;p&gt;
FEATURES&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;20Hz update rate&lt;/li&gt;
&lt;li&gt;-148dBm cold start sensitivity&lt;/li&gt;
&lt;li&gt;-165dBm tracking sensitivity&lt;/li&gt;
&lt;li&gt;29 second cold start TTFF&lt;/li&gt;
&lt;li&gt;3.5 second TTFF with AGPS&lt;/li&gt;
&lt;li&gt;1 second hot start&lt;/li&gt;
&lt;li&gt;2.5m accuracy&lt;/li&gt;
&lt;li&gt;Multipath detection and suppression&lt;/li&gt;
&lt;li&gt;Jamming detection and mitigation&lt;/li&gt;
&lt;li&gt;SBAS (WAAS / EGNOS) support&lt;/li&gt;
&lt;li&gt;7-day extended ephemeris AGPS&lt;/li&gt;
&lt;li&gt;67mW full power navigation&lt;/li&gt;
&lt;li&gt;Works directly with active or passive antenna&lt;/li&gt;
&lt;li&gt;Internal flash for optional 75K point data logging&lt;/li&gt;
&lt;li&gt;Supports external SPI flash memory data logging&lt;/li&gt;
&lt;li&gt;Complete receiver in 10mm x 10mm x 1.3mm size&lt;/li&gt;
&lt;li&gt;Contains LNA, SAW Filter, TCXO, RTC Xtal, LDO&lt;/li&gt;
&lt;li&gt;Pb-free RoHS compliant&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="VENUS638FLPX-L"/>
</gates>
<devices>
<device name="" package="VENUS638FLPX">
<connects>
<connect gate="G$1" pin="BTSEL" pad="9"/>
<connect gate="G$1" pin="CLK" pad="41"/>
<connect gate="G$1" pin="CSN" pad="43"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@49" pad="49"/>
<connect gate="G$1" pin="GND@60" pad="60"/>
<connect gate="G$1" pin="GND@64" pad="64"/>
<connect gate="G$1" pin="GNDRF@21" pad="21"/>
<connect gate="G$1" pin="GNDRF@22" pad="22"/>
<connect gate="G$1" pin="GNDRF@24" pad="24"/>
<connect gate="G$1" pin="GNDRF@25" pad="25"/>
<connect gate="G$1" pin="GNDRF@27" pad="27"/>
<connect gate="G$1" pin="GNDRF@28" pad="28"/>
<connect gate="G$1" pin="GNDRF@29" pad="29"/>
<connect gate="G$1" pin="GNDRF@31" pad="31"/>
<connect gate="G$1" pin="GNDRF@33" pad="33"/>
<connect gate="G$1" pin="GNDRF@61" pad="61"/>
<connect gate="G$1" pin="GNDRF@62" pad="62"/>
<connect gate="G$1" pin="GNDRF@65" pad="65"/>
<connect gate="G$1" pin="GNDRF@69" pad="69"/>
<connect gate="G$1" pin="GPIO1" pad="6"/>
<connect gate="G$1" pin="GPIO2" pad="5"/>
<connect gate="G$1" pin="GPIO20" pad="14"/>
<connect gate="G$1" pin="GPIO22" pad="12"/>
<connect gate="G$1" pin="GPIO23" pad="13"/>
<connect gate="G$1" pin="GPIO24" pad="8"/>
<connect gate="G$1" pin="GPIO25" pad="53"/>
<connect gate="G$1" pin="GPIO28" pad="59"/>
<connect gate="G$1" pin="GPIO29" pad="16"/>
<connect gate="G$1" pin="GPIO3" pad="48"/>
<connect gate="G$1" pin="GPIO30" pad="54"/>
<connect gate="G$1" pin="GPIO4" pad="47"/>
<connect gate="G$1" pin="GPIO6" pad="63"/>
<connect gate="G$1" pin="LED/GPIO0" pad="7"/>
<connect gate="G$1" pin="MISO" pad="39"/>
<connect gate="G$1" pin="MOSI" pad="38"/>
<connect gate="G$1" pin="PIO11" pad="51"/>
<connect gate="G$1" pin="PIO12" pad="4"/>
<connect gate="G$1" pin="PIO14" pad="37"/>
<connect gate="G$1" pin="PIO15" pad="55"/>
<connect gate="G$1" pin="PIO5" pad="50"/>
<connect gate="G$1" pin="PPS" pad="40"/>
<connect gate="G$1" pin="REGEN" pad="36"/>
<connect gate="G$1" pin="RFIN" pad="32"/>
<connect gate="G$1" pin="RSTN" pad="1"/>
<connect gate="G$1" pin="RTC" pad="17"/>
<connect gate="G$1" pin="RXD0" pad="42"/>
<connect gate="G$1" pin="RXD1" pad="52"/>
<connect gate="G$1" pin="SCL" pad="46"/>
<connect gate="G$1" pin="SDA" pad="45"/>
<connect gate="G$1" pin="TXD0" pad="44"/>
<connect gate="G$1" pin="TXD1" pad="57"/>
<connect gate="G$1" pin="VBAT" pad="18"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VCC@58" pad="58"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5007" prefix="U">
<description>&lt;h3&gt;LM5007&lt;/h3&gt;
High Voltage (80V) Step-down switching regulator&lt;br&gt;

http://www.national.com/ds/LM/LM5007.pdf&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="LM5007"/>
</gates>
<devices>
<device name="" package="MSOP-8-EP">
<connects>
<connect gate="G$1" pin="BST" pad="2"/>
<connect gate="G$1" pin="EP" pad="EP"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="RCL" pad="3"/>
<connect gate="G$1" pin="RON" pad="6"/>
<connect gate="G$1" pin="RTN" pad="4"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5574" prefix="U">
<description>&lt;h3&gt;LM5574&lt;/h3&gt;
Simple Switcher 75V, 0.5A Step-down switching regulator</description>
<gates>
<gate name="G$1" symbol="LM5574"/>
</gates>
<devices>
<device name="" package="TSSOP-16">
<connects>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="BST" pad="16"/>
<connect gate="G$1" pin="COMP" pad="5"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="IS" pad="13"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="PGND" pad="12"/>
<connect gate="G$1" pin="PRE" pad="15"/>
<connect gate="G$1" pin="RAMP" pad="8"/>
<connect gate="G$1" pin="RT" pad="7"/>
<connect gate="G$1" pin="SD" pad="2"/>
<connect gate="G$1" pin="SS" pad="10"/>
<connect gate="G$1" pin="SW" pad="14"/>
<connect gate="G$1" pin="SYNC" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<description>&lt;b&gt;Inductors&lt;/b&gt;
Basic Inductor/Choke - 0603 and 1206. Footprints are not proven and vary greatly between part numbers.</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="H*" package="INDUCTOR-1206">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="1206"/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR54" package="CR54">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PWR" package="CDRH125">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B82462G" package="B82462G">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR75" package="CR75">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1007" package="1007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="COOPER_UP4B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-" package="CDRH3D28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR75_V2" package="CR75_V2">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="." package="CDRH2D09">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NPI75" package="NPI75C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SRU5028" package="SRU5028">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SRU1038" package="SRU1038">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR54-KIT" package="CR54-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;b&gt;Diode&lt;/b&gt;
These are standard reverse protection diodes and small signal diodes. SMA package can handle up to about 1A. SOD-323 can handle about 200mA. What the SOD-323 package when ordering, there are some mfgs out there that are 5-pin packages.</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="SMA" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="DIODE-1N4001">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1N4148" package="DIODE-1N4148">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMB" package="SMB-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HV" package="DIODE-HV">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMA-ALT" package="SMA-DIODE_ALT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMA-KIT" package="SMA-DIODE-KIT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_POL" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor Polarized&lt;/b&gt;
These are standard SMD and PTH capacitors. Normally 10uF, 47uF, and 100uF in electrolytic and tantalum varieties. Always verify the external diameter of the through hole cap, it varies with capacity, voltage, and manufacturer. The EIA devices should be standard.</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="1206" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CPOL-RADIAL-100UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CPOL-RADIAL-10UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="7343" package="EIA7343">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F80" package="NIPPON_F80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CPOL-RADIAL-1000UF-63V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="CPOL-RADIAL-1000UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="VISHAY_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H13" package="PANASONIC_H13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6032" package="EIA6032">
<connects>
<connect gate="G$1" pin="+" pad="P$1"/>
<connect gate="G$1" pin="-" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EN_J2" package="EN_J2">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528-KIT" package="EIA3528-KIT">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206-KIT" package="EIA3216-KIT">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUZZER" prefix="SG">
<description>&lt;b&gt;Buzzer 12mm&lt;/b&gt;
Spark Fun Electronics SKU : Comp-Buzzer</description>
<gates>
<gate name="G$1" symbol="BUZZER"/>
</gates>
<devices>
<device name="PTH" package="BUZZER-12MM">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="BUZZER-CMT1603">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="BUZZER-CCV">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD3" package="BUZZER-CMT1102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NS" package="BUZZER-12MM-NS">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-NS-KIT" package="BUZZER-12MM-NS-KIT">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2-KIT" package="BUZZER-CCV-KIT">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA8452Q" prefix="U">
<description>&lt;h3&gt;MMA8452Q 3-Axis, 12/8-bit Digital Accelerometer&lt;/h3&gt;
&lt;ul&gt;
&lt;li&gt;&lt;B&gt;Supply Voltage:&lt;/b&gt; 1.6-3.6V&lt;/li&gt;
&lt;li&gt;&lt;B&gt;Range:&lt;/b&gt; +/- 2g, 4g, 8g&lt;/li&gt;
&lt;li&gt;&lt;B&gt;Interface:&lt;/b&gt; I&lt;sup&gt;2&lt;/sup&gt;C, 12-bit and 8-bit&lt;/li&gt;
&lt;li&gt;&lt;b&gt;ODR:&lt;/b&gt; 1.56 Hz - 800 Hz&lt;/li&gt;
&lt;li&gt;&lt;B&gt;Package:&lt;/b&gt; QFN-16&lt;/li&gt;
&lt;/ul&gt;
&lt;br&gt;
&lt;br&gt;
http://cache.freescale.com/files/sensors/doc/data_sheet/MMA8452Q.pdf</description>
<gates>
<gate name="G$1" symbol="MMA8452Q"/>
</gates>
<devices>
<device name="" package="QFN-16_0.5MM">
<connects>
<connect gate="G$1" pin="BYP" pad="2"/>
<connect gate="G$1" pin="GND@0" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="SA0" pad="7"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6675">
<gates>
<gate name="G$1" symbol="MAX6675"/>
</gates>
<devices>
<device name="" package="SO08-MAX6675">
<connects>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="556">
<gates>
<gate name="G$1" symbol="556_TIMER_DUAL"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="CV" pad="3"/>
<connect gate="G$1" pin="CV2" pad="11"/>
<connect gate="G$1" pin="DIS" pad="1"/>
<connect gate="G$1" pin="DIS2" pad="13"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RST2" pad="10"/>
<connect gate="G$1" pin="THR" pad="2"/>
<connect gate="G$1" pin="THR2" pad="12"/>
<connect gate="G$1" pin="TRIG" pad="6"/>
<connect gate="G$1" pin="TRIG2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFM22">
<description>&lt;b&gt;Description:&lt;/b&gt; The RFM22 is a low-power, low cost radio that is capable of operating in the 434MHz and 900MHz open bands. It's frequency is software defined and there are some very good libraries written for it.</description>
<gates>
<gate name="G$1" symbol="RFM22"/>
</gates>
<devices>
<device name="SMD" package="RFM22-XXX-S2">
<connects>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="16"/>
<connect gate="G$1" pin="GPIO0" pad="6"/>
<connect gate="G$1" pin="GPIO1" pad="7"/>
<connect gate="G$1" pin="GPIO2" pad="8"/>
<connect gate="G$1" pin="NIRQ" pad="14"/>
<connect gate="G$1" pin="NSEL" pad="13"/>
<connect gate="G$1" pin="RXANT" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="12"/>
<connect gate="G$1" pin="SDI" pad="11"/>
<connect gate="G$1" pin="SDN" pad="15"/>
<connect gate="G$1" pin="SDO" pad="10"/>
<connect gate="G$1" pin="TXANT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32U4">
<gates>
<gate name="G$1" symbol="ATMEGA32U4"/>
</gates>
<devices>
<device name="QFN" package="QFN-44">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN2" package="QFN-44-NOPAD">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANDROID-ELECTRIC_SHEEP_LOGO">
<gates>
<gate name="G$1" symbol="ANDROID-ELECTRIC_SHEEP_LOGO"/>
</gates>
<devices>
<device name="_" package="ANDROID-ELECTRIC_SHEEP_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="ANDROID-ELECTRIC_SHEEP_LOGO_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM386" prefix="U">
<description>low voltage audio power amplifier</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="" package="DIP08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GP-2106" prefix="U">
<description>GP-2106 GPS SiRF IV</description>
<gates>
<gate name="G$1" symbol="GP-2106"/>
</gates>
<devices>
<device name="" package="GP-2106">
<connects>
<connect gate="G$1" pin="1PPS" pad="1PPS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ONOFF" pad="ONOFF"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT_SWITCH" prefix="U" uservalue="yes">
<description>Potentiometer w/ switch.</description>
<gates>
<gate name="G$1" symbol="POT"/>
<gate name="G$2" symbol="SWITCH-MOMENTARY-2-1"/>
</gates>
<devices>
<device name="" package="POT_PTH">
<connects>
<connect gate="G$1" pin="A" pad="E@1"/>
<connect gate="G$1" pin="E" pad="E@2"/>
<connect gate="G$1" pin="S" pad="WAND"/>
<connect gate="G$2" pin="1" pad="S1"/>
<connect gate="G$2" pin="2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_MIC5235" prefix="U">
<gates>
<gate name="G$1" symbol="V-REG-LDO-ADJ"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SP3T" prefix="S" uservalue="yes">
<gates>
<gate name="G$1" symbol="SWITCH-SP3T"/>
</gates>
<devices>
<device name="" package="SWITCH-SP3T-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*08" prefix="U">
<gates>
<gate name="G$1" symbol="74AHC1G08"/>
</gates>
<devices>
<device name="SE" package="SOT353">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*32" prefix="U">
<description>Single 2-input OR gate</description>
<gates>
<gate name="G$1" symbol="OR-SINGLE"/>
</gates>
<devices>
<device name="SE" package="SOT353">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HT8950">
<gates>
<gate name="G$1" symbol="HT8950"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="AIN" pad="6"/>
<connect gate="G$1" pin="AO" pad="5"/>
<connect gate="G$1" pin="AUDIO" pad="9"/>
<connect gate="G$1" pin="FVIB" pad="12"/>
<connect gate="G$1" pin="LAMP" pad="8"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="13"/>
<connect gate="G$1" pin="ROB" pad="18"/>
<connect gate="G$1" pin="SW0" pad="1"/>
<connect gate="G$1" pin="SW1" pad="2"/>
<connect gate="G$1" pin="SW2" pad="3"/>
<connect gate="G$1" pin="TGD" pad="17"/>
<connect gate="G$1" pin="TGU" pad="16"/>
<connect gate="G$1" pin="TS" pad="11"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VIB" pad="15"/>
<connect gate="G$1" pin="VREF" pad="10"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P8X32A-Q44">
<gates>
<gate name="P" symbol="4VDD4VSS"/>
<gate name="P8X32A-Q44" symbol="P8X32A"/>
</gates>
<devices>
<device name="" package="P8X32A-Q44">
<connects>
<connect gate="P" pin="VDD@1" pad="8"/>
<connect gate="P" pin="VDD@2" pad="18"/>
<connect gate="P" pin="VDD@3" pad="30"/>
<connect gate="P" pin="VDD@4" pad="40"/>
<connect gate="P" pin="VSS@1" pad="5"/>
<connect gate="P" pin="VSS@2" pad="17"/>
<connect gate="P" pin="VSS@3" pad="27"/>
<connect gate="P" pin="VSS@4" pad="39"/>
<connect gate="P8X32A-Q44" pin="BOE/" pad="6"/>
<connect gate="P8X32A-Q44" pin="P0" pad="41"/>
<connect gate="P8X32A-Q44" pin="P1" pad="42"/>
<connect gate="P8X32A-Q44" pin="P10" pad="11"/>
<connect gate="P8X32A-Q44" pin="P11" pad="12"/>
<connect gate="P8X32A-Q44" pin="P12" pad="13"/>
<connect gate="P8X32A-Q44" pin="P13" pad="14"/>
<connect gate="P8X32A-Q44" pin="P14" pad="15"/>
<connect gate="P8X32A-Q44" pin="P15" pad="16"/>
<connect gate="P8X32A-Q44" pin="P16" pad="19"/>
<connect gate="P8X32A-Q44" pin="P17" pad="20"/>
<connect gate="P8X32A-Q44" pin="P18" pad="21"/>
<connect gate="P8X32A-Q44" pin="P19" pad="22"/>
<connect gate="P8X32A-Q44" pin="P2" pad="43"/>
<connect gate="P8X32A-Q44" pin="P20" pad="23"/>
<connect gate="P8X32A-Q44" pin="P21" pad="24"/>
<connect gate="P8X32A-Q44" pin="P22" pad="25"/>
<connect gate="P8X32A-Q44" pin="P23" pad="26"/>
<connect gate="P8X32A-Q44" pin="P24" pad="31"/>
<connect gate="P8X32A-Q44" pin="P25" pad="32"/>
<connect gate="P8X32A-Q44" pin="P26" pad="33"/>
<connect gate="P8X32A-Q44" pin="P27" pad="34"/>
<connect gate="P8X32A-Q44" pin="P28" pad="35"/>
<connect gate="P8X32A-Q44" pin="P29" pad="36"/>
<connect gate="P8X32A-Q44" pin="P3" pad="44"/>
<connect gate="P8X32A-Q44" pin="P30" pad="37"/>
<connect gate="P8X32A-Q44" pin="P31" pad="38"/>
<connect gate="P8X32A-Q44" pin="P4" pad="1"/>
<connect gate="P8X32A-Q44" pin="P5" pad="2"/>
<connect gate="P8X32A-Q44" pin="P6" pad="3"/>
<connect gate="P8X32A-Q44" pin="P7" pad="4"/>
<connect gate="P8X32A-Q44" pin="P8" pad="9"/>
<connect gate="P8X32A-Q44" pin="P9" pad="10"/>
<connect gate="P8X32A-Q44" pin="RES/" pad="7"/>
<connect gate="P8X32A-Q44" pin="XI" pad="28"/>
<connect gate="P8X32A-Q44" pin="XO" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR-ARRAY" prefix="R" uservalue="yes">
<description>&lt;b&gt;Array Chip Resistor&lt;/b&gt;&lt;p&gt;
Source: RS Component / Phycomp</description>
<gates>
<gate name="A" symbol="RESISTOR-1"/>
<gate name="B" symbol="RESISTOR-1"/>
<gate name="C" symbol="RESISTOR-1"/>
<gate name="D" symbol="RESISTOR-1"/>
</gates>
<devices>
<device name="0603-ARV" package="0603-ARV">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER_RGB_CA" prefix="SW" uservalue="yes">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ RGB LED and select switch&lt;/h3&gt;

EC12PLRGBSDVBF-D: http://top-up.so-buy.com/front/bin/ptdetail.phtml?Part=EC12PLRGBSDVBF-D</description>
<gates>
<gate name="G$1" symbol="ENCODER_LED_3_CA"/>
</gates>
<devices>
<device name="" package="ENCODER_LED_3">
<connects>
<connect gate="G$1" pin="+" pad="5"/>
<connect gate="G$1" pin="-B" pad="4"/>
<connect gate="G$1" pin="-G" pad="2"/>
<connect gate="G$1" pin="-R" pad="1"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
