<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="S44">
<description>&lt;B&gt;Throughhole Plastic J-Leaded Chip Carrier Socket&lt;/B&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;B&gt;Plastic J-Leaded Chip Carrier&lt;/B&gt;</description>
</package>
<package name="PLCC-SM44">
<description>&lt;B&gt;SMD Plastic J-Leaded Chip Carrier Socket&lt;/B&gt;</description>
</package>
<package name="SSOP20D8">
<description>&lt;B&gt;Plastic Shrink Small Outline Package&lt;/B&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="SO20L">
<description>&lt;B&gt;Small Outline Package&lt;/B&gt; SOIC 0.300"</description>
</package>
<package name="TQFP48">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="SOIC20S">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="LOGO">
<description>&lt;B&gt;Logo&lt;/B&gt;</description>
</package>
<package name="PQFP44">
<description>&lt;B&gt;Plastic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="PLCC32R">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
rectangle</description>
</package>
<package name="TSOP32">
<description>&lt;b&gt;TSOP32&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
<package name="DIL32">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO32X">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
extra wide body 8.9 mm/JEDEC MO-120AC</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="PSSO20">
<description>&lt;b&gt;PSSO20&lt;/b&gt;</description>
</package>
<package name="TQFP144">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PLCC52">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="SSOP24">
<description>&lt;b&gt; SSOP 24&lt;/b&gt;&lt;p&gt;
Source: Uploaded by Heiko Künzel &lt;heiko.kuenzel@atg-gera.de&gt; from ATG Automatisierungstechnik Gera&lt;br&gt;
Mon Mar 10 13:32:48 2003 Atmel-Library mit zusätzlich T83C5121-Prozessor im SSOP24-Package.&lt;br&gt;
Package centre and &amp;lt;NAME &amp; &amp;lt;VALUE placed by librarian@cadsoft.de.</description>
</package>
<package name="PLCC84">
<description>&lt;b&gt;Plastic J-Lead Chip Carrier&lt;/b&gt;</description>
</package>
<package name="TQFP80">
<description>&lt;b&gt;TQFP 80&lt;/b&gt; thin quad flat pack&lt;p&gt;
Source: www.atmwel.com .. doc4109.pdf</description>
</package>
<package name="BGA81">
<description>&lt;b&gt;Ball Grid Array&lt;/b&gt; 81 leads&lt;p&gt;
Source: www.atmwel.com .. doc4109.pdf</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AB&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="SO24W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AA&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="PLCC28">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="VQFP32">
<description>&lt;b&gt;Quad Flat Pack&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="LFBGA256_A_291X326">
<description>Auto generated by &lt;b&gt;make-symbol-device-package(bsdl).ulp&lt;/b&gt;&lt;p&gt;Source: at91rm9200_bga.bsd</description>
</package>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="PLCC20">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;</description>
</package>
<package name="MLF64">
<description>&lt;b&gt;64M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="TQFP64">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;&lt;p&gt;
Updated from atml.lbr 17.01.2005 alf@cadsoft.de</description>
</package>
<package name="VQFP64">
<description>&lt;b&gt;64-lead VQVP&lt;/b&gt;&lt;p&gt;
Source. http://www.atmel.com/dyn/resources/prod_documents/doc4136.pdf</description>
</package>
<package name="MLF64-TH">
<description>&lt;b&gt;64M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF32-TH">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF16-TH">
<description>&lt;b&gt;HP-VFQFP-N16&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF20-5X5-TH">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; QFN 20  -5  x 5 mm Micro Lead Frame package (MLF)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4533.pdf</description>
</package>
<package name="MLF16">
<description>&lt;b&gt;HP-VFQFP-N16&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF20-5X5">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; 5 x 5 mm Micro Lead Frame package (MLF)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4533.pdf</description>
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF44">
<description>&lt;b&gt;44M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="QFN44ML8X8">
<description>&lt;b&gt;44-Lead Plastic Quad Flat No Lead Package (ML)&lt;/b&gt; 8x8 mm Body (QFN)&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
</package>
<package name="LQFP100">
<description>&lt;b&gt;LQFP 100&lt;/b&gt;&lt;p&gt;
Source: 6120s.pdf</description>
</package>
<package name="TFBGA100">
<description>&lt;b&gt;TFBGA 100&lt;/b&gt;&lt;p&gt;
Source: 6120s.pdf</description>
</package>
<package name="TSSOP8">
<description>&lt;b&gt;8A2-TSSOP&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc5089.pdf</description>
</package>
<package name="10M1">
<description>&lt;b&gt;10M1&lt;/b&gt; 10-pad, 3 x 3 x 1.0 mm Body&lt;p&gt;
Lead Pitch 0.50 mm, 1.64 x 2.60 mm Exposed Pad, Micro Lead Frame Package&lt;br&gt;
MLF10, QFN10&lt;/b&gt;&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
<package name="8S2">
<description>&lt;b&gt;8S2&lt;/b&gt; 8-lead, 0.208 Body&lt;p&gt;
Plastic Small Outline Package (EIAJ)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
<package name="8S1">
<description>&lt;b&gt;8S1&lt;/b&gt; 8-lead (0.150" Wide Body)&lt;p&gt;
Plastic Gull Wing Small Outline (JEDEC SOIC)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
<package name="20M1">
<description>&lt;b&gt;20M1&lt;/b&gt; 20-pad, 4 x 4 x 0.8 mm Body&lt;p&gt;
Lead Pitch 0.50 mm, 2.6 mm Exposed Pad, Micro Lead Frame Package (MLF)&lt;br&gt;

Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
<package name="TQFP44">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="MLF44-TH">
<description>&lt;b&gt;44M1&lt;/b&gt; Micro Lead Frame package (MLF)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2593.pdf</description>
</package>
<package name="TQFP100">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="64M1">
<description>&lt;b&gt;64M1&lt;/b&gt;&lt;p&gt; 64-pad, 9 x 9 x 1.0 mm&lt;p&gt;
 Lead Pitch 0.50 mm, 5.40 mm Exposed Pad, Micro Lead Frame Package (MLF)&lt;br&gt;
Source: http://www.atmel.com .. doc8023.pdf</description>
</package>
<package name="28T-TSOP-1">
<description>&lt;b&gt;28T&lt;/b&gt; 28-lead (8 x 13.4 mm) Plastic Thin Small Outline Type I (TSOP)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc3542.pdf</description>
</package>
<package name="VDFN-8">
<description>&lt;b&gt;8M1-A-MLF (VDFN)&lt;/b&gt; 6 x 5 mm&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc3500.pdf</description>
</package>
<package name="VQFN64-9X9X1">
</package>
<package name="LQFP144">
<description>LQFP144 Package</description>
</package>
<package name="TQFP64-10X10">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="AVR-JTAG-10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 10 Pin, 0.1" Straight</description>
</package>
<package name="AVR-JTAG-10R">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 10 Pin, 0.1" Right Angle</description>
</package>
<package name="PQFN64-1">
<description>&lt;b&gt;Plastic Quad Flat Non-leaded package&lt;/b&gt; 64 pins, 9 × 9 × 0.85 mm³, 0.5 mm pitch&lt;p&gt;
Source: https://www.micronas.com .. mas35x9f_3ds.pdf</description>
</package>
<package name="PDIP08_300MIL">
<description>&lt;b&gt;DIL08 300mil&lt;/b&gt;</description>
</package>
<package name="SOIC8_EIAJ_208MIL">
<description>&lt;B&gt;Small Outline Medium Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
208-mil body</description>
</package>
<package name="SOIC08_JEDEC_150MIL">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body</description>
</package>
<package name="TSSOP8_4MM4">
<description>&lt;b&gt;TSSOP 8-lead, 4.4mm&lt;/b&gt;</description>
</package>
<package name="TQFP-44A-44">
<description>&lt;b&gt;44A&lt;/b&gt;, 44-lead, 10 x 10 mm Body Size, 1.0 mm Body Thickness, 0.8 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP)</description>
</package>
<package name="MLF-(VQFN)-44M1-44">
<description>&lt;b&gt;44M1&lt;/b&gt;, 44-pad, 7 x 7 x 1.0 mm Body, Lead Pitch 0.50 mm, 5.20 mm Exposed Pad, Thermally Enhanced Plastic Very Thin Quad Flat No Lead Package (VQFN)</description>
</package>
<package name="VFBGA-49C2-49">
<description>&lt;b&gt;49C2&lt;/b&gt;, 49-ball (7 x 7 Array), 0.65 mm Pitch, 5.0 x 5.0 x 1.0 mm, Very Thin, Fine-Pitch Ball Grid Array Package (VFBGA)</description>
</package>
<package name="TQFP-100A-100">
<description>&lt;b&gt;100A&lt;/b&gt;, 100-lead, 14 x 14 mm Body Size, 1.0 mm Body Thickness,
0.5 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP)</description>
</package>
<package name="CBGA-100C1-100">
<description>&lt;b&gt;100C1&lt;/b&gt;, 100-ball, 9 x 9 x 1.2 mm Body, Ball Pitch 0.80 mm Chip Array BGA Package (CBGA)</description>
</package>
<package name="VFBGA-100C2-100">
<description>&lt;b&gt;100C2&lt;/b&gt;, 100-ball (10 x 10 Array), 0.65 mm Pitch, 7.0 x 7.0 x 1.0 mm, Very Thin, Fine-Pitch Ball Grid Array Package (VFBGA)</description>
</package>
<package name="TQFP-64A-64">
<description>&lt;b&gt;64A&lt;/b&gt;, 64-lead, 14 x 14 mm Body Size, 1.0 mm Body Thickness, 0.8 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP)</description>
</package>
<package name="MLF-(VQFN)-64M2-64">
<description>&lt;b&gt;64M2&lt;/b&gt;, 64-pad, 9 x 9 x 1.0 mm Body, Lead Pitch 0.50 mm, 7.65 mm Exposed Pad, Micro Lead Frame Package (MLF)</description>
</package>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
<package name="AVR-ISP-6R">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; AVR ISP 6 Pin, 0.1" Right Angle</description>
</package>
<package name="6PAD_ISP">
</package>
<package name="AVR-ISP-10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; AVR ISP 10 Pin, 0.1" Straight</description>
</package>
<package name="AVR-ISP-10R">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; AVR ISP 10 Pin, 0.1" Right Angle</description>
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="QFN/MLF20">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="SO20L$">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
<package name="MLF20">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="JTAG-ARM">
</package>
<package name="PAK100/2500-20">
<description>&lt;b&gt;3M (TM) Pak 100 4-Wall Header&lt;/b&gt; Straight&lt;p&gt;
Source: 3M</description>
</package>
<package name="5103309-5">
<description>VERTICAL HEADER&lt;p&gt;
20 position</description>
</package>
<package name="CABGA324">
<description>&lt;b&gt;CABGA-324&lt;/b&gt;&lt;p&gt;
pitch 0.80, outline 15x15 mm</description>
</package>
<package name="PQFP208">
<description>&lt;b&gt;Plastic Quad Flat Pack 208-pin&lt;/b&gt;</description>
</package>
<package name="LFBGA217">
</package>
<package name="LQFP64">
<description>&lt;b&gt;LQFP64&lt;/b&gt;</description>
</package>
<package name="ATMEGA8535PLC44">
<description>PLCC44 dla ATMEGA 8535</description>
</package>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="QFN10">
<description>&lt;b&gt;QFN10&lt;P&gt;

10M1, 10-pad, 3 x 3 x 1.0 mm Body, Lead Pitch 0.50 mm,
1.64 x 2.60 mm Exposed Pad,JEDEC reference MO-229C,</description>
</package>
</packages>
<symbols>
<symbol name="6-I/O-1">
<pin name="(XTAL2)PB4"/>
<pin name="(XTAL1)PB3"/>
<pin name="(RESET)PB5"/>
<pin name="(T0)PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="6-I/O-2">
<pin name="(XTAL2)PB4"/>
<pin name="(XTAL1)PB3"/>
<pin name="(RESET)PB5"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="5-I/O-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PB4"/>
<pin name="(CLOCK)PB3"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
</symbol>
<symbol name="6-I/O-3">
<pin name="(ADC3)PB4"/>
<pin name="(ADC2)PB3"/>
<pin name="(ADC0)PB5"/>
<pin name="(ADC1)PB2"/>
<pin name="(OCP)PB1"/>
<pin name="(AREF)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="16-I/O-1">
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="(ADC3)PB4"/>
<pin name="(ADC2)PB3"/>
<pin name="(ADC1)PB2"/>
<pin name="(OCP)PB1"/>
<pin name="(AVREF)PB0"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PC7"/>
<pin name="(ADC0)PB5"/>
</symbol>
<symbol name="15-I/O-1">
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="PB4"/>
<pin name="PB3"/>
<pin name="PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="(T0)PD4"/>
<pin name="PD3"/>
<pin name="(INT0)PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" function="dot"/>
</symbol>
<symbol name="3-I/O-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
</symbol>
<symbol name="20-I/O-1">
<pin name="(ADC5)PC5"/>
<pin name="(ADC4)PC4"/>
<pin name="(ADC3)PC3"/>
<pin name="(ADC2)PC2"/>
<pin name="(ADC1)PC1"/>
<pin name="(ADC0)PC0"/>
<pin name="(SCK)PB5"/>
<pin name="(MISO)PB4"/>
<pin name="(MOSI)PB3"/>
<pin name="(SS)PB2"/>
<pin name="(OC1)PB1"/>
<pin name="(ICP)PB0"/>
<pin name="(AIN1)PD7"/>
<pin name="(AIN0)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="NC4" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="32-I/O-1">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="OC1B"/>
<pin name="ALE"/>
<pin name="ICP"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
</symbol>
<symbol name="32-I/O-2">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="OC1B"/>
<pin name="ALE"/>
<pin name="ICP"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="48-I/O-1">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4)" direction="in"/>
<pin name="PF5(ADC5)" direction="in"/>
<pin name="PF6(ADC6)" direction="in"/>
<pin name="PF7(ADC7)" direction="in"/>
<pin name="(RXD)PE0"/>
<pin name="(TXD)PE1"/>
<pin name="(AC+)PE2"/>
<pin name="(AC-)PE3"/>
<pin name="(INT4)PE4"/>
<pin name="(INT5)PE5"/>
<pin name="(INT6)PE6"/>
<pin name="(INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(INT3)PD3"/>
<pin name="(INT2)PD2"/>
<pin name="(INT1)PD1"/>
<pin name="(INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TOSC2"/>
<pin name="TOSC1"/>
<pin name="WR" function="dot"/>
<pin name="RD" function="dot"/>
<pin name="ALE"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="15-I/O-2">
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="PB4"/>
<pin name="(OCI)PB3"/>
<pin name="PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="(ICP)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" function="dot"/>
</symbol>
<symbol name="20-I/O-2">
<pin name="(ADC5)PC5"/>
<pin name="(ADC4)PC4"/>
<pin name="(ADC3)PC3"/>
<pin name="(ADC2)PC2"/>
<pin name="(ADC1)PC1"/>
<pin name="(ADC0)PC0)"/>
<pin name="(SCK)PB5"/>
<pin name="(MISO)PB4"/>
<pin name="(MOSI)PB3"/>
<pin name="(SS)PB2"/>
<pin name="(OC1)PB1"/>
<pin name="(ICP)PB0"/>
<pin name="(AIN1)PD7"/>
<pin name="(AIN0)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-3">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-4">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="15-I/O-3">
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="INT1" direction="in"/>
<pin name="INT0" direction="in"/>
<pin name="AVCC" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ADIN5" direction="in"/>
<pin name="ADIN4" direction="in"/>
<pin name="ADIN3" direction="in"/>
<pin name="ADIN2" direction="in"/>
<pin name="ADIN1" direction="in"/>
<pin name="ADIN0" direction="in"/>
<pin name="NC13" direction="nc"/>
<pin name="NC12" direction="nc"/>
<pin name="NC11" direction="nc"/>
<pin name="NC10" direction="nc"/>
<pin name="NC9" direction="nc"/>
<pin name="NC8" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="NC6" direction="nc"/>
<pin name="NC5" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC14" direction="nc"/>
<pin name="NC15" direction="nc"/>
<pin name="NC16" direction="nc"/>
<pin name="NC17" direction="nc"/>
<pin name="NC18" direction="nc"/>
<pin name="NC19" direction="nc"/>
<pin name="NC20" direction="nc"/>
<pin name="NC21" direction="nc"/>
<pin name="NC22" direction="nc"/>
<pin name="NC23" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="NC24" direction="nc"/>
<pin name="NC25" direction="nc"/>
<pin name="NC26" direction="nc"/>
</symbol>
<symbol name="35-I/O-1">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(TXD1)PB3"/>
<pin name="(RXD1)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(RD)PD7"/>
<pin name="(WR)PD6"/>
<pin name="(TOSC2)PD5"/>
<pin name="(TOSC1)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD0)PD1"/>
<pin name="(RXD0)PD0"/>
<pin name="(OC1B)PE2"/>
<pin name="(ALE)PE1"/>
<pin name="(INT2)PE0"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="in"/>
</symbol>
<symbol name="35-I/O-2">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(TXD1)PB3"/>
<pin name="(RXD1)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(RD)PD7"/>
<pin name="(WR)PD6"/>
<pin name="(TOSC2)PD5"/>
<pin name="(TOSC1)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD0)PD1"/>
<pin name="(RXD0)PD0"/>
<pin name="(OC1B)PE2"/>
<pin name="(ALE)PE1"/>
<pin name="(INT2)PE0"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="32-I/O-5">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-6">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="20-I/O-3">
<pin name="PB5" direction="in"/>
<pin name="PB4(INT1)" direction="in"/>
<pin name="PB3(INT0)" direction="in"/>
<pin name="PB2(T0)" direction="in"/>
<pin name="PB1(AIN1)" direction="in"/>
<pin name="PB0(AIN0)" direction="in"/>
<pin name="PA3"/>
<pin name="(IR)PA2" direction="out"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="PB7" direction="in"/>
<pin name="PB6" direction="in"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC1" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="20-I/O-4">
<pin name="PB5" direction="in"/>
<pin name="PB4(INT1)" direction="in"/>
<pin name="PB3(INT0)" direction="in"/>
<pin name="PB2(T0)" direction="in"/>
<pin name="PB1(AIN1)" direction="in"/>
<pin name="PB0(AIN0)" direction="in"/>
<pin name="PA3"/>
<pin name="(IR)PA2" direction="out"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="PB7" direction="in"/>
<pin name="PB6" direction="in"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC1" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="NC5" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="24CXX">
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="250X0">
<pin name="HOLD/" direction="in"/>
<pin name="CS/" direction="in"/>
<pin name="SO" direction="in"/>
<pin name="WP/" direction="in"/>
<pin name="SCK"/>
<pin name="SI"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="SDE2506">
<pin name="CLK" direction="in"/>
<pin name="CE/" direction="in"/>
<pin name="D"/>
<pin name="NC" direction="nc"/>
<pin name="TP" direction="in"/>
<pin name="TG"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="93CX6">
<pin name="DO" direction="out"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SK"/>
<pin name="ORG" direction="in"/>
<pin name="DC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="15IO-1">
<pin name="AIN0-PB0"/>
<pin name="AIN1-PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="MOSI-PB5"/>
<pin name="MISO-PB6"/>
<pin name="SCK-PB7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="INT0-PD2"/>
<pin name="PD3"/>
<pin name="T0-PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="RST/"/>
</symbol>
<symbol name="5IO-1">
<pin name="MOSI-PB0"/>
<pin name="MISO-PB1"/>
<pin name="SCK-PB2"/>
<pin name="CLK-PB3"/>
<pin name="PB4"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RST/"/>
</symbol>
<symbol name="32IO-1">
<pin name="AD7-PA7"/>
<pin name="AD6-PA6"/>
<pin name="AD5-PA5"/>
<pin name="AD4-PA4"/>
<pin name="AD3-PA3"/>
<pin name="AD2-PA2"/>
<pin name="AD1-PA1"/>
<pin name="AD0-PA0"/>
<pin name="A15-PC7"/>
<pin name="A14-PC6"/>
<pin name="A13-PC5"/>
<pin name="A12-PC4"/>
<pin name="A11-PC3"/>
<pin name="A10-PC2"/>
<pin name="A9-PC1"/>
<pin name="A8-PC0"/>
<pin name="PB7-SCK"/>
<pin name="PB6-MISO"/>
<pin name="PB5-MOSI"/>
<pin name="PB4-SS/"/>
<pin name="PB3-AIN1"/>
<pin name="PB2-AIN0"/>
<pin name="PB1-T1"/>
<pin name="PB0-T0"/>
<pin name="PD0-RXD"/>
<pin name="PD1-TXD"/>
<pin name="PD2-INT0"/>
<pin name="PD3-INT1"/>
<pin name="PD4"/>
<pin name="PD5-OC1A"/>
<pin name="PD6-WR/"/>
<pin name="PD7-RD/"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RST/" direction="in"/>
<pin name="ICP"/>
<pin name="ALE"/>
<pin name="OC1B"/>
</symbol>
<symbol name="89C2051">
<pin name="P3.7"/>
<pin name="P3.5-T1"/>
<pin name="P3.4-T0"/>
<pin name="P3.3-INT1/"/>
<pin name="P3.2-INTO/"/>
<pin name="P3.1-TXD"/>
<pin name="P3.0-RXD"/>
<pin name="P1.7"/>
<pin name="P1.6"/>
<pin name="P1.5"/>
<pin name="P1.4"/>
<pin name="P1.3"/>
<pin name="P1.2"/>
<pin name="AIN1-P1.1"/>
<pin name="AIN0-P1.0"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RST-VPP" direction="in"/>
</symbol>
<symbol name="48-I/O-2">
<pin name="ADC0-PF0" direction="in"/>
<pin name="ADC1-PF1" direction="in"/>
<pin name="ADC2-PF2" direction="in"/>
<pin name="ADC3-PF3" direction="in"/>
<pin name="ADC4-PF4" direction="in"/>
<pin name="ADC5-PF5" direction="in"/>
<pin name="ADC6-PF6" direction="in"/>
<pin name="ADC7-PF7" direction="in"/>
<pin name="RXD-PE0" direction="out"/>
<pin name="TXD-PE1" direction="out"/>
<pin name="AC+_PE2" direction="out"/>
<pin name="AC-_PE3" direction="out"/>
<pin name="INT4-PE4" direction="out"/>
<pin name="INT5-PE5" direction="out"/>
<pin name="INT6-PE6" direction="out"/>
<pin name="INT7-PE7" direction="out"/>
<pin name="PD7-T2"/>
<pin name="PD6-T1"/>
<pin name="PD5"/>
<pin name="PD4-IC1"/>
<pin name="PD3-INT3"/>
<pin name="PD2-INT2"/>
<pin name="PD1-INT1"/>
<pin name="PD0-INT0"/>
<pin name="A15-PC7"/>
<pin name="A14-PC6"/>
<pin name="A13-PC5"/>
<pin name="A12-PC4"/>
<pin name="A11-PC3"/>
<pin name="A10-PC2"/>
<pin name="A9-PC1"/>
<pin name="A8-PC0"/>
<pin name="OC2-PB7"/>
<pin name="OC1B-PB6"/>
<pin name="OC1A-PB5"/>
<pin name="OC0-PB4"/>
<pin name="MISO-PB3"/>
<pin name="MOSI-PB2"/>
<pin name="SCK-PB1"/>
<pin name="SS-PB0"/>
<pin name="AD6-PA6"/>
<pin name="AD7-PA7"/>
<pin name="AD5-PA5"/>
<pin name="AD4-PA4"/>
<pin name="AD3-PA3"/>
<pin name="AD2-PA2"/>
<pin name="AD1-PA1"/>
<pin name="AD0-PA0"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="AVREF"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="01" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="02" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TOSC2"/>
<pin name="TOSC1"/>
<pin name="WR/"/>
<pin name="RD/"/>
<pin name="ALE"/>
<pin name="RESET/" direction="in"/>
<pin name="PEN/" direction="in"/>
</symbol>
<symbol name="AT89C52">
<pin name="EA" direction="in"/>
<pin name="P0.0AD0"/>
<pin name="P0.1AD1"/>
<pin name="P0.2AD2"/>
<pin name="P0.3AD3"/>
<pin name="P0.4AD4"/>
<pin name="P0.5AD5"/>
<pin name="P0.6AD6"/>
<pin name="P0.7AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0_T2"/>
<pin name="P1.1_T2EX"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR"/>
<pin name="P3.7/RD"/>
</symbol>
<symbol name="VCCGND">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="27C080">
<pin name="A16" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE!VPP" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
</symbol>
<symbol name="AT91R4008">
<pin name="NCS0" direction="out"/>
<pin name="NCS1" direction="out"/>
<pin name="NWAIT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="NWDOVF" direction="out"/>
<pin name="MCKI" direction="in"/>
<pin name="NRW0/NWE" direction="out"/>
<pin name="NRD/NOE" direction="out"/>
<pin name="NRW1/NUB" direction="out"/>
<pin name="NRST" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
</symbol>
<symbol name="ICE-TEST">
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
</symbol>
<symbol name="AT91R4008-PARPORT">
<pin name="P0/TCLK0"/>
<pin name="P1/TIOA0"/>
<pin name="P2/TIOB0"/>
<pin name="P3/TCLK1"/>
<pin name="P4/TIOA1"/>
<pin name="P5/TIOB1"/>
<pin name="P6/TCLK2"/>
<pin name="P7/TIOA2"/>
<pin name="P8/TIOB2"/>
<pin name="P9/IRQ0"/>
<pin name="P10/IRQ1"/>
<pin name="P11/IRQ2"/>
<pin name="P12/FIQ"/>
<pin name="P13/SCK0"/>
<pin name="P14/TXD0"/>
<pin name="P15/RXD0"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20/SCK1"/>
<pin name="P21/TXD1/NTRI"/>
<pin name="P22/RXD1"/>
<pin name="P23"/>
<pin name="P24/BMS"/>
<pin name="P25/MCKO"/>
<pin name="P26/NCS2"/>
<pin name="P27/NCS3"/>
</symbol>
<symbol name="AT91R4008-ADR">
<pin name="P31/CS4/A23" direction="out"/>
<pin name="P30/CS5/A22" direction="out"/>
<pin name="P29/CS6/A21" direction="out"/>
<pin name="P28/CS7/A20" direction="out"/>
<pin name="NLB/A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
</symbol>
<symbol name="D0-32">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
<pin name="D16" direction="hiz"/>
<pin name="D17" direction="hiz"/>
<pin name="D18" direction="hiz"/>
<pin name="D19" direction="hiz"/>
<pin name="D20" direction="hiz"/>
<pin name="D21" direction="hiz"/>
<pin name="D22" direction="hiz"/>
<pin name="D23" direction="hiz"/>
<pin name="D24" direction="hiz"/>
<pin name="D25" direction="hiz"/>
<pin name="D26" direction="hiz"/>
<pin name="D27" direction="hiz"/>
<pin name="D28" direction="hiz"/>
<pin name="D29" direction="hiz"/>
<pin name="D30" direction="hiz"/>
<pin name="D31" direction="hiz"/>
</symbol>
<symbol name="D0-15">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="VDDIO">
<pin name="VDDIO" direction="pwr"/>
</symbol>
<symbol name="VDDCORE">
<pin name="VDDCORE" direction="pwr"/>
</symbol>
<symbol name="TINY26">
<pin name="(ADC8/XTAL2)PB5"/>
<pin name="(ADC7/XTAL1)PB4"/>
<pin name="(OC1B)PB3"/>
<pin name="(SCK/SCL/!OC1B!)PB2"/>
<pin name="(MISO/DO/OC1A)PB1"/>
<pin name="(MOSI/DI/SDA/!OC1A!)PB0"/>
<pin name="(ADC6/AIN1)PA7"/>
<pin name="(ADC5/AIN0)PA6"/>
<pin name="(ADC4)PA5"/>
<pin name="(ADC3)PA4"/>
<pin name="(AREF)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="(ADC10/!RESET!)PB7"/>
<pin name="(ADC9/INT0/T0)PB6"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="SAM9708">
<pin name="READY" direction="hiz"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="IRQ" direction="hiz"/>
<pin name="!CS" direction="in"/>
<pin name="OVCK-OUT" direction="out"/>
<pin name="X1" direction="out"/>
<pin name="X2" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="LDTEST" direction="in"/>
<pin name="!PWDN" direction="in"/>
<pin name="!IO16" direction="hiz"/>
<pin name="!RAS"/>
<pin name="!CAS"/>
<pin name="!REFRESH"/>
<pin name="RBS" direction="out"/>
<pin name="CK_OUT" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="WD15">
<pin name="WD0"/>
<pin name="WD1"/>
<pin name="WD2"/>
<pin name="WD3"/>
<pin name="WD4"/>
<pin name="WD5"/>
<pin name="WD6"/>
<pin name="WD7"/>
<pin name="WD8"/>
<pin name="WD9"/>
<pin name="WD10"/>
<pin name="WD11"/>
<pin name="WD12"/>
<pin name="WD13"/>
<pin name="WD14"/>
<pin name="WD15"/>
</symbol>
<symbol name="WA27">
<pin name="WA0" direction="out"/>
<pin name="WA1" direction="out"/>
<pin name="WA2" direction="out"/>
<pin name="WA3" direction="out"/>
<pin name="WA4" direction="out"/>
<pin name="WA5" direction="out"/>
<pin name="WA6" direction="out"/>
<pin name="WA7" direction="out"/>
<pin name="WA8" direction="out"/>
<pin name="WA9" direction="out"/>
<pin name="WA10" direction="out"/>
<pin name="WA11" direction="out"/>
<pin name="WA12" direction="out"/>
<pin name="WA13" direction="out"/>
<pin name="WA14" direction="out"/>
<pin name="WA15" direction="out"/>
<pin name="WA16" direction="out"/>
<pin name="WA17" direction="out"/>
<pin name="WA18" direction="out"/>
<pin name="WA19" direction="out"/>
<pin name="WA20" direction="out"/>
<pin name="WA21" direction="out"/>
<pin name="WA22" direction="out"/>
<pin name="WA23" direction="out"/>
<pin name="WA24" direction="out"/>
<pin name="WA25" direction="out"/>
<pin name="WA26" direction="out"/>
</symbol>
<symbol name="SAM9708-SND">
<pin name="MIDI1_OUT" direction="in"/>
<pin name="MIDI2_OUT" direction="in"/>
<pin name="MIDI1_IN" direction="in"/>
<pin name="MIDI2_IN" direction="in"/>
<pin name="SD-IN0"/>
<pin name="SD-IN1"/>
<pin name="SD-IN2"/>
<pin name="SD-IN3"/>
<pin name="SD-OUT0" direction="out"/>
<pin name="SD-OUT1" direction="out"/>
<pin name="SD-OUT2" direction="out"/>
<pin name="SD-OUT3" direction="out"/>
<pin name="WS-OUT" direction="out"/>
<pin name="BCK-OUT" direction="out"/>
<pin name="SD-IN4"/>
<pin name="SD-IN5"/>
<pin name="SD-IN6"/>
<pin name="SD-IN7"/>
<pin name="SD-OUT4" direction="out"/>
<pin name="SD-OUT5" direction="out"/>
<pin name="SD-OUT6" direction="out"/>
<pin name="SD-OUT7" direction="out"/>
<pin name="LFT" direction="pas"/>
<pin name="!WCS0" direction="out"/>
<pin name="!WCS1" direction="out"/>
<pin name="!WWE" direction="out"/>
<pin name="!WOE" direction="out"/>
</symbol>
<symbol name="VCC1">
<pin name="VCC1" direction="pwr"/>
</symbol>
<symbol name="VCC2">
<pin name="VCC2" direction="pwr"/>
</symbol>
<symbol name="VC3">
<pin name="VC3" direction="pwr"/>
</symbol>
<symbol name="T8XC5121">
<pin name="CVSS" direction="pwr"/>
<pin name="LI" direction="pwr"/>
<pin name="CVCC" direction="pwr"/>
<pin name="P1.5/CRST"/>
<pin name="P1.4/CCLK"/>
<pin name="P1.3/CC4"/>
<pin name="P1.2/CPRES"/>
<pin name="P1.1/CC8"/>
<pin name="P1.0/CIO"/>
<pin name="RST"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="out"/>
<pin name="P3.7/CRST1/LED1"/>
<pin name="P3.6/CCLK1/LED0"/>
<pin name="P3.5/CIO1"/>
<pin name="P3.2/INT0"/>
<pin name="P3.4/T0"/>
<pin name="P3.3/INT1"/>
<pin name="P3.1/TXD"/>
<pin name="P3.0/RXD"/>
<pin name="VSS" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="EVCC" direction="pas"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="T8X5121-PLCC52">
<pin name="CVSS" direction="pwr"/>
<pin name="LI" direction="pwr"/>
<pin name="CVCC" direction="pwr"/>
<pin name="P1.5/CRST"/>
<pin name="P1.4/CCLK"/>
<pin name="P1.3/CC4"/>
<pin name="P1.2/CPRES"/>
<pin name="P1.1/CC8"/>
<pin name="P1.0/CIO"/>
<pin name="!RST"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="out"/>
<pin name="P3.7/CRST1/LED1"/>
<pin name="P3.6/CCLK1/LED0"/>
<pin name="P3.5/CIO1"/>
<pin name="P3.2/INT0"/>
<pin name="P3.4/T0"/>
<pin name="P3.3/INT1"/>
<pin name="P3.1/TXD"/>
<pin name="P3.0/RXD"/>
<pin name="VSS" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="EVCC" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="EA"/>
<pin name="PSEN"/>
<pin name="ALE"/>
<pin name="P2.7/A15"/>
<pin name="P2.6/A14"/>
<pin name="P2.5/A13"/>
<pin name="P2.4/A12"/>
<pin name="P0.5/AD5"/>
<pin name="P2.3/A11"/>
<pin name="P2.2/A10"/>
<pin name="P2.1/A9"/>
<pin name="P2.0/A8"/>
<pin name="P0.7/AD7"/>
<pin name="P0.4/AD4"/>
<pin name="P0.6/AD6"/>
<pin name="P0.1/AD1"/>
<pin name="P0.2/AD2"/>
<pin name="P0.3/AD3"/>
<pin name="P0.0/AD0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
</symbol>
<symbol name="AT89C51SND1C">
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AREFN" direction="in"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="P3.1/TXD"/>
<pin name="P3.0/RXD"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P4.3/!SS" direction="in"/>
<pin name="P4.0/MISO" direction="in"/>
<pin name="P4.1/MOSI" direction="out"/>
<pin name="P4.2/SCK" direction="out"/>
<pin name="P1.6/SCL"/>
<pin name="P1.7/SDA"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="FILT" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="out"/>
<pin name="RST" direction="in"/>
<pin name="!ISP" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="DCLK" direction="out"/>
<pin name="DESL" direction="out"/>
<pin name="SCLK" direction="out"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="MCLK" direction="out"/>
<pin name="MDAT"/>
<pin name="MCMD"/>
<pin name="P1.0/KIN0"/>
<pin name="P1.1/KIN1"/>
<pin name="P1.2/KIN2"/>
<pin name="P1.3/KIN3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.1"/>
<pin name="P5.0"/>
<pin name="P0.0/AD0"/>
<pin name="P0.1/AD1"/>
<pin name="P0.2/AD2"/>
<pin name="P0.3/AD3"/>
<pin name="P0.4/AD4"/>
<pin name="P0.5/AD5"/>
<pin name="P0.6/AD6"/>
<pin name="P0.7/AD7"/>
<pin name="P2.0/A8"/>
<pin name="P2.1/A9"/>
<pin name="P2.2/A10"/>
<pin name="P2.3/A11"/>
<pin name="P2.4/A12"/>
<pin name="P2.5/A13"/>
<pin name="P2.6/A14"/>
<pin name="P2.7/A15"/>
<pin name="P4.4" direction="in"/>
<pin name="P4.5" direction="in"/>
<pin name="P4.6" direction="in"/>
<pin name="P4.7" direction="in"/>
<pin name="AREFP" direction="in"/>
<pin name="!TST" direction="in"/>
</symbol>
<symbol name="P-AT89C51SND1C">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="PVSS" direction="pwr"/>
<pin name="UVDD" direction="pwr"/>
<pin name="UVSS" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
</symbol>
<symbol name="AT89C51">
<pin name="!EA!/VPP" direction="in"/>
<pin name="P0.0_AD0"/>
<pin name="P0.1_AD1"/>
<pin name="P0.2_AD2"/>
<pin name="P0.3_AD3"/>
<pin name="P0.4_AD4"/>
<pin name="P0.5_AD5"/>
<pin name="P0.6_AD6"/>
<pin name="P0.7_AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE/!PROG" direction="out"/>
<pin name="!PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AT89S51">
<pin name="!EA!/VPP" direction="in"/>
<pin name="P0.0_AD0"/>
<pin name="P0.1_AD1"/>
<pin name="P0.2_AD2"/>
<pin name="P0.3_AD3"/>
<pin name="P0.4_AD4"/>
<pin name="P0.5_AD5"/>
<pin name="P0.6_AD6"/>
<pin name="P0.7_AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE/!PROG" direction="out"/>
<pin name="!PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5_MOSI"/>
<pin name="P1.6_MISO"/>
<pin name="P1.7_SCK"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="T89C51CC02">
<pin name="P4.0/RXDC"/>
<pin name="P4.1/TXDC"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="P2.0"/>
<pin name="P2.1"/>
<pin name="P1.0/AN0/T2"/>
<pin name="P1.1/AN1/T2EX"/>
<pin name="P1.2/AN2/ECI"/>
<pin name="P1.3/AN3/CEX0"/>
<pin name="P1.4/AN4/CEX1"/>
<pin name="P1.5/AN5"/>
<pin name="P1.6/AN6"/>
<pin name="P1.7/AN7"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6"/>
<pin name="P3.7"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VAREF" direction="in"/>
<pin name="VAGND" direction="in"/>
<pin name="VAVCC" direction="in"/>
</symbol>
<symbol name="T89C51CC02-SO24">
<pin name="P4.0/RXDC"/>
<pin name="P4.1/TXDC"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="P1.0/AN0/T2"/>
<pin name="P1.1/AN1/T2EX"/>
<pin name="P1.2/AN2/ECI"/>
<pin name="P1.3/AN3/CEX0"/>
<pin name="P1.4/AN4/CEX1"/>
<pin name="P1.5/AN5"/>
<pin name="P1.6/AN6"/>
<pin name="P1.7/AN7"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VAREF" direction="in"/>
<pin name="VAGND" direction="in"/>
<pin name="VAVCC" direction="in"/>
</symbol>
<symbol name="AT91RM9200_BGA">
<pin name="ICETCK" direction="in"/>
<pin name="ICETDI" direction="in"/>
<pin name="ICETMS" direction="in"/>
<pin name="JTAGSEL" direction="in"/>
<pin name="NTRST" direction="in"/>
<pin name="TST0" direction="in"/>
<pin name="TST1" direction="in"/>
<pin name="D_0"/>
<pin name="D_1"/>
<pin name="D_10"/>
<pin name="D_11"/>
<pin name="D_12"/>
<pin name="D_13"/>
<pin name="D_14"/>
<pin name="D_15"/>
<pin name="D_2"/>
<pin name="D_3"/>
<pin name="D_4"/>
<pin name="D_5"/>
<pin name="D_6"/>
<pin name="D_7"/>
<pin name="D_8"/>
<pin name="D_9"/>
<pin name="NRW0NWE"/>
<pin name="NRW1_NUB_DQM1"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PA16"/>
<pin name="PA17"/>
<pin name="PA18"/>
<pin name="PA19"/>
<pin name="PA2"/>
<pin name="PA20"/>
<pin name="PA21"/>
<pin name="PA22"/>
<pin name="PA23"/>
<pin name="PA24"/>
<pin name="PA25"/>
<pin name="PA26"/>
<pin name="PA27"/>
<pin name="PA28"/>
<pin name="PA29"/>
<pin name="PA3"/>
<pin name="PA30"/>
<pin name="PA31"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PB16"/>
<pin name="PB17"/>
<pin name="PB18"/>
<pin name="PB19"/>
<pin name="PB2"/>
<pin name="PB20"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB24"/>
<pin name="PB25"/>
<pin name="PB26"/>
<pin name="PB27"/>
<pin name="PB28"/>
<pin name="PB29"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC16"/>
<pin name="PC17"/>
<pin name="PC18"/>
<pin name="PC19"/>
<pin name="PC2"/>
<pin name="PC20"/>
<pin name="PC21"/>
<pin name="PC22"/>
<pin name="PC23"/>
<pin name="PC24"/>
<pin name="PC25"/>
<pin name="PC26"/>
<pin name="PC27"/>
<pin name="PC28"/>
<pin name="PC29"/>
<pin name="PC3"/>
<pin name="PC30"/>
<pin name="PC31"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PD16"/>
<pin name="PD17"/>
<pin name="PD18"/>
<pin name="PD19"/>
<pin name="PD2"/>
<pin name="PD20"/>
<pin name="PD21"/>
<pin name="PD22"/>
<pin name="PD23"/>
<pin name="PD24"/>
<pin name="PD25"/>
<pin name="PD26"/>
<pin name="PD27"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="A_10" direction="out"/>
<pin name="A10_SDRAM" direction="out"/>
<pin name="A_11" direction="out"/>
<pin name="A_12" direction="out"/>
<pin name="A_13" direction="out"/>
<pin name="A_14" direction="out"/>
<pin name="A_15" direction="out"/>
<pin name="A16_BA0" direction="out"/>
<pin name="A17_BA1" direction="out"/>
<pin name="A_18" direction="out"/>
<pin name="A_19" direction="out"/>
<pin name="A1_DQM2" direction="out"/>
<pin name="A_2" direction="out"/>
<pin name="A_20" direction="out"/>
<pin name="A_21" direction="out"/>
<pin name="A_22" direction="out"/>
<pin name="A_3" direction="out"/>
<pin name="A_4" direction="out"/>
<pin name="A_5" direction="out"/>
<pin name="A_6" direction="out"/>
<pin name="A_7" direction="out"/>
<pin name="A_8" direction="out"/>
<pin name="A_9" direction="out"/>
<pin name="CAS" direction="out"/>
<pin name="ICETDO" direction="out"/>
<pin name="NBS3" direction="out"/>
<pin name="NCS0_BFCS" direction="out"/>
<pin name="NCS1_SDCS" direction="out"/>
<pin name="NCS2" direction="out"/>
<pin name="NCS3" direction="out"/>
<pin name="NLBA0_DQM0" direction="out"/>
<pin name="NRDNOE" direction="out"/>
<pin name="RAS" direction="out"/>
<pin name="SDRAMCKE" direction="out"/>
<pin name="WE" direction="out"/>
<pin name="DM" direction="pwr"/>
<pin name="DP" direction="pwr"/>
<pin name="HDMA" direction="pwr"/>
<pin name="HDMB" direction="pwr"/>
<pin name="HDPA" direction="pwr"/>
<pin name="HDPB" direction="pwr"/>
<pin name="NRST" direction="pwr"/>
<pin name="OSC32K_XIN" direction="pwr"/>
<pin name="OSC32K_XOUT" direction="pwr"/>
<pin name="OSC9M_XIN" direction="pwr"/>
<pin name="OSC9M_XOUT" direction="pwr"/>
<pin name="PLL_A_RC" direction="pwr"/>
<pin name="PLL_B_RC" direction="pwr"/>
<pin name="SDRAMCLK" direction="pwr"/>
<pin name="MIX33VDD@1" direction="pwr"/>
<pin name="MIX33VDD@2" direction="pwr"/>
<pin name="MIX33VDD@3" direction="pwr"/>
<pin name="MIX33VDD@4" direction="pwr"/>
<pin name="MIX33VDD@5" direction="pwr"/>
<pin name="MIX33VDD@6" direction="pwr"/>
<pin name="MIX33VDD@7" direction="pwr"/>
<pin name="MIX33VDD@8" direction="pwr"/>
<pin name="MIX33VDD@9" direction="pwr"/>
<pin name="MIX33VDD@10" direction="pwr"/>
<pin name="MIX33VDD@11" direction="pwr"/>
<pin name="MIX33VDD@12" direction="pwr"/>
<pin name="MIX33VDD@13" direction="pwr"/>
<pin name="MIX33VDD@14" direction="pwr"/>
<pin name="MIX33VDD@15" direction="pwr"/>
<pin name="MIX33VDD@16" direction="pwr"/>
<pin name="MIX33VDD@17" direction="pwr"/>
<pin name="MIX33VDD@18" direction="pwr"/>
<pin name="MIX33VDD@19" direction="pwr"/>
<pin name="MIX33VDD@20" direction="pwr"/>
<pin name="MIX33VDD@21" direction="pwr"/>
<pin name="MIX33VSS@1" direction="pwr"/>
<pin name="MIX33VSS@2" direction="pwr"/>
<pin name="MIX33VSS@3" direction="pwr"/>
<pin name="MIX33VSS@4" direction="pwr"/>
<pin name="MIX33VSS@5" direction="pwr"/>
<pin name="MIX33VSS@6" direction="pwr"/>
<pin name="MIX33VSS@7" direction="pwr"/>
<pin name="MIX33VSS@8" direction="pwr"/>
<pin name="MIX33VSS@9" direction="pwr"/>
<pin name="MIX33VSS@10" direction="pwr"/>
<pin name="MIX33VSS@11" direction="pwr"/>
<pin name="MIX33VSS@12" direction="pwr"/>
<pin name="MIX33VSS@13" direction="pwr"/>
<pin name="MIX33VSS@14" direction="pwr"/>
<pin name="MIX33VSS@15" direction="pwr"/>
<pin name="MIX33VSS@16" direction="pwr"/>
<pin name="MIX33VSS@17" direction="pwr"/>
<pin name="MIX33VSS@18" direction="pwr"/>
<pin name="MIX33VSS@19" direction="pwr"/>
<pin name="MIX33VSS@20" direction="pwr"/>
<pin name="MIX33VSS@21" direction="pwr"/>
<pin name="VDDI@1" direction="pwr"/>
<pin name="VDDI@2" direction="pwr"/>
<pin name="VDDI@3" direction="pwr"/>
<pin name="VDDI@4" direction="pwr"/>
<pin name="VDDI@5" direction="pwr"/>
<pin name="VDDI@6" direction="pwr"/>
<pin name="VDDI@7" direction="pwr"/>
<pin name="VDDI@8" direction="pwr"/>
<pin name="VDDI@9" direction="pwr"/>
<pin name="VSSI@1" direction="pwr"/>
<pin name="VSSI@2" direction="pwr"/>
<pin name="VSSI@3" direction="pwr"/>
<pin name="VSSI@4" direction="pwr"/>
<pin name="VSSI@5" direction="pwr"/>
<pin name="VSSI@6" direction="pwr"/>
<pin name="VSSI@7" direction="pwr"/>
<pin name="VSSI@8" direction="pwr"/>
<pin name="VSSI@9" direction="pwr"/>
</symbol>
<symbol name="ATF16V8B">
<pin name="CLK" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
<pin name="O4" direction="out"/>
<pin name="O5" direction="out"/>
<pin name="O6" direction="out"/>
<pin name="O7" direction="out"/>
<pin name="O8" direction="out"/>
<pin name="OE" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="23-I/O-2">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="32-I/O-M16-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M16-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-M32-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M32-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="MEGA64">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="MEGA128">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="MEGA169">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PCINT0)PE0"/>
<pin name="(TXD/PCINT1)PE1"/>
<pin name="(XCK0/AIN0/PCINT2)PE2"/>
<pin name="(AIN1/PCINT3)PE3"/>
<pin name="(USCK/SCL/PCINT4)PE4"/>
<pin name="(DI/SDA/PCINT5)PE5"/>
<pin name="(DO/PCINT6)PE6"/>
<pin name="(CLKO/PCINT7)PE7"/>
<pin name="(SEG15)PD7"/>
<pin name="(SEG16)PD6"/>
<pin name="(SEG17)PD5"/>
<pin name="(SEG18)PD4"/>
<pin name="(SEG19)PD3"/>
<pin name="(SEG20)PD2"/>
<pin name="(SEG21/INT0)PD1"/>
<pin name="(SEG22/ICP)PD0"/>
<pin name="(SEG5)PC7" direction="out"/>
<pin name="(SEG6)PC6" direction="out"/>
<pin name="(SEG7)PC5" direction="out"/>
<pin name="(SEG8)PC4" direction="out"/>
<pin name="(SEG9)PC3" direction="out"/>
<pin name="(SEG10)PC2" direction="out"/>
<pin name="(SEG11)PC1" direction="out"/>
<pin name="(SEG12)PC0" direction="out"/>
<pin name="(OC2A/PCINT15)PB7"/>
<pin name="(OC1B/PCINT14)PB6"/>
<pin name="(OC1A/PCINT13)PB5"/>
<pin name="(OC0A/PCINT12)PB4"/>
<pin name="(MISO/PCINT11)PB3"/>
<pin name="(MOSI/PCINT10)PB2"/>
<pin name="(SCK/PCINT9)PB1"/>
<pin name="(SS/PCINT8)PB0"/>
<pin name="(SEG2)PA6"/>
<pin name="(SEG3)PA7"/>
<pin name="(SEG1)PA5"/>
<pin name="(SEG0)PA4"/>
<pin name="(COM3)PA3"/>
<pin name="(COM2)PA2"/>
<pin name="(COM1)PA1"/>
<pin name="(COM0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1(TOSC1)"/>
<pin name="XTAL2(TOSC2)"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(T1/SEG24)"/>
<pin name="PG4(T0/SEG23)"/>
<pin name="PG0(SEG14)"/>
<pin name="PG1(SEG13)"/>
<pin name="PG2(SEG4)"/>
<pin name="PG5(RESET)" direction="in" function="dot"/>
<pin name="LCDCAP" direction="in"/>
</symbol>
<symbol name="MEGA323-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MEGA323">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-M8515-A">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(XCK)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="32-I/O-7">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(XCK)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
</symbol>
<symbol name="32-I/O-M8535-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M8535-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/INT2)PB3"/>
<pin name="(AIN0/OC0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="AT89C5131">
<pin name="!EA!/VPP" direction="in"/>
<pin name="P0.0_AD0"/>
<pin name="P0.1_AD1"/>
<pin name="P0.2_AD2"/>
<pin name="P0.3_AD3"/>
<pin name="P0.4_AD4"/>
<pin name="P0.5_AD5"/>
<pin name="P0.6_AD6"/>
<pin name="P0.7_AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="ALE"/>
<pin name="!PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0/T2/KIN0"/>
<pin name="P1.1/T2EX/KIN1/SS"/>
<pin name="P1.2/ECI/KIN2"/>
<pin name="P1.3/CEX0/KIN3"/>
<pin name="P1.4/CEX1/KIN4"/>
<pin name="P1.5/CEX2/KIN5/MISO"/>
<pin name="P1.6/CEX3/KIN6/SCK"/>
<pin name="P1.7/CEX4/KIN7/MOSI"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="PLLF"/>
<pin name="FREV"/>
<pin name="P4.0/SCL"/>
<pin name="P4.1/SDA"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="AT89C5132">
<pin name="VDD@1" direction="pwr"/>
<pin name="P0.0_AD0"/>
<pin name="P0.1_AD1"/>
<pin name="P0.2_AD2"/>
<pin name="P0.3_AD3"/>
<pin name="P0.4_AD4"/>
<pin name="P0.5_AD5"/>
<pin name="P0.6_AD6"/>
<pin name="P0.7_AD7"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE"/>
<pin name="P4.3/!SS"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0/KIN0"/>
<pin name="P1.1/KIN1"/>
<pin name="P1.2/KIN2"/>
<pin name="P1.3/KIN3"/>
<pin name="P1.6/SCL"/>
<pin name="P1.7/SDA"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="P4.0/MISO"/>
<pin name="P4.1/MOSI"/>
<pin name="P4.2/SCK"/>
<pin name="P4.4"/>
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="FILT" direction="in"/>
<pin name="DCLK" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="DSEL" direction="out"/>
<pin name="SCLK" direction="out"/>
<pin name="MCLK" direction="out"/>
<pin name="MCMD"/>
<pin name="MDAT"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AREFP" direction="in"/>
<pin name="AREFN" direction="in"/>
<pin name="!ISP"/>
<pin name="!TST" direction="in"/>
<pin name="UVDD" direction="pwr"/>
<pin name="UVSS" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="PVSS" direction="pwr"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
</symbol>
<symbol name="23-I/O_MI">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
<pin name="THERMAL" direction="pas"/>
</symbol>
<symbol name="32-I/O-M16-A_M">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="32-I/O-M32-A_M">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="MEGA64-M">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="MEGA128-M">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="MEGA169-M">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PCINT0)PE0"/>
<pin name="(TXD/PCINT1)PE1"/>
<pin name="(XCK0/AIN0/PCINT2)PE2"/>
<pin name="(AIN1/PCINT3)PE3"/>
<pin name="(USCK/SCL/PCINT4)PE4"/>
<pin name="(DI/SDA/PCINT5)PE5"/>
<pin name="(DO/PCINT6)PE6"/>
<pin name="(CLKO/PCINT7)PE7"/>
<pin name="(SEG15)PD7"/>
<pin name="(SEG16)PD6"/>
<pin name="(SEG17)PD5"/>
<pin name="(SEG18)PD4"/>
<pin name="(SEG19)PD3"/>
<pin name="(SEG20)PD2"/>
<pin name="(SEG21/INT0)PD1"/>
<pin name="(SEG22/ICP)PD0"/>
<pin name="(SEG5)PC7" direction="out"/>
<pin name="(SEG6)PC6" direction="out"/>
<pin name="(SEG7)PC5" direction="out"/>
<pin name="(SEG8)PC4" direction="out"/>
<pin name="(SEG9)PC3" direction="out"/>
<pin name="(SEG10)PC2" direction="out"/>
<pin name="(SEG11)PC1" direction="out"/>
<pin name="(SEG12)PC0" direction="out"/>
<pin name="(OC2A/PCINT15)PB7"/>
<pin name="(OC1B/PCINT14)PB6"/>
<pin name="(OC1A/PCINT13)PB5"/>
<pin name="(OC0A/PCINT12)PB4"/>
<pin name="(MISO/PCINT11)PB3"/>
<pin name="(MOSI/PCINT10)PB2"/>
<pin name="(SCK/PCINT9)PB1"/>
<pin name="(SS/PCINT8)PB0"/>
<pin name="(SEG2)PA6"/>
<pin name="(SEG3)PA7"/>
<pin name="(SEG1)PA5"/>
<pin name="(SEG0)PA4"/>
<pin name="(COM3)PA3"/>
<pin name="(COM2)PA2"/>
<pin name="(COM1)PA1"/>
<pin name="(COM0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1(TOSC1)"/>
<pin name="XTAL2(TOSC2)"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(T1/SEG24)"/>
<pin name="PG4(T0/SEG23)"/>
<pin name="PG0(SEG14)"/>
<pin name="PG1(SEG13)"/>
<pin name="PG2(SEG4)"/>
<pin name="PG5(RESET)" direction="in" function="dot"/>
<pin name="LCDCAP" direction="in"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="32-I/O-M8515-A_M">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(XCK)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="32-I/O-M8535-A_M">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="TINY26_M">
<pin name="(ADC8/XTAL2)PB5"/>
<pin name="(ADC7/XTAL1)PB4"/>
<pin name="(OC1B)PB3"/>
<pin name="(SCK/SCL/!OC1B!)PB2"/>
<pin name="(MISO/DO/OC1A)PB1"/>
<pin name="(MOSI/DI/SDA/!OC1A!)PB0"/>
<pin name="(ADC6/AIN1)PA7"/>
<pin name="(ADC5/AIN0)PA6"/>
<pin name="(ADC4)PA5"/>
<pin name="(ADC3)PA4"/>
<pin name="(AREF)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="(ADC10/!RESET!)PB7"/>
<pin name="(ADC9/INT0/T0)PB6"/>
<pin name="GND@1" direction="pwr"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="ATMEGA644">
<pin name="(PCINT31/OC2A)PD7"/>
<pin name="(PCINT30/OC2B/ICP)PD6"/>
<pin name="(PCINT29/OC1A)PD5"/>
<pin name="(PCINT28/OC1B)PD4"/>
<pin name="(PCINT27/INT1)PD3"/>
<pin name="(PCINT26/INT0)PD2"/>
<pin name="(PCINT25/TXD0)PD1"/>
<pin name="(PCINT24/RXD0)PD0"/>
<pin name="(PCINT23/TOSC2)PC7" direction="out"/>
<pin name="(PCINT22/TOSC1)PC6" direction="out"/>
<pin name="(PCINT21/TDI)PC5" direction="out"/>
<pin name="(PCINT20/TDO)PC4" direction="out"/>
<pin name="(PCINT19/TMS)PC3" direction="out"/>
<pin name="(PCINT18/TCK)PC2" direction="out"/>
<pin name="(PCINT17/SDA)PC1" direction="out"/>
<pin name="(PCINT16/SCL)PC0" direction="out"/>
<pin name="(PCINT15/SCK)PB7"/>
<pin name="(PCINT14/MISO)PB6"/>
<pin name="(PCINT13/MOSI)PB5"/>
<pin name="(PCINT12/OC0B/!SS!)PB4"/>
<pin name="(PCINT11/OC0A/AIN1)PB3"/>
<pin name="(PCINT10/INT2/AIN0)PB2"/>
<pin name="(PCINT9/CLKO/T1)PB1"/>
<pin name="(PCINT8/XCK0/T0)PB0"/>
<pin name="(PCINT6/ADC6)PA6"/>
<pin name="(PCINT7/ADC7)PA7"/>
<pin name="(PCINT5/ADC5)PA5"/>
<pin name="(PCINT4/ADC4)PA4"/>
<pin name="(PCINT3/ADC3)PA3"/>
<pin name="(PCINT2/ADC2)PA2"/>
<pin name="(PCINT1/ADC1)PA1"/>
<pin name="(PCINT0/ADC0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="ATMEGA644E">
<pin name="(PCINT31/OC2A)PD7"/>
<pin name="(PCINT30/OC2B/ICP)PD6"/>
<pin name="(PCINT29/OC1A)PD5"/>
<pin name="(PCINT28/OC1B)PD4"/>
<pin name="(PCINT27/INT1)PD3"/>
<pin name="(PCINT26/INT0)PD2"/>
<pin name="(PCINT25/TXD0)PD1"/>
<pin name="(PCINT24/RXD0)PD0"/>
<pin name="(PCINT23/TOSC2)PC7" direction="out"/>
<pin name="(PCINT22/TOSC1)PC6" direction="out"/>
<pin name="(PCINT21/TDI)PC5" direction="out"/>
<pin name="(PCINT20/TDO)PC4" direction="out"/>
<pin name="(PCINT19/TMS)PC3" direction="out"/>
<pin name="(PCINT18/TCK)PC2" direction="out"/>
<pin name="(PCINT17/SDA)PC1" direction="out"/>
<pin name="(PCINT16/SCL)PC0" direction="out"/>
<pin name="(PCINT15/SCK)PB7"/>
<pin name="(PCINT14/MISO)PB6"/>
<pin name="(PCINT13/MOSI)PB5"/>
<pin name="(PCINT12/OC0B/!SS!)PB4"/>
<pin name="(PCINT11/OC0A/AIN1)PB3"/>
<pin name="(PCINT10/INT2/AIN0)PB2"/>
<pin name="(PCINT9/CLKO/T1)PB1"/>
<pin name="(PCINT8/XCK0/T0)PB0"/>
<pin name="(PCINT6/ADC6)PA6"/>
<pin name="(PCINT7/ADC7)PA7"/>
<pin name="(PCINT5/ADC5)PA5"/>
<pin name="(PCINT4/ADC4)PA4"/>
<pin name="(PCINT3/ADC3)PA3"/>
<pin name="(PCINT2/ADC2)PA2"/>
<pin name="(PCINT1/ADC1)PA1"/>
<pin name="(PCINT0/ADC0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="EXP" direction="pwr"/>
</symbol>
<symbol name="AT91SAM7X">
<pin name="ADVREF"/>
<pin name="GND@1"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="VDDOUT@1"/>
<pin name="VDDIN@1"/>
<pin name="PB27/AD0"/>
<pin name="PB28/AD1"/>
<pin name="PB29/AD2"/>
<pin name="PB30/AD3"/>
<pin name="PA8/PGMM0"/>
<pin name="PA9/PGMM1"/>
<pin name="VDDCORE@1"/>
<pin name="GND@2"/>
<pin name="VDDIO@1"/>
<pin name="PA10/PGMM2"/>
<pin name="PA11/PGMM3"/>
<pin name="PA12/PGMD0"/>
<pin name="PA13/PGMD1"/>
<pin name="PA14/PGMD2"/>
<pin name="PA15/PGMD3"/>
<pin name="PA16/PGMD4"/>
<pin name="PA17/PGMD5"/>
<pin name="PA18/PGMD6"/>
<pin name="PB9"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PB16"/>
<pin name="PB17"/>
<pin name="PB18"/>
<pin name="PA19/PGMD7"/>
<pin name="PA20/PGMD8"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB24"/>
<pin name="PB25"/>
<pin name="PB26"/>
<pin name="GND@3"/>
<pin name="VDDIO@2"/>
<pin name="VDDCORE@2"/>
<pin name="PB0"/>
<pin name="VDDIO@3"/>
<pin name="PA21/PGMD9"/>
<pin name="PA22/PGMD10"/>
<pin name="TDI"/>
<pin name="GND@4"/>
<pin name="PA23/PGMD11"/>
<pin name="PA24/PGMD12"/>
<pin name="NRST"/>
<pin name="TST"/>
<pin name="PA25/PGMD13"/>
<pin name="PA26/PGMD14"/>
<pin name="VDDIO@4"/>
<pin name="VDDCORE@3"/>
<pin name="PB19"/>
<pin name="PB20"/>
<pin name="GND@5"/>
<pin name="PA27/PGMD15"/>
<pin name="PA28"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4/PGMNCMD"/>
<pin name="PA5/PGMRDY"/>
<pin name="PA6/PGMNOE"/>
<pin name="PA7/PGMNVALID"/>
<pin name="PA29"/>
<pin name="TDO"/>
<pin name="JTAGSEL"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="PA30"/>
<pin name="PA0/PGMEN0"/>
<pin name="PA1/PGMEN1"/>
<pin name="GND@6"/>
<pin name="VDDIO@5"/>
<pin name="VDDCORE@4"/>
<pin name="ERASE"/>
<pin name="DDM"/>
<pin name="DDP"/>
<pin name="VDDFLASH"/>
<pin name="GND@7"/>
<pin name="XOUT"/>
<pin name="PLLRC"/>
<pin name="VDDPLL"/>
<pin name="XIN/PGMCK"/>
</symbol>
<symbol name="AT91SAM7X-BGA">
<pin name="ADVREF"/>
<pin name="GND@1"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="VDDOUT@1" direction="out"/>
<pin name="VDDIN@1"/>
<pin name="PB27/AD0"/>
<pin name="PB28/AD1"/>
<pin name="PB29/AD2"/>
<pin name="PB30/AD3"/>
<pin name="PA8/PGMM0"/>
<pin name="PA9/PGMM1"/>
<pin name="VDDCORE@1"/>
<pin name="GND@2"/>
<pin name="VDDIO@1"/>
<pin name="PA10/PGMM2"/>
<pin name="PA11/PGMM3"/>
<pin name="PA12/PGMD0"/>
<pin name="PA13/PGMD1"/>
<pin name="PA14/PGMD2"/>
<pin name="PA15/PGMD3"/>
<pin name="PA16/PGMD4"/>
<pin name="PA17/PGMD5"/>
<pin name="PA18/PGMD6"/>
<pin name="PB9"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PB16"/>
<pin name="PB17"/>
<pin name="PB18"/>
<pin name="PA19/PGMD7"/>
<pin name="PA20/PGMD8"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB24"/>
<pin name="PB25"/>
<pin name="PB26"/>
<pin name="GND@3"/>
<pin name="VDDIO@2"/>
<pin name="VDDCORE@2"/>
<pin name="PB0"/>
<pin name="VDDIO@3"/>
<pin name="PA21/PGMD9"/>
<pin name="PA22/PGMD10"/>
<pin name="TDI"/>
<pin name="GND@4"/>
<pin name="PA23/PGMD11"/>
<pin name="PA24/PGMD12"/>
<pin name="NRST"/>
<pin name="TST"/>
<pin name="PA25/PGMD13"/>
<pin name="PA26/PGMD14"/>
<pin name="VDDIO@4"/>
<pin name="VDDCORE@3"/>
<pin name="PB19"/>
<pin name="PB20"/>
<pin name="GND@5"/>
<pin name="PA27/PGMD15"/>
<pin name="PA28"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4/PGMNCMD"/>
<pin name="PA5/PGMRDY"/>
<pin name="PA6/PGMNOE"/>
<pin name="PA7/PGMNVALID"/>
<pin name="PA29"/>
<pin name="TDO"/>
<pin name="JTAGSEL"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="PA30"/>
<pin name="PA0/PGMEN0"/>
<pin name="PA1/PGMEN1"/>
<pin name="GND@6"/>
<pin name="VDDCORE@5"/>
<pin name="VDDCORE@4"/>
<pin name="ERASE"/>
<pin name="DDM"/>
<pin name="DDP"/>
<pin name="VDDFLASH"/>
<pin name="GND@7"/>
<pin name="XOUT" direction="out"/>
<pin name="PLLRC"/>
<pin name="VDDPLL"/>
<pin name="XIN/PGMCK"/>
</symbol>
<symbol name="AT93C46A">
<pin name="DO" direction="out"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SK" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="DC" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TINY13">
<pin name="PB5/PCINT5/!RESET!/ADC0/DW"/>
<pin name="PB3/PCINT3/CLKI/ADC3"/>
<pin name="PB4/PCINT4/ADC2"/>
<pin name="PB0/PCINT0/AIN0/OC0A/MOSI"/>
<pin name="PB1/PCINT1/AIN1/OC0B/INT0/MISO"/>
<pin name="PB2/PCINT2/SCK/ADC1/T0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="T7024">
<pin name="RX_ON" direction="in"/>
<pin name="PU" direction="in"/>
<pin name="VS_LNA" direction="in"/>
<pin name="LNA_OUT" direction="in"/>
<pin name="LNA_IN" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="PA_IN" direction="in"/>
<pin name="V3_PA_OUT@1" direction="pas"/>
<pin name="V1_PA" direction="pas"/>
<pin name="V2_PA@1" direction="pas"/>
<pin name="R_SWITCH" direction="in"/>
<pin name="SWITCH_OUT" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="V3_PA_OUT@2" direction="pas"/>
<pin name="V3_PA_OUT@3" direction="pas"/>
<pin name="V2_PA@2" direction="pas"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="XMEGA16A4">
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="PC7"/>
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="PB3"/>
<pin name="PB2"/>
<pin name="PB1"/>
<pin name="PB0"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="PR0(XT2)"/>
<pin name="PR1(XT1)"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PDI_DATA"/>
<pin name="GND2" direction="pwr"/>
<pin name="!RESET!/PDI_CLK"/>
</symbol>
<symbol name="XMEGA128A1">
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="PC7"/>
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="PB0"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="AVCC1" direction="pwr"/>
<pin name="GND9" direction="pwr"/>
<pin name="PDI_DATA"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET!/PDI_CLK" direction="in"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND6" direction="pwr"/>
<pin name="GND7" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND8" direction="pwr"/>
<pin name="PH0"/>
<pin name="PH1"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PJ0"/>
<pin name="PJ1"/>
<pin name="PJ2"/>
<pin name="PJ3"/>
<pin name="PJ4"/>
<pin name="PJ5"/>
<pin name="PJ6"/>
<pin name="PJ7"/>
<pin name="PK0"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="PK3"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PK6"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0(XT2)"/>
<pin name="PR1(XT1)"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
</symbol>
<symbol name="ATMEGA325P">
<pin name="DNC" direction="in"/>
<pin name="RXD/PCINT0/PE0"/>
<pin name="TXD/PCINT1/PE1"/>
<pin name="XCK/AIN0/PCINT2/PE2"/>
<pin name="AIN1/PCINT3/PE3"/>
<pin name="USCK/SCL/PCINT4/PE4"/>
<pin name="DI/SDA/PCINT5/PE5"/>
<pin name="DO/PCINT6/PE6"/>
<pin name="CLKO/PCINT7/PE7"/>
<pin name="!SS!/PCINT8/PB0"/>
<pin name="SCK/PCINT9/PB1"/>
<pin name="MOSI/PCINT10/PB2"/>
<pin name="MISO/PCINT11/PB3"/>
<pin name="OC0A/PCINT12/PB4"/>
<pin name="OC1B/PCINT14/PB6"/>
<pin name="OC1A/PCINT13/PB5"/>
<pin name="OC2A/PCINT15/PB7"/>
<pin name="T1/PG3"/>
<pin name="T0/PG4"/>
<pin name="!RESET!/PG5" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TOSC2/XTAL2" direction="out"/>
<pin name="TOSC1/XTAL1" direction="in"/>
<pin name="ICP1/PD0"/>
<pin name="INT0/PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PG2"/>
<pin name="PC2"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="ADC7/TDI/PF7"/>
<pin name="ADC6/TDO/PF6"/>
<pin name="ADC5/TMS/PF5"/>
<pin name="ADC4/TCK/PF4"/>
<pin name="ADC3/PF3"/>
<pin name="ADC2/PF2"/>
<pin name="ADC1/PF1"/>
<pin name="ADC0/PF0"/>
<pin name="AREF" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="AT45DB642D">
<pin name="SI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="!WP" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="RDY/!BUSY" direction="out"/>
<pin name="I/O3"/>
<pin name="I/O2"/>
<pin name="I/O1"/>
<pin name="I/O0"/>
<pin name="SER/!BYTE" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SCK/CLK" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="I/O7"/>
<pin name="I/O6"/>
<pin name="I/O5"/>
<pin name="I/O4"/>
<pin name="VCCP" direction="pwr"/>
<pin name="GNDP" direction="pwr"/>
</symbol>
<symbol name="ATMEGA644-20PU">
<pin name="PCINT8/XCK0/T0_PB0"/>
<pin name="PCINT9/CLKO/T1_PB1"/>
<pin name="PCINT10/INT2/AIN0_PB2"/>
<pin name="PCINT11/OC0A/AIN1_PB3"/>
<pin name="PCINT12/OC0B/SS_PB4"/>
<pin name="PCINT13/MOSI_PB5"/>
<pin name="PCINT14/MISO_PB6"/>
<pin name="PCINT15/SCK_PB7"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="PCINT24/RXD0_PD0"/>
<pin name="PCINT25/TXD0_PD1"/>
<pin name="PCINT26/INT0_PD2"/>
<pin name="PCINT27/INT1_PD3"/>
<pin name="PCINT28/OC1B_PD4"/>
<pin name="PCINT29/OC1A_PD5"/>
<pin name="PCINT30/OC2B/ICP_PD6"/>
<pin name="PCINT31/OC2A_PD7"/>
<pin name="PCINT16/SCL_PC0"/>
<pin name="PCINT17/SDA_PC1"/>
<pin name="PCINT18/TCK_PC2"/>
<pin name="PCINT19/TMS_PC3"/>
<pin name="PCINT20/TDO_PC4"/>
<pin name="PCINT21/TDI_PC5"/>
<pin name="PCINT22/TOSC1_PC6"/>
<pin name="PCINT23/TOSC2_PC7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="PCINT7/ADC7_PA7"/>
<pin name="PCINT6/ADC6_PA6"/>
<pin name="PCINT5/ADC5_PA5"/>
<pin name="PCINT4/ADC4_PA4"/>
<pin name="PCINT3/ADC3_PA3"/>
<pin name="PCINT2/ADC2_PA2"/>
<pin name="PCINT1/ADC1_PA1"/>
<pin name="PCINT0/ADC0_PA0"/>
</symbol>
<symbol name="AT45DB161D">
<pin name="!CS" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="!WP" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="RDY/!BUSY" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AT45DB161VFN8">
<pin name="!CS" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!WP" direction="in"/>
</symbol>
<symbol name="ATXMEGA64C3">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="14GND" direction="pwr"/>
<pin name="15VDD" direction="pwr"/>
<pin name="24GND" direction="pwr"/>
<pin name="25VDD" direction="pwr"/>
<pin name="34GND" direction="pwr"/>
<pin name="35VCC" direction="pwr"/>
<pin name="44GND" direction="pwr"/>
<pin name="45VCC" direction="pwr"/>
<pin name="52GND" direction="pwr"/>
<pin name="53VCC" direction="pwr"/>
<pin name="60GND" direction="pwr"/>
<pin name="61AVCC" direction="pwr"/>
<pin name="57RESET/PDI"/>
<pin name="58PRO"/>
<pin name="59PR1"/>
<pin name="56PDI"/>
</symbol>
<symbol name="AT32UC3A0XXX-P">
<pin name="VDDIO@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="VDDOUT" direction="pwr"/>
<pin name="VDDIN" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="VDDCORE@29" direction="pwr"/>
<pin name="VDDIO@36" direction="pwr"/>
<pin name="GND@37" direction="pwr"/>
<pin name="VDDCORE@51" direction="pwr"/>
<pin name="GND@52" direction="pwr"/>
<pin name="VDDCORE@55" direction="pwr"/>
<pin name="VDDIO@69" direction="pwr"/>
<pin name="GND@72" direction="pwr"/>
<pin name="VDDANA" direction="pwr"/>
<pin name="ADVREF" direction="pwr"/>
<pin name="GNDANA" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="VDDIO@92" direction="pwr"/>
<pin name="VDDIO@93" direction="pwr"/>
<pin name="GND@94" direction="pwr"/>
<pin name="VDDIO@108" direction="pwr"/>
<pin name="GND@109" direction="pwr"/>
<pin name="VDDIO@116" direction="pwr"/>
<pin name="GND@117" direction="pwr"/>
<pin name="VDDCORE@138" direction="pwr"/>
</symbol>
<symbol name="AT32UC3A0XXX-IO">
<pin name="PX00/EBI-DATA[10]/USART0-RXD"/>
<pin name="PX01/EBI-DATA[9]/USART0-TXD"/>
<pin name="PX02/EBI-DATA[8]/USART0-CTS"/>
<pin name="PX03/EBI-DATA[7]/USART0-RTS"/>
<pin name="PX04/EBI-DATA[6]/USART1-RXD"/>
<pin name="PX05/EBI-DATA[5]/USART1-TXD"/>
<pin name="PX06/EBI-DATA[4]/USART1-CTS"/>
<pin name="PX07/EBI-DATA[3]/USART1-RTS"/>
<pin name="PX08/EBI-DATA[2]/USART3-RXD"/>
<pin name="PX09/EBI-DATA[1]/USART3-TXD"/>
<pin name="PX10/EBI-DATA[0]/USART2-RXD"/>
<pin name="PX11/EBI-NWE1/USART2-TXD"/>
<pin name="PX12/EBI-NWE0/USART2-CTS"/>
<pin name="PX13/EBI-NRD/USART2-RTS"/>
<pin name="PX14/EBI-NCS[1]/TC-A0"/>
<pin name="PX15/EBI-ADDR[19]/USART3-RTS/TC-B0"/>
<pin name="PX16/EBI-ADDR[18]/USART3-CTS/TC-A1"/>
<pin name="PX17/EBI-ADDR[17]/TC-B1"/>
<pin name="PX18/EBI-ADDR[16]/TC-A2"/>
<pin name="PX19/EBI-ADDR[15]/EIM-SCAN[0]/TC-B2"/>
<pin name="PX20/EBI-ADDR[14]/EIM-SCAN[1]/TC-CLK0"/>
<pin name="PX21/EBI-ADDR[13]/EIM-SCAN[2]/TC-CLK1"/>
<pin name="PX22/EBI-ADDR[12]/EIM-SCAN[3]/TC-CLK2"/>
<pin name="PX23/EBI-ADDR[11]/EIM-SCAN[4]"/>
<pin name="PX24/EBI-ADDR[10]/EIM-SCAN[5]"/>
<pin name="PX25/EBI-ADDR[9]/EIM-SCAN[6]"/>
<pin name="PX26/EBI-ADDR[8]/EIM-SCAN[7]"/>
<pin name="PX27/EBI-ADDR[7]/SPI0-MISO"/>
<pin name="PX28/EBI-ADDR[6]/SPI0-MOSI"/>
<pin name="PX29/EBI-ADDR[5]/SPI0-SCK"/>
<pin name="PX30/EBI-ADDR[4]/SPI0-NPCS[0]"/>
<pin name="PX31/EBI-ADDR[3]/SPI0-NPCS[1]"/>
<pin name="PX32/EBI-ADDR[2]/SPI0-NPCS[2]"/>
<pin name="PX33/EBI-ADDR[1]/SPI0-NPCS[3]"/>
<pin name="PX34/EBI-ADDR[0]/SPI1-MISO"/>
<pin name="PX35/EBI-DATA[15]/SPI1-MOSI"/>
<pin name="PX36/EBI-DATA[14]/SPI1-SCK"/>
<pin name="PX37/EBI-DATA[13]/SPI1-NPCS[0]"/>
<pin name="PX38/EBI-DATA[12]/SPI1-NPCS[1]"/>
<pin name="PX39/EBI-DATA[11]/SPI1-NPCS[2]"/>
<pin name="TC-CLK0/USART0-RXD/PA00"/>
<pin name="TC-CLK1/USART0-TXD/PA01"/>
<pin name="TC-CLK2/USART0-CLK/PA02"/>
<pin name="DAC-DATA[0]/EIM-EXTINT[4]/USART0-RTS/PA03"/>
<pin name="DAC-DATAN[0]/EIM-EXTINT[5]/USART0-CTS/PA04"/>
<pin name="PWM-PWM[4]/USART1-RXD/PA05"/>
<pin name="PWM-PWM[5]/USART1-TXD/PA06"/>
<pin name="SPI0-NPCS[3]/PM-GCLK[0]/USART1-CLK/PA07"/>
<pin name="EIM-EXTINT[7]/SPI0-NPCS[1]/USART1-RTS/PA08"/>
<pin name="MACB-WOL/SPI0-NPCS[2]/USART1-CTS/PA09"/>
<pin name="EIM-EXTINT[6]/SPI0-NPCS[0]/PA10"/>
<pin name="USB-USB_ID/SPI0-MISO/PA11"/>
<pin name="USB-USB_VBOF/SPI0-MOSI/PA12"/>
<pin name="SPI0-SCK/PA13"/>
<pin name="EBI-NCS[0]/SPI1-NPCS[0]/SSC-TX_FRAME_SYNC/PA14"/>
<pin name="EBI-ADDR[20]/SPI1-SCK/SSC-TX_CLOCK/PA15"/>
<pin name="EBI-ADDR[21]/SPI1-MOSI/SSC-TX_DATA/PA16"/>
<pin name="EBI-ADDR[22]/SPI1-MISO/SSC-RX_DATA/PA17"/>
<pin name="MACB-WOL/SPI1-NPCS[1]/SSC-RX_CLOCK/PA18"/>
<pin name="SPI1-NPCS[2]/SSC-RX_FRAME_SYNC/PA19"/>
<pin name="SPI1-NPCS[3]/EIM-EXTINT[8]/PA20"/>
<pin name="USB-USB_ID/EIM-EXTINT[0]/ADC-AD[0]/PA21"/>
<pin name="USB-USB_VBOF/EIM-EXTINT[1]/ADC-AD[1]/PA22"/>
<pin name="DAC-DATA[1]/EIM-EXTINT[2]/ADC-AD[2]/PA23"/>
<pin name="DAC-DATAN[1]/EIM-EXTINT[3]/ADC-AD[3]/PA24"/>
<pin name="EBI-NCS[0]/EIM-SCAN[0]/ADC-AD[4]/PA25"/>
<pin name="EBI-ADDR[20]/EIM-SCAN[1]/ADC-AD[5]/PA26"/>
<pin name="EBI-ADDR[21]/EIM-SCAN[2]/ADC-AD[6]/PA27"/>
<pin name="EBI-ADDR[22]/EIM-SCAN[3]/ADC-AD[7]/PA28"/>
<pin name="USART2-RTS/TWI-SDA/PA29"/>
<pin name="USART2-CTS/TWI-SCL/PA30"/>
<pin name="EIM-SCAN[5]/PM-GCLK[1]/PWM-PWM[1]/PB20"/>
<pin name="EIM-SCAN[6]/PM-GCLK[2]/PWM-PWM[2]/PB21"/>
<pin name="EIM-SCAN[7]/PM-GCLK[3]/PWM-PWM[3]/PB22"/>
<pin name="USART1-DCD/TC-A0/PB23"/>
<pin name="USART1-DSR/TC-B0/PB24"/>
<pin name="USART1-DTR/TC-A1/PB25"/>
<pin name="USART1-RI/TC-B1/PB26"/>
<pin name="PWM-PWM[4]/TC-A2/PB27"/>
<pin name="PWM-PWM[5]/TC-B2/PB28"/>
<pin name="EBI-NCS[2]/PM-GCLK[1]/USART2-RXD/PB29"/>
<pin name="EBI-SDCS/PM-GCLK[2]/USART2-TXD/PB30"/>
<pin name="EBI-NWAIT/PM-GCLK[3]/USART2-CLK/PB31"/>
<pin name="USART3-RTS/USART2-RTS/MACB-TX_CLK/PB00"/>
<pin name="USART3-CTS/USART2-CTS/MACB-TX_EN/PB01"/>
<pin name="DAC-DATA[0]/MACB-TXD[0]/PB02"/>
<pin name="DAC-DATAN[0]/MACB-TXD[1]/PB03"/>
<pin name="EBI-NCS[3]/USART3-CLK/MACB-CRS/PB04"/>
<pin name="DAC-DATA[1]/MACB-RXD[0]/PB05"/>
<pin name="DAC-DATAN[1]/MACB-RXD[1]/PB06"/>
<pin name="MACB-RX_ER/PB07"/>
<pin name="MACB-MDC/PB08"/>
<pin name="MACB-MDIO/PB09"/>
<pin name="EBI-SDCK/USART3-RXD/MACB-TXD[2]/PB10"/>
<pin name="EBI-SDCKE/USART3-TXD/MACB-TXD[3]/PB11"/>
<pin name="EBI-RAS/TC-CLK0/MACB-TX_ER/PB12"/>
<pin name="EBI-CAS/TC-CLK1/MACB-RXD[2]/PB13"/>
<pin name="EBI-SDWE/TC-CLK2/MACB-RXD[3]/PB14"/>
<pin name="MACB-RX_DV/PB15"/>
<pin name="EBI-SDA10/USB-USB_ID/MACB-COL/PB16"/>
<pin name="EBI-ADDR[23]/USB-USB_VBOF/MACB-RX_CLK/PB17"/>
<pin name="PWM-PWM[6]/ADC-TRIGGER/MACB-SPEED/PB18"/>
<pin name="EIM-SCAN[4]/PM-GCLK[0]/PWM-PWM[0]/PB19"/>
<pin name="PC00/XIN32"/>
<pin name="PC01/XOUT32"/>
<pin name="PC02/XIN0"/>
<pin name="PC03/XOUT0"/>
<pin name="PC04/XIN1"/>
<pin name="PC05/XOUT1"/>
<pin name="VBUS"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="TDO"/>
<pin name="TDI"/>
<pin name="!RESET" direction="in"/>
<pin name="NC@49" direction="nc"/>
</symbol>
<symbol name="AT32UC3A1XXX">
<pin name="EIM-SCAN[5]/PM-GCLK[1]/PWM-PWM[1]/PB20"/>
<pin name="EIM-SCAN[6]/PM-GCLK[2]/PWM-PWM[2]/PB21"/>
<pin name="EIM-SCAN[7]/PM-GCLK[3]/PWM-PWM[3]/PB22"/>
<pin name="VDDIO@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="USART1-DCD/TC-A0/PB23"/>
<pin name="USART1-DSR/TC-B0/PB24"/>
<pin name="USART1-DTR/TC-A1/PB25"/>
<pin name="USART1-RI/TC-B1/PB26"/>
<pin name="PWM-PWM[4]/TC-A2/PB27"/>
<pin name="VDDOUT" direction="pwr"/>
<pin name="VDDIN" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="PWM-PWM[5]/TC-B2/PB28"/>
<pin name="EBI-NCS[2]/PM-GCLK[1]/USART2-RXD/PB29"/>
<pin name="EBI-SDCS/PM-GCLK[2]/USART2-TXD/PB30"/>
<pin name="EBI-NWAIT/PM-GCLK[3]/USART2-CLK/PB31"/>
<pin name="!RESET" direction="in"/>
<pin name="TC-CLK0/USART0-RXD/PA00"/>
<pin name="TC-CLK1/USART0-TXD/PA01"/>
<pin name="GND@21" direction="pwr"/>
<pin name="VDDCORE@22" direction="pwr"/>
<pin name="TC-CLK2/USART0-CLK/PA02"/>
<pin name="DAC-DATA[0]/EIM-EXTINT[4]/USART0-RTS/PA03"/>
<pin name="DAC-DATAN[0]/EIM-EXTINT[5]/USART0-CTS/PA04"/>
<pin name="PWM-PWM[4]/USART1-RXD/PA05"/>
<pin name="PWM-PWM[5]/USART1-TXD/PA06"/>
<pin name="SPI0-NPCS[3]/PM-GCLK[0]/USART1-CLK/PA07"/>
<pin name="EIM-EXTINT[7]/SPI0-NPCS[1]/USART1-RTS/PA08"/>
<pin name="MACB-WOL/SPI0-NPCS[2]/USART1-CTS/PA09"/>
<pin name="EIM-EXTINT[6]/SPI0-NPCS[0]/PA10"/>
<pin name="NC@32" direction="nc"/>
<pin name="USB-USB_ID/SPI0-MISO/PA11"/>
<pin name="VDDCORE@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="USB-USB_VBOF/SPI0-MOSI/PA12"/>
<pin name="SPI0-SCK/PA13"/>
<pin name="VDDCORE@38" direction="pwr"/>
<pin name="EBI-NCS[0]/SPI1-NPCS[0]/SSC-TX_FRAME_SYNC/PA14"/>
<pin name="EBI-ADDR[20]/SPI1-SCK/SSC-TX_CLOCK/PA15"/>
<pin name="EBI-ADDR[21]/SPI1-MOSI/SSC-TX_DATA/PA16"/>
<pin name="EBI-ADDR[22]/SPI1-MISO/SSC-RX_DATA/PA17"/>
<pin name="MACB-WOL/SPI1-NPCS[1]/SSC-RX_CLOCK/PA18"/>
<pin name="SPI1-NPCS[2]/SSC-RX_FRAME_SYNC/PA19"/>
<pin name="SPI1-NPCS[3]/EIM-EXTINT[8]/PA20"/>
<pin name="VBUS"/>
<pin name="VDDIO@47" direction="pwr"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="GND@50" direction="pwr"/>
<pin name="USB-USB_ID/EIM-EXTINT[0]/ADC-AD[0]/PA21"/>
<pin name="USB-USB_VBOF/EIM-EXTINT[1]/ADC-AD[1]/PA22"/>
<pin name="DAC-DATA[1]/EIM-EXTINT[2]/ADC-AD[2]/PA23"/>
<pin name="DAC-DATAN[1]/EIM-EXTINT[3]/ADC-AD[3]/PA24"/>
<pin name="EBI-NCS[0]/EIM-SCAN[0]/ADC-AD[4]/PA25"/>
<pin name="EBI-ADDR[20]/EIM-SCAN[1]/ADC-AD[5]/PA26"/>
<pin name="EBI-ADDR[21]/EIM-SCAN[2]/ADC-AD[6]/PA27"/>
<pin name="EBI-ADDR[22]/EIM-SCAN[3]/ADC-AD[7]/PA28"/>
<pin name="VDDANA" direction="pwr"/>
<pin name="ADVREF" direction="pwr"/>
<pin name="GNDANA" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="PC00/XIN32"/>
<pin name="PC01/XOUT32"/>
<pin name="USART3-RTS/USART2-RTS/MACB-TX_CLK/PB00"/>
<pin name="USART3-CTS/USART2-CTS/MACB-TX_EN/PB01"/>
<pin name="VDDIO@67" direction="pwr"/>
<pin name="VDDIO@68" direction="pwr"/>
<pin name="GND@69" direction="pwr"/>
<pin name="DAC-DATA[0]/MACB-TXD[0]/PB02"/>
<pin name="DAC-DATAN[0]/MACB-TXD[1]/PB03"/>
<pin name="EBI-NCS[3]/USART3-CLK/MACB-CRS/PB04"/>
<pin name="DAC-DATA[1]/MACB-RXD[0]/PB05"/>
<pin name="DAC-DATAN[1]/MACB-RXD[1]/PB06"/>
<pin name="MACB-RX_ER/PB07"/>
<pin name="MACB-MDC/PB08"/>
<pin name="MACB-MDIO/PB09"/>
<pin name="EBI-SDCK/USART3-RXD/MACB-TXD[2]/PB10"/>
<pin name="VDDIO@79" direction="pwr"/>
<pin name="GND@80" direction="pwr"/>
<pin name="EBI-SDCKE/USART3-TXD/MACB-TXD[3]/PB11"/>
<pin name="EBI-RAS/TC-CLK0/MACB-TX_ER/PB12"/>
<pin name="USART2-RTS/TWI-SDA/PA29"/>
<pin name="USART2-CTS/TWI-SCL/PA30"/>
<pin name="PC02/XIN0"/>
<pin name="PC03/XOUT0"/>
<pin name="EBI-CAS/TC-CLK1/MACB-RXD[2]/PB13"/>
<pin name="EBI-SDWE/TC-CLK2/MACB-RXD[3]/PB14"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="TDO"/>
<pin name="TDI"/>
<pin name="PC04/XIN1"/>
<pin name="PC05/XOUT1"/>
<pin name="MACB-RX_DV/PB15"/>
<pin name="EBI-SDA10/USB-USB_ID/MACB-COL/PB16"/>
<pin name="VDDCORE@97" direction="pwr"/>
<pin name="EBI-ADDR[23]/USB-USB_VBOF/MACB-RX_CLK/PB17"/>
<pin name="PWM-PWM[6]/ADC-TRIGGER/MACB-SPEED/PB18"/>
<pin name="EIM-SCAN[4]/PM-GCLK[0]/PWM-PWM[0]/PB19"/>
</symbol>
<symbol name="AT32UC3B0XXX">
<pin name="PA06/GPIO6/ADC3/USART1-DSR" direction="in"/>
<pin name="GND@49" direction="pwr"/>
<pin name="PA07/GPIO7/PWM0/ADC4/USART1-DTR" direction="in"/>
<pin name="VDDIO@64" direction="pwr"/>
<pin name="PA08/GPIO8/PWM1/ADC5/USART1-RI" direction="in"/>
<pin name="PA09/GPIO9/SCL/SPI-CS2/USART1-CTS" direction="in"/>
<pin name="PA10/GPIO10/SDA/SI-CS3/USART1-RTS" direction="in"/>
<pin name="VDDCORE@56" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="USB_DM"/>
<pin name="VBUS" direction="in"/>
<pin name="!RESET"/>
<pin name="PB10/GPIO42/SSC-TX_DATA/TC-A2/USART0-RXD"/>
<pin name="VDDANA" direction="pwr"/>
<pin name="VDDOUT" direction="pwr"/>
<pin name="VDDIN" direction="pwr"/>
<pin name="PA22/GPIO22/PWM6/TC-B1/ADC-TRIGGER"/>
<pin name="PA23/GPIO23/USART1-TXD/SPI-CS1/EXTIN3"/>
<pin name="PA24/GPIO24/USART1-RXD/SPIC-CS0/EXTINT4"/>
<pin name="PA25/GPIO25/SPI-MISO/PWM3/EXTINT5"/>
<pin name="PA26/GPIO26/USB_ID/USART2-TXD/TC-A0"/>
<pin name="PA27/GPIO27/USB_VBOF/USART2-RXD/TC-B0"/>
<pin name="PB03/GPIO35/EXTINT7/TC-B1/USART1-RXD"/>
<pin name="PB02/GPIO34/EXTINT6/TC-A1/USART1-TXD"/>
<pin name="PB07/GPIO39/SSC-RX_DATA/USART-DSR/EIC-SCAN5"/>
<pin name="PB06/GPIO38/SSC-RX_CLOCK/USART-DCD/EIC-SCAN4"/>
<pin name="PA11/GPIO11/USART0-RTS/TC-A2/PWM0/XIN32"/>
<pin name="PB11/GPIO43/SSC-TX_FRAME_SYNC/TC-B2/USART0-TXD"/>
<pin name="PB05/GPIO37/USART1-RTS/SPI-CS2/PWM5"/>
<pin name="PB04/GPIO36/USART1-CTS/SPI-CS3/TC-CLK2"/>
<pin name="PA19/GPIO19/USART0-TXD/PWM6/SPI-MOSI/XOUT"/>
<pin name="PA20/GPIO20/USART1-CLK/TC-CLK0/USART2-RXD"/>
<pin name="GND@17" direction="pwr"/>
<pin name="USB_DP"/>
<pin name="PB00/GPIO32/TC-A0/EIC-SCAN2/USART2-CTS"/>
<pin name="PA03/GPIO3/ADC0/GCLK0/USB_ID"/>
<pin name="PA13/GPIO13/NMI/PWM2/USART0-CLK"/>
<pin name="VDDCORE@8" direction="pwr"/>
<pin name="PB09/GPIO41/SSC-TX_CLOCK/USART1-RI/EIC-SCAN7"/>
<pin name="PA12/GPIO12/USART0-CTS/TC-B2/PWM1/XOUT32"/>
<pin name="VDDIO@48" direction="pwr"/>
<pin name="PA17/GPIO17/SPI-CS1/TC-CLK2/SPI-SCK"/>
<pin name="GND@23" direction="pwr"/>
<pin name="PA16/GPIO16/SPI-CS0/TC-CLK1"/>
<pin name="PA15/GPIO15/SPI-SCK/PWM4/USART2-CLK"/>
<pin name="TDO/GPIO1"/>
<pin name="PA14/GPIO14/SPI-MOSI/PWM3/EXTINT2"/>
<pin name="TMS/GPIO2"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="PA04/GPIO4/ADC1/USB_VBOF"/>
<pin name="PA05/GPIO5/EXTINT0/ADC2/USART1-DCD"/>
<pin name="VDDCORE@22" direction="pwr"/>
<pin name="PB01/GPIO33/TC-B0/EIC-SCAN3/USART2-RTS"/>
<pin name="PB08/GPIO40/SSC-RX_FRAME_SYNC/USART1-DTR/EIC-SCAN6"/>
<pin name="PA29/GPIO29/TC-CLK0/TC-CLK1/SPI-MOSI/XOUT1"/>
<pin name="TCK" direction="in"/>
<pin name="PA28/GPIO28/USART0-CLK/PWM4/SPI-MISO/XIN1"/>
<pin name="VDDIO@32" direction="pwr"/>
<pin name="PA31/GPIO31/ADC7/EIC-SCAN1"/>
<pin name="TDI/GPIO0"/>
<pin name="PA21/GPIO21/PWM2/TC-A1/USART2-TXD"/>
<pin name="PA18/GPIO18/USART0-RXD/PWM5/SPI-MISO/XIN"/>
<pin name="PA30/GPIO30/ADC6/EIC-SCAN0/GCLK2" direction="in"/>
<pin name="ADVREF" direction="pwr"/>
</symbol>
<symbol name="AT32UC3B1XXX">
<pin name="GND@1"/>
<pin name="TCK"/>
<pin name="TDI/GPIO0"/>
<pin name="TDO/GPIO1"/>
<pin name="TMS/GPIO2"/>
<pin name="VDDCORE@6"/>
<pin name="PA03/GPIO3/ADC0/GCLK0/USB_ID"/>
<pin name="PA04/GPIO4/ADC1/USB_VBOF"/>
<pin name="PA05/GPIO5/EXTINT0/ADC2/USART1-DCD"/>
<pin name="PA06/GPIO6/ADC3/USART1-DSR"/>
<pin name="PA07/GPIO7/PWM0/ADC4/USART1-DTR"/>
<pin name="PA08/GPIO8/PWM1/ADC5/USART1-RI"/>
<pin name="GND@13"/>
<pin name="ADVREF"/>
<pin name="VDDANA"/>
<pin name="VDDOUT"/>
<pin name="VDDIN"/>
<pin name="VDDCORE@18"/>
<pin name="GND@19"/>
<pin name="PA09/GPIO9/SCL/SPI-CS2/USART1-CTS"/>
<pin name="PA10/GPIO10/SDA/SI-CS3/USART1-RTS"/>
<pin name="PA11/GPIO11/USART0-RTS/TC-A2/PWM0/XIN32"/>
<pin name="PA12/GPIO12/USART0-CTS/TC-B2/PWM1/XOUT32"/>
<pin name="VDDIO@24"/>
<pin name="PA13/GPIO13/NMI/PWM2/USART0-CLK"/>
<pin name="PA14/GPIO14/SPI-MOSI/PWM3/EXTINT2"/>
<pin name="PA15/GPIO15/SPI-SCK/PWM4/USART2-CLK"/>
<pin name="PA16/GPIO16/SPI-CS0/TC-CLK1"/>
<pin name="PA17/GPIO17/SPI-CS1/TC-CLK2/SPI-SCK"/>
<pin name="PA18/GPIO18/USART0-RXD/PWM5/SPI-MISO/XIN"/>
<pin name="PA19/GPIO19/USART0-TXD/PWM6/SPI-MOSI/XOUT"/>
<pin name="PA20/GPIO20/USART1-CLK/TC-CLK0/USART2-RXD"/>
<pin name="PA21/GPIO21/PWM2/TC-A1/USART2-TXD"/>
<pin name="PA22/GPIO22/PWM6/TC-B1/ADC-TRIGGER"/>
<pin name="PA23/GPIO23/USART1-TXD/SPI-CS1/EXTIN3"/>
<pin name="VDDIO@36"/>
<pin name="GND@37"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="VBUS"/>
<pin name="VDDPLL"/>
<pin name="VDDCORE@42"/>
<pin name="PA24/GPIO24/USART1-RXD/SPIC-CS0/EXTINT4"/>
<pin name="PA25/GPIO25/SPI-MISO/PWM3/EXTINT5"/>
<pin name="PA26/GPIO26/USB_ID/USART2-TXD/TC-A0"/>
<pin name="PA27/GPIO27/USB_VBOF/USART2-RXD/TC-B0"/>
<pin name="!RESET"/>
<pin name="VDDIO@48"/>
</symbol>
<symbol name="AT32UC3LXXXX">
<pin name="PA00"/>
<pin name="PA01"/>
<pin name="PA02"/>
<pin name="PA03"/>
<pin name="PA04"/>
<pin name="PA05"/>
<pin name="PA06"/>
<pin name="PA07"/>
<pin name="PA08"/>
<pin name="PA09"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PA16"/>
<pin name="PA17"/>
<pin name="PB00"/>
<pin name="PB01"/>
<pin name="PB03"/>
<pin name="PB04"/>
<pin name="PB05"/>
<pin name="PB06"/>
<pin name="PB07"/>
<pin name="PB08"/>
<pin name="PB09"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="VDDANA"/>
<pin name="VDDCORE"/>
<pin name="VDDIN"/>
<pin name="VDDIO@42"/>
<pin name="VDDIO@48"/>
<pin name="ADVREFP"/>
<pin name="GNDANA"/>
<pin name="GND@43"/>
<pin name="GND@45"/>
<pin name="GND@1"/>
<pin name="GND@19"/>
<pin name="PA18"/>
<pin name="PA19"/>
<pin name="PA20"/>
<pin name="PA21"/>
<pin name="PA22"/>
<pin name="PB02"/>
<pin name="RESET_N"/>
</symbol>
<symbol name="AVR-JTAG-10">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="AT32UC3C0">
<pin name="VDD_5"/>
<pin name="VDDIO2"/>
<pin name="VDDANA"/>
<pin name="VDD_33"/>
<pin name="VDDIO1"/>
<pin name="VDDIO3"/>
<pin name="VDDCORE"/>
<pin name="VDDIO4"/>
<pin name="ADCVREFP"/>
<pin name="!RESET"/>
<pin name="ADCVREFN"/>
<pin name="GNDCORE"/>
<pin name="GNDANA"/>
<pin name="GNDIO1"/>
<pin name="GNDIO2"/>
<pin name="GNDIO3"/>
<pin name="GNDIO4"/>
<pin name="VBUS"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="GNDPLL"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PA16"/>
<pin name="PA19"/>
<pin name="PA20"/>
<pin name="PA21"/>
<pin name="PA22"/>
<pin name="PA23"/>
<pin name="PA24"/>
<pin name="PA25"/>
<pin name="PA26"/>
<pin name="PA27"/>
<pin name="PA28"/>
<pin name="PA29"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PB16"/>
<pin name="PB17"/>
<pin name="PB18"/>
<pin name="PB19"/>
<pin name="PB20"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB24"/>
<pin name="PB25"/>
<pin name="PB26"/>
<pin name="PB27"/>
<pin name="PB28"/>
<pin name="PB29"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC16"/>
<pin name="PC17"/>
<pin name="PC18"/>
<pin name="PC19"/>
<pin name="PC20"/>
<pin name="PC21"/>
<pin name="PC22"/>
<pin name="PC23"/>
<pin name="PC24"/>
<pin name="PC25"/>
<pin name="PC26"/>
<pin name="PC27"/>
<pin name="PC28"/>
<pin name="PC29"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PD16"/>
<pin name="PD17"/>
<pin name="PD18"/>
<pin name="PD19"/>
<pin name="PD20"/>
<pin name="PD21"/>
<pin name="PD22"/>
<pin name="PD23"/>
<pin name="PD24"/>
<pin name="PD25"/>
<pin name="PD26"/>
<pin name="PD27"/>
<pin name="PD28"/>
<pin name="PD29"/>
<pin name="PB30"/>
<pin name="PB31"/>
<pin name="PC30"/>
<pin name="PC31"/>
<pin name="PD30"/>
</symbol>
<symbol name="AT32UC3C1">
<pin name="ADCREFP"/>
<pin name="VDDCORE"/>
<pin name="VDDANA"/>
<pin name="VDDIO3"/>
<pin name="VDDIO2"/>
<pin name="VDDIO1"/>
<pin name="VDD_33"/>
<pin name="VDD_5"/>
<pin name="!RESET"/>
<pin name="GNDIO1"/>
<pin name="GNDIO2"/>
<pin name="GNDIO3"/>
<pin name="GNDANA"/>
<pin name="GNDCORE"/>
<pin name="ADCREFN"/>
<pin name="VBUS"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="GNDPLL"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB19"/>
<pin name="PB20"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB30"/>
<pin name="PB31"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC16"/>
<pin name="PC17"/>
<pin name="PC18"/>
<pin name="PC19"/>
<pin name="PC20"/>
<pin name="PC21"/>
<pin name="PC22"/>
<pin name="PC23"/>
<pin name="PC24"/>
<pin name="PC31"/>
<pin name="PD30"/>
<pin name="PD29"/>
<pin name="PD28"/>
<pin name="PD27"/>
<pin name="PD24"/>
<pin name="PD23"/>
<pin name="PD22"/>
<pin name="PD21"/>
<pin name="PD14"/>
<pin name="PD13"/>
<pin name="PD12"/>
<pin name="PD11"/>
<pin name="PD10"/>
<pin name="PD9"/>
<pin name="PD8"/>
<pin name="PD7"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="PA25"/>
<pin name="PA24"/>
<pin name="PA23"/>
<pin name="PA22"/>
<pin name="PA21"/>
<pin name="PA20"/>
<pin name="PA16"/>
<pin name="PA19"/>
</symbol>
<symbol name="AT32UC3C2">
<pin name="VDD33"/>
<pin name="VDDIO1"/>
<pin name="VDDIO2"/>
<pin name="VDDIO3"/>
<pin name="VDDANA"/>
<pin name="VDDCORE"/>
<pin name="GNDCORE"/>
<pin name="GNDANA"/>
<pin name="VDD5"/>
<pin name="GNDIO1"/>
<pin name="GNDIO2"/>
<pin name="GNDIO3"/>
<pin name="GNDPLL"/>
<pin name="!RESET"/>
<pin name="ADCVREFN"/>
<pin name="ADCVREFP"/>
<pin name="VBUS"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA16"/>
<pin name="PA19"/>
<pin name="PA20"/>
<pin name="PA21"/>
<pin name="PA22"/>
<pin name="PA23"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD21"/>
<pin name="PD27"/>
<pin name="PD28"/>
<pin name="PD29"/>
<pin name="PD30"/>
<pin name="PB31"/>
<pin name="PB30"/>
<pin name="PB1"/>
<pin name="PB0"/>
<pin name="PC22"/>
<pin name="PC21"/>
<pin name="PC20"/>
<pin name="PC19"/>
<pin name="PC18"/>
<pin name="PC17"/>
<pin name="PC16"/>
<pin name="PC15"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
</symbol>
<symbol name="ATTINY25_45_85">
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="NRES/PB5"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="A4U">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="C4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="D4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="A4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="A1">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PH0"/>
<pin name="PJ0"/>
<pin name="PK0"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PH1"/>
<pin name="PJ1"/>
<pin name="PK1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PH2"/>
<pin name="PJ2"/>
<pin name="PK2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PH3"/>
<pin name="PJ3"/>
<pin name="PK3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PH4"/>
<pin name="PJ4"/>
<pin name="PK4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PH5"/>
<pin name="PJ5"/>
<pin name="PK5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PH6"/>
<pin name="PJ6"/>
<pin name="PK6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="PH7"/>
<pin name="PJ7"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="A1U">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PH0"/>
<pin name="PJ0"/>
<pin name="PK0"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PH1"/>
<pin name="PJ1"/>
<pin name="PK1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PH2"/>
<pin name="PJ2"/>
<pin name="PK2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PH3"/>
<pin name="PJ3"/>
<pin name="PK3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PH4"/>
<pin name="PJ4"/>
<pin name="PK4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PH5"/>
<pin name="PJ5"/>
<pin name="PK5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PH6"/>
<pin name="PJ6"/>
<pin name="PK6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="PH7"/>
<pin name="PJ7"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="A3">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET!/PDI"/>
<pin name="PDI"/>
</symbol>
<symbol name="B1">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PE3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PE4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PE5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PE6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PE7"/>
<pin name="SEG0"/>
<pin name="SEG1"/>
<pin name="SEG2"/>
<pin name="SEG3"/>
<pin name="SEG4"/>
<pin name="SEG5"/>
<pin name="SEG6"/>
<pin name="SEG7"/>
<pin name="SEG8"/>
<pin name="SEG9"/>
<pin name="SEG10"/>
<pin name="SEG11"/>
<pin name="SEG12"/>
<pin name="SEG13"/>
<pin name="SEG14"/>
<pin name="SEG15"/>
<pin name="SEG16"/>
<pin name="SEG17"/>
<pin name="SEG18"/>
<pin name="SEG19"/>
<pin name="SEG20"/>
<pin name="SEG21"/>
<pin name="SEG22"/>
<pin name="SEG23"/>
<pin name="COM0"/>
<pin name="COM1"/>
<pin name="COM2"/>
<pin name="COM3"/>
<pin name="VCC"/>
<pin name="AVCC"/>
<pin name="GND"/>
<pin name="AGND"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="BIAS1"/>
<pin name="BIAS2"/>
<pin name="CAPL"/>
<pin name="CAPH"/>
<pin name="VLCD"/>
<pin name="PG0/SEG39"/>
<pin name="PG1/SEG38"/>
<pin name="PG2/SEG37"/>
<pin name="PG3/SEG36"/>
<pin name="PG4/SEG35"/>
<pin name="PG5/SEG34"/>
<pin name="PG6/SEG33"/>
<pin name="PG7/SEG32"/>
<pin name="PM0/SEG31"/>
<pin name="PM1/SEG30"/>
<pin name="PM2/SEG29"/>
<pin name="PM3/SEG28"/>
<pin name="PM4/SEG27"/>
<pin name="PM5/SEG26"/>
<pin name="PM6/SEG25"/>
<pin name="PM7/SEG24"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
</symbol>
<symbol name="B3">
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="SEG0"/>
<pin name="SEG1"/>
<pin name="SEG2"/>
<pin name="SEG3"/>
<pin name="SEG4"/>
<pin name="SEG5"/>
<pin name="SEG6"/>
<pin name="SEG7"/>
<pin name="SEG8"/>
<pin name="COM0"/>
<pin name="COM1"/>
<pin name="COM2"/>
<pin name="COM3"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="BIAS1"/>
<pin name="BIAS2"/>
<pin name="VLCD"/>
<pin name="CAPL"/>
<pin name="CAPH"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PG0/SEG24"/>
<pin name="PG1/SEG23"/>
<pin name="PG2/SEG22"/>
<pin name="PG3/SEG21"/>
<pin name="PG4/SEG20"/>
<pin name="PG5/SEG19"/>
<pin name="PG6/SEG18"/>
<pin name="PG7/SEG17"/>
<pin name="PM0/SEG16"/>
<pin name="PM1/SEG15"/>
<pin name="PM2/SEG14"/>
<pin name="PM3/SEG13"/>
<pin name="PM4/SEG12"/>
<pin name="PM5/SEG11"/>
<pin name="PM6/SEG10"/>
<pin name="PM7/SEG9"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="C3">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET!/PDI"/>
<pin name="PDI"/>
</symbol>
<symbol name="D3">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET!/PDI"/>
<pin name="PDI"/>
</symbol>
<symbol name="AVR-ISP-6">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6PAD_ISP">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
<symbol name="AVR-ISP-10">
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="AVR-PDI">
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="AVR-TPI">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="ATMEGA48/88/168-TQFP/QFN32">
<pin name="PB5(SCK/PCINT5)"/>
<pin name="PB7(XTAL2/TOSC2/PCINT7)"/>
<pin name="PB6(XTAL1/TOSC1/PCINT6)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pas"/>
<pin name="PB4(MISO/PCINT4)"/>
<pin name="PB3(MOSI/OC2A/PCINT3)"/>
<pin name="PB2(SS/OC1B/PCINT2)"/>
<pin name="PB1(OC1A/PCINT1)"/>
<pin name="PB0(ICP1/CLKO/PCINT0)"/>
<pin name="PD7(AIN1/PCINT23)"/>
<pin name="PD6(AIN0/OC0A/PCINT22)"/>
<pin name="PD5(T1/OC0B/PCINT21)"/>
<pin name="PD4(T0/XCK/PCINT20)"/>
<pin name="PD3(INT1/OC2B/PCINT19)"/>
<pin name="PD2(INT0/PCINT18)"/>
<pin name="PD1(TXD/PCINT17)"/>
<pin name="PD0(RXD/PCINT16)"/>
<pin name="PC5(ADC5/SCL/PCINT13)"/>
<pin name="PC4(ADC4/SDA/PCINT12)"/>
<pin name="PC3(ADC3/PCINT11)"/>
<pin name="PC2(ADC2/PCINT10)"/>
<pin name="PC1(ADC1/PCINT9)"/>
<pin name="PC0(ADC0/PCINT8)"/>
<pin name="PC6(/RESET/PCINT14)"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="ADC7" direction="pas"/>
<pin name="ADC6" direction="pas"/>
</symbol>
<symbol name="ATMEGA48/88/168">
<pin name="PB5(SCK/PCINT5)"/>
<pin name="PB7(XTAL2/TOSC2/PCINT7)"/>
<pin name="PB6(XTAL1/TOSC1/PCINT6)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pas"/>
<pin name="PB4(MISO/PCINT4)"/>
<pin name="PB3(MOSI/OC2A/PCINT3)"/>
<pin name="PB2(SS/OC1B/PCINT2)"/>
<pin name="PB1(OC1A/PCINT1)"/>
<pin name="PB0(ICP1/CLKO/PCINT0)"/>
<pin name="PD7(AIN1/PCINT23)"/>
<pin name="PD6(AIN0/OC0A/PCINT22)"/>
<pin name="PD5(T1/OC0B/PCINT21)"/>
<pin name="PD4(T0/XCK/PCINT20)"/>
<pin name="PD3(INT1/OC2B/PCINT19)"/>
<pin name="PD2(INT0/PCINT18)"/>
<pin name="PD1(TXD/PCINT17)"/>
<pin name="PD0(RXD/PCINT16)"/>
<pin name="PC5(ADC5/SCLPCINT13)"/>
<pin name="PC4(ADC4/SDA/PCINT12)"/>
<pin name="PC3(ADC3/PCINT11)"/>
<pin name="PC2(ADC2/PCINT10)"/>
<pin name="PC1(ADC1/PCINT9)"/>
<pin name="PC0(ADC0/PCINT8)"/>
<pin name="PC6(/RESET/PCINT14)"/>
</symbol>
<symbol name="ATMEGA164P/324P/644P-TQFP">
<pin name="(XCK0/T0/PCINT8)PB0"/>
<pin name="(CLKO/T1/PCINT9)PB1"/>
<pin name="(INT2/AIN0/PCINT10)PB2"/>
<pin name="(OC0A/AIN1/PCINT11)PB3"/>
<pin name="(OC0B/!SS!/PCINT12)PB4"/>
<pin name="(MOSI/PCINT13)PB5"/>
<pin name="(MISO/PCINT14)PB6"/>
<pin name="(SCK/PCINT15)PB7"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="(RXD0/PCINT24)PD0"/>
<pin name="(TXD0/PCINT25)PD1"/>
<pin name="(RXD1/INT0/PCINT26)PD2"/>
<pin name="(TXD1/INT1/PCINT27)PD3"/>
<pin name="(XCK1/OC1B/PCINT28)PD4"/>
<pin name="(OC1A/PCINT29)PD5"/>
<pin name="(OC2B/ICP/PCINT30)PD6"/>
<pin name="(OC2A/PCINT31)PD7"/>
<pin name="(SCL/PCINT16)PC0"/>
<pin name="(SDA/PCINT17)PC1"/>
<pin name="(TCK/PCINT18)PC2"/>
<pin name="(TMS/PCINT19)PC3"/>
<pin name="(TDO/PCINT20)PC4"/>
<pin name="(TDI/PCINT21)PC5"/>
<pin name="(TOSC1/PCINT22)PC6"/>
<pin name="(TOSC2/PCINT23)PC7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="(ADC7/PCINT7)PA7"/>
<pin name="(ADC6/PCINT6)PA6"/>
<pin name="(ADC5/PCINT5)PA5"/>
<pin name="(ADC4/PCINT4)PA4"/>
<pin name="(ADC3/PCINT3)PA3"/>
<pin name="(ADC2/PCINT2)PA2"/>
<pin name="(ADC1/PCINT1)PA1"/>
<pin name="(ADC0/PCINT0)PA0"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="ATMEGA164P/324P/644P">
<pin name="(XCK0/T0/PCINT8)PB0"/>
<pin name="(CLKO/T1/PCINT9)PB1"/>
<pin name="(INT2/AIN0/PCINT10)PB2"/>
<pin name="(OC0A/AIN1/PCINT11)PB3"/>
<pin name="(OC0B/!SS!/PCINT12)PB4"/>
<pin name="(MOSI/PCINT13)PB5"/>
<pin name="(MISO/PCINT14)PB6"/>
<pin name="(SCK/PCINT15)PB7"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="(RXD0/PCINT24)PD0"/>
<pin name="(TXD0/PCINT25)PD1"/>
<pin name="(RXD1/INT0/PCINT26)PD2"/>
<pin name="(TXD1/INT1/PCINT27)PD3"/>
<pin name="(XCK1/OC1B/PCINT28)PD4"/>
<pin name="(OC1A/PCINT29)PD5"/>
<pin name="(OC2B/ICP/PCINT30)PD6"/>
<pin name="(OC2A/PCINT31)PD7"/>
<pin name="(SCL/PCINT16)PC0"/>
<pin name="(SDA/PCINT17)PC1"/>
<pin name="(TCK/PCINT18)PC2"/>
<pin name="(TMS/PCINT19)PC3"/>
<pin name="(TDO/PCINT20)PC4"/>
<pin name="(TDI/PCINT21)PC5"/>
<pin name="(TOSC1/PCINT22)PC6"/>
<pin name="(TOSC2/PCINT23)PC7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="(ADC7/PCINT7)PA7"/>
<pin name="(ADC6/PCINT6)PA6"/>
<pin name="(ADC5/PCINT5)PA5"/>
<pin name="(ADC4/PCINT4)PA4"/>
<pin name="(ADC3/PCINT3)PA3"/>
<pin name="(ADC2/PCINT2)PA2"/>
<pin name="(ADC1/PCINT1)PA1"/>
<pin name="(ADC0/PCINT0)PA0"/>
</symbol>
<symbol name="ATTINY24/44/84">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT11/RESET/DW)PB3"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
</symbol>
<symbol name="6-I/O-4">
<pin name="(ADC2)PB4"/>
<pin name="(ADC3)PB3"/>
<pin name="(ADC0)PB5"/>
<pin name="(ADC1)PB2"/>
<pin name="(OCP)PB1"/>
<pin name="(AREF)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="18-I/O-1">
<pin name="(MOSI)PB5"/>
<pin name="(OC1B)PB4"/>
<pin name="(OC1A)PB3"/>
<pin name="(OC0A)PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="(ICP)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PA0(XTAL1)"/>
<pin name="PA1(XTAL2)"/>
<pin name="PA2(/RESET)" direction="in" function="dot"/>
<pin name="(MISO)PB6"/>
<pin name="(UCSK)PB7"/>
</symbol>
<symbol name="JTAG-ARM">
<pin name="VREF" direction="pas"/>
<pin name="VTAR" direction="pas"/>
<pin name="NTRST" direction="pas"/>
<pin name="GND@4" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="GND@6" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="GND@8" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="GND@10" direction="pas"/>
<pin name="RTCK" direction="pas"/>
<pin name="GND@12" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="GND@14" direction="pas"/>
<pin name="RST" direction="pas"/>
<pin name="GND@16" direction="pas"/>
<pin name="OBGRQ" direction="pas"/>
<pin name="GND@18" direction="pas"/>
<pin name="OBGACK" direction="pas"/>
<pin name="GND@20" direction="pas"/>
</symbol>
<symbol name="AT572D940HF">
<pin name="NC@A1" direction="pas"/>
<pin name="NC@A18" direction="pas"/>
<pin name="NC@V1" direction="pas"/>
<pin name="NC@V18" direction="pas"/>
<pin name="GND@U10" direction="pas"/>
<pin name="GND@J14" direction="pas"/>
<pin name="GND@E10" direction="pas"/>
<pin name="GND@R16" direction="pas"/>
<pin name="GND@V11" direction="pas"/>
<pin name="GND@J12" direction="pas"/>
<pin name="GND@C9" direction="pas"/>
<pin name="GND@R17" direction="pas"/>
<pin name="GND@R11" direction="pas"/>
<pin name="GND@H12" direction="pas"/>
<pin name="GND@C8" direction="pas"/>
<pin name="GND@M15" direction="pas"/>
<pin name="GND@V12" direction="pas"/>
<pin name="GND@G15" direction="pas"/>
<pin name="GND@C7" direction="pas"/>
<pin name="GND@C18" direction="pas"/>
<pin name="GND@R13" direction="pas"/>
<pin name="GND@F15" direction="pas"/>
<pin name="GND@E6" direction="pas"/>
<pin name="GND@C17" direction="pas"/>
<pin name="GND@U14" direction="pas"/>
<pin name="GND@D18" direction="pas"/>
<pin name="GND@A3" direction="pas"/>
<pin name="GND@B18" direction="pas"/>
<pin name="GND@U16" direction="pas"/>
<pin name="GND@D17" direction="pas"/>
<pin name="GND@C4" direction="pas"/>
<pin name="GND@C3" direction="pas"/>
<pin name="GND@P15" direction="pas"/>
<pin name="GND@B15" direction="pas"/>
<pin name="GND@U6" direction="pas"/>
<pin name="GND@B1" direction="pas"/>
<pin name="GND@P18" direction="pas"/>
<pin name="GND@B14" direction="pas"/>
<pin name="GND@V4" direction="pas"/>
<pin name="GND@T6" direction="pas"/>
<pin name="GND@N18" direction="pas"/>
<pin name="GND@B13" direction="pas"/>
<pin name="GND@M8" direction="pas"/>
<pin name="GND@R6" direction="pas"/>
<pin name="GND@L14" direction="pas"/>
<pin name="GND@C12" direction="pas"/>
<pin name="GND@U9" direction="pas"/>
<pin name="GND@J11" direction="pas"/>
<pin name="GND@J16" direction="pas"/>
<pin name="GND@E11" direction="pas"/>
<pin name="GND@T11" direction="pas"/>
<pin name="GNDOSC32@T5" direction="pas"/>
<pin name="GND@L17" direction="pas"/>
<pin name="GND@F8" direction="pas"/>
<pin name="GND@U1" direction="pas"/>
<pin name="GNDOSCM@P7" direction="pas"/>
<pin name="GND@K18" direction="pas"/>
<pin name="GND@F10" direction="pas"/>
<pin name="GND@A14" direction="pas"/>
<pin name="GNDPLLA@U3" direction="pas"/>
<pin name="VDDCORE@F4" direction="pas"/>
<pin name="VDDIOM@B3" direction="pas"/>
<pin name="VDDIOP@T9" direction="pas"/>
<pin name="VDDPLLA@T3" direction="pas"/>
<pin name="VDDCORE@J4" direction="pas"/>
<pin name="VDDIOM@E5" direction="pas"/>
<pin name="VDDIOP@V8" direction="pas"/>
<pin name="GND@D2" direction="pas"/>
<pin name="VDDCORE@L6" direction="pas"/>
<pin name="VDDIOM@E1" direction="pas"/>
<pin name="VDDIOP@F14" direction="pas"/>
<pin name="GND@E2" direction="pas"/>
<pin name="VDDCORE@T2" direction="pas"/>
<pin name="VDDIOM@G4" direction="pas"/>
<pin name="VDDIOP@G16" direction="pas"/>
<pin name="GND@F5" direction="pas"/>
<pin name="VDDCORE@M9" direction="pas"/>
<pin name="VDDIOM@H4" direction="pas"/>
<pin name="VDDIOP@H18" direction="pas"/>
<pin name="GND@G5" direction="pas"/>
<pin name="VDDCORE@P11" direction="pas"/>
<pin name="VDDIOM@J5" direction="pas"/>
<pin name="VDDIOP@J15" direction="pas"/>
<pin name="GND@H5" direction="pas"/>
<pin name="VDDCORE@T14" direction="pas"/>
<pin name="VDDIOM@K3" direction="pas"/>
<pin name="VDDIOP@K13" direction="pas"/>
<pin name="GND@J6" direction="pas"/>
<pin name="VDDCORE@N13" direction="pas"/>
<pin name="VDDIOM@M2" direction="pas"/>
<pin name="VDDIOP@L16" direction="pas"/>
<pin name="GND@J3" direction="pas"/>
<pin name="VDDCORE@L15" direction="pas"/>
<pin name="VDDIOM@N3" direction="pas"/>
<pin name="VDDIOP@M12" direction="pas"/>
<pin name="GND@K4" direction="pas"/>
<pin name="VDDCORE@J13" direction="pas"/>
<pin name="VDDIOM@P2" direction="pas"/>
<pin name="VDDIOP@N14" direction="pas"/>
<pin name="GND@L3" direction="pas"/>
<pin name="VDDCORE@H11" direction="pas"/>
<pin name="VDDIOMP@E9" direction="pas"/>
<pin name="VDDIOP@U17" direction="pas"/>
<pin name="GND@M1" direction="pas"/>
<pin name="VDDCORE@D16" direction="pas"/>
<pin name="VDDIOMP@G8" direction="pas"/>
<pin name="VDDIOP@P14" direction="pas"/>
<pin name="GND@N2" direction="pas"/>
<pin name="VDDCORE@E13" direction="pas"/>
<pin name="VDDIOP@C10" direction="pas"/>
<pin name="VDDIOP@P12" direction="pas"/>
<pin name="GND@N6" direction="pas"/>
<pin name="VDDCORE@H9" direction="pas"/>
<pin name="VDDIOP@D11" direction="pas"/>
<pin name="VDDIOP@U11" direction="pas"/>
<pin name="GND@R4" direction="pas"/>
<pin name="VDDCORE@E8" direction="pas"/>
<pin name="VDDIOP@G11" direction="pas"/>
<pin name="VDDIOP@R10" direction="pas"/>
<pin name="GND@T1" direction="pas"/>
<pin name="VDDCORE@A2" direction="pas"/>
<pin name="VDDIOP@A13" direction="pas"/>
<pin name="VDDIOP@V6" direction="pas"/>
<pin name="GND@T8" direction="pas"/>
<pin name="VDDIOM@D7" direction="pas"/>
<pin name="VDDIOP@A15" direction="pas"/>
<pin name="VDDOSC32@U4" direction="pas"/>
<pin name="GND@R8" direction="pas"/>
<pin name="VDDIOM@A5" direction="pas"/>
<pin name="VDDIOP@C16" direction="pas"/>
<pin name="VDDOSCM@R5" direction="pas"/>
<pin name="GND@N9" direction="pas"/>
<pin name="PIOB29" direction="pas"/>
<pin name="PIOC11" direction="pas"/>
<pin name="PIOC25" direction="pas"/>
<pin name="SD_NWE" direction="pas"/>
<pin name="PIOB30" direction="pas"/>
<pin name="PIOC12" direction="pas"/>
<pin name="PIOC26" direction="pas"/>
<pin name="TEST" direction="pas"/>
<pin name="PIOB31" direction="pas"/>
<pin name="PIOC13" direction="pas"/>
<pin name="PIOC27" direction="pas"/>
<pin name="USBD_M" direction="pas"/>
<pin name="PIOC0" direction="pas"/>
<pin name="PIOC14" direction="pas"/>
<pin name="PIOC28" direction="pas"/>
<pin name="USBD_P" direction="pas"/>
<pin name="PIOC1" direction="pas"/>
<pin name="PIOC15" direction="pas"/>
<pin name="PIOC29" direction="pas"/>
<pin name="USBHA_M" direction="pas"/>
<pin name="PIOC2" direction="pas"/>
<pin name="PIOC16" direction="pas"/>
<pin name="PIOC30" direction="pas"/>
<pin name="USBHA_P" direction="pas"/>
<pin name="PIOC3" direction="pas"/>
<pin name="PIOC17" direction="pas"/>
<pin name="PIOC31" direction="pas"/>
<pin name="USBHB_M" direction="pas"/>
<pin name="PIOC4" direction="pas"/>
<pin name="PIOC18" direction="pas"/>
<pin name="PLL_RCA" direction="pas"/>
<pin name="USBHB_P" direction="pas"/>
<pin name="PIOC5" direction="pas"/>
<pin name="PIOC19" direction="pas"/>
<pin name="PLL_RCB" direction="pas"/>
<pin name="XIN" direction="pas"/>
<pin name="PIOC6" direction="pas"/>
<pin name="PIOC20" direction="pas"/>
<pin name="SD_A10" direction="pas"/>
<pin name="XOUT" direction="pas"/>
<pin name="PIOC7" direction="pas"/>
<pin name="PIOC21" direction="pas"/>
<pin name="SD_CK" direction="pas"/>
<pin name="X32EN" direction="pas"/>
<pin name="PIOC8" direction="pas"/>
<pin name="PIOC22" direction="pas"/>
<pin name="SD_CKE" direction="pas"/>
<pin name="X32IN" direction="pas"/>
<pin name="PIOC9" direction="pas"/>
<pin name="PIOC23" direction="pas"/>
<pin name="SD_NCAS" direction="pas"/>
<pin name="X32OUT" direction="pas"/>
<pin name="PIOC10" direction="pas"/>
<pin name="PIOC24" direction="pas"/>
<pin name="SD_NRAS" direction="pas"/>
<pin name="A0/NBS0" direction="pas"/>
<pin name="D5" direction="pas"/>
<pin name="NCS2" direction="pas"/>
<pin name="PIOA27" direction="pas"/>
<pin name="A1/NBS2/NWR2" direction="pas"/>
<pin name="D6" direction="pas"/>
<pin name="NCS3/SM_NCS" direction="pas"/>
<pin name="PIOA28" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="D7" direction="pas"/>
<pin name="NRD/NOE/CF_NOE" direction="pas"/>
<pin name="PIOA29" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="D8" direction="pas"/>
<pin name="NRST" direction="pas"/>
<pin name="PIOA30" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="D9" direction="pas"/>
<pin name="NWR0/NWE/CF_NWE" direction="pas"/>
<pin name="PIOA31" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="D10" direction="pas"/>
<pin name="NWR1/NBS1/CF_NIOR" direction="pas"/>
<pin name="PIOB0" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="D11" direction="pas"/>
<pin name="NWR3/NBS3/CF_NIOW" direction="pas"/>
<pin name="PIOB1" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="D12" direction="pas"/>
<pin name="PIOA0" direction="pas"/>
<pin name="PIOB2" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="D13" direction="pas"/>
<pin name="PIOA1" direction="pas"/>
<pin name="PIOB3" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="D14" direction="pas"/>
<pin name="PIOA2" direction="pas"/>
<pin name="PIOB4" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="D15" direction="pas"/>
<pin name="PIOA3" direction="pas"/>
<pin name="PIOB5" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="D16" direction="pas"/>
<pin name="PIOA4" direction="pas"/>
<pin name="PIOB6" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="D17" direction="pas"/>
<pin name="PIOA5" direction="pas"/>
<pin name="PIOB7" direction="pas"/>
<pin name="A13" direction="pas"/>
<pin name="D18" direction="pas"/>
<pin name="PIOA6" direction="pas"/>
<pin name="PIOB8" direction="pas"/>
<pin name="A14" direction="pas"/>
<pin name="D19" direction="pas"/>
<pin name="PIOA7" direction="pas"/>
<pin name="PIOB9" direction="pas"/>
<pin name="A15" direction="pas"/>
<pin name="D20" direction="pas"/>
<pin name="PIOA8" direction="pas"/>
<pin name="PIOB10" direction="pas"/>
<pin name="A16/SD_BA0" direction="pas"/>
<pin name="D21" direction="pas"/>
<pin name="PIOA9" direction="pas"/>
<pin name="PIOB11" direction="pas"/>
<pin name="A17/SD_BA1" direction="pas"/>
<pin name="D22" direction="pas"/>
<pin name="PIOA10" direction="pas"/>
<pin name="PIOB12" direction="pas"/>
<pin name="A18" direction="pas"/>
<pin name="D23" direction="pas"/>
<pin name="PIOA11" direction="pas"/>
<pin name="PIOB13" direction="pas"/>
<pin name="A19" direction="pas"/>
<pin name="D24" direction="pas"/>
<pin name="PIOA12" direction="pas"/>
<pin name="PIOB14" direction="pas"/>
<pin name="A20" direction="pas"/>
<pin name="D25" direction="pas"/>
<pin name="PIOA13" direction="pas"/>
<pin name="PIOB15" direction="pas"/>
<pin name="A21" direction="pas"/>
<pin name="D26" direction="pas"/>
<pin name="PIOA14" direction="pas"/>
<pin name="PIOB16" direction="pas"/>
<pin name="A_JCFG" direction="pas"/>
<pin name="D27" direction="pas"/>
<pin name="PIOA15" direction="pas"/>
<pin name="PIOB17" direction="pas"/>
<pin name="A_RTCK" direction="pas"/>
<pin name="D28" direction="pas"/>
<pin name="PIOA16" direction="pas"/>
<pin name="PIOB18" direction="pas"/>
<pin name="A_TCK" direction="pas"/>
<pin name="D29" direction="pas"/>
<pin name="PIOA17" direction="pas"/>
<pin name="PIOB19" direction="pas"/>
<pin name="A_TDI" direction="pas"/>
<pin name="D30" direction="pas"/>
<pin name="PIOA18" direction="pas"/>
<pin name="PIOB20" direction="pas"/>
<pin name="A_TDO" direction="pas"/>
<pin name="D31" direction="pas"/>
<pin name="PIOA19" direction="pas"/>
<pin name="PIOB21" direction="pas"/>
<pin name="A_TMS" direction="pas"/>
<pin name="M_NTRST" direction="pas"/>
<pin name="PIOA20" direction="pas"/>
<pin name="PIOB22" direction="pas"/>
<pin name="A_NTRST" direction="pas"/>
<pin name="M_TCK" direction="pas"/>
<pin name="PIOA21" direction="pas"/>
<pin name="PIOB23" direction="pas"/>
<pin name="D0" direction="pas"/>
<pin name="M_TDI" direction="pas"/>
<pin name="PIOA22" direction="pas"/>
<pin name="PIOB24" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="M_TDO" direction="pas"/>
<pin name="PIOA23" direction="pas"/>
<pin name="PIOB25" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="M_TMS" direction="pas"/>
<pin name="PIOA24" direction="pas"/>
<pin name="PIOB26" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="NCS0" direction="pas"/>
<pin name="PIOA25" direction="pas"/>
<pin name="PIOB27" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="NCS1/SD_CS" direction="pas"/>
<pin name="PIOA26" direction="pas"/>
<pin name="PIOB28" direction="pas"/>
</symbol>
<symbol name="AT91SAM9260B-QU">
<pin name="PA0/SPI0_MISO/MCDB0"/>
<pin name="PA1/SPI0_MOSI/MCCDB"/>
<pin name="PA2/SPI0_SPCK"/>
<pin name="PA3/SPI0_NPCS0/MCDB3"/>
<pin name="PA4/RTS2/MCDB2"/>
<pin name="PA5/CTS2/MCDB1"/>
<pin name="PA6/MCDA0"/>
<pin name="PA7/MCCDA"/>
<pin name="PA8/MCCK"/>
<pin name="PA9/MCDA1"/>
<pin name="PA10/MCDA2/ETX2"/>
<pin name="PA11/MCDA3/ETX3"/>
<pin name="PA12/ETX0"/>
<pin name="PA13/ETX1"/>
<pin name="PA14/ERX0"/>
<pin name="PA15/ERX1"/>
<pin name="PA16/ETXEN"/>
<pin name="PA17/ERXDV"/>
<pin name="PA18/ERXER"/>
<pin name="PA19/ETXCK"/>
<pin name="PA20/EMDC"/>
<pin name="PA21/EMDIO"/>
<pin name="PA22/ADTRG/ETXER"/>
<pin name="PA23/TWD/ETX2"/>
<pin name="PA24/TWCK/ETX3"/>
<pin name="PA25/TLCK0/ERX2"/>
<pin name="PA26/TIOA0/ERX3"/>
<pin name="PA27/TIOA1/ERXCK"/>
<pin name="PA28/TIOA2/ECRS"/>
<pin name="PA29/SCK1/ECOL"/>
<pin name="HDPA"/>
<pin name="HDMA"/>
<pin name="DDP"/>
<pin name="DDM"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="RTCK" direction="out"/>
<pin name="JTAGSEL"/>
<pin name="NTRST"/>
<pin name="XOUT" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT32" direction="out"/>
<pin name="XIN32" direction="in"/>
<pin name="OSCSEL" direction="in"/>
<pin name="PLLRCA" direction="in"/>
<pin name="WKUP" direction="in"/>
<pin name="SHDN" direction="out"/>
<pin name="VDDBU" direction="pwr"/>
<pin name="GNDBU" direction="pwr"/>
<pin name="VDDCORE@38" direction="pwr"/>
<pin name="VDDCORE@77" direction="pwr"/>
<pin name="VDDCORE@147" direction="pwr"/>
<pin name="VDDCORE@174" direction="pwr"/>
<pin name="VDDC0RE@203" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@39" direction="pwr"/>
<pin name="GND@53" direction="pwr"/>
<pin name="GND@66" direction="pwr"/>
<pin name="GND@78" direction="pwr"/>
<pin name="GND@91" direction="pwr"/>
<pin name="GND@113" direction="pwr"/>
<pin name="GND@133" direction="pwr"/>
<pin name="GND@146" direction="pwr"/>
<pin name="GND@170" direction="pwr"/>
<pin name="GND@173" direction="pwr"/>
<pin name="GND@188" direction="pwr"/>
<pin name="GND@200" direction="pwr"/>
<pin name="GND@204" direction="pwr"/>
<pin name="VDDIOM@65" direction="pwr"/>
<pin name="VDDIOM@90" direction="pwr"/>
<pin name="VDDIOM@114" direction="pwr"/>
<pin name="VDDIOM@132" direction="pwr"/>
<pin name="VDDIOP0@5" direction="pwr"/>
<pin name="VDDIOP0@13" direction="pwr"/>
<pin name="VDDIOP0@24" direction="pwr"/>
<pin name="VDDIOP0@32" direction="pwr"/>
<pin name="VDDIOP0@52" direction="pwr"/>
<pin name="VDDIOP0@187" direction="pwr"/>
<pin name="VDDIOP0@199" direction="pwr"/>
<pin name="VDDIOP1" direction="pwr"/>
<pin name="VDDPLL@155" direction="pwr"/>
<pin name="VDDPLL@148" direction="pwr"/>
<pin name="GNDPLL@153" direction="pwr"/>
<pin name="GNDPLL@151" direction="pwr"/>
<pin name="VDDANA" direction="pwr"/>
<pin name="GNDANA" direction="pwr"/>
<pin name="ADVREF"/>
<pin name="NC@152" direction="nc"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="NBS0/A0"/>
<pin name="NWR2/NBS2/A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="BA0/A16"/>
<pin name="BA1/A17"/>
<pin name="A18"/>
<pin name="A19"/>
<pin name="A20"/>
<pin name="A21"/>
<pin name="A22"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!SDWE" direction="out"/>
<pin name="SDA10" direction="out"/>
<pin name="SDCKE" direction="out"/>
<pin name="SDCK" direction="out"/>
<pin name="SDCS/NCS1" direction="out"/>
<pin name="NCSO" direction="out"/>
<pin name="CFOE/NRD" direction="out"/>
<pin name="CFWE/NWE/NWR0" direction="out"/>
<pin name="CFIOR/NBS1/NWR1" direction="out"/>
<pin name="CFIOW/NBS3/NWR3" direction="out"/>
<pin name="NANDOE" direction="out"/>
<pin name="NANDWE" direction="out"/>
<pin name="NRST"/>
<pin name="BMS" direction="in"/>
<pin name="TST" direction="in"/>
<pin name="TIOA3/SPI1_MISO/PB0"/>
<pin name="TIOB3/SPI1_MOSI/PB1"/>
<pin name="TIOA4/SPI1_SPCK/PB2"/>
<pin name="TIOA5/SPI1_NPCS0/PB3"/>
<pin name="TXD0/PB4"/>
<pin name="RXD0/PB5"/>
<pin name="TCLK1/TXD1/PB6"/>
<pin name="TCLK2/RXD1/PB7"/>
<pin name="TXD2/PB8"/>
<pin name="RXD2/PB9"/>
<pin name="ISI_D8/TXD3/PB10"/>
<pin name="ISI_D9/RXD3/PB11"/>
<pin name="DRXD/PB14"/>
<pin name="DTXD/PB15"/>
<pin name="TCLK3/TK0/PB16"/>
<pin name="TCLK4/TF0/PB17"/>
<pin name="TIOB4/TD0/PB18"/>
<pin name="TIOB5/RD0/PB19"/>
<pin name="ISI_D0/RK0/PB20"/>
<pin name="ISI_D1/RF0/PB21"/>
<pin name="ISI_D2/DSR0/PB22"/>
<pin name="ISI_D3/DCD0/PB23"/>
<pin name="ISI_D4/DTR0/PB24"/>
<pin name="ISI_D5/RI0/PB25"/>
<pin name="ISI_D6/RTS0/PB26"/>
<pin name="ISI_D7/CTS0/PB27"/>
<pin name="ISI_PCK/RTS1/PB28"/>
<pin name="ISI_VSYNC/CTS1/PB29"/>
<pin name="ISI_HSYNC/PCK0/PB30"/>
<pin name="ISI_MCK/PCK1/PB31"/>
<pin name="SCK3/AD0/PC0"/>
<pin name="PCK0/AD1/PC1"/>
<pin name="SPI1_NPCS2/A23/PC4"/>
<pin name="SPI1_NPCS1/A24/PC5"/>
<pin name="CFCE1/TIOB2/PC6"/>
<pin name="CFCE2/TIOB1/PC7"/>
<pin name="RTS3/NCS4_CFCS0/PC8"/>
<pin name="TIOB0/NCS5_CFCS1/PC9"/>
<pin name="CTS3/A25_CFRNW/PC10"/>
<pin name="SPI0_NPCS1/NCS2/PC11"/>
<pin name="NCS6/FIQ/PC13"/>
<pin name="IRQ2/NCS3_NANDCS/PC14"/>
<pin name="IRQ1/NWAIT/PC15"/>
<pin name="SPI0_NPCS2/D16/PC16"/>
<pin name="SPI0_NPCS3/D17/PC17"/>
<pin name="SPI1_NPCS1/D18/PC18"/>
<pin name="SPI1_NPCS2/D19/PC19"/>
<pin name="SPI1_NPCS3/D20/PC20"/>
<pin name="EF100/D21/PC21"/>
<pin name="TCLK5/D22/PC22"/>
<pin name="D23/PC23"/>
<pin name="D24/PC24"/>
<pin name="D25/PC25"/>
<pin name="D26/PC26"/>
<pin name="D27/PC27"/>
<pin name="D28/PC28"/>
<pin name="D29/PC29"/>
<pin name="D30/PC30"/>
<pin name="D31/PC31"/>
</symbol>
<symbol name="AT91SAM9260B-CU">
<pin name="PA0/SPI0_MISO/MCDB0"/>
<pin name="PA1/SPI0_MOSI/MCCDB"/>
<pin name="PA2/SPI0_SPCK"/>
<pin name="PA3/SPI0_NPCS0/MCDB3"/>
<pin name="PA4/RTS2/MCDB2"/>
<pin name="PA5/CTS2/MCDB1"/>
<pin name="PA6/MCDA0"/>
<pin name="PA7/MCCDA"/>
<pin name="PA8/MCCK"/>
<pin name="PA9/MCDA1"/>
<pin name="PA10/MCDA2/ETX2"/>
<pin name="PA11/MCDA3/ETX3"/>
<pin name="PA12/ETX0"/>
<pin name="PA13/ETX1"/>
<pin name="PA14/ERX0"/>
<pin name="PA15/ERX1"/>
<pin name="PA16/ETXEN"/>
<pin name="PA17/ERXDV"/>
<pin name="PA18/ERXER"/>
<pin name="PA19/ETXCK"/>
<pin name="PA20/EMDC"/>
<pin name="PA21/EMDIO"/>
<pin name="PA22/ADTRG/ETXER"/>
<pin name="PA23/TWD/ETX2"/>
<pin name="PA24/TWCK/ETX3"/>
<pin name="PA25/TLCK0/ERX2"/>
<pin name="PA26/TIOA0/ERX3"/>
<pin name="PA27/TIOA1/ERXCK"/>
<pin name="PA28/TIOA2/ECRS"/>
<pin name="PA29/SCK1/ECOL"/>
<pin name="HDPA"/>
<pin name="HDMA"/>
<pin name="DDP"/>
<pin name="DDM"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="RTCK" direction="out"/>
<pin name="JTAGSEL"/>
<pin name="NTRST"/>
<pin name="XOUT" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT32" direction="out"/>
<pin name="XIN32" direction="in"/>
<pin name="OSCSEL" direction="in"/>
<pin name="PLLRCA" direction="in"/>
<pin name="WKUP" direction="in"/>
<pin name="SHDN" direction="out"/>
<pin name="VDDBU" direction="pwr"/>
<pin name="GNDBU" direction="pwr"/>
<pin name="VDDCORE@H14" direction="pwr"/>
<pin name="VDDCORE@M1" direction="pwr"/>
<pin name="VDDCORE@D9" direction="pwr"/>
<pin name="VDDCORE@T13" direction="pwr"/>
<pin name="GND@D8" direction="pwr"/>
<pin name="GND@D6" direction="pwr"/>
<pin name="GND@D10" direction="pwr"/>
<pin name="GND@D12" direction="pwr"/>
<pin name="GND@F4" direction="pwr"/>
<pin name="GND@G14" direction="pwr"/>
<pin name="GND@H8" direction="pwr"/>
<pin name="GND@H9" direction="pwr"/>
<pin name="GND@H10" direction="pwr"/>
<pin name="GND@K8" direction="pwr"/>
<pin name="GND@K9" direction="pwr"/>
<pin name="GND@K10" direction="pwr"/>
<pin name="GND@K16" direction="pwr"/>
<pin name="GND@L1" direction="pwr"/>
<pin name="GND@M3" direction="pwr"/>
<pin name="GND@R7" direction="pwr"/>
<pin name="GND@T7" direction="pwr"/>
<pin name="GND@T15" direction="pwr"/>
<pin name="VDDIOM@D11" direction="pwr"/>
<pin name="VDDIOM@G4" direction="pwr"/>
<pin name="HDPB"/>
<pin name="PA31/SCK0/TXD4"/>
<pin name="VDDIOP0@L4" direction="pwr"/>
<pin name="VDDIOP0@C16" direction="pwr"/>
<pin name="VDDIOP0@U17" direction="pwr"/>
<pin name="VDDIOP0@J3" direction="pwr"/>
<pin name="PA30/SCK2/RXD4"/>
<pin name="ISI_D11/RXD5/PB13"/>
<pin name="ISI_D10/TXD5/PB12"/>
<pin name="VDDIOP1@P8" direction="pwr"/>
<pin name="VDDPLL@P2" direction="pwr"/>
<pin name="VDDPLL@N2" direction="pwr"/>
<pin name="GNDPLL@U1" direction="pwr"/>
<pin name="GNDPLL@T2" direction="pwr"/>
<pin name="VDDANA" direction="pwr"/>
<pin name="GNDANA" direction="pwr"/>
<pin name="ADVREF"/>
<pin name="NC@D15" direction="nc"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="NBS0/A0"/>
<pin name="NWR2/NBS2/A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="BA0/A16"/>
<pin name="BA1/A17"/>
<pin name="A18"/>
<pin name="A19"/>
<pin name="A20"/>
<pin name="A21"/>
<pin name="A22"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!SDWE" direction="out"/>
<pin name="SDA10" direction="out"/>
<pin name="SDCKE" direction="out"/>
<pin name="SDCK" direction="out"/>
<pin name="SDCS/NCS1" direction="out"/>
<pin name="NCSO" direction="out"/>
<pin name="CFOE/NRD" direction="out"/>
<pin name="CFWE/NWE/NWR0" direction="out"/>
<pin name="CFIOR/NBS1/NWR1" direction="out"/>
<pin name="CFIOW/NBS3/NWR3" direction="out"/>
<pin name="NANDOE" direction="out"/>
<pin name="NANDWE" direction="out"/>
<pin name="NRST"/>
<pin name="BMS" direction="in"/>
<pin name="TST" direction="in"/>
<pin name="TIOA3/SPI1_MISO/PB0"/>
<pin name="TIOB3/SPI1_MOSI/PB1"/>
<pin name="TIOA4/SPI1_SPCK/PB2"/>
<pin name="TIOA5/SPI1_NPCS0/PB3"/>
<pin name="TXD0/PB4"/>
<pin name="RXD0/PB5"/>
<pin name="TCLK1/TXD1/PB6"/>
<pin name="TCLK2/RXD1/PB7"/>
<pin name="TXD2/PB8"/>
<pin name="RXD2/PB9"/>
<pin name="ISI_D8/TXD3/PB10"/>
<pin name="ISI_D9/RXD3/PB11"/>
<pin name="DRXD/PB14"/>
<pin name="DTXD/PB15"/>
<pin name="TCLK3/TK0/PB16"/>
<pin name="TCLK4/TF0/PB17"/>
<pin name="TIOB4/TD0/PB18"/>
<pin name="TIOB5/RD0/PB19"/>
<pin name="ISI_D0/RK0/PB20"/>
<pin name="ISI_D1/RF0/PB21"/>
<pin name="ISI_D2/DSR0/PB22"/>
<pin name="ISI_D3/DCD0/PB23"/>
<pin name="ISI_D4/DTR0/PB24"/>
<pin name="ISI_D5/RI0/PB25"/>
<pin name="ISI_D6/RTS0/PB26"/>
<pin name="ISI_D7/CTS0/PB27"/>
<pin name="ISI_PCK/RTS1/PB28"/>
<pin name="ISI_VSYNC/CTS1/PB29"/>
<pin name="ISI_HSYNC/PCK0/PB30"/>
<pin name="ISI_MCK/PCK1/PB31"/>
<pin name="SCK3/AD0/PC0"/>
<pin name="PCK0/AD1/PC1"/>
<pin name="SPI1_NPCS2/A23/PC4"/>
<pin name="SPI1_NPCS1/A24/PC5"/>
<pin name="CFCE1/TIOB2/PC6"/>
<pin name="CFCE2/TIOB1/PC7"/>
<pin name="RTS3/NCS4_CFCS0/PC8"/>
<pin name="TIOB0/NCS5_CFCS1/PC9"/>
<pin name="CTS3/A25_CFRNW/PC10"/>
<pin name="SPI0_NPCS1/NCS2/PC11"/>
<pin name="NCS6/FIQ/PC13"/>
<pin name="IRQ2/NCS3_NANDCS/PC14"/>
<pin name="IRQ1/NWAIT/PC15"/>
<pin name="SPI0_NPCS2/D16/PC16"/>
<pin name="SPI0_NPCS3/D17/PC17"/>
<pin name="SPI1_NPCS1/D18/PC18"/>
<pin name="SPI1_NPCS2/D19/PC19"/>
<pin name="SPI1_NPCS3/D20/PC20"/>
<pin name="EF100/D21/PC21"/>
<pin name="TCLK5/D22/PC22"/>
<pin name="D23/PC23"/>
<pin name="D24/PC24"/>
<pin name="D25/PC25"/>
<pin name="D26/PC26"/>
<pin name="D27/PC27"/>
<pin name="D28/PC28"/>
<pin name="D29/PC29"/>
<pin name="D30/PC30"/>
<pin name="D31/PC31"/>
<pin name="NC@C15"/>
<pin name="GND@J8"/>
<pin name="GND@J9"/>
<pin name="GND@J10"/>
<pin name="NC@R1"/>
<pin name="NCS7/IRQ0/PC12"/>
<pin name="PCK1/AD2/PC2"/>
<pin name="SPI1_NPCS3/AD3/PC3"/>
<pin name="HDMB"/>
</symbol>
<symbol name="AT91SAM7S512/256/128/64/321">
<pin name="ADVREF"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="VDDIN" direction="pwr"/>
<pin name="VDDOUT"/>
<pin name="AD0/PCK1/TD/PA17"/>
<pin name="AD1/PCK2/RD/PA18"/>
<pin name="PCK1/RXD1/PA21"/>
<pin name="VDDCORE@12"/>
<pin name="AD2/FIQ/RK/PA19"/>
<pin name="NPCS3/TXD1/PA22"/>
<pin name="PWM0/SCK1/PA23"/>
<pin name="AD3/IRQ0/RF/PA20"/>
<pin name="GND@17" direction="pwr"/>
<pin name="VDDIO@18" direction="pwr"/>
<pin name="TK/TIOB1/PA16"/>
<pin name="TIOA1/TF/PA15"/>
<pin name="PWM3/SPCK/PA14"/>
<pin name="PWM2/MOSI/PA13"/>
<pin name="PWM1/RTS1/PA24"/>
<pin name="VDDCORE@24"/>
<pin name="PWM2/CTS1/PA25"/>
<pin name="TIOA2/DCD1/PA26"/>
<pin name="PWM1/MISO/PA12"/>
<pin name="PWM0/NPCS0/PA11"/>
<pin name="NPCS2/DTXD/PA10"/>
<pin name="NPCS1/DRXD/PA9"/>
<pin name="ADTRG/CTS0/PA8"/>
<pin name="PWM3/RTS0/PA7"/>
<pin name="TDI"/>
<pin name="PCK0/TXD0/PA6"/>
<pin name="NPCS3/RXD0/PA5"/>
<pin name="TCLK0/TWCK/PA4"/>
<pin name="TIOB2/DTR1/PA27"/>
<pin name="TCLK1/DSR1/PA28"/>
<pin name="NRST"/>
<pin name="TST"/>
<pin name="TCLK2/RI1/PA29"/>
<pin name="NPCS2/IRQ1/PA30"/>
<pin name="NPCS3/TWD/PA3"/>
<pin name="SCK0/PWM2/PA2"/>
<pin name="VDDIO@45" direction="pwr"/>
<pin name="GND@46" direction="pwr"/>
<pin name="TIOB0/PWM1/PA1"/>
<pin name="TIOA0/PWM0/PA0"/>
<pin name="TDO"/>
<pin name="JTAGSEL"/>
<pin name="TMS"/>
<pin name="PCK2/NPCS1/PA31"/>
<pin name="TCK"/>
<pin name="VDDCORE@54"/>
<pin name="ERASE"/>
<pin name="DDM"/>
<pin name="DDP"/>
<pin name="VDDIO@58" direction="pwr"/>
<pin name="VDDFLASH" direction="pwr"/>
<pin name="GND@60" direction="pwr"/>
<pin name="XOUT"/>
<pin name="XIN/PGMCK"/>
<pin name="PLLRC"/>
<pin name="VDDPLL"/>
</symbol>
<symbol name="ATMEGA8535PLC44">
<description>ATMEGA 8535</description>
<pin name="PB0(XCK/T0)"/>
<pin name="PB1(T1)"/>
<pin name="PB2(AIN0/INT2)"/>
<pin name="PB3(AIN1/OC0)"/>
<pin name="PB4(SS)"/>
<pin name="PB5(MOSI)"/>
<pin name="PB6(MISO)"/>
<pin name="PB7(SCK)"/>
<pin name="PD0(RXD)"/>
<pin name="PD1(TXD)"/>
<pin name="PD2(INT0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD4(OC1B)"/>
<pin name="PD6(OC1A)"/>
<pin name="PD6(ICP1)"/>
<pin name="PD7(OC2)"/>
<pin name="PC0(SCL)"/>
<pin name="PC1(SDA)"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6(TOSC1)"/>
<pin name="PC7(TOSC2)"/>
<pin name="RESET" function="dot"/>
<pin name="PA0(ADC0)"/>
<pin name="PA1(ADC1)"/>
<pin name="PA2(ADC2)"/>
<pin name="PA3(ADC3)"/>
<pin name="PA4(ADC4)"/>
<pin name="PA5(ADC5)"/>
<pin name="PA6(ADC6)"/>
<pin name="PA7(ADC7)"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="AVCC"/>
<pin name="AREF"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="VCC3"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
</symbol>
<symbol name="AT93C46B">
<pin name="CS" direction="in"/>
<pin name="SK" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="DO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="U642B">
<pin name="INT"/>
<pin name="CT"/>
<pin name="RT"/>
<pin name="PARK"/>
<pin name="WASH"/>
<pin name="GND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="U643B">
<pin name="DGND" direction="pwr"/>
<pin name="+V" direction="pwr"/>
<pin name="OUT/REL" direction="out"/>
<pin name="COSC"/>
<pin name="ROSC"/>
<pin name="NC" direction="nc"/>
<pin name="LFD" direction="out"/>
<pin name="STR" direction="in"/>
</symbol>
<symbol name="ATMEGA32-PU">
<pin name="33/(ADC7)PA7"/>
<pin name="34/(ADC6)PA6"/>
<pin name="35/(ADC5)PA5"/>
<pin name="36/(ADC4)PA4"/>
<pin name="37/(ADC3)PA3"/>
<pin name="38/(ADC2)PA2"/>
<pin name="39/(ADC1)PA1"/>
<pin name="40/(ADC0)PA0"/>
<pin name="8/(SCK)PB7"/>
<pin name="7/(MISO)PB6"/>
<pin name="6/(MOSI)PB5"/>
<pin name="5/(SS)PB4"/>
<pin name="4/(AIN1/OC0)PB3"/>
<pin name="3/(AIN0/INT2)PB2"/>
<pin name="2/(T1)PB1"/>
<pin name="1/(T0/XCK)PB0"/>
<pin name="29/(TOSC2)PC7"/>
<pin name="28/(TOSC1)PC6"/>
<pin name="27/(TDI)PC5"/>
<pin name="26/(TDO)PC4"/>
<pin name="25/(TMS)PC3"/>
<pin name="24/(TCK)PC2"/>
<pin name="23/(SDA)PC1"/>
<pin name="22/(SCL)PC0"/>
<pin name="31/GND" direction="pwr"/>
<pin name="30/AVCC" direction="pwr"/>
<pin name="32/AREF" direction="pas"/>
<pin name="13/XTAL1"/>
<pin name="12/XTAL2"/>
<pin name="10/VCC" direction="pwr"/>
<pin name="11/GND" direction="pwr"/>
<pin name="9/RESET" direction="in" function="dot"/>
<pin name="14/(RXD)PD0"/>
<pin name="15/(TXD)PD1"/>
<pin name="16/(INT0)PD2"/>
<pin name="17/(INT1)PD3"/>
<pin name="18/(OC1B)PD4"/>
<pin name="19/(OC1A)PD5"/>
<pin name="20/(ICP)PD6"/>
<pin name="21/(OC2)PD7"/>
</symbol>
<symbol name="ATTINY13-20MMU">
<pin name="PB5"/>
<pin name="PB3"/>
<pin name="3/DNC" direction="nc"/>
<pin name="PB4"/>
<pin name="GND" direction="pwr"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="8/DNC" direction="nc"/>
<pin name="PB2"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ATXMEGA32E5/16E5/8E5">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PD5"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD4"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND18" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="PDI/RESET"/>
<pin name="PD7"/>
<pin name="PD6"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AT90*4434P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC0" pad="22"/>
<connect gate="G$1" pin="PC1" pad="23"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*4434" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (LS)&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-4"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="44"/>
<connect gate="G$1" pin="VCC2" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0" pad="19"/>
<connect gate="G$1" pin="PC1" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*8535P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC0" pad="22"/>
<connect gate="G$1" pin="PC1" pad="23"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*8535" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-4"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0" pad="19"/>
<connect gate="G$1" pin="PC1" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S4414" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="ICP" pad="31"/>
<connect gate="G$1" pin="OC1B" pad="29"/>
<connect gate="G$1" pin="PD4" pad="14"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J1" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J2" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J3" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515-A" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-2"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-2"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-1"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="ICP" pad="31"/>
<connect gate="G$1" pin="OC1B" pad="29"/>
<connect gate="G$1" pin="PD4" pad="14"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2333A" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10-bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-1"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="10"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(ICP)PB0" pad="12"/>
<connect gate="G$1" pin="(INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(INT1)PD3" pad="1"/>
<connect gate="G$1" pin="(MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1)PB1" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(SS)PB2" pad="14"/>
<connect gate="G$1" pin="(T0)PD4" pad="2"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="31"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="NC3" pad="19"/>
<connect gate="G$1" pin="NC4" pad="22"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2333P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10-bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-2"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="12"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(ICP)PB0" pad="14"/>
<connect gate="G$1" pin="(INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(INT1)PD3" pad="5"/>
<connect gate="G$1" pin="(MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="17"/>
<connect gate="G$1" pin="(OC1)PB1" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(SS)PB2" pad="16"/>
<connect gate="G$1" pin="(T0)PD4" pad="6"/>
<connect gate="G$1" pin="(T1)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S4433" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="12"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(ICP)PB0" pad="14"/>
<connect gate="G$1" pin="(INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(INT1)PD3" pad="5"/>
<connect gate="G$1" pin="(MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="17"/>
<connect gate="G$1" pin="(OC1)PB1" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(SS)PB2" pad="16"/>
<connect gate="G$1" pin="(T0)PD4" pad="6"/>
<connect gate="G$1" pin="(T1)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="10"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(ICP)PB0" pad="12"/>
<connect gate="G$1" pin="(INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(INT1)PD3" pad="1"/>
<connect gate="G$1" pin="(MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1)PB1" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(SS)PB2" pad="14"/>
<connect gate="G$1" pin="(T0)PD4" pad="2"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="31"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*2323" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="3-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*2343" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="5-I/O-1"/>
</gates>
<devices>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2313" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="15-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(OCI)PB3" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(OCI)PB3" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S1200" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="15-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="Y" package="SSOP20D8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY10" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes ROM</description>
<gates>
<gate name="G$1" symbol="6-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY11*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="6-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="3617970"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="3617970"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY12*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="6-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY22" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1K ROM&lt;p&gt;
128 bytes RAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="5-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA103*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (L)&lt;br&gt;
128 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
2 Kbytes EEPROM&lt;br&gt;
UART&lt;br&gt;
RTC&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="48-I/O-1"/>
</gates>
<devices>
<device name="" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AC+)PE2" pad="4"/>
<connect gate="G$1" pin="(AC-)PE3" pad="5"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(TXD)PE1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="ALE" pad="43"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="54"/>
<connect gate="G$1" pin="RD" pad="34"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="TOSC1" pad="19"/>
<connect gate="G$1" pin="TOSC2" pad="18"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="WR" pad="33"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90C8534" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
256 bytes SRAM&lt;p&gt;
6-channel&lt;p&gt;
10-bit A/D</description>
<gates>
<gate name="G$1" symbol="15-I/O-3"/>
</gates>
<devices>
<device name="A" package="TQFP48">
<connects>
<connect gate="G$1" pin="ADIN0" pad="1"/>
<connect gate="G$1" pin="ADIN1" pad="13"/>
<connect gate="G$1" pin="ADIN2" pad="14"/>
<connect gate="G$1" pin="ADIN3" pad="15"/>
<connect gate="G$1" pin="ADIN4" pad="16"/>
<connect gate="G$1" pin="ADIN5" pad="17"/>
<connect gate="G$1" pin="AGND" pad="11"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="31"/>
<connect gate="G$1" pin="INT0" pad="35"/>
<connect gate="G$1" pin="INT1" pad="34"/>
<connect gate="G$1" pin="NC1" pad="2"/>
<connect gate="G$1" pin="NC10" pad="12"/>
<connect gate="G$1" pin="NC11" pad="19"/>
<connect gate="G$1" pin="NC12" pad="21"/>
<connect gate="G$1" pin="NC13" pad="25"/>
<connect gate="G$1" pin="NC14" pad="26"/>
<connect gate="G$1" pin="NC15" pad="27"/>
<connect gate="G$1" pin="NC16" pad="28"/>
<connect gate="G$1" pin="NC17" pad="29"/>
<connect gate="G$1" pin="NC18" pad="30"/>
<connect gate="G$1" pin="NC19" pad="32"/>
<connect gate="G$1" pin="NC2" pad="3"/>
<connect gate="G$1" pin="NC20" pad="36"/>
<connect gate="G$1" pin="NC21" pad="37"/>
<connect gate="G$1" pin="NC22" pad="40"/>
<connect gate="G$1" pin="NC23" pad="41"/>
<connect gate="G$1" pin="NC24" pad="42"/>
<connect gate="G$1" pin="NC25" pad="43"/>
<connect gate="G$1" pin="NC26" pad="48"/>
<connect gate="G$1" pin="NC3" pad="4"/>
<connect gate="G$1" pin="NC4" pad="5"/>
<connect gate="G$1" pin="NC5" pad="6"/>
<connect gate="G$1" pin="NC6" pad="7"/>
<connect gate="G$1" pin="NC7" pad="8"/>
<connect gate="G$1" pin="NC8" pad="9"/>
<connect gate="G$1" pin="NC9" pad="10"/>
<connect gate="G$1" pin="PA0" pad="47"/>
<connect gate="G$1" pin="PA1" pad="46"/>
<connect gate="G$1" pin="PA2" pad="45"/>
<connect gate="G$1" pin="PA3" pad="44"/>
<connect gate="G$1" pin="PA4" pad="39"/>
<connect gate="G$1" pin="PA5" pad="38"/>
<connect gate="G$1" pin="PA6" pad="33"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA161*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
dual UART&lt;br&gt;
hardware multiplier&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="35-I/O-1"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(ALE)PE1" pad="30"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(INT2)PE0" pad="31"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="29"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="10"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="3"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="14"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="15"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="11"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="4"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16PU"/>
<attribute name="OC_FARNELL" value="9171142"/>
<attribute name="OC_NEWARK" value="98M0167"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16PU"/>
<attribute name="OC_FARNELL" value="9171142"/>
<attribute name="OC_NEWARK" value="98M0167"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA161*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
dual UART&lt;br&gt;
hardware multiplier&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="35-I/O-2"/>
</gates>
<devices>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(ALE)PE1" pad="27"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(INT2)PE0" pad="29"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="26"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="5"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="42"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="10"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="7"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="43"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16AU"/>
<attribute name="OC_FARNELL" value="9171134"/>
<attribute name="OC_NEWARK" value="96K6515"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY15L" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2.7 V&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM&lt;p&gt;
4-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="6-I/O-3"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(ADC0)PB5" pad="1"/>
<connect gate="G$1" pin="(ADC1)PB2" pad="7"/>
<connect gate="G$1" pin="(ADC2)PB3" pad="3"/>
<connect gate="G$1" pin="(ADC3)PB4" pad="2"/>
<connect gate="G$1" pin="(AREF)PB0" pad="5"/>
<connect gate="G$1" pin="(OCP)PB1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(ADC0)PB5" pad="1"/>
<connect gate="G$1" pin="(ADC1)PB2" pad="7"/>
<connect gate="G$1" pin="(ADC2)PB3" pad="3"/>
<connect gate="G$1" pin="(ADC3)PB4" pad="2"/>
<connect gate="G$1" pin="(AREF)PB0" pad="5"/>
<connect gate="G$1" pin="(OCP)PB1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA163*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 Kbytes &lt;B&gt;EEPROM&lt;/B&gt;&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
UART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
hardware multiplier&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-5"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA163*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
UART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
hardware multiplier&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-6"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY28*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1.8 V&lt;p&gt;
2 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="20-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(IR)PA2" pad="25"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND1" pad="22"/>
<connect gate="G$1" pin="NC1" pad="21"/>
<connect gate="G$1" pin="PA0" pad="28"/>
<connect gate="G$1" pin="PA1" pad="27"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PB0(AIN0)" pad="14"/>
<connect gate="G$1" pin="PB1(AIN1)" pad="15"/>
<connect gate="G$1" pin="PB2(T0)" pad="16"/>
<connect gate="G$1" pin="PB3(INT0)" pad="17"/>
<connect gate="G$1" pin="PB4(INT1)" pad="18"/>
<connect gate="G$1" pin="PB5" pad="19"/>
<connect gate="G$1" pin="PB6" pad="23"/>
<connect gate="G$1" pin="PB7" pad="24"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD2" pad="4"/>
<connect gate="G$1" pin="PD3" pad="5"/>
<connect gate="G$1" pin="PD4" pad="6"/>
<connect gate="G$1" pin="PD5" pad="11"/>
<connect gate="G$1" pin="PD6" pad="12"/>
<connect gate="G$1" pin="PD7" pad="13"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY28*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1.8 V&lt;p&gt;
2 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="20-I/O-4"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(IR)PA2" pad="25"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND1" pad="21"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="NC3" pad="19"/>
<connect gate="G$1" pin="NC4" pad="20"/>
<connect gate="G$1" pin="NC5" pad="22"/>
<connect gate="G$1" pin="PA0" pad="28"/>
<connect gate="G$1" pin="PA1" pad="27"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PB0(AIN0)" pad="12"/>
<connect gate="G$1" pin="PB1(AIN1)" pad="13"/>
<connect gate="G$1" pin="PB2(T0)" pad="14"/>
<connect gate="G$1" pin="PB3(INT0)" pad="15"/>
<connect gate="G$1" pin="PB4(INT1)" pad="16"/>
<connect gate="G$1" pin="PB5" pad="17"/>
<connect gate="G$1" pin="PB6" pad="23"/>
<connect gate="G$1" pin="PB7" pad="24"/>
<connect gate="G$1" pin="PD0" pad="30"/>
<connect gate="G$1" pin="PD1" pad="31"/>
<connect gate="G$1" pin="PD2" pad="32"/>
<connect gate="G$1" pin="PD3" pad="1"/>
<connect gate="G$1" pin="PD4" pad="2"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="10"/>
<connect gate="G$1" pin="PD7" pad="11"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VCC1" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT25*" prefix="IC">
<description>SPI bus serial &lt;B&gt;EEPROM&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="250X0"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CS/" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD/" pad="7"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP/" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT25040LI-G"/>
<attribute name="OC_FARNELL" value="1718045"/>
<attribute name="OC_NEWARK" value="06R0588"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT24C*" prefix="IC">
<description>2-wire serial &lt;B&gt;EEPROM&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="24CXX"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C1024BW-SH-B"/>
<attribute name="OC_FARNELL" value="1362646"/>
<attribute name="OC_NEWARK" value="03P2044"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDE2506" prefix="IC">
<description>I2C/MicroWire &lt;B&gt;EEPROM&lt;/B&gt; (24xxx)</description>
<gates>
<gate name="G$1" symbol="SDE2506"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CE/" pad="2"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="TG" pad="8"/>
<connect gate="G$1" pin="TP" pad="7"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT93C*6" prefix="IC">
<description>3-wire serial EEPROM</description>
<gates>
<gate name="G$1" symbol="93CX6"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DC" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT93C46D-PU"/>
<attribute name="OC_FARNELL" value="1362666"/>
<attribute name="OC_NEWARK" value="50M3339"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C2051" prefix="IC">
<description>80C31 &lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
2.7 V</description>
<gates>
<gate name="G$1" symbol="89C2051"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="AIN0-P1.0" pad="12"/>
<connect gate="G$1" pin="AIN1-P1.1" pad="13"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="P1.2" pad="14"/>
<connect gate="G$1" pin="P1.3" pad="15"/>
<connect gate="G$1" pin="P1.4" pad="16"/>
<connect gate="G$1" pin="P1.5" pad="17"/>
<connect gate="G$1" pin="P1.6" pad="18"/>
<connect gate="G$1" pin="P1.7" pad="19"/>
<connect gate="G$1" pin="P3.0-RXD" pad="2"/>
<connect gate="G$1" pin="P3.1-TXD" pad="3"/>
<connect gate="G$1" pin="P3.2-INTO/" pad="6"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="7"/>
<connect gate="G$1" pin="P3.4-T0" pad="8"/>
<connect gate="G$1" pin="P3.5-T1" pad="9"/>
<connect gate="G$1" pin="P3.7" pad="11"/>
<connect gate="G$1" pin="RST-VPP" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C2051-12PU"/>
<attribute name="OC_FARNELL" value="1699389"/>
<attribute name="OC_NEWARK" value="80P3687"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC20S">
<connects>
<connect gate="G$1" pin="AIN0-P1.0" pad="12"/>
<connect gate="G$1" pin="AIN1-P1.1" pad="13"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="P1.2" pad="14"/>
<connect gate="G$1" pin="P1.3" pad="15"/>
<connect gate="G$1" pin="P1.4" pad="16"/>
<connect gate="G$1" pin="P1.5" pad="17"/>
<connect gate="G$1" pin="P1.6" pad="18"/>
<connect gate="G$1" pin="P1.7" pad="19"/>
<connect gate="G$1" pin="P3.0-RXD" pad="2"/>
<connect gate="G$1" pin="P3.1-TXD" pad="3"/>
<connect gate="G$1" pin="P3.2-INTO/" pad="6"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="7"/>
<connect gate="G$1" pin="P3.4-T0" pad="8"/>
<connect gate="G$1" pin="P3.5-T1" pad="9"/>
<connect gate="G$1" pin="P3.7" pad="11"/>
<connect gate="G$1" pin="RST-VPP" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C2051-12SU"/>
<attribute name="OC_FARNELL" value="1699390"/>
<attribute name="OC_NEWARK" value="80P3688"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA103*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (L)&lt;p&gt;
128 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
2 Kbytes EEPROM&lt;p&gt;
UART&lt;p&gt;
RTC&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="48-I/O-2"/>
</gates>
<devices>
<device name="" package="TQFP64">
<connects>
<connect gate="G$1" pin="01" pad="21"/>
<connect gate="G$1" pin="02" pad="22"/>
<connect gate="G$1" pin="A10-PC2" pad="37"/>
<connect gate="G$1" pin="A11-PC3" pad="38"/>
<connect gate="G$1" pin="A12-PC4" pad="39"/>
<connect gate="G$1" pin="A13-PC5" pad="40"/>
<connect gate="G$1" pin="A14-PC6" pad="41"/>
<connect gate="G$1" pin="A15-PC7" pad="42"/>
<connect gate="G$1" pin="A8-PC0" pad="35"/>
<connect gate="G$1" pin="A9-PC1" pad="36"/>
<connect gate="G$1" pin="AC+_PE2" pad="4"/>
<connect gate="G$1" pin="AC-_PE3" pad="5"/>
<connect gate="G$1" pin="AD0-PA0" pad="51"/>
<connect gate="G$1" pin="AD1-PA1" pad="50"/>
<connect gate="G$1" pin="AD2-PA2" pad="49"/>
<connect gate="G$1" pin="AD3-PA3" pad="48"/>
<connect gate="G$1" pin="AD4-PA4" pad="47"/>
<connect gate="G$1" pin="AD5-PA5" pad="46"/>
<connect gate="G$1" pin="AD6-PA6" pad="45"/>
<connect gate="G$1" pin="AD7-PA7" pad="44"/>
<connect gate="G$1" pin="ADC0-PF0" pad="61"/>
<connect gate="G$1" pin="ADC1-PF1" pad="60"/>
<connect gate="G$1" pin="ADC2-PF2" pad="59"/>
<connect gate="G$1" pin="ADC3-PF3" pad="58"/>
<connect gate="G$1" pin="ADC4-PF4" pad="57"/>
<connect gate="G$1" pin="ADC5-PF5" pad="56"/>
<connect gate="G$1" pin="ADC6-PF6" pad="55"/>
<connect gate="G$1" pin="ADC7-PF7" pad="54"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="ALE" pad="43"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="AVREF" pad="62"/>
<connect gate="G$1" pin="GND" pad="53"/>
<connect gate="G$1" pin="INT4-PE4" pad="6"/>
<connect gate="G$1" pin="INT5-PE5" pad="7"/>
<connect gate="G$1" pin="INT6-PE6" pad="8"/>
<connect gate="G$1" pin="INT7-PE7" pad="9"/>
<connect gate="G$1" pin="MISO-PB3" pad="13"/>
<connect gate="G$1" pin="MOSI-PB2" pad="12"/>
<connect gate="G$1" pin="OC0-PB4" pad="14"/>
<connect gate="G$1" pin="OC1A-PB5" pad="15"/>
<connect gate="G$1" pin="OC1B-PB6" pad="16"/>
<connect gate="G$1" pin="OC2-PB7" pad="17"/>
<connect gate="G$1" pin="PD0-INT0" pad="25"/>
<connect gate="G$1" pin="PD1-INT1" pad="26"/>
<connect gate="G$1" pin="PD2-INT2" pad="27"/>
<connect gate="G$1" pin="PD3-INT3" pad="28"/>
<connect gate="G$1" pin="PD4-IC1" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6-T1" pad="31"/>
<connect gate="G$1" pin="PD7-T2" pad="32"/>
<connect gate="G$1" pin="PEN/" pad="1"/>
<connect gate="G$1" pin="RD/" pad="34"/>
<connect gate="G$1" pin="RESET/" pad="20"/>
<connect gate="G$1" pin="RXD-PE0" pad="2"/>
<connect gate="G$1" pin="SCK-PB1" pad="11"/>
<connect gate="G$1" pin="SS-PB0" pad="10"/>
<connect gate="G$1" pin="TOSC1" pad="19"/>
<connect gate="G$1" pin="TOSC2" pad="18"/>
<connect gate="G$1" pin="TXD-PE1" pad="3"/>
<connect gate="G$1" pin="VCC" pad="52"/>
<connect gate="G$1" pin="WR/" pad="33"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C*52" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH; 2K Bytes EEPROM&lt;br&gt;
Compatible with MCS-51 Products&lt;br&gt;
at89s8252.pdf</description>
<gates>
<gate name="G$1" symbol="AT89C52"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="P6" package="DIL40">
<connects>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="EA" pad="31"/>
<connect gate="G$1" pin="P0.0AD0" pad="39"/>
<connect gate="G$1" pin="P0.1AD1" pad="38"/>
<connect gate="G$1" pin="P0.2AD2" pad="37"/>
<connect gate="G$1" pin="P0.3AD3" pad="36"/>
<connect gate="G$1" pin="P0.4AD4" pad="35"/>
<connect gate="G$1" pin="P0.5AD5" pad="34"/>
<connect gate="G$1" pin="P0.6AD6" pad="33"/>
<connect gate="G$1" pin="P0.7AD7" pad="32"/>
<connect gate="G$1" pin="P1.0_T2" pad="1"/>
<connect gate="G$1" pin="P1.1_T2EX" pad="2"/>
<connect gate="G$1" pin="P1.2" pad="3"/>
<connect gate="G$1" pin="P1.3" pad="4"/>
<connect gate="G$1" pin="P1.4" pad="5"/>
<connect gate="G$1" pin="P1.5" pad="6"/>
<connect gate="G$1" pin="P1.6" pad="7"/>
<connect gate="G$1" pin="P1.7" pad="8"/>
<connect gate="G$1" pin="P2.0_A8" pad="21"/>
<connect gate="G$1" pin="P2.1_A9" pad="22"/>
<connect gate="G$1" pin="P2.2_A10" pad="23"/>
<connect gate="G$1" pin="P2.3_A11" pad="24"/>
<connect gate="G$1" pin="P2.4_A12" pad="25"/>
<connect gate="G$1" pin="P2.5_A13" pad="26"/>
<connect gate="G$1" pin="P2.6_A14" pad="27"/>
<connect gate="G$1" pin="P2.7_A15" pad="28"/>
<connect gate="G$1" pin="P3.0" pad="10"/>
<connect gate="G$1" pin="P3.1" pad="11"/>
<connect gate="G$1" pin="P3.2" pad="12"/>
<connect gate="G$1" pin="P3.3" pad="13"/>
<connect gate="G$1" pin="P3.4/T0" pad="14"/>
<connect gate="G$1" pin="P3.5/T1" pad="15"/>
<connect gate="G$1" pin="P3.6/WR" pad="16"/>
<connect gate="G$1" pin="P3.7/RD" pad="17"/>
<connect gate="G$1" pin="PSEN" pad="29"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="EA" pad="35"/>
<connect gate="G$1" pin="P0.0AD0" pad="43"/>
<connect gate="G$1" pin="P0.1AD1" pad="42"/>
<connect gate="G$1" pin="P0.2AD2" pad="41"/>
<connect gate="G$1" pin="P0.3AD3" pad="40"/>
<connect gate="G$1" pin="P0.4AD4" pad="39"/>
<connect gate="G$1" pin="P0.5AD5" pad="38"/>
<connect gate="G$1" pin="P0.6AD6" pad="37"/>
<connect gate="G$1" pin="P0.7AD7" pad="36"/>
<connect gate="G$1" pin="P1.0_T2" pad="2"/>
<connect gate="G$1" pin="P1.1_T2EX" pad="3"/>
<connect gate="G$1" pin="P1.2" pad="4"/>
<connect gate="G$1" pin="P1.3" pad="5"/>
<connect gate="G$1" pin="P1.4" pad="6"/>
<connect gate="G$1" pin="P1.5" pad="7"/>
<connect gate="G$1" pin="P1.6" pad="8"/>
<connect gate="G$1" pin="P1.7" pad="9"/>
<connect gate="G$1" pin="P2.0_A8" pad="24"/>
<connect gate="G$1" pin="P2.1_A9" pad="25"/>
<connect gate="G$1" pin="P2.2_A10" pad="26"/>
<connect gate="G$1" pin="P2.3_A11" pad="27"/>
<connect gate="G$1" pin="P2.4_A12" pad="28"/>
<connect gate="G$1" pin="P2.5_A13" pad="29"/>
<connect gate="G$1" pin="P2.6_A14" pad="30"/>
<connect gate="G$1" pin="P2.7_A15" pad="31"/>
<connect gate="G$1" pin="P3.0" pad="11"/>
<connect gate="G$1" pin="P3.1" pad="13"/>
<connect gate="G$1" pin="P3.2" pad="14"/>
<connect gate="G$1" pin="P3.3" pad="15"/>
<connect gate="G$1" pin="P3.4/T0" pad="16"/>
<connect gate="G$1" pin="P3.5/T1" pad="17"/>
<connect gate="G$1" pin="P3.6/WR" pad="18"/>
<connect gate="G$1" pin="P3.7/RD" pad="19"/>
<connect gate="G$1" pin="PSEN" pad="32"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="VCC" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="Q" package="PQFP44">
<connects>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="EA" pad="29"/>
<connect gate="G$1" pin="P0.0AD0" pad="37"/>
<connect gate="G$1" pin="P0.1AD1" pad="36"/>
<connect gate="G$1" pin="P0.2AD2" pad="35"/>
<connect gate="G$1" pin="P0.3AD3" pad="34"/>
<connect gate="G$1" pin="P0.4AD4" pad="33"/>
<connect gate="G$1" pin="P0.5AD5" pad="32"/>
<connect gate="G$1" pin="P0.6AD6" pad="31"/>
<connect gate="G$1" pin="P0.7AD7" pad="30"/>
<connect gate="G$1" pin="P1.0_T2" pad="40"/>
<connect gate="G$1" pin="P1.1_T2EX" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5" pad="1"/>
<connect gate="G$1" pin="P1.6" pad="2"/>
<connect gate="G$1" pin="P1.7" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0" pad="5"/>
<connect gate="G$1" pin="P3.1" pad="7"/>
<connect gate="G$1" pin="P3.2" pad="8"/>
<connect gate="G$1" pin="P3.3" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/WR" pad="12"/>
<connect gate="G$1" pin="P3.7/RD" pad="13"/>
<connect gate="G$1" pin="PSEN" pad="26"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="EA" pad="29"/>
<connect gate="G$1" pin="P0.0AD0" pad="37"/>
<connect gate="G$1" pin="P0.1AD1" pad="36"/>
<connect gate="G$1" pin="P0.2AD2" pad="35"/>
<connect gate="G$1" pin="P0.3AD3" pad="34"/>
<connect gate="G$1" pin="P0.4AD4" pad="33"/>
<connect gate="G$1" pin="P0.5AD5" pad="32"/>
<connect gate="G$1" pin="P0.6AD6" pad="31"/>
<connect gate="G$1" pin="P0.7AD7" pad="30"/>
<connect gate="G$1" pin="P1.0_T2" pad="40"/>
<connect gate="G$1" pin="P1.1_T2EX" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5" pad="1"/>
<connect gate="G$1" pin="P1.6" pad="2"/>
<connect gate="G$1" pin="P1.7" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0" pad="5"/>
<connect gate="G$1" pin="P3.1" pad="7"/>
<connect gate="G$1" pin="P3.2" pad="8"/>
<connect gate="G$1" pin="P3.3" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/WR" pad="12"/>
<connect gate="G$1" pin="P3.7/RD" pad="13"/>
<connect gate="G$1" pin="PSEN" pad="26"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27C080" prefix="IC">
<description>&lt;b&gt;8-Megabit (1Mx8) OTP EPROM&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="27C080"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="32P6" package="DIL32">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE!VPP" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A19" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="O0" pad="13"/>
<connect gate="G$1" pin="O1" pad="14"/>
<connect gate="G$1" pin="O2" pad="15"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="18"/>
<connect gate="G$1" pin="O5" pad="19"/>
<connect gate="G$1" pin="O6" pad="20"/>
<connect gate="G$1" pin="O7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT27C080-90PU"/>
<attribute name="OC_FARNELL" value="1455026"/>
<attribute name="OC_NEWARK" value="58M3824"/>
</technology>
</technologies>
</device>
<device name="R" package="SO32X">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE!VPP" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A19" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="O0" pad="13"/>
<connect gate="G$1" pin="O1" pad="14"/>
<connect gate="G$1" pin="O2" pad="15"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="18"/>
<connect gate="G$1" pin="O5" pad="19"/>
<connect gate="G$1" pin="O6" pad="20"/>
<connect gate="G$1" pin="O7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC32R">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE!VPP" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A19" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="O0" pad="13"/>
<connect gate="G$1" pin="O1" pad="14"/>
<connect gate="G$1" pin="O2" pad="15"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="18"/>
<connect gate="G$1" pin="O5" pad="19"/>
<connect gate="G$1" pin="O6" pad="20"/>
<connect gate="G$1" pin="O7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT27C080-90JU"/>
<attribute name="OC_FARNELL" value="1455025"/>
<attribute name="OC_NEWARK" value="58M3823"/>
</technology>
</technologies>
</device>
<device name="T" package="TSOP32">
<connects>
<connect gate="G$1" pin="!CE" pad="30"/>
<connect gate="G$1" pin="!OE!VPP" pad="32"/>
<connect gate="G$1" pin="A0" pad="20"/>
<connect gate="G$1" pin="A1" pad="19"/>
<connect gate="G$1" pin="A10" pad="31"/>
<connect gate="G$1" pin="A11" pad="1"/>
<connect gate="G$1" pin="A12" pad="12"/>
<connect gate="G$1" pin="A13" pad="4"/>
<connect gate="G$1" pin="A14" pad="5"/>
<connect gate="G$1" pin="A15" pad="11"/>
<connect gate="G$1" pin="A16" pad="10"/>
<connect gate="G$1" pin="A17" pad="6"/>
<connect gate="G$1" pin="A18" pad="7"/>
<connect gate="G$1" pin="A19" pad="9"/>
<connect gate="G$1" pin="A2" pad="18"/>
<connect gate="G$1" pin="A3" pad="17"/>
<connect gate="G$1" pin="A4" pad="16"/>
<connect gate="G$1" pin="A5" pad="15"/>
<connect gate="G$1" pin="A6" pad="14"/>
<connect gate="G$1" pin="A7" pad="13"/>
<connect gate="G$1" pin="A8" pad="3"/>
<connect gate="G$1" pin="A9" pad="2"/>
<connect gate="G$1" pin="O0" pad="21"/>
<connect gate="G$1" pin="O1" pad="22"/>
<connect gate="G$1" pin="O2" pad="23"/>
<connect gate="G$1" pin="O3" pad="25"/>
<connect gate="G$1" pin="O4" pad="26"/>
<connect gate="G$1" pin="O5" pad="27"/>
<connect gate="G$1" pin="O6" pad="28"/>
<connect gate="G$1" pin="O7" pad="29"/>
<connect gate="P" pin="GND" pad="24"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91R4008" prefix="IC">
<description>&lt;b&gt;AT91 ARM® Thumb® RISC-Controller&lt;/b&gt;&lt;p&gt;
Microcontroller AT91R40008</description>
<gates>
<gate name="A" symbol="AT91R4008"/>
<gate name="B" symbol="AT91R4008-PARPORT"/>
<gate name="C" symbol="AT91R4008-ADR"/>
<gate name="D" symbol="D0-15"/>
<gate name="P1" symbol="GND"/>
<gate name="P2" symbol="GND"/>
<gate name="P3" symbol="GND"/>
<gate name="P4" symbol="GND"/>
<gate name="P5" symbol="GND"/>
<gate name="P15" symbol="VDDIO"/>
<gate name="P16" symbol="VDDIO"/>
<gate name="P17" symbol="VDDIO"/>
<gate name="P6" symbol="GND"/>
<gate name="P7" symbol="GND"/>
<gate name="P8" symbol="GND"/>
<gate name="P9" symbol="GND"/>
<gate name="P10" symbol="VDDIO"/>
<gate name="P11" symbol="VDDIO"/>
<gate name="P12" symbol="VDDCORE"/>
<gate name="P13" symbol="VDDCORE"/>
<gate name="P14" symbol="VDDCORE"/>
<gate name="P18" symbol="VDDIO"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="A" pin="GND" pad="78"/>
<connect gate="A" pin="MCKI" pad="82"/>
<connect gate="A" pin="NCS0" pad="97"/>
<connect gate="A" pin="NCS1" pad="98"/>
<connect gate="A" pin="NRD/NOE" pad="92"/>
<connect gate="A" pin="NRST" pad="79"/>
<connect gate="A" pin="NRW0/NWE" pad="93"/>
<connect gate="A" pin="NRW1/NUB" pad="77"/>
<connect gate="A" pin="NWAIT" pad="96"/>
<connect gate="A" pin="NWDOVF" pad="80"/>
<connect gate="A" pin="TCK" pad="91"/>
<connect gate="A" pin="TDI" pad="89"/>
<connect gate="A" pin="TDO" pad="90"/>
<connect gate="A" pin="TMS" pad="88"/>
<connect gate="B" pin="P0/TCLK0" pad="49"/>
<connect gate="B" pin="P1/TIOA0" pad="50"/>
<connect gate="B" pin="P10/IRQ1" pad="63"/>
<connect gate="B" pin="P11/IRQ2" pad="64"/>
<connect gate="B" pin="P12/FIQ" pad="66"/>
<connect gate="B" pin="P13/SCK0" pad="67"/>
<connect gate="B" pin="P14/TXD0" pad="68"/>
<connect gate="B" pin="P15/RXD0" pad="69"/>
<connect gate="B" pin="P16" pad="70"/>
<connect gate="B" pin="P17" pad="71"/>
<connect gate="B" pin="P18" pad="72"/>
<connect gate="B" pin="P19" pad="73"/>
<connect gate="B" pin="P2/TIOB0" pad="51"/>
<connect gate="B" pin="P20/SCK1" pad="74"/>
<connect gate="B" pin="P21/TXD1/NTRI" pad="75"/>
<connect gate="B" pin="P22/RXD1" pad="76"/>
<connect gate="B" pin="P23" pad="83"/>
<connect gate="B" pin="P24/BMS" pad="84"/>
<connect gate="B" pin="P25/MCKO" pad="85"/>
<connect gate="B" pin="P26/NCS2" pad="99"/>
<connect gate="B" pin="P27/NCS3" pad="100"/>
<connect gate="B" pin="P3/TCLK1" pad="54"/>
<connect gate="B" pin="P4/TIOA1" pad="55"/>
<connect gate="B" pin="P5/TIOB1" pad="56"/>
<connect gate="B" pin="P6/TCLK2" pad="57"/>
<connect gate="B" pin="P7/TIOA2" pad="58"/>
<connect gate="B" pin="P8/TIOB2" pad="59"/>
<connect gate="B" pin="P9/IRQ0" pad="60"/>
<connect gate="C" pin="A1" pad="3"/>
<connect gate="C" pin="A10" pad="13"/>
<connect gate="C" pin="A11" pad="14"/>
<connect gate="C" pin="A12" pad="15"/>
<connect gate="C" pin="A13" pad="16"/>
<connect gate="C" pin="A14" pad="17"/>
<connect gate="C" pin="A15" pad="20"/>
<connect gate="C" pin="A16" pad="21"/>
<connect gate="C" pin="A17" pad="22"/>
<connect gate="C" pin="A18" pad="23"/>
<connect gate="C" pin="A19" pad="24"/>
<connect gate="C" pin="A2" pad="4"/>
<connect gate="C" pin="A3" pad="5"/>
<connect gate="C" pin="A4" pad="6"/>
<connect gate="C" pin="A5" pad="7"/>
<connect gate="C" pin="A6" pad="8"/>
<connect gate="C" pin="A7" pad="9"/>
<connect gate="C" pin="A8" pad="11"/>
<connect gate="C" pin="A9" pad="12"/>
<connect gate="C" pin="NLB/A0" pad="1"/>
<connect gate="C" pin="P28/CS7/A20" pad="25"/>
<connect gate="C" pin="P29/CS6/A21" pad="26"/>
<connect gate="C" pin="P30/CS5/A22" pad="29"/>
<connect gate="C" pin="P31/CS4/A23" pad="30"/>
<connect gate="D" pin="D0" pad="31"/>
<connect gate="D" pin="D1" pad="32"/>
<connect gate="D" pin="D10" pad="42"/>
<connect gate="D" pin="D11" pad="43"/>
<connect gate="D" pin="D12" pad="45"/>
<connect gate="D" pin="D13" pad="46"/>
<connect gate="D" pin="D14" pad="47"/>
<connect gate="D" pin="D15" pad="48"/>
<connect gate="D" pin="D2" pad="33"/>
<connect gate="D" pin="D3" pad="34"/>
<connect gate="D" pin="D4" pad="35"/>
<connect gate="D" pin="D5" pad="37"/>
<connect gate="D" pin="D6" pad="38"/>
<connect gate="D" pin="D7" pad="39"/>
<connect gate="D" pin="D8" pad="40"/>
<connect gate="D" pin="D9" pad="41"/>
<connect gate="P1" pin="GND" pad="2"/>
<connect gate="P10" pin="VDDIO" pad="62"/>
<connect gate="P11" pin="VDDIO" pad="81"/>
<connect gate="P12" pin="VDDCORE" pad="27"/>
<connect gate="P13" pin="VDDCORE" pad="61"/>
<connect gate="P14" pin="VDDCORE" pad="94"/>
<connect gate="P15" pin="VDDIO" pad="10"/>
<connect gate="P16" pin="VDDIO" pad="28"/>
<connect gate="P17" pin="VDDIO" pad="44"/>
<connect gate="P18" pin="VDDIO" pad="95"/>
<connect gate="P2" pin="GND" pad="18"/>
<connect gate="P3" pin="GND" pad="19"/>
<connect gate="P4" pin="GND" pad="36"/>
<connect gate="P5" pin="GND" pad="52"/>
<connect gate="P6" pin="GND" pad="53"/>
<connect gate="P7" pin="GND" pad="65"/>
<connect gate="P8" pin="GND" pad="86"/>
<connect gate="P9" pin="GND" pad="87"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY26*" prefix="IC">
<description>&lt;b&gt;8-bit AVR Microcontroller with 2K Bytes Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com .. doc1477.pdf</description>
<gates>
<gate name="G$1" symbol="TINY26"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="20"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="19"/>
<connect gate="G$1" pin="(ADC10/!RESET!)PB7" pad="10"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="18"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="14"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="13"/>
<connect gate="G$1" pin="(ADC5/AIN0)PA6" pad="12"/>
<connect gate="G$1" pin="(ADC6/AIN1)PA7" pad="11"/>
<connect gate="G$1" pin="(ADC7/XTAL1)PB4" pad="7"/>
<connect gate="G$1" pin="(ADC8/XTAL2)PB5" pad="8"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="9"/>
<connect gate="G$1" pin="(AREF)PA3" pad="17"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="2"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/!OC1A!)PB0" pad="1"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="4"/>
<connect gate="G$1" pin="(SCK/SCL/!OC1B!)PB2" pad="3"/>
<connect gate="G$1" pin="AVCC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY261-20PU"/>
<attribute name="OC_FARNELL" value="1455146"/>
<attribute name="OC_NEWARK" value="58M3782"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY26L-8PU"/>
<attribute name="OC_FARNELL" value="9171657"/>
<attribute name="OC_NEWARK" value="01M6920"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="20"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="19"/>
<connect gate="G$1" pin="(ADC10/!RESET!)PB7" pad="10"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="18"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="14"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="13"/>
<connect gate="G$1" pin="(ADC5/AIN0)PA6" pad="12"/>
<connect gate="G$1" pin="(ADC6/AIN1)PA7" pad="11"/>
<connect gate="G$1" pin="(ADC7/XTAL1)PB4" pad="7"/>
<connect gate="G$1" pin="(ADC8/XTAL2)PB5" pad="8"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="9"/>
<connect gate="G$1" pin="(AREF)PA3" pad="17"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="2"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/!OC1A!)PB0" pad="1"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="4"/>
<connect gate="G$1" pin="(SCK/SCL/!OC1B!)PB2" pad="3"/>
<connect gate="G$1" pin="AVCC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY261-20SU"/>
<attribute name="OC_FARNELL" value="1455147"/>
<attribute name="OC_NEWARK" value="58M3783"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY26L-8SU"/>
<attribute name="OC_FARNELL" value="9171665"/>
<attribute name="OC_NEWARK" value="01M6921"/>
</technology>
</technologies>
</device>
<device name="M" package="MLF32">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="26"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="25"/>
<connect gate="G$1" pin="(ADC10/!RESET!)PB7" pad="11"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="23"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="17"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="15"/>
<connect gate="G$1" pin="(ADC5/AIN0)PA6" pad="14"/>
<connect gate="G$1" pin="(ADC6/AIN1)PA7" pad="13"/>
<connect gate="G$1" pin="(ADC7/XTAL1)PB4" pad="7"/>
<connect gate="G$1" pin="(ADC8/XTAL2)PB5" pad="8"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="10"/>
<connect gate="G$1" pin="(AREF)PA3" pad="22"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="31"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/!OC1A!)PB0" pad="30"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="2"/>
<connect gate="G$1" pin="(SCK/SCL/!OC1B!)PB2" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="21"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAM9708" prefix="SAM9708">
<description>&lt;b&gt;128-voice Integrated Sound Synthesizer&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SAM9708"/>
<gate name="C" symbol="SAM9708-SND"/>
<gate name="B" symbol="D0-15"/>
<gate name="D" symbol="WA27"/>
<gate name="E" symbol="WD15"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="V1" symbol="VCC1"/>
<gate name="V2" symbol="VCC1"/>
<gate name="V3" symbol="VCC1"/>
<gate name="V4" symbol="VCC1"/>
<gate name="V5" symbol="VCC1"/>
<gate name="V6" symbol="VCC2"/>
<gate name="V7" symbol="VCC2"/>
<gate name="V8" symbol="VCC2"/>
<gate name="V9" symbol="VCC2"/>
<gate name="V10" symbol="VCC2"/>
<gate name="V11" symbol="VC3"/>
<gate name="V12" symbol="VC3"/>
<gate name="V13" symbol="VC3"/>
<gate name="V14" symbol="VC3"/>
<gate name="V15" symbol="VC3"/>
<gate name="V16" symbol="VC3"/>
<gate name="V17" symbol="VC3"/>
<gate name="V18" symbol="VC3"/>
</gates>
<devices>
<device name="" package="TQFP144">
<connects>
<connect gate="A" pin="!CAS" pad="104"/>
<connect gate="A" pin="!CS" pad="16"/>
<connect gate="A" pin="!IO16" pad="4"/>
<connect gate="A" pin="!PWDN" pad="137"/>
<connect gate="A" pin="!RAS" pad="103"/>
<connect gate="A" pin="!RD" pad="10"/>
<connect gate="A" pin="!REFRESH" pad="105"/>
<connect gate="A" pin="!RESET" pad="134"/>
<connect gate="A" pin="!WR" pad="11"/>
<connect gate="A" pin="A0" pad="12"/>
<connect gate="A" pin="A1" pad="13"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="CK_OUT" pad="91"/>
<connect gate="A" pin="IRQ" pad="14"/>
<connect gate="A" pin="LDTEST" pad="136"/>
<connect gate="A" pin="OVCK-OUT" pad="47"/>
<connect gate="A" pin="RBS" pad="92"/>
<connect gate="A" pin="READY" pad="7"/>
<connect gate="A" pin="TEST" pad="135"/>
<connect gate="A" pin="X1" pad="61"/>
<connect gate="A" pin="X2" pad="62"/>
<connect gate="B" pin="D0" pad="19"/>
<connect gate="B" pin="D1" pad="22"/>
<connect gate="B" pin="D10" pad="1"/>
<connect gate="B" pin="D11" pad="144"/>
<connect gate="B" pin="D12" pad="141"/>
<connect gate="B" pin="D13" pad="140"/>
<connect gate="B" pin="D14" pad="139"/>
<connect gate="B" pin="D15" pad="138"/>
<connect gate="B" pin="D2" pad="23"/>
<connect gate="B" pin="D3" pad="24"/>
<connect gate="B" pin="D4" pad="25"/>
<connect gate="B" pin="D5" pad="26"/>
<connect gate="B" pin="D6" pad="27"/>
<connect gate="B" pin="D7" pad="28"/>
<connect gate="B" pin="D8" pad="3"/>
<connect gate="B" pin="D9" pad="2"/>
<connect gate="C" pin="!WCS0" pad="89"/>
<connect gate="C" pin="!WCS1" pad="90"/>
<connect gate="C" pin="!WOE" pad="88"/>
<connect gate="C" pin="!WWE" pad="87"/>
<connect gate="C" pin="BCK-OUT" pad="46"/>
<connect gate="C" pin="LFT" pad="60"/>
<connect gate="C" pin="MIDI1_IN" pad="29"/>
<connect gate="C" pin="MIDI1_OUT" pad="31"/>
<connect gate="C" pin="MIDI2_IN" pad="30"/>
<connect gate="C" pin="MIDI2_OUT" pad="32"/>
<connect gate="C" pin="SD-IN0" pad="33"/>
<connect gate="C" pin="SD-IN1" pad="34"/>
<connect gate="C" pin="SD-IN2" pad="37"/>
<connect gate="C" pin="SD-IN3" pad="38"/>
<connect gate="C" pin="SD-IN4" pad="48"/>
<connect gate="C" pin="SD-IN5" pad="49"/>
<connect gate="C" pin="SD-IN6" pad="50"/>
<connect gate="C" pin="SD-IN7" pad="53"/>
<connect gate="C" pin="SD-OUT0" pad="39"/>
<connect gate="C" pin="SD-OUT1" pad="40"/>
<connect gate="C" pin="SD-OUT2" pad="43"/>
<connect gate="C" pin="SD-OUT3" pad="44"/>
<connect gate="C" pin="SD-OUT4" pad="54"/>
<connect gate="C" pin="SD-OUT5" pad="55"/>
<connect gate="C" pin="SD-OUT6" pad="56"/>
<connect gate="C" pin="SD-OUT7" pad="57"/>
<connect gate="C" pin="WS-OUT" pad="45"/>
<connect gate="D" pin="WA0" pad="93"/>
<connect gate="D" pin="WA1" pad="94"/>
<connect gate="D" pin="WA10" pad="114"/>
<connect gate="D" pin="WA11" pad="115"/>
<connect gate="D" pin="WA12" pad="116"/>
<connect gate="D" pin="WA13" pad="117"/>
<connect gate="D" pin="WA14" pad="118"/>
<connect gate="D" pin="WA15" pad="119"/>
<connect gate="D" pin="WA16" pad="120"/>
<connect gate="D" pin="WA17" pad="121"/>
<connect gate="D" pin="WA18" pad="122"/>
<connect gate="D" pin="WA19" pad="123"/>
<connect gate="D" pin="WA2" pad="95"/>
<connect gate="D" pin="WA20" pad="126"/>
<connect gate="D" pin="WA21" pad="127"/>
<connect gate="D" pin="WA22" pad="128"/>
<connect gate="D" pin="WA23" pad="129"/>
<connect gate="D" pin="WA24" pad="130"/>
<connect gate="D" pin="WA25" pad="131"/>
<connect gate="D" pin="WA26" pad="132"/>
<connect gate="D" pin="WA3" pad="96"/>
<connect gate="D" pin="WA4" pad="101"/>
<connect gate="D" pin="WA5" pad="102"/>
<connect gate="D" pin="WA6" pad="106"/>
<connect gate="D" pin="WA7" pad="107"/>
<connect gate="D" pin="WA8" pad="108"/>
<connect gate="D" pin="WA9" pad="111"/>
<connect gate="E" pin="WD0" pad="86"/>
<connect gate="E" pin="WD1" pad="85"/>
<connect gate="E" pin="WD10" pad="72"/>
<connect gate="E" pin="WD11" pad="71"/>
<connect gate="E" pin="WD12" pad="68"/>
<connect gate="E" pin="WD13" pad="67"/>
<connect gate="E" pin="WD14" pad="66"/>
<connect gate="E" pin="WD15" pad="65"/>
<connect gate="E" pin="WD2" pad="84"/>
<connect gate="E" pin="WD3" pad="79"/>
<connect gate="E" pin="WD4" pad="78"/>
<connect gate="E" pin="WD5" pad="77"/>
<connect gate="E" pin="WD6" pad="76"/>
<connect gate="E" pin="WD7" pad="75"/>
<connect gate="E" pin="WD8" pad="74"/>
<connect gate="E" pin="WD9" pad="73"/>
<connect gate="G1" pin="GND" pad="6"/>
<connect gate="G10" pin="GND" pad="70"/>
<connect gate="G11" pin="GND" pad="82"/>
<connect gate="G12" pin="GND" pad="83"/>
<connect gate="G13" pin="GND" pad="98"/>
<connect gate="G14" pin="GND" pad="100"/>
<connect gate="G15" pin="GND" pad="110"/>
<connect gate="G16" pin="GND" pad="113"/>
<connect gate="G17" pin="GND" pad="125"/>
<connect gate="G18" pin="GND" pad="133"/>
<connect gate="G19" pin="GND" pad="143"/>
<connect gate="G2" pin="GND" pad="9"/>
<connect gate="G3" pin="GND" pad="18"/>
<connect gate="G4" pin="GND" pad="21"/>
<connect gate="G5" pin="GND" pad="36"/>
<connect gate="G6" pin="GND" pad="42"/>
<connect gate="G7" pin="GND" pad="51"/>
<connect gate="G8" pin="GND" pad="59"/>
<connect gate="G9" pin="GND" pad="64"/>
<connect gate="V1" pin="VCC1" pad="5"/>
<connect gate="V10" pin="VCC2" pad="124"/>
<connect gate="V11" pin="VC3" pad="8"/>
<connect gate="V12" pin="VC3" pad="17"/>
<connect gate="V13" pin="VC3" pad="41"/>
<connect gate="V14" pin="VC3" pad="58"/>
<connect gate="V15" pin="VC3" pad="63"/>
<connect gate="V16" pin="VC3" pad="80"/>
<connect gate="V17" pin="VC3" pad="99"/>
<connect gate="V18" pin="VC3" pad="112"/>
<connect gate="V2" pin="VCC1" pad="20"/>
<connect gate="V3" pin="VCC1" pad="35"/>
<connect gate="V4" pin="VCC1" pad="52"/>
<connect gate="V5" pin="VCC1" pad="142"/>
<connect gate="V6" pin="VCC2" pad="69"/>
<connect gate="V7" pin="VCC2" pad="81"/>
<connect gate="V8" pin="VCC2" pad="97"/>
<connect gate="V9" pin="VCC2" pad="109"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T8*C5121" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with Multiprotocol Smart Card Interface&lt;/b&gt;&lt;p&gt;
Source: Uploaded by Heiko Künzel &lt;heiko.kuenzel@atg-gera.de&gt; from ATG Automatisierungstechnik Gera&lt;br&gt;
Mon Mar 10 13:32:48 2003 Atmel-Library mit zusätzlich T83C5121-Prozessor im SSOP24-Package.</description>
<gates>
<gate name="G$1" symbol="T8XC5121"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="CVCC" pad="3"/>
<connect gate="G$1" pin="CVSS" pad="1"/>
<connect gate="G$1" pin="DVCC" pad="22"/>
<connect gate="G$1" pin="EVCC" pad="23"/>
<connect gate="G$1" pin="LI" pad="2"/>
<connect gate="G$1" pin="P1.0/CIO" pad="9"/>
<connect gate="G$1" pin="P1.1/CC8" pad="8"/>
<connect gate="G$1" pin="P1.2/CPRES" pad="7"/>
<connect gate="G$1" pin="P1.3/CC4" pad="6"/>
<connect gate="G$1" pin="P1.4/CCLK" pad="5"/>
<connect gate="G$1" pin="P1.5/CRST" pad="4"/>
<connect gate="G$1" pin="P3.0/RXD" pad="20"/>
<connect gate="G$1" pin="P3.1/TXD" pad="19"/>
<connect gate="G$1" pin="P3.2/INT0" pad="16"/>
<connect gate="G$1" pin="P3.3/INT1" pad="18"/>
<connect gate="G$1" pin="P3.4/T0" pad="17"/>
<connect gate="G$1" pin="P3.5/CIO1" pad="15"/>
<connect gate="G$1" pin="P3.6/CCLK1/LED0" pad="14"/>
<connect gate="G$1" pin="P3.7/CRST1/LED1" pad="13"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="VCC" pad="24"/>
<connect gate="G$1" pin="VSS" pad="21"/>
<connect gate="G$1" pin="XTAL1" pad="12"/>
<connect gate="G$1" pin="XTAL2" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T8?C5121" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with Multiprotocol Smart Card Interface&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/...doc4164.pdf</description>
<gates>
<gate name="G$1" symbol="T8X5121-PLCC52"/>
</gates>
<devices>
<device name="3" package="PLCC52">
<connects>
<connect gate="G$1" pin="!RST" pad="20"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="CVCC" pad="6"/>
<connect gate="G$1" pin="CVSS" pad="2"/>
<connect gate="G$1" pin="DVCC" pad="46"/>
<connect gate="G$1" pin="EA" pad="10"/>
<connect gate="G$1" pin="EVCC" pad="51"/>
<connect gate="G$1" pin="LI" pad="3"/>
<connect gate="G$1" pin="P0.0/AD0" pad="42"/>
<connect gate="G$1" pin="P0.1/AD1" pad="41"/>
<connect gate="G$1" pin="P0.2/AD2" pad="40"/>
<connect gate="G$1" pin="P0.3/AD3" pad="39"/>
<connect gate="G$1" pin="P0.4/AD4" pad="33"/>
<connect gate="G$1" pin="P0.5/AD5" pad="21"/>
<connect gate="G$1" pin="P0.6/AD6" pad="38"/>
<connect gate="G$1" pin="P0.7/AD7" pad="30"/>
<connect gate="G$1" pin="P1.0/CIO" pad="18"/>
<connect gate="G$1" pin="P1.1/CC8" pad="17"/>
<connect gate="G$1" pin="P1.2/CPRES" pad="16"/>
<connect gate="G$1" pin="P1.3/CC4" pad="9"/>
<connect gate="G$1" pin="P1.4/CCLK" pad="8"/>
<connect gate="G$1" pin="P1.5/CRST" pad="7"/>
<connect gate="G$1" pin="P2.0/A8" pad="29"/>
<connect gate="G$1" pin="P2.1/A9" pad="28"/>
<connect gate="G$1" pin="P2.2/A10" pad="27"/>
<connect gate="G$1" pin="P2.3/A11" pad="26"/>
<connect gate="G$1" pin="P2.4/A12" pad="19"/>
<connect gate="G$1" pin="P2.5/A13" pad="15"/>
<connect gate="G$1" pin="P2.6/A14" pad="14"/>
<connect gate="G$1" pin="P2.7/A15" pad="13"/>
<connect gate="G$1" pin="P3.0/RXD" pad="44"/>
<connect gate="G$1" pin="P3.1/TXD" pad="43"/>
<connect gate="G$1" pin="P3.2/INT0" pad="35"/>
<connect gate="G$1" pin="P3.3/INT1" pad="37"/>
<connect gate="G$1" pin="P3.4/T0" pad="36"/>
<connect gate="G$1" pin="P3.5/CIO1" pad="34"/>
<connect gate="G$1" pin="P3.6/CCLK1/LED0" pad="32"/>
<connect gate="G$1" pin="P3.7/CRST1/LED1" pad="31"/>
<connect gate="G$1" pin="PSEN" pad="11"/>
<connect gate="G$1" pin="VCC" pad="24"/>
<connect gate="G$1" pin="VCC@1" pad="1"/>
<connect gate="G$1" pin="VSS" pad="25"/>
<connect gate="G$1" pin="VSS@1" pad="45"/>
<connect gate="G$1" pin="XTAL1" pad="23"/>
<connect gate="G$1" pin="XTAL2" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5" package="PLCC52">
<connects>
<connect gate="G$1" pin="!RST" pad="20"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="CVCC" pad="6"/>
<connect gate="G$1" pin="CVSS" pad="2"/>
<connect gate="G$1" pin="DVCC" pad="46"/>
<connect gate="G$1" pin="EA" pad="10"/>
<connect gate="G$1" pin="EVCC" pad="51"/>
<connect gate="G$1" pin="LI" pad="3"/>
<connect gate="G$1" pin="P0.0/AD0" pad="42"/>
<connect gate="G$1" pin="P0.1/AD1" pad="41"/>
<connect gate="G$1" pin="P0.2/AD2" pad="40"/>
<connect gate="G$1" pin="P0.3/AD3" pad="39"/>
<connect gate="G$1" pin="P0.4/AD4" pad="33"/>
<connect gate="G$1" pin="P0.5/AD5" pad="21"/>
<connect gate="G$1" pin="P0.6/AD6" pad="38"/>
<connect gate="G$1" pin="P0.7/AD7" pad="30"/>
<connect gate="G$1" pin="P1.0/CIO" pad="18"/>
<connect gate="G$1" pin="P1.1/CC8" pad="17"/>
<connect gate="G$1" pin="P1.2/CPRES" pad="16"/>
<connect gate="G$1" pin="P1.3/CC4" pad="9"/>
<connect gate="G$1" pin="P1.4/CCLK" pad="8"/>
<connect gate="G$1" pin="P1.5/CRST" pad="7"/>
<connect gate="G$1" pin="P2.0/A8" pad="29"/>
<connect gate="G$1" pin="P2.1/A9" pad="28"/>
<connect gate="G$1" pin="P2.2/A10" pad="27"/>
<connect gate="G$1" pin="P2.3/A11" pad="26"/>
<connect gate="G$1" pin="P2.4/A12" pad="19"/>
<connect gate="G$1" pin="P2.5/A13" pad="15"/>
<connect gate="G$1" pin="P2.6/A14" pad="14"/>
<connect gate="G$1" pin="P2.7/A15" pad="13"/>
<connect gate="G$1" pin="P3.0/RXD" pad="44"/>
<connect gate="G$1" pin="P3.1/TXD" pad="43"/>
<connect gate="G$1" pin="P3.2/INT0" pad="35"/>
<connect gate="G$1" pin="P3.3/INT1" pad="37"/>
<connect gate="G$1" pin="P3.4/T0" pad="36"/>
<connect gate="G$1" pin="P3.5/CIO1" pad="34"/>
<connect gate="G$1" pin="P3.6/CCLK1/LED0" pad="32"/>
<connect gate="G$1" pin="P3.7/CRST1/LED1" pad="31"/>
<connect gate="G$1" pin="PSEN" pad="11"/>
<connect gate="G$1" pin="VCC" pad="24"/>
<connect gate="G$1" pin="VCC@1" pad="1"/>
<connect gate="G$1" pin="VSS" pad="25"/>
<connect gate="G$1" pin="VSS@1" pad="45"/>
<connect gate="G$1" pin="XTAL1" pad="23"/>
<connect gate="G$1" pin="XTAL2" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="9" package="PLCC52">
<connects>
<connect gate="G$1" pin="!RST" pad="20"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="CVCC" pad="6"/>
<connect gate="G$1" pin="CVSS" pad="2"/>
<connect gate="G$1" pin="DVCC" pad="46"/>
<connect gate="G$1" pin="EA" pad="10"/>
<connect gate="G$1" pin="EVCC" pad="51"/>
<connect gate="G$1" pin="LI" pad="3"/>
<connect gate="G$1" pin="P0.0/AD0" pad="42"/>
<connect gate="G$1" pin="P0.1/AD1" pad="41"/>
<connect gate="G$1" pin="P0.2/AD2" pad="40"/>
<connect gate="G$1" pin="P0.3/AD3" pad="39"/>
<connect gate="G$1" pin="P0.4/AD4" pad="33"/>
<connect gate="G$1" pin="P0.5/AD5" pad="21"/>
<connect gate="G$1" pin="P0.6/AD6" pad="38"/>
<connect gate="G$1" pin="P0.7/AD7" pad="30"/>
<connect gate="G$1" pin="P1.0/CIO" pad="18"/>
<connect gate="G$1" pin="P1.1/CC8" pad="17"/>
<connect gate="G$1" pin="P1.2/CPRES" pad="16"/>
<connect gate="G$1" pin="P1.3/CC4" pad="9"/>
<connect gate="G$1" pin="P1.4/CCLK" pad="8"/>
<connect gate="G$1" pin="P1.5/CRST" pad="7"/>
<connect gate="G$1" pin="P2.0/A8" pad="29"/>
<connect gate="G$1" pin="P2.1/A9" pad="28"/>
<connect gate="G$1" pin="P2.2/A10" pad="27"/>
<connect gate="G$1" pin="P2.3/A11" pad="26"/>
<connect gate="G$1" pin="P2.4/A12" pad="19"/>
<connect gate="G$1" pin="P2.5/A13" pad="15"/>
<connect gate="G$1" pin="P2.6/A14" pad="14"/>
<connect gate="G$1" pin="P2.7/A15" pad="13"/>
<connect gate="G$1" pin="P3.0/RXD" pad="44"/>
<connect gate="G$1" pin="P3.1/TXD" pad="43"/>
<connect gate="G$1" pin="P3.2/INT0" pad="35"/>
<connect gate="G$1" pin="P3.3/INT1" pad="37"/>
<connect gate="G$1" pin="P3.4/T0" pad="36"/>
<connect gate="G$1" pin="P3.5/CIO1" pad="34"/>
<connect gate="G$1" pin="P3.6/CCLK1/LED0" pad="32"/>
<connect gate="G$1" pin="P3.7/CRST1/LED1" pad="31"/>
<connect gate="G$1" pin="PSEN" pad="11"/>
<connect gate="G$1" pin="VCC" pad="24"/>
<connect gate="G$1" pin="VCC@1" pad="1"/>
<connect gate="G$1" pin="VSS" pad="25"/>
<connect gate="G$1" pin="VSS@1" pad="45"/>
<connect gate="G$1" pin="XTAL1" pad="23"/>
<connect gate="G$1" pin="XTAL2" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT8*C51SND1C" prefix="IC">
<description>&lt;b&gt;Single-Chip Flash Microcontroller&lt;/b&gt;&lt;p&gt;
with MP3 Decoder and Human Interface&lt;br&gt;
Source: www.atmel.com .. doc4109.pdf</description>
<gates>
<gate name="G$1" symbol="AT89C51SND1C"/>
<gate name="P" symbol="P-AT89C51SND1C"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="G$1" pin="!ISP" pad="13"/>
<connect gate="G$1" pin="!TST" pad="30"/>
<connect gate="G$1" pin="AIN0" pad="49"/>
<connect gate="G$1" pin="AIN1" pad="50"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="AREFN" pad="48"/>
<connect gate="G$1" pin="AREFP" pad="47"/>
<connect gate="G$1" pin="AVDD" pad="45"/>
<connect gate="G$1" pin="AVSS" pad="46"/>
<connect gate="G$1" pin="D+" pad="33"/>
<connect gate="G$1" pin="D-" pad="34"/>
<connect gate="G$1" pin="DCLK" pad="57"/>
<connect gate="G$1" pin="DESL" pad="58"/>
<connect gate="G$1" pin="DOUT" pad="56"/>
<connect gate="G$1" pin="FILT" pad="24"/>
<connect gate="G$1" pin="MCLK" pad="63"/>
<connect gate="G$1" pin="MCMD" pad="61"/>
<connect gate="G$1" pin="MDAT" pad="62"/>
<connect gate="G$1" pin="P0.0/AD0" pad="8"/>
<connect gate="G$1" pin="P0.1/AD1" pad="7"/>
<connect gate="G$1" pin="P0.2/AD2" pad="6"/>
<connect gate="G$1" pin="P0.3/AD3" pad="5"/>
<connect gate="G$1" pin="P0.4/AD4" pad="4"/>
<connect gate="G$1" pin="P0.5/AD5" pad="3"/>
<connect gate="G$1" pin="P0.6/AD6" pad="84"/>
<connect gate="G$1" pin="P0.7/AD7" pad="83"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="14"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="15"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="16"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="17"/>
<connect gate="G$1" pin="P1.4" pad="18"/>
<connect gate="G$1" pin="P1.5" pad="19"/>
<connect gate="G$1" pin="P1.6/SCL" pad="20"/>
<connect gate="G$1" pin="P1.7/SDA" pad="21"/>
<connect gate="G$1" pin="P2.0/A8" pad="78"/>
<connect gate="G$1" pin="P2.1/A9" pad="77"/>
<connect gate="G$1" pin="P2.2/A10" pad="71"/>
<connect gate="G$1" pin="P2.3/A11" pad="70"/>
<connect gate="G$1" pin="P2.4/A12" pad="69"/>
<connect gate="G$1" pin="P2.5/A13" pad="68"/>
<connect gate="G$1" pin="P2.6/A14" pad="67"/>
<connect gate="G$1" pin="P2.7/A15" pad="66"/>
<connect gate="G$1" pin="P3.0/RXD" pad="37"/>
<connect gate="G$1" pin="P3.1/TXD" pad="38"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="39"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="40"/>
<connect gate="G$1" pin="P3.4/T0" pad="41"/>
<connect gate="G$1" pin="P3.5/T1" pad="42"/>
<connect gate="G$1" pin="P3.6/!WR" pad="43"/>
<connect gate="G$1" pin="P3.7/!RD" pad="44"/>
<connect gate="G$1" pin="P4.0/MISO" pad="79"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="80"/>
<connect gate="G$1" pin="P4.2/SCK" pad="81"/>
<connect gate="G$1" pin="P4.3/!SS" pad="82"/>
<connect gate="G$1" pin="P4.4" pad="72"/>
<connect gate="G$1" pin="P4.5" pad="73"/>
<connect gate="G$1" pin="P4.6" pad="75"/>
<connect gate="G$1" pin="P4.7" pad="76"/>
<connect gate="G$1" pin="P5.0" pad="9"/>
<connect gate="G$1" pin="P5.1" pad="10"/>
<connect gate="G$1" pin="P5.2" pad="51"/>
<connect gate="G$1" pin="P5.3" pad="52"/>
<connect gate="G$1" pin="RST" pad="60"/>
<connect gate="G$1" pin="SCLK" pad="59"/>
<connect gate="G$1" pin="X1" pad="29"/>
<connect gate="G$1" pin="X2" pad="27"/>
<connect gate="P" pin="PVDD" pad="23"/>
<connect gate="P" pin="PVSS" pad="25"/>
<connect gate="P" pin="UVDD" pad="31"/>
<connect gate="P" pin="UVSS" pad="32"/>
<connect gate="P" pin="VDD@1" pad="1"/>
<connect gate="P" pin="VDD@2" pad="22"/>
<connect gate="P" pin="VDD@3" pad="35"/>
<connect gate="P" pin="VDD@4" pad="54"/>
<connect gate="P" pin="VDD@5" pad="64"/>
<connect gate="P" pin="VSS@1" pad="2"/>
<connect gate="P" pin="VSS@2" pad="26"/>
<connect gate="P" pin="VSS@3" pad="36"/>
<connect gate="P" pin="VSS@4" pad="55"/>
<connect gate="P" pin="VSS@5" pad="65"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1095728"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-RO" package="TQFP80">
<connects>
<connect gate="G$1" pin="!ISP" pad="2"/>
<connect gate="G$1" pin="!TST" pad="18"/>
<connect gate="G$1" pin="AIN0" pad="37"/>
<connect gate="G$1" pin="AIN1" pad="38"/>
<connect gate="G$1" pin="ALE" pad="1"/>
<connect gate="G$1" pin="AREFN" pad="36"/>
<connect gate="G$1" pin="AREFP" pad="35"/>
<connect gate="G$1" pin="AVDD" pad="33"/>
<connect gate="G$1" pin="AVSS" pad="34"/>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="22"/>
<connect gate="G$1" pin="DCLK" pad="44"/>
<connect gate="G$1" pin="DESL" pad="45"/>
<connect gate="G$1" pin="DOUT" pad="43"/>
<connect gate="G$1" pin="FILT" pad="13"/>
<connect gate="G$1" pin="MCLK" pad="50"/>
<connect gate="G$1" pin="MCMD" pad="48"/>
<connect gate="G$1" pin="MDAT" pad="49"/>
<connect gate="G$1" pin="P0.0/AD0" pad="78"/>
<connect gate="G$1" pin="P0.1/AD1" pad="77"/>
<connect gate="G$1" pin="P0.2/AD2" pad="76"/>
<connect gate="G$1" pin="P0.3/AD3" pad="75"/>
<connect gate="G$1" pin="P0.4/AD4" pad="74"/>
<connect gate="G$1" pin="P0.5/AD5" pad="73"/>
<connect gate="G$1" pin="P0.6/AD6" pad="70"/>
<connect gate="G$1" pin="P0.7/AD7" pad="69"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="3"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="4"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="5"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="6"/>
<connect gate="G$1" pin="P1.4" pad="7"/>
<connect gate="G$1" pin="P1.5" pad="8"/>
<connect gate="G$1" pin="P1.6/SCL" pad="9"/>
<connect gate="G$1" pin="P1.7/SDA" pad="10"/>
<connect gate="G$1" pin="P2.0/A8" pad="64"/>
<connect gate="G$1" pin="P2.1/A9" pad="63"/>
<connect gate="G$1" pin="P2.2/A10" pad="58"/>
<connect gate="G$1" pin="P2.3/A11" pad="57"/>
<connect gate="G$1" pin="P2.4/A12" pad="56"/>
<connect gate="G$1" pin="P2.5/A13" pad="55"/>
<connect gate="G$1" pin="P2.6/A14" pad="54"/>
<connect gate="G$1" pin="P2.7/A15" pad="53"/>
<connect gate="G$1" pin="P3.0/RXD" pad="25"/>
<connect gate="G$1" pin="P3.1/TXD" pad="26"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="27"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="28"/>
<connect gate="G$1" pin="P3.4/T0" pad="29"/>
<connect gate="G$1" pin="P3.5/T1" pad="30"/>
<connect gate="G$1" pin="P3.6/!WR" pad="31"/>
<connect gate="G$1" pin="P3.7/!RD" pad="32"/>
<connect gate="G$1" pin="P4.0/MISO" pad="65"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="66"/>
<connect gate="G$1" pin="P4.2/SCK" pad="67"/>
<connect gate="G$1" pin="P4.3/!SS" pad="68"/>
<connect gate="G$1" pin="P4.4" pad="59"/>
<connect gate="G$1" pin="P4.5" pad="60"/>
<connect gate="G$1" pin="P4.6" pad="61"/>
<connect gate="G$1" pin="P4.7" pad="62"/>
<connect gate="G$1" pin="P5.0" pad="79"/>
<connect gate="G$1" pin="P5.1" pad="80"/>
<connect gate="G$1" pin="P5.2" pad="39"/>
<connect gate="G$1" pin="P5.3" pad="40"/>
<connect gate="G$1" pin="RST" pad="47"/>
<connect gate="G$1" pin="SCLK" pad="46"/>
<connect gate="G$1" pin="X1" pad="17"/>
<connect gate="G$1" pin="X2" pad="16"/>
<connect gate="P" pin="PVDD" pad="51"/>
<connect gate="P" pin="PVSS" pad="14"/>
<connect gate="P" pin="UVDD" pad="19"/>
<connect gate="P" pin="UVSS" pad="20"/>
<connect gate="P" pin="VDD@1" pad="11"/>
<connect gate="P" pin="VDD@2" pad="12"/>
<connect gate="P" pin="VDD@3" pad="23"/>
<connect gate="P" pin="VDD@4" pad="41"/>
<connect gate="P" pin="VDD@5" pad="71"/>
<connect gate="P" pin="VSS@1" pad="15"/>
<connect gate="P" pin="VSS@2" pad="24"/>
<connect gate="P" pin="VSS@3" pad="42"/>
<connect gate="P" pin="VSS@4" pad="52"/>
<connect gate="P" pin="VSS@5" pad="72"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1095728"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-7H" package="BGA81">
<connects>
<connect gate="G$1" pin="!ISP" pad="B2"/>
<connect gate="G$1" pin="!TST" pad="G2"/>
<connect gate="G$1" pin="AIN0" pad="H5"/>
<connect gate="G$1" pin="AIN1" pad="H7"/>
<connect gate="G$1" pin="ALE" pad="A1"/>
<connect gate="G$1" pin="AREFN" pad="J6"/>
<connect gate="G$1" pin="AREFP" pad="J7"/>
<connect gate="G$1" pin="AVDD" pad="F5"/>
<connect gate="G$1" pin="AVSS" pad="H6"/>
<connect gate="G$1" pin="D+" pad="J1"/>
<connect gate="G$1" pin="D-" pad="H2"/>
<connect gate="G$1" pin="DCLK" pad="H9"/>
<connect gate="G$1" pin="DESL" pad="G9"/>
<connect gate="G$1" pin="DOUT" pad="G7"/>
<connect gate="G$1" pin="FILT" pad="E4"/>
<connect gate="G$1" pin="MCLK" pad="F7"/>
<connect gate="G$1" pin="MCMD" pad="F8"/>
<connect gate="G$1" pin="MDAT" pad="F6"/>
<connect gate="G$1" pin="P0.0/AD0" pad="B3"/>
<connect gate="G$1" pin="P0.1/AD1" pad="B5"/>
<connect gate="G$1" pin="P0.2/AD2" pad="A4"/>
<connect gate="G$1" pin="P0.3/AD3" pad="A3"/>
<connect gate="G$1" pin="P0.4/AD4" pad="B4"/>
<connect gate="G$1" pin="P0.5/AD5" pad="D5"/>
<connect gate="G$1" pin="P0.6/AD6" pad="C6"/>
<connect gate="G$1" pin="P0.7/AD7" pad="D6"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="C3"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="B1"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="C1"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="C2"/>
<connect gate="G$1" pin="P1.4" pad="D1"/>
<connect gate="G$1" pin="P1.5" pad="D2"/>
<connect gate="G$1" pin="P1.6/SCL" pad="D4"/>
<connect gate="G$1" pin="P1.7/SDA" pad="D3"/>
<connect gate="G$1" pin="P2.0/A8" pad="A8"/>
<connect gate="G$1" pin="P2.1/A9" pad="C7"/>
<connect gate="G$1" pin="P2.2/A10" pad="C8"/>
<connect gate="G$1" pin="P2.3/A11" pad="E8"/>
<connect gate="G$1" pin="P2.4/A12" pad="D9"/>
<connect gate="G$1" pin="P2.5/A13" pad="C9"/>
<connect gate="G$1" pin="P2.6/A14" pad="D8"/>
<connect gate="G$1" pin="P2.7/A15" pad="E6"/>
<connect gate="G$1" pin="P3.0/RXD" pad="J3"/>
<connect gate="G$1" pin="P3.1/TXD" pad="H3"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="J4"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="H4"/>
<connect gate="G$1" pin="P3.4/T0" pad="F4"/>
<connect gate="G$1" pin="P3.5/T1" pad="G4"/>
<connect gate="G$1" pin="P3.6/!WR" pad="J5"/>
<connect gate="G$1" pin="P3.7/!RD" pad="G5"/>
<connect gate="G$1" pin="P4.0/MISO" pad="A7"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="B7"/>
<connect gate="G$1" pin="P4.2/SCK" pad="A6"/>
<connect gate="G$1" pin="P4.3/!SS" pad="B6"/>
<connect gate="G$1" pin="P4.4" pad="B9"/>
<connect gate="G$1" pin="P4.5" pad="D7"/>
<connect gate="G$1" pin="P4.6" pad="A9"/>
<connect gate="G$1" pin="P4.7" pad="B8"/>
<connect gate="G$1" pin="P5.0" pad="A2"/>
<connect gate="G$1" pin="P5.1" pad="C4"/>
<connect gate="G$1" pin="P5.2" pad="J8"/>
<connect gate="G$1" pin="P5.3" pad="G6"/>
<connect gate="G$1" pin="RST" pad="F9"/>
<connect gate="G$1" pin="SCLK" pad="G8"/>
<connect gate="G$1" pin="X1" pad="E2"/>
<connect gate="G$1" pin="X2" pad="F1"/>
<connect gate="P" pin="PVDD" pad="E3"/>
<connect gate="P" pin="PVSS" pad="F2"/>
<connect gate="P" pin="UVDD" pad="H1"/>
<connect gate="P" pin="UVSS" pad="F3"/>
<connect gate="P" pin="VDD@1" pad="A5"/>
<connect gate="P" pin="VDD@2" pad="E1"/>
<connect gate="P" pin="VDD@3" pad="E9"/>
<connect gate="P" pin="VDD@4" pad="G3"/>
<connect gate="P" pin="VDD@5" pad="J9"/>
<connect gate="P" pin="VSS@1" pad="C5"/>
<connect gate="P" pin="VSS@2" pad="E7"/>
<connect gate="P" pin="VSS@3" pad="G1"/>
<connect gate="P" pin="VSS@4" pad="H8"/>
<connect gate="P" pin="VSS@5" pad="J2"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C51-*" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 4K Bytes Flash&lt;/b&gt;&lt;p&gt;
&lt;font color="red"&gt;Not Recommended for New Designs. Use AT89S51.&lt;/font&gt;&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc0265.</description>
<gates>
<gate name="G$1" symbol="AT89C51"/>
</gates>
<devices>
<device name="PC" package="DIL40">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="31"/>
<connect gate="G$1" pin="!PSEN" pad="29"/>
<connect gate="G$1" pin="ALE/!PROG" pad="30"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="P0.0_AD0" pad="39"/>
<connect gate="G$1" pin="P0.1_AD1" pad="38"/>
<connect gate="G$1" pin="P0.2_AD2" pad="37"/>
<connect gate="G$1" pin="P0.3_AD3" pad="36"/>
<connect gate="G$1" pin="P0.4_AD4" pad="35"/>
<connect gate="G$1" pin="P0.5_AD5" pad="34"/>
<connect gate="G$1" pin="P0.6_AD6" pad="33"/>
<connect gate="G$1" pin="P0.7_AD7" pad="32"/>
<connect gate="G$1" pin="P1.0" pad="1"/>
<connect gate="G$1" pin="P1.1" pad="2"/>
<connect gate="G$1" pin="P1.2" pad="3"/>
<connect gate="G$1" pin="P1.3" pad="4"/>
<connect gate="G$1" pin="P1.4" pad="5"/>
<connect gate="G$1" pin="P1.5" pad="6"/>
<connect gate="G$1" pin="P1.6" pad="7"/>
<connect gate="G$1" pin="P1.7" pad="8"/>
<connect gate="G$1" pin="P2.0_A8" pad="21"/>
<connect gate="G$1" pin="P2.1_A9" pad="22"/>
<connect gate="G$1" pin="P2.2_A10" pad="23"/>
<connect gate="G$1" pin="P2.3_A11" pad="24"/>
<connect gate="G$1" pin="P2.4_A12" pad="25"/>
<connect gate="G$1" pin="P2.5_A13" pad="26"/>
<connect gate="G$1" pin="P2.6_A14" pad="27"/>
<connect gate="G$1" pin="P2.7_A15" pad="28"/>
<connect gate="G$1" pin="P3.0/RXD" pad="10"/>
<connect gate="G$1" pin="P3.1/TXD" pad="11"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="12"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="13"/>
<connect gate="G$1" pin="P3.4/T0" pad="14"/>
<connect gate="G$1" pin="P3.5/T1" pad="15"/>
<connect gate="G$1" pin="P3.6/!WR" pad="16"/>
<connect gate="G$1" pin="P3.7/!RD" pad="17"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="16">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="20">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="JC" package="PLCC44">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="32"/>
<connect gate="G$1" pin="ALE/!PROG" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="P0.0_AD0" pad="43"/>
<connect gate="G$1" pin="P0.1_AD1" pad="42"/>
<connect gate="G$1" pin="P0.2_AD2" pad="41"/>
<connect gate="G$1" pin="P0.3_AD3" pad="40"/>
<connect gate="G$1" pin="P0.4_AD4" pad="39"/>
<connect gate="G$1" pin="P0.5_AD5" pad="38"/>
<connect gate="G$1" pin="P0.6_AD6" pad="37"/>
<connect gate="G$1" pin="P0.7_AD7" pad="36"/>
<connect gate="G$1" pin="P1.0" pad="2"/>
<connect gate="G$1" pin="P1.1" pad="3"/>
<connect gate="G$1" pin="P1.2" pad="4"/>
<connect gate="G$1" pin="P1.3" pad="5"/>
<connect gate="G$1" pin="P1.4" pad="6"/>
<connect gate="G$1" pin="P1.5" pad="7"/>
<connect gate="G$1" pin="P1.6" pad="8"/>
<connect gate="G$1" pin="P1.7" pad="9"/>
<connect gate="G$1" pin="P2.0_A8" pad="24"/>
<connect gate="G$1" pin="P2.1_A9" pad="25"/>
<connect gate="G$1" pin="P2.2_A10" pad="26"/>
<connect gate="G$1" pin="P2.3_A11" pad="27"/>
<connect gate="G$1" pin="P2.4_A12" pad="28"/>
<connect gate="G$1" pin="P2.5_A13" pad="29"/>
<connect gate="G$1" pin="P2.6_A14" pad="30"/>
<connect gate="G$1" pin="P2.7_A15" pad="31"/>
<connect gate="G$1" pin="P3.0/RXD" pad="11"/>
<connect gate="G$1" pin="P3.1/TXD" pad="13"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="14"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="15"/>
<connect gate="G$1" pin="P3.4/T0" pad="16"/>
<connect gate="G$1" pin="P3.5/T1" pad="17"/>
<connect gate="G$1" pin="P3.6/!WR" pad="18"/>
<connect gate="G$1" pin="P3.7/!RD" pad="19"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51ED2-SLSUM"/>
<attribute name="OC_FARNELL" value="1095722"/>
<attribute name="OC_NEWARK" value="78K5790"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51ED2-SLSUM"/>
<attribute name="OC_FARNELL" value="1095722"/>
<attribute name="OC_NEWARK" value="78K5790"/>
</technology>
<technology name="16">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51RE2-SLSUM"/>
<attribute name="OC_FARNELL" value="1455062"/>
<attribute name="OC_NEWARK" value="58M3857"/>
</technology>
<technology name="20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51ED2-RLTUM"/>
<attribute name="OC_FARNELL" value="1095726"/>
<attribute name="OC_NEWARK" value="51P1802"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51ED2-SLSUM"/>
<attribute name="OC_FARNELL" value="1095722"/>
<attribute name="OC_NEWARK" value="78K5790"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C51?*" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 4K Bytes Flash&lt;/b&gt;&lt;p&gt;
&lt;font color="red"&gt;Not Recommended for New Designs. Use AT89S51.&lt;/font&gt;&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc0265.</description>
<gates>
<gate name="G$1" symbol="AT89C51"/>
<gate name="P" symbol="GND"/>
</gates>
<devices>
<device name="AC" package="TQFP44">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE/!PROG" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="P0.0_AD0" pad="37"/>
<connect gate="G$1" pin="P0.1_AD1" pad="36"/>
<connect gate="G$1" pin="P0.2_AD2" pad="35"/>
<connect gate="G$1" pin="P0.3_AD3" pad="34"/>
<connect gate="G$1" pin="P0.4_AD4" pad="33"/>
<connect gate="G$1" pin="P0.5_AD5" pad="32"/>
<connect gate="G$1" pin="P0.6_AD6" pad="31"/>
<connect gate="G$1" pin="P0.7_AD7" pad="30"/>
<connect gate="G$1" pin="P1.0" pad="40"/>
<connect gate="G$1" pin="P1.1" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5" pad="1"/>
<connect gate="G$1" pin="P1.6" pad="2"/>
<connect gate="G$1" pin="P1.7" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0/RXD" pad="5"/>
<connect gate="G$1" pin="P3.1/TXD" pad="7"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="8"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/!WR" pad="12"/>
<connect gate="G$1" pin="P3.7/!RD" pad="13"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="17"/>
</connects>
<technologies>
<technology name="-12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-16">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="QC" package="PQFP44">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE/!PROG" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="P0.0_AD0" pad="37"/>
<connect gate="G$1" pin="P0.1_AD1" pad="36"/>
<connect gate="G$1" pin="P0.2_AD2" pad="35"/>
<connect gate="G$1" pin="P0.3_AD3" pad="34"/>
<connect gate="G$1" pin="P0.4_AD4" pad="33"/>
<connect gate="G$1" pin="P0.5_AD5" pad="32"/>
<connect gate="G$1" pin="P0.6_AD6" pad="31"/>
<connect gate="G$1" pin="P0.7_AD7" pad="30"/>
<connect gate="G$1" pin="P1.0" pad="40"/>
<connect gate="G$1" pin="P1.1" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5" pad="1"/>
<connect gate="G$1" pin="P1.6" pad="2"/>
<connect gate="G$1" pin="P1.7" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0/RXD" pad="5"/>
<connect gate="G$1" pin="P3.1/TXD" pad="7"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="8"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/!WR" pad="12"/>
<connect gate="G$1" pin="P3.7/!RD" pad="13"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="17"/>
</connects>
<technologies>
<technology name="-12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-16">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89S51-*" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 4K BytesIn-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2487.pdf</description>
<gates>
<gate name="P" symbol="AT89S51"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="P" pin="!EA!/VPP" pad="31"/>
<connect gate="P" pin="!PSEN" pad="29"/>
<connect gate="P" pin="ALE/!PROG" pad="30"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="P0.0_AD0" pad="39"/>
<connect gate="P" pin="P0.1_AD1" pad="38"/>
<connect gate="P" pin="P0.2_AD2" pad="37"/>
<connect gate="P" pin="P0.3_AD3" pad="36"/>
<connect gate="P" pin="P0.4_AD4" pad="35"/>
<connect gate="P" pin="P0.5_AD5" pad="34"/>
<connect gate="P" pin="P0.6_AD6" pad="33"/>
<connect gate="P" pin="P0.7_AD7" pad="32"/>
<connect gate="P" pin="P1.0" pad="1"/>
<connect gate="P" pin="P1.1" pad="2"/>
<connect gate="P" pin="P1.2" pad="3"/>
<connect gate="P" pin="P1.3" pad="4"/>
<connect gate="P" pin="P1.4" pad="5"/>
<connect gate="P" pin="P1.5_MOSI" pad="6"/>
<connect gate="P" pin="P1.6_MISO" pad="7"/>
<connect gate="P" pin="P1.7_SCK" pad="8"/>
<connect gate="P" pin="P2.0_A8" pad="21"/>
<connect gate="P" pin="P2.1_A9" pad="22"/>
<connect gate="P" pin="P2.2_A10" pad="23"/>
<connect gate="P" pin="P2.3_A11" pad="24"/>
<connect gate="P" pin="P2.4_A12" pad="25"/>
<connect gate="P" pin="P2.5_A13" pad="26"/>
<connect gate="P" pin="P2.6_A14" pad="27"/>
<connect gate="P" pin="P2.7_A15" pad="28"/>
<connect gate="P" pin="P3.0/RXD" pad="10"/>
<connect gate="P" pin="P3.1/TXD" pad="11"/>
<connect gate="P" pin="P3.2/!INT0" pad="12"/>
<connect gate="P" pin="P3.3/!INT1" pad="13"/>
<connect gate="P" pin="P3.4/T0" pad="14"/>
<connect gate="P" pin="P3.5/T1" pad="15"/>
<connect gate="P" pin="P3.6/!WR" pad="16"/>
<connect gate="P" pin="P3.7/!RD" pad="17"/>
<connect gate="P" pin="RST" pad="9"/>
<connect gate="P" pin="VCC" pad="40"/>
<connect gate="P" pin="XTAL1" pad="19"/>
<connect gate="P" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89S51-24PU"/>
<attribute name="OC_FARNELL" value="1095739"/>
<attribute name="OC_NEWARK" value="96K6578"/>
</technology>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89S51-24PU"/>
<attribute name="OC_FARNELL" value="1095739"/>
<attribute name="OC_NEWARK" value="96K6578"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="P" pin="!EA!/VPP" pad="35"/>
<connect gate="P" pin="!PSEN" pad="32"/>
<connect gate="P" pin="ALE/!PROG" pad="33"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="P0.0_AD0" pad="43"/>
<connect gate="P" pin="P0.1_AD1" pad="42"/>
<connect gate="P" pin="P0.2_AD2" pad="41"/>
<connect gate="P" pin="P0.3_AD3" pad="40"/>
<connect gate="P" pin="P0.4_AD4" pad="39"/>
<connect gate="P" pin="P0.5_AD5" pad="38"/>
<connect gate="P" pin="P0.6_AD6" pad="37"/>
<connect gate="P" pin="P0.7_AD7" pad="36"/>
<connect gate="P" pin="P1.0" pad="2"/>
<connect gate="P" pin="P1.1" pad="3"/>
<connect gate="P" pin="P1.2" pad="4"/>
<connect gate="P" pin="P1.3" pad="5"/>
<connect gate="P" pin="P1.4" pad="6"/>
<connect gate="P" pin="P1.5_MOSI" pad="7"/>
<connect gate="P" pin="P1.6_MISO" pad="8"/>
<connect gate="P" pin="P1.7_SCK" pad="9"/>
<connect gate="P" pin="P2.0_A8" pad="24"/>
<connect gate="P" pin="P2.1_A9" pad="25"/>
<connect gate="P" pin="P2.2_A10" pad="26"/>
<connect gate="P" pin="P2.3_A11" pad="27"/>
<connect gate="P" pin="P2.4_A12" pad="28"/>
<connect gate="P" pin="P2.5_A13" pad="29"/>
<connect gate="P" pin="P2.6_A14" pad="30"/>
<connect gate="P" pin="P2.7_A15" pad="31"/>
<connect gate="P" pin="P3.0/RXD" pad="11"/>
<connect gate="P" pin="P3.1/TXD" pad="13"/>
<connect gate="P" pin="P3.2/!INT0" pad="14"/>
<connect gate="P" pin="P3.3/!INT1" pad="15"/>
<connect gate="P" pin="P3.4/T0" pad="16"/>
<connect gate="P" pin="P3.5/T1" pad="17"/>
<connect gate="P" pin="P3.6/!WR" pad="18"/>
<connect gate="P" pin="P3.7/!RD" pad="19"/>
<connect gate="P" pin="RST" pad="10"/>
<connect gate="P" pin="VCC" pad="44"/>
<connect gate="P" pin="XTAL1" pad="21"/>
<connect gate="P" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89S51-24JU"/>
<attribute name="OC_FARNELL" value="1095738"/>
<attribute name="OC_NEWARK" value="96K6577"/>
</technology>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1095738"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="S44">
<connects>
<connect gate="P" pin="!EA!/VPP" pad="35"/>
<connect gate="P" pin="!PSEN" pad="32"/>
<connect gate="P" pin="ALE/!PROG" pad="33"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="P0.0_AD0" pad="43"/>
<connect gate="P" pin="P0.1_AD1" pad="42"/>
<connect gate="P" pin="P0.2_AD2" pad="41"/>
<connect gate="P" pin="P0.3_AD3" pad="40"/>
<connect gate="P" pin="P0.4_AD4" pad="39"/>
<connect gate="P" pin="P0.5_AD5" pad="38"/>
<connect gate="P" pin="P0.6_AD6" pad="37"/>
<connect gate="P" pin="P0.7_AD7" pad="36"/>
<connect gate="P" pin="P1.0" pad="2"/>
<connect gate="P" pin="P1.1" pad="3"/>
<connect gate="P" pin="P1.2" pad="4"/>
<connect gate="P" pin="P1.3" pad="5"/>
<connect gate="P" pin="P1.4" pad="6"/>
<connect gate="P" pin="P1.5_MOSI" pad="7"/>
<connect gate="P" pin="P1.6_MISO" pad="8"/>
<connect gate="P" pin="P1.7_SCK" pad="9"/>
<connect gate="P" pin="P2.0_A8" pad="24"/>
<connect gate="P" pin="P2.1_A9" pad="25"/>
<connect gate="P" pin="P2.2_A10" pad="26"/>
<connect gate="P" pin="P2.3_A11" pad="27"/>
<connect gate="P" pin="P2.4_A12" pad="28"/>
<connect gate="P" pin="P2.5_A13" pad="29"/>
<connect gate="P" pin="P2.6_A14" pad="30"/>
<connect gate="P" pin="P2.7_A15" pad="31"/>
<connect gate="P" pin="P3.0/RXD" pad="11"/>
<connect gate="P" pin="P3.1/TXD" pad="13"/>
<connect gate="P" pin="P3.2/!INT0" pad="14"/>
<connect gate="P" pin="P3.3/!INT1" pad="15"/>
<connect gate="P" pin="P3.4/T0" pad="16"/>
<connect gate="P" pin="P3.5/T1" pad="17"/>
<connect gate="P" pin="P3.6/!WR" pad="18"/>
<connect gate="P" pin="P3.7/!RD" pad="19"/>
<connect gate="P" pin="RST" pad="10"/>
<connect gate="P" pin="VCC" pad="44"/>
<connect gate="P" pin="XTAL1" pad="21"/>
<connect gate="P" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89S51*P" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 4K BytesIn-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2487.pdf</description>
<gates>
<gate name="G$1" symbol="AT89S51"/>
<gate name="P" symbol="GND"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE/!PROG" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="P0.0_AD0" pad="37"/>
<connect gate="G$1" pin="P0.1_AD1" pad="36"/>
<connect gate="G$1" pin="P0.2_AD2" pad="35"/>
<connect gate="G$1" pin="P0.3_AD3" pad="34"/>
<connect gate="G$1" pin="P0.4_AD4" pad="33"/>
<connect gate="G$1" pin="P0.5_AD5" pad="32"/>
<connect gate="G$1" pin="P0.6_AD6" pad="31"/>
<connect gate="G$1" pin="P0.7_AD7" pad="30"/>
<connect gate="G$1" pin="P1.0" pad="40"/>
<connect gate="G$1" pin="P1.1" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5_MOSI" pad="1"/>
<connect gate="G$1" pin="P1.6_MISO" pad="2"/>
<connect gate="G$1" pin="P1.7_SCK" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0/RXD" pad="5"/>
<connect gate="G$1" pin="P3.1/TXD" pad="7"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="8"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/!WR" pad="12"/>
<connect gate="G$1" pin="P3.7/!RD" pad="13"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="17"/>
</connects>
<technologies>
<technology name="-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-33">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T89C51CC02*-?IM" prefix="IC">
<description>&lt;b&gt;Enhanced 8-bit Microcontroller with CAN Controller and Flash&lt;/b&gt; 80C51 Core Architecture&lt;p&gt; 
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.</description>
<gates>
<gate name="G$1" symbol="T89C51CC02"/>
</gates>
<devices>
<device name="TIS" package="SO28W">
<connects>
<connect gate="G$1" pin="P1.0/AN0/T2" pad="28"/>
<connect gate="G$1" pin="P1.1/AN1/T2EX" pad="27"/>
<connect gate="G$1" pin="P1.2/AN2/ECI" pad="26"/>
<connect gate="G$1" pin="P1.3/AN3/CEX0" pad="25"/>
<connect gate="G$1" pin="P1.4/AN4/CEX1" pad="24"/>
<connect gate="G$1" pin="P1.5/AN5" pad="23"/>
<connect gate="G$1" pin="P1.6/AN6" pad="22"/>
<connect gate="G$1" pin="P1.7/AN7" pad="21"/>
<connect gate="G$1" pin="P2.0" pad="20"/>
<connect gate="G$1" pin="P2.1" pad="6"/>
<connect gate="G$1" pin="P3.0/RXD" pad="14"/>
<connect gate="G$1" pin="P3.1/TXD" pad="13"/>
<connect gate="G$1" pin="P3.2/!INT" pad="12"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="11"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="9"/>
<connect gate="G$1" pin="P3.6" pad="8"/>
<connect gate="G$1" pin="P3.7" pad="7"/>
<connect gate="G$1" pin="P4.0/RXDC" pad="5"/>
<connect gate="G$1" pin="P4.1/TXDC" pad="4"/>
<connect gate="G$1" pin="RST" pad="19"/>
<connect gate="G$1" pin="VAGND" pad="2"/>
<connect gate="G$1" pin="VAREF" pad="1"/>
<connect gate="G$1" pin="VAVCC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="17"/>
<connect gate="G$1" pin="VSS" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="16"/>
<connect gate="G$1" pin="XTAL2" pad="15"/>
</connects>
<technologies>
<technology name="CA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIL40/SOIC28ZIFAWM-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M9134"/>
</technology>
<technology name="UA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIL40/SOIC28ZIFAWM-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M9134"/>
</technology>
</technologies>
</device>
<device name="SIS" package="PLCC28">
<connects>
<connect gate="G$1" pin="P1.0/AN0/T2" pad="28"/>
<connect gate="G$1" pin="P1.1/AN1/T2EX" pad="27"/>
<connect gate="G$1" pin="P1.2/AN2/ECI" pad="26"/>
<connect gate="G$1" pin="P1.3/AN3/CEX0" pad="25"/>
<connect gate="G$1" pin="P1.4/AN4/CEX1" pad="24"/>
<connect gate="G$1" pin="P1.5/AN5" pad="23"/>
<connect gate="G$1" pin="P1.6/AN6" pad="22"/>
<connect gate="G$1" pin="P1.7/AN7" pad="21"/>
<connect gate="G$1" pin="P2.0" pad="20"/>
<connect gate="G$1" pin="P2.1" pad="6"/>
<connect gate="G$1" pin="P3.0/RXD" pad="14"/>
<connect gate="G$1" pin="P3.1/TXD" pad="13"/>
<connect gate="G$1" pin="P3.2/!INT" pad="12"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="11"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="9"/>
<connect gate="G$1" pin="P3.6" pad="8"/>
<connect gate="G$1" pin="P3.7" pad="7"/>
<connect gate="G$1" pin="P4.0/RXDC" pad="5"/>
<connect gate="G$1" pin="P4.1/TXDC" pad="4"/>
<connect gate="G$1" pin="RST" pad="19"/>
<connect gate="G$1" pin="VAGND" pad="2"/>
<connect gate="G$1" pin="VAREF" pad="1"/>
<connect gate="G$1" pin="VAVCC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="17"/>
<connect gate="G$1" pin="VSS" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="16"/>
<connect gate="G$1" pin="XTAL2" pad="15"/>
</connects>
<technologies>
<technology name="CA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIL40/PLCC28ZIFAWM-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M9105"/>
</technology>
<technology name="UA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIL40/PLCC28ZIFAWM-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M9105"/>
</technology>
</technologies>
</device>
<device name="RAT" package="VQFP32">
<connects>
<connect gate="G$1" pin="P1.0/AN0/T2" pad="27"/>
<connect gate="G$1" pin="P1.1/AN1/T2EX" pad="26"/>
<connect gate="G$1" pin="P1.2/AN2/ECI" pad="25"/>
<connect gate="G$1" pin="P1.3/AN3/CEX0" pad="24"/>
<connect gate="G$1" pin="P1.4/AN4/CEX1" pad="23"/>
<connect gate="G$1" pin="P1.5/AN5" pad="22"/>
<connect gate="G$1" pin="P1.6/AN6" pad="21"/>
<connect gate="G$1" pin="P1.7/AN7" pad="20"/>
<connect gate="G$1" pin="P2.0" pad="19"/>
<connect gate="G$1" pin="P2.1" pad="2"/>
<connect gate="G$1" pin="P3.0/RXD" pad="11"/>
<connect gate="G$1" pin="P3.1/TXD" pad="10"/>
<connect gate="G$1" pin="P3.2/!INT" pad="9"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="8"/>
<connect gate="G$1" pin="P3.4/T0" pad="6"/>
<connect gate="G$1" pin="P3.5/T1" pad="5"/>
<connect gate="G$1" pin="P3.6" pad="4"/>
<connect gate="G$1" pin="P3.7" pad="3"/>
<connect gate="G$1" pin="P4.0/RXDC" pad="1"/>
<connect gate="G$1" pin="P4.1/TXDC" pad="32"/>
<connect gate="G$1" pin="RST" pad="17"/>
<connect gate="G$1" pin="VAGND" pad="29"/>
<connect gate="G$1" pin="VAREF" pad="28"/>
<connect gate="G$1" pin="VAVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="CA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="UA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T89C51CC02*-TDSIM" prefix="IC">
<description>&lt;b&gt;Enhanced 8-bit Microcontroller with CAN Controller and Flash&lt;/b&gt; 80C51 Core Architecture&lt;p&gt; 
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.</description>
<gates>
<gate name="G$1" symbol="T89C51CC02-SO24"/>
</gates>
<devices>
<device name="" package="SO24W">
<connects>
<connect gate="G$1" pin="P1.0/AN0/T2" pad="24"/>
<connect gate="G$1" pin="P1.1/AN1/T2EX" pad="23"/>
<connect gate="G$1" pin="P1.2/AN2/ECI" pad="22"/>
<connect gate="G$1" pin="P1.3/AN3/CEX0" pad="21"/>
<connect gate="G$1" pin="P1.4/AN4/CEX1" pad="20"/>
<connect gate="G$1" pin="P1.5/AN5" pad="19"/>
<connect gate="G$1" pin="P1.6/AN6" pad="18"/>
<connect gate="G$1" pin="P1.7/AN7" pad="17"/>
<connect gate="G$1" pin="P3.0/RXD" pad="11"/>
<connect gate="G$1" pin="P3.1/TXD" pad="10"/>
<connect gate="G$1" pin="P3.2/!INT" pad="9"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="8"/>
<connect gate="G$1" pin="P3.4/T0" pad="7"/>
<connect gate="G$1" pin="P3.5/T1" pad="6"/>
<connect gate="G$1" pin="P4.0/RXDC" pad="5"/>
<connect gate="G$1" pin="P4.1/TXDC" pad="4"/>
<connect gate="G$1" pin="RST" pad="16"/>
<connect gate="G$1" pin="VAGND" pad="2"/>
<connect gate="G$1" pin="VAREF" pad="1"/>
<connect gate="G$1" pin="VAVCC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VSS" pad="15"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="CA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="UA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91RM9200" prefix="IC">
<description>Auto generated by &lt;b&gt;make-symbol-device-package(bsdl).ulp&lt;/b&gt;&lt;p&gt;
Source: at91rm9200_bga.bsd</description>
<gates>
<gate name="G$1" symbol="AT91RM9200_BGA"/>
</gates>
<devices>
<device name="" package="LFBGA256_A_291X326">
<connects>
<connect gate="G$1" pin="A10_SDRAM" pad="N6"/>
<connect gate="G$1" pin="A16_BA0" pad="U3"/>
<connect gate="G$1" pin="A17_BA1" pad="T3"/>
<connect gate="G$1" pin="A1_DQM2" pad="M4"/>
<connect gate="G$1" pin="A_10" pad="M5"/>
<connect gate="G$1" pin="A_11" pad="P5"/>
<connect gate="G$1" pin="A_12" pad="P3"/>
<connect gate="G$1" pin="A_13" pad="P2"/>
<connect gate="G$1" pin="A_14" pad="N5"/>
<connect gate="G$1" pin="A_15" pad="T1"/>
<connect gate="G$1" pin="A_18" pad="R3"/>
<connect gate="G$1" pin="A_19" pad="U4"/>
<connect gate="G$1" pin="A_2" pad="M6"/>
<connect gate="G$1" pin="A_20" pad="R4"/>
<connect gate="G$1" pin="A_21" pad="N8"/>
<connect gate="G$1" pin="A_22" pad="P6"/>
<connect gate="G$1" pin="A_3" pad="M3"/>
<connect gate="G$1" pin="A_4" pad="N4"/>
<connect gate="G$1" pin="A_5" pad="N2"/>
<connect gate="G$1" pin="A_6" pad="L4"/>
<connect gate="G$1" pin="A_7" pad="P1"/>
<connect gate="G$1" pin="A_8" pad="N7"/>
<connect gate="G$1" pin="A_9" pad="N3"/>
<connect gate="G$1" pin="CAS" pad="U8"/>
<connect gate="G$1" pin="DM" pad="K2"/>
<connect gate="G$1" pin="DP" pad="K5"/>
<connect gate="G$1" pin="D_0" pad="R9"/>
<connect gate="G$1" pin="D_1" pad="P10"/>
<connect gate="G$1" pin="D_10" pad="P12"/>
<connect gate="G$1" pin="D_11" pad="U12"/>
<connect gate="G$1" pin="D_12" pad="T12"/>
<connect gate="G$1" pin="D_13" pad="R12"/>
<connect gate="G$1" pin="D_14" pad="U13"/>
<connect gate="G$1" pin="D_15" pad="P13"/>
<connect gate="G$1" pin="D_2" pad="N11"/>
<connect gate="G$1" pin="D_3" pad="U9"/>
<connect gate="G$1" pin="D_4" pad="M11"/>
<connect gate="G$1" pin="D_5" pad="P11"/>
<connect gate="G$1" pin="D_6" pad="U10"/>
<connect gate="G$1" pin="D_7" pad="U11"/>
<connect gate="G$1" pin="D_8" pad="R11"/>
<connect gate="G$1" pin="D_9" pad="T11"/>
<connect gate="G$1" pin="HDMA" pad="K3"/>
<connect gate="G$1" pin="HDMB" pad="L3"/>
<connect gate="G$1" pin="HDPA" pad="K1"/>
<connect gate="G$1" pin="HDPB" pad="L2"/>
<connect gate="G$1" pin="ICETCK" pad="E5"/>
<connect gate="G$1" pin="ICETDI" pad="A1"/>
<connect gate="G$1" pin="ICETDO" pad="B1"/>
<connect gate="G$1" pin="ICETMS" pad="C1"/>
<connect gate="G$1" pin="JTAGSEL" pad="A2"/>
<connect gate="G$1" pin="MIX33VDD@1" pad="P16"/>
<connect gate="G$1" pin="MIX33VDD@10" pad="D5"/>
<connect gate="G$1" pin="MIX33VDD@11" pad="D2"/>
<connect gate="G$1" pin="MIX33VDD@12" pad="D3"/>
<connect gate="G$1" pin="MIX33VDD@13" pad="H5"/>
<connect gate="G$1" pin="MIX33VDD@14" pad="K4"/>
<connect gate="G$1" pin="MIX33VDD@15" pad="L6"/>
<connect gate="G$1" pin="MIX33VDD@16" pad="M1"/>
<connect gate="G$1" pin="MIX33VDD@17" pad="P4"/>
<connect gate="G$1" pin="MIX33VDD@18" pad="R6"/>
<connect gate="G$1" pin="MIX33VDD@19" pad="T5"/>
<connect gate="G$1" pin="MIX33VDD@2" pad="R17"/>
<connect gate="G$1" pin="MIX33VDD@20" pad="R10"/>
<connect gate="G$1" pin="MIX33VDD@21" pad="R14"/>
<connect gate="G$1" pin="MIX33VDD@3" pad="K16"/>
<connect gate="G$1" pin="MIX33VDD@4" pad="H14"/>
<connect gate="G$1" pin="MIX33VDD@5" pad="A16"/>
<connect gate="G$1" pin="MIX33VDD@6" pad="A11"/>
<connect gate="G$1" pin="MIX33VDD@7" pad="B11"/>
<connect gate="G$1" pin="MIX33VDD@8" pad="D8"/>
<connect gate="G$1" pin="MIX33VDD@9" pad="A7"/>
<connect gate="G$1" pin="MIX33VSS@1" pad="M12"/>
<connect gate="G$1" pin="MIX33VSS@10" pad="E6"/>
<connect gate="G$1" pin="MIX33VSS@11" pad="D4"/>
<connect gate="G$1" pin="MIX33VSS@12" pad="E3"/>
<connect gate="G$1" pin="MIX33VSS@13" pad="G3"/>
<connect gate="G$1" pin="MIX33VSS@14" pad="L1"/>
<connect gate="G$1" pin="MIX33VSS@15" pad="L5"/>
<connect gate="G$1" pin="MIX33VSS@16" pad="M2"/>
<connect gate="G$1" pin="MIX33VSS@17" pad="R1"/>
<connect gate="G$1" pin="MIX33VSS@18" pad="M7"/>
<connect gate="G$1" pin="MIX33VSS@19" pad="U5"/>
<connect gate="G$1" pin="MIX33VSS@2" pad="P17"/>
<connect gate="G$1" pin="MIX33VSS@20" pad="T9"/>
<connect gate="G$1" pin="MIX33VSS@21" pad="T13"/>
<connect gate="G$1" pin="MIX33VSS@3" pad="J12"/>
<connect gate="G$1" pin="MIX33VSS@4" pad="H16"/>
<connect gate="G$1" pin="MIX33VSS@5" pad="C15"/>
<connect gate="G$1" pin="MIX33VSS@6" pad="C11"/>
<connect gate="G$1" pin="MIX33VSS@7" pad="D11"/>
<connect gate="G$1" pin="MIX33VSS@8" pad="B7"/>
<connect gate="G$1" pin="MIX33VSS@9" pad="E8"/>
<connect gate="G$1" pin="NBS3" pad="R8"/>
<connect gate="G$1" pin="NCS0_BFCS" pad="U6"/>
<connect gate="G$1" pin="NCS1_SDCS" pad="M9"/>
<connect gate="G$1" pin="NCS2" pad="T6"/>
<connect gate="G$1" pin="NCS3" pad="R7"/>
<connect gate="G$1" pin="NLBA0_DQM0" pad="N1"/>
<connect gate="G$1" pin="NRDNOE" pad="N9"/>
<connect gate="G$1" pin="NRST" pad="E1"/>
<connect gate="G$1" pin="NRW0NWE" pad="P8"/>
<connect gate="G$1" pin="NRW1_NUB_DQM1" pad="T7"/>
<connect gate="G$1" pin="NTRST" pad="E2"/>
<connect gate="G$1" pin="OSC32K_XIN" pad="G17"/>
<connect gate="G$1" pin="OSC32K_XOUT" pad="H17"/>
<connect gate="G$1" pin="OSC9M_XIN" pad="J17"/>
<connect gate="G$1" pin="OSC9M_XOUT" pad="K17"/>
<connect gate="G$1" pin="PA0" pad="G13"/>
<connect gate="G$1" pin="PA1" pad="G14"/>
<connect gate="G$1" pin="PA10" pad="D15"/>
<connect gate="G$1" pin="PA11" pad="B15"/>
<connect gate="G$1" pin="PA12" pad="B16"/>
<connect gate="G$1" pin="PA13" pad="A17"/>
<connect gate="G$1" pin="PA14" pad="A15"/>
<connect gate="G$1" pin="PA15" pad="B14"/>
<connect gate="G$1" pin="PA16" pad="D14"/>
<connect gate="G$1" pin="PA17" pad="B13"/>
<connect gate="G$1" pin="PA18" pad="C13"/>
<connect gate="G$1" pin="PA19" pad="A13"/>
<connect gate="G$1" pin="PA2" pad="G15"/>
<connect gate="G$1" pin="PA20" pad="C12"/>
<connect gate="G$1" pin="PA21" pad="D13"/>
<connect gate="G$1" pin="PA22" pad="D12"/>
<connect gate="G$1" pin="PA23" pad="A12"/>
<connect gate="G$1" pin="PA24" pad="B12"/>
<connect gate="G$1" pin="PA25" pad="E13"/>
<connect gate="G$1" pin="PA26" pad="E12"/>
<connect gate="G$1" pin="PA27" pad="G12"/>
<connect gate="G$1" pin="PA28" pad="F12"/>
<connect gate="G$1" pin="PA29" pad="E11"/>
<connect gate="G$1" pin="PA3" pad="G16"/>
<connect gate="G$1" pin="PA30" pad="F11"/>
<connect gate="G$1" pin="PA31" pad="A10"/>
<connect gate="G$1" pin="PA4" pad="F13"/>
<connect gate="G$1" pin="PA5" pad="F16"/>
<connect gate="G$1" pin="PA6" pad="E15"/>
<connect gate="G$1" pin="PA7" pad="B17"/>
<connect gate="G$1" pin="PA8" pad="C16"/>
<connect gate="G$1" pin="PA9" pad="E14"/>
<connect gate="G$1" pin="PB0" pad="B10"/>
<connect gate="G$1" pin="PB1" pad="C10"/>
<connect gate="G$1" pin="PB10" pad="B8"/>
<connect gate="G$1" pin="PB11" pad="F9"/>
<connect gate="G$1" pin="PB12" pad="C8"/>
<connect gate="G$1" pin="PB13" pad="C7"/>
<connect gate="G$1" pin="PB14" pad="D7"/>
<connect gate="G$1" pin="PB15" pad="E7"/>
<connect gate="G$1" pin="PB16" pad="F7"/>
<connect gate="G$1" pin="PB17" pad="A4"/>
<connect gate="G$1" pin="PB18" pad="B3"/>
<connect gate="G$1" pin="PB19" pad="C5"/>
<connect gate="G$1" pin="PB2" pad="D10"/>
<connect gate="G$1" pin="PB20" pad="A3"/>
<connect gate="G$1" pin="PB21" pad="B4"/>
<connect gate="G$1" pin="PB22" pad="C4"/>
<connect gate="G$1" pin="PB23" pad="F3"/>
<connect gate="G$1" pin="PB24" pad="F5"/>
<connect gate="G$1" pin="PB25" pad="F4"/>
<connect gate="G$1" pin="PB26" pad="G4"/>
<connect gate="G$1" pin="PB27" pad="G6"/>
<connect gate="G$1" pin="PB28" pad="J5"/>
<connect gate="G$1" pin="PB29" pad="J6"/>
<connect gate="G$1" pin="PB3" pad="E10"/>
<connect gate="G$1" pin="PB4" pad="A9"/>
<connect gate="G$1" pin="PB5" pad="B9"/>
<connect gate="G$1" pin="PB6" pad="C9"/>
<connect gate="G$1" pin="PB7" pad="E9"/>
<connect gate="G$1" pin="PB8" pad="D9"/>
<connect gate="G$1" pin="PB9" pad="A8"/>
<connect gate="G$1" pin="PC0" pad="M15"/>
<connect gate="G$1" pin="PC1" pad="M14"/>
<connect gate="G$1" pin="PC10" pad="L12"/>
<connect gate="G$1" pin="PC11" pad="N16"/>
<connect gate="G$1" pin="PC12" pad="N17"/>
<connect gate="G$1" pin="PC13" pad="M13"/>
<connect gate="G$1" pin="PC14" pad="M17"/>
<connect gate="G$1" pin="PC15" pad="L13"/>
<connect gate="G$1" pin="PC16" pad="U14"/>
<connect gate="G$1" pin="PC17" pad="R13"/>
<connect gate="G$1" pin="PC18" pad="U15"/>
<connect gate="G$1" pin="PC19" pad="T14"/>
<connect gate="G$1" pin="PC2" pad="L14"/>
<connect gate="G$1" pin="PC20" pad="U16"/>
<connect gate="G$1" pin="PC21" pad="T15"/>
<connect gate="G$1" pin="PC22" pad="U17"/>
<connect gate="G$1" pin="PC23" pad="T16"/>
<connect gate="G$1" pin="PC24" pad="R15"/>
<connect gate="G$1" pin="PC25" pad="T17"/>
<connect gate="G$1" pin="PC26" pad="P14"/>
<connect gate="G$1" pin="PC27" pad="P15"/>
<connect gate="G$1" pin="PC28" pad="N13"/>
<connect gate="G$1" pin="PC29" pad="R16"/>
<connect gate="G$1" pin="PC3" pad="L15"/>
<connect gate="G$1" pin="PC30" pad="N15"/>
<connect gate="G$1" pin="PC31" pad="N14"/>
<connect gate="G$1" pin="PC4" pad="K14"/>
<connect gate="G$1" pin="PC5" pad="K13"/>
<connect gate="G$1" pin="PC6" pad="K15"/>
<connect gate="G$1" pin="PC7" pad="T4"/>
<connect gate="G$1" pin="PC8" pad="R5"/>
<connect gate="G$1" pin="PC9" pad="P7"/>
<connect gate="G$1" pin="PD0" pad="E17"/>
<connect gate="G$1" pin="PD1" pad="F15"/>
<connect gate="G$1" pin="PD10" pad="C6"/>
<connect gate="G$1" pin="PD11" pad="A5"/>
<connect gate="G$1" pin="PD12" pad="B5"/>
<connect gate="G$1" pin="PD13" pad="B2"/>
<connect gate="G$1" pin="PD14" pad="C3"/>
<connect gate="G$1" pin="PD15" pad="C2"/>
<connect gate="G$1" pin="PD16" pad="F1"/>
<connect gate="G$1" pin="PD17" pad="G2"/>
<connect gate="G$1" pin="PD18" pad="G5"/>
<connect gate="G$1" pin="PD19" pad="G1"/>
<connect gate="G$1" pin="PD2" pad="F14"/>
<connect gate="G$1" pin="PD20" pad="H2"/>
<connect gate="G$1" pin="PD21" pad="H4"/>
<connect gate="G$1" pin="PD22" pad="H3"/>
<connect gate="G$1" pin="PD23" pad="H1"/>
<connect gate="G$1" pin="PD24" pad="J3"/>
<connect gate="G$1" pin="PD25" pad="J1"/>
<connect gate="G$1" pin="PD26" pad="J4"/>
<connect gate="G$1" pin="PD27" pad="J2"/>
<connect gate="G$1" pin="PD3" pad="E16"/>
<connect gate="G$1" pin="PD4" pad="D17"/>
<connect gate="G$1" pin="PD5" pad="C17"/>
<connect gate="G$1" pin="PD6" pad="D16"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PD8" pad="A6"/>
<connect gate="G$1" pin="PD9" pad="B6"/>
<connect gate="G$1" pin="PLL_A_RC" pad="L17"/>
<connect gate="G$1" pin="PLL_B_RC" pad="F17"/>
<connect gate="G$1" pin="RAS" pad="N10"/>
<connect gate="G$1" pin="SDRAMCKE" pad="P9"/>
<connect gate="G$1" pin="SDRAMCLK" pad="U7"/>
<connect gate="G$1" pin="TST0" pad="E4"/>
<connect gate="G$1" pin="TST1" pad="D1"/>
<connect gate="G$1" pin="VDDI@1" pad="L16"/>
<connect gate="G$1" pin="VDDI@2" pad="C14"/>
<connect gate="G$1" pin="VDDI@3" pad="F6"/>
<connect gate="G$1" pin="VDDI@4" pad="U1"/>
<connect gate="G$1" pin="VDDI@5" pad="T2"/>
<connect gate="G$1" pin="VDDI@6" pad="T10"/>
<connect gate="G$1" pin="VDDI@7" pad="J15"/>
<connect gate="G$1" pin="VDDI@8" pad="J14"/>
<connect gate="G$1" pin="VDDI@9" pad="H13"/>
<connect gate="G$1" pin="VSSI@1" pad="M16"/>
<connect gate="G$1" pin="VSSI@2" pad="A14"/>
<connect gate="G$1" pin="VSSI@3" pad="F2"/>
<connect gate="G$1" pin="VSSI@4" pad="U2"/>
<connect gate="G$1" pin="VSSI@5" pad="R2"/>
<connect gate="G$1" pin="VSSI@6" pad="N12"/>
<connect gate="G$1" pin="VSSI@7" pad="J16"/>
<connect gate="G$1" pin="VSSI@8" pad="J13"/>
<connect gate="G$1" pin="VSSI@9" pad="H15"/>
<connect gate="G$1" pin="WE" pad="T8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT91RM9200-EK"/>
<attribute name="OC_FARNELL" value="1629536"/>
<attribute name="OC_NEWARK" value="02P6234"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATF16V8B" prefix="IC">
<description>&lt;b&gt;High perfomance CMOS (electrically erasable) programmable logic device (PLD)&lt;/b&gt;&lt;p&gt;
ABLE-Atmel-ABEL - P18V8R, P16V8C, P16V8AS, P17V8&lt;br&gt;
COPL Atmel-WinCUPL - G16V8MS, G16V8MA, G16V8AS, G16V8&lt;br&gt;
LOG/IC - GAL16V8_R, GAL16V8_G7, GAL16V8_C), GAL16V8&lt;br&gt;
Tango-PLD - G16V8R, G16V8C, G16V8AS, G16V8&lt;br&gt;


Source: http://www.atmel.com/dyn/resources/prod_documents/DOC0364.PDF</description>
<gates>
<gate name="G$1" symbol="ATF16V8B"/>
</gates>
<devices>
<device name="X" package="TSSOP20">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="O1" pad="19"/>
<connect gate="G$1" pin="O2" pad="18"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="15"/>
<connect gate="G$1" pin="O6" pad="14"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC20">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="O1" pad="19"/>
<connect gate="G$1" pin="O2" pad="18"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="15"/>
<connect gate="G$1" pin="O6" pad="14"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATF16V8CZ-15JU"/>
<attribute name="OC_FARNELL" value="1551767"/>
<attribute name="OC_NEWARK" value="94M6253"/>
</technology>
</technologies>
</device>
<device name="P3" package="DIL20">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="O1" pad="19"/>
<connect gate="G$1" pin="O2" pad="18"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="15"/>
<connect gate="G$1" pin="O6" pad="14"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATF16V8CZ-15PU"/>
<attribute name="OC_FARNELL" value="1551768"/>
<attribute name="OC_NEWARK" value="94M6254"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="O1" pad="19"/>
<connect gate="G$1" pin="O2" pad="18"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="15"/>
<connect gate="G$1" pin="O6" pad="14"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH, 1 kbytes SRAM, 512 bytes EEPROM, USART, 6-channel 10 bit ADC, 2-channel 8 bit ADC&lt;br&gt;
Pin compatible with Atmega48, ATMega88, ATMega168&lt;br&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="-MI" package="MLF32">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA88PA-MU"/>
<attribute name="OC_FARNELL" value="1715491"/>
<attribute name="OC_NEWARK" value="15R0272"/>
</technology>
</technologies>
</device>
<device name="-AI" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="OC_NEWARK" value="73M8863"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH, 1 kbytes SRAM, 512 bytes EEPROM, USART, 4-channel 10 bit ADC, 2-channel 8 bit ADC&lt;br&gt;
Pin compatible with Atmega48, ATMega88, ATMega168&lt;br&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="23-I/O-2"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA16" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M16-A"/>
</gates>
<devices>
<device name="-M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16MU"/>
<attribute name="OC_FARNELL" value="1455107"/>
<attribute name="OC_NEWARK" value="58M3723"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16AU"/>
<attribute name="OC_FARNELL" value="9171134"/>
<attribute name="OC_NEWARK" value="96K6515"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA16-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M16-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="31"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16PU"/>
<attribute name="OC_FARNELL" value="9171142"/>
<attribute name="OC_NEWARK" value="01M6885"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32-A,M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
Source: www.atmel.com .. doc2503.pdf</description>
<gates>
<gate name="G$1" symbol="32-I/O-M32-A"/>
</gates>
<devices>
<device name="-M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16MU"/>
<attribute name="OC_FARNELL" value="1455108"/>
<attribute name="OC_NEWARK" value="58M3733"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16AU"/>
<attribute name="OC_FARNELL" value="9171274"/>
<attribute name="OC_NEWARK" value="69K6677"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA64" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
2 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA64"/>
</gates>
<devices>
<device name="-M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA64-16MU"/>
<attribute name="OC_FARNELL" value="1455120"/>
<attribute name="OC_NEWARK" value="58M3742"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA64-16AU"/>
<attribute name="OC_FARNELL" value="9171355"/>
<attribute name="OC_NEWARK" value="01M6899"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA128" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
128 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
4 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA128"/>
</gates>
<devices>
<device name="-M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA128-16MU"/>
<attribute name="OC_FARNELL" value="1455093"/>
<attribute name="OC_NEWARK" value="58M3717"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA128-16AU"/>
<attribute name="OC_FARNELL" value="9171118"/>
<attribute name="OC_NEWARK" value="95K7364"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA169" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
4x25 Segment LCD Driver&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA169"/>
</gates>
<devices>
<device name="-M" package="MLF64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(MISO/PCINT11)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCINT10)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT12)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A/PCINT13)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCINT14)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCINT15)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCINT9)PB1" pad="11"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21/INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22/ICP)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(SS/PCINT8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(SEG14)" pad="33"/>
<connect gate="G$1" pin="PG1(SEG13)" pad="34"/>
<connect gate="G$1" pin="PG2(SEG4)" pad="43"/>
<connect gate="G$1" pin="PG3(T1/SEG24)" pad="18"/>
<connect gate="G$1" pin="PG4(T0/SEG23)" pad="19"/>
<connect gate="G$1" pin="PG5(RESET)" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(MISO/PCINT11)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCINT10)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT12)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A/PCINT13)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCINT14)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCINT15)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCINT9)PB1" pad="11"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21/INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22/ICP)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(SS/PCINT8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(SEG14)" pad="33"/>
<connect gate="G$1" pin="PG1(SEG13)" pad="34"/>
<connect gate="G$1" pin="PG2(SEG4)" pad="43"/>
<connect gate="G$1" pin="PG3(T1/SEG24)" pad="18"/>
<connect gate="G$1" pin="PG4(T0/SEG23)" pad="19"/>
<connect gate="G$1" pin="PG5(RESET)" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA169PV-8AU"/>
<attribute name="OC_FARNELL" value="1617046"/>
<attribute name="OC_NEWARK" value="03P4011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA323" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA323-A"/>
</gates>
<devices>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA323-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA323"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8515" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8515-A"/>
</gates>
<devices>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK)PD4" pad="10"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8515-16AU"/>
<attribute name="OC_FARNELL" value="9171410"/>
<attribute name="OC_NEWARK" value="01M6904"/>
</technology>
</technologies>
</device>
<device name="-M" package="MLF44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK)PD4" pad="10"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="(XCK)PD4" pad="16"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="35"/>
<connect gate="G$1" pin="PE1(ALE)" pad="33"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="32"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8515-16JU"/>
<attribute name="OC_FARNELL" value="1562625"/>
<attribute name="OC_NEWARK" value="94M6261"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8515-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-7"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="(XCK)PD4" pad="14"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="31"/>
<connect gate="G$1" pin="PE1(ALE)" pad="30"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="29"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8515-16PU"/>
<attribute name="OC_FARNELL" value="9171401"/>
<attribute name="OC_NEWARK" value="01M6905"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8535" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-A"/>
</gates>
<devices>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8535-16AU"/>
<attribute name="OC_FARNELL" value="1528437"/>
<attribute name="OC_NEWARK" value="01M6908"/>
</technology>
</technologies>
</device>
<device name="-M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="GND@1" pad="34"/>
<connect gate="G$1" pin="PC0(SCL)" pad="25"/>
<connect gate="G$1" pin="PC1(SDA)" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8535-16JU"/>
<attribute name="OC_FARNELL" value="1562626"/>
<attribute name="OC_NEWARK" value="94M6263"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8535-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/OC0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/INT2)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="31"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8535-16PU"/>
<attribute name="OC_FARNELL" value="9171444"/>
<attribute name="OC_NEWARK" value="01M6909"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C513*-" prefix="IC">
<description>&lt;b&gt;8-bit Flash Microcontroller with Full Speed USB Device&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4136.pdf&lt;p&gt;
&lt;b&gt;&lt;i&gt;Data sheet mistake:&lt;/i&gt; &lt;/b&gt;define Packge type pin description for MLF48 but Order Number for QFN32 !?</description>
<gates>
<gate name="G$1" symbol="AT89C5131"/>
</gates>
<devices>
<device name="S" package="PLCC52">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="26"/>
<connect gate="G$1" pin="!PSEN" pad="28"/>
<connect gate="G$1" pin="!RST" pad="43"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="19"/>
<connect gate="G$1" pin="D+" pad="23"/>
<connect gate="G$1" pin="D-" pad="22"/>
<connect gate="G$1" pin="FREV" pad="24"/>
<connect gate="G$1" pin="P0.0_AD0" pad="52"/>
<connect gate="G$1" pin="P0.1_AD1" pad="45"/>
<connect gate="G$1" pin="P0.2_AD2" pad="44"/>
<connect gate="G$1" pin="P0.3_AD3" pad="42"/>
<connect gate="G$1" pin="P0.4_AD4" pad="40"/>
<connect gate="G$1" pin="P0.5_AD5" pad="38"/>
<connect gate="G$1" pin="P0.6_AD6" pad="37"/>
<connect gate="G$1" pin="P0.7_AD7" pad="36"/>
<connect gate="G$1" pin="P1.0/T2/KIN0" pad="47"/>
<connect gate="G$1" pin="P1.1/T2EX/KIN1/SS" pad="48"/>
<connect gate="G$1" pin="P1.2/ECI/KIN2" pad="49"/>
<connect gate="G$1" pin="P1.3/CEX0/KIN3" pad="50"/>
<connect gate="G$1" pin="P1.4/CEX1/KIN4" pad="51"/>
<connect gate="G$1" pin="P1.5/CEX2/KIN5/MISO" pad="4"/>
<connect gate="G$1" pin="P1.6/CEX3/KIN6/SCK" pad="5"/>
<connect gate="G$1" pin="P1.7/CEX4/KIN7/MOSI" pad="6"/>
<connect gate="G$1" pin="P2.0_A8" pad="1"/>
<connect gate="G$1" pin="P2.1_A9" pad="2"/>
<connect gate="G$1" pin="P2.2_A10" pad="3"/>
<connect gate="G$1" pin="P2.3_A11" pad="9"/>
<connect gate="G$1" pin="P2.4_A12" pad="10"/>
<connect gate="G$1" pin="P2.5_A13" pad="11"/>
<connect gate="G$1" pin="P2.6_A14" pad="14"/>
<connect gate="G$1" pin="P2.7_A15" pad="15"/>
<connect gate="G$1" pin="P3.0/RXD" pad="20"/>
<connect gate="G$1" pin="P3.1/TXD" pad="29"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="30"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="31"/>
<connect gate="G$1" pin="P3.4/T0" pad="32"/>
<connect gate="G$1" pin="P3.5/T1" pad="33"/>
<connect gate="G$1" pin="P3.6/!WR" pad="35"/>
<connect gate="G$1" pin="P3.7/!RD" pad="39"/>
<connect gate="G$1" pin="P4.0/SCL" pad="7"/>
<connect gate="G$1" pin="P4.1/SDA" pad="8"/>
<connect gate="G$1" pin="PLLF" pad="21"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C5131A-S3SUM"/>
<attribute name="OC_FARNELL" value="1095721"/>
<attribute name="OC_NEWARK" value="96K6570"/>
</technology>
</technologies>
</device>
<device name="R" package="VQFP64">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="24"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="!RST" pad="44"/>
<connect gate="G$1" pin="ALE" pad="25"/>
<connect gate="G$1" pin="AVDD" pad="10"/>
<connect gate="G$1" pin="AVSS" pad="12"/>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="20"/>
<connect gate="G$1" pin="FREV" pad="22"/>
<connect gate="G$1" pin="P0.0_AD0" pad="55"/>
<connect gate="G$1" pin="P0.1_AD1" pad="46"/>
<connect gate="G$1" pin="P0.2_AD2" pad="45"/>
<connect gate="G$1" pin="P0.3_AD3" pad="43"/>
<connect gate="G$1" pin="P0.4_AD4" pad="40"/>
<connect gate="G$1" pin="P0.5_AD5" pad="38"/>
<connect gate="G$1" pin="P0.6_AD6" pad="37"/>
<connect gate="G$1" pin="P0.7_AD7" pad="36"/>
<connect gate="G$1" pin="P1.0/T2/KIN0" pad="50"/>
<connect gate="G$1" pin="P1.1/T2EX/KIN1/SS" pad="51"/>
<connect gate="G$1" pin="P1.2/ECI/KIN2" pad="52"/>
<connect gate="G$1" pin="P1.3/CEX0/KIN3" pad="53"/>
<connect gate="G$1" pin="P1.4/CEX1/KIN4" pad="54"/>
<connect gate="G$1" pin="P1.5/CEX2/KIN5/MISO" pad="59"/>
<connect gate="G$1" pin="P1.6/CEX3/KIN6/SCK" pad="60"/>
<connect gate="G$1" pin="P1.7/CEX4/KIN7/MOSI" pad="61"/>
<connect gate="G$1" pin="P2.0_A8" pad="56"/>
<connect gate="G$1" pin="P2.1_A9" pad="57"/>
<connect gate="G$1" pin="P2.2_A10" pad="58"/>
<connect gate="G$1" pin="P2.3_A11" pad="2"/>
<connect gate="G$1" pin="P2.4_A12" pad="3"/>
<connect gate="G$1" pin="P2.5_A13" pad="4"/>
<connect gate="G$1" pin="P2.6_A14" pad="7"/>
<connect gate="G$1" pin="P2.7_A15" pad="8"/>
<connect gate="G$1" pin="P3.0/RXD" pad="14"/>
<connect gate="G$1" pin="P3.1/TXD" pad="27"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="28"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="29"/>
<connect gate="G$1" pin="P3.4/T0" pad="30"/>
<connect gate="G$1" pin="P3.5/T1" pad="31"/>
<connect gate="G$1" pin="P3.6/!WR" pad="35"/>
<connect gate="G$1" pin="P3.7/!RD" pad="39"/>
<connect gate="G$1" pin="P4.0/SCL" pad="62"/>
<connect gate="G$1" pin="P4.1/SDA" pad="63"/>
<connect gate="G$1" pin="PLLF" pad="19"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="42"/>
<connect gate="G$1" pin="XTAL1" pad="6"/>
<connect gate="G$1" pin="XTAL2" pad="5"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C5132" prefix="IC">
<description>&lt;b&gt;USB Microcontroller with 64K Bytes Flash Memory&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4173.pdf</description>
<gates>
<gate name="G$1" symbol="AT89C5132"/>
</gates>
<devices>
<device name="" package="TQFP80">
<connects>
<connect gate="G$1" pin="!ISP" pad="2"/>
<connect gate="G$1" pin="!TST" pad="18"/>
<connect gate="G$1" pin="AIN0" pad="37"/>
<connect gate="G$1" pin="AIN1" pad="38"/>
<connect gate="G$1" pin="ALE" pad="1"/>
<connect gate="G$1" pin="AREFN" pad="36"/>
<connect gate="G$1" pin="AREFP" pad="35"/>
<connect gate="G$1" pin="AVDD" pad="33"/>
<connect gate="G$1" pin="AVSS" pad="34"/>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="22"/>
<connect gate="G$1" pin="DCLK" pad="44"/>
<connect gate="G$1" pin="DOUT" pad="43"/>
<connect gate="G$1" pin="DSEL" pad="45"/>
<connect gate="G$1" pin="FILT" pad="13"/>
<connect gate="G$1" pin="MCLK" pad="50"/>
<connect gate="G$1" pin="MCMD" pad="48"/>
<connect gate="G$1" pin="MDAT" pad="49"/>
<connect gate="G$1" pin="P0.0_AD0" pad="78"/>
<connect gate="G$1" pin="P0.1_AD1" pad="77"/>
<connect gate="G$1" pin="P0.2_AD2" pad="76"/>
<connect gate="G$1" pin="P0.3_AD3" pad="75"/>
<connect gate="G$1" pin="P0.4_AD4" pad="74"/>
<connect gate="G$1" pin="P0.5_AD5" pad="73"/>
<connect gate="G$1" pin="P0.6_AD6" pad="70"/>
<connect gate="G$1" pin="P0.7_AD7" pad="69"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="3"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="4"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="5"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="6"/>
<connect gate="G$1" pin="P1.4" pad="7"/>
<connect gate="G$1" pin="P1.5" pad="8"/>
<connect gate="G$1" pin="P1.6/SCL" pad="9"/>
<connect gate="G$1" pin="P1.7/SDA" pad="10"/>
<connect gate="G$1" pin="P2.0_A8" pad="64"/>
<connect gate="G$1" pin="P2.1_A9" pad="63"/>
<connect gate="G$1" pin="P2.2_A10" pad="58"/>
<connect gate="G$1" pin="P2.3_A11" pad="57"/>
<connect gate="G$1" pin="P2.4_A12" pad="56"/>
<connect gate="G$1" pin="P2.5_A13" pad="55"/>
<connect gate="G$1" pin="P2.6_A14" pad="54"/>
<connect gate="G$1" pin="P2.7_A15" pad="53"/>
<connect gate="G$1" pin="P3.0/RXD" pad="25"/>
<connect gate="G$1" pin="P3.1/TXD" pad="26"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="27"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="28"/>
<connect gate="G$1" pin="P3.4/T0" pad="29"/>
<connect gate="G$1" pin="P3.5/T1" pad="30"/>
<connect gate="G$1" pin="P3.6/!WR" pad="31"/>
<connect gate="G$1" pin="P3.7/!RD" pad="32"/>
<connect gate="G$1" pin="P4.0/MISO" pad="65"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="66"/>
<connect gate="G$1" pin="P4.2/SCK" pad="67"/>
<connect gate="G$1" pin="P4.3/!SS" pad="68"/>
<connect gate="G$1" pin="P4.4" pad="59"/>
<connect gate="G$1" pin="P4.5" pad="60"/>
<connect gate="G$1" pin="P4.6" pad="61"/>
<connect gate="G$1" pin="P4.7" pad="62"/>
<connect gate="G$1" pin="P5.0" pad="79"/>
<connect gate="G$1" pin="P5.1" pad="80"/>
<connect gate="G$1" pin="P5.2" pad="39"/>
<connect gate="G$1" pin="P5.3" pad="40"/>
<connect gate="G$1" pin="PVDD" pad="12"/>
<connect gate="G$1" pin="PVSS" pad="14"/>
<connect gate="G$1" pin="RST" pad="47"/>
<connect gate="G$1" pin="SCLK" pad="46"/>
<connect gate="G$1" pin="UVDD" pad="19"/>
<connect gate="G$1" pin="UVSS" pad="20"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="23"/>
<connect gate="G$1" pin="VDD@2" pad="41"/>
<connect gate="G$1" pin="VDD@3" pad="51"/>
<connect gate="G$1" pin="VDD@4" pad="71"/>
<connect gate="G$1" pin="VSS" pad="15"/>
<connect gate="G$1" pin="VSS@1" pad="24"/>
<connect gate="G$1" pin="VSS@2" pad="42"/>
<connect gate="G$1" pin="VSS@3" pad="52"/>
<connect gate="G$1" pin="VSS@4" pad="72"/>
<connect gate="G$1" pin="X1" pad="17"/>
<connect gate="G$1" pin="X2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="DEVELOP" package="PLCC84">
<connects>
<connect gate="G$1" pin="!ISP" pad="13"/>
<connect gate="G$1" pin="!TST" pad="30"/>
<connect gate="G$1" pin="AIN0" pad="49"/>
<connect gate="G$1" pin="AIN1" pad="50"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="AREFN" pad="48"/>
<connect gate="G$1" pin="AREFP" pad="47"/>
<connect gate="G$1" pin="AVDD" pad="45"/>
<connect gate="G$1" pin="AVSS" pad="46"/>
<connect gate="G$1" pin="D+" pad="33"/>
<connect gate="G$1" pin="D-" pad="34"/>
<connect gate="G$1" pin="DCLK" pad="57"/>
<connect gate="G$1" pin="DOUT" pad="56"/>
<connect gate="G$1" pin="DSEL" pad="58"/>
<connect gate="G$1" pin="FILT" pad="24"/>
<connect gate="G$1" pin="MCLK" pad="63"/>
<connect gate="G$1" pin="MCMD" pad="61"/>
<connect gate="G$1" pin="MDAT" pad="62"/>
<connect gate="G$1" pin="P0.0_AD0" pad="8"/>
<connect gate="G$1" pin="P0.1_AD1" pad="7"/>
<connect gate="G$1" pin="P0.2_AD2" pad="6"/>
<connect gate="G$1" pin="P0.3_AD3" pad="5"/>
<connect gate="G$1" pin="P0.4_AD4" pad="4"/>
<connect gate="G$1" pin="P0.5_AD5" pad="3"/>
<connect gate="G$1" pin="P0.6_AD6" pad="84"/>
<connect gate="G$1" pin="P0.7_AD7" pad="83"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="14"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="15"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="16"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="17"/>
<connect gate="G$1" pin="P1.4" pad="18"/>
<connect gate="G$1" pin="P1.5" pad="19"/>
<connect gate="G$1" pin="P1.6/SCL" pad="20"/>
<connect gate="G$1" pin="P1.7/SDA" pad="21"/>
<connect gate="G$1" pin="P2.0_A8" pad="78"/>
<connect gate="G$1" pin="P2.1_A9" pad="77"/>
<connect gate="G$1" pin="P2.2_A10" pad="71"/>
<connect gate="G$1" pin="P2.3_A11" pad="70"/>
<connect gate="G$1" pin="P2.4_A12" pad="69"/>
<connect gate="G$1" pin="P2.5_A13" pad="68"/>
<connect gate="G$1" pin="P2.6_A14" pad="67"/>
<connect gate="G$1" pin="P2.7_A15" pad="66"/>
<connect gate="G$1" pin="P3.0/RXD" pad="37"/>
<connect gate="G$1" pin="P3.1/TXD" pad="38"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="39"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="40"/>
<connect gate="G$1" pin="P3.4/T0" pad="41"/>
<connect gate="G$1" pin="P3.5/T1" pad="42"/>
<connect gate="G$1" pin="P3.6/!WR" pad="43"/>
<connect gate="G$1" pin="P3.7/!RD" pad="44"/>
<connect gate="G$1" pin="P4.0/MISO" pad="79"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="80"/>
<connect gate="G$1" pin="P4.2/SCK" pad="81"/>
<connect gate="G$1" pin="P4.3/!SS" pad="82"/>
<connect gate="G$1" pin="P4.4" pad="72"/>
<connect gate="G$1" pin="P4.5" pad="73"/>
<connect gate="G$1" pin="P4.6" pad="75"/>
<connect gate="G$1" pin="P4.7" pad="76"/>
<connect gate="G$1" pin="P5.0" pad="9"/>
<connect gate="G$1" pin="P5.1" pad="10"/>
<connect gate="G$1" pin="P5.2" pad="51"/>
<connect gate="G$1" pin="P5.3" pad="52"/>
<connect gate="G$1" pin="PVDD" pad="23"/>
<connect gate="G$1" pin="PVSS" pad="25"/>
<connect gate="G$1" pin="RST" pad="60"/>
<connect gate="G$1" pin="SCLK" pad="59"/>
<connect gate="G$1" pin="UVDD" pad="31"/>
<connect gate="G$1" pin="UVSS" pad="32"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="22"/>
<connect gate="G$1" pin="VDD@2" pad="35"/>
<connect gate="G$1" pin="VDD@3" pad="54"/>
<connect gate="G$1" pin="VDD@4" pad="64"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="VSS@1" pad="26"/>
<connect gate="G$1" pin="VSS@2" pad="36"/>
<connect gate="G$1" pin="VSS@3" pad="55"/>
<connect gate="G$1" pin="VSS@4" pad="65"/>
<connect gate="G$1" pin="X1" pad="29"/>
<connect gate="G$1" pin="X2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8-MI" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH, 1 kbytes SRAM, 512 bytes EEPROM, USART, 6-channel 10 bit ADC, 2-channel 8 bit ADC&lt;br&gt;
Pin compatible with Atmega48, ATMega88, ATMega168&lt;br&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="23-I/O_MI"/>
</gates>
<devices>
<device name="" package="MLF32-TH">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA88PA-MU"/>
<attribute name="OC_FARNELL" value="1715491"/>
<attribute name="OC_NEWARK" value="15R0272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA16-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M16-A_M"/>
</gates>
<devices>
<device name="" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16MU"/>
<attribute name="OC_FARNELL" value="1455097"/>
<attribute name="OC_NEWARK" value="58M3723"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
Source: www.atmel.com .. doc2503.pdf</description>
<gates>
<gate name="G$1" symbol="32-I/O-M32-A_M"/>
</gates>
<devices>
<device name="" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16MU"/>
<attribute name="OC_FARNELL" value="1455108"/>
<attribute name="OC_NEWARK" value="58M3733"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA64-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
2 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA64-M"/>
</gates>
<devices>
<device name="" package="MLF64-TH">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA64-16MU"/>
<attribute name="OC_FARNELL" value="1455120"/>
<attribute name="OC_NEWARK" value="58M3742"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA128-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
128 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
4 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA128-M"/>
</gates>
<devices>
<device name="" package="MLF64-TH">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA128-16MU"/>
<attribute name="OC_FARNELL" value="1455093"/>
<attribute name="OC_NEWARK" value="58M3717"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA169-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
4x25 Segment LCD Driver&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA169-M"/>
</gates>
<devices>
<device name="" package="MLF64-TH">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(MISO/PCINT11)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCINT10)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT12)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A/PCINT13)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCINT14)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCINT15)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCINT9)PB1" pad="11"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21/INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22/ICP)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(SS/PCINT8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(SEG14)" pad="33"/>
<connect gate="G$1" pin="PG1(SEG13)" pad="34"/>
<connect gate="G$1" pin="PG2(SEG4)" pad="43"/>
<connect gate="G$1" pin="PG3(T1/SEG24)" pad="18"/>
<connect gate="G$1" pin="PG4(T0/SEG23)" pad="19"/>
<connect gate="G$1" pin="PG5(RESET)" pad="20"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8515-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8515-A_M"/>
</gates>
<devices>
<device name="-M" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK)PD4" pad="10"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8535_M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-A_M"/>
</gates>
<devices>
<device name="-M" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY26*-M" prefix="IC">
<description>&lt;b&gt;8-bit AVR Microcontroller with 2K Bytes Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com .. doc1477.pdf</description>
<gates>
<gate name="G$1" symbol="TINY26_M"/>
</gates>
<devices>
<device name="" package="MLF32-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="26"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="25"/>
<connect gate="G$1" pin="(ADC10/!RESET!)PB7" pad="11"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="23"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="17"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="15"/>
<connect gate="G$1" pin="(ADC5/AIN0)PA6" pad="14"/>
<connect gate="G$1" pin="(ADC6/AIN1)PA7" pad="13"/>
<connect gate="G$1" pin="(ADC7/XTAL1)PB4" pad="7"/>
<connect gate="G$1" pin="(ADC8/XTAL2)PB5" pad="8"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="10"/>
<connect gate="G$1" pin="(AREF)PA3" pad="22"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="31"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/!OC1A!)PB0" pad="30"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="2"/>
<connect gate="G$1" pin="(SCK/SCL/!OC1B!)PB2" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="21"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA644" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller&lt;/b&gt; with 64K Bytes In-System Programmable Flash&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2593.pdf</description>
<gates>
<gate name="G$1" symbol="ATMEGA644"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(PCINT0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCINT1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCINT10/INT2/AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(PCINT11/OC0A/AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(PCINT12/OC0B/!SS!)PB4" pad="44"/>
<connect gate="G$1" pin="(PCINT13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCINT14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCINT15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCINT16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCINT17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCINT18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCINT19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCINT2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCINT20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCINT21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCINT22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCINT23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCINT24/RXD0)PD0" pad="9"/>
<connect gate="G$1" pin="(PCINT25/TXD0)PD1" pad="10"/>
<connect gate="G$1" pin="(PCINT26/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCINT27/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCINT28/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCINT29/OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCINT3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCINT30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCINT31/OC2A)PD7" pad="16"/>
<connect gate="G$1" pin="(PCINT4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCINT5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCINT6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCINT7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCINT8/XCK0/T0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCINT9/CLKO/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="17"/>
<connect gate="G$1" pin="VCC@2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644PV-10AU"/>
<attribute name="OC_FARNELL" value="1455123"/>
<attribute name="OC_NEWARK" value="58M3748"/>
</technology>
</technologies>
</device>
<device name="M" package="QFN44ML8X8">
<connects>
<connect gate="G$1" pin="(PCINT0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCINT1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCINT10/INT2/AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(PCINT11/OC0A/AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(PCINT12/OC0B/!SS!)PB4" pad="44"/>
<connect gate="G$1" pin="(PCINT13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCINT14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCINT15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCINT16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCINT17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCINT18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCINT19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCINT2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCINT20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCINT21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCINT22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCINT23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCINT24/RXD0)PD0" pad="9"/>
<connect gate="G$1" pin="(PCINT25/TXD0)PD1" pad="10"/>
<connect gate="G$1" pin="(PCINT26/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCINT27/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCINT28/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCINT29/OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCINT3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCINT30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCINT31/OC2A)PD7" pad="16"/>
<connect gate="G$1" pin="(PCINT4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCINT5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCINT6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCINT7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCINT8/XCK0/T0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCINT9/CLKO/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="17"/>
<connect gate="G$1" pin="VCC@2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644PV-10MU"/>
<attribute name="OC_FARNELL" value="1748529"/>
<attribute name="OC_NEWARK" value="26R5637"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA644*" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller&lt;/b&gt; with 64K Bytes In-System Programmable Flash&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2593.pdf</description>
<gates>
<gate name="G$1" symbol="ATMEGA644E"/>
</gates>
<devices>
<device name="M" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(PCINT0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCINT1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCINT10/INT2/AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(PCINT11/OC0A/AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(PCINT12/OC0B/!SS!)PB4" pad="44"/>
<connect gate="G$1" pin="(PCINT13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCINT14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCINT15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCINT16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCINT17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCINT18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCINT19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCINT2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCINT20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCINT21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCINT22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCINT23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCINT24/RXD0)PD0" pad="9"/>
<connect gate="G$1" pin="(PCINT25/TXD0)PD1" pad="10"/>
<connect gate="G$1" pin="(PCINT26/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCINT27/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCINT28/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCINT29/OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCINT3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCINT30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCINT31/OC2A)PD7" pad="16"/>
<connect gate="G$1" pin="(PCINT4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCINT5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCINT6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCINT7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCINT8/XCK0/T0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCINT9/CLKO/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="EXP" pad="TH"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="17"/>
<connect gate="G$1" pin="VCC@2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644P-20MU"/>
<attribute name="OC_FARNELL" value="1748528"/>
<attribute name="OC_NEWARK" value="26R5636"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91SAM7X*-AU" prefix="IC">
<description>&lt;b&gt;Highly integrated Flash microcontrollers based on the 32-bit ARM RISC processor&lt;/b&gt;&lt;p&gt;
512/256/128 Kbyte high-speed Flash and 128/64/32 Kbyte SRAM, a large set of peripherals, including an 802.3 Ethernet MAC and a CAN controller&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/6120s.pdf</description>
<gates>
<gate name="G$1" symbol="AT91SAM7X"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="G$1" pin="AD4" pad="3"/>
<connect gate="G$1" pin="AD5" pad="4"/>
<connect gate="G$1" pin="AD6" pad="5"/>
<connect gate="G$1" pin="AD7" pad="6"/>
<connect gate="G$1" pin="ADVREF" pad="1"/>
<connect gate="G$1" pin="DDM" pad="93"/>
<connect gate="G$1" pin="DDP" pad="94"/>
<connect gate="G$1" pin="ERASE" pad="92"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="16"/>
<connect gate="G$1" pin="GND@3" pad="32"/>
<connect gate="G$1" pin="GND@4" pad="52"/>
<connect gate="G$1" pin="GND@5" pad="68"/>
<connect gate="G$1" pin="GND@6" pad="83"/>
<connect gate="G$1" pin="GND@7" pad="96"/>
<connect gate="G$1" pin="JTAGSEL" pad="77"/>
<connect gate="G$1" pin="NRST" pad="57"/>
<connect gate="G$1" pin="PA0/PGMEN0" pad="81"/>
<connect gate="G$1" pin="PA1/PGMEN1" pad="82"/>
<connect gate="G$1" pin="PA10/PGMM2" pad="18"/>
<connect gate="G$1" pin="PA11/PGMM3" pad="19"/>
<connect gate="G$1" pin="PA12/PGMD0" pad="20"/>
<connect gate="G$1" pin="PA13/PGMD1" pad="21"/>
<connect gate="G$1" pin="PA14/PGMD2" pad="22"/>
<connect gate="G$1" pin="PA15/PGMD3" pad="23"/>
<connect gate="G$1" pin="PA16/PGMD4" pad="24"/>
<connect gate="G$1" pin="PA17/PGMD5" pad="25"/>
<connect gate="G$1" pin="PA18/PGMD6" pad="26"/>
<connect gate="G$1" pin="PA19/PGMD7" pad="46"/>
<connect gate="G$1" pin="PA2" pad="86"/>
<connect gate="G$1" pin="PA20/PGMD8" pad="47"/>
<connect gate="G$1" pin="PA21/PGMD9" pad="49"/>
<connect gate="G$1" pin="PA22/PGMD10" pad="50"/>
<connect gate="G$1" pin="PA23/PGMD11" pad="55"/>
<connect gate="G$1" pin="PA24/PGMD12" pad="56"/>
<connect gate="G$1" pin="PA25/PGMD13" pad="59"/>
<connect gate="G$1" pin="PA26/PGMD14" pad="60"/>
<connect gate="G$1" pin="PA27/PGMD15" pad="73"/>
<connect gate="G$1" pin="PA28" pad="74"/>
<connect gate="G$1" pin="PA29" pad="75"/>
<connect gate="G$1" pin="PA3" pad="85"/>
<connect gate="G$1" pin="PA30" pad="80"/>
<connect gate="G$1" pin="PA4/PGMNCMD" pad="88"/>
<connect gate="G$1" pin="PA5/PGMRDY" pad="89"/>
<connect gate="G$1" pin="PA6/PGMNOE" pad="90"/>
<connect gate="G$1" pin="PA7/PGMNVALID" pad="91"/>
<connect gate="G$1" pin="PA8/PGMM0" pad="13"/>
<connect gate="G$1" pin="PA9/PGMM1" pad="14"/>
<connect gate="G$1" pin="PB0" pad="40"/>
<connect gate="G$1" pin="PB1" pad="41"/>
<connect gate="G$1" pin="PB10" pad="44"/>
<connect gate="G$1" pin="PB11" pad="45"/>
<connect gate="G$1" pin="PB12" pad="39"/>
<connect gate="G$1" pin="PB13" pad="30"/>
<connect gate="G$1" pin="PB14" pad="29"/>
<connect gate="G$1" pin="PB15" pad="35"/>
<connect gate="G$1" pin="PB16" pad="53"/>
<connect gate="G$1" pin="PB17" pad="36"/>
<connect gate="G$1" pin="PB18" pad="63"/>
<connect gate="G$1" pin="PB19" pad="64"/>
<connect gate="G$1" pin="PB2" pad="42"/>
<connect gate="G$1" pin="PB20" pad="65"/>
<connect gate="G$1" pin="PB21" pad="66"/>
<connect gate="G$1" pin="PB22" pad="67"/>
<connect gate="G$1" pin="PB23" pad="69"/>
<connect gate="G$1" pin="PB24" pad="70"/>
<connect gate="G$1" pin="PB25" pad="71"/>
<connect gate="G$1" pin="PB26" pad="72"/>
<connect gate="G$1" pin="PB27/AD0" pad="9"/>
<connect gate="G$1" pin="PB28/AD1" pad="10"/>
<connect gate="G$1" pin="PB29/AD2" pad="11"/>
<connect gate="G$1" pin="PB3" pad="43"/>
<connect gate="G$1" pin="PB30/AD3" pad="12"/>
<connect gate="G$1" pin="PB4" pad="54"/>
<connect gate="G$1" pin="PB5" pad="34"/>
<connect gate="G$1" pin="PB6" pad="31"/>
<connect gate="G$1" pin="PB7" pad="38"/>
<connect gate="G$1" pin="PB8" pad="28"/>
<connect gate="G$1" pin="PB9" pad="27"/>
<connect gate="G$1" pin="PLLRC" pad="99"/>
<connect gate="G$1" pin="TCK" pad="79"/>
<connect gate="G$1" pin="TDI" pad="51"/>
<connect gate="G$1" pin="TDO" pad="76"/>
<connect gate="G$1" pin="TMS" pad="78"/>
<connect gate="G$1" pin="TST" pad="58"/>
<connect gate="G$1" pin="VDDCORE@1" pad="15"/>
<connect gate="G$1" pin="VDDCORE@2" pad="37"/>
<connect gate="G$1" pin="VDDCORE@3" pad="62"/>
<connect gate="G$1" pin="VDDCORE@4" pad="87"/>
<connect gate="G$1" pin="VDDFLASH" pad="95"/>
<connect gate="G$1" pin="VDDIN@1" pad="8"/>
<connect gate="G$1" pin="VDDIO@1" pad="17"/>
<connect gate="G$1" pin="VDDIO@2" pad="33"/>
<connect gate="G$1" pin="VDDIO@3" pad="48"/>
<connect gate="G$1" pin="VDDIO@4" pad="61"/>
<connect gate="G$1" pin="VDDIO@5" pad="84"/>
<connect gate="G$1" pin="VDDOUT@1" pad="7"/>
<connect gate="G$1" pin="VDDPLL" pad="100"/>
<connect gate="G$1" pin="XIN/PGMCK" pad="97"/>
<connect gate="G$1" pin="XOUT" pad="98"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT91SAM7X128B-AU"/>
<attribute name="OC_FARNELL" value="1288326"/>
<attribute name="OC_NEWARK" value="26R5682"/>
</technology>
<technology name="256">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT91SAM7X256B-AU"/>
<attribute name="OC_FARNELL" value="1288327"/>
<attribute name="OC_NEWARK" value="26R5683"/>
</technology>
<technology name="512">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT91SAM7X512-AU"/>
<attribute name="OC_FARNELL" value="1288328"/>
<attribute name="OC_NEWARK" value="23M5090"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91SAM7X*-CU" prefix="IC">
<description>&lt;b&gt;Highly integrated Flash microcontrollers based on the 32-bit ARM RISC processor&lt;/b&gt;&lt;p&gt;
512/256/128 Kbyte high-speed Flash and 128/64/32 Kbyte SRAM, a large set of peripherals, including an 802.3 Ethernet MAC and a CAN controller&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/6120s.pdf</description>
<gates>
<gate name="G$1" symbol="AT91SAM7X-BGA"/>
</gates>
<devices>
<device name="" package="TFBGA100">
<connects>
<connect gate="G$1" pin="AD4" pad="K9"/>
<connect gate="G$1" pin="AD5" pad="K8"/>
<connect gate="G$1" pin="AD6" pad="K7"/>
<connect gate="G$1" pin="AD7" pad="K6"/>
<connect gate="G$1" pin="ADVREF" pad="K10"/>
<connect gate="G$1" pin="DDM" pad="K4"/>
<connect gate="G$1" pin="DDP" pad="K3"/>
<connect gate="G$1" pin="ERASE" pad="F7"/>
<connect gate="G$1" pin="GND@1" pad="E6"/>
<connect gate="G$1" pin="GND@2" pad="E10"/>
<connect gate="G$1" pin="GND@3" pad="F9"/>
<connect gate="G$1" pin="GND@4" pad="G8"/>
<connect gate="G$1" pin="GND@5" pad="J6"/>
<connect gate="G$1" pin="GND@6" pad="J9"/>
<connect gate="G$1" pin="GND@7" pad="K5"/>
<connect gate="G$1" pin="JTAGSEL" pad="H3"/>
<connect gate="G$1" pin="NRST" pad="D3"/>
<connect gate="G$1" pin="PA0/PGMEN0" pad="J3"/>
<connect gate="G$1" pin="PA1/PGMEN1" pad="J4"/>
<connect gate="G$1" pin="PA10/PGMM2" pad="D7"/>
<connect gate="G$1" pin="PA11/PGMM3" pad="D10"/>
<connect gate="G$1" pin="PA12/PGMD0" pad="C9"/>
<connect gate="G$1" pin="PA13/PGMD1" pad="C8"/>
<connect gate="G$1" pin="PA14/PGMD2" pad="B8"/>
<connect gate="G$1" pin="PA15/PGMD3" pad="C10"/>
<connect gate="G$1" pin="PA16/PGMD4" pad="B9"/>
<connect gate="G$1" pin="PA17/PGMD5" pad="B10"/>
<connect gate="G$1" pin="PA18/PGMD6" pad="A9"/>
<connect gate="G$1" pin="PA19/PGMD7" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="G5"/>
<connect gate="G$1" pin="PA20/PGMD8" pad="A3"/>
<connect gate="G$1" pin="PA21/PGMD9" pad="A2"/>
<connect gate="G$1" pin="PA22/PGMD10" pad="A1"/>
<connect gate="G$1" pin="PA23/PGMD11" pad="D1"/>
<connect gate="G$1" pin="PA24/PGMD12" pad="D2"/>
<connect gate="G$1" pin="PA25/PGMD13" pad="E1"/>
<connect gate="G$1" pin="PA26/PGMD14" pad="E2"/>
<connect gate="G$1" pin="PA27/PGMD15" pad="G3"/>
<connect gate="G$1" pin="PA28" pad="H2"/>
<connect gate="G$1" pin="PA29" pad="J1"/>
<connect gate="G$1" pin="PA3" pad="H4"/>
<connect gate="G$1" pin="PA30" pad="J2"/>
<connect gate="G$1" pin="PA4/PGMNCMD" pad="H5"/>
<connect gate="G$1" pin="PA5/PGMRDY" pad="G6"/>
<connect gate="G$1" pin="PA6/PGMNOE" pad="F6"/>
<connect gate="G$1" pin="PA7/PGMNVALID" pad="H6"/>
<connect gate="G$1" pin="PA8/PGMM0" pad="H8"/>
<connect gate="G$1" pin="PA9/PGMM1" pad="H7"/>
<connect gate="G$1" pin="PB0" pad="C5"/>
<connect gate="G$1" pin="PB1" pad="A4"/>
<connect gate="G$1" pin="PB10" pad="C3"/>
<connect gate="G$1" pin="PB11" pad="B3"/>
<connect gate="G$1" pin="PB12" pad="B5"/>
<connect gate="G$1" pin="PB13" pad="C7"/>
<connect gate="G$1" pin="PB14" pad="B7"/>
<connect gate="G$1" pin="PB15" pad="B6"/>
<connect gate="G$1" pin="PB16" pad="C1"/>
<connect gate="G$1" pin="PB17" pad="C6"/>
<connect gate="G$1" pin="PB18" pad="E3"/>
<connect gate="G$1" pin="PB19" pad="D5"/>
<connect gate="G$1" pin="PB2" pad="B4"/>
<connect gate="G$1" pin="PB20" pad="E4"/>
<connect gate="G$1" pin="PB21" pad="F1"/>
<connect gate="G$1" pin="PB22" pad="G1"/>
<connect gate="G$1" pin="PB23" pad="F2"/>
<connect gate="G$1" pin="PB24" pad="G2"/>
<connect gate="G$1" pin="PB25" pad="F3"/>
<connect gate="G$1" pin="PB26" pad="F4"/>
<connect gate="G$1" pin="PB27/AD0" pad="D9"/>
<connect gate="G$1" pin="PB28/AD1" pad="E8"/>
<connect gate="G$1" pin="PB29/AD2" pad="H9"/>
<connect gate="G$1" pin="PB3" pad="C4"/>
<connect gate="G$1" pin="PB30/AD3" pad="G9"/>
<connect gate="G$1" pin="PB4" pad="C2"/>
<connect gate="G$1" pin="PB5" pad="A6"/>
<connect gate="G$1" pin="PB6" pad="D6"/>
<connect gate="G$1" pin="PB7" pad="A5"/>
<connect gate="G$1" pin="PB8" pad="A7"/>
<connect gate="G$1" pin="PB9" pad="A8"/>
<connect gate="G$1" pin="PLLRC" pad="H10"/>
<connect gate="G$1" pin="TCK" pad="F5"/>
<connect gate="G$1" pin="TDI" pad="B1"/>
<connect gate="G$1" pin="TDO" pad="G4"/>
<connect gate="G$1" pin="TMS" pad="E5"/>
<connect gate="G$1" pin="TST" pad="D4"/>
<connect gate="G$1" pin="VDDCORE@1" pad="F8"/>
<connect gate="G$1" pin="VDDCORE@2" pad="G7"/>
<connect gate="G$1" pin="VDDCORE@3" pad="H1"/>
<connect gate="G$1" pin="VDDCORE@4" pad="K1"/>
<connect gate="G$1" pin="VDDCORE@5" pad="K2"/>
<connect gate="G$1" pin="VDDFLASH" pad="J5"/>
<connect gate="G$1" pin="VDDIN@1" pad="F10"/>
<connect gate="G$1" pin="VDDIO@1" pad="A10"/>
<connect gate="G$1" pin="VDDIO@2" pad="D8"/>
<connect gate="G$1" pin="VDDIO@3" pad="E7"/>
<connect gate="G$1" pin="VDDIO@4" pad="E9"/>
<connect gate="G$1" pin="VDDOUT@1" pad="G10"/>
<connect gate="G$1" pin="VDDPLL" pad="J10"/>
<connect gate="G$1" pin="XIN/PGMCK" pad="J7"/>
<connect gate="G$1" pin="XOUT" pad="J8"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="256">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT93C46A-10?Q-2.7" prefix="IC">
<description>&lt;b&gt;Three-wire Automotive Temperature Serial EEPROM&lt;/b&gt; 1K (64 x 16)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc5089.pdf</description>
<gates>
<gate name="G$1" symbol="AT93C46A"/>
</gates>
<devices>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DC" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT93C46DN-SH-B"/>
<attribute name="OC_FARNELL" value="1455086"/>
<attribute name="OC_NEWARK" value="58M3879"/>
</technology>
</technologies>
</device>
<device name="T" package="TSSOP8">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DC" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY13" prefix="IC">
<description>&lt;b&gt; 8-bit AVR Microcontroller with 1K Bytes In-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
<gates>
<gate name="G$1" symbol="TINY13"/>
</gates>
<devices>
<device name="PU" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="5"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="6"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="7"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13-20PU"/>
<attribute name="OC_FARNELL" value="9171550"/>
<attribute name="OC_NEWARK" value="96K6521"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10PU"/>
<attribute name="OC_FARNELL" value="9171576"/>
<attribute name="OC_NEWARK" value="96K6523"/>
</technology>
</technologies>
</device>
<device name="SSU" package="8S1">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="5"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="6"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="7"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13-20SSU"/>
<attribute name="OC_FARNELL" value="1455133"/>
<attribute name="OC_NEWARK" value="58M3771"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10SSU"/>
<attribute name="OC_FARNELL" value="1455135"/>
<attribute name="OC_NEWARK" value="58M3773"/>
</technology>
</technologies>
</device>
<device name="SU" package="8S2">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="5"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="6"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="7"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13-20SU"/>
<attribute name="OC_FARNELL" value="9171568"/>
<attribute name="OC_NEWARK" value="96K6522"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10SU"/>
<attribute name="OC_FARNELL" value="9171584"/>
<attribute name="OC_NEWARK" value="96K6524"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY13*" prefix="IC">
<description>&lt;b&gt; 8-bit AVR Microcontroller with 1K Bytes In-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
<gates>
<gate name="G$1" symbol="TINY13"/>
<gate name="P" symbol="GND"/>
</gates>
<devices>
<device name="MM0" package="10M1">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="6"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="7"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="9"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="4"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="P" pin="GND" pad="11"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13A-MMU"/>
<attribute name="OC_FARNELL" value="1715516"/>
<attribute name="OC_NEWARK" value="15R0298"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13A-MMU"/>
<attribute name="OC_FARNELL" value="1715516"/>
<attribute name="OC_NEWARK" value="15R0298"/>
</technology>
</technologies>
</device>
<device name="MU" package="20M1">
<connects>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="11"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="12"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="14"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="5"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13A-MU"/>
<attribute name="OC_FARNELL" value="1715517"/>
<attribute name="OC_NEWARK" value="15R0299"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10MU"/>
<attribute name="OC_FARNELL" value="1455134"/>
<attribute name="OC_NEWARK" value="58M3772"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T7024" prefix="IC">
<description>&lt;b&gt;Bluetooth/ISM 2.4-GHz Front-End IC&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4533.pdf</description>
<gates>
<gate name="G$1" symbol="T7024"/>
</gates>
<devices>
<device name="" package="MLF20-5X5-TH">
<connects>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="GND@3" pad="10"/>
<connect gate="G$1" pin="GND@4" pad="14"/>
<connect gate="G$1" pin="GND@5" pad="18"/>
<connect gate="G$1" pin="LNA_IN" pad="7"/>
<connect gate="G$1" pin="LNA_OUT" pad="1"/>
<connect gate="G$1" pin="PA_IN" pad="20"/>
<connect gate="G$1" pin="PU" pad="3"/>
<connect gate="G$1" pin="RAMP" pad="15"/>
<connect gate="G$1" pin="RX_ON" pad="2"/>
<connect gate="G$1" pin="R_SWITCH" pad="4"/>
<connect gate="G$1" pin="SWITCH_OUT" pad="5"/>
<connect gate="G$1" pin="V1_PA" pad="19"/>
<connect gate="G$1" pin="V2_PA@1" pad="16"/>
<connect gate="G$1" pin="V2_PA@2" pad="17"/>
<connect gate="G$1" pin="V3_PA_OUT@1" pad="11"/>
<connect gate="G$1" pin="V3_PA_OUT@2" pad="12"/>
<connect gate="G$1" pin="V3_PA_OUT@3" pad="13"/>
<connect gate="G$1" pin="VS_LNA" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA16A4" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;
&lt;h2&gt;Features&lt;/h2&gt;
&lt;ul&gt;&lt;li&gt; High-performance, Low-power 8/16-bit AVR XMEGA Microcontroller&lt;/li&gt;
&lt;li&gt; Non-Volatile Program and Data Memories&lt;/li&gt;
- 16 KB - 128 KB of In-System Self-Programmable Flash&lt;br&gt;
- 4 KB - 8 KB Boot Code Section with Independent Lock Bits&lt;br&gt;
- 1 KB - 2 KB EEPROM&lt;br&gt;
- 2 KB - 8 KB Internal SRAM
&lt;li&gt; Peripheral Features&lt;/li&gt;
- Four-channel DMA Controller with support for external requests&lt;br&gt;
- Eight-channel Event System&lt;br&gt;
- Five 16-bit Timer/Counters
&lt;ul&gt;Three Timer/Counters with 4 Output Compare or Input Capture channels&lt;/ul&gt;
&lt;ul&gt;Two Timer/Counters with 2 Output Compare or Input Capture channels&lt;/ul&gt;
&lt;ul&gt;High-Resolution Extensions on all Timer/Counters&lt;/ul&gt;
&lt;ul&gt;Advanced Waveform Extension on one Timer/Counter&lt;/ul&gt;
- Five USARTs
&lt;ul&gt;IrDA Extension on one USART&lt;/ul&gt;
- Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)&lt;br&gt;
- Two SPIs (Serial Peripheral Interfaces) peripherals&lt;br&gt;
- AES and DES Crypto Engine&lt;br&gt;
- 16-bit Real Time Counter with Separate Oscillator&lt;br&gt;
- One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter&lt;br&gt;
- One Two-channel, 12-bit, 1 Msps Digital to Analog Converter&lt;br&gt;
- Two Analog Comparators with Window compare function&lt;br&gt;
- External Interrupts on all General Purpose I/O pins&lt;br&gt;
- Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;li&gt; Special Microcontroller Features&lt;/li&gt;&lt;br&gt;
- Power-on Reset and Programmable Brown-out Detection&lt;br&gt;
- Internal and External Clock Options with PLL&lt;br&gt;
- Programmable Multi-level Interrupt Controller&lt;br&gt;
- Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby&lt;br&gt;
- Advanced Programming, Test and Debugging Interfaces
&lt;ul&gt;PDI (Program and Debug Interface) for programming, test and debugging&lt;/ul&gt;
&lt;li&gt; I/O and Packages&lt;/li&gt;
- 34 Programmable I/O Lines&lt;br&gt;
- 44 - lead TQFP&lt;br&gt;
- 44 - pad VQFN/QFN&lt;br&gt;
- 49 - ball VFBGA
&lt;li&gt; Operating Voltage&lt;/li&gt;
- 1.6 - 3.6V
&lt;li&gt; Speed performance&lt;/li&gt;
- 0 - 12 MHz @ 1.6 - 3.6V&lt;br&gt;
- 0 - 32 MHz @ 2.7 - 3.6V&lt;br&gt;&lt;/ul&gt;
&lt;p&gt;&lt;author&gt;Drawn by Dipl.-Ing. (FH) Robert Siegler&lt;/author&gt;&lt;/p&gt;
Created: 27.05.09</description>
<gates>
<gate name="G$1" symbol="XMEGA16A4"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI_CLK" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="30"/>
<connect gate="G$1" pin="GND3" pad="38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI_DATA" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0(XT2)" pad="36"/>
<connect gate="G$1" pin="PR1(XT1)" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="19"/>
<connect gate="G$1" pin="VCC2" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="M1" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="!RESET!/PDI_CLK" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="30"/>
<connect gate="G$1" pin="GND3" pad="38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI_DATA" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0(XT2)" pad="36"/>
<connect gate="G$1" pin="PR1(XT1)" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="19"/>
<connect gate="G$1" pin="VCC2" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA128A1" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;
&lt;h2&gt;Features&lt;/h2&gt;
&lt;ul&gt;&lt;li&gt;High-performance, Low-power 8/16-bit AVR XMEGA Microcontroller&lt;/li&gt;
&lt;li&gt; Non-Volatile Program and Data Memories&lt;/li&gt;
- 64K - 384K Bytes of In-System Self-Programmable Flash&lt;br&gt;
- 4K - 8K Bytes Boot Section with Independent Lock Bits&lt;br&gt;
- 2 KB - 4 KB EEPROM&lt;br&gt;
- 4 KB - 32 KB Internal SRAM
&lt;ul&gt;External Bus Interface for up to 16M bytes SRAM&lt;/ul&gt;
&lt;ul&gt;External Bus Interface for up to 128M bit SDRAM&lt;/ul&gt;
&lt;li&gt; Peripheral Features&lt;/li&gt;
- Four-channel DMA Controller with support for external requests&lt;br&gt;
- Eight-channel Event System&lt;br&gt;
- Eight 16-bit Timer/Counters
&lt;ul&gt;Four Timer/Counters with 4 Output Compare or Input Capture channels&lt;/ul&gt;
&lt;ul&gt;Four Timer/Counters with 2 Output Compare or Input Capture channels&lt;/ul&gt;
&lt;ul&gt;High-Resolution Extension on all Timer/Counters&lt;/ul&gt;
&lt;ul&gt;Advanced Waveform Extension on two Timer/Counters&lt;/ul&gt;
- Eight USARTs
&lt;ul&gt;IrDA modulation/demodulation for one USART&lt;/ul&gt;
- Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)&lt;br&gt;
- Four SPI (Serial Peripheral Interface) peripherals&lt;br&gt;
- AES and DES Crypto Engine&lt;br&gt;
- 16-bit Real Time Counter with separate Oscillator&lt;br&gt;
- Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters&lt;br&gt;
- Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters&lt;br&gt;
- Four Analog Comparators with Window compare function&lt;br&gt;
- External Interrupts on all General Purpose I/O pins&lt;br&gt;
- Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;li&gt; Special Microcontroller Features&lt;/li&gt;
- Power-on Reset and Programmable Brown-out Detection&lt;br&gt;
- Internal and External Clock Options with PLL and Prescaler&lt;br&gt;
- Programmable Multi-level Interrupt Controller&lt;br&gt;
- Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby&lt;br&gt;
- Advanced Programming, Test and Debugging Interfaces
&lt;ul&gt;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging&lt;/ul&gt;
&lt;ul&gt;PDI (Program and Debug Interface) for programming and debugging&lt;/ul&gt;
&lt;li&gt; I/O and Packages&lt;/li&gt;
- 78 Programmable I/O Lines&lt;br&gt;
- 100 - lead TQFP&lt;br&gt;
- 100 - ball CBGA&lt;br&gt;
- 100 - ball VFBGA
&lt;li&gt; Operating Voltage&lt;/li&gt;
- 1.6 - 3.6V
&lt;li&gt; Speed performance&lt;/li&gt;
- 0 - 12 MHz @ 1.6 - 3.6V&lt;br&gt;
- 0 - 32 MHz @ 2.7 - 3.6V&lt;br&gt;&lt;/ul&gt;
&lt;p&gt;&lt;author&gt;Drawn by Dipl.-Ing. (FH) Robert Siegler&lt;/author&gt;&lt;/p&gt;
Created: 27.05.09</description>
<gates>
<gate name="G$1" symbol="XMEGA128A1"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI_CLK" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4"/>
<connect gate="G$1" pin="AVCC1" pad="94"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND1" pad="13"/>
<connect gate="G$1" pin="GND2" pad="23"/>
<connect gate="G$1" pin="GND3" pad="33"/>
<connect gate="G$1" pin="GND4" pad="43"/>
<connect gate="G$1" pin="GND5" pad="53"/>
<connect gate="G$1" pin="GND6" pad="63"/>
<connect gate="G$1" pin="GND7" pad="73"/>
<connect gate="G$1" pin="GND8" pad="84"/>
<connect gate="G$1" pin="GND9" pad="93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI_DATA" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0(XT2)" pad="91"/>
<connect gate="G$1" pin="PR1(XT1)" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VCC1" pad="24"/>
<connect gate="G$1" pin="VCC2" pad="34"/>
<connect gate="G$1" pin="VCC3" pad="44"/>
<connect gate="G$1" pin="VCC4" pad="54"/>
<connect gate="G$1" pin="VCC5" pad="64"/>
<connect gate="G$1" pin="VCC6" pad="74"/>
<connect gate="G$1" pin="VCC7" pad="83"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA325P" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 32K Bytes In-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com .. doc8023.pdf</description>
<gates>
<gate name="G$1" symbol="ATMEGA325P"/>
</gates>
<devices>
<device name="" package="64M1">
<connects>
<connect gate="G$1" pin="!RESET!/PG5" pad="20"/>
<connect gate="G$1" pin="!SS!/PCINT8/PB0" pad="10"/>
<connect gate="G$1" pin="ADC0/PF0" pad="61"/>
<connect gate="G$1" pin="ADC1/PF1" pad="60"/>
<connect gate="G$1" pin="ADC2/PF2" pad="59"/>
<connect gate="G$1" pin="ADC3/PF3" pad="58"/>
<connect gate="G$1" pin="ADC4/TCK/PF4" pad="57"/>
<connect gate="G$1" pin="ADC5/TMS/PF5" pad="56"/>
<connect gate="G$1" pin="ADC6/TDO/PF6" pad="55"/>
<connect gate="G$1" pin="ADC7/TDI/PF7" pad="54"/>
<connect gate="G$1" pin="AIN1/PCINT3/PE3" pad="5"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="CLKO/PCINT7/PE7" pad="9"/>
<connect gate="G$1" pin="DI/SDA/PCINT5/PE5" pad="7"/>
<connect gate="G$1" pin="DNC" pad="1"/>
<connect gate="G$1" pin="DO/PCINT6/PE6" pad="8"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="53"/>
<connect gate="G$1" pin="GND@2" pad="63"/>
<connect gate="G$1" pin="ICP1/PD0" pad="25"/>
<connect gate="G$1" pin="INT0/PD1" pad="26"/>
<connect gate="G$1" pin="MISO/PCINT11/PB3" pad="13"/>
<connect gate="G$1" pin="MOSI/PCINT10/PB2" pad="12"/>
<connect gate="G$1" pin="OC0A/PCINT12/PB4" pad="14"/>
<connect gate="G$1" pin="OC1A/PCINT13/PB5" pad="16"/>
<connect gate="G$1" pin="OC1B/PCINT14/PB6" pad="15"/>
<connect gate="G$1" pin="OC2A/PCINT15/PB7" pad="17"/>
<connect gate="G$1" pin="PA0" pad="51"/>
<connect gate="G$1" pin="PA1" pad="50"/>
<connect gate="G$1" pin="PA2" pad="49"/>
<connect gate="G$1" pin="PA3" pad="48"/>
<connect gate="G$1" pin="PA4" pad="47"/>
<connect gate="G$1" pin="PA5" pad="46"/>
<connect gate="G$1" pin="PA6" pad="45"/>
<connect gate="G$1" pin="PA7" pad="44"/>
<connect gate="G$1" pin="PC0" pad="35"/>
<connect gate="G$1" pin="PC1" pad="36"/>
<connect gate="G$1" pin="PC2" pad="37"/>
<connect gate="G$1" pin="PC3" pad="38"/>
<connect gate="G$1" pin="PC4" pad="39"/>
<connect gate="G$1" pin="PC5" pad="40"/>
<connect gate="G$1" pin="PC6" pad="41"/>
<connect gate="G$1" pin="PC7" pad="42"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PG0" pad="33"/>
<connect gate="G$1" pin="PG1" pad="34"/>
<connect gate="G$1" pin="PG2" pad="43"/>
<connect gate="G$1" pin="RXD/PCINT0/PE0" pad="2"/>
<connect gate="G$1" pin="SCK/PCINT9/PB1" pad="11"/>
<connect gate="G$1" pin="T0/PG4" pad="19"/>
<connect gate="G$1" pin="T1/PG3" pad="18"/>
<connect gate="G$1" pin="TOSC1/XTAL1" pad="24"/>
<connect gate="G$1" pin="TOSC2/XTAL2" pad="23"/>
<connect gate="G$1" pin="TXD/PCINT1/PE1" pad="3"/>
<connect gate="G$1" pin="USCK/SCL/PCINT4/PE4" pad="6"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XCK/AIN0/PCINT2/PE2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA325PV-10AU"/>
<attribute name="OC_FARNELL" value="1636939"/>
<attribute name="OC_NEWARK" value="03P2025"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB642D" prefix="IC">
<description>&lt;b&gt;Flash-Memory 64-Megabit&lt;/b&gt; 2 .7-volt, Dual-interface, DataFlash&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc3542.pdf</description>
<gates>
<gate name="G$1" symbol="AT45DB642D"/>
</gates>
<devices>
<device name="" package="28T-TSOP-1">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="!RESET" pad="2"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GNDP" pad="21"/>
<connect gate="G$1" pin="I/O0" pad="17"/>
<connect gate="G$1" pin="I/O1" pad="18"/>
<connect gate="G$1" pin="I/O2" pad="19"/>
<connect gate="G$1" pin="I/O3" pad="20"/>
<connect gate="G$1" pin="I/O4" pad="23"/>
<connect gate="G$1" pin="I/O5" pad="24"/>
<connect gate="G$1" pin="I/O6" pad="25"/>
<connect gate="G$1" pin="I/O7" pad="26"/>
<connect gate="G$1" pin="RDY/!BUSY" pad="1"/>
<connect gate="G$1" pin="SCK/CLK" pad="12"/>
<connect gate="G$1" pin="SER/!BYTE" pad="16"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="SO" pad="14"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VCCP" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT45DB642D-TU"/>
<attribute name="OC_FARNELL" value="1095799"/>
<attribute name="OC_NEWARK" value="51P1801"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA644-*PU" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 64K Bytes In-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2593.pdf</description>
<gates>
<gate name="G$1" symbol="ATMEGA644-20PU"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!RESET" pad="9"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="31"/>
<connect gate="G$1" pin="PCINT0/ADC0_PA0" pad="40"/>
<connect gate="G$1" pin="PCINT1/ADC1_PA1" pad="39"/>
<connect gate="G$1" pin="PCINT10/INT2/AIN0_PB2" pad="3"/>
<connect gate="G$1" pin="PCINT11/OC0A/AIN1_PB3" pad="4"/>
<connect gate="G$1" pin="PCINT12/OC0B/SS_PB4" pad="5"/>
<connect gate="G$1" pin="PCINT13/MOSI_PB5" pad="6"/>
<connect gate="G$1" pin="PCINT14/MISO_PB6" pad="7"/>
<connect gate="G$1" pin="PCINT15/SCK_PB7" pad="8"/>
<connect gate="G$1" pin="PCINT16/SCL_PC0" pad="22"/>
<connect gate="G$1" pin="PCINT17/SDA_PC1" pad="23"/>
<connect gate="G$1" pin="PCINT18/TCK_PC2" pad="24"/>
<connect gate="G$1" pin="PCINT19/TMS_PC3" pad="25"/>
<connect gate="G$1" pin="PCINT2/ADC2_PA2" pad="38"/>
<connect gate="G$1" pin="PCINT20/TDO_PC4" pad="26"/>
<connect gate="G$1" pin="PCINT21/TDI_PC5" pad="27"/>
<connect gate="G$1" pin="PCINT22/TOSC1_PC6" pad="28"/>
<connect gate="G$1" pin="PCINT23/TOSC2_PC7" pad="29"/>
<connect gate="G$1" pin="PCINT24/RXD0_PD0" pad="14"/>
<connect gate="G$1" pin="PCINT25/TXD0_PD1" pad="15"/>
<connect gate="G$1" pin="PCINT26/INT0_PD2" pad="16"/>
<connect gate="G$1" pin="PCINT27/INT1_PD3" pad="17"/>
<connect gate="G$1" pin="PCINT28/OC1B_PD4" pad="18"/>
<connect gate="G$1" pin="PCINT29/OC1A_PD5" pad="19"/>
<connect gate="G$1" pin="PCINT3/ADC3_PA3" pad="37"/>
<connect gate="G$1" pin="PCINT30/OC2B/ICP_PD6" pad="20"/>
<connect gate="G$1" pin="PCINT31/OC2A_PD7" pad="21"/>
<connect gate="G$1" pin="PCINT4/ADC4_PA4" pad="36"/>
<connect gate="G$1" pin="PCINT5/ADC5_PA5" pad="35"/>
<connect gate="G$1" pin="PCINT6/ADC6_PA6" pad="34"/>
<connect gate="G$1" pin="PCINT7/ADC7_PA7" pad="33"/>
<connect gate="G$1" pin="PCINT8/XCK0/T0_PB0" pad="1"/>
<connect gate="G$1" pin="PCINT9/CLKO/T1_PB1" pad="2"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644V-10PU"/>
<attribute name="OC_FARNELL" value="1288342"/>
<attribute name="OC_NEWARK" value="23M5062"/>
</technology>
<technology name="20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644-20PU"/>
<attribute name="OC_FARNELL" value="1288340"/>
<attribute name="OC_NEWARK" value="23M5060"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB161D" prefix="IC">
<description>&lt;b&gt;16-megabit 2.5V or 2.7V DataFlash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc3500.pdf</description>
<gates>
<gate name="G$1" symbol="AT45DB161VFN8"/>
</gates>
<devices>
<device name="-MU" package="VDFN-8">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="!RESET" pad="3"/>
<connect gate="G$1" pin="!WP" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ATMEL"/>
<attribute name="MPN" value="AT45DB161D-SU"/>
<attribute name="OC_FARNELL" value="1455040"/>
</technology>
</technologies>
</device>
<device name="-SU" package="8S2">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="!RESET" pad="3"/>
<connect gate="G$1" pin="!WP" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ATMEL"/>
<attribute name="MPN" value="AT45DB161D-SU"/>
<attribute name="OC_FARNELL" value="1455040"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA64C3" prefix="IC" uservalue="yes">
<description>High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
 Nonvolatile program and data memories
 64K - 256KBytes of In-System Self-Programmable Flash
 4K - 8KBytes Boot Code Section with Independent Lock Bits
 2K - 4KBytes EEPROM
 4K - 16KBytes Internal SRAM
 Peripheral features
 Four-channel event system
 Five 16-bit timer/counters
 Four timer/counters with four output compare or input capture channels
 One timer/counter with two output compare or input capture channels
 High resolution extension on two timer/counters
 Advanced waveform extension (AWeX) on one timer/counter
 One USB device interface
 USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
 32 Endpoints with full configuration flexibility
 Three USARTs with IrDA support for one USART
 Two two-wire interfaces with dual address match (I2C and SMBus compatible)
 Two serial peripheral interfaces (SPIs)
 CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
 16-bit real time counter (RTC) with separate oscillator
 One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
 Two Analog Comparators with window compare function, and current sources
 External interrupts on all general purpose I/O pins
 Programmable watchdog timer with separate on-chip ultra low power oscillator
 QTouch® library support
 Capacitive touch buttons, sliders and wheels
 Special microcontroller features
 Power-on reset and programmable brown-out detection
 Internal and external clock options with PLL and prescaler
 Programmable multilevel interrupt controller
 Five sleep modes
 Programming and debug interface
 PDI (program and debug interface)
 I/O and packages
 50 programmable I/O pins
 64-lead TQFP
 64-pad QFN
 Operating voltage
 1.6 – 3.6V
 Operating frequency
 0 – 12MHz from 1.6V
 0 – 32MHz from 2.7V</description>
<gates>
<gate name="G$1" symbol="ATXMEGA64C3"/>
</gates>
<devices>
<device name="" package="VQFN64-9X9X1">
<connects>
<connect gate="G$1" pin="14GND" pad="14"/>
<connect gate="G$1" pin="15VDD" pad="15"/>
<connect gate="G$1" pin="24GND" pad="24"/>
<connect gate="G$1" pin="25VDD" pad="25"/>
<connect gate="G$1" pin="34GND" pad="34"/>
<connect gate="G$1" pin="35VCC" pad="35"/>
<connect gate="G$1" pin="44GND" pad="44"/>
<connect gate="G$1" pin="45VCC" pad="45"/>
<connect gate="G$1" pin="52GND" pad="52"/>
<connect gate="G$1" pin="53VCC" pad="53"/>
<connect gate="G$1" pin="56PDI" pad="56"/>
<connect gate="G$1" pin="57RESET/PDI" pad="57"/>
<connect gate="G$1" pin="58PRO" pad="58"/>
<connect gate="G$1" pin="59PR1" pad="59"/>
<connect gate="G$1" pin="60GND" pad="60"/>
<connect gate="G$1" pin="61AVCC" pad="61"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TQFP64" package="TQFP64">
<connects>
<connect gate="G$1" pin="14GND" pad="14"/>
<connect gate="G$1" pin="15VDD" pad="15"/>
<connect gate="G$1" pin="24GND" pad="24"/>
<connect gate="G$1" pin="25VDD" pad="25"/>
<connect gate="G$1" pin="34GND" pad="34"/>
<connect gate="G$1" pin="35VCC" pad="35"/>
<connect gate="G$1" pin="44GND" pad="44"/>
<connect gate="G$1" pin="45VCC" pad="45"/>
<connect gate="G$1" pin="52GND" pad="52"/>
<connect gate="G$1" pin="53VCC" pad="53"/>
<connect gate="G$1" pin="56PDI" pad="56"/>
<connect gate="G$1" pin="57RESET/PDI" pad="57"/>
<connect gate="G$1" pin="58PRO" pad="58"/>
<connect gate="G$1" pin="59PR1" pad="59"/>
<connect gate="G$1" pin="60GND" pad="60"/>
<connect gate="G$1" pin="61AVCC" pad="61"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT32UC3A0128/0256/0512" prefix="U">
<description>AT32UC3A0128/0256/0512</description>
<gates>
<gate name="P" symbol="AT32UC3A0XXX-P"/>
<gate name="&gt;NAME" symbol="AT32UC3A0XXX-IO"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="&gt;NAME" pin="!RESET" pad="23"/>
<connect gate="&gt;NAME" pin="DAC-DATAN[0]/EIM-EXTINT[5]/USART0-CTS/PA04" pad="34"/>
<connect gate="&gt;NAME" pin="DAC-DATAN[0]/MACB-TXD[1]/PB03" pad="98"/>
<connect gate="&gt;NAME" pin="DAC-DATAN[1]/EIM-EXTINT[3]/ADC-AD[3]/PA24" pad="76"/>
<connect gate="&gt;NAME" pin="DAC-DATAN[1]/MACB-RXD[1]/PB06" pad="104"/>
<connect gate="&gt;NAME" pin="DAC-DATA[0]/EIM-EXTINT[4]/USART0-RTS/PA03" pad="32"/>
<connect gate="&gt;NAME" pin="DAC-DATA[0]/MACB-TXD[0]/PB02" pad="96"/>
<connect gate="&gt;NAME" pin="DAC-DATA[1]/EIM-EXTINT[2]/ADC-AD[2]/PA23" pad="75"/>
<connect gate="&gt;NAME" pin="DAC-DATA[1]/MACB-RXD[0]/PB05" pad="102"/>
<connect gate="&gt;NAME" pin="DM" pad="70"/>
<connect gate="&gt;NAME" pin="DP" pad="71"/>
<connect gate="&gt;NAME" pin="EBI-ADDR[20]/EIM-SCAN[1]/ADC-AD[5]/PA26" pad="78"/>
<connect gate="&gt;NAME" pin="EBI-ADDR[20]/SPI1-SCK/SSC-TX_CLOCK/PA15" pad="57"/>
<connect gate="&gt;NAME" pin="EBI-ADDR[21]/EIM-SCAN[2]/ADC-AD[6]/PA27" pad="79"/>
<connect gate="&gt;NAME" pin="EBI-ADDR[21]/SPI1-MOSI/SSC-TX_DATA/PA16" pad="58"/>
<connect gate="&gt;NAME" pin="EBI-ADDR[22]/EIM-SCAN[3]/ADC-AD[7]/PA28" pad="80"/>
<connect gate="&gt;NAME" pin="EBI-ADDR[22]/SPI1-MISO/SSC-RX_DATA/PA17" pad="60"/>
<connect gate="&gt;NAME" pin="EBI-ADDR[23]/USB-USB_VBOF/MACB-RX_CLK/PB17" pad="139"/>
<connect gate="&gt;NAME" pin="EBI-CAS/TC-CLK1/MACB-RXD[2]/PB13" pad="126"/>
<connect gate="&gt;NAME" pin="EBI-NCS[0]/EIM-SCAN[0]/ADC-AD[4]/PA25" pad="77"/>
<connect gate="&gt;NAME" pin="EBI-NCS[0]/SPI1-NPCS[0]/SSC-TX_FRAME_SYNC/PA14" pad="56"/>
<connect gate="&gt;NAME" pin="EBI-NCS[2]/PM-GCLK[1]/USART2-RXD/PB29" pad="20"/>
<connect gate="&gt;NAME" pin="EBI-NCS[3]/USART3-CLK/MACB-CRS/PB04" pad="100"/>
<connect gate="&gt;NAME" pin="EBI-NWAIT/PM-GCLK[3]/USART2-CLK/PB31" pad="22"/>
<connect gate="&gt;NAME" pin="EBI-RAS/TC-CLK0/MACB-TX_ER/PB12" pad="121"/>
<connect gate="&gt;NAME" pin="EBI-SDA10/USB-USB_ID/MACB-COL/PB16" pad="136"/>
<connect gate="&gt;NAME" pin="EBI-SDCK/USART3-RXD/MACB-TXD[2]/PB10" pad="115"/>
<connect gate="&gt;NAME" pin="EBI-SDCKE/USART3-TXD/MACB-TXD[3]/PB11" pad="119"/>
<connect gate="&gt;NAME" pin="EBI-SDCS/PM-GCLK[2]/USART2-TXD/PB30" pad="21"/>
<connect gate="&gt;NAME" pin="EBI-SDWE/TC-CLK2/MACB-RXD[3]/PB14" pad="127"/>
<connect gate="&gt;NAME" pin="EIM-EXTINT[6]/SPI0-NPCS[0]/PA10" pad="48"/>
<connect gate="&gt;NAME" pin="EIM-EXTINT[7]/SPI0-NPCS[1]/USART1-RTS/PA08" pad="45"/>
<connect gate="&gt;NAME" pin="EIM-SCAN[4]/PM-GCLK[0]/PWM-PWM[0]/PB19" pad="143"/>
<connect gate="&gt;NAME" pin="EIM-SCAN[5]/PM-GCLK[1]/PWM-PWM[1]/PB20" pad="3"/>
<connect gate="&gt;NAME" pin="EIM-SCAN[6]/PM-GCLK[2]/PWM-PWM[2]/PB21" pad="5"/>
<connect gate="&gt;NAME" pin="EIM-SCAN[7]/PM-GCLK[3]/PWM-PWM[3]/PB22" pad="6"/>
<connect gate="&gt;NAME" pin="MACB-MDC/PB08" pad="111"/>
<connect gate="&gt;NAME" pin="MACB-MDIO/PB09" pad="113"/>
<connect gate="&gt;NAME" pin="MACB-RX_DV/PB15" pad="134"/>
<connect gate="&gt;NAME" pin="MACB-RX_ER/PB07" pad="106"/>
<connect gate="&gt;NAME" pin="MACB-WOL/SPI0-NPCS[2]/USART1-CTS/PA09" pad="47"/>
<connect gate="&gt;NAME" pin="MACB-WOL/SPI1-NPCS[1]/SSC-RX_CLOCK/PA18" pad="62"/>
<connect gate="&gt;NAME" pin="NC@49" pad="49"/>
<connect gate="&gt;NAME" pin="PC00/XIN32" pad="85"/>
<connect gate="&gt;NAME" pin="PC01/XOUT32" pad="86"/>
<connect gate="&gt;NAME" pin="PC02/XIN0" pad="124"/>
<connect gate="&gt;NAME" pin="PC03/XOUT0" pad="125"/>
<connect gate="&gt;NAME" pin="PC04/XIN1" pad="132"/>
<connect gate="&gt;NAME" pin="PC05/XOUT1" pad="133"/>
<connect gate="&gt;NAME" pin="PWM-PWM[4]/TC-A2/PB27" pad="15"/>
<connect gate="&gt;NAME" pin="PWM-PWM[4]/USART1-RXD/PA05" pad="39"/>
<connect gate="&gt;NAME" pin="PWM-PWM[5]/TC-B2/PB28" pad="19"/>
<connect gate="&gt;NAME" pin="PWM-PWM[5]/USART1-TXD/PA06" pad="41"/>
<connect gate="&gt;NAME" pin="PWM-PWM[6]/ADC-TRIGGER/MACB-SPEED/PB18" pad="141"/>
<connect gate="&gt;NAME" pin="PX00/EBI-DATA[10]/USART0-RXD" pad="1"/>
<connect gate="&gt;NAME" pin="PX01/EBI-DATA[9]/USART0-TXD" pad="2"/>
<connect gate="&gt;NAME" pin="PX02/EBI-DATA[8]/USART0-CTS" pad="4"/>
<connect gate="&gt;NAME" pin="PX03/EBI-DATA[7]/USART0-RTS" pad="10"/>
<connect gate="&gt;NAME" pin="PX04/EBI-DATA[6]/USART1-RXD" pad="12"/>
<connect gate="&gt;NAME" pin="PX05/EBI-DATA[5]/USART1-TXD" pad="24"/>
<connect gate="&gt;NAME" pin="PX06/EBI-DATA[4]/USART1-CTS" pad="26"/>
<connect gate="&gt;NAME" pin="PX07/EBI-DATA[3]/USART1-RTS" pad="31"/>
<connect gate="&gt;NAME" pin="PX08/EBI-DATA[2]/USART3-RXD" pad="33"/>
<connect gate="&gt;NAME" pin="PX09/EBI-DATA[1]/USART3-TXD" pad="35"/>
<connect gate="&gt;NAME" pin="PX10/EBI-DATA[0]/USART2-RXD" pad="38"/>
<connect gate="&gt;NAME" pin="PX11/EBI-NWE1/USART2-TXD" pad="40"/>
<connect gate="&gt;NAME" pin="PX12/EBI-NWE0/USART2-CTS" pad="42"/>
<connect gate="&gt;NAME" pin="PX13/EBI-NRD/USART2-RTS" pad="44"/>
<connect gate="&gt;NAME" pin="PX14/EBI-NCS[1]/TC-A0" pad="46"/>
<connect gate="&gt;NAME" pin="PX15/EBI-ADDR[19]/USART3-RTS/TC-B0" pad="59"/>
<connect gate="&gt;NAME" pin="PX16/EBI-ADDR[18]/USART3-CTS/TC-A1" pad="61"/>
<connect gate="&gt;NAME" pin="PX17/EBI-ADDR[17]/TC-B1" pad="63"/>
<connect gate="&gt;NAME" pin="PX18/EBI-ADDR[16]/TC-A2" pad="65"/>
<connect gate="&gt;NAME" pin="PX19/EBI-ADDR[15]/EIM-SCAN[0]/TC-B2" pad="67"/>
<connect gate="&gt;NAME" pin="PX20/EBI-ADDR[14]/EIM-SCAN[1]/TC-CLK0" pad="87"/>
<connect gate="&gt;NAME" pin="PX21/EBI-ADDR[13]/EIM-SCAN[2]/TC-CLK1" pad="89"/>
<connect gate="&gt;NAME" pin="PX22/EBI-ADDR[12]/EIM-SCAN[3]/TC-CLK2" pad="91"/>
<connect gate="&gt;NAME" pin="PX23/EBI-ADDR[11]/EIM-SCAN[4]" pad="95"/>
<connect gate="&gt;NAME" pin="PX24/EBI-ADDR[10]/EIM-SCAN[5]" pad="97"/>
<connect gate="&gt;NAME" pin="PX25/EBI-ADDR[9]/EIM-SCAN[6]" pad="99"/>
<connect gate="&gt;NAME" pin="PX26/EBI-ADDR[8]/EIM-SCAN[7]" pad="101"/>
<connect gate="&gt;NAME" pin="PX27/EBI-ADDR[7]/SPI0-MISO" pad="103"/>
<connect gate="&gt;NAME" pin="PX28/EBI-ADDR[6]/SPI0-MOSI" pad="105"/>
<connect gate="&gt;NAME" pin="PX29/EBI-ADDR[5]/SPI0-SCK" pad="107"/>
<connect gate="&gt;NAME" pin="PX30/EBI-ADDR[4]/SPI0-NPCS[0]" pad="110"/>
<connect gate="&gt;NAME" pin="PX31/EBI-ADDR[3]/SPI0-NPCS[1]" pad="112"/>
<connect gate="&gt;NAME" pin="PX32/EBI-ADDR[2]/SPI0-NPCS[2]" pad="114"/>
<connect gate="&gt;NAME" pin="PX33/EBI-ADDR[1]/SPI0-NPCS[3]" pad="118"/>
<connect gate="&gt;NAME" pin="PX34/EBI-ADDR[0]/SPI1-MISO" pad="120"/>
<connect gate="&gt;NAME" pin="PX35/EBI-DATA[15]/SPI1-MOSI" pad="135"/>
<connect gate="&gt;NAME" pin="PX36/EBI-DATA[14]/SPI1-SCK" pad="137"/>
<connect gate="&gt;NAME" pin="PX37/EBI-DATA[13]/SPI1-NPCS[0]" pad="140"/>
<connect gate="&gt;NAME" pin="PX38/EBI-DATA[12]/SPI1-NPCS[1]" pad="142"/>
<connect gate="&gt;NAME" pin="PX39/EBI-DATA[11]/SPI1-NPCS[2]" pad="144"/>
<connect gate="&gt;NAME" pin="SPI0-NPCS[3]/PM-GCLK[0]/USART1-CLK/PA07" pad="43"/>
<connect gate="&gt;NAME" pin="SPI0-SCK/PA13" pad="54"/>
<connect gate="&gt;NAME" pin="SPI1-NPCS[2]/SSC-RX_FRAME_SYNC/PA19" pad="64"/>
<connect gate="&gt;NAME" pin="SPI1-NPCS[3]/EIM-EXTINT[8]/PA20" pad="66"/>
<connect gate="&gt;NAME" pin="TC-CLK0/USART0-RXD/PA00" pad="25"/>
<connect gate="&gt;NAME" pin="TC-CLK1/USART0-TXD/PA01" pad="27"/>
<connect gate="&gt;NAME" pin="TC-CLK2/USART0-CLK/PA02" pad="30"/>
<connect gate="&gt;NAME" pin="TCK" pad="129"/>
<connect gate="&gt;NAME" pin="TDI" pad="131"/>
<connect gate="&gt;NAME" pin="TDO" pad="130"/>
<connect gate="&gt;NAME" pin="TMS" pad="128"/>
<connect gate="&gt;NAME" pin="USART1-DCD/TC-A0/PB23" pad="9"/>
<connect gate="&gt;NAME" pin="USART1-DSR/TC-B0/PB24" pad="11"/>
<connect gate="&gt;NAME" pin="USART1-DTR/TC-A1/PB25" pad="13"/>
<connect gate="&gt;NAME" pin="USART1-RI/TC-B1/PB26" pad="14"/>
<connect gate="&gt;NAME" pin="USART2-CTS/TWI-SCL/PA30" pad="123"/>
<connect gate="&gt;NAME" pin="USART2-RTS/TWI-SDA/PA29" pad="122"/>
<connect gate="&gt;NAME" pin="USART3-CTS/USART2-CTS/MACB-TX_EN/PB01" pad="90"/>
<connect gate="&gt;NAME" pin="USART3-RTS/USART2-RTS/MACB-TX_CLK/PB00" pad="88"/>
<connect gate="&gt;NAME" pin="USB-USB_ID/EIM-EXTINT[0]/ADC-AD[0]/PA21" pad="73"/>
<connect gate="&gt;NAME" pin="USB-USB_ID/SPI0-MISO/PA11" pad="50"/>
<connect gate="&gt;NAME" pin="USB-USB_VBOF/EIM-EXTINT[1]/ADC-AD[1]/PA22" pad="74"/>
<connect gate="&gt;NAME" pin="USB-USB_VBOF/SPI0-MOSI/PA12" pad="53"/>
<connect gate="&gt;NAME" pin="VBUS" pad="68"/>
<connect gate="P" pin="ADVREF" pad="82"/>
<connect gate="P" pin="GND@109" pad="109"/>
<connect gate="P" pin="GND@117" pad="117"/>
<connect gate="P" pin="GND@18" pad="18"/>
<connect gate="P" pin="GND@28" pad="28"/>
<connect gate="P" pin="GND@37" pad="37"/>
<connect gate="P" pin="GND@52" pad="52"/>
<connect gate="P" pin="GND@72" pad="72"/>
<connect gate="P" pin="GND@8" pad="8"/>
<connect gate="P" pin="GND@94" pad="94"/>
<connect gate="P" pin="GNDANA" pad="83"/>
<connect gate="P" pin="VDDANA" pad="81"/>
<connect gate="P" pin="VDDCORE@138" pad="138"/>
<connect gate="P" pin="VDDCORE@29" pad="29"/>
<connect gate="P" pin="VDDCORE@51" pad="51"/>
<connect gate="P" pin="VDDCORE@55" pad="55"/>
<connect gate="P" pin="VDDIN" pad="17"/>
<connect gate="P" pin="VDDIO@108" pad="108"/>
<connect gate="P" pin="VDDIO@116" pad="116"/>
<connect gate="P" pin="VDDIO@36" pad="36"/>
<connect gate="P" pin="VDDIO@69" pad="69"/>
<connect gate="P" pin="VDDIO@7" pad="7"/>
<connect gate="P" pin="VDDIO@92" pad="92"/>
<connect gate="P" pin="VDDIO@93" pad="93"/>
<connect gate="P" pin="VDDOUT" pad="16"/>
<connect gate="P" pin="VDDPLL" pad="84"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT32UC3A1512/1256/1128" prefix="U">
<description>AT32UC3A1512/1256/1128</description>
<gates>
<gate name="NAME" symbol="AT32UC3A1XXX"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="NAME" pin="!RESET" pad="18"/>
<connect gate="NAME" pin="ADVREF" pad="60"/>
<connect gate="NAME" pin="DAC-DATAN[0]/EIM-EXTINT[5]/USART0-CTS/PA04" pad="25"/>
<connect gate="NAME" pin="DAC-DATAN[0]/MACB-TXD[1]/PB03" pad="71"/>
<connect gate="NAME" pin="DAC-DATAN[1]/EIM-EXTINT[3]/ADC-AD[3]/PA24" pad="54"/>
<connect gate="NAME" pin="DAC-DATAN[1]/MACB-RXD[1]/PB06" pad="74"/>
<connect gate="NAME" pin="DAC-DATA[0]/EIM-EXTINT[4]/USART0-RTS/PA03" pad="24"/>
<connect gate="NAME" pin="DAC-DATA[0]/MACB-TXD[0]/PB02" pad="70"/>
<connect gate="NAME" pin="DAC-DATA[1]/EIM-EXTINT[2]/ADC-AD[2]/PA23" pad="53"/>
<connect gate="NAME" pin="DAC-DATA[1]/MACB-RXD[0]/PB05" pad="73"/>
<connect gate="NAME" pin="DM" pad="48"/>
<connect gate="NAME" pin="DP" pad="49"/>
<connect gate="NAME" pin="EBI-ADDR[20]/EIM-SCAN[1]/ADC-AD[5]/PA26" pad="56"/>
<connect gate="NAME" pin="EBI-ADDR[20]/SPI1-SCK/SSC-TX_CLOCK/PA15" pad="40"/>
<connect gate="NAME" pin="EBI-ADDR[21]/EIM-SCAN[2]/ADC-AD[6]/PA27" pad="57"/>
<connect gate="NAME" pin="EBI-ADDR[21]/SPI1-MOSI/SSC-TX_DATA/PA16" pad="41"/>
<connect gate="NAME" pin="EBI-ADDR[22]/EIM-SCAN[3]/ADC-AD[7]/PA28" pad="58"/>
<connect gate="NAME" pin="EBI-ADDR[22]/SPI1-MISO/SSC-RX_DATA/PA17" pad="42"/>
<connect gate="NAME" pin="EBI-ADDR[23]/USB-USB_VBOF/MACB-RX_CLK/PB17" pad="98"/>
<connect gate="NAME" pin="EBI-CAS/TC-CLK1/MACB-RXD[2]/PB13" pad="87"/>
<connect gate="NAME" pin="EBI-NCS[0]/EIM-SCAN[0]/ADC-AD[4]/PA25" pad="55"/>
<connect gate="NAME" pin="EBI-NCS[0]/SPI1-NPCS[0]/SSC-TX_FRAME_SYNC/PA14" pad="39"/>
<connect gate="NAME" pin="EBI-NCS[2]/PM-GCLK[1]/USART2-RXD/PB29" pad="15"/>
<connect gate="NAME" pin="EBI-NCS[3]/USART3-CLK/MACB-CRS/PB04" pad="72"/>
<connect gate="NAME" pin="EBI-NWAIT/PM-GCLK[3]/USART2-CLK/PB31" pad="17"/>
<connect gate="NAME" pin="EBI-RAS/TC-CLK0/MACB-TX_ER/PB12" pad="82"/>
<connect gate="NAME" pin="EBI-SDA10/USB-USB_ID/MACB-COL/PB16" pad="96"/>
<connect gate="NAME" pin="EBI-SDCK/USART3-RXD/MACB-TXD[2]/PB10" pad="78"/>
<connect gate="NAME" pin="EBI-SDCKE/USART3-TXD/MACB-TXD[3]/PB11" pad="81"/>
<connect gate="NAME" pin="EBI-SDCS/PM-GCLK[2]/USART2-TXD/PB30" pad="16"/>
<connect gate="NAME" pin="EBI-SDWE/TC-CLK2/MACB-RXD[3]/PB14" pad="88"/>
<connect gate="NAME" pin="EIM-EXTINT[6]/SPI0-NPCS[0]/PA10" pad="31"/>
<connect gate="NAME" pin="EIM-EXTINT[7]/SPI0-NPCS[1]/USART1-RTS/PA08" pad="29"/>
<connect gate="NAME" pin="EIM-SCAN[4]/PM-GCLK[0]/PWM-PWM[0]/PB19" pad="100"/>
<connect gate="NAME" pin="EIM-SCAN[5]/PM-GCLK[1]/PWM-PWM[1]/PB20" pad="1"/>
<connect gate="NAME" pin="EIM-SCAN[6]/PM-GCLK[2]/PWM-PWM[2]/PB21" pad="2"/>
<connect gate="NAME" pin="EIM-SCAN[7]/PM-GCLK[3]/PWM-PWM[3]/PB22" pad="3"/>
<connect gate="NAME" pin="GND@13" pad="13"/>
<connect gate="NAME" pin="GND@21" pad="21"/>
<connect gate="NAME" pin="GND@35" pad="35"/>
<connect gate="NAME" pin="GND@5" pad="5"/>
<connect gate="NAME" pin="GND@50" pad="50"/>
<connect gate="NAME" pin="GND@69" pad="69"/>
<connect gate="NAME" pin="GND@80" pad="80"/>
<connect gate="NAME" pin="GNDANA" pad="61"/>
<connect gate="NAME" pin="MACB-MDC/PB08" pad="76"/>
<connect gate="NAME" pin="MACB-MDIO/PB09" pad="77"/>
<connect gate="NAME" pin="MACB-RX_DV/PB15" pad="95"/>
<connect gate="NAME" pin="MACB-RX_ER/PB07" pad="75"/>
<connect gate="NAME" pin="MACB-WOL/SPI0-NPCS[2]/USART1-CTS/PA09" pad="30"/>
<connect gate="NAME" pin="MACB-WOL/SPI1-NPCS[1]/SSC-RX_CLOCK/PA18" pad="43"/>
<connect gate="NAME" pin="NC@32" pad="32"/>
<connect gate="NAME" pin="PC00/XIN32" pad="63"/>
<connect gate="NAME" pin="PC01/XOUT32" pad="64"/>
<connect gate="NAME" pin="PC02/XIN0" pad="85"/>
<connect gate="NAME" pin="PC03/XOUT0" pad="86"/>
<connect gate="NAME" pin="PC04/XIN1" pad="93"/>
<connect gate="NAME" pin="PC05/XOUT1" pad="94"/>
<connect gate="NAME" pin="PWM-PWM[4]/TC-A2/PB27" pad="10"/>
<connect gate="NAME" pin="PWM-PWM[4]/USART1-RXD/PA05" pad="26"/>
<connect gate="NAME" pin="PWM-PWM[5]/TC-B2/PB28" pad="14"/>
<connect gate="NAME" pin="PWM-PWM[5]/USART1-TXD/PA06" pad="27"/>
<connect gate="NAME" pin="PWM-PWM[6]/ADC-TRIGGER/MACB-SPEED/PB18" pad="99"/>
<connect gate="NAME" pin="SPI0-NPCS[3]/PM-GCLK[0]/USART1-CLK/PA07" pad="28"/>
<connect gate="NAME" pin="SPI0-SCK/PA13" pad="37"/>
<connect gate="NAME" pin="SPI1-NPCS[2]/SSC-RX_FRAME_SYNC/PA19" pad="44"/>
<connect gate="NAME" pin="SPI1-NPCS[3]/EIM-EXTINT[8]/PA20" pad="45"/>
<connect gate="NAME" pin="TC-CLK0/USART0-RXD/PA00" pad="19"/>
<connect gate="NAME" pin="TC-CLK1/USART0-TXD/PA01" pad="20"/>
<connect gate="NAME" pin="TC-CLK2/USART0-CLK/PA02" pad="23"/>
<connect gate="NAME" pin="TCK" pad="90"/>
<connect gate="NAME" pin="TDI" pad="92"/>
<connect gate="NAME" pin="TDO" pad="91"/>
<connect gate="NAME" pin="TMS" pad="89"/>
<connect gate="NAME" pin="USART1-DCD/TC-A0/PB23" pad="6"/>
<connect gate="NAME" pin="USART1-DSR/TC-B0/PB24" pad="7"/>
<connect gate="NAME" pin="USART1-DTR/TC-A1/PB25" pad="8"/>
<connect gate="NAME" pin="USART1-RI/TC-B1/PB26" pad="9"/>
<connect gate="NAME" pin="USART2-CTS/TWI-SCL/PA30" pad="84"/>
<connect gate="NAME" pin="USART2-RTS/TWI-SDA/PA29" pad="83"/>
<connect gate="NAME" pin="USART3-CTS/USART2-CTS/MACB-TX_EN/PB01" pad="66"/>
<connect gate="NAME" pin="USART3-RTS/USART2-RTS/MACB-TX_CLK/PB00" pad="65"/>
<connect gate="NAME" pin="USB-USB_ID/EIM-EXTINT[0]/ADC-AD[0]/PA21" pad="51"/>
<connect gate="NAME" pin="USB-USB_ID/SPI0-MISO/PA11" pad="33"/>
<connect gate="NAME" pin="USB-USB_VBOF/EIM-EXTINT[1]/ADC-AD[1]/PA22" pad="52"/>
<connect gate="NAME" pin="USB-USB_VBOF/SPI0-MOSI/PA12" pad="36"/>
<connect gate="NAME" pin="VBUS" pad="46"/>
<connect gate="NAME" pin="VDDANA" pad="59"/>
<connect gate="NAME" pin="VDDCORE@22" pad="22"/>
<connect gate="NAME" pin="VDDCORE@34" pad="34"/>
<connect gate="NAME" pin="VDDCORE@38" pad="38"/>
<connect gate="NAME" pin="VDDCORE@97" pad="97"/>
<connect gate="NAME" pin="VDDIN" pad="12"/>
<connect gate="NAME" pin="VDDIO@4" pad="4"/>
<connect gate="NAME" pin="VDDIO@47" pad="47"/>
<connect gate="NAME" pin="VDDIO@67" pad="67"/>
<connect gate="NAME" pin="VDDIO@68" pad="68"/>
<connect gate="NAME" pin="VDDIO@79" pad="79"/>
<connect gate="NAME" pin="VDDOUT" pad="11"/>
<connect gate="NAME" pin="VDDPLL" pad="62"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT32UC3B064/0128/0256" prefix="U">
<description>AT32UC3B0128/0256/0512</description>
<gates>
<gate name="NAME" symbol="AT32UC3B0XXX"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="NAME" pin="!RESET" pad="63"/>
<connect gate="NAME" pin="ADVREF" pad="18"/>
<connect gate="NAME" pin="GND@1" pad="1"/>
<connect gate="NAME" pin="GND@17" pad="17"/>
<connect gate="NAME" pin="GND@23" pad="23"/>
<connect gate="NAME" pin="GND@49" pad="49"/>
<connect gate="NAME" pin="PA03/GPIO3/ADC0/GCLK0/USB_ID" pad="9"/>
<connect gate="NAME" pin="PA04/GPIO4/ADC1/USB_VBOF" pad="10"/>
<connect gate="NAME" pin="PA05/GPIO5/EXTINT0/ADC2/USART1-DCD" pad="11"/>
<connect gate="NAME" pin="PA06/GPIO6/ADC3/USART1-DSR" pad="12"/>
<connect gate="NAME" pin="PA07/GPIO7/PWM0/ADC4/USART1-DTR" pad="13"/>
<connect gate="NAME" pin="PA08/GPIO8/PWM1/ADC5/USART1-RI" pad="14"/>
<connect gate="NAME" pin="PA09/GPIO9/SCL/SPI-CS2/USART1-CTS" pad="28"/>
<connect gate="NAME" pin="PA10/GPIO10/SDA/SI-CS3/USART1-RTS" pad="29"/>
<connect gate="NAME" pin="PA11/GPIO11/USART0-RTS/TC-A2/PWM0/XIN32" pad="30"/>
<connect gate="NAME" pin="PA12/GPIO12/USART0-CTS/TC-B2/PWM1/XOUT32" pad="31"/>
<connect gate="NAME" pin="PA13/GPIO13/NMI/PWM2/USART0-CLK" pad="33"/>
<connect gate="NAME" pin="PA14/GPIO14/SPI-MOSI/PWM3/EXTINT2" pad="34"/>
<connect gate="NAME" pin="PA15/GPIO15/SPI-SCK/PWM4/USART2-CLK" pad="35"/>
<connect gate="NAME" pin="PA16/GPIO16/SPI-CS0/TC-CLK1" pad="36"/>
<connect gate="NAME" pin="PA17/GPIO17/SPI-CS1/TC-CLK2/SPI-SCK" pad="37"/>
<connect gate="NAME" pin="PA18/GPIO18/USART0-RXD/PWM5/SPI-MISO/XIN" pad="39"/>
<connect gate="NAME" pin="PA19/GPIO19/USART0-TXD/PWM6/SPI-MOSI/XOUT" pad="40"/>
<connect gate="NAME" pin="PA20/GPIO20/USART1-CLK/TC-CLK0/USART2-RXD" pad="44"/>
<connect gate="NAME" pin="PA21/GPIO21/PWM2/TC-A1/USART2-TXD" pad="45"/>
<connect gate="NAME" pin="PA22/GPIO22/PWM6/TC-B1/ADC-TRIGGER" pad="46"/>
<connect gate="NAME" pin="PA23/GPIO23/USART1-TXD/SPI-CS1/EXTIN3" pad="47"/>
<connect gate="NAME" pin="PA24/GPIO24/USART1-RXD/SPIC-CS0/EXTINT4" pad="59"/>
<connect gate="NAME" pin="PA25/GPIO25/SPI-MISO/PWM3/EXTINT5" pad="60"/>
<connect gate="NAME" pin="PA26/GPIO26/USB_ID/USART2-TXD/TC-A0" pad="61"/>
<connect gate="NAME" pin="PA27/GPIO27/USB_VBOF/USART2-RXD/TC-B0" pad="62"/>
<connect gate="NAME" pin="PA28/GPIO28/USART0-CLK/PWM4/SPI-MISO/XIN1" pad="41"/>
<connect gate="NAME" pin="PA29/GPIO29/TC-CLK0/TC-CLK1/SPI-MOSI/XOUT1" pad="42"/>
<connect gate="NAME" pin="PA30/GPIO30/ADC6/EIC-SCAN0/GCLK2" pad="15"/>
<connect gate="NAME" pin="PA31/GPIO31/ADC7/EIC-SCAN1" pad="16"/>
<connect gate="NAME" pin="PB00/GPIO32/TC-A0/EIC-SCAN2/USART2-CTS" pad="6"/>
<connect gate="NAME" pin="PB01/GPIO33/TC-B0/EIC-SCAN3/USART2-RTS" pad="7"/>
<connect gate="NAME" pin="PB02/GPIO34/EXTINT6/TC-A1/USART1-TXD" pad="24"/>
<connect gate="NAME" pin="PB03/GPIO35/EXTINT7/TC-B1/USART1-RXD" pad="25"/>
<connect gate="NAME" pin="PB04/GPIO36/USART1-CTS/SPI-CS3/TC-CLK2" pad="26"/>
<connect gate="NAME" pin="PB05/GPIO37/USART1-RTS/SPI-CS2/PWM5" pad="27"/>
<connect gate="NAME" pin="PB06/GPIO38/SSC-RX_CLOCK/USART-DCD/EIC-SCAN4" pad="38"/>
<connect gate="NAME" pin="PB07/GPIO39/SSC-RX_DATA/USART-DSR/EIC-SCAN5" pad="43"/>
<connect gate="NAME" pin="PB08/GPIO40/SSC-RX_FRAME_SYNC/USART1-DTR/EIC-SCAN6" pad="54"/>
<connect gate="NAME" pin="PB09/GPIO41/SSC-TX_CLOCK/USART1-RI/EIC-SCAN7" pad="55"/>
<connect gate="NAME" pin="PB10/GPIO42/SSC-TX_DATA/TC-A2/USART0-RXD" pad="57"/>
<connect gate="NAME" pin="PB11/GPIO43/SSC-TX_FRAME_SYNC/TC-B2/USART0-TXD" pad="58"/>
<connect gate="NAME" pin="TCK" pad="2"/>
<connect gate="NAME" pin="TDI/GPIO0" pad="3"/>
<connect gate="NAME" pin="TDO/GPIO1" pad="4"/>
<connect gate="NAME" pin="TMS/GPIO2" pad="5"/>
<connect gate="NAME" pin="USB_DM" pad="51"/>
<connect gate="NAME" pin="USB_DP" pad="50"/>
<connect gate="NAME" pin="VBUS" pad="52"/>
<connect gate="NAME" pin="VDDANA" pad="19"/>
<connect gate="NAME" pin="VDDCORE@22" pad="22"/>
<connect gate="NAME" pin="VDDCORE@56" pad="56"/>
<connect gate="NAME" pin="VDDCORE@8" pad="8"/>
<connect gate="NAME" pin="VDDIN" pad="21"/>
<connect gate="NAME" pin="VDDIO@32" pad="32"/>
<connect gate="NAME" pin="VDDIO@48" pad="48"/>
<connect gate="NAME" pin="VDDIO@64" pad="64"/>
<connect gate="NAME" pin="VDDOUT" pad="20"/>
<connect gate="NAME" pin="VDDPLL" pad="53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT32UC3B164/1128/1256" prefix="U">
<description>AT32UB3C1128/1256/1512</description>
<gates>
<gate name="NAME" symbol="AT32UC3B1XXX"/>
</gates>
<devices>
<device name="" package="TQFP48">
<connects>
<connect gate="NAME" pin="!RESET" pad="47"/>
<connect gate="NAME" pin="ADVREF" pad="14"/>
<connect gate="NAME" pin="GND@1" pad="1"/>
<connect gate="NAME" pin="GND@13" pad="13"/>
<connect gate="NAME" pin="GND@19" pad="19"/>
<connect gate="NAME" pin="GND@37" pad="37"/>
<connect gate="NAME" pin="PA03/GPIO3/ADC0/GCLK0/USB_ID" pad="7"/>
<connect gate="NAME" pin="PA04/GPIO4/ADC1/USB_VBOF" pad="8"/>
<connect gate="NAME" pin="PA05/GPIO5/EXTINT0/ADC2/USART1-DCD" pad="9"/>
<connect gate="NAME" pin="PA06/GPIO6/ADC3/USART1-DSR" pad="10"/>
<connect gate="NAME" pin="PA07/GPIO7/PWM0/ADC4/USART1-DTR" pad="11"/>
<connect gate="NAME" pin="PA08/GPIO8/PWM1/ADC5/USART1-RI" pad="12"/>
<connect gate="NAME" pin="PA09/GPIO9/SCL/SPI-CS2/USART1-CTS" pad="20"/>
<connect gate="NAME" pin="PA10/GPIO10/SDA/SI-CS3/USART1-RTS" pad="21"/>
<connect gate="NAME" pin="PA11/GPIO11/USART0-RTS/TC-A2/PWM0/XIN32" pad="22"/>
<connect gate="NAME" pin="PA12/GPIO12/USART0-CTS/TC-B2/PWM1/XOUT32" pad="23"/>
<connect gate="NAME" pin="PA13/GPIO13/NMI/PWM2/USART0-CLK" pad="25"/>
<connect gate="NAME" pin="PA14/GPIO14/SPI-MOSI/PWM3/EXTINT2" pad="26"/>
<connect gate="NAME" pin="PA15/GPIO15/SPI-SCK/PWM4/USART2-CLK" pad="27"/>
<connect gate="NAME" pin="PA16/GPIO16/SPI-CS0/TC-CLK1" pad="28"/>
<connect gate="NAME" pin="PA17/GPIO17/SPI-CS1/TC-CLK2/SPI-SCK" pad="29"/>
<connect gate="NAME" pin="PA18/GPIO18/USART0-RXD/PWM5/SPI-MISO/XIN" pad="30"/>
<connect gate="NAME" pin="PA19/GPIO19/USART0-TXD/PWM6/SPI-MOSI/XOUT" pad="31"/>
<connect gate="NAME" pin="PA20/GPIO20/USART1-CLK/TC-CLK0/USART2-RXD" pad="32"/>
<connect gate="NAME" pin="PA21/GPIO21/PWM2/TC-A1/USART2-TXD" pad="33"/>
<connect gate="NAME" pin="PA22/GPIO22/PWM6/TC-B1/ADC-TRIGGER" pad="34"/>
<connect gate="NAME" pin="PA23/GPIO23/USART1-TXD/SPI-CS1/EXTIN3" pad="35"/>
<connect gate="NAME" pin="PA24/GPIO24/USART1-RXD/SPIC-CS0/EXTINT4" pad="43"/>
<connect gate="NAME" pin="PA25/GPIO25/SPI-MISO/PWM3/EXTINT5" pad="44"/>
<connect gate="NAME" pin="PA26/GPIO26/USB_ID/USART2-TXD/TC-A0" pad="45"/>
<connect gate="NAME" pin="PA27/GPIO27/USB_VBOF/USART2-RXD/TC-B0" pad="46"/>
<connect gate="NAME" pin="TCK" pad="2"/>
<connect gate="NAME" pin="TDI/GPIO0" pad="3"/>
<connect gate="NAME" pin="TDO/GPIO1" pad="4"/>
<connect gate="NAME" pin="TMS/GPIO2" pad="5"/>
<connect gate="NAME" pin="USB_DM" pad="39"/>
<connect gate="NAME" pin="USB_DP" pad="38"/>
<connect gate="NAME" pin="VBUS" pad="40"/>
<connect gate="NAME" pin="VDDANA" pad="15"/>
<connect gate="NAME" pin="VDDCORE@18" pad="18"/>
<connect gate="NAME" pin="VDDCORE@42" pad="42"/>
<connect gate="NAME" pin="VDDCORE@6" pad="6"/>
<connect gate="NAME" pin="VDDIN" pad="17"/>
<connect gate="NAME" pin="VDDIO@24" pad="24"/>
<connect gate="NAME" pin="VDDIO@36" pad="36"/>
<connect gate="NAME" pin="VDDIO@48" pad="48"/>
<connect gate="NAME" pin="VDDOUT" pad="16"/>
<connect gate="NAME" pin="VDDPLL" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT32UC3L016/32/64">
<description>AT32UC3L016/32/64 Low power AVR32 device</description>
<gates>
<gate name="G$1" symbol="AT32UC3LXXXX"/>
</gates>
<devices>
<device name="" package="TQFP48">
<connects>
<connect gate="G$1" pin="ADVREFP" pad="34"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="GND@45" pad="45"/>
<connect gate="G$1" pin="GNDANA" pad="33"/>
<connect gate="G$1" pin="PA00" pad="11"/>
<connect gate="G$1" pin="PA01" pad="14"/>
<connect gate="G$1" pin="PA02" pad="13"/>
<connect gate="G$1" pin="PA03" pad="4"/>
<connect gate="G$1" pin="PA04" pad="28"/>
<connect gate="G$1" pin="PA05" pad="12"/>
<connect gate="G$1" pin="PA06" pad="10"/>
<connect gate="G$1" pin="PA07" pad="15"/>
<connect gate="G$1" pin="PA08" pad="3"/>
<connect gate="G$1" pin="PA09" pad="2"/>
<connect gate="G$1" pin="PA10" pad="46"/>
<connect gate="G$1" pin="PA11" pad="27"/>
<connect gate="G$1" pin="PA12" pad="47"/>
<connect gate="G$1" pin="PA13" pad="26"/>
<connect gate="G$1" pin="PA14" pad="36"/>
<connect gate="G$1" pin="PA15" pad="37"/>
<connect gate="G$1" pin="PA16" pad="38"/>
<connect gate="G$1" pin="PA17" pad="39"/>
<connect gate="G$1" pin="PA18" pad="41"/>
<connect gate="G$1" pin="PA19" pad="40"/>
<connect gate="G$1" pin="PA20" pad="25"/>
<connect gate="G$1" pin="PA21" pad="24"/>
<connect gate="G$1" pin="PA22" pad="9"/>
<connect gate="G$1" pin="PB00" pad="6"/>
<connect gate="G$1" pin="PB01" pad="16"/>
<connect gate="G$1" pin="PB02" pad="7"/>
<connect gate="G$1" pin="PB03" pad="8"/>
<connect gate="G$1" pin="PB04" pad="21"/>
<connect gate="G$1" pin="PB05" pad="20"/>
<connect gate="G$1" pin="PB06" pad="30"/>
<connect gate="G$1" pin="PB07" pad="31"/>
<connect gate="G$1" pin="PB08" pad="32"/>
<connect gate="G$1" pin="PB09" pad="29"/>
<connect gate="G$1" pin="PB10" pad="23"/>
<connect gate="G$1" pin="PB11" pad="44"/>
<connect gate="G$1" pin="PB12" pad="5"/>
<connect gate="G$1" pin="RESET_N" pad="22"/>
<connect gate="G$1" pin="VDDANA" pad="35"/>
<connect gate="G$1" pin="VDDCORE" pad="18"/>
<connect gate="G$1" pin="VDDIN" pad="17"/>
<connect gate="G$1" pin="VDDIO@42" pad="42"/>
<connect gate="G$1" pin="VDDIO@48" pad="48"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-JTAG-10" prefix="JP">
<description>&lt;b&gt;AVR JTAG&lt;/b&gt;&lt;p&gt; Debug/Programming Header</description>
<gates>
<gate name="NAME" symbol="AVR-JTAG-10"/>
</gates>
<devices>
<device name="" package="AVR-JTAG-10">
<connects>
<connect gate="NAME" pin="1" pad="1"/>
<connect gate="NAME" pin="10" pad="10"/>
<connect gate="NAME" pin="2" pad="2"/>
<connect gate="NAME" pin="3" pad="3"/>
<connect gate="NAME" pin="4" pad="4"/>
<connect gate="NAME" pin="5" pad="5"/>
<connect gate="NAME" pin="6" pad="6"/>
<connect gate="NAME" pin="7" pad="7"/>
<connect gate="NAME" pin="8" pad="8"/>
<connect gate="NAME" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-R" package="AVR-JTAG-10R">
<connects>
<connect gate="NAME" pin="1" pad="1"/>
<connect gate="NAME" pin="10" pad="10"/>
<connect gate="NAME" pin="2" pad="2"/>
<connect gate="NAME" pin="3" pad="3"/>
<connect gate="NAME" pin="4" pad="4"/>
<connect gate="NAME" pin="5" pad="5"/>
<connect gate="NAME" pin="6" pad="6"/>
<connect gate="NAME" pin="7" pad="7"/>
<connect gate="NAME" pin="8" pad="8"/>
<connect gate="NAME" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT32UC3C0">
<description>ATMEL 32-bit Microcontroller 64KB, 128KB, 256KB, 512KB
144-pin LQFP (123 GPIO pins)
http://www.atmel.com/Images/32117s.pdf</description>
<gates>
<gate name="G$1" symbol="AT32UC3C0"/>
</gates>
<devices>
<device name="" package="TQFP144">
<connects>
<connect gate="G$1" pin="!RESET" pad="142"/>
<connect gate="G$1" pin="ADCVREFN" pad="35"/>
<connect gate="G$1" pin="ADCVREFP" pad="34"/>
<connect gate="G$1" pin="DM" pad="50"/>
<connect gate="G$1" pin="DP" pad="51"/>
<connect gate="G$1" pin="GNDANA" pad="37"/>
<connect gate="G$1" pin="GNDCORE" pad="56"/>
<connect gate="G$1" pin="GNDIO1" pad="6"/>
<connect gate="G$1" pin="GNDIO2" pad="76"/>
<connect gate="G$1" pin="GNDIO3" pad="104"/>
<connect gate="G$1" pin="GNDIO4" pad="119"/>
<connect gate="G$1" pin="GNDPLL" pad="52"/>
<connect gate="G$1" pin="PA0" pad="1"/>
<connect gate="G$1" pin="PA1" pad="2"/>
<connect gate="G$1" pin="PA10" pad="27"/>
<connect gate="G$1" pin="PA11" pad="28"/>
<connect gate="G$1" pin="PA12" pad="29"/>
<connect gate="G$1" pin="PA13" pad="30"/>
<connect gate="G$1" pin="PA14" pad="31"/>
<connect gate="G$1" pin="PA15" pad="32"/>
<connect gate="G$1" pin="PA16" pad="33"/>
<connect gate="G$1" pin="PA19" pad="36"/>
<connect gate="G$1" pin="PA2" pad="3"/>
<connect gate="G$1" pin="PA20" pad="39"/>
<connect gate="G$1" pin="PA21" pad="40"/>
<connect gate="G$1" pin="PA22" pad="41"/>
<connect gate="G$1" pin="PA23" pad="42"/>
<connect gate="G$1" pin="PA24" pad="43"/>
<connect gate="G$1" pin="PA25" pad="44"/>
<connect gate="G$1" pin="PA26" pad="45"/>
<connect gate="G$1" pin="PA27" pad="46"/>
<connect gate="G$1" pin="PA28" pad="47"/>
<connect gate="G$1" pin="PA29" pad="48"/>
<connect gate="G$1" pin="PA3" pad="4"/>
<connect gate="G$1" pin="PA4" pad="21"/>
<connect gate="G$1" pin="PA5" pad="22"/>
<connect gate="G$1" pin="PA6" pad="23"/>
<connect gate="G$1" pin="PA7" pad="24"/>
<connect gate="G$1" pin="PA8" pad="25"/>
<connect gate="G$1" pin="PA9" pad="26"/>
<connect gate="G$1" pin="PB0" pad="140"/>
<connect gate="G$1" pin="PB1" pad="141"/>
<connect gate="G$1" pin="PB10" pad="13"/>
<connect gate="G$1" pin="PB11" pad="14"/>
<connect gate="G$1" pin="PB12" pad="15"/>
<connect gate="G$1" pin="PB13" pad="16"/>
<connect gate="G$1" pin="PB14" pad="17"/>
<connect gate="G$1" pin="PB15" pad="18"/>
<connect gate="G$1" pin="PB16" pad="19"/>
<connect gate="G$1" pin="PB17" pad="20"/>
<connect gate="G$1" pin="PB18" pad="57"/>
<connect gate="G$1" pin="PB19" pad="58"/>
<connect gate="G$1" pin="PB2" pad="143"/>
<connect gate="G$1" pin="PB20" pad="59"/>
<connect gate="G$1" pin="PB21" pad="60"/>
<connect gate="G$1" pin="PB22" pad="61"/>
<connect gate="G$1" pin="PB23" pad="62"/>
<connect gate="G$1" pin="PB24" pad="63"/>
<connect gate="G$1" pin="PB25" pad="64"/>
<connect gate="G$1" pin="PB26" pad="65"/>
<connect gate="G$1" pin="PB27" pad="66"/>
<connect gate="G$1" pin="PB28" pad="67"/>
<connect gate="G$1" pin="PB29" pad="68"/>
<connect gate="G$1" pin="PB3" pad="144"/>
<connect gate="G$1" pin="PB30" pad="69"/>
<connect gate="G$1" pin="PB31" pad="70"/>
<connect gate="G$1" pin="PB4" pad="7"/>
<connect gate="G$1" pin="PB5" pad="8"/>
<connect gate="G$1" pin="PB6" pad="9"/>
<connect gate="G$1" pin="PB7" pad="10"/>
<connect gate="G$1" pin="PB8" pad="11"/>
<connect gate="G$1" pin="PB9" pad="12"/>
<connect gate="G$1" pin="PC0" pad="71"/>
<connect gate="G$1" pin="PC1" pad="72"/>
<connect gate="G$1" pin="PC10" pad="83"/>
<connect gate="G$1" pin="PC11" pad="84"/>
<connect gate="G$1" pin="PC12" pad="85"/>
<connect gate="G$1" pin="PC13" pad="86"/>
<connect gate="G$1" pin="PC14" pad="87"/>
<connect gate="G$1" pin="PC15" pad="88"/>
<connect gate="G$1" pin="PC16" pad="89"/>
<connect gate="G$1" pin="PC17" pad="90"/>
<connect gate="G$1" pin="PC18" pad="91"/>
<connect gate="G$1" pin="PC19" pad="92"/>
<connect gate="G$1" pin="PC2" pad="73"/>
<connect gate="G$1" pin="PC20" pad="93"/>
<connect gate="G$1" pin="PC21" pad="94"/>
<connect gate="G$1" pin="PC22" pad="95"/>
<connect gate="G$1" pin="PC23" pad="96"/>
<connect gate="G$1" pin="PC24" pad="97"/>
<connect gate="G$1" pin="PC25" pad="98"/>
<connect gate="G$1" pin="PC26" pad="99"/>
<connect gate="G$1" pin="PC27" pad="100"/>
<connect gate="G$1" pin="PC28" pad="101"/>
<connect gate="G$1" pin="PC29" pad="102"/>
<connect gate="G$1" pin="PC3" pad="74"/>
<connect gate="G$1" pin="PC30" pad="105"/>
<connect gate="G$1" pin="PC31" pad="106"/>
<connect gate="G$1" pin="PC4" pad="77"/>
<connect gate="G$1" pin="PC5" pad="78"/>
<connect gate="G$1" pin="PC6" pad="79"/>
<connect gate="G$1" pin="PC7" pad="80"/>
<connect gate="G$1" pin="PC8" pad="81"/>
<connect gate="G$1" pin="PC9" pad="82"/>
<connect gate="G$1" pin="PD0" pad="107"/>
<connect gate="G$1" pin="PD1" pad="108"/>
<connect gate="G$1" pin="PD10" pad="117"/>
<connect gate="G$1" pin="PD11" pad="120"/>
<connect gate="G$1" pin="PD12" pad="121"/>
<connect gate="G$1" pin="PD13" pad="122"/>
<connect gate="G$1" pin="PD14" pad="123"/>
<connect gate="G$1" pin="PD15" pad="124"/>
<connect gate="G$1" pin="PD16" pad="125"/>
<connect gate="G$1" pin="PD17" pad="126"/>
<connect gate="G$1" pin="PD18" pad="127"/>
<connect gate="G$1" pin="PD19" pad="128"/>
<connect gate="G$1" pin="PD2" pad="109"/>
<connect gate="G$1" pin="PD20" pad="129"/>
<connect gate="G$1" pin="PD21" pad="130"/>
<connect gate="G$1" pin="PD22" pad="131"/>
<connect gate="G$1" pin="PD23" pad="132"/>
<connect gate="G$1" pin="PD24" pad="133"/>
<connect gate="G$1" pin="PD25" pad="134"/>
<connect gate="G$1" pin="PD26" pad="135"/>
<connect gate="G$1" pin="PD27" pad="136"/>
<connect gate="G$1" pin="PD28" pad="137"/>
<connect gate="G$1" pin="PD29" pad="138"/>
<connect gate="G$1" pin="PD3" pad="110"/>
<connect gate="G$1" pin="PD30" pad="139"/>
<connect gate="G$1" pin="PD4" pad="111"/>
<connect gate="G$1" pin="PD5" pad="112"/>
<connect gate="G$1" pin="PD6" pad="113"/>
<connect gate="G$1" pin="PD7" pad="114"/>
<connect gate="G$1" pin="PD8" pad="115"/>
<connect gate="G$1" pin="PD9" pad="116"/>
<connect gate="G$1" pin="VBUS" pad="49"/>
<connect gate="G$1" pin="VDDANA" pad="38"/>
<connect gate="G$1" pin="VDDCORE" pad="55"/>
<connect gate="G$1" pin="VDDIO1" pad="5"/>
<connect gate="G$1" pin="VDDIO2" pad="75"/>
<connect gate="G$1" pin="VDDIO3" pad="103"/>
<connect gate="G$1" pin="VDDIO4" pad="118"/>
<connect gate="G$1" pin="VDD_33" pad="54"/>
<connect gate="G$1" pin="VDD_5" pad="53"/>
</connects>
<technologies>
<technology name=""/>
<technology name="064">
<attribute name="FLASH" value="64KB"/>
</technology>
<technology name="128">
<attribute name="FLASH" value="128KB"/>
</technology>
<technology name="256">
<attribute name="FLASH" value="256KB"/>
</technology>
<technology name="512">
<attribute name="FLASH" value="512KB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT32UC3C1">
<description>ATMEL 32-bit Microcontroller 64KB, 128KB, 256KB, 512KB
100-pin TQFP (81 GPIO pins)
http://www.atmel.com/Images/32117s.pdf</description>
<gates>
<gate name="G$1" symbol="AT32UC3C1"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G$1" pin="!RESET" pad="98"/>
<connect gate="G$1" pin="ADCREFN" pad="24"/>
<connect gate="G$1" pin="ADCREFP" pad="23"/>
<connect gate="G$1" pin="DM" pad="35"/>
<connect gate="G$1" pin="DP" pad="36"/>
<connect gate="G$1" pin="GNDANA" pad="26"/>
<connect gate="G$1" pin="GNDCORE" pad="41"/>
<connect gate="G$1" pin="GNDIO1" pad="6"/>
<connect gate="G$1" pin="GNDIO2" pad="54"/>
<connect gate="G$1" pin="GNDIO3" pad="83"/>
<connect gate="G$1" pin="GNDPLL" pad="37"/>
<connect gate="G$1" pin="PA0" pad="1"/>
<connect gate="G$1" pin="PA1" pad="2"/>
<connect gate="G$1" pin="PA10" pad="16"/>
<connect gate="G$1" pin="PA11" pad="17"/>
<connect gate="G$1" pin="PA12" pad="18"/>
<connect gate="G$1" pin="PA13" pad="19"/>
<connect gate="G$1" pin="PA14" pad="20"/>
<connect gate="G$1" pin="PA15" pad="21"/>
<connect gate="G$1" pin="PA16" pad="22"/>
<connect gate="G$1" pin="PA19" pad="25"/>
<connect gate="G$1" pin="PA2" pad="3"/>
<connect gate="G$1" pin="PA20" pad="28"/>
<connect gate="G$1" pin="PA21" pad="29"/>
<connect gate="G$1" pin="PA22" pad="30"/>
<connect gate="G$1" pin="PA23" pad="31"/>
<connect gate="G$1" pin="PA24" pad="32"/>
<connect gate="G$1" pin="PA25" pad="33"/>
<connect gate="G$1" pin="PA3" pad="4"/>
<connect gate="G$1" pin="PA4" pad="10"/>
<connect gate="G$1" pin="PA5" pad="11"/>
<connect gate="G$1" pin="PA6" pad="12"/>
<connect gate="G$1" pin="PA7" pad="13"/>
<connect gate="G$1" pin="PA8" pad="14"/>
<connect gate="G$1" pin="PA9" pad="15"/>
<connect gate="G$1" pin="PB0" pad="96"/>
<connect gate="G$1" pin="PB1" pad="97"/>
<connect gate="G$1" pin="PB19" pad="42"/>
<connect gate="G$1" pin="PB2" pad="99"/>
<connect gate="G$1" pin="PB20" pad="43"/>
<connect gate="G$1" pin="PB21" pad="44"/>
<connect gate="G$1" pin="PB22" pad="45"/>
<connect gate="G$1" pin="PB23" pad="46"/>
<connect gate="G$1" pin="PB3" pad="100"/>
<connect gate="G$1" pin="PB30" pad="47"/>
<connect gate="G$1" pin="PB31" pad="48"/>
<connect gate="G$1" pin="PB4" pad="7"/>
<connect gate="G$1" pin="PB5" pad="8"/>
<connect gate="G$1" pin="PB6" pad="9"/>
<connect gate="G$1" pin="PC0" pad="49"/>
<connect gate="G$1" pin="PC1" pad="50"/>
<connect gate="G$1" pin="PC11" pad="59"/>
<connect gate="G$1" pin="PC12" pad="60"/>
<connect gate="G$1" pin="PC13" pad="61"/>
<connect gate="G$1" pin="PC14" pad="62"/>
<connect gate="G$1" pin="PC15" pad="63"/>
<connect gate="G$1" pin="PC16" pad="64"/>
<connect gate="G$1" pin="PC17" pad="65"/>
<connect gate="G$1" pin="PC18" pad="66"/>
<connect gate="G$1" pin="PC19" pad="67"/>
<connect gate="G$1" pin="PC2" pad="51"/>
<connect gate="G$1" pin="PC20" pad="68"/>
<connect gate="G$1" pin="PC21" pad="69"/>
<connect gate="G$1" pin="PC22" pad="70"/>
<connect gate="G$1" pin="PC23" pad="71"/>
<connect gate="G$1" pin="PC24" pad="72"/>
<connect gate="G$1" pin="PC3" pad="52"/>
<connect gate="G$1" pin="PC31" pad="73"/>
<connect gate="G$1" pin="PC4" pad="55"/>
<connect gate="G$1" pin="PC5" pad="56"/>
<connect gate="G$1" pin="PC6" pad="57"/>
<connect gate="G$1" pin="PC7" pad="58"/>
<connect gate="G$1" pin="PD0" pad="74"/>
<connect gate="G$1" pin="PD1" pad="75"/>
<connect gate="G$1" pin="PD10" pad="81"/>
<connect gate="G$1" pin="PD11" pad="84"/>
<connect gate="G$1" pin="PD12" pad="85"/>
<connect gate="G$1" pin="PD13" pad="86"/>
<connect gate="G$1" pin="PD14" pad="87"/>
<connect gate="G$1" pin="PD2" pad="76"/>
<connect gate="G$1" pin="PD21" pad="88"/>
<connect gate="G$1" pin="PD22" pad="89"/>
<connect gate="G$1" pin="PD23" pad="90"/>
<connect gate="G$1" pin="PD24" pad="91"/>
<connect gate="G$1" pin="PD27" pad="92"/>
<connect gate="G$1" pin="PD28" pad="93"/>
<connect gate="G$1" pin="PD29" pad="94"/>
<connect gate="G$1" pin="PD3" pad="77"/>
<connect gate="G$1" pin="PD30" pad="95"/>
<connect gate="G$1" pin="PD7" pad="78"/>
<connect gate="G$1" pin="PD8" pad="79"/>
<connect gate="G$1" pin="PD9" pad="80"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VDDANA" pad="27"/>
<connect gate="G$1" pin="VDDCORE" pad="40"/>
<connect gate="G$1" pin="VDDIO1" pad="5"/>
<connect gate="G$1" pin="VDDIO2" pad="53"/>
<connect gate="G$1" pin="VDDIO3" pad="82"/>
<connect gate="G$1" pin="VDD_33" pad="39"/>
<connect gate="G$1" pin="VDD_5" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="FLASH" value=""/>
</technology>
<technology name="064">
<attribute name="FLASH" value="64KB"/>
</technology>
<technology name="128">
<attribute name="FLASH" value="128KB"/>
</technology>
<technology name="256">
<attribute name="FLASH" value="256KB"/>
</technology>
<technology name="512">
<attribute name="FLASH" value="512KB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT32UC3C2">
<description>ATMEL 32-bit Microcontroller 64KB, 128KB, 256KB, 512KB
64-pin TQFP or PQFN (45 GPIO pins)
http://www.atmel.com/Images/32117s.pdf</description>
<gates>
<gate name="AT32UC3C2" symbol="AT32UC3C2"/>
</gates>
<devices>
<device name="TQFP" package="TQFP64-10X10">
<connects>
<connect gate="AT32UC3C2" pin="!RESET" pad="64"/>
<connect gate="AT32UC3C2" pin="ADCVREFN" pad="15"/>
<connect gate="AT32UC3C2" pin="ADCVREFP" pad="14"/>
<connect gate="AT32UC3C2" pin="DM" pad="24"/>
<connect gate="AT32UC3C2" pin="DP" pad="25"/>
<connect gate="AT32UC3C2" pin="GNDANA" pad="17"/>
<connect gate="AT32UC3C2" pin="GNDCORE" pad="30"/>
<connect gate="AT32UC3C2" pin="GNDIO1" pad="6"/>
<connect gate="AT32UC3C2" pin="GNDIO2" pad="36"/>
<connect gate="AT32UC3C2" pin="GNDIO3" pad="52"/>
<connect gate="AT32UC3C2" pin="GNDPLL" pad="26"/>
<connect gate="AT32UC3C2" pin="PA0" pad="1"/>
<connect gate="AT32UC3C2" pin="PA1" pad="2"/>
<connect gate="AT32UC3C2" pin="PA16" pad="13"/>
<connect gate="AT32UC3C2" pin="PA19" pad="16"/>
<connect gate="AT32UC3C2" pin="PA2" pad="3"/>
<connect gate="AT32UC3C2" pin="PA20" pad="19"/>
<connect gate="AT32UC3C2" pin="PA21" pad="20"/>
<connect gate="AT32UC3C2" pin="PA22" pad="21"/>
<connect gate="AT32UC3C2" pin="PA23" pad="22"/>
<connect gate="AT32UC3C2" pin="PA3" pad="4"/>
<connect gate="AT32UC3C2" pin="PA4" pad="7"/>
<connect gate="AT32UC3C2" pin="PA5" pad="8"/>
<connect gate="AT32UC3C2" pin="PA6" pad="9"/>
<connect gate="AT32UC3C2" pin="PA7" pad="10"/>
<connect gate="AT32UC3C2" pin="PA8" pad="11"/>
<connect gate="AT32UC3C2" pin="PA9" pad="12"/>
<connect gate="AT32UC3C2" pin="PB0" pad="62"/>
<connect gate="AT32UC3C2" pin="PB1" pad="63"/>
<connect gate="AT32UC3C2" pin="PB30" pad="31"/>
<connect gate="AT32UC3C2" pin="PB31" pad="32"/>
<connect gate="AT32UC3C2" pin="PC15" pad="39"/>
<connect gate="AT32UC3C2" pin="PC16" pad="40"/>
<connect gate="AT32UC3C2" pin="PC17" pad="41"/>
<connect gate="AT32UC3C2" pin="PC18" pad="42"/>
<connect gate="AT32UC3C2" pin="PC19" pad="43"/>
<connect gate="AT32UC3C2" pin="PC2" pad="33"/>
<connect gate="AT32UC3C2" pin="PC20" pad="44"/>
<connect gate="AT32UC3C2" pin="PC21" pad="45"/>
<connect gate="AT32UC3C2" pin="PC22" pad="46"/>
<connect gate="AT32UC3C2" pin="PC3" pad="34"/>
<connect gate="AT32UC3C2" pin="PC4" pad="37"/>
<connect gate="AT32UC3C2" pin="PC5" pad="38"/>
<connect gate="AT32UC3C2" pin="PD0" pad="47"/>
<connect gate="AT32UC3C2" pin="PD1" pad="48"/>
<connect gate="AT32UC3C2" pin="PD11" pad="53"/>
<connect gate="AT32UC3C2" pin="PD12" pad="54"/>
<connect gate="AT32UC3C2" pin="PD13" pad="55"/>
<connect gate="AT32UC3C2" pin="PD14" pad="56"/>
<connect gate="AT32UC3C2" pin="PD2" pad="49"/>
<connect gate="AT32UC3C2" pin="PD21" pad="57"/>
<connect gate="AT32UC3C2" pin="PD27" pad="58"/>
<connect gate="AT32UC3C2" pin="PD28" pad="59"/>
<connect gate="AT32UC3C2" pin="PD29" pad="60"/>
<connect gate="AT32UC3C2" pin="PD3" pad="50"/>
<connect gate="AT32UC3C2" pin="PD30" pad="61"/>
<connect gate="AT32UC3C2" pin="VBUS" pad="23"/>
<connect gate="AT32UC3C2" pin="VDD33" pad="28"/>
<connect gate="AT32UC3C2" pin="VDD5" pad="27"/>
<connect gate="AT32UC3C2" pin="VDDANA" pad="18"/>
<connect gate="AT32UC3C2" pin="VDDCORE" pad="29"/>
<connect gate="AT32UC3C2" pin="VDDIO1" pad="5"/>
<connect gate="AT32UC3C2" pin="VDDIO2" pad="35"/>
<connect gate="AT32UC3C2" pin="VDDIO3" pad="51"/>
</connects>
<technologies>
<technology name=""/>
<technology name="064"/>
<technology name="128"/>
<technology name="256"/>
<technology name="512"/>
</technologies>
</device>
<device name="TQFN" package="PQFN64-1">
<connects>
<connect gate="AT32UC3C2" pin="!RESET" pad="64"/>
<connect gate="AT32UC3C2" pin="ADCVREFN" pad="15"/>
<connect gate="AT32UC3C2" pin="ADCVREFP" pad="14"/>
<connect gate="AT32UC3C2" pin="DM" pad="24"/>
<connect gate="AT32UC3C2" pin="DP" pad="25"/>
<connect gate="AT32UC3C2" pin="GNDANA" pad="17"/>
<connect gate="AT32UC3C2" pin="GNDCORE" pad="30 EXP"/>
<connect gate="AT32UC3C2" pin="GNDIO1" pad="6"/>
<connect gate="AT32UC3C2" pin="GNDIO2" pad="36"/>
<connect gate="AT32UC3C2" pin="GNDIO3" pad="52"/>
<connect gate="AT32UC3C2" pin="GNDPLL" pad="26"/>
<connect gate="AT32UC3C2" pin="PA0" pad="1"/>
<connect gate="AT32UC3C2" pin="PA1" pad="2"/>
<connect gate="AT32UC3C2" pin="PA16" pad="13"/>
<connect gate="AT32UC3C2" pin="PA19" pad="16"/>
<connect gate="AT32UC3C2" pin="PA2" pad="3"/>
<connect gate="AT32UC3C2" pin="PA20" pad="19"/>
<connect gate="AT32UC3C2" pin="PA21" pad="20"/>
<connect gate="AT32UC3C2" pin="PA22" pad="21"/>
<connect gate="AT32UC3C2" pin="PA23" pad="22"/>
<connect gate="AT32UC3C2" pin="PA3" pad="4"/>
<connect gate="AT32UC3C2" pin="PA4" pad="7"/>
<connect gate="AT32UC3C2" pin="PA5" pad="8"/>
<connect gate="AT32UC3C2" pin="PA6" pad="9"/>
<connect gate="AT32UC3C2" pin="PA7" pad="10"/>
<connect gate="AT32UC3C2" pin="PA8" pad="11"/>
<connect gate="AT32UC3C2" pin="PA9" pad="12"/>
<connect gate="AT32UC3C2" pin="PB0" pad="62"/>
<connect gate="AT32UC3C2" pin="PB1" pad="63"/>
<connect gate="AT32UC3C2" pin="PB30" pad="31"/>
<connect gate="AT32UC3C2" pin="PB31" pad="32"/>
<connect gate="AT32UC3C2" pin="PC15" pad="39"/>
<connect gate="AT32UC3C2" pin="PC16" pad="40"/>
<connect gate="AT32UC3C2" pin="PC17" pad="41"/>
<connect gate="AT32UC3C2" pin="PC18" pad="42"/>
<connect gate="AT32UC3C2" pin="PC19" pad="43"/>
<connect gate="AT32UC3C2" pin="PC2" pad="33"/>
<connect gate="AT32UC3C2" pin="PC20" pad="44"/>
<connect gate="AT32UC3C2" pin="PC21" pad="45"/>
<connect gate="AT32UC3C2" pin="PC22" pad="46"/>
<connect gate="AT32UC3C2" pin="PC3" pad="34"/>
<connect gate="AT32UC3C2" pin="PC4" pad="37"/>
<connect gate="AT32UC3C2" pin="PC5" pad="38"/>
<connect gate="AT32UC3C2" pin="PD0" pad="47"/>
<connect gate="AT32UC3C2" pin="PD1" pad="48"/>
<connect gate="AT32UC3C2" pin="PD11" pad="53"/>
<connect gate="AT32UC3C2" pin="PD12" pad="54"/>
<connect gate="AT32UC3C2" pin="PD13" pad="55"/>
<connect gate="AT32UC3C2" pin="PD14" pad="56"/>
<connect gate="AT32UC3C2" pin="PD2" pad="49"/>
<connect gate="AT32UC3C2" pin="PD21" pad="57"/>
<connect gate="AT32UC3C2" pin="PD27" pad="58"/>
<connect gate="AT32UC3C2" pin="PD28" pad="59"/>
<connect gate="AT32UC3C2" pin="PD29" pad="60"/>
<connect gate="AT32UC3C2" pin="PD3" pad="50"/>
<connect gate="AT32UC3C2" pin="PD30" pad="61"/>
<connect gate="AT32UC3C2" pin="VBUS" pad="23"/>
<connect gate="AT32UC3C2" pin="VDD33" pad="28"/>
<connect gate="AT32UC3C2" pin="VDD5" pad="27"/>
<connect gate="AT32UC3C2" pin="VDDANA" pad="18"/>
<connect gate="AT32UC3C2" pin="VDDCORE" pad="29"/>
<connect gate="AT32UC3C2" pin="VDDIO1" pad="5"/>
<connect gate="AT32UC3C2" pin="VDDIO2" pad="35"/>
<connect gate="AT32UC3C2" pin="VDDIO3" pad="51"/>
</connects>
<technologies>
<technology name=""/>
<technology name="064">
<attribute name="FLASH" value="64KB"/>
</technology>
<technology name="128">
<attribute name="FLASH" value="128KB"/>
</technology>
<technology name="256">
<attribute name="FLASH" value="256KB"/>
</technology>
<technology name="512">
<attribute name="FLASH" value="512KB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY25*" prefix="U">
<description>&lt;h3&gt;ATMEL ATtiny 25&lt;/h3&gt;

&lt;p&gt;&lt;br /&gt;&lt;b&gt;&lt;u&gt;Packages:&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;P&lt;/b&gt; &amp;nbsp; = PDIP 08 30mil&lt;br /&gt;
&lt;b&gt;S&lt;/b&gt; &amp;nbsp; = SOIC 08 EIAJ 208mil&lt;br /&gt;
&lt;b&gt;SS&lt;/b&gt; = SOIC 08 JEDEC 150mil&lt;/p&gt;

&lt;p&gt;&lt;b&gt;&lt;u&gt;Technologies&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
Note: for complete ordering code  (temp. range, finish, tape&amp;reel etc.) see www.atmel.com&lt;br /&gt;
&amp;bull; Supply Voltage:
  &lt;b&gt;V&lt;/b&gt; = (1.8&amp;hellip;5.5)V | &lt;b&gt;[blank]&lt;/b&gt; = (2.7&amp;hellip;5.5)V&lt;br /&gt;
&amp;bull; Speed:
  &lt;b&gt;10&lt;/b&gt; = 10 MHz | &lt;b&gt;20&lt;/b&gt; = 20 MHz
&lt;/pre&gt;&lt;/p&gt;
&lt;hr /&gt;

&lt;author&gt;
&lt;p&gt;&lt;u&gt;Author:&lt;/u&gt;&lt;br /&gt;
Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn (Heilbronn University), &lt;i&gt;rainer.bayer@hs-heilbronn.de&lt;/i&gt;&lt;br /&gt;
Ingenieurbüro ing-rb, &lt;i&gt;mail@ing-rb.de&lt;/i&gt;&lt;/p&gt;&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="ATTINY25_45_85"/>
</gates>
<devices>
<device name="P" package="PDIP08_300MIL">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NRES/PB5" pad="1"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-"/>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="S" package="SOIC8_EIAJ_208MIL">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NRES/PB5" pad="1"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-"/>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="SS" package="SOIC08_JEDEC_150MIL">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NRES/PB5" pad="1"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-"/>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45*" prefix="U">
<description>&lt;h3&gt;ATMEL ATtiny 45&lt;/h3&gt;

&lt;p&gt;&lt;br /&gt;&lt;b&gt;&lt;u&gt;Packages:&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;P&lt;/b&gt; = PDIP 08 30mil&lt;br /&gt;
&lt;b&gt;S&lt;/b&gt; = SOIC 08 EIAJ 208mil&lt;br&gt;
&lt;b&gt;X&lt;/b&gt; = TSSOP 08 4.4mm&lt;/p&gt;

&lt;p&gt;&lt;b&gt;&lt;u&gt;Technologies&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
Note: for complete ordering code  (temp. range, finish, tape&amp;reel etc.) see www.atmel.com&lt;br /&gt;
&amp;bull; Supply Voltage:
  &lt;b&gt;V&lt;/b&gt; = (1.8&amp;hellip;5.5)V | &lt;b&gt;[blank]&lt;/b&gt; = (2.7&amp;hellip;5.5)V&lt;br /&gt;
&amp;bull; Speed:
  &lt;b&gt;10&lt;/b&gt; = 10 MHz | &lt;b&gt;20&lt;/b&gt; = 20 MHz
&lt;/pre&gt;&lt;/p&gt;
&lt;hr /&gt;

&lt;author&gt;
&lt;p&gt;&lt;u&gt;Author:&lt;/u&gt;&lt;br /&gt;
Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn (Heilbronn University), &lt;i&gt;rainer.bayer@hs-heilbronn.de&lt;/i&gt;&lt;br /&gt;
Ingenieurbüro ing-rb, &lt;i&gt;mail@ing-rb.de&lt;/i&gt;&lt;/p&gt;&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="ATTINY25_45_85"/>
</gates>
<devices>
<device name="P" package="PDIP08_300MIL">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NRES/PB5" pad="1"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-"/>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="S" package="SOIC8_EIAJ_208MIL">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NRES/PB5" pad="1"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-"/>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="X" package="TSSOP8_4MM4">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NRES/PB5" pad="1"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-"/>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY85*" prefix="U">
<description>&lt;h3&gt;ATMEL ATtiny 85&lt;/h3&gt;

&lt;p&gt;&lt;br /&gt;&lt;b&gt;&lt;u&gt;Packages:&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;P&lt;/b&gt; = PDIP 08 30mil&lt;br /&gt;
&lt;b&gt;S&lt;/b&gt; = SOIC 08 EIAJ 208mil&lt;/p&gt;

&lt;p&gt;&lt;b&gt;&lt;u&gt;Technologies&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
Note: for complete ordering code  (temp. range, finish, tape&amp;reel etc.) see www.atmel.com&lt;br /&gt;
&amp;bull; Supply Voltage:
  &lt;b&gt;V&lt;/b&gt; = (1.8&amp;hellip;5.5)V | &lt;b&gt;[blank]&lt;/b&gt; = (2.7&amp;hellip;5.5)V&lt;br /&gt;
&amp;bull; Speed:
  &lt;b&gt;10&lt;/b&gt; = 10 MHz | &lt;b&gt;20&lt;/b&gt; = 20 MHz
&lt;/pre&gt;&lt;/p&gt;
&lt;hr /&gt;

&lt;author&gt;
&lt;p&gt;&lt;u&gt;Author:&lt;/u&gt;&lt;br /&gt;
Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn (Heilbronn University), &lt;i&gt;rainer.bayer@hs-heilbronn.de&lt;/i&gt;&lt;br /&gt;
Ingenieurbüro ing-rb, &lt;i&gt;mail@ing-rb.de&lt;/i&gt;&lt;/p&gt;&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="ATTINY25_45_85"/>
</gates>
<devices>
<device name="P" package="PDIP08_300MIL">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NRES/PB5" pad="1"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-"/>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="S" package="SOIC8_EIAJ_208MIL">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NRES/PB5" pad="1"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-"/>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA16A4U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 16K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 1K - 2KBytes EEPROM
&lt;dd&gt;– 2K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-resolution extensions on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Five USARTs with IrDA support for one USART
&lt;dd&gt;– Two Two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One twelve-channel, 12-bit, 2mspsAnalog to Digital Converter
&lt;dd&gt;– One two-channel, 12-bit, 1msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;il&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O pins
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5" route="any"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA16C4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt; – 16K - 32KBytes of In-System Self-Programmable Flash
&lt;dd&gt; – 4KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt; – 1KBytes EEPROM
&lt;dd&gt; – 2K - 4KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt; – Four-channel event system
&lt;dd&gt; – Four 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt; – One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt; – Three USARTs with IrDA support for one USART
&lt;dd&gt; – Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt; – Two serial peripheral interfaces (SPIs)
&lt;dd&gt; – CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt; – 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt; – One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt; – Two Analog Comparators with window compare function, and current sources
&lt;dd&gt; – External interrupts on all general purpose I/O pins
&lt;dd&gt; – Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt; – QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt; – Power-on reset and programmable brown-out detection
&lt;dd&gt; – Internal and external clock options with PLL and prescaler
&lt;dd&gt; – Programmable multilevel interrupt controller
&lt;dd&gt; – Five sleep modes
&lt;dd&gt; – Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt; – 34 programmable I/O pins
&lt;dd&gt; – 44-lead TQFP
&lt;dd&gt; – 44-pad QFN
&lt;dd&gt; – 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt; – 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-UC" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA16D4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA® Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Four 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counter with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Two USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 200 ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44-lead TQFP
&lt;dd&gt;– 44-pad VQFN/QFN
&lt;dd&gt;– 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32A4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA™ Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Five USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillato
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32A4U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 16K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 1K - 2KBytes EEPROM
&lt;dd&gt;– 2K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-resolution extensions on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Five USARTs with IrDA support for one USART
&lt;dd&gt;– Two Two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One twelve-channel, 12-bit, 2mspsAnalog to Digital Converter
&lt;dd&gt;– One two-channel, 12-bit, 1msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;il&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O pins
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5" route="any"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32C4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt; – 16K - 32KBytes of In-System Self-Programmable Flash
&lt;dd&gt; – 4KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt; – 1KBytes EEPROM
&lt;dd&gt; – 2K - 4KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt; – Four-channel event system
&lt;dd&gt; – Four 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt; – One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt; – Three USARTs with IrDA support for one USART
&lt;dd&gt; – Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt; – Two serial peripheral interfaces (SPIs)
&lt;dd&gt; – CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt; – 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt; – One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt; – Two Analog Comparators with window compare function, and current sources
&lt;dd&gt; – External interrupts on all general purpose I/O pins
&lt;dd&gt; – Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt; – QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt; – Power-on reset and programmable brown-out detection
&lt;dd&gt; – Internal and external clock options with PLL and prescaler
&lt;dd&gt; – Programmable multilevel interrupt controller
&lt;dd&gt; – Five sleep modes
&lt;dd&gt; – Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt; – 34 programmable I/O pins
&lt;dd&gt; – 44-lead TQFP
&lt;dd&gt; – 44-pad QFN
&lt;dd&gt; – 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt; – 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-UC" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32D4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA® Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Four 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counter with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Two USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 200 ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44-lead TQFP
&lt;dd&gt;– 44-pad VQFN/QFN
&lt;dd&gt;– 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A1U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatileprogram and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External bus interface for up to 16Mbytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External bus interface for up to 128Mbit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Eight 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on two timer/counters
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Eight USARTs with IrDA support for one USART
&lt;dd&gt;– Four two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– Two sixteen channel, 12-bit, 2msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators (ACs) with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O pins
&lt;dd&gt;– 100 lead TQFP
&lt;dd&gt;– 100 ball BGA
&lt;dd&gt;– 100 ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93" route="any"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64 KB - 256 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 16 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Seven 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Seven USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– Two Two-wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Three SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for test, debug and programming
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA™ Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Five USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillato
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A4U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 16K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 1K - 2KBytes EEPROM
&lt;dd&gt;– 2K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-resolution extensions on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Five USARTs with IrDA support for one USART
&lt;dd&gt;– Two Two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One twelve-channel, 12-bit, 2mspsAnalog to Digital Converter
&lt;dd&gt;– One two-channel, 12-bit, 1msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;il&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O pins
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5" route="any"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64B1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA B1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Two-channel DMA controller
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Three 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extensions one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Split mode on two timer/counters
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Two USARTs with IrDA support for one USART
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– One two-wire interface with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– One serial peripheral interface (SPI)
&lt;dd&gt;– 16-bit Real Time Counter (RTC) with separate oscillator
&lt;dd&gt;– Liquid Crystal Display
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Up to 4x40 segment driver
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Built in contrast control
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;ASCII character mapping
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Flexible SWAP of segment and common terminals buses
&lt;dd&gt;– Two eight-channel, 12-bit, 300 thousand SPS Analog to Digital Converters
&lt;dd&gt;– Four Analog Comparators with window compare function, and current source feature
&lt;dd&gt;– External interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 53 Programmable I/O pins
&lt;dd&gt;– 100-lead TQFP
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="B1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64B3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA B3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Two-channel DMA controller
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Two 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extensions one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Split mode on timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– One USART with IrDA support
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE 802.3) generator
&lt;dd&gt;– One two-wire interface with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– One serial peripheral interface (SPI)
&lt;dd&gt;– 16-bit Real Time Counter (RTC) with separate oscillator
&lt;dd&gt;– Liquid Crystal Display
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;4x25 segment driver
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Built in contrast control
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;ASCII character mappingGra
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Flexible SWAP of segment and common terminals buses
&lt;dd&gt;– One eight-channel, 12-bit, 300 thousand SPS Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current source feature
&lt;dd&gt;– External interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 36 Programmable I/O pins
&lt;dd&gt;– 64 - lead TQFP
&lt;dd&gt;– 64 - pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="B3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="13"/>
<connect gate="G$1" pin="AGND" pad="55"/>
<connect gate="G$1" pin="AVCC" pad="56"/>
<connect gate="G$1" pin="BIAS1" pad="44"/>
<connect gate="G$1" pin="BIAS2" pad="45"/>
<connect gate="G$1" pin="CAPH" pad="48"/>
<connect gate="G$1" pin="CAPL" pad="47"/>
<connect gate="G$1" pin="COM0" pad="49"/>
<connect gate="G$1" pin="COM1" pad="50"/>
<connect gate="G$1" pin="COM2" pad="51"/>
<connect gate="G$1" pin="COM3" pad="52"/>
<connect gate="G$1" pin="GND" pad="9 15 42"/>
<connect gate="G$1" pin="PB0" pad="57"/>
<connect gate="G$1" pin="PB1" pad="58"/>
<connect gate="G$1" pin="PB2" pad="59"/>
<connect gate="G$1" pin="PB3" pad="60"/>
<connect gate="G$1" pin="PB4" pad="61"/>
<connect gate="G$1" pin="PB5" pad="62"/>
<connect gate="G$1" pin="PB6" pad="63"/>
<connect gate="G$1" pin="PB7" pad="64"/>
<connect gate="G$1" pin="PC0" pad="1"/>
<connect gate="G$1" pin="PC1" pad="2"/>
<connect gate="G$1" pin="PC2" pad="3"/>
<connect gate="G$1" pin="PC3" pad="4"/>
<connect gate="G$1" pin="PC4" pad="5"/>
<connect gate="G$1" pin="PC5" pad="6"/>
<connect gate="G$1" pin="PC6" pad="7"/>
<connect gate="G$1" pin="PC7" pad="8"/>
<connect gate="G$1" pin="PD0" pad="11"/>
<connect gate="G$1" pin="PD1" pad="12"/>
<connect gate="G$1" pin="PDI" pad="14"/>
<connect gate="G$1" pin="PG0/SEG24" pad="17"/>
<connect gate="G$1" pin="PG1/SEG23" pad="18"/>
<connect gate="G$1" pin="PG2/SEG22" pad="19"/>
<connect gate="G$1" pin="PG3/SEG21" pad="20"/>
<connect gate="G$1" pin="PG4/SEG20" pad="21"/>
<connect gate="G$1" pin="PG5/SEG19" pad="22"/>
<connect gate="G$1" pin="PG6/SEG18" pad="23"/>
<connect gate="G$1" pin="PG7/SEG17" pad="24"/>
<connect gate="G$1" pin="PM0/SEG16" pad="25"/>
<connect gate="G$1" pin="PM1/SEG15" pad="26"/>
<connect gate="G$1" pin="PM2/SEG14" pad="27"/>
<connect gate="G$1" pin="PM3/SEG13" pad="28"/>
<connect gate="G$1" pin="PM4/SEG12" pad="29"/>
<connect gate="G$1" pin="PM5/SEG11" pad="30"/>
<connect gate="G$1" pin="PM6/SEG10" pad="31"/>
<connect gate="G$1" pin="PM7/SEG9" pad="32"/>
<connect gate="G$1" pin="PR0" pad="53"/>
<connect gate="G$1" pin="PR1" pad="54"/>
<connect gate="G$1" pin="SEG0" pad="41"/>
<connect gate="G$1" pin="SEG1" pad="40"/>
<connect gate="G$1" pin="SEG2" pad="39"/>
<connect gate="G$1" pin="SEG3" pad="38"/>
<connect gate="G$1" pin="SEG4" pad="37"/>
<connect gate="G$1" pin="SEG5" pad="36"/>
<connect gate="G$1" pin="SEG6" pad="35"/>
<connect gate="G$1" pin="SEG7" pad="34"/>
<connect gate="G$1" pin="SEG8" pad="33"/>
<connect gate="G$1" pin="VCC" pad="10 16 43"/>
<connect gate="G$1" pin="VLCD" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="13"/>
<connect gate="G$1" pin="AGND" pad="55"/>
<connect gate="G$1" pin="AVCC" pad="56"/>
<connect gate="G$1" pin="BIAS1" pad="44"/>
<connect gate="G$1" pin="BIAS2" pad="45"/>
<connect gate="G$1" pin="CAPH" pad="48"/>
<connect gate="G$1" pin="CAPL" pad="47"/>
<connect gate="G$1" pin="COM0" pad="49"/>
<connect gate="G$1" pin="COM1" pad="50"/>
<connect gate="G$1" pin="COM2" pad="51"/>
<connect gate="G$1" pin="COM3" pad="52"/>
<connect gate="G$1" pin="GND" pad="9 15 42 TH"/>
<connect gate="G$1" pin="PB0" pad="57"/>
<connect gate="G$1" pin="PB1" pad="58"/>
<connect gate="G$1" pin="PB2" pad="59"/>
<connect gate="G$1" pin="PB3" pad="60"/>
<connect gate="G$1" pin="PB4" pad="61"/>
<connect gate="G$1" pin="PB5" pad="62"/>
<connect gate="G$1" pin="PB6" pad="63"/>
<connect gate="G$1" pin="PB7" pad="64"/>
<connect gate="G$1" pin="PC0" pad="1"/>
<connect gate="G$1" pin="PC1" pad="2"/>
<connect gate="G$1" pin="PC2" pad="3"/>
<connect gate="G$1" pin="PC3" pad="4"/>
<connect gate="G$1" pin="PC4" pad="5"/>
<connect gate="G$1" pin="PC5" pad="6"/>
<connect gate="G$1" pin="PC6" pad="7"/>
<connect gate="G$1" pin="PC7" pad="8"/>
<connect gate="G$1" pin="PD0" pad="11"/>
<connect gate="G$1" pin="PD1" pad="12"/>
<connect gate="G$1" pin="PDI" pad="14"/>
<connect gate="G$1" pin="PG0/SEG24" pad="17"/>
<connect gate="G$1" pin="PG1/SEG23" pad="18"/>
<connect gate="G$1" pin="PG2/SEG22" pad="19"/>
<connect gate="G$1" pin="PG3/SEG21" pad="20"/>
<connect gate="G$1" pin="PG4/SEG20" pad="21"/>
<connect gate="G$1" pin="PG5/SEG19" pad="22"/>
<connect gate="G$1" pin="PG6/SEG18" pad="23"/>
<connect gate="G$1" pin="PG7/SEG17" pad="24"/>
<connect gate="G$1" pin="PM0/SEG16" pad="25"/>
<connect gate="G$1" pin="PM1/SEG15" pad="26"/>
<connect gate="G$1" pin="PM2/SEG14" pad="27"/>
<connect gate="G$1" pin="PM3/SEG13" pad="28"/>
<connect gate="G$1" pin="PM4/SEG12" pad="29"/>
<connect gate="G$1" pin="PM5/SEG11" pad="30"/>
<connect gate="G$1" pin="PM6/SEG10" pad="31"/>
<connect gate="G$1" pin="PM7/SEG9" pad="32"/>
<connect gate="G$1" pin="PR0" pad="53"/>
<connect gate="G$1" pin="PR1" pad="54"/>
<connect gate="G$1" pin="SEG0" pad="41"/>
<connect gate="G$1" pin="SEG1" pad="40"/>
<connect gate="G$1" pin="SEG2" pad="39"/>
<connect gate="G$1" pin="SEG3" pad="38"/>
<connect gate="G$1" pin="SEG4" pad="37"/>
<connect gate="G$1" pin="SEG5" pad="36"/>
<connect gate="G$1" pin="SEG6" pad="35"/>
<connect gate="G$1" pin="SEG7" pad="34"/>
<connect gate="G$1" pin="SEG8" pad="33"/>
<connect gate="G$1" pin="VCC" pad="10 16 43"/>
<connect gate="G$1" pin="VLCD" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64C3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt; High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt; Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256KBytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4KBytes EEPROM
&lt;dd&gt;– 4K - 16KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Three USARTs with IrDA support for one USART
&lt;dd&gt;– Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 50 programmable I/O pins
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64D3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4K Bytes EEPROM
&lt;dd&gt;– 4K - 16K Bytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Three USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match(I2C and SMBus compatible)
&lt;dd&gt;– Two SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Sixteen-channel, 12-bit, 200ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64D4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA® Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Four 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counter with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Two USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 200 ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44-lead TQFP
&lt;dd&gt;– 44-pad VQFN/QFN
&lt;dd&gt;– 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A1U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatileprogram and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External bus interface for up to 16Mbytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External bus interface for up to 128Mbit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Eight 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on two timer/counters
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Eight USARTs with IrDA support for one USART
&lt;dd&gt;– Four two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– Two sixteen channel, 12-bit, 2msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators (ACs) with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O pins
&lt;dd&gt;– 100 lead TQFP
&lt;dd&gt;– 100 ball BGA
&lt;dd&gt;– 100 ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93" route="any"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64 KB - 256 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 16 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Seven 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Seven USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– Two Two-wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Three SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for test, debug and programming
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA™ Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Five USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillato
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A4U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 16K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 1K - 2KBytes EEPROM
&lt;dd&gt;– 2K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-resolution extensions on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Five USARTs with IrDA support for one USART
&lt;dd&gt;– Two Two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One twelve-channel, 12-bit, 2mspsAnalog to Digital Converter
&lt;dd&gt;– One two-channel, 12-bit, 1msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;il&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O pins
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5" route="any"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128B1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA B1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Two-channel DMA controller
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Three 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extensions one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Split mode on two timer/counters
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Two USARTs with IrDA support for one USART
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– One two-wire interface with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– One serial peripheral interface (SPI)
&lt;dd&gt;– 16-bit Real Time Counter (RTC) with separate oscillator
&lt;dd&gt;– Liquid Crystal Display
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Up to 4x40 segment driver
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Built in contrast control
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;ASCII character mapping
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Flexible SWAP of segment and common terminals buses
&lt;dd&gt;– Two eight-channel, 12-bit, 300 thousand SPS Analog to Digital Converters
&lt;dd&gt;– Four Analog Comparators with window compare function, and current source feature
&lt;dd&gt;– External interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 53 Programmable I/O pins
&lt;dd&gt;– 100-lead TQFP
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="B1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128B3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA B3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Two-channel DMA controller
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Two 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extensions one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Split mode on timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– One USART with IrDA support
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE 802.3) generator
&lt;dd&gt;– One two-wire interface with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– One serial peripheral interface (SPI)
&lt;dd&gt;– 16-bit Real Time Counter (RTC) with separate oscillator
&lt;dd&gt;– Liquid Crystal Display
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;4x25 segment driver
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Built in contrast control
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;ASCII character mappingGra
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Flexible SWAP of segment and common terminals buses
&lt;dd&gt;– One eight-channel, 12-bit, 300 thousand SPS Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current source feature
&lt;dd&gt;– External interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 36 Programmable I/O pins
&lt;dd&gt;– 64 - lead TQFP
&lt;dd&gt;– 64 - pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="B3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="13"/>
<connect gate="G$1" pin="AGND" pad="55"/>
<connect gate="G$1" pin="AVCC" pad="56"/>
<connect gate="G$1" pin="BIAS1" pad="44"/>
<connect gate="G$1" pin="BIAS2" pad="45"/>
<connect gate="G$1" pin="CAPH" pad="48"/>
<connect gate="G$1" pin="CAPL" pad="47"/>
<connect gate="G$1" pin="COM0" pad="49"/>
<connect gate="G$1" pin="COM1" pad="50"/>
<connect gate="G$1" pin="COM2" pad="51"/>
<connect gate="G$1" pin="COM3" pad="52"/>
<connect gate="G$1" pin="GND" pad="9 15 42"/>
<connect gate="G$1" pin="PB0" pad="57"/>
<connect gate="G$1" pin="PB1" pad="58"/>
<connect gate="G$1" pin="PB2" pad="59"/>
<connect gate="G$1" pin="PB3" pad="60"/>
<connect gate="G$1" pin="PB4" pad="61"/>
<connect gate="G$1" pin="PB5" pad="62"/>
<connect gate="G$1" pin="PB6" pad="63"/>
<connect gate="G$1" pin="PB7" pad="64"/>
<connect gate="G$1" pin="PC0" pad="1"/>
<connect gate="G$1" pin="PC1" pad="2"/>
<connect gate="G$1" pin="PC2" pad="3"/>
<connect gate="G$1" pin="PC3" pad="4"/>
<connect gate="G$1" pin="PC4" pad="5"/>
<connect gate="G$1" pin="PC5" pad="6"/>
<connect gate="G$1" pin="PC6" pad="7"/>
<connect gate="G$1" pin="PC7" pad="8"/>
<connect gate="G$1" pin="PD0" pad="11"/>
<connect gate="G$1" pin="PD1" pad="12"/>
<connect gate="G$1" pin="PDI" pad="14"/>
<connect gate="G$1" pin="PG0/SEG24" pad="17"/>
<connect gate="G$1" pin="PG1/SEG23" pad="18"/>
<connect gate="G$1" pin="PG2/SEG22" pad="19"/>
<connect gate="G$1" pin="PG3/SEG21" pad="20"/>
<connect gate="G$1" pin="PG4/SEG20" pad="21"/>
<connect gate="G$1" pin="PG5/SEG19" pad="22"/>
<connect gate="G$1" pin="PG6/SEG18" pad="23"/>
<connect gate="G$1" pin="PG7/SEG17" pad="24"/>
<connect gate="G$1" pin="PM0/SEG16" pad="25"/>
<connect gate="G$1" pin="PM1/SEG15" pad="26"/>
<connect gate="G$1" pin="PM2/SEG14" pad="27"/>
<connect gate="G$1" pin="PM3/SEG13" pad="28"/>
<connect gate="G$1" pin="PM4/SEG12" pad="29"/>
<connect gate="G$1" pin="PM5/SEG11" pad="30"/>
<connect gate="G$1" pin="PM6/SEG10" pad="31"/>
<connect gate="G$1" pin="PM7/SEG9" pad="32"/>
<connect gate="G$1" pin="PR0" pad="53"/>
<connect gate="G$1" pin="PR1" pad="54"/>
<connect gate="G$1" pin="SEG0" pad="41"/>
<connect gate="G$1" pin="SEG1" pad="40"/>
<connect gate="G$1" pin="SEG2" pad="39"/>
<connect gate="G$1" pin="SEG3" pad="38"/>
<connect gate="G$1" pin="SEG4" pad="37"/>
<connect gate="G$1" pin="SEG5" pad="36"/>
<connect gate="G$1" pin="SEG6" pad="35"/>
<connect gate="G$1" pin="SEG7" pad="34"/>
<connect gate="G$1" pin="SEG8" pad="33"/>
<connect gate="G$1" pin="VCC" pad="10 16 43"/>
<connect gate="G$1" pin="VLCD" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="13"/>
<connect gate="G$1" pin="AGND" pad="55"/>
<connect gate="G$1" pin="AVCC" pad="56"/>
<connect gate="G$1" pin="BIAS1" pad="44"/>
<connect gate="G$1" pin="BIAS2" pad="45"/>
<connect gate="G$1" pin="CAPH" pad="48"/>
<connect gate="G$1" pin="CAPL" pad="47"/>
<connect gate="G$1" pin="COM0" pad="49"/>
<connect gate="G$1" pin="COM1" pad="50"/>
<connect gate="G$1" pin="COM2" pad="51"/>
<connect gate="G$1" pin="COM3" pad="52"/>
<connect gate="G$1" pin="GND" pad="9 15 42 TH"/>
<connect gate="G$1" pin="PB0" pad="57"/>
<connect gate="G$1" pin="PB1" pad="58"/>
<connect gate="G$1" pin="PB2" pad="59"/>
<connect gate="G$1" pin="PB3" pad="60"/>
<connect gate="G$1" pin="PB4" pad="61"/>
<connect gate="G$1" pin="PB5" pad="62"/>
<connect gate="G$1" pin="PB6" pad="63"/>
<connect gate="G$1" pin="PB7" pad="64"/>
<connect gate="G$1" pin="PC0" pad="1"/>
<connect gate="G$1" pin="PC1" pad="2"/>
<connect gate="G$1" pin="PC2" pad="3"/>
<connect gate="G$1" pin="PC3" pad="4"/>
<connect gate="G$1" pin="PC4" pad="5"/>
<connect gate="G$1" pin="PC5" pad="6"/>
<connect gate="G$1" pin="PC6" pad="7"/>
<connect gate="G$1" pin="PC7" pad="8"/>
<connect gate="G$1" pin="PD0" pad="11"/>
<connect gate="G$1" pin="PD1" pad="12"/>
<connect gate="G$1" pin="PDI" pad="14"/>
<connect gate="G$1" pin="PG0/SEG24" pad="17"/>
<connect gate="G$1" pin="PG1/SEG23" pad="18"/>
<connect gate="G$1" pin="PG2/SEG22" pad="19"/>
<connect gate="G$1" pin="PG3/SEG21" pad="20"/>
<connect gate="G$1" pin="PG4/SEG20" pad="21"/>
<connect gate="G$1" pin="PG5/SEG19" pad="22"/>
<connect gate="G$1" pin="PG6/SEG18" pad="23"/>
<connect gate="G$1" pin="PG7/SEG17" pad="24"/>
<connect gate="G$1" pin="PM0/SEG16" pad="25"/>
<connect gate="G$1" pin="PM1/SEG15" pad="26"/>
<connect gate="G$1" pin="PM2/SEG14" pad="27"/>
<connect gate="G$1" pin="PM3/SEG13" pad="28"/>
<connect gate="G$1" pin="PM4/SEG12" pad="29"/>
<connect gate="G$1" pin="PM5/SEG11" pad="30"/>
<connect gate="G$1" pin="PM6/SEG10" pad="31"/>
<connect gate="G$1" pin="PM7/SEG9" pad="32"/>
<connect gate="G$1" pin="PR0" pad="53"/>
<connect gate="G$1" pin="PR1" pad="54"/>
<connect gate="G$1" pin="SEG0" pad="41"/>
<connect gate="G$1" pin="SEG1" pad="40"/>
<connect gate="G$1" pin="SEG2" pad="39"/>
<connect gate="G$1" pin="SEG3" pad="38"/>
<connect gate="G$1" pin="SEG4" pad="37"/>
<connect gate="G$1" pin="SEG5" pad="36"/>
<connect gate="G$1" pin="SEG6" pad="35"/>
<connect gate="G$1" pin="SEG7" pad="34"/>
<connect gate="G$1" pin="SEG8" pad="33"/>
<connect gate="G$1" pin="VCC" pad="10 16 43"/>
<connect gate="G$1" pin="VLCD" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128C3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt; High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt; Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256KBytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4KBytes EEPROM
&lt;dd&gt;– 4K - 16KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Three USARTs with IrDA support for one USART
&lt;dd&gt;– Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 50 programmable I/O pins
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128D3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4K Bytes EEPROM
&lt;dd&gt;– 4K - 16K Bytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Three USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match(I2C and SMBus compatible)
&lt;dd&gt;– Two SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Sixteen-channel, 12-bit, 200ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128D4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA® Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Four 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counter with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Two USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 200 ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44-lead TQFP
&lt;dd&gt;– 44-pad VQFN/QFN
&lt;dd&gt;– 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA192A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA192A3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64 KB - 256 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 16 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Seven 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Seven USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– Two Two-wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Three SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for test, debug and programming
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA192C3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt; High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt; Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256KBytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4KBytes EEPROM
&lt;dd&gt;– 4K - 16KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Three USARTs with IrDA support for one USART
&lt;dd&gt;– Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 50 programmable I/O pins
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA192D3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4K Bytes EEPROM
&lt;dd&gt;– 4K - 16K Bytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Three USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match(I2C and SMBus compatible)
&lt;dd&gt;– Two SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Sixteen-channel, 12-bit, 200ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA256A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA256A3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64 KB - 256 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 16 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Seven 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Seven USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– Two Two-wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Three SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for test, debug and programming
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA256C3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt; High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt; Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256KBytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4KBytes EEPROM
&lt;dd&gt;– 4K - 16KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Three USARTs with IrDA support for one USART
&lt;dd&gt;– Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 50 programmable I/O pins
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA256D3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4K Bytes EEPROM
&lt;dd&gt;– 4K - 16K Bytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Three USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match(I2C and SMBus compatible)
&lt;dd&gt;– Two SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Sixteen-channel, 12-bit, 200ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA384A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA16A4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA™ Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Five USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillato
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-ISP-6" prefix="JP">
<description>&lt;b&gt;AVR ISP-6&lt;/b&gt;&lt;p&gt; Serial Programming Header</description>
<gates>
<gate name="G$1" symbol="AVR-ISP-6"/>
</gates>
<devices>
<device name="VERT" package="AVR-ISP-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HORZ" package="AVR-ISP-6R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-ISP-6-EDGE">
<description>&lt;b&gt;6 pin edge connector for ISP with ATMEL MCUs.&lt;/b&gt;&lt;br&gt;
Developed by Craig Moates (craig at moates dot net).&lt;br&gt;
Library by David Blundell (blundar at gmail dot com).&lt;br&gt;
&lt;br&gt;
Often, even a 6 pin header is really inconvenient for board layout and/or production.  This SMD-only header is our de-facto standard for using an edge connector for programming with the help of a 6pin/10pin to edge card adapter.</description>
<gates>
<gate name="G$1" symbol="6PAD_ISP"/>
</gates>
<devices>
<device name="" package="6PAD_ISP">
<connects>
<connect gate="G$1" pin="P$1" pad="MISO"/>
<connect gate="G$1" pin="P$2" pad="SCK"/>
<connect gate="G$1" pin="P$3" pad="RST"/>
<connect gate="G$1" pin="P$4" pad="GND"/>
<connect gate="G$1" pin="P$5" pad="MOSI"/>
<connect gate="G$1" pin="P$6" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-ISP-10" prefix="JP">
<description>&lt;b&gt;AVR ISP-10&lt;/b&gt;&lt;p&gt; Serial Programming Header</description>
<gates>
<gate name="G$1" symbol="AVR-ISP-10"/>
</gates>
<devices>
<device name="" package="AVR-ISP-10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R" package="AVR-ISP-10R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-PDI">
<description>AVR PDI programming interface connector</description>
<gates>
<gate name="G$1" symbol="AVR-PDI"/>
</gates>
<devices>
<device name="VERT" package="AVR-ISP-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HORZ" package="AVR-ISP-6R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-TPI">
<description>AVR TPI connector</description>
<gates>
<gate name="G$1" symbol="AVR-TPI"/>
</gates>
<devices>
<device name="VERT" package="AVR-ISP-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HORZ" package="AVR-ISP-6R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA48/88/168" prefix="IC">
<gates>
<gate name="1" symbol="ATMEGA48/88/168-TQFP/QFN32"/>
</gates>
<devices>
<device name="-MU" package="MLF32">
<connects>
<connect gate="1" pin="ADC6" pad="19"/>
<connect gate="1" pin="ADC7" pad="22"/>
<connect gate="1" pin="AGND" pad="21"/>
<connect gate="1" pin="AREF" pad="20"/>
<connect gate="1" pin="AVCC" pad="18"/>
<connect gate="1" pin="GND@1" pad="3"/>
<connect gate="1" pin="GND@2" pad="5"/>
<connect gate="1" pin="PB0(ICP1/CLKO/PCINT0)" pad="12"/>
<connect gate="1" pin="PB1(OC1A/PCINT1)" pad="13"/>
<connect gate="1" pin="PB2(SS/OC1B/PCINT2)" pad="14"/>
<connect gate="1" pin="PB3(MOSI/OC2A/PCINT3)" pad="15"/>
<connect gate="1" pin="PB4(MISO/PCINT4)" pad="16"/>
<connect gate="1" pin="PB5(SCK/PCINT5)" pad="17"/>
<connect gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)" pad="7"/>
<connect gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)" pad="8"/>
<connect gate="1" pin="PC0(ADC0/PCINT8)" pad="23"/>
<connect gate="1" pin="PC1(ADC1/PCINT9)" pad="24"/>
<connect gate="1" pin="PC2(ADC2/PCINT10)" pad="25"/>
<connect gate="1" pin="PC3(ADC3/PCINT11)" pad="26"/>
<connect gate="1" pin="PC4(ADC4/SDA/PCINT12)" pad="27"/>
<connect gate="1" pin="PC5(ADC5/SCL/PCINT13)" pad="28"/>
<connect gate="1" pin="PC6(/RESET/PCINT14)" pad="29"/>
<connect gate="1" pin="PD0(RXD/PCINT16)" pad="30"/>
<connect gate="1" pin="PD1(TXD/PCINT17)" pad="31"/>
<connect gate="1" pin="PD2(INT0/PCINT18)" pad="32"/>
<connect gate="1" pin="PD3(INT1/OC2B/PCINT19)" pad="1"/>
<connect gate="1" pin="PD4(T0/XCK/PCINT20)" pad="2"/>
<connect gate="1" pin="PD5(T1/OC0B/PCINT21)" pad="9"/>
<connect gate="1" pin="PD6(AIN0/OC0A/PCINT22)" pad="10"/>
<connect gate="1" pin="PD7(AIN1/PCINT23)" pad="11"/>
<connect gate="1" pin="VCC@1" pad="4"/>
<connect gate="1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AU" package="TQFP32-08">
<connects>
<connect gate="1" pin="ADC6" pad="19"/>
<connect gate="1" pin="ADC7" pad="22"/>
<connect gate="1" pin="AGND" pad="21"/>
<connect gate="1" pin="AREF" pad="20"/>
<connect gate="1" pin="AVCC" pad="18"/>
<connect gate="1" pin="GND@1" pad="3"/>
<connect gate="1" pin="GND@2" pad="5"/>
<connect gate="1" pin="PB0(ICP1/CLKO/PCINT0)" pad="12"/>
<connect gate="1" pin="PB1(OC1A/PCINT1)" pad="13"/>
<connect gate="1" pin="PB2(SS/OC1B/PCINT2)" pad="14"/>
<connect gate="1" pin="PB3(MOSI/OC2A/PCINT3)" pad="15"/>
<connect gate="1" pin="PB4(MISO/PCINT4)" pad="16"/>
<connect gate="1" pin="PB5(SCK/PCINT5)" pad="17"/>
<connect gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)" pad="7"/>
<connect gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)" pad="8"/>
<connect gate="1" pin="PC0(ADC0/PCINT8)" pad="23"/>
<connect gate="1" pin="PC1(ADC1/PCINT9)" pad="24"/>
<connect gate="1" pin="PC2(ADC2/PCINT10)" pad="25"/>
<connect gate="1" pin="PC3(ADC3/PCINT11)" pad="26"/>
<connect gate="1" pin="PC4(ADC4/SDA/PCINT12)" pad="27"/>
<connect gate="1" pin="PC5(ADC5/SCL/PCINT13)" pad="28"/>
<connect gate="1" pin="PC6(/RESET/PCINT14)" pad="29"/>
<connect gate="1" pin="PD0(RXD/PCINT16)" pad="30"/>
<connect gate="1" pin="PD1(TXD/PCINT17)" pad="31"/>
<connect gate="1" pin="PD2(INT0/PCINT18)" pad="32"/>
<connect gate="1" pin="PD3(INT1/OC2B/PCINT19)" pad="1"/>
<connect gate="1" pin="PD4(T0/XCK/PCINT20)" pad="2"/>
<connect gate="1" pin="PD5(T1/OC0B/PCINT21)" pad="9"/>
<connect gate="1" pin="PD6(AIN0/OC0A/PCINT22)" pad="10"/>
<connect gate="1" pin="PD7(AIN1/PCINT23)" pad="11"/>
<connect gate="1" pin="VCC@1" pad="4"/>
<connect gate="1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA48/88/168-PU" prefix="IC">
<gates>
<gate name="1" symbol="ATMEGA48/88/168"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="1" pin="AGND" pad="22"/>
<connect gate="1" pin="AREF" pad="21"/>
<connect gate="1" pin="AVCC" pad="20"/>
<connect gate="1" pin="GND@1" pad="8"/>
<connect gate="1" pin="PB0(ICP1/CLKO/PCINT0)" pad="14"/>
<connect gate="1" pin="PB1(OC1A/PCINT1)" pad="15"/>
<connect gate="1" pin="PB2(SS/OC1B/PCINT2)" pad="16"/>
<connect gate="1" pin="PB3(MOSI/OC2A/PCINT3)" pad="17"/>
<connect gate="1" pin="PB4(MISO/PCINT4)" pad="18"/>
<connect gate="1" pin="PB5(SCK/PCINT5)" pad="19"/>
<connect gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)" pad="9"/>
<connect gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)" pad="10"/>
<connect gate="1" pin="PC0(ADC0/PCINT8)" pad="23"/>
<connect gate="1" pin="PC1(ADC1/PCINT9)" pad="24"/>
<connect gate="1" pin="PC2(ADC2/PCINT10)" pad="25"/>
<connect gate="1" pin="PC3(ADC3/PCINT11)" pad="26"/>
<connect gate="1" pin="PC4(ADC4/SDA/PCINT12)" pad="27"/>
<connect gate="1" pin="PC5(ADC5/SCLPCINT13)" pad="28"/>
<connect gate="1" pin="PC6(/RESET/PCINT14)" pad="1"/>
<connect gate="1" pin="PD0(RXD/PCINT16)" pad="2"/>
<connect gate="1" pin="PD1(TXD/PCINT17)" pad="3"/>
<connect gate="1" pin="PD2(INT0/PCINT18)" pad="4"/>
<connect gate="1" pin="PD3(INT1/OC2B/PCINT19)" pad="5"/>
<connect gate="1" pin="PD4(T0/XCK/PCINT20)" pad="6"/>
<connect gate="1" pin="PD5(T1/OC0B/PCINT21)" pad="11"/>
<connect gate="1" pin="PD6(AIN0/OC0A/PCINT22)" pad="12"/>
<connect gate="1" pin="PD7(AIN1/PCINT23)" pad="13"/>
<connect gate="1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA164P/324P/644P-AU" prefix="IC">
<gates>
<gate name="G$1" symbol="ATMEGA164P/324P/644P-TQFP"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!RESET" pad="4"/>
<connect gate="G$1" pin="(ADC0/PCINT0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1/PCINT1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2/PCINT2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3/PCINT3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4/PCINT4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5/PCINT5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6/PCINT6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7/PCINT7)PA7" pad="30"/>
<connect gate="G$1" pin="(CLKO/T1/PCINT9)PB1" pad="41"/>
<connect gate="G$1" pin="(INT2/AIN0/PCINT10)PB2" pad="42"/>
<connect gate="G$1" pin="(MISO/PCINT14)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI/PCINT13)PB5" pad="1"/>
<connect gate="G$1" pin="(OC0A/AIN1/PCINT11)PB3" pad="43"/>
<connect gate="G$1" pin="(OC0B/!SS!/PCINT12)PB4" pad="44"/>
<connect gate="G$1" pin="(OC1A/PCINT29)PD5" pad="14"/>
<connect gate="G$1" pin="(OC2A/PCINT31)PD7" pad="16"/>
<connect gate="G$1" pin="(OC2B/ICP/PCINT30)PD6" pad="15"/>
<connect gate="G$1" pin="(RXD0/PCINT24)PD0" pad="9"/>
<connect gate="G$1" pin="(RXD1/INT0/PCINT26)PD2" pad="11"/>
<connect gate="G$1" pin="(SCK/PCINT15)PB7" pad="3"/>
<connect gate="G$1" pin="(SCL/PCINT16)PC0" pad="19"/>
<connect gate="G$1" pin="(SDA/PCINT17)PC1" pad="20"/>
<connect gate="G$1" pin="(TCK/PCINT18)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI/PCINT21)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO/PCINT20)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS/PCINT19)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1/PCINT22)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2/PCINT23)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD0/PCINT25)PD1" pad="10"/>
<connect gate="G$1" pin="(TXD1/INT1/PCINT27)PD3" pad="12"/>
<connect gate="G$1" pin="(XCK0/T0/PCINT8)PB0" pad="40"/>
<connect gate="G$1" pin="(XCK1/OC1B/PCINT28)PD4" pad="13"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="39"/>
<connect gate="G$1" pin="VCC@1" pad="5"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA164P/324P/644P-PU" prefix="IC">
<gates>
<gate name="G$1" symbol="ATMEGA164P/324P/644P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!RESET" pad="9"/>
<connect gate="G$1" pin="(ADC0/PCINT0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1/PCINT1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2/PCINT2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3/PCINT3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4/PCINT4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5/PCINT5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6/PCINT6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7/PCINT7)PA7" pad="33"/>
<connect gate="G$1" pin="(CLKO/T1/PCINT9)PB1" pad="2"/>
<connect gate="G$1" pin="(INT2/AIN0/PCINT10)PB2" pad="3"/>
<connect gate="G$1" pin="(MISO/PCINT14)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI/PCINT13)PB5" pad="6"/>
<connect gate="G$1" pin="(OC0A/AIN1/PCINT11)PB3" pad="4"/>
<connect gate="G$1" pin="(OC0B/!SS!/PCINT12)PB4" pad="5"/>
<connect gate="G$1" pin="(OC1A/PCINT29)PD5" pad="19"/>
<connect gate="G$1" pin="(OC2A/PCINT31)PD7" pad="21"/>
<connect gate="G$1" pin="(OC2B/ICP/PCINT30)PD6" pad="20"/>
<connect gate="G$1" pin="(RXD0/PCINT24)PD0" pad="14"/>
<connect gate="G$1" pin="(RXD1/INT0/PCINT26)PD2" pad="16"/>
<connect gate="G$1" pin="(SCK/PCINT15)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL/PCINT16)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA/PCINT17)PC1" pad="23"/>
<connect gate="G$1" pin="(TCK/PCINT18)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI/PCINT21)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO/PCINT20)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS/PCINT19)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1/PCINT22)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2/PCINT23)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD0/PCINT25)PD1" pad="15"/>
<connect gate="G$1" pin="(TXD1/INT1/PCINT27)PD3" pad="17"/>
<connect gate="G$1" pin="(XCK0/T0/PCINT8)PB0" pad="1"/>
<connect gate="G$1" pin="(XCK1/OC1B/PCINT28)PD4" pad="18"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="31"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY24/44/84" prefix="IC" uservalue="yes">
<description>• High Performance, Low Power AVR® 8-bit Microcontroller
• Advanced RISC Architecture
– 120 Powerful Instructions – Most Single Clock Cycle Execution
– 32 x 8 General Purpose Working Registers
– Fully Static Operation
• High Endurance, Non-volatile Memory Segments
– 2K/4K/8K Bytes of In-System, Self-programmable Flash Program Memory
• Endurance: 10,000 Write/Erase Cycles
– 128/256/512 Bytes of In-System Programmable EEPROM
• Endurance: 100,000 Write/Erase Cycles
– 128/256/512 Bytes of Internal SRAM
– Data Retention: 20 years at 85°C / 100 years at 25°C
– Programming Lock for Self-programming Flash &amp; EEPROM Data Security
• Peripheral Features
– One 8-bit and One 16-bit Timer/Counter with Two PWM Channels, Each
– 10-bit ADC
• 8 Single-ended Channels
• 12 Differential ADC Channel Pairs with Programmable Gain (1x / 20x)
– Programmable Watchdog Timer with Separate On-chip Oscillator
– On-chip Analog Comparator
– Universal Serial Interface
• Special Microcontroller Features
– debugWIRE On-chip Debug System
– In-System Programmable via SPI Port
– Internal and External Interrupt Sources
• Pin Change Interrupt on 12 Pins
– Low Power Idle, ADC Noise Reduction, Standby and Power-down Modes
– Enhanced Power-on Reset Circuit
– Programmable Brown-out Detection Circuit with Software Disable Function
– Internal Calibrated Oscillator
– On-chip Temperature Sensor
• I/O and Packages
– Available in 20-pin QFN/MLF/VQFN, 14-pin SOIC, 14-pin PDIP and 15-ball UFBGA
– Twelve Programmable I/O Lines
• Operating Voltage:
– 1.8 – 5.5V
• Speed Grade:
– 0 – 4 MHz @ 1.8 – 5.5V
– 0 – 10 MHz @ 2.7 – 5.5V
– 0 – 20 MHz @ 4.5 – 5.5V
• Industrial Temperature Range: -40°C to +85°C
• Low Power Consumption
– Active Mode:
• 210 μA at 1.8V and 1 MHz
– Idle Mode:
• 33 μA at 1.8V and 1 MHz
– Power-down Mode:
• 0.1 μA at 1.8V and 25°C</description>
<gates>
<gate name="1" symbol="ATTINY24/44/84"/>
</gates>
<devices>
<device name="-SSU" package="SOIC14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PU" package="DIL14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MU" package="QFN/MLF20">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="5"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="4"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="14"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="13"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="3"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="2"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="1"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="20"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="16"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="15"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="11"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="12"/>
<connect gate="1" pin="GND" pad="8"/>
<connect gate="1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY25/45/85">
<gates>
<gate name="G$1" symbol="6-I/O-4"/>
</gates>
<devices>
<device name="-20SU" package="SOIC8">
<connects>
<connect gate="G$1" pin="(ADC0)PB5" pad="1"/>
<connect gate="G$1" pin="(ADC1)PB2" pad="7"/>
<connect gate="G$1" pin="(ADC2)PB4" pad="3"/>
<connect gate="G$1" pin="(ADC3)PB3" pad="2"/>
<connect gate="G$1" pin="(AREF)PB0" pad="5"/>
<connect gate="G$1" pin="(OCP)PB1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY2313*">
<description>Atmel Tiny2313
2K Flash, 128 bytes EEPROM, 128 bytes RAM</description>
<gates>
<gate name="G$1" symbol="18-I/O-1"/>
</gates>
<devices>
<device name="-*P*" package="DIL20">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(OC0A)PB2" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB4" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="(UCSK)PB7" pad="19"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PA0(XTAL1)" pad="5"/>
<connect gate="G$1" pin="PA1(XTAL2)" pad="4"/>
<connect gate="G$1" pin="PA2(/RESET)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-*S*" package="SO20L$">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(OC0A)PB2" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB4" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="(UCSK)PB7" pad="19"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PA0(XTAL1)" pad="5"/>
<connect gate="G$1" pin="PA1(XTAL2)" pad="4"/>
<connect gate="G$1" pin="PA2(/RESET)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-*M*" package="MLF20">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="P$10"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="P$11"/>
<connect gate="G$1" pin="(ICP)PD6" pad="P$9"/>
<connect gate="G$1" pin="(INT0)PD2" pad="P$4"/>
<connect gate="G$1" pin="(INT1)PD3" pad="P$5"/>
<connect gate="G$1" pin="(MISO)PB6" pad="P$16"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="P$15"/>
<connect gate="G$1" pin="(OC0A)PB2" pad="P$12"/>
<connect gate="G$1" pin="(OC1A)PB3" pad="P$13"/>
<connect gate="G$1" pin="(OC1B)PB4" pad="P$14"/>
<connect gate="G$1" pin="(RXD)PD0" pad="P$20"/>
<connect gate="G$1" pin="(T0)PD4" pad="P$6"/>
<connect gate="G$1" pin="(T1)PD5" pad="P$7"/>
<connect gate="G$1" pin="(TXD)PD1" pad="P$1"/>
<connect gate="G$1" pin="(UCSK)PB7" pad="P$17"/>
<connect gate="G$1" pin="GND" pad="P$8"/>
<connect gate="G$1" pin="PA0(XTAL1)" pad="P$3"/>
<connect gate="G$1" pin="PA1(XTAL2)" pad="P$2"/>
<connect gate="G$1" pin="PA2(/RESET)" pad="P$19"/>
<connect gate="G$1" pin="VCC" pad="P$18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JTAG-ARM-" prefix="J">
<description>JTAG Programming/Debug Connector</description>
<gates>
<gate name="G$1" symbol="JTAG-ARM"/>
</gates>
<devices>
<device name="HDR100" package="JTAG-ARM">
<connects>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="NTRST" pad="3"/>
<connect gate="G$1" pin="OBGACK" pad="19"/>
<connect gate="G$1" pin="OBGRQ" pad="17"/>
<connect gate="G$1" pin="RST" pad="15"/>
<connect gate="G$1" pin="RTCK" pad="11"/>
<connect gate="G$1" pin="TCK" pad="9"/>
<connect gate="G$1" pin="TDI" pad="5"/>
<connect gate="G$1" pin="TDO" pad="13"/>
<connect gate="G$1" pin="TMS" pad="7"/>
<connect gate="G$1" pin="VREF" pad="1"/>
<connect gate="G$1" pin="VTAR" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PAK100/2500-20" package="PAK100/2500-20">
<connects>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="NTRST" pad="3"/>
<connect gate="G$1" pin="OBGACK" pad="19"/>
<connect gate="G$1" pin="OBGRQ" pad="17"/>
<connect gate="G$1" pin="RST" pad="15"/>
<connect gate="G$1" pin="RTCK" pad="11"/>
<connect gate="G$1" pin="TCK" pad="9"/>
<connect gate="G$1" pin="TDI" pad="5"/>
<connect gate="G$1" pin="TDO" pad="13"/>
<connect gate="G$1" pin="TMS" pad="7"/>
<connect gate="G$1" pin="VREF" pad="1"/>
<connect gate="G$1" pin="VTAR" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5103309-5" package="5103309-5">
<connects>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="NTRST" pad="3"/>
<connect gate="G$1" pin="OBGACK" pad="19"/>
<connect gate="G$1" pin="OBGRQ" pad="17"/>
<connect gate="G$1" pin="RST" pad="15"/>
<connect gate="G$1" pin="RTCK" pad="11"/>
<connect gate="G$1" pin="TCK" pad="9"/>
<connect gate="G$1" pin="TDI" pad="5"/>
<connect gate="G$1" pin="TDO" pad="13"/>
<connect gate="G$1" pin="TMS" pad="7"/>
<connect gate="G$1" pin="VREF" pad="1"/>
<connect gate="G$1" pin="VTAR" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT572D940HF" prefix="U">
<gates>
<gate name="G$1" symbol="AT572D940HF"/>
</gates>
<devices>
<device name="" package="CABGA324">
<connects>
<connect gate="G$1" pin="A0/NBS0" pad="B2"/>
<connect gate="G$1" pin="A1/NBS2/NWR2" pad="C2"/>
<connect gate="G$1" pin="A10" pad="F3"/>
<connect gate="G$1" pin="A11" pad="H8"/>
<connect gate="G$1" pin="A12" pad="F2"/>
<connect gate="G$1" pin="A13" pad="F1"/>
<connect gate="G$1" pin="A14" pad="G3"/>
<connect gate="G$1" pin="A15" pad="H7"/>
<connect gate="G$1" pin="A16/SD_BA0" pad="G1"/>
<connect gate="G$1" pin="A17/SD_BA1" pad="G2"/>
<connect gate="G$1" pin="A18" pad="H6"/>
<connect gate="G$1" pin="A19" pad="H3"/>
<connect gate="G$1" pin="A2" pad="C1"/>
<connect gate="G$1" pin="A20" pad="J8"/>
<connect gate="G$1" pin="A21" pad="H2"/>
<connect gate="G$1" pin="A3" pad="D4"/>
<connect gate="G$1" pin="A4" pad="D3"/>
<connect gate="G$1" pin="A5" pad="D1"/>
<connect gate="G$1" pin="A6" pad="E4"/>
<connect gate="G$1" pin="A7" pad="E3"/>
<connect gate="G$1" pin="A8" pad="F6"/>
<connect gate="G$1" pin="A9" pad="G6"/>
<connect gate="G$1" pin="A_JCFG" pad="N16"/>
<connect gate="G$1" pin="A_NTRST" pad="M13"/>
<connect gate="G$1" pin="A_RTCK" pad="M17"/>
<connect gate="G$1" pin="A_TCK" pad="N17"/>
<connect gate="G$1" pin="A_TDI" pad="M14"/>
<connect gate="G$1" pin="A_TDO" pad="M16"/>
<connect gate="G$1" pin="A_TMS" pad="N15"/>
<connect gate="G$1" pin="D0" pad="H1"/>
<connect gate="G$1" pin="D1" pad="J7"/>
<connect gate="G$1" pin="D10" pad="K8"/>
<connect gate="G$1" pin="D11" pad="L5"/>
<connect gate="G$1" pin="D12" pad="L1"/>
<connect gate="G$1" pin="D13" pad="L2"/>
<connect gate="G$1" pin="D14" pad="L4"/>
<connect gate="G$1" pin="D15" pad="L7"/>
<connect gate="G$1" pin="D16" pad="M3"/>
<connect gate="G$1" pin="D17" pad="L8"/>
<connect gate="G$1" pin="D18" pad="M4"/>
<connect gate="G$1" pin="D19" pad="M5"/>
<connect gate="G$1" pin="D2" pad="J2"/>
<connect gate="G$1" pin="D20" pad="M6"/>
<connect gate="G$1" pin="D21" pad="N1"/>
<connect gate="G$1" pin="D22" pad="M7"/>
<connect gate="G$1" pin="D23" pad="N4"/>
<connect gate="G$1" pin="D24" pad="N5"/>
<connect gate="G$1" pin="D25" pad="P1"/>
<connect gate="G$1" pin="D26" pad="P3"/>
<connect gate="G$1" pin="D27" pad="P4"/>
<connect gate="G$1" pin="D28" pad="P5"/>
<connect gate="G$1" pin="D29" pad="R1"/>
<connect gate="G$1" pin="D3" pad="J1"/>
<connect gate="G$1" pin="D30" pad="R2"/>
<connect gate="G$1" pin="D31" pad="R3"/>
<connect gate="G$1" pin="D4" pad="K9"/>
<connect gate="G$1" pin="D5" pad="K7"/>
<connect gate="G$1" pin="D6" pad="K5"/>
<connect gate="G$1" pin="D7" pad="K1"/>
<connect gate="G$1" pin="D8" pad="K2"/>
<connect gate="G$1" pin="D9" pad="K6"/>
<connect gate="G$1" pin="GND@A14" pad="A14"/>
<connect gate="G$1" pin="GND@A3" pad="A3"/>
<connect gate="G$1" pin="GND@B1" pad="B1"/>
<connect gate="G$1" pin="GND@B13" pad="B13"/>
<connect gate="G$1" pin="GND@B14" pad="B14"/>
<connect gate="G$1" pin="GND@B15" pad="B15"/>
<connect gate="G$1" pin="GND@B18" pad="B18"/>
<connect gate="G$1" pin="GND@C12" pad="C12"/>
<connect gate="G$1" pin="GND@C17" pad="C17"/>
<connect gate="G$1" pin="GND@C18" pad="C18"/>
<connect gate="G$1" pin="GND@C3" pad="C3"/>
<connect gate="G$1" pin="GND@C4" pad="C4"/>
<connect gate="G$1" pin="GND@C7" pad="C7"/>
<connect gate="G$1" pin="GND@C8" pad="C8"/>
<connect gate="G$1" pin="GND@C9" pad="C9"/>
<connect gate="G$1" pin="GND@D17" pad="D17"/>
<connect gate="G$1" pin="GND@D18" pad="D18"/>
<connect gate="G$1" pin="GND@D2" pad="D2"/>
<connect gate="G$1" pin="GND@E10" pad="E10"/>
<connect gate="G$1" pin="GND@E11" pad="E11"/>
<connect gate="G$1" pin="GND@E2" pad="E2"/>
<connect gate="G$1" pin="GND@E6" pad="E6"/>
<connect gate="G$1" pin="GND@F10" pad="F10"/>
<connect gate="G$1" pin="GND@F15" pad="F15"/>
<connect gate="G$1" pin="GND@F5" pad="F5"/>
<connect gate="G$1" pin="GND@F8" pad="F8"/>
<connect gate="G$1" pin="GND@G15" pad="G15"/>
<connect gate="G$1" pin="GND@G5" pad="G5"/>
<connect gate="G$1" pin="GND@H12" pad="H12"/>
<connect gate="G$1" pin="GND@H5" pad="H5"/>
<connect gate="G$1" pin="GND@J11" pad="J11"/>
<connect gate="G$1" pin="GND@J12" pad="J12"/>
<connect gate="G$1" pin="GND@J14" pad="J14"/>
<connect gate="G$1" pin="GND@J16" pad="J16"/>
<connect gate="G$1" pin="GND@J3" pad="J3"/>
<connect gate="G$1" pin="GND@J6" pad="J6"/>
<connect gate="G$1" pin="GND@K18" pad="K18"/>
<connect gate="G$1" pin="GND@K4" pad="K4"/>
<connect gate="G$1" pin="GND@L14" pad="L14"/>
<connect gate="G$1" pin="GND@L17" pad="L17"/>
<connect gate="G$1" pin="GND@L3" pad="L3"/>
<connect gate="G$1" pin="GND@M1" pad="M1"/>
<connect gate="G$1" pin="GND@M15" pad="M15"/>
<connect gate="G$1" pin="GND@M8" pad="M8"/>
<connect gate="G$1" pin="GND@N18" pad="N18"/>
<connect gate="G$1" pin="GND@N2" pad="N2"/>
<connect gate="G$1" pin="GND@N6" pad="N6"/>
<connect gate="G$1" pin="GND@N9" pad="N9"/>
<connect gate="G$1" pin="GND@P15" pad="P15"/>
<connect gate="G$1" pin="GND@P18" pad="P18"/>
<connect gate="G$1" pin="GND@R11" pad="R11"/>
<connect gate="G$1" pin="GND@R13" pad="R13"/>
<connect gate="G$1" pin="GND@R16" pad="R16"/>
<connect gate="G$1" pin="GND@R17" pad="R17"/>
<connect gate="G$1" pin="GND@R4" pad="R4"/>
<connect gate="G$1" pin="GND@R6" pad="R6"/>
<connect gate="G$1" pin="GND@R8" pad="R8"/>
<connect gate="G$1" pin="GND@T1" pad="T1"/>
<connect gate="G$1" pin="GND@T11" pad="T11"/>
<connect gate="G$1" pin="GND@T6" pad="T6"/>
<connect gate="G$1" pin="GND@T8" pad="T8"/>
<connect gate="G$1" pin="GND@U1" pad="U1"/>
<connect gate="G$1" pin="GND@U10" pad="U10"/>
<connect gate="G$1" pin="GND@U14" pad="U14"/>
<connect gate="G$1" pin="GND@U16" pad="U16"/>
<connect gate="G$1" pin="GND@U6" pad="U6"/>
<connect gate="G$1" pin="GND@U9" pad="U9"/>
<connect gate="G$1" pin="GND@V11" pad="V11"/>
<connect gate="G$1" pin="GND@V12" pad="V12"/>
<connect gate="G$1" pin="GND@V4" pad="V4"/>
<connect gate="G$1" pin="GNDOSC32@T5" pad="T5"/>
<connect gate="G$1" pin="GNDOSCM@P7" pad="P7"/>
<connect gate="G$1" pin="GNDPLLA@U3" pad="U3"/>
<connect gate="G$1" pin="M_NTRST" pad="E16"/>
<connect gate="G$1" pin="M_TCK" pad="F13"/>
<connect gate="G$1" pin="M_TDI" pad="E15"/>
<connect gate="G$1" pin="M_TDO" pad="E14"/>
<connect gate="G$1" pin="M_TMS" pad="E17"/>
<connect gate="G$1" pin="NC@A1" pad="A1"/>
<connect gate="G$1" pin="NC@A18" pad="A18"/>
<connect gate="G$1" pin="NC@V1" pad="V1"/>
<connect gate="G$1" pin="NC@V18" pad="V18"/>
<connect gate="G$1" pin="NCS0" pad="F7"/>
<connect gate="G$1" pin="NCS1/SD_CS" pad="A6"/>
<connect gate="G$1" pin="NCS2" pad="B7"/>
<connect gate="G$1" pin="NCS3/SM_NCS" pad="E7"/>
<connect gate="G$1" pin="NRD/NOE/CF_NOE" pad="B6"/>
<connect gate="G$1" pin="NRST" pad="J17"/>
<connect gate="G$1" pin="NWR0/NWE/CF_NWE" pad="C6"/>
<connect gate="G$1" pin="NWR1/NBS1/CF_NIOR" pad="D6"/>
<connect gate="G$1" pin="NWR3/NBS3/CF_NIOW" pad="G7"/>
<connect gate="G$1" pin="PIOA0" pad="F11"/>
<connect gate="G$1" pin="PIOA1" pad="C11"/>
<connect gate="G$1" pin="PIOA10" pad="A16"/>
<connect gate="G$1" pin="PIOA11" pad="C15"/>
<connect gate="G$1" pin="PIOA12" pad="H17"/>
<connect gate="G$1" pin="PIOA13" pad="V15"/>
<connect gate="G$1" pin="PIOA14" pad="U15"/>
<connect gate="G$1" pin="PIOA15" pad="V16"/>
<connect gate="G$1" pin="PIOA16" pad="T15"/>
<connect gate="G$1" pin="PIOA17" pad="V17"/>
<connect gate="G$1" pin="PIOA18" pad="T16"/>
<connect gate="G$1" pin="PIOA19" pad="T17"/>
<connect gate="G$1" pin="PIOA2" pad="A11"/>
<connect gate="G$1" pin="PIOA20" pad="U18"/>
<connect gate="G$1" pin="PIOA21" pad="T18"/>
<connect gate="G$1" pin="PIOA22" pad="R15"/>
<connect gate="G$1" pin="PIOA23" pad="R18"/>
<connect gate="G$1" pin="PIOA24" pad="H16"/>
<connect gate="G$1" pin="PIOA25" pad="B9"/>
<connect gate="G$1" pin="PIOA26" pad="D9"/>
<connect gate="G$1" pin="PIOA27" pad="G9"/>
<connect gate="G$1" pin="PIOA28" pad="J9"/>
<connect gate="G$1" pin="PIOA29" pad="A8"/>
<connect gate="G$1" pin="PIOA3" pad="B11"/>
<connect gate="G$1" pin="PIOA30" pad="D8"/>
<connect gate="G$1" pin="PIOA31" pad="B8"/>
<connect gate="G$1" pin="PIOA4" pad="H10"/>
<connect gate="G$1" pin="PIOA5" pad="G10"/>
<connect gate="G$1" pin="PIOA6" pad="D10"/>
<connect gate="G$1" pin="PIOA7" pad="B17"/>
<connect gate="G$1" pin="PIOA8" pad="A17"/>
<connect gate="G$1" pin="PIOA9" pad="B16"/>
<connect gate="G$1" pin="PIOB0" pad="U8"/>
<connect gate="G$1" pin="PIOB1" pad="L9"/>
<connect gate="G$1" pin="PIOB10" pad="M10"/>
<connect gate="G$1" pin="PIOB11" pad="N11"/>
<connect gate="G$1" pin="PIOB12" pad="M11"/>
<connect gate="G$1" pin="PIOB13" pad="L11"/>
<connect gate="G$1" pin="PIOB14" pad="U12"/>
<connect gate="G$1" pin="PIOB15" pad="T12"/>
<connect gate="G$1" pin="PIOB16" pad="R12"/>
<connect gate="G$1" pin="PIOB17" pad="N12"/>
<connect gate="G$1" pin="PIOB18" pad="V13"/>
<connect gate="G$1" pin="PIOB19" pad="U13"/>
<connect gate="G$1" pin="PIOB2" pad="P9"/>
<connect gate="G$1" pin="PIOB20" pad="T13"/>
<connect gate="G$1" pin="PIOB21" pad="P13"/>
<connect gate="G$1" pin="PIOB22" pad="V14"/>
<connect gate="G$1" pin="PIOB23" pad="R14"/>
<connect gate="G$1" pin="PIOB24" pad="J10"/>
<connect gate="G$1" pin="PIOB25" pad="H15"/>
<connect gate="G$1" pin="PIOB26" pad="B12"/>
<connect gate="G$1" pin="PIOB27" pad="A12"/>
<connect gate="G$1" pin="PIOB28" pad="F9"/>
<connect gate="G$1" pin="PIOB29" pad="B10"/>
<connect gate="G$1" pin="PIOB3" pad="R9"/>
<connect gate="G$1" pin="PIOB30" pad="A10"/>
<connect gate="G$1" pin="PIOB31" pad="A9"/>
<connect gate="G$1" pin="PIOB4" pad="V9"/>
<connect gate="G$1" pin="PIOB5" pad="L10"/>
<connect gate="G$1" pin="PIOB6" pad="N10"/>
<connect gate="G$1" pin="PIOB7" pad="V10"/>
<connect gate="G$1" pin="PIOB8" pad="T10"/>
<connect gate="G$1" pin="PIOB9" pad="P10"/>
<connect gate="G$1" pin="PIOC0" pad="D15"/>
<connect gate="G$1" pin="PIOC1" pad="D14"/>
<connect gate="G$1" pin="PIOC10" pad="L12"/>
<connect gate="G$1" pin="PIOC11" pad="L13"/>
<connect gate="G$1" pin="PIOC12" pad="L18"/>
<connect gate="G$1" pin="PIOC13" pad="K12"/>
<connect gate="G$1" pin="PIOC14" pad="H13"/>
<connect gate="G$1" pin="PIOC15" pad="G17"/>
<connect gate="G$1" pin="PIOC16" pad="G18"/>
<connect gate="G$1" pin="PIOC17" pad="G14"/>
<connect gate="G$1" pin="PIOC18" pad="F17"/>
<connect gate="G$1" pin="PIOC19" pad="H14"/>
<connect gate="G$1" pin="PIOC2" pad="C14"/>
<connect gate="G$1" pin="PIOC20" pad="F16"/>
<connect gate="G$1" pin="PIOC21" pad="E18"/>
<connect gate="G$1" pin="PIOC22" pad="K14"/>
<connect gate="G$1" pin="PIOC23" pad="K16"/>
<connect gate="G$1" pin="PIOC24" pad="K17"/>
<connect gate="G$1" pin="PIOC25" pad="K15"/>
<connect gate="G$1" pin="PIOC26" pad="K11"/>
<connect gate="G$1" pin="PIOC27" pad="K10"/>
<connect gate="G$1" pin="PIOC28" pad="E12"/>
<connect gate="G$1" pin="PIOC29" pad="D12"/>
<connect gate="G$1" pin="PIOC3" pad="D13"/>
<connect gate="G$1" pin="PIOC30" pad="P16"/>
<connect gate="G$1" pin="PIOC31" pad="P17"/>
<connect gate="G$1" pin="PIOC4" pad="C13"/>
<connect gate="G$1" pin="PIOC5" pad="G12"/>
<connect gate="G$1" pin="PIOC6" pad="F12"/>
<connect gate="G$1" pin="PIOC7" pad="G13"/>
<connect gate="G$1" pin="PIOC8" pad="F18"/>
<connect gate="G$1" pin="PIOC9" pad="M18"/>
<connect gate="G$1" pin="PLL_RCA" pad="U2"/>
<connect gate="G$1" pin="PLL_RCB" pad="P6"/>
<connect gate="G$1" pin="SD_A10" pad="A7"/>
<connect gate="G$1" pin="SD_CK" pad="B5"/>
<connect gate="G$1" pin="SD_CKE" pad="C5"/>
<connect gate="G$1" pin="SD_NCAS" pad="A4"/>
<connect gate="G$1" pin="SD_NRAS" pad="D5"/>
<connect gate="G$1" pin="SD_NWE" pad="B4"/>
<connect gate="G$1" pin="TEST" pad="J18"/>
<connect gate="G$1" pin="USBD_M" pad="N8"/>
<connect gate="G$1" pin="USBD_P" pad="P8"/>
<connect gate="G$1" pin="USBHA_M" pad="R7"/>
<connect gate="G$1" pin="USBHA_P" pad="T7"/>
<connect gate="G$1" pin="USBHB_M" pad="U7"/>
<connect gate="G$1" pin="USBHB_P" pad="V7"/>
<connect gate="G$1" pin="VDDCORE@A2" pad="A2"/>
<connect gate="G$1" pin="VDDCORE@D16" pad="D16"/>
<connect gate="G$1" pin="VDDCORE@E13" pad="E13"/>
<connect gate="G$1" pin="VDDCORE@E8" pad="E8"/>
<connect gate="G$1" pin="VDDCORE@F4" pad="F4"/>
<connect gate="G$1" pin="VDDCORE@H11" pad="H11"/>
<connect gate="G$1" pin="VDDCORE@H9" pad="H9"/>
<connect gate="G$1" pin="VDDCORE@J13" pad="J13"/>
<connect gate="G$1" pin="VDDCORE@J4" pad="J4"/>
<connect gate="G$1" pin="VDDCORE@L15" pad="L15"/>
<connect gate="G$1" pin="VDDCORE@L6" pad="L6"/>
<connect gate="G$1" pin="VDDCORE@M9" pad="M9"/>
<connect gate="G$1" pin="VDDCORE@N13" pad="N13"/>
<connect gate="G$1" pin="VDDCORE@P11" pad="P11"/>
<connect gate="G$1" pin="VDDCORE@T14" pad="T14"/>
<connect gate="G$1" pin="VDDCORE@T2" pad="T2"/>
<connect gate="G$1" pin="VDDIOM@A5" pad="A5"/>
<connect gate="G$1" pin="VDDIOM@B3" pad="B3"/>
<connect gate="G$1" pin="VDDIOM@D7" pad="D7"/>
<connect gate="G$1" pin="VDDIOM@E1" pad="E1"/>
<connect gate="G$1" pin="VDDIOM@E5" pad="E5"/>
<connect gate="G$1" pin="VDDIOM@G4" pad="G4"/>
<connect gate="G$1" pin="VDDIOM@H4" pad="H4"/>
<connect gate="G$1" pin="VDDIOM@J5" pad="J5"/>
<connect gate="G$1" pin="VDDIOM@K3" pad="K3"/>
<connect gate="G$1" pin="VDDIOM@M2" pad="M2"/>
<connect gate="G$1" pin="VDDIOM@N3" pad="N3"/>
<connect gate="G$1" pin="VDDIOM@P2" pad="P2"/>
<connect gate="G$1" pin="VDDIOMP@E9" pad="E9"/>
<connect gate="G$1" pin="VDDIOMP@G8" pad="G8"/>
<connect gate="G$1" pin="VDDIOP@A13" pad="A13"/>
<connect gate="G$1" pin="VDDIOP@A15" pad="A15"/>
<connect gate="G$1" pin="VDDIOP@C10" pad="C10"/>
<connect gate="G$1" pin="VDDIOP@C16" pad="C16"/>
<connect gate="G$1" pin="VDDIOP@D11" pad="D11"/>
<connect gate="G$1" pin="VDDIOP@F14" pad="F14"/>
<connect gate="G$1" pin="VDDIOP@G11" pad="G11"/>
<connect gate="G$1" pin="VDDIOP@G16" pad="G16"/>
<connect gate="G$1" pin="VDDIOP@H18" pad="H18"/>
<connect gate="G$1" pin="VDDIOP@J15" pad="J15"/>
<connect gate="G$1" pin="VDDIOP@K13" pad="K13"/>
<connect gate="G$1" pin="VDDIOP@L16" pad="L16"/>
<connect gate="G$1" pin="VDDIOP@M12" pad="M12"/>
<connect gate="G$1" pin="VDDIOP@N14" pad="N14"/>
<connect gate="G$1" pin="VDDIOP@P12" pad="P12"/>
<connect gate="G$1" pin="VDDIOP@P14" pad="P14"/>
<connect gate="G$1" pin="VDDIOP@R10" pad="R10"/>
<connect gate="G$1" pin="VDDIOP@T9" pad="T9"/>
<connect gate="G$1" pin="VDDIOP@U11" pad="U11"/>
<connect gate="G$1" pin="VDDIOP@U17" pad="U17"/>
<connect gate="G$1" pin="VDDIOP@V6" pad="V6"/>
<connect gate="G$1" pin="VDDIOP@V8" pad="V8"/>
<connect gate="G$1" pin="VDDOSC32@U4" pad="U4"/>
<connect gate="G$1" pin="VDDOSCM@R5" pad="R5"/>
<connect gate="G$1" pin="VDDPLLA@T3" pad="T3"/>
<connect gate="G$1" pin="X32EN" pad="N7"/>
<connect gate="G$1" pin="X32IN" pad="V2"/>
<connect gate="G$1" pin="X32OUT" pad="V3"/>
<connect gate="G$1" pin="XIN" pad="U5"/>
<connect gate="G$1" pin="XOUT" pad="V5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91SAM9260B-QU" prefix="U">
<description>AT91SAM9260 MCU&lt;p&gt;
AT91 ARM-9 Thumb Microcontroller</description>
<gates>
<gate name="G$1" symbol="AT91SAM9260B-QU"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="G$1" pin="!CAS" pad="104"/>
<connect gate="G$1" pin="!RAS" pad="105"/>
<connect gate="G$1" pin="!SDWE" pad="116"/>
<connect gate="G$1" pin="A10" pad="87"/>
<connect gate="G$1" pin="A11" pad="86"/>
<connect gate="G$1" pin="A12" pad="85"/>
<connect gate="G$1" pin="A13" pad="84"/>
<connect gate="G$1" pin="A14" pad="83"/>
<connect gate="G$1" pin="A15" pad="82"/>
<connect gate="G$1" pin="A18" pad="79"/>
<connect gate="G$1" pin="A19" pad="76"/>
<connect gate="G$1" pin="A2" pad="97"/>
<connect gate="G$1" pin="A20" pad="75"/>
<connect gate="G$1" pin="A21" pad="74"/>
<connect gate="G$1" pin="A22" pad="73"/>
<connect gate="G$1" pin="A3" pad="96"/>
<connect gate="G$1" pin="A4" pad="95"/>
<connect gate="G$1" pin="A5" pad="94"/>
<connect gate="G$1" pin="A6" pad="93"/>
<connect gate="G$1" pin="A7" pad="92"/>
<connect gate="G$1" pin="A8" pad="89"/>
<connect gate="G$1" pin="A9" pad="88"/>
<connect gate="G$1" pin="ADVREF" pad="157"/>
<connect gate="G$1" pin="BA0/A16" pad="81"/>
<connect gate="G$1" pin="BA1/A17" pad="80"/>
<connect gate="G$1" pin="BMS" pad="40"/>
<connect gate="G$1" pin="CFCE1/TIOB2/PC6" pad="63"/>
<connect gate="G$1" pin="CFCE2/TIOB1/PC7" pad="64"/>
<connect gate="G$1" pin="CFIOR/NBS1/NWR1" pad="102"/>
<connect gate="G$1" pin="CFIOW/NBS3/NWR3" pad="101"/>
<connect gate="G$1" pin="CFOE/NRD" pad="69"/>
<connect gate="G$1" pin="CFWE/NWE/NWR0" pad="70"/>
<connect gate="G$1" pin="CTS3/A25_CFRNW/PC10" pad="58"/>
<connect gate="G$1" pin="D0" pad="106"/>
<connect gate="G$1" pin="D1" pad="107"/>
<connect gate="G$1" pin="D10" pad="121"/>
<connect gate="G$1" pin="D11" pad="122"/>
<connect gate="G$1" pin="D12" pad="123"/>
<connect gate="G$1" pin="D13" pad="124"/>
<connect gate="G$1" pin="D14" pad="125"/>
<connect gate="G$1" pin="D15" pad="126"/>
<connect gate="G$1" pin="D2" pad="108"/>
<connect gate="G$1" pin="D23/PC23" pad="137"/>
<connect gate="G$1" pin="D24/PC24" pad="138"/>
<connect gate="G$1" pin="D25/PC25" pad="139"/>
<connect gate="G$1" pin="D26/PC26" pad="140"/>
<connect gate="G$1" pin="D27/PC27" pad="141"/>
<connect gate="G$1" pin="D28/PC28" pad="142"/>
<connect gate="G$1" pin="D29/PC29" pad="143"/>
<connect gate="G$1" pin="D3" pad="109"/>
<connect gate="G$1" pin="D30/PC30" pad="144"/>
<connect gate="G$1" pin="D31/PC31" pad="145"/>
<connect gate="G$1" pin="D4" pad="110"/>
<connect gate="G$1" pin="D5" pad="111"/>
<connect gate="G$1" pin="D6" pad="112"/>
<connect gate="G$1" pin="D7" pad="118"/>
<connect gate="G$1" pin="D8" pad="119"/>
<connect gate="G$1" pin="D9" pad="120"/>
<connect gate="G$1" pin="DDM" pad="54"/>
<connect gate="G$1" pin="DDP" pad="55"/>
<connect gate="G$1" pin="DRXD/PB14" pad="21"/>
<connect gate="G$1" pin="DTXD/PB15" pad="22"/>
<connect gate="G$1" pin="EF100/D21/PC21" pad="135"/>
<connect gate="G$1" pin="GND@113" pad="113"/>
<connect gate="G$1" pin="GND@133" pad="133"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@146" pad="146"/>
<connect gate="G$1" pin="GND@170" pad="170"/>
<connect gate="G$1" pin="GND@173" pad="173"/>
<connect gate="G$1" pin="GND@188" pad="188"/>
<connect gate="G$1" pin="GND@200" pad="200"/>
<connect gate="G$1" pin="GND@204" pad="204"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@33" pad="33"/>
<connect gate="G$1" pin="GND@39" pad="39"/>
<connect gate="G$1" pin="GND@53" pad="53"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@66" pad="66"/>
<connect gate="G$1" pin="GND@78" pad="78"/>
<connect gate="G$1" pin="GND@91" pad="91"/>
<connect gate="G$1" pin="GNDANA" pad="156"/>
<connect gate="G$1" pin="GNDBU" pad="44"/>
<connect gate="G$1" pin="GNDPLL@151" pad="151"/>
<connect gate="G$1" pin="GNDPLL@153" pad="153"/>
<connect gate="G$1" pin="HDMA" pad="50"/>
<connect gate="G$1" pin="HDPA" pad="51"/>
<connect gate="G$1" pin="IRQ1/NWAIT/PC15" pad="127"/>
<connect gate="G$1" pin="IRQ2/NCS3_NANDCS/PC14" pad="59"/>
<connect gate="G$1" pin="ISI_D0/RK0/PB20" pad="163"/>
<connect gate="G$1" pin="ISI_D1/RF0/PB21" pad="164"/>
<connect gate="G$1" pin="ISI_D2/DSR0/PB22" pad="165"/>
<connect gate="G$1" pin="ISI_D3/DCD0/PB23" pad="166"/>
<connect gate="G$1" pin="ISI_D4/DTR0/PB24" pad="167"/>
<connect gate="G$1" pin="ISI_D5/RI0/PB25" pad="168"/>
<connect gate="G$1" pin="ISI_D6/RTS0/PB26" pad="171"/>
<connect gate="G$1" pin="ISI_D7/CTS0/PB27" pad="172"/>
<connect gate="G$1" pin="ISI_D8/TXD3/PB10" pad="161"/>
<connect gate="G$1" pin="ISI_D9/RXD3/PB11" pad="162"/>
<connect gate="G$1" pin="ISI_HSYNC/PCK0/PB30" pad="177"/>
<connect gate="G$1" pin="ISI_MCK/PCK1/PB31" pad="178"/>
<connect gate="G$1" pin="ISI_PCK/RTS1/PB28" pad="175"/>
<connect gate="G$1" pin="ISI_VSYNC/CTS1/PB29" pad="176"/>
<connect gate="G$1" pin="JTAGSEL" pad="43"/>
<connect gate="G$1" pin="NANDOE" pad="71"/>
<connect gate="G$1" pin="NANDWE" pad="72"/>
<connect gate="G$1" pin="NBS0/A0" pad="99"/>
<connect gate="G$1" pin="NC@152" pad="152"/>
<connect gate="G$1" pin="NCS6/FIQ/PC13" pad="56"/>
<connect gate="G$1" pin="NCSO" pad="68"/>
<connect gate="G$1" pin="NRST" pad="36"/>
<connect gate="G$1" pin="NTRST" pad="35"/>
<connect gate="G$1" pin="NWR2/NBS2/A1" pad="98"/>
<connect gate="G$1" pin="OSCSEL" pad="41"/>
<connect gate="G$1" pin="PA0/SPI0_MISO/MCDB0" pad="179"/>
<connect gate="G$1" pin="PA1/SPI0_MOSI/MCCDB" pad="180"/>
<connect gate="G$1" pin="PA10/MCDA2/ETX2" pad="191"/>
<connect gate="G$1" pin="PA11/MCDA3/ETX3" pad="192"/>
<connect gate="G$1" pin="PA12/ETX0" pad="193"/>
<connect gate="G$1" pin="PA13/ETX1" pad="194"/>
<connect gate="G$1" pin="PA14/ERX0" pad="195"/>
<connect gate="G$1" pin="PA15/ERX1" pad="196"/>
<connect gate="G$1" pin="PA16/ETXEN" pad="197"/>
<connect gate="G$1" pin="PA17/ERXDV" pad="198"/>
<connect gate="G$1" pin="PA18/ERXER" pad="201"/>
<connect gate="G$1" pin="PA19/ETXCK" pad="202"/>
<connect gate="G$1" pin="PA2/SPI0_SPCK" pad="181"/>
<connect gate="G$1" pin="PA20/EMDC" pad="205"/>
<connect gate="G$1" pin="PA21/EMDIO" pad="206"/>
<connect gate="G$1" pin="PA22/ADTRG/ETXER" pad="207"/>
<connect gate="G$1" pin="PA23/TWD/ETX2" pad="208"/>
<connect gate="G$1" pin="PA24/TWCK/ETX3" pad="1"/>
<connect gate="G$1" pin="PA25/TLCK0/ERX2" pad="2"/>
<connect gate="G$1" pin="PA26/TIOA0/ERX3" pad="3"/>
<connect gate="G$1" pin="PA27/TIOA1/ERXCK" pad="4"/>
<connect gate="G$1" pin="PA28/TIOA2/ECRS" pad="7"/>
<connect gate="G$1" pin="PA29/SCK1/ECOL" pad="8"/>
<connect gate="G$1" pin="PA3/SPI0_NPCS0/MCDB3" pad="182"/>
<connect gate="G$1" pin="PA4/RTS2/MCDB2" pad="183"/>
<connect gate="G$1" pin="PA5/CTS2/MCDB1" pad="184"/>
<connect gate="G$1" pin="PA6/MCDA0" pad="185"/>
<connect gate="G$1" pin="PA7/MCCDA" pad="186"/>
<connect gate="G$1" pin="PA8/MCCK" pad="189"/>
<connect gate="G$1" pin="PA9/MCDA1" pad="190"/>
<connect gate="G$1" pin="PCK0/AD1/PC1" pad="159"/>
<connect gate="G$1" pin="PLLRCA" pad="154"/>
<connect gate="G$1" pin="RTCK" pad="37"/>
<connect gate="G$1" pin="RTS3/NCS4_CFCS0/PC8" pad="61"/>
<connect gate="G$1" pin="RXD0/PB5" pad="16"/>
<connect gate="G$1" pin="RXD2/PB9" pad="20"/>
<connect gate="G$1" pin="SCK3/AD0/PC0" pad="158"/>
<connect gate="G$1" pin="SDA10" pad="100"/>
<connect gate="G$1" pin="SDCK" pad="115"/>
<connect gate="G$1" pin="SDCKE" pad="117"/>
<connect gate="G$1" pin="SDCS/NCS1" pad="103"/>
<connect gate="G$1" pin="SHDN" pad="49"/>
<connect gate="G$1" pin="SPI0_NPCS1/NCS2/PC11" pad="57"/>
<connect gate="G$1" pin="SPI0_NPCS2/D16/PC16" pad="128"/>
<connect gate="G$1" pin="SPI0_NPCS3/D17/PC17" pad="129"/>
<connect gate="G$1" pin="SPI1_NPCS1/A24/PC5" pad="67"/>
<connect gate="G$1" pin="SPI1_NPCS1/D18/PC18" pad="130"/>
<connect gate="G$1" pin="SPI1_NPCS2/A23/PC4" pad="62"/>
<connect gate="G$1" pin="SPI1_NPCS2/D19/PC19" pad="131"/>
<connect gate="G$1" pin="SPI1_NPCS3/D20/PC20" pad="134"/>
<connect gate="G$1" pin="TCK" pad="34"/>
<connect gate="G$1" pin="TCLK1/TXD1/PB6" pad="17"/>
<connect gate="G$1" pin="TCLK2/RXD1/PB7" pad="18"/>
<connect gate="G$1" pin="TCLK3/TK0/PB16" pad="23"/>
<connect gate="G$1" pin="TCLK4/TF0/PB17" pad="26"/>
<connect gate="G$1" pin="TCLK5/D22/PC22" pad="136"/>
<connect gate="G$1" pin="TDI" pad="30"/>
<connect gate="G$1" pin="TDO" pad="29"/>
<connect gate="G$1" pin="TIOA3/SPI1_MISO/PB0" pad="9"/>
<connect gate="G$1" pin="TIOA4/SPI1_SPCK/PB2" pad="11"/>
<connect gate="G$1" pin="TIOA5/SPI1_NPCS0/PB3" pad="12"/>
<connect gate="G$1" pin="TIOB0/NCS5_CFCS1/PC9" pad="60"/>
<connect gate="G$1" pin="TIOB3/SPI1_MOSI/PB1" pad="10"/>
<connect gate="G$1" pin="TIOB4/TD0/PB18" pad="27"/>
<connect gate="G$1" pin="TIOB5/RD0/PB19" pad="28"/>
<connect gate="G$1" pin="TMS" pad="31"/>
<connect gate="G$1" pin="TST" pad="42"/>
<connect gate="G$1" pin="TXD0/PB4" pad="15"/>
<connect gate="G$1" pin="TXD2/PB8" pad="19"/>
<connect gate="G$1" pin="VDDANA" pad="160"/>
<connect gate="G$1" pin="VDDBU" pad="47"/>
<connect gate="G$1" pin="VDDC0RE@203" pad="203"/>
<connect gate="G$1" pin="VDDCORE@147" pad="147"/>
<connect gate="G$1" pin="VDDCORE@174" pad="174"/>
<connect gate="G$1" pin="VDDCORE@38" pad="38"/>
<connect gate="G$1" pin="VDDCORE@77" pad="77"/>
<connect gate="G$1" pin="VDDIOM@114" pad="114"/>
<connect gate="G$1" pin="VDDIOM@132" pad="132"/>
<connect gate="G$1" pin="VDDIOM@65" pad="65"/>
<connect gate="G$1" pin="VDDIOM@90" pad="90"/>
<connect gate="G$1" pin="VDDIOP0@13" pad="13"/>
<connect gate="G$1" pin="VDDIOP0@187" pad="187"/>
<connect gate="G$1" pin="VDDIOP0@199" pad="199"/>
<connect gate="G$1" pin="VDDIOP0@24" pad="24"/>
<connect gate="G$1" pin="VDDIOP0@32" pad="32"/>
<connect gate="G$1" pin="VDDIOP0@5" pad="5"/>
<connect gate="G$1" pin="VDDIOP0@52" pad="52"/>
<connect gate="G$1" pin="VDDIOP1" pad="169"/>
<connect gate="G$1" pin="VDDPLL@148" pad="148"/>
<connect gate="G$1" pin="VDDPLL@155" pad="155"/>
<connect gate="G$1" pin="WKUP" pad="48"/>
<connect gate="G$1" pin="XIN" pad="149"/>
<connect gate="G$1" pin="XIN32" pad="46"/>
<connect gate="G$1" pin="XOUT" pad="150"/>
<connect gate="G$1" pin="XOUT32" pad="45"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91SAM9260B-CU" prefix="U">
<description>AT91SAM9260 MCU&lt;p&gt;
AT91 ARM-9 Thumb Microcontroller</description>
<gates>
<gate name="G$1" symbol="AT91SAM9260B-CU"/>
</gates>
<devices>
<device name="" package="LFBGA217">
<connects>
<connect gate="G$1" pin="!CAS" pad="C3"/>
<connect gate="G$1" pin="!RAS" pad="D3"/>
<connect gate="G$1" pin="!SDWE" pad="F2"/>
<connect gate="G$1" pin="A10" pad="D7"/>
<connect gate="G$1" pin="A11" pad="A6"/>
<connect gate="G$1" pin="A12" pad="B7"/>
<connect gate="G$1" pin="A13" pad="A7"/>
<connect gate="G$1" pin="A14" pad="C7"/>
<connect gate="G$1" pin="A15" pad="B8"/>
<connect gate="G$1" pin="A18" pad="A9"/>
<connect gate="G$1" pin="A19" pad="C9"/>
<connect gate="G$1" pin="A2" pad="C4"/>
<connect gate="G$1" pin="A20" pad="B9"/>
<connect gate="G$1" pin="A21" pad="A10"/>
<connect gate="G$1" pin="A22" pad="A11"/>
<connect gate="G$1" pin="A3" pad="B5"/>
<connect gate="G$1" pin="A4" pad="C5"/>
<connect gate="G$1" pin="A5" pad="D5"/>
<connect gate="G$1" pin="A6" pad="A4"/>
<connect gate="G$1" pin="A7" pad="B6"/>
<connect gate="G$1" pin="A8" pad="A5"/>
<connect gate="G$1" pin="A9" pad="C6"/>
<connect gate="G$1" pin="ADVREF" pad="U2"/>
<connect gate="G$1" pin="BA0/A16" pad="A8"/>
<connect gate="G$1" pin="BA1/A17" pad="C8"/>
<connect gate="G$1" pin="BMS" pad="F15"/>
<connect gate="G$1" pin="CFCE1/TIOB2/PC6" pad="A16"/>
<connect gate="G$1" pin="CFCE2/TIOB1/PC7" pad="B11"/>
<connect gate="G$1" pin="CFIOR/NBS1/NWR1" pad="B2"/>
<connect gate="G$1" pin="CFIOW/NBS3/NWR3" pad="A1"/>
<connect gate="G$1" pin="CFOE/NRD" pad="A13"/>
<connect gate="G$1" pin="CFWE/NWE/NWR0" pad="A12"/>
<connect gate="G$1" pin="CTS3/A25_CFRNW/PC10" pad="B12"/>
<connect gate="G$1" pin="D0" pad="D4"/>
<connect gate="G$1" pin="D1" pad="C2"/>
<connect gate="G$1" pin="D10" pad="E1"/>
<connect gate="G$1" pin="D11" pad="H4"/>
<connect gate="G$1" pin="D12" pad="H3"/>
<connect gate="G$1" pin="D13" pad="F1"/>
<connect gate="G$1" pin="D14" pad="H2"/>
<connect gate="G$1" pin="D15" pad="K3"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D23/PC23" pad="N3"/>
<connect gate="G$1" pin="D24/PC24" pad="K1"/>
<connect gate="G$1" pin="D25/PC25" pad="L3"/>
<connect gate="G$1" pin="D26/PC26" pad="L2"/>
<connect gate="G$1" pin="D27/PC27" pad="N4"/>
<connect gate="G$1" pin="D28/PC28" pad="P4"/>
<connect gate="G$1" pin="D29/PC29" pad="R3"/>
<connect gate="G$1" pin="D3" pad="E3"/>
<connect gate="G$1" pin="D30/PC30" pad="P3"/>
<connect gate="G$1" pin="D31/PC31" pad="M2"/>
<connect gate="G$1" pin="D4" pad="E4"/>
<connect gate="G$1" pin="D5" pad="E2"/>
<connect gate="G$1" pin="D6" pad="F3"/>
<connect gate="G$1" pin="D7" pad="G2"/>
<connect gate="G$1" pin="D8" pad="C1"/>
<connect gate="G$1" pin="D9" pad="D1"/>
<connect gate="G$1" pin="DDM" pad="D13"/>
<connect gate="G$1" pin="DDP" pad="C13"/>
<connect gate="G$1" pin="DRXD/PB14" pad="L17"/>
<connect gate="G$1" pin="DTXD/PB15" pad="K17"/>
<connect gate="G$1" pin="EF100/D21/PC21" pad="K4"/>
<connect gate="G$1" pin="GND@D10" pad="D10"/>
<connect gate="G$1" pin="GND@D12" pad="D12"/>
<connect gate="G$1" pin="GND@D6" pad="D6"/>
<connect gate="G$1" pin="GND@D8" pad="D8"/>
<connect gate="G$1" pin="GND@F4" pad="F4"/>
<connect gate="G$1" pin="GND@G14" pad="G14"/>
<connect gate="G$1" pin="GND@H10" pad="H10"/>
<connect gate="G$1" pin="GND@H8" pad="H8"/>
<connect gate="G$1" pin="GND@H9" pad="H9"/>
<connect gate="G$1" pin="GND@J10" pad="J10"/>
<connect gate="G$1" pin="GND@J8" pad="J8"/>
<connect gate="G$1" pin="GND@J9" pad="J9"/>
<connect gate="G$1" pin="GND@K10" pad="K10"/>
<connect gate="G$1" pin="GND@K16" pad="K16"/>
<connect gate="G$1" pin="GND@K8" pad="K8"/>
<connect gate="G$1" pin="GND@K9" pad="K9"/>
<connect gate="G$1" pin="GND@L1" pad="L1"/>
<connect gate="G$1" pin="GND@M3" pad="M3"/>
<connect gate="G$1" pin="GND@R7" pad="R7"/>
<connect gate="G$1" pin="GND@T15" pad="T15"/>
<connect gate="G$1" pin="GND@T7" pad="T7"/>
<connect gate="G$1" pin="GNDANA" pad="R2"/>
<connect gate="G$1" pin="GNDBU" pad="E16"/>
<connect gate="G$1" pin="GNDPLL@T2" pad="T2"/>
<connect gate="G$1" pin="GNDPLL@U1" pad="U1"/>
<connect gate="G$1" pin="HDMA" pad="E15"/>
<connect gate="G$1" pin="HDMB" pad="C14"/>
<connect gate="G$1" pin="HDPA" pad="E14"/>
<connect gate="G$1" pin="HDPB" pad="D14"/>
<connect gate="G$1" pin="IRQ1/NWAIT/PC15" pad="G1"/>
<connect gate="G$1" pin="IRQ2/NCS3_NANDCS/PC14" pad="B15"/>
<connect gate="G$1" pin="ISI_D0/RK0/PB20" pad="U5"/>
<connect gate="G$1" pin="ISI_D1/RF0/PB21" pad="U6"/>
<connect gate="G$1" pin="ISI_D10/TXD5/PB12" pad="R5"/>
<connect gate="G$1" pin="ISI_D11/RXD5/PB13" pad="P6"/>
<connect gate="G$1" pin="ISI_D2/DSR0/PB22" pad="T6"/>
<connect gate="G$1" pin="ISI_D3/DCD0/PB23" pad="R6"/>
<connect gate="G$1" pin="ISI_D4/DTR0/PB24" pad="P7"/>
<connect gate="G$1" pin="ISI_D5/RI0/PB25" pad="U7"/>
<connect gate="G$1" pin="ISI_D6/RTS0/PB26" pad="R8"/>
<connect gate="G$1" pin="ISI_D7/CTS0/PB27" pad="U8"/>
<connect gate="G$1" pin="ISI_D8/TXD3/PB10" pad="T5"/>
<connect gate="G$1" pin="ISI_D9/RXD3/PB11" pad="P5"/>
<connect gate="G$1" pin="ISI_HSYNC/PCK0/PB30" pad="P9"/>
<connect gate="G$1" pin="ISI_MCK/PCK1/PB31" pad="P10"/>
<connect gate="G$1" pin="ISI_PCK/RTS1/PB28" pad="R9"/>
<connect gate="G$1" pin="ISI_VSYNC/CTS1/PB29" pad="T8"/>
<connect gate="G$1" pin="JTAGSEL" pad="F16"/>
<connect gate="G$1" pin="NANDOE" pad="C10"/>
<connect gate="G$1" pin="NANDWE" pad="B10"/>
<connect gate="G$1" pin="NBS0/A0" pad="A2"/>
<connect gate="G$1" pin="NC@C15" pad="C15"/>
<connect gate="G$1" pin="NC@D15" pad="D15"/>
<connect gate="G$1" pin="NC@R1" pad="R1"/>
<connect gate="G$1" pin="NCS6/FIQ/PC13" pad="B13"/>
<connect gate="G$1" pin="NCS7/IRQ0/PC12" pad="C12"/>
<connect gate="G$1" pin="NCSO" pad="A14"/>
<connect gate="G$1" pin="NRST" pad="G15"/>
<connect gate="G$1" pin="NTRST" pad="H16"/>
<connect gate="G$1" pin="NWR2/NBS2/A1" pad="A3"/>
<connect gate="G$1" pin="OSCSEL" pad="F14"/>
<connect gate="G$1" pin="PA0/SPI0_MISO/MCDB0" pad="R10"/>
<connect gate="G$1" pin="PA1/SPI0_MOSI/MCCDB" pad="P11"/>
<connect gate="G$1" pin="PA10/MCDA2/ETX2" pad="R13"/>
<connect gate="G$1" pin="PA11/MCDA3/ETX3" pad="T12"/>
<connect gate="G$1" pin="PA12/ETX0" pad="U9"/>
<connect gate="G$1" pin="PA13/ETX1" pad="U10"/>
<connect gate="G$1" pin="PA14/ERX0" pad="U11"/>
<connect gate="G$1" pin="PA15/ERX1" pad="U12"/>
<connect gate="G$1" pin="PA16/ETXEN" pad="U15"/>
<connect gate="G$1" pin="PA17/ERXDV" pad="U14"/>
<connect gate="G$1" pin="PA18/ERXER" pad="U16"/>
<connect gate="G$1" pin="PA19/ETXCK" pad="U13"/>
<connect gate="G$1" pin="PA2/SPI0_SPCK" pad="T9"/>
<connect gate="G$1" pin="PA20/EMDC" pad="T14"/>
<connect gate="G$1" pin="PA21/EMDIO" pad="R14"/>
<connect gate="G$1" pin="PA22/ADTRG/ETXER" pad="T16"/>
<connect gate="G$1" pin="PA23/TWD/ETX2" pad="R15"/>
<connect gate="G$1" pin="PA24/TWCK/ETX3" pad="R16"/>
<connect gate="G$1" pin="PA25/TLCK0/ERX2" pad="P16"/>
<connect gate="G$1" pin="PA26/TIOA0/ERX3" pad="P15"/>
<connect gate="G$1" pin="PA27/TIOA1/ERXCK" pad="T17"/>
<connect gate="G$1" pin="PA28/TIOA2/ECRS" pad="L14"/>
<connect gate="G$1" pin="PA29/SCK1/ECOL" pad="R17"/>
<connect gate="G$1" pin="PA3/SPI0_NPCS0/MCDB3" pad="P12"/>
<connect gate="G$1" pin="PA30/SCK2/RXD4" pad="N15"/>
<connect gate="G$1" pin="PA31/SCK0/TXD4" pad="N14"/>
<connect gate="G$1" pin="PA4/RTS2/MCDB2" pad="R11"/>
<connect gate="G$1" pin="PA5/CTS2/MCDB1" pad="R12"/>
<connect gate="G$1" pin="PA6/MCDA0" pad="T10"/>
<connect gate="G$1" pin="PA7/MCCDA" pad="P13"/>
<connect gate="G$1" pin="PA8/MCCK" pad="T11"/>
<connect gate="G$1" pin="PA9/MCDA1" pad="P14"/>
<connect gate="G$1" pin="PCK0/AD1/PC1" pad="T4"/>
<connect gate="G$1" pin="PCK1/AD2/PC2" pad="U3"/>
<connect gate="G$1" pin="PLLRCA" pad="T1"/>
<connect gate="G$1" pin="RTCK" pad="G16"/>
<connect gate="G$1" pin="RTS3/NCS4_CFCS0/PC8" pad="B16"/>
<connect gate="G$1" pin="RXD0/PB5" pad="P17"/>
<connect gate="G$1" pin="RXD2/PB9" pad="L15"/>
<connect gate="G$1" pin="SCK3/AD0/PC0" pad="T3"/>
<connect gate="G$1" pin="SDA10" pad="B4"/>
<connect gate="G$1" pin="SDCK" pad="B1"/>
<connect gate="G$1" pin="SDCKE" pad="G3"/>
<connect gate="G$1" pin="SDCS/NCS1" pad="B3"/>
<connect gate="G$1" pin="SHDN" pad="C17"/>
<connect gate="G$1" pin="SPI0_NPCS1/NCS2/PC11" pad="B14"/>
<connect gate="G$1" pin="SPI0_NPCS2/D16/PC16" pad="J4"/>
<connect gate="G$1" pin="SPI0_NPCS3/D17/PC17" pad="J2"/>
<connect gate="G$1" pin="SPI1_NPCS1/A24/PC5" pad="A15"/>
<connect gate="G$1" pin="SPI1_NPCS1/D18/PC18" pad="H1"/>
<connect gate="G$1" pin="SPI1_NPCS2/A23/PC4" pad="A17"/>
<connect gate="G$1" pin="SPI1_NPCS2/D19/PC19" pad="J1"/>
<connect gate="G$1" pin="SPI1_NPCS3/AD3/PC3" pad="U4"/>
<connect gate="G$1" pin="SPI1_NPCS3/D20/PC20" pad="K2"/>
<connect gate="G$1" pin="TCK" pad="H15"/>
<connect gate="G$1" pin="TCLK1/TXD1/PB6" pad="N17"/>
<connect gate="G$1" pin="TCLK2/RXD1/PB7" pad="M17"/>
<connect gate="G$1" pin="TCLK3/TK0/PB16" pad="J17"/>
<connect gate="G$1" pin="TCLK4/TF0/PB17" pad="K15"/>
<connect gate="G$1" pin="TCLK5/D22/PC22" pad="M4"/>
<connect gate="G$1" pin="TDI" pad="J16"/>
<connect gate="G$1" pin="TDO" pad="J14"/>
<connect gate="G$1" pin="TIOA3/SPI1_MISO/PB0" pad="N16"/>
<connect gate="G$1" pin="TIOA4/SPI1_SPCK/PB2" pad="M15"/>
<connect gate="G$1" pin="TIOA5/SPI1_NPCS0/PB3" pad="M16"/>
<connect gate="G$1" pin="TIOB0/NCS5_CFCS1/PC9" pad="C11"/>
<connect gate="G$1" pin="TIOB3/SPI1_MOSI/PB1" pad="M14"/>
<connect gate="G$1" pin="TIOB4/TD0/PB18" pad="H17"/>
<connect gate="G$1" pin="TIOB5/RD0/PB19" pad="J15"/>
<connect gate="G$1" pin="TMS" pad="G17"/>
<connect gate="G$1" pin="TST" pad="F17"/>
<connect gate="G$1" pin="TXD0/PB4" pad="K14"/>
<connect gate="G$1" pin="TXD2/PB8" pad="L16"/>
<connect gate="G$1" pin="VDDANA" pad="R4"/>
<connect gate="G$1" pin="VDDBU" pad="D16"/>
<connect gate="G$1" pin="VDDCORE@D9" pad="D9"/>
<connect gate="G$1" pin="VDDCORE@H14" pad="H14"/>
<connect gate="G$1" pin="VDDCORE@M1" pad="M1"/>
<connect gate="G$1" pin="VDDCORE@T13" pad="T13"/>
<connect gate="G$1" pin="VDDIOM@D11" pad="D11"/>
<connect gate="G$1" pin="VDDIOM@G4" pad="G4"/>
<connect gate="G$1" pin="VDDIOP0@C16" pad="C16"/>
<connect gate="G$1" pin="VDDIOP0@J3" pad="J3"/>
<connect gate="G$1" pin="VDDIOP0@L4" pad="L4"/>
<connect gate="G$1" pin="VDDIOP0@U17" pad="U17"/>
<connect gate="G$1" pin="VDDIOP1@P8" pad="P8"/>
<connect gate="G$1" pin="VDDPLL@N2" pad="N2"/>
<connect gate="G$1" pin="VDDPLL@P2" pad="P2"/>
<connect gate="G$1" pin="WKUP" pad="B17"/>
<connect gate="G$1" pin="XIN" pad="N1"/>
<connect gate="G$1" pin="XIN32" pad="D17"/>
<connect gate="G$1" pin="XOUT" pad="P1"/>
<connect gate="G$1" pin="XOUT32" pad="E17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91SAM7S512/256/128/64/321" prefix="U">
<description>AT91SAM7S512/256/128/64/321&lt;p&gt;
ARM7 Processor</description>
<gates>
<gate name="G$1" symbol="AT91SAM7S512/256/128/64/321"/>
</gates>
<devices>
<device name="-AU" package="LQFP64">
<connects>
<connect gate="G$1" pin="AD0/PCK1/TD/PA17" pad="9"/>
<connect gate="G$1" pin="AD1/PCK2/RD/PA18" pad="10"/>
<connect gate="G$1" pin="AD2/FIQ/RK/PA19" pad="13"/>
<connect gate="G$1" pin="AD3/IRQ0/RF/PA20" pad="16"/>
<connect gate="G$1" pin="AD4" pad="3"/>
<connect gate="G$1" pin="AD5" pad="4"/>
<connect gate="G$1" pin="AD6" pad="5"/>
<connect gate="G$1" pin="AD7" pad="6"/>
<connect gate="G$1" pin="ADTRG/CTS0/PA8" pad="31"/>
<connect gate="G$1" pin="ADVREF" pad="1"/>
<connect gate="G$1" pin="DDM" pad="56"/>
<connect gate="G$1" pin="DDP" pad="57"/>
<connect gate="G$1" pin="ERASE" pad="55"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@46" pad="46"/>
<connect gate="G$1" pin="GND@60" pad="60"/>
<connect gate="G$1" pin="JTAGSEL" pad="50"/>
<connect gate="G$1" pin="NPCS1/DRXD/PA9" pad="30"/>
<connect gate="G$1" pin="NPCS2/DTXD/PA10" pad="29"/>
<connect gate="G$1" pin="NPCS2/IRQ1/PA30" pad="42"/>
<connect gate="G$1" pin="NPCS3/RXD0/PA5" pad="35"/>
<connect gate="G$1" pin="NPCS3/TWD/PA3" pad="43"/>
<connect gate="G$1" pin="NPCS3/TXD1/PA22" pad="14"/>
<connect gate="G$1" pin="NRST" pad="39"/>
<connect gate="G$1" pin="PCK0/TXD0/PA6" pad="34"/>
<connect gate="G$1" pin="PCK1/RXD1/PA21" pad="11"/>
<connect gate="G$1" pin="PCK2/NPCS1/PA31" pad="52"/>
<connect gate="G$1" pin="PLLRC" pad="63"/>
<connect gate="G$1" pin="PWM0/NPCS0/PA11" pad="28"/>
<connect gate="G$1" pin="PWM0/SCK1/PA23" pad="15"/>
<connect gate="G$1" pin="PWM1/MISO/PA12" pad="27"/>
<connect gate="G$1" pin="PWM1/RTS1/PA24" pad="23"/>
<connect gate="G$1" pin="PWM2/CTS1/PA25" pad="25"/>
<connect gate="G$1" pin="PWM2/MOSI/PA13" pad="22"/>
<connect gate="G$1" pin="PWM3/RTS0/PA7" pad="32"/>
<connect gate="G$1" pin="PWM3/SPCK/PA14" pad="21"/>
<connect gate="G$1" pin="SCK0/PWM2/PA2" pad="44"/>
<connect gate="G$1" pin="TCK" pad="53"/>
<connect gate="G$1" pin="TCLK0/TWCK/PA4" pad="36"/>
<connect gate="G$1" pin="TCLK1/DSR1/PA28" pad="38"/>
<connect gate="G$1" pin="TCLK2/RI1/PA29" pad="41"/>
<connect gate="G$1" pin="TDI" pad="33"/>
<connect gate="G$1" pin="TDO" pad="49"/>
<connect gate="G$1" pin="TIOA0/PWM0/PA0" pad="48"/>
<connect gate="G$1" pin="TIOA1/TF/PA15" pad="20"/>
<connect gate="G$1" pin="TIOA2/DCD1/PA26" pad="26"/>
<connect gate="G$1" pin="TIOB0/PWM1/PA1" pad="47"/>
<connect gate="G$1" pin="TIOB2/DTR1/PA27" pad="37"/>
<connect gate="G$1" pin="TK/TIOB1/PA16" pad="19"/>
<connect gate="G$1" pin="TMS" pad="51"/>
<connect gate="G$1" pin="TST" pad="40"/>
<connect gate="G$1" pin="VDDCORE@12" pad="12"/>
<connect gate="G$1" pin="VDDCORE@24" pad="24"/>
<connect gate="G$1" pin="VDDCORE@54" pad="54"/>
<connect gate="G$1" pin="VDDFLASH" pad="59"/>
<connect gate="G$1" pin="VDDIN" pad="7"/>
<connect gate="G$1" pin="VDDIO@18" pad="18"/>
<connect gate="G$1" pin="VDDIO@45" pad="45"/>
<connect gate="G$1" pin="VDDIO@58" pad="58"/>
<connect gate="G$1" pin="VDDOUT" pad="8"/>
<connect gate="G$1" pin="VDDPLL" pad="64"/>
<connect gate="G$1" pin="XIN/PGMCK" pad="62"/>
<connect gate="G$1" pin="XOUT" pad="61"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8535-AM" prefix="IC" uservalue="yes">
<description>• Advanced RISC Architecture
– 130 Powerful Instructions – Most Single Clock Cycle Execution
– 32 x 8 General Purpose Working Registers
– Fully Static Operation
– Up to 16 MIPS Throughput at 16 MHz
– On-chip 2-cycle Multiplier
• Nonvolatile Program and Data Memories
– 8K Bytes of In-System Self-Programmable Flash
Endurance: 10,000 Write/Erase Cycles
– Optional Boot Code Section with Independent Lock Bits
In-System Programming by On-chip Boot Program
True Read-While-Write Operation
– 512 Bytes EEPROM
Endurance: 100,000 Write/Erase Cycles
– 512 Bytes Internal SRAM
– Programming Lock for Software Security
• Peripheral Features
– Two 8-bit Timer/Counters with Separate Prescalers and Compare Modes
– One 16-bit Timer/Counter with Separate Prescaler, Compare Mode, and Capture
Mode
– Real Time Counter with Separate Oscillator
– Four PWM Channels
– 8-channel, 10-bit ADC
8 Single-ended Channels
7 Differential Channels for TQFP Package Only
2 Differential Channels with Programmable Gain at 1x, 10x, or 200x for TQFP
Package Only
– Byte-oriented Two-wire Serial Interface
– Programmable Serial USART
– Master/Slave SPI Serial Interface
– Programmable Watchdog Timer with Separate On-chip Oscillator
– On-chip Analog Comparator
• Special Microcontroller Features
– Power-on Reset and Programmable Brown-out Detection
– Internal Calibrated RC Oscillator
– External and Internal Interrupt Sources
– Six Sleep Modes: Idle, ADC Noise Reduction, Power-save, Power-down, Standby
and Extended Standby
• I/O and Packages
– 32 Programmable I/O Lines
– 40-pin PDIP, 44-lead TQFP, 44-lead PLCC, and 44-pad MLF
• Operating Voltages
– 2.7 - 5.5V for ATmega8535L
– 4.5 - 5.5V for ATmega8535
• Speed Grades
– 0 - 8 MHz for ATmega8535L
– 0 - 16 MHz for ATmega8535</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-A"/>
</gates>
<devices>
<device name="MLF44-TH" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="28"/>
<connect gate="G$1" pin="GND@1" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TQF-44A-44" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="28"/>
<connect gate="G$1" pin="GND@1" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="GND@1" pad="34"/>
<connect gate="G$1" pin="PC0(SCL)" pad="25"/>
<connect gate="G$1" pin="PC1(SDA)" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8535-P" prefix="IC" uservalue="yes">
<description>• High-performance, Low-power AVR® 8-bit Microcontroller
• Advanced RISC Architecture
– 130 Powerful Instructions – Most Single Clock Cycle Execution
– 32 x 8 General Purpose Working Registers
– Fully Static Operation
– Up to 16 MIPS Throughput at 16 MHz
– On-chip 2-cycle Multiplier
• Nonvolatile Program and Data Memories
– 8K Bytes of In-System Self-Programmable Flash
Endurance: 10,000 Write/Erase Cycles
– Optional Boot Code Section with Independent Lock Bits
In-System Programming by On-chip Boot Program
True Read-While-Write Operation
– 512 Bytes EEPROM
Endurance: 100,000 Write/Erase Cycles
– 512 Bytes Internal SRAM
– Programming Lock for Software Security
• Peripheral Features
– Two 8-bit Timer/Counters with Separate Prescalers and Compare Modes
– One 16-bit Timer/Counter with Separate Prescaler, Compare Mode, and Capture
Mode
– Real Time Counter with Separate Oscillator
– Four PWM Channels
– 8-channel, 10-bit ADC
8 Single-ended Channels
7 Differential Channels for TQFP Package Only
2 Differential Channels with Programmable Gain at 1x, 10x, or 200x for TQFP
Package Only
– Byte-oriented Two-wire Serial Interface
– Programmable Serial USART
– Master/Slave SPI Serial Interface
– Programmable Watchdog Timer with Separate On-chip Oscillator
– On-chip Analog Comparator
• Special Microcontroller Features
– Power-on Reset and Programmable Brown-out Detection
– Internal Calibrated RC Oscillator
– External and Internal Interrupt Sources
– Six Sleep Modes: Idle, ADC Noise Reduction, Power-save, Power-down, Standby
and Extended Standby
• I/O and Packages
– 32 Programmable I/O Lines
– 40-pin PDIP, 44-lead TQFP, 44-lead PLCC, and 44-pad MLF
• Operating Voltages
– 2.7 - 5.5V for ATmega8535L
– 4.5 - 5.5V for ATmega8535
• Speed Grades
– 0 - 8 MHz for ATmega8535L
– 0 - 16 MHz for ATmega8535</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/OC0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/INT2)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="31"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT93C46B" prefix="IC" uservalue="yes">
<description>The AT93C46B provides 1024 bits of serial electrically erasable programmable read
only memory (EEPROM) organized as 64 words of 16 bits each. The device is optimized
for use in many industrial and commercial applications where low power and
low voltage operation are essential. The AT93C46B is available in space saving 8-pin
PDIP and 8-pin JEDEC packages.
The AT93C46B is enabled through the Chip Select pin (CS), and accessed via a 3-
wire serial interface consisting of Data Input (DI), Data Output (DO), and Shift Clock
(SK). Upon receiving a READ instruction at DI, the address is decoded and the data is
clocked out serially on the data output pin DO. The WRITE cycle is completely selftimed
and no separate ERASE cycle is required before WRITE. The WRITE cycle is
only enabled when the part is in the ERASE/WRITE ENABLE state. When CS is
brought “high” following the initiation of a WRITE cycle, the DO pin outputs the
READY/BUSY status of the part.
The AT93C46B is available in 4.5V to 5.5V, 2.7V to 5.5V, and 2.5V to 5.5V versions.</description>
<gates>
<gate name="G$1" symbol="AT93C46B"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC1" pad="7"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC8" package="SOIC8">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC1" pad="7"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U642B" prefix="IC" uservalue="yes">
<description>As a convenience feature of the windshield wiper, intermittent and wipe/wash operation
fuctions are implemented in most of the automobiles. The U642B is a
cost-effective solution for an accurate timing function control. Wipe/wash mode has
priority over interval mode. Interval pause and after-wiping time can be set to fixed values
by using resistors in a broad time range. Added value can be provided with an
individual, continuous adjustment of the interval pause by a potentiometer which may
be built into the stalk. For proper operation, it is mandatory to feed the signal of the
wiper motor's park switch into U642B.</description>
<gates>
<gate name="U642B" symbol="U642B"/>
</gates>
<devices>
<device name="DIL08" package="DIL08">
<connects>
<connect gate="U642B" pin="CT" pad="3"/>
<connect gate="U642B" pin="GND" pad="1"/>
<connect gate="U642B" pin="INT" pad="2"/>
<connect gate="U642B" pin="OUT" pad="7"/>
<connect gate="U642B" pin="PARK" pad="6"/>
<connect gate="U642B" pin="RT" pad="4"/>
<connect gate="U642B" pin="VSS" pad="8"/>
<connect gate="U642B" pin="WASH" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO08" package="SO08">
<connects>
<connect gate="U642B" pin="CT" pad="3"/>
<connect gate="U642B" pin="GND" pad="1"/>
<connect gate="U642B" pin="INT" pad="2"/>
<connect gate="U642B" pin="OUT" pad="7"/>
<connect gate="U642B" pin="PARK" pad="6"/>
<connect gate="U642B" pin="RT" pad="4"/>
<connect gate="U642B" pin="VSS" pad="8"/>
<connect gate="U642B" pin="WASH" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U643B" prefix="IC" uservalue="yes">
<description>The L9686 is a two frequency oscillator particularly
suitable as relay driver for flashing light control
in automotive applications. The circuit may be
also used for other warning lamps like ”handbrake
on” etc. The lamp failure detection is given by
doubling the flash repetition frequency. The
L9686 is supplied in minidip 8-lead and SO8 plastic
packages.</description>
<gates>
<gate name="G$1" symbol="U643B"/>
</gates>
<devices>
<device name="SO8" package="SO08">
<connects>
<connect gate="G$1" pin="+V" pad="2"/>
<connect gate="G$1" pin="COSC" pad="4"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="LFD" pad="7"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT/REL" pad="3"/>
<connect gate="G$1" pin="ROSC" pad="5"/>
<connect gate="G$1" pin="STR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="DIP08">
<connects>
<connect gate="G$1" pin="+V" pad="2"/>
<connect gate="G$1" pin="COSC" pad="4"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="LFD" pad="7"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT/REL" pad="3"/>
<connect gate="G$1" pin="ROSC" pad="5"/>
<connect gate="G$1" pin="STR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32-PU" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
Source: www.atmel.com .. doc2503.pdf</description>
<gates>
<gate name="ATMEGA32-PU" symbol="ATMEGA32-PU"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="ATMEGA32-PU" pin="1/(T0/XCK)PB0" pad="1"/>
<connect gate="ATMEGA32-PU" pin="10/VCC" pad="10"/>
<connect gate="ATMEGA32-PU" pin="11/GND" pad="11"/>
<connect gate="ATMEGA32-PU" pin="12/XTAL2" pad="12"/>
<connect gate="ATMEGA32-PU" pin="13/XTAL1" pad="13"/>
<connect gate="ATMEGA32-PU" pin="14/(RXD)PD0" pad="14"/>
<connect gate="ATMEGA32-PU" pin="15/(TXD)PD1" pad="15"/>
<connect gate="ATMEGA32-PU" pin="16/(INT0)PD2" pad="16"/>
<connect gate="ATMEGA32-PU" pin="17/(INT1)PD3" pad="17"/>
<connect gate="ATMEGA32-PU" pin="18/(OC1B)PD4" pad="18"/>
<connect gate="ATMEGA32-PU" pin="19/(OC1A)PD5" pad="19"/>
<connect gate="ATMEGA32-PU" pin="2/(T1)PB1" pad="2"/>
<connect gate="ATMEGA32-PU" pin="20/(ICP)PD6" pad="20"/>
<connect gate="ATMEGA32-PU" pin="21/(OC2)PD7" pad="21"/>
<connect gate="ATMEGA32-PU" pin="22/(SCL)PC0" pad="22"/>
<connect gate="ATMEGA32-PU" pin="23/(SDA)PC1" pad="23"/>
<connect gate="ATMEGA32-PU" pin="24/(TCK)PC2" pad="24"/>
<connect gate="ATMEGA32-PU" pin="25/(TMS)PC3" pad="25"/>
<connect gate="ATMEGA32-PU" pin="26/(TDO)PC4" pad="26"/>
<connect gate="ATMEGA32-PU" pin="27/(TDI)PC5" pad="27"/>
<connect gate="ATMEGA32-PU" pin="28/(TOSC1)PC6" pad="28"/>
<connect gate="ATMEGA32-PU" pin="29/(TOSC2)PC7" pad="29"/>
<connect gate="ATMEGA32-PU" pin="3/(AIN0/INT2)PB2" pad="3"/>
<connect gate="ATMEGA32-PU" pin="30/AVCC" pad="30"/>
<connect gate="ATMEGA32-PU" pin="31/GND" pad="31"/>
<connect gate="ATMEGA32-PU" pin="32/AREF" pad="32"/>
<connect gate="ATMEGA32-PU" pin="33/(ADC7)PA7" pad="33"/>
<connect gate="ATMEGA32-PU" pin="34/(ADC6)PA6" pad="34"/>
<connect gate="ATMEGA32-PU" pin="35/(ADC5)PA5" pad="35"/>
<connect gate="ATMEGA32-PU" pin="36/(ADC4)PA4" pad="36"/>
<connect gate="ATMEGA32-PU" pin="37/(ADC3)PA3" pad="37"/>
<connect gate="ATMEGA32-PU" pin="38/(ADC2)PA2" pad="38"/>
<connect gate="ATMEGA32-PU" pin="39/(ADC1)PA1" pad="39"/>
<connect gate="ATMEGA32-PU" pin="4/(AIN1/OC0)PB3" pad="4"/>
<connect gate="ATMEGA32-PU" pin="40/(ADC0)PA0" pad="40"/>
<connect gate="ATMEGA32-PU" pin="5/(SS)PB4" pad="5"/>
<connect gate="ATMEGA32-PU" pin="6/(MOSI)PB5" pad="6"/>
<connect gate="ATMEGA32-PU" pin="7/(MISO)PB6" pad="7"/>
<connect gate="ATMEGA32-PU" pin="8/(SCK)PB7" pad="8"/>
<connect gate="ATMEGA32-PU" pin="9/RESET" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16PU"/>
<attribute name="OC_FARNELL" value="1661729"/>
<attribute name="OC_NEWARK" value="51P1794"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13-20MMU" prefix="IC" uservalue="yes">
<description>8-bit
Microcontroller
with 1K Bytes
In-System
Programmable
Flash</description>
<gates>
<gate name="G$1" symbol="ATTINY13-20MMU"/>
</gates>
<devices>
<device name="" package="QFN10">
<connects>
<connect gate="G$1" pin="3/DNC" pad="3"/>
<connect gate="G$1" pin="8/DNC" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="9"/>
<connect gate="G$1" pin="PB3" pad="2"/>
<connect gate="G$1" pin="PB4" pad="4"/>
<connect gate="G$1" pin="PB5" pad="1"/>
<connect gate="G$1" pin="VCC" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32E5/16E5/8E5" prefix="IC" uservalue="yes">
<description>8/16-bit Atmel AVR XMEGA Microcontrollers</description>
<gates>
<gate name="G$1" symbol="ATXMEGA32E5/16E5/8E5"/>
</gates>
<devices>
<device name="ATXMEGA32E5-AU" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND18" pad="18"/>
<connect gate="G$1" pin="PA0" pad="6"/>
<connect gate="G$1" pin="PA1" pad="5"/>
<connect gate="G$1" pin="PA2" pad="4"/>
<connect gate="G$1" pin="PA3" pad="3"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="31"/>
<connect gate="G$1" pin="PA6" pad="30"/>
<connect gate="G$1" pin="PA7" pad="29"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="15"/>
<connect gate="G$1" pin="PC2" pad="14"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="12"/>
<connect gate="G$1" pin="PC5" pad="11"/>
<connect gate="G$1" pin="PC6" pad="10"/>
<connect gate="G$1" pin="PC7" pad="9"/>
<connect gate="G$1" pin="PD0" pad="28"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="26"/>
<connect gate="G$1" pin="PD3" pad="25"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="23"/>
<connect gate="G$1" pin="PD6" pad="22"/>
<connect gate="G$1" pin="PD7" pad="21"/>
<connect gate="G$1" pin="PDI" pad="7"/>
<connect gate="G$1" pin="PDI/RESET" pad="8"/>
<connect gate="G$1" pin="PR0" pad="20"/>
<connect gate="G$1" pin="PR1" pad="19"/>
<connect gate="G$1" pin="VCC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
