<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>&lt;b&gt;&lt;font size=75 face=arial color="#007FFF"&gt;Atmel&lt;/font&gt;&lt;/b&gt;
&lt;p&gt;

&lt;b&gt;&lt;font size=4&gt;XMega Devices&lt;/font&gt;&lt;/b&gt;
&lt;p&gt;

&lt;table border=0 cellspacing=1 cellpadding=2&gt;
  &lt;tr&gt;
    &lt;td colspan=5 bgcolor="#cccccc"&gt;
      &lt;font color="#0000FF" size=3 face=arial&gt;&lt;b&gt;100-Pins Package&lt;/b&gt;&lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td align=center bgcolor="#eeeeee" width="20%"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Devices Name&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd" width="10%"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Flash (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee" width="10%"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;SRAM (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd" width="10%"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;EEPROM (Bytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Packages&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      ATxmega64A1&lt;br&gt;
      ATxmega64A1U&lt;br&gt;
      ATxmega64B1&lt;br&gt;
      ATxmega128A1&lt;br&gt;
      ATxmega128A1U&lt;br&gt;
      ATxmega128B1&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center&gt;&lt;font face=arial size=3&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center nowrap&gt;&lt;font face=arial size=3&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center&gt;&lt;font face=arial size=3&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      CBGA 100C1 100,TQFP 100A 100,VFBGA 100C2 100 (10x10)&lt;br&gt;
      CBGA 100C1 100,TQFP 100A 100,VFBGA 100C2 100 (10x10)&lt;br&gt;
      TQFP 100A 100&lt;br&gt;
      CBGA 100C1 100,TQFP 100A 100,VFBGA 100C2 100 (10x10)&lt;br&gt;
      CBGA 100C1 100,TQFP 100A 100,VFBGA 100C2 100 (10x10)&lt;br&gt;
      TQFP 100A 100&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td colspan=5 bgcolor="#cccccc"&gt;
      &lt;font color="#0000FF" size=3 face=arial&gt;&lt;b&gt;64-Pins Package&lt;/b&gt;&lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Devices Name&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Flash (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;SRAM (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;EEPROM (Bytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Packages&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      ATxmega64A3&lt;br&gt;
      ATxmega64A3U&lt;br&gt;
      ATxmega64B3&lt;br&gt;
      ATxmega64C3&lt;br&gt;
      ATxmega64D3&lt;br&gt;
      ATxmega128A3&lt;br&gt;
      ATxmega128A3U&lt;br&gt;
      ATxmega128B3&lt;br&gt;
      ATxmega128C3&lt;br&gt;
      ATxmega128D3&lt;br&gt;
      ATxmega192A3&lt;br&gt;
      ATxmega192A3U&lt;br&gt;
      ATxmega192C3&lt;br&gt;
      ATxmega192D3&lt;br&gt;
      ATxmega256A3&lt;br&gt;
      ATxmega256A3B&lt;br&gt;
      ATxmega256A3BU&lt;br&gt;
      ATxmega256A3U&lt;br&gt;
      ATxmega256C3&lt;br&gt;
      ATxmega256D3&lt;br&gt;
      ATxmega384C3&lt;br&gt;
      ATxmega384D3&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center&gt;&lt;font face=arial size=3&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      192&lt;br&gt;
      192&lt;br&gt;
      192&lt;br&gt;
      192&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      384&lt;br&gt;
      384&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      4&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      32&lt;br&gt;
      32&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center nowrap&gt;&lt;font face=arial size=3&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M1 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M1 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M1 64,TQFP 64A 64&lt;br&gt;
      TQFP MF 64,VQFN (Sawn) PJ 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      TQFP MF 64,VQFN (Sawn) PJ 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M1 64,MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      TQFP MF 64,VQFN (Sawn) PJ 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      TQFP 64A 64,VQFN (Sawn) PJ 64&lt;br&gt;
      TQFP 64A 64,VQFN (Sawn) PJ 64&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td colspan=5 bgcolor="#cccccc"&gt;
      &lt;font color="#0000FF" size=3 face=arial&gt;&lt;b&gt;44-Pins Package&lt;/b&gt;&lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Devices Name&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Flash (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;SRAM (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd"&gt;		
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;EEPROM (Bytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Packages&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      ATxmega16A4&lt;br&gt;
      ATxmega16A4U&lt;br&gt;
      ATxmega16C4&lt;br&gt;
      ATxmega16D4&lt;br&gt;
      ATxmega32A4&lt;br&gt;
      ATxmega32A4U&lt;br&gt;
      ATxmega32C4&lt;br&gt;
      ATxmega32D4&lt;br&gt;
      ATxmega64A4U&lt;br&gt;
      ATxmega64D4&lt;br&gt;
      ATxmega128A4U&lt;br&gt;
      ATxmega128D4&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center&gt;&lt;font face=arial size=3&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      32&lt;br&gt;
      32&lt;br&gt;
      32&lt;br&gt;
      32&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      3.3&lt;br&gt;
      3.3&lt;br&gt;
      4&lt;br&gt;
      2&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center nowrap&gt;&lt;font face=arial size=3&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44&lt;br&gt;
     &lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

&lt;/table&gt;</description>
<packages>
<package name="TQFP-64A-64">
<description>&lt;b&gt;64A&lt;/b&gt;, 64-lead, 14 x 14 mm Body Size, 1.0 mm Body Thickness, 0.8 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP)</description>
</package>
<package name="MLF-(VQFN)-64M2-64">
<description>&lt;b&gt;64M2&lt;/b&gt;, 64-pad, 9 x 9 x 1.0 mm Body, Lead Pitch 0.50 mm, 7.65 mm Exposed Pad, Micro Lead Frame Package (MLF)</description>
</package>
<package name="TQFP-44A-44">
<description>&lt;b&gt;44A&lt;/b&gt;, 44-lead, 10 x 10 mm Body Size, 1.0 mm Body Thickness, 0.8 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP)</description>
</package>
<package name="TQFP-100A-100">
<description>&lt;b&gt;100A&lt;/b&gt;, 100-lead, 14 x 14 mm Body Size, 1.0 mm Body Thickness,
0.5 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP)</description>
</package>
<package name="MLF-(VQFN)-44M1-44">
<description>&lt;b&gt;44M1&lt;/b&gt;, 44-pad, 7 x 7 x 1.0 mm Body, Lead Pitch 0.50 mm, 5.20 mm Exposed Pad, Thermally Enhanced Plastic Very Thin Quad Flat No Lead Package (VQFN)</description>
</package>
<package name="VFBGA-49C2-49">
<description>&lt;b&gt;49C2&lt;/b&gt;, 49-ball (7 x 7 Array), 0.65 mm Pitch, 5.0 x 5.0 x 1.0 mm, Very Thin, Fine-Pitch Ball Grid Array Package (VFBGA)</description>
</package>
<package name="CBGA-100C1-100">
<description>&lt;b&gt;100C1&lt;/b&gt;, 100-ball, 9 x 9 x 1.2 mm Body, Ball Pitch 0.80 mm Chip Array BGA Package (CBGA)</description>
</package>
<package name="VFBGA-100C2-100">
<description>&lt;b&gt;100C2&lt;/b&gt;, 100-ball (10 x 10 Array), 0.65 mm Pitch, 7.0 x 7.0 x 1.0 mm, Very Thin, Fine-Pitch Ball Grid Array Package (VFBGA)</description>
</package>
</packages>
<symbols>
<symbol name="A4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="A4U">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="C4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="D4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="A3">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET!/PDI"/>
<pin name="PDI"/>
</symbol>
<symbol name="B3">
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="SEG0"/>
<pin name="SEG1"/>
<pin name="SEG2"/>
<pin name="SEG3"/>
<pin name="SEG4"/>
<pin name="SEG5"/>
<pin name="SEG6"/>
<pin name="SEG7"/>
<pin name="SEG8"/>
<pin name="COM0"/>
<pin name="COM1"/>
<pin name="COM2"/>
<pin name="COM3"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="BIAS1"/>
<pin name="BIAS2"/>
<pin name="VLCD"/>
<pin name="CAPL"/>
<pin name="CAPH"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PG0/SEG24"/>
<pin name="PG1/SEG23"/>
<pin name="PG2/SEG22"/>
<pin name="PG3/SEG21"/>
<pin name="PG4/SEG20"/>
<pin name="PG5/SEG19"/>
<pin name="PG6/SEG18"/>
<pin name="PG7/SEG17"/>
<pin name="PM0/SEG16"/>
<pin name="PM1/SEG15"/>
<pin name="PM2/SEG14"/>
<pin name="PM3/SEG13"/>
<pin name="PM4/SEG12"/>
<pin name="PM5/SEG11"/>
<pin name="PM6/SEG10"/>
<pin name="PM7/SEG9"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="C3">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET!/PDI"/>
<pin name="PDI"/>
</symbol>
<symbol name="D3">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET!/PDI"/>
<pin name="PDI"/>
</symbol>
<symbol name="A1">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PH0"/>
<pin name="PJ0"/>
<pin name="PK0"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PH1"/>
<pin name="PJ1"/>
<pin name="PK1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PH2"/>
<pin name="PJ2"/>
<pin name="PK2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PH3"/>
<pin name="PJ3"/>
<pin name="PK3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PH4"/>
<pin name="PJ4"/>
<pin name="PK4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PH5"/>
<pin name="PJ5"/>
<pin name="PK5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PH6"/>
<pin name="PJ6"/>
<pin name="PK6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="PH7"/>
<pin name="PJ7"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="A1U">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PF0"/>
<pin name="PH0"/>
<pin name="PJ0"/>
<pin name="PK0"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PF1"/>
<pin name="PH1"/>
<pin name="PJ1"/>
<pin name="PK1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PF2"/>
<pin name="PH2"/>
<pin name="PJ2"/>
<pin name="PK2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PD3"/>
<pin name="PE3"/>
<pin name="PF3"/>
<pin name="PH3"/>
<pin name="PJ3"/>
<pin name="PK3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PD4"/>
<pin name="PE4"/>
<pin name="PF4"/>
<pin name="PH4"/>
<pin name="PJ4"/>
<pin name="PK4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PD5"/>
<pin name="PE5"/>
<pin name="PF5"/>
<pin name="PH5"/>
<pin name="PJ5"/>
<pin name="PK5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PD6"/>
<pin name="PE6"/>
<pin name="PF6"/>
<pin name="PH6"/>
<pin name="PJ6"/>
<pin name="PK6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PD7"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="PH7"/>
<pin name="PJ7"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="B1">
<pin name="PA0"/>
<pin name="PB0"/>
<pin name="PC0"/>
<pin name="PD0"/>
<pin name="PE0"/>
<pin name="PA1"/>
<pin name="PB1"/>
<pin name="PC1"/>
<pin name="PD1"/>
<pin name="PE1"/>
<pin name="PA2"/>
<pin name="PB2"/>
<pin name="PC2"/>
<pin name="PD2"/>
<pin name="PE2"/>
<pin name="PA3"/>
<pin name="PB3"/>
<pin name="PC3"/>
<pin name="PE3"/>
<pin name="PA4"/>
<pin name="PB4"/>
<pin name="PC4"/>
<pin name="PE4"/>
<pin name="PA5"/>
<pin name="PB5"/>
<pin name="PC5"/>
<pin name="PE5"/>
<pin name="PA6"/>
<pin name="PB6"/>
<pin name="PC6"/>
<pin name="PE6"/>
<pin name="PA7"/>
<pin name="PB7"/>
<pin name="PC7"/>
<pin name="PE7"/>
<pin name="SEG0"/>
<pin name="SEG1"/>
<pin name="SEG2"/>
<pin name="SEG3"/>
<pin name="SEG4"/>
<pin name="SEG5"/>
<pin name="SEG6"/>
<pin name="SEG7"/>
<pin name="SEG8"/>
<pin name="SEG9"/>
<pin name="SEG10"/>
<pin name="SEG11"/>
<pin name="SEG12"/>
<pin name="SEG13"/>
<pin name="SEG14"/>
<pin name="SEG15"/>
<pin name="SEG16"/>
<pin name="SEG17"/>
<pin name="SEG18"/>
<pin name="SEG19"/>
<pin name="SEG20"/>
<pin name="SEG21"/>
<pin name="SEG22"/>
<pin name="SEG23"/>
<pin name="COM0"/>
<pin name="COM1"/>
<pin name="COM2"/>
<pin name="COM3"/>
<pin name="VCC"/>
<pin name="AVCC"/>
<pin name="GND"/>
<pin name="AGND"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="BIAS1"/>
<pin name="BIAS2"/>
<pin name="CAPL"/>
<pin name="CAPH"/>
<pin name="VLCD"/>
<pin name="PG0/SEG39"/>
<pin name="PG1/SEG38"/>
<pin name="PG2/SEG37"/>
<pin name="PG3/SEG36"/>
<pin name="PG4/SEG35"/>
<pin name="PG5/SEG34"/>
<pin name="PG6/SEG33"/>
<pin name="PG7/SEG32"/>
<pin name="PM0/SEG31"/>
<pin name="PM1/SEG30"/>
<pin name="PM2/SEG29"/>
<pin name="PM3/SEG28"/>
<pin name="PM4/SEG27"/>
<pin name="PM5/SEG26"/>
<pin name="PM6/SEG25"/>
<pin name="PM7/SEG24"/>
<pin name="PDI"/>
<pin name="!RESET!/PDI"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATXMEGA16A4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA™ Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Five USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillato
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA16A4U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 16K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 1K - 2KBytes EEPROM
&lt;dd&gt;– 2K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-resolution extensions on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Five USARTs with IrDA support for one USART
&lt;dd&gt;– Two Two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One twelve-channel, 12-bit, 2mspsAnalog to Digital Converter
&lt;dd&gt;– One two-channel, 12-bit, 1msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;il&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O pins
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5" route="any"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA16C4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt; – 16K - 32KBytes of In-System Self-Programmable Flash
&lt;dd&gt; – 4KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt; – 1KBytes EEPROM
&lt;dd&gt; – 2K - 4KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt; – Four-channel event system
&lt;dd&gt; – Four 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt; – One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt; – Three USARTs with IrDA support for one USART
&lt;dd&gt; – Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt; – Two serial peripheral interfaces (SPIs)
&lt;dd&gt; – CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt; – 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt; – One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt; – Two Analog Comparators with window compare function, and current sources
&lt;dd&gt; – External interrupts on all general purpose I/O pins
&lt;dd&gt; – Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt; – QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt; – Power-on reset and programmable brown-out detection
&lt;dd&gt; – Internal and external clock options with PLL and prescaler
&lt;dd&gt; – Programmable multilevel interrupt controller
&lt;dd&gt; – Five sleep modes
&lt;dd&gt; – Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt; – 34 programmable I/O pins
&lt;dd&gt; – 44-lead TQFP
&lt;dd&gt; – 44-pad QFN
&lt;dd&gt; – 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt; – 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-UC" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA16D4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA® Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Four 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counter with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Two USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 200 ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44-lead TQFP
&lt;dd&gt;– 44-pad VQFN/QFN
&lt;dd&gt;– 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32A4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA™ Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Five USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillato
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA™ Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Five USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillato
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA™ Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Five USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillato
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32A4U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 16K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 1K - 2KBytes EEPROM
&lt;dd&gt;– 2K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-resolution extensions on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Five USARTs with IrDA support for one USART
&lt;dd&gt;– Two Two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One twelve-channel, 12-bit, 2mspsAnalog to Digital Converter
&lt;dd&gt;– One two-channel, 12-bit, 1msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;il&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O pins
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5" route="any"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A4U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 16K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 1K - 2KBytes EEPROM
&lt;dd&gt;– 2K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-resolution extensions on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Five USARTs with IrDA support for one USART
&lt;dd&gt;– Two Two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One twelve-channel, 12-bit, 2mspsAnalog to Digital Converter
&lt;dd&gt;– One two-channel, 12-bit, 1msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;il&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O pins
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5" route="any"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A4U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A4U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 16K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 1K - 2KBytes EEPROM
&lt;dd&gt;– 2K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-resolution extensions on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Five USARTs with IrDA support for one USART
&lt;dd&gt;– Two Two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One twelve-channel, 12-bit, 2mspsAnalog to Digital Converter
&lt;dd&gt;– One two-channel, 12-bit, 1msps Digital to Analog Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;il&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O pins
&lt;dd&gt;– 44 - lead TQFP
&lt;dd&gt;– 44 - pad VQFN/QFN
&lt;dd&gt;– 49 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5" route="any"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32D4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA® Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Four 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counter with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Two USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 200 ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44-lead TQFP
&lt;dd&gt;– 44-pad VQFN/QFN
&lt;dd&gt;– 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64D4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA® Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Four 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counter with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Two USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 200 ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44-lead TQFP
&lt;dd&gt;– 44-pad VQFN/QFN
&lt;dd&gt;– 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128D4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGA® Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 16 KB - 128 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 1 KB - 2 KB EEPROM
&lt;dd&gt;– 2 KB - 8 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Four 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counter with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Two USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on one USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two SPIs (Serial Peripheral Interfaces) peripherals
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Twelve-channel, 12-bit, 200 ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 34 Programmable I/O Lines
&lt;dd&gt;– 44-lead TQFP
&lt;dd&gt;– 44-pad VQFN/QFN
&lt;dd&gt;– 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA32C4" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C4&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt; – 16K - 32KBytes of In-System Self-Programmable Flash
&lt;dd&gt; – 4KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt; – 1KBytes EEPROM
&lt;dd&gt; – 2K - 4KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt; – Four-channel event system
&lt;dd&gt; – Four 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt; – One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt; – Three USARTs with IrDA support for one USART
&lt;dd&gt; – Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt; – Two serial peripheral interfaces (SPIs)
&lt;dd&gt; – CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt; – 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt; – One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt; – Two Analog Comparators with window compare function, and current sources
&lt;dd&gt; – External interrupts on all general purpose I/O pins
&lt;dd&gt; – Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt; – QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt; – Power-on reset and programmable brown-out detection
&lt;dd&gt; – Internal and external clock options with PLL and prescaler
&lt;dd&gt; – Programmable multilevel interrupt controller
&lt;dd&gt; – Five sleep modes
&lt;dd&gt; – Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt; – 34 programmable I/O pins
&lt;dd&gt; – 44-lead TQFP
&lt;dd&gt; – 44-pad QFN
&lt;dd&gt; – 49-ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt; – 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C4"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44A-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-44M1-44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 18 30 38 TH"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0" pad="36"/>
<connect gate="G$1" pin="PR1" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9 19 31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-UC" package="VFBGA-49C2-49">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="B5"/>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A3 B4 C5 C7 D5 E1 E2 E4 G5"/>
<connect gate="G$1" pin="PA0" pad="B3"/>
<connect gate="G$1" pin="PA1" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="C2"/>
<connect gate="G$1" pin="PA3" pad="A1"/>
<connect gate="G$1" pin="PA4" pad="B1"/>
<connect gate="G$1" pin="PA5" pad="C1"/>
<connect gate="G$1" pin="PA6" pad="C3"/>
<connect gate="G$1" pin="PA7" pad="C4"/>
<connect gate="G$1" pin="PB0" pad="D4"/>
<connect gate="G$1" pin="PB1" pad="D1"/>
<connect gate="G$1" pin="PB2" pad="D2"/>
<connect gate="G$1" pin="PB3" pad="D3"/>
<connect gate="G$1" pin="PC0" pad="F2"/>
<connect gate="G$1" pin="PC1" pad="G1"/>
<connect gate="G$1" pin="PC2" pad="G2"/>
<connect gate="G$1" pin="PC3" pad="E3"/>
<connect gate="G$1" pin="PC4" pad="F3"/>
<connect gate="G$1" pin="PC5" pad="G3"/>
<connect gate="G$1" pin="PC6" pad="F4"/>
<connect gate="G$1" pin="PC7" pad="G4"/>
<connect gate="G$1" pin="PD0" pad="F5"/>
<connect gate="G$1" pin="PD1" pad="F6"/>
<connect gate="G$1" pin="PD2" pad="G7"/>
<connect gate="G$1" pin="PD3" pad="F7"/>
<connect gate="G$1" pin="PD4" pad="E5"/>
<connect gate="G$1" pin="PD5" pad="E6"/>
<connect gate="G$1" pin="PD6" pad="E7"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PDI" pad="A6"/>
<connect gate="G$1" pin="PE0" pad="D7"/>
<connect gate="G$1" pin="PE1" pad="C6"/>
<connect gate="G$1" pin="PE2" pad="B6"/>
<connect gate="G$1" pin="PE3" pad="A7"/>
<connect gate="G$1" pin="PR0" pad="A5"/>
<connect gate="G$1" pin="PR1" pad="A4"/>
<connect gate="G$1" pin="VCC" pad="B7 F1 G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64B3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA B3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Two-channel DMA controller
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Two 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extensions one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Split mode on timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– One USART with IrDA support
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE 802.3) generator
&lt;dd&gt;– One two-wire interface with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– One serial peripheral interface (SPI)
&lt;dd&gt;– 16-bit Real Time Counter (RTC) with separate oscillator
&lt;dd&gt;– Liquid Crystal Display
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;4x25 segment driver
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Built in contrast control
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;ASCII character mappingGra
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Flexible SWAP of segment and common terminals buses
&lt;dd&gt;– One eight-channel, 12-bit, 300 thousand SPS Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current source feature
&lt;dd&gt;– External interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 36 Programmable I/O pins
&lt;dd&gt;– 64 - lead TQFP
&lt;dd&gt;– 64 - pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="B3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="13"/>
<connect gate="G$1" pin="AGND" pad="55"/>
<connect gate="G$1" pin="AVCC" pad="56"/>
<connect gate="G$1" pin="BIAS1" pad="44"/>
<connect gate="G$1" pin="BIAS2" pad="45"/>
<connect gate="G$1" pin="CAPH" pad="48"/>
<connect gate="G$1" pin="CAPL" pad="47"/>
<connect gate="G$1" pin="COM0" pad="49"/>
<connect gate="G$1" pin="COM1" pad="50"/>
<connect gate="G$1" pin="COM2" pad="51"/>
<connect gate="G$1" pin="COM3" pad="52"/>
<connect gate="G$1" pin="GND" pad="9 15 42"/>
<connect gate="G$1" pin="PB0" pad="57"/>
<connect gate="G$1" pin="PB1" pad="58"/>
<connect gate="G$1" pin="PB2" pad="59"/>
<connect gate="G$1" pin="PB3" pad="60"/>
<connect gate="G$1" pin="PB4" pad="61"/>
<connect gate="G$1" pin="PB5" pad="62"/>
<connect gate="G$1" pin="PB6" pad="63"/>
<connect gate="G$1" pin="PB7" pad="64"/>
<connect gate="G$1" pin="PC0" pad="1"/>
<connect gate="G$1" pin="PC1" pad="2"/>
<connect gate="G$1" pin="PC2" pad="3"/>
<connect gate="G$1" pin="PC3" pad="4"/>
<connect gate="G$1" pin="PC4" pad="5"/>
<connect gate="G$1" pin="PC5" pad="6"/>
<connect gate="G$1" pin="PC6" pad="7"/>
<connect gate="G$1" pin="PC7" pad="8"/>
<connect gate="G$1" pin="PD0" pad="11"/>
<connect gate="G$1" pin="PD1" pad="12"/>
<connect gate="G$1" pin="PDI" pad="14"/>
<connect gate="G$1" pin="PG0/SEG24" pad="17"/>
<connect gate="G$1" pin="PG1/SEG23" pad="18"/>
<connect gate="G$1" pin="PG2/SEG22" pad="19"/>
<connect gate="G$1" pin="PG3/SEG21" pad="20"/>
<connect gate="G$1" pin="PG4/SEG20" pad="21"/>
<connect gate="G$1" pin="PG5/SEG19" pad="22"/>
<connect gate="G$1" pin="PG6/SEG18" pad="23"/>
<connect gate="G$1" pin="PG7/SEG17" pad="24"/>
<connect gate="G$1" pin="PM0/SEG16" pad="25"/>
<connect gate="G$1" pin="PM1/SEG15" pad="26"/>
<connect gate="G$1" pin="PM2/SEG14" pad="27"/>
<connect gate="G$1" pin="PM3/SEG13" pad="28"/>
<connect gate="G$1" pin="PM4/SEG12" pad="29"/>
<connect gate="G$1" pin="PM5/SEG11" pad="30"/>
<connect gate="G$1" pin="PM6/SEG10" pad="31"/>
<connect gate="G$1" pin="PM7/SEG9" pad="32"/>
<connect gate="G$1" pin="PR0" pad="53"/>
<connect gate="G$1" pin="PR1" pad="54"/>
<connect gate="G$1" pin="SEG0" pad="41"/>
<connect gate="G$1" pin="SEG1" pad="40"/>
<connect gate="G$1" pin="SEG2" pad="39"/>
<connect gate="G$1" pin="SEG3" pad="38"/>
<connect gate="G$1" pin="SEG4" pad="37"/>
<connect gate="G$1" pin="SEG5" pad="36"/>
<connect gate="G$1" pin="SEG6" pad="35"/>
<connect gate="G$1" pin="SEG7" pad="34"/>
<connect gate="G$1" pin="SEG8" pad="33"/>
<connect gate="G$1" pin="VCC" pad="10 16 43"/>
<connect gate="G$1" pin="VLCD" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="13"/>
<connect gate="G$1" pin="AGND" pad="55"/>
<connect gate="G$1" pin="AVCC" pad="56"/>
<connect gate="G$1" pin="BIAS1" pad="44"/>
<connect gate="G$1" pin="BIAS2" pad="45"/>
<connect gate="G$1" pin="CAPH" pad="48"/>
<connect gate="G$1" pin="CAPL" pad="47"/>
<connect gate="G$1" pin="COM0" pad="49"/>
<connect gate="G$1" pin="COM1" pad="50"/>
<connect gate="G$1" pin="COM2" pad="51"/>
<connect gate="G$1" pin="COM3" pad="52"/>
<connect gate="G$1" pin="GND" pad="9 15 42 TH"/>
<connect gate="G$1" pin="PB0" pad="57"/>
<connect gate="G$1" pin="PB1" pad="58"/>
<connect gate="G$1" pin="PB2" pad="59"/>
<connect gate="G$1" pin="PB3" pad="60"/>
<connect gate="G$1" pin="PB4" pad="61"/>
<connect gate="G$1" pin="PB5" pad="62"/>
<connect gate="G$1" pin="PB6" pad="63"/>
<connect gate="G$1" pin="PB7" pad="64"/>
<connect gate="G$1" pin="PC0" pad="1"/>
<connect gate="G$1" pin="PC1" pad="2"/>
<connect gate="G$1" pin="PC2" pad="3"/>
<connect gate="G$1" pin="PC3" pad="4"/>
<connect gate="G$1" pin="PC4" pad="5"/>
<connect gate="G$1" pin="PC5" pad="6"/>
<connect gate="G$1" pin="PC6" pad="7"/>
<connect gate="G$1" pin="PC7" pad="8"/>
<connect gate="G$1" pin="PD0" pad="11"/>
<connect gate="G$1" pin="PD1" pad="12"/>
<connect gate="G$1" pin="PDI" pad="14"/>
<connect gate="G$1" pin="PG0/SEG24" pad="17"/>
<connect gate="G$1" pin="PG1/SEG23" pad="18"/>
<connect gate="G$1" pin="PG2/SEG22" pad="19"/>
<connect gate="G$1" pin="PG3/SEG21" pad="20"/>
<connect gate="G$1" pin="PG4/SEG20" pad="21"/>
<connect gate="G$1" pin="PG5/SEG19" pad="22"/>
<connect gate="G$1" pin="PG6/SEG18" pad="23"/>
<connect gate="G$1" pin="PG7/SEG17" pad="24"/>
<connect gate="G$1" pin="PM0/SEG16" pad="25"/>
<connect gate="G$1" pin="PM1/SEG15" pad="26"/>
<connect gate="G$1" pin="PM2/SEG14" pad="27"/>
<connect gate="G$1" pin="PM3/SEG13" pad="28"/>
<connect gate="G$1" pin="PM4/SEG12" pad="29"/>
<connect gate="G$1" pin="PM5/SEG11" pad="30"/>
<connect gate="G$1" pin="PM6/SEG10" pad="31"/>
<connect gate="G$1" pin="PM7/SEG9" pad="32"/>
<connect gate="G$1" pin="PR0" pad="53"/>
<connect gate="G$1" pin="PR1" pad="54"/>
<connect gate="G$1" pin="SEG0" pad="41"/>
<connect gate="G$1" pin="SEG1" pad="40"/>
<connect gate="G$1" pin="SEG2" pad="39"/>
<connect gate="G$1" pin="SEG3" pad="38"/>
<connect gate="G$1" pin="SEG4" pad="37"/>
<connect gate="G$1" pin="SEG5" pad="36"/>
<connect gate="G$1" pin="SEG6" pad="35"/>
<connect gate="G$1" pin="SEG7" pad="34"/>
<connect gate="G$1" pin="SEG8" pad="33"/>
<connect gate="G$1" pin="VCC" pad="10 16 43"/>
<connect gate="G$1" pin="VLCD" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128B3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA B3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Two-channel DMA controller
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Two 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extensions one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Split mode on timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– One USART with IrDA support
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE 802.3) generator
&lt;dd&gt;– One two-wire interface with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– One serial peripheral interface (SPI)
&lt;dd&gt;– 16-bit Real Time Counter (RTC) with separate oscillator
&lt;dd&gt;– Liquid Crystal Display
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;4x25 segment driver
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Built in contrast control
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;ASCII character mappingGra
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Flexible SWAP of segment and common terminals buses
&lt;dd&gt;– One eight-channel, 12-bit, 300 thousand SPS Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current source feature
&lt;dd&gt;– External interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 36 Programmable I/O pins
&lt;dd&gt;– 64 - lead TQFP
&lt;dd&gt;– 64 - pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="B3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="13"/>
<connect gate="G$1" pin="AGND" pad="55"/>
<connect gate="G$1" pin="AVCC" pad="56"/>
<connect gate="G$1" pin="BIAS1" pad="44"/>
<connect gate="G$1" pin="BIAS2" pad="45"/>
<connect gate="G$1" pin="CAPH" pad="48"/>
<connect gate="G$1" pin="CAPL" pad="47"/>
<connect gate="G$1" pin="COM0" pad="49"/>
<connect gate="G$1" pin="COM1" pad="50"/>
<connect gate="G$1" pin="COM2" pad="51"/>
<connect gate="G$1" pin="COM3" pad="52"/>
<connect gate="G$1" pin="GND" pad="9 15 42"/>
<connect gate="G$1" pin="PB0" pad="57"/>
<connect gate="G$1" pin="PB1" pad="58"/>
<connect gate="G$1" pin="PB2" pad="59"/>
<connect gate="G$1" pin="PB3" pad="60"/>
<connect gate="G$1" pin="PB4" pad="61"/>
<connect gate="G$1" pin="PB5" pad="62"/>
<connect gate="G$1" pin="PB6" pad="63"/>
<connect gate="G$1" pin="PB7" pad="64"/>
<connect gate="G$1" pin="PC0" pad="1"/>
<connect gate="G$1" pin="PC1" pad="2"/>
<connect gate="G$1" pin="PC2" pad="3"/>
<connect gate="G$1" pin="PC3" pad="4"/>
<connect gate="G$1" pin="PC4" pad="5"/>
<connect gate="G$1" pin="PC5" pad="6"/>
<connect gate="G$1" pin="PC6" pad="7"/>
<connect gate="G$1" pin="PC7" pad="8"/>
<connect gate="G$1" pin="PD0" pad="11"/>
<connect gate="G$1" pin="PD1" pad="12"/>
<connect gate="G$1" pin="PDI" pad="14"/>
<connect gate="G$1" pin="PG0/SEG24" pad="17"/>
<connect gate="G$1" pin="PG1/SEG23" pad="18"/>
<connect gate="G$1" pin="PG2/SEG22" pad="19"/>
<connect gate="G$1" pin="PG3/SEG21" pad="20"/>
<connect gate="G$1" pin="PG4/SEG20" pad="21"/>
<connect gate="G$1" pin="PG5/SEG19" pad="22"/>
<connect gate="G$1" pin="PG6/SEG18" pad="23"/>
<connect gate="G$1" pin="PG7/SEG17" pad="24"/>
<connect gate="G$1" pin="PM0/SEG16" pad="25"/>
<connect gate="G$1" pin="PM1/SEG15" pad="26"/>
<connect gate="G$1" pin="PM2/SEG14" pad="27"/>
<connect gate="G$1" pin="PM3/SEG13" pad="28"/>
<connect gate="G$1" pin="PM4/SEG12" pad="29"/>
<connect gate="G$1" pin="PM5/SEG11" pad="30"/>
<connect gate="G$1" pin="PM6/SEG10" pad="31"/>
<connect gate="G$1" pin="PM7/SEG9" pad="32"/>
<connect gate="G$1" pin="PR0" pad="53"/>
<connect gate="G$1" pin="PR1" pad="54"/>
<connect gate="G$1" pin="SEG0" pad="41"/>
<connect gate="G$1" pin="SEG1" pad="40"/>
<connect gate="G$1" pin="SEG2" pad="39"/>
<connect gate="G$1" pin="SEG3" pad="38"/>
<connect gate="G$1" pin="SEG4" pad="37"/>
<connect gate="G$1" pin="SEG5" pad="36"/>
<connect gate="G$1" pin="SEG6" pad="35"/>
<connect gate="G$1" pin="SEG7" pad="34"/>
<connect gate="G$1" pin="SEG8" pad="33"/>
<connect gate="G$1" pin="VCC" pad="10 16 43"/>
<connect gate="G$1" pin="VLCD" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="13"/>
<connect gate="G$1" pin="AGND" pad="55"/>
<connect gate="G$1" pin="AVCC" pad="56"/>
<connect gate="G$1" pin="BIAS1" pad="44"/>
<connect gate="G$1" pin="BIAS2" pad="45"/>
<connect gate="G$1" pin="CAPH" pad="48"/>
<connect gate="G$1" pin="CAPL" pad="47"/>
<connect gate="G$1" pin="COM0" pad="49"/>
<connect gate="G$1" pin="COM1" pad="50"/>
<connect gate="G$1" pin="COM2" pad="51"/>
<connect gate="G$1" pin="COM3" pad="52"/>
<connect gate="G$1" pin="GND" pad="9 15 42 TH"/>
<connect gate="G$1" pin="PB0" pad="57"/>
<connect gate="G$1" pin="PB1" pad="58"/>
<connect gate="G$1" pin="PB2" pad="59"/>
<connect gate="G$1" pin="PB3" pad="60"/>
<connect gate="G$1" pin="PB4" pad="61"/>
<connect gate="G$1" pin="PB5" pad="62"/>
<connect gate="G$1" pin="PB6" pad="63"/>
<connect gate="G$1" pin="PB7" pad="64"/>
<connect gate="G$1" pin="PC0" pad="1"/>
<connect gate="G$1" pin="PC1" pad="2"/>
<connect gate="G$1" pin="PC2" pad="3"/>
<connect gate="G$1" pin="PC3" pad="4"/>
<connect gate="G$1" pin="PC4" pad="5"/>
<connect gate="G$1" pin="PC5" pad="6"/>
<connect gate="G$1" pin="PC6" pad="7"/>
<connect gate="G$1" pin="PC7" pad="8"/>
<connect gate="G$1" pin="PD0" pad="11"/>
<connect gate="G$1" pin="PD1" pad="12"/>
<connect gate="G$1" pin="PDI" pad="14"/>
<connect gate="G$1" pin="PG0/SEG24" pad="17"/>
<connect gate="G$1" pin="PG1/SEG23" pad="18"/>
<connect gate="G$1" pin="PG2/SEG22" pad="19"/>
<connect gate="G$1" pin="PG3/SEG21" pad="20"/>
<connect gate="G$1" pin="PG4/SEG20" pad="21"/>
<connect gate="G$1" pin="PG5/SEG19" pad="22"/>
<connect gate="G$1" pin="PG6/SEG18" pad="23"/>
<connect gate="G$1" pin="PG7/SEG17" pad="24"/>
<connect gate="G$1" pin="PM0/SEG16" pad="25"/>
<connect gate="G$1" pin="PM1/SEG15" pad="26"/>
<connect gate="G$1" pin="PM2/SEG14" pad="27"/>
<connect gate="G$1" pin="PM3/SEG13" pad="28"/>
<connect gate="G$1" pin="PM4/SEG12" pad="29"/>
<connect gate="G$1" pin="PM5/SEG11" pad="30"/>
<connect gate="G$1" pin="PM6/SEG10" pad="31"/>
<connect gate="G$1" pin="PM7/SEG9" pad="32"/>
<connect gate="G$1" pin="PR0" pad="53"/>
<connect gate="G$1" pin="PR1" pad="54"/>
<connect gate="G$1" pin="SEG0" pad="41"/>
<connect gate="G$1" pin="SEG1" pad="40"/>
<connect gate="G$1" pin="SEG2" pad="39"/>
<connect gate="G$1" pin="SEG3" pad="38"/>
<connect gate="G$1" pin="SEG4" pad="37"/>
<connect gate="G$1" pin="SEG5" pad="36"/>
<connect gate="G$1" pin="SEG6" pad="35"/>
<connect gate="G$1" pin="SEG7" pad="34"/>
<connect gate="G$1" pin="SEG8" pad="33"/>
<connect gate="G$1" pin="VCC" pad="10 16 43"/>
<connect gate="G$1" pin="VLCD" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64 KB - 256 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 16 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Seven 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Seven USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– Two Two-wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Three SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for test, debug and programming
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64 KB - 256 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 16 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Seven 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Seven USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– Two Two-wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Three SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for test, debug and programming
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA192A3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64 KB - 256 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 16 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Seven 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Seven USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– Two Two-wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Three SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for test, debug and programming
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA256A3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64 KB - 256 KB of In-System Self-Programmable Flash
&lt;dd&gt;– 4 KB - 8 KB Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 16 KB Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Seven 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Three Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Seven USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– Two Two-wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Three SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– One Two-channel, 12-bit, 1 Msps Digital to Analog Converter
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for test, debug and programming
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64C3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt; High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt; Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256KBytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4KBytes EEPROM
&lt;dd&gt;– 4K - 16KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Three USARTs with IrDA support for one USART
&lt;dd&gt;– Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 50 programmable I/O pins
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128C3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt; High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt; Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256KBytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4KBytes EEPROM
&lt;dd&gt;– 4K - 16KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Three USARTs with IrDA support for one USART
&lt;dd&gt;– Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 50 programmable I/O pins
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA192C3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt; High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt; Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256KBytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4KBytes EEPROM
&lt;dd&gt;– 4K - 16KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Three USARTs with IrDA support for one USART
&lt;dd&gt;– Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 50 programmable I/O pins
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA256C3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt; High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt; Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256KBytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8KBytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4KBytes EEPROM
&lt;dd&gt;– 4K - 16KBytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Five 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with four output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with two output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on two timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Three USARTs with IrDA support for one USART
&lt;dd&gt;– Two two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Two serial peripheral interfaces (SPIs)
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE®802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– One sixteen-channel, 12-bit, 300ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (program and debug interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 50 programmable I/O pins
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="C3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64D3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4K Bytes EEPROM
&lt;dd&gt;– 4K - 16K Bytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Three USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match(I2C and SMBus compatible)
&lt;dd&gt;– Two SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Sixteen-channel, 12-bit, 200ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128D3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4K Bytes EEPROM
&lt;dd&gt;– 4K - 16K Bytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Three USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match(I2C and SMBus compatible)
&lt;dd&gt;– Two SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Sixteen-channel, 12-bit, 200ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA192D3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4K Bytes EEPROM
&lt;dd&gt;– 4K - 16K Bytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Three USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match(I2C and SMBus compatible)
&lt;dd&gt;– Two SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Sixteen-channel, 12-bit, 200ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA256D3" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA C3&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 256K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Code Section with Independent Lock Bits
&lt;dd&gt;– 2K - 4K Bytes EEPROM
&lt;dd&gt;– 4K - 16K Bytes Internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel Event System
&lt;dd&gt;– Five 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High Resolution Extensions on two Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on one Timer/Counter
&lt;dd&gt;– Three USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA Extension on 1 USART
&lt;dd&gt;– Two Two-Wire Interfaces with dual address match(I2C and SMBus compatible)
&lt;dd&gt;– Two SPI (Serial Peripheral Interfaces)
&lt;dd&gt;– 16-bit Real Time Counter with Separate Oscillator
&lt;dd&gt;– One Sixteen-channel, 12-bit, 200ksps Analog to Digital Converter
&lt;dd&gt;– Two Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming, test and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 50 Programmable I/O Lines
&lt;dd&gt;– 64-lead TQFP
&lt;dd&gt;– 64-pad QFN
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="D3"/>
</gates>
<devices>
<device name="-AU" package="TQFP-64A-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="MLF-(VQFN)-64M2-64">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="57"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND" pad="14 24 34 44 52 60 TH"/>
<connect gate="G$1" pin="PA0" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="PB3" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0" pad="16"/>
<connect gate="G$1" pin="PC1" pad="17"/>
<connect gate="G$1" pin="PC2" pad="18"/>
<connect gate="G$1" pin="PC3" pad="19"/>
<connect gate="G$1" pin="PC4" pad="20"/>
<connect gate="G$1" pin="PC5" pad="21"/>
<connect gate="G$1" pin="PC6" pad="22"/>
<connect gate="G$1" pin="PC7" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1" pad="27"/>
<connect gate="G$1" pin="PD2" pad="28"/>
<connect gate="G$1" pin="PD3" pad="29"/>
<connect gate="G$1" pin="PD4" pad="30"/>
<connect gate="G$1" pin="PD5" pad="31"/>
<connect gate="G$1" pin="PD6" pad="32"/>
<connect gate="G$1" pin="PD7" pad="33"/>
<connect gate="G$1" pin="PDI" pad="56"/>
<connect gate="G$1" pin="PE0" pad="36"/>
<connect gate="G$1" pin="PE1" pad="37"/>
<connect gate="G$1" pin="PE2" pad="38"/>
<connect gate="G$1" pin="PE3" pad="39"/>
<connect gate="G$1" pin="PE4" pad="40"/>
<connect gate="G$1" pin="PE5" pad="41"/>
<connect gate="G$1" pin="PE6" pad="42"/>
<connect gate="G$1" pin="PE7" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1" pad="47"/>
<connect gate="G$1" pin="PF2" pad="48"/>
<connect gate="G$1" pin="PF3" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0" pad="58"/>
<connect gate="G$1" pin="PR1" pad="59"/>
<connect gate="G$1" pin="VCC" pad="15 25 35 45 53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA192A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA256A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA384A1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, Low-power 8/16-bit Atmel® AVR® XMEGATM Microcontroller
&lt;li&gt;Non-Volatile Program and Data Memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 384K Bytes of In-System Self-Programmable Flash
&lt;dd&gt;– 4K - 8K Bytes Boot Section with Independent Lock Bits
&lt;dd&gt;– 2 KB - 4 KB EEPROM
&lt;dd&gt;– 4 KB - 32 KB Internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 16M bytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External Bus Interface for up to 128M bit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA Controller with support for external requests
&lt;dd&gt;– Eight-channel Event System
&lt;dd&gt;– Eight 16-bit Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 4 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four Timer/Counters with 2 Output Compare or Input Capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High-Resolution Extension on all Timer/Counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced Waveform Extension on two Timer/Counters
&lt;dd&gt;– Eight USARTs
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;IrDA modulation/demodulation for one USART
&lt;dd&gt;– Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four SPI (Serial Peripheral Interface) peripherals
&lt;dd&gt;– AES and DES Crypto Engine
&lt;dd&gt;– 16-bit Real Time Counter with separate Oscillator
&lt;dd&gt;– Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators with Window compare function
&lt;dd&gt;– External Interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;/dl&gt;
&lt;li&gt;Special Microcontroller Features
&lt;dl&gt;
&lt;dd&gt;– Power-on Reset and Programmable Brown-out Detection
&lt;dd&gt;– Internal and External Clock Options with PLL and Prescaler
&lt;dd&gt;– Programmable Multi-level Interrupt Controller
&lt;dd&gt;– Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby
&lt;dd&gt;– Advanced Programming, Test and Debugging Interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface) for programming and debugging
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O Lines
&lt;dd&gt;– 100 - lead TQFP
&lt;dd&gt;– 100 - ball CBGA
&lt;dd&gt;– 100 - ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Speed performance
&lt;dl&gt;
&lt;dd&gt;– 0 – 12 MHz @ 1.6 – 3.6V
&lt;dd&gt;– 0 – 32 MHz @ 2.7 – 3.6V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64A1U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatileprogram and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External bus interface for up to 16Mbytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External bus interface for up to 128Mbit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Eight 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on two timer/counters
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Eight USARTs with IrDA support for one USART
&lt;dd&gt;– Four two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– Two sixteen channel, 12-bit, 2msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators (ACs) with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O pins
&lt;dd&gt;– 100 lead TQFP
&lt;dd&gt;– 100 ball BGA
&lt;dd&gt;– 100 ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93" route="any"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128A1U" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA A1U&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatileprogram and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External bus interface for up to 16Mbytes SRAM
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;External bus interface for up to 128Mbit SDRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral features
&lt;dl&gt;
&lt;dd&gt;– Four-channel DMA controller
&lt;dd&gt;– Eight-channel event system
&lt;dd&gt;– Eight 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Four timer/counters with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extension on all timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on two timer/counters
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Eight USARTs with IrDA support for one USART
&lt;dd&gt;– Four two-wire interfaces with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– Four serial peripheral interfaces (SPIs)
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– 16-bit real time counter (RTC) with separate oscillator
&lt;dd&gt;– Two sixteen channel, 12-bit, 2msps Analog to Digital Converters
&lt;dd&gt;– Two Two-channel, 12-bit, 1msps Digital to Analog Converters
&lt;dd&gt;– Four Analog Comparators (ACs) with window compare function, and current sources
&lt;dd&gt;– External interrupts on all general purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL and prescaler
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and packages
&lt;dl&gt;
&lt;dd&gt;– 78 Programmable I/O pins
&lt;dd&gt;– 100 lead TQFP
&lt;dd&gt;– 100 ball BGA
&lt;dd&gt;– 100 ball VFBGA
&lt;/dl&gt;
&lt;li&gt;Operating voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="A1U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4 94"/>
<connect gate="G$1" pin="GND" pad="3 13 23 33 43 53 63 73 84 93" route="any"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14 24 34 44 54 64 74 83"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CU" package="CBGA-100C1-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C7U" package="VFBGA-100C2-100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI" pad="F3"/>
<connect gate="G$1" pin="AVCC" pad="H1 K4"/>
<connect gate="G$1" pin="GND" pad="A3 A6 A8 D1 D10 G1 G10 K3 K7 K9"/>
<connect gate="G$1" pin="PA0" pad="J1"/>
<connect gate="G$1" pin="PA1" pad="G2"/>
<connect gate="G$1" pin="PA2" pad="H2"/>
<connect gate="G$1" pin="PA3" pad="J2"/>
<connect gate="G$1" pin="PA4" pad="G3"/>
<connect gate="G$1" pin="PA5" pad="H3"/>
<connect gate="G$1" pin="PA6" pad="K1"/>
<connect gate="G$1" pin="PA7" pad="K2"/>
<connect gate="G$1" pin="PB0" pad="J3"/>
<connect gate="G$1" pin="PB1" pad="J4"/>
<connect gate="G$1" pin="PB2" pad="H4"/>
<connect gate="G$1" pin="PB3" pad="G4"/>
<connect gate="G$1" pin="PB4" pad="G5"/>
<connect gate="G$1" pin="PB5" pad="H5"/>
<connect gate="G$1" pin="PB6" pad="J5"/>
<connect gate="G$1" pin="PB7" pad="K5"/>
<connect gate="G$1" pin="PC0" pad="H6"/>
<connect gate="G$1" pin="PC1" pad="G6"/>
<connect gate="G$1" pin="PC2" pad="F6"/>
<connect gate="G$1" pin="PC3" pad="J6"/>
<connect gate="G$1" pin="PC4" pad="J7"/>
<connect gate="G$1" pin="PC5" pad="H7"/>
<connect gate="G$1" pin="PC6" pad="G7"/>
<connect gate="G$1" pin="PC7" pad="J8"/>
<connect gate="G$1" pin="PD0" pad="K10"/>
<connect gate="G$1" pin="PD1" pad="J10"/>
<connect gate="G$1" pin="PD2" pad="J9"/>
<connect gate="G$1" pin="PD3" pad="H10"/>
<connect gate="G$1" pin="PD4" pad="H9"/>
<connect gate="G$1" pin="PD5" pad="H8"/>
<connect gate="G$1" pin="PD6" pad="G9"/>
<connect gate="G$1" pin="PD7" pad="G8"/>
<connect gate="G$1" pin="PDI" pad="F4"/>
<connect gate="G$1" pin="PE0" pad="F9"/>
<connect gate="G$1" pin="PE1" pad="F8"/>
<connect gate="G$1" pin="PE2" pad="F7"/>
<connect gate="G$1" pin="PE3" pad="E10"/>
<connect gate="G$1" pin="PE4" pad="E9"/>
<connect gate="G$1" pin="PE5" pad="E8"/>
<connect gate="G$1" pin="PE6" pad="E7"/>
<connect gate="G$1" pin="PE7" pad="E6"/>
<connect gate="G$1" pin="PF0" pad="D7"/>
<connect gate="G$1" pin="PF1" pad="D8"/>
<connect gate="G$1" pin="PF2" pad="C8"/>
<connect gate="G$1" pin="PF3" pad="C9"/>
<connect gate="G$1" pin="PF4" pad="D9"/>
<connect gate="G$1" pin="PF5" pad="B10"/>
<connect gate="G$1" pin="PF6" pad="B9"/>
<connect gate="G$1" pin="PF7" pad="A10"/>
<connect gate="G$1" pin="PH0" pad="B8"/>
<connect gate="G$1" pin="PH1" pad="A7"/>
<connect gate="G$1" pin="PH2" pad="B7"/>
<connect gate="G$1" pin="PH3" pad="C7"/>
<connect gate="G$1" pin="PH4" pad="B6"/>
<connect gate="G$1" pin="PH5" pad="C6"/>
<connect gate="G$1" pin="PH6" pad="D6"/>
<connect gate="G$1" pin="PH7" pad="B5"/>
<connect gate="G$1" pin="PJ0" pad="C5"/>
<connect gate="G$1" pin="PJ1" pad="D5"/>
<connect gate="G$1" pin="PJ2" pad="E5"/>
<connect gate="G$1" pin="PJ3" pad="A4"/>
<connect gate="G$1" pin="PJ4" pad="B4"/>
<connect gate="G$1" pin="PJ5" pad="C4"/>
<connect gate="G$1" pin="PJ6" pad="D4"/>
<connect gate="G$1" pin="PJ7" pad="E4"/>
<connect gate="G$1" pin="PK0" pad="A1"/>
<connect gate="G$1" pin="PK1" pad="B3"/>
<connect gate="G$1" pin="PK2" pad="B2"/>
<connect gate="G$1" pin="PK3" pad="B1"/>
<connect gate="G$1" pin="PK4" pad="C3"/>
<connect gate="G$1" pin="PK5" pad="C2"/>
<connect gate="G$1" pin="PK6" pad="D2"/>
<connect gate="G$1" pin="PK7" pad="D3"/>
<connect gate="G$1" pin="PQ0" pad="E1"/>
<connect gate="G$1" pin="PQ1" pad="E2"/>
<connect gate="G$1" pin="PQ2" pad="E3"/>
<connect gate="G$1" pin="PQ3" pad="F5"/>
<connect gate="G$1" pin="PR0" pad="F2"/>
<connect gate="G$1" pin="PR1" pad="F1"/>
<connect gate="G$1" pin="VCC" pad="A2 A5 A9 C1 C10 F10 K6 K8" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA64B1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA B1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Two-channel DMA controller
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Three 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extensions one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Split mode on two timer/counters
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Two USARTs with IrDA support for one USART
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– One two-wire interface with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– One serial peripheral interface (SPI)
&lt;dd&gt;– 16-bit Real Time Counter (RTC) with separate oscillator
&lt;dd&gt;– Liquid Crystal Display
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Up to 4x40 segment driver
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Built in contrast control
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;ASCII character mapping
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Flexible SWAP of segment and common terminals buses
&lt;dd&gt;– Two eight-channel, 12-bit, 300 thousand SPS Analog to Digital Converters
&lt;dd&gt;– Four Analog Comparators with window compare function, and current source feature
&lt;dd&gt;– External interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 53 Programmable I/O pins
&lt;dd&gt;– 100-lead TQFP
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="B1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA128B1" prefix="U">
<description>8/16-bit &lt;b&gt;XMEGA B1&lt;/b&gt; Microcontroller&lt;p&gt;

&lt;b&gt;&lt;font size=4 &gt;Features&lt;/font&gt;&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;High-performance, low-power Atmel® AVR® XMEGA® 8/16-bit Microcontroller
&lt;li&gt;Nonvolatile program and data memories
&lt;dl&gt;
&lt;dd&gt;– 64K - 128KBytes of in-system self-programmable flash
&lt;dd&gt;– 4K - 8KBytes boot section
&lt;dd&gt;– 2KBytes EEPROM
&lt;dd&gt;– 4K - 8KBytes internal SRAM
&lt;/dl&gt;
&lt;li&gt;Peripheral Features
&lt;dl&gt;
&lt;dd&gt;– Two-channel DMA controller
&lt;dd&gt;– Four-channel event system
&lt;dd&gt;– Three 16-bit timer/counters
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Two timer/counters with 4 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;One timer/counter with 2 output compare or input capture channels
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;High resolution extensions one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Advanced waveform extension (AWeX) on one timer/counter
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Split mode on two timer/counters
&lt;dd&gt;– One USB device interface
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;USB 2.0 full speed (12Mbps) and low speed (1.5Mbps) device compliant
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;32 Endpoints with full configuration flexibility
&lt;dd&gt;– Two USARTs with IrDA support for one USART
&lt;dd&gt;– AES and DES crypto engine
&lt;dd&gt;– CRC-16 (CRC-CCITT) and CRC-32 (IEEE® 802.3) generator
&lt;dd&gt;– One two-wire interface with dual address match (I2C and SMBus compatible)
&lt;dd&gt;– One serial peripheral interface (SPI)
&lt;dd&gt;– 16-bit Real Time Counter (RTC) with separate oscillator
&lt;dd&gt;– Liquid Crystal Display
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Up to 4x40 segment driver
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Built in contrast control
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;ASCII character mapping
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Flexible SWAP of segment and common terminals buses
&lt;dd&gt;– Two eight-channel, 12-bit, 300 thousand SPS Analog to Digital Converters
&lt;dd&gt;– Four Analog Comparators with window compare function, and current source feature
&lt;dd&gt;– External interrupts on all General Purpose I/O pins
&lt;dd&gt;– Programmable watchdog timer with separate on-chip ultra low power oscillator
&lt;dd&gt;– QTouch® library support
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;Capacitive touch buttons, sliders and wheels
&lt;/dl&gt;
&lt;li&gt;Special microcontroller features
&lt;dl&gt;
&lt;dd&gt;– Power-on reset and programmable brown-out detection
&lt;dd&gt;– Internal and external clock options with PLL
&lt;dd&gt;– Programmable multilevel interrupt controller
&lt;dd&gt;– Five sleep modes
&lt;dd&gt;– Programming and debug interfaces
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;JTAG (IEEE 1149.1 Compliant) interface, including boundary scan
&lt;dd&gt;&lt;i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;PDI (Program and Debug Interface)
&lt;/dl&gt;
&lt;li&gt;I/O and Packages
&lt;dl&gt;
&lt;dd&gt;– 53 Programmable I/O pins
&lt;dd&gt;– 100-lead TQFP
&lt;/dl&gt;
&lt;li&gt;Operating Voltage
&lt;dl&gt;
&lt;dd&gt;– 1.6 – 3.6V
&lt;/dl&gt;
&lt;li&gt;Operating frequency
&lt;dl&gt;
&lt;dd&gt;– 0 – 12MHz from 1.6V
&lt;dd&gt;– 0 – 32MHz from 2.7V
&lt;/dl&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="B1"/>
</gates>
<devices>
<device name="-AU" package="TQFP-100A-100">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
