<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL18">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="SO-18W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="DIL28-6">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="DIL28-SP">
<description>&lt;b&gt;28-Lead Skinny Plastic Dual In-Line (SP) – 300 mil Body [SPDIP]l&lt;/b&gt;</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AB</description>
</package>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="PLCC-44">
<description>Plastic &lt;B&gt;LCC&lt;/B&gt;&lt;p&gt;
square&lt;p&gt;
package type L</description>
</package>
<package name="MQFP44-2">
<description>&lt;b&gt;Plastic Metric Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type PQ</description>
</package>
<package name="DIL8">
<description>&lt;B&gt;DIL&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="PLCC-68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square, package type L</description>
</package>
<package name="DIL64">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body&lt;p&gt;
package type SN</description>
</package>
<package name="SO-08W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="SOIC-14">
<description>14-Lead Plastic Small Outline (SL) – Narrow, 150 mil (SOIC)</description>
</package>
<package name="SO-08M">
<description>&lt;B&gt;Small Outline Medium Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
207-mil body, package type SM</description>
</package>
<package name="DIL24-6">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="PLCC-32">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
rectangle, package type L</description>
</package>
<package name="TSOP28">
<description>&lt;b&gt;Thin Small Outline Package Gull Wing&lt;/b&gt;&lt;p&gt;
type I, package type TS</description>
</package>
<package name="LCC44">
<description>&lt;b&gt;CERAMIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square, package type K</description>
</package>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="TSSOP8">
<description>&lt;b&gt;Thin Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type ST</description>
</package>
<package name="VSOP28-8X13">
<description>&lt;b&gt;Very Small Outline Package&lt;/b&gt;&lt;p&gt;
8 x 13.4 mm, package type VS</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="TQFP64-10X10">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="LOGO">
<description>&lt;B&gt;LOGO&lt;/B&gt;</description>
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
<package name="PLCC20S">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square, package type L</description>
</package>
<package name="S44">
<description>&lt;b&gt;PLCC SOCKET&lt;/b&gt;</description>
</package>
<package name="SSOP18">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS&lt;br&gt;
Source: ww1.microchip.com/downloads/en/DeviceDoc/39605c.pdf</description>
</package>
<package name="QFN28">
<description>&lt;b&gt;28-Lead Plastic Quad Flat No Lead Package (ML)&lt;/b&gt;&lt;br&gt;
 6x6 mm Body, Punch Singulated (QFN)&lt;p&gt;
Source: ww1.microchip.com/downloads/en/DeviceDoc/39605c.pdf</description>
</package>
<package name="DFN-S">
<description>&lt;b&gt;8-Lead Plastic Dual Flat No Lead Package (MF)&lt;/b&gt; 6x5 mm Body (DFN-S)&lt;p&gt;
Source: http://www.microchip.com .. 41190c.pdf</description>
</package>
<package name="QFN28-ML_6X6MM">
<description>&lt;b&gt;QFN28-ML_6X6MM&lt;/b&gt;&lt;p&gt;
Source: http://www.microchip.com .. 39637a.pdf</description>
</package>
<package name="TQFP80-12X12">
<description>&lt;b&gt;TQFP80&lt;/b&gt; 12x12x1 mm Body&lt;p&gt;
Source: http://www.microchip.com/ .. 39663c.pdf</description>
</package>
<package name="QFN44ML8X8">
<description>&lt;b&gt;44-Lead Plastic Quad Flat No Lead Package (ML)&lt;/b&gt; 8x8 mm Body (QFN)&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
</package>
<package name="DFN-2X3">
<description>&lt;b&gt;8-Lead Plastic Dual Flat No Lead Package (MC)&lt;/b&gt; 2x3x0.9 mm Body (DFN) - Saw Singulated&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21796H.pdf</description>
</package>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;Micro Small Outline Package&lt;/b&gt; Grid 0.65mm&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21796H.pdf</description>
</package>
<package name="SO-14DW">
<description>&lt;b&gt;Small Outline Integrated Circuit&lt;/b&gt; wide</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO-16DW">
<description>&lt;b&gt;Small Outline Integrated Circuit&lt;/b&gt; wide</description>
</package>
<package name="TQFP100-14X14">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt; 14x14 mm&lt;p&gt;</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="DFN8-4X4">
<description>&lt;b&gt;8-Lead Plastic Dual Flat, No Lead Package (MD)&lt;/b&gt; 4x4x0.9 mm Body [DFN]&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41211D_.pdf</description>
</package>
<package name="QFN40ML6X6MM">
<description>&lt;b&gt;40-Lead Plastic Quad Flat&lt;/b&gt; 6x6x0.9 mm Body [QFN]&lt;p&gt;
With 0.40 mm Contact Length&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39776a.pdf</description>
</package>
<package name="SS20">
<description>&lt;b&gt;20-Lead Plastic Shrink Small Outline&lt;/b&gt; K04-072 (SS) - 5.30 mm&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/40300C.pdf</description>
</package>
<package name="SQFP-S-12X12-100">
<description>&lt;b&gt;QFP100&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="QFN16-4X4">
<description>&lt;b&gt;16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9mm Body [QFN]&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41203E.pdf</description>
</package>
<package name="TQFP64-10X10X1MM">
<description>&lt;b&gt;64-Lead Plastic Thin Quad Flatpak (PT) - 10x10x1 mm Body&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 37&lt;/i&gt;&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/61143G.pdf</description>
</package>
<package name="TQFP100-12X12">
<description>&lt;b&gt;TQFP100_12X12&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 41&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="UQFN28_4X4MM">
<description>&lt;b&gt;28-Lead Platic Ultra Thin Quad Flat, No Lead Package (MV) - 4x4x0.5 mm Body [UQFN]&lt;p&gt;
Source: PIC16F1516.pdf</description>
</package>
<package name="UQFN40ML5X5MM">
<description>&lt;b&gt;40-Lead Platic Ultra Thin Quad Flat, No Lead Package (MV) - 5x5mm Body [UQFN]&lt;/b&gt;&lt;p&gt;
Source: www.microchip.com PIC16F1516.pdf</description>
</package>
<package name="DFN8-3X3">
<description>&lt;b&gt;DD Package 8-Lead Plastic DFN (3mm × 3mm)&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
</package>
<package name="SOIC8">
<description>&lt;b&gt;SOIC-8&lt;/b&gt; CASE 751-07&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF&lt;p&gt;
&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;PLATIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
</package>
<package name="DFN10-3X3">
</package>
<package name="MSOP10">
<description>&lt;b&gt;10-Lead Mini Small Outline Package [MSOP]&lt;/b&gt; (RM-10)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/35641221898805SSM2167_b.pdf&lt;br&gt;
COMPLIANT TO JEDEC STANDARDS MO-187BA</description>
</package>
<package name="QFN64_9X9MC">
<description>QFN64 9x9</description>
</package>
<package name="QFP64-10X10MC">
<description>QFP64 10x10</description>
</package>
<package name="XBGA121_10X10MC">
<description>XBGA121 10X10</description>
</package>
<package name="TQFP100_14X14MC">
<description>TQFP100 14X14</description>
</package>
<package name="TQFP100_12X12MC">
<description>TQFP100 12X12</description>
</package>
<package name="TQFP144_16X16MC">
<description>TQFP144 16X16</description>
</package>
<package name="LQFP144_20X20MC">
<description>LQFP144 20X20</description>
</package>
<package name="SO_28W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body&lt;p&gt;
package type SO</description>
</package>
<package name="SOIC20">
<description>&lt;b&gt;Plastic Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SO</description>
</package>
<package name="QFN20-5X5">
<description>20-Lead Plastic Quad Flat,No Lead Package (MQ)-5x5 mm</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="QFN33-5X5">
<description>&lt;b&gt;QFN33 &lt;/b&gt;&lt;p&gt;Plastic thermal enhanced quad flat package; 33 terminals; body 5x5x0.75 mm;</description>
</package>
<package name="MRF89XAMXA">
<description>Microchip MRF89XAMxA Module Footprint</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO20W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AC</description>
</package>
<package name="QFP-44">
<description>&lt;b&gt;Quad Flat Package&lt;/b&gt;</description>
</package>
<package name="PQFP44">
<description>&lt;B&gt;Plastic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOIC16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SOIC28W">
<description>&lt;b&gt;28-Lead Plastic Small Outline (SO) – Wide, 300 mil Body (SOIC)) &lt;/b&gt;&lt;p&gt;
Source: www.microchip.com</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="QFN44-8X8">
<description>&lt;b&gt;Quad Flat No Lead&lt;/b&gt;</description>
</package>
<package name="SOT23B-3">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SO18W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="QFN-S28-6X6">
<description>&lt;b&gt;Quad Flat No Lead&lt;/b&gt;</description>
</package>
<package name="TQFP64_10X10">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="TQFP80_12X12">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP80_917">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP64">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="SO-28W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="MSOP-8">
<description>&lt;b&gt;Micro Small Outline Package&lt;/b&gt;</description>
</package>
<package name="QFN16">
<description>&lt;b&gt;QFN 16&lt;/b&gt; 3x3 mm&lt;p&gt;</description>
</package>
<package name="QFN10_2,1X1,6">
<description>&lt;B&gt;10 pin, 1.6mm x 2.1mm QFN Package Outline</description>
</package>
<package name="QFN10_1,3X1,8">
<description>&lt;B&gt;10 pin, 1.3mm x 1.8mm QFN Package Outline</description>
</package>
</packages>
<symbols>
<symbol name="13IO-2">
<pin name="T0CKI" direction="in"/>
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="OSC2" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="13IO-1SS">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="OSC2" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
</symbol>
<symbol name="13IO-1">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="T0CKI/RA4"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="OSC2" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="20IO-2">
<pin name="T0CKI" direction="in"/>
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="OSC2" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="33IO-MQ">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RA5"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="OSC2" direction="out"/>
<pin name="RB0"/>
<pin name="RA4"/>
</symbol>
<symbol name="33IO-1A">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RA5"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RC0" direction="out"/>
<pin name="RC1" direction="out"/>
<pin name="RC2" direction="out"/>
<pin name="RC3" direction="out"/>
<pin name="RC4" direction="out"/>
<pin name="RC5" direction="out"/>
<pin name="RC6" direction="out"/>
<pin name="RC7" direction="out"/>
<pin name="RB7"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="OSC2" direction="out"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
</symbol>
<symbol name="13IO-2SS">
<pin name="T0CKI" direction="in"/>
<pin name="!MCLR" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC1" direction="in"/>
</symbol>
<symbol name="22IO-1">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RA5"/>
<pin name="OSC2"/>
<pin name="RC7"/>
<pin name="RC6"/>
<pin name="RC5"/>
<pin name="RC4"/>
<pin name="RC3"/>
<pin name="RC2"/>
<pin name="RC1"/>
<pin name="RC0"/>
<pin name="RB7"/>
<pin name="RB6"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="33IO-1MQ">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RA5"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="RB7"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="OSC2" direction="out"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="33IO-1">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RA5"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RC0" direction="out"/>
<pin name="RC1" direction="out"/>
<pin name="RC2" direction="out"/>
<pin name="RC3" direction="out"/>
<pin name="RC4" direction="out"/>
<pin name="RC5" direction="out"/>
<pin name="RC6" direction="out"/>
<pin name="RC7" direction="out"/>
<pin name="RB7"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="OSC2" direction="out"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
</symbol>
<symbol name="6IO">
<pin name="GP0"/>
<pin name="GP1"/>
<pin name="GP2"/>
<pin name="GP3/MC" direction="in"/>
<pin name="GP4/COUT"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="GP5/CIN"/>
</symbol>
<symbol name="14000">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="VREG" direction="out"/>
<pin name="SUM" direction="out"/>
<pin name="OSC2" direction="out"/>
<pin name="RC7"/>
<pin name="RC6"/>
<pin name="RC5"/>
<pin name="RC4"/>
<pin name="RC3"/>
<pin name="RC2"/>
<pin name="RC1"/>
<pin name="RC0"/>
<pin name="RD7"/>
<pin name="RD6"/>
<pin name="RD5"/>
<pin name="RD4"/>
<pin name="RD3"/>
<pin name="RD2"/>
<pin name="RD1"/>
<pin name="RD0"/>
<pin name="CDAC" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="16C9P">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RA5"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="C1" direction="in"/>
<pin name="C2" direction="in"/>
<pin name="VLCD1" direction="in"/>
<pin name="VLCDADJ" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="OSC2" direction="out"/>
<pin name="RB0"/>
<pin name="RA4"/>
<pin name="RE3"/>
<pin name="RE4"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RF2"/>
<pin name="RF3"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF6"/>
<pin name="RF7"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="RG2"/>
<pin name="RG3"/>
<pin name="RG4"/>
<pin name="RG5"/>
<pin name="RG6"/>
<pin name="COM0" direction="out"/>
<pin name="VLCD2" direction="in"/>
<pin name="VLCD3" direction="in"/>
</symbol>
<symbol name="16C9L">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RA5"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="C1" direction="in"/>
<pin name="C2" direction="in"/>
<pin name="VLCD1" direction="in"/>
<pin name="VLCDADJ" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="OSC2" direction="out"/>
<pin name="RB0"/>
<pin name="RA4"/>
<pin name="RE3"/>
<pin name="RE4"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RF2"/>
<pin name="RF3"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF6"/>
<pin name="RF7"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="RG2"/>
<pin name="RG3"/>
<pin name="RG4"/>
<pin name="RG5"/>
<pin name="RG6"/>
<pin name="COM0" direction="out"/>
<pin name="VLCD2" direction="in"/>
<pin name="VLCD3" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RE7"/>
<pin name="RG7"/>
</symbol>
<symbol name="SEEPROM">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="TST" direction="pas"/>
</symbol>
<symbol name="24C02">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="59C11">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DO" direction="hiz"/>
<pin name="RDY" direction="out"/>
<pin name="ORG" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="85C72">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA" direction="hiz"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="SCL" direction="in"/>
</symbol>
<symbol name="93C06">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DO" direction="hiz"/>
<pin name="DI" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="93C56">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DO" direction="hiz"/>
<pin name="TST" direction="pas"/>
<pin name="ORG" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="93LC46">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DO" direction="hiz"/>
<pin name="NU" direction="pas"/>
<pin name="ORG" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="37LV">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DATA" direction="hiz"/>
<pin name="!OE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="VPP" direction="in"/>
<pin name="!CEO" direction="out"/>
</symbol>
<symbol name="24AA">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="24C65">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="28C04">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="NC19" direction="nc"/>
<pin name="NC22" direction="nc"/>
</symbol>
<symbol name="28C16">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
</symbol>
<symbol name="28C17">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="RDY/!BSY" direction="out"/>
</symbol>
<symbol name="28C64">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="RDY/!BSY" direction="out"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
</symbol>
<symbol name="27C64">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="PGM" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="VPP" direction="in"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="27C128">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!PGM" direction="pas"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="VPP" direction="in"/>
<pin name="A13" direction="in"/>
</symbol>
<symbol name="27C256">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="VPP" direction="in"/>
<pin name="A13" direction="in"/>
</symbol>
<symbol name="27C512">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="VPP/!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A13" direction="in"/>
</symbol>
<symbol name="27HC1616">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="VPP" direction="pas"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="NU36" direction="nc"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="NU37" direction="nc"/>
<pin name="A13" direction="in"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
<pin name="GND@1" direction="pwr"/>
<pin name="!OE" direction="in"/>
<pin name="PGM" direction="pas"/>
<pin name="NU38" direction="nc"/>
</symbol>
<symbol name="AY0438">
<pin name="SEG1" direction="out"/>
<pin name="SEG2" direction="out"/>
<pin name="SEG3" direction="out"/>
<pin name="SEG4" direction="out"/>
<pin name="SEG5" direction="out"/>
<pin name="SEG6" direction="out"/>
<pin name="SEG7" direction="out"/>
<pin name="SEG8" direction="out"/>
<pin name="SEG9" direction="out"/>
<pin name="SEG10" direction="out"/>
<pin name="SEG11" direction="out"/>
<pin name="SEG12" direction="out"/>
<pin name="SEG13" direction="out"/>
<pin name="SEG14" direction="out"/>
<pin name="SEG15" direction="out"/>
<pin name="SEG16" direction="out"/>
<pin name="SEG17" direction="out"/>
<pin name="SEG18" direction="out"/>
<pin name="SEG19" direction="out"/>
<pin name="SEG20" direction="out"/>
<pin name="SEG21" direction="out"/>
<pin name="SEG22" direction="out"/>
<pin name="SEG23" direction="out"/>
<pin name="SEG24" direction="out"/>
<pin name="SEG25" direction="out"/>
<pin name="SEG26" direction="out"/>
<pin name="SEG27" direction="out"/>
<pin name="SEG28" direction="out"/>
<pin name="SEG29" direction="out"/>
<pin name="SEG30" direction="out"/>
<pin name="SEG31" direction="out"/>
<pin name="SEG32" direction="out"/>
<pin name="DO" direction="out"/>
<pin name="LOAD" direction="in"/>
<pin name="LCD0" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="BP" direction="out"/>
</symbol>
<symbol name="PIC16C54">
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RTCC" direction="in"/>
<pin name="MCLR" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC2" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="PIC16C56">
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RTCC" direction="in"/>
<pin name="MCLR" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC2" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="PIC16C55">
<pin name="RTCC" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="N/C@1" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="N/C@2" direction="nc"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="OSC2" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="MCLR" direction="in"/>
</symbol>
<symbol name="PIC16C71">
<pin name="RA2/AIN2"/>
<pin name="RA3/AIN3"/>
<pin name="RA4/T0CKI" direction="in"/>
<pin name="MCLR" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC2" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="RA0/AIN0"/>
<pin name="RA1/AIN1"/>
</symbol>
<symbol name="HCS410">
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="LC0"/>
<pin name="LC1"/>
<pin name="S2/LED"/>
<pin name="PWM"/>
</symbol>
<symbol name="93LC46B">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DO" direction="hiz"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="SERIALEEPROM">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
</symbol>
<symbol name="SERIAL-EEPROM-DUAL">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="VCLK" direction="in"/>
<pin name="!WP" direction="in"/>
</symbol>
<symbol name="24-LC">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="VCLK" direction="in"/>
</symbol>
<symbol name="24LC41">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DSCL" direction="in"/>
<pin name="DSDA"/>
<pin name="MWP" direction="in"/>
<pin name="MSDA"/>
<pin name="!DWP" direction="in"/>
<pin name="MSCL" direction="in"/>
</symbol>
<symbol name="24LC61">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="!EDS" direction="out"/>
<pin name="SCL" direction="in"/>
</symbol>
<symbol name="24AA32">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="93LCS">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DO" direction="hiz"/>
<pin name="PRE" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="25SERIAL">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!CS" direction="in"/>
<pin name="SO"/>
<pin name="!HOLD" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="!WP" direction="in"/>
</symbol>
<symbol name="PIC16F871">
<pin name="!MCLR/THV" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="RE0/!RD/AN5"/>
<pin name="RE1/!WR/AN6"/>
<pin name="RE2/!CS/AN7"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="OSC2/CLKOUT" direction="out"/>
<pin name="RC0/T1OSO"/>
<pin name="RC1/T1OSI"/>
<pin name="RC2/CCP1"/>
<pin name="RC3"/>
<pin name="RD0/PSP0"/>
<pin name="RD1/PSP1"/>
<pin name="RD2/PSP2"/>
<pin name="RD3/PSP3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="TX/RC6"/>
<pin name="RX/RC7"/>
<pin name="PSP4/RD4"/>
<pin name="PSP5/RD5"/>
<pin name="PSP6/RD6"/>
<pin name="PSP7/RD7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="PGM/RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="PGC/RB6"/>
<pin name="PGD/RB7"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="PIC16F870">
<pin name="!MCLR/THV" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="OSC2/CLKOUT" direction="out"/>
<pin name="RC0/T1OSO"/>
<pin name="RC1/T1OSI"/>
<pin name="RC2/CCP1"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="TX/RC6"/>
<pin name="RX/RC7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="PGM/RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="PGC/RB6"/>
<pin name="PGD/RB7"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="PIC16F872">
<pin name="!MCLR/THV" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="OSC2/CLKOUT" direction="out"/>
<pin name="RC0/T1OSO"/>
<pin name="RC1/T1OSI"/>
<pin name="RC2/CCP1"/>
<pin name="RC3/SCK"/>
<pin name="SDI/RC4"/>
<pin name="SDO/RC5"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="PGM/RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="PGC/RB6"/>
<pin name="PGD/RB7"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="PIC17F874">
<pin name="!MCLR/THV" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="RE0/!RD/AN5"/>
<pin name="RE1/!WR/AN6"/>
<pin name="RE2/!CS/AN7"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="OSC2/CLKOUT" direction="out"/>
<pin name="RC0/T1OSO"/>
<pin name="RC1/T1OSI"/>
<pin name="RC2/CCP1"/>
<pin name="RC3/SCK"/>
<pin name="RD0/PSP0"/>
<pin name="RD1/PSP1"/>
<pin name="RD2/PSP2"/>
<pin name="RD3/PSP3"/>
<pin name="SDI/RC4"/>
<pin name="SDO/RC5"/>
<pin name="TX/RC6"/>
<pin name="RX/RC7"/>
<pin name="PSP4/RD4"/>
<pin name="PSP5/RD5"/>
<pin name="PSP6/RD6"/>
<pin name="PSP7/RD7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="PGM/RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="PGC/RB6"/>
<pin name="PGD/RB7"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="PIC17C75X">
<pin name="RD0/AD8"/>
<pin name="RD1/AD9"/>
<pin name="RD2/AD10"/>
<pin name="RD3/AD11"/>
<pin name="RD4/AD12"/>
<pin name="RD5/AD13"/>
<pin name="RD6/AD14"/>
<pin name="RD7/AD15"/>
<pin name="RE0/ALE"/>
<pin name="RE1/!OE"/>
<pin name="RE2/!WR"/>
<pin name="RE3/CAP4"/>
<pin name="!MCLR" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="RF0/AN4"/>
<pin name="RF1/AN5"/>
<pin name="RF2/AN6"/>
<pin name="RF3/AN7"/>
<pin name="RF4/AN8"/>
<pin name="RF5/AN9"/>
<pin name="RF6/AN10"/>
<pin name="RF7/AN11"/>
<pin name="RG0/AN3"/>
<pin name="RG1/AN2"/>
<pin name="RG2/AN1"/>
<pin name="RG3/AN0"/>
<pin name="RG4/CAP3"/>
<pin name="RG5/PWM3"/>
<pin name="RG6/RX2"/>
<pin name="RG7/TX2"/>
<pin name="RA0/INT" direction="in"/>
<pin name="RA1/TOCKI" direction="in"/>
<pin name="RA2/SCL"/>
<pin name="RA3/SDA"/>
<pin name="RA4/RX1"/>
<pin name="RA5/TX1"/>
<pin name="RB0/CAP1"/>
<pin name="RB1/CAP2"/>
<pin name="RB2/PWM1"/>
<pin name="RB3/PWM2"/>
<pin name="RB4/TCLK12"/>
<pin name="RB5/TCLK3"/>
<pin name="RB6/SCK"/>
<pin name="RB7/SDO"/>
<pin name="RC0/AD0"/>
<pin name="RC1/AD1"/>
<pin name="RC2/AD2"/>
<pin name="RC3/AD3"/>
<pin name="RC4/AD4"/>
<pin name="RC5/AD5"/>
<pin name="RC6/AD6"/>
<pin name="RC7/AD7"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="OSC1/CKIN" direction="in"/>
<pin name="OSC2/CKOUT" direction="out"/>
</symbol>
<symbol name="VSS">
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="VDD">
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PIC18F1220">
<pin name="RA2/AN2/VREF-"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/!MCLR" direction="in"/>
<pin name="VSS@AVSS" direction="pwr"/>
<pin name="INT0/AN4/RB0"/>
<pin name="INT1/CK/TX/AN5/RB1"/>
<pin name="INT2/P1B/RB2"/>
<pin name="P1A/CCP1/RB3"/>
<pin name="BKI0/DT/RX/AN6/RB4"/>
<pin name="KBI1/PGM/RB5"/>
<pin name="KBI2/P1C/T13CKI/T1OSO/RB6"/>
<pin name="KBI3/P1D/T1OSI/PGD/RB7"/>
<pin name="VDD@AVDD" direction="pwr"/>
<pin name="RA6/CLKO/OSC2"/>
<pin name="RA7/CLKI/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1/LVDIN"/>
</symbol>
<symbol name="PIC18F1320">
<pin name="RA2/AN2/VREF-"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/!MCLR" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="INT0/AN4/RB0"/>
<pin name="INT1/CK/TX/AN5/RB1"/>
<pin name="INT2/P1B/RB2"/>
<pin name="P1A/CCP1/RB3"/>
<pin name="BKI0/DT/RX/AN6/RB4"/>
<pin name="KBI1/PGM/RB5"/>
<pin name="KBI2/P1C/T13CKI/T1OSO/RB6"/>
<pin name="KBI3/P1D/T1OSI/PGD/RB7"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA6/CLKO/OSC2"/>
<pin name="RA7/CLKI/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1/LVDIN"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="PIC12F629">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="GP5/CLKIN"/>
<pin name="GP0"/>
<pin name="GP4/CLKOUT"/>
<pin name="GP2"/>
<pin name="GP1"/>
<pin name="GP3" direction="in"/>
</symbol>
<symbol name="PIC18F2580">
<pin name="RE3/!MCLR/VPP" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4/!SS/HLVDIN"/>
<pin name="VSS" direction="pwr"/>
<pin name="RA7/CLKI/OSC1" direction="in"/>
<pin name="RA6/CLKO/OSC2" direction="out"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC1/T1OSI"/>
<pin name="RC2/CCP1"/>
<pin name="RC3/SCK/SCL"/>
<pin name="RC4/SDI/SDA"/>
<pin name="RC5/SDO"/>
<pin name="RC6/TX/CK"/>
<pin name="RC7/RX/DT"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INT0/AN10/RB0"/>
<pin name="INT1/AN8/RB1"/>
<pin name="INT2/CANTX/RB2"/>
<pin name="CANRX/RB3"/>
<pin name="KBI0/AN9/RB4"/>
<pin name="KBI1/PGM/RB5"/>
<pin name="KBI2/PGC/RB6"/>
<pin name="KBI3/PGD/RB7"/>
</symbol>
<symbol name="PIC18F6XJ10">
<pin name="RE1/!WR/P2C"/>
<pin name="RE0/!RD/P2D"/>
<pin name="RG0/ECCP3/P3A"/>
<pin name="RG1/TX2/CK2"/>
<pin name="RG2/RX2/DT2"/>
<pin name="RG3/CCP4/P3D"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP" direction="pwr"/>
<pin name="RF7/!SS1"/>
<pin name="RF6/AN11"/>
<pin name="RF5/AN10/CVREF"/>
<pin name="RF4/AN9"/>
<pin name="RF3/AN8"/>
<pin name="RF2/AN7/C1OUT"/>
<pin name="RF1/AN6/C2OUT"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/AN1"/>
<pin name="RA0/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RA5/AN4"/>
<pin name="RA4/T0CK"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1"/>
<pin name="RB7/KBI2/PGD"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="OSC2/CLKO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1"/>
<pin name="RB4/KBI0"/>
<pin name="RB3/INT3"/>
<pin name="RB2/INT2"/>
<pin name="RB1/INT1"/>
<pin name="RB0/INT0/FLT0"/>
<pin name="RD7/PSP7/!SS2"/>
<pin name="RD6/PSP6/SCK2/SCL2"/>
<pin name="RD5/PSP5/SDI2/SDA2"/>
<pin name="RD4/PSP4/SDO2"/>
<pin name="RD3/PSP3"/>
<pin name="RD2/PSP2"/>
<pin name="RD1/PSP1"/>
<pin name="RD0/PSP0"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RE7/ECCP2/P2A"/>
<pin name="RE6/P1B"/>
<pin name="RE5/P1C"/>
<pin name="RE4/P3B"/>
<pin name="RE3/P3C"/>
<pin name="RE2/!CS/P2B"/>
</symbol>
<symbol name="PIC18F87J10">
<pin name="RE1/AD9/!WR/P2C"/>
<pin name="RE0/AD8/!RD/P2D"/>
<pin name="RG0/ECCP3/P3A"/>
<pin name="RG1/TX2/CK2"/>
<pin name="RG2/RX2/DT2"/>
<pin name="RG3/CCP4/P3D"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP" direction="pwr"/>
<pin name="RF7/!SS1"/>
<pin name="RF6/AN11"/>
<pin name="RF5/AN10/CVREF"/>
<pin name="RF4/AN9"/>
<pin name="RF3/AN8"/>
<pin name="RF2/AN7/C1OUT"/>
<pin name="RF1/AN6/C2OUT"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/AN1"/>
<pin name="RA0/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RA5/AN4"/>
<pin name="RA4/T0CK"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1"/>
<pin name="RB7/KBI2/PGD"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="OSC2/CLKO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1"/>
<pin name="RB4/KBI0"/>
<pin name="RB3/INT3/ACCP2/P2A"/>
<pin name="RB2/INT2"/>
<pin name="RB1/INT1"/>
<pin name="RB0/INT0/FLT0"/>
<pin name="RD7/AD7/PSP7/!SS2"/>
<pin name="RD6/AD6/PSP6/SCK2/SCL2"/>
<pin name="RD5/AD5/PSP5/SDI2/SDA2"/>
<pin name="RD4/AD4/PSP4/SDO2"/>
<pin name="RD3/AD3/PSP3"/>
<pin name="RD2/AD2/PSP2"/>
<pin name="RD1/AD1/PSP1"/>
<pin name="RD0/AD0/PSP0"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RE7/AD15/ECCP2/P2A"/>
<pin name="RE6/AD14/P1B"/>
<pin name="RE5/AD13/P1C"/>
<pin name="RE4/AD12/P3B"/>
<pin name="RE3/AD11/P3C"/>
<pin name="RE2/!AD10CS/P2B"/>
<pin name="RH2/A18"/>
<pin name="RH3/A19"/>
<pin name="RH7/AN15/P1B"/>
<pin name="RH6/AN14/P1C"/>
<pin name="RH5/AN13/P3B"/>
<pin name="RH4/AN12/P3C"/>
<pin name="RJ4/BA0"/>
<pin name="RJ5/!CE"/>
<pin name="RJ6/!LB"/>
<pin name="RJ7/!UB"/>
<pin name="RJ3/!WRH"/>
<pin name="RJ2/!WRL"/>
<pin name="RJ1/!OE"/>
<pin name="RJ0/ALE"/>
<pin name="RH0/A16"/>
<pin name="RH1/A17"/>
</symbol>
<symbol name="PIC18F4455_44TQFP">
<pin name="RC7/RX/DT/SDO"/>
<pin name="RD4/SPP4"/>
<pin name="RD5/SPP5/P1B"/>
<pin name="RD6/SPP6/P1C"/>
<pin name="RD7/SPP7/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/AN12/INT0/LFT0/SDI/SDA"/>
<pin name="RB1/AN10/INT1/SCK/SCL"/>
<pin name="RB2/AN8/INT2/VMO"/>
<pin name="RB3/AN9/CCP2/VPO"/>
<pin name="NC/ICCK/ICPGC"/>
<pin name="NC/ICDT/ICPGD"/>
<pin name="RB4/AN11/KBI0/CSSPP"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/BKI3/PGD"/>
<pin name="!MCLR!/VPP/RE3" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF-/CVREF"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI/CIOUT/RCV"/>
<pin name="RA5/AN4/!SS!/HLVDIN/C2OUT"/>
<pin name="RE0/AN5/CK1SPP"/>
<pin name="RE1/AN6/CK2SPP"/>
<pin name="RE2/AN7/OESPP"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RA6/OSC2/CLKO" direction="out"/>
<pin name="RC0/TIOSO/T13CKI"/>
<pin name="NC/!ICRST!/IVVPP" direction="in"/>
<pin name="NC/ICPORTS" direction="in"/>
<pin name="RC1/T1OSI/ICCP2/!UOE"/>
<pin name="RC2/CCP1/P1A"/>
<pin name="VUSB"/>
<pin name="RD0/SPP0"/>
<pin name="RD1/SPP1"/>
<pin name="RD2/SPP2"/>
<pin name="RD3/SPP3"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/TX/CK"/>
</symbol>
<symbol name="PIC18F4455_44QFN">
<pin name="RC7/RX/DT/SDO"/>
<pin name="RD4/SPP4"/>
<pin name="RD5/SPP5/P1B"/>
<pin name="RD6/SPP6/P1C"/>
<pin name="RD7/SPP7/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/AN12/INT0/LFT0/SDI/SDA"/>
<pin name="RB1/AN10/INT1/SCK/SCL"/>
<pin name="RB2/AN8/INT2/VMO"/>
<pin name="RB3/AN9/CCP2/VPO"/>
<pin name="NC"/>
<pin name="RB4/AN11/KBI0/CSSPP"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/BKI3/PGD"/>
<pin name="!MCLR!/VPP/RE3" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF-/CVREF"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI/CIOUT/RCV"/>
<pin name="RA5/AN4/!SS!/HLVDIN/C2OUT"/>
<pin name="RE0/AN5/CK1SPP"/>
<pin name="RE1/AN6/CK2SPP"/>
<pin name="RE2/AN7/OESPP"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RA6/OSC2/CLKO" direction="out"/>
<pin name="RC0/TIOSO/T13CKI"/>
<pin name="RC1/T1OSI/ICCP2/!UOE"/>
<pin name="RC2/CCP1/P1A"/>
<pin name="VUSB"/>
<pin name="RD0/SPP0"/>
<pin name="RD1/SPP1"/>
<pin name="RD2/SPP2"/>
<pin name="RD3/SPP3"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/TX/CK"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="PIC18F4455_40">
<pin name="RC7/RX/DT/SDO"/>
<pin name="RD4/SPP4"/>
<pin name="RD5/SPP5/P1B"/>
<pin name="RD6/SPP6/P1C"/>
<pin name="RD7/SPP7/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/AN12/INT0/LFT0/SDI/SDA"/>
<pin name="RB1/AN10/INT1/SCK/SCL"/>
<pin name="RB2/AN8/INT2/VMO"/>
<pin name="RB3/AN9/CCP2/VPO"/>
<pin name="RB4/AN11/KBI0/CSSPP"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/BKI3/PGD"/>
<pin name="!MCLR!/VPP/RE3" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF-/CVREF"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI/CIOUT/RCV"/>
<pin name="RA5/AN4/!SS!/HLVDIN/C2OUT"/>
<pin name="RE0/AN5/CK1SPP"/>
<pin name="RE1/AN6/CK2SPP"/>
<pin name="RE2/AN7/OESPP"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RA6/OSC2/CLKO" direction="out"/>
<pin name="RC0/TIOSO/T13CKI"/>
<pin name="RC1/T1OSI/ICCP2/!UOE"/>
<pin name="RC2/CCP1/P1A"/>
<pin name="VUSB"/>
<pin name="RD0/SPP0"/>
<pin name="RD1/SPP1"/>
<pin name="RD2/SPP2"/>
<pin name="RD3/SPP3"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/TX/CK"/>
</symbol>
<symbol name="PIC18F4455_28">
<pin name="RC7/RX/DT/SDO"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/AN12/INT0/LFT0/SDI/SDA"/>
<pin name="RB1/AN10/INT1/SCK/SCL"/>
<pin name="RB2/AN8/INT2/VMO"/>
<pin name="RB3/AN9/CCP2/VPO"/>
<pin name="RB4/AN11/KBI0/CSSPP"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/BKI3/PGD"/>
<pin name="!MCLR!/VPP/RE3" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF-/CVREF"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI/CIOUT/RCV"/>
<pin name="RA5/AN4/!SS!/HLVDIN/C2OUT"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RA6/OSC2/CLKO" direction="out"/>
<pin name="RC0/TIOSO/T13CKI"/>
<pin name="RC1/T1OSI/ICCP2/!UOE"/>
<pin name="RC2/CCP1/P1A"/>
<pin name="VUSB"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/TX/CK"/>
</symbol>
<symbol name="MCP23S17">
<pin name="!CS" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="INTA" direction="out"/>
<pin name="INTB" direction="out"/>
<pin name="GPB0"/>
<pin name="GPB1"/>
<pin name="GPB2"/>
<pin name="GPB3"/>
<pin name="GPB4"/>
<pin name="GPB5"/>
<pin name="GPB6"/>
<pin name="GPB7"/>
<pin name="GPA0"/>
<pin name="GPA1"/>
<pin name="GPA2"/>
<pin name="GPA3"/>
<pin name="GPA4"/>
<pin name="GPA5"/>
<pin name="GPA6"/>
<pin name="GPA7"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MCP23017">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="INTA" direction="out"/>
<pin name="INTB" direction="out"/>
<pin name="GPB0"/>
<pin name="GPB1"/>
<pin name="GPB2"/>
<pin name="GPB3"/>
<pin name="GPB4"/>
<pin name="GPB5"/>
<pin name="GPB6"/>
<pin name="GPB7"/>
<pin name="GPA0"/>
<pin name="GPA1"/>
<pin name="GPA2"/>
<pin name="GPA3"/>
<pin name="GPA4"/>
<pin name="GPA5"/>
<pin name="GPA6"/>
<pin name="GPA7"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PIC16F62X">
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF"/>
<pin name="RA3/AN3/CMP1"/>
<pin name="RB0/INT"/>
<pin name="RB1/RX/DT"/>
<pin name="RB2/TX/CK"/>
<pin name="RB3/CCP1"/>
<pin name="RB4/PGM"/>
<pin name="RB5"/>
<pin name="RB6/T1OSO/1ICKI/PGC"/>
<pin name="RB7/T1OSI/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA4/TOCKI/CMP2"/>
<pin name="RA5/MCLR/VPP" direction="in"/>
<pin name="RA6/OSC2/CLKOUT"/>
<pin name="RA7/ASC1/CLKIN"/>
</symbol>
<symbol name="PIC16F62X-SSOP">
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF"/>
<pin name="RA3/AN3/CMP1"/>
<pin name="RB0/INT"/>
<pin name="RB1/RX/DT"/>
<pin name="RB2/TX/CK"/>
<pin name="RB3/CCP1"/>
<pin name="RB4/PGM"/>
<pin name="RB5"/>
<pin name="RB6/T1OSO/1ICKI/PGC"/>
<pin name="RB7/T1OSI/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA4/TOCKI/CMP2"/>
<pin name="RA5/MCLR/VPP" direction="in"/>
<pin name="RA6/OSC2/CLKOUT"/>
<pin name="RA7/ASC1/CLKIN"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="93AA76">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DO" direction="hiz"/>
<pin name="ORG" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="93AA76-OT">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DO" direction="hiz"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="TC4467">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="TC4468">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="TC4469">
<pin name="A" direction="in"/>
<pin name="B" direction="in" function="dot"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="VDD-VSS">
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="VDD-GND-2">
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="PIC18F97J60-100">
<pin name="RE1/AD9/!WR/P2C"/>
<pin name="RE0/AD8/!RD/P2D"/>
<pin name="RG0/ECCP3/P3A"/>
<pin name="RG1/TX2/CK2"/>
<pin name="RG2/RX2/DT2"/>
<pin name="RG3/CCP4/P3D"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP" direction="pwr"/>
<pin name="RF7/!SS1"/>
<pin name="RF6/AN11"/>
<pin name="RF5/AN10/CVREF"/>
<pin name="RF4/AN9"/>
<pin name="RF3/AN8"/>
<pin name="RF2/AN7/C1OUT"/>
<pin name="RF1/AN6/C2OUT"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/AN1"/>
<pin name="RA0/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RA5/AN4"/>
<pin name="RA4/T0CK"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1"/>
<pin name="RB7/KBI2/PGD"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="OSC2/CLKO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1"/>
<pin name="RB4/KBI0"/>
<pin name="RB3/INT3/ACCP2/P2A"/>
<pin name="RB2/INT2"/>
<pin name="RB1/INT1"/>
<pin name="RB0/INT0/FLT0"/>
<pin name="RD7/AD7/PSP7/!SS2"/>
<pin name="RD6/AD6/PSP6/SCK2/SCL2"/>
<pin name="RD5/AD5/PSP5/SDI2/SDA2"/>
<pin name="RD4/AD4/PSP4/SDO2"/>
<pin name="RD3/AD3/PSP3"/>
<pin name="RD2/AD2/PSP2"/>
<pin name="RD1/AD1/PSP1"/>
<pin name="RD0/AD0/PSP0"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RE7/AD15/ECCP2/P2A"/>
<pin name="RE6/AD14/P1B"/>
<pin name="RE5/AD13/P1C"/>
<pin name="RE4/AD12/P3B"/>
<pin name="RE3/AD11/P3C"/>
<pin name="RE2/!AD10CS/P2B"/>
<pin name="RH2/A18"/>
<pin name="RH3/A19"/>
<pin name="RH7/AN15/P1B"/>
<pin name="RH6/AN14/P1C"/>
<pin name="RH5/AN13/P3B"/>
<pin name="RH4/AN12/P3C"/>
<pin name="RJ4/BA0"/>
<pin name="RJ5/!CE"/>
<pin name="RJ6/!LB"/>
<pin name="RJ7/!UB"/>
<pin name="RJ3/!WRH"/>
<pin name="RJ2/!WRL"/>
<pin name="RJ1/!OE"/>
<pin name="RJ0/ALE"/>
<pin name="RH0/A16"/>
<pin name="RH1/A17"/>
<pin name="RG5"/>
<pin name="RG6"/>
<pin name="RF0/AN5"/>
<pin name="RG7"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSSRX" direction="pwr"/>
<pin name="TPIN-" direction="in"/>
<pin name="TPIN+" direction="in"/>
<pin name="VDDRX" direction="pwr"/>
<pin name="VDDTX" direction="pwr"/>
<pin name="TPOUT-" direction="out"/>
<pin name="TPOUT+" direction="out"/>
<pin name="VSSTX" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RBIAS"/>
</symbol>
<symbol name="PIC18F86-80">
<pin name="RE1/AD9/!WR/P2C"/>
<pin name="RE0/AD8/!RD/P2D"/>
<pin name="RG0/ECCP3/P3A"/>
<pin name="RG1/TX2/CK2"/>
<pin name="RG2/RX2/DT2"/>
<pin name="RG3/CCP4/P3D"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP" direction="pwr"/>
<pin name="RF7/!SS1"/>
<pin name="RF6/AN11"/>
<pin name="RF5/AN10/CVREF"/>
<pin name="RF4/AN9"/>
<pin name="RF3/AN8"/>
<pin name="RF2/AN7/C1OUT"/>
<pin name="RF1/AN6/C2OUT"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/AN1"/>
<pin name="RA0/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RA5/AN4"/>
<pin name="RA4/T0CK"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1"/>
<pin name="RB7/KBI2/PGD"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="OSC2/CLKO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1"/>
<pin name="RB4/KBI0"/>
<pin name="RB3/INT3/ACCP2/P2A"/>
<pin name="RB2/INT2"/>
<pin name="VSSRX"/>
<pin name="TPIN-"/>
<pin name="TPOUT+"/>
<pin name="VSSTX"/>
<pin name="RBIAS"/>
<pin name="VDDPLL"/>
<pin name="VSSPLL"/>
<pin name="RD2"/>
<pin name="RD1"/>
<pin name="RD0/AD0/PSP0"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RE7/AD15/ECCP2/P2A"/>
<pin name="RE6/AD14/P1B"/>
<pin name="RE5/AD13/P1C"/>
<pin name="RE4/AD12/P3B"/>
<pin name="RE3/AD11/P3C"/>
<pin name="RE2/!AD10CS/P2B"/>
<pin name="RH2"/>
<pin name="RH3"/>
<pin name="RH7/AN15/P1B"/>
<pin name="RH6/AN14/P1C"/>
<pin name="RH5/AN13/P3B"/>
<pin name="RH4/AN12/P3C"/>
<pin name="RJ4/BA0"/>
<pin name="RJ5/!CE"/>
<pin name="RB1/INT1"/>
<pin name="RB0/INT0/FLT0"/>
<pin name="TPIN+"/>
<pin name="VDDRX"/>
<pin name="VDDTX"/>
<pin name="TPOUT-"/>
<pin name="RH0/A16"/>
<pin name="RH1/A17"/>
</symbol>
<symbol name="PIC12F675">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GP5/CLKIN"/>
<pin name="GP0/AN0"/>
<pin name="GP4/AN3"/>
<pin name="GP2/AN2"/>
<pin name="VREF/GP1/AN1"/>
<pin name="GP3/!MCLR" direction="in"/>
</symbol>
<symbol name="PIC24FJ128GA010">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="PMD5/RE5"/>
<pin name="PMD6/RE6"/>
<pin name="PMD7/RE7"/>
<pin name="T2CK/RC1"/>
<pin name="T3CK/RC2"/>
<pin name="T4CK/RC3"/>
<pin name="T5CK/RC4"/>
<pin name="PMA5/SCK2/CN8/RG6"/>
<pin name="PMA4/SDI2/CN9/RG7"/>
<pin name="PMA3/SDO2/CN10/RG8"/>
<pin name="!MCLR"/>
<pin name="PMA2/!SS2/CN11/RG9"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS/RA0"/>
<pin name="INT1/RE8"/>
<pin name="INT2/RE9"/>
<pin name="C1IN+/AN5/CN7/RB5"/>
<pin name="C1IN-/AN4/CN6/RB4"/>
<pin name="C2IN+/AN3/CN5/RB3"/>
<pin name="C2IN-/AN2/SS1/CN4/RB2"/>
<pin name="PGC1/EMUC1/AN1/CN3/RB1"/>
<pin name="PGD1/EMUD1/AN0/CN2/RB0"/>
<pin name="PGC2/EMUC2/AN6/OCFA/RB6"/>
<pin name="PGD2/EMUD2/AN7/RB7"/>
<pin name="PMA7/VREF-/RA9"/>
<pin name="PMA6/VREF+/RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="C1OUT/AN8/RB8"/>
<pin name="C2OUT/AN9/RB9"/>
<pin name="PMA13/CVREF/AN10/RB10"/>
<pin name="PMA12/AN11/RB11"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK/RA1"/>
<pin name="!U2RTS/BCLK2/RF13"/>
<pin name="!U2CTS/RF12"/>
<pin name="PMA11/AN12/RB12"/>
<pin name="PMA10/AN13/RB13"/>
<pin name="PMA1/AN14/RB14"/>
<pin name="PMA0/AN15/OCFB/CN12/RB15"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="!U1CTS/CN20/RD14"/>
<pin name="!U1RTS/BCLK1/CN21/RD15"/>
<pin name="PMA9/U2RX/CN17/RF4"/>
<pin name="PMA8/U2TX/CN18/RF5"/>
<pin name="U1TX/RF3"/>
<pin name="U1RX/RF2"/>
<pin name="SDO1/RF8"/>
<pin name="SDI1/RF7"/>
<pin name="SCK1/INT0/RF6"/>
<pin name="SDA1/RG3"/>
<pin name="SCL1/RG2"/>
<pin name="SCL2/RA2"/>
<pin name="SDA2/RA3"/>
<pin name="TDI/RA4"/>
<pin name="TDO/RA5"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="OSC1/CLKI/RC12"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="INT3/RA14"/>
<pin name="INT4/RA15"/>
<pin name="IC1/RTCC/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/PMCS2/RD10"/>
<pin name="IC4/PMCS1/RD11"/>
<pin name="OC1/RD0"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="PMBE/OC4/RD3"/>
<pin name="IC5/RD12"/>
<pin name="CN19/RD13"/>
<pin name="PMWR/OC5/CN13/RD4"/>
<pin name="PMRD/CN14/RD5"/>
<pin name="CN15/RD6"/>
<pin name="CN16/RD7"/>
<pin name="VCAP/VDDCORE"/>
<pin name="ENVREG"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="PMD0/RE0"/>
<pin name="PMD1/RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="PMD2/RE2"/>
<pin name="PMD3/RE3"/>
<pin name="PMD4/RE4"/>
</symbol>
<symbol name="PIC24FJ128GA008">
<pin name="PMD5/RE5"/>
<pin name="PMD6/RE6"/>
<pin name="PMD7/RE7"/>
<pin name="T2CK/RC1"/>
<pin name="T4CK/RC3"/>
<pin name="PMA5/SCK2/CN8/RG6"/>
<pin name="PMA4/SDI2/CN9/RG7"/>
<pin name="PMA3/SDO2/CN10/RG8"/>
<pin name="!MCLR"/>
<pin name="PMA2/!SS2/CN11/RG9"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS/INT1/RE8"/>
<pin name="C1IN+/AN5/CN7/RB5"/>
<pin name="C1IN-/AN4/CN6/RB4"/>
<pin name="C2IN+/AN3/CN5/RB3"/>
<pin name="C2IN-/AN2/SS1/CN4/RB2"/>
<pin name="PGC1/EMUC1/AN1/CN3/RB1"/>
<pin name="PGD1/EMUD1/AN0/CN2/RB0"/>
<pin name="PGC2/EMUC2/AN6/OCFA/RB6"/>
<pin name="PGD2/EMUD2/AN7/RB7"/>
<pin name="PMA7/VREF-/RA9"/>
<pin name="PMA6/VREF+/RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="!U2CTS/C1OUT/AN8/RB8"/>
<pin name="C2OUT/AN9/RB9"/>
<pin name="PMA13/CVREF/AN10/RB10"/>
<pin name="PMA12/AN11/RB11"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK/PMA11/AN12/RB12"/>
<pin name="TDI/PMA10/AN13/RB13"/>
<pin name="PMA1/!U2RTS/BCLK2/AN14/RB14"/>
<pin name="PMA0/AN15/OCFB/CN12/RB15"/>
<pin name="!U1CTS/CN20/RD14"/>
<pin name="!U1RTS/BCLK1/CN21/RD15"/>
<pin name="PMA9/U2RX/CN17/RF4"/>
<pin name="PMA8/U2TX/CN18/RF5"/>
<pin name="U1TX/RF3"/>
<pin name="U1RX/RF2"/>
<pin name="SDO1/RF8"/>
<pin name="SDI1/RF7"/>
<pin name="SCK1/INT0/RF6"/>
<pin name="SDA1/RG3"/>
<pin name="SCL1/RG2"/>
<pin name="SCL2/INT3/RA14"/>
<pin name="SDA2/INT4/RA15"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="OSC1/CLKI/RC12"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="IC1/RTCC/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/PMCS2/RD10"/>
<pin name="IC4/PMCS1/RD11"/>
<pin name="OC1/RD0"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="PMBE/OC4/RD3"/>
<pin name="IC5/RD12"/>
<pin name="CN19/RD13"/>
<pin name="PMWR/OC5/CN13/RD4"/>
<pin name="PMRD/CN14/RD5"/>
<pin name="CN15/RD6"/>
<pin name="CN16/RD7"/>
<pin name="VCAP/VDDCORE"/>
<pin name="ENVREG"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="PMD0/RE0"/>
<pin name="PMD1/RE1"/>
<pin name="PMD2/RE2"/>
<pin name="PMD3/RE3"/>
<pin name="PMD4/RE4"/>
<pin name="TDO/INT2/RE9"/>
</symbol>
<symbol name="PIC24FJ128GA006">
<pin name="PMD5/RE5"/>
<pin name="PMD6/RE6"/>
<pin name="PMD7/RE7"/>
<pin name="PMA5/SCK2/CN8/RG6"/>
<pin name="PMA4/SDI2/CN9/RG7"/>
<pin name="PMA3/SDO2/CN10/RG8"/>
<pin name="!MCLR"/>
<pin name="PMA2/!SS2/CN11/RG9"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="C1IN+/AN5/CN7/RB5"/>
<pin name="C1IN-/AN4/CN6/RB4"/>
<pin name="C2IN+/AN3/CN5/RB3"/>
<pin name="C2IN-/AN2/SS1/CN4/RB2"/>
<pin name="PGC1/EMUC1/AN1/CN3/RB1"/>
<pin name="PGD1/EMUD1/AN0/CN2/RB0"/>
<pin name="PGC2/EMUC2/AN6/OCFA/RB6"/>
<pin name="PGD2/EMUD2/AN7/RB7"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="!U2CTS/C1OUT/AN8/RB8"/>
<pin name="PMA7/C2OUT/AN9/RB9"/>
<pin name="TMS/PMA13/CVREF/AN10/RB10"/>
<pin name="TDO/PMA12/AN11/RB11"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK/PMA11/AN12/RB12"/>
<pin name="TDI/PMA10/AN13/RB13"/>
<pin name="PMA1/!U2RTS/BCLK2/AN14/RB14"/>
<pin name="PMA0/AN15/OCFB/CN12/RB15"/>
<pin name="PMA9/U2RX/SDA2/CN17/RF4"/>
<pin name="PMA8/U2TX/SCL2/CN18/RF5"/>
<pin name="U1TX/RF3"/>
<pin name="U1RX/RF2"/>
<pin name="!U1RTS/BCLK1/SCK1/INT0/RF6"/>
<pin name="SDA1/RG3"/>
<pin name="SCL1/RG2"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="OSC1/CLKI/RC12"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="IC1/RTCC/INT1/RD8"/>
<pin name="IC2/!U1CTS/INT2/RD9"/>
<pin name="IC3/PMCS2/INT3/RD10"/>
<pin name="IC4/PMCS1/INT4/RD11"/>
<pin name="OC1/RD0"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="PMBE/OC4/RD3"/>
<pin name="PMWR/OC5/CN13/RD4"/>
<pin name="PMRD/CN14/RD5"/>
<pin name="CN15/RD6"/>
<pin name="CN16/RD7"/>
<pin name="VCAP/VDDCORE"/>
<pin name="ENVREG"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="PMD0/RE0"/>
<pin name="PMD1/RE1"/>
<pin name="PMD2/RE2"/>
<pin name="PMD3/RE3"/>
<pin name="PMD4/RE4"/>
</symbol>
<symbol name="PIC16F676">
<pin name="VDD" direction="pwr"/>
<pin name="OSC1/CLKIN/T1CKI/RA5"/>
<pin name="T1G/OSC2/CLKOUT/AN3/RA4"/>
<pin name="VPP/MCLR/RA3" direction="in"/>
<pin name="RC5"/>
<pin name="RC4"/>
<pin name="RC3/AN7"/>
<pin name="RC2/AN6"/>
<pin name="RC1/AN5"/>
<pin name="RC0/AN4"/>
<pin name="COUT/T0CKI/INT/AN2/RA2"/>
<pin name="CIN-/VREF/ICSPCLK/AN1/RA1"/>
<pin name="CIN+/ICSPDAT/AN0/RA0"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PIC18F452-44">
<pin name="RC7/RX/DT"/>
<pin name="RD4/PSP4"/>
<pin name="RD5/PSP5"/>
<pin name="RD6/PSP6"/>
<pin name="RD7/PSP7"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RB0/INT0"/>
<pin name="RB1/INT1"/>
<pin name="RB2/INT2"/>
<pin name="RB3/CCP2"/>
<pin name="NC" direction="nc"/>
<pin name="RB4"/>
<pin name="RB5/PGM"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="!MCLR!/VPP" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4/!SS!/LVDIN"/>
<pin name="RE0/AN5/!RD"/>
<pin name="RE1/AN6/!WR"/>
<pin name="RE2/AN7/!CS"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RA6/OSC2/CLKO" direction="out"/>
<pin name="RC0/T1OSO/T1CKI"/>
<pin name="RC1/T1OSI/ICCP2"/>
<pin name="RC2/CCP1"/>
<pin name="RD0/PSP0"/>
<pin name="RD1/PSP1"/>
<pin name="RD2/PSP2"/>
<pin name="RD3/PSP3"/>
<pin name="RC4/SDI/SDA"/>
<pin name="RC5/SDO"/>
<pin name="RC6/TX/CK"/>
<pin name="RC3/SCK/SCL"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
</symbol>
<symbol name="MCP1525">
<pin name="VIN" direction="in"/>
<pin name="VO" direction="out"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="PIC18F6XJ5X">
<pin name="RE1/PMWR/P2C"/>
<pin name="RE0/PMRD/P2D"/>
<pin name="RG0/PMA8/ECCP3/P3A"/>
<pin name="RG1/PMA7/TX2/CK2"/>
<pin name="RG2/PMA6/RX2/DT2"/>
<pin name="RG3/PMCS1/CCP4/P3D"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/PMCS2/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP"/>
<pin name="RF7/!SS1!/C1OUT"/>
<pin name="RF6/AN11/C1INA"/>
<pin name="RF5/AN10/C1INB/CVREF"/>
<pin name="RF4/D+"/>
<pin name="RF3/DRF2/"/>
<pin name="PMA5/AN7/C2INB"/>
<pin name="VUSB"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/AN1"/>
<pin name="RA0/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA5/AN4/C2INA"/>
<pin name="RA4/T0CKI"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1/C2OUT"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="OSC1/CLKI/RA7"/>
<pin name="OSC2/CLKO/RA6"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1/PMA0"/>
<pin name="RB4/KBI0/PMA1"/>
<pin name="RB3/INT3/PMA2"/>
<pin name="RB2/INT2/PMA3"/>
<pin name="RB1/INT1/PMA4"/>
<pin name="RB0/FLT0/INT0"/>
<pin name="RD7/PMD7/!SS2"/>
<pin name="RD6/PMD6/SCK2/SCL2"/>
<pin name="RD5/PMD5/SDI2/SDA2"/>
<pin name="RD4/PMD4/SDO2"/>
<pin name="RD3/PMD3"/>
<pin name="RD2/PMD2"/>
<pin name="RD1/PMD1"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RD0/PMD0"/>
<pin name="RE7/PMA9/ECCP2/P2A"/>
<pin name="RE6/PMA10/P1B"/>
<pin name="RE5/PMA11/P1C"/>
<pin name="RE4/PMA12/P3B"/>
<pin name="RE3/PMA13/P3C/REFO"/>
<pin name="RE2/PMBE/P2B"/>
</symbol>
<symbol name="PIC18F8XJ5X">
<pin name="RH2/A18/PMD7"/>
<pin name="RH3/A19/PMD6"/>
<pin name="RE1/AD9/PMWR/P2C"/>
<pin name="RE0/AD8/PMRD/P2D"/>
<pin name="RG0/PMA8/ECCP3/P3A"/>
<pin name="RG1/PMA7/TX2/CK2"/>
<pin name="RG2/PMA6/RX2/DT2"/>
<pin name="RG3/PMCS1/CCP4/P3D"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/PMCS2/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP"/>
<pin name="RF7/PMD0/!SS1!/C1OUT"/>
<pin name="RF6/PMD1/AN11/C1INA"/>
<pin name="RF5/PMD2/AN10/C1INB/CVREF"/>
<pin name="RF4/D+"/>
<pin name="RF3/D-"/>
<pin name="RF2/PMA5/AN7/C2INB"/>
<pin name="RH7/PMWR/AN15/P1B"/>
<pin name="RH6/PMRD/AN14/P1C/C1INC"/>
<pin name="RH5/PMBE/AN13/P3B/C2IND"/>
<pin name="RH4/PMD3/AN12/P3C/C2INC"/>
<pin name="VUSB" direction="in"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/AN1"/>
<pin name="RA0/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA5/PMD4/AN4/C2INA"/>
<pin name="RA4/PMD5/T0CKI"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RJ4/BA0"/>
<pin name="RJ5/!CE"/>
<pin name="RJ6/!LB"/>
<pin name="RJ7/!UB"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1/C2OUT"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="OSC1/CLKI/RA7"/>
<pin name="OSC2/CLKO/RA6"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1/PMA0"/>
<pin name="RB4/KBI0/PMA1"/>
<pin name="RB3/INT3/ECCP2/P2A/PMA2"/>
<pin name="RB2/INT2/PMA3"/>
<pin name="RB1/INT1/PMA4"/>
<pin name="RB0/FLT0/INT0"/>
<pin name="RJ3/!WRH"/>
<pin name="RJ2/!WRL"/>
<pin name="RJ1/!OE"/>
<pin name="RJ0/ALE"/>
<pin name="RD7/AD7/PMD7/!SS2"/>
<pin name="RD6/AD6/PMD6/SCK2/SCL2"/>
<pin name="RD5/AD5/PMD5/SDI2/SDA2"/>
<pin name="RD4/AD4/PMD4/SDO2"/>
<pin name="RD3/AD3/PMD3"/>
<pin name="RD2/AD2/PMD2"/>
<pin name="RD1/AD1/PMD1"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RD0/AD0/PMD0"/>
<pin name="RE7/AD15/PMA9/ECCP2/P2A"/>
<pin name="RE6/AD14/PMA10/P1B"/>
<pin name="RE5/AD13/PMA11/P1C"/>
<pin name="RE4/AD12/PMA12/P3B"/>
<pin name="RE3/AD11/PMA13/P3C/REFO"/>
<pin name="RE2/AD10/PMBE/P2B"/>
<pin name="RH0/A16"/>
<pin name="RH1/A17"/>
</symbol>
<symbol name="PIC18F6XJ6X">
<pin name="RE1/P2C"/>
<pin name="RE0/P2D"/>
<pin name="RB0/INT0/FLT0"/>
<pin name="RB1/INT1"/>
<pin name="RB2/INT2"/>
<pin name="RB3/INT3"/>
<pin name="!MCLR"/>
<pin name="RG4/CCP5/P1D"/>
<pin name="VSS"/>
<pin name="VDDCORE/VCAP"/>
<pin name="RF7/!SS1"/>
<pin name="RF6/AN11"/>
<pin name="RF5/AN10/CVREF"/>
<pin name="RF4/AN9"/>
<pin name="RF3/AN8"/>
<pin name="RF2/AN7/C1OUT"/>
<pin name="RF1/AN6/C2OUT"/>
<pin name="ENVREG"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/LEDB/AN1"/>
<pin name="RA0/LEDA/AN0"/>
<pin name="VSS@1"/>
<pin name="VDD"/>
<pin name="RA5/AN4"/>
<pin name="RA4/T0CKI"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="VDD@1"/>
<pin name="OSC1/CLKI"/>
<pin name="OSC2/CLKO"/>
<pin name="VSS@2"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1"/>
<pin name="RB4/KBI0"/>
<pin name="VSSRX"/>
<pin name="TPIN-"/>
<pin name="TPIN+"/>
<pin name="VDDRX"/>
<pin name="VDDTX"/>
<pin name="TPOUT-"/>
<pin name="TPOUT+"/>
<pin name="VSSTX"/>
<pin name="RBIAS"/>
<pin name="VDDPLL"/>
<pin name="VSSPLL"/>
<pin name="VSS@3"/>
<pin name="VDD@2"/>
<pin name="RD2/CCP4/P3D"/>
<pin name="RD1/ECCP3/P3A"/>
<pin name="RD0/P1B"/>
<pin name="RE5/P1C"/>
<pin name="RE4/P3B"/>
<pin name="RE3/P3C"/>
<pin name="RE2/P2B"/>
</symbol>
<symbol name="PIC18F8XJ6X">
<pin name="RH2"/>
<pin name="RH3"/>
<pin name="RE1/P2C"/>
<pin name="RE0/P2D"/>
<pin name="RB0/INT0/FLT0"/>
<pin name="RB1/INT1"/>
<pin name="RB2/INT2"/>
<pin name="RB3/INT3"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP" direction="in"/>
<pin name="RF7/!SS1"/>
<pin name="RF6/AN11"/>
<pin name="RF5/AN10/CVREF"/>
<pin name="RF4/AN9"/>
<pin name="RF3/AN8"/>
<pin name="RF2/AN7/C1OUT"/>
<pin name="RH7/AN15/P1B"/>
<pin name="RH6/AN14/P1C"/>
<pin name="RH5/AN13/P3B"/>
<pin name="RH4/AN12/P3C"/>
<pin name="RF1/AN6/C2OUT"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="AVSS" direction="in"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/LEDB/AN1"/>
<pin name="RA0/LEDA/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA5/AN4"/>
<pin name="RA4/T0CKI"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RJ5"/>
<pin name="RJ4"/>
<pin name="RG3/CCP4/P3D"/>
<pin name="RG2/RX2/DT2"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="OSC2/CLKO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1"/>
<pin name="RB4/KBI0"/>
<pin name="RG1/TX2/CK2"/>
<pin name="RG0/ECCP3/P3A"/>
<pin name="VSSRX" direction="in"/>
<pin name="TPIN-" direction="in"/>
<pin name="TPIN+" direction="in"/>
<pin name="VDDRX" direction="in"/>
<pin name="VDDTX" direction="in"/>
<pin name="TPOUT-" direction="out"/>
<pin name="TPOUT+" direction="out"/>
<pin name="VSSTX" direction="in"/>
<pin name="RBIAS" direction="in"/>
<pin name="VDDPLL" direction="in"/>
<pin name="VSSPLL" direction="in"/>
<pin name="RD2"/>
<pin name="RD1"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RD0"/>
<pin name="RE7/ECCP2/P2A"/>
<pin name="RE6/P1B"/>
<pin name="RE5/P1C"/>
<pin name="RE4/P3B"/>
<pin name="RE3/P3C"/>
<pin name="RE2/P2B"/>
<pin name="RH0"/>
<pin name="RH1"/>
</symbol>
<symbol name="PIC18F9XJ6">
<pin name="RH2/A18"/>
<pin name="RH3/A19"/>
<pin name="RE1/AD9/!WR!/P2C"/>
<pin name="RE0/AD8/!RD!/P2D/T"/>
<pin name="RB0/INT0/FLT0"/>
<pin name="RB1/INT1"/>
<pin name="RB2/INT2"/>
<pin name="RB3/INT3/ECCP2/P2A"/>
<pin name="NC" direction="nc"/>
<pin name="RG6"/>
<pin name="RG5"/>
<pin name="RF0/AN5"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP3"/>
<pin name="VDD" direction="pwr"/>
<pin name="RF7/!SS1"/>
<pin name="RF6/AN11"/>
<pin name="RF5/AN10/CVREF"/>
<pin name="RF4/AN9"/>
<pin name="RF3/AN8"/>
<pin name="RF2/AN7/C1OUT"/>
<pin name="RH7/AN15/P1B"/>
<pin name="RH6/AN14/P1C"/>
<pin name="RH5/AN13/P3B"/>
<pin name="RH4/AN12/P3C"/>
<pin name="RF1/AN6/C2OUT"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="AVSS" direction="in"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/LEDB/AN1"/>
<pin name="RA0/LEDA/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RG7"/>
<pin name="RJ7/!UB"/>
<pin name="VSS@2"/>
<pin name="RA5/AN4"/>
<pin name="RA4/T0CKI"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RJ4/BA0"/>
<pin name="RJ5/!CE"/>
<pin name="RJ0/ALE"/>
<pin name="RJ1/!OE"/>
<pin name="RG3/CCP4/P3D"/>
<pin name="RG2/RX2/DT2"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="RJ6/!LB"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="RJ3/!WRH"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="OSC2/CLKO" direction="out"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="RJ2/!WRL"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1"/>
<pin name="RB4/KBI0"/>
<pin name="RG1/TX2/CK2"/>
<pin name="RG0/ECCP3/P3A"/>
<pin name="VSSRX" direction="in"/>
<pin name="TPIN-" direction="in"/>
<pin name="TPIN+" direction="in"/>
<pin name="VDDRX" direction="in"/>
<pin name="VDDTX" direction="in"/>
<pin name="TPOUT-"/>
<pin name="TPOUT+"/>
<pin name="VSSTX" direction="in"/>
<pin name="RBIAS" direction="in"/>
<pin name="VDDPLL" direction="in"/>
<pin name="VSSPLL" direction="in"/>
<pin name="D7/AD7/PSP7/!SS2"/>
<pin name="RD6/AD6/PSP6/SCK2/SCL2"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD5/AD5/PSP5/SDI2/SDA2"/>
<pin name="RD4/AD4/PSP4/SDO2/SD"/>
<pin name="RD3/AD3/PSP3"/>
<pin name="RD2/AD2/PSP2"/>
<pin name="RD1/AD1/PSP1"/>
<pin name="RD0/AD0/PSP0"/>
<pin name="RE7/AD15/ECCP2/P2A"/>
<pin name="RE6/AD14/P1B"/>
<pin name="RE5/AD13/P1C"/>
<pin name="RE4/AD12/P3B"/>
<pin name="RE3/AD11/P3C"/>
<pin name="RE2/AD10/!CS!/P2B"/>
<pin name="RH0/A16"/>
<pin name="RH1/A17"/>
</symbol>
<symbol name="PIC12F683">
<pin name="VDD" direction="pwr"/>
<pin name="GP5/T1CKI/OSC1/CLKIN"/>
<pin name="GP4/AN3/T1G/OSC2/CLKOUT"/>
<pin name="GP3/!MCLR!/VPP"/>
<pin name="GP2/AN2/T0CKI/INT/COUT/CCP1"/>
<pin name="GP1/AN1/CIN-/VREF/ICSPCLK"/>
<pin name="GP0/AN0/CIN+/ICSPDAT/ULPWU"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MCP3550">
<pin name="VREF" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="!CS" direction="in"/>
<pin name="SDO/!RDY" direction="out"/>
<pin name="SCK" direction="in"/>
</symbol>
<symbol name="ENC28J60">
<pin name="VCAP" direction="in"/>
<pin name="VSS" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="!INT" direction="out"/>
<pin name="NC*" direction="out"/>
<pin name="SO" direction="out"/>
<pin name="SI" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VSSRX" direction="in"/>
<pin name="TPIN+" direction="in"/>
<pin name="TPIN-" direction="in"/>
<pin name="RBIAS" direction="in"/>
<pin name="VDDTX" direction="in"/>
<pin name="TPOUT-" direction="out"/>
<pin name="TPOUT+" direction="out"/>
<pin name="VSSTX" direction="in"/>
<pin name="VDDRX" direction="in"/>
<pin name="VDDPLL" direction="in"/>
<pin name="VSSPLL" direction="in"/>
<pin name="VSSOSC" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="VDDOSC" direction="in"/>
<pin name="LEDB" direction="out"/>
<pin name="LEDA" direction="out"/>
<pin name="VDD" direction="in"/>
</symbol>
<symbol name="MCP3202">
<pin name="!CS!/SHDN" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="VSS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VDD/VREF" direction="in"/>
</symbol>
<symbol name="PIC24FJ256GB110">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="VBUS" direction="pas"/>
<pin name="VUSB" direction="pas"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="ENVREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX320F064H">
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX320F128L">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="RF7"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX360F512L">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="RF7"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX440F256H">
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="VBUS"/>
<pin name="VUSB" direction="pas"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX460F512L">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="VBUS"/>
<pin name="VUSB" direction="pas"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX460F256L">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="VBUS"/>
<pin name="VUSB" direction="pas"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX320F032H">
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX420F032H">
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="VBUS"/>
<pin name="VUSB" direction="pas"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX360F256L">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="RF7"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC24FJ64GA002">
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
</symbol>
<symbol name="PIC24FJ64GA002_QFN">
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="PIC24FJ48GA002">
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
</symbol>
<symbol name="PIC24FJ48GA002_QFN">
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="PIC24FJ32GA002">
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
</symbol>
<symbol name="PIC24FJ32GA002_QFN">
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="PIC24FJ16GA002">
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
</symbol>
<symbol name="PIC24FJ16GA002_QFN">
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="PIC24FJ256GB108">
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC3"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR"/>
<pin name="RG9"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="VBUS" direction="pas"/>
<pin name="VUSB" direction="pas"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="ENVREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC24FJ64GB110">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="VBUS" direction="pas"/>
<pin name="VUSB" direction="pas"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="ENVREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC32MX440F128L">
<pin name="RG15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG9"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="VBUS"/>
<pin name="VUSB" direction="pas"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC24FJ64GA004">
<pin name="RB9"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="RC8"/>
<pin name="RC9"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDO" direction="out"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="TDI" direction="in"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RB8"/>
</symbol>
<symbol name="PIC24FJ48GA004">
<pin name="RB9"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="RC8"/>
<pin name="RC9"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDO" direction="out"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="TDI" direction="in"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RB8"/>
</symbol>
<symbol name="PIC24HJ64GP506">
<pin name="RG15"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR"/>
<pin name="RG9"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
</symbol>
<symbol name="PIC24FJ32GA004">
<pin name="RB9"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="RC8"/>
<pin name="RC9"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDO" direction="out"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="TDI" direction="in"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RB8"/>
</symbol>
<symbol name="PIC24FJ256GB106">
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="!MCLR"/>
<pin name="RG9"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="VBUS" direction="pas"/>
<pin name="VUSB" direction="pas"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="ENVREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC24HJ12GP202">
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="DSPIC33FJ12MC202">
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="DSPIC33FJ12GP202">
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD1" direction="pwr"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
</symbol>
<symbol name="DSPIC33FJ128GP710">
<pin name="RG15"/>
<pin name="VDD1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="MCLR"/>
<pin name="RG9"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS3" direction="pwr"/>
<pin name="VDD3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS4" direction="pwr"/>
<pin name="VDD4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="RF7"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="DSPIC33FJ256MC510">
<pin name="RG15"/>
<pin name="VDD1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="MCLR"/>
<pin name="RG9"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS3" direction="pwr"/>
<pin name="VDD3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS4" direction="pwr"/>
<pin name="VDD4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="RF7"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="MRF24J40">
<pin name="VDD" direction="pwr"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO0" direction="in"/>
<pin name="GPIO1" direction="in"/>
<pin name="GPIO5" direction="in"/>
<pin name="GPIO4" direction="in"/>
<pin name="GPIO2" direction="in"/>
<pin name="GPIO3" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="WAKE" direction="in"/>
<pin name="INT" direction="out"/>
<pin name="SOUT" direction="in"/>
<pin name="SIN" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="CLKOUT" direction="in"/>
<pin name="LPOSC2" direction="in"/>
<pin name="LPOSC1" direction="in"/>
<pin name="RXIP" direction="out"/>
<pin name="RXQP" direction="out"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="OSC2" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="LCAP" direction="nc"/>
</symbol>
<symbol name="PIC16F62*">
<pin name="RA2/AN2/VREF"/>
<pin name="RA3/AN3/CMP1"/>
<pin name="RA4/TOCKI/CMP2"/>
<pin name="RA5/MCLR/VPP"/>
<pin name="VSS" direction="pwr"/>
<pin name="RB0/INT"/>
<pin name="RB1/RX/DT"/>
<pin name="RB2/TX/CK"/>
<pin name="RB3/CCP1"/>
<pin name="RB4/PGM"/>
<pin name="RB5"/>
<pin name="RB6/T1OSO/T1CKI/PGC"/>
<pin name="RB7/T1OSI/PGD"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA6/OSC2/CLKOUT"/>
<pin name="RA7/OSC1/CLKIN"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
</symbol>
<symbol name="PIC16F62-SSOP">
<pin name="RA2/AN2/VREF"/>
<pin name="RA3/AN3/CMP1"/>
<pin name="RA4/TOCKI/CMP2"/>
<pin name="RA5/MCLR/VPP"/>
<pin name="VSS" direction="pwr"/>
<pin name="RB0/INT"/>
<pin name="RB1/RX/DT"/>
<pin name="RB2/TX/CK"/>
<pin name="RB3/CCP1"/>
<pin name="RB4/PGM"/>
<pin name="RB5"/>
<pin name="RB6/T1OSO/T1CKI/PGC"/>
<pin name="RB7/T1OSI/PGD"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA6/OSC2/CLKOUT"/>
<pin name="RA7/OSC1/CLKIN"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="PIC16F688">
<pin name="VDD" direction="pwr"/>
<pin name="RA4/AN3/!T1G!/OSC2/CLKOUT"/>
<pin name="RA3/!MCLR!/VPP"/>
<pin name="RA5/T1CKI/OSC1/CLKIN" direction="in"/>
<pin name="RA0/AN0/C1IN+/ICSPDAT/ULPWU"/>
<pin name="RA1/AN1/C1IN-/VREF/ICSPCLK"/>
<pin name="RA2/AN2/T0CKI/INT/C1OUT"/>
<pin name="RC2/AN6"/>
<pin name="RC1/AN5/C2IN"/>
<pin name="RC0/AN4/C2IN+"/>
<pin name="RC5/RX/DT"/>
<pin name="RC4/C2OUT/TX/CK"/>
<pin name="RC3/AN7"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="EXPOSED">
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="PIC16F193X">
</symbol>
<symbol name="PIC16F1934/7/9">
<pin name="SEG8/DT/RX/RC7"/>
<pin name="SEG17/P2D/CPS12/RD4"/>
<pin name="SEG18/P1B/CPS13/RD5"/>
<pin name="SEG19/P1C/CPS14/RD6"/>
<pin name="SEG20/P1D/CPS15/RD7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SEG0/INT/SRI/CPS0/AN12/RB0"/>
<pin name="VLCD1/CPS1/C12IN3-/AN10/RB1"/>
<pin name="VLCD2/CPS2/AN8/RB2"/>
<pin name="VLCD3/P2A/CCP2/CPS3/C12IN2-/AN9/RB3"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="COM0/CPS4/AN11/RB4"/>
<pin name="COM1/T1G/P3A/CCP3/CPS5/AN13/RB5"/>
<pin name="SEG14/ICDCLK/ICSPCLK/RB6"/>
<pin name="SEG13/ICDDAT/ICSPDAT/RB7"/>
<pin name="VPP/!MCLR!/RE3" direction="in"/>
<pin name="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0"/>
<pin name="SEG7/C12IN1-/AN1/RA1"/>
<pin name="COM2/DACOUT/VREF-/C2IN+/AN2/RA2"/>
<pin name="SEG15/VREF+/C1IN+/AN3/RA3"/>
<pin name="RA4/C1OUT/CPS6/T0CKI/SRQ/SEG4"/>
<pin name="RA5/AN4/C2OUT/CPS7/SRNQ/!SS!/VCAP/SEG5"/>
<pin name="RE0/AN5/CCP3/P3A/SEG21"/>
<pin name="RE1/AN6/P3B/SEG22"/>
<pin name="RE2/AN7/CCP5/SEG23"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA7/OSC1/CLKIN/SEG2"/>
<pin name="RA6/OSC2/CLKOUT/VCAP/SEG1"/>
<pin name="RC0/T1OSO/T1CKI/P2B"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="RC1/T1OSI/CCP2/P2A"/>
<pin name="RC2/CCP1/P1A/SEG3"/>
<pin name="RC3/SCL/SCK/SEG6"/>
<pin name="RD0/CPS8/COM3"/>
<pin name="RD1/CPS9/CCP4"/>
<pin name="RD2/CPS10/P2B"/>
<pin name="RD3/CPS11/P2C/SEG16"/>
<pin name="RC4/SDI/SDA/T1G/SEG11"/>
<pin name="RC5/SDO/SEG10"/>
<pin name="RC6/TX/CK/SEG9"/>
</symbol>
<symbol name="PIC16F1933/1936/1938">
<pin name="VPP/!MCLR!/RE3" direction="in"/>
<pin name="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0"/>
<pin name="SEG7/C12IN1-/AN1/RA1"/>
<pin name="COM2/DACOUT/VREF-/C2IN+/AN2/RA2"/>
<pin name="SEG15/COM3/VREF+/C1IN+/AN3/RA3"/>
<pin name="SEG4/CCP5/SRQ/T0CKI/CPS6/C1OUT/RA4"/>
<pin name="SEG5/VCAP/SS/SRNQ/CPS7/C2OUT/AN4/RA5"/>
<pin name="VSS" direction="pwr"/>
<pin name="SEG2/CLKIN/OSC1/RA7"/>
<pin name="SEG1/VCAP/CLKOUT/OSC2/RA6"/>
<pin name="P2B/T1CKI/T1OSO/RC0"/>
<pin name="P2A/CCP2/T1OSI/RC1"/>
<pin name="SEG3/P1A/CCP1/RC2"/>
<pin name="SEG6/SCL/SCK/RC3"/>
<pin name="RC4/SDI/SDA/T1G/SEG11"/>
<pin name="RC5/SDO/SEG10"/>
<pin name="RC6/TX/CK/CCP3/P3A/SEG9"/>
<pin name="RC7/RX/DT/P3B/SEG8"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/AN12/CPS0/CCP4/SRI/INT/SEG0"/>
<pin name="RB1/AN10/C12IN3-/CPS1/P1C/VLCD1"/>
<pin name="RB2/AN8/CPS2/P1B/VLCD2"/>
<pin name="RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3"/>
<pin name="RB4/AN11/CPS4/P1D/COM0"/>
<pin name="RB5/AN13/CPS5/P2B/CCP3/P3A/T1G/COM1"/>
<pin name="RB6/ICSPCLK/ICDCLK/SEG14"/>
<pin name="RB7/ICSPDAT/ICDDAT/SEG13"/>
</symbol>
<symbol name="PIC16LF1934/7/9">
<pin name="VPP/!MCLR!/RE3" direction="in"/>
<pin name="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0"/>
<pin name="SEG7/C12IN1-/AN1/RA1"/>
<pin name="COM2/DACOUT/VREF-/C2IN+/AN2/RA2"/>
<pin name="SEG15/VREF+/C1IN+/AN3/RA3"/>
<pin name="SEG4/SRQ/T0CKI/CPS6/C1OUT/RA4"/>
<pin name="SEG5/VCAP/!SS!/SRNQ/CPS7/C2OUT/AN4/RA5"/>
<pin name="SEG21/CCP3/P3A/AN5/RE0"/>
<pin name="SEG22/P3B/AN6/RE1"/>
<pin name="SEG23/CCP5/AN7/RE2"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="SEG2/CLKIN/OSC1/RA7"/>
<pin name="SEG1/VCAP/CLKOUT/OSC2/RA6"/>
<pin name="P2B/T1CKI/T1OSO/RC0"/>
<pin name="P2A/CCP2/T1OSI/RC1"/>
<pin name="SEG3/P1A/CCP1/RC2"/>
<pin name="SEG6/SCK/SCL/RC3"/>
<pin name="COM3/CPS8/RD0"/>
<pin name="CCP4/CPS9/RD1"/>
<pin name="RD2/CPS10/P2B"/>
<pin name="RD3/CPS11/P2C/SEG16"/>
<pin name="RC4/SDI/SDA/T1G/SEG11"/>
<pin name="RC5/SDO/SEG10"/>
<pin name="RC6/TX/CK/SEG9"/>
<pin name="RC7/RX/DT/SEG8"/>
<pin name="RD4/CPS12/P2D/SEG17"/>
<pin name="RD5/CPS13/P1B/SEG18"/>
<pin name="RD6/CPS14/P1C/SEG19"/>
<pin name="RD7/CPS15/P1D/SEG20"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB0/AN12/CPS0/SRI/INT/SEG0"/>
<pin name="RB1/AN10/C12IN3-/CPS1/VLCD1"/>
<pin name="RB2/AN8/CPS2/VLCD2"/>
<pin name="RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3"/>
<pin name="RB4/AN11/CPS4/COM0"/>
<pin name="RB5/AN13/CPS5/CCP3/P3A/T1G/COM1"/>
<pin name="RB7/ICSPDAT/ICDDAT/SEG13"/>
<pin name="RB6/ICSPCLK/ICDCLK/SEG14"/>
</symbol>
<symbol name="PIC16F1934/7/9-QFN44">
<pin name="SEG8/DT/RX/RC7"/>
<pin name="SEG17/P2D/CPS12/RD4"/>
<pin name="SEG18/P1B/CPS13/RD5"/>
<pin name="SEG19/P1C/CPS14/RD6"/>
<pin name="SEG20/P1D/CPS15/RD7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SEG0/INT/SRI/CPS0/AN12/RB0"/>
<pin name="VLCD1/CPS1/C12IN3-/AN10/RB1"/>
<pin name="VLCD2/CPS2/AN8/RB2"/>
<pin name="VLCD3/P2A/CCP2/CPS3/C12IN2-/AN9/RB3"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="COM0/CPS4/AN11/RB4"/>
<pin name="COM1/T1G/P3A/CCP3/CPS5/AN13/RB5"/>
<pin name="SEG14/ICDCLK/ICSPCLK/RB6"/>
<pin name="SEG13/ICDDAT/ICSPDAT/RB7"/>
<pin name="VPP/!MCLR!/RE3" direction="in"/>
<pin name="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0"/>
<pin name="SEG7/C12IN1-/AN1/RA1"/>
<pin name="COM2/DACOUT/VREF-/C2IN+/AN2/RA2"/>
<pin name="SEG15/VREF+/C1IN+/AN3/RA3"/>
<pin name="RA4/C1OUT/CPS6/T0CKI/SRQ/SEG4"/>
<pin name="RA5/AN4/C2OUT/CPS7/SRNQ/!SS!/VCAP/SEG5"/>
<pin name="RE0/AN5/CCP3/P3A/SEG21"/>
<pin name="RE1/AN6/P3B/SEG22"/>
<pin name="RE2/AN7/CCP5/SEG23"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA7/OSC1/CLKIN/SEG2"/>
<pin name="RA6/OSC2/CLKOUT/VCAP/SEG1"/>
<pin name="RC0/T1OSO/T1CKI/P2B"/>
<pin name="RC1/T1OSI/CCP2/P2A"/>
<pin name="RC2/CCP1/P1A/SEG3"/>
<pin name="RC3/SCL/SCK/SEG6"/>
<pin name="RD0/CPS8/COM3"/>
<pin name="RD1/CPS9/CCP4"/>
<pin name="RD2/CPS10/P2B"/>
<pin name="RD3/CPS11/P2C/SEG16"/>
<pin name="RC4/SDI/SDA/T1G/SEG11"/>
<pin name="RC5/SDO/SEG10"/>
<pin name="RC6/TX/CK/SEG9"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="PIC18F27J53_28">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1/CLKI/RA7"/>
<pin name="OSC2/CLKO/RA6"/>
<pin name="RA0/AN0/C1INA/ULPWU/RP0"/>
<pin name="RA1/AN1/C2INA/VBG/RP1"/>
<pin name="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF"/>
<pin name="RA3/AN3/C1INB/VREF+"/>
<pin name="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2"/>
<pin name="RB0/AN12/C3IND/INT0/RP3"/>
<pin name="RB1/AN10/C3INC/RTCC/RP4"/>
<pin name="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5"/>
<pin name="RB3/AN9/C3INA/CTED2/VPO/RP6"/>
<pin name="RB4/CCP4/KBI0/SCK1/SCL1/RP7"/>
<pin name="RB5/CCP5/KBI1/SDI1/SDA1/RP8"/>
<pin name="RB6/CCP6/KBI2/PGC/RP9"/>
<pin name="RB7/CCP7/KBI3/PGD/RP10"/>
<pin name="RC0/T1OSO/T1CKI/RP11"/>
<pin name="RC1/CCP8/T1OSI/!UOE!/RP12"/>
<pin name="RC2/AN11/C2IND/CTPLS/RP13"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/CCP9/TX1/CK1/RP17"/>
<pin name="RC7/CCP10/RX1/DT1/SDO1/RP18"/>
<pin name="VSS1" direction="in"/>
<pin name="VSS2" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="VDDCORE/VCAP" direction="in"/>
<pin name="VUSB" direction="in"/>
</symbol>
<symbol name="PIC18F47J53ML">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1/CLKI/RA7"/>
<pin name="OSC2/CLKO/RA6"/>
<pin name="RA0/AN0/C1INA/ULPWU/RP0"/>
<pin name="RA1/AN1/C2INA/VBG/RP1"/>
<pin name="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF"/>
<pin name="RA3/AN3/C1INB/VREF+"/>
<pin name="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2"/>
<pin name="RB0/AN12/C3IND/INT0/RP3"/>
<pin name="RB1/AN10/C3INC/RTCC/RP4"/>
<pin name="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5"/>
<pin name="RB3/AN9/C3INA/CTED2/VPO/RP6"/>
<pin name="RB4/CCP4/KBI0/SCK1/SCL1/RP7"/>
<pin name="RB5/CCP5/KBI1/SDI1/SDA1/RP8"/>
<pin name="RB6/CCP6/KBI2/PGC/RP9"/>
<pin name="RB7/CCP7/KBI3/PGD/RP10"/>
<pin name="RC0/T1OSO/T1CKI/RP11"/>
<pin name="RC1/CCP8/T1OSI/!UOE!/RP12"/>
<pin name="RC2/AN11/C2IND/CTPLS/RP13"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/CCP9/TX1/CK1/RP17"/>
<pin name="RC7/CCP10/RX1/DT1/SDO1/RP18"/>
<pin name="VSS1" direction="in"/>
<pin name="VSS2" direction="in"/>
<pin name="VDD1" direction="in"/>
<pin name="VDDCORE/VCAP" direction="in"/>
<pin name="VUSB" direction="in"/>
<pin name="RD0/PMD0/SCL2"/>
<pin name="RD1/PMD1/SDA2"/>
<pin name="RD2/PMD2/RP19"/>
<pin name="RD3/PMD3/RP20"/>
<pin name="RD4/PMD4/RP21"/>
<pin name="RD5/PMD5/RP22"/>
<pin name="RD6/PMD6/RP23"/>
<pin name="RD7/PMD7/RP24"/>
<pin name="RE0/AN5/PMRD"/>
<pin name="RE1/AN6/PMWR"/>
<pin name="RE2/AN7/PMCS"/>
<pin name="AVSS1" direction="in"/>
<pin name="VDD2" direction="in"/>
<pin name="AVDD1" direction="in"/>
<pin name="AVDD2" direction="in"/>
</symbol>
<symbol name="PIC18F47J53TQ">
<pin name="!MCLR" direction="in"/>
<pin name="OSC1/CLKI/RA7"/>
<pin name="OSC2/CLKO/RA6"/>
<pin name="RA0/AN0/C1INA/ULPWU/RP0"/>
<pin name="RA1/AN1/C2INA/VBG/RP1"/>
<pin name="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF"/>
<pin name="RA3/AN3/C1INB/VREF+"/>
<pin name="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2"/>
<pin name="RB0/AN12/C3IND/INT0/RP3"/>
<pin name="RB1/AN10/C3INC/RTCC/RP4"/>
<pin name="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5"/>
<pin name="RB3/AN9/C3INA/CTED2/VPO/RP6"/>
<pin name="RB4/CCP4/KBI0/SCK1/SCL1/RP7"/>
<pin name="RB5/CCP5/KBI1/SDI1/SDA1/RP8"/>
<pin name="RB6/CCP6/KBI2/PGC/RP9"/>
<pin name="RB7/CCP7/KBI3/PGD/RP10"/>
<pin name="RC0/T1OSO/T1CKI/RP11"/>
<pin name="RC1/CCP8/T1OSI/!UOE!/RP12"/>
<pin name="RC2/AN11/C2IND/CTPLS/RP13"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/CCP9/TX1/CK1/RP17"/>
<pin name="RC7/CCP10/RX1/DT1/SDO1/RP18"/>
<pin name="VSS1" direction="in"/>
<pin name="VSS2" direction="in"/>
<pin name="VDD1" direction="in"/>
<pin name="VDDCORE/VCAP" direction="in"/>
<pin name="VUSB" direction="in"/>
<pin name="RD0/PMD0/SCL2"/>
<pin name="RD1/PMD1/SDA2"/>
<pin name="RD2/PMD2/RP19"/>
<pin name="RD3/PMD3/RP20"/>
<pin name="RD4/PMD4/RP21"/>
<pin name="RD5/PMD5/RP22"/>
<pin name="RD6/PMD6/RP23"/>
<pin name="RD7/PMD7/RP24"/>
<pin name="RE0/AN5/PMRD"/>
<pin name="RE1/AN6/PMWR"/>
<pin name="RE2/AN7/PMCS"/>
<pin name="VDD2" direction="in"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_TQFP">
<pin name="RG15"/>
<pin name="VDD1" direction="pwr"/>
<pin name="RE5"/>
<pin name="RE6"/>
<pin name="RE7"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RG6"/>
<pin name="RG7"/>
<pin name="RG8"/>
<pin name="MCLR"/>
<pin name="RG9"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="RE8"/>
<pin name="RE9"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RB3"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RB0"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA9"/>
<pin name="RA10"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="RB10"/>
<pin name="RB11"/>
<pin name="VSS3" direction="pwr"/>
<pin name="VDD3" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="RF13"/>
<pin name="RF12"/>
<pin name="RB12"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS4" direction="pwr"/>
<pin name="VDD4" direction="pwr"/>
<pin name="RD14"/>
<pin name="RD15"/>
<pin name="RF4"/>
<pin name="RF5"/>
<pin name="RF3"/>
<pin name="RF2"/>
<pin name="RF8"/>
<pin name="RF7"/>
<pin name="RF6"/>
<pin name="RG3"/>
<pin name="RG2"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD5" direction="pwr"/>
<pin name="RC12"/>
<pin name="RC15"/>
<pin name="VSS5" direction="pwr"/>
<pin name="RA14"/>
<pin name="RA15"/>
<pin name="RD8"/>
<pin name="RD9"/>
<pin name="RD10"/>
<pin name="RD11"/>
<pin name="RD0"/>
<pin name="RC13"/>
<pin name="RC14"/>
<pin name="VSS1" direction="pwr"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RD12"/>
<pin name="RD13"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VREG" direction="pas"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RG1"/>
<pin name="RG0"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RE0"/>
<pin name="RE1"/>
<pin name="RG14"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
</symbol>
<symbol name="PIC16LF1826">
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RA0"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="RA5/!MCLR!/VPP"/>
</symbol>
<symbol name="PIC16F1516">
<pin name="VPP/!MCLR!/RE3"/>
<pin name="!SS!/AN0/RA0"/>
<pin name="AN1/RA1"/>
<pin name="AN2/RA2"/>
<pin name="VREF+/AN3/RA3"/>
<pin name="T0CKI/RA4"/>
<pin name="VCAP/!SS!/AN4/RA5"/>
<pin name="CLKIN/OSC1/RA7"/>
<pin name="CLKOUT/OSC2/RA6"/>
<pin name="T1CKI/SOSCO/RC0"/>
<pin name="CCP2/SOSCI/RC1"/>
<pin name="CCP1/AN14/RC2"/>
<pin name="SCL/SCK/AN15/RC3"/>
<pin name="RC4/AN16/SDI/SDA"/>
<pin name="RC5/AN17/SDO"/>
<pin name="RC6/AN18/TX/CK"/>
<pin name="RC7/AN19/RX/DT"/>
<pin name="RB0/AN12/INT"/>
<pin name="RB1/AN10"/>
<pin name="RB2/AN8"/>
<pin name="RB3/AN9/CCP2"/>
<pin name="RB4/AN11"/>
<pin name="RB5/AN13/T1G"/>
<pin name="RB6/ICSPCLK/ICDCLK"/>
<pin name="RB7/ICSPDAT/ICDDAT"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PIC16F1517/19">
<pin name="DT/RX/AN19/RC7"/>
<pin name="AN24/RD4"/>
<pin name="AN25/RD5"/>
<pin name="AN26/RD6"/>
<pin name="AN27/RD7"/>
<pin name="INT/AN12/RB0"/>
<pin name="AN10/RB1"/>
<pin name="AN8/RB2"/>
<pin name="CCP2/AN9/RB3"/>
<pin name="AN11/RB4"/>
<pin name="T1G/AN13/RB5"/>
<pin name="ICDCLK/ICSPCLK/RB6"/>
<pin name="ICDDAT/ICSPDAT/RB7"/>
<pin name="VPP/!MCLR!/RE3" direction="in"/>
<pin name="!SS!/AN0/RA0"/>
<pin name="AN1/RA1"/>
<pin name="AN2/RA2"/>
<pin name="VREF+/AN3/RA3"/>
<pin name="RA4/TOCKI"/>
<pin name="RA5/AN4/!SS!/VCAP"/>
<pin name="RE0/AN5"/>
<pin name="RE1/AN6"/>
<pin name="RA7/OSC1/CLKIN"/>
<pin name="RA6/OSC2/CLKOUT"/>
<pin name="RC0/SOSCO/T1CKI"/>
<pin name="RC1/SOSCI/CCP2"/>
<pin name="RC2/AN14/CCP1"/>
<pin name="RC3/AN15/SCK/SCL"/>
<pin name="RD0/AN20"/>
<pin name="RD1/AN21"/>
<pin name="RD2/AN22"/>
<pin name="RD3/AN23"/>
<pin name="RC4/AN16/SDI/SDA"/>
<pin name="RC5/AN17/SDO"/>
<pin name="RC6/AN18/TX/CK"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE2/AN7"/>
</symbol>
<symbol name="MCP14628">
<pin name="BOOT"/>
<pin name="PWM"/>
<pin name="FCCM"/>
<pin name="PSE"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="HDR" direction="out"/>
<pin name="LDR" direction="out"/>
</symbol>
<symbol name="MCP73833/4">
<pin name="1VD" direction="pwr"/>
<pin name="2VD" direction="pwr"/>
<pin name="3ST1"/>
<pin name="4ST2"/>
<pin name="5VS" direction="pwr"/>
<pin name="6PR"/>
<pin name="7PG"/>
<pin name="8T"/>
<pin name="9VB" direction="pwr"/>
<pin name="10VB" direction="pwr"/>
</symbol>
<symbol name="MCP73831-SOT">
<pin name="P$1"/>
<pin name="P$2" direction="pwr"/>
<pin name="P$3" direction="pwr"/>
<pin name="P$4" direction="pwr"/>
<pin name="P$5" direction="pwr"/>
</symbol>
<symbol name="MCP73831-DFN">
<pin name="P$1" direction="pwr"/>
<pin name="P$2" direction="pwr"/>
<pin name="P$3" direction="pwr"/>
<pin name="P$4" direction="pwr"/>
<pin name="P$5"/>
<pin name="P$6" direction="pwr"/>
<pin name="P$7" direction="nc"/>
<pin name="P$8"/>
</symbol>
<symbol name="DSPIC33EP256MU806-X_MR">
<pin name="AN29/PWM3H/PMD5/RP85/RE5" direction="pas"/>
<pin name="AN30/PWM4L/PMD6/RP86/RE6" direction="pas"/>
<pin name="AN31/PWM4H/PMD7/RP87/RE7" direction="pas"/>
<pin name="C1IND/SCK2/PMA5/RP118/RG6" direction="pas"/>
<pin name="C1INC/SDI2/PMA4/RP119/RG7" direction="pas"/>
<pin name="C2IND/SDO2/PMA3/RP120/RG8" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2INC/PMA2/RP121/RG9" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" direction="pas"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="PGEC3/AN1/VREF-/RP33/RB1" direction="pas"/>
<pin name="PGED3/AN0/VREF+/RP32/RB0" direction="pas"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AN8/PMA6/RP40/RB8" direction="pas"/>
<pin name="AN9/PMA7/RP41/RB9" direction="pas"/>
<pin name="TMS/AN10/CVREF/PMA13/RP42/RB10" direction="pas"/>
<pin name="TDO/AN11/PMA12/RP43/RB11" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="TCK/AN12/PMA11/RP44/RB12" direction="pas"/>
<pin name="TDI/AN13/PMA10/RP45/RB13" direction="pas"/>
<pin name="AN14/PMA1/RP46/RB14" direction="pas"/>
<pin name="AN15/PMA0/RP47/RB15" direction="pas"/>
<pin name="SDA2/PMA9/RP100/RF4" direction="pas"/>
<pin name="SCL2/PMA8/RP101/RF5" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="AN28/PWM3L/PMD4/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/PMD3/RP83/RE3" direction="pas"/>
<pin name="AN26/PWM2L/PMD2/RP82/RE2" direction="pas"/>
<pin name="AN25/PWM1H/PMD1/RP81/RE1" direction="pas"/>
<pin name="AN24/PWM1L/PMD0/RP80/RE0" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="PMRD/RP69/RD5" direction="pas"/>
<pin name="PMWR/RP68/RD4" direction="pas"/>
<pin name="PMBE/RP67/RD3" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="PMCS1/RP75/RD11" direction="pas"/>
<pin name="ASCL1/PMCS2/RP74/RD10" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="VUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
</symbol>
<symbol name="DSPIC33EP256MU806-X_PT">
<pin name="AN29/PWM3H/PMD5/RP85/RE5" direction="pas"/>
<pin name="AN30/PWM4L/PMD6/RP86/RE6" direction="pas"/>
<pin name="AN31/PWM4H/PMD7/RP87/RE7" direction="pas"/>
<pin name="C1IND/SCK2/PMA5/RP118/RG6" direction="pas"/>
<pin name="C1INC/SDI2/PMA4/RP119/RG7" direction="pas"/>
<pin name="C2IND/SDO2/PMA3/RP120/RG8" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2INC/PMA2/RP121/RG9" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" direction="pas"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="PGEC3/AN1/VREF-/RP33/RB1" direction="pas"/>
<pin name="PGED3/AN0/VREF+/RP32/RB0" direction="pas"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AN8/PMA6/RP40/RB8" direction="pas"/>
<pin name="AN9/PMA7/RP41/RB9" direction="pas"/>
<pin name="TMS/AN10/CVREF/PMA13/RP42/RB10" direction="pas"/>
<pin name="TDO/AN11/PMA12/RP43/RB11" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="TCK/AN12/PMA11/RP44/RB12" direction="pas"/>
<pin name="TDI/AN13/PMA10/RP45/RB13" direction="pas"/>
<pin name="AN14/PMA1/RP46/RB14" direction="pas"/>
<pin name="AN15/PMA0/RP47/RB15" direction="pas"/>
<pin name="SDA2/PMA9/RP100/RF4" direction="pas"/>
<pin name="SCL2/PMA8/RP101/RF5" direction="pas"/>
<pin name="AN28/PWM3L/PMD4/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/PMD3/RP83/RE3" direction="pas"/>
<pin name="AN26/PWM2L/PMD2/RP82/RE2" direction="pas"/>
<pin name="AN25/PWM1H/PMD1/RP81/RE1" direction="pas"/>
<pin name="AN24/PWM1L/PMD0/RP80/RE0" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="PMRD/RP69/RD5" direction="pas"/>
<pin name="PMWR/RP68/RD4" direction="pas"/>
<pin name="PMBE/RP67/RD3" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="PMCS1/RP75/RD11" direction="pas"/>
<pin name="ASCL1/PMCS2/RP74/RD10" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="VUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
</symbol>
<symbol name="DSPIC33EP256MU810-X_BG">
<pin name="AN28/PWM3L/PMD4/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/PMD3/RP83/RE3" direction="pas"/>
<pin name="RP125/RG13" direction="pas"/>
<pin name="AN24/PWM1L/PMD0/RP80/RE0" direction="pas"/>
<pin name="RP112/RG0" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="NO_CONNECT" direction="nc"/>
<pin name="RP76/RD12" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="NO_CONNECT_2" direction="nc"/>
<pin name="RP127/RG15" direction="pas"/>
<pin name="AN26/PWM2L/PMD2/RP82/RE2" direction="pas"/>
<pin name="AN25/PWM1H/PMD1/RP81/RE1" direction="pas"/>
<pin name="AN23/RP23/RA7" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VCAP" direction="pwr"/>
<pin name="PMRD/RP69/RD5" direction="pas"/>
<pin name="PMBE/RP67/RD3" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="AN30/PWM4L/PMD6/RP86/RE6" direction="pas"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="RP124/RG12" direction="pas"/>
<pin name="RP126/RG14" direction="pas"/>
<pin name="AN22/RP22/RA6" direction="pas"/>
<pin name="NO_CONNECT_3" direction="nc"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="PMWR/RP68/RD4" direction="pas"/>
<pin name="NO_CONNECT_4" direction="nc"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="PMCS1/RP75/RD11" direction="pas"/>
<pin name="AN16/PWM5L/RP49/RC1" direction="pas"/>
<pin name="AN31/PWM4H/PMD7/RP87/RE7" direction="pas"/>
<pin name="AN29/PWM3H/PMD5/RP85/RE5" direction="pas"/>
<pin name="NO_CONNECT_5" direction="nc"/>
<pin name="NO_CONNECT_6" direction="nc"/>
<pin name="NO_CONNECT_7" direction="nc"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="RP77/RD13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="NO_CONNECT_8" direction="nc"/>
<pin name="ASCL1/PMCS2/RP74/RD10" direction="pas"/>
<pin name="AN19/PWM6H/RP52/RC4" direction="pas"/>
<pin name="AN18/PWM6L/RP51/RC3" direction="pas"/>
<pin name="C1IND/SCK2/PMA5/RP118/RG6" direction="pas"/>
<pin name="AN17/PWM5H/RP50/RC2" direction="pas"/>
<pin name="NO_CONNECT_9" direction="nc"/>
<pin name="RP113/RG1" direction="pas"/>
<pin name="NO_CONNECT_10" direction="nc"/>
<pin name="RP31/RA15" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RP30/RA14" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2IND/SDO2/PMA3/RP120/RG8" direction="pas"/>
<pin name="C2INC/PMA2/RP121/RG9" direction="pas"/>
<pin name="C1INC/SDI2/PMA4/RP119/RG7" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="SCL2/PMA8/RP101/RF5" direction="pas"/>
<pin name="SDA2/PMA9/RP100/RF4" direction="pas"/>
<pin name="RP78/RD14" direction="pas"/>
<pin name="AN15/PMA0/RP47/RB15" direction="pas"/>
<pin name="AN13/PMA10/RP45/RB13" direction="pas"/>
<pin name="RP109/RF13" direction="pas"/>
<pin name="AN10/CVREF/PMA13/RP42/RB10" direction="pas"/>
<pin name="AN9/PMA7//RP41/RB9" direction="pas"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VREF-/RA9" direction="pas"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="RP98/RF2" direction="pas"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
<pin name="RP79/RD15" direction="pas"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="AN14/PMA1/RP46/RB14" direction="pas"/>
<pin name="RP108/RF12" direction="pas"/>
<pin name="NO_CONNECT_11" direction="nc"/>
<pin name="AN8/PMA6/RP40/RB8" direction="pas"/>
<pin name="VREF+/RA10" direction="pas"/>
<pin name="PGED3/AN0/RP32/RB0" direction="pas"/>
<pin name="PGEC3/AN1/RP33/RB1" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="RP104/RF8" direction="pas"/>
<pin name="NO_CONNECT_12" direction="nc"/>
<pin name="NO_CONNECT_13" direction="nc"/>
<pin name="AN12/PMA11/RP44/RB12" direction="pas"/>
<pin name="TCK/RP17/RA1" direction="pas"/>
<pin name="AN11/PMA12/RP43/RB11" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="ASCL2/RP18/RA2" direction="pas"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="VUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="NO_CONNECT_14" direction="nc"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="NO_CONNECT_15" direction="nc"/>
<pin name="NO_CONNECT_16" direction="nc"/>
<pin name="NO_CONNECT_17" direction="nc"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" direction="pas"/>
<pin name="TDI/RP20/RA4" direction="pas"/>
<pin name="ASDA2/RP19/RA3" direction="pas"/>
<pin name="TDO/RP21/RA5" direction="pas"/>
<pin name="NO_CONNECT_18" direction="nc"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="NO_CONNECT_19" direction="nc"/>
<pin name="TMS/RP16/RA0" direction="pas"/>
<pin name="AN21/RP89/RE9" direction="pas"/>
<pin name="AN20/RP88/RE8" direction="pas"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="NO_CONNECT_20" direction="nc"/>
<pin name="NO_CONNECT_21" direction="nc"/>
</symbol>
<symbol name="DSPIC33EP256MU810-X_PF">
<pin name="RP127/RG15" direction="pas"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="AN29/PWM3H/PMD5/RP85/RE5" direction="pas"/>
<pin name="AN30/PWM4L/PMD6/RP86/RE6" direction="pas"/>
<pin name="AN31/PWM4H/PMD7/RP87/RE7" direction="pas"/>
<pin name="AN16/PWM5L/RP49/RC1" direction="pas"/>
<pin name="AN17/PWM5H/RP50/RC2" direction="pas"/>
<pin name="AN18/PWM6L/RP51/RC3" direction="pas"/>
<pin name="AN19/PWM6H/RP52/RC4" direction="pas"/>
<pin name="C1IND/SCK2/PMA5/RP118/RG6" direction="pas"/>
<pin name="C1INC/SDI2/PMA4/RP119/RG7" direction="pas"/>
<pin name="C2IND/SDO2/PMA3/RP120/RG8" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2INC/PMA2/RP121/RG9" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="TMS/RP16/RA0" direction="pas"/>
<pin name="AN20/RP88/RE8" direction="pas"/>
<pin name="AN21/RP89/RE9" direction="pas"/>
<pin name="AN5/C1INA/VBUSON//VBUSST/RP37/RB5" direction="pas"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="PGEC3/AN1/RP33/RB1" direction="pas"/>
<pin name="PGED3/AN0/RP32/RB0" direction="pas"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="VREF-/RA9" direction="pas"/>
<pin name="VREF+/RA10" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AN8/PMA6/RP40/RB8" direction="pas"/>
<pin name="AN9/PMA7//RP41/RB9" direction="pas"/>
<pin name="AN10/CVREF/PMA13/RP42/RB10" direction="pas"/>
<pin name="AN11/PMA12/RP43/RB11" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="TCK/RP17/RA1" direction="pas"/>
<pin name="RP109/RF13" direction="pas"/>
<pin name="RP108/RF12" direction="pas"/>
<pin name="AN12/PMA11/RP44/RB12" direction="pas"/>
<pin name="AN13/PMA10/RP45/RB13" direction="pas"/>
<pin name="AN14/PMA1/RP46/RB14" direction="pas"/>
<pin name="AN15/PMA0/RP47/RB15" direction="pas"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="RP78/RD14" direction="pas"/>
<pin name="RP79/RD15" direction="pas"/>
<pin name="SDA2/PMA9/RP100/RF4" direction="pas"/>
<pin name="SCL2/PMA8/RP101/RF5" direction="pas"/>
<pin name="AN28/PWM3L/PMD4/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/PMD3/RP83/RE3" direction="pas"/>
<pin name="AN26/PWM2L/PMD2/RP82/RE2" direction="pas"/>
<pin name="RP125/RG13" direction="pas"/>
<pin name="RP124/RG12" direction="pas"/>
<pin name="RP126/RG14" direction="pas"/>
<pin name="AN25/PWM1H/PMD1/RP81/RE1" direction="pas"/>
<pin name="AN24/PWM1L/PMD0/RP80/RE0" direction="pas"/>
<pin name="AN23/RP23/RA7" direction="pas"/>
<pin name="AN22/RP22/RA6" direction="pas"/>
<pin name="RP112/RG0" direction="pas"/>
<pin name="RP113/RG1" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="PMRD/RP69/RD5" direction="pas"/>
<pin name="PMWR/RP68/RD4" direction="pas"/>
<pin name="RP77/RD13" direction="pas"/>
<pin name="RP76/RD12" direction="pas"/>
<pin name="PMBE/RP67/RD3" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="PMCS1/RP75/RD11" direction="pas"/>
<pin name="ASCL1/PMCS2/RP74/RD10" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="RP31/RA15" direction="pas"/>
<pin name="RP30/RA14" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="TDO/RP21/RA5" direction="pas"/>
<pin name="TDI/RP20/RA4" direction="pas"/>
<pin name="ASDA2/RP19/RA3" direction="pas"/>
<pin name="ASCL2/RP18/RA2" direction="pas"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="BUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="RP104/RF8" direction="pas"/>
<pin name="RP98/RF2" direction="pas"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
</symbol>
<symbol name="DSPIC33EP256MU810-X_PT">
<pin name="RP127/RG15" direction="pas"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="AN29/PWM3H/PMD5/RP85/RE5" direction="pas"/>
<pin name="AN30/PWM4L/PMD6/RP86/RE6" direction="pas"/>
<pin name="AN31/PWM4H/PMD7/RP87/RE7" direction="pas"/>
<pin name="AN16/PWM5L/RP49/RC1" direction="pas"/>
<pin name="AN17/PWM5H/RP50/RC2" direction="pas"/>
<pin name="AN18/PWM6L/RP51/RC3" direction="pas"/>
<pin name="AN19/PWM6H/RP52/RC4" direction="pas"/>
<pin name="C1IND/SCK2/PMA5/RP118/RG6" direction="pas"/>
<pin name="C1INC/SDI2/PMA4/RP119/RG7" direction="pas"/>
<pin name="C2IND/SDO2/PMA3/RP120/RG8" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2INC/PMA2/RP121/RG9" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="TMS/RP16/RA0" direction="pas"/>
<pin name="AN20/RP88/RE8" direction="pas"/>
<pin name="AN21/RP89/RE9" direction="pas"/>
<pin name="AN5/C1INA/VBUSON//VBUSST/RP37/RB5" direction="pas"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="PGEC3/AN1/RP33/RB1" direction="pas"/>
<pin name="PGED3/AN0/RP32/RB0" direction="pas"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="VREF-/RA9" direction="pas"/>
<pin name="VREF+/RA10" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AN8/PMA6/RP40/RB8" direction="pas"/>
<pin name="AN9/PMA7//RP41/RB9" direction="pas"/>
<pin name="AN10/CVREF/PMA13/RP42/RB10" direction="pas"/>
<pin name="AN11/PMA12/RP43/RB11" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="TCK/RP17/RA1" direction="pas"/>
<pin name="RP109/RF13" direction="pas"/>
<pin name="RP108/RF12" direction="pas"/>
<pin name="AN12/PMA11/RP44/RB12" direction="pas"/>
<pin name="AN13/PMA10/RP45/RB13" direction="pas"/>
<pin name="AN14/PMA1/RP46/RB14" direction="pas"/>
<pin name="AN15/PMA0/RP47/RB15" direction="pas"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="RP78/RD14" direction="pas"/>
<pin name="RP79/RD15" direction="pas"/>
<pin name="SDA2/PMA9/RP100/RF4" direction="pas"/>
<pin name="SCL2/PMA8/RP101/RF5" direction="pas"/>
<pin name="AN28/PWM3L/PMD4/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/PMD3/RP83/RE3" direction="pas"/>
<pin name="AN26/PWM2L/PMD2/RP82/RE2" direction="pas"/>
<pin name="RP125/RG13" direction="pas"/>
<pin name="RP124/RG12" direction="pas"/>
<pin name="RP126/RG14" direction="pas"/>
<pin name="AN25/PWM1H/PMD1/RP81/RE1" direction="pas"/>
<pin name="AN24/PWM1L/PMD0/RP80/RE0" direction="pas"/>
<pin name="AN23/RP23/RA7" direction="pas"/>
<pin name="AN22/RP22/RA6" direction="pas"/>
<pin name="RP112/RG0" direction="pas"/>
<pin name="RP113/RG1" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="PMRD/RP69/RD5" direction="pas"/>
<pin name="PMWR/RP68/RD4" direction="pas"/>
<pin name="RP77/RD13" direction="pas"/>
<pin name="RP76/RD12" direction="pas"/>
<pin name="PMBE/RP67/RD3" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="PMCS1/RP75/RD11" direction="pas"/>
<pin name="ASCL1/PMCS2/RP74/RD10" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="RP31/RA15" direction="pas"/>
<pin name="RP30/RA14" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="TDO/RP21/RA5" direction="pas"/>
<pin name="TDI/RP20/RA4" direction="pas"/>
<pin name="ASDA2/RP19/RA3" direction="pas"/>
<pin name="ASCL2/RP18/RA2" direction="pas"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="BUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="RP104/RF8" direction="pas"/>
<pin name="RP98/RF2" direction="pas"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
</symbol>
<symbol name="DSPIC33EP512MU810-X_BG_A">
<pin name="AN28/PWM3L/PMD4/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/PMD3/RP83/RE3" direction="pas"/>
<pin name="RP125/RG13" direction="pas"/>
<pin name="AN24/PWM1L/PMD0/RP80/RE0" direction="pas"/>
<pin name="RP112/RG0" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="NO_CONNECT" direction="nc"/>
<pin name="RP76/RD12" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="NO_CONNECT_2" direction="nc"/>
<pin name="RP127/RG15" direction="pas"/>
<pin name="AN26/PWM2L/PMD2/RP82/RE2" direction="pas"/>
<pin name="AN25/PWM1H/PMD1/RP81/RE1" direction="pas"/>
<pin name="AN23/RP23/RA7" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VCAP" direction="pwr"/>
<pin name="PMRD/RP69/RD5" direction="pas"/>
<pin name="PMBE/RP67/RD3" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="AN30/PWM4L/PMD6/RP86/RE6" direction="pas"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="RP124/RG12" direction="pas"/>
<pin name="RP126/RG14" direction="pas"/>
<pin name="AN22/RP22/RA6" direction="pas"/>
<pin name="NO_CONNECT_3" direction="nc"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="PMWR/RP68/RD4" direction="pas"/>
<pin name="NO_CONNECT_4" direction="nc"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="PMCS1/RP75/RD11" direction="pas"/>
<pin name="AN16/PWM5L/RP49/RC1" direction="pas"/>
<pin name="AN31/PWM4H/PMD7/RP87/RE7" direction="pas"/>
<pin name="AN29/PWM3H/PMD5/RP85/RE5" direction="pas"/>
<pin name="NO_CONNECT_5" direction="nc"/>
<pin name="NO_CONNECT_6" direction="nc"/>
<pin name="NO_CONNECT_7" direction="nc"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="RP77/RD13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="NO_CONNECT_8" direction="nc"/>
<pin name="ASCL1/PMCS2/RP74/RD10" direction="pas"/>
<pin name="AN19/PWM6H/RP52/RC4" direction="pas"/>
<pin name="AN18/PWM6L/RP51/RC3" direction="pas"/>
<pin name="C1IND/SCK2/PMA5/RP118/RG6" direction="pas"/>
<pin name="AN17/PWM5H/RP50/RC2" direction="pas"/>
<pin name="NO_CONNECT_9" direction="nc"/>
<pin name="RP113/RG1" direction="pas"/>
<pin name="NO_CONNECT_10" direction="nc"/>
<pin name="RP31/RA15" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RP30/RA14" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2IND/SDO2/PMA3/RP120/RG8" direction="pas"/>
<pin name="C2INC/PMA2/RP121/RG9" direction="pas"/>
<pin name="C1INC/SDI2/PMA4/RP119/RG7" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="SCL2/PMA8/RP101/RF5" direction="pas"/>
<pin name="SDA2/PMA9/RP100/RF4" direction="pas"/>
<pin name="RP78/RD14" direction="pas"/>
<pin name="AN15/PMA0/RP47/RB15" direction="pas"/>
<pin name="AN13/PMA10/RP45/RB13" direction="pas"/>
<pin name="RP109/RF13" direction="pas"/>
<pin name="AN10/CVREF/PMA13/RP42/RB10" direction="pas"/>
<pin name="AN9/PMA7//RP41/RB9" direction="pas"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VREF-/RA9" direction="pas"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="RP98/RF2" direction="pas"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
<pin name="RP79/RD15" direction="pas"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="AN14/PMA1/RP46/RB14" direction="pas"/>
<pin name="RP108/RF12" direction="pas"/>
<pin name="NO_CONNECT_11" direction="nc"/>
<pin name="AN8/PMA6/RP40/RB8" direction="pas"/>
<pin name="VREF+/RA10" direction="pas"/>
<pin name="PGED3/AN0/RP32/RB0" direction="pas"/>
<pin name="PGEC3/AN1/RP33/RB1" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="RP104/RF8" direction="pas"/>
<pin name="NO_CONNECT_12" direction="nc"/>
<pin name="NO_CONNECT_13" direction="nc"/>
<pin name="AN12/PMA11/RP44/RB12" direction="pas"/>
<pin name="TCK/RP17/RA1" direction="pas"/>
<pin name="AN11/PMA12/RP43/RB11" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="ASCL2/RP18/RA2" direction="pas"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="VUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="NO_CONNECT_14" direction="nc"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="NO_CONNECT_15" direction="nc"/>
<pin name="NO_CONNECT_16" direction="nc"/>
<pin name="NO_CONNECT_17" direction="nc"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" direction="pas"/>
<pin name="TDI/RP20/RA4" direction="pas"/>
<pin name="ASDA2/RP19/RA3" direction="pas"/>
<pin name="TDO/RP21/RA5" direction="pas"/>
<pin name="NO_CONNECT_18" direction="nc"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="NO_CONNECT_19" direction="nc"/>
<pin name="TMS/RP16/RA0" direction="pas"/>
<pin name="AN21/RP89/RE9" direction="pas"/>
<pin name="AN20/RP88/RE8" direction="pas"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="NO_CONNECT_20" direction="nc"/>
<pin name="NO_CONNECT_21" direction="nc"/>
</symbol>
<symbol name="DSPIC33EP512MU810-X_PF">
<pin name="RP127/RG15" direction="pas"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="AN29/PWM3H/PMD5/RP85/RE5" direction="pas"/>
<pin name="AN30/PWM4L/PMD6/RP86/RE6" direction="pas"/>
<pin name="AN31/PWM4H/PMD7/RP87/RE7" direction="pas"/>
<pin name="AN16/PWM5L/RP49/RC1" direction="pas"/>
<pin name="AN17/PWM5H/RP50/RC2" direction="pas"/>
<pin name="AN18/PWM6L/RP51/RC3" direction="pas"/>
<pin name="AN19/PWM6H/RP52/RC4" direction="pas"/>
<pin name="C1IND/SCK2/PMA5/RP118/RG6" direction="pas"/>
<pin name="C1INC/SDI2/PMA4/RP119/RG7" direction="pas"/>
<pin name="C2IND/SDO2/PMA3/RP120/RG8" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2INC/PMA2/RP121/RG9" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="TMS/RP16/RA0" direction="pas"/>
<pin name="AN20/RP88/RE8" direction="pas"/>
<pin name="AN21/RP89/RE9" direction="pas"/>
<pin name="AN5/C1INA/VBUSON//VBUSST/RP37/RB5" direction="pas"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="PGEC3/AN1/RP33/RB1" direction="pas"/>
<pin name="PGED3/AN0/RP32/RB0" direction="pas"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="VREF-/RA9" direction="pas"/>
<pin name="VREF+/RA10" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AN8/PMA6/RP40/RB8" direction="pas"/>
<pin name="AN9/PMA7//RP41/RB9" direction="pas"/>
<pin name="AN10/CVREF/PMA13/RP42/RB10" direction="pas"/>
<pin name="AN11/PMA12/RP43/RB11" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="TCK/RP17/RA1" direction="pas"/>
<pin name="RP109/RF13" direction="pas"/>
<pin name="RP108/RF12" direction="pas"/>
<pin name="AN12/PMA11/RP44/RB12" direction="pas"/>
<pin name="AN13/PMA10/RP45/RB13" direction="pas"/>
<pin name="AN14/PMA1/RP46/RB14" direction="pas"/>
<pin name="AN15/PMA0/RP47/RB15" direction="pas"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="RP78/RD14" direction="pas"/>
<pin name="RP79/RD15" direction="pas"/>
<pin name="SDA2/PMA9/RP100/RF4" direction="pas"/>
<pin name="SCL2/PMA8/RP101/RF5" direction="pas"/>
<pin name="AN28/PWM3L/PMD4/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/PMD3/RP83/RE3" direction="pas"/>
<pin name="AN26/PWM2L/PMD2/RP82/RE2" direction="pas"/>
<pin name="RP125/RG13" direction="pas"/>
<pin name="RP124/RG12" direction="pas"/>
<pin name="RP126/RG14" direction="pas"/>
<pin name="AN25/PWM1H/PMD1/RP81/RE1" direction="pas"/>
<pin name="AN24/PWM1L/PMD0/RP80/RE0" direction="pas"/>
<pin name="AN23/RP23/RA7" direction="pas"/>
<pin name="AN22/RP22/RA6" direction="pas"/>
<pin name="RP112/RG0" direction="pas"/>
<pin name="RP113/RG1" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="PMRD/RP69/RD5" direction="pas"/>
<pin name="PMWR/RP68/RD4" direction="pas"/>
<pin name="RP77/RD13" direction="pas"/>
<pin name="RP76/RD12" direction="pas"/>
<pin name="PMBE/RP67/RD3" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="PMCS1/RP75/RD11" direction="pas"/>
<pin name="ASCL1/PMCS2/RP74/RD10" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="RP31/RA15" direction="pas"/>
<pin name="RP30/RA14" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="TDO/RP21/RA5" direction="pas"/>
<pin name="TDI/RP20/RA4" direction="pas"/>
<pin name="ASDA2/RP19/RA3" direction="pas"/>
<pin name="ASCL2/RP18/RA2" direction="pas"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="BUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="RP104/RF8" direction="pas"/>
<pin name="RP98/RF2" direction="pas"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
<pin name="MCLR*" direction="in"/>
</symbol>
<symbol name="DSPIC33EP512MU810-X_PT">
<pin name="RP127/RG15" direction="pas"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="AN29/PWM3H/PMD5/RP85/RE5" direction="pas"/>
<pin name="AN30/PWM4L/PMD6/RP86/RE6" direction="pas"/>
<pin name="AN31/PWM4H/PMD7/RP87/RE7" direction="pas"/>
<pin name="AN16/PWM5L/RP49/RC1" direction="pas"/>
<pin name="AN17/PWM5H/RP50/RC2" direction="pas"/>
<pin name="AN18/PWM6L/RP51/RC3" direction="pas"/>
<pin name="AN19/PWM6H/RP52/RC4" direction="pas"/>
<pin name="C1IND/SCK2/PMA5/RP118/RG6" direction="pas"/>
<pin name="C1INC/SDI2/PMA4/RP119/RG7" direction="pas"/>
<pin name="C2IND/SDO2/PMA3/RP120/RG8" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2INC/PMA2/RP121/RG9" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="TMS/RP16/RA0" direction="pas"/>
<pin name="AN20/RP88/RE8" direction="pas"/>
<pin name="AN21/RP89/RE9" direction="pas"/>
<pin name="AN5/C1INA/VBUSON//VBUSST/RP37/RB5" direction="pas"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="PGEC3/AN1/RP33/RB1" direction="pas"/>
<pin name="PGED3/AN0/RP32/RB0" direction="pas"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="VREF-/RA9" direction="pas"/>
<pin name="VREF+/RA10" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AN8/PMA6/RP40/RB8" direction="pas"/>
<pin name="AN9/PMA7//RP41/RB9" direction="pas"/>
<pin name="AN10/CVREF/PMA13/RP42/RB10" direction="pas"/>
<pin name="AN11/PMA12/RP43/RB11" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="TCK/RP17/RA1" direction="pas"/>
<pin name="RP109/RF13" direction="pas"/>
<pin name="RP108/RF12" direction="pas"/>
<pin name="AN12/PMA11/RP44/RB12" direction="pas"/>
<pin name="AN13/PMA10/RP45/RB13" direction="pas"/>
<pin name="AN14/PMA1/RP46/RB14" direction="pas"/>
<pin name="AN15/PMA0/RP47/RB15" direction="pas"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="RP78/RD14" direction="pas"/>
<pin name="RP79/RD15" direction="pas"/>
<pin name="SDA2/PMA9/RP100/RF4" direction="pas"/>
<pin name="SCL2/PMA8/RP101/RF5" direction="pas"/>
<pin name="AN28/PWM3L/PMD4/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/PMD3/RP83/RE3" direction="pas"/>
<pin name="AN26/PWM2L/PMD2/RP82/RE2" direction="pas"/>
<pin name="RP125/RG13" direction="pas"/>
<pin name="RP124/RG12" direction="pas"/>
<pin name="RP126/RG14" direction="pas"/>
<pin name="AN25/PWM1H/PMD1/RP81/RE1" direction="pas"/>
<pin name="AN24/PWM1L/PMD0/RP80/RE0" direction="pas"/>
<pin name="AN23/RP23/RA7" direction="pas"/>
<pin name="AN22/RP22/RA6" direction="pas"/>
<pin name="RP112/RG0" direction="pas"/>
<pin name="RP113/RG1" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="PMRD/RP69/RD5" direction="pas"/>
<pin name="PMWR/RP68/RD4" direction="pas"/>
<pin name="RP77/RD13" direction="pas"/>
<pin name="RP76/RD12" direction="pas"/>
<pin name="PMBE/RP67/RD3" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="PMCS1/RP75/RD11" direction="pas"/>
<pin name="ASCL1/PMCS2/RP74/RD10" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="RP31/RA15" direction="pas"/>
<pin name="RP30/RA14" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="TDO/RP21/RA5" direction="pas"/>
<pin name="TDI/RP20/RA4" direction="pas"/>
<pin name="ASDA2/RP19/RA3" direction="pas"/>
<pin name="ASCL2/RP18/RA2" direction="pas"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="BUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="RP104/RF8" direction="pas"/>
<pin name="RP98/RF2" direction="pas"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
</symbol>
<symbol name="DSPIC33EP512MU814-X_PH_A">
<pin name="RP127/RG15" direction="pas"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="AN29/PWM3H/RP85/RE5" direction="pas"/>
<pin name="AN30/PWM4L/RP86/RE6" direction="pas"/>
<pin name="AN31/PWM4H/RP87/RE7" direction="pas"/>
<pin name="PWM7L/PMA8/RJ8" direction="pas"/>
<pin name="PWM7H/PMA9/RJ9" direction="pas"/>
<pin name="PMA10/RJ10" direction="pas"/>
<pin name="PMA11/RJ11" direction="pas"/>
<pin name="AN16/PWM5L/RP49/RC1" direction="pas"/>
<pin name="AN17/PWM5H/RP50/RC2" direction="pas"/>
<pin name="AN18/PWM6L/RP51/RC3" direction="pas"/>
<pin name="AN19/PWM6H/RP52/RC4" direction="pas"/>
<pin name="PMA12/RJ12" direction="pas"/>
<pin name="PMA13/RJ13" direction="pas"/>
<pin name="C1IND/SCK2/RP118/RG6" direction="pas"/>
<pin name="C1INC/SDI2/RP119/RG7" direction="pas"/>
<pin name="C2IND/SDO2/RP120/RG8" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2INC/RP121/RG9" direction="pas"/>
<pin name="RJ14" direction="pas"/>
<pin name="RJ15" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="TMS/RP16/RA0" direction="pas"/>
<pin name="AN20/RP88/RE8" direction="pas"/>
<pin name="AN21/RP89/RE9" direction="pas"/>
<pin name="RK0" direction="pas"/>
<pin name="RK1" direction="pas"/>
<pin name="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" direction="pas"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="PGEC3/AN1/RP33/RB1" direction="pas"/>
<pin name="PGED3/AN0/RP32/RB0" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="VREF-/RA9" direction="pas"/>
<pin name="VREF+/RA10" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="PMD0/RH0" direction="pas"/>
<pin name="PMD1/RH1" direction="pas"/>
<pin name="PMD2/RH2" direction="pas"/>
<pin name="PMD3/RH3" direction="pas"/>
<pin name="AN8/RP40/RB8" direction="pas"/>
<pin name="AN9/RP41/RB9" direction="pas"/>
<pin name="AN10/CVREF/RP42/RB10" direction="pas"/>
<pin name="AN11/RP43/RB11" direction="pas"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="PMRD/RK15" direction="pas"/>
<pin name="PMWR/RK14" direction="pas"/>
<pin name="PMBE/RK13" direction="pas"/>
<pin name="TCK/RP17/RA1" direction="pas"/>
<pin name="RP109/RF13" direction="pas"/>
<pin name="RP108/RF12" direction="pas"/>
<pin name="AN12/RP44/RB12" direction="pas"/>
<pin name="AN13/RP45/RB13" direction="pas"/>
<pin name="AN14/RP46/RB14" direction="pas"/>
<pin name="AN15/RP47/RB15" direction="pas"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="PMD4/RH4" direction="pas"/>
<pin name="PMD5/RH5" direction="pas"/>
<pin name="PMD6/RH6" direction="pas"/>
<pin name="PMD7/RH7" direction="pas"/>
<pin name="RP78/RD14" direction="pas"/>
<pin name="RP79/RD15" direction="pas"/>
<pin name="SDA2/RP100/RF4" direction="pas"/>
<pin name="SCL2/RP101/RF5" direction="pas"/>
<pin name="AN28/PWM3L/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/RP83/RE3" direction="pas"/>
<pin name="AN26/PWM2L/RP82/RE2" direction="pas"/>
<pin name="VSS_6" direction="pwr"/>
<pin name="RP125/RG13" direction="pas"/>
<pin name="RP124/RG12" direction="pas"/>
<pin name="RP126/RG14" direction="pas"/>
<pin name="AN25/PWM1H/RP81/RE1" direction="pas"/>
<pin name="AN24/PWM1L/RP80/RE0" direction="pas"/>
<pin name="PMA7/RJ7" direction="pas"/>
<pin name="PMA6/RJ6" direction="pas"/>
<pin name="PMA5/RJ5" direction="pas"/>
<pin name="PMA4/RJ4" direction="pas"/>
<pin name="AN23/RP23/RA7" direction="pas"/>
<pin name="AN22/RP22/RA6" direction="pas"/>
<pin name="RP112/RG0" direction="pas"/>
<pin name="RP113/RG1" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VSS_7" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="RP69/RD5" direction="pas"/>
<pin name="RP68/RD4" direction="pas"/>
<pin name="PMA3/RJ3" direction="pas"/>
<pin name="PMA2/RJ2" direction="pas"/>
<pin name="PMA1/RJ1" direction="pas"/>
<pin name="PMA0/RJ0" direction="pas"/>
<pin name="RP77/RD13" direction="pas"/>
<pin name="RP76/RD12" direction="pas"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="RP67/RD3" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="VSS_8" direction="pwr"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="RH15" direction="pas"/>
<pin name="RH14" direction="pas"/>
<pin name="RH13" direction="pas"/>
<pin name="RH12" direction="pas"/>
<pin name="RP75/RD11" direction="pas"/>
<pin name="ASCL1/RP74/RD10" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="RP31/RA15" direction="pas"/>
<pin name="RP30/RA14" direction="pas"/>
<pin name="PMCS1/RK11" direction="pas"/>
<pin name="PMCS2/RK12" direction="pas"/>
<pin name="VSS_9" direction="pwr"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="TDO/RP21/RA5" direction="pas"/>
<pin name="TDI/RP20/RA4" direction="pas"/>
<pin name="ASDA2/RP19/RA3" direction="pas"/>
<pin name="ASCL2/RP18/RA2" direction="pas"/>
<pin name="RH11" direction="pas"/>
<pin name="RH10" direction="pas"/>
<pin name="RH9" direction="pas"/>
<pin name="RH8" direction="pas"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="VUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="RP104/RF8" direction="pas"/>
<pin name="RP98/RF2" direction="pas"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC33EP512MU814-X_PL_A">
<pin name="RP127/RG15" direction="pas"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="AN29/PWM3H/RP85/RE5" direction="pas"/>
<pin name="AN30/PWM4L/RP86/RE6" direction="pas"/>
<pin name="AN31/PWM4H/RP87/RE7" direction="pas"/>
<pin name="PWM7L/PMA8/RJ8" direction="pas"/>
<pin name="PWM7H/PMA9/RJ9" direction="pas"/>
<pin name="PMA10/RJ10" direction="pas"/>
<pin name="PMA11/RJ11" direction="pas"/>
<pin name="AN16/PWM5L/RP49/RC1" direction="pas"/>
<pin name="AN17/PWM5H/RP50/RC2" direction="pas"/>
<pin name="AN18/PWM6L/RP51/RC3" direction="pas"/>
<pin name="AN19/PWM6H/RP52/RC4" direction="pas"/>
<pin name="PMA12/RJ12" direction="pas"/>
<pin name="PMA13/RJ13" direction="pas"/>
<pin name="C1IND/SCK2/RP118/RG6" direction="pas"/>
<pin name="C1INC/SDI2/RP119/RG7" direction="pas"/>
<pin name="C2IND/SDO2/RP120/RG8" direction="pas"/>
<pin name="!MCLR" direction="in"/>
<pin name="C2INC/RP121/RG9" direction="pas"/>
<pin name="RJ14" direction="pas"/>
<pin name="RJ15" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="TMS/RP16/RA0" direction="pas"/>
<pin name="AN20/RP88/RE8" direction="pas"/>
<pin name="AN21/RP89/RE9" direction="pas"/>
<pin name="RK0" direction="pas"/>
<pin name="RK1" direction="pas"/>
<pin name="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" direction="pas"/>
<pin name="AN4/C1INB/USBOEN/RP36/RB4" direction="pas"/>
<pin name="AN3/C2INA/VPIO/RP35/RB3" direction="pas"/>
<pin name="AN2/C2INB/VMIO/RP34/RB2" direction="pas"/>
<pin name="PGEC3/AN1/RP33/RB1" direction="pas"/>
<pin name="PGED3/AN0/RP32/RB0" direction="pas"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="PGEC1/AN6/RP38/RB6" direction="pas"/>
<pin name="PGED1/AN7/RCV/RP39/RB7" direction="pas"/>
<pin name="VREF-/RA9" direction="pas"/>
<pin name="VREF+/RA10" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="PMD0/RH0" direction="pas"/>
<pin name="PMD1/RH1" direction="pas"/>
<pin name="PMD2/RH2" direction="pas"/>
<pin name="PMD3/RH3" direction="pas"/>
<pin name="AN8/RP40/RB8" direction="pas"/>
<pin name="AN9/RP41/RB9" direction="pas"/>
<pin name="AN10/CVREF/RP42/RB10" direction="pas"/>
<pin name="AN11/RP43/RB11" direction="pas"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="PMRD/RK15" direction="pas"/>
<pin name="PMWR/RK14" direction="pas"/>
<pin name="PMBE/RK13" direction="pas"/>
<pin name="TCK/RP17/RA1" direction="pas"/>
<pin name="RP109/RF13" direction="pas"/>
<pin name="RP108/RF12" direction="pas"/>
<pin name="AN12/RP44/RB12" direction="pas"/>
<pin name="AN13/RP45/RB13" direction="pas"/>
<pin name="AN14/RP46/RB14" direction="pas"/>
<pin name="AN15/RP47/RB15" direction="pas"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="PMD4/RH4" direction="pas"/>
<pin name="PMD5/RH5" direction="pas"/>
<pin name="PMD6/RH6" direction="pas"/>
<pin name="PMD7/RH7" direction="pas"/>
<pin name="RP78/RD14" direction="pas"/>
<pin name="RP79/RD15" direction="pas"/>
<pin name="SDA2/RP100/RF4" direction="pas"/>
<pin name="SCL2/RP101/RF5" direction="pas"/>
<pin name="AN28/PWM3L/RP84/RE4" direction="pas"/>
<pin name="AN27/PWM2H/RP83/RE3" direction="pas"/>
<pin name="AN26/PWM2L/RP82/RE2" direction="pas"/>
<pin name="VSS_6" direction="pwr"/>
<pin name="RP125/RG13" direction="pas"/>
<pin name="RP124/RG12" direction="pas"/>
<pin name="RP126/RG14" direction="pas"/>
<pin name="AN25/PWM1H/RP81/RE1" direction="pas"/>
<pin name="AN24/PWM1L/RP80/RE0" direction="pas"/>
<pin name="PMA7/RJ7" direction="pas"/>
<pin name="PMA6/RJ6" direction="pas"/>
<pin name="PMA5/RJ5" direction="pas"/>
<pin name="PMA4/RJ4" direction="pas"/>
<pin name="AN23/RP23/RA7" direction="pas"/>
<pin name="AN22/RP22/RA6" direction="pas"/>
<pin name="RP112/RG0" direction="pas"/>
<pin name="RP113/RG1" direction="pas"/>
<pin name="VCMPST2/RP97/RF1" direction="pas"/>
<pin name="VCMPST1/RP96/RF0" direction="pas"/>
<pin name="VSS_7" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="C3INA/VCMPST3/RP71/RD7" direction="pas"/>
<pin name="C3INB/RP70/RD6" direction="pas"/>
<pin name="RP69/RD5" direction="pas"/>
<pin name="RP68/RD4" direction="pas"/>
<pin name="PMA3/RJ3" direction="pas"/>
<pin name="PMA2/RJ2" direction="pas"/>
<pin name="PMA1/RJ1" direction="pas"/>
<pin name="PMA0/RJ0" direction="pas"/>
<pin name="RP77/RD13" direction="pas"/>
<pin name="RP76/RD12" direction="pas"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="RP67/RD3" direction="pas"/>
<pin name="DPH/RP66/RD2" direction="pas"/>
<pin name="VCPCON/RP65/RD1" direction="pas"/>
<pin name="VSS_8" direction="pwr"/>
<pin name="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" direction="pas"/>
<pin name="PGED2/SOSCI/C3IND/RP61/RC13" direction="pas"/>
<pin name="INT0/DMH/RP64/RD0" direction="pas"/>
<pin name="RH15" direction="pas"/>
<pin name="RH14" direction="pas"/>
<pin name="RH13" direction="pas"/>
<pin name="RH12" direction="pas"/>
<pin name="RP75/RD11" direction="pas"/>
<pin name="ASCL1/RP74/RD10" direction="pas"/>
<pin name="ASDA1/DPLN/RP73/RD9" direction="pas"/>
<pin name="RTCC/DMLN/RP72/RD8" direction="pas"/>
<pin name="RP31/RA15" direction="pas"/>
<pin name="RP30/RA14" direction="pas"/>
<pin name="PMCS1/RK11" direction="pas"/>
<pin name="PMCS2/RK12" direction="pas"/>
<pin name="VSS_9" direction="pwr"/>
<pin name="OSC2/CLKO/RC15" direction="pas"/>
<pin name="OSC1/RP60/RC12" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="TDO/RP21/RA5" direction="pas"/>
<pin name="TDI/RP20/RA4" direction="pas"/>
<pin name="ASDA2/RP19/RA3" direction="pas"/>
<pin name="ASCL2/RP18/RA2" direction="pas"/>
<pin name="RH11" direction="pas"/>
<pin name="RH10" direction="pas"/>
<pin name="RH9" direction="pas"/>
<pin name="RH8" direction="pas"/>
<pin name="D+/RG2" direction="pas"/>
<pin name="D-/RG3" direction="pas"/>
<pin name="VUSB" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="RP104/RF8" direction="pas"/>
<pin name="RP98/RF2" direction="pas"/>
<pin name="USBID/RP99/RF3" direction="pas"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MCP42XX">
<pin name="A0" direction="pas"/>
<pin name="W0" direction="pas"/>
<pin name="B0" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="W1" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="RS" direction="in" function="dot"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
</symbol>
<symbol name="ABC">
<pin name="MCLR#/VPP" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="OSC2/CLKOUT" direction="out"/>
<pin name="T1OSO/RC0"/>
<pin name="T1OSI/RC1"/>
<pin name="CCP1/RC2"/>
<pin name="SCK/RC3"/>
<pin name="SDI/RC4"/>
<pin name="SDO/RC5"/>
<pin name="TX/RC6"/>
<pin name="RX/RC7"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="PGM/RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="PGC/RB6"/>
<pin name="PGD/RB7"/>
</symbol>
<symbol name="VCC1">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="GND1">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ABCDE">
<pin name="MCLR#/VPP" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="RD#/AN5/RE0"/>
<pin name="WR#/AN6/RE1"/>
<pin name="CS#/AN7/RE2"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="OSC2/CLKOUT" direction="out"/>
<pin name="T1OSO/RC0"/>
<pin name="T1OSI/RC1"/>
<pin name="CCP1/RC2"/>
<pin name="SCK/RC3"/>
<pin name="RD0/PSP0"/>
<pin name="RD1/PSP1"/>
<pin name="RD2/PSP2"/>
<pin name="RD3/PSP3"/>
<pin name="SDI/RC4"/>
<pin name="SDO/RC5"/>
<pin name="TX/RC6"/>
<pin name="RX/RC7"/>
<pin name="RD4/PSP4"/>
<pin name="RD5/PSP5"/>
<pin name="RD6/PSP6"/>
<pin name="RD7/PSP7"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="PGM/RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="PGC/RB6"/>
<pin name="PGD/RB7"/>
</symbol>
<symbol name="GNDVCC">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PIC180X0">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="RB5" direction="in"/>
<pin name="RB2" direction="hiz"/>
<pin name="RB4" direction="in"/>
<pin name="RB3" direction="in"/>
<pin name="RB0" direction="in"/>
<pin name="RB1" direction="out"/>
</symbol>
<symbol name="MCP2200">
<pin name="VUSB"/>
<pin name="VDD"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="RST"/>
<pin name="TXLED"/>
<pin name="RXLED"/>
<pin name="SSPND"/>
<pin name="USBCFG"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="CTS"/>
<pin name="RTS"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
</symbol>
<symbol name="MCP4725">
<pin name="VOUT"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="A0"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="MRF49XA">
<description>Microchip MRF49XA</description>
<pin name="!IRO"/>
<pin name="!CS" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="!INT!/DIO"/>
<pin name="FSK/DATA/!FSEL"/>
<pin name="CLKOUT" direction="out"/>
<pin name="RCLKOUT/FCAP/FINT"/>
<pin name="!RESET"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="RSSIO"/>
<pin name="RFXTL/EXTREF"/>
</symbol>
<symbol name="MRF89XA">
<description>Microchip MRF89XA</description>
<pin name="!CSDAT" direction="in"/>
<pin name="!CSCON" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="IRQ0" direction="out"/>
<pin name="IRQ1" direction="out"/>
<pin name="DATA"/>
<pin name="PLOCK" direction="out"/>
<pin name="CLKOUT" direction="out"/>
<pin name="TEST0" direction="in"/>
<pin name="TEST1" direction="in"/>
<pin name="TEST2" direction="in"/>
<pin name="TEST3" direction="in"/>
<pin name="TEST4" direction="in"/>
<pin name="TEST5" direction="in"/>
<pin name="TEST6" direction="in"/>
<pin name="TEST7" direction="in"/>
<pin name="TEST8" direction="in"/>
<pin name="PLLN"/>
<pin name="PLLP"/>
<pin name="VCOTN"/>
<pin name="VCOTP"/>
<pin name="VCORS" direction="out"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="AVRS" direction="out"/>
<pin name="DVRS" direction="out"/>
<pin name="PARS" direction="out"/>
<pin name="RFIO"/>
<pin name="NC" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MRF89XAMXA">
<pin name="!CSDAT" direction="in"/>
<pin name="!CSCON" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="IRQ0" direction="out"/>
<pin name="IRQ1" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="RESET" direction="in"/>
</symbol>
<symbol name="PIC24FVXXKA301">
<pin name="RA0/CN2/SCK2/PGEC2/AN0"/>
<pin name="RA1/CN3/SDO2/PGED2/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/SCL2/!SS1!/CN11/RB15"/>
<pin name="AN10/INT1/SDI1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/INT2/SCK1/!SS2!/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4"/>
<pin name="AN4/SDA2/U1RX/CN6/RB2"/>
<pin name="AN3/PGEC1/U2RX/CN5/RB1"/>
<pin name="AN2/PGED1/U2TX/SDI2/CN4/RB0"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VCAP" direction="pas"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO/PGEC3"/>
</symbol>
<symbol name="PIC24FVXXKA302">
<pin name="RA0/CN2/AN0"/>
<pin name="RA1/CN3/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/!SS1!/CN11/RB15"/>
<pin name="AN10/INT1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/INT2/!SS2!/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="AN15/SOSCI/!U2RTS!/CN1/RB4"/>
<pin name="AN4/SDA2/U1RX/CN6/RB2"/>
<pin name="AN3/PGEC1/U2RX/CN5/RB1"/>
<pin name="AN2/PGED1/U2TX/CN4/RB0"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCAP" direction="pas"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO"/>
<pin name="RA7/CN9/SDI2"/>
<pin name="AN5/SCL2/CN7/RB3"/>
<pin name="PGED3/ASDA1/SCK2/CN27/RB5"/>
<pin name="PGEC3/ASCL1/SDO2/CN24/RB6"/>
<pin name="PGED2/SDI1/CN16/RB10"/>
<pin name="PGEC2/SCK1/CN15/RB11"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="PIC24FVXXKA304">
<pin name="RA0/CN2/AN0"/>
<pin name="RA1/CN3/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/!SS1!/CN11/RB15"/>
<pin name="AN10/INT1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/INT2/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/CN22/RB8"/>
<pin name="INT0/CN23/RB7"/>
<pin name="SOSCI/AN15/!U2RTS!/CN1/RB4"/>
<pin name="AN4/SDA2/CN6/RB2"/>
<pin name="PGEC1/AN3/U2RX/CN5/RB1"/>
<pin name="PGED1/AN2/U2TX/CN4/RB0"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCAP" direction="pas"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO"/>
<pin name="RA7/CN9"/>
<pin name="AN5/SCL2/CN7/RB3"/>
<pin name="PGED3/ASDA1/CN27/RB5"/>
<pin name="PGEC3/ASCL1/CN24/RB6"/>
<pin name="PGED2/SDI1/CN16/RB10"/>
<pin name="PGEC2/SCK1/CN15/RB11"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RA8/CN33"/>
<pin name="RA9/CN34/!SS2!"/>
<pin name="RA10/CN35"/>
<pin name="RA11/CN36"/>
<pin name="AN6/CN32/RC0"/>
<pin name="AN7/CN31/RC1"/>
<pin name="AN8/CN10/RC2"/>
<pin name="SDI2/CN28/RC3"/>
<pin name="SDO2/CN25/RC4"/>
<pin name="SCK2/CN26/RC5"/>
<pin name="U1RX/CN18/RC6"/>
<pin name="U1TX/CN17/RC7"/>
<pin name="CN20/RC8"/>
<pin name="CN19/RC9"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
</symbol>
<symbol name="PIC24FXXKA301">
<pin name="RA0/CN2/SCK2/PGEC2/AN0"/>
<pin name="RA1/CN3/SDO2/PGED2/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/SCL2/!SS1!/CN11/RB15"/>
<pin name="AN10/INT1/SDI1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/SCK1/!SS2!/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4"/>
<pin name="AN4/SDA2/U1RX/CN6/RB2"/>
<pin name="AN3/PGEC1/U2RX/CN5/RB1"/>
<pin name="AN2/PGED1/U2TX/SDI2/CN4/RB0"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO/PGEC3"/>
</symbol>
<symbol name="PIC24FXXKA302">
<pin name="RA0/CN2/AN0"/>
<pin name="RA1/CN3/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/!SS1!/CN11/RB15"/>
<pin name="AN10/INT1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/!SS2!/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="AN15/SOSCI/!U2RTS!/CN1/RB4"/>
<pin name="AN4/SDA2/U1RX/CN6/RB2"/>
<pin name="AN3/PGEC1/U2RX/CN5/RB1"/>
<pin name="AN2/PGED1/U2TX/CN4/RB0"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO"/>
<pin name="RA7/CN9/SDI2"/>
<pin name="AN5/SCL2/CN7/RB3"/>
<pin name="PGED3/ASDA1/SCK2/CN27/RB5"/>
<pin name="PGEC3/ASCL1/SDO2/CN24/RB6"/>
<pin name="PGED2/SDI1/CN16/RB10"/>
<pin name="PGEC2/SCK1/CN15/RB11"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="PIC24FXXKA304">
<pin name="RA0/CN2/AN0"/>
<pin name="RA1/CN3/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/!SS1!/CN11/RB15"/>
<pin name="AN10/INT1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/CN22/RB8"/>
<pin name="INT0/CN23/RB7"/>
<pin name="SOSCI/AN15/!U2RTS!/CN1/RB4"/>
<pin name="AN4/SDA2/CN6/RB2"/>
<pin name="PGEC1/AN3/U2RX/CN5/RB1"/>
<pin name="PGED1/AN2/U2TX/CN4/RB0"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO"/>
<pin name="RA7/CN9"/>
<pin name="AN5/SCL2/CN7/RB3"/>
<pin name="PGED3/ASDA1/CN27/RB5"/>
<pin name="PGEC3/ASCL1/CN24/RB6"/>
<pin name="PGED2/SDI1/CN16/RB10"/>
<pin name="PGEC2/SCK1/CN15/RB11"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RA8/CN33"/>
<pin name="RA9/CN34/!SS2!"/>
<pin name="RA10/CN35"/>
<pin name="RA11/CN36"/>
<pin name="AN6/CN32/RC0"/>
<pin name="AN7/CN31/RC1"/>
<pin name="AN8/CN10/RC2"/>
<pin name="SDI2/CN28/RC3"/>
<pin name="SDO2/CN25/RC4"/>
<pin name="SCK2/CN26/RC5"/>
<pin name="U1RX/CN18/RC6"/>
<pin name="U1TX/CN17/RC7"/>
<pin name="CN20/RC8"/>
<pin name="CN19/RC9"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
</symbol>
<symbol name="PIC24FXXKL100">
<pin name="RA0/CN2/PGEC2"/>
<pin name="RA1/CN3/PGED2"/>
<pin name="RA2/CN30/OSCI"/>
<pin name="RA3/CN29/OSCO"/>
<pin name="RA5/!MCLR"/>
<pin name="INT0/!SS1!/U1RX/CN11/RB15"/>
<pin name="INT1/SDI1/U1TX/CN12/RB14"/>
<pin name="SDA1/SDO1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/SCK1/!U1CTS!/CN22/RB8"/>
<pin name="PGED3/SOSCI/CN1/RB4"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/SOSCO/PGEC3"/>
</symbol>
<symbol name="PIC24FXXKL101">
<pin name="RA0/CN2/PGEC2"/>
<pin name="RA1/CN3/PGED2"/>
<pin name="RA2/CN30/OSCI"/>
<pin name="RA3/CN29/OSCO"/>
<pin name="RA5/!MCLR"/>
<pin name="CN11/RB15"/>
<pin name="INT1/SDI1/CN12/RB14"/>
<pin name="SDO1/CN13/RB13"/>
<pin name="SCK1/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/!SS1!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="PGED3/SOSCI/CN1/RB4"/>
<pin name="U1RX/CN6/RB2"/>
<pin name="PGEC1/CN5/RB1"/>
<pin name="PGED1/CN4/RB0"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/SOSCO/PGEC3"/>
</symbol>
<symbol name="PIC24FXXKL200">
<pin name="RA0/CN2/PGEC2/AN0"/>
<pin name="RA1/CN3/PGED2/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/INT0/!SS1!/U1RX/CN11/RB15"/>
<pin name="AN10/INT1/SDI1/U1TX/CN12/RB14"/>
<pin name="SDA1/SDO1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/SCK1/!U1CTS!/CN22/RB8"/>
<pin name="AN15/PGED3/SOSCI/CN1/RB4"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/SOSCO/PGEC3"/>
</symbol>
<symbol name="PIC24FXXKL201">
<pin name="RA0/CN2/PGEC2/AN0"/>
<pin name="RA1/CN3/PGED2/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/CN11/RB15"/>
<pin name="AN10/INT1/SDI1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/SCK1/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/!SS1!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="AN15/PGED3/SOSCI/CN1/RB4"/>
<pin name="U1RX/CN6/RB2"/>
<pin name="PGEC1/CN5/RB1"/>
<pin name="PGED1/CN4/RB0"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/SOSCO/PGEC3"/>
</symbol>
<symbol name="PIC24FXXKL301">
<pin name="RA0/CN2/SDA2/SDI2/PGEC2"/>
<pin name="RA1/CN3/SDO2/PGED2"/>
<pin name="RA2/CN30/OSCI"/>
<pin name="RA3/CN29/OSCO"/>
<pin name="RA5/!MCLR"/>
<pin name="SCL2/SCK2/CN11/RB15"/>
<pin name="INT1/SDI1/CN12/RB14"/>
<pin name="SDO1/CN13/RB13"/>
<pin name="!SS2!/SCK1/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/!SS1!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="PGED3/SOSCI/!U2RTS!/CN1/RB4"/>
<pin name="U1RX/CN6/RB2"/>
<pin name="PGEC1/U2RX/CN5/RB1"/>
<pin name="PGED1/U2TX/CN4/RB0"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO/PGEC3"/>
</symbol>
<symbol name="PIC24FXXKL302">
<pin name="RA0/CN2/SDA2"/>
<pin name="RA1/CN3"/>
<pin name="RA2/CN30/OSCI"/>
<pin name="RA3/CN29/OSCO"/>
<pin name="RA5/!MCLR"/>
<pin name="!SS1!/CN11/RB15"/>
<pin name="INT1/CN12/RB14"/>
<pin name="SDO1/CN13/RB13"/>
<pin name="!SS2!/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="SOSCI/!U2RTS!/CN1/RB4"/>
<pin name="U1RX/CN6/RB2"/>
<pin name="PGEC1/U2RX/CN5/RB1"/>
<pin name="PGED1/U2TX/CN4/RB0"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO"/>
<pin name="RA7/CN9/SDI2"/>
<pin name="SCL2/CN7/RB3"/>
<pin name="PGED3/ASDA1/SCK2/CN27/RB5"/>
<pin name="PGEC3/ASCL1/SDO2/CN24/RB6"/>
<pin name="PGED2/SDI1/CN16/RB10"/>
<pin name="PGEC2/SCK1/CN15/RB11"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="PIC24FXXKL401">
<pin name="RA0/CN2/SDA2/SDI2/PGEC2/AN0"/>
<pin name="RA1/CN3/SDO2/PGED2/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/SCL2/SCK2/CN11/RB15"/>
<pin name="AN10/INT1/SDI1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/!SS2!/SCK1/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/!SS1!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4"/>
<pin name="U1RX/CN6/RB2"/>
<pin name="PGEC1/U2RX/CN5/RB1"/>
<pin name="PGED1/U2TX/CN4/RB0"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO/PGEC3"/>
</symbol>
<symbol name="PIC24FXXKL402">
<pin name="RA0/CN2/SDA2/AN0"/>
<pin name="RA1/CN3/AN1"/>
<pin name="RA2/CN30/OSCI/AN13"/>
<pin name="RA3/CN29/OSCO/AN14"/>
<pin name="RA5/!MCLR"/>
<pin name="AN9/!SS1!/CN11/RB15"/>
<pin name="AN10/INT1/CN12/RB14"/>
<pin name="AN11/SDO1/CN13/RB13"/>
<pin name="AN12/!SS2!/CN14/RB12"/>
<pin name="SDA1/!U1RTS!/CN21/RB9"/>
<pin name="SCL1/!U1CTS!/CN22/RB8"/>
<pin name="INT0/U1TX/CN23/RB7"/>
<pin name="AN15/SOSCI/!U2RTS!/CN1/RB4"/>
<pin name="U1RX/CN6/RB2"/>
<pin name="PGEC1/U2RX/CN5/RB1"/>
<pin name="PGED1/U2TX/CN4/RB0"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RA6/CN8/INT2"/>
<pin name="RA4/CN0/!U2CTS!/SOSCO"/>
<pin name="RA7/CN9/SDI2"/>
<pin name="SCL2/CN7/RB3"/>
<pin name="PGED3/ASDA1/SCK2/CN27/RB5"/>
<pin name="PGEC3/ASCL1/SDO2/CN24/RB6"/>
<pin name="PGED2/SDI1/CN16/RB10"/>
<pin name="PGEC2/SCK1/CN15/RB11"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="TC7129">
<pin name="OSC1" direction="in"/>
<pin name="OSC3" direction="out"/>
<pin name="ANNUN" direction="out"/>
<pin name="B1C1CONT" direction="out"/>
<pin name="A1G1D1" direction="out"/>
<pin name="F1E1DP1" direction="out"/>
<pin name="B2C2BAT" direction="out"/>
<pin name="A2G2D2" direction="out"/>
<pin name="F2E2DP2" direction="out"/>
<pin name="B3C3MINUS" direction="out"/>
<pin name="A3G3D3" direction="out"/>
<pin name="F3E3DP3" direction="out"/>
<pin name="B4C4BC5" direction="out"/>
<pin name="A4D4G4" direction="out"/>
<pin name="F4E4DP4" direction="out"/>
<pin name="BP3" direction="out"/>
<pin name="BP2" direction="out"/>
<pin name="BP1" direction="out"/>
<pin name="VDISP"/>
<pin name="DP4/OR"/>
<pin name="DP3/UR"/>
<pin name="LAT/HOLD"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="INTIN" direction="in"/>
<pin name="INTOUT" direction="out"/>
<pin name="CONTINU"/>
<pin name="COMMON"/>
<pin name="CREF+"/>
<pin name="CREF-"/>
<pin name="BUFFER" direction="out"/>
<pin name="INLO" direction="in"/>
<pin name="INHI" direction="in"/>
<pin name="REFHI"/>
<pin name="REFLO"/>
<pin name="DGND" direction="pwr"/>
<pin name="RANGE"/>
<pin name="DP2"/>
<pin name="DP1"/>
<pin name="OSC2" direction="out"/>
</symbol>
<symbol name="TC7660">
<pin name="1/NC" direction="nc"/>
<pin name="2/CAP+"/>
<pin name="3/GND" direction="pwr"/>
<pin name="4/CAP-"/>
<pin name="5/VOUT" direction="out"/>
<pin name="6/LO_V"/>
<pin name="7/OSC"/>
<pin name="8/V+" direction="pwr"/>
</symbol>
<symbol name="TC7126">
<pin name="V+" direction="pwr"/>
<pin name="D1" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="G1" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="C2" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="E2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="E3" direction="out"/>
<pin name="AB4" direction="out"/>
<pin name="POL(-SIG)" direction="out"/>
<pin name="BP" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="C3" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="V-" direction="pwr"/>
<pin name="VINT" direction="in"/>
<pin name="VBUFF" direction="in"/>
<pin name="CAZ"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="ANA_COMM"/>
<pin name="CREF-"/>
<pin name="CREF+"/>
<pin name="VREF-"/>
<pin name="VREF+"/>
<pin name="TEST"/>
<pin name="OSC3"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
</symbol>
<symbol name="MCP3302">
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="NC5" direction="in"/>
<pin name="NC6" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="CS/SH"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="CLK"/>
<pin name="AGND" direction="pwr"/>
<pin name="VREF"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MCP3304">
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="CS_SH"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="VREF" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PIC16F914">
<pin name="RE3/MCRL#/VPP" direction="in"/>
<pin name="RA0/AN0/C1-/SEG12"/>
<pin name="RA1/AN1/C2-/SEG7"/>
<pin name="RA2/AN2/C2+/VREF-/COM2"/>
<pin name="RA3/AN3/C1+/VREF+/SEG15"/>
<pin name="RA4/C1OUT/T0CKI/SEG4"/>
<pin name="RA5/AN4/C2OUT/SS#/SEG5"/>
<pin name="RD3/SEG16"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/INT/SEG0"/>
<pin name="RB1/SEG1"/>
<pin name="RB2/SEG2"/>
<pin name="RB3/SEG3"/>
<pin name="RB4/COM0"/>
<pin name="RB5/COM1"/>
<pin name="RB6/ICSPCLK/ICDCK/SEG14"/>
<pin name="RB7/ICSPDAT/ICDDAT/SEG13"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RE2/AN7/SEG23"/>
<pin name="RE1/AN6/SEG22"/>
<pin name="RE0/AN5/SEG21"/>
<pin name="RA6/OSC2/CLKO/T1OSO"/>
<pin name="RA7/OSC1/CLKI/T1OSI"/>
<pin name="RC0/VLCD1"/>
<pin name="RC1/VLCD2"/>
<pin name="RC2/VLCD3"/>
<pin name="RC3/SEG6"/>
<pin name="RD0/COM3"/>
<pin name="RD1"/>
<pin name="RD7/SEG20"/>
<pin name="RD6/SEG19"/>
<pin name="RD5/SEG18"/>
<pin name="RD4/SEG17"/>
<pin name="RC7/RX/DT/SDI/SDA/SEG8"/>
<pin name="RC6/TX/CK/SCK/SCL/SEG9"/>
<pin name="RC5/T1CKI/CCP1/SEG10"/>
<pin name="RC4/T1G#/SDO/SEG11"/>
<pin name="RD2/CCP2"/>
</symbol>
<symbol name="PIC16F914/917-I/ML">
<description>&lt;b&gt;I/ML</description>
<pin name="RE3/MCRL#/VPP" direction="in"/>
<pin name="RA0/AN0/C1-/SEG12"/>
<pin name="RA1/AN1/C2-/SEG7"/>
<pin name="RA2/AN2/C2+/VREF-/COM2"/>
<pin name="RA3/AN3/C1+/VREF+/SEG15"/>
<pin name="RA4/C1OUT/T0CKI/SEG4"/>
<pin name="RA5/AN4/C2OUT/SS#/SEG5"/>
<pin name="RD3/SEG16"/>
<pin name="VSS_30" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="RB0/INT/SEG0"/>
<pin name="RB1/SEG1"/>
<pin name="RB2/SEG2"/>
<pin name="RB3/SEG3"/>
<pin name="RB4/COM0"/>
<pin name="RB5/COM1"/>
<pin name="RB6/ICSPCLK/ICDCK/SEG14"/>
<pin name="RB7/ICSPDAT/ICDDAT/SEG13"/>
<pin name="VSS_6" direction="pwr"/>
<pin name="VDD_8" direction="pwr"/>
<pin name="RE2/AN7/SEG23"/>
<pin name="RE1/AN6/SEG22"/>
<pin name="RE0/AN5/SEG21"/>
<pin name="RA6/OSC2/CLKO/T1OSO"/>
<pin name="RA7/OSC1/CLKI/T1OSI"/>
<pin name="RC0/VLCD1"/>
<pin name="RC1/VLCD2"/>
<pin name="RC2/VLCD3"/>
<pin name="RC3/SEG6"/>
<pin name="RD0/COM3"/>
<pin name="RD1"/>
<pin name="RD7/SEG20"/>
<pin name="RD6/SEG19"/>
<pin name="RD5/SEG18"/>
<pin name="RD4/SEG17"/>
<pin name="RC7/RX/DT/SDI/SDA/SEG8"/>
<pin name="RC6/TX/CK/SCK/SCL/SEG9"/>
<pin name="RC5/T1CKI/CCP1/SEG10"/>
<pin name="RC4/T1G#/SDO/SEG11"/>
<pin name="RD2/CCP2"/>
<pin name="VSS_31" direction="pwr"/>
<pin name="VDD_28" direction="pwr"/>
</symbol>
<symbol name="PIC16F913/916">
<pin name="RE3/MCLR/VPP" direction="in"/>
<pin name="RA0/AN0/C1/SEG12"/>
<pin name="RA1/AN1/C2/SEG7"/>
<pin name="RA2/AN2/C2/VR/COM2"/>
<pin name="RA3/AN3/C1/VR/COM3/SEG15"/>
<pin name="RA4/CIOUT/T0CKI/SEG4"/>
<pin name="RA5/AN4/C2OUT/SS/SEG5"/>
<pin name="VSS" direction="pwr"/>
<pin name="RA7/OSC1/CLKI/T1OSI"/>
<pin name="RA6/OSC2/CLKKO/T1OSO"/>
<pin name="RC0/VLCD1"/>
<pin name="RC1/VLCD2"/>
<pin name="RC3/SEG6"/>
<pin name="RC2/VLCD3" direction="pwr"/>
<pin name="RC4/T1G/SDO/SEG11" direction="pwr"/>
<pin name="RC5/T1CKI/CCP1/SEG10" direction="pwr"/>
<pin name="RC6/TX/CK/SCK/SCL/SEG9" direction="pwr"/>
<pin name="RC7/RX/DT/SDI/SDA/SEG8/" direction="pwr"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/INT/SEG0"/>
<pin name="RB1/SEG1/"/>
<pin name="RB2/SEG2"/>
<pin name="RB3/SEG3"/>
<pin name="RB4/COM0"/>
<pin name="RB5/COM1"/>
<pin name="RB6/ICSPCLK/ICDCK/SEG14"/>
<pin name="RB7/ICSPDAT/ICDDAT/SEG13"/>
</symbol>
<symbol name="TC9400/01/02">
<pin name="1/IBIAS"/>
<pin name="2/ADJ" direction="in"/>
<pin name="3/I_IN" direction="in"/>
<pin name="4/VSS" direction="pwr"/>
<pin name="5/V_OUT" direction="out"/>
<pin name="6/GND" direction="pwr"/>
<pin name="7/VREF" direction="in"/>
<pin name="8/PULS" direction="out"/>
<pin name="9/COMM" direction="out"/>
<pin name="10/F2_OUT" direction="out"/>
<pin name="11/THRE" direction="in"/>
<pin name="12/AMP_UOT" direction="out"/>
<pin name="13/NC" direction="nc"/>
<pin name="14/VDD" direction="pwr"/>
</symbol>
<symbol name="TCN75">
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="INT/CM" direction="oc"/>
<pin name="GND" direction="pwr"/>
<pin name="A2" direction="pwr"/>
<pin name="A1" direction="pwr"/>
<pin name="A0" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PS501-0901">
<pin name="1/VDDD" direction="pwr"/>
<pin name="2/GPIO4"/>
<pin name="3/GPIO5"/>
<pin name="4/GPIO6"/>
<pin name="5/GPIO7"/>
<pin name="6/SMB-CLK"/>
<pin name="7/SMB-DTA"/>
<pin name="8/RSV1" direction="in"/>
<pin name="9/RSV2" direction="in"/>
<pin name="10/RSV3" direction="in"/>
<pin name="11/VC1" direction="in"/>
<pin name="12/VDDA" direction="pwr"/>
<pin name="13/VSSA" direction="pwr"/>
<pin name="14/RSHP" direction="in"/>
<pin name="15/RSHN" direction="in"/>
<pin name="16/VNTC" direction="in"/>
<pin name="17/VREFT" direction="out"/>
<pin name="18/ROSC" direction="in"/>
<pin name="19/GPIO8"/>
<pin name="20/GPIO9"/>
<pin name="21/GPIOHV1"/>
<pin name="22/MCLR" direction="in"/>
<pin name="23/HV2"/>
<pin name="24/GPIO0"/>
<pin name="25/GPIO1"/>
<pin name="26/GPIO2"/>
<pin name="27/GPIO3"/>
<pin name="28/VSSD" direction="pwr"/>
</symbol>
<symbol name="PS700">
<pin name="VC2/IO1" direction="in"/>
<pin name="VC1" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="ROSC"/>
<pin name="NTC/IO0"/>
<pin name="GND" direction="pwr"/>
<pin name="SR" direction="in"/>
</symbol>
<symbol name="MCP23S08">
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="RESET#" direction="in"/>
<pin name="CS#" direction="in"/>
<pin name="INT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="GP7"/>
<pin name="GP5"/>
<pin name="GP6"/>
<pin name="GP4"/>
<pin name="GP3"/>
<pin name="GP2"/>
<pin name="GP1"/>
<pin name="GP0"/>
</symbol>
<symbol name="MCP2551">
<pin name="TXD" direction="in"/>
<pin name="RXD" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CANH"/>
<pin name="CANL"/>
<pin name="RS" direction="in"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="MCP23008">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="RESET#" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="INT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="GP7"/>
<pin name="GP6"/>
<pin name="GP5"/>
<pin name="GP4"/>
<pin name="GP3"/>
<pin name="GP2"/>
<pin name="GP1"/>
<pin name="GP0"/>
</symbol>
<symbol name="PIC18F4455/4550">
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VR-/CVR"/>
<pin name="RA3/AN3/VR+"/>
<pin name="RA4/T0CKI/C1OUT/RCV"/>
<pin name="RA5/AN4/SS/HLVDIN/C2OUT"/>
<pin name="OSC2/CLKO/RA6"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RB0/AN12/INT0/FLT0/SDI/SDA"/>
<pin name="RB1/AN10/INT1/SCK/SCL"/>
<pin name="RB2/AN8/INT2/VMO"/>
<pin name="RB3/AN9/CCP2/VPO"/>
<pin name="RB4/KBI0/AN11/CSSPP"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="T13CKI/T1OSO/RC0"/>
<pin name="UOE/CCP2/T1OSI/RC1"/>
<pin name="CCP1/P1A/RC2"/>
<pin name="VM/D-/RC4"/>
<pin name="VP/D+/RC5"/>
<pin name="CK/TX/RC6"/>
<pin name="SDO/DT/RX/RC7"/>
<pin name="SPP0/RD0"/>
<pin name="SPP1/RD1"/>
<pin name="SPP2/RD2"/>
<pin name="SPP3/RD3"/>
<pin name="SPP4/RD4"/>
<pin name="P1B/SPP5/RD5"/>
<pin name="P1C/SPP6/RD6"/>
<pin name="P1D/SPP7/RD7"/>
<pin name="MCLR/VPP/RE3" direction="in"/>
<pin name="RE0/AN5/CK1SPP"/>
<pin name="RE1/AN6/CK2SPP"/>
<pin name="OESPP/AN7/RE2"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VUSB" direction="pwr"/>
</symbol>
<symbol name="RESETS23">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET#" direction="out"/>
</symbol>
<symbol name="DSPIC30F2011/3012">
<pin name="RB0/AN0/CN2/VR+"/>
<pin name="RB1/AN1/CN3/VR-"/>
<pin name="RB2/AN2/CN4/LVDIN/SS1"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/U1TX/SDO1/SCL/EMUD/PGD"/>
<pin name="RB5/AN5/CN7/U1RX/SDI1/SDA/EMUC/PGC"/>
<pin name="RB6/AN6/INT0/SCK1/OCFA"/>
<pin name="RB7/AN7/IC2/OC2/EMUD2"/>
<pin name="EMUD1/SOSCI/T2CK/U1ATX/CN1/RC13"/>
<pin name="EMUC1/SOSCO/T1CK/U1ARX/CN0/RC14"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="CLKI/OSC1"/>
<pin name="EMUC2/OC1/IC1/INT1/RD0"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F3011">
<pin name="RB0/AN0/CN2/EMUD3/VR+"/>
<pin name="RB1/AN1/CN3/EMUC3/VR-"/>
<pin name="RB2/AN2/CN4/SS1"/>
<pin name="RB3/AN3/CN5/INDX"/>
<pin name="RB4/AN4/CN6/IC7/QEA"/>
<pin name="RB5/AN5/CN7/IC8/QEB"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RC13/CN1/T2CK/U1ATX/SOSCI/EMUD1"/>
<pin name="RC14/CN0/T1CK/U1ARX/SOSCO/EMUC1"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RD0/INT1/IC1/OC1/EMUC2"/>
<pin name="RD1/INT2/IC2/OC2/EMUD2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="PWM1L/RE0"/>
<pin name="PWM1H/RE1"/>
<pin name="PWM2L/RE2"/>
<pin name="PWM2H/RE3"/>
<pin name="PWM3L/RE4"/>
<pin name="PWM3H/RE5"/>
<pin name="FLTA/INT0/RE8"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="PGC/EMUC/SDI1/SDA/U1RX/RF2"/>
<pin name="PGD/EMUD/SDO1/SCL/U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="SCK1/RF6"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F3014">
<pin name="RB0/AN0/CN2"/>
<pin name="RB1/AN1/CN3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/EMUC/PGC/OCFA"/>
<pin name="RB7/AN7/EMUD/PGD"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RA11/INT0"/>
<pin name="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="EMUC2/OC1/RD0"/>
<pin name="EMUD2/OC2/RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="INT1/IC1/RD8"/>
<pin name="INT2/IC2/RD9"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="U1RX/SDI1/SDA/RF2"/>
<pin name="EMUD3/U1TX/SDO1/SCL/RF3"/>
<pin name="U2RX/CN17/RF4"/>
<pin name="U2TX/CN18/RF5"/>
<pin name="EMUC3/SCK1/RF6"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="MCLR" direction="in"/>
</symbol>
<symbol name="DSPIC30F4011">
<pin name="RB0/AN0/CN2/EMUD3/VR+"/>
<pin name="RB1/AN1/CN3/EMUC3/VR-"/>
<pin name="RB2/AN2/CN4/SS1"/>
<pin name="RB3/AN3/CN5/INDX"/>
<pin name="RB4/AN4/CN6/IC7/QEA"/>
<pin name="RB5/AN5/CN7/IC8/QEB"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RC13/CN1/T2CK/U1ATX/SOSCI/EMUD1"/>
<pin name="RC14/CN0/T1CK/U1ARX/SOSCO/EMUC1"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RD0/INT1/IC1/OC1/EMUC2"/>
<pin name="RD1/INT2/IC2/OC2/EMUD2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="PWM1L/RE0"/>
<pin name="PWM1H/RE1"/>
<pin name="PWM2L/RE2"/>
<pin name="PWM2H/RE3"/>
<pin name="PWM3L/RE4"/>
<pin name="PWM3H/RE5"/>
<pin name="FLTA/INT0/RE8"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="PGC/EMUC/SDI1/SDA/U1RX/RF2"/>
<pin name="PGD/EMUD/SDO1/SCL/U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="SCK1/RF6"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F4013">
<pin name="RB0/AN0/CN2"/>
<pin name="RB1/AN1/CN3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/IC7"/>
<pin name="RB5/AN5/CN7/IC8"/>
<pin name="RB6/AN6/EMUC/PGC/OCFA"/>
<pin name="RB7/AN7/EMUD/PGD"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9/CSCK"/>
<pin name="RB10/AN10/CSDI"/>
<pin name="RB11/AN11/CSDO"/>
<pin name="RB12/AN12/COFS"/>
<pin name="RA11/INT0"/>
<pin name="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="EMUC2/OC1/RD0"/>
<pin name="EMUD2/OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="INT1/IC1/RD8"/>
<pin name="INT2/IC2/RD9"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="U1RX/SDI1/SDA/RF2"/>
<pin name="EMUD3/U1TX/SDO1/SCL/RF3"/>
<pin name="U2RX/CN17/RF4"/>
<pin name="U2TX/CN18/RF5"/>
<pin name="EMUC3/SCK1/RF6"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="MCLR" direction="in"/>
</symbol>
<symbol name="DSPIC30F5011">
<pin name="RB0/AN0/CN2/VR+"/>
<pin name="RB1/AN1/CN3/VR-"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/OCFA/EMUC/PGC"/>
<pin name="RB7/AN7/EMUD/PGD"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1/EMUC2"/>
<pin name="RD1/OC2/EMUD2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="CLKI/OSC1" direction="in"/>
<pin name="T2CK/RC1"/>
<pin name="T3CK/RC2"/>
<pin name="SOSCI/T4CK/EMUD1/CN1/RC13"/>
<pin name="SOSCO/T1CK/EMUC1/CN0/RC14"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="EMUD3/SDO1/U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="INT0/EMUC3/SCK1/RF6"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F5013">
<pin name="RA6/CN22"/>
<pin name="RA7/CN23"/>
<pin name="RA9/VR-"/>
<pin name="RA10/VR+"/>
<pin name="RA12/INT1"/>
<pin name="RA13/INT2"/>
<pin name="RA14/INT3"/>
<pin name="RA15/INT4"/>
<pin name="RB0/AN0/CN2/EMUD/PGD"/>
<pin name="RB1/AN1/CN3/EMUC/PGC"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RC1/T2CK"/>
<pin name="RC2/T3CK"/>
<pin name="RC3/T4CK"/>
<pin name="RC4/T5CK"/>
<pin name="RC13/CN1/EMUD1/SOSCI"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="EMUC2/OC1/RD0"/>
<pin name="EMUD2/OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="CN13/OC5/RD4"/>
<pin name="CN14/OC6/RD5"/>
<pin name="CN15/OC7/RD6"/>
<pin name="CN16/OC8/RD7"/>
<pin name="IC1/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/RD10"/>
<pin name="IC4/RD11"/>
<pin name="IC5/RD12"/>
<pin name="CN19/IC6/RD13"/>
<pin name="CN20/IC7/RD14"/>
<pin name="CN21/IC8/RD15"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="EMUC3/SCK1/INT0/RF6"/>
<pin name="SDI1/RF7"/>
<pin name="EMUD3/SDO1/RF8"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="MCLR/VPP" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F5015">
<pin name="RB0/AN0/CN2/VR+"/>
<pin name="RB1/AN1/CN3/VR-"/>
<pin name="RB2/AN2/CN4/SS1"/>
<pin name="RB3/AN3/CN5/INDX"/>
<pin name="RB4/AN4/CN6/QEA"/>
<pin name="RB5/AN5/CN7/QEB"/>
<pin name="RB6/AN6/EMUC/OCFA/PGC"/>
<pin name="RB7/AN7/EMUD/PGD"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12"/>
<pin name="RC13/CN1/EMUD1/SOSCI/T4CK"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="EMUC2/OC1/RD0"/>
<pin name="EMUD2/OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="IC5/CN13/RD4"/>
<pin name="IC6/CN14/RD5"/>
<pin name="CN15/RD6"/>
<pin name="UPDN/CN16/RD7"/>
<pin name="FLTA/IC1/INT1/RD8"/>
<pin name="FLTB/IC2/INT2/RD9"/>
<pin name="IC3/INT3/RD10"/>
<pin name="IC4/INT4/RD11"/>
<pin name="PWM1L/RE0"/>
<pin name="PWM1H/RE1"/>
<pin name="PWM2L/RE2"/>
<pin name="PWM2H/RE3"/>
<pin name="PWM3L/RE4"/>
<pin name="PWM3H/RE5"/>
<pin name="PWM4L/RE6"/>
<pin name="PWM4H/RE7"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="RF0/C1RX"/>
<pin name="RF1/C1TX"/>
<pin name="RF2/U1RX/SDI1"/>
<pin name="RF3/U1TX/SDO1/EMUD3"/>
<pin name="RF4/CN17"/>
<pin name="RF5/CN18"/>
<pin name="RF6/INT0/SCK1/EMUC3"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="SCK2/CN8/RG6"/>
<pin name="SDI2/CN9/RG7"/>
<pin name="SDO2/CN10/RG8"/>
<pin name="SS2/CN11/RG9"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F5016">
<pin name="RE0/PWM1L"/>
<pin name="RE1/PWM1H"/>
<pin name="RA9/VR-"/>
<pin name="RA10/VR+"/>
<pin name="RE8/INT1/FLTA"/>
<pin name="RE9/INT2/FLTB"/>
<pin name="RA14/INT3"/>
<pin name="RA15/INT4"/>
<pin name="RB0/AN0/CN2/EMUD/PGD"/>
<pin name="RB1/AN1/CN3/EMUC/PGC"/>
<pin name="RB2/AN2/CN4/SS1"/>
<pin name="RB3/AN3/CN5/INDX"/>
<pin name="RB4/AN4/CN6/QEA"/>
<pin name="RB5/AN5/CN7/QEB"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12"/>
<pin name="RC1/T2CK"/>
<pin name="RE7/PWM4H"/>
<pin name="RC3/T4CK"/>
<pin name="RE6/PWM4L"/>
<pin name="RC13/CN1/EMUD1/SOSCI"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="EMUC2/OC1/RD0"/>
<pin name="EMUD2/OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="CN13/RD4"/>
<pin name="CN14/RD5"/>
<pin name="CN15/RD6"/>
<pin name="UPDN/CN16/RD7"/>
<pin name="IC1/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/RD10"/>
<pin name="IC4/RD11"/>
<pin name="RD12"/>
<pin name="CN19/RD13"/>
<pin name="CN20/RD14"/>
<pin name="CN21/RD15"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF3"/>
<pin name="CN17/RF4"/>
<pin name="CN18/RF5"/>
<pin name="EMUC3/SCK1/INT0/RF6"/>
<pin name="SDI1/RF7"/>
<pin name="EMUD3/SDO1/RF8"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="RE3/PWM2H"/>
<pin name="RE4/PWM3L"/>
<pin name="RE2/PWM2L"/>
<pin name="RE5/PWM3H"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F6010">
<pin name="RE0/PWM1L"/>
<pin name="RE1/PWM1H"/>
<pin name="RA9/VR-"/>
<pin name="RA10/VR+"/>
<pin name="RE8/INT1/FLTA"/>
<pin name="RE9/INT2/FLTB"/>
<pin name="RA14/INT3"/>
<pin name="RA15/INT4"/>
<pin name="RB0/AN0/CN2/EMUD/PGD"/>
<pin name="RB1/AN1/CN3/EMUC/PGC"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5/INDX"/>
<pin name="RB4/AN4/CN6/QEA"/>
<pin name="RB5/AN5/CN7/QEB"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RC1/T2CK"/>
<pin name="RE7/PWM4H"/>
<pin name="RC3/T4CK"/>
<pin name="RE6/PWM4L"/>
<pin name="RC13/CN1/EMUD1/SOSCI"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="EMUC2/OC1/RD0"/>
<pin name="EMUD2/OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="CN13/OC5/RD4"/>
<pin name="CN14/OC6/RD5"/>
<pin name="CN15/OC7/RD6"/>
<pin name="UPDN/CN16/OC8/RD7"/>
<pin name="IC1/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/RD10"/>
<pin name="IC4/RD11"/>
<pin name="IC5/RD12"/>
<pin name="CN19/IC6/RD13"/>
<pin name="CN20/IC7/RD14"/>
<pin name="CN21/IC8/RD15"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="EMUC3/SCK1/INT0/RF6"/>
<pin name="SDI1/RF7"/>
<pin name="EMUD3/SDO1/RF8"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="RE3/PWM2H"/>
<pin name="RE4/PWM3L"/>
<pin name="RE2/PWM2L"/>
<pin name="RE5/PWM3H"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F6011">
<pin name="RB0/AN0/CN2/EMUD/PGD"/>
<pin name="RB1/AN1/CN3/EMUC/PGC"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1/EMUC2"/>
<pin name="RD1/OC2/EMUD2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="CLKI/OSC1" direction="in"/>
<pin name="T2CK/RC1"/>
<pin name="T3CK/RC2"/>
<pin name="SOSCI/T4CK/EMUD1/CN1/RC13"/>
<pin name="SOSCO/T1CK/EMUC1/CN0/RC14"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="EMUD3/SDO1/U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="INT0/EMUC3/SCK1/RF6"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RG14"/>
<pin name="RG15"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F6012">
<pin name="RB0/AN0/CN2/EMUD/PGD"/>
<pin name="RB1/AN1/CN3/EMUC/PGC"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1/EMUC2"/>
<pin name="RD1/OC2/EMUD2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="CLKI/OSC1" direction="in"/>
<pin name="T2CK/RC1"/>
<pin name="T3CK/RC2"/>
<pin name="SOSCI/T4CK/EMUD1/CN1/RC13"/>
<pin name="SOSCO/T1CK/EMUC1/CN0/RC14"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="EMUD3/SDO1/U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="INT0/EMUC3/SCK1/RF6"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F6013">
<pin name="RA6/CN22"/>
<pin name="RA7/CN23"/>
<pin name="RA9/VR-"/>
<pin name="RA10/VR+"/>
<pin name="RA12/INT1"/>
<pin name="RA13/INT2"/>
<pin name="RA14/INT3"/>
<pin name="RA15/INT4"/>
<pin name="RB0/AN0/CN2/EMUD/PGD"/>
<pin name="RB1/AN1/CN3/EMUC/PGC"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RC1/T2CK"/>
<pin name="RC2/T3CK"/>
<pin name="RC3/T4CK"/>
<pin name="RC4/T5CK"/>
<pin name="RC13/CN1/EMUD1/SOSCI"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="EMUC2/OC1/RD0"/>
<pin name="EMUD2/OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="CN13/OC5/RD4"/>
<pin name="CN14/OC6/RD5"/>
<pin name="CN15/OC7/RD6"/>
<pin name="CN16/OC8/RD7"/>
<pin name="IC1/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/RD10"/>
<pin name="IC4/RD11"/>
<pin name="IC5/RD12"/>
<pin name="CN19/IC6/RD13"/>
<pin name="CN20/IC7/RD14"/>
<pin name="CN21/IC8/RD15"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="EMUC3/SCK1/INT0/RF6"/>
<pin name="SDI1/RF7"/>
<pin name="EMUD3/SDO1/RF8"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RG14"/>
<pin name="RG15"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="MCLR/VPP" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F6014">
<pin name="RA6/CN22"/>
<pin name="RA7/CN23"/>
<pin name="RA9/VR-"/>
<pin name="RA10/VR+"/>
<pin name="RA12/INT1"/>
<pin name="RA13/INT2"/>
<pin name="RA14/INT3"/>
<pin name="RA15/INT4"/>
<pin name="RB0/AN0/CN2/EMUD/PGD"/>
<pin name="RB1/AN1/CN3/EMUC/PGC"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RB14/AN14"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RC1/T2CK"/>
<pin name="RC2/T3CK"/>
<pin name="RC3/T4CK"/>
<pin name="RC4/T5CK"/>
<pin name="RC13/CN1/EMUD1/SOSCI"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="EMUC2/OC1/RD0"/>
<pin name="EMUD2/OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="CN13/OC5/RD4"/>
<pin name="CN14/OC6/RD5"/>
<pin name="CN15/OC7/RD6"/>
<pin name="CN16/OC8/RD7"/>
<pin name="IC1/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/RD10"/>
<pin name="IC4/RD11"/>
<pin name="IC5/RD12"/>
<pin name="CN19/IC6/RD13"/>
<pin name="CN20/IC7/RD14"/>
<pin name="CN21/IC8/RD15"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="EMUC3/SCK1/INT0/RF6"/>
<pin name="SDI1/RF7"/>
<pin name="EMUD3/SDO1/RF8"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL/RG2"/>
<pin name="SDA/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="MCLR/VPP" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC33FJ12GP201">
<pin name="RA0/CN2/AN0/VREF+/EMUD2/PGD2"/>
<pin name="RA1/CN3/AN1/VREF-/EMUC2/PGC2"/>
<pin name="RA2/OSCI/CLKI/CN30"/>
<pin name="RA3/OSCO/CLKO/CN29"/>
<pin name="RA4/CN0/T1CK/SOSCO/EMUC3/PGC3"/>
<pin name="PGD1/EMUD1/RP0/AN2/CN4/RB0"/>
<pin name="PGC1/EMUC1/RP1/AN3/CN5/RB1"/>
<pin name="RB4/CN1/RP4/SOSCI/EMUD3/PGD3"/>
<pin name="INT0/RP7/CN23/RB7"/>
<pin name="SDA1/RP8/CN22/RB8"/>
<pin name="SCL1/RP9/CN21/RB9"/>
<pin name="RP14/AN7/CN12/RB14"/>
<pin name="RP15/AN6/CN11/RB15"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="MCLR#" direction="in"/>
</symbol>
<symbol name="DSPIC33FJXXGP206">
<pin name="RB0/AN0/CN2/VR+/PGD3/EMUD3"/>
<pin name="RB1/AN1/CN3/VR-/PGC3/EMUC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/IC7"/>
<pin name="RB5/AN5/CN7/IC8"/>
<pin name="RB6/AN6/OCFA/EMUC1/PGC1"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10/TMS"/>
<pin name="RB11/AN11/TDO"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2/U1CTS"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="AN16/T2CK/T7CK/RC1"/>
<pin name="AN17/T3CK/T6CK/RC2"/>
<pin name="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13"/>
<pin name="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="INT0/U1RTS/SCK1/RF6"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="T5CK/CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="DSPIC33FJXXGP306">
<pin name="RB0/AN0/CN2/VR+/PGD3/EMUD3"/>
<pin name="RB1/AN1/CN3/VR-/PGC3/EMUC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/IC7"/>
<pin name="RB5/AN5/CN7/IC8"/>
<pin name="RB6/AN6/OCFA/EMUC1/PGC1"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10/TMS"/>
<pin name="RB11/AN11/TDO"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2/U1CTS"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="AN16/T2CK/T7CK/RC1"/>
<pin name="AN17/T3CK/T6CK/RC2"/>
<pin name="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13"/>
<pin name="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="SDA2/CN17/U2RX/RF4"/>
<pin name="SCL2/CN18/U2TX/RF5"/>
<pin name="INT0/U1RTS/SCK1/RF6"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="T5CK/CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="DSPIC33FJXXGP706">
<pin name="RB0/AN0/CN2/VR+/PGD3/EMUD3"/>
<pin name="RB1/AN1/CN3/VR-/PGC3/EMUC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/IC7"/>
<pin name="RB5/AN5/CN7/IC8"/>
<pin name="RB6/AN6/OCFA/EMUC1/PGC1"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10/TMS"/>
<pin name="RB11/AN11/TDO"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2/U1CTS"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="AN16/T2CK/T7CK/RC1"/>
<pin name="AN17/T3CK/T6CK/RC2"/>
<pin name="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13"/>
<pin name="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="SDA2/CN17/U2RX/RF4"/>
<pin name="SCL2/CN18/U2TX/RF5"/>
<pin name="INT0/U1RTS/SCK1/RF6"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="T5CK/CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="DSPIC33FJXXGP708">
<pin name="RA6/AN22/CN22"/>
<pin name="RA7/AN23/CN23"/>
<pin name="RA9/VR-"/>
<pin name="RA10/VR+"/>
<pin name="RE8/AN20/INT1/TMS"/>
<pin name="RE9/AN21/INT2/TDO"/>
<pin name="RA14/INT3/SCL2"/>
<pin name="RA15/INT4/SDA2"/>
<pin name="RB0/AN0/CN2/EMUD3/PGD3"/>
<pin name="RB1/AN1/CN3/EMUC3/PGC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/EMUC1/PGC1/OCFA"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RC1/AN16/T2CK/T7CK"/>
<pin name="RC2/AN17/T3CK/T6CK"/>
<pin name="RC3/AN18/T4CK/T9CK"/>
<pin name="RC4/AN19/T5CK/T8CK"/>
<pin name="RC13/CN1/EMUD2/SOSCI"/>
<pin name="RC14/CN0/EMUC2/SOSCO/T1CK"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OC1/RD0"/>
<pin name="OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="CN13/OC5/RD4"/>
<pin name="CN14/OC6/RD5"/>
<pin name="CN15/OC7/RD6"/>
<pin name="CN16/OC8/RD7"/>
<pin name="IC1/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/RD10"/>
<pin name="IC4/RD11"/>
<pin name="IC5/RD12"/>
<pin name="CN19/IC6/RD13"/>
<pin name="U1CTS/CN20/IC7/RD14"/>
<pin name="U1RTS/CN21/IC8/RD15"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="SCK1/INT0/RF6"/>
<pin name="SDI1/RF7"/>
<pin name="SDO1/RF8"/>
<pin name="C2RX/RG0"/>
<pin name="C2TX/RG1"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="OSC1/CLKI/RC12"/>
<pin name="MCLR" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC33FJXXMC506">
<pin name="RB0/AN0/CN2/VR+/PGD3/EMUD3"/>
<pin name="RB1/AN1/CN3/VR-/PGC3/EMUC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5/INDX"/>
<pin name="RB4/AN4/CN6/QEA/IC7"/>
<pin name="RB5/AN5/CN7/QEB/IC8"/>
<pin name="RB6/AN6/OCFA/EMUC1/PGC1"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10/TMS"/>
<pin name="RB11/AN11/TDO"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16/UPDN"/>
<pin name="RD8/IC1/INT1/FLTA"/>
<pin name="RD9/IC2/INT2/FLTB/U1CTS"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="PWM4L/RE6"/>
<pin name="PWM4H/RE7"/>
<pin name="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13"/>
<pin name="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="INT0/U1RTS/SCK1/RF6"/>
<pin name="PWM1H/RE1"/>
<pin name="PWM1L/RE0"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="T5CK/CN11/SS2/RG9"/>
<pin name="PWM2H/RE3"/>
<pin name="PWM3L/RE4"/>
<pin name="PWM2L/RE2"/>
<pin name="PWM3H/RE5"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="DSPIC33FJXXMC708">
<pin name="PWM1L/RE0"/>
<pin name="PWM1H/RE1"/>
<pin name="RA9/VR-"/>
<pin name="RA10/VR+"/>
<pin name="TMS/FLTA/INT1/RE8"/>
<pin name="TDO/FLTB/INT2/RE9"/>
<pin name="RA14/INT3/SCL2"/>
<pin name="RA15/INT4/SDA2"/>
<pin name="RB0/AN0/CN2/EMUD3/PGD3"/>
<pin name="RB1/AN1/CN3/EMUC3/PGC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5/INDX"/>
<pin name="RB4/AN4/CN6/QEA"/>
<pin name="RB5/AN5/CN7/QEB"/>
<pin name="RB6/AN6/EMUC1/PGC1/OCFA"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RC1/AN16/T2CK/T7CK"/>
<pin name="RC2/AN17/T3CK/T6CK"/>
<pin name="PWM4L/RE6"/>
<pin name="PWM4H/RE7"/>
<pin name="RC13/CN1/EMUD2/SOSCI"/>
<pin name="RC14/CN0/EMUC2/SOSCO/T1CK"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OC1/RD0"/>
<pin name="OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="CN13/OC5/RD4"/>
<pin name="CN14/OC6/RD5"/>
<pin name="CN15/OC7/RD6"/>
<pin name="UPDN/CN16/OC8/RD7"/>
<pin name="IC1/RD8"/>
<pin name="IC2/RD9"/>
<pin name="IC3/RD10"/>
<pin name="IC4/RD11"/>
<pin name="IC5/RD12"/>
<pin name="CN19/IC6/RD13"/>
<pin name="U1CTS/CN20/IC7/RD14"/>
<pin name="U1RTS/CN21/IC8/RD15"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="SCK1/INT0/RF6"/>
<pin name="SDI1/RF7"/>
<pin name="SDO1/RF8"/>
<pin name="RG0/C2RX"/>
<pin name="RG1/C2TX"/>
<pin name="RG2/SCL1"/>
<pin name="RG3/SDA1"/>
<pin name="RG6/CN8/SCK2"/>
<pin name="RG7/CN9/SDI2"/>
<pin name="RG8/CN10/SDO2"/>
<pin name="RG9/CN11/SS2"/>
<pin name="PWM2H/RE3"/>
<pin name="PWM3L/RE4"/>
<pin name="PWM2L/RE2"/>
<pin name="PWM3H/RE5"/>
<pin name="OSC1/CLKI/RC12"/>
<pin name="MCLR" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC33FJXXGP506">
<pin name="RB0/AN0/CN2/VR+/PGD3/EMUD3"/>
<pin name="RB1/AN1/CN3/VR-/PGC3/EMUC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/IC7"/>
<pin name="RB5/AN5/CN7/IC8"/>
<pin name="RB6/AN6/OCFA/EMUC1/PGC1"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10/TMS"/>
<pin name="RB11/AN11/TDO"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2/U1CTS"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="AN16/T2CK/T7CK/RC1"/>
<pin name="AN17/T3CK/T6CK/RC2"/>
<pin name="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13"/>
<pin name="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="SDA2/CN17/U2RX/RF4"/>
<pin name="SCL2/CN18/U2TX/RF5"/>
<pin name="INT0/U1RTS/SCK1/RF6"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="T5CK/CN11/SS2/RG9"/>
<pin name="CSDI/RG12"/>
<pin name="CSDO/RG13"/>
<pin name="CSCK/RG14"/>
<pin name="COFS/RG15"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F2010">
<pin name="RB0/CN2/AN0/EMUD3/VR+"/>
<pin name="RB1/CN3/AN1/EMUC3/VR-"/>
<pin name="RB2/CN4/AN2/SS1"/>
<pin name="RB3/CN5/AN3/INDX"/>
<pin name="RB4/CN6/AN4/QEA/IC7"/>
<pin name="RB5/CN7/AN5/QEB/IC8"/>
<pin name="RC13/CN1/EMUD1/ATX/T2C"/>
<pin name="RC14/CN0/EMUC1/ARX/T1C"/>
<pin name="RC15/OSC2/CLKO"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RD0/INT1/EMUC2/OC1/IC1"/>
<pin name="INT2/EMUD2/OC2/IC2/RD1"/>
<pin name="PWM1L/RE0"/>
<pin name="PWM1H/RE1"/>
<pin name="PWM2L/RE2"/>
<pin name="PWM2H/RE3"/>
<pin name="PWM3L/RE4"/>
<pin name="PWM3H/RE5"/>
<pin name="INT0/FLTA/SCK1/OCFA/RE8"/>
<pin name="PGC/EMUC/RX/SDI1/SDA/RF2"/>
<pin name="PGD/EMUD/TX/SDO1/SCL/RF3"/>
<pin name="VPP/MCLR" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F2012">
<pin name="RB0/AN0/CN2/EMUD3/VR+"/>
<pin name="RB1/AN1/CN3/EMUC3/VR-"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7/EMUD2"/>
<pin name="RB8/AN8/OC1"/>
<pin name="RB9/AN9/OC2"/>
<pin name="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="EMUC2/IC1/INT1/RD8"/>
<pin name="IC2/INT2/RD9"/>
<pin name="PGC/EMUC/U1RX/SDI1/SDA/RF2"/>
<pin name="PGD/EMUD/U1TX/SDO1/SCL/RF3"/>
<pin name="CN17/RF4"/>
<pin name="CN18/RF5"/>
<pin name="SCK1/INT0/RF6"/>
<pin name="MCLR/VPP" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="DSPIC30F3013">
<pin name="RB0/AN0/CN2/EMUD3/VR+"/>
<pin name="RB1/AN1/CN3/EMUC3/VR-"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6"/>
<pin name="RB5/AN5/CN7"/>
<pin name="RB6/AN6/OCFA"/>
<pin name="RB7/AN7/EMUD2"/>
<pin name="RB8/AN8/OC1"/>
<pin name="RB9/AN9/OC2"/>
<pin name="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX"/>
<pin name="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="EMUC2/IC1/INT1/RD8"/>
<pin name="IC2/INT2/RD9"/>
<pin name="PGC/EMUC/U1RX/SDI1/SDA/RF2"/>
<pin name="PGD/EMUD/U1TX/SDO1/SCL/RF3"/>
<pin name="U2RX/CN17/RF4"/>
<pin name="U2TX/CN18/RF5"/>
<pin name="SCK1/INT0/RF6"/>
<pin name="MCLR/VPP" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="MCP1252/3">
<pin name="PGOOD" direction="oc"/>
<pin name="VOUT" direction="sup"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="C-" direction="pas"/>
<pin name="C+" direction="pas"/>
<pin name="SHDN#" direction="in"/>
<pin name="SELECT" direction="in"/>
</symbol>
<symbol name="MCP1252/3-ADJ">
<pin name="PGOOD" direction="oc"/>
<pin name="VOUT" direction="sup"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="C-" direction="pas"/>
<pin name="C+" direction="pas"/>
<pin name="SHDN#" direction="in"/>
<pin name="FB" direction="in"/>
</symbol>
<symbol name="MCP23016">
<pin name="GP1.0"/>
<pin name="GP1.1"/>
<pin name="GP1.2"/>
<pin name="GP1.3"/>
<pin name="GP1.4"/>
<pin name="GP1.5"/>
<pin name="GP1.6"/>
<pin name="GP1.7"/>
<pin name="GP0.0"/>
<pin name="GP0.1"/>
<pin name="GP0.2"/>
<pin name="GP0.3"/>
<pin name="GP0.4"/>
<pin name="GP0.5"/>
<pin name="GP0.6"/>
<pin name="GP0.7"/>
<pin name="CLK" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="TP" direction="out"/>
<pin name="INT#" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PIC18F2445/2550">
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VR-/CVREF"/>
<pin name="RA3/AN3/VR+"/>
<pin name="RA4/T0CKI/C1OUT/RCV"/>
<pin name="RA5/AN4/SS/HLVDIN/C2OUT"/>
<pin name="RA6/CLKO/OSC2"/>
<pin name="CLKIN/OSC1" direction="in"/>
<pin name="RB0/SDA/SDI/AN12/INT0/FLT0"/>
<pin name="RB1/SCL/SCK/AN10/INT1"/>
<pin name="RB2/AN8/INT2/VMO"/>
<pin name="RB3/AN9/CCP2/VPO"/>
<pin name="RB4/AN11/KBI0"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="T13CKI/T1OSO/RC0"/>
<pin name="UOE/CCP2/T1OSI/RC1"/>
<pin name="CCP1/RC2"/>
<pin name="VM/D-/RC4"/>
<pin name="VP/D+/RC5"/>
<pin name="CK/TX/RC6"/>
<pin name="SDO/DT/RX/RC7"/>
<pin name="RE3/VPP/MCLR"/>
<pin name="VDD" direction="pwr"/>
<pin name="VUSB" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="PIC18F6680">
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VR-"/>
<pin name="RA3/AN3/VR+"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4/LVDIN"/>
<pin name="RB0/INT0"/>
<pin name="RB1/INT1"/>
<pin name="RB2/INT2"/>
<pin name="RB3/INT3"/>
<pin name="RB4/KBI0"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="RC0/T1O/T13C"/>
<pin name="RC1/T1I/CCP2"/>
<pin name="RC2/CCP1/P1A"/>
<pin name="RC3/SCK/SCL"/>
<pin name="RC4/SDI/SDA"/>
<pin name="RC5/SDO"/>
<pin name="RC6/TX/CK"/>
<pin name="RC7/RX/DT"/>
<pin name="PSP0/RD0"/>
<pin name="PSP1/RD1"/>
<pin name="PSP2/RD2"/>
<pin name="PSP3/RD3"/>
<pin name="PSP4/RD4"/>
<pin name="PSP5/RD5"/>
<pin name="PSP6/RD6"/>
<pin name="PSP7/RD7"/>
<pin name="RD/RE0"/>
<pin name="WR/RE1"/>
<pin name="CS/RE2"/>
<pin name="RE3"/>
<pin name="RE4"/>
<pin name="P1C/RE5"/>
<pin name="P1B/RE6"/>
<pin name="CCP2/RE7"/>
<pin name="AN5/RF0"/>
<pin name="AN6/C2O/RF1"/>
<pin name="AN7/C1O/RF2"/>
<pin name="AN8/C2I+/RF3"/>
<pin name="AN9/C2I-/RF4"/>
<pin name="AN10/C1I+/CVR/RF5"/>
<pin name="AN11/C1I-/RF6"/>
<pin name="SS/RF7"/>
<pin name="RG0/CANTX1"/>
<pin name="RG1/CANTX2"/>
<pin name="RG2/CANRX"/>
<pin name="RG3"/>
<pin name="RG4/P1D"/>
<pin name="RG5/MCLR/VPP"/>
<pin name="CLKI/OSC1" direction="in"/>
<pin name="CLKO/RA6/OSC2" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="PIC18F8490">
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VR-/S16"/>
<pin name="RA3/AN3/VR+/S17"/>
<pin name="RA4/T0CKI/S14"/>
<pin name="RA5/AN4/HLVDIN/S15"/>
<pin name="OSC2/CLKO/RA6"/>
<pin name="OSC1/CLKI/RA7"/>
<pin name="RB0/INT0"/>
<pin name="RB1/INT1/S8"/>
<pin name="RB2/INT2/S9"/>
<pin name="RB3/INT3/S10"/>
<pin name="RB4/KBI0/S11"/>
<pin name="RB5/KBI1"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/KBI3/PGD"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC1/T1OSI/CCP2"/>
<pin name="RC2/CCP1/S13"/>
<pin name="RC3/SCK/SCL"/>
<pin name="RC4/SDI/SDA"/>
<pin name="RC5/SDO/S12"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RD0/S0"/>
<pin name="RD1/S1"/>
<pin name="RD2/S2"/>
<pin name="RD3/S3"/>
<pin name="RD4/S4"/>
<pin name="RD5/S5"/>
<pin name="RD6/S6"/>
<pin name="RD7/S7"/>
<pin name="MCLR/VPP/RG5" direction="in"/>
<pin name="LCDBIAS1" direction="in"/>
<pin name="LCDBIAS2" direction="in"/>
<pin name="LCDBIAS3" direction="in"/>
<pin name="COM0" direction="out"/>
<pin name="COM1/RE4"/>
<pin name="COM2/RE5"/>
<pin name="COM3/RE6"/>
<pin name="S31/CCP2/RE7"/>
<pin name="S18/AN5/RF0"/>
<pin name="C2OUT/S19/AN6/RF1"/>
<pin name="C1OUT/S20/AN7/RF2"/>
<pin name="S21/AN8/RF3"/>
<pin name="S22/AN9/RF4"/>
<pin name="CVREF/S23/AN10/RF5"/>
<pin name="S24/AN11/RF6"/>
<pin name="S25/SS/RF7"/>
<pin name="S30/RG0"/>
<pin name="CK2/TX2/S29/RG1"/>
<pin name="DT2/RX2/S28/RG2"/>
<pin name="S27/RG3"/>
<pin name="S26/RG4"/>
<pin name="S47/RH0"/>
<pin name="S46/RH1"/>
<pin name="S45/RH2"/>
<pin name="S44/RH3"/>
<pin name="S40/RH4"/>
<pin name="S41/RH5"/>
<pin name="S42/RH6"/>
<pin name="S43/RH7"/>
<pin name="S32/RJ0"/>
<pin name="S33/RJ1"/>
<pin name="S34/RJ2"/>
<pin name="S35/RJ3"/>
<pin name="S39/RJ4"/>
<pin name="S38/RJ5"/>
<pin name="S37/RJ6"/>
<pin name="S36/RJ7"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="PIC24XJXXXGP206">
<pin name="RB0/AN0/CN2/VR+/PGD3/EMUD3"/>
<pin name="RB1/AN1/CN3/VR-/PGC3/EMUC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/IC7"/>
<pin name="RB5/AN5/CN7/IC8"/>
<pin name="RB6/AN6/OCFA/EMUC1/PGC1"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10/TMS"/>
<pin name="RB11/AN11/TDO"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2/U1CTS"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="AN16/T2CK/T7CK/RC1"/>
<pin name="AN17/T3CK/T6CK/RC2"/>
<pin name="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13"/>
<pin name="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="CN17/U2RX/RF4"/>
<pin name="CN18/U2TX/RF5"/>
<pin name="INT0/U1RTS/SCK1/RF6"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="T5CK/CN11/SS2/RG9"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RG14"/>
<pin name="RG15"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="PIC24XJXXXGP306">
<pin name="RB0/AN0/CN2/VR+/PGD3/EMUD3"/>
<pin name="RB1/AN1/CN3/VR-/PGC3/EMUC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/IC7"/>
<pin name="RB5/AN5/CN7/IC8"/>
<pin name="RB6/AN6/OCFA/EMUC1/PGC1"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10/TMS"/>
<pin name="RB11/AN11/TDO"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2/U1CTS"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="AN16/T2CK/T7CK/RC1"/>
<pin name="AN17/T3CK/T6CK/RC2"/>
<pin name="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13"/>
<pin name="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="SDA2/CN17/U2RX/RF4"/>
<pin name="SCL2/CN18/U2TX/RF5"/>
<pin name="INT0/U1RTS/SCK1/RF6"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="T5CK/CN11/SS2/RG9"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RG14"/>
<pin name="RG15"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="PIC24XJXXXGP506">
<pin name="RB0/AN0/CN2/VR+/PGD3/EMUD3"/>
<pin name="RB1/AN1/CN3/VR-/PGC3/EMUC3"/>
<pin name="RB2/AN2/CN4/SS1/LVDIN"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/IC7"/>
<pin name="RB5/AN5/CN7/IC8"/>
<pin name="RB6/AN6/OCFA/EMUC1/PGC1"/>
<pin name="RB7/AN7/EMUD1/PGD1"/>
<pin name="RB8/AN8/U2CTS"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10/TMS"/>
<pin name="RB11/AN11/TDO"/>
<pin name="RB12/AN12/TCK"/>
<pin name="RB13/AN13/TDI"/>
<pin name="RB14/AN14/U2RTS"/>
<pin name="RB15/AN15/CN12/OCFB"/>
<pin name="RD0/OC1"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5/IC5/CN13"/>
<pin name="RD5/OC6/IC6/CN14"/>
<pin name="RD6/OC7/CN15"/>
<pin name="RD7/OC8/CN16"/>
<pin name="RD8/IC1/INT1"/>
<pin name="RD9/IC2/INT2/U1CTS"/>
<pin name="RD10/IC3/INT3"/>
<pin name="RD11/IC4/INT4"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="AN16/T2CK/T7CK/RC1"/>
<pin name="AN17/T3CK/T6CK/RC2"/>
<pin name="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13"/>
<pin name="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14"/>
<pin name="C1RX/RF0"/>
<pin name="C1TX/RF1"/>
<pin name="SDI1/U1RX/RF2"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="SDA2/CN17/U2RX/RF4"/>
<pin name="SCL2/CN18/U2TX/RF5"/>
<pin name="INT0/U1RTS/SCK1/RF6"/>
<pin name="RG0"/>
<pin name="RG1"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="CN8/SCK2/RG6"/>
<pin name="CN9/SDI2/RG7"/>
<pin name="CN10/SDO2/RG8"/>
<pin name="T5CK/CN11/SS2/RG9"/>
<pin name="RG12"/>
<pin name="RG13"/>
<pin name="RG14"/>
<pin name="RG15"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="USB3750">
<pin name="DP_1" direction="in"/>
<pin name="2/VBUS" direction="out"/>
<pin name="3/VBUS" direction="out"/>
<pin name="4/VBUS" direction="out"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="INT_B" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="9/VOUT" direction="out"/>
<pin name="10/VOUT" direction="out"/>
<pin name="11/VOUT" direction="out"/>
<pin name="DM_2" direction="in"/>
<pin name="DP_2" direction="in"/>
<pin name="DM" direction="out"/>
<pin name="DP" direction="out"/>
<pin name="DM_1" direction="in"/>
</symbol>
<symbol name="USB3751">
<pin name="1/DP1" direction="in"/>
<pin name="2/VBUS" direction="out"/>
<pin name="3/VBUS" direction="out"/>
<pin name="4/VBUS" direction="out"/>
<pin name="5/SDA"/>
<pin name="6/SCL" direction="in"/>
<pin name="7/INTB" direction="out"/>
<pin name="8/GND" direction="pwr"/>
<pin name="9/VOUT" direction="out"/>
<pin name="10/VOUT" direction="out"/>
<pin name="11/VOUT" direction="out"/>
<pin name="14/DM" direction="out"/>
<pin name="15/DP" direction="out"/>
<pin name="16/DM1" direction="in"/>
</symbol>
<symbol name="USB3740">
<pin name="1/DM1" direction="in"/>
<pin name="2/DP1" direction="in"/>
<pin name="3/OEN" direction="in"/>
<pin name="4/S" direction="in"/>
<pin name="5/VDD" direction="pwr"/>
<pin name="6/DP2" direction="in"/>
<pin name="7/DM2" direction="in"/>
<pin name="8/GND" direction="pwr"/>
<pin name="9/DM" direction="out"/>
<pin name="10/DP" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PIC16C*" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;PIC16C5X family: EPROM/ROM-based
&lt;li&gt;PIC16C55X family: EPROM-based
&lt;li&gt;PIC16C6X family
&lt;li&gt;PIC16CE62X family: analog comparators/EEPROM data memory
&lt;li&gt;PIC16C7X family: A/D converter
&lt;li&gt;PIC16C71X family: A/D converter
&lt;li&gt;PIC16F8X family: flash EEPROM
&lt;/ul&gt;&lt;p&gt;
Pin compatible devices:&lt;p&gt;
PIC16C154, PIC16CR154, PIC16C156, PIC16CR156, PIC16C158&lt;p&gt;
PIC16CR158, PIC16C52, PIC16C54, PIC16C54A, PIC16CR54A&lt;p&gt;
PIC16C56, PIC16C58A, PIC16CR58A, PIC16C61, PIC16C554&lt;p&gt;
PIC16C556, PIC16C558, PIC16C620, PIC16C621, PIC16C622&lt;p&gt;
PIC16C641, PIC16C642, PIC16C661, PIC16C662, PIC16C71&lt;p&gt;
PIC16C710, PIC16C711, PIC16C715, PIC126F83, PIC16CR83&lt;p&gt;
PIC16F84A, PIC16CR84&lt;p&gt;
see also &lt;a href=DEVICE:PIC16F8*&gt;PIC16F8*&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="13IO-2"/>
</gates>
<devices>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="154">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="156">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="158">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="52">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="54">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C54-RCI/P"/>
<attribute name="OC_FARNELL" value="1084285"/>
<attribute name="OC_NEWARK" value="23C3204"/>
</technology>
<technology name="54A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C54A-04/P"/>
<attribute name="OC_FARNELL" value="1196847"/>
<attribute name="OC_NEWARK" value="61K3438"/>
</technology>
<technology name="55">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C558-04/P"/>
<attribute name="OC_FARNELL" value="1084353"/>
<attribute name="OC_NEWARK" value="96K3797"/>
</technology>
<technology name="554">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C554-04I/P"/>
<attribute name="OC_FARNELL" value="9759204"/>
<attribute name="OC_NEWARK" value="23C3455"/>
</technology>
<technology name="556">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="558">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C558-20/P"/>
<attribute name="OC_FARNELL" value="9759220"/>
<attribute name="OC_NEWARK" value="97K7200"/>
</technology>
<technology name="56">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C56-HS/P"/>
<attribute name="OC_FARNELL" value="1084307"/>
<attribute name="OC_NEWARK" value="23C3511"/>
</technology>
<technology name="58A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C58B-04/P"/>
<attribute name="OC_FARNELL" value="9759417"/>
<attribute name="OC_NEWARK" value="23C3736"/>
</technology>
<technology name="61">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="620">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C620-04/P"/>
<attribute name="OC_FARNELL" value="1196828"/>
<attribute name="OC_NEWARK" value="24M5866"/>
</technology>
<technology name="621">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C621-04I/P"/>
<attribute name="OC_FARNELL" value="1196829"/>
<attribute name="OC_NEWARK" value="23C3904"/>
</technology>
<technology name="622">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C622A-04I/P"/>
<attribute name="OC_FARNELL" value="9759549"/>
<attribute name="OC_NEWARK" value="23C3984"/>
</technology>
<technology name="641">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="661">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C71-20I/P"/>
<attribute name="OC_FARNELL" value="1196825"/>
<attribute name="OC_NEWARK" value="73K1290"/>
</technology>
<technology name="710">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C71-04/P"/>
<attribute name="OC_FARNELL" value="9759778"/>
<attribute name="OC_NEWARK" value="69K7626"/>
</technology>
<technology name="711">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C711-04I/P"/>
<attribute name="OC_FARNELL" value="1084359"/>
<attribute name="OC_NEWARK" value="68K5331"/>
</technology>
<technology name="715">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C715-20/P"/>
<attribute name="OC_FARNELL" value="1084360"/>
<attribute name="OC_NEWARK" value="97K7271"/>
</technology>
<technology name="84">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F83">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R154">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R156">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R158">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R54">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R54A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R58A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R83">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R84">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO-18W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="154">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="156">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="158">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="52">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="54">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C54-XT/SO"/>
<attribute name="OC_FARNELL" value="9759182"/>
<attribute name="OC_NEWARK" value="23C3207"/>
</technology>
<technology name="54A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C54A-04I/SO"/>
<attribute name="OC_FARNELL" value="1084342"/>
<attribute name="OC_NEWARK" value="23C3231"/>
</technology>
<technology name="55">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="554">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C554-04/SO"/>
<attribute name="OC_FARNELL" value="1084352"/>
<attribute name="OC_NEWARK" value="97K7196"/>
</technology>
<technology name="556">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="558">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C558-04/SO"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3481"/>
</technology>
<technology name="58A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="61">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="620">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C620-04/SO"/>
<attribute name="OC_FARNELL" value="9759468"/>
<attribute name="OC_NEWARK" value="23C3838"/>
</technology>
<technology name="621">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C621-04I/SO"/>
<attribute name="OC_FARNELL" value="9759492"/>
<attribute name="OC_NEWARK" value="23C3905"/>
</technology>
<technology name="622">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C622A-04I/SO"/>
<attribute name="OC_FARNELL" value="9759522"/>
<attribute name="OC_NEWARK" value="23C3985"/>
</technology>
<technology name="71">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="710">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C710-20/SO"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4447"/>
</technology>
<technology name="711">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C711-20/SO"/>
<attribute name="OC_FARNELL" value="9759808"/>
<attribute name="OC_NEWARK" value="12C1918"/>
</technology>
<technology name="715">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C715-04I/SO"/>
<attribute name="OC_FARNELL" value="1084362"/>
<attribute name="OC_NEWARK" value="23C4530"/>
</technology>
<technology name="84">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R154">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R156">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R158">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R54">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R54A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R58A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R83">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R84">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C52" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="13IO-2"/>
</gates>
<devices>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="JW" package="DIL18">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO-18W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C56*SS" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based</description>
<gates>
<gate name="G$1" symbol="13IO-1SS"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="18"/>
<connect gate="G$1" pin="OSC2" pad="17"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RB0" pad="7"/>
<connect gate="G$1" pin="RB1" pad="8"/>
<connect gate="G$1" pin="RB2" pad="9"/>
<connect gate="G$1" pin="RB3" pad="10"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="12"/>
<connect gate="G$1" pin="RB6" pad="13"/>
<connect gate="G$1" pin="RB7" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C56A-04/SS"/>
<attribute name="OC_FARNELL" value="116506"/>
<attribute name="OC_NEWARK" value="23C3557"/>
</technology>
<technology name="A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C56A-04/SS"/>
<attribute name="OC_FARNELL" value="116506"/>
<attribute name="OC_NEWARK" value="23C3557"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C62*" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based</description>
<gates>
<gate name="G$1" symbol="13IO-1SS"/>
</gates>
<devices>
<device name="SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="18"/>
<connect gate="G$1" pin="OSC2" pad="17"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RB0" pad="7"/>
<connect gate="G$1" pin="RB1" pad="8"/>
<connect gate="G$1" pin="RB2" pad="9"/>
<connect gate="G$1" pin="RB3" pad="10"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="12"/>
<connect gate="G$1" pin="RB6" pad="13"/>
<connect gate="G$1" pin="RB7" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C620A-40/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C4421"/>
</technology>
<technology name="1">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C621-20I/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3915"/>
</technology>
<technology name="2">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C622A-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3980"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C5*" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based</description>
<gates>
<gate name="G$1" symbol="20IO-2"/>
</gates>
<devices>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!MCLR" pad="28"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="27"/>
<connect gate="G$1" pin="OSC2" pad="26"/>
<connect gate="G$1" pin="RA0" pad="6"/>
<connect gate="G$1" pin="RA1" pad="7"/>
<connect gate="G$1" pin="RA2" pad="8"/>
<connect gate="G$1" pin="RA3" pad="9"/>
<connect gate="G$1" pin="RB0" pad="10"/>
<connect gate="G$1" pin="RB1" pad="11"/>
<connect gate="G$1" pin="RB2" pad="12"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="18"/>
<connect gate="G$1" pin="RC1" pad="19"/>
<connect gate="G$1" pin="RC2" pad="20"/>
<connect gate="G$1" pin="RC3" pad="21"/>
<connect gate="G$1" pin="RC4" pad="22"/>
<connect gate="G$1" pin="RC5" pad="23"/>
<connect gate="G$1" pin="RC6" pad="24"/>
<connect gate="G$1" pin="RC7" pad="25"/>
<connect gate="G$1" pin="T0CKI" pad="1"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="5">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C55-LPI/P"/>
<attribute name="OC_FARNELL" value="9759271"/>
<attribute name="OC_NEWARK" value="23C3344"/>
</technology>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C57-HS/P"/>
<attribute name="OC_FARNELL" value="1523927"/>
<attribute name="OC_NEWARK" value="61K3440"/>
</technology>
<technology name="7A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C57-HS/P"/>
<attribute name="OC_FARNELL" value="1084260"/>
<attribute name="OC_NEWARK" value="61K3440"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="28"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="27"/>
<connect gate="G$1" pin="OSC2" pad="26"/>
<connect gate="G$1" pin="RA0" pad="6"/>
<connect gate="G$1" pin="RA1" pad="7"/>
<connect gate="G$1" pin="RA2" pad="8"/>
<connect gate="G$1" pin="RA3" pad="9"/>
<connect gate="G$1" pin="RB0" pad="10"/>
<connect gate="G$1" pin="RB1" pad="11"/>
<connect gate="G$1" pin="RB2" pad="12"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="18"/>
<connect gate="G$1" pin="RC1" pad="19"/>
<connect gate="G$1" pin="RC2" pad="20"/>
<connect gate="G$1" pin="RC3" pad="21"/>
<connect gate="G$1" pin="RC4" pad="22"/>
<connect gate="G$1" pin="RC5" pad="23"/>
<connect gate="G$1" pin="RC6" pad="24"/>
<connect gate="G$1" pin="RC7" pad="25"/>
<connect gate="G$1" pin="T0CKI" pad="1"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="5">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C55A-04/SO"/>
<attribute name="OC_FARNELL" value="9759280"/>
<attribute name="OC_NEWARK" value="96K3793"/>
</technology>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C57-HS/SO"/>
<attribute name="OC_FARNELL" value="9759395"/>
<attribute name="OC_NEWARK" value="23C3614"/>
</technology>
<technology name="7A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C57-XTI/P"/>
<attribute name="OC_FARNELL" value="9759395"/>
<attribute name="OC_NEWARK" value="88K1971"/>
</technology>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!MCLR" pad="28"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="27"/>
<connect gate="G$1" pin="OSC2" pad="26"/>
<connect gate="G$1" pin="RA0" pad="6"/>
<connect gate="G$1" pin="RA1" pad="7"/>
<connect gate="G$1" pin="RA2" pad="8"/>
<connect gate="G$1" pin="RA3" pad="9"/>
<connect gate="G$1" pin="RB0" pad="10"/>
<connect gate="G$1" pin="RB1" pad="11"/>
<connect gate="G$1" pin="RB2" pad="12"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="18"/>
<connect gate="G$1" pin="RC1" pad="19"/>
<connect gate="G$1" pin="RC2" pad="20"/>
<connect gate="G$1" pin="RC3" pad="21"/>
<connect gate="G$1" pin="RC4" pad="22"/>
<connect gate="G$1" pin="RC5" pad="23"/>
<connect gate="G$1" pin="RC6" pad="24"/>
<connect gate="G$1" pin="RC7" pad="25"/>
<connect gate="G$1" pin="T0CKI" pad="1"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="5">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C55A-20E/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3402"/>
</technology>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C57C-04I/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3683"/>
</technology>
<technology name="7A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C57C-04I/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3683"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C65*?-40" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="33IO-1A"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6" pad="39"/>
<connect gate="G$1" pin="RB7" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0" pad="8"/>
<connect gate="G$1" pin="RE1" pad="9"/>
<connect gate="G$1" pin="RE2" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C65B-20/P"/>
<attribute name="OC_FARNELL" value="9759670"/>
<attribute name="OC_NEWARK" value="12C1910"/>
</technology>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/P"/>
<attribute name="OC_FARNELL" value="9759670"/>
<attribute name="OC_NEWARK" value="97K7249"/>
</technology>
<technology name="B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C65B-04/P"/>
<attribute name="OC_FARNELL" value="9759719"/>
<attribute name="OC_NEWARK" value="23C4232"/>
</technology>
</technologies>
</device>
<device name="JW" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6" pad="39"/>
<connect gate="G$1" pin="RB7" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0" pad="8"/>
<connect gate="G$1" pin="RE1" pad="9"/>
<connect gate="G$1" pin="RE2" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="97K7249"/>
</technology>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/P"/>
<attribute name="OC_FARNELL" value="9759670"/>
<attribute name="OC_NEWARK" value="97K7249"/>
</technology>
<technology name="B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C65B/JW"/>
<attribute name="OC_FARNELL" value="9759719"/>
<attribute name="OC_NEWARK" value="96K3817"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C*?-40" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
8-Bit CMOS&lt;p&gt;
Pin compatible:&lt;p&gt;
PIC16CR64, PIC16C64A, PIC16C65A, 
PIC16CR65, PIC16C67, PIC16C74A, PIC16C77</description>
<gates>
<gate name="G$1" symbol="33IO-1A"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6" pad="39"/>
<connect gate="G$1" pin="RB7" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0" pad="8"/>
<connect gate="G$1" pin="RE1" pad="9"/>
<connect gate="G$1" pin="RE2" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="64A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C64A-04I/P"/>
<attribute name="OC_FARNELL" value="1084225"/>
<attribute name="OC_NEWARK" value="24M5871"/>
</technology>
<technology name="65A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/P"/>
<attribute name="OC_FARNELL" value="9759670"/>
<attribute name="OC_NEWARK" value="97K7249"/>
</technology>
<technology name="67">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C67-20/P"/>
<attribute name="OC_FARNELL" value="9759751"/>
<attribute name="OC_NEWARK" value="72K7295"/>
</technology>
<technology name="74A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C74A-04I/P"/>
<attribute name="OC_FARNELL" value="9760059"/>
<attribute name="OC_NEWARK" value="31M5834"/>
</technology>
<technology name="77">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C77-20I/P"/>
<attribute name="OC_FARNELL" value="9760172"/>
<attribute name="OC_NEWARK" value="96K3855"/>
</technology>
<technology name="R64">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="JW" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6" pad="39"/>
<connect gate="G$1" pin="RB7" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0" pad="8"/>
<connect gate="G$1" pin="RE1" pad="9"/>
<connect gate="G$1" pin="RE2" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="64A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C64A-04I/P"/>
<attribute name="OC_FARNELL" value="1084225"/>
<attribute name="OC_NEWARK" value="24M5871"/>
</technology>
<technology name="65A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/P"/>
<attribute name="OC_FARNELL" value="9759670"/>
<attribute name="OC_NEWARK" value="97K7249"/>
</technology>
<technology name="67">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C67-04/P"/>
<attribute name="OC_FARNELL" value="9759751"/>
<attribute name="OC_NEWARK" value="61K3443"/>
</technology>
<technology name="74A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C74A-10/P"/>
<attribute name="OC_FARNELL" value="1084347"/>
<attribute name="OC_NEWARK" value="97K7294"/>
</technology>
<technology name="77">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C77-20/P"/>
<attribute name="OC_FARNELL" value="9760172"/>
<attribute name="OC_NEWARK" value="12C1937"/>
</technology>
<technology name="R64">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C64*?-40" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="33IO-1A"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6" pad="39"/>
<connect gate="G$1" pin="RB7" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0" pad="8"/>
<connect gate="G$1" pin="RE1" pad="9"/>
<connect gate="G$1" pin="RE2" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A-04/P"/>
<attribute name="OC_FARNELL" value="1084225"/>
<attribute name="OC_NEWARK" value="23C4077"/>
</technology>
</technologies>
</device>
<device name="JW" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6" pad="39"/>
<connect gate="G$1" pin="RB7" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0" pad="8"/>
<connect gate="G$1" pin="RE1" pad="9"/>
<connect gate="G$1" pin="RE2" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A/JW"/>
<attribute name="OC_FARNELL" value="1084225"/>
<attribute name="OC_NEWARK" value="96K3814"/>
</technology>
<technology name="A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A-04/P"/>
<attribute name="OC_FARNELL" value="1084225"/>
<attribute name="OC_NEWARK" value="23C4077"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C6*?-40" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based</description>
<gates>
<gate name="G$1" symbol="33IO-1A"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6" pad="39"/>
<connect gate="G$1" pin="RB7" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0" pad="8"/>
<connect gate="G$1" pin="RE1" pad="9"/>
<connect gate="G$1" pin="RE2" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C64A-04I/P"/>
<attribute name="OC_FARNELL" value="1084225"/>
<attribute name="OC_NEWARK" value="24M5871"/>
</technology>
<technology name="5">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C65B-04/P"/>
<attribute name="OC_FARNELL" value="9759670"/>
<attribute name="OC_NEWARK" value="23C4232"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C65*?-44" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="33IO-MQ"/>
</gates>
<devices>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="17"/>
<connect gate="G$1" pin="NC@2" pad="28"/>
<connect gate="G$1" pin="NC@3" pad="40"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="3"/>
<connect gate="G$1" pin="RA1" pad="4"/>
<connect gate="G$1" pin="RA2" pad="5"/>
<connect gate="G$1" pin="RA3" pad="6"/>
<connect gate="G$1" pin="RA4" pad="7"/>
<connect gate="G$1" pin="RA5" pad="8"/>
<connect gate="G$1" pin="RB0" pad="36"/>
<connect gate="G$1" pin="RB1" pad="37"/>
<connect gate="G$1" pin="RB2" pad="38"/>
<connect gate="G$1" pin="RB3" pad="39"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5" pad="42"/>
<connect gate="G$1" pin="RB6" pad="43"/>
<connect gate="G$1" pin="RB7" pad="44"/>
<connect gate="G$1" pin="RC0" pad="16"/>
<connect gate="G$1" pin="RC1" pad="18"/>
<connect gate="G$1" pin="RC2" pad="19"/>
<connect gate="G$1" pin="RC3" pad="20"/>
<connect gate="G$1" pin="RC4" pad="25"/>
<connect gate="G$1" pin="RC5" pad="26"/>
<connect gate="G$1" pin="RC6" pad="27"/>
<connect gate="G$1" pin="RC7" pad="29"/>
<connect gate="G$1" pin="RD0" pad="21"/>
<connect gate="G$1" pin="RD1" pad="22"/>
<connect gate="G$1" pin="RD2" pad="23"/>
<connect gate="G$1" pin="RD3" pad="24"/>
<connect gate="G$1" pin="RD4" pad="30"/>
<connect gate="G$1" pin="RD5" pad="31"/>
<connect gate="G$1" pin="RD6" pad="32"/>
<connect gate="G$1" pin="RD7" pad="33"/>
<connect gate="G$1" pin="RE0" pad="9"/>
<connect gate="G$1" pin="RE1" pad="10"/>
<connect gate="G$1" pin="RE2" pad="11"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="35"/>
<connect gate="G$1" pin="VSS" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/L"/>
<attribute name="OC_FARNELL" value="9759700"/>
<attribute name="OC_NEWARK" value="97K7248"/>
</technology>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/L"/>
<attribute name="OC_FARNELL" value="9759662"/>
<attribute name="OC_NEWARK" value="97K7248"/>
</technology>
<technology name="B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C65B-20/L"/>
<attribute name="OC_FARNELL" value="9759689"/>
<attribute name="OC_NEWARK" value="96K3816"/>
</technology>
</technologies>
</device>
<device name="PQ" package="MQFP44-2">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="21"/>
<connect gate="G$1" pin="RA3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5" pad="24"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RC6" pad="44"/>
<connect gate="G$1" pin="RC7" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0" pad="25"/>
<connect gate="G$1" pin="RE1" pad="26"/>
<connect gate="G$1" pin="RE2" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TQ" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="21"/>
<connect gate="G$1" pin="RA3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5" pad="24"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RC6" pad="44"/>
<connect gate="G$1" pin="RC7" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0" pad="25"/>
<connect gate="G$1" pin="RE1" pad="26"/>
<connect gate="G$1" pin="RE2" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C65B-20/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4244"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C74*-44" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based&lt;br&gt;
Source: http://www.microchip.com/.. 30390e.pdf&lt;br&gt;
Note:This product is obsolete.</description>
<gates>
<gate name="G$1" symbol="33IO-MQ"/>
</gates>
<devices>
<device name="PQ" package="MQFP44-2">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="21"/>
<connect gate="G$1" pin="RA3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5" pad="24"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RC6" pad="44"/>
<connect gate="G$1" pin="RC7" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0" pad="25"/>
<connect gate="G$1" pin="RE1" pad="26"/>
<connect gate="G$1" pin="RE2" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C74B-20I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4798"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="17"/>
<connect gate="G$1" pin="NC@2" pad="28"/>
<connect gate="G$1" pin="NC@3" pad="40"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="3"/>
<connect gate="G$1" pin="RA1" pad="4"/>
<connect gate="G$1" pin="RA2" pad="5"/>
<connect gate="G$1" pin="RA3" pad="6"/>
<connect gate="G$1" pin="RA4" pad="7"/>
<connect gate="G$1" pin="RA5" pad="8"/>
<connect gate="G$1" pin="RB0" pad="36"/>
<connect gate="G$1" pin="RB1" pad="37"/>
<connect gate="G$1" pin="RB2" pad="38"/>
<connect gate="G$1" pin="RB3" pad="39"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5" pad="42"/>
<connect gate="G$1" pin="RB6" pad="43"/>
<connect gate="G$1" pin="RB7" pad="44"/>
<connect gate="G$1" pin="RC0" pad="16"/>
<connect gate="G$1" pin="RC1" pad="18"/>
<connect gate="G$1" pin="RC2" pad="19"/>
<connect gate="G$1" pin="RC3" pad="20"/>
<connect gate="G$1" pin="RC4" pad="25"/>
<connect gate="G$1" pin="RC5" pad="26"/>
<connect gate="G$1" pin="RC6" pad="27"/>
<connect gate="G$1" pin="RC7" pad="29"/>
<connect gate="G$1" pin="RD0" pad="21"/>
<connect gate="G$1" pin="RD1" pad="22"/>
<connect gate="G$1" pin="RD2" pad="23"/>
<connect gate="G$1" pin="RD3" pad="24"/>
<connect gate="G$1" pin="RD4" pad="30"/>
<connect gate="G$1" pin="RD5" pad="31"/>
<connect gate="G$1" pin="RD6" pad="32"/>
<connect gate="G$1" pin="RD7" pad="33"/>
<connect gate="G$1" pin="RE0" pad="9"/>
<connect gate="G$1" pin="RE1" pad="10"/>
<connect gate="G$1" pin="RE2" pad="11"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="35"/>
<connect gate="G$1" pin="VSS" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C74B-20/L"/>
<attribute name="OC_FARNELL" value="9760113"/>
<attribute name="OC_NEWARK" value="96K3846"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C*?-44" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
8-Bit CMOS&lt;p&gt;
Pin compatible:&lt;p&gt;
PIC16CR64, PIC16C64A, PIC16C65A, 
PIC16CR65, PIC16C67, PIC16C74A, PIC16C77</description>
<gates>
<gate name="G$1" symbol="33IO-MQ"/>
</gates>
<devices>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="17"/>
<connect gate="G$1" pin="NC@2" pad="28"/>
<connect gate="G$1" pin="NC@3" pad="40"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="3"/>
<connect gate="G$1" pin="RA1" pad="4"/>
<connect gate="G$1" pin="RA2" pad="5"/>
<connect gate="G$1" pin="RA3" pad="6"/>
<connect gate="G$1" pin="RA4" pad="7"/>
<connect gate="G$1" pin="RA5" pad="8"/>
<connect gate="G$1" pin="RB0" pad="36"/>
<connect gate="G$1" pin="RB1" pad="37"/>
<connect gate="G$1" pin="RB2" pad="38"/>
<connect gate="G$1" pin="RB3" pad="39"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5" pad="42"/>
<connect gate="G$1" pin="RB6" pad="43"/>
<connect gate="G$1" pin="RB7" pad="44"/>
<connect gate="G$1" pin="RC0" pad="16"/>
<connect gate="G$1" pin="RC1" pad="18"/>
<connect gate="G$1" pin="RC2" pad="19"/>
<connect gate="G$1" pin="RC3" pad="20"/>
<connect gate="G$1" pin="RC4" pad="25"/>
<connect gate="G$1" pin="RC5" pad="26"/>
<connect gate="G$1" pin="RC6" pad="27"/>
<connect gate="G$1" pin="RC7" pad="29"/>
<connect gate="G$1" pin="RD0" pad="21"/>
<connect gate="G$1" pin="RD1" pad="22"/>
<connect gate="G$1" pin="RD2" pad="23"/>
<connect gate="G$1" pin="RD3" pad="24"/>
<connect gate="G$1" pin="RD4" pad="30"/>
<connect gate="G$1" pin="RD5" pad="31"/>
<connect gate="G$1" pin="RD6" pad="32"/>
<connect gate="G$1" pin="RD7" pad="33"/>
<connect gate="G$1" pin="RE0" pad="9"/>
<connect gate="G$1" pin="RE1" pad="10"/>
<connect gate="G$1" pin="RE2" pad="11"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="35"/>
<connect gate="G$1" pin="VSS" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="34"/>
</connects>
<technologies>
<technology name="64A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A-04/L"/>
<attribute name="OC_FARNELL" value="9759646"/>
<attribute name="OC_NEWARK" value="96K3813"/>
</technology>
<technology name="65A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/L"/>
<attribute name="OC_FARNELL" value="9759662"/>
<attribute name="OC_NEWARK" value="97K7248"/>
</technology>
<technology name="67">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C67-04/L"/>
<attribute name="OC_FARNELL" value="9759743"/>
<attribute name="OC_NEWARK" value="97K7255"/>
</technology>
<technology name="74A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C74A-10/L"/>
<attribute name="OC_FARNELL" value="9760067"/>
<attribute name="OC_NEWARK" value="01M8478"/>
</technology>
<technology name="77">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C77-20I/L"/>
<attribute name="OC_FARNELL" value="1196837"/>
<attribute name="OC_NEWARK" value="96K3854"/>
</technology>
<technology name="R64">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="PQ" package="MQFP44-2">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="21"/>
<connect gate="G$1" pin="RA3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5" pad="24"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RC6" pad="44"/>
<connect gate="G$1" pin="RC7" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0" pad="25"/>
<connect gate="G$1" pin="RE1" pad="26"/>
<connect gate="G$1" pin="RE2" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="64A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A-10I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4098"/>
</technology>
<technology name="65A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C65B-20/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4244"/>
</technology>
<technology name="67">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C67-04/PQ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4363"/>
</technology>
<technology name="74A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C74A-10I/PQ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4735"/>
</technology>
<technology name="77">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C774-E/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C4482"/>
</technology>
<technology name="R64">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C64*?-44" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="33IO-MQ"/>
</gates>
<devices>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="17"/>
<connect gate="G$1" pin="NC@2" pad="28"/>
<connect gate="G$1" pin="NC@3" pad="40"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="3"/>
<connect gate="G$1" pin="RA1" pad="4"/>
<connect gate="G$1" pin="RA2" pad="5"/>
<connect gate="G$1" pin="RA3" pad="6"/>
<connect gate="G$1" pin="RA4" pad="7"/>
<connect gate="G$1" pin="RA5" pad="8"/>
<connect gate="G$1" pin="RB0" pad="36"/>
<connect gate="G$1" pin="RB1" pad="37"/>
<connect gate="G$1" pin="RB2" pad="38"/>
<connect gate="G$1" pin="RB3" pad="39"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5" pad="42"/>
<connect gate="G$1" pin="RB6" pad="43"/>
<connect gate="G$1" pin="RB7" pad="44"/>
<connect gate="G$1" pin="RC0" pad="16"/>
<connect gate="G$1" pin="RC1" pad="18"/>
<connect gate="G$1" pin="RC2" pad="19"/>
<connect gate="G$1" pin="RC3" pad="20"/>
<connect gate="G$1" pin="RC4" pad="25"/>
<connect gate="G$1" pin="RC5" pad="26"/>
<connect gate="G$1" pin="RC6" pad="27"/>
<connect gate="G$1" pin="RC7" pad="29"/>
<connect gate="G$1" pin="RD0" pad="21"/>
<connect gate="G$1" pin="RD1" pad="22"/>
<connect gate="G$1" pin="RD2" pad="23"/>
<connect gate="G$1" pin="RD3" pad="24"/>
<connect gate="G$1" pin="RD4" pad="30"/>
<connect gate="G$1" pin="RD5" pad="31"/>
<connect gate="G$1" pin="RD6" pad="32"/>
<connect gate="G$1" pin="RD7" pad="33"/>
<connect gate="G$1" pin="RE0" pad="9"/>
<connect gate="G$1" pin="RE1" pad="10"/>
<connect gate="G$1" pin="RE2" pad="11"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="35"/>
<connect gate="G$1" pin="VSS" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A-20/L"/>
<attribute name="OC_FARNELL" value="9759646"/>
<attribute name="OC_NEWARK" value="23C4099"/>
</technology>
</technologies>
</device>
<device name="PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="21"/>
<connect gate="G$1" pin="RA3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5" pad="24"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RC6" pad="44"/>
<connect gate="G$1" pin="RC7" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0" pad="25"/>
<connect gate="G$1" pin="RE1" pad="26"/>
<connect gate="G$1" pin="RE2" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C6*?-44" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based</description>
<gates>
<gate name="G$1" symbol="33IO-MQ"/>
</gates>
<devices>
<device name="PQ" package="MQFP44-2">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="21"/>
<connect gate="G$1" pin="RA3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5" pad="24"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RC6" pad="44"/>
<connect gate="G$1" pin="RC7" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0" pad="25"/>
<connect gate="G$1" pin="RE1" pad="26"/>
<connect gate="G$1" pin="RE2" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A-10I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4098"/>
</technology>
<technology name="4A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="21"/>
<connect gate="G$1" pin="RA3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5" pad="24"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RC6" pad="44"/>
<connect gate="G$1" pin="RC7" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0" pad="25"/>
<connect gate="G$1" pin="RE1" pad="26"/>
<connect gate="G$1" pin="RE2" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A-04/L"/>
<attribute name="OC_FARNELL" value="9759646"/>
<attribute name="OC_NEWARK" value="96K3813"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C65A-04/L"/>
<attribute name="OC_FARNELL" value="9759700"/>
<attribute name="OC_NEWARK" value="97K7248"/>
</technology>
</technologies>
</device>
<device name="TQ" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="21"/>
<connect gate="G$1" pin="RA3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5" pad="24"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="16"/>
<connect gate="G$1" pin="RB7" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RC6" pad="44"/>
<connect gate="G$1" pin="RC7" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0" pad="25"/>
<connect gate="G$1" pin="RE1" pad="26"/>
<connect gate="G$1" pin="RE2" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="4A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C64A-10I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4098"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C74" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based</description>
<gates>
<gate name="G$1" symbol="33IO-1A"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6" pad="39"/>
<connect gate="G$1" pin="RB7" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0" pad="8"/>
<connect gate="G$1" pin="RE1" pad="9"/>
<connect gate="G$1" pin="RE2" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C74B-04/P"/>
<attribute name="OC_FARNELL" value="1084347"/>
<attribute name="OC_NEWARK" value="01M8479"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C84" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based</description>
<gates>
<gate name="G$1" symbol="13IO-1"/>
</gates>
<devices>
<device name="SO" package="SO-18W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI/RA4" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI/RA4" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F8*" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
8-Bit PIC16F8X Family - CMOS Flash/&lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
Pin Compatible :&lt;p&gt;
PIC16F83, PIC16CR83, PIC16F84A, PIC16CR84&lt;p&gt;
see also &lt;a href=DEVICE:PIC16C*&gt;PIC16C*&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="13IO-1"/>
</gates>
<devices>
<device name="SO" package="SO-18W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI/RA4" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F83-04/SO"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4997"/>
</technology>
<technology name="4A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F84A-04/SO"/>
<attribute name="OC_FARNELL" value="9760890"/>
<attribute name="OC_NEWARK" value="69K7634"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="T0CKI/RA4" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F83-04/P"/>
<attribute name="OC_FARNELL" value="1084354"/>
<attribute name="OC_NEWARK" value="97K7388"/>
</technology>
<technology name="4A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F84A-04I/P"/>
<attribute name="OC_FARNELL" value="9760865"/>
<attribute name="OC_NEWARK" value="69K7635"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C*?-28" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
8-Bit&lt;B&gt;EPROM&lt;/B&gt;/ROM-based&lt;p&gt;
Pin compatible:&lt;p&gt;
PIC16CR62, PIC16C62A, PIC16C63, PIC16CR63&lt;p&gt;
PIC16C66, PIC16C72, PIC16C73A, PIC16C76</description>
<gates>
<gate name="G$1" symbol="22IO-1"/>
</gates>
<devices>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="62A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C62A-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3766"/>
</technology>
<technology name="63">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C63A-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K3811"/>
</technology>
<technology name="66">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="72">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C72A-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4612"/>
</technology>
<technology name="73A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C73B-20I/SS"/>
<attribute name="OC_FARNELL" value="1137313"/>
<attribute name="OC_NEWARK" value="24M5884"/>
</technology>
<technology name="76">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R62">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R63">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="62A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C62A-10/SP"/>
<attribute name="OC_FARNELL" value="9759557"/>
<attribute name="OC_NEWARK" value="23C3774"/>
</technology>
<technology name="63">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C63-04I/SP"/>
<attribute name="OC_FARNELL" value="9759590"/>
<attribute name="OC_NEWARK" value="23C4025"/>
</technology>
<technology name="66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C66-04I/SP"/>
<attribute name="OC_FARNELL" value="9759735"/>
<attribute name="OC_NEWARK" value="23C4276"/>
</technology>
<technology name="72">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C72-04/SO"/>
<attribute name="OC_FARNELL" value="1196858"/>
<attribute name="OC_NEWARK" value="23C4583"/>
</technology>
<technology name="73A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C73A-20I/SP"/>
<attribute name="OC_FARNELL" value="1815911"/>
<attribute name="OC_NEWARK" value="23C4675"/>
</technology>
<technology name="76">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C76-20/SP"/>
<attribute name="OC_FARNELL" value="1196859"/>
<attribute name="OC_NEWARK" value="12C1934"/>
</technology>
<technology name="R62">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R63">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="62A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C62A-20/SO"/>
<attribute name="OC_FARNELL" value="9759573"/>
<attribute name="OC_NEWARK" value="23C3782"/>
</technology>
<technology name="63">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C63-04/SO"/>
<attribute name="OC_FARNELL" value="9759581"/>
<attribute name="OC_NEWARK" value="97K7237"/>
</technology>
<technology name="66">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C66-10/SO"/>
<attribute name="OC_FARNELL" value="9759727"/>
<attribute name="OC_NEWARK" value="97K7254"/>
</technology>
<technology name="72">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C72-04/SO"/>
<attribute name="OC_FARNELL" value="9759891"/>
<attribute name="OC_NEWARK" value="23C4583"/>
</technology>
<technology name="73A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C73A-04/SO"/>
<attribute name="OC_FARNELL" value="9759930"/>
<attribute name="OC_NEWARK" value="97K7282"/>
</technology>
<technology name="76">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C76-20/SO"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="65K1040"/>
</technology>
<technology name="R62">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R63">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="PS" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="62">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C62B-20/SP"/>
<attribute name="OC_FARNELL" value="9759565"/>
<attribute name="OC_NEWARK" value="12C1900"/>
</technology>
<technology name="62A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C62A-10/SP"/>
<attribute name="OC_FARNELL" value="1818502"/>
<attribute name="OC_NEWARK" value="23C3774"/>
</technology>
<technology name="63">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C63-04I/SP"/>
<attribute name="OC_FARNELL" value="9759590"/>
<attribute name="OC_NEWARK" value="23C4025"/>
</technology>
<technology name="66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C66-04I/SP"/>
<attribute name="OC_FARNELL" value="685999"/>
<attribute name="OC_NEWARK" value="23C4276"/>
</technology>
<technology name="72">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C72A-04/SP"/>
<attribute name="OC_FARNELL" value="1196858"/>
<attribute name="OC_NEWARK" value="12C1924"/>
</technology>
<technology name="73A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C73A-20/SP"/>
<attribute name="OC_FARNELL" value="1196850"/>
<attribute name="OC_NEWARK" value="69K7069"/>
</technology>
<technology name="76">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C76-04/SP"/>
<attribute name="OC_FARNELL" value="1196836"/>
<attribute name="OC_NEWARK" value="96K3849"/>
</technology>
<technology name="R63">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="JW" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="62A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C62A-10/SP"/>
<attribute name="OC_FARNELL" value="9759557"/>
<attribute name="OC_NEWARK" value="23C3774"/>
</technology>
<technology name="63">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C63-04/SP"/>
<attribute name="OC_FARNELL" value="1084289"/>
<attribute name="OC_NEWARK" value="97K7238"/>
</technology>
<technology name="66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C66/JW"/>
<attribute name="OC_FARNELL" value="685999"/>
<attribute name="OC_NEWARK" value="96K3820"/>
</technology>
<technology name="72">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C72-20/SP"/>
<attribute name="OC_FARNELL" value="1196858"/>
<attribute name="OC_NEWARK" value="23C4602"/>
</technology>
<technology name="73A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C73A-10/SP"/>
<attribute name="OC_FARNELL" value="9759948"/>
<attribute name="OC_NEWARK" value="97K7284"/>
</technology>
<technology name="76">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C76-04/SP"/>
<attribute name="OC_FARNELL" value="1196836"/>
<attribute name="OC_NEWARK" value="97K7307"/>
</technology>
<technology name="R62">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R63">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C73" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM/ROM-based</description>
<gates>
<gate name="G$1" symbol="22IO-1"/>
</gates>
<devices>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C73B-20/SO"/>
<attribute name="OC_FARNELL" value="9759999"/>
<attribute name="OC_NEWARK" value="12C1926"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C73B-04I/SP"/>
<attribute name="OC_FARNELL" value="9759980"/>
<attribute name="OC_NEWARK" value="96K3842"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C66" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="22IO-1"/>
</gates>
<devices>
<device name="P" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C66-04I/SP"/>
<attribute name="OC_FARNELL" value="9759735"/>
<attribute name="OC_NEWARK" value="23C4276"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16C66-10/SO"/>
<attribute name="OC_FARNELL" value="9759727"/>
<attribute name="OC_NEWARK" value="97K7254"/>
</technology>
</technologies>
</device>
<device name="JW" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C66/JW"/>
<attribute name="OC_FARNELL" value="685999"/>
<attribute name="OC_NEWARK" value="96K3820"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC17C4*" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM-based</description>
<gates>
<gate name="G$1" symbol="33IO-1MQ"/>
</gates>
<devices>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="35"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="OSC1" pad="21"/>
<connect gate="G$1" pin="OSC2" pad="22"/>
<connect gate="G$1" pin="RA0" pad="28"/>
<connect gate="G$1" pin="RA1" pad="27"/>
<connect gate="G$1" pin="RA2" pad="26"/>
<connect gate="G$1" pin="RA3" pad="25"/>
<connect gate="G$1" pin="RA4" pad="24"/>
<connect gate="G$1" pin="RA5" pad="23"/>
<connect gate="G$1" pin="RB0" pad="13"/>
<connect gate="G$1" pin="RB1" pad="14"/>
<connect gate="G$1" pin="RB2" pad="15"/>
<connect gate="G$1" pin="RB3" pad="16"/>
<connect gate="G$1" pin="RB4" pad="17"/>
<connect gate="G$1" pin="RB5" pad="18"/>
<connect gate="G$1" pin="RB6" pad="19"/>
<connect gate="G$1" pin="RB7" pad="20"/>
<connect gate="G$1" pin="RC0" pad="3"/>
<connect gate="G$1" pin="RC1" pad="4"/>
<connect gate="G$1" pin="RC2" pad="5"/>
<connect gate="G$1" pin="RC3" pad="6"/>
<connect gate="G$1" pin="RC4" pad="7"/>
<connect gate="G$1" pin="RC5" pad="8"/>
<connect gate="G$1" pin="RC6" pad="9"/>
<connect gate="G$1" pin="RC7" pad="10"/>
<connect gate="G$1" pin="RD0" pad="43"/>
<connect gate="G$1" pin="RD1" pad="42"/>
<connect gate="G$1" pin="RD2" pad="41"/>
<connect gate="G$1" pin="RD3" pad="40"/>
<connect gate="G$1" pin="RD4" pad="39"/>
<connect gate="G$1" pin="RD5" pad="38"/>
<connect gate="G$1" pin="RD6" pad="37"/>
<connect gate="G$1" pin="RD7" pad="36"/>
<connect gate="G$1" pin="RE0" pad="32"/>
<connect gate="G$1" pin="RE1" pad="31"/>
<connect gate="G$1" pin="RE2" pad="30"/>
<connect gate="G$1" pin="TEST" pad="29"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="44"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
<connect gate="G$1" pin="VSS@2" pad="33"/>
<connect gate="G$1" pin="VSS@3" pad="34"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C42A-25I/L"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C5787"/>
</technology>
<technology name="3">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C43-16/L"/>
<attribute name="OC_FARNELL" value="9761861"/>
<attribute name="OC_NEWARK" value="23C5830"/>
</technology>
<technology name="4">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C44-16/L"/>
<attribute name="OC_FARNELL" value="9761918"/>
<attribute name="OC_NEWARK" value="69K7642"/>
</technology>
</technologies>
</device>
<device name="PQ" package="MQFP44-2">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="NC" pad="18"/>
<connect gate="G$1" pin="OSC1" pad="37"/>
<connect gate="G$1" pin="OSC2" pad="38"/>
<connect gate="G$1" pin="RA0" pad="44"/>
<connect gate="G$1" pin="RA1" pad="43"/>
<connect gate="G$1" pin="RA2" pad="42"/>
<connect gate="G$1" pin="RA3" pad="41"/>
<connect gate="G$1" pin="RA4" pad="40"/>
<connect gate="G$1" pin="RA5" pad="39"/>
<connect gate="G$1" pin="RB0" pad="29"/>
<connect gate="G$1" pin="RB1" pad="30"/>
<connect gate="G$1" pin="RB2" pad="31"/>
<connect gate="G$1" pin="RB3" pad="32"/>
<connect gate="G$1" pin="RB4" pad="33"/>
<connect gate="G$1" pin="RB5" pad="34"/>
<connect gate="G$1" pin="RB6" pad="35"/>
<connect gate="G$1" pin="RB7" pad="36"/>
<connect gate="G$1" pin="RC0" pad="19"/>
<connect gate="G$1" pin="RC1" pad="20"/>
<connect gate="G$1" pin="RC2" pad="21"/>
<connect gate="G$1" pin="RC3" pad="22"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="15"/>
<connect gate="G$1" pin="RD1" pad="14"/>
<connect gate="G$1" pin="RD2" pad="13"/>
<connect gate="G$1" pin="RD3" pad="12"/>
<connect gate="G$1" pin="RD4" pad="11"/>
<connect gate="G$1" pin="RD5" pad="10"/>
<connect gate="G$1" pin="RD6" pad="9"/>
<connect gate="G$1" pin="RD7" pad="8"/>
<connect gate="G$1" pin="RE0" pad="4"/>
<connect gate="G$1" pin="RE1" pad="3"/>
<connect gate="G$1" pin="RE2" pad="2"/>
<connect gate="G$1" pin="TEST" pad="1"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VDD@1" pad="17"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="27"/>
<connect gate="G$1" pin="VSS@3" pad="28"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C42A-16/PQ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C5769"/>
</technology>
<technology name="3">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C43-33/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C5857"/>
</technology>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC17C4*?-40" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
EPROM-based</description>
<gates>
<gate name="G$1" symbol="33IO-1"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR" pad="32"/>
<connect gate="G$1" pin="OSC1" pad="19"/>
<connect gate="G$1" pin="OSC2" pad="20"/>
<connect gate="G$1" pin="RA0" pad="26"/>
<connect gate="G$1" pin="RA1" pad="25"/>
<connect gate="G$1" pin="RA2" pad="24"/>
<connect gate="G$1" pin="RA3" pad="23"/>
<connect gate="G$1" pin="RA4" pad="22"/>
<connect gate="G$1" pin="RA5" pad="21"/>
<connect gate="G$1" pin="RB0" pad="11"/>
<connect gate="G$1" pin="RB1" pad="12"/>
<connect gate="G$1" pin="RB2" pad="13"/>
<connect gate="G$1" pin="RB3" pad="14"/>
<connect gate="G$1" pin="RB4" pad="15"/>
<connect gate="G$1" pin="RB5" pad="16"/>
<connect gate="G$1" pin="RB6" pad="17"/>
<connect gate="G$1" pin="RB7" pad="18"/>
<connect gate="G$1" pin="RC0" pad="2"/>
<connect gate="G$1" pin="RC1" pad="3"/>
<connect gate="G$1" pin="RC2" pad="4"/>
<connect gate="G$1" pin="RC3" pad="5"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="7"/>
<connect gate="G$1" pin="RC6" pad="8"/>
<connect gate="G$1" pin="RC7" pad="9"/>
<connect gate="G$1" pin="RD0" pad="40"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="38"/>
<connect gate="G$1" pin="RD3" pad="37"/>
<connect gate="G$1" pin="RD4" pad="36"/>
<connect gate="G$1" pin="RD5" pad="35"/>
<connect gate="G$1" pin="RD6" pad="34"/>
<connect gate="G$1" pin="RD7" pad="33"/>
<connect gate="G$1" pin="RE0" pad="30"/>
<connect gate="G$1" pin="RE1" pad="29"/>
<connect gate="G$1" pin="RE2" pad="28"/>
<connect gate="G$1" pin="TEST" pad="27"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="10"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C42A-16/P"/>
<attribute name="OC_FARNELL" value="1196768"/>
<attribute name="OC_NEWARK" value="23C5768"/>
</technology>
<technology name="3">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C43-16/P"/>
<attribute name="OC_FARNELL" value="1084356"/>
<attribute name="OC_NEWARK" value="63K6089"/>
</technology>
<technology name="4">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C44-33/P"/>
<attribute name="OC_FARNELL" value="1084221"/>
<attribute name="OC_NEWARK" value="23C5919"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C*?-20" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
Pin compatible devices
&lt;ul&gt;
&lt;li&gt;PIC16C5X family: EPROM/ROM-based
&lt;li&gt;PIC16C55X family: EPROM-based
&lt;li&gt;PIC16C6X family
&lt;li&gt;PIC16CE62X family: analog comparators/EEPROM data memory
&lt;li&gt;PIC16C7X family: A/D converter
&lt;li&gt;PIC16C71X family: A/D converter
&lt;/ul&gt;
Pin compatible devices:
&lt;p&gt;PIC16C154, PIC16CR154, PIC16C156, PIC16CR156, PIC16C158&lt;p&gt;
PIC16CR158, PIC16C52, PIC16C54, PIC16C54A, PIC16CR54A&lt;p&gt;
PIC16C56, PIC16C58A, PIC16CR58A, PIC16C61, PIC16C554&lt;p&gt;
PIC16C556, PIC16C558, PIC16C620, PIC16C621, PIC16C622&lt;p&gt;
PIC16C641, PIC16C642, PIC16C661, PIC16C662, PIC16C71&lt;p&gt;
PIC16C710, PIC16C711, PIC16C715, PIC126F83, PIC16CR83&lt;p&gt;
PIC16F84A, PIC16CR84</description>
<gates>
<gate name="G$1" symbol="13IO-1SS"/>
</gates>
<devices>
<device name="SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="!MCLR" pad="4"/>
<connect gate="G$1" pin="OSC1" pad="18"/>
<connect gate="G$1" pin="OSC2" pad="17"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RB0" pad="7"/>
<connect gate="G$1" pin="RB1" pad="8"/>
<connect gate="G$1" pin="RB2" pad="9"/>
<connect gate="G$1" pin="RB3" pad="10"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="12"/>
<connect gate="G$1" pin="RB6" pad="13"/>
<connect gate="G$1" pin="RB7" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
</connects>
<technologies>
<technology name="154">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="156">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="158">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="54">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C54-RCI/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3206"/>
</technology>
<technology name="54A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="554">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="556">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="558">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C558-20I/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3497"/>
</technology>
<technology name="56">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C56-HSI/SS"/>
<attribute name="OC_FARNELL" value="116506"/>
<attribute name="OC_NEWARK" value="23C3519"/>
</technology>
<technology name="58A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C58B-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3738"/>
</technology>
<technology name="620">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C620A-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3858"/>
</technology>
<technology name="621">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C621-20I/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3915"/>
</technology>
<technology name="622">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C622A-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3980"/>
</technology>
<technology name="710">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="711">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C711-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4469"/>
</technology>
<technology name="715">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C715-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4525"/>
</technology>
<technology name="R154">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R156">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R158">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R54A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R58A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC12C*?" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="6IO"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3/MC" pad="4"/>
<connect gate="G$1" pin="GP4/COUT" pad="3"/>
<connect gate="G$1" pin="GP5/CIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="508">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C508A-04I/P"/>
<attribute name="OC_FARNELL" value="9758763"/>
<attribute name="OC_NEWARK" value="12C1849"/>
</technology>
<technology name="509">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C509-04/P"/>
<attribute name="OC_FARNELL" value="9758810"/>
<attribute name="OC_NEWARK" value="54K2820"/>
</technology>
<technology name="671">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C671-10/P"/>
<attribute name="OC_FARNELL" value="9758860"/>
<attribute name="OC_NEWARK" value="23C2974"/>
</technology>
<technology name="672">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C672-04/P"/>
<attribute name="OC_FARNELL" value="9758887"/>
<attribute name="OC_NEWARK" value="59K0241"/>
</technology>
</technologies>
</device>
<device name="JN" package="DIL8">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3/MC" pad="4"/>
<connect gate="G$1" pin="GP4/COUT" pad="3"/>
<connect gate="G$1" pin="GP5/CIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="508">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C508-04/P"/>
<attribute name="OC_FARNELL" value="9758771"/>
<attribute name="OC_NEWARK" value="60K6710"/>
</technology>
<technology name="509">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C509A-04I/P"/>
<attribute name="OC_FARNELL" value="9758828"/>
<attribute name="OC_NEWARK" value="23C2958"/>
</technology>
<technology name="671">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC12C671-10I/P"/>
<attribute name="OC_FARNELL" value="1084238"/>
<attribute name="OC_NEWARK" value="34M7956"/>
</technology>
<technology name="672">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C672-04/P"/>
<attribute name="OC_FARNELL" value="9758887"/>
<attribute name="OC_NEWARK" value="59K0241"/>
</technology>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3/MC" pad="4"/>
<connect gate="G$1" pin="GP4/COUT" pad="3"/>
<connect gate="G$1" pin="GP5/CIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="508">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C508-04I/SM"/>
<attribute name="OC_FARNELL" value="1196846"/>
<attribute name="OC_NEWARK" value="96K3762"/>
</technology>
<technology name="509">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C509A-04I/SM"/>
<attribute name="OC_FARNELL" value="9758844"/>
<attribute name="OC_NEWARK" value="65K1035"/>
</technology>
<technology name="671">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC12C671-10I/SM"/>
<attribute name="OC_FARNELL" value="1196776"/>
<attribute name="OC_NEWARK" value="24M5845"/>
</technology>
<technology name="672">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12C672-04/SM"/>
<attribute name="OC_FARNELL" value="1137297"/>
<attribute name="OC_NEWARK" value="72K7294"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC14000*" prefix="IC">
<description>&lt;B&gt;MIXED SIGNAL CONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="14000"/>
</gates>
<devices>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!MCLR" pad="14"/>
<connect gate="G$1" pin="CDAC" pad="22"/>
<connect gate="G$1" pin="OSC1" pad="8"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="1"/>
<connect gate="G$1" pin="RA2" pad="28"/>
<connect gate="G$1" pin="RA3" pad="27"/>
<connect gate="G$1" pin="RC0" pad="19"/>
<connect gate="G$1" pin="RC1" pad="18"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="16"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="13"/>
<connect gate="G$1" pin="RC6" pad="12"/>
<connect gate="G$1" pin="RC7" pad="11"/>
<connect gate="G$1" pin="RD0" pad="6"/>
<connect gate="G$1" pin="RD1" pad="5"/>
<connect gate="G$1" pin="RD2" pad="4"/>
<connect gate="G$1" pin="RD3" pad="3"/>
<connect gate="G$1" pin="RD4" pad="26"/>
<connect gate="G$1" pin="RD5" pad="25"/>
<connect gate="G$1" pin="RD6" pad="24"/>
<connect gate="G$1" pin="RD7" pad="23"/>
<connect gate="G$1" pin="SUM" pad="21"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VREG" pad="10"/>
<connect gate="G$1" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC14000-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12C1860"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="14"/>
<connect gate="G$1" pin="CDAC" pad="22"/>
<connect gate="G$1" pin="OSC1" pad="8"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="1"/>
<connect gate="G$1" pin="RA2" pad="28"/>
<connect gate="G$1" pin="RA3" pad="27"/>
<connect gate="G$1" pin="RC0" pad="19"/>
<connect gate="G$1" pin="RC1" pad="18"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="16"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="13"/>
<connect gate="G$1" pin="RC6" pad="12"/>
<connect gate="G$1" pin="RC7" pad="11"/>
<connect gate="G$1" pin="RD0" pad="6"/>
<connect gate="G$1" pin="RD1" pad="5"/>
<connect gate="G$1" pin="RD2" pad="4"/>
<connect gate="G$1" pin="RD3" pad="3"/>
<connect gate="G$1" pin="RD4" pad="26"/>
<connect gate="G$1" pin="RD5" pad="25"/>
<connect gate="G$1" pin="RD6" pad="24"/>
<connect gate="G$1" pin="RD7" pad="23"/>
<connect gate="G$1" pin="SUM" pad="21"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VREG" pad="10"/>
<connect gate="G$1" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC14000-04/SO"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C3058"/>
</technology>
</technologies>
</device>
<device name="SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="14"/>
<connect gate="G$1" pin="CDAC" pad="22"/>
<connect gate="G$1" pin="OSC1" pad="8"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="1"/>
<connect gate="G$1" pin="RA2" pad="28"/>
<connect gate="G$1" pin="RA3" pad="27"/>
<connect gate="G$1" pin="RC0" pad="19"/>
<connect gate="G$1" pin="RC1" pad="18"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="16"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="13"/>
<connect gate="G$1" pin="RC6" pad="12"/>
<connect gate="G$1" pin="RC7" pad="11"/>
<connect gate="G$1" pin="RD0" pad="6"/>
<connect gate="G$1" pin="RD1" pad="5"/>
<connect gate="G$1" pin="RD2" pad="4"/>
<connect gate="G$1" pin="RD3" pad="3"/>
<connect gate="G$1" pin="RD4" pad="26"/>
<connect gate="G$1" pin="RD5" pad="25"/>
<connect gate="G$1" pin="RD6" pad="24"/>
<connect gate="G$1" pin="RD7" pad="23"/>
<connect gate="G$1" pin="SUM" pad="21"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VREG" pad="10"/>
<connect gate="G$1" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC14000-04I/SP"/>
<attribute name="OC_FARNELL" value="9759069"/>
<attribute name="OC_NEWARK" value="23C3061"/>
</technology>
</technologies>
</device>
<device name="JW" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!MCLR" pad="14"/>
<connect gate="G$1" pin="CDAC" pad="22"/>
<connect gate="G$1" pin="OSC1" pad="8"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="1"/>
<connect gate="G$1" pin="RA2" pad="28"/>
<connect gate="G$1" pin="RA3" pad="27"/>
<connect gate="G$1" pin="RC0" pad="19"/>
<connect gate="G$1" pin="RC1" pad="18"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="16"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="13"/>
<connect gate="G$1" pin="RC6" pad="12"/>
<connect gate="G$1" pin="RC7" pad="11"/>
<connect gate="G$1" pin="RD0" pad="6"/>
<connect gate="G$1" pin="RD1" pad="5"/>
<connect gate="G$1" pin="RD2" pad="4"/>
<connect gate="G$1" pin="RD3" pad="3"/>
<connect gate="G$1" pin="RD4" pad="26"/>
<connect gate="G$1" pin="RD5" pad="25"/>
<connect gate="G$1" pin="RD6" pad="24"/>
<connect gate="G$1" pin="RD7" pad="23"/>
<connect gate="G$1" pin="SUM" pad="21"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VREG" pad="10"/>
<connect gate="G$1" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C9*?-68" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
with LCD driver</description>
<gates>
<gate name="G$1" symbol="16C9L"/>
</gates>
<devices>
<device name="L" package="PLCC-68">
<connects>
<connect gate="G$1" pin="!MCLR" pad="2"/>
<connect gate="G$1" pin="C1" pad="17"/>
<connect gate="G$1" pin="C2" pad="18"/>
<connect gate="G$1" pin="COM0" pad="63"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="24"/>
<connect gate="G$1" pin="OSC2" pad="25"/>
<connect gate="G$1" pin="RA0" pad="5"/>
<connect gate="G$1" pin="RA1" pad="6"/>
<connect gate="G$1" pin="RA2" pad="8"/>
<connect gate="G$1" pin="RA3" pad="9"/>
<connect gate="G$1" pin="RA4" pad="10"/>
<connect gate="G$1" pin="RA5" pad="11"/>
<connect gate="G$1" pin="RB0" pad="13"/>
<connect gate="G$1" pin="RB1" pad="12"/>
<connect gate="G$1" pin="RB2" pad="4"/>
<connect gate="G$1" pin="RB3" pad="3"/>
<connect gate="G$1" pin="RB4" pad="68"/>
<connect gate="G$1" pin="RB5" pad="67"/>
<connect gate="G$1" pin="RB6" pad="65"/>
<connect gate="G$1" pin="RB7" pad="66"/>
<connect gate="G$1" pin="RC0" pad="26"/>
<connect gate="G$1" pin="RC1" pad="27"/>
<connect gate="G$1" pin="RC2" pad="28"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RD0" pad="31"/>
<connect gate="G$1" pin="RD1" pad="32"/>
<connect gate="G$1" pin="RD2" pad="33"/>
<connect gate="G$1" pin="RD3" pad="34"/>
<connect gate="G$1" pin="RD4" pad="35"/>
<connect gate="G$1" pin="RD5" pad="60"/>
<connect gate="G$1" pin="RD6" pad="61"/>
<connect gate="G$1" pin="RD7" pad="62"/>
<connect gate="G$1" pin="RE0" pad="37"/>
<connect gate="G$1" pin="RE1" pad="38"/>
<connect gate="G$1" pin="RE2" pad="39"/>
<connect gate="G$1" pin="RE3" pad="40"/>
<connect gate="G$1" pin="RE4" pad="41"/>
<connect gate="G$1" pin="RE5" pad="42"/>
<connect gate="G$1" pin="RE6" pad="43"/>
<connect gate="G$1" pin="RE7" pad="36"/>
<connect gate="G$1" pin="RF0" pad="44"/>
<connect gate="G$1" pin="RF1" pad="45"/>
<connect gate="G$1" pin="RF2" pad="46"/>
<connect gate="G$1" pin="RF3" pad="47"/>
<connect gate="G$1" pin="RF4" pad="48"/>
<connect gate="G$1" pin="RF5" pad="49"/>
<connect gate="G$1" pin="RF6" pad="50"/>
<connect gate="G$1" pin="RF7" pad="51"/>
<connect gate="G$1" pin="RG0" pad="53"/>
<connect gate="G$1" pin="RG1" pad="54"/>
<connect gate="G$1" pin="RG2" pad="55"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG4" pad="57"/>
<connect gate="G$1" pin="RG5" pad="58"/>
<connect gate="G$1" pin="RG6" pad="59"/>
<connect gate="G$1" pin="RG7" pad="52"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VDD@1" pad="22"/>
<connect gate="G$1" pin="VDD@2" pad="64"/>
<connect gate="G$1" pin="VLCD1" pad="29"/>
<connect gate="G$1" pin="VLCD2" pad="19"/>
<connect gate="G$1" pin="VLCD3" pad="20"/>
<connect gate="G$1" pin="VLCDADJ" pad="30"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="VSS@1" pad="23"/>
</connects>
<technologies>
<technology name="23">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C923-04/L"/>
<attribute name="OC_FARNELL" value="1196843"/>
<attribute name="OC_NEWARK" value="23C4927"/>
</technology>
<technology name="24">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C924-08I/L"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4949"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16C92*?-64" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
with LCD driver</description>
<gates>
<gate name="G$1" symbol="16C9P"/>
</gates>
<devices>
<device name="PS" package="DIL64">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="C1" pad="16"/>
<connect gate="G$1" pin="C2" pad="17"/>
<connect gate="G$1" pin="COM0" pad="59"/>
<connect gate="G$1" pin="OSC1" pad="22"/>
<connect gate="G$1" pin="OSC2" pad="23"/>
<connect gate="G$1" pin="RA0" pad="4"/>
<connect gate="G$1" pin="RA1" pad="5"/>
<connect gate="G$1" pin="RA2" pad="7"/>
<connect gate="G$1" pin="RA3" pad="8"/>
<connect gate="G$1" pin="RA4" pad="9"/>
<connect gate="G$1" pin="RA5" pad="10"/>
<connect gate="G$1" pin="RB0" pad="12"/>
<connect gate="G$1" pin="RB1" pad="11"/>
<connect gate="G$1" pin="RB2" pad="3"/>
<connect gate="G$1" pin="RB3" pad="2"/>
<connect gate="G$1" pin="RB4" pad="64"/>
<connect gate="G$1" pin="RB5" pad="63"/>
<connect gate="G$1" pin="RB6" pad="61"/>
<connect gate="G$1" pin="RB7" pad="62"/>
<connect gate="G$1" pin="RC0" pad="24"/>
<connect gate="G$1" pin="RC1" pad="25"/>
<connect gate="G$1" pin="RC2" pad="26"/>
<connect gate="G$1" pin="RC3" pad="13"/>
<connect gate="G$1" pin="RC4" pad="14"/>
<connect gate="G$1" pin="RC5" pad="15"/>
<connect gate="G$1" pin="RD0" pad="29"/>
<connect gate="G$1" pin="RD1" pad="30"/>
<connect gate="G$1" pin="RD2" pad="31"/>
<connect gate="G$1" pin="RD3" pad="32"/>
<connect gate="G$1" pin="RD4" pad="33"/>
<connect gate="G$1" pin="RD5" pad="56"/>
<connect gate="G$1" pin="RD6" pad="57"/>
<connect gate="G$1" pin="RD7" pad="58"/>
<connect gate="G$1" pin="RE0" pad="34"/>
<connect gate="G$1" pin="RE1" pad="35"/>
<connect gate="G$1" pin="RE2" pad="36"/>
<connect gate="G$1" pin="RE3" pad="37"/>
<connect gate="G$1" pin="RE4" pad="38"/>
<connect gate="G$1" pin="RE5" pad="39"/>
<connect gate="G$1" pin="RE6" pad="40"/>
<connect gate="G$1" pin="RF0" pad="41"/>
<connect gate="G$1" pin="RF1" pad="42"/>
<connect gate="G$1" pin="RF2" pad="43"/>
<connect gate="G$1" pin="RF3" pad="44"/>
<connect gate="G$1" pin="RF4" pad="45"/>
<connect gate="G$1" pin="RF5" pad="46"/>
<connect gate="G$1" pin="RF6" pad="47"/>
<connect gate="G$1" pin="RF7" pad="48"/>
<connect gate="G$1" pin="RG0" pad="49"/>
<connect gate="G$1" pin="RG1" pad="50"/>
<connect gate="G$1" pin="RG2" pad="51"/>
<connect gate="G$1" pin="RG3" pad="52"/>
<connect gate="G$1" pin="RG4" pad="53"/>
<connect gate="G$1" pin="RG5" pad="54"/>
<connect gate="G$1" pin="RG6" pad="55"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="60"/>
<connect gate="G$1" pin="VLCD1" pad="27"/>
<connect gate="G$1" pin="VLCD2" pad="18"/>
<connect gate="G$1" pin="VLCD3" pad="19"/>
<connect gate="G$1" pin="VLCDADJ" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="21"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TQ" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="57"/>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="C2" pad="9"/>
<connect gate="G$1" pin="COM0" pad="51"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="RA0" pad="60"/>
<connect gate="G$1" pin="RA1" pad="61"/>
<connect gate="G$1" pin="RA2" pad="63"/>
<connect gate="G$1" pin="RA3" pad="64"/>
<connect gate="G$1" pin="RA4" pad="1"/>
<connect gate="G$1" pin="RA5" pad="2"/>
<connect gate="G$1" pin="RB0" pad="4"/>
<connect gate="G$1" pin="RB1" pad="3"/>
<connect gate="G$1" pin="RB2" pad="59"/>
<connect gate="G$1" pin="RB3" pad="58"/>
<connect gate="G$1" pin="RB4" pad="56"/>
<connect gate="G$1" pin="RB5" pad="55"/>
<connect gate="G$1" pin="RB6" pad="53"/>
<connect gate="G$1" pin="RB7" pad="54"/>
<connect gate="G$1" pin="RC0" pad="16"/>
<connect gate="G$1" pin="RC1" pad="17"/>
<connect gate="G$1" pin="RC2" pad="18"/>
<connect gate="G$1" pin="RC3" pad="5"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="7"/>
<connect gate="G$1" pin="RD0" pad="21"/>
<connect gate="G$1" pin="RD1" pad="22"/>
<connect gate="G$1" pin="RD2" pad="23"/>
<connect gate="G$1" pin="RD3" pad="24"/>
<connect gate="G$1" pin="RD4" pad="25"/>
<connect gate="G$1" pin="RD5" pad="48"/>
<connect gate="G$1" pin="RD6" pad="49"/>
<connect gate="G$1" pin="RD7" pad="50"/>
<connect gate="G$1" pin="RE0" pad="26"/>
<connect gate="G$1" pin="RE1" pad="27"/>
<connect gate="G$1" pin="RE2" pad="28"/>
<connect gate="G$1" pin="RE3" pad="29"/>
<connect gate="G$1" pin="RE4" pad="30"/>
<connect gate="G$1" pin="RE5" pad="31"/>
<connect gate="G$1" pin="RE6" pad="32"/>
<connect gate="G$1" pin="RF0" pad="33"/>
<connect gate="G$1" pin="RF1" pad="34"/>
<connect gate="G$1" pin="RF2" pad="35"/>
<connect gate="G$1" pin="RF3" pad="36"/>
<connect gate="G$1" pin="RF4" pad="37"/>
<connect gate="G$1" pin="RF5" pad="38"/>
<connect gate="G$1" pin="RF6" pad="39"/>
<connect gate="G$1" pin="RF7" pad="40"/>
<connect gate="G$1" pin="RG0" pad="41"/>
<connect gate="G$1" pin="RG1" pad="42"/>
<connect gate="G$1" pin="RG2" pad="43"/>
<connect gate="G$1" pin="RG3" pad="44"/>
<connect gate="G$1" pin="RG4" pad="45"/>
<connect gate="G$1" pin="RG5" pad="46"/>
<connect gate="G$1" pin="RG6" pad="47"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="52"/>
<connect gate="G$1" pin="VLCD1" pad="19"/>
<connect gate="G$1" pin="VLCD2" pad="10"/>
<connect gate="G$1" pin="VLCD3" pad="11"/>
<connect gate="G$1" pin="VLCDADJ" pad="20"/>
<connect gate="G$1" pin="VSS" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="62"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16C923-04I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C4930"/>
</technology>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24C*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
1 K/2 K/4 K</description>
<gates>
<gate name="G$1" symbol="24AA"/>
</gates>
<devices>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT24C01WI-GT3"/>
<attribute name="OC_FARNELL" value="1718117"/>
<attribute name="OC_NEWARK" value="06R0487"/>
</technology>
<technology name="01A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C01BN-SH-B"/>
<attribute name="OC_FARNELL" value="1362638"/>
<attribute name="OC_NEWARK" value="50M3313"/>
</technology>
<technology name="01C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C01C/SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4061"/>
</technology>
<technology name="02">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="02A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="02C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C02C/SN"/>
<attribute name="OC_FARNELL" value="1607552"/>
<attribute name="OC_NEWARK" value="96K4065"/>
</technology>
<technology name="04">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C04-WMN6P"/>
<attribute name="OC_FARNELL" value="9882812"/>
<attribute name="OC_NEWARK" value="83K1376"/>
</technology>
<technology name="04A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="04C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C01-WMN6P"/>
<attribute name="OC_FARNELL" value="9882790"/>
<attribute name="OC_NEWARK" value="24M5068"/>
</technology>
<technology name="01A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C01BN-SH-B"/>
<attribute name="OC_FARNELL" value="1362638"/>
<attribute name="OC_NEWARK" value="50M3313"/>
</technology>
<technology name="01C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C01-WMN6P"/>
<attribute name="OC_FARNELL" value="9882790"/>
<attribute name="OC_NEWARK" value="24M5068"/>
</technology>
<technology name="02">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C02C-I/SN"/>
<attribute name="OC_FARNELL" value="1084339"/>
<attribute name="OC_NEWARK" value="96K4063"/>
</technology>
<technology name="02A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C02-WMN6P"/>
<attribute name="OC_FARNELL" value="9882804"/>
<attribute name="OC_NEWARK" value="10M9771"/>
</technology>
<technology name="02C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C02C-I/SN"/>
<attribute name="OC_FARNELL" value="1084339"/>
<attribute name="OC_NEWARK" value="96K4063"/>
</technology>
<technology name="04">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT24C04WI-G"/>
<attribute name="OC_FARNELL" value="1631136"/>
<attribute name="OC_NEWARK" value="06R0507"/>
</technology>
<technology name="04A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C04BN-SH-B"/>
<attribute name="OC_FARNELL" value="1362643"/>
<attribute name="OC_NEWARK" value="50M3316"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C01C-I/P"/>
<attribute name="OC_FARNELL" value="1847800"/>
<attribute name="OC_NEWARK" value="92C6948"/>
</technology>
<technology name="01A">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="M24C01-WBN6P"/>
<attribute name="OC_FARNELL" value="9882782"/>
<attribute name="OC_NEWARK" value="93K7306"/>
</technology>
<technology name="01C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C01C/P"/>
<attribute name="OC_FARNELL" value="3662901"/>
<attribute name="OC_NEWARK" value="96K4060"/>
</technology>
<technology name="02">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="02A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C02-WBN6P"/>
<attribute name="OC_FARNELL" value="1094256"/>
<attribute name="OC_NEWARK" value="11M0888"/>
</technology>
<technology name="02C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C02C/P"/>
<attribute name="OC_FARNELL" value="1296567"/>
<attribute name="OC_NEWARK" value="96K4064"/>
</technology>
<technology name="04">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C04-WBN6P"/>
<attribute name="OC_FARNELL" value="1094258"/>
<attribute name="OC_NEWARK" value="02M5802"/>
</technology>
<technology name="04A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C04B-PU"/>
<attribute name="OC_FARNELL" value="1362642"/>
<attribute name="OC_NEWARK" value="50M3315"/>
</technology>
<technology name="04C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT24C04LI-G"/>
<attribute name="OC_FARNELL" value="1718374"/>
<attribute name="OC_NEWARK" value="73P4460"/>
</technology>
</technologies>
</device>
<device name="SL" package="SOIC-14">
<connects>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="WP" pad="12"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="02">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="04">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24C0*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
128 bit/1 K/2 K, I2C</description>
<gates>
<gate name="G$1" symbol="SERIALEEPROM"/>
</gates>
<devices>
<device name="SO" package="SO-08W">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C00/SN"/>
<attribute name="OC_FARNELL" value="1847799"/>
<attribute name="OC_NEWARK" value="96K4059"/>
</technology>
<technology name="1B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C01BN-SH-B"/>
<attribute name="OC_FARNELL" value="1362638"/>
<attribute name="OC_NEWARK" value="50M3313"/>
</technology>
<technology name="2B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="IS24C02B-2GLI"/>
<attribute name="OC_FARNELL" value="1455010"/>
<attribute name="OC_NEWARK" value="43M4517"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C00/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4058"/>
</technology>
<technology name="1B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C01B-PU"/>
<attribute name="OC_FARNELL" value="1362637"/>
<attribute name="OC_NEWARK" value="50M3312"/>
</technology>
<technology name="2B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C02B-PU"/>
<attribute name="OC_FARNELL" value="1362639"/>
<attribute name="OC_NEWARK" value="50M3314"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSSOP8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C00T-E/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="68H9684"/>
</technology>
</technologies>
</device>
<device name="OT" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C00T-I/OT"/>
<attribute name="OC_FARNELL" value="1818713"/>
<attribute name="OC_NEWARK" value="92C6937"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="59C11" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
1 K, 5.0 V, CMOS</description>
<gates>
<gate name="G$1" symbol="59C11"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="RDY" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="RDY" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="RDY" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="85C*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
1 K/2 K/4 K, 5.0 V, CMOS&lt;p&gt;
85C72/82/92</description>
<gates>
<gate name="G$1" symbol="85C72"/>
<gate name="7" symbol="NC"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="7" pin="NC" pad="7"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="72">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="92">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="7" pin="NC" pad="7"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="72">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="92">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="93-*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
512 x 8 bit/256 x 16 bit/1 K/4 K, 5.0 V, Microwire</description>
<gates>
<gate name="G$1" symbol="93C06"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="C46A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C46A-I/P"/>
<attribute name="OC_FARNELL" value="1847808"/>
<attribute name="OC_NEWARK" value="92C7591"/>
</technology>
<technology name="C46B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C46B/P"/>
<attribute name="OC_FARNELL" value="1084337"/>
<attribute name="OC_NEWARK" value="69K7676"/>
</technology>
<technology name="C56A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C56A-E/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7619"/>
</technology>
<technology name="C56B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C56B-I/P"/>
<attribute name="OC_FARNELL" value="1718065"/>
<attribute name="OC_NEWARK" value="61H6567"/>
</technology>
<technology name="C66A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C66A-I/P"/>
<attribute name="OC_FARNELL" value="1818607"/>
<attribute name="OC_NEWARK" value="61H6596"/>
</technology>
<technology name="C66B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C66B-I/P"/>
<attribute name="OC_FARNELL" value="1818523"/>
<attribute name="OC_NEWARK" value="61H6625"/>
</technology>
<technology name="LC56A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56A/P"/>
<attribute name="OC_FARNELL" value="1212671"/>
<attribute name="OC_NEWARK" value="75K5894"/>
</technology>
<technology name="LC56B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56B/P"/>
<attribute name="OC_FARNELL" value="1084250"/>
<attribute name="OC_NEWARK" value="96K4108"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="C46A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C46A-I/SN"/>
<attribute name="OC_FARNELL" value="1816075"/>
<attribute name="OC_NEWARK" value="92C7592"/>
</technology>
<technology name="C46B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C46B/SN"/>
<attribute name="OC_FARNELL" value="9758178"/>
<attribute name="OC_NEWARK" value="75K5893"/>
</technology>
<technology name="C56A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C56A-I/SN"/>
<attribute name="OC_FARNELL" value="1815962"/>
<attribute name="OC_NEWARK" value="61H6540"/>
</technology>
<technology name="C56B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C56B-I/SN"/>
<attribute name="OC_FARNELL" value="1847100"/>
<attribute name="OC_NEWARK" value="61H6569"/>
</technology>
<technology name="C66A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C66A-I/SN"/>
<attribute name="OC_FARNELL" value="1847311"/>
<attribute name="OC_NEWARK" value="61H6598"/>
</technology>
<technology name="C66B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC56A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56A/SN"/>
<attribute name="OC_FARNELL" value="1212672"/>
<attribute name="OC_NEWARK" value="33C3019"/>
</technology>
<technology name="LC56B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56B/SN"/>
<attribute name="OC_FARNELL" value="9758240"/>
<attribute name="OC_NEWARK" value="96K4109"/>
</technology>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="C46A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT93C46YI-G"/>
<attribute name="OC_FARNELL" value="1718375"/>
<attribute name="OC_NEWARK" value="74P0100"/>
</technology>
<technology name="C46B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C46B/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7605"/>
</technology>
<technology name="LC56A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56A-E/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="30H4734"/>
</technology>
<technology name="LC56B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56B-E/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="30H4749"/>
</technology>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="C46A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C46A-I/SN"/>
<attribute name="OC_FARNELL" value="1816075"/>
<attribute name="OC_NEWARK" value="92C7592"/>
</technology>
<technology name="C46B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C46B/SN"/>
<attribute name="OC_FARNELL" value="9758178"/>
<attribute name="OC_NEWARK" value="75K5893"/>
</technology>
<technology name="LC56A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56A/SN"/>
<attribute name="OC_FARNELL" value="1212672"/>
<attribute name="OC_NEWARK" value="33C3019"/>
</technology>
<technology name="LC56B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56B/SN"/>
<attribute name="OC_FARNELL" value="9758240"/>
<attribute name="OC_NEWARK" value="96K4109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="93LCS*" prefix="IC">
<description>&lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
2 K/4 K, 2.5 V&lt;p&gt;
Microwire with software write protect</description>
<gates>
<gate name="G$1" symbol="93LCS"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PE" pad="6"/>
<connect gate="G$1" pin="PRE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="56">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="66">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SL" package="SOIC-14">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="DO" pad="6"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="PE" pad="10"/>
<connect gate="G$1" pin="PRE" pad="12"/>
<connect gate="G$1" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="56">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="66">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PE" pad="6"/>
<connect gate="G$1" pin="PRE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="56">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="66">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PE" pad="6"/>
<connect gate="G$1" pin="PRE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="56">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="66">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="93*" prefix="IC">
<description>Serial &lt;B&gt;EPROM&lt;/B&gt;&lt;p&gt;
1 K/2 K/4 K, low voltage, Microwire</description>
<gates>
<gate name="G$1" symbol="93LC46"/>
</gates>
<devices>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NU" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA46">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA46/SN"/>
<attribute name="OC_FARNELL" value="1331414"/>
<attribute name="OC_NEWARK" value="96K4100"/>
</technology>
<technology name="AA56">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA56/SN"/>
<attribute name="OC_FARNELL" value="1816074"/>
<attribute name="OC_NEWARK" value="92C7564"/>
</technology>
<technology name="AA66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA66C-I/SN"/>
<attribute name="OC_FARNELL" value="1331441"/>
<attribute name="OC_NEWARK" value="30H4582"/>
</technology>
<technology name="LC45">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC46">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC46/SN"/>
<attribute name="OC_FARNELL" value="9758194"/>
<attribute name="OC_NEWARK" value="12C2030"/>
</technology>
<technology name="LC66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC66/SN"/>
<attribute name="OC_FARNELL" value="1296586"/>
<attribute name="OC_NEWARK" value="65K1154"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NU" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA46">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA46/P"/>
<attribute name="OC_FARNELL" value="1331412"/>
<attribute name="OC_NEWARK" value="96K4099"/>
</technology>
<technology name="AA56">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA56C-I/P"/>
<attribute name="OC_FARNELL" value="1331421"/>
<attribute name="OC_NEWARK" value="30H4522"/>
</technology>
<technology name="AA66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA66/P"/>
<attribute name="OC_FARNELL" value="1331440"/>
<attribute name="OC_NEWARK" value="92C7573"/>
</technology>
<technology name="LC46">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC46/P"/>
<attribute name="OC_FARNELL" value="1212720"/>
<attribute name="OC_NEWARK" value="33C3013"/>
</technology>
<technology name="LC56">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56/P"/>
<attribute name="OC_FARNELL" value="1556157"/>
<attribute name="OC_NEWARK" value="96K4105"/>
</technology>
<technology name="LC66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC66/P"/>
<attribute name="OC_FARNELL" value="1556169"/>
<attribute name="OC_NEWARK" value="62K2086"/>
</technology>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NU" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA46">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA46A-I/SN"/>
<attribute name="OC_FARNELL" value="1331414"/>
<attribute name="OC_NEWARK" value="96K4101"/>
</technology>
<technology name="AA56">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA56/SN"/>
<attribute name="OC_FARNELL" value="1331418"/>
<attribute name="OC_NEWARK" value="92C7564"/>
</technology>
<technology name="AA66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA66C-I/SN"/>
<attribute name="OC_FARNELL" value="1331432"/>
<attribute name="OC_NEWARK" value="30H4582"/>
</technology>
<technology name="LC46">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC46B/SN"/>
<attribute name="OC_FARNELL" value="1084341"/>
<attribute name="OC_NEWARK" value="65K1153"/>
</technology>
<technology name="LC56">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56T/SN"/>
<attribute name="OC_FARNELL" value="9758240"/>
<attribute name="OC_NEWARK" value="92C7699"/>
</technology>
<technology name="LC66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC66/SN"/>
<attribute name="OC_FARNELL" value="1296586"/>
<attribute name="OC_NEWARK" value="65K1154"/>
</technology>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NU" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="LC46">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC46C-I/ST"/>
<attribute name="OC_FARNELL" value="1817225"/>
<attribute name="OC_NEWARK" value="30H4716"/>
</technology>
<technology name="LC56">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC56B-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7687"/>
</technology>
<technology name="LC66">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC66C-I/ST"/>
<attribute name="OC_FARNELL" value="1846729"/>
<attribute name="OC_NEWARK" value="30H4846"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
I2C</description>
<gates>
<gate name="G$1" symbol="24AA"/>
</gates>
<devices>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="AA01">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA01-I/SN"/>
<attribute name="OC_FARNELL" value="1331268"/>
<attribute name="OC_NEWARK" value="92C6793"/>
</technology>
<technology name="AA02">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA02-I/SN"/>
<attribute name="OC_FARNELL" value="1331272"/>
<attribute name="OC_NEWARK" value="92C6803"/>
</technology>
<technology name="AA04">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA04-I/SN"/>
<attribute name="OC_FARNELL" value="1331276"/>
<attribute name="OC_NEWARK" value="92C6814"/>
</technology>
<technology name="AA08">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA08-I/SN"/>
<attribute name="OC_FARNELL" value="1331282"/>
<attribute name="OC_NEWARK" value="92C6826"/>
</technology>
<technology name="AA128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA128-I/MS"/>
<attribute name="OC_FARNELL" value="1331285"/>
<attribute name="OC_NEWARK" value="92C6839"/>
</technology>
<technology name="AA16">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA16-I/SN"/>
<attribute name="OC_FARNELL" value="1331289"/>
<attribute name="OC_NEWARK" value="96K4056"/>
</technology>
<technology name="AA32A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA32A-I/SN"/>
<attribute name="OC_FARNELL" value="1617659"/>
<attribute name="OC_NEWARK" value="83C5815"/>
</technology>
<technology name="C01A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C01C/SN"/>
<attribute name="OC_FARNELL" value="1362638"/>
<attribute name="OC_NEWARK" value="96K4061"/>
</technology>
<technology name="C02A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C02C/SN"/>
<attribute name="OC_FARNELL" value="1084339"/>
<attribute name="OC_NEWARK" value="96K4065"/>
</technology>
<technology name="C04A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C04-WMN6P"/>
<attribute name="OC_FARNELL" value="9882812"/>
<attribute name="OC_NEWARK" value="83K1376"/>
</technology>
<technology name="C08B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C08BN-SH-B"/>
<attribute name="OC_FARNELL" value="1362645"/>
<attribute name="OC_NEWARK" value="50M3318"/>
</technology>
<technology name="C32A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="IS24C32A-2GLI"/>
<attribute name="OC_FARNELL" value="1718129"/>
<attribute name="OC_NEWARK" value="43M4588"/>
</technology>
<technology name="C64">
<attribute name="MF" value="RAMTRON INTERNATIONAL CORP"/>
<attribute name="MPN" value="FM24C64-S"/>
<attribute name="OC_FARNELL" value="9882685"/>
<attribute name="OC_NEWARK" value="98H0189"/>
</technology>
<technology name="CL04B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="FM24CL04-S"/>
<attribute name="OC_FARNELL" value="1607928"/>
<attribute name="OC_NEWARK" value="97H6443"/>
</technology>
<technology name="LC08B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC08BT-I/SN"/>
<attribute name="OC_FARNELL" value="1818714"/>
<attribute name="OC_NEWARK" value="92C7127"/>
</technology>
<technology name="LC128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC128-I/SM"/>
<attribute name="OC_FARNELL" value="9757937"/>
<attribute name="OC_NEWARK" value="92C7134"/>
</technology>
<technology name="LC16B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC16B/SN"/>
<attribute name="OC_FARNELL" value="9757945"/>
<attribute name="OC_NEWARK" value="12C2012"/>
</technology>
<technology name="LC32A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC32A/SM"/>
<attribute name="OC_FARNELL" value="1212670"/>
<attribute name="OC_NEWARK" value="96K4080"/>
</technology>
<technology name="LC64">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC64T-I/SN"/>
<attribute name="OC_FARNELL" value="9758070"/>
<attribute name="OC_NEWARK" value="12C2021"/>
</technology>
</technologies>
</device>
<device name="SL" package="SOIC-14">
<connects>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="WP" pad="12"/>
</connects>
<technologies>
<technology name="AA04">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="AA08">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="AA16">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C01A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C02A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C04A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C08B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C16B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="CL04A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC08B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC16B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="AA01">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24AA01-I/P"/>
<attribute name="OC_FARNELL" value="1331266"/>
<attribute name="OC_NEWARK" value="35M0692"/>
</technology>
<technology name="AA02">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24AA02-I/P"/>
<attribute name="OC_FARNELL" value="1331271"/>
<attribute name="OC_NEWARK" value="95M2072"/>
</technology>
<technology name="AA04">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24AA04-I/P"/>
<attribute name="OC_FARNELL" value="1331275"/>
<attribute name="OC_NEWARK" value="35M0696"/>
</technology>
<technology name="AA08">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA08-I/P"/>
<attribute name="OC_FARNELL" value="1331281"/>
<attribute name="OC_NEWARK" value="92C6825"/>
</technology>
<technology name="AA128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA128-I/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C6840"/>
</technology>
<technology name="AA16">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24AA16-I/P"/>
<attribute name="OC_FARNELL" value="1331287"/>
<attribute name="OC_NEWARK" value="35M0705"/>
</technology>
<technology name="AA256">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA256-I/P"/>
<attribute name="OC_FARNELL" value="1331294"/>
<attribute name="OC_NEWARK" value="92C6872"/>
</technology>
<technology name="AA32A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA32A-I/P"/>
<attribute name="OC_FARNELL" value="1331297"/>
<attribute name="OC_NEWARK" value="92C6885"/>
</technology>
<technology name="AA64">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA64-I/P"/>
<attribute name="OC_FARNELL" value="1331303"/>
<attribute name="OC_NEWARK" value="92C6909"/>
</technology>
<technology name="C01A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C01-WBN6P"/>
<attribute name="OC_FARNELL" value="9882782"/>
<attribute name="OC_NEWARK" value="24M5067"/>
</technology>
<technology name="C02A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C02C-I/P"/>
<attribute name="OC_FARNELL" value="1755843"/>
<attribute name="OC_NEWARK" value="96K4062"/>
</technology>
<technology name="C04A">
<attribute name="MF" value="RAMTRON INTERNATIONAL CORP"/>
<attribute name="MPN" value="FM24C04A-P"/>
<attribute name="OC_FARNELL" value="1094258"/>
<attribute name="OC_NEWARK" value="97H6447"/>
</technology>
<technology name="C08B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C08B-PU"/>
<attribute name="OC_FARNELL" value="1362644"/>
<attribute name="OC_NEWARK" value="50M3317"/>
</technology>
<technology name="C16B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C16B-PU"/>
<attribute name="OC_FARNELL" value="1362650"/>
<attribute name="OC_NEWARK" value="50M3323"/>
</technology>
<technology name="C32A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C32C-PU"/>
<attribute name="OC_FARNELL" value="1362652"/>
<attribute name="OC_NEWARK" value="50M3325"/>
</technology>
<technology name="C64">
<attribute name="MF" value="RAMTRON INTERNATIONAL CORP"/>
<attribute name="MPN" value="FM24C64-P"/>
<attribute name="OC_FARNELL" value="1362657"/>
<attribute name="OC_NEWARK" value="97H6452"/>
</technology>
<technology name="CL04B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC01">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24LC01BH-I/P"/>
<attribute name="OC_FARNELL" value="1200025"/>
<attribute name="OC_NEWARK" value="77M3542"/>
</technology>
<technology name="LC024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24LC024-I/P"/>
<attribute name="OC_FARNELL" value="1331317"/>
<attribute name="OC_NEWARK" value="35M0731"/>
</technology>
<technology name="LC025">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC025-I/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7098"/>
</technology>
<technology name="LC04">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC04B-I/P"/>
<attribute name="OC_FARNELL" value="1196811"/>
<attribute name="OC_NEWARK" value="62K0576"/>
</technology>
<technology name="LC08B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC08B/P"/>
<attribute name="OC_FARNELL" value="1084245"/>
<attribute name="OC_NEWARK" value="96K4073"/>
</technology>
<technology name="LC128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC128-I/P"/>
<attribute name="OC_FARNELL" value="9757929"/>
<attribute name="OC_NEWARK" value="12C2007"/>
</technology>
<technology name="LC16B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC16B/P"/>
<attribute name="OC_FARNELL" value="1200026"/>
<attribute name="OC_NEWARK" value="69K7671"/>
</technology>
<technology name="LC256">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC256-E/P"/>
<attribute name="OC_FARNELL" value="9757970"/>
<attribute name="OC_NEWARK" value="92C7169"/>
</technology>
<technology name="LC32A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC32A/P"/>
<attribute name="OC_FARNELL" value="1084246"/>
<attribute name="OC_NEWARK" value="75K1884"/>
</technology>
<technology name="LC64">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC64-I/P"/>
<attribute name="OC_FARNELL" value="9758054"/>
<attribute name="OC_NEWARK" value="62K0584"/>
</technology>
<technology name="LCS52">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LCS52-I/PG"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89H3098"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="AA01">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA01/SN"/>
<attribute name="OC_FARNELL" value="1331268"/>
<attribute name="OC_NEWARK" value="89C9792"/>
</technology>
<technology name="AA02">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24AA02/SN"/>
<attribute name="OC_FARNELL" value="1331272"/>
<attribute name="OC_NEWARK" value="89C9793"/>
</technology>
<technology name="AA04">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA04/SN"/>
<attribute name="OC_FARNELL" value="1331276"/>
<attribute name="OC_NEWARK" value="92C6818"/>
</technology>
<technology name="AA08">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA08-I/SN"/>
<attribute name="OC_FARNELL" value="1579568"/>
<attribute name="OC_NEWARK" value="92C6826"/>
</technology>
<technology name="AA128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA128-I/SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C6842"/>
</technology>
<technology name="AA16">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA16-I/SN"/>
<attribute name="OC_FARNELL" value="1331289"/>
<attribute name="OC_NEWARK" value="96K4056"/>
</technology>
<technology name="AA256">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24AA256T-I/SM"/>
<attribute name="OC_FARNELL" value="1579570"/>
<attribute name="OC_NEWARK" value="08N6838"/>
</technology>
<technology name="AA32A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA32A-I/SN"/>
<attribute name="OC_FARNELL" value="1617659"/>
<attribute name="OC_NEWARK" value="83C5815"/>
</technology>
<technology name="AA64">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA64-I/SN"/>
<attribute name="OC_FARNELL" value="1331304"/>
<attribute name="OC_NEWARK" value="85C2288"/>
</technology>
<technology name="C08B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C08BN-SH-B"/>
<attribute name="OC_FARNELL" value="1362645"/>
<attribute name="OC_NEWARK" value="50M3318"/>
</technology>
<technology name="C16B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C16BN-SH-B"/>
<attribute name="OC_FARNELL" value="1362651"/>
<attribute name="OC_NEWARK" value="50M3324"/>
</technology>
<technology name="C32A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="IS24C32A-2GLI"/>
<attribute name="OC_FARNELL" value="1224413"/>
<attribute name="OC_NEWARK" value="43M4588"/>
</technology>
<technology name="CL04B">
<attribute name="MF" value="RAMTRON INTERNATIONAL CORP"/>
<attribute name="MPN" value="FM24CL04-G"/>
<attribute name="OC_FARNELL" value="1607928"/>
<attribute name="OC_NEWARK" value="10J0444"/>
</technology>
<technology name="LC024">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC024/SN"/>
<attribute name="OC_FARNELL" value="1659744"/>
<attribute name="OC_NEWARK" value="92C7092"/>
</technology>
<technology name="LC025">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC025/SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7103"/>
</technology>
<technology name="LC08B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24LC08B/SN"/>
<attribute name="OC_FARNELL" value="1212669"/>
<attribute name="OC_NEWARK" value="12C2005"/>
</technology>
<technology name="LC128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC128-I/SNG"/>
<attribute name="OC_FARNELL" value="9757937"/>
<attribute name="OC_NEWARK" value="30H1511"/>
</technology>
<technology name="LC16B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC16B/SN"/>
<attribute name="OC_FARNELL" value="9757945"/>
<attribute name="OC_NEWARK" value="12C2012"/>
</technology>
<technology name="LC256">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC256-I/SN"/>
<attribute name="OC_FARNELL" value="9757996"/>
<attribute name="OC_NEWARK" value="27C9144"/>
</technology>
<technology name="LC32A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC32A/SN"/>
<attribute name="OC_FARNELL" value="9758003"/>
<attribute name="OC_NEWARK" value="33C2976"/>
</technology>
<technology name="LC64">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC64-I/SN"/>
<attribute name="OC_FARNELL" value="9758070"/>
<attribute name="OC_NEWARK" value="12C2020"/>
</technology>
<technology name="LCS52">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LCS52-I/SN"/>
<attribute name="OC_FARNELL" value="1816066"/>
<attribute name="OC_NEWARK" value="92C7032"/>
</technology>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="AA128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA128-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C6843"/>
</technology>
<technology name="AA64">
<attribute name="MF" value=""/>
<attribute name="MPN" value="25AA640A-I/ST"/>
<attribute name="OC_FARNELL" value="1818513"/>
<attribute name="OC_NEWARK" value="27M1300"/>
</technology>
<technology name="C64">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT24C64YI-GT3"/>
<attribute name="OC_FARNELL" value="1718133"/>
<attribute name="OC_NEWARK" value="08R5418"/>
</technology>
<technology name="LC024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24LC024H-I/ST"/>
<attribute name="OC_FARNELL" value="1659745"/>
<attribute name="OC_NEWARK" value="77M3584"/>
</technology>
<technology name="LC025">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC025-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7100"/>
</technology>
<technology name="LC128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC128-I/ST"/>
<attribute name="OC_FARNELL" value="1296573"/>
<attribute name="OC_NEWARK" value="62K0578"/>
</technology>
<technology name="LC64">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC64X-I/ST"/>
<attribute name="OC_FARNELL" value="1296582"/>
<attribute name="OC_NEWARK" value="96K4081"/>
</technology>
<technology name="LCS52">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LCS52T/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7040"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="28*04A" prefix="IC">
<description>CMOS &lt;B&gt;EPROM&lt;/B&gt; 4 K (512 x 8)&lt;p&gt;
Source: ww1.microchip.com/downloads/en/DeviceDoc/11126H.pdf</description>
<gates>
<gate name="G$1" symbol="28C04"/>
</gates>
<devices>
<device name="P" package="DIL24-6">
<connects>
<connect gate="G$1" pin="!CE" pad="18"/>
<connect gate="G$1" pin="!OE" pad="20"/>
<connect gate="G$1" pin="!WE" pad="21"/>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="4"/>
<connect gate="G$1" pin="A5" pad="3"/>
<connect gate="G$1" pin="A6" pad="2"/>
<connect gate="G$1" pin="A7" pad="1"/>
<connect gate="G$1" pin="A8" pad="23"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="14"/>
<connect gate="G$1" pin="D5" pad="15"/>
<connect gate="G$1" pin="D6" pad="16"/>
<connect gate="G$1" pin="D7" pad="17"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC19" pad="19"/>
<connect gate="G$1" pin="NC22" pad="22"/>
<connect gate="G$1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC-32">
<connects>
<connect gate="G$1" pin="!CE" pad="23"/>
<connect gate="G$1" pin="!OE" pad="25"/>
<connect gate="G$1" pin="!WE" pad="31"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="21"/>
<connect gate="G$1" pin="D7" pad="22"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC19" pad="1"/>
<connect gate="G$1" pin="NC22" pad="17"/>
<connect gate="G$1" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="28*16A" prefix="IC">
<description>CMOS &lt;B&gt;EPROM&lt;/B&gt; 16 K (2 K x 8)&lt;p&gt;
Source: ww1.microchip.com/downloads/en/DeviceDoc/11125J.pdf</description>
<gates>
<gate name="G$1" symbol="28C16"/>
</gates>
<devices>
<device name="L" package="PLCC-32">
<connects>
<connect gate="G$1" pin="!CE" pad="23"/>
<connect gate="G$1" pin="!OE" pad="25"/>
<connect gate="G$1" pin="!WE" pad="31"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="A9" pad="28"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="21"/>
<connect gate="G$1" pin="D7" pad="22"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT28C16AGI-12"/>
<attribute name="OC_FARNELL" value="1718288"/>
<attribute name="OC_NEWARK" value="06R0639"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL24-6">
<connects>
<connect gate="G$1" pin="!CE" pad="18"/>
<connect gate="G$1" pin="!OE" pad="20"/>
<connect gate="G$1" pin="!WE" pad="21"/>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="A10" pad="19"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="4"/>
<connect gate="G$1" pin="A5" pad="3"/>
<connect gate="G$1" pin="A6" pad="2"/>
<connect gate="G$1" pin="A7" pad="1"/>
<connect gate="G$1" pin="A8" pad="23"/>
<connect gate="G$1" pin="A9" pad="22"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="14"/>
<connect gate="G$1" pin="D5" pad="15"/>
<connect gate="G$1" pin="D6" pad="16"/>
<connect gate="G$1" pin="D7" pad="17"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT28C16ALI-12"/>
<attribute name="OC_FARNELL" value="1718292"/>
<attribute name="OC_NEWARK" value="06R0648"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSOP28">
<connects>
<connect gate="G$1" pin="!CE" pad="27"/>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="!WE" pad="6"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A10" pad="28"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="3"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="D5" pad="24"/>
<connect gate="G$1" pin="D6" pad="25"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="VS" package="VSOP28-8X13">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1718287"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="28*17A" prefix="IC">
<description>CMOS &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
16 K (2 K x 8)</description>
<gates>
<gate name="G$1" symbol="28C17"/>
<gate name="2" symbol="NC"/>
<gate name="23" symbol="NC"/>
<gate name="26" symbol="NC"/>
</gates>
<devices>
<device name="P" package="DIL28-6">
<connects>
<connect gate="2" pin="NC" pad="2"/>
<connect gate="23" pin="NC" pad="23"/>
<connect gate="26" pin="NC" pad="26"/>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="RDY/!BSY" pad="1"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT28C17ALI20"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="71R7405"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC-32">
<connects>
<connect gate="2" pin="NC" pad="1"/>
<connect gate="23" pin="NC" pad="3"/>
<connect gate="26" pin="NC" pad="12"/>
<connect gate="G$1" pin="!CE" pad="23"/>
<connect gate="G$1" pin="!OE" pad="25"/>
<connect gate="G$1" pin="!WE" pad="31"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="A9" pad="28"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="21"/>
<connect gate="G$1" pin="D7" pad="22"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="RDY/!BSY" pad="2"/>
<connect gate="G$1" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="VS" package="VSOP28-8X13">
<connects>
<connect gate="2" pin="NC" pad="2"/>
<connect gate="23" pin="NC" pad="23"/>
<connect gate="26" pin="NC" pad="26"/>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="RDY/!BSY" pad="1"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSOP28">
<connects>
<connect gate="2" pin="NC" pad="2"/>
<connect gate="23" pin="NC" pad="5"/>
<connect gate="26" pin="NC" pad="9"/>
<connect gate="G$1" pin="!CE" pad="27"/>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="!WE" pad="6"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A10" pad="28"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="3"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="D5" pad="24"/>
<connect gate="G$1" pin="D6" pad="25"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="RDY/!BSY" pad="8"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="2" pin="NC" pad="2"/>
<connect gate="23" pin="NC" pad="23"/>
<connect gate="26" pin="NC" pad="26"/>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="RDY/!BSY" pad="1"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="28*64A" prefix="IC">
<description>CMOS &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
64 K (8 K x 8), low voltage</description>
<gates>
<gate name="G$1" symbol="28C64"/>
</gates>
<devices>
<device name="L" package="PLCC-32">
<connects>
<connect gate="G$1" pin="!CE" pad="23"/>
<connect gate="G$1" pin="!OE" pad="25"/>
<connect gate="G$1" pin="!WE" pad="31"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A11" pad="27"/>
<connect gate="G$1" pin="A12" pad="3"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="A9" pad="28"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="21"/>
<connect gate="G$1" pin="D7" pad="22"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="RDY/!BSY" pad="2"/>
<connect gate="G$1" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT28C64BGI-12T"/>
<attribute name="OC_FARNELL" value="1718494"/>
<attribute name="OC_NEWARK" value="08R5439"/>
</technology>
<technology name="VL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="RDY/!BSY" pad="1"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT28C64B-15PU"/>
<attribute name="OC_FARNELL" value="1631144"/>
<attribute name="OC_NEWARK" value="96K6557"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT28LV64LI-25"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="06R0912"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="RDY/!BSY" pad="1"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT28C64BWI-12"/>
<attribute name="OC_FARNELL" value="1718312"/>
<attribute name="OC_NEWARK" value="06R0739"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT28LV64W-25"/>
<attribute name="OC_FARNELL" value="1718338"/>
<attribute name="OC_NEWARK" value="06R0915"/>
</technology>
</technologies>
</device>
<device name="VS" package="VSOP28-8X13">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="RDY/!BSY" pad="1"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSOP28">
<connects>
<connect gate="G$1" pin="!CE" pad="27"/>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="!WE" pad="6"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A10" pad="28"/>
<connect gate="G$1" pin="A11" pad="2"/>
<connect gate="G$1" pin="A12" pad="9"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="3"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="D5" pad="24"/>
<connect gate="G$1" pin="D6" pad="25"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="RDY/!BSY" pad="8"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT28LV64H13-20"/>
<attribute name="OC_FARNELL" value="1718417"/>
<attribute name="OC_NEWARK" value="06R0901"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27*128" prefix="IC">
<description>CMOS &lt;B&gt;EPROM&lt;/B&gt;&lt;p&gt;
128 K (16 K x 8)</description>
<gates>
<gate name="G$1" symbol="27C128"/>
</gates>
<devices>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!PGM" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC-32">
<connects>
<connect gate="G$1" pin="!CE" pad="23"/>
<connect gate="G$1" pin="!OE" pad="25"/>
<connect gate="G$1" pin="!PGM" pad="31"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A11" pad="27"/>
<connect gate="G$1" pin="A12" pad="3"/>
<connect gate="G$1" pin="A13" pad="30"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="A9" pad="28"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="21"/>
<connect gate="G$1" pin="D7" pad="22"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="32"/>
<connect gate="G$1" pin="VPP" pad="2"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSOP28">
<connects>
<connect gate="G$1" pin="!CE" pad="27"/>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="!PGM" pad="6"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A10" pad="28"/>
<connect gate="G$1" pin="A11" pad="2"/>
<connect gate="G$1" pin="A12" pad="9"/>
<connect gate="G$1" pin="A13" pad="5"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="3"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="D5" pad="24"/>
<connect gate="G$1" pin="D6" pad="25"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VPP" pad="8"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27*256" prefix="IC">
<description>CMOS &lt;B&gt;EPROM&lt;/B&gt;&lt;p&gt;
256 K (32 K x 8), low voltage</description>
<gates>
<gate name="G$1" symbol="27C256"/>
</gates>
<devices>
<device name="L" package="PLCC-32">
<connects>
<connect gate="G$1" pin="!CE" pad="23"/>
<connect gate="G$1" pin="!OE" pad="25"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A11" pad="27"/>
<connect gate="G$1" pin="A12" pad="3"/>
<connect gate="G$1" pin="A13" pad="30"/>
<connect gate="G$1" pin="A14" pad="31"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="A9" pad="28"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="21"/>
<connect gate="G$1" pin="D7" pad="22"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="32"/>
<connect gate="G$1" pin="VPP" pad="2"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT27C256R-70JU"/>
<attribute name="OC_FARNELL" value="1095779"/>
<attribute name="OC_NEWARK" value="96K6554"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="M27C256B15F1"/>
<attribute name="OC_FARNELL" value="1125431"/>
<attribute name="OC_NEWARK" value="93K7335"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="VS" package="VSOP28-8X13">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSOP28">
<connects>
<connect gate="G$1" pin="!CE" pad="27"/>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A10" pad="28"/>
<connect gate="G$1" pin="A11" pad="2"/>
<connect gate="G$1" pin="A12" pad="9"/>
<connect gate="G$1" pin="A13" pad="5"/>
<connect gate="G$1" pin="A14" pad="6"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="3"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="D5" pad="24"/>
<connect gate="G$1" pin="D6" pad="25"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VPP" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27*512A" prefix="IC">
<description>CMOS &lt;B&gt;EPROM&lt;/B&gt;&lt;p&gt;
512 K (64 K x 8)</description>
<gates>
<gate name="G$1" symbol="27C512"/>
</gates>
<devices>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP/!OE" pad="22"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M27C512-90B6"/>
<attribute name="OC_FARNELL" value="1642690"/>
<attribute name="OC_NEWARK" value="20M6389"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP/!OE" pad="22"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC-32">
<connects>
<connect gate="G$1" pin="!CE" pad="23"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A11" pad="27"/>
<connect gate="G$1" pin="A12" pad="3"/>
<connect gate="G$1" pin="A13" pad="30"/>
<connect gate="G$1" pin="A14" pad="31"/>
<connect gate="G$1" pin="A15" pad="2"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="A9" pad="28"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="21"/>
<connect gate="G$1" pin="D7" pad="22"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="32"/>
<connect gate="G$1" pin="VPP/!OE" pad="25"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M27C512-90C1"/>
<attribute name="OC_FARNELL" value="1218315"/>
<attribute name="OC_NEWARK" value="24M5090"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSOP28">
<connects>
<connect gate="G$1" pin="!CE" pad="27"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A10" pad="28"/>
<connect gate="G$1" pin="A11" pad="2"/>
<connect gate="G$1" pin="A12" pad="9"/>
<connect gate="G$1" pin="A13" pad="5"/>
<connect gate="G$1" pin="A14" pad="6"/>
<connect gate="G$1" pin="A15" pad="8"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="3"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="D5" pad="24"/>
<connect gate="G$1" pin="D6" pad="25"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VPP/!OE" pad="1"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="VS" package="VSOP28-8X13">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP/!OE" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27*1616" prefix="IC">
<description>&lt;B&gt;EPROM&lt;/B&gt; Obsolete/EOL</description>
<gates>
<gate name="G$1" symbol="27HC1616"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!CE" pad="2"/>
<connect gate="G$1" pin="!OE" pad="20"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="22"/>
<connect gate="G$1" pin="A10" pad="32"/>
<connect gate="G$1" pin="A11" pad="33"/>
<connect gate="G$1" pin="A12" pad="34"/>
<connect gate="G$1" pin="A13" pad="35"/>
<connect gate="G$1" pin="A2" pad="23"/>
<connect gate="G$1" pin="A3" pad="24"/>
<connect gate="G$1" pin="A4" pad="25"/>
<connect gate="G$1" pin="A5" pad="26"/>
<connect gate="G$1" pin="A6" pad="27"/>
<connect gate="G$1" pin="A7" pad="28"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="A9" pad="31"/>
<connect gate="G$1" pin="D0" pad="19"/>
<connect gate="G$1" pin="D1" pad="18"/>
<connect gate="G$1" pin="D10" pad="8"/>
<connect gate="G$1" pin="D11" pad="7"/>
<connect gate="G$1" pin="D12" pad="6"/>
<connect gate="G$1" pin="D13" pad="5"/>
<connect gate="G$1" pin="D14" pad="4"/>
<connect gate="G$1" pin="D15" pad="3"/>
<connect gate="G$1" pin="D2" pad="17"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="12"/>
<connect gate="G$1" pin="D8" pad="10"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="30"/>
<connect gate="G$1" pin="NU36" pad="36"/>
<connect gate="G$1" pin="NU37" pad="37"/>
<connect gate="G$1" pin="NU38" pad="38"/>
<connect gate="G$1" pin="PGM" pad="39"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="LCC44">
<connects>
<connect gate="G$1" pin="!CE" pad="3"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="25"/>
<connect gate="G$1" pin="A10" pad="36"/>
<connect gate="G$1" pin="A11" pad="37"/>
<connect gate="G$1" pin="A12" pad="38"/>
<connect gate="G$1" pin="A13" pad="39"/>
<connect gate="G$1" pin="A2" pad="26"/>
<connect gate="G$1" pin="A3" pad="27"/>
<connect gate="G$1" pin="A4" pad="28"/>
<connect gate="G$1" pin="A5" pad="29"/>
<connect gate="G$1" pin="A6" pad="30"/>
<connect gate="G$1" pin="A7" pad="31"/>
<connect gate="G$1" pin="A8" pad="32"/>
<connect gate="G$1" pin="A9" pad="35"/>
<connect gate="G$1" pin="D0" pad="21"/>
<connect gate="G$1" pin="D1" pad="20"/>
<connect gate="G$1" pin="D10" pad="9"/>
<connect gate="G$1" pin="D11" pad="8"/>
<connect gate="G$1" pin="D12" pad="7"/>
<connect gate="G$1" pin="D13" pad="6"/>
<connect gate="G$1" pin="D14" pad="5"/>
<connect gate="G$1" pin="D15" pad="4"/>
<connect gate="G$1" pin="D2" pad="19"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="16"/>
<connect gate="G$1" pin="D6" pad="15"/>
<connect gate="G$1" pin="D7" pad="14"/>
<connect gate="G$1" pin="D8" pad="11"/>
<connect gate="G$1" pin="D9" pad="10"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="34"/>
<connect gate="G$1" pin="NU36" pad="13"/>
<connect gate="G$1" pin="NU37" pad="23"/>
<connect gate="G$1" pin="NU38" pad="33"/>
<connect gate="G$1" pin="PGM" pad="43"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="VPP" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27*64" prefix="IC">
<description>CMOS &lt;B&gt;EPROM&lt;/B&gt;&lt;p&gt;
64 K (8 K x 8), low voltage</description>
<gates>
<gate name="G$1" symbol="27C64"/>
</gates>
<devices>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="NC" pad="26"/>
<connect gate="G$1" pin="PGM" pad="27"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="NC" pad="26"/>
<connect gate="G$1" pin="PGM" pad="27"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="M27C64A-10F1"/>
<attribute name="OC_FARNELL" value="1094265"/>
<attribute name="OC_NEWARK" value="93K7339"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC-32">
<connects>
<connect gate="G$1" pin="!CE" pad="23"/>
<connect gate="G$1" pin="!OE" pad="25"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A11" pad="27"/>
<connect gate="G$1" pin="A12" pad="3"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="29"/>
<connect gate="G$1" pin="A9" pad="28"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="21"/>
<connect gate="G$1" pin="D7" pad="22"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="PGM" pad="31"/>
<connect gate="G$1" pin="VCC" pad="32"/>
<connect gate="G$1" pin="VPP" pad="2"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSOP28">
<connects>
<connect gate="G$1" pin="!CE" pad="27"/>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A10" pad="28"/>
<connect gate="G$1" pin="A11" pad="2"/>
<connect gate="G$1" pin="A12" pad="9"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="3"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="D5" pad="24"/>
<connect gate="G$1" pin="D6" pad="25"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="PGM" pad="6"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VPP" pad="8"/>
</connects>
<technologies>
<technology name="LV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AY0438" prefix="IC">
<description>&lt;B&gt;LCD DRIVER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="AY0438"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="BP" pad="30"/>
<connect gate="G$1" pin="CLK" pad="40"/>
<connect gate="G$1" pin="DI" pad="34"/>
<connect gate="G$1" pin="DO" pad="35"/>
<connect gate="G$1" pin="GND" pad="36"/>
<connect gate="G$1" pin="LCD0" pad="31"/>
<connect gate="G$1" pin="LOAD" pad="2"/>
<connect gate="G$1" pin="SEG1" pad="39"/>
<connect gate="G$1" pin="SEG10" pad="25"/>
<connect gate="G$1" pin="SEG11" pad="24"/>
<connect gate="G$1" pin="SEG12" pad="23"/>
<connect gate="G$1" pin="SEG13" pad="22"/>
<connect gate="G$1" pin="SEG14" pad="21"/>
<connect gate="G$1" pin="SEG15" pad="20"/>
<connect gate="G$1" pin="SEG16" pad="19"/>
<connect gate="G$1" pin="SEG17" pad="18"/>
<connect gate="G$1" pin="SEG18" pad="17"/>
<connect gate="G$1" pin="SEG19" pad="16"/>
<connect gate="G$1" pin="SEG2" pad="38"/>
<connect gate="G$1" pin="SEG20" pad="15"/>
<connect gate="G$1" pin="SEG21" pad="14"/>
<connect gate="G$1" pin="SEG22" pad="13"/>
<connect gate="G$1" pin="SEG23" pad="12"/>
<connect gate="G$1" pin="SEG24" pad="11"/>
<connect gate="G$1" pin="SEG25" pad="10"/>
<connect gate="G$1" pin="SEG26" pad="9"/>
<connect gate="G$1" pin="SEG27" pad="8"/>
<connect gate="G$1" pin="SEG28" pad="7"/>
<connect gate="G$1" pin="SEG29" pad="6"/>
<connect gate="G$1" pin="SEG3" pad="37"/>
<connect gate="G$1" pin="SEG30" pad="5"/>
<connect gate="G$1" pin="SEG31" pad="4"/>
<connect gate="G$1" pin="SEG32" pad="3"/>
<connect gate="G$1" pin="SEG4" pad="33"/>
<connect gate="G$1" pin="SEG5" pad="32"/>
<connect gate="G$1" pin="SEG6" pad="29"/>
<connect gate="G$1" pin="SEG7" pad="28"/>
<connect gate="G$1" pin="SEG8" pad="27"/>
<connect gate="G$1" pin="SEG9" pad="26"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="AY0438/P"/>
<attribute name="OC_FARNELL" value="1627184"/>
<attribute name="OC_NEWARK" value="23C2747"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="BP" pad="33"/>
<connect gate="G$1" pin="CLK" pad="44"/>
<connect gate="G$1" pin="DI" pad="37"/>
<connect gate="G$1" pin="DO" pad="38"/>
<connect gate="G$1" pin="GND" pad="40"/>
<connect gate="G$1" pin="LCD0" pad="34"/>
<connect gate="G$1" pin="LOAD" pad="2"/>
<connect gate="G$1" pin="SEG1" pad="43"/>
<connect gate="G$1" pin="SEG10" pad="26"/>
<connect gate="G$1" pin="SEG11" pad="25"/>
<connect gate="G$1" pin="SEG12" pad="24"/>
<connect gate="G$1" pin="SEG13" pad="23"/>
<connect gate="G$1" pin="SEG14" pad="22"/>
<connect gate="G$1" pin="SEG15" pad="21"/>
<connect gate="G$1" pin="SEG16" pad="20"/>
<connect gate="G$1" pin="SEG17" pad="19"/>
<connect gate="G$1" pin="SEG18" pad="18"/>
<connect gate="G$1" pin="SEG19" pad="17"/>
<connect gate="G$1" pin="SEG2" pad="42"/>
<connect gate="G$1" pin="SEG20" pad="16"/>
<connect gate="G$1" pin="SEG21" pad="15"/>
<connect gate="G$1" pin="SEG22" pad="14"/>
<connect gate="G$1" pin="SEG23" pad="13"/>
<connect gate="G$1" pin="SEG24" pad="12"/>
<connect gate="G$1" pin="SEG25" pad="11"/>
<connect gate="G$1" pin="SEG26" pad="10"/>
<connect gate="G$1" pin="SEG27" pad="9"/>
<connect gate="G$1" pin="SEG28" pad="8"/>
<connect gate="G$1" pin="SEG29" pad="7"/>
<connect gate="G$1" pin="SEG3" pad="41"/>
<connect gate="G$1" pin="SEG30" pad="5"/>
<connect gate="G$1" pin="SEG31" pad="4"/>
<connect gate="G$1" pin="SEG32" pad="3"/>
<connect gate="G$1" pin="SEG4" pad="36"/>
<connect gate="G$1" pin="SEG5" pad="35"/>
<connect gate="G$1" pin="SEG6" pad="32"/>
<connect gate="G$1" pin="SEG7" pad="31"/>
<connect gate="G$1" pin="SEG8" pad="30"/>
<connect gate="G$1" pin="SEG9" pad="27"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="AY0438/L"/>
<attribute name="OC_FARNELL" value="1467690"/>
<attribute name="OC_NEWARK" value="96K3652"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HCS410" prefix="IC">
<description>&lt;B&gt;ENCODER&lt;/B&gt;&lt;p&gt;
code hopping encoder and transponder</description>
<gates>
<gate name="P1" symbol="HCS410"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="P1" pin="GND" pad="5"/>
<connect gate="P1" pin="LC0" pad="7"/>
<connect gate="P1" pin="LC1" pad="4"/>
<connect gate="P1" pin="PWM" pad="6"/>
<connect gate="P1" pin="S0" pad="1"/>
<connect gate="P1" pin="S1" pad="2"/>
<connect gate="P1" pin="S2/LED" pad="3"/>
<connect gate="P1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="HCS410-I/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K3679"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO-08">
<connects>
<connect gate="P1" pin="GND" pad="5"/>
<connect gate="P1" pin="LC0" pad="7"/>
<connect gate="P1" pin="LC1" pad="4"/>
<connect gate="P1" pin="PWM" pad="6"/>
<connect gate="P1" pin="S0" pad="1"/>
<connect gate="P1" pin="S1" pad="2"/>
<connect gate="P1" pin="S2/LED" pad="3"/>
<connect gate="P1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSSOP8">
<connects>
<connect gate="P1" pin="GND" pad="3"/>
<connect gate="P1" pin="LC0" pad="5"/>
<connect gate="P1" pin="LC1" pad="2"/>
<connect gate="P1" pin="PWM" pad="4"/>
<connect gate="P1" pin="S0" pad="7"/>
<connect gate="P1" pin="S1" pad="8"/>
<connect gate="P1" pin="S2/LED" pad="1"/>
<connect gate="P1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="HCS410-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33C0783"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24*00" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
128 bit, I2C (AA = 1.8 V/LC = 2.5 V/C = 5.0 V)</description>
<gates>
<gate name="G$1" symbol="SERIALEEPROM"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA00-I/P"/>
<attribute name="OC_FARNELL" value="1331262"/>
<attribute name="OC_NEWARK" value="68K7385"/>
</technology>
<technology name="C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C00/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4058"/>
</technology>
<technology name="LC">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC00/P"/>
<attribute name="OC_FARNELL" value="9757856"/>
<attribute name="OC_NEWARK" value="96K4068"/>
</technology>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA00-I/STG"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89H3037"/>
</technology>
<technology name="C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C00-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C6932"/>
</technology>
<technology name="LC">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC00-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4067"/>
</technology>
</technologies>
</device>
<device name="OT" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA00T-I/OTG"/>
<attribute name="OC_FARNELL" value="1331264"/>
<attribute name="OC_NEWARK" value="89H3038"/>
</technology>
<technology name="C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C00T-I/OT"/>
<attribute name="OC_FARNELL" value="1818713"/>
<attribute name="OC_NEWARK" value="92C6937"/>
</technology>
<technology name="LC">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC00T-I/OT"/>
<attribute name="OC_FARNELL" value="9757864"/>
<attribute name="OC_NEWARK" value="62K0574"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA00-I/SN"/>
<attribute name="OC_FARNELL" value="1331263"/>
<attribute name="OC_NEWARK" value="92C6779"/>
</technology>
<technology name="C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C00/SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4059"/>
</technology>
<technology name="LC">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC00/SN"/>
<attribute name="OC_FARNELL" value="1137303"/>
<attribute name="OC_NEWARK" value="69K7667"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24LC*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
128 byte/1 K, 2.5 V, dual mode I2C</description>
<gates>
<gate name="G$1" symbol="SERIAL-EEPROM-DUAL"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VCLK" pad="7"/>
</connects>
<technologies>
<technology name="S21A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LCS21A/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7023"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VCLK" pad="7"/>
</connects>
<technologies>
<technology name="S21A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LCS21A/SN"/>
<attribute name="OC_FARNELL" value="1847803"/>
<attribute name="OC_NEWARK" value="92C7025"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24L*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
128 byte/1 K</description>
<gates>
<gate name="G$1" symbol="24-LC"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VCLK" pad="7"/>
</connects>
<technologies>
<technology name="C21">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC21/P"/>
<attribute name="OC_FARNELL" value="1818716"/>
<attribute name="OC_NEWARK" value="92C7157"/>
</technology>
<technology name="C21A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC21A-I/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C7160"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VCLK" pad="7"/>
</connects>
<technologies>
<technology name="C21">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC21/SN"/>
<attribute name="OC_FARNELL" value="1816067"/>
<attribute name="OC_NEWARK" value="92C7159"/>
</technology>
<technology name="C21A">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC21A/SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89C9809"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24LC41A" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
128/512 byte, dual port</description>
<gates>
<gate name="G$1" symbol="24LC41"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="!DWP" pad="2"/>
<connect gate="G$1" pin="DSCL" pad="1"/>
<connect gate="G$1" pin="DSDA" pad="8"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MSCL" pad="5"/>
<connect gate="G$1" pin="MSDA" pad="4"/>
<connect gate="G$1" pin="MWP" pad="6"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24LCS6*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
1 K/2 K</description>
<gates>
<gate name="G$1" symbol="24LC61"/>
</gates>
<devices>
<device name="N" package="DIL8">
<connects>
<connect gate="G$1" pin="!EDS" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="!EDS" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="!EDS" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24-*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
32 K/64 K, 1.8 V, I2C</description>
<gates>
<gate name="G$1" symbol="24AA32"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA65">
<attribute name="MF" value=""/>
<attribute name="MPN" value="24AA65/P"/>
<attribute name="OC_FARNELL" value="1331306"/>
<attribute name="OC_NEWARK" value="35M0721"/>
</technology>
<technology name="C32">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C32C-PU"/>
<attribute name="OC_FARNELL" value="1362652"/>
<attribute name="OC_NEWARK" value="50M3325"/>
</technology>
<technology name="C65">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C65/P"/>
<attribute name="OC_FARNELL" value="9757821"/>
<attribute name="OC_NEWARK" value="89C9798"/>
</technology>
<technology name="FC32">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="FC65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC32">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC32A/P"/>
<attribute name="OC_FARNELL" value="1084246"/>
<attribute name="OC_NEWARK" value="75K1884"/>
</technology>
<technology name="LC65">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC65/P"/>
<attribute name="OC_FARNELL" value="9758089"/>
<attribute name="OC_NEWARK" value="88K1357"/>
</technology>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA65">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24AA65/SM"/>
<attribute name="OC_FARNELL" value="1331307"/>
<attribute name="OC_NEWARK" value="92C6926"/>
</technology>
<technology name="C32">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M24C32-WMN6P"/>
<attribute name="OC_FARNELL" value="1362654"/>
<attribute name="OC_NEWARK" value="56P9110"/>
</technology>
<technology name="C65">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24C65/SM"/>
<attribute name="OC_FARNELL" value="1467721"/>
<attribute name="OC_NEWARK" value="96K4066"/>
</technology>
<technology name="FC32">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="FC65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC32">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC32A/SM"/>
<attribute name="OC_FARNELL" value="1212670"/>
<attribute name="OC_NEWARK" value="96K4080"/>
</technology>
<technology name="LC65">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="24LC65/SM"/>
<attribute name="OC_FARNELL" value="9758097"/>
<attribute name="OC_NEWARK" value="96K4082"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="37LV*" prefix="IC">
<description>Serial &lt;B&gt;EPROM&lt;/B&gt;&lt;p&gt;
36 K/64 K/128 K</description>
<gates>
<gate name="G$1" symbol="37LV"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="!CE" pad="4"/>
<connect gate="G$1" pin="!CEO" pad="6"/>
<connect gate="G$1" pin="!OE" pad="3"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="DATA" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VPP" pad="7"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="!CE" pad="4"/>
<connect gate="G$1" pin="!CEO" pad="6"/>
<connect gate="G$1" pin="!OE" pad="3"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="DATA" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VPP" pad="7"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC20S">
<connects>
<connect gate="G$1" pin="!CE" pad="8"/>
<connect gate="G$1" pin="!CEO" pad="14"/>
<connect gate="G$1" pin="!OE" pad="6"/>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VPP" pad="17"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="25*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt; 4K/ 8K , SPI bus&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="25SERIAL"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA040">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25AA040-I/P"/>
<attribute name="OC_FARNELL" value="1331347"/>
<attribute name="OC_NEWARK" value="92C7334"/>
</technology>
<technology name="AA080">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25AA080/P"/>
<attribute name="OC_FARNELL" value="1331352"/>
<attribute name="OC_NEWARK" value="92C7349"/>
</technology>
<technology name="C040">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25C040/P"/>
<attribute name="OC_FARNELL" value="1607554"/>
<attribute name="OC_NEWARK" value="96K4084"/>
</technology>
<technology name="C080">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25C080-I/P"/>
<attribute name="OC_FARNELL" value="1816073"/>
<attribute name="OC_NEWARK" value="92C7398"/>
</technology>
<technology name="LC040">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25LC040/P"/>
<attribute name="OC_FARNELL" value="9758100"/>
<attribute name="OC_NEWARK" value="96K4091"/>
</technology>
<technology name="LC080">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25LC080/P"/>
<attribute name="OC_FARNELL" value="1556143"/>
<attribute name="OC_NEWARK" value="92C7440"/>
</technology>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA040">
<attribute name="MF" value=""/>
<attribute name="MPN" value="25AA040A-I/MS"/>
<attribute name="OC_FARNELL" value="1331345"/>
<attribute name="OC_NEWARK" value="35M0801"/>
</technology>
<technology name="C040">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25C040T/SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="30C5312"/>
</technology>
<technology name="LC040">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25LC040A-I/ST"/>
<attribute name="OC_FARNELL" value="1815998"/>
<attribute name="OC_NEWARK" value="72J3684"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA080">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25AA080/SN"/>
<attribute name="OC_FARNELL" value="1816072"/>
<attribute name="OC_NEWARK" value="92C7351"/>
</technology>
<technology name="C080">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25C080/SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4086"/>
</technology>
<technology name="LC080">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="25LC080/SN"/>
<attribute name="OC_FARNELL" value="1137302"/>
<attribute name="OC_NEWARK" value="96K4092"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*870" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
flash type</description>
<gates>
<gate name="G$1" symbol="PIC16F870"/>
</gates>
<devices>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F870-I/SO"/>
<attribute name="OC_FARNELL" value="9760946"/>
<attribute name="OC_NEWARK" value="61K3457"/>
</technology>
<technology name="LF">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF870-I/SO"/>
<attribute name="OC_FARNELL" value="1815914"/>
<attribute name="OC_NEWARK" value="23C5702"/>
</technology>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F870-I/SS"/>
<attribute name="OC_FARNELL" value="9760962"/>
<attribute name="OC_NEWARK" value="96K3885"/>
</technology>
<technology name="LF">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF870-I/SS"/>
<attribute name="OC_FARNELL" value="1818506"/>
<attribute name="OC_NEWARK" value="23C5704"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F870-I/SP"/>
<attribute name="OC_FARNELL" value="9760954"/>
<attribute name="OC_NEWARK" value="19C7275"/>
</technology>
<technology name="LF">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF870-I/SP"/>
<attribute name="OC_FARNELL" value="1579594"/>
<attribute name="OC_NEWARK" value="69K7641"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*871" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
flash type</description>
<gates>
<gate name="G$1" symbol="PIC16F871"/>
</gates>
<devices>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="2"/>
<connect gate="G$1" pin="INT/RB0" pad="36"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="14"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="15"/>
<connect gate="G$1" pin="PGC/RB6" pad="43"/>
<connect gate="G$1" pin="PGD/RB7" pad="44"/>
<connect gate="G$1" pin="PGM/RB3" pad="39"/>
<connect gate="G$1" pin="PSP4/RD4" pad="30"/>
<connect gate="G$1" pin="PSP5/RD5" pad="31"/>
<connect gate="G$1" pin="PSP6/RD6" pad="32"/>
<connect gate="G$1" pin="PSP7/RD7" pad="33"/>
<connect gate="G$1" pin="RA0/AN0" pad="3"/>
<connect gate="G$1" pin="RA1/AN1" pad="4"/>
<connect gate="G$1" pin="RA2/AN2" pad="5"/>
<connect gate="G$1" pin="RA3/AN3" pad="6"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="7"/>
<connect gate="G$1" pin="RA5/AN4" pad="8"/>
<connect gate="G$1" pin="RB1" pad="37"/>
<connect gate="G$1" pin="RB2" pad="38"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5" pad="42"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="16"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="18"/>
<connect gate="G$1" pin="RC2/CCP1" pad="19"/>
<connect gate="G$1" pin="RC3" pad="20"/>
<connect gate="G$1" pin="RC4" pad="25"/>
<connect gate="G$1" pin="RC5" pad="26"/>
<connect gate="G$1" pin="RD0/PSP0" pad="21"/>
<connect gate="G$1" pin="RD1/PSP1" pad="22"/>
<connect gate="G$1" pin="RD2/PSP2" pad="23"/>
<connect gate="G$1" pin="RD3/PSP3" pad="24"/>
<connect gate="G$1" pin="RE0/!RD/AN5" pad="9"/>
<connect gate="G$1" pin="RE1/!WR/AN6" pad="10"/>
<connect gate="G$1" pin="RE2/!CS/AN7" pad="11"/>
<connect gate="G$1" pin="RX/RC7" pad="29"/>
<connect gate="G$1" pin="TX/RC6" pad="27"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="35"/>
<connect gate="G$1" pin="VSS" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="34"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="9760970"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LF">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF871-I/L"/>
<attribute name="OC_FARNELL" value="9761705"/>
<attribute name="OC_NEWARK" value="23C5707"/>
</technology>
</technologies>
</device>
<device name="T" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="18"/>
<connect gate="G$1" pin="INT/RB0" pad="8"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="30"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="31"/>
<connect gate="G$1" pin="PGC/RB6" pad="16"/>
<connect gate="G$1" pin="PGD/RB7" pad="17"/>
<connect gate="G$1" pin="PGM/RB3" pad="11"/>
<connect gate="G$1" pin="PSP4/RD4" pad="2"/>
<connect gate="G$1" pin="PSP5/RD5" pad="3"/>
<connect gate="G$1" pin="PSP6/RD6" pad="4"/>
<connect gate="G$1" pin="PSP7/RD7" pad="5"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="32"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1" pad="36"/>
<connect gate="G$1" pin="RC3" pad="37"/>
<connect gate="G$1" pin="RC4" pad="42"/>
<connect gate="G$1" pin="RC5" pad="43"/>
<connect gate="G$1" pin="RD0/PSP0" pad="38"/>
<connect gate="G$1" pin="RD1/PSP1" pad="39"/>
<connect gate="G$1" pin="RD2/PSP2" pad="40"/>
<connect gate="G$1" pin="RD3/PSP3" pad="41"/>
<connect gate="G$1" pin="RE0/!RD/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/!WR/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/!CS/AN7" pad="27"/>
<connect gate="G$1" pin="RX/RC7" pad="1"/>
<connect gate="G$1" pin="TX/RC6" pad="44"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F871-I/PT"/>
<attribute name="OC_FARNELL" value="9760997"/>
<attribute name="OC_NEWARK" value="23C5040"/>
</technology>
<technology name="LF">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF871-I/PT"/>
<attribute name="OC_FARNELL" value="9761713"/>
<attribute name="OC_NEWARK" value="23C5709"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="33"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="13"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="14"/>
<connect gate="G$1" pin="PGC/RB6" pad="39"/>
<connect gate="G$1" pin="PGD/RB7" pad="40"/>
<connect gate="G$1" pin="PGM/RB3" pad="36"/>
<connect gate="G$1" pin="PSP4/RD4" pad="27"/>
<connect gate="G$1" pin="PSP5/RD5" pad="28"/>
<connect gate="G$1" pin="PSP6/RD6" pad="29"/>
<connect gate="G$1" pin="PSP7/RD7" pad="30"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="15"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="16"/>
<connect gate="G$1" pin="RC2/CCP1" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RD0/PSP0" pad="19"/>
<connect gate="G$1" pin="RD1/PSP1" pad="20"/>
<connect gate="G$1" pin="RD2/PSP2" pad="21"/>
<connect gate="G$1" pin="RD3/PSP3" pad="22"/>
<connect gate="G$1" pin="RE0/!RD/AN5" pad="8"/>
<connect gate="G$1" pin="RE1/!WR/AN6" pad="9"/>
<connect gate="G$1" pin="RE2/!CS/AN7" pad="10"/>
<connect gate="G$1" pin="RX/RC7" pad="26"/>
<connect gate="G$1" pin="TX/RC6" pad="25"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F871-I/P"/>
<attribute name="OC_FARNELL" value="9760989"/>
<attribute name="OC_NEWARK" value="80K6048"/>
</technology>
<technology name="LF">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16LF871-I/P"/>
<attribute name="OC_FARNELL" value="1084329"/>
<attribute name="OC_NEWARK" value="97K7488"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*872" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
flash type</description>
<gates>
<gate name="G$1" symbol="PIC16F872"/>
</gates>
<devices>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F872-I/SO"/>
<attribute name="OC_FARNELL" value="9761004"/>
<attribute name="OC_NEWARK" value="96K3886"/>
</technology>
<technology name="LF">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF872-I/SO"/>
<attribute name="OC_FARNELL" value="9761721"/>
<attribute name="OC_NEWARK" value="68K5334"/>
</technology>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F872-I/SS"/>
<attribute name="OC_FARNELL" value="1084299"/>
<attribute name="OC_NEWARK" value="96K3887"/>
</technology>
<technology name="LF">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF872-I/SS"/>
<attribute name="OC_FARNELL" value="9761748"/>
<attribute name="OC_NEWARK" value="23C5714"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F872-I/SP"/>
<attribute name="OC_FARNELL" value="9761012"/>
<attribute name="OC_NEWARK" value="12C1945"/>
</technology>
<technology name="LF">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16LF872-I/SP"/>
<attribute name="OC_FARNELL" value="9761730"/>
<attribute name="OC_NEWARK" value="97K7491"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F87*" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="PIC17F874"/>
</gates>
<devices>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="2"/>
<connect gate="G$1" pin="INT/RB0" pad="36"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="14"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="15"/>
<connect gate="G$1" pin="PGC/RB6" pad="43"/>
<connect gate="G$1" pin="PGD/RB7" pad="44"/>
<connect gate="G$1" pin="PGM/RB3" pad="39"/>
<connect gate="G$1" pin="PSP4/RD4" pad="30"/>
<connect gate="G$1" pin="PSP5/RD5" pad="31"/>
<connect gate="G$1" pin="PSP6/RD6" pad="32"/>
<connect gate="G$1" pin="PSP7/RD7" pad="33"/>
<connect gate="G$1" pin="RA0/AN0" pad="3"/>
<connect gate="G$1" pin="RA1/AN1" pad="4"/>
<connect gate="G$1" pin="RA2/AN2" pad="5"/>
<connect gate="G$1" pin="RA3/AN3" pad="6"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="7"/>
<connect gate="G$1" pin="RA5/AN4" pad="8"/>
<connect gate="G$1" pin="RB1" pad="37"/>
<connect gate="G$1" pin="RB2" pad="38"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5" pad="42"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="16"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="18"/>
<connect gate="G$1" pin="RC2/CCP1" pad="19"/>
<connect gate="G$1" pin="RC3/SCK" pad="20"/>
<connect gate="G$1" pin="RD0/PSP0" pad="21"/>
<connect gate="G$1" pin="RD1/PSP1" pad="22"/>
<connect gate="G$1" pin="RD2/PSP2" pad="23"/>
<connect gate="G$1" pin="RD3/PSP3" pad="24"/>
<connect gate="G$1" pin="RE0/!RD/AN5" pad="9"/>
<connect gate="G$1" pin="RE1/!WR/AN6" pad="10"/>
<connect gate="G$1" pin="RE2/!CS/AN7" pad="11"/>
<connect gate="G$1" pin="RX/RC7" pad="29"/>
<connect gate="G$1" pin="SDI/RC4" pad="25"/>
<connect gate="G$1" pin="SDO/RC5" pad="26"/>
<connect gate="G$1" pin="TX/RC6" pad="27"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="35"/>
<connect gate="G$1" pin="VSS" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="34"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F874-04/L"/>
<attribute name="OC_FARNELL" value="9761160"/>
<attribute name="OC_NEWARK" value="23C5056"/>
</technology>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F877-20/L"/>
<attribute name="OC_FARNELL" value="1660042"/>
<attribute name="OC_NEWARK" value="12C1952"/>
</technology>
</technologies>
</device>
<device name="PQ" package="MQFP44-2">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="18"/>
<connect gate="G$1" pin="INT/RB0" pad="8"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="30"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="31"/>
<connect gate="G$1" pin="PGC/RB6" pad="16"/>
<connect gate="G$1" pin="PGD/RB7" pad="17"/>
<connect gate="G$1" pin="PGM/RB3" pad="11"/>
<connect gate="G$1" pin="PSP4/RD4" pad="2"/>
<connect gate="G$1" pin="PSP5/RD5" pad="3"/>
<connect gate="G$1" pin="PSP6/RD6" pad="4"/>
<connect gate="G$1" pin="PSP7/RD7" pad="5"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="32"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1" pad="36"/>
<connect gate="G$1" pin="RC3/SCK" pad="37"/>
<connect gate="G$1" pin="RD0/PSP0" pad="38"/>
<connect gate="G$1" pin="RD1/PSP1" pad="39"/>
<connect gate="G$1" pin="RD2/PSP2" pad="40"/>
<connect gate="G$1" pin="RD3/PSP3" pad="41"/>
<connect gate="G$1" pin="RE0/!RD/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/!WR/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/!CS/AN7" pad="27"/>
<connect gate="G$1" pin="RX/RC7" pad="1"/>
<connect gate="G$1" pin="SDI/RC4" pad="42"/>
<connect gate="G$1" pin="SDO/RC5" pad="43"/>
<connect gate="G$1" pin="TX/RC6" pad="44"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F874-20I/PQ"/>
<attribute name="OC_FARNELL" value="1084251"/>
<attribute name="OC_NEWARK" value="97K7435"/>
</technology>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F877-04/PQ"/>
<attribute name="OC_FARNELL" value="9761357"/>
<attribute name="OC_NEWARK" value="23C5094"/>
</technology>
</technologies>
</device>
<device name="PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="18"/>
<connect gate="G$1" pin="INT/RB0" pad="8"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="30"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="31"/>
<connect gate="G$1" pin="PGC/RB6" pad="16"/>
<connect gate="G$1" pin="PGD/RB7" pad="17"/>
<connect gate="G$1" pin="PGM/RB3" pad="11"/>
<connect gate="G$1" pin="PSP4/RD4" pad="2"/>
<connect gate="G$1" pin="PSP5/RD5" pad="3"/>
<connect gate="G$1" pin="PSP6/RD6" pad="4"/>
<connect gate="G$1" pin="PSP7/RD7" pad="5"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="32"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1" pad="36"/>
<connect gate="G$1" pin="RC3/SCK" pad="37"/>
<connect gate="G$1" pin="RD0/PSP0" pad="38"/>
<connect gate="G$1" pin="RD1/PSP1" pad="39"/>
<connect gate="G$1" pin="RD2/PSP2" pad="40"/>
<connect gate="G$1" pin="RD3/PSP3" pad="41"/>
<connect gate="G$1" pin="RE0/!RD/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/!WR/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/!CS/AN7" pad="27"/>
<connect gate="G$1" pin="RX/RC7" pad="1"/>
<connect gate="G$1" pin="SDI/RC4" pad="42"/>
<connect gate="G$1" pin="SDO/RC5" pad="43"/>
<connect gate="G$1" pin="TX/RC6" pad="44"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F874-04/PQ"/>
<attribute name="OC_FARNELL" value="1084251"/>
<attribute name="OC_NEWARK" value="97K7429"/>
</technology>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F877-04/PQ"/>
<attribute name="OC_FARNELL" value="9761411"/>
<attribute name="OC_NEWARK" value="23C5094"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="33"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="13"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="14"/>
<connect gate="G$1" pin="PGC/RB6" pad="39"/>
<connect gate="G$1" pin="PGD/RB7" pad="40"/>
<connect gate="G$1" pin="PGM/RB3" pad="36"/>
<connect gate="G$1" pin="PSP4/RD4" pad="27"/>
<connect gate="G$1" pin="PSP5/RD5" pad="28"/>
<connect gate="G$1" pin="PSP6/RD6" pad="29"/>
<connect gate="G$1" pin="PSP7/RD7" pad="30"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="15"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="16"/>
<connect gate="G$1" pin="RC2/CCP1" pad="17"/>
<connect gate="G$1" pin="RC3/SCK" pad="18"/>
<connect gate="G$1" pin="RD0/PSP0" pad="19"/>
<connect gate="G$1" pin="RD1/PSP1" pad="20"/>
<connect gate="G$1" pin="RD2/PSP2" pad="21"/>
<connect gate="G$1" pin="RD3/PSP3" pad="22"/>
<connect gate="G$1" pin="RE0/!RD/AN5" pad="8"/>
<connect gate="G$1" pin="RE1/!WR/AN6" pad="9"/>
<connect gate="G$1" pin="RE2/!CS/AN7" pad="10"/>
<connect gate="G$1" pin="RX/RC7" pad="26"/>
<connect gate="G$1" pin="SDI/RC4" pad="23"/>
<connect gate="G$1" pin="SDO/RC5" pad="24"/>
<connect gate="G$1" pin="TX/RC6" pad="25"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F874-04I/P"/>
<attribute name="OC_FARNELL" value="1196797"/>
<attribute name="OC_NEWARK" value="24M5903"/>
</technology>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F877-04/P"/>
<attribute name="OC_FARNELL" value="9761349"/>
<attribute name="OC_NEWARK" value="61K3463"/>
</technology>
</technologies>
</device>
<device name="SO" package="S44">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="2"/>
<connect gate="G$1" pin="INT/RB0" pad="36"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="14"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="15"/>
<connect gate="G$1" pin="PGC/RB6" pad="43"/>
<connect gate="G$1" pin="PGD/RB7" pad="44"/>
<connect gate="G$1" pin="PGM/RB3" pad="39"/>
<connect gate="G$1" pin="PSP4/RD4" pad="30"/>
<connect gate="G$1" pin="PSP5/RD5" pad="31"/>
<connect gate="G$1" pin="PSP6/RD6" pad="32"/>
<connect gate="G$1" pin="PSP7/RD7" pad="33"/>
<connect gate="G$1" pin="RA0/AN0" pad="3"/>
<connect gate="G$1" pin="RA1/AN1" pad="4"/>
<connect gate="G$1" pin="RA2/AN2" pad="5"/>
<connect gate="G$1" pin="RA3/AN3" pad="6"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="7"/>
<connect gate="G$1" pin="RA5/AN4" pad="8"/>
<connect gate="G$1" pin="RB1" pad="37"/>
<connect gate="G$1" pin="RB2" pad="38"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5" pad="42"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="16"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="18"/>
<connect gate="G$1" pin="RC2/CCP1" pad="19"/>
<connect gate="G$1" pin="RC3/SCK" pad="20"/>
<connect gate="G$1" pin="RD0/PSP0" pad="21"/>
<connect gate="G$1" pin="RD1/PSP1" pad="22"/>
<connect gate="G$1" pin="RD2/PSP2" pad="23"/>
<connect gate="G$1" pin="RD3/PSP3" pad="24"/>
<connect gate="G$1" pin="RE0/!RD/AN5" pad="9"/>
<connect gate="G$1" pin="RE1/!WR/AN6" pad="10"/>
<connect gate="G$1" pin="RE2/!CS/AN7" pad="11"/>
<connect gate="G$1" pin="RX/RC7" pad="29"/>
<connect gate="G$1" pin="SDI/RC4" pad="25"/>
<connect gate="G$1" pin="SDO/RC5" pad="26"/>
<connect gate="G$1" pin="TX/RC6" pad="27"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="35"/>
<connect gate="G$1" pin="VSS" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="34"/>
</connects>
<technologies>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*873" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
flash type</description>
<gates>
<gate name="G$1" symbol="PIC16F872"/>
</gates>
<devices>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*876" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
flash type</description>
<gates>
<gate name="G$1" symbol="PIC16F872"/>
</gates>
<devices>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="F">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F876-20/SO"/>
<attribute name="OC_FARNELL" value="9761268"/>
<attribute name="OC_NEWARK" value="12C1950"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR/THV" pad="1"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RC0/T1OSO" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC17C75XPT" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="PIC17C75X"/>
<gate name="P1" symbol="VDD"/>
<gate name="P2" symbol="VDD"/>
<gate name="P3" symbol="VDD"/>
<gate name="P4" symbol="VDD"/>
<gate name="P5" symbol="VSS"/>
<gate name="P6" symbol="VSS"/>
<gate name="P7" symbol="VSS"/>
<gate name="P8" symbol="VSS"/>
</gates>
<devices>
<device name="T" package="TQFP64-10X10X1MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="OSC1/CKIN" pad="39"/>
<connect gate="G$1" pin="OSC2/CKOUT" pad="40"/>
<connect gate="G$1" pin="RA0/INT" pad="48"/>
<connect gate="G$1" pin="RA1/TOCKI" pad="33"/>
<connect gate="G$1" pin="RA2/SCL" pad="34"/>
<connect gate="G$1" pin="RA3/SDA" pad="35"/>
<connect gate="G$1" pin="RA4/RX1" pad="32"/>
<connect gate="G$1" pin="RA5/TX1" pad="31"/>
<connect gate="G$1" pin="RB0/CAP1" pad="47"/>
<connect gate="G$1" pin="RB1/CAP2" pad="46"/>
<connect gate="G$1" pin="RB2/PWM1" pad="42"/>
<connect gate="G$1" pin="RB3/PWM2" pad="45"/>
<connect gate="G$1" pin="RB4/TCLK12" pad="44"/>
<connect gate="G$1" pin="RB5/TCLK3" pad="43"/>
<connect gate="G$1" pin="RB6/SCK" pad="36"/>
<connect gate="G$1" pin="RB7/SDO" pad="37"/>
<connect gate="G$1" pin="RC0/AD0" pad="58"/>
<connect gate="G$1" pin="RC1/AD1" pad="55"/>
<connect gate="G$1" pin="RC2/AD2" pad="54"/>
<connect gate="G$1" pin="RC3/AD3" pad="53"/>
<connect gate="G$1" pin="RC4/AD4" pad="52"/>
<connect gate="G$1" pin="RC5/AD5" pad="51"/>
<connect gate="G$1" pin="RC6/AD6" pad="50"/>
<connect gate="G$1" pin="RC7/AD7" pad="49"/>
<connect gate="G$1" pin="RD0/AD8" pad="2"/>
<connect gate="G$1" pin="RD1/AD9" pad="1"/>
<connect gate="G$1" pin="RD2/AD10" pad="64"/>
<connect gate="G$1" pin="RD3/AD11" pad="63"/>
<connect gate="G$1" pin="RD4/AD12" pad="62"/>
<connect gate="G$1" pin="RD5/AD13" pad="61"/>
<connect gate="G$1" pin="RD6/AD14" pad="60"/>
<connect gate="G$1" pin="RD7/AD15" pad="59"/>
<connect gate="G$1" pin="RE0/ALE" pad="3"/>
<connect gate="G$1" pin="RE1/!OE" pad="4"/>
<connect gate="G$1" pin="RE2/!WR" pad="5"/>
<connect gate="G$1" pin="RE3/CAP4" pad="6"/>
<connect gate="G$1" pin="RF0/AN4" pad="18"/>
<connect gate="G$1" pin="RF1/AN5" pad="17"/>
<connect gate="G$1" pin="RF2/AN6" pad="16"/>
<connect gate="G$1" pin="RF3/AN7" pad="15"/>
<connect gate="G$1" pin="RF4/AN8" pad="14"/>
<connect gate="G$1" pin="RF5/AN9" pad="13"/>
<connect gate="G$1" pin="RF6/AN10" pad="12"/>
<connect gate="G$1" pin="RF7/AN11" pad="11"/>
<connect gate="G$1" pin="RG0/AN3" pad="24"/>
<connect gate="G$1" pin="RG1/AN2" pad="23"/>
<connect gate="G$1" pin="RG2/AN1" pad="22"/>
<connect gate="G$1" pin="RG3/AN0" pad="21"/>
<connect gate="G$1" pin="RG4/CAP3" pad="27"/>
<connect gate="G$1" pin="RG5/PWM3" pad="28"/>
<connect gate="G$1" pin="RG6/RX2" pad="29"/>
<connect gate="G$1" pin="RG7/TX2" pad="30"/>
<connect gate="G$1" pin="TEST" pad="8"/>
<connect gate="P1" pin="VDD" pad="10"/>
<connect gate="P2" pin="VDD" pad="26"/>
<connect gate="P3" pin="VDD" pad="38"/>
<connect gate="P4" pin="VDD" pad="57"/>
<connect gate="P5" pin="VSS" pad="9"/>
<connect gate="P6" pin="VSS" pad="25"/>
<connect gate="P7" pin="VSS" pad="41"/>
<connect gate="P8" pin="VSS" pad="56"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC17C756A-33I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C5980"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F1*20" prefix="IC">
<description>&lt;b&gt;18/20/28-Pin High-Performance, Enhanced Flash Microcontrollers&lt;/b&gt;&lt;br&gt;
with 10-bit A/D and nanoWatt Technology&lt;p&gt;

Source: ww1.microchip.com/downloads/en/DeviceDoc/39605c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F1220"/>
</gates>
<devices>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="BKI0/DT/RX/AN6/RB4" pad="10"/>
<connect gate="G$1" pin="INT0/AN4/RB0" pad="8"/>
<connect gate="G$1" pin="INT1/CK/TX/AN5/RB1" pad="9"/>
<connect gate="G$1" pin="INT2/P1B/RB2" pad="17"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="11"/>
<connect gate="G$1" pin="KBI2/P1C/T13CKI/T1OSO/RB6" pad="12"/>
<connect gate="G$1" pin="KBI3/P1D/T1OSI/PGD/RB7" pad="13"/>
<connect gate="G$1" pin="P1A/CCP1/RB3" pad="18"/>
<connect gate="G$1" pin="RA0/AN0" pad="1"/>
<connect gate="G$1" pin="RA1/AN1/LVDIN" pad="2"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="6"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="7"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="3"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="4"/>
<connect gate="G$1" pin="RA6/CLKO/OSC2" pad="15"/>
<connect gate="G$1" pin="RA7/CLKI/OSC1" pad="16"/>
<connect gate="G$1" pin="VDD@AVDD" pad="14"/>
<connect gate="G$1" pin="VSS@AVSS" pad="5"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F1220-I/P"/>
<attribute name="OC_FARNELL" value="9761977"/>
<attribute name="OC_NEWARK" value="92C2429"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO-18W">
<connects>
<connect gate="G$1" pin="BKI0/DT/RX/AN6/RB4" pad="10"/>
<connect gate="G$1" pin="INT0/AN4/RB0" pad="8"/>
<connect gate="G$1" pin="INT1/CK/TX/AN5/RB1" pad="9"/>
<connect gate="G$1" pin="INT2/P1B/RB2" pad="17"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="11"/>
<connect gate="G$1" pin="KBI2/P1C/T13CKI/T1OSO/RB6" pad="12"/>
<connect gate="G$1" pin="KBI3/P1D/T1OSI/PGD/RB7" pad="13"/>
<connect gate="G$1" pin="P1A/CCP1/RB3" pad="18"/>
<connect gate="G$1" pin="RA0/AN0" pad="1"/>
<connect gate="G$1" pin="RA1/AN1/LVDIN" pad="2"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="6"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="7"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="3"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="4"/>
<connect gate="G$1" pin="RA6/CLKO/OSC2" pad="15"/>
<connect gate="G$1" pin="RA7/CLKI/OSC1" pad="16"/>
<connect gate="G$1" pin="VDD@AVDD" pad="14"/>
<connect gate="G$1" pin="VSS@AVSS" pad="5"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F1220-I/SO"/>
<attribute name="OC_FARNELL" value="9761985"/>
<attribute name="OC_NEWARK" value="92C2430"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F1*20?" prefix="IC">
<description>&lt;b&gt;18/20/28-Pin High-Performance, Enhanced Flash Microcontrollers&lt;/b&gt;&lt;br&gt;
with 10-bit A/D and nanoWatt Technology&lt;p&gt;

Source: ww1.microchip.com/downloads/en/DeviceDoc/39605c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F1320"/>
</gates>
<devices>
<device name="SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="AVDD" pad="15"/>
<connect gate="G$1" pin="AVSS" pad="6"/>
<connect gate="G$1" pin="BKI0/DT/RX/AN6/RB4" pad="11"/>
<connect gate="G$1" pin="INT0/AN4/RB0" pad="9"/>
<connect gate="G$1" pin="INT1/CK/TX/AN5/RB1" pad="10"/>
<connect gate="G$1" pin="INT2/P1B/RB2" pad="19"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="12"/>
<connect gate="G$1" pin="KBI2/P1C/T13CKI/T1OSO/RB6" pad="13"/>
<connect gate="G$1" pin="KBI3/P1D/T1OSI/PGD/RB7" pad="14"/>
<connect gate="G$1" pin="P1A/CCP1/RB3" pad="20"/>
<connect gate="G$1" pin="RA0/AN0" pad="1"/>
<connect gate="G$1" pin="RA1/AN1/LVDIN" pad="2"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="7"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="8"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="3"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="4"/>
<connect gate="G$1" pin="RA6/CLKO/OSC2" pad="17"/>
<connect gate="G$1" pin="RA7/CLKI/OSC1" pad="18"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F1220-E/SS"/>
<attribute name="OC_FARNELL" value="9761993"/>
<attribute name="OC_NEWARK" value="92C4995"/>
</technology>
<technology name="3">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F1320-I/SS"/>
<attribute name="OC_FARNELL" value="1084333"/>
<attribute name="OC_NEWARK" value="92C5009"/>
</technology>
</technologies>
</device>
<device name="ML" package="QFN28">
<connects>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="5"/>
<connect gate="G$1" pin="BKI0/DT/RX/AN6/RB4" pad="12"/>
<connect gate="G$1" pin="INT0/AN4/RB0" pad="9"/>
<connect gate="G$1" pin="INT1/CK/TX/AN5/RB1" pad="10"/>
<connect gate="G$1" pin="INT2/P1B/RB2" pad="23"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="13"/>
<connect gate="G$1" pin="KBI2/P1C/T13CKI/T1OSO/RB6" pad="15"/>
<connect gate="G$1" pin="KBI3/P1D/T1OSI/PGD/RB7" pad="16"/>
<connect gate="G$1" pin="P1A/CCP1/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="26"/>
<connect gate="G$1" pin="RA1/AN1/LVDIN" pad="27"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="7"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="8"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="28"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CLKO/OSC2" pad="20"/>
<connect gate="G$1" pin="RA7/CLKI/OSC1" pad="21"/>
<connect gate="G$1" pin="VDD" pad="19"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F1220-I/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C4996"/>
</technology>
<technology name="3">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F1320-I/ML"/>
<attribute name="OC_FARNELL" value="9762000"/>
<attribute name="OC_NEWARK" value="92C5008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC12F6*" prefix="IC">
<description>&lt;b&gt;Data Sheet 8-Pin FLASH-Based 8-Bit CMOS Microcontrollers&lt;/b&gt;&lt;p&gt;
Source: http://www.microchip.com .. 41190c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC12F629"/>
</gates>
<devices>
<device name="MF" package="DFN-S">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3" pad="4"/>
<connect gate="G$1" pin="GP4/CLKOUT" pad="3"/>
<connect gate="G$1" pin="GP5/CLKIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="29">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F629-I/MD"/>
<attribute name="OC_FARNELL" value="1618004"/>
<attribute name="OC_NEWARK" value="56K7222"/>
</technology>
<technology name="75">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC12F675-I/MD"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="56K7227"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3" pad="4"/>
<connect gate="G$1" pin="GP4/CLKOUT" pad="3"/>
<connect gate="G$1" pin="GP5/CLKIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="29">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F629-I/SN"/>
<attribute name="OC_FARNELL" value="9759000"/>
<attribute name="OC_NEWARK" value="61K3433"/>
</technology>
<technology name="75">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F675-E/SN"/>
<attribute name="OC_FARNELL" value="9759026"/>
<attribute name="OC_NEWARK" value="92C4341"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3" pad="4"/>
<connect gate="G$1" pin="GP4/CLKOUT" pad="3"/>
<connect gate="G$1" pin="GP5/CLKIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="29">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F629-I/P"/>
<attribute name="OC_FARNELL" value="1292253"/>
<attribute name="OC_NEWARK" value="67K0822"/>
</technology>
<technology name="75">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F675-E/P"/>
<attribute name="OC_FARNELL" value="9759018"/>
<attribute name="OC_NEWARK" value="92C4340"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2*80" prefix="IC">
<description>&lt;b&gt;28-Pin Enhanced Flash Microcontrollers with ECAN(TM) Technology&lt;/b&gt;&lt;br&gt;
10-Bit A/D and nanoWatt Technology&lt;p&gt;
Source: http://www.microchip.com .. 39637a.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F2580"/>
</gates>
<devices>
<device name="-I/ML" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="CANRX/RB3" pad="21"/>
<connect gate="G$1" pin="INT0/AN10/RB0" pad="18"/>
<connect gate="G$1" pin="INT1/AN8/RB1" pad="19"/>
<connect gate="G$1" pin="INT2/CANTX/RB2" pad="20"/>
<connect gate="G$1" pin="KBI0/AN9/RB4" pad="22"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="23"/>
<connect gate="G$1" pin="KBI2/PGC/RB6" pad="24"/>
<connect gate="G$1" pin="KBI3/PGD/RB7" pad="25"/>
<connect gate="G$1" pin="RA0/AN0" pad="27"/>
<connect gate="G$1" pin="RA1/AN1" pad="28"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="2"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="3"/>
<connect gate="G$1" pin="RA5/AN4/!SS/HLVDIN" pad="4"/>
<connect gate="G$1" pin="RA6/CLKO/OSC2" pad="7"/>
<connect gate="G$1" pin="RA7/CLKI/OSC1" pad="6"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="8"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="9"/>
<connect gate="G$1" pin="RC2/CCP1" pad="10"/>
<connect gate="G$1" pin="RC3/SCK/SCL" pad="11"/>
<connect gate="G$1" pin="RC4/SDI/SDA" pad="12"/>
<connect gate="G$1" pin="RC5/SDO" pad="13"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="14"/>
<connect gate="G$1" pin="RC7/RX/DT" pad="15"/>
<connect gate="G$1" pin="RE3/!MCLR/VPP" pad="26"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="16"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2480-I/ML"/>
<attribute name="OC_FARNELL" value="1556179"/>
<attribute name="OC_NEWARK" value="71J7235"/>
</technology>
<technology name="5">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2580-I/ML"/>
<attribute name="OC_FARNELL" value="1556180"/>
<attribute name="OC_NEWARK" value="71J7242"/>
</technology>
</technologies>
</device>
<device name="-E/SO" package="SO28W">
<connects>
<connect gate="G$1" pin="CANRX/RB3" pad="24"/>
<connect gate="G$1" pin="INT0/AN10/RB0" pad="21"/>
<connect gate="G$1" pin="INT1/AN8/RB1" pad="22"/>
<connect gate="G$1" pin="INT2/CANTX/RB2" pad="23"/>
<connect gate="G$1" pin="KBI0/AN9/RB4" pad="25"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="26"/>
<connect gate="G$1" pin="KBI2/PGC/RB6" pad="27"/>
<connect gate="G$1" pin="KBI3/PGD/RB7" pad="28"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/!SS/HLVDIN" pad="7"/>
<connect gate="G$1" pin="RA6/CLKO/OSC2" pad="10"/>
<connect gate="G$1" pin="RA7/CLKI/OSC1" pad="9"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK/SCL" pad="14"/>
<connect gate="G$1" pin="RC4/SDI/SDA" pad="15"/>
<connect gate="G$1" pin="RC5/SDO" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT" pad="18"/>
<connect gate="G$1" pin="RE3/!MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="5">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2580-I/SO"/>
<attribute name="OC_FARNELL" value="9321284"/>
<attribute name="OC_NEWARK" value="71J7243"/>
</technology>
</technologies>
</device>
<device name="-I/SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="CANRX/RB3" pad="24"/>
<connect gate="G$1" pin="INT0/AN10/RB0" pad="21"/>
<connect gate="G$1" pin="INT1/AN8/RB1" pad="22"/>
<connect gate="G$1" pin="INT2/CANTX/RB2" pad="23"/>
<connect gate="G$1" pin="KBI0/AN9/RB4" pad="25"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="26"/>
<connect gate="G$1" pin="KBI2/PGC/RB6" pad="27"/>
<connect gate="G$1" pin="KBI3/PGD/RB7" pad="28"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/!SS/HLVDIN" pad="7"/>
<connect gate="G$1" pin="RA6/CLKO/OSC2" pad="10"/>
<connect gate="G$1" pin="RA7/CLKI/OSC1" pad="9"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1" pad="13"/>
<connect gate="G$1" pin="RC3/SCK/SCL" pad="14"/>
<connect gate="G$1" pin="RC4/SDI/SDA" pad="15"/>
<connect gate="G$1" pin="RC5/SDO" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT" pad="18"/>
<connect gate="G$1" pin="RE3/!MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2480-I/SP"/>
<attribute name="OC_FARNELL" value="9321217"/>
<attribute name="OC_NEWARK" value="71J7237"/>
</technology>
<technology name="5">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2580-I/SP"/>
<attribute name="OC_FARNELL" value="9321276"/>
<attribute name="OC_NEWARK" value="71J7244"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F6*" prefix="IC">
<description>&lt;b&gt;PIC18F87J10 FAMILY&lt;/b&gt; 64/80-Pin, High-Performance, 1-Mbit Flash Microcontrollers with nanoWatt Technology&lt;p&gt;
Source: http://www.microchip.com/ .. 39663c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F6XJ10"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="ENVREG" pad="18"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="39"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="40"/>
<connect gate="G$1" pin="RA0/AN0" pad="24"/>
<connect gate="G$1" pin="RA1/AN1" pad="23"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="22"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="21"/>
<connect gate="G$1" pin="RA4/T0CK" pad="28"/>
<connect gate="G$1" pin="RA5/AN4" pad="27"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="48"/>
<connect gate="G$1" pin="RB1/INT1" pad="47"/>
<connect gate="G$1" pin="RB2/INT2" pad="46"/>
<connect gate="G$1" pin="RB3/INT3" pad="45"/>
<connect gate="G$1" pin="RB4/KBI0" pad="44"/>
<connect gate="G$1" pin="RB5/KBI1" pad="43"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="42"/>
<connect gate="G$1" pin="RB7/KBI2/PGD" pad="37"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="30"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="29"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="33"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="34"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="35"/>
<connect gate="G$1" pin="RC5/SDO1" pad="36"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="31"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="32"/>
<connect gate="G$1" pin="RD0/PSP0" pad="58"/>
<connect gate="G$1" pin="RD1/PSP1" pad="55"/>
<connect gate="G$1" pin="RD2/PSP2" pad="54"/>
<connect gate="G$1" pin="RD3/PSP3" pad="53"/>
<connect gate="G$1" pin="RD4/PSP4/SDO2" pad="52"/>
<connect gate="G$1" pin="RD5/PSP5/SDI2/SDA2" pad="51"/>
<connect gate="G$1" pin="RD6/PSP6/SCK2/SCL2" pad="50"/>
<connect gate="G$1" pin="RD7/PSP7/!SS2" pad="49"/>
<connect gate="G$1" pin="RE0/!RD/P2D" pad="2"/>
<connect gate="G$1" pin="RE1/!WR/P2C" pad="1"/>
<connect gate="G$1" pin="RE2/!CS/P2B" pad="64"/>
<connect gate="G$1" pin="RE3/P3C" pad="63"/>
<connect gate="G$1" pin="RE4/P3B" pad="62"/>
<connect gate="G$1" pin="RE5/P1C" pad="61"/>
<connect gate="G$1" pin="RE6/P1B" pad="60"/>
<connect gate="G$1" pin="RE7/ECCP2/P2A" pad="59"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="17"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="16"/>
<connect gate="G$1" pin="RF3/AN8" pad="15"/>
<connect gate="G$1" pin="RF4/AN9" pad="14"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="13"/>
<connect gate="G$1" pin="RF6/AN11" pad="12"/>
<connect gate="G$1" pin="RF7/!SS1" pad="11"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="3"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="4"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="5"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="6"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="8"/>
<connect gate="G$1" pin="VDD" pad="38"/>
<connect gate="G$1" pin="VDD@1" pad="26"/>
<connect gate="G$1" pin="VDD@2" pad="57"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="10"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSS@1" pad="25"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="VSS@3" pad="56"/>
</connects>
<technologies>
<technology name="5J10">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F65J10-I/PT"/>
<attribute name="OC_FARNELL" value="1332280"/>
<attribute name="OC_NEWARK" value="71J7261"/>
</technology>
<technology name="5J15">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F65J15T-I/PT"/>
<attribute name="OC_FARNELL" value="1579611"/>
<attribute name="OC_NEWARK" value="71J7264"/>
</technology>
<technology name="6J10">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F66J10-I/PT"/>
<attribute name="OC_FARNELL" value="1332281"/>
<attribute name="OC_NEWARK" value="71J7266"/>
</technology>
<technology name="6J15">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F66J15-I/PT"/>
<attribute name="OC_FARNELL" value="1556181"/>
<attribute name="OC_NEWARK" value="71J7268"/>
</technology>
<technology name="7J10">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F67J10-I/PT"/>
<attribute name="OC_FARNELL" value="1332283"/>
<attribute name="OC_NEWARK" value="71J7273"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F8*" prefix="IC">
<description>&lt;b&gt;PIC18F87J10 FAMILY&lt;/b&gt; 64/80-Pin, High-Performance, 1-Mbit Flash Microcontrollers with nanoWatt Technology&lt;p&gt;
Source: http://www.microchip.com/ .. 39663c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F87J10"/>
</gates>
<devices>
<device name="" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ENVREG" pad="24"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="49"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="50"/>
<connect gate="G$1" pin="RA0/AN0" pad="30"/>
<connect gate="G$1" pin="RA1/AN1" pad="29"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="28"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="27"/>
<connect gate="G$1" pin="RA4/T0CK" pad="34"/>
<connect gate="G$1" pin="RA5/AN4" pad="33"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="58"/>
<connect gate="G$1" pin="RB1/INT1" pad="57"/>
<connect gate="G$1" pin="RB2/INT2" pad="56"/>
<connect gate="G$1" pin="RB3/INT3/ACCP2/P2A" pad="55"/>
<connect gate="G$1" pin="RB4/KBI0" pad="54"/>
<connect gate="G$1" pin="RB5/KBI1" pad="53"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="52"/>
<connect gate="G$1" pin="RB7/KBI2/PGD" pad="47"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="36"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="43"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="44"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="45"/>
<connect gate="G$1" pin="RC5/SDO1" pad="46"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="37"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="38"/>
<connect gate="G$1" pin="RD0/AD0/PSP0" pad="72"/>
<connect gate="G$1" pin="RD1/AD1/PSP1" pad="69"/>
<connect gate="G$1" pin="RD2/AD2/PSP2" pad="68"/>
<connect gate="G$1" pin="RD3/AD3/PSP3" pad="67"/>
<connect gate="G$1" pin="RD4/AD4/PSP4/SDO2" pad="66"/>
<connect gate="G$1" pin="RD5/AD5/PSP5/SDI2/SDA2" pad="65"/>
<connect gate="G$1" pin="RD6/AD6/PSP6/SCK2/SCL2" pad="64"/>
<connect gate="G$1" pin="RD7/AD7/PSP7/!SS2" pad="63"/>
<connect gate="G$1" pin="RE0/AD8/!RD/P2D" pad="4"/>
<connect gate="G$1" pin="RE1/AD9/!WR/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/!AD10CS/P2B" pad="78"/>
<connect gate="G$1" pin="RE3/AD11/P3C" pad="77"/>
<connect gate="G$1" pin="RE4/AD12/P3B" pad="76"/>
<connect gate="G$1" pin="RE5/AD13/P1C" pad="75"/>
<connect gate="G$1" pin="RE6/AD14/P1B" pad="74"/>
<connect gate="G$1" pin="RE7/AD15/ECCP2/P2A" pad="73"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="23"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="18"/>
<connect gate="G$1" pin="RF3/AN8" pad="17"/>
<connect gate="G$1" pin="RF4/AN9" pad="16"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="15"/>
<connect gate="G$1" pin="RF6/AN11" pad="14"/>
<connect gate="G$1" pin="RF7/!SS1" pad="13"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="5"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="6"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="7"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="8"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="10"/>
<connect gate="G$1" pin="RH0/A16" pad="79"/>
<connect gate="G$1" pin="RH1/A17" pad="80"/>
<connect gate="G$1" pin="RH2/A18" pad="1"/>
<connect gate="G$1" pin="RH3/A19" pad="2"/>
<connect gate="G$1" pin="RH4/AN12/P3C" pad="22"/>
<connect gate="G$1" pin="RH5/AN13/P3B" pad="21"/>
<connect gate="G$1" pin="RH6/AN14/P1C" pad="20"/>
<connect gate="G$1" pin="RH7/AN15/P1B" pad="19"/>
<connect gate="G$1" pin="RJ0/ALE" pad="62"/>
<connect gate="G$1" pin="RJ1/!OE" pad="61"/>
<connect gate="G$1" pin="RJ2/!WRL" pad="60"/>
<connect gate="G$1" pin="RJ3/!WRH" pad="59"/>
<connect gate="G$1" pin="RJ4/BA0" pad="39"/>
<connect gate="G$1" pin="RJ5/!CE" pad="40"/>
<connect gate="G$1" pin="RJ6/!LB" pad="41"/>
<connect gate="G$1" pin="RJ7/!UB" pad="42"/>
<connect gate="G$1" pin="VDD" pad="48"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VDD@2" pad="71"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="12"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
<connect gate="G$1" pin="VSS@2" pad="51"/>
<connect gate="G$1" pin="VSS@3" pad="70"/>
</connects>
<technologies>
<technology name="5J10">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F85J10-I/PT"/>
<attribute name="OC_FARNELL" value="1847396"/>
<attribute name="OC_NEWARK" value="71J7277"/>
</technology>
<technology name="5J15">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F85J15-I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="71J7279"/>
</technology>
<technology name="6J10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F86J10-I/PT"/>
<attribute name="OC_FARNELL" value="1332288"/>
<attribute name="OC_NEWARK" value="34M8058"/>
</technology>
<technology name="6J15">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F86J15-I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="71J7284"/>
</technology>
<technology name="7J10">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F87J10-I/PT"/>
<attribute name="OC_FARNELL" value="1332290"/>
<attribute name="OC_NEWARK" value="71J7289"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4*_TQFP" prefix="IC">
<description>&lt;b&gt;USB Microcontrollers with nanoWatt Technology&lt;/b&gt; High-Performance, Enhanced Flash, 28/40/44-Pin, &lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F4455_44TQFP"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3" pad="18"/>
<connect gate="G$1" pin="NC/!ICRST!/IVVPP" pad="33"/>
<connect gate="G$1" pin="NC/ICCK/ICPGC" pad="12"/>
<connect gate="G$1" pin="NC/ICDT/ICPGD" pad="13"/>
<connect gate="G$1" pin="NC/ICPORTS" pad="34"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="30"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="21"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI/CIOUT/RCV" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/HLVDIN/C2OUT" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="31"/>
<connect gate="G$1" pin="RB0/AN12/INT0/LFT0/SDI/SDA" pad="8"/>
<connect gate="G$1" pin="RB1/AN10/INT1/SCK/SCL" pad="9"/>
<connect gate="G$1" pin="RB2/AN8/INT2/VMO" pad="10"/>
<connect gate="G$1" pin="RB3/AN9/CCP2/VPO" pad="11"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/CSSPP" pad="14"/>
<connect gate="G$1" pin="RB5/KBI1/PGM" pad="15"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/BKI3/PGD" pad="17"/>
<connect gate="G$1" pin="RC0/TIOSO/T13CKI" pad="32"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2/!UOE" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1/P1A" pad="36"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="42"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="43"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="44"/>
<connect gate="G$1" pin="RC7/RX/DT/SDO" pad="1"/>
<connect gate="G$1" pin="RD0/SPP0" pad="38"/>
<connect gate="G$1" pin="RD1/SPP1" pad="39"/>
<connect gate="G$1" pin="RD2/SPP2" pad="40"/>
<connect gate="G$1" pin="RD3/SPP3" pad="41"/>
<connect gate="G$1" pin="RD4/SPP4" pad="2"/>
<connect gate="G$1" pin="RD5/SPP5/P1B" pad="3"/>
<connect gate="G$1" pin="RD6/SPP6/P1C" pad="4"/>
<connect gate="G$1" pin="RD7/SPP7/P1D" pad="5"/>
<connect gate="G$1" pin="RE0/AN5/CK1SPP" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/CK2SPP" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/OESPP" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
<connect gate="G$1" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name="455">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F4455-I/PT"/>
<attribute name="OC_FARNELL" value="9321322"/>
<attribute name="OC_NEWARK" value="08J9628"/>
</technology>
<technology name="550">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F4550-I/PT"/>
<attribute name="OC_FARNELL" value="9321365"/>
<attribute name="OC_NEWARK" value="08J9633"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4*_QFN" prefix="IC">
<description>&lt;b&gt;USB Microcontrollers with nanoWatt Technology&lt;/b&gt; High-Performance, Enhanced Flash, 28/40/44-Pin, &lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F4455_44QFN"/>
</gates>
<devices>
<device name="" package="QFN44ML8X8">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3" pad="18"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="32"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="21"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI/CIOUT/RCV" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/HLVDIN/C2OUT" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="33"/>
<connect gate="G$1" pin="RB0/AN12/INT0/LFT0/SDI/SDA" pad="9"/>
<connect gate="G$1" pin="RB1/AN10/INT1/SCK/SCL" pad="10"/>
<connect gate="G$1" pin="RB2/AN8/INT2/VMO" pad="11"/>
<connect gate="G$1" pin="RB3/AN9/CCP2/VPO" pad="12"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/CSSPP" pad="14"/>
<connect gate="G$1" pin="RB5/KBI1/PGM" pad="15"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/BKI3/PGD" pad="17"/>
<connect gate="G$1" pin="RC0/TIOSO/T13CKI" pad="34"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2/!UOE" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1/P1A" pad="36"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="42"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="43"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="44"/>
<connect gate="G$1" pin="RC7/RX/DT/SDO" pad="1"/>
<connect gate="G$1" pin="RD0/SPP0" pad="38"/>
<connect gate="G$1" pin="RD1/SPP1" pad="39"/>
<connect gate="G$1" pin="RD2/SPP2" pad="40"/>
<connect gate="G$1" pin="RD3/SPP3" pad="41"/>
<connect gate="G$1" pin="RD4/SPP4" pad="2"/>
<connect gate="G$1" pin="RD5/SPP5/P1B" pad="3"/>
<connect gate="G$1" pin="RD6/SPP6/P1C" pad="4"/>
<connect gate="G$1" pin="RD7/SPP7/P1D" pad="5"/>
<connect gate="G$1" pin="RE0/AN5/CK1SPP" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/CK2SPP" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/OESPP" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="8"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VDD@3" pad="29"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="30"/>
<connect gate="G$1" pin="VSS@2" pad="31"/>
<connect gate="G$1" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name="455">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F4455T-I/ML"/>
<attribute name="OC_FARNELL" value="9321314"/>
<attribute name="OC_NEWARK" value="08J9629"/>
</technology>
<technology name="550">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F4550-I/ML"/>
<attribute name="OC_FARNELL" value="1292276"/>
<attribute name="OC_NEWARK" value="08J9631"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4*_40" prefix="IC">
<description>&lt;b&gt;USB Microcontrollers with nanoWatt Technology&lt;/b&gt; High-Performance, Enhanced Flash, 28/40/44-Pin, &lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F4455_40"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="13"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI/CIOUT/RCV" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/HLVDIN/C2OUT" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="14"/>
<connect gate="G$1" pin="RB0/AN12/INT0/LFT0/SDI/SDA" pad="33"/>
<connect gate="G$1" pin="RB1/AN10/INT1/SCK/SCL" pad="34"/>
<connect gate="G$1" pin="RB2/AN8/INT2/VMO" pad="35"/>
<connect gate="G$1" pin="RB3/AN9/CCP2/VPO" pad="36"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/CSSPP" pad="37"/>
<connect gate="G$1" pin="RB5/KBI1/PGM" pad="38"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="39"/>
<connect gate="G$1" pin="RB7/BKI3/PGD" pad="40"/>
<connect gate="G$1" pin="RC0/TIOSO/T13CKI" pad="15"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2/!UOE" pad="16"/>
<connect gate="G$1" pin="RC2/CCP1/P1A" pad="17"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="23"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="24"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="25"/>
<connect gate="G$1" pin="RC7/RX/DT/SDO" pad="26"/>
<connect gate="G$1" pin="RD0/SPP0" pad="19"/>
<connect gate="G$1" pin="RD1/SPP1" pad="20"/>
<connect gate="G$1" pin="RD2/SPP2" pad="21"/>
<connect gate="G$1" pin="RD3/SPP3" pad="22"/>
<connect gate="G$1" pin="RD4/SPP4" pad="27"/>
<connect gate="G$1" pin="RD5/SPP5/P1B" pad="28"/>
<connect gate="G$1" pin="RD6/SPP6/P1C" pad="29"/>
<connect gate="G$1" pin="RD7/SPP7/P1D" pad="30"/>
<connect gate="G$1" pin="RE0/AN5/CK1SPP" pad="8"/>
<connect gate="G$1" pin="RE1/AN6/CK2SPP" pad="9"/>
<connect gate="G$1" pin="RE2/AN7/OESPP" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
<connect gate="G$1" pin="VUSB" pad="18"/>
</connects>
<technologies>
<technology name="455">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F4455-I/P"/>
<attribute name="OC_FARNELL" value="9321314"/>
<attribute name="OC_NEWARK" value="05K2028"/>
</technology>
<technology name="550">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F4550-I/P"/>
<attribute name="OC_FARNELL" value="9321357"/>
<attribute name="OC_NEWARK" value="74K8623"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2*_28" prefix="IC">
<description>&lt;b&gt;USB Microcontrollers with nanoWatt Technology&lt;/b&gt; High-Performance, Enhanced Flash, 28/40/44-Pin, &lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F4455_28"/>
</gates>
<devices>
<device name="DIP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="9"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI/CIOUT/RCV" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/HLVDIN/C2OUT" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="10"/>
<connect gate="G$1" pin="RB0/AN12/INT0/LFT0/SDI/SDA" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/INT1/SCK/SCL" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/INT2/VMO" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/CCP2/VPO" pad="24"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/CSSPP" pad="25"/>
<connect gate="G$1" pin="RB5/KBI1/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/BKI3/PGD" pad="28"/>
<connect gate="G$1" pin="RC0/TIOSO/T13CKI" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2/!UOE" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1/P1A" pad="13"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="15"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/SDO" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name="455">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2455-I/SP"/>
<attribute name="OC_FARNELL" value="1579600"/>
<attribute name="OC_NEWARK" value="01M8485"/>
</technology>
<technology name="550">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2550-I/SP"/>
<attribute name="OC_FARNELL" value="1523822"/>
<attribute name="OC_NEWARK" value="80K6054"/>
</technology>
</technologies>
</device>
<device name="W" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="9"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI/CIOUT/RCV" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/HLVDIN/C2OUT" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="10"/>
<connect gate="G$1" pin="RB0/AN12/INT0/LFT0/SDI/SDA" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/INT1/SCK/SCL" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/INT2/VMO" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/CCP2/VPO" pad="24"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/CSSPP" pad="25"/>
<connect gate="G$1" pin="RB5/KBI1/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/BKI3/PGD" pad="28"/>
<connect gate="G$1" pin="RC0/TIOSO/T13CKI" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2/!UOE" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1/P1A" pad="13"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="15"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/SDO" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name="455">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2455-I/SO"/>
<attribute name="OC_FARNELL" value="1579598"/>
<attribute name="OC_NEWARK" value="64J3768"/>
</technology>
<technology name="550">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F2550-I/SO"/>
<attribute name="OC_FARNELL" value="9321268"/>
<attribute name="OC_NEWARK" value="73K1297"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP23017" prefix="IC">
<description>&lt;b&gt;http://ww1.microchip.com/downloads/en/DeviceDoc/21952a.pdf&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21952a.pdf</description>
<gates>
<gate name="G$1" symbol="MCP23017"/>
</gates>
<devices>
<device name="SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23017-E/SP"/>
<attribute name="OC_FARNELL" value="1332088"/>
<attribute name="OC_NEWARK" value="31K2959"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23017-E/SO"/>
<attribute name="OC_FARNELL" value="1332087"/>
<attribute name="OC_NEWARK" value="31K2958"/>
</technology>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23017-E/SS"/>
<attribute name="OC_FARNELL" value="1467674"/>
<attribute name="OC_NEWARK" value="31K2960"/>
</technology>
</technologies>
</device>
<device name="ML" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!RESET" pad="14"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="12"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="GPA0" pad="17"/>
<connect gate="G$1" pin="GPA1" pad="18"/>
<connect gate="G$1" pin="GPA2" pad="19"/>
<connect gate="G$1" pin="GPA3" pad="20"/>
<connect gate="G$1" pin="GPA4" pad="21"/>
<connect gate="G$1" pin="GPA5" pad="22"/>
<connect gate="G$1" pin="GPA6" pad="23"/>
<connect gate="G$1" pin="GPA7" pad="24"/>
<connect gate="G$1" pin="GPB0" pad="25"/>
<connect gate="G$1" pin="GPB1" pad="26"/>
<connect gate="G$1" pin="GPB2" pad="27"/>
<connect gate="G$1" pin="GPB3" pad="28"/>
<connect gate="G$1" pin="GPB4" pad="1"/>
<connect gate="G$1" pin="GPB5" pad="2"/>
<connect gate="G$1" pin="GPB6" pad="3"/>
<connect gate="G$1" pin="GPB7" pad="4"/>
<connect gate="G$1" pin="INTA" pad="16"/>
<connect gate="G$1" pin="INTB" pad="15"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23017-E/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="31K2957"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP23S17" prefix="IC">
<description>&lt;b&gt;http://ww1.microchip.com/downloads/en/DeviceDoc/21952a.pdf&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21952a.pdf</description>
<gates>
<gate name="G$1" symbol="MCP23S17"/>
</gates>
<devices>
<device name="SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCK" pad="12"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="SO" pad="14"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23S17-E/SP"/>
<attribute name="OC_FARNELL" value="1292238"/>
<attribute name="OC_NEWARK" value="31K2951"/>
</technology>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCK" pad="12"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="SO" pad="14"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23S17-E/SS"/>
<attribute name="OC_FARNELL" value="1467675"/>
<attribute name="OC_NEWARK" value="31K2952"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCK" pad="12"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="SO" pad="14"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23S17-E/SO"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="31K2950"/>
</technology>
</technologies>
</device>
<device name="ML" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="!RESET" pad="14"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="12"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="GPA0" pad="17"/>
<connect gate="G$1" pin="GPA1" pad="18"/>
<connect gate="G$1" pin="GPA2" pad="19"/>
<connect gate="G$1" pin="GPA3" pad="20"/>
<connect gate="G$1" pin="GPA4" pad="21"/>
<connect gate="G$1" pin="GPA5" pad="22"/>
<connect gate="G$1" pin="GPA6" pad="23"/>
<connect gate="G$1" pin="GPA7" pad="24"/>
<connect gate="G$1" pin="GPB0" pad="25"/>
<connect gate="G$1" pin="GPB1" pad="26"/>
<connect gate="G$1" pin="GPB2" pad="27"/>
<connect gate="G$1" pin="GPB3" pad="28"/>
<connect gate="G$1" pin="GPB4" pad="1"/>
<connect gate="G$1" pin="GPB5" pad="2"/>
<connect gate="G$1" pin="GPB6" pad="3"/>
<connect gate="G$1" pin="GPB7" pad="4"/>
<connect gate="G$1" pin="INTA" pad="16"/>
<connect gate="G$1" pin="INTB" pad="15"/>
<connect gate="G$1" pin="SCK" pad="8"/>
<connect gate="G$1" pin="SI" pad="9"/>
<connect gate="G$1" pin="SO" pad="10"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23S17-E/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="31K2949"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*F62" prefix="IC">
<description>&lt;b&gt;FLASH-Based 8-Bit CMOS Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/40300C.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F62X"/>
</gates>
<devices>
<device name="7P" package="DIL18">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="17"/>
<connect gate="G$1" pin="RA1/AN1" pad="18"/>
<connect gate="G$1" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="G$1" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="15"/>
<connect gate="G$1" pin="RA7/ASC1/CLKIN" pad="16"/>
<connect gate="G$1" pin="RB0/INT" pad="6"/>
<connect gate="G$1" pin="RB1/RX/DT" pad="7"/>
<connect gate="G$1" pin="RB2/TX/CK" pad="8"/>
<connect gate="G$1" pin="RB3/CCP1" pad="9"/>
<connect gate="G$1" pin="RB4/PGM" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6/T1OSO/1ICKI/PGC" pad="12"/>
<connect gate="G$1" pin="RB7/T1OSI/PGD" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F627-20I/P"/>
<attribute name="OC_FARNELL" value="1084298"/>
<attribute name="OC_NEWARK" value="23C4967"/>
</technology>
<technology name="L">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF627-04/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="23C5660"/>
</technology>
</technologies>
</device>
<device name="7SO" package="SO-18W">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="17"/>
<connect gate="G$1" pin="RA1/AN1" pad="18"/>
<connect gate="G$1" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="G$1" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="15"/>
<connect gate="G$1" pin="RA7/ASC1/CLKIN" pad="16"/>
<connect gate="G$1" pin="RB0/INT" pad="6"/>
<connect gate="G$1" pin="RB1/RX/DT" pad="7"/>
<connect gate="G$1" pin="RB2/TX/CK" pad="8"/>
<connect gate="G$1" pin="RB3/CCP1" pad="9"/>
<connect gate="G$1" pin="RB4/PGM" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6/T1OSO/1ICKI/PGC" pad="12"/>
<connect gate="G$1" pin="RB7/T1OSI/PGD" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F627-04/SO"/>
<attribute name="OC_FARNELL" value="1084265"/>
<attribute name="OC_NEWARK" value="69K7632"/>
</technology>
<technology name="L">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF627A-I/SO"/>
<attribute name="OC_FARNELL" value="1579593"/>
<attribute name="OC_NEWARK" value="92C4841"/>
</technology>
</technologies>
</device>
<device name="8P" package="DIL18">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="17"/>
<connect gate="G$1" pin="RA1/AN1" pad="18"/>
<connect gate="G$1" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="G$1" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="15"/>
<connect gate="G$1" pin="RA7/ASC1/CLKIN" pad="16"/>
<connect gate="G$1" pin="RB0/INT" pad="6"/>
<connect gate="G$1" pin="RB1/RX/DT" pad="7"/>
<connect gate="G$1" pin="RB2/TX/CK" pad="8"/>
<connect gate="G$1" pin="RB3/CCP1" pad="9"/>
<connect gate="G$1" pin="RB4/PGM" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6/T1OSO/1ICKI/PGC" pad="12"/>
<connect gate="G$1" pin="RB7/T1OSI/PGD" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F628-20/P"/>
<attribute name="OC_FARNELL" value="9760423"/>
<attribute name="OC_NEWARK" value="23C4982"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16LF628-04I/P"/>
<attribute name="OC_FARNELL" value="9761594"/>
<attribute name="OC_NEWARK" value="97K7476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*F62?SS" prefix="IC">
<description>&lt;b&gt;FLASH-Based 8-Bit CMOS Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/40300C.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F62X-SSOP"/>
</gates>
<devices>
<device name="7" package="SSOP20">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="G$1" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="17"/>
<connect gate="G$1" pin="RA7/ASC1/CLKIN" pad="18"/>
<connect gate="G$1" pin="RB0/INT" pad="7"/>
<connect gate="G$1" pin="RB1/RX/DT" pad="8"/>
<connect gate="G$1" pin="RB2/TX/CK" pad="9"/>
<connect gate="G$1" pin="RB3/CCP1" pad="10"/>
<connect gate="G$1" pin="RB4/PGM" pad="11"/>
<connect gate="G$1" pin="RB5" pad="12"/>
<connect gate="G$1" pin="RB6/T1OSO/1ICKI/PGC" pad="13"/>
<connect gate="G$1" pin="RB7/T1OSI/PGD" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F627-04I/SS"/>
<attribute name="OC_FARNELL" value="9760300"/>
<attribute name="OC_NEWARK" value="97K7324"/>
</technology>
<technology name="L">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16LF627-04/SS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88K1158"/>
</technology>
</technologies>
</device>
<device name="8" package="SSOP20">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="G$1" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="17"/>
<connect gate="G$1" pin="RA7/ASC1/CLKIN" pad="18"/>
<connect gate="G$1" pin="RB0/INT" pad="7"/>
<connect gate="G$1" pin="RB1/RX/DT" pad="8"/>
<connect gate="G$1" pin="RB2/TX/CK" pad="9"/>
<connect gate="G$1" pin="RB3/CCP1" pad="10"/>
<connect gate="G$1" pin="RB4/PGM" pad="11"/>
<connect gate="G$1" pin="RB5" pad="12"/>
<connect gate="G$1" pin="RB6/T1OSO/1ICKI/PGC" pad="13"/>
<connect gate="G$1" pin="RB7/T1OSI/PGD" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F628-20/SS"/>
<attribute name="OC_FARNELL" value="9760440"/>
<attribute name="OC_NEWARK" value="23C4984"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="93*76C" prefix="IC">
<description>&lt;b&gt;8K Microwire Compatible Serial EEPROM&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21796H.pdf</description>
<gates>
<gate name="G$1" symbol="93AA76"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="PE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA76C-I/P"/>
<attribute name="OC_FARNELL" value="1331446"/>
<attribute name="OC_NEWARK" value="61H6457"/>
</technology>
<technology name="C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C76C-I/P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="61H6696"/>
</technology>
<technology name="LC">
<attribute name="MF" value=""/>
<attribute name="MPN" value="93LC76C-I/P"/>
<attribute name="OC_FARNELL" value="1556171"/>
<attribute name="OC_NEWARK" value="95M3420"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="PE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="93AA76C-I/SN"/>
<attribute name="OC_FARNELL" value="1331447"/>
<attribute name="OC_NEWARK" value="35M2485"/>
</technology>
<technology name="C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C76C-I/SN"/>
<attribute name="OC_FARNELL" value="1815963"/>
<attribute name="OC_NEWARK" value="61H6698"/>
</technology>
<technology name="LC">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC76C-I/SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4113"/>
</technology>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="PE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93AA76CT-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="61H6467"/>
</technology>
<technology name="C">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93C76CT-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="61H6709"/>
</technology>
<technology name="LC">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC76C-I/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4114"/>
</technology>
</technologies>
</device>
<device name="MS" package="MSOP8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="PE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="93AA76C-I/MS"/>
<attribute name="OC_FARNELL" value="1331445"/>
<attribute name="OC_NEWARK" value="35M2483"/>
</technology>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC">
<attribute name="MF" value=""/>
<attribute name="MPN" value="93LC76C-I/MS"/>
<attribute name="OC_FARNELL" value="1331476"/>
<attribute name="OC_NEWARK" value="35M2509"/>
</technology>
</technologies>
</device>
<device name="MC" package="DFN-2X3">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="PE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="93*76?" prefix="IC">
<description>&lt;b&gt;8K Microwire Compatible Serial EEPROM&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21796H.pdf</description>
<gates>
<gate name="G$1" symbol="93AA76-OT"/>
</gates>
<devices>
<device name="A" package="SOT23-6">
<connects>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="93AA76AT-I/OT"/>
<attribute name="OC_FARNELL" value="1331443"/>
<attribute name="OC_NEWARK" value="35M2481"/>
</technology>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC76AT-I/OT"/>
<attribute name="OC_FARNELL" value="1556170"/>
<attribute name="OC_NEWARK" value="61H6824"/>
</technology>
</technologies>
</device>
<device name="B" package="SOT23-6">
<connects>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="AA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="93AA76BT-I/OT"/>
<attribute name="OC_FARNELL" value="1331444"/>
<attribute name="OC_NEWARK" value="35M2482"/>
</technology>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="LC">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC76BT-I/OT"/>
<attribute name="OC_FARNELL" value="1556170"/>
<attribute name="OC_NEWARK" value="61H6848"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC4467" prefix="IC">
<description>&lt;b&gt;Logic-Input CMOS Quad Drivers&lt;/b&gt;&lt;p&gt;
Source: TC 4469-MOSFET-DRIVER.pdf</description>
<gates>
<gate name="A" symbol="TC4467"/>
<gate name="B" symbol="TC4467"/>
<gate name="C" symbol="TC4467"/>
<gate name="D" symbol="TC4467"/>
<gate name="P" symbol="VDD-VSS"/>
</gates>
<devices>
<device name="DP" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="13"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="12"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="11"/>
<connect gate="D" pin="A" pad="8"/>
<connect gate="D" pin="B" pad="9"/>
<connect gate="D" pin="Y" pad="10"/>
<connect gate="P" pin="VDD" pad="7"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="TC4467CPD"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C6150"/>
</technology>
</technologies>
</device>
<device name="JD" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="13"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="12"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="11"/>
<connect gate="D" pin="A" pad="8"/>
<connect gate="D" pin="B" pad="9"/>
<connect gate="D" pin="Y" pad="10"/>
<connect gate="P" pin="VDD" pad="7"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="TC4467CPD"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C6150"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC4467OE" prefix="IC">
<description>&lt;b&gt;Logic-Input CMOS Quad Drivers&lt;/b&gt;&lt;p&gt;
Source: TC 4469-MOSFET-DRIVER.pdf</description>
<gates>
<gate name="A" symbol="TC4467"/>
<gate name="B" symbol="TC4467"/>
<gate name="C" symbol="TC4467"/>
<gate name="D" symbol="TC4467"/>
<gate name="P" symbol="VDD-GND-2"/>
</gates>
<devices>
<device name="" package="SO-16DW">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="14"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="13"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="12"/>
<connect gate="D" pin="A" pad="9"/>
<connect gate="D" pin="B" pad="10"/>
<connect gate="D" pin="Y" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="GND@1" pad="8"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VDD@1" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="TC4467COE"/>
<attribute name="OC_FARNELL" value="1836408"/>
<attribute name="OC_NEWARK" value="92C6148"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC4468OE" prefix="IC">
<description>&lt;b&gt;Logic-Input CMOS Quad Drivers&lt;/b&gt;&lt;p&gt;
Source: TC 4469-MOSFET-DRIVER.pdf</description>
<gates>
<gate name="A" symbol="TC4468"/>
<gate name="B" symbol="TC4468"/>
<gate name="C" symbol="TC4468"/>
<gate name="D" symbol="TC4468"/>
<gate name="P" symbol="VDD-GND-2"/>
</gates>
<devices>
<device name="" package="SO-16DW">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="14"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="13"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="12"/>
<connect gate="D" pin="A" pad="9"/>
<connect gate="D" pin="B" pad="10"/>
<connect gate="D" pin="Y" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="GND@1" pad="8"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VDD@1" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="TC4468EOE"/>
<attribute name="OC_FARNELL" value="1840858"/>
<attribute name="OC_NEWARK" value="56J8344"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC4468" prefix="IC">
<description>&lt;b&gt;Logic-Input CMOS Quad Drivers&lt;/b&gt;&lt;p&gt;
Source: TC 4469-MOSFET-DRIVER.pdf</description>
<gates>
<gate name="A" symbol="TC4468"/>
<gate name="B" symbol="TC4468"/>
<gate name="C" symbol="TC4468"/>
<gate name="D" symbol="TC4468"/>
<gate name="P" symbol="VDD-VSS"/>
</gates>
<devices>
<device name="DP" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="13"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="12"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="11"/>
<connect gate="D" pin="A" pad="8"/>
<connect gate="D" pin="B" pad="9"/>
<connect gate="D" pin="Y" pad="10"/>
<connect gate="P" pin="VDD" pad="7"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="TC4468CPD"/>
<attribute name="OC_FARNELL" value="1557406"/>
<attribute name="OC_NEWARK" value="54K2859"/>
</technology>
</technologies>
</device>
<device name="JD" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="13"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="12"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="11"/>
<connect gate="D" pin="A" pad="8"/>
<connect gate="D" pin="B" pad="9"/>
<connect gate="D" pin="Y" pad="10"/>
<connect gate="P" pin="VDD" pad="7"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC4469OE" prefix="IC">
<description>&lt;b&gt;Logic-Input CMOS Quad Drivers&lt;/b&gt;&lt;p&gt;
Source: TC 4469-MOSFET-DRIVER.pdf</description>
<gates>
<gate name="A" symbol="TC4469"/>
<gate name="B" symbol="TC4469"/>
<gate name="C" symbol="TC4469"/>
<gate name="D" symbol="TC4469"/>
<gate name="P" symbol="VDD-GND-2"/>
</gates>
<devices>
<device name="" package="SO-16DW">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="14"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="13"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="12"/>
<connect gate="D" pin="A" pad="9"/>
<connect gate="D" pin="B" pad="10"/>
<connect gate="D" pin="Y" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="GND@1" pad="8"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VDD@1" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="TC4469COE"/>
<attribute name="OC_FARNELL" value="1292288"/>
<attribute name="OC_NEWARK" value="92C6158"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC4469" prefix="IC">
<description>&lt;b&gt;Logic-Input CMOS Quad Drivers&lt;/b&gt;&lt;p&gt;
Source: TC 4469-MOSFET-DRIVER.pdf</description>
<gates>
<gate name="A" symbol="TC4469"/>
<gate name="B" symbol="TC4469"/>
<gate name="C" symbol="TC4469"/>
<gate name="D" symbol="TC4469"/>
<gate name="P" symbol="VDD-VSS"/>
</gates>
<devices>
<device name="DP" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="13"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="12"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="11"/>
<connect gate="D" pin="A" pad="8"/>
<connect gate="D" pin="B" pad="9"/>
<connect gate="D" pin="Y" pad="10"/>
<connect gate="P" pin="VDD" pad="7"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="TC4469CPD"/>
<attribute name="OC_FARNELL" value="1439739"/>
<attribute name="OC_NEWARK" value="92C6160"/>
</technology>
</technologies>
</device>
<device name="JD" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="Y" pad="13"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="B" pad="4"/>
<connect gate="B" pin="Y" pad="12"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="B" pad="6"/>
<connect gate="C" pin="Y" pad="11"/>
<connect gate="D" pin="A" pad="8"/>
<connect gate="D" pin="B" pad="9"/>
<connect gate="D" pin="Y" pad="10"/>
<connect gate="P" pin="VDD" pad="7"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F9*" prefix="IC">
<description>&lt;b&gt;1-Mbit Flash Microcontrollers with Ethernet&lt;/b&gt; 100-Pin High-Performance&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39762c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F97J60-100"/>
</gates>
<devices>
<device name="T" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="ENVREG" pad="29"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="63"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="64"/>
<connect gate="G$1" pin="RA0/AN0" pad="35"/>
<connect gate="G$1" pin="RA1/AN1" pad="34"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="33"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="32"/>
<connect gate="G$1" pin="RA4/T0CK" pad="42"/>
<connect gate="G$1" pin="RA5/AN4" pad="41"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="5"/>
<connect gate="G$1" pin="RB1/INT1" pad="6"/>
<connect gate="G$1" pin="RB2/INT2" pad="7"/>
<connect gate="G$1" pin="RB3/INT3/ACCP2/P2A" pad="8"/>
<connect gate="G$1" pin="RB4/KBI0" pad="69"/>
<connect gate="G$1" pin="RB5/KBI1" pad="68"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="67"/>
<connect gate="G$1" pin="RB7/KBI2/PGD" pad="57"/>
<connect gate="G$1" pin="RBIAS" pad="80"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="44"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="43"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="53"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="54"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="55"/>
<connect gate="G$1" pin="RC5/SDO1" pad="56"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="45"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="46"/>
<connect gate="G$1" pin="RD0/AD0/PSP0" pad="92"/>
<connect gate="G$1" pin="RD1/AD1/PSP1" pad="91"/>
<connect gate="G$1" pin="RD2/AD2/PSP2" pad="90"/>
<connect gate="G$1" pin="RD3/AD3/PSP3" pad="89"/>
<connect gate="G$1" pin="RD4/AD4/PSP4/SDO2" pad="88"/>
<connect gate="G$1" pin="RD5/AD5/PSP5/SDI2/SDA2" pad="87"/>
<connect gate="G$1" pin="RD6/AD6/PSP6/SCK2/SCL2" pad="84"/>
<connect gate="G$1" pin="RD7/AD7/PSP7/!SS2" pad="83"/>
<connect gate="G$1" pin="RE0/AD8/!RD/P2D" pad="4"/>
<connect gate="G$1" pin="RE1/AD9/!WR/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/!AD10CS/P2B" pad="98"/>
<connect gate="G$1" pin="RE3/AD11/P3C" pad="97"/>
<connect gate="G$1" pin="RE4/AD12/P3B" pad="96"/>
<connect gate="G$1" pin="RE5/AD13/P1C" pad="95"/>
<connect gate="G$1" pin="RE6/AD14/P1B" pad="94"/>
<connect gate="G$1" pin="RE7/AD15/ECCP2/P2A" pad="93"/>
<connect gate="G$1" pin="RF0/AN5" pad="12"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="28"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="23"/>
<connect gate="G$1" pin="RF3/AN8" pad="22"/>
<connect gate="G$1" pin="RF4/AN9" pad="21"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="20"/>
<connect gate="G$1" pin="RF6/AN11" pad="19"/>
<connect gate="G$1" pin="RF7/!SS1" pad="18"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="71"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="70"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="52"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="51"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="14"/>
<connect gate="G$1" pin="RG5" pad="11"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="38"/>
<connect gate="G$1" pin="RH0/A16" pad="99"/>
<connect gate="G$1" pin="RH1/A17" pad="100"/>
<connect gate="G$1" pin="RH2/A18" pad="1"/>
<connect gate="G$1" pin="RH3/A19" pad="2"/>
<connect gate="G$1" pin="RH4/AN12/P3C" pad="27"/>
<connect gate="G$1" pin="RH5/AN13/P3B" pad="26"/>
<connect gate="G$1" pin="RH6/AN14/P1C" pad="25"/>
<connect gate="G$1" pin="RH7/AN15/P1B" pad="24"/>
<connect gate="G$1" pin="RJ0/ALE" pad="49"/>
<connect gate="G$1" pin="RJ1/!OE" pad="50"/>
<connect gate="G$1" pin="RJ2/!WRL" pad="66"/>
<connect gate="G$1" pin="RJ3/!WRH" pad="61"/>
<connect gate="G$1" pin="RJ4/BA0" pad="47"/>
<connect gate="G$1" pin="RJ5/!CE" pad="48"/>
<connect gate="G$1" pin="RJ6/!LB" pad="58"/>
<connect gate="G$1" pin="RJ7/!UB" pad="39"/>
<connect gate="G$1" pin="TPIN+" pad="74"/>
<connect gate="G$1" pin="TPIN-" pad="73"/>
<connect gate="G$1" pin="TPOUT+" pad="78"/>
<connect gate="G$1" pin="TPOUT-" pad="77"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VDD@1" pad="37"/>
<connect gate="G$1" pin="VDD@2" pad="59"/>
<connect gate="G$1" pin="VDD@3" pad="62"/>
<connect gate="G$1" pin="VDD@4" pad="86"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="16"/>
<connect gate="G$1" pin="VDDPLL" pad="81"/>
<connect gate="G$1" pin="VDDRX" pad="75"/>
<connect gate="G$1" pin="VDDTX" pad="76"/>
<connect gate="G$1" pin="VSS" pad="15"/>
<connect gate="G$1" pin="VSS@1" pad="36"/>
<connect gate="G$1" pin="VSS@2" pad="40"/>
<connect gate="G$1" pin="VSS@3" pad="60"/>
<connect gate="G$1" pin="VSS@4" pad="65"/>
<connect gate="G$1" pin="VSS@5" pad="85"/>
<connect gate="G$1" pin="VSSPLL" pad="82"/>
<connect gate="G$1" pin="VSSRX" pad="72"/>
<connect gate="G$1" pin="VSSTX" pad="79"/>
</connects>
<technologies>
<technology name="6J60">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F96J60T-I/PT"/>
<attribute name="OC_FARNELL" value="1332292"/>
<attribute name="OC_NEWARK" value="54M5051"/>
</technology>
<technology name="6J65">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F96J65T-I/PT"/>
<attribute name="OC_FARNELL" value="1564573"/>
<attribute name="OC_NEWARK" value="74K8624"/>
</technology>
<technology name="7J60">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F97J60T-I/PT"/>
<attribute name="OC_FARNELL" value="1439573"/>
<attribute name="OC_NEWARK" value="59M1140"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F86" prefix="IC">
<description>&lt;b&gt;1-Mbit Flash Microcontrollers with Ethernet&lt;/b&gt; 80-Pin High-Performance&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39762c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F86-80"/>
</gates>
<devices>
<device name="" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ENVREG" pad="24"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="49"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="50"/>
<connect gate="G$1" pin="RA0/AN0" pad="30"/>
<connect gate="G$1" pin="RA1/AN1" pad="29"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="28"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="27"/>
<connect gate="G$1" pin="RA4/T0CK" pad="34"/>
<connect gate="G$1" pin="RA5/AN4" pad="33"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="5"/>
<connect gate="G$1" pin="RB1/INT1" pad="6"/>
<connect gate="G$1" pin="RB2/INT2" pad="7"/>
<connect gate="G$1" pin="RB3/INT3/ACCP2/P2A" pad="8"/>
<connect gate="G$1" pin="RB4/KBI0" pad="54"/>
<connect gate="G$1" pin="RB5/KBI1" pad="53"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="52"/>
<connect gate="G$1" pin="RB7/KBI2/PGD" pad="47"/>
<connect gate="G$1" pin="RBIAS" pad="65"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="36"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="43"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="44"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="45"/>
<connect gate="G$1" pin="RC5/SDO1" pad="46"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="37"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="38"/>
<connect gate="G$1" pin="RD0/AD0/PSP0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="69"/>
<connect gate="G$1" pin="RD2" pad="68"/>
<connect gate="G$1" pin="RE0/AD8/!RD/P2D" pad="4"/>
<connect gate="G$1" pin="RE1/AD9/!WR/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/!AD10CS/P2B" pad="78"/>
<connect gate="G$1" pin="RE3/AD11/P3C" pad="77"/>
<connect gate="G$1" pin="RE4/AD12/P3B" pad="76"/>
<connect gate="G$1" pin="RE5/AD13/P1C" pad="75"/>
<connect gate="G$1" pin="RE6/AD14/P1B" pad="74"/>
<connect gate="G$1" pin="RE7/AD15/ECCP2/P2A" pad="73"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="23"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="18"/>
<connect gate="G$1" pin="RF3/AN8" pad="17"/>
<connect gate="G$1" pin="RF4/AN9" pad="16"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="15"/>
<connect gate="G$1" pin="RF6/AN11" pad="14"/>
<connect gate="G$1" pin="RF7/!SS1" pad="13"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="56"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="55"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="42"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="41"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="10"/>
<connect gate="G$1" pin="RH0/A16" pad="79"/>
<connect gate="G$1" pin="RH1/A17" pad="80"/>
<connect gate="G$1" pin="RH2" pad="1"/>
<connect gate="G$1" pin="RH3" pad="2"/>
<connect gate="G$1" pin="RH4/AN12/P3C" pad="22"/>
<connect gate="G$1" pin="RH5/AN13/P3B" pad="21"/>
<connect gate="G$1" pin="RH6/AN14/P1C" pad="20"/>
<connect gate="G$1" pin="RH7/AN15/P1B" pad="19"/>
<connect gate="G$1" pin="RJ4/BA0" pad="39"/>
<connect gate="G$1" pin="RJ5/!CE" pad="40"/>
<connect gate="G$1" pin="TPIN+" pad="59"/>
<connect gate="G$1" pin="TPIN-" pad="58"/>
<connect gate="G$1" pin="TPOUT+" pad="63"/>
<connect gate="G$1" pin="TPOUT-" pad="62"/>
<connect gate="G$1" pin="VDD" pad="32"/>
<connect gate="G$1" pin="VDD@1" pad="48"/>
<connect gate="G$1" pin="VDD@2" pad="71"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="12"/>
<connect gate="G$1" pin="VDDPLL" pad="66"/>
<connect gate="G$1" pin="VDDRX" pad="60"/>
<connect gate="G$1" pin="VDDTX" pad="61"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
<connect gate="G$1" pin="VSS@2" pad="51"/>
<connect gate="G$1" pin="VSS@3" pad="70"/>
<connect gate="G$1" pin="VSSPLL" pad="67"/>
<connect gate="G$1" pin="VSSRX" pad="57"/>
<connect gate="G$1" pin="VSSTX" pad="64"/>
</connects>
<technologies>
<technology name="6J60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6J65">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7J60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC12F675" prefix="IC">
<description>&lt;b&gt;8-Pin FLASH-Based 8-Bit CMOS Microcontroller&lt;/b&gt;&lt;p&gt;
&lt;b&gt;&lt;i&gt;Precision Internal 4 MHz oscillator factory calibrated to ±1%&lt;/i&gt;&lt;/b&gt;&lt;br&gt;
Low Power Features:&lt;br&gt;
&lt;i&gt;Standby Current&lt;/i&gt;:&lt;br&gt;
 - 1 nA @ 2.0V, typical&lt;br&gt;
&lt;i&gt;Operating Current&lt;/i&gt;:&lt;br&gt;
 - 8.5&amp;micro;A @ 32 kHz, 2.0V, typical&lt;br&gt;
 - 100&amp;micro;A @ 1 MHz, 2.0V, typical &lt;br&gt;
&lt;i&gt;Watchdog Timer Current&lt;/i&gt;:&lt;br&gt;
 - 300 nA @ 2.0V, typical&lt;br&gt;
&lt;i&gt;Timer1 oscillator current&lt;/i&gt;:&lt;br&gt;
- 4&amp;micro;A @ 32 kHz, 2.0V, typical&lt;br&gt;
&lt;i&gt;Analog-to-Digital Converter module&lt;/i&gt;:&lt;br&gt;
- 10-bit resolution&lt;br&gt;
- Programmable 4-channel input&lt;br&gt;
- Voltage reference input&lt;p&gt;

Source: http://www.microchip.com .. 41190E.pdf</description>
<gates>
<gate name="G$1" symbol="PIC12F675"/>
</gates>
<devices>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GP0/AN0" pad="7"/>
<connect gate="G$1" pin="GP2/AN2" pad="5"/>
<connect gate="G$1" pin="GP3/!MCLR" pad="4"/>
<connect gate="G$1" pin="GP4/AN3" pad="3"/>
<connect gate="G$1" pin="GP5/CLKIN" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF/GP1/AN1" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F675-E/SN"/>
<attribute name="OC_FARNELL" value="9759026"/>
<attribute name="OC_NEWARK" value="92C4341"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GP0/AN0" pad="7"/>
<connect gate="G$1" pin="GP2/AN2" pad="5"/>
<connect gate="G$1" pin="GP3/!MCLR" pad="4"/>
<connect gate="G$1" pin="GP4/AN3" pad="3"/>
<connect gate="G$1" pin="GP5/CLKIN" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF/GP1/AN1" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F675-E/P"/>
<attribute name="OC_FARNELL" value="9759018"/>
<attribute name="OC_NEWARK" value="92C4340"/>
</technology>
</technologies>
</device>
<device name="MF" package="DFN-S">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GP0/AN0" pad="7"/>
<connect gate="G$1" pin="GP2/AN2" pad="5"/>
<connect gate="G$1" pin="GP3/!MCLR" pad="4"/>
<connect gate="G$1" pin="GP4/AN3" pad="3"/>
<connect gate="G$1" pin="GP5/CLKIN" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF/GP1/AN1" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F675-I/MF"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K3774"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ*GA010" prefix="IC">
<description>&lt;b&gt;64/80/100-Pin General Purpose, 16-Bit Flash Microcontrollers&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39747d.pdf</description>
<gates>
<gate name="G$1" symbol="PIC24FJ128GA010"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="!U1CTS/CN20/RD14" pad="47"/>
<connect gate="G$1" pin="!U1RTS/BCLK1/CN21/RD15" pad="48"/>
<connect gate="G$1" pin="!U2CTS/RF12" pad="40"/>
<connect gate="G$1" pin="!U2RTS/BCLK2/RF13" pad="39"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="C1IN+/AN5/CN7/RB5" pad="20"/>
<connect gate="G$1" pin="C1IN-/AN4/CN6/RB4" pad="21"/>
<connect gate="G$1" pin="C1OUT/AN8/RB8" pad="32"/>
<connect gate="G$1" pin="C2IN+/AN3/CN5/RB3" pad="22"/>
<connect gate="G$1" pin="C2IN-/AN2/SS1/CN4/RB2" pad="23"/>
<connect gate="G$1" pin="C2OUT/AN9/RB9" pad="33"/>
<connect gate="G$1" pin="CN15/RD6" pad="83"/>
<connect gate="G$1" pin="CN16/RD7" pad="84"/>
<connect gate="G$1" pin="CN19/RD13" pad="80"/>
<connect gate="G$1" pin="ENVREG" pad="86"/>
<connect gate="G$1" pin="IC1/RTCC/RD8" pad="68"/>
<connect gate="G$1" pin="IC2/RD9" pad="69"/>
<connect gate="G$1" pin="IC3/PMCS2/RD10" pad="70"/>
<connect gate="G$1" pin="IC4/PMCS1/RD11" pad="71"/>
<connect gate="G$1" pin="IC5/RD12" pad="79"/>
<connect gate="G$1" pin="INT1/RE8" pad="18"/>
<connect gate="G$1" pin="INT2/RE9" pad="19"/>
<connect gate="G$1" pin="INT3/RA14" pad="66"/>
<connect gate="G$1" pin="INT4/RA15" pad="67"/>
<connect gate="G$1" pin="OC1/RD0" pad="72"/>
<connect gate="G$1" pin="OC2/RD1" pad="76"/>
<connect gate="G$1" pin="OC3/RD2" pad="77"/>
<connect gate="G$1" pin="OSC1/CLKI/RC12" pad="63"/>
<connect gate="G$1" pin="OSC2/CLKO/RC15" pad="64"/>
<connect gate="G$1" pin="PGC1/EMUC1/AN1/CN3/RB1" pad="24"/>
<connect gate="G$1" pin="PGC2/EMUC2/AN6/OCFA/RB6" pad="26"/>
<connect gate="G$1" pin="PGD1/EMUD1/AN0/CN2/RB0" pad="25"/>
<connect gate="G$1" pin="PGD2/EMUD2/AN7/RB7" pad="27"/>
<connect gate="G$1" pin="PMA0/AN15/OCFB/CN12/RB15" pad="44"/>
<connect gate="G$1" pin="PMA1/AN14/RB14" pad="43"/>
<connect gate="G$1" pin="PMA10/AN13/RB13" pad="42"/>
<connect gate="G$1" pin="PMA11/AN12/RB12" pad="41"/>
<connect gate="G$1" pin="PMA12/AN11/RB11" pad="35"/>
<connect gate="G$1" pin="PMA13/CVREF/AN10/RB10" pad="34"/>
<connect gate="G$1" pin="PMA2/!SS2/CN11/RG9" pad="14"/>
<connect gate="G$1" pin="PMA3/SDO2/CN10/RG8" pad="12"/>
<connect gate="G$1" pin="PMA4/SDI2/CN9/RG7" pad="11"/>
<connect gate="G$1" pin="PMA5/SCK2/CN8/RG6" pad="10"/>
<connect gate="G$1" pin="PMA6/VREF+/RA10" pad="29"/>
<connect gate="G$1" pin="PMA7/VREF-/RA9" pad="28"/>
<connect gate="G$1" pin="PMA8/U2TX/CN18/RF5" pad="50"/>
<connect gate="G$1" pin="PMA9/U2RX/CN17/RF4" pad="49"/>
<connect gate="G$1" pin="PMBE/OC4/RD3" pad="78"/>
<connect gate="G$1" pin="PMD0/RE0" pad="93"/>
<connect gate="G$1" pin="PMD1/RE1" pad="94"/>
<connect gate="G$1" pin="PMD2/RE2" pad="98"/>
<connect gate="G$1" pin="PMD3/RE3" pad="99"/>
<connect gate="G$1" pin="PMD4/RE4" pad="100"/>
<connect gate="G$1" pin="PMD5/RE5" pad="3"/>
<connect gate="G$1" pin="PMD6/RE6" pad="4"/>
<connect gate="G$1" pin="PMD7/RE7" pad="5"/>
<connect gate="G$1" pin="PMRD/CN14/RD5" pad="82"/>
<connect gate="G$1" pin="PMWR/OC5/CN13/RD4" pad="81"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="SCK1/INT0/RF6" pad="55"/>
<connect gate="G$1" pin="SCL1/RG2" pad="57"/>
<connect gate="G$1" pin="SCL2/RA2" pad="58"/>
<connect gate="G$1" pin="SDA1/RG3" pad="56"/>
<connect gate="G$1" pin="SDA2/RA3" pad="59"/>
<connect gate="G$1" pin="SDI1/RF7" pad="54"/>
<connect gate="G$1" pin="SDO1/RF8" pad="53"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="73"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="74"/>
<connect gate="G$1" pin="T2CK/RC1" pad="6"/>
<connect gate="G$1" pin="T3CK/RC2" pad="7"/>
<connect gate="G$1" pin="T4CK/RC3" pad="8"/>
<connect gate="G$1" pin="T5CK/RC4" pad="9"/>
<connect gate="G$1" pin="TCK/RA1" pad="38"/>
<connect gate="G$1" pin="TDI/RA4" pad="60"/>
<connect gate="G$1" pin="TDO/RA5" pad="61"/>
<connect gate="G$1" pin="TMS/RA0" pad="17"/>
<connect gate="G$1" pin="U1RX/RF2" pad="52"/>
<connect gate="G$1" pin="U1TX/RF3" pad="51"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="85"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VSS@1" pad="15"/>
<connect gate="G$1" pin="VSS@2" pad="36"/>
<connect gate="G$1" pin="VSS@3" pad="45"/>
<connect gate="G$1" pin="VSS@4" pad="65"/>
<connect gate="G$1" pin="VSS@5" pad="75"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ128GA010-I/PT"/>
<attribute name="OC_FARNELL" value="1146522"/>
<attribute name="OC_NEWARK" value="56K7341"/>
</technology>
<technology name="64">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ64GA010-I/PT"/>
<attribute name="OC_FARNELL" value="1146526"/>
<attribute name="OC_NEWARK" value="56K7347"/>
</technology>
<technology name="96">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ96GA010-I/PT"/>
<attribute name="OC_FARNELL" value="1778488"/>
<attribute name="OC_NEWARK" value="56K7353"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ*GA008" prefix="IC">
<description>&lt;b&gt;64/80/100-Pin General Purpose, 16-Bit Flash Microcontrollers&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39747d.pdf</description>
<gates>
<gate name="G$1" symbol="PIC24FJ128GA008"/>
</gates>
<devices>
<device name="" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="!U1CTS/CN20/RD14" pad="37"/>
<connect gate="G$1" pin="!U1RTS/BCLK1/CN21/RD15" pad="38"/>
<connect gate="G$1" pin="!U2CTS/C1OUT/AN8/RB8" pad="27"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="C1IN+/AN5/CN7/RB5" pad="15"/>
<connect gate="G$1" pin="C1IN-/AN4/CN6/RB4" pad="16"/>
<connect gate="G$1" pin="C2IN+/AN3/CN5/RB3" pad="17"/>
<connect gate="G$1" pin="C2IN-/AN2/SS1/CN4/RB2" pad="18"/>
<connect gate="G$1" pin="C2OUT/AN9/RB9" pad="28"/>
<connect gate="G$1" pin="CN15/RD6" pad="68"/>
<connect gate="G$1" pin="CN16/RD7" pad="69"/>
<connect gate="G$1" pin="CN19/RD13" pad="65"/>
<connect gate="G$1" pin="ENVREG" pad="71"/>
<connect gate="G$1" pin="IC1/RTCC/RD8" pad="54"/>
<connect gate="G$1" pin="IC2/RD9" pad="55"/>
<connect gate="G$1" pin="IC3/PMCS2/RD10" pad="56"/>
<connect gate="G$1" pin="IC4/PMCS1/RD11" pad="57"/>
<connect gate="G$1" pin="IC5/RD12" pad="64"/>
<connect gate="G$1" pin="OC1/RD0" pad="58"/>
<connect gate="G$1" pin="OC2/RD1" pad="61"/>
<connect gate="G$1" pin="OC3/RD2" pad="62"/>
<connect gate="G$1" pin="OSC1/CLKI/RC12" pad="49"/>
<connect gate="G$1" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="G$1" pin="PGC1/EMUC1/AN1/CN3/RB1" pad="19"/>
<connect gate="G$1" pin="PGC2/EMUC2/AN6/OCFA/RB6" pad="21"/>
<connect gate="G$1" pin="PGD1/EMUD1/AN0/CN2/RB0" pad="20"/>
<connect gate="G$1" pin="PGD2/EMUD2/AN7/RB7" pad="22"/>
<connect gate="G$1" pin="PMA0/AN15/OCFB/CN12/RB15" pad="36"/>
<connect gate="G$1" pin="PMA1/!U2RTS/BCLK2/AN14/RB14" pad="35"/>
<connect gate="G$1" pin="PMA12/AN11/RB11" pad="30"/>
<connect gate="G$1" pin="PMA13/CVREF/AN10/RB10" pad="29"/>
<connect gate="G$1" pin="PMA2/!SS2/CN11/RG9" pad="10"/>
<connect gate="G$1" pin="PMA3/SDO2/CN10/RG8" pad="8"/>
<connect gate="G$1" pin="PMA4/SDI2/CN9/RG7" pad="7"/>
<connect gate="G$1" pin="PMA5/SCK2/CN8/RG6" pad="6"/>
<connect gate="G$1" pin="PMA6/VREF+/RA10" pad="24"/>
<connect gate="G$1" pin="PMA7/VREF-/RA9" pad="23"/>
<connect gate="G$1" pin="PMA8/U2TX/CN18/RF5" pad="40"/>
<connect gate="G$1" pin="PMA9/U2RX/CN17/RF4" pad="39"/>
<connect gate="G$1" pin="PMBE/OC4/RD3" pad="63"/>
<connect gate="G$1" pin="PMD0/RE0" pad="76"/>
<connect gate="G$1" pin="PMD1/RE1" pad="77"/>
<connect gate="G$1" pin="PMD2/RE2" pad="78"/>
<connect gate="G$1" pin="PMD3/RE3" pad="79"/>
<connect gate="G$1" pin="PMD4/RE4" pad="80"/>
<connect gate="G$1" pin="PMD5/RE5" pad="1"/>
<connect gate="G$1" pin="PMD6/RE6" pad="2"/>
<connect gate="G$1" pin="PMD7/RE7" pad="3"/>
<connect gate="G$1" pin="PMRD/CN14/RD5" pad="67"/>
<connect gate="G$1" pin="PMWR/OC5/CN13/RD4" pad="66"/>
<connect gate="G$1" pin="RF0" pad="72"/>
<connect gate="G$1" pin="RF1" pad="73"/>
<connect gate="G$1" pin="RG0" pad="75"/>
<connect gate="G$1" pin="RG1" pad="74"/>
<connect gate="G$1" pin="SCK1/INT0/RF6" pad="45"/>
<connect gate="G$1" pin="SCL1/RG2" pad="47"/>
<connect gate="G$1" pin="SCL2/INT3/RA14" pad="52"/>
<connect gate="G$1" pin="SDA1/RG3" pad="46"/>
<connect gate="G$1" pin="SDA2/INT4/RA15" pad="53"/>
<connect gate="G$1" pin="SDI1/RF7" pad="44"/>
<connect gate="G$1" pin="SDO1/RF8" pad="43"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="59"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="60"/>
<connect gate="G$1" pin="T2CK/RC1" pad="4"/>
<connect gate="G$1" pin="T4CK/RC3" pad="5"/>
<connect gate="G$1" pin="TCK/PMA11/AN12/RB12" pad="33"/>
<connect gate="G$1" pin="TDI/PMA10/AN13/RB13" pad="34"/>
<connect gate="G$1" pin="TDO/INT2/RE9" pad="14"/>
<connect gate="G$1" pin="TMS/INT1/RE8" pad="13"/>
<connect gate="G$1" pin="U1RX/RF2" pad="42"/>
<connect gate="G$1" pin="U1TX/RF3" pad="41"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="70"/>
<connect gate="G$1" pin="VDD@2" pad="12"/>
<connect gate="G$1" pin="VDD@3" pad="32"/>
<connect gate="G$1" pin="VDD@5" pad="48"/>
<connect gate="G$1" pin="VSS@1" pad="11"/>
<connect gate="G$1" pin="VSS@2" pad="31"/>
<connect gate="G$1" pin="VSS@4" pad="51"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC24FJ128GA008-I/PT"/>
<attribute name="OC_FARNELL" value="1146521"/>
<attribute name="OC_NEWARK" value="56K7339"/>
</technology>
<technology name="64">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ64GA008-I/PT"/>
<attribute name="OC_FARNELL" value="1146525"/>
<attribute name="OC_NEWARK" value="56K7345"/>
</technology>
<technology name="96">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ96GA008-I/PT"/>
<attribute name="OC_FARNELL" value="1146529"/>
<attribute name="OC_NEWARK" value="56K7351"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ*GA006" prefix="IC">
<description>&lt;b&gt;64/80/100-Pin General Purpose, 16-Bit Flash Microcontrollers&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39747d.pdf</description>
<gates>
<gate name="G$1" symbol="PIC24FJ128GA006"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="!U1RTS/BCLK1/SCK1/INT0/RF6" pad="35"/>
<connect gate="G$1" pin="!U2CTS/C1OUT/AN8/RB8" pad="21"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="C1IN+/AN5/CN7/RB5" pad="11"/>
<connect gate="G$1" pin="C1IN-/AN4/CN6/RB4" pad="12"/>
<connect gate="G$1" pin="C2IN+/AN3/CN5/RB3" pad="13"/>
<connect gate="G$1" pin="C2IN-/AN2/SS1/CN4/RB2" pad="14"/>
<connect gate="G$1" pin="CN15/RD6" pad="54"/>
<connect gate="G$1" pin="CN16/RD7" pad="55"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="IC1/RTCC/INT1/RD8" pad="42"/>
<connect gate="G$1" pin="IC2/!U1CTS/INT2/RD9" pad="43"/>
<connect gate="G$1" pin="IC3/PMCS2/INT3/RD10" pad="44"/>
<connect gate="G$1" pin="IC4/PMCS1/INT4/RD11" pad="45"/>
<connect gate="G$1" pin="OC1/RD0" pad="46"/>
<connect gate="G$1" pin="OC2/RD1" pad="49"/>
<connect gate="G$1" pin="OC3/RD2" pad="50"/>
<connect gate="G$1" pin="OSC1/CLKI/RC12" pad="39"/>
<connect gate="G$1" pin="OSC2/CLKO/RC15" pad="40"/>
<connect gate="G$1" pin="PGC1/EMUC1/AN1/CN3/RB1" pad="15"/>
<connect gate="G$1" pin="PGC2/EMUC2/AN6/OCFA/RB6" pad="17"/>
<connect gate="G$1" pin="PGD1/EMUD1/AN0/CN2/RB0" pad="16"/>
<connect gate="G$1" pin="PGD2/EMUD2/AN7/RB7" pad="18"/>
<connect gate="G$1" pin="PMA0/AN15/OCFB/CN12/RB15" pad="30"/>
<connect gate="G$1" pin="PMA1/!U2RTS/BCLK2/AN14/RB14" pad="29"/>
<connect gate="G$1" pin="PMA2/!SS2/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="PMA3/SDO2/CN10/RG8" pad="6"/>
<connect gate="G$1" pin="PMA4/SDI2/CN9/RG7" pad="5"/>
<connect gate="G$1" pin="PMA5/SCK2/CN8/RG6" pad="4"/>
<connect gate="G$1" pin="PMA7/C2OUT/AN9/RB9" pad="22"/>
<connect gate="G$1" pin="PMA8/U2TX/SCL2/CN18/RF5" pad="32"/>
<connect gate="G$1" pin="PMA9/U2RX/SDA2/CN17/RF4" pad="31"/>
<connect gate="G$1" pin="PMBE/OC4/RD3" pad="51"/>
<connect gate="G$1" pin="PMD0/RE0" pad="60"/>
<connect gate="G$1" pin="PMD1/RE1" pad="61"/>
<connect gate="G$1" pin="PMD2/RE2" pad="62"/>
<connect gate="G$1" pin="PMD3/RE3" pad="63"/>
<connect gate="G$1" pin="PMD4/RE4" pad="64"/>
<connect gate="G$1" pin="PMD5/RE5" pad="1"/>
<connect gate="G$1" pin="PMD6/RE6" pad="2"/>
<connect gate="G$1" pin="PMD7/RE7" pad="3"/>
<connect gate="G$1" pin="PMRD/CN14/RD5" pad="53"/>
<connect gate="G$1" pin="PMWR/OC5/CN13/RD4" pad="52"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="SCL1/RG2" pad="37"/>
<connect gate="G$1" pin="SDA1/RG3" pad="36"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="TCK/PMA11/AN12/RB12" pad="27"/>
<connect gate="G$1" pin="TDI/PMA10/AN13/RB13" pad="28"/>
<connect gate="G$1" pin="TDO/PMA12/AN11/RB11" pad="24"/>
<connect gate="G$1" pin="TMS/PMA13/CVREF/AN10/RB10" pad="23"/>
<connect gate="G$1" pin="U1RX/RF2" pad="34"/>
<connect gate="G$1" pin="U1TX/RF3" pad="33"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="56"/>
<connect gate="G$1" pin="VDD@2" pad="10"/>
<connect gate="G$1" pin="VDD@3" pad="26"/>
<connect gate="G$1" pin="VDD@5" pad="38"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@4" pad="41"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC24FJ128GA006-I/PT"/>
<attribute name="OC_FARNELL" value="1146519"/>
<attribute name="OC_NEWARK" value="56K7337"/>
</technology>
<technology name="64">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ64GA006-I/PT"/>
<attribute name="OC_FARNELL" value="1146524"/>
<attribute name="OC_NEWARK" value="56K7343"/>
</technology>
<technology name="69">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F676" prefix="IC">
<description>&lt;b&gt;14-Pin, Flash-Based 8-Bit&lt;/b&gt; CMOS Microcontroller&lt;p&gt;
High Performance RISC CPU:&lt;br&gt;
* Only 35 instructions to learn&lt;br&gt;
- All single-cycle instructions except branches&lt;br&gt;
* Operating speed:&lt;br&gt;
- DC - 20 MHz oscillator/clock input&lt;br&gt;
- DC - 200 ns instruction cycle&lt;br&gt;
&lt;br&gt;
* Internal and external oscillator options&lt;br&gt;
- Precision Internal 4 MHz oscillator factory calibrated to ±1%&lt;br&gt;
- External Oscillator support for crystals and resonators&lt;br&gt;
- 5?s wake-up from SLEEP, 3.0V, typical&lt;br&gt;
* Power saving SLEEP mode&lt;br&gt;
* Wide operating voltage range - 2.0V to 5.5V&lt;br&gt;
* Industrial and Extended temperature range&lt;br&gt;
* Low power Power-on Reset (POR)&lt;br&gt;
* Power-up Timer (PWRT) and Oscillator Start-up Timer (OST)&lt;br&gt;
* Brown-out Detect (BOD)&lt;br&gt;
* Watchdog Timer (WDT) with independent oscillator for reliable operation&lt;br&gt;
* Multiplexed MCLR/Input-pin&lt;br&gt;
* Interrupt-on-pin change&lt;br&gt;
* Individual programmable weak pull-ups&lt;br&gt;
* Programmable code protection&lt;br&gt;
* High Endurance FLASH/EEPROM Cell&lt;br&gt;
- 100,000 write FLASH endurance&lt;br&gt;
- 1,000,000 write EEPROM endurance&lt;br&gt;
- FLASH/Data EEPROM Retention: &gt; 40 years&lt;br&gt;
&lt;br&gt;
* Standby Current:&lt;br&gt;
- 1 nA @ 2.0V, typical&lt;br&gt;
* Operating Current:&lt;br&gt;
- 8.5?A @ 32 kHz, 2.0V, typical&lt;br&gt;
- 100?A @ 1 MHz, 2.0V, typical&lt;br&gt;
* Watchdog Timer Current&lt;br&gt;
- 300 nA @ 2.0V, typical&lt;br&gt;
* Timer1 oscillator current:&lt;br&gt;
- 4?A @ 32 kHz, 2.0V, typical&lt;br&gt;
&lt;br&gt;
* 12 I/O pins with individual direction control&lt;br&gt;
* High current sink/source for direct LED drive&lt;br&gt;
&lt;br&gt;
* Analog-to-Digital Converter module (PIC16F676):&lt;br&gt;
- 10-bit resolution&lt;br&gt;
- Programmable 8-channel input&lt;br&gt;
- Voltage reference input&lt;br&gt;
&lt;br&gt;
* In-Circuit Serial ProgrammingTM (ICSPTM) via two pins
&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/40039E.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F676"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="G$1" pin="CIN+/ICSPDAT/AN0/RA0" pad="13"/>
<connect gate="G$1" pin="CIN-/VREF/ICSPCLK/AN1/RA1" pad="12"/>
<connect gate="G$1" pin="COUT/T0CKI/INT/AN2/RA2" pad="11"/>
<connect gate="G$1" pin="OSC1/CLKIN/T1CKI/RA5" pad="2"/>
<connect gate="G$1" pin="RC0/AN4" pad="10"/>
<connect gate="G$1" pin="RC1/AN5" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="5"/>
<connect gate="G$1" pin="T1G/OSC2/CLKOUT/AN3/RA4" pad="3"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VPP/MCLR/RA3" pad="4"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F676-I/P"/>
<attribute name="OC_FARNELL" value="9760512"/>
<attribute name="OC_NEWARK" value="54K2829"/>
</technology>
</technologies>
</device>
<device name="SL" package="SOIC-14">
<connects>
<connect gate="G$1" pin="CIN+/ICSPDAT/AN0/RA0" pad="13"/>
<connect gate="G$1" pin="CIN-/VREF/ICSPCLK/AN1/RA1" pad="12"/>
<connect gate="G$1" pin="COUT/T0CKI/INT/AN2/RA2" pad="11"/>
<connect gate="G$1" pin="OSC1/CLKIN/T1CKI/RA5" pad="2"/>
<connect gate="G$1" pin="RC0/AN4" pad="10"/>
<connect gate="G$1" pin="RC1/AN5" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="5"/>
<connect gate="G$1" pin="T1G/OSC2/CLKOUT/AN3/RA4" pad="3"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VPP/MCLR/RA3" pad="4"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F676-I/SL"/>
<attribute name="OC_FARNELL" value="9760520"/>
<attribute name="OC_NEWARK" value="92C4557"/>
</technology>
</technologies>
</device>
<device name="TS" package="TSSOP14">
<connects>
<connect gate="G$1" pin="CIN+/ICSPDAT/AN0/RA0" pad="13"/>
<connect gate="G$1" pin="CIN-/VREF/ICSPCLK/AN1/RA1" pad="12"/>
<connect gate="G$1" pin="COUT/T0CKI/INT/AN2/RA2" pad="11"/>
<connect gate="G$1" pin="OSC1/CLKIN/T1CKI/RA5" pad="2"/>
<connect gate="G$1" pin="RC0/AN4" pad="10"/>
<connect gate="G$1" pin="RC1/AN5" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="5"/>
<connect gate="G$1" pin="T1G/OSC2/CLKOUT/AN3/RA4" pad="3"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VPP/MCLR/RA3" pad="4"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F676-E/ST"/>
<attribute name="OC_FARNELL" value="9760539"/>
<attribute name="OC_NEWARK" value="92C4552"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F*2" prefix="IC">
<description>&lt;b&gt;High-Performance, Enhanced Flash Microcontrollers with 10-Bit A/D&lt;/b&gt;&lt;p&gt;
Source: http://www.microchip.com .. 39564c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F452-44"/>
</gates>
<devices>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP" pad="2"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="34"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="17"/>
<connect gate="G$1" pin="NC@2" pad="28"/>
<connect gate="G$1" pin="NC@3" pad="40"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="14"/>
<connect gate="G$1" pin="RA0/AN0" pad="3"/>
<connect gate="G$1" pin="RA1/AN1" pad="4"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="5"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="6"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="7"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/LVDIN" pad="8"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="15"/>
<connect gate="G$1" pin="RB0/INT0" pad="36"/>
<connect gate="G$1" pin="RB1/INT1" pad="37"/>
<connect gate="G$1" pin="RB2/INT2" pad="38"/>
<connect gate="G$1" pin="RB3/CCP2" pad="39"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5/PGM" pad="42"/>
<connect gate="G$1" pin="RB6/PGC" pad="43"/>
<connect gate="G$1" pin="RB7/PGD" pad="44"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI" pad="16"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2" pad="18"/>
<connect gate="G$1" pin="RC2/CCP1" pad="19"/>
<connect gate="G$1" pin="RC3/SCK/SCL" pad="20"/>
<connect gate="G$1" pin="RC4/SDI/SDA" pad="25"/>
<connect gate="G$1" pin="RC5/SDO" pad="26"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="27"/>
<connect gate="G$1" pin="RC7/RX/DT" pad="29"/>
<connect gate="G$1" pin="RD0/PSP0" pad="21"/>
<connect gate="G$1" pin="RD1/PSP1" pad="22"/>
<connect gate="G$1" pin="RD2/PSP2" pad="23"/>
<connect gate="G$1" pin="RD3/PSP3" pad="24"/>
<connect gate="G$1" pin="RD4/PSP4" pad="30"/>
<connect gate="G$1" pin="RD5/PSP5" pad="31"/>
<connect gate="G$1" pin="RD6/PSP6" pad="32"/>
<connect gate="G$1" pin="RD7/PSP7" pad="33"/>
<connect gate="G$1" pin="RE0/AN5/!RD" pad="9"/>
<connect gate="G$1" pin="RE1/AN6/!WR" pad="10"/>
<connect gate="G$1" pin="RE2/AN7/!CS" pad="11"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VCC@1" pad="35"/>
</connects>
<technologies>
<technology name="44">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F442-E/L"/>
<attribute name="OC_FARNELL" value="9762175"/>
<attribute name="OC_NEWARK" value="72C4322"/>
</technology>
<technology name="45">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F452I/L"/>
<attribute name="OC_FARNELL" value="9762221"/>
<attribute name="OC_NEWARK" value="34C8340"/>
</technology>
</technologies>
</device>
<device name="PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP" pad="18"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="29"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="30"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="21"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/LVDIN" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="31"/>
<connect gate="G$1" pin="RB0/INT0" pad="8"/>
<connect gate="G$1" pin="RB1/INT1" pad="9"/>
<connect gate="G$1" pin="RB2/INT2" pad="10"/>
<connect gate="G$1" pin="RB3/CCP2" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5/PGM" pad="15"/>
<connect gate="G$1" pin="RB6/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/PGD" pad="17"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI" pad="32"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1" pad="36"/>
<connect gate="G$1" pin="RC3/SCK/SCL" pad="37"/>
<connect gate="G$1" pin="RC4/SDI/SDA" pad="42"/>
<connect gate="G$1" pin="RC5/SDO" pad="43"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="44"/>
<connect gate="G$1" pin="RC7/RX/DT" pad="1"/>
<connect gate="G$1" pin="RD0/PSP0" pad="38"/>
<connect gate="G$1" pin="RD1/PSP1" pad="39"/>
<connect gate="G$1" pin="RD2/PSP2" pad="40"/>
<connect gate="G$1" pin="RD3/PSP3" pad="41"/>
<connect gate="G$1" pin="RD4/PSP4" pad="2"/>
<connect gate="G$1" pin="RD5/PSP5" pad="3"/>
<connect gate="G$1" pin="RD6/PSP6" pad="4"/>
<connect gate="G$1" pin="RD7/PSP7" pad="5"/>
<connect gate="G$1" pin="RE0/AN5/!RD" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/!WR" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/!CS" pad="27"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VCC@1" pad="28"/>
</connects>
<technologies>
<technology name="44">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F442-I/PT"/>
<attribute name="OC_FARNELL" value="1084324"/>
<attribute name="OC_NEWARK" value="61K3472"/>
</technology>
<technology name="45">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F452-E/PT"/>
<attribute name="OC_FARNELL" value="9762248"/>
<attribute name="OC_NEWARK" value="72C4329"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC15*" prefix="IC">
<description>&lt;b&gt;2.5V and 4.096V Voltage References&lt;/b&gt;&lt;p&gt;
Source: http://www.microchip.com .. 21653b.pdf</description>
<gates>
<gate name="G$1" symbol="MCP1525"/>
</gates>
<devices>
<device name="TT" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="25">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="41">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TO" package="TO92">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="25">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="41">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F6*J5" prefix="IC">
<description>&lt;b&gt;PIC18F87J50 Family&lt;/b&gt;&lt;p&gt;
64/80-Pin High-Performance, 1-Mbit Flash USB Microcontrollers with nanoWatt Technology&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39775b.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F6XJ5X"/>
</gates>
<devices>
<device name="0" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="ENVREG" pad="18"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="39"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="40"/>
<connect gate="G$1" pin="PMA5/AN7/C2INB" pad="16"/>
<connect gate="G$1" pin="RA0/AN0" pad="24"/>
<connect gate="G$1" pin="RA1/AN1" pad="23"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="22"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="21"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="28"/>
<connect gate="G$1" pin="RA5/AN4/C2INA" pad="27"/>
<connect gate="G$1" pin="RB0/FLT0/INT0" pad="48"/>
<connect gate="G$1" pin="RB1/INT1/PMA4" pad="47"/>
<connect gate="G$1" pin="RB2/INT2/PMA3" pad="46"/>
<connect gate="G$1" pin="RB3/INT3/PMA2" pad="45"/>
<connect gate="G$1" pin="RB4/KBI0/PMA1" pad="44"/>
<connect gate="G$1" pin="RB5/KBI1/PMA0" pad="43"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="42"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="37"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="30"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="29"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="33"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="34"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="35"/>
<connect gate="G$1" pin="RC5/SDO1/C2OUT" pad="36"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="31"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="32"/>
<connect gate="G$1" pin="RD0/PMD0" pad="58"/>
<connect gate="G$1" pin="RD1/PMD1" pad="55"/>
<connect gate="G$1" pin="RD2/PMD2" pad="54"/>
<connect gate="G$1" pin="RD3/PMD3" pad="53"/>
<connect gate="G$1" pin="RD4/PMD4/SDO2" pad="52"/>
<connect gate="G$1" pin="RD5/PMD5/SDI2/SDA2" pad="51"/>
<connect gate="G$1" pin="RD6/PMD6/SCK2/SCL2" pad="50"/>
<connect gate="G$1" pin="RD7/PMD7/!SS2" pad="49"/>
<connect gate="G$1" pin="RE0/PMRD/P2D" pad="2"/>
<connect gate="G$1" pin="RE1/PMWR/P2C" pad="1"/>
<connect gate="G$1" pin="RE2/PMBE/P2B" pad="64"/>
<connect gate="G$1" pin="RE3/PMA13/P3C/REFO" pad="63"/>
<connect gate="G$1" pin="RE4/PMA12/P3B" pad="62"/>
<connect gate="G$1" pin="RE5/PMA11/P1C" pad="61"/>
<connect gate="G$1" pin="RE6/PMA10/P1B" pad="60"/>
<connect gate="G$1" pin="RE7/PMA9/ECCP2/P2A" pad="59"/>
<connect gate="G$1" pin="RF3/DRF2/" pad="15"/>
<connect gate="G$1" pin="RF4/D+" pad="14"/>
<connect gate="G$1" pin="RF5/AN10/C1INB/CVREF" pad="13"/>
<connect gate="G$1" pin="RF6/AN11/C1INA" pad="12"/>
<connect gate="G$1" pin="RF7/!SS1!/C1OUT" pad="11"/>
<connect gate="G$1" pin="RG0/PMA8/ECCP3/P3A" pad="3"/>
<connect gate="G$1" pin="RG1/PMA7/TX2/CK2" pad="4"/>
<connect gate="G$1" pin="RG2/PMA6/RX2/DT2" pad="5"/>
<connect gate="G$1" pin="RG3/PMCS1/CCP4/P3D" pad="6"/>
<connect gate="G$1" pin="RG4/PMCS2/CCP5/P1D" pad="8"/>
<connect gate="G$1" pin="VDD" pad="26"/>
<connect gate="G$1" pin="VDD@1" pad="38"/>
<connect gate="G$1" pin="VDD@2" pad="57"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="10"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSS@1" pad="25"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="VSS@3" pad="56"/>
<connect gate="G$1" pin="VUSB" pad="17"/>
</connects>
<technologies>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F65J50-I/PT"/>
<attribute name="OC_FARNELL" value="1439552"/>
<attribute name="OC_NEWARK" value="17M0960"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F66J50-I/PT"/>
<attribute name="OC_FARNELL" value="1439555"/>
<attribute name="OC_NEWARK" value="17M0966"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F67J50-I/PT"/>
<attribute name="OC_FARNELL" value="1439559"/>
<attribute name="OC_NEWARK" value="17M0972"/>
</technology>
</technologies>
</device>
<device name="5" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="ENVREG" pad="18"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="39"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="40"/>
<connect gate="G$1" pin="PMA5/AN7/C2INB" pad="16"/>
<connect gate="G$1" pin="RA0/AN0" pad="24"/>
<connect gate="G$1" pin="RA1/AN1" pad="23"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="22"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="21"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="28"/>
<connect gate="G$1" pin="RA5/AN4/C2INA" pad="27"/>
<connect gate="G$1" pin="RB0/FLT0/INT0" pad="48"/>
<connect gate="G$1" pin="RB1/INT1/PMA4" pad="47"/>
<connect gate="G$1" pin="RB2/INT2/PMA3" pad="46"/>
<connect gate="G$1" pin="RB3/INT3/PMA2" pad="45"/>
<connect gate="G$1" pin="RB4/KBI0/PMA1" pad="44"/>
<connect gate="G$1" pin="RB5/KBI1/PMA0" pad="43"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="42"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="37"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="30"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="29"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="33"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="34"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="35"/>
<connect gate="G$1" pin="RC5/SDO1/C2OUT" pad="36"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="31"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="32"/>
<connect gate="G$1" pin="RD0/PMD0" pad="58"/>
<connect gate="G$1" pin="RD1/PMD1" pad="55"/>
<connect gate="G$1" pin="RD2/PMD2" pad="54"/>
<connect gate="G$1" pin="RD3/PMD3" pad="53"/>
<connect gate="G$1" pin="RD4/PMD4/SDO2" pad="52"/>
<connect gate="G$1" pin="RD5/PMD5/SDI2/SDA2" pad="51"/>
<connect gate="G$1" pin="RD6/PMD6/SCK2/SCL2" pad="50"/>
<connect gate="G$1" pin="RD7/PMD7/!SS2" pad="49"/>
<connect gate="G$1" pin="RE0/PMRD/P2D" pad="2"/>
<connect gate="G$1" pin="RE1/PMWR/P2C" pad="1"/>
<connect gate="G$1" pin="RE2/PMBE/P2B" pad="64"/>
<connect gate="G$1" pin="RE3/PMA13/P3C/REFO" pad="63"/>
<connect gate="G$1" pin="RE4/PMA12/P3B" pad="62"/>
<connect gate="G$1" pin="RE5/PMA11/P1C" pad="61"/>
<connect gate="G$1" pin="RE6/PMA10/P1B" pad="60"/>
<connect gate="G$1" pin="RE7/PMA9/ECCP2/P2A" pad="59"/>
<connect gate="G$1" pin="RF3/DRF2/" pad="15"/>
<connect gate="G$1" pin="RF4/D+" pad="14"/>
<connect gate="G$1" pin="RF5/AN10/C1INB/CVREF" pad="13"/>
<connect gate="G$1" pin="RF6/AN11/C1INA" pad="12"/>
<connect gate="G$1" pin="RF7/!SS1!/C1OUT" pad="11"/>
<connect gate="G$1" pin="RG0/PMA8/ECCP3/P3A" pad="3"/>
<connect gate="G$1" pin="RG1/PMA7/TX2/CK2" pad="4"/>
<connect gate="G$1" pin="RG2/PMA6/RX2/DT2" pad="5"/>
<connect gate="G$1" pin="RG3/PMCS1/CCP4/P3D" pad="6"/>
<connect gate="G$1" pin="RG4/PMCS2/CCP5/P1D" pad="8"/>
<connect gate="G$1" pin="VDD" pad="26"/>
<connect gate="G$1" pin="VDD@1" pad="38"/>
<connect gate="G$1" pin="VDD@2" pad="57"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="10"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSS@1" pad="25"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="VSS@3" pad="56"/>
<connect gate="G$1" pin="VUSB" pad="17"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F66J55-I/PT"/>
<attribute name="OC_FARNELL" value="1439556"/>
<attribute name="OC_NEWARK" value="17M0968"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F8*J5" prefix="IC">
<description>&lt;b&gt;PIC18F87J50 Family&lt;/b&gt;&lt;p&gt;
64/80-Pin High-Performance, 1-Mbit Flash USB Microcontrollers with nanoWatt Technology&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39775b.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F8XJ5X"/>
</gates>
<devices>
<device name="0" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ENVREG" pad="24"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="49"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="50"/>
<connect gate="G$1" pin="RA0/AN0" pad="30"/>
<connect gate="G$1" pin="RA1/AN1" pad="29"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="28"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="27"/>
<connect gate="G$1" pin="RA4/PMD5/T0CKI" pad="34"/>
<connect gate="G$1" pin="RA5/PMD4/AN4/C2INA" pad="33"/>
<connect gate="G$1" pin="RB0/FLT0/INT0" pad="58"/>
<connect gate="G$1" pin="RB1/INT1/PMA4" pad="57"/>
<connect gate="G$1" pin="RB2/INT2/PMA3" pad="56"/>
<connect gate="G$1" pin="RB3/INT3/ECCP2/P2A/PMA2" pad="55"/>
<connect gate="G$1" pin="RB4/KBI0/PMA1" pad="54"/>
<connect gate="G$1" pin="RB5/KBI1/PMA0" pad="53"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="52"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="47"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="36"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="43"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="44"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="45"/>
<connect gate="G$1" pin="RC5/SDO1/C2OUT" pad="46"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="37"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="38"/>
<connect gate="G$1" pin="RD0/AD0/PMD0" pad="72"/>
<connect gate="G$1" pin="RD1/AD1/PMD1" pad="69"/>
<connect gate="G$1" pin="RD2/AD2/PMD2" pad="68"/>
<connect gate="G$1" pin="RD3/AD3/PMD3" pad="67"/>
<connect gate="G$1" pin="RD4/AD4/PMD4/SDO2" pad="66"/>
<connect gate="G$1" pin="RD5/AD5/PMD5/SDI2/SDA2" pad="65"/>
<connect gate="G$1" pin="RD6/AD6/PMD6/SCK2/SCL2" pad="64"/>
<connect gate="G$1" pin="RD7/AD7/PMD7/!SS2" pad="63"/>
<connect gate="G$1" pin="RE0/AD8/PMRD/P2D" pad="4"/>
<connect gate="G$1" pin="RE1/AD9/PMWR/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/AD10/PMBE/P2B" pad="78"/>
<connect gate="G$1" pin="RE3/AD11/PMA13/P3C/REFO" pad="77"/>
<connect gate="G$1" pin="RE4/AD12/PMA12/P3B" pad="76"/>
<connect gate="G$1" pin="RE5/AD13/PMA11/P1C" pad="75"/>
<connect gate="G$1" pin="RE6/AD14/PMA10/P1B" pad="74"/>
<connect gate="G$1" pin="RE7/AD15/PMA9/ECCP2/P2A" pad="73"/>
<connect gate="G$1" pin="RF2/PMA5/AN7/C2INB" pad="18"/>
<connect gate="G$1" pin="RF3/D-" pad="17"/>
<connect gate="G$1" pin="RF4/D+" pad="16"/>
<connect gate="G$1" pin="RF5/PMD2/AN10/C1INB/CVREF" pad="15"/>
<connect gate="G$1" pin="RF6/PMD1/AN11/C1INA" pad="14"/>
<connect gate="G$1" pin="RF7/PMD0/!SS1!/C1OUT" pad="13"/>
<connect gate="G$1" pin="RG0/PMA8/ECCP3/P3A" pad="5"/>
<connect gate="G$1" pin="RG1/PMA7/TX2/CK2" pad="6"/>
<connect gate="G$1" pin="RG2/PMA6/RX2/DT2" pad="7"/>
<connect gate="G$1" pin="RG3/PMCS1/CCP4/P3D" pad="8"/>
<connect gate="G$1" pin="RG4/PMCS2/CCP5/P1D" pad="10"/>
<connect gate="G$1" pin="RH0/A16" pad="79"/>
<connect gate="G$1" pin="RH1/A17" pad="80"/>
<connect gate="G$1" pin="RH2/A18/PMD7" pad="1"/>
<connect gate="G$1" pin="RH3/A19/PMD6" pad="2"/>
<connect gate="G$1" pin="RH4/PMD3/AN12/P3C/C2INC" pad="22"/>
<connect gate="G$1" pin="RH5/PMBE/AN13/P3B/C2IND" pad="21"/>
<connect gate="G$1" pin="RH6/PMRD/AN14/P1C/C1INC" pad="20"/>
<connect gate="G$1" pin="RH7/PMWR/AN15/P1B" pad="19"/>
<connect gate="G$1" pin="RJ0/ALE" pad="62"/>
<connect gate="G$1" pin="RJ1/!OE" pad="61"/>
<connect gate="G$1" pin="RJ2/!WRL" pad="60"/>
<connect gate="G$1" pin="RJ3/!WRH" pad="59"/>
<connect gate="G$1" pin="RJ4/BA0" pad="39"/>
<connect gate="G$1" pin="RJ5/!CE" pad="40"/>
<connect gate="G$1" pin="RJ6/!LB" pad="41"/>
<connect gate="G$1" pin="RJ7/!UB" pad="42"/>
<connect gate="G$1" pin="VDD" pad="32"/>
<connect gate="G$1" pin="VDD@1" pad="48"/>
<connect gate="G$1" pin="VDD@2" pad="71"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="12"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
<connect gate="G$1" pin="VSS@2" pad="51"/>
<connect gate="G$1" pin="VSS@3" pad="70"/>
<connect gate="G$1" pin="VUSB" pad="23"/>
</connects>
<technologies>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F85J50-I/PT"/>
<attribute name="OC_FARNELL" value="1439565"/>
<attribute name="OC_NEWARK" value="59M1134"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F86J50-I/PT"/>
<attribute name="OC_FARNELL" value="1439569"/>
<attribute name="OC_NEWARK" value="59M1137"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F87J50-I/PT"/>
<attribute name="OC_FARNELL" value="1439572"/>
<attribute name="OC_NEWARK" value="17M0986"/>
</technology>
</technologies>
</device>
<device name="5" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ENVREG" pad="24"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="49"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="50"/>
<connect gate="G$1" pin="RA0/AN0" pad="30"/>
<connect gate="G$1" pin="RA1/AN1" pad="29"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="28"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="27"/>
<connect gate="G$1" pin="RA4/PMD5/T0CKI" pad="34"/>
<connect gate="G$1" pin="RA5/PMD4/AN4/C2INA" pad="33"/>
<connect gate="G$1" pin="RB0/FLT0/INT0" pad="58"/>
<connect gate="G$1" pin="RB1/INT1/PMA4" pad="57"/>
<connect gate="G$1" pin="RB2/INT2/PMA3" pad="56"/>
<connect gate="G$1" pin="RB3/INT3/ECCP2/P2A/PMA2" pad="55"/>
<connect gate="G$1" pin="RB4/KBI0/PMA1" pad="54"/>
<connect gate="G$1" pin="RB5/KBI1/PMA0" pad="53"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="52"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="47"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="36"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="43"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="44"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="45"/>
<connect gate="G$1" pin="RC5/SDO1/C2OUT" pad="46"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="37"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="38"/>
<connect gate="G$1" pin="RD0/AD0/PMD0" pad="72"/>
<connect gate="G$1" pin="RD1/AD1/PMD1" pad="69"/>
<connect gate="G$1" pin="RD2/AD2/PMD2" pad="68"/>
<connect gate="G$1" pin="RD3/AD3/PMD3" pad="67"/>
<connect gate="G$1" pin="RD4/AD4/PMD4/SDO2" pad="66"/>
<connect gate="G$1" pin="RD5/AD5/PMD5/SDI2/SDA2" pad="65"/>
<connect gate="G$1" pin="RD6/AD6/PMD6/SCK2/SCL2" pad="64"/>
<connect gate="G$1" pin="RD7/AD7/PMD7/!SS2" pad="63"/>
<connect gate="G$1" pin="RE0/AD8/PMRD/P2D" pad="4"/>
<connect gate="G$1" pin="RE1/AD9/PMWR/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/AD10/PMBE/P2B" pad="78"/>
<connect gate="G$1" pin="RE3/AD11/PMA13/P3C/REFO" pad="77"/>
<connect gate="G$1" pin="RE4/AD12/PMA12/P3B" pad="76"/>
<connect gate="G$1" pin="RE5/AD13/PMA11/P1C" pad="75"/>
<connect gate="G$1" pin="RE6/AD14/PMA10/P1B" pad="74"/>
<connect gate="G$1" pin="RE7/AD15/PMA9/ECCP2/P2A" pad="73"/>
<connect gate="G$1" pin="RF2/PMA5/AN7/C2INB" pad="18"/>
<connect gate="G$1" pin="RF3/D-" pad="17"/>
<connect gate="G$1" pin="RF4/D+" pad="16"/>
<connect gate="G$1" pin="RF5/PMD2/AN10/C1INB/CVREF" pad="15"/>
<connect gate="G$1" pin="RF6/PMD1/AN11/C1INA" pad="14"/>
<connect gate="G$1" pin="RF7/PMD0/!SS1!/C1OUT" pad="13"/>
<connect gate="G$1" pin="RG0/PMA8/ECCP3/P3A" pad="5"/>
<connect gate="G$1" pin="RG1/PMA7/TX2/CK2" pad="6"/>
<connect gate="G$1" pin="RG2/PMA6/RX2/DT2" pad="7"/>
<connect gate="G$1" pin="RG3/PMCS1/CCP4/P3D" pad="8"/>
<connect gate="G$1" pin="RG4/PMCS2/CCP5/P1D" pad="10"/>
<connect gate="G$1" pin="RH0/A16" pad="79"/>
<connect gate="G$1" pin="RH1/A17" pad="80"/>
<connect gate="G$1" pin="RH2/A18/PMD7" pad="1"/>
<connect gate="G$1" pin="RH3/A19/PMD6" pad="2"/>
<connect gate="G$1" pin="RH4/PMD3/AN12/P3C/C2INC" pad="22"/>
<connect gate="G$1" pin="RH5/PMBE/AN13/P3B/C2IND" pad="21"/>
<connect gate="G$1" pin="RH6/PMRD/AN14/P1C/C1INC" pad="20"/>
<connect gate="G$1" pin="RH7/PMWR/AN15/P1B" pad="19"/>
<connect gate="G$1" pin="RJ0/ALE" pad="62"/>
<connect gate="G$1" pin="RJ1/!OE" pad="61"/>
<connect gate="G$1" pin="RJ2/!WRL" pad="60"/>
<connect gate="G$1" pin="RJ3/!WRH" pad="59"/>
<connect gate="G$1" pin="RJ4/BA0" pad="39"/>
<connect gate="G$1" pin="RJ5/!CE" pad="40"/>
<connect gate="G$1" pin="RJ6/!LB" pad="41"/>
<connect gate="G$1" pin="RJ7/!UB" pad="42"/>
<connect gate="G$1" pin="VDD" pad="32"/>
<connect gate="G$1" pin="VDD@1" pad="48"/>
<connect gate="G$1" pin="VDD@2" pad="71"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="12"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
<connect gate="G$1" pin="VSS@2" pad="51"/>
<connect gate="G$1" pin="VSS@3" pad="70"/>
<connect gate="G$1" pin="VUSB" pad="23"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F86J55-I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="17M0982"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F6*J6" prefix="IC">
<description>&lt;b&gt;PIC18F97J60 Family&lt;/b&gt;&lt;p&gt;
64/80/100-Pin High-Performance, 1-Mbit Flash Microcontrollers with Ethernet&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39762d.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F6XJ6X"/>
</gates>
<devices>
<device name="0" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="ENVREG" pad="18"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="39"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="40"/>
<connect gate="G$1" pin="RA0/LEDA/AN0" pad="24"/>
<connect gate="G$1" pin="RA1/LEDB/AN1" pad="23"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="22"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="21"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="28"/>
<connect gate="G$1" pin="RA5/AN4" pad="27"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="3"/>
<connect gate="G$1" pin="RB1/INT1" pad="4"/>
<connect gate="G$1" pin="RB2/INT2" pad="5"/>
<connect gate="G$1" pin="RB3/INT3" pad="6"/>
<connect gate="G$1" pin="RB4/KBI0" pad="44"/>
<connect gate="G$1" pin="RB5/KBI1" pad="43"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="42"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="37"/>
<connect gate="G$1" pin="RBIAS" pad="53"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="30"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="29"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="33"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="34"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="35"/>
<connect gate="G$1" pin="RC5/SDO1" pad="36"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="31"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="32"/>
<connect gate="G$1" pin="RD0/P1B" pad="60"/>
<connect gate="G$1" pin="RD1/ECCP3/P3A" pad="59"/>
<connect gate="G$1" pin="RD2/CCP4/P3D" pad="58"/>
<connect gate="G$1" pin="RE0/P2D" pad="2"/>
<connect gate="G$1" pin="RE1/P2C" pad="1"/>
<connect gate="G$1" pin="RE2/P2B" pad="64"/>
<connect gate="G$1" pin="RE3/P3C" pad="63"/>
<connect gate="G$1" pin="RE4/P3B" pad="62"/>
<connect gate="G$1" pin="RE5/P1C" pad="61"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="17"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="16"/>
<connect gate="G$1" pin="RF3/AN8" pad="15"/>
<connect gate="G$1" pin="RF4/AN9" pad="14"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="13"/>
<connect gate="G$1" pin="RF6/AN11" pad="12"/>
<connect gate="G$1" pin="RF7/!SS1" pad="11"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="8"/>
<connect gate="G$1" pin="TPIN+" pad="47"/>
<connect gate="G$1" pin="TPIN-" pad="46"/>
<connect gate="G$1" pin="TPOUT+" pad="51"/>
<connect gate="G$1" pin="TPOUT-" pad="50"/>
<connect gate="G$1" pin="VDD" pad="26"/>
<connect gate="G$1" pin="VDD@1" pad="38"/>
<connect gate="G$1" pin="VDD@2" pad="57"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="10"/>
<connect gate="G$1" pin="VDDPLL" pad="54"/>
<connect gate="G$1" pin="VDDRX" pad="48"/>
<connect gate="G$1" pin="VDDTX" pad="49"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSS@1" pad="25"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="VSS@3" pad="56"/>
<connect gate="G$1" pin="VSSPLL" pad="55"/>
<connect gate="G$1" pin="VSSRX" pad="45"/>
<connect gate="G$1" pin="VSSTX" pad="52"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F66J60-I/PT"/>
<attribute name="OC_FARNELL" value="1332282"/>
<attribute name="OC_NEWARK" value="56K7296"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F67J60-I/PT"/>
<attribute name="OC_FARNELL" value="1332285"/>
<attribute name="OC_NEWARK" value="56K7302"/>
</technology>
</technologies>
</device>
<device name="5" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="ENVREG" pad="18"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="39"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="40"/>
<connect gate="G$1" pin="RA0/LEDA/AN0" pad="24"/>
<connect gate="G$1" pin="RA1/LEDB/AN1" pad="23"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="22"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="21"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="28"/>
<connect gate="G$1" pin="RA5/AN4" pad="27"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="3"/>
<connect gate="G$1" pin="RB1/INT1" pad="4"/>
<connect gate="G$1" pin="RB2/INT2" pad="5"/>
<connect gate="G$1" pin="RB3/INT3" pad="6"/>
<connect gate="G$1" pin="RB4/KBI0" pad="44"/>
<connect gate="G$1" pin="RB5/KBI1" pad="43"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="42"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="37"/>
<connect gate="G$1" pin="RBIAS" pad="53"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="30"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="29"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="33"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="34"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="35"/>
<connect gate="G$1" pin="RC5/SDO1" pad="36"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="31"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="32"/>
<connect gate="G$1" pin="RD0/P1B" pad="60"/>
<connect gate="G$1" pin="RD1/ECCP3/P3A" pad="59"/>
<connect gate="G$1" pin="RD2/CCP4/P3D" pad="58"/>
<connect gate="G$1" pin="RE0/P2D" pad="2"/>
<connect gate="G$1" pin="RE1/P2C" pad="1"/>
<connect gate="G$1" pin="RE2/P2B" pad="64"/>
<connect gate="G$1" pin="RE3/P3C" pad="63"/>
<connect gate="G$1" pin="RE4/P3B" pad="62"/>
<connect gate="G$1" pin="RE5/P1C" pad="61"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="17"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="16"/>
<connect gate="G$1" pin="RF3/AN8" pad="15"/>
<connect gate="G$1" pin="RF4/AN9" pad="14"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="13"/>
<connect gate="G$1" pin="RF6/AN11" pad="12"/>
<connect gate="G$1" pin="RF7/!SS1" pad="11"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="8"/>
<connect gate="G$1" pin="TPIN+" pad="47"/>
<connect gate="G$1" pin="TPIN-" pad="46"/>
<connect gate="G$1" pin="TPOUT+" pad="51"/>
<connect gate="G$1" pin="TPOUT-" pad="50"/>
<connect gate="G$1" pin="VDD" pad="26"/>
<connect gate="G$1" pin="VDD@1" pad="38"/>
<connect gate="G$1" pin="VDD@2" pad="57"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="10"/>
<connect gate="G$1" pin="VDDPLL" pad="54"/>
<connect gate="G$1" pin="VDDRX" pad="48"/>
<connect gate="G$1" pin="VDDTX" pad="49"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSS@1" pad="25"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="VSS@3" pad="56"/>
<connect gate="G$1" pin="VSSPLL" pad="55"/>
<connect gate="G$1" pin="VSSRX" pad="45"/>
<connect gate="G$1" pin="VSSTX" pad="52"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F66J65-I/PT"/>
<attribute name="OC_FARNELL" value="1579612"/>
<attribute name="OC_NEWARK" value="56K7298"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F8*J6" prefix="IC">
<description>&lt;b&gt;PIC18F97J60 Family&lt;/b&gt;&lt;p&gt;
64/80/100-Pin High-Performance, 1-Mbit Flash Microcontrollers with Ethernet&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39762d.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F8XJ6X"/>
</gates>
<devices>
<device name="0" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ENVREG" pad="24"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="49"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="50"/>
<connect gate="G$1" pin="RA0/LEDA/AN0" pad="30"/>
<connect gate="G$1" pin="RA1/LEDB/AN1" pad="29"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="28"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="27"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="34"/>
<connect gate="G$1" pin="RA5/AN4" pad="33"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="5"/>
<connect gate="G$1" pin="RB1/INT1" pad="6"/>
<connect gate="G$1" pin="RB2/INT2" pad="7"/>
<connect gate="G$1" pin="RB3/INT3" pad="8"/>
<connect gate="G$1" pin="RB4/KBI0" pad="54"/>
<connect gate="G$1" pin="RB5/KBI1" pad="53"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="52"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="47"/>
<connect gate="G$1" pin="RBIAS" pad="65"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="36"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="43"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="44"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="45"/>
<connect gate="G$1" pin="RC5/SDO1" pad="46"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="37"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="38"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="69"/>
<connect gate="G$1" pin="RD2" pad="68"/>
<connect gate="G$1" pin="RE0/P2D" pad="4"/>
<connect gate="G$1" pin="RE1/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/P2B" pad="78"/>
<connect gate="G$1" pin="RE3/P3C" pad="77"/>
<connect gate="G$1" pin="RE4/P3B" pad="76"/>
<connect gate="G$1" pin="RE5/P1C" pad="75"/>
<connect gate="G$1" pin="RE6/P1B" pad="74"/>
<connect gate="G$1" pin="RE7/ECCP2/P2A" pad="73"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="23"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="18"/>
<connect gate="G$1" pin="RF3/AN8" pad="17"/>
<connect gate="G$1" pin="RF4/AN9" pad="16"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="15"/>
<connect gate="G$1" pin="RF6/AN11" pad="14"/>
<connect gate="G$1" pin="RF7/!SS1" pad="13"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="56"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="55"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="42"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="41"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="10"/>
<connect gate="G$1" pin="RH0" pad="79"/>
<connect gate="G$1" pin="RH1" pad="80"/>
<connect gate="G$1" pin="RH2" pad="1"/>
<connect gate="G$1" pin="RH3" pad="2"/>
<connect gate="G$1" pin="RH4/AN12/P3C" pad="22"/>
<connect gate="G$1" pin="RH5/AN13/P3B" pad="21"/>
<connect gate="G$1" pin="RH6/AN14/P1C" pad="20"/>
<connect gate="G$1" pin="RH7/AN15/P1B" pad="19"/>
<connect gate="G$1" pin="RJ4" pad="40"/>
<connect gate="G$1" pin="RJ5" pad="39"/>
<connect gate="G$1" pin="TPIN+" pad="59"/>
<connect gate="G$1" pin="TPIN-" pad="58"/>
<connect gate="G$1" pin="TPOUT+" pad="63"/>
<connect gate="G$1" pin="TPOUT-" pad="62"/>
<connect gate="G$1" pin="VDD" pad="32"/>
<connect gate="G$1" pin="VDD@1" pad="48"/>
<connect gate="G$1" pin="VDD@2" pad="71"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="12"/>
<connect gate="G$1" pin="VDDPLL" pad="66"/>
<connect gate="G$1" pin="VDDRX" pad="60"/>
<connect gate="G$1" pin="VDDTX" pad="61"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
<connect gate="G$1" pin="VSS@2" pad="51"/>
<connect gate="G$1" pin="VSS@3" pad="70"/>
<connect gate="G$1" pin="VSSPLL" pad="67"/>
<connect gate="G$1" pin="VSSRX" pad="57"/>
<connect gate="G$1" pin="VSSTX" pad="64"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F86J60-I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="56K7306"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F87J60-I/PT"/>
<attribute name="OC_FARNELL" value="1332291"/>
<attribute name="OC_NEWARK" value="56K7312"/>
</technology>
</technologies>
</device>
<device name="5" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ENVREG" pad="24"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="49"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="50"/>
<connect gate="G$1" pin="RA0/LEDA/AN0" pad="30"/>
<connect gate="G$1" pin="RA1/LEDB/AN1" pad="29"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="28"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="27"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="34"/>
<connect gate="G$1" pin="RA5/AN4" pad="33"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="5"/>
<connect gate="G$1" pin="RB1/INT1" pad="6"/>
<connect gate="G$1" pin="RB2/INT2" pad="7"/>
<connect gate="G$1" pin="RB3/INT3" pad="8"/>
<connect gate="G$1" pin="RB4/KBI0" pad="54"/>
<connect gate="G$1" pin="RB5/KBI1" pad="53"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="52"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="47"/>
<connect gate="G$1" pin="RBIAS" pad="65"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="36"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="43"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="44"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="45"/>
<connect gate="G$1" pin="RC5/SDO1" pad="46"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="37"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="38"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="69"/>
<connect gate="G$1" pin="RD2" pad="68"/>
<connect gate="G$1" pin="RE0/P2D" pad="4"/>
<connect gate="G$1" pin="RE1/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/P2B" pad="78"/>
<connect gate="G$1" pin="RE3/P3C" pad="77"/>
<connect gate="G$1" pin="RE4/P3B" pad="76"/>
<connect gate="G$1" pin="RE5/P1C" pad="75"/>
<connect gate="G$1" pin="RE6/P1B" pad="74"/>
<connect gate="G$1" pin="RE7/ECCP2/P2A" pad="73"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="23"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="18"/>
<connect gate="G$1" pin="RF3/AN8" pad="17"/>
<connect gate="G$1" pin="RF4/AN9" pad="16"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="15"/>
<connect gate="G$1" pin="RF6/AN11" pad="14"/>
<connect gate="G$1" pin="RF7/!SS1" pad="13"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="56"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="55"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="42"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="41"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="10"/>
<connect gate="G$1" pin="RH0" pad="79"/>
<connect gate="G$1" pin="RH1" pad="80"/>
<connect gate="G$1" pin="RH2" pad="1"/>
<connect gate="G$1" pin="RH3" pad="2"/>
<connect gate="G$1" pin="RH4/AN12/P3C" pad="22"/>
<connect gate="G$1" pin="RH5/AN13/P3B" pad="21"/>
<connect gate="G$1" pin="RH6/AN14/P1C" pad="20"/>
<connect gate="G$1" pin="RH7/AN15/P1B" pad="19"/>
<connect gate="G$1" pin="RJ4" pad="40"/>
<connect gate="G$1" pin="RJ5" pad="39"/>
<connect gate="G$1" pin="TPIN+" pad="59"/>
<connect gate="G$1" pin="TPIN-" pad="58"/>
<connect gate="G$1" pin="TPOUT+" pad="63"/>
<connect gate="G$1" pin="TPOUT-" pad="62"/>
<connect gate="G$1" pin="VDD" pad="32"/>
<connect gate="G$1" pin="VDD@1" pad="48"/>
<connect gate="G$1" pin="VDD@2" pad="71"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="12"/>
<connect gate="G$1" pin="VDDPLL" pad="66"/>
<connect gate="G$1" pin="VDDRX" pad="60"/>
<connect gate="G$1" pin="VDDTX" pad="61"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
<connect gate="G$1" pin="VSS@2" pad="51"/>
<connect gate="G$1" pin="VSS@3" pad="70"/>
<connect gate="G$1" pin="VSSPLL" pad="67"/>
<connect gate="G$1" pin="VSSRX" pad="57"/>
<connect gate="G$1" pin="VSSTX" pad="64"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F86J65-I/PT"/>
<attribute name="OC_FARNELL" value="1564571"/>
<attribute name="OC_NEWARK" value="95M7065"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F9*J6" prefix="IC">
<description>&lt;b&gt;PIC18F97J60 Family&lt;/b&gt;&lt;p&gt;
64/80/100-Pin High-Performance, 1-Mbit Flash Microcontrollers with Ethernet&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39762d.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F9XJ6"/>
</gates>
<devices>
<device name="0" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="D7/AD7/PSP7/!SS2" pad="83"/>
<connect gate="G$1" pin="ENVREG" pad="29"/>
<connect gate="G$1" pin="NC" pad="9"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="63"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="64"/>
<connect gate="G$1" pin="RA0/LEDA/AN0" pad="35"/>
<connect gate="G$1" pin="RA1/LEDB/AN1" pad="34"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="33"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="32"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="42"/>
<connect gate="G$1" pin="RA5/AN4" pad="41"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="5"/>
<connect gate="G$1" pin="RB1/INT1" pad="6"/>
<connect gate="G$1" pin="RB2/INT2" pad="7"/>
<connect gate="G$1" pin="RB3/INT3/ECCP2/P2A" pad="8"/>
<connect gate="G$1" pin="RB4/KBI0" pad="69"/>
<connect gate="G$1" pin="RB5/KBI1" pad="68"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="67"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="57"/>
<connect gate="G$1" pin="RBIAS" pad="80"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="44"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="43"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="53"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="54"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="55"/>
<connect gate="G$1" pin="RC5/SDO1" pad="56"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="45"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="46"/>
<connect gate="G$1" pin="RD0/AD0/PSP0" pad="92"/>
<connect gate="G$1" pin="RD1/AD1/PSP1" pad="91"/>
<connect gate="G$1" pin="RD2/AD2/PSP2" pad="90"/>
<connect gate="G$1" pin="RD3/AD3/PSP3" pad="89"/>
<connect gate="G$1" pin="RD4/AD4/PSP4/SDO2/SD" pad="88"/>
<connect gate="G$1" pin="RD5/AD5/PSP5/SDI2/SDA2" pad="87"/>
<connect gate="G$1" pin="RD6/AD6/PSP6/SCK2/SCL2" pad="84"/>
<connect gate="G$1" pin="RE0/AD8/!RD!/P2D/T" pad="4"/>
<connect gate="G$1" pin="RE1/AD9/!WR!/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/AD10/!CS!/P2B" pad="98"/>
<connect gate="G$1" pin="RE3/AD11/P3C" pad="97"/>
<connect gate="G$1" pin="RE4/AD12/P3B" pad="96"/>
<connect gate="G$1" pin="RE5/AD13/P1C" pad="95"/>
<connect gate="G$1" pin="RE6/AD14/P1B" pad="94"/>
<connect gate="G$1" pin="RE7/AD15/ECCP2/P2A" pad="93"/>
<connect gate="G$1" pin="RF0/AN5" pad="12"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="28"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="23"/>
<connect gate="G$1" pin="RF3/AN8" pad="22"/>
<connect gate="G$1" pin="RF4/AN9" pad="21"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="20"/>
<connect gate="G$1" pin="RF6/AN11" pad="19"/>
<connect gate="G$1" pin="RF7/!SS1" pad="18"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="71"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="70"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="52"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="51"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="14"/>
<connect gate="G$1" pin="RG5" pad="11"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="38"/>
<connect gate="G$1" pin="RH0/A16" pad="99"/>
<connect gate="G$1" pin="RH1/A17" pad="100"/>
<connect gate="G$1" pin="RH2/A18" pad="1"/>
<connect gate="G$1" pin="RH3/A19" pad="2"/>
<connect gate="G$1" pin="RH4/AN12/P3C" pad="27"/>
<connect gate="G$1" pin="RH5/AN13/P3B" pad="26"/>
<connect gate="G$1" pin="RH6/AN14/P1C" pad="25"/>
<connect gate="G$1" pin="RH7/AN15/P1B" pad="24"/>
<connect gate="G$1" pin="RJ0/ALE" pad="49"/>
<connect gate="G$1" pin="RJ1/!OE" pad="50"/>
<connect gate="G$1" pin="RJ2/!WRL" pad="66"/>
<connect gate="G$1" pin="RJ3/!WRH" pad="61"/>
<connect gate="G$1" pin="RJ4/BA0" pad="47"/>
<connect gate="G$1" pin="RJ5/!CE" pad="48"/>
<connect gate="G$1" pin="RJ6/!LB" pad="58"/>
<connect gate="G$1" pin="RJ7/!UB" pad="39"/>
<connect gate="G$1" pin="TPIN+" pad="74"/>
<connect gate="G$1" pin="TPIN-" pad="73"/>
<connect gate="G$1" pin="TPOUT+" pad="78"/>
<connect gate="G$1" pin="TPOUT-" pad="77"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VDD@1" pad="37"/>
<connect gate="G$1" pin="VDD@2" pad="59"/>
<connect gate="G$1" pin="VDD@3" pad="62"/>
<connect gate="G$1" pin="VDD@4" pad="86"/>
<connect gate="G$1" pin="VDDCORE/VCAP3" pad="16"/>
<connect gate="G$1" pin="VDDPLL" pad="81"/>
<connect gate="G$1" pin="VDDRX" pad="75"/>
<connect gate="G$1" pin="VDDTX" pad="76"/>
<connect gate="G$1" pin="VSS" pad="15"/>
<connect gate="G$1" pin="VSS@1" pad="36"/>
<connect gate="G$1" pin="VSS@2" pad="40"/>
<connect gate="G$1" pin="VSS@3" pad="60"/>
<connect gate="G$1" pin="VSS@4" pad="65"/>
<connect gate="G$1" pin="VSS@5" pad="85"/>
<connect gate="G$1" pin="VSSPLL" pad="82"/>
<connect gate="G$1" pin="VSSRX" pad="72"/>
<connect gate="G$1" pin="VSSTX" pad="79"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F96J60-I/PT"/>
<attribute name="OC_FARNELL" value="1332292"/>
<attribute name="OC_NEWARK" value="56K7316"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F97J60-I/PT"/>
<attribute name="OC_FARNELL" value="1439573"/>
<attribute name="OC_NEWARK" value="56K7318"/>
</technology>
</technologies>
</device>
<device name="5" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="D7/AD7/PSP7/!SS2" pad="83"/>
<connect gate="G$1" pin="ENVREG" pad="29"/>
<connect gate="G$1" pin="NC" pad="9"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="63"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="64"/>
<connect gate="G$1" pin="RA0/LEDA/AN0" pad="35"/>
<connect gate="G$1" pin="RA1/LEDB/AN1" pad="34"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="33"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="32"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="42"/>
<connect gate="G$1" pin="RA5/AN4" pad="41"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="5"/>
<connect gate="G$1" pin="RB1/INT1" pad="6"/>
<connect gate="G$1" pin="RB2/INT2" pad="7"/>
<connect gate="G$1" pin="RB3/INT3/ECCP2/P2A" pad="8"/>
<connect gate="G$1" pin="RB4/KBI0" pad="69"/>
<connect gate="G$1" pin="RB5/KBI1" pad="68"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="67"/>
<connect gate="G$1" pin="RB7/KBI3/PGD" pad="57"/>
<connect gate="G$1" pin="RBIAS" pad="80"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="44"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="43"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="53"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="54"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="55"/>
<connect gate="G$1" pin="RC5/SDO1" pad="56"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="45"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="46"/>
<connect gate="G$1" pin="RD0/AD0/PSP0" pad="92"/>
<connect gate="G$1" pin="RD1/AD1/PSP1" pad="91"/>
<connect gate="G$1" pin="RD2/AD2/PSP2" pad="90"/>
<connect gate="G$1" pin="RD3/AD3/PSP3" pad="89"/>
<connect gate="G$1" pin="RD4/AD4/PSP4/SDO2/SD" pad="88"/>
<connect gate="G$1" pin="RD5/AD5/PSP5/SDI2/SDA2" pad="87"/>
<connect gate="G$1" pin="RD6/AD6/PSP6/SCK2/SCL2" pad="84"/>
<connect gate="G$1" pin="RE0/AD8/!RD!/P2D/T" pad="4"/>
<connect gate="G$1" pin="RE1/AD9/!WR!/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/AD10/!CS!/P2B" pad="98"/>
<connect gate="G$1" pin="RE3/AD11/P3C" pad="97"/>
<connect gate="G$1" pin="RE4/AD12/P3B" pad="96"/>
<connect gate="G$1" pin="RE5/AD13/P1C" pad="95"/>
<connect gate="G$1" pin="RE6/AD14/P1B" pad="94"/>
<connect gate="G$1" pin="RE7/AD15/ECCP2/P2A" pad="93"/>
<connect gate="G$1" pin="RF0/AN5" pad="12"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="28"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="23"/>
<connect gate="G$1" pin="RF3/AN8" pad="22"/>
<connect gate="G$1" pin="RF4/AN9" pad="21"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="20"/>
<connect gate="G$1" pin="RF6/AN11" pad="19"/>
<connect gate="G$1" pin="RF7/!SS1" pad="18"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="71"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="70"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="52"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="51"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="14"/>
<connect gate="G$1" pin="RG5" pad="11"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="38"/>
<connect gate="G$1" pin="RH0/A16" pad="99"/>
<connect gate="G$1" pin="RH1/A17" pad="100"/>
<connect gate="G$1" pin="RH2/A18" pad="1"/>
<connect gate="G$1" pin="RH3/A19" pad="2"/>
<connect gate="G$1" pin="RH4/AN12/P3C" pad="27"/>
<connect gate="G$1" pin="RH5/AN13/P3B" pad="26"/>
<connect gate="G$1" pin="RH6/AN14/P1C" pad="25"/>
<connect gate="G$1" pin="RH7/AN15/P1B" pad="24"/>
<connect gate="G$1" pin="RJ0/ALE" pad="49"/>
<connect gate="G$1" pin="RJ1/!OE" pad="50"/>
<connect gate="G$1" pin="RJ2/!WRL" pad="66"/>
<connect gate="G$1" pin="RJ3/!WRH" pad="61"/>
<connect gate="G$1" pin="RJ4/BA0" pad="47"/>
<connect gate="G$1" pin="RJ5/!CE" pad="48"/>
<connect gate="G$1" pin="RJ6/!LB" pad="58"/>
<connect gate="G$1" pin="RJ7/!UB" pad="39"/>
<connect gate="G$1" pin="TPIN+" pad="74"/>
<connect gate="G$1" pin="TPIN-" pad="73"/>
<connect gate="G$1" pin="TPOUT+" pad="78"/>
<connect gate="G$1" pin="TPOUT-" pad="77"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VDD@1" pad="37"/>
<connect gate="G$1" pin="VDD@2" pad="59"/>
<connect gate="G$1" pin="VDD@3" pad="62"/>
<connect gate="G$1" pin="VDD@4" pad="86"/>
<connect gate="G$1" pin="VDDCORE/VCAP3" pad="16"/>
<connect gate="G$1" pin="VDDPLL" pad="81"/>
<connect gate="G$1" pin="VDDRX" pad="75"/>
<connect gate="G$1" pin="VDDTX" pad="76"/>
<connect gate="G$1" pin="VSS" pad="15"/>
<connect gate="G$1" pin="VSS@1" pad="36"/>
<connect gate="G$1" pin="VSS@2" pad="40"/>
<connect gate="G$1" pin="VSS@3" pad="60"/>
<connect gate="G$1" pin="VSS@4" pad="65"/>
<connect gate="G$1" pin="VSS@5" pad="85"/>
<connect gate="G$1" pin="VSSPLL" pad="82"/>
<connect gate="G$1" pin="VSSRX" pad="72"/>
<connect gate="G$1" pin="VSSTX" pad="79"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F96J65-I/PT"/>
<attribute name="OC_FARNELL" value="1564573"/>
<attribute name="OC_NEWARK" value="56K7317"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC12F683" prefix="IC">
<description>&lt;b&gt;8-Pin Flash-Based, 8-Bit CMOS Microcontrollers with nanoWatt Technology&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41211D_.pdf</description>
<gates>
<gate name="G$1" symbol="PIC12F683"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="GP0/AN0/CIN+/ICSPDAT/ULPWU" pad="7"/>
<connect gate="G$1" pin="GP1/AN1/CIN-/VREF/ICSPCLK" pad="6"/>
<connect gate="G$1" pin="GP2/AN2/T0CKI/INT/COUT/CCP1" pad="5"/>
<connect gate="G$1" pin="GP3/!MCLR!/VPP" pad="4"/>
<connect gate="G$1" pin="GP4/AN3/T1G/OSC2/CLKOUT" pad="3"/>
<connect gate="G$1" pin="GP5/T1CKI/OSC1/CLKIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F683-I/P"/>
<attribute name="OC_FARNELL" value="9759034"/>
<attribute name="OC_NEWARK" value="89H0442"/>
</technology>
</technologies>
</device>
<device name="DS" package="DFN-S">
<connects>
<connect gate="G$1" pin="GP0/AN0/CIN+/ICSPDAT/ULPWU" pad="7"/>
<connect gate="G$1" pin="GP1/AN1/CIN-/VREF/ICSPCLK" pad="6"/>
<connect gate="G$1" pin="GP2/AN2/T0CKI/INT/COUT/CCP1" pad="5"/>
<connect gate="G$1" pin="GP3/!MCLR!/VPP" pad="4"/>
<connect gate="G$1" pin="GP4/AN3/T1G/OSC2/CLKOUT" pad="3"/>
<connect gate="G$1" pin="GP5/T1CKI/OSC1/CLKIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F683-I/MF"/>
<attribute name="OC_FARNELL" value="1137331"/>
<attribute name="OC_NEWARK" value="89H0441"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="GP0/AN0/CIN+/ICSPDAT/ULPWU" pad="7"/>
<connect gate="G$1" pin="GP1/AN1/CIN-/VREF/ICSPCLK" pad="6"/>
<connect gate="G$1" pin="GP2/AN2/T0CKI/INT/COUT/CCP1" pad="5"/>
<connect gate="G$1" pin="GP3/!MCLR!/VPP" pad="4"/>
<connect gate="G$1" pin="GP4/AN3/T1G/OSC2/CLKOUT" pad="3"/>
<connect gate="G$1" pin="GP5/T1CKI/OSC1/CLKIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F683-I/SN"/>
<attribute name="OC_FARNELL" value="9759042"/>
<attribute name="OC_NEWARK" value="61K3434"/>
</technology>
</technologies>
</device>
<device name="MD" package="DFN8-4X4">
<connects>
<connect gate="G$1" pin="GP0/AN0/CIN+/ICSPDAT/ULPWU" pad="7"/>
<connect gate="G$1" pin="GP1/AN1/CIN-/VREF/ICSPCLK" pad="6"/>
<connect gate="G$1" pin="GP2/AN2/T0CKI/INT/COUT/CCP1" pad="5"/>
<connect gate="G$1" pin="GP3/!MCLR!/VPP" pad="4"/>
<connect gate="G$1" pin="GP4/AN3/T1G/OSC2/CLKOUT" pad="3"/>
<connect gate="G$1" pin="GP5/T1CKI/OSC1/CLKIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC12F683-I/MD"/>
<attribute name="OC_FARNELL" value="4057368"/>
<attribute name="OC_NEWARK" value="56K7230"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP355*" prefix="IC">
<description>&lt;b&gt;Low-Power, Single-Channel 22-Bit Delta-Sigma ADCs&lt;br&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21950c.pdf</description>
<gates>
<gate name="-1" symbol="MCP3550"/>
</gates>
<devices>
<device name="MS" package="MSOP8">
<connects>
<connect gate="-1" pin="!CS" pad="7"/>
<connect gate="-1" pin="SCK" pad="5"/>
<connect gate="-1" pin="SDO/!RDY" pad="6"/>
<connect gate="-1" pin="VDD" pad="8"/>
<connect gate="-1" pin="VIN+" pad="2"/>
<connect gate="-1" pin="VIN-" pad="3"/>
<connect gate="-1" pin="VREF" pad="1"/>
<connect gate="-1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="0-50">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3550-50E/MS"/>
<attribute name="OC_FARNELL" value="1627198"/>
<attribute name="OC_NEWARK" value="69K0130"/>
</technology>
<technology name="0-60">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3550-60E/MS"/>
<attribute name="OC_FARNELL" value="1840933"/>
<attribute name="OC_NEWARK" value="69K0134"/>
</technology>
<technology name="1">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3551-E/MS"/>
<attribute name="OC_FARNELL" value="1084624"/>
<attribute name="OC_NEWARK" value="22K1368"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCP3553-E/MS"/>
<attribute name="OC_FARNELL" value="1439515"/>
<attribute name="OC_NEWARK" value="56K7003"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="-1" pin="!CS" pad="7"/>
<connect gate="-1" pin="SCK" pad="5"/>
<connect gate="-1" pin="SDO/!RDY" pad="6"/>
<connect gate="-1" pin="VDD" pad="8"/>
<connect gate="-1" pin="VIN+" pad="2"/>
<connect gate="-1" pin="VIN-" pad="3"/>
<connect gate="-1" pin="VREF" pad="1"/>
<connect gate="-1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="0-50">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3550-50-E/SN"/>
<attribute name="OC_FARNELL" value="1557411"/>
<attribute name="OC_NEWARK" value="69K0131"/>
</technology>
<technology name="0-60">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3550-60E/SN"/>
<attribute name="OC_FARNELL" value="1840934"/>
<attribute name="OC_NEWARK" value="69K0135"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCP3551-E/SN"/>
<attribute name="OC_FARNELL" value="1084625"/>
<attribute name="OC_NEWARK" value="97K4494"/>
</technology>
<technology name="3">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3553-E/SN"/>
<attribute name="OC_FARNELL" value="1605569"/>
<attribute name="OC_NEWARK" value="56K7004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENC28J60" prefix="IC">
<description>&lt;b&gt;Stand-Alone Ethernet Controller with SPI Interface&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39662c.pdf</description>
<gates>
<gate name="G$1" symbol="ENC28J60"/>
</gates>
<devices>
<device name="SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!CS" pad="9"/>
<connect gate="G$1" pin="!INT" pad="4"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="CLKOUT" pad="3"/>
<connect gate="G$1" pin="LEDA" pad="27"/>
<connect gate="G$1" pin="LEDB" pad="26"/>
<connect gate="G$1" pin="NC*" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="23"/>
<connect gate="G$1" pin="OSC2" pad="24"/>
<connect gate="G$1" pin="RBIAS" pad="14"/>
<connect gate="G$1" pin="SCK" pad="8"/>
<connect gate="G$1" pin="SI" pad="7"/>
<connect gate="G$1" pin="SO" pad="6"/>
<connect gate="G$1" pin="TPIN+" pad="13"/>
<connect gate="G$1" pin="TPIN-" pad="12"/>
<connect gate="G$1" pin="TPOUT+" pad="17"/>
<connect gate="G$1" pin="TPOUT-" pad="16"/>
<connect gate="G$1" pin="VCAP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VDDOSC" pad="25"/>
<connect gate="G$1" pin="VDDPLL" pad="20"/>
<connect gate="G$1" pin="VDDRX" pad="19"/>
<connect gate="G$1" pin="VDDTX" pad="15"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="VSSOSC" pad="22"/>
<connect gate="G$1" pin="VSSPLL" pad="21"/>
<connect gate="G$1" pin="VSSRX" pad="11"/>
<connect gate="G$1" pin="VSSTX" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="ENC28J60/SP"/>
<attribute name="OC_FARNELL" value="1084619"/>
<attribute name="OC_NEWARK" value="96K3661"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP3202" prefix="IC">
<description>&lt;b&gt;2.7V Dual Channel 12-Bit A/D Converter with SPI Serial Interface&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21034D.pdf</description>
<gates>
<gate name="P" symbol="MCP3202"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="P" pin="!CS!/SHDN" pad="1"/>
<connect gate="P" pin="CH0" pad="2"/>
<connect gate="P" pin="CH1" pad="3"/>
<connect gate="P" pin="CLK" pad="7"/>
<connect gate="P" pin="DIN" pad="5"/>
<connect gate="P" pin="DOUT" pad="6"/>
<connect gate="P" pin="VDD/VREF" pad="8"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3202-CI/P"/>
<attribute name="OC_FARNELL" value="1196794"/>
<attribute name="OC_NEWARK" value="72K7287"/>
</technology>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="P" pin="!CS!/SHDN" pad="1"/>
<connect gate="P" pin="CH0" pad="2"/>
<connect gate="P" pin="CH1" pad="3"/>
<connect gate="P" pin="CLK" pad="7"/>
<connect gate="P" pin="DIN" pad="5"/>
<connect gate="P" pin="DOUT" pad="6"/>
<connect gate="P" pin="VDD/VREF" pad="8"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3202-CI/SN"/>
<attribute name="OC_FARNELL" value="1196803"/>
<attribute name="OC_NEWARK" value="19C7207"/>
</technology>
</technologies>
</device>
<device name="MS" package="MSOP8">
<connects>
<connect gate="P" pin="!CS!/SHDN" pad="1"/>
<connect gate="P" pin="CH0" pad="2"/>
<connect gate="P" pin="CH1" pad="3"/>
<connect gate="P" pin="CLK" pad="7"/>
<connect gate="P" pin="DIN" pad="5"/>
<connect gate="P" pin="DOUT" pad="6"/>
<connect gate="P" pin="VDD/VREF" pad="8"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3202-CI/MS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="68H9370"/>
</technology>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="P" pin="!CS!/SHDN" pad="1"/>
<connect gate="P" pin="CH0" pad="2"/>
<connect gate="P" pin="CH1" pad="3"/>
<connect gate="P" pin="CLK" pad="7"/>
<connect gate="P" pin="DIN" pad="5"/>
<connect gate="P" pin="DOUT" pad="6"/>
<connect gate="P" pin="VDD/VREF" pad="8"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP3202-CI/ST"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K0226"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ256GB110" prefix="IC">
<description>&lt;b&gt;PIC24FJ256GB110&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ256GB110.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ256GB110"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="ENVREG" pad="86"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="57"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="VBUS" pad="54"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VSS@1" pad="75"/>
<connect gate="G$1" pin="VSS@2" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="36"/>
<connect gate="G$1" pin="VSS@4" pad="45"/>
<connect gate="G$1" pin="VSS@5" pad="65"/>
<connect gate="G$1" pin="VUSB" pad="55"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ256GB110-I/PF"/>
<attribute name="OC_FARNELL" value="1576870"/>
<attribute name="OC_NEWARK" value="54M5133"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX320F*H" prefix="IC">
<description>&lt;b&gt;PIC32MX320FxxxH&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/61143E.pdf, PIC32MX320F064H.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX320F064H"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="RB0" pad="16"/>
<connect gate="G$1" pin="RB1" pad="15"/>
<connect gate="G$1" pin="RB14" pad="29"/>
<connect gate="G$1" pin="RB15" pad="30"/>
<connect gate="G$1" pin="RB2" pad="14"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="12"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="17"/>
<connect gate="G$1" pin="RB7" pad="18"/>
<connect gate="G$1" pin="RB8" pad="21"/>
<connect gate="G$1" pin="RB9" pad="22"/>
<connect gate="G$1" pin="RC12" pad="39"/>
<connect gate="G$1" pin="RC13" pad="47"/>
<connect gate="G$1" pin="RC14" pad="48"/>
<connect gate="G$1" pin="RC15" pad="40"/>
<connect gate="G$1" pin="RD0" pad="46"/>
<connect gate="G$1" pin="RD1" pad="49"/>
<connect gate="G$1" pin="RD10" pad="44"/>
<connect gate="G$1" pin="RD11" pad="45"/>
<connect gate="G$1" pin="RD2" pad="50"/>
<connect gate="G$1" pin="RD3" pad="51"/>
<connect gate="G$1" pin="RD4" pad="52"/>
<connect gate="G$1" pin="RD5" pad="53"/>
<connect gate="G$1" pin="RD6" pad="54"/>
<connect gate="G$1" pin="RD7" pad="55"/>
<connect gate="G$1" pin="RD8" pad="42"/>
<connect gate="G$1" pin="RD9" pad="43"/>
<connect gate="G$1" pin="RE0" pad="60"/>
<connect gate="G$1" pin="RE1" pad="61"/>
<connect gate="G$1" pin="RE2" pad="62"/>
<connect gate="G$1" pin="RE3" pad="63"/>
<connect gate="G$1" pin="RE4" pad="64"/>
<connect gate="G$1" pin="RE5" pad="1"/>
<connect gate="G$1" pin="RE6" pad="2"/>
<connect gate="G$1" pin="RE7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF2" pad="34"/>
<connect gate="G$1" pin="RF3" pad="33"/>
<connect gate="G$1" pin="RF4" pad="31"/>
<connect gate="G$1" pin="RF5" pad="32"/>
<connect gate="G$1" pin="RF6" pad="35"/>
<connect gate="G$1" pin="RG2" pad="37"/>
<connect gate="G$1" pin="RG3" pad="36"/>
<connect gate="G$1" pin="RG6" pad="4"/>
<connect gate="G$1" pin="RG7" pad="5"/>
<connect gate="G$1" pin="RG8" pad="6"/>
<connect gate="G$1" pin="RG9" pad="8"/>
<connect gate="G$1" pin="TCK" pad="27"/>
<connect gate="G$1" pin="TDI" pad="28"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="23"/>
<connect gate="G$1" pin="VDD@2" pad="10"/>
<connect gate="G$1" pin="VDD@3" pad="26"/>
<connect gate="G$1" pin="VDD@5" pad="38"/>
<connect gate="G$1" pin="VDDCORE" pad="56"/>
<connect gate="G$1" pin="VREG" pad="57"/>
<connect gate="G$1" pin="VSS@2" pad="9"/>
<connect gate="G$1" pin="VSS@3" pad="25"/>
<connect gate="G$1" pin="VSS@5" pad="41"/>
</connects>
<technologies>
<technology name="032">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX320F032H-40I/PT"/>
<attribute name="OC_FARNELL" value="1523318"/>
<attribute name="OC_NEWARK" value="98M1928"/>
</technology>
<technology name="064">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX320F064H-80I/PT"/>
<attribute name="OC_FARNELL" value="1778934"/>
<attribute name="OC_NEWARK" value="77M3147"/>
</technology>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX320F128H-80I/PT"/>
<attribute name="OC_FARNELL" value="1523320"/>
<attribute name="OC_NEWARK" value="77M3148"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX320F128L" prefix="IC">
<description>&lt;b&gt;PIC32MX320F128L&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX320F128L.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX320F128L"/>
</gates>
<devices>
<device name="" package="SQFP-S-12X12-100">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF6" pad="55"/>
<connect gate="G$1" pin="RF7" pad="54"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="57"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS@1" pad="75"/>
<connect gate="G$1" pin="VSS@2" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="36"/>
<connect gate="G$1" pin="VSS@4" pad="45"/>
<connect gate="G$1" pin="VSS@5" pad="65"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX320F128L-80I/PT"/>
<attribute name="OC_FARNELL" value="1523321"/>
<attribute name="OC_NEWARK" value="77M3149"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX360F512L" prefix="IC">
<description>&lt;b&gt;PIC32MX360F512L&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX360F512L.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX360F512L"/>
</gates>
<devices>
<device name="" package="SQFP-S-12X12-100">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF6" pad="55"/>
<connect gate="G$1" pin="RF7" pad="54"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="57"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS@1" pad="75"/>
<connect gate="G$1" pin="VSS@2" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="36"/>
<connect gate="G$1" pin="VSS@4" pad="45"/>
<connect gate="G$1" pin="VSS@5" pad="65"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX360F512L-80I/PT"/>
<attribute name="OC_FARNELL" value="1523324"/>
<attribute name="OC_NEWARK" value="77M3152"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX440F256H" prefix="IC">
<description>&lt;b&gt;PIC32MX440F256H&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX440F256H.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX440F256H"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="RB0" pad="16"/>
<connect gate="G$1" pin="RB1" pad="15"/>
<connect gate="G$1" pin="RB14" pad="29"/>
<connect gate="G$1" pin="RB15" pad="30"/>
<connect gate="G$1" pin="RB2" pad="14"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="12"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="17"/>
<connect gate="G$1" pin="RB7" pad="18"/>
<connect gate="G$1" pin="RB8" pad="21"/>
<connect gate="G$1" pin="RB9" pad="22"/>
<connect gate="G$1" pin="RC12" pad="39"/>
<connect gate="G$1" pin="RC13" pad="47"/>
<connect gate="G$1" pin="RC14" pad="48"/>
<connect gate="G$1" pin="RC15" pad="40"/>
<connect gate="G$1" pin="RD0" pad="46"/>
<connect gate="G$1" pin="RD1" pad="49"/>
<connect gate="G$1" pin="RD10" pad="44"/>
<connect gate="G$1" pin="RD11" pad="45"/>
<connect gate="G$1" pin="RD2" pad="50"/>
<connect gate="G$1" pin="RD3" pad="51"/>
<connect gate="G$1" pin="RD4" pad="52"/>
<connect gate="G$1" pin="RD5" pad="53"/>
<connect gate="G$1" pin="RD6" pad="54"/>
<connect gate="G$1" pin="RD7" pad="55"/>
<connect gate="G$1" pin="RD8" pad="42"/>
<connect gate="G$1" pin="RD9" pad="43"/>
<connect gate="G$1" pin="RE0" pad="60"/>
<connect gate="G$1" pin="RE1" pad="61"/>
<connect gate="G$1" pin="RE2" pad="62"/>
<connect gate="G$1" pin="RE3" pad="63"/>
<connect gate="G$1" pin="RE4" pad="64"/>
<connect gate="G$1" pin="RE5" pad="1"/>
<connect gate="G$1" pin="RE6" pad="2"/>
<connect gate="G$1" pin="RE7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF3" pad="33"/>
<connect gate="G$1" pin="RF4" pad="31"/>
<connect gate="G$1" pin="RF5" pad="32"/>
<connect gate="G$1" pin="RG6" pad="4"/>
<connect gate="G$1" pin="RG7" pad="5"/>
<connect gate="G$1" pin="RG8" pad="6"/>
<connect gate="G$1" pin="RG9" pad="8"/>
<connect gate="G$1" pin="TCK" pad="27"/>
<connect gate="G$1" pin="TDI" pad="28"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="23"/>
<connect gate="G$1" pin="USBDM" pad="36"/>
<connect gate="G$1" pin="USBDP" pad="37"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VDD@2" pad="10"/>
<connect gate="G$1" pin="VDD@3" pad="26"/>
<connect gate="G$1" pin="VDD@5" pad="38"/>
<connect gate="G$1" pin="VDDCORE" pad="56"/>
<connect gate="G$1" pin="VREG" pad="57"/>
<connect gate="G$1" pin="VSS@2" pad="9"/>
<connect gate="G$1" pin="VSS@3" pad="25"/>
<connect gate="G$1" pin="VSS@5" pad="41"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX440F256H-80I/PT"/>
<attribute name="OC_FARNELL" value="1778947"/>
<attribute name="OC_NEWARK" value="98M1935"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX460F512L" prefix="IC">
<description>&lt;b&gt;PIC32MX460F512L&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX460F512L.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX460F512L"/>
</gates>
<devices>
<device name="" package="SQFP-S-12X12-100">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="USBDM" pad="56"/>
<connect gate="G$1" pin="USBDP" pad="57"/>
<connect gate="G$1" pin="VBUS" pad="54"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS@1" pad="75"/>
<connect gate="G$1" pin="VSS@2" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="36"/>
<connect gate="G$1" pin="VSS@4" pad="45"/>
<connect gate="G$1" pin="VSS@5" pad="65"/>
<connect gate="G$1" pin="VUSB" pad="55"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX460F512L-80I/PT"/>
<attribute name="OC_FARNELL" value="1640233"/>
<attribute name="OC_NEWARK" value="98M1938"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX460F256L" prefix="IC">
<description>&lt;b&gt;PIC32MX460F256L&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX460F256L.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX460F256L"/>
</gates>
<devices>
<device name="" package="SQFP-S-12X12-100">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="USBDM" pad="56"/>
<connect gate="G$1" pin="USBDP" pad="57"/>
<connect gate="G$1" pin="VBUS" pad="54"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS@1" pad="75"/>
<connect gate="G$1" pin="VSS@2" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="36"/>
<connect gate="G$1" pin="VSS@4" pad="45"/>
<connect gate="G$1" pin="VSS@5" pad="65"/>
<connect gate="G$1" pin="VUSB" pad="55"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX460F256L-80I/PT"/>
<attribute name="OC_FARNELL" value="1778952"/>
<attribute name="OC_NEWARK" value="98M1937"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX320F032H" prefix="IC">
<description>&lt;b&gt;PIC32MX320F032H&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX320F032H.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX320F032H"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="RB0" pad="16"/>
<connect gate="G$1" pin="RB1" pad="15"/>
<connect gate="G$1" pin="RB14" pad="29"/>
<connect gate="G$1" pin="RB15" pad="30"/>
<connect gate="G$1" pin="RB2" pad="14"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="12"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="17"/>
<connect gate="G$1" pin="RB7" pad="18"/>
<connect gate="G$1" pin="RB8" pad="21"/>
<connect gate="G$1" pin="RB9" pad="22"/>
<connect gate="G$1" pin="RC12" pad="39"/>
<connect gate="G$1" pin="RC13" pad="47"/>
<connect gate="G$1" pin="RC14" pad="48"/>
<connect gate="G$1" pin="RC15" pad="40"/>
<connect gate="G$1" pin="RD0" pad="46"/>
<connect gate="G$1" pin="RD1" pad="49"/>
<connect gate="G$1" pin="RD10" pad="44"/>
<connect gate="G$1" pin="RD11" pad="45"/>
<connect gate="G$1" pin="RD2" pad="50"/>
<connect gate="G$1" pin="RD3" pad="51"/>
<connect gate="G$1" pin="RD4" pad="52"/>
<connect gate="G$1" pin="RD5" pad="53"/>
<connect gate="G$1" pin="RD6" pad="54"/>
<connect gate="G$1" pin="RD7" pad="55"/>
<connect gate="G$1" pin="RD8" pad="42"/>
<connect gate="G$1" pin="RD9" pad="43"/>
<connect gate="G$1" pin="RE0" pad="60"/>
<connect gate="G$1" pin="RE1" pad="61"/>
<connect gate="G$1" pin="RE2" pad="62"/>
<connect gate="G$1" pin="RE3" pad="63"/>
<connect gate="G$1" pin="RE4" pad="64"/>
<connect gate="G$1" pin="RE5" pad="1"/>
<connect gate="G$1" pin="RE6" pad="2"/>
<connect gate="G$1" pin="RE7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF2" pad="34"/>
<connect gate="G$1" pin="RF3" pad="33"/>
<connect gate="G$1" pin="RF4" pad="31"/>
<connect gate="G$1" pin="RF5" pad="32"/>
<connect gate="G$1" pin="RF6" pad="35"/>
<connect gate="G$1" pin="RG2" pad="37"/>
<connect gate="G$1" pin="RG3" pad="36"/>
<connect gate="G$1" pin="RG6" pad="4"/>
<connect gate="G$1" pin="RG7" pad="5"/>
<connect gate="G$1" pin="RG8" pad="6"/>
<connect gate="G$1" pin="RG9" pad="8"/>
<connect gate="G$1" pin="TCK" pad="27"/>
<connect gate="G$1" pin="TDI" pad="28"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="23"/>
<connect gate="G$1" pin="VDD@2" pad="10"/>
<connect gate="G$1" pin="VDD@3" pad="26"/>
<connect gate="G$1" pin="VDD@5" pad="38"/>
<connect gate="G$1" pin="VDDCORE" pad="56"/>
<connect gate="G$1" pin="VREG" pad="57"/>
<connect gate="G$1" pin="VSS@2" pad="9"/>
<connect gate="G$1" pin="VSS@3" pad="25"/>
<connect gate="G$1" pin="VSS@5" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX320F032H-40I/PT"/>
<attribute name="OC_FARNELL" value="1523318"/>
<attribute name="OC_NEWARK" value="98M1928"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX420F032H" prefix="IC">
<description>&lt;b&gt;PIC32MX420F032H&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX420F032H.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX420F032H"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10X1MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="RB0" pad="16"/>
<connect gate="G$1" pin="RB1" pad="15"/>
<connect gate="G$1" pin="RB14" pad="29"/>
<connect gate="G$1" pin="RB15" pad="30"/>
<connect gate="G$1" pin="RB2" pad="14"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="12"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="17"/>
<connect gate="G$1" pin="RB7" pad="18"/>
<connect gate="G$1" pin="RB8" pad="21"/>
<connect gate="G$1" pin="RB9" pad="22"/>
<connect gate="G$1" pin="RC12" pad="39"/>
<connect gate="G$1" pin="RC13" pad="47"/>
<connect gate="G$1" pin="RC14" pad="48"/>
<connect gate="G$1" pin="RC15" pad="40"/>
<connect gate="G$1" pin="RD0" pad="46"/>
<connect gate="G$1" pin="RD1" pad="49"/>
<connect gate="G$1" pin="RD10" pad="44"/>
<connect gate="G$1" pin="RD11" pad="45"/>
<connect gate="G$1" pin="RD2" pad="50"/>
<connect gate="G$1" pin="RD3" pad="51"/>
<connect gate="G$1" pin="RD4" pad="52"/>
<connect gate="G$1" pin="RD5" pad="53"/>
<connect gate="G$1" pin="RD6" pad="54"/>
<connect gate="G$1" pin="RD7" pad="55"/>
<connect gate="G$1" pin="RD8" pad="42"/>
<connect gate="G$1" pin="RD9" pad="43"/>
<connect gate="G$1" pin="RE0" pad="60"/>
<connect gate="G$1" pin="RE1" pad="61"/>
<connect gate="G$1" pin="RE2" pad="62"/>
<connect gate="G$1" pin="RE3" pad="63"/>
<connect gate="G$1" pin="RE4" pad="64"/>
<connect gate="G$1" pin="RE5" pad="1"/>
<connect gate="G$1" pin="RE6" pad="2"/>
<connect gate="G$1" pin="RE7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF3" pad="33"/>
<connect gate="G$1" pin="RF4" pad="31"/>
<connect gate="G$1" pin="RF5" pad="32"/>
<connect gate="G$1" pin="RG6" pad="4"/>
<connect gate="G$1" pin="RG7" pad="5"/>
<connect gate="G$1" pin="RG8" pad="6"/>
<connect gate="G$1" pin="RG9" pad="8"/>
<connect gate="G$1" pin="TCK" pad="27"/>
<connect gate="G$1" pin="TDI" pad="28"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="23"/>
<connect gate="G$1" pin="USBDM" pad="36"/>
<connect gate="G$1" pin="USBDP" pad="37"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VDD@2" pad="10"/>
<connect gate="G$1" pin="VDD@3" pad="26"/>
<connect gate="G$1" pin="VDD@5" pad="38"/>
<connect gate="G$1" pin="VDDCORE" pad="56"/>
<connect gate="G$1" pin="VREG" pad="57"/>
<connect gate="G$1" pin="VSS@2" pad="9"/>
<connect gate="G$1" pin="VSS@3" pad="25"/>
<connect gate="G$1" pin="VSS@5" pad="41"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC32MX420F032H-40I/PT"/>
<attribute name="OC_FARNELL" value="1640230"/>
<attribute name="OC_NEWARK" value="98M1932"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX360F256L" prefix="IC">
<description>&lt;b&gt;PIC32MX360F256L&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX360F256L.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX360F256L"/>
</gates>
<devices>
<device name="" package="SQFP-S-12X12-100">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF6" pad="55"/>
<connect gate="G$1" pin="RF7" pad="54"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="57"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS@1" pad="75"/>
<connect gate="G$1" pin="VSS@2" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="36"/>
<connect gate="G$1" pin="VSS@4" pad="45"/>
<connect gate="G$1" pin="VSS@5" pad="65"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX360F256L-80I/PT"/>
<attribute name="OC_FARNELL" value="1523323"/>
<attribute name="OC_NEWARK" value="77M3151"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ64GA002" prefix="IC">
<description>&lt;b&gt;PIC24FJ64GA002&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ64GA002.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ64GA002"/>
</gates>
<devices>
<device name="" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="DISVREG" pad="19"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="9"/>
<connect gate="G$1" pin="RA3" pad="10"/>
<connect gate="G$1" pin="RA4" pad="12"/>
<connect gate="G$1" pin="RB0" pad="4"/>
<connect gate="G$1" pin="RB1" pad="5"/>
<connect gate="G$1" pin="RB12" pad="23"/>
<connect gate="G$1" pin="RB13" pad="24"/>
<connect gate="G$1" pin="RB14" pad="25"/>
<connect gate="G$1" pin="RB15" pad="26"/>
<connect gate="G$1" pin="RB2" pad="6"/>
<connect gate="G$1" pin="RB3" pad="7"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="14"/>
<connect gate="G$1" pin="RB6" pad="15"/>
<connect gate="G$1" pin="RB7" pad="16"/>
<connect gate="G$1" pin="TCK" pad="17"/>
<connect gate="G$1" pin="TDI" pad="21"/>
<connect gate="G$1" pin="TDO" pad="18"/>
<connect gate="G$1" pin="TMS" pad="22"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VDDCORE" pad="20"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ64GA002-I/SP"/>
<attribute name="OC_FARNELL" value="1332298"/>
<attribute name="OC_NEWARK" value="88K6132"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ64GA002_QFN" prefix="IC">
<description>&lt;b&gt;PIC24FJ64GA002_QFN&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ64GA002_QFN.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ64GA002_QFN"/>
</gates>
<devices>
<device name="" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="26"/>
<connect gate="G$1" pin="DISVREG" pad="16"/>
<connect gate="G$1" pin="RA0" pad="27"/>
<connect gate="G$1" pin="RA1" pad="28"/>
<connect gate="G$1" pin="RA2" pad="6"/>
<connect gate="G$1" pin="RA3" pad="7"/>
<connect gate="G$1" pin="RA4" pad="9"/>
<connect gate="G$1" pin="RB0" pad="1"/>
<connect gate="G$1" pin="RB1" pad="2"/>
<connect gate="G$1" pin="RB12" pad="20"/>
<connect gate="G$1" pin="RB13" pad="21"/>
<connect gate="G$1" pin="RB14" pad="22"/>
<connect gate="G$1" pin="RB15" pad="23"/>
<connect gate="G$1" pin="RB2" pad="3"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="8"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="TCK" pad="14"/>
<connect gate="G$1" pin="TDI" pad="18"/>
<connect gate="G$1" pin="TDO" pad="15"/>
<connect gate="G$1" pin="TMS" pad="19"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="25"/>
<connect gate="G$1" pin="VDDCORE" pad="17"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ64GA002-E/ML"/>
<attribute name="OC_FARNELL" value="1818728"/>
<attribute name="OC_NEWARK" value="98M1922"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ48GA002" prefix="IC">
<description>&lt;b&gt;PIC24FJ48GA002&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ48GA002.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ48GA002"/>
</gates>
<devices>
<device name="" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="DISVREG" pad="19"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="9"/>
<connect gate="G$1" pin="RA3" pad="10"/>
<connect gate="G$1" pin="RA4" pad="12"/>
<connect gate="G$1" pin="RB0" pad="4"/>
<connect gate="G$1" pin="RB1" pad="5"/>
<connect gate="G$1" pin="RB12" pad="23"/>
<connect gate="G$1" pin="RB13" pad="24"/>
<connect gate="G$1" pin="RB14" pad="25"/>
<connect gate="G$1" pin="RB15" pad="26"/>
<connect gate="G$1" pin="RB2" pad="6"/>
<connect gate="G$1" pin="RB3" pad="7"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="14"/>
<connect gate="G$1" pin="RB6" pad="15"/>
<connect gate="G$1" pin="RB7" pad="16"/>
<connect gate="G$1" pin="TCK" pad="17"/>
<connect gate="G$1" pin="TDI" pad="21"/>
<connect gate="G$1" pin="TDO" pad="18"/>
<connect gate="G$1" pin="TMS" pad="22"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VDDCORE" pad="20"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ48GA002-I/SP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="40M1440"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ48GA002_QFN" prefix="IC">
<description>&lt;b&gt;PIC24FJ48GA002_QFN&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ48GA002_QFN.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ48GA002_QFN"/>
</gates>
<devices>
<device name="" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="26"/>
<connect gate="G$1" pin="DISVREG" pad="16"/>
<connect gate="G$1" pin="RA0" pad="27"/>
<connect gate="G$1" pin="RA1" pad="28"/>
<connect gate="G$1" pin="RA2" pad="6"/>
<connect gate="G$1" pin="RA3" pad="7"/>
<connect gate="G$1" pin="RA4" pad="9"/>
<connect gate="G$1" pin="RB0" pad="1"/>
<connect gate="G$1" pin="RB1" pad="2"/>
<connect gate="G$1" pin="RB12" pad="20"/>
<connect gate="G$1" pin="RB13" pad="21"/>
<connect gate="G$1" pin="RB14" pad="22"/>
<connect gate="G$1" pin="RB15" pad="23"/>
<connect gate="G$1" pin="RB2" pad="3"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="8"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="TCK" pad="14"/>
<connect gate="G$1" pin="TDI" pad="18"/>
<connect gate="G$1" pin="TDO" pad="15"/>
<connect gate="G$1" pin="TMS" pad="19"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="25"/>
<connect gate="G$1" pin="VDDCORE" pad="17"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ48GA002-E/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="98M1916"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ32GA002" prefix="IC">
<description>&lt;b&gt;PIC24FJ32GA002&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ32GA002.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ32GA002"/>
</gates>
<devices>
<device name="" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="DISVREG" pad="19"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="9"/>
<connect gate="G$1" pin="RA3" pad="10"/>
<connect gate="G$1" pin="RA4" pad="12"/>
<connect gate="G$1" pin="RB0" pad="4"/>
<connect gate="G$1" pin="RB1" pad="5"/>
<connect gate="G$1" pin="RB12" pad="23"/>
<connect gate="G$1" pin="RB13" pad="24"/>
<connect gate="G$1" pin="RB14" pad="25"/>
<connect gate="G$1" pin="RB15" pad="26"/>
<connect gate="G$1" pin="RB2" pad="6"/>
<connect gate="G$1" pin="RB3" pad="7"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="14"/>
<connect gate="G$1" pin="RB6" pad="15"/>
<connect gate="G$1" pin="RB7" pad="16"/>
<connect gate="G$1" pin="TCK" pad="17"/>
<connect gate="G$1" pin="TDI" pad="21"/>
<connect gate="G$1" pin="TDO" pad="18"/>
<connect gate="G$1" pin="TMS" pad="22"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VDDCORE" pad="20"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ32GA002-I/SP"/>
<attribute name="OC_FARNELL" value="1332294"/>
<attribute name="OC_NEWARK" value="88K6123"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ32GA002_QFN" prefix="IC">
<description>&lt;b&gt;PIC24FJ32GA002_QFN&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ32GA002_QFN.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ32GA002_QFN"/>
</gates>
<devices>
<device name="" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="26"/>
<connect gate="G$1" pin="DISVREG" pad="16"/>
<connect gate="G$1" pin="RA0" pad="27"/>
<connect gate="G$1" pin="RA1" pad="28"/>
<connect gate="G$1" pin="RA2" pad="6"/>
<connect gate="G$1" pin="RA3" pad="7"/>
<connect gate="G$1" pin="RA4" pad="9"/>
<connect gate="G$1" pin="RB0" pad="1"/>
<connect gate="G$1" pin="RB1" pad="2"/>
<connect gate="G$1" pin="RB12" pad="20"/>
<connect gate="G$1" pin="RB13" pad="21"/>
<connect gate="G$1" pin="RB14" pad="22"/>
<connect gate="G$1" pin="RB15" pad="23"/>
<connect gate="G$1" pin="RB2" pad="3"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="8"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="TCK" pad="14"/>
<connect gate="G$1" pin="TDI" pad="18"/>
<connect gate="G$1" pin="TDO" pad="15"/>
<connect gate="G$1" pin="TMS" pad="19"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="25"/>
<connect gate="G$1" pin="VDDCORE" pad="17"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ32GA002-I/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88K6121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ16GA002" prefix="IC">
<description>&lt;b&gt;PIC24FJ16GA002&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ16GA002.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ16GA002"/>
</gates>
<devices>
<device name="" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="DISVREG" pad="19"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="9"/>
<connect gate="G$1" pin="RA3" pad="10"/>
<connect gate="G$1" pin="RA4" pad="12"/>
<connect gate="G$1" pin="RB0" pad="4"/>
<connect gate="G$1" pin="RB1" pad="5"/>
<connect gate="G$1" pin="RB12" pad="23"/>
<connect gate="G$1" pin="RB13" pad="24"/>
<connect gate="G$1" pin="RB14" pad="25"/>
<connect gate="G$1" pin="RB15" pad="26"/>
<connect gate="G$1" pin="RB2" pad="6"/>
<connect gate="G$1" pin="RB3" pad="7"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="14"/>
<connect gate="G$1" pin="RB6" pad="15"/>
<connect gate="G$1" pin="RB7" pad="16"/>
<connect gate="G$1" pin="TCK" pad="17"/>
<connect gate="G$1" pin="TDI" pad="21"/>
<connect gate="G$1" pin="TDO" pad="18"/>
<connect gate="G$1" pin="TMS" pad="22"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VDDCORE" pad="20"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ16GA002-I/SP"/>
<attribute name="OC_FARNELL" value="1816078"/>
<attribute name="OC_NEWARK" value="40M1427"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ16GA002_QFN" prefix="IC">
<description>&lt;b&gt;PIC24FJ16GA002_QFN&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ16GA002_QFN.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ16GA002_QFN"/>
</gates>
<devices>
<device name="" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="26"/>
<connect gate="G$1" pin="DISVREG" pad="16"/>
<connect gate="G$1" pin="RA0" pad="27"/>
<connect gate="G$1" pin="RA1" pad="28"/>
<connect gate="G$1" pin="RA2" pad="6"/>
<connect gate="G$1" pin="RA3" pad="7"/>
<connect gate="G$1" pin="RA4" pad="9"/>
<connect gate="G$1" pin="RB0" pad="1"/>
<connect gate="G$1" pin="RB1" pad="2"/>
<connect gate="G$1" pin="RB12" pad="20"/>
<connect gate="G$1" pin="RB13" pad="21"/>
<connect gate="G$1" pin="RB14" pad="22"/>
<connect gate="G$1" pin="RB15" pad="23"/>
<connect gate="G$1" pin="RB2" pad="3"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="8"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="TCK" pad="14"/>
<connect gate="G$1" pin="TDI" pad="18"/>
<connect gate="G$1" pin="TDO" pad="15"/>
<connect gate="G$1" pin="TMS" pad="19"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="25"/>
<connect gate="G$1" pin="VDDCORE" pad="17"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ16GA002-I/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="40M1425"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ256GB108" prefix="IC">
<description>&lt;b&gt;PIC24FJ256GB108&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ256GB108.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ256GB108"/>
</gates>
<devices>
<device name="" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ENVREG" pad="71"/>
<connect gate="G$1" pin="RA10" pad="24"/>
<connect gate="G$1" pin="RA14" pad="52"/>
<connect gate="G$1" pin="RA15" pad="53"/>
<connect gate="G$1" pin="RA9" pad="23"/>
<connect gate="G$1" pin="RB0" pad="20"/>
<connect gate="G$1" pin="RB1" pad="19"/>
<connect gate="G$1" pin="RB10" pad="29"/>
<connect gate="G$1" pin="RB11" pad="30"/>
<connect gate="G$1" pin="RB14" pad="35"/>
<connect gate="G$1" pin="RB15" pad="36"/>
<connect gate="G$1" pin="RB2" pad="18"/>
<connect gate="G$1" pin="RB3" pad="17"/>
<connect gate="G$1" pin="RB4" pad="16"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6" pad="21"/>
<connect gate="G$1" pin="RB7" pad="22"/>
<connect gate="G$1" pin="RB8" pad="27"/>
<connect gate="G$1" pin="RB9" pad="28"/>
<connect gate="G$1" pin="RC1" pad="4"/>
<connect gate="G$1" pin="RC12" pad="49"/>
<connect gate="G$1" pin="RC13" pad="59"/>
<connect gate="G$1" pin="RC14" pad="60"/>
<connect gate="G$1" pin="RC15" pad="50"/>
<connect gate="G$1" pin="RC3" pad="5"/>
<connect gate="G$1" pin="RD0" pad="58"/>
<connect gate="G$1" pin="RD1" pad="61"/>
<connect gate="G$1" pin="RD10" pad="56"/>
<connect gate="G$1" pin="RD11" pad="57"/>
<connect gate="G$1" pin="RD12" pad="64"/>
<connect gate="G$1" pin="RD13" pad="65"/>
<connect gate="G$1" pin="RD14" pad="37"/>
<connect gate="G$1" pin="RD15" pad="38"/>
<connect gate="G$1" pin="RD2" pad="62"/>
<connect gate="G$1" pin="RD3" pad="63"/>
<connect gate="G$1" pin="RD4" pad="66"/>
<connect gate="G$1" pin="RD5" pad="67"/>
<connect gate="G$1" pin="RD6" pad="68"/>
<connect gate="G$1" pin="RD7" pad="69"/>
<connect gate="G$1" pin="RD8" pad="54"/>
<connect gate="G$1" pin="RD9" pad="55"/>
<connect gate="G$1" pin="RE0" pad="76"/>
<connect gate="G$1" pin="RE1" pad="77"/>
<connect gate="G$1" pin="RE2" pad="78"/>
<connect gate="G$1" pin="RE3" pad="79"/>
<connect gate="G$1" pin="RE4" pad="80"/>
<connect gate="G$1" pin="RE5" pad="1"/>
<connect gate="G$1" pin="RE6" pad="2"/>
<connect gate="G$1" pin="RE7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="72"/>
<connect gate="G$1" pin="RF1" pad="73"/>
<connect gate="G$1" pin="RF2" pad="42"/>
<connect gate="G$1" pin="RF3" pad="41"/>
<connect gate="G$1" pin="RF4" pad="39"/>
<connect gate="G$1" pin="RF5" pad="40"/>
<connect gate="G$1" pin="RF8" pad="43"/>
<connect gate="G$1" pin="RG0" pad="75"/>
<connect gate="G$1" pin="RG1" pad="74"/>
<connect gate="G$1" pin="RG2" pad="47"/>
<connect gate="G$1" pin="RG3" pad="46"/>
<connect gate="G$1" pin="RG6" pad="6"/>
<connect gate="G$1" pin="RG7" pad="7"/>
<connect gate="G$1" pin="RG8" pad="8"/>
<connect gate="G$1" pin="RG9" pad="10"/>
<connect gate="G$1" pin="TCK" pad="33"/>
<connect gate="G$1" pin="TDI" pad="34"/>
<connect gate="G$1" pin="TDO" pad="14"/>
<connect gate="G$1" pin="TMS" pad="13"/>
<connect gate="G$1" pin="VBUS" pad="44"/>
<connect gate="G$1" pin="VDD@1" pad="12"/>
<connect gate="G$1" pin="VDD@2" pad="32"/>
<connect gate="G$1" pin="VDD@3" pad="48"/>
<connect gate="G$1" pin="VDDCORE" pad="70"/>
<connect gate="G$1" pin="VSS@1" pad="11"/>
<connect gate="G$1" pin="VSS@2" pad="31"/>
<connect gate="G$1" pin="VSS@3" pad="51"/>
<connect gate="G$1" pin="VUSB" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ256GB108-I/PT"/>
<attribute name="OC_FARNELL" value="1576869"/>
<attribute name="OC_NEWARK" value="54M5131"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ64GB110" prefix="IC">
<description>&lt;b&gt;PIC24FJ64GB110&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ64GB110.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ64GB110"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="ENVREG" pad="86"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="57"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="VBUS" pad="54"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VSS@1" pad="75"/>
<connect gate="G$1" pin="VSS@2" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="36"/>
<connect gate="G$1" pin="VSS@4" pad="45"/>
<connect gate="G$1" pin="VSS@5" pad="65"/>
<connect gate="G$1" pin="VUSB" pad="55"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ64GB110-I/PT"/>
<attribute name="OC_FARNELL" value="1576875"/>
<attribute name="OC_NEWARK" value="54M5142"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX440F128L" prefix="IC">
<description>&lt;b&gt;PIC32MX440F128L&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC32MX440F128L.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX440F128L"/>
</gates>
<devices>
<device name="" package="SQFP-S-12X12-100">
<connects>
<connect gate="G$1" pin="!MCLR" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="USBDM" pad="56"/>
<connect gate="G$1" pin="USBDP" pad="57"/>
<connect gate="G$1" pin="VBUS" pad="54"/>
<connect gate="G$1" pin="VDD@1" pad="2"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="37"/>
<connect gate="G$1" pin="VDD@4" pad="46"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS@1" pad="75"/>
<connect gate="G$1" pin="VSS@2" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="36"/>
<connect gate="G$1" pin="VSS@4" pad="45"/>
<connect gate="G$1" pin="VSS@5" pad="65"/>
<connect gate="G$1" pin="VUSB" pad="55"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX440F128L-80I/PT"/>
<attribute name="OC_FARNELL" value="1640231"/>
<attribute name="OC_NEWARK" value="98M1934"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ64GA004" prefix="IC">
<description>&lt;b&gt;PIC24FJ64GA004&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ64GA004.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ64GA004"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="16"/>
<connect gate="G$1" pin="DISVREG" pad="6"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="30"/>
<connect gate="G$1" pin="RA3" pad="31"/>
<connect gate="G$1" pin="RA4" pad="34"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB10" pad="8"/>
<connect gate="G$1" pin="RB11" pad="9"/>
<connect gate="G$1" pin="RB12" pad="10"/>
<connect gate="G$1" pin="RB13" pad="11"/>
<connect gate="G$1" pin="RB14" pad="14"/>
<connect gate="G$1" pin="RB15" pad="15"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="33"/>
<connect gate="G$1" pin="RB5" pad="41"/>
<connect gate="G$1" pin="RB6" pad="42"/>
<connect gate="G$1" pin="RB7" pad="43"/>
<connect gate="G$1" pin="RB8" pad="44"/>
<connect gate="G$1" pin="RB9" pad="1"/>
<connect gate="G$1" pin="RC0" pad="25"/>
<connect gate="G$1" pin="RC1" pad="26"/>
<connect gate="G$1" pin="RC2" pad="27"/>
<connect gate="G$1" pin="RC3" pad="36"/>
<connect gate="G$1" pin="RC4" pad="37"/>
<connect gate="G$1" pin="RC5" pad="38"/>
<connect gate="G$1" pin="RC6" pad="2"/>
<connect gate="G$1" pin="RC7" pad="3"/>
<connect gate="G$1" pin="RC8" pad="4"/>
<connect gate="G$1" pin="RC9" pad="5"/>
<connect gate="G$1" pin="TCK" pad="13"/>
<connect gate="G$1" pin="TDI" pad="35"/>
<connect gate="G$1" pin="TDO" pad="32"/>
<connect gate="G$1" pin="TMS" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VDD@2" pad="40"/>
<connect gate="G$1" pin="VDDCORE" pad="7"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
<connect gate="G$1" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ64GA004-E/PT"/>
<attribute name="OC_FARNELL" value="1332299"/>
<attribute name="OC_NEWARK" value="98M1927"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ48GA004" prefix="IC">
<description>&lt;b&gt;PIC24FJ48GA004&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ48GA004.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ48GA004"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="16"/>
<connect gate="G$1" pin="DISVREG" pad="6"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="30"/>
<connect gate="G$1" pin="RA3" pad="31"/>
<connect gate="G$1" pin="RA4" pad="34"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB10" pad="8"/>
<connect gate="G$1" pin="RB11" pad="9"/>
<connect gate="G$1" pin="RB12" pad="10"/>
<connect gate="G$1" pin="RB13" pad="11"/>
<connect gate="G$1" pin="RB14" pad="14"/>
<connect gate="G$1" pin="RB15" pad="15"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="33"/>
<connect gate="G$1" pin="RB5" pad="41"/>
<connect gate="G$1" pin="RB6" pad="42"/>
<connect gate="G$1" pin="RB7" pad="43"/>
<connect gate="G$1" pin="RB8" pad="44"/>
<connect gate="G$1" pin="RB9" pad="1"/>
<connect gate="G$1" pin="RC0" pad="25"/>
<connect gate="G$1" pin="RC1" pad="26"/>
<connect gate="G$1" pin="RC2" pad="27"/>
<connect gate="G$1" pin="RC3" pad="36"/>
<connect gate="G$1" pin="RC4" pad="37"/>
<connect gate="G$1" pin="RC5" pad="38"/>
<connect gate="G$1" pin="RC6" pad="2"/>
<connect gate="G$1" pin="RC7" pad="3"/>
<connect gate="G$1" pin="RC8" pad="4"/>
<connect gate="G$1" pin="RC9" pad="5"/>
<connect gate="G$1" pin="TCK" pad="13"/>
<connect gate="G$1" pin="TDI" pad="35"/>
<connect gate="G$1" pin="TDO" pad="32"/>
<connect gate="G$1" pin="TMS" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VDD@2" pad="40"/>
<connect gate="G$1" pin="VDDCORE" pad="7"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
<connect gate="G$1" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ48GA004-I/PT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="40M1446"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ64GP506" prefix="IC">
<description>&lt;b&gt;PIC24HJ64GP506&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24HJ64GP506.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24HJ64GP506"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="RB0" pad="16"/>
<connect gate="G$1" pin="RB1" pad="15"/>
<connect gate="G$1" pin="RB14" pad="29"/>
<connect gate="G$1" pin="RB15" pad="30"/>
<connect gate="G$1" pin="RB2" pad="14"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="12"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="17"/>
<connect gate="G$1" pin="RB7" pad="18"/>
<connect gate="G$1" pin="RB8" pad="21"/>
<connect gate="G$1" pin="RB9" pad="22"/>
<connect gate="G$1" pin="RC1" pad="2"/>
<connect gate="G$1" pin="RC12" pad="39"/>
<connect gate="G$1" pin="RC13" pad="47"/>
<connect gate="G$1" pin="RC14" pad="48"/>
<connect gate="G$1" pin="RC15" pad="40"/>
<connect gate="G$1" pin="RC2" pad="3"/>
<connect gate="G$1" pin="RD0" pad="46"/>
<connect gate="G$1" pin="RD1" pad="49"/>
<connect gate="G$1" pin="RD10" pad="44"/>
<connect gate="G$1" pin="RD11" pad="45"/>
<connect gate="G$1" pin="RD2" pad="50"/>
<connect gate="G$1" pin="RD3" pad="51"/>
<connect gate="G$1" pin="RD4" pad="52"/>
<connect gate="G$1" pin="RD5" pad="53"/>
<connect gate="G$1" pin="RD6" pad="54"/>
<connect gate="G$1" pin="RD7" pad="55"/>
<connect gate="G$1" pin="RD8" pad="42"/>
<connect gate="G$1" pin="RD9" pad="43"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF2" pad="34"/>
<connect gate="G$1" pin="RF3" pad="33"/>
<connect gate="G$1" pin="RF4" pad="31"/>
<connect gate="G$1" pin="RF5" pad="32"/>
<connect gate="G$1" pin="RF6" pad="35"/>
<connect gate="G$1" pin="RG0" pad="61"/>
<connect gate="G$1" pin="RG1" pad="60"/>
<connect gate="G$1" pin="RG12" pad="63"/>
<connect gate="G$1" pin="RG13" pad="64"/>
<connect gate="G$1" pin="RG14" pad="62"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="37"/>
<connect gate="G$1" pin="RG3" pad="36"/>
<connect gate="G$1" pin="RG6" pad="4"/>
<connect gate="G$1" pin="RG7" pad="5"/>
<connect gate="G$1" pin="RG8" pad="6"/>
<connect gate="G$1" pin="RG9" pad="8"/>
<connect gate="G$1" pin="TCK" pad="27"/>
<connect gate="G$1" pin="TDI" pad="28"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="23"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VDD@4" pad="57"/>
<connect gate="G$1" pin="VDDCORE" pad="56"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24HJ64GP506A-I/PT"/>
<attribute name="OC_FARNELL" value="1146551"/>
<attribute name="OC_NEWARK" value="45P4882"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ32GA004" prefix="IC">
<description>&lt;b&gt;PIC24FJ32GA004&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ32GA004.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ32GA004"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="16"/>
<connect gate="G$1" pin="DISVREG" pad="6"/>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="30"/>
<connect gate="G$1" pin="RA3" pad="31"/>
<connect gate="G$1" pin="RA4" pad="34"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB10" pad="8"/>
<connect gate="G$1" pin="RB11" pad="9"/>
<connect gate="G$1" pin="RB12" pad="10"/>
<connect gate="G$1" pin="RB13" pad="11"/>
<connect gate="G$1" pin="RB14" pad="14"/>
<connect gate="G$1" pin="RB15" pad="15"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="33"/>
<connect gate="G$1" pin="RB5" pad="41"/>
<connect gate="G$1" pin="RB6" pad="42"/>
<connect gate="G$1" pin="RB7" pad="43"/>
<connect gate="G$1" pin="RB8" pad="44"/>
<connect gate="G$1" pin="RB9" pad="1"/>
<connect gate="G$1" pin="RC0" pad="25"/>
<connect gate="G$1" pin="RC1" pad="26"/>
<connect gate="G$1" pin="RC2" pad="27"/>
<connect gate="G$1" pin="RC3" pad="36"/>
<connect gate="G$1" pin="RC4" pad="37"/>
<connect gate="G$1" pin="RC5" pad="38"/>
<connect gate="G$1" pin="RC6" pad="2"/>
<connect gate="G$1" pin="RC7" pad="3"/>
<connect gate="G$1" pin="RC8" pad="4"/>
<connect gate="G$1" pin="RC9" pad="5"/>
<connect gate="G$1" pin="TCK" pad="13"/>
<connect gate="G$1" pin="TDI" pad="35"/>
<connect gate="G$1" pin="TDO" pad="32"/>
<connect gate="G$1" pin="TMS" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VDD@2" pad="40"/>
<connect gate="G$1" pin="VDDCORE" pad="7"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
<connect gate="G$1" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ32GA004-E/PT"/>
<attribute name="OC_FARNELL" value="1332295"/>
<attribute name="OC_NEWARK" value="98M1915"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ256GB106" prefix="IC">
<description>&lt;b&gt;PIC24FJ256GB106&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24FJ256GB106.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24FJ256GB106"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="RB0" pad="16"/>
<connect gate="G$1" pin="RB1" pad="15"/>
<connect gate="G$1" pin="RB14" pad="29"/>
<connect gate="G$1" pin="RB15" pad="30"/>
<connect gate="G$1" pin="RB2" pad="14"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="12"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="17"/>
<connect gate="G$1" pin="RB7" pad="18"/>
<connect gate="G$1" pin="RB8" pad="21"/>
<connect gate="G$1" pin="RB9" pad="22"/>
<connect gate="G$1" pin="RC12" pad="39"/>
<connect gate="G$1" pin="RC13" pad="47"/>
<connect gate="G$1" pin="RC14" pad="48"/>
<connect gate="G$1" pin="RC15" pad="40"/>
<connect gate="G$1" pin="RD0" pad="46"/>
<connect gate="G$1" pin="RD1" pad="49"/>
<connect gate="G$1" pin="RD10" pad="44"/>
<connect gate="G$1" pin="RD11" pad="45"/>
<connect gate="G$1" pin="RD2" pad="50"/>
<connect gate="G$1" pin="RD3" pad="51"/>
<connect gate="G$1" pin="RD4" pad="52"/>
<connect gate="G$1" pin="RD5" pad="53"/>
<connect gate="G$1" pin="RD6" pad="54"/>
<connect gate="G$1" pin="RD7" pad="55"/>
<connect gate="G$1" pin="RD8" pad="42"/>
<connect gate="G$1" pin="RD9" pad="43"/>
<connect gate="G$1" pin="RE0" pad="60"/>
<connect gate="G$1" pin="RE1" pad="61"/>
<connect gate="G$1" pin="RE2" pad="62"/>
<connect gate="G$1" pin="RE3" pad="63"/>
<connect gate="G$1" pin="RE4" pad="64"/>
<connect gate="G$1" pin="RE5" pad="1"/>
<connect gate="G$1" pin="RE6" pad="2"/>
<connect gate="G$1" pin="RE7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF3" pad="33"/>
<connect gate="G$1" pin="RF4" pad="31"/>
<connect gate="G$1" pin="RF5" pad="32"/>
<connect gate="G$1" pin="RG2" pad="37"/>
<connect gate="G$1" pin="RG3" pad="36"/>
<connect gate="G$1" pin="RG6" pad="4"/>
<connect gate="G$1" pin="RG7" pad="5"/>
<connect gate="G$1" pin="RG8" pad="6"/>
<connect gate="G$1" pin="RG9" pad="8"/>
<connect gate="G$1" pin="TCK" pad="27"/>
<connect gate="G$1" pin="TDI" pad="28"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="23"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VDDCORE" pad="56"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24FJ256GB106-I/PT"/>
<attribute name="OC_FARNELL" value="1576868"/>
<attribute name="OC_NEWARK" value="54M5129"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ12GP202" prefix="IC">
<description>&lt;b&gt;PIC24HJ12GP202&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: PIC24HJ12GP202.bsd</description>
<gates>
<gate name="G$1" symbol="PIC24HJ12GP202"/>
</gates>
<devices>
<device name="" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="24"/>
<connect gate="G$1" pin="RA0" pad="27"/>
<connect gate="G$1" pin="RA1" pad="28"/>
<connect gate="G$1" pin="RA2" pad="6"/>
<connect gate="G$1" pin="RA3" pad="7"/>
<connect gate="G$1" pin="RA4" pad="9"/>
<connect gate="G$1" pin="RB0" pad="1"/>
<connect gate="G$1" pin="RB1" pad="2"/>
<connect gate="G$1" pin="RB12" pad="20"/>
<connect gate="G$1" pin="RB13" pad="21"/>
<connect gate="G$1" pin="RB14" pad="22"/>
<connect gate="G$1" pin="RB15" pad="23"/>
<connect gate="G$1" pin="RB2" pad="3"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="8"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="TCK" pad="14"/>
<connect gate="G$1" pin="TDI" pad="18"/>
<connect gate="G$1" pin="TDO" pad="15"/>
<connect gate="G$1" pin="TMS" pad="19"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDDCORE" pad="17"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC24HJ12GP202-I/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88K6139"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ12MC202" prefix="IC">
<description>&lt;b&gt;dsPIC33FJ12MC202&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: dsPIC33FJ12MC202.bsd</description>
<gates>
<gate name="G$1" symbol="DSPIC33FJ12MC202"/>
</gates>
<devices>
<device name="" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="24"/>
<connect gate="G$1" pin="MCLR" pad="26"/>
<connect gate="G$1" pin="RA0" pad="27"/>
<connect gate="G$1" pin="RA1" pad="28"/>
<connect gate="G$1" pin="RA2" pad="6"/>
<connect gate="G$1" pin="RA3" pad="7"/>
<connect gate="G$1" pin="RA4" pad="9"/>
<connect gate="G$1" pin="RB0" pad="1"/>
<connect gate="G$1" pin="RB1" pad="2"/>
<connect gate="G$1" pin="RB12" pad="20"/>
<connect gate="G$1" pin="RB13" pad="21"/>
<connect gate="G$1" pin="RB14" pad="22"/>
<connect gate="G$1" pin="RB15" pad="23"/>
<connect gate="G$1" pin="RB2" pad="3"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="8"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="TCK" pad="14"/>
<connect gate="G$1" pin="TDI" pad="18"/>
<connect gate="G$1" pin="TDO" pad="15"/>
<connect gate="G$1" pin="TMS" pad="19"/>
<connect gate="G$1" pin="VDD1" pad="10"/>
<connect gate="G$1" pin="VDDCORE" pad="17"/>
<connect gate="G$1" pin="VSS1" pad="5"/>
<connect gate="G$1" pin="VSS2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DSPIC33FJ12MC202-I/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88K3897"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ12GP202" prefix="IC">
<description>&lt;b&gt;dsPIC33FJ12GP202&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: dsPIC33FJ12GP202.bsd</description>
<gates>
<gate name="G$1" symbol="DSPIC33FJ12GP202"/>
</gates>
<devices>
<device name="" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="24"/>
<connect gate="G$1" pin="MCLR" pad="26"/>
<connect gate="G$1" pin="RA0" pad="27"/>
<connect gate="G$1" pin="RA1" pad="28"/>
<connect gate="G$1" pin="RA2" pad="6"/>
<connect gate="G$1" pin="RA3" pad="7"/>
<connect gate="G$1" pin="RA4" pad="9"/>
<connect gate="G$1" pin="RB0" pad="1"/>
<connect gate="G$1" pin="RB1" pad="2"/>
<connect gate="G$1" pin="RB12" pad="20"/>
<connect gate="G$1" pin="RB13" pad="21"/>
<connect gate="G$1" pin="RB14" pad="22"/>
<connect gate="G$1" pin="RB15" pad="23"/>
<connect gate="G$1" pin="RB2" pad="3"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="8"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="TCK" pad="14"/>
<connect gate="G$1" pin="TDI" pad="18"/>
<connect gate="G$1" pin="TDO" pad="15"/>
<connect gate="G$1" pin="TMS" pad="19"/>
<connect gate="G$1" pin="VDD1" pad="10"/>
<connect gate="G$1" pin="VDDCORE" pad="17"/>
<connect gate="G$1" pin="VSS1" pad="5"/>
<connect gate="G$1" pin="VSS2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DSPIC33FJ12GP202-I/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88K3892"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ128GP710" prefix="IC">
<description>&lt;b&gt;dsPIC33FJ128GP710&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: dsPIC33FJ128GP710.bsd</description>
<gates>
<gate name="G$1" symbol="DSPIC33FJ128GP710"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="MCLR" pad="13"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF6" pad="55"/>
<connect gate="G$1" pin="RF7" pad="54"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="57"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VDD3" pad="37"/>
<connect gate="G$1" pin="VDD4" pad="46"/>
<connect gate="G$1" pin="VDD5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS1" pad="75"/>
<connect gate="G$1" pin="VSS2" pad="15"/>
<connect gate="G$1" pin="VSS3" pad="36"/>
<connect gate="G$1" pin="VSS4" pad="45"/>
<connect gate="G$1" pin="VSS5" pad="65"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DSPIC33FJ128GP710-I/PF"/>
<attribute name="OC_FARNELL" value="1818690"/>
<attribute name="OC_NEWARK" value="74K4953"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ256MC510" prefix="IC">
<description>&lt;b&gt;dsPIC33FJ256MC510&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 25&lt;/i&gt;&lt;br&gt;
Source: dsPIC33FJ256MC510.bsd</description>
<gates>
<gate name="G$1" symbol="DSPIC33FJ256MC510"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="MCLR" pad="13"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF6" pad="55"/>
<connect gate="G$1" pin="RF7" pad="54"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="57"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VDD3" pad="37"/>
<connect gate="G$1" pin="VDD4" pad="46"/>
<connect gate="G$1" pin="VDD5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS1" pad="75"/>
<connect gate="G$1" pin="VSS2" pad="15"/>
<connect gate="G$1" pin="VSS3" pad="36"/>
<connect gate="G$1" pin="VSS4" pad="45"/>
<connect gate="G$1" pin="VSS5" pad="65"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DSPIC33FJ256MC510-I/PT"/>
<attribute name="OC_FARNELL" value="1332044"/>
<attribute name="OC_NEWARK" value="56K6751"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MRF24J40" prefix="IC">
<description>&lt;b&gt;IEEE 802.15.4? 2.4 GHz RF Transceiver&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39776a.pdf</description>
<gates>
<gate name="G$1" symbol="MRF24J40"/>
</gates>
<devices>
<device name="" package="QFN40ML6X6MM">
<connects>
<connect gate="G$1" pin="CLKOUT" pad="26"/>
<connect gate="G$1" pin="CS" pad="20"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="GND@3" pad="24"/>
<connect gate="G$1" pin="GND@4" pad="25"/>
<connect gate="G$1" pin="GND@5" pad="36"/>
<connect gate="G$1" pin="GPIO0" pad="7"/>
<connect gate="G$1" pin="GPIO1" pad="8"/>
<connect gate="G$1" pin="GPIO2" pad="11"/>
<connect gate="G$1" pin="GPIO3" pad="12"/>
<connect gate="G$1" pin="GPIO4" pad="10"/>
<connect gate="G$1" pin="GPIO5" pad="9"/>
<connect gate="G$1" pin="INT" pad="16"/>
<connect gate="G$1" pin="LCAP" pad="40"/>
<connect gate="G$1" pin="LPOSC1" pad="28"/>
<connect gate="G$1" pin="LPOSC2" pad="27"/>
<connect gate="G$1" pin="NC" pad="23"/>
<connect gate="G$1" pin="NC@1" pad="38"/>
<connect gate="G$1" pin="OSC1" pad="34"/>
<connect gate="G$1" pin="OSC2" pad="33"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="G$1" pin="RFN" pad="3"/>
<connect gate="G$1" pin="RFP" pad="2"/>
<connect gate="G$1" pin="RXIP" pad="29"/>
<connect gate="G$1" pin="RXQP" pad="30"/>
<connect gate="G$1" pin="SCK" pad="19"/>
<connect gate="G$1" pin="SIN" pad="18"/>
<connect gate="G$1" pin="SOUT" pad="17"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="4"/>
<connect gate="G$1" pin="VDD@2" pad="5"/>
<connect gate="G$1" pin="VDD@3" pad="21"/>
<connect gate="G$1" pin="VDD@4" pad="31"/>
<connect gate="G$1" pin="VDD@5" pad="32"/>
<connect gate="G$1" pin="VDD@6" pad="35"/>
<connect gate="G$1" pin="VDD@7" pad="37"/>
<connect gate="G$1" pin="VDD@8" pad="39"/>
<connect gate="G$1" pin="WAKE" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MRF24J40-I/ML"/>
<attribute name="OC_FARNELL" value="1436019"/>
<attribute name="OC_NEWARK" value="17M0699"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX340F*H" prefix="IC">
<description>&lt;b&gt;PIC32MX340FxxxH&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/61143E.pdf, PIC32MX320F064H.bsdl</description>
<gates>
<gate name="G$1" symbol="PIC32MX320F064H"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="RB0" pad="16"/>
<connect gate="G$1" pin="RB1" pad="15"/>
<connect gate="G$1" pin="RB14" pad="29"/>
<connect gate="G$1" pin="RB15" pad="30"/>
<connect gate="G$1" pin="RB2" pad="14"/>
<connect gate="G$1" pin="RB3" pad="13"/>
<connect gate="G$1" pin="RB4" pad="12"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="17"/>
<connect gate="G$1" pin="RB7" pad="18"/>
<connect gate="G$1" pin="RB8" pad="21"/>
<connect gate="G$1" pin="RB9" pad="22"/>
<connect gate="G$1" pin="RC12" pad="39"/>
<connect gate="G$1" pin="RC13" pad="47"/>
<connect gate="G$1" pin="RC14" pad="48"/>
<connect gate="G$1" pin="RC15" pad="40"/>
<connect gate="G$1" pin="RD0" pad="46"/>
<connect gate="G$1" pin="RD1" pad="49"/>
<connect gate="G$1" pin="RD10" pad="44"/>
<connect gate="G$1" pin="RD11" pad="45"/>
<connect gate="G$1" pin="RD2" pad="50"/>
<connect gate="G$1" pin="RD3" pad="51"/>
<connect gate="G$1" pin="RD4" pad="52"/>
<connect gate="G$1" pin="RD5" pad="53"/>
<connect gate="G$1" pin="RD6" pad="54"/>
<connect gate="G$1" pin="RD7" pad="55"/>
<connect gate="G$1" pin="RD8" pad="42"/>
<connect gate="G$1" pin="RD9" pad="43"/>
<connect gate="G$1" pin="RE0" pad="60"/>
<connect gate="G$1" pin="RE1" pad="61"/>
<connect gate="G$1" pin="RE2" pad="62"/>
<connect gate="G$1" pin="RE3" pad="63"/>
<connect gate="G$1" pin="RE4" pad="64"/>
<connect gate="G$1" pin="RE5" pad="1"/>
<connect gate="G$1" pin="RE6" pad="2"/>
<connect gate="G$1" pin="RE7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF2" pad="34"/>
<connect gate="G$1" pin="RF3" pad="33"/>
<connect gate="G$1" pin="RF4" pad="31"/>
<connect gate="G$1" pin="RF5" pad="32"/>
<connect gate="G$1" pin="RF6" pad="35"/>
<connect gate="G$1" pin="RG2" pad="37"/>
<connect gate="G$1" pin="RG3" pad="36"/>
<connect gate="G$1" pin="RG6" pad="4"/>
<connect gate="G$1" pin="RG7" pad="5"/>
<connect gate="G$1" pin="RG8" pad="6"/>
<connect gate="G$1" pin="RG9" pad="8"/>
<connect gate="G$1" pin="TCK" pad="27"/>
<connect gate="G$1" pin="TDI" pad="28"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="23"/>
<connect gate="G$1" pin="VDD@2" pad="10"/>
<connect gate="G$1" pin="VDD@3" pad="26"/>
<connect gate="G$1" pin="VDD@5" pad="38"/>
<connect gate="G$1" pin="VDDCORE" pad="56"/>
<connect gate="G$1" pin="VREG" pad="57"/>
<connect gate="G$1" pin="VSS@2" pad="9"/>
<connect gate="G$1" pin="VSS@3" pad="25"/>
<connect gate="G$1" pin="VSS@5" pad="41"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX340F128H-80I/PT"/>
<attribute name="OC_FARNELL" value="1677914"/>
<attribute name="OC_NEWARK" value="98M1929"/>
</technology>
<technology name="256">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX340F256H-80I/PT"/>
<attribute name="OC_FARNELL" value="1523322"/>
<attribute name="OC_NEWARK" value="77M3150"/>
</technology>
<technology name="512">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC32MX340F512H-80I/PT"/>
<attribute name="OC_FARNELL" value="1677915"/>
<attribute name="OC_NEWARK" value="98M1931"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F62*" prefix="IC">
<description>&lt;b&gt;FLASH-Based 8-Bit CMOS Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/40300C.pdf</description>
<gates>
<gate name="PIC16F62*" symbol="PIC16F62*"/>
</gates>
<devices>
<device name="-I/SO" package="SO-18W">
<connects>
<connect gate="PIC16F62*" pin="RA0/AN0" pad="17"/>
<connect gate="PIC16F62*" pin="RA1/AN1" pad="18"/>
<connect gate="PIC16F62*" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="PIC16F62*" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="PIC16F62*" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="PIC16F62*" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="PIC16F62*" pin="RA6/OSC2/CLKOUT" pad="15"/>
<connect gate="PIC16F62*" pin="RA7/OSC1/CLKIN" pad="16"/>
<connect gate="PIC16F62*" pin="RB0/INT" pad="6"/>
<connect gate="PIC16F62*" pin="RB1/RX/DT" pad="7"/>
<connect gate="PIC16F62*" pin="RB2/TX/CK" pad="8"/>
<connect gate="PIC16F62*" pin="RB3/CCP1" pad="9"/>
<connect gate="PIC16F62*" pin="RB4/PGM" pad="10"/>
<connect gate="PIC16F62*" pin="RB5" pad="11"/>
<connect gate="PIC16F62*" pin="RB6/T1OSO/T1CKI/PGC" pad="12"/>
<connect gate="PIC16F62*" pin="RB7/T1OSI/PGD" pad="13"/>
<connect gate="PIC16F62*" pin="VDD" pad="14"/>
<connect gate="PIC16F62*" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F627-04I/SO"/>
<attribute name="OC_FARNELL" value="9760296"/>
<attribute name="OC_NEWARK" value="19C7271"/>
</technology>
<technology name="8">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F628-20I/SO"/>
<attribute name="OC_FARNELL" value="9760415"/>
<attribute name="OC_NEWARK" value="23C4986"/>
</technology>
</technologies>
</device>
<device name="-I/P" package="DIL18">
<connects>
<connect gate="PIC16F62*" pin="RA0/AN0" pad="17"/>
<connect gate="PIC16F62*" pin="RA1/AN1" pad="18"/>
<connect gate="PIC16F62*" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="PIC16F62*" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="PIC16F62*" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="PIC16F62*" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="PIC16F62*" pin="RA6/OSC2/CLKOUT" pad="15"/>
<connect gate="PIC16F62*" pin="RA7/OSC1/CLKIN" pad="16"/>
<connect gate="PIC16F62*" pin="RB0/INT" pad="6"/>
<connect gate="PIC16F62*" pin="RB1/RX/DT" pad="7"/>
<connect gate="PIC16F62*" pin="RB2/TX/CK" pad="8"/>
<connect gate="PIC16F62*" pin="RB3/CCP1" pad="9"/>
<connect gate="PIC16F62*" pin="RB4/PGM" pad="10"/>
<connect gate="PIC16F62*" pin="RB5" pad="11"/>
<connect gate="PIC16F62*" pin="RB6/T1OSO/T1CKI/PGC" pad="12"/>
<connect gate="PIC16F62*" pin="RB7/T1OSI/PGD" pad="13"/>
<connect gate="PIC16F62*" pin="VDD" pad="14"/>
<connect gate="PIC16F62*" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="7">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F627-04/P"/>
<attribute name="OC_FARNELL" value="1084298"/>
<attribute name="OC_NEWARK" value="23C4960"/>
</technology>
<technology name="8">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F628-04I/P"/>
<attribute name="OC_FARNELL" value="9760407"/>
<attribute name="OC_NEWARK" value="19C7272"/>
</technology>
</technologies>
</device>
<device name="-I/SS" package="SSOP20">
<connects>
<connect gate="PIC16F62*" pin="RA0/AN0" pad="19"/>
<connect gate="PIC16F62*" pin="RA1/AN1" pad="20"/>
<connect gate="PIC16F62*" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="PIC16F62*" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="PIC16F62*" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="PIC16F62*" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="PIC16F62*" pin="RA6/OSC2/CLKOUT" pad="17"/>
<connect gate="PIC16F62*" pin="RA7/OSC1/CLKIN" pad="18"/>
<connect gate="PIC16F62*" pin="RB0/INT" pad="7"/>
<connect gate="PIC16F62*" pin="RB1/RX/DT" pad="8"/>
<connect gate="PIC16F62*" pin="RB2/TX/CK" pad="9"/>
<connect gate="PIC16F62*" pin="RB3/CCP1" pad="10"/>
<connect gate="PIC16F62*" pin="RB4/PGM" pad="11"/>
<connect gate="PIC16F62*" pin="RB5" pad="12"/>
<connect gate="PIC16F62*" pin="RB6/T1OSO/T1CKI/PGC" pad="13"/>
<connect gate="PIC16F62*" pin="RB7/T1OSI/PGD" pad="14"/>
<connect gate="PIC16F62*" pin="VDD" pad="15 16"/>
<connect gate="PIC16F62*" pin="VSS" pad="5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-I/ML" package="QFN28-ML_6X6MM">
<connects>
<connect gate="PIC16F62*" pin="RA0/AN0" pad="23"/>
<connect gate="PIC16F62*" pin="RA1/AN1" pad="24"/>
<connect gate="PIC16F62*" pin="RA2/AN2/VREF" pad="26"/>
<connect gate="PIC16F62*" pin="RA3/AN3/CMP1" pad="27"/>
<connect gate="PIC16F62*" pin="RA4/TOCKI/CMP2" pad="28"/>
<connect gate="PIC16F62*" pin="RA5/MCLR/VPP" pad="1"/>
<connect gate="PIC16F62*" pin="RA6/OSC2/CLKOUT" pad="20"/>
<connect gate="PIC16F62*" pin="RA7/OSC1/CLKIN" pad="21"/>
<connect gate="PIC16F62*" pin="RB0/INT" pad="7"/>
<connect gate="PIC16F62*" pin="RB1/RX/DT" pad="8"/>
<connect gate="PIC16F62*" pin="RB2/TX/CK" pad="9"/>
<connect gate="PIC16F62*" pin="RB3/CCP1" pad="10"/>
<connect gate="PIC16F62*" pin="RB4/PGM" pad="12"/>
<connect gate="PIC16F62*" pin="RB5" pad="13"/>
<connect gate="PIC16F62*" pin="RB6/T1OSO/T1CKI/PGC" pad="15"/>
<connect gate="PIC16F62*" pin="RB7/T1OSI/PGD" pad="16"/>
<connect gate="PIC16F62*" pin="VDD" pad="17 19"/>
<connect gate="PIC16F62*" pin="VSS" pad="3 5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F628SS" prefix="IC">
<description>&lt;b&gt;FLASH-Based 8-Bit CMOS Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/40300C.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F62-SSOP"/>
</gates>
<devices>
<device name="" package="SS20">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/VREF" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/CMP1" pad="2"/>
<connect gate="G$1" pin="RA4/TOCKI/CMP2" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR/VPP" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="17"/>
<connect gate="G$1" pin="RA7/OSC1/CLKIN" pad="18"/>
<connect gate="G$1" pin="RB0/INT" pad="7"/>
<connect gate="G$1" pin="RB1/RX/DT" pad="8"/>
<connect gate="G$1" pin="RB2/TX/CK" pad="9"/>
<connect gate="G$1" pin="RB3/CCP1" pad="10"/>
<connect gate="G$1" pin="RB4/PGM" pad="11"/>
<connect gate="G$1" pin="RB5" pad="12"/>
<connect gate="G$1" pin="RB6/T1OSO/T1CKI/PGC" pad="13"/>
<connect gate="G$1" pin="RB7/T1OSI/PGD" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F628-20I/SS"/>
<attribute name="OC_FARNELL" value="1084266"/>
<attribute name="OC_NEWARK" value="23C4987"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F688" prefix="IC">
<description>&lt;b&gt;14-Pin Flash-Based, 8-Bit CMOS Microcontrollers with nanoWatt Technology&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41203E.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F688"/>
<gate name="EXP" symbol="EXPOSED"/>
</gates>
<devices>
<device name="" package="QFN16-4X4">
<connects>
<connect gate="EXP" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="RA0/AN0/C1IN+/ICSPDAT/ULPWU" pad="12"/>
<connect gate="G$1" pin="RA1/AN1/C1IN-/VREF/ICSPCLK" pad="11"/>
<connect gate="G$1" pin="RA2/AN2/T0CKI/INT/C1OUT" pad="10"/>
<connect gate="G$1" pin="RA3/!MCLR!/VPP" pad="3"/>
<connect gate="G$1" pin="RA4/AN3/!T1G!/OSC2/CLKOUT" pad="2"/>
<connect gate="G$1" pin="RA5/T1CKI/OSC1/CLKIN" pad="1"/>
<connect gate="G$1" pin="RC0/AN4/C2IN+" pad="9"/>
<connect gate="G$1" pin="RC1/AN5/C2IN" pad="8"/>
<connect gate="G$1" pin="RC2/AN6" pad="7"/>
<connect gate="G$1" pin="RC3/AN7" pad="6"/>
<connect gate="G$1" pin="RC4/C2OUT/TX/CK" pad="5"/>
<connect gate="G$1" pin="RC5/RX/DT" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F688-I/ML"/>
<attribute name="OC_FARNELL" value="1579588"/>
<attribute name="OC_NEWARK" value="56K7280"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F193*" prefix="IC">
<description>&lt;b&gt;Flash-Based, 8-Bit CMOS Microcontrollers wtih LCD Driver and nanoWatt XLP Technology&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41364D.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F1934/7/9"/>
</gates>
<devices>
<device name="PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="COM0/CPS4/AN11/RB4" pad="14"/>
<connect gate="G$1" pin="COM1/T1G/P3A/CCP3/CPS5/AN13/RB5" pad="15"/>
<connect gate="G$1" pin="COM2/DACOUT/VREF-/C2IN+/AN2/RA2" pad="21"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="33"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="RA4/C1OUT/CPS6/T0CKI/SRQ/SEG4" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/CPS7/SRNQ/!SS!/VCAP/SEG5" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT/VCAP/SEG1" pad="31"/>
<connect gate="G$1" pin="RA7/OSC1/CLKIN/SEG2" pad="30"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI/P2B" pad="32"/>
<connect gate="G$1" pin="RC1/T1OSI/CCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1/P1A/SEG3" pad="36"/>
<connect gate="G$1" pin="RC3/SCL/SCK/SEG6" pad="37"/>
<connect gate="G$1" pin="RC4/SDI/SDA/T1G/SEG11" pad="42"/>
<connect gate="G$1" pin="RC5/SDO/SEG10" pad="43"/>
<connect gate="G$1" pin="RC6/TX/CK/SEG9" pad="44"/>
<connect gate="G$1" pin="RD0/CPS8/COM3" pad="38"/>
<connect gate="G$1" pin="RD1/CPS9/CCP4" pad="39"/>
<connect gate="G$1" pin="RD2/CPS10/P2B" pad="40"/>
<connect gate="G$1" pin="RD3/CPS11/P2C/SEG16" pad="41"/>
<connect gate="G$1" pin="RE0/AN5/CCP3/P3A/SEG21" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/P3B/SEG22" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/CCP5/SEG23" pad="27"/>
<connect gate="G$1" pin="SEG0/INT/SRI/CPS0/AN12/RB0" pad="8"/>
<connect gate="G$1" pin="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0" pad="19"/>
<connect gate="G$1" pin="SEG13/ICDDAT/ICSPDAT/RB7" pad="17"/>
<connect gate="G$1" pin="SEG14/ICDCLK/ICSPCLK/RB6" pad="16"/>
<connect gate="G$1" pin="SEG15/VREF+/C1IN+/AN3/RA3" pad="22"/>
<connect gate="G$1" pin="SEG17/P2D/CPS12/RD4" pad="2"/>
<connect gate="G$1" pin="SEG18/P1B/CPS13/RD5" pad="3"/>
<connect gate="G$1" pin="SEG19/P1C/CPS14/RD6" pad="4"/>
<connect gate="G$1" pin="SEG20/P1D/CPS15/RD7" pad="5"/>
<connect gate="G$1" pin="SEG7/C12IN1-/AN1/RA1" pad="20"/>
<connect gate="G$1" pin="SEG8/DT/RX/RC7" pad="1"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VLCD1/CPS1/C12IN3-/AN10/RB1" pad="9"/>
<connect gate="G$1" pin="VLCD2/CPS2/AN8/RB2" pad="10"/>
<connect gate="G$1" pin="VLCD3/P2A/CCP2/CPS3/C12IN2-/AN9/RB3" pad="11"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="18"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1934-I/PT"/>
<attribute name="OC_FARNELL" value="1755818"/>
<attribute name="OC_NEWARK" value="34R4514"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1937-I/PT"/>
<attribute name="OC_FARNELL" value="1755826"/>
<attribute name="OC_NEWARK" value="34R4521"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1939-I/PT"/>
<attribute name="OC_FARNELL" value="1755834"/>
<attribute name="OC_NEWARK" value="08R1959"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F19*" prefix="IC">
<description>&lt;b&gt;Flash-Based, 8-Bit CMOS Microcontrollers wtih LCD Driver and nanoWatt XLP Technology&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41364D.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F1933/1936/1938"/>
</gates>
<devices>
<device name="SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="COM2/DACOUT/VREF-/C2IN+/AN2/RA2" pad="4"/>
<connect gate="G$1" pin="P2A/CCP2/T1OSI/RC1" pad="12"/>
<connect gate="G$1" pin="P2B/T1CKI/T1OSO/RC0" pad="11"/>
<connect gate="G$1" pin="RB0/AN12/CPS0/CCP4/SRI/INT/SEG0" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/C12IN3-/CPS1/P1C/VLCD1" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/CPS2/P1B/VLCD2" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3" pad="24"/>
<connect gate="G$1" pin="RB4/AN11/CPS4/P1D/COM0" pad="25"/>
<connect gate="G$1" pin="RB5/AN13/CPS5/P2B/CCP3/P3A/T1G/COM1" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK/SEG14" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="28"/>
<connect gate="G$1" pin="RC4/SDI/SDA/T1G/SEG11" pad="15"/>
<connect gate="G$1" pin="RC5/SDO/SEG10" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK/CCP3/P3A/SEG9" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/P3B/SEG8" pad="18"/>
<connect gate="G$1" pin="SEG1/VCAP/CLKOUT/OSC2/RA6" pad="10"/>
<connect gate="G$1" pin="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0" pad="2"/>
<connect gate="G$1" pin="SEG15/COM3/VREF+/C1IN+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="SEG2/CLKIN/OSC1/RA7" pad="9"/>
<connect gate="G$1" pin="SEG3/P1A/CCP1/RC2" pad="13"/>
<connect gate="G$1" pin="SEG4/CCP5/SRQ/T0CKI/CPS6/C1OUT/RA4" pad="6"/>
<connect gate="G$1" pin="SEG5/VCAP/SS/SRNQ/CPS7/C2OUT/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="SEG6/SCL/SCK/RC3" pad="14"/>
<connect gate="G$1" pin="SEG7/C12IN1-/AN1/RA1" pad="3"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1933-I/SP"/>
<attribute name="OC_FARNELL" value="1755814"/>
<attribute name="OC_NEWARK" value="08R1938"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1936-I/SP"/>
<attribute name="OC_FARNELL" value="1755822"/>
<attribute name="OC_NEWARK" value="45P4765"/>
</technology>
<technology name="38">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1938-I/SP"/>
<attribute name="OC_FARNELL" value="1755829"/>
<attribute name="OC_NEWARK" value="08R1949"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="COM2/DACOUT/VREF-/C2IN+/AN2/RA2" pad="4"/>
<connect gate="G$1" pin="P2A/CCP2/T1OSI/RC1" pad="12"/>
<connect gate="G$1" pin="P2B/T1CKI/T1OSO/RC0" pad="11"/>
<connect gate="G$1" pin="RB0/AN12/CPS0/CCP4/SRI/INT/SEG0" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/C12IN3-/CPS1/P1C/VLCD1" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/CPS2/P1B/VLCD2" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3" pad="24"/>
<connect gate="G$1" pin="RB4/AN11/CPS4/P1D/COM0" pad="25"/>
<connect gate="G$1" pin="RB5/AN13/CPS5/P2B/CCP3/P3A/T1G/COM1" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK/SEG14" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="28"/>
<connect gate="G$1" pin="RC4/SDI/SDA/T1G/SEG11" pad="15"/>
<connect gate="G$1" pin="RC5/SDO/SEG10" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK/CCP3/P3A/SEG9" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/P3B/SEG8" pad="18"/>
<connect gate="G$1" pin="SEG1/VCAP/CLKOUT/OSC2/RA6" pad="10"/>
<connect gate="G$1" pin="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0" pad="2"/>
<connect gate="G$1" pin="SEG15/COM3/VREF+/C1IN+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="SEG2/CLKIN/OSC1/RA7" pad="9"/>
<connect gate="G$1" pin="SEG3/P1A/CCP1/RC2" pad="13"/>
<connect gate="G$1" pin="SEG4/CCP5/SRQ/T0CKI/CPS6/C1OUT/RA4" pad="6"/>
<connect gate="G$1" pin="SEG5/VCAP/SS/SRNQ/CPS7/C2OUT/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="SEG6/SCL/SCK/RC3" pad="14"/>
<connect gate="G$1" pin="SEG7/C12IN1-/AN1/RA1" pad="3"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1933-I/SO"/>
<attribute name="OC_FARNELL" value="1755812"/>
<attribute name="OC_NEWARK" value="08R1937"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1936-I/SO"/>
<attribute name="OC_FARNELL" value="1755819"/>
<attribute name="OC_NEWARK" value="34R4516"/>
</technology>
<technology name="38">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1938-I/SO"/>
<attribute name="OC_FARNELL" value="1755828"/>
<attribute name="OC_NEWARK" value="08R1948"/>
</technology>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="COM2/DACOUT/VREF-/C2IN+/AN2/RA2" pad="4"/>
<connect gate="G$1" pin="P2A/CCP2/T1OSI/RC1" pad="12"/>
<connect gate="G$1" pin="P2B/T1CKI/T1OSO/RC0" pad="11"/>
<connect gate="G$1" pin="RB0/AN12/CPS0/CCP4/SRI/INT/SEG0" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/C12IN3-/CPS1/P1C/VLCD1" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/CPS2/P1B/VLCD2" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3" pad="24"/>
<connect gate="G$1" pin="RB4/AN11/CPS4/P1D/COM0" pad="25"/>
<connect gate="G$1" pin="RB5/AN13/CPS5/P2B/CCP3/P3A/T1G/COM1" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK/SEG14" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="28"/>
<connect gate="G$1" pin="RC4/SDI/SDA/T1G/SEG11" pad="15"/>
<connect gate="G$1" pin="RC5/SDO/SEG10" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK/CCP3/P3A/SEG9" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/P3B/SEG8" pad="18"/>
<connect gate="G$1" pin="SEG1/VCAP/CLKOUT/OSC2/RA6" pad="10"/>
<connect gate="G$1" pin="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0" pad="2"/>
<connect gate="G$1" pin="SEG15/COM3/VREF+/C1IN+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="SEG2/CLKIN/OSC1/RA7" pad="9"/>
<connect gate="G$1" pin="SEG3/P1A/CCP1/RC2" pad="13"/>
<connect gate="G$1" pin="SEG4/CCP5/SRQ/T0CKI/CPS6/C1OUT/RA4" pad="6"/>
<connect gate="G$1" pin="SEG5/VCAP/SS/SRNQ/CPS7/C2OUT/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="SEG6/SCL/SCK/RC3" pad="14"/>
<connect gate="G$1" pin="SEG7/C12IN1-/AN1/RA1" pad="3"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1933T-I/SS"/>
<attribute name="OC_FARNELL" value="1755815"/>
<attribute name="OC_NEWARK" value="08R1942"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1936-E/SS"/>
<attribute name="OC_FARNELL" value="1755823"/>
<attribute name="OC_NEWARK" value="45P4762"/>
</technology>
<technology name="38">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1938-E/SS"/>
<attribute name="OC_FARNELL" value="1755830"/>
<attribute name="OC_NEWARK" value="08R1946"/>
</technology>
</technologies>
</device>
<device name="QF" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="COM2/DACOUT/VREF-/C2IN+/AN2/RA2" pad="1"/>
<connect gate="G$1" pin="P2A/CCP2/T1OSI/RC1" pad="9"/>
<connect gate="G$1" pin="P2B/T1CKI/T1OSO/RC0" pad="8"/>
<connect gate="G$1" pin="RB0/AN12/CPS0/CCP4/SRI/INT/SEG0" pad="18"/>
<connect gate="G$1" pin="RB1/AN10/C12IN3-/CPS1/P1C/VLCD1" pad="19"/>
<connect gate="G$1" pin="RB2/AN8/CPS2/P1B/VLCD2" pad="20"/>
<connect gate="G$1" pin="RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3" pad="21"/>
<connect gate="G$1" pin="RB4/AN11/CPS4/P1D/COM0" pad="22"/>
<connect gate="G$1" pin="RB5/AN13/CPS5/P2B/CCP3/P3A/T1G/COM1" pad="23"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK/SEG14" pad="24"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="25"/>
<connect gate="G$1" pin="RC4/SDI/SDA/T1G/SEG11" pad="12"/>
<connect gate="G$1" pin="RC5/SDO/SEG10" pad="13"/>
<connect gate="G$1" pin="RC6/TX/CK/CCP3/P3A/SEG9" pad="14"/>
<connect gate="G$1" pin="RC7/RX/DT/P3B/SEG8" pad="15"/>
<connect gate="G$1" pin="SEG1/VCAP/CLKOUT/OSC2/RA6" pad="7"/>
<connect gate="G$1" pin="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0" pad="27"/>
<connect gate="G$1" pin="SEG15/COM3/VREF+/C1IN+/AN3/RA3" pad="2"/>
<connect gate="G$1" pin="SEG2/CLKIN/OSC1/RA7" pad="6"/>
<connect gate="G$1" pin="SEG3/P1A/CCP1/RC2" pad="10"/>
<connect gate="G$1" pin="SEG4/CCP5/SRQ/T0CKI/CPS6/C1OUT/RA4" pad="3"/>
<connect gate="G$1" pin="SEG5/VCAP/SS/SRNQ/CPS7/C2OUT/AN4/RA5" pad="4"/>
<connect gate="G$1" pin="SEG6/SCL/SCK/RC3" pad="11"/>
<connect gate="G$1" pin="SEG7/C12IN1-/AN1/RA1" pad="28"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="26"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="16"/>
</connects>
<technologies>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1933-I/ML"/>
<attribute name="OC_FARNELL" value="1755812"/>
<attribute name="OC_NEWARK" value="08R1936"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1936-I/ML"/>
<attribute name="OC_FARNELL" value="1755819"/>
<attribute name="OC_NEWARK" value="34R4515"/>
</technology>
<technology name="38">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1938-E/ML"/>
<attribute name="OC_FARNELL" value="1755827"/>
<attribute name="OC_NEWARK" value="08R1943"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F193*?" prefix="IC">
<description>&lt;b&gt;Flash-Based, 8-Bit CMOS Microcontrollers wtih LCD Driver and nanoWatt XLP Technology&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41364D.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16LF1934/7/9"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="CCP4/CPS9/RD1" pad="20"/>
<connect gate="G$1" pin="COM2/DACOUT/VREF-/C2IN+/AN2/RA2" pad="4"/>
<connect gate="G$1" pin="COM3/CPS8/RD0" pad="19"/>
<connect gate="G$1" pin="P2A/CCP2/T1OSI/RC1" pad="16"/>
<connect gate="G$1" pin="P2B/T1CKI/T1OSO/RC0" pad="15"/>
<connect gate="G$1" pin="RB0/AN12/CPS0/SRI/INT/SEG0" pad="33"/>
<connect gate="G$1" pin="RB1/AN10/C12IN3-/CPS1/VLCD1" pad="34"/>
<connect gate="G$1" pin="RB2/AN8/CPS2/VLCD2" pad="35"/>
<connect gate="G$1" pin="RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3" pad="36"/>
<connect gate="G$1" pin="RB4/AN11/CPS4/COM0" pad="37"/>
<connect gate="G$1" pin="RB5/AN13/CPS5/CCP3/P3A/T1G/COM1" pad="38"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK/SEG14" pad="40"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="39"/>
<connect gate="G$1" pin="RC4/SDI/SDA/T1G/SEG11" pad="23"/>
<connect gate="G$1" pin="RC5/SDO/SEG10" pad="24"/>
<connect gate="G$1" pin="RC6/TX/CK/SEG9" pad="25"/>
<connect gate="G$1" pin="RC7/RX/DT/SEG8" pad="26"/>
<connect gate="G$1" pin="RD2/CPS10/P2B" pad="21"/>
<connect gate="G$1" pin="RD3/CPS11/P2C/SEG16" pad="22"/>
<connect gate="G$1" pin="RD4/CPS12/P2D/SEG17" pad="27"/>
<connect gate="G$1" pin="RD5/CPS13/P1B/SEG18" pad="28"/>
<connect gate="G$1" pin="RD6/CPS14/P1C/SEG19" pad="29"/>
<connect gate="G$1" pin="RD7/CPS15/P1D/SEG20" pad="30"/>
<connect gate="G$1" pin="SEG1/VCAP/CLKOUT/OSC2/RA6" pad="14"/>
<connect gate="G$1" pin="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0" pad="2"/>
<connect gate="G$1" pin="SEG15/VREF+/C1IN+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="SEG2/CLKIN/OSC1/RA7" pad="13"/>
<connect gate="G$1" pin="SEG21/CCP3/P3A/AN5/RE0" pad="8"/>
<connect gate="G$1" pin="SEG22/P3B/AN6/RE1" pad="9"/>
<connect gate="G$1" pin="SEG23/CCP5/AN7/RE2" pad="10"/>
<connect gate="G$1" pin="SEG3/P1A/CCP1/RC2" pad="17"/>
<connect gate="G$1" pin="SEG4/SRQ/T0CKI/CPS6/C1OUT/RA4" pad="6"/>
<connect gate="G$1" pin="SEG5/VCAP/!SS!/SRNQ/CPS7/C2OUT/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="SEG6/SCK/SCL/RC3" pad="18"/>
<connect gate="G$1" pin="SEG7/C12IN1-/AN1/RA1" pad="3"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1934-I/P"/>
<attribute name="OC_FARNELL" value="1755817"/>
<attribute name="OC_NEWARK" value="45P4755"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1937-I/P"/>
<attribute name="OC_FARNELL" value="1755825"/>
<attribute name="OC_NEWARK" value="45P4774"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1939-I/P"/>
<attribute name="OC_FARNELL" value="1755832"/>
<attribute name="OC_NEWARK" value="08R1958"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F193*ML" prefix="IC">
<description>&lt;b&gt;Flash-Based, 8-Bit CMOS Microcontrollers wtih LCD Driver and nanoWatt XLP Technology&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41364D.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F1934/7/9-QFN44"/>
</gates>
<devices>
<device name="" package="QFN44ML8X8">
<connects>
<connect gate="G$1" pin="COM0/CPS4/AN11/RB4" pad="14"/>
<connect gate="G$1" pin="COM1/T1G/P3A/CCP3/CPS5/AN13/RB5" pad="15"/>
<connect gate="G$1" pin="COM2/DACOUT/VREF-/C2IN+/AN2/RA2" pad="21"/>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="NC@1" pad="29"/>
<connect gate="G$1" pin="RA4/C1OUT/CPS6/T0CKI/SRQ/SEG4" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/CPS7/SRNQ/!SS!/VCAP/SEG5" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT/VCAP/SEG1" pad="33"/>
<connect gate="G$1" pin="RA7/OSC1/CLKIN/SEG2" pad="32"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI/P2B" pad="34"/>
<connect gate="G$1" pin="RC1/T1OSI/CCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1/P1A/SEG3" pad="36"/>
<connect gate="G$1" pin="RC3/SCL/SCK/SEG6" pad="37"/>
<connect gate="G$1" pin="RC4/SDI/SDA/T1G/SEG11" pad="42"/>
<connect gate="G$1" pin="RC5/SDO/SEG10" pad="43"/>
<connect gate="G$1" pin="RC6/TX/CK/SEG9" pad="44"/>
<connect gate="G$1" pin="RD0/CPS8/COM3" pad="38"/>
<connect gate="G$1" pin="RD1/CPS9/CCP4" pad="39"/>
<connect gate="G$1" pin="RD2/CPS10/P2B" pad="40"/>
<connect gate="G$1" pin="RD3/CPS11/P2C/SEG16" pad="41"/>
<connect gate="G$1" pin="RE0/AN5/CCP3/P3A/SEG21" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/P3B/SEG22" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/CCP5/SEG23" pad="27"/>
<connect gate="G$1" pin="SEG0/INT/SRI/CPS0/AN12/RB0" pad="9"/>
<connect gate="G$1" pin="SEG12/VCAP/SS/SRNQ/C2OUT/C12IN0-/AN0/RA0" pad="19"/>
<connect gate="G$1" pin="SEG13/ICDDAT/ICSPDAT/RB7" pad="17"/>
<connect gate="G$1" pin="SEG14/ICDCLK/ICSPCLK/RB6" pad="16"/>
<connect gate="G$1" pin="SEG15/VREF+/C1IN+/AN3/RA3" pad="22"/>
<connect gate="G$1" pin="SEG17/P2D/CPS12/RD4" pad="2"/>
<connect gate="G$1" pin="SEG18/P1B/CPS13/RD5" pad="3"/>
<connect gate="G$1" pin="SEG19/P1C/CPS14/RD6" pad="4"/>
<connect gate="G$1" pin="SEG20/P1D/CPS15/RD7" pad="5"/>
<connect gate="G$1" pin="SEG7/C12IN1-/AN1/RA1" pad="20"/>
<connect gate="G$1" pin="SEG8/DT/RX/RC7" pad="1"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VDD@2" pad="8"/>
<connect gate="G$1" pin="VLCD1/CPS1/C12IN3-/AN10/RB1" pad="10"/>
<connect gate="G$1" pin="VLCD2/CPS2/AN8/RB2" pad="11"/>
<connect gate="G$1" pin="VLCD3/P2A/CCP2/CPS3/C12IN2-/AN9/RB3" pad="12"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="18"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="30"/>
<connect gate="G$1" pin="VSS@2" pad="31"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1934-I/ML"/>
<attribute name="OC_FARNELL" value="1755816"/>
<attribute name="OC_NEWARK" value="34R4512"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1937-I/ML"/>
<attribute name="OC_FARNELL" value="1755824"/>
<attribute name="OC_NEWARK" value="34R4519"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F1939-I/ML"/>
<attribute name="OC_FARNELL" value="1755831"/>
<attribute name="OC_NEWARK" value="08R1957"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2*J53" prefix="IC">
<description>&lt;b&gt;PIC18F47J53 Family&lt;/b&gt; High-Performance USB Microcontrollers with nanoWatt XLP Technology&lt;p&gt;
Source: &lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/39964B.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="PIC18F27J53_28"/>
</gates>
<devices>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="10"/>
<connect gate="G$1" pin="RA0/AN0/C1INA/ULPWU/RP0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/C2INA/VBG/RP1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/C1INB/VREF+" pad="5"/>
<connect gate="G$1" pin="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2" pad="7"/>
<connect gate="G$1" pin="RB0/AN12/C3IND/INT0/RP3" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/C3INC/RTCC/RP4" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/C3INA/CTED2/VPO/RP6" pad="24"/>
<connect gate="G$1" pin="RB4/CCP4/KBI0/SCK1/SCL1/RP7" pad="25"/>
<connect gate="G$1" pin="RB5/CCP5/KBI1/SDI1/SDA1/RP8" pad="26"/>
<connect gate="G$1" pin="RB6/CCP6/KBI2/PGC/RP9" pad="27"/>
<connect gate="G$1" pin="RB7/CCP7/KBI3/PGD/RP10" pad="28"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI/RP11" pad="11"/>
<connect gate="G$1" pin="RC1/CCP8/T1OSI/!UOE!/RP12" pad="12"/>
<connect gate="G$1" pin="RC2/AN11/C2IND/CTPLS/RP13" pad="13"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="15"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="16"/>
<connect gate="G$1" pin="RC6/CCP9/TX1/CK1/RP17" pad="17"/>
<connect gate="G$1" pin="RC7/CCP10/RX1/DT1/SDO1/RP18" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="6"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="10"/>
<connect gate="G$1" pin="RA0/AN0/C1INA/ULPWU/RP0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/C2INA/VBG/RP1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/C1INB/VREF+" pad="5"/>
<connect gate="G$1" pin="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2" pad="7"/>
<connect gate="G$1" pin="RB0/AN12/C3IND/INT0/RP3" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/C3INC/RTCC/RP4" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/C3INA/CTED2/VPO/RP6" pad="24"/>
<connect gate="G$1" pin="RB4/CCP4/KBI0/SCK1/SCL1/RP7" pad="25"/>
<connect gate="G$1" pin="RB5/CCP5/KBI1/SDI1/SDA1/RP8" pad="26"/>
<connect gate="G$1" pin="RB6/CCP6/KBI2/PGC/RP9" pad="27"/>
<connect gate="G$1" pin="RB7/CCP7/KBI3/PGD/RP10" pad="28"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI/RP11" pad="11"/>
<connect gate="G$1" pin="RC1/CCP8/T1OSI/!UOE!/RP12" pad="12"/>
<connect gate="G$1" pin="RC2/AN11/C2IND/CTPLS/RP13" pad="13"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="15"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="16"/>
<connect gate="G$1" pin="RC6/CCP9/TX1/CK1/RP17" pad="17"/>
<connect gate="G$1" pin="RC7/CCP10/RX1/DT1/SDO1/RP18" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="6"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F26J53-I/SO"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="63R7830"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F27J53-I/SO"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="63R7838"/>
</technology>
</technologies>
</device>
<device name="ML" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="26"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="6"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="7"/>
<connect gate="G$1" pin="RA0/AN0/C1INA/ULPWU/RP0" pad="27"/>
<connect gate="G$1" pin="RA1/AN1/C2INA/VBG/RP1" pad="28"/>
<connect gate="G$1" pin="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/C1INB/VREF+" pad="2"/>
<connect gate="G$1" pin="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2" pad="4"/>
<connect gate="G$1" pin="RB0/AN12/C3IND/INT0/RP3" pad="18"/>
<connect gate="G$1" pin="RB1/AN10/C3INC/RTCC/RP4" pad="19"/>
<connect gate="G$1" pin="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5" pad="20"/>
<connect gate="G$1" pin="RB3/AN9/C3INA/CTED2/VPO/RP6" pad="21"/>
<connect gate="G$1" pin="RB4/CCP4/KBI0/SCK1/SCL1/RP7" pad="22"/>
<connect gate="G$1" pin="RB5/CCP5/KBI1/SDI1/SDA1/RP8" pad="23"/>
<connect gate="G$1" pin="RB6/CCP6/KBI2/PGC/RP9" pad="24"/>
<connect gate="G$1" pin="RB7/CCP7/KBI3/PGD/RP10" pad="25"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI/RP11" pad="8"/>
<connect gate="G$1" pin="RC1/CCP8/T1OSI/!UOE!/RP12" pad="9"/>
<connect gate="G$1" pin="RC2/AN11/C2IND/CTPLS/RP13" pad="10"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="12"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="13"/>
<connect gate="G$1" pin="RC6/CCP9/TX1/CK1/RP17" pad="14"/>
<connect gate="G$1" pin="RC7/CCP10/RX1/DT1/SDO1/RP18" pad="15"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="3"/>
<connect gate="G$1" pin="VSS1" pad="5"/>
<connect gate="G$1" pin="VSS2" pad="16"/>
<connect gate="G$1" pin="VUSB" pad="11"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F26J53-I/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="63R7829"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F27J53-I/ML"/>
<attribute name="OC_FARNELL" value="1814994"/>
<attribute name="OC_NEWARK" value="63R7837"/>
</technology>
</technologies>
</device>
<device name="SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="10"/>
<connect gate="G$1" pin="RA0/AN0/C1INA/ULPWU/RP0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/C2INA/VBG/RP1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/C1INB/VREF+" pad="5"/>
<connect gate="G$1" pin="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2" pad="7"/>
<connect gate="G$1" pin="RB0/AN12/C3IND/INT0/RP3" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/C3INC/RTCC/RP4" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/C3INA/CTED2/VPO/RP6" pad="24"/>
<connect gate="G$1" pin="RB4/CCP4/KBI0/SCK1/SCL1/RP7" pad="25"/>
<connect gate="G$1" pin="RB5/CCP5/KBI1/SDI1/SDA1/RP8" pad="26"/>
<connect gate="G$1" pin="RB6/CCP6/KBI2/PGC/RP9" pad="27"/>
<connect gate="G$1" pin="RB7/CCP7/KBI3/PGD/RP10" pad="28"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI/RP11" pad="11"/>
<connect gate="G$1" pin="RC1/CCP8/T1OSI/!UOE!/RP12" pad="12"/>
<connect gate="G$1" pin="RC2/AN11/C2IND/CTPLS/RP13" pad="13"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="15"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="16"/>
<connect gate="G$1" pin="RC6/CCP9/TX1/CK1/RP17" pad="17"/>
<connect gate="G$1" pin="RC7/CCP10/RX1/DT1/SDO1/RP18" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="6"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F26J53-I/SP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="63R7831"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F27J53-I/SP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="63R7839"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4*J53ML" prefix="IC">
<description>&lt;b&gt;PIC18F47J53 Family&lt;/b&gt; High-Performance USB Microcontrollers with nanoWatt XLP Technology&lt;p&gt;
Source: &lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/39964B.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="PIC18F47J53ML"/>
</gates>
<devices>
<device name="" package="QFN44ML8X8">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="AVDD1" pad="7"/>
<connect gate="G$1" pin="AVDD2" pad="28"/>
<connect gate="G$1" pin="AVSS1" pad="30"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="32"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="33"/>
<connect gate="G$1" pin="RA0/AN0/C1INA/ULPWU/RP0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1/C2INA/VBG/RP1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF" pad="21"/>
<connect gate="G$1" pin="RA3/AN3/C1INB/VREF+" pad="22"/>
<connect gate="G$1" pin="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2" pad="24"/>
<connect gate="G$1" pin="RB0/AN12/C3IND/INT0/RP3" pad="9"/>
<connect gate="G$1" pin="RB1/AN10/C3INC/RTCC/RP4" pad="10"/>
<connect gate="G$1" pin="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5" pad="11"/>
<connect gate="G$1" pin="RB3/AN9/C3INA/CTED2/VPO/RP6" pad="12"/>
<connect gate="G$1" pin="RB4/CCP4/KBI0/SCK1/SCL1/RP7" pad="14"/>
<connect gate="G$1" pin="RB5/CCP5/KBI1/SDI1/SDA1/RP8" pad="15"/>
<connect gate="G$1" pin="RB6/CCP6/KBI2/PGC/RP9" pad="16"/>
<connect gate="G$1" pin="RB7/CCP7/KBI3/PGD/RP10" pad="17"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI/RP11" pad="34"/>
<connect gate="G$1" pin="RC1/CCP8/T1OSI/!UOE!/RP12" pad="35"/>
<connect gate="G$1" pin="RC2/AN11/C2IND/CTPLS/RP13" pad="36"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="42"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="43"/>
<connect gate="G$1" pin="RC6/CCP9/TX1/CK1/RP17" pad="44"/>
<connect gate="G$1" pin="RC7/CCP10/RX1/DT1/SDO1/RP18" pad="1"/>
<connect gate="G$1" pin="RD0/PMD0/SCL2" pad="38"/>
<connect gate="G$1" pin="RD1/PMD1/SDA2" pad="39"/>
<connect gate="G$1" pin="RD2/PMD2/RP19" pad="40"/>
<connect gate="G$1" pin="RD3/PMD3/RP20" pad="41"/>
<connect gate="G$1" pin="RD4/PMD4/RP21" pad="2"/>
<connect gate="G$1" pin="RD5/PMD5/RP22" pad="3"/>
<connect gate="G$1" pin="RD6/PMD6/RP23" pad="4"/>
<connect gate="G$1" pin="RD7/PMD7/RP24" pad="5"/>
<connect gate="G$1" pin="RE0/AN5/PMRD" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/PMWR" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/PMCS" pad="27"/>
<connect gate="G$1" pin="VDD1" pad="8"/>
<connect gate="G$1" pin="VDD2" pad="29"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="23"/>
<connect gate="G$1" pin="VSS1" pad="6"/>
<connect gate="G$1" pin="VSS2" pad="31"/>
<connect gate="G$1" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F46J53-I/ML"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="63R7851"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F47J53-I/ML"/>
<attribute name="OC_FARNELL" value="1815000"/>
<attribute name="OC_NEWARK" value="63R7855"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F47J53PT" prefix="IC">
<description>&lt;b&gt;PIC18F47J53 Family&lt;/b&gt; High-Performance USB Microcontrollers with nanoWatt XLP Technology&lt;p&gt;
Source: &lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/39964B.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="PIC18F47J53TQ"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="30"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="31"/>
<connect gate="G$1" pin="RA0/AN0/C1INA/ULPWU/RP0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1/C2INA/VBG/RP1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/C2INB/C1IND/C3INB/VREF-/CVREF" pad="21"/>
<connect gate="G$1" pin="RA3/AN3/C1INB/VREF+" pad="22"/>
<connect gate="G$1" pin="RA5/AN4/C1INC/!SS1!/HLVDIN/RCV/RP2" pad="24"/>
<connect gate="G$1" pin="RB0/AN12/C3IND/INT0/RP3" pad="8"/>
<connect gate="G$1" pin="RB1/AN10/C3INC/RTCC/RP4" pad="9"/>
<connect gate="G$1" pin="RB2/AN8/C2INC/CTED1/VMO/REFO/RP5" pad="10"/>
<connect gate="G$1" pin="RB3/AN9/C3INA/CTED2/VPO/RP6" pad="11"/>
<connect gate="G$1" pin="RB4/CCP4/KBI0/SCK1/SCL1/RP7" pad="14"/>
<connect gate="G$1" pin="RB5/CCP5/KBI1/SDI1/SDA1/RP8" pad="15"/>
<connect gate="G$1" pin="RB6/CCP6/KBI2/PGC/RP9" pad="16"/>
<connect gate="G$1" pin="RB7/CCP7/KBI3/PGD/RP10" pad="17"/>
<connect gate="G$1" pin="RC0/T1OSO/T1CKI/RP11" pad="32"/>
<connect gate="G$1" pin="RC1/CCP8/T1OSI/!UOE!/RP12" pad="35"/>
<connect gate="G$1" pin="RC2/AN11/C2IND/CTPLS/RP13" pad="36"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="42"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="43"/>
<connect gate="G$1" pin="RC6/CCP9/TX1/CK1/RP17" pad="44"/>
<connect gate="G$1" pin="RC7/CCP10/RX1/DT1/SDO1/RP18" pad="1"/>
<connect gate="G$1" pin="RD0/PMD0/SCL2" pad="38"/>
<connect gate="G$1" pin="RD1/PMD1/SDA2" pad="39"/>
<connect gate="G$1" pin="RD2/PMD2/RP19" pad="40"/>
<connect gate="G$1" pin="RD3/PMD3/RP20" pad="41"/>
<connect gate="G$1" pin="RD4/PMD4/RP21" pad="2"/>
<connect gate="G$1" pin="RD5/PMD5/RP22" pad="3"/>
<connect gate="G$1" pin="RD6/PMD6/RP23" pad="4"/>
<connect gate="G$1" pin="RD7/PMD7/RP24" pad="5"/>
<connect gate="G$1" pin="RE0/AN5/PMRD" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/PMWR" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/PMCS" pad="27"/>
<connect gate="G$1" pin="VDD1" pad="7"/>
<connect gate="G$1" pin="VDD2" pad="28"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="23"/>
<connect gate="G$1" pin="VSS1" pad="6"/>
<connect gate="G$1" pin="VSS2" pad="29"/>
<connect gate="G$1" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC18F47J53-I/PT"/>
<attribute name="OC_FARNELL" value="1815001"/>
<attribute name="OC_NEWARK" value="63R7856"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ256GP710" prefix="IC">
<description>&lt;b&gt;dsPIC33FJ256GP710_TQFP&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 41&lt;/i&gt;&lt;br&gt;
Source: dsPIC33FJ256GP710_TQFP.bsd</description>
<gates>
<gate name="G$1" symbol="DSPIC33FJ256GP710_TQFP"/>
</gates>
<devices>
<device name="" package="TQFP100-12X12">
<connects>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="MCLR" pad="13"/>
<connect gate="G$1" pin="RA10" pad="29"/>
<connect gate="G$1" pin="RA14" pad="66"/>
<connect gate="G$1" pin="RA15" pad="67"/>
<connect gate="G$1" pin="RA2" pad="58"/>
<connect gate="G$1" pin="RA3" pad="59"/>
<connect gate="G$1" pin="RA6" pad="91"/>
<connect gate="G$1" pin="RA7" pad="92"/>
<connect gate="G$1" pin="RA9" pad="28"/>
<connect gate="G$1" pin="RB0" pad="25"/>
<connect gate="G$1" pin="RB1" pad="24"/>
<connect gate="G$1" pin="RB10" pad="34"/>
<connect gate="G$1" pin="RB11" pad="35"/>
<connect gate="G$1" pin="RB12" pad="41"/>
<connect gate="G$1" pin="RB13" pad="42"/>
<connect gate="G$1" pin="RB14" pad="43"/>
<connect gate="G$1" pin="RB15" pad="44"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4" pad="21"/>
<connect gate="G$1" pin="RB5" pad="20"/>
<connect gate="G$1" pin="RB6" pad="26"/>
<connect gate="G$1" pin="RB7" pad="27"/>
<connect gate="G$1" pin="RB8" pad="32"/>
<connect gate="G$1" pin="RB9" pad="33"/>
<connect gate="G$1" pin="RC1" pad="6"/>
<connect gate="G$1" pin="RC12" pad="63"/>
<connect gate="G$1" pin="RC13" pad="73"/>
<connect gate="G$1" pin="RC14" pad="74"/>
<connect gate="G$1" pin="RC15" pad="64"/>
<connect gate="G$1" pin="RC2" pad="7"/>
<connect gate="G$1" pin="RC3" pad="8"/>
<connect gate="G$1" pin="RC4" pad="9"/>
<connect gate="G$1" pin="RD0" pad="72"/>
<connect gate="G$1" pin="RD1" pad="76"/>
<connect gate="G$1" pin="RD10" pad="70"/>
<connect gate="G$1" pin="RD11" pad="71"/>
<connect gate="G$1" pin="RD12" pad="79"/>
<connect gate="G$1" pin="RD13" pad="80"/>
<connect gate="G$1" pin="RD14" pad="47"/>
<connect gate="G$1" pin="RD15" pad="48"/>
<connect gate="G$1" pin="RD2" pad="77"/>
<connect gate="G$1" pin="RD3" pad="78"/>
<connect gate="G$1" pin="RD4" pad="81"/>
<connect gate="G$1" pin="RD5" pad="82"/>
<connect gate="G$1" pin="RD6" pad="83"/>
<connect gate="G$1" pin="RD7" pad="84"/>
<connect gate="G$1" pin="RD8" pad="68"/>
<connect gate="G$1" pin="RD9" pad="69"/>
<connect gate="G$1" pin="RE0" pad="93"/>
<connect gate="G$1" pin="RE1" pad="94"/>
<connect gate="G$1" pin="RE2" pad="98"/>
<connect gate="G$1" pin="RE3" pad="99"/>
<connect gate="G$1" pin="RE4" pad="100"/>
<connect gate="G$1" pin="RE5" pad="3"/>
<connect gate="G$1" pin="RE6" pad="4"/>
<connect gate="G$1" pin="RE7" pad="5"/>
<connect gate="G$1" pin="RE8" pad="18"/>
<connect gate="G$1" pin="RE9" pad="19"/>
<connect gate="G$1" pin="RF0" pad="87"/>
<connect gate="G$1" pin="RF1" pad="88"/>
<connect gate="G$1" pin="RF12" pad="40"/>
<connect gate="G$1" pin="RF13" pad="39"/>
<connect gate="G$1" pin="RF2" pad="52"/>
<connect gate="G$1" pin="RF3" pad="51"/>
<connect gate="G$1" pin="RF4" pad="49"/>
<connect gate="G$1" pin="RF5" pad="50"/>
<connect gate="G$1" pin="RF6" pad="55"/>
<connect gate="G$1" pin="RF7" pad="54"/>
<connect gate="G$1" pin="RF8" pad="53"/>
<connect gate="G$1" pin="RG0" pad="90"/>
<connect gate="G$1" pin="RG1" pad="89"/>
<connect gate="G$1" pin="RG12" pad="96"/>
<connect gate="G$1" pin="RG13" pad="97"/>
<connect gate="G$1" pin="RG14" pad="95"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="RG2" pad="57"/>
<connect gate="G$1" pin="RG3" pad="56"/>
<connect gate="G$1" pin="RG6" pad="10"/>
<connect gate="G$1" pin="RG7" pad="11"/>
<connect gate="G$1" pin="RG8" pad="12"/>
<connect gate="G$1" pin="RG9" pad="14"/>
<connect gate="G$1" pin="TCK" pad="38"/>
<connect gate="G$1" pin="TDI" pad="60"/>
<connect gate="G$1" pin="TDO" pad="61"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VDD3" pad="37"/>
<connect gate="G$1" pin="VDD4" pad="46"/>
<connect gate="G$1" pin="VDD5" pad="62"/>
<connect gate="G$1" pin="VDDCORE" pad="85"/>
<connect gate="G$1" pin="VREG" pad="86"/>
<connect gate="G$1" pin="VSS1" pad="75"/>
<connect gate="G$1" pin="VSS2" pad="15"/>
<connect gate="G$1" pin="VSS3" pad="36"/>
<connect gate="G$1" pin="VSS4" pad="45"/>
<connect gate="G$1" pin="VSS5" pad="65"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*F1826/27" prefix="IC">
<description>&lt;b&gt;18/20/28-Pin Flash Microcontrollers with nanoWatt XLP Technology&lt;/b&gt;&lt;p&gt;
Source: www.microchip.com PIC16F1827.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16LF1826"/>
</gates>
<devices>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RA5/!MCLR!/VPP" pad="4"/>
<connect gate="G$1" pin="RA6" pad="15"/>
<connect gate="G$1" pin="RA7" pad="16"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="L"/>
</technologies>
</device>
<device name="SO" package="SO-18W">
<connects>
<connect gate="G$1" pin="RA0" pad="17"/>
<connect gate="G$1" pin="RA1" pad="18"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RA5/!MCLR!/VPP" pad="4"/>
<connect gate="G$1" pin="RA6" pad="15"/>
<connect gate="G$1" pin="RA7" pad="16"/>
<connect gate="G$1" pin="RB0" pad="6"/>
<connect gate="G$1" pin="RB1" pad="7"/>
<connect gate="G$1" pin="RB2" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4" pad="10"/>
<connect gate="G$1" pin="RB5" pad="11"/>
<connect gate="G$1" pin="RB6" pad="12"/>
<connect gate="G$1" pin="RB7" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="L"/>
</technologies>
</device>
<device name="SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="RA0" pad="19"/>
<connect gate="G$1" pin="RA1" pad="20"/>
<connect gate="G$1" pin="RA2" pad="1"/>
<connect gate="G$1" pin="RA3" pad="2"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RA5/!MCLR!/VPP" pad="4"/>
<connect gate="G$1" pin="RA6" pad="17"/>
<connect gate="G$1" pin="RA7" pad="18"/>
<connect gate="G$1" pin="RB0" pad="7"/>
<connect gate="G$1" pin="RB1" pad="8"/>
<connect gate="G$1" pin="RB2" pad="9"/>
<connect gate="G$1" pin="RB3" pad="10"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="12"/>
<connect gate="G$1" pin="RB6" pad="13"/>
<connect gate="G$1" pin="RB7" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15 16"/>
<connect gate="G$1" pin="VSS" pad="5 6"/>
</connects>
<technologies>
<technology name=""/>
<technology name="L"/>
</technologies>
</device>
<device name="ML" package="QFN28">
<connects>
<connect gate="G$1" pin="RA0" pad="23"/>
<connect gate="G$1" pin="RA1" pad="24"/>
<connect gate="G$1" pin="RA2" pad="26"/>
<connect gate="G$1" pin="RA3" pad="27"/>
<connect gate="G$1" pin="RA4" pad="28"/>
<connect gate="G$1" pin="RA5/!MCLR!/VPP" pad="1"/>
<connect gate="G$1" pin="RA6" pad="20"/>
<connect gate="G$1" pin="RA7" pad="21"/>
<connect gate="G$1" pin="RB0" pad="7"/>
<connect gate="G$1" pin="RB1" pad="8"/>
<connect gate="G$1" pin="RB2" pad="9"/>
<connect gate="G$1" pin="RB3" pad="10"/>
<connect gate="G$1" pin="RB4" pad="12"/>
<connect gate="G$1" pin="RB5" pad="13"/>
<connect gate="G$1" pin="RB6" pad="15"/>
<connect gate="G$1" pin="RB7" pad="16"/>
<connect gate="G$1" pin="VDD" pad="17 19"/>
<connect gate="G$1" pin="VSS" pad="3 5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="L"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*F1516/18" prefix="IC">
<description>&lt;b&gt;28/40/44-Pin Flash Microcontrollers with nanoWatt XLP Technology&lt;/b&gt;&lt;p&gt;
PIC16F1516/1518 AND PIC16LF1516/1518&lt;br&gt;
Source: www.microchip.com PIC16F1516.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F1516"/>
</gates>
<devices>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!SS!/AN0/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/RA1" pad="3"/>
<connect gate="G$1" pin="AN2/RA2" pad="4"/>
<connect gate="G$1" pin="CCP1/AN14/RC2" pad="13"/>
<connect gate="G$1" pin="CCP2/SOSCI/RC1" pad="12"/>
<connect gate="G$1" pin="CLKIN/OSC1/RA7" pad="9"/>
<connect gate="G$1" pin="CLKOUT/OSC2/RA6" pad="10"/>
<connect gate="G$1" pin="RB0/AN12/INT" pad="21"/>
<connect gate="G$1" pin="RB1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/CCP2" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/AN13/T1G" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT" pad="28"/>
<connect gate="G$1" pin="RC4/AN16/SDI/SDA" pad="15"/>
<connect gate="G$1" pin="RC5/AN17/SDO" pad="16"/>
<connect gate="G$1" pin="RC6/AN18/TX/CK" pad="17"/>
<connect gate="G$1" pin="RC7/AN19/RX/DT" pad="18"/>
<connect gate="G$1" pin="SCL/SCK/AN15/RC3" pad="14"/>
<connect gate="G$1" pin="T0CKI/RA4" pad="6"/>
<connect gate="G$1" pin="T1CKI/SOSCO/RC0" pad="11"/>
<connect gate="G$1" pin="VCAP/!SS!/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
<technology name="L"/>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!SS!/AN0/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/RA1" pad="3"/>
<connect gate="G$1" pin="AN2/RA2" pad="4"/>
<connect gate="G$1" pin="CCP1/AN14/RC2" pad="13"/>
<connect gate="G$1" pin="CCP2/SOSCI/RC1" pad="12"/>
<connect gate="G$1" pin="CLKIN/OSC1/RA7" pad="9"/>
<connect gate="G$1" pin="CLKOUT/OSC2/RA6" pad="10"/>
<connect gate="G$1" pin="RB0/AN12/INT" pad="21"/>
<connect gate="G$1" pin="RB1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/CCP2" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/AN13/T1G" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT" pad="28"/>
<connect gate="G$1" pin="RC4/AN16/SDI/SDA" pad="15"/>
<connect gate="G$1" pin="RC5/AN17/SDO" pad="16"/>
<connect gate="G$1" pin="RC6/AN18/TX/CK" pad="17"/>
<connect gate="G$1" pin="RC7/AN19/RX/DT" pad="18"/>
<connect gate="G$1" pin="SCL/SCK/AN15/RC3" pad="14"/>
<connect gate="G$1" pin="T0CKI/RA4" pad="6"/>
<connect gate="G$1" pin="T1CKI/SOSCO/RC0" pad="11"/>
<connect gate="G$1" pin="VCAP/!SS!/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
<technology name="L"/>
</technologies>
</device>
<device name="P" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!SS!/AN0/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/RA1" pad="3"/>
<connect gate="G$1" pin="AN2/RA2" pad="4"/>
<connect gate="G$1" pin="CCP1/AN14/RC2" pad="13"/>
<connect gate="G$1" pin="CCP2/SOSCI/RC1" pad="12"/>
<connect gate="G$1" pin="CLKIN/OSC1/RA7" pad="9"/>
<connect gate="G$1" pin="CLKOUT/OSC2/RA6" pad="10"/>
<connect gate="G$1" pin="RB0/AN12/INT" pad="21"/>
<connect gate="G$1" pin="RB1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/CCP2" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/AN13/T1G" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT" pad="28"/>
<connect gate="G$1" pin="RC4/AN16/SDI/SDA" pad="15"/>
<connect gate="G$1" pin="RC5/AN17/SDO" pad="16"/>
<connect gate="G$1" pin="RC6/AN18/TX/CK" pad="17"/>
<connect gate="G$1" pin="RC7/AN19/RX/DT" pad="18"/>
<connect gate="G$1" pin="SCL/SCK/AN15/RC3" pad="14"/>
<connect gate="G$1" pin="T0CKI/RA4" pad="6"/>
<connect gate="G$1" pin="T1CKI/SOSCO/RC0" pad="11"/>
<connect gate="G$1" pin="VCAP/!SS!/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
<technology name="L"/>
</technologies>
</device>
<device name="ML" package="UQFN28_4X4MM">
<connects>
<connect gate="G$1" pin="!SS!/AN0/RA0" pad="27"/>
<connect gate="G$1" pin="AN1/RA1" pad="28"/>
<connect gate="G$1" pin="AN2/RA2" pad="1"/>
<connect gate="G$1" pin="CCP1/AN14/RC2" pad="10"/>
<connect gate="G$1" pin="CCP2/SOSCI/RC1" pad="9"/>
<connect gate="G$1" pin="CLKIN/OSC1/RA7" pad="6"/>
<connect gate="G$1" pin="CLKOUT/OSC2/RA6" pad="7"/>
<connect gate="G$1" pin="RB0/AN12/INT" pad="18"/>
<connect gate="G$1" pin="RB1/AN10" pad="19"/>
<connect gate="G$1" pin="RB2/AN8" pad="20"/>
<connect gate="G$1" pin="RB3/AN9/CCP2" pad="21"/>
<connect gate="G$1" pin="RB4/AN11" pad="22"/>
<connect gate="G$1" pin="RB5/AN13/T1G" pad="23"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCLK" pad="24"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT" pad="25"/>
<connect gate="G$1" pin="RC4/AN16/SDI/SDA" pad="12"/>
<connect gate="G$1" pin="RC5/AN17/SDO" pad="13"/>
<connect gate="G$1" pin="RC6/AN18/TX/CK" pad="14"/>
<connect gate="G$1" pin="RC7/AN19/RX/DT" pad="15"/>
<connect gate="G$1" pin="SCL/SCK/AN15/RC3" pad="11"/>
<connect gate="G$1" pin="T0CKI/RA4" pad="3"/>
<connect gate="G$1" pin="T1CKI/SOSCO/RC0" pad="8"/>
<connect gate="G$1" pin="VCAP/!SS!/AN4/RA5" pad="4"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="26"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="2"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16*F1517/19" prefix="IC">
<description>&lt;b&gt;28/40/44-Pin Flash Microcontrollers with nanoWatt XLP Technology&lt;/b&gt;&lt;p&gt;
PIC16F1517/1519 AND PIC16LF1517/1519&lt;br&gt;
Source: www.microchip.com PIC16F1516.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F1517/19"/>
</gates>
<devices>
<device name="MV" package="UQFN40ML5X5MM">
<connects>
<connect gate="G$1" pin="!SS!/AN0/RA0" pad="17"/>
<connect gate="G$1" pin="AN1/RA1" pad="18"/>
<connect gate="G$1" pin="AN10/RB1" pad="9"/>
<connect gate="G$1" pin="AN11/RB4" pad="12"/>
<connect gate="G$1" pin="AN2/RA2" pad="19"/>
<connect gate="G$1" pin="AN24/RD4" pad="2"/>
<connect gate="G$1" pin="AN25/RD5" pad="3"/>
<connect gate="G$1" pin="AN26/RD6" pad="4"/>
<connect gate="G$1" pin="AN27/RD7" pad="5"/>
<connect gate="G$1" pin="AN8/RB2" pad="10"/>
<connect gate="G$1" pin="CCP2/AN9/RB3" pad="11"/>
<connect gate="G$1" pin="DT/RX/AN19/RC7" pad="1"/>
<connect gate="G$1" pin="ICDCLK/ICSPCLK/RB6" pad="14"/>
<connect gate="G$1" pin="ICDDAT/ICSPDAT/RB7" pad="15"/>
<connect gate="G$1" pin="INT/AN12/RB0" pad="8"/>
<connect gate="G$1" pin="RA4/TOCKI" pad="21"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/VCAP" pad="22"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="29"/>
<connect gate="G$1" pin="RA7/OSC1/CLKIN" pad="28"/>
<connect gate="G$1" pin="RC0/SOSCO/T1CKI" pad="30"/>
<connect gate="G$1" pin="RC1/SOSCI/CCP2" pad="31"/>
<connect gate="G$1" pin="RC2/AN14/CCP1" pad="32"/>
<connect gate="G$1" pin="RC3/AN15/SCK/SCL" pad="33"/>
<connect gate="G$1" pin="RC4/AN16/SDI/SDA" pad="38"/>
<connect gate="G$1" pin="RC5/AN17/SDO" pad="39"/>
<connect gate="G$1" pin="RC6/AN18/TX/CK" pad="40"/>
<connect gate="G$1" pin="RD0/AN20" pad="34"/>
<connect gate="G$1" pin="RD1/AN21" pad="35"/>
<connect gate="G$1" pin="RD2/AN22" pad="36"/>
<connect gate="G$1" pin="RD3/AN23" pad="37"/>
<connect gate="G$1" pin="RE0/AN5" pad="23"/>
<connect gate="G$1" pin="RE1/AN6" pad="24"/>
<connect gate="G$1" pin="RE2/AN7" pad="25"/>
<connect gate="G$1" pin="T1G/AN13/RB5" pad="13"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="26"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="16"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="20"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="!SS!/AN0/RA0" pad="19"/>
<connect gate="G$1" pin="AN1/RA1" pad="20"/>
<connect gate="G$1" pin="AN10/RB1" pad="9"/>
<connect gate="G$1" pin="AN11/RB4" pad="14"/>
<connect gate="G$1" pin="AN2/RA2" pad="21"/>
<connect gate="G$1" pin="AN24/RD4" pad="2"/>
<connect gate="G$1" pin="AN25/RD5" pad="3"/>
<connect gate="G$1" pin="AN26/RD6" pad="4"/>
<connect gate="G$1" pin="AN27/RD7" pad="5"/>
<connect gate="G$1" pin="AN8/RB2" pad="10"/>
<connect gate="G$1" pin="CCP2/AN9/RB3" pad="11"/>
<connect gate="G$1" pin="DT/RX/AN19/RC7" pad="1"/>
<connect gate="G$1" pin="ICDCLK/ICSPCLK/RB6" pad="16"/>
<connect gate="G$1" pin="ICDDAT/ICSPDAT/RB7" pad="17"/>
<connect gate="G$1" pin="INT/AN12/RB0" pad="8"/>
<connect gate="G$1" pin="RA4/TOCKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/VCAP" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="31"/>
<connect gate="G$1" pin="RA7/OSC1/CLKIN" pad="30"/>
<connect gate="G$1" pin="RC0/SOSCO/T1CKI" pad="32"/>
<connect gate="G$1" pin="RC1/SOSCI/CCP2" pad="35"/>
<connect gate="G$1" pin="RC2/AN14/CCP1" pad="36"/>
<connect gate="G$1" pin="RC3/AN15/SCK/SCL" pad="37"/>
<connect gate="G$1" pin="RC4/AN16/SDI/SDA" pad="42"/>
<connect gate="G$1" pin="RC5/AN17/SDO" pad="43"/>
<connect gate="G$1" pin="RC6/AN18/TX/CK" pad="44"/>
<connect gate="G$1" pin="RD0/AN20" pad="38"/>
<connect gate="G$1" pin="RD1/AN21" pad="39"/>
<connect gate="G$1" pin="RD2/AN22" pad="40"/>
<connect gate="G$1" pin="RD3/AN23" pad="41"/>
<connect gate="G$1" pin="RE0/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/AN7" pad="27"/>
<connect gate="G$1" pin="T1G/AN13/RB5" pad="15"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="18"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="22"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="!SS!/AN0/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/RA1" pad="3"/>
<connect gate="G$1" pin="AN10/RB1" pad="34"/>
<connect gate="G$1" pin="AN11/RB4" pad="37"/>
<connect gate="G$1" pin="AN2/RA2" pad="4"/>
<connect gate="G$1" pin="AN24/RD4" pad="27"/>
<connect gate="G$1" pin="AN25/RD5" pad="28"/>
<connect gate="G$1" pin="AN26/RD6" pad="29"/>
<connect gate="G$1" pin="AN27/RD7" pad="30"/>
<connect gate="G$1" pin="AN8/RB2" pad="35"/>
<connect gate="G$1" pin="CCP2/AN9/RB3" pad="36"/>
<connect gate="G$1" pin="DT/RX/AN19/RC7" pad="26"/>
<connect gate="G$1" pin="ICDCLK/ICSPCLK/RB6" pad="39"/>
<connect gate="G$1" pin="ICDDAT/ICSPDAT/RB7" pad="40"/>
<connect gate="G$1" pin="INT/AN12/RB0" pad="33"/>
<connect gate="G$1" pin="RA4/TOCKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/VCAP" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKOUT" pad="14"/>
<connect gate="G$1" pin="RA7/OSC1/CLKIN" pad="13"/>
<connect gate="G$1" pin="RC0/SOSCO/T1CKI" pad="15"/>
<connect gate="G$1" pin="RC1/SOSCI/CCP2" pad="16"/>
<connect gate="G$1" pin="RC2/AN14/CCP1" pad="17"/>
<connect gate="G$1" pin="RC3/AN15/SCK/SCL" pad="18"/>
<connect gate="G$1" pin="RC4/AN16/SDI/SDA" pad="23"/>
<connect gate="G$1" pin="RC5/AN17/SDO" pad="24"/>
<connect gate="G$1" pin="RC6/AN18/TX/CK" pad="25"/>
<connect gate="G$1" pin="RD0/AN20" pad="19"/>
<connect gate="G$1" pin="RD1/AN21" pad="20"/>
<connect gate="G$1" pin="RD2/AN22" pad="21"/>
<connect gate="G$1" pin="RD3/AN23" pad="22"/>
<connect gate="G$1" pin="RE0/AN5" pad="8"/>
<connect gate="G$1" pin="RE1/AN6" pad="9"/>
<connect gate="G$1" pin="RE2/AN7" pad="10"/>
<connect gate="G$1" pin="T1G/AN13/RB5" pad="38"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VPP/!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name=""/>
<technology name="L"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP14628" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="MCP14628"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="BOOT" pad="2"/>
<connect gate="G$1" pin="FCCM" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HDR" pad="1"/>
<connect gate="G$1" pin="LDR" pad="5"/>
<connect gate="G$1" pin="PSE" pad="8"/>
<connect gate="G$1" pin="PWM" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DFN8-3X3" package="DFN8-3X3">
<connects>
<connect gate="G$1" pin="BOOT" pad="2"/>
<connect gate="G$1" pin="FCCM" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HDR" pad="1"/>
<connect gate="G$1" pin="LDR" pad="5"/>
<connect gate="G$1" pin="PSE" pad="8"/>
<connect gate="G$1" pin="PWM" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73833/4" prefix="IC" uservalue="yes">
<description>Stand-Alone Linear Li-Ion / Li-Polymer Charge
Management Controller</description>
<gates>
<gate name="G$1" symbol="MCP73833/4"/>
</gates>
<devices>
<device name="" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="10VB" pad="P$10"/>
<connect gate="G$1" pin="1VD" pad="P$1"/>
<connect gate="G$1" pin="2VD" pad="P$2"/>
<connect gate="G$1" pin="3ST1" pad="P$3"/>
<connect gate="G$1" pin="4ST2" pad="P$4"/>
<connect gate="G$1" pin="5VS" pad="P$5"/>
<connect gate="G$1" pin="6PR" pad="P$6"/>
<connect gate="G$1" pin="7PG" pad="P$7"/>
<connect gate="G$1" pin="8T" pad="P$8"/>
<connect gate="G$1" pin="9VB" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MSOP10" package="MSOP10">
<connects>
<connect gate="G$1" pin="10VB" pad="10"/>
<connect gate="G$1" pin="1VD" pad="1"/>
<connect gate="G$1" pin="2VD" pad="2"/>
<connect gate="G$1" pin="3ST1" pad="3"/>
<connect gate="G$1" pin="4ST2" pad="4"/>
<connect gate="G$1" pin="5VS" pad="5"/>
<connect gate="G$1" pin="6PR" pad="6"/>
<connect gate="G$1" pin="7PG" pad="7"/>
<connect gate="G$1" pin="8T" pad="8"/>
<connect gate="G$1" pin="9VB" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73831-SOT23-5L" prefix="IC" uservalue="yes">
<description>Miniature Single Cell, Fully Integrated Li-Ion,
Li-Polymer Charge Management Controller</description>
<gates>
<gate name="G$1" symbol="MCP73831-SOT"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73831-DFN8" prefix="IC" uservalue="yes">
<description>Miniature Single Cell, Fully Integrated Li-Ion,
Li-Polymer Charge Management Controller</description>
<gates>
<gate name="G$1" symbol="MCP73831-DFN"/>
</gates>
<devices>
<device name="" package="DFN-2X3">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP256MU806-X_MR" prefix="IC">
<description>dsPIC33EP256MU806-X_MR</description>
<gates>
<gate name="A" symbol="DSPIC33EP256MU806-X_MR"/>
</gates>
<devices>
<device name="" package="QFN64_9X9MC">
<connects>
<connect gate="A" pin="!MCLR" pad="7"/>
<connect gate="A" pin="AN14/PMA1/RP46/RB14" pad="29"/>
<connect gate="A" pin="AN15/PMA0/RP47/RB15" pad="30"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="14"/>
<connect gate="A" pin="AN24/PWM1L/PMD0/RP80/RE0" pad="60"/>
<connect gate="A" pin="AN25/PWM1H/PMD1/RP81/RE1" pad="61"/>
<connect gate="A" pin="AN26/PWM2L/PMD2/RP82/RE2" pad="62"/>
<connect gate="A" pin="AN27/PWM2H/PMD3/RP83/RE3" pad="63"/>
<connect gate="A" pin="AN28/PWM3L/PMD4/RP84/RE4" pad="64"/>
<connect gate="A" pin="AN29/PWM3H/PMD5/RP85/RE5" pad="1"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="13"/>
<connect gate="A" pin="AN30/PWM4L/PMD6/RP86/RE6" pad="2"/>
<connect gate="A" pin="AN31/PWM4H/PMD7/RP87/RE7" pad="3"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="12"/>
<connect gate="A" pin="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" pad="11"/>
<connect gate="A" pin="AN8/PMA6/RP40/RB8" pad="21"/>
<connect gate="A" pin="AN9/PMA7/RP41/RB9" pad="22"/>
<connect gate="A" pin="ASCL1/PMCS2/RP74/RD10" pad="44"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="43"/>
<connect gate="A" pin="AVDD" pad="19"/>
<connect gate="A" pin="AVSS" pad="20"/>
<connect gate="A" pin="C1INC/SDI2/PMA4/RP119/RG7" pad="5"/>
<connect gate="A" pin="C1IND/SCK2/PMA5/RP118/RG6" pad="4"/>
<connect gate="A" pin="C2INC/PMA2/RP121/RG9" pad="8"/>
<connect gate="A" pin="C2IND/SDO2/PMA3/RP120/RG8" pad="6"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="55"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="54"/>
<connect gate="A" pin="D+/RG2" pad="37"/>
<connect gate="A" pin="D-/RG3" pad="36"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="50"/>
<connect gate="A" pin="EP" pad="65"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="46"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="39"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="40"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="17"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="48"/>
<connect gate="A" pin="PGEC3/AN1/VREF-/RP33/RB1" pad="15"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="18"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="47"/>
<connect gate="A" pin="PGED3/AN0/VREF+/RP32/RB0" pad="16"/>
<connect gate="A" pin="PMBE/RP67/RD3" pad="51"/>
<connect gate="A" pin="PMCS1/RP75/RD11" pad="45"/>
<connect gate="A" pin="PMRD/RP69/RD5" pad="53"/>
<connect gate="A" pin="PMWR/RP68/RD4" pad="52"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="42"/>
<connect gate="A" pin="SCL2/PMA8/RP101/RF5" pad="32"/>
<connect gate="A" pin="SDA2/PMA9/RP100/RF4" pad="31"/>
<connect gate="A" pin="TCK/AN12/PMA11/RP44/RB12" pad="27"/>
<connect gate="A" pin="TDI/AN13/PMA10/RP45/RB13" pad="28"/>
<connect gate="A" pin="TDO/AN11/PMA12/RP43/RB11" pad="24"/>
<connect gate="A" pin="TMS/AN10/CVREF/PMA13/RP42/RB10" pad="23"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="33"/>
<connect gate="A" pin="VBUS" pad="34"/>
<connect gate="A" pin="VCAP" pad="56"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="58"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="59"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="49"/>
<connect gate="A" pin="VDD" pad="38"/>
<connect gate="A" pin="VDD_2" pad="10"/>
<connect gate="A" pin="VDD_3" pad="26"/>
<connect gate="A" pin="VDD_4" pad="57"/>
<connect gate="A" pin="VSS" pad="41"/>
<connect gate="A" pin="VSS_2" pad="9"/>
<connect gate="A" pin="VSS_3" pad="25"/>
<connect gate="A" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP256MU806-X_PT" prefix="IC">
<description>dsPIC33EP256MU806-X_PT QFP64 10x10</description>
<gates>
<gate name="A" symbol="DSPIC33EP256MU806-X_PT"/>
</gates>
<devices>
<device name="" package="QFP64-10X10MC">
<connects>
<connect gate="A" pin="!MCLR" pad="7"/>
<connect gate="A" pin="AN14/PMA1/RP46/RB14" pad="29"/>
<connect gate="A" pin="AN15/PMA0/RP47/RB15" pad="30"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="14"/>
<connect gate="A" pin="AN24/PWM1L/PMD0/RP80/RE0" pad="60"/>
<connect gate="A" pin="AN25/PWM1H/PMD1/RP81/RE1" pad="61"/>
<connect gate="A" pin="AN26/PWM2L/PMD2/RP82/RE2" pad="62"/>
<connect gate="A" pin="AN27/PWM2H/PMD3/RP83/RE3" pad="63"/>
<connect gate="A" pin="AN28/PWM3L/PMD4/RP84/RE4" pad="64"/>
<connect gate="A" pin="AN29/PWM3H/PMD5/RP85/RE5" pad="1"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="13"/>
<connect gate="A" pin="AN30/PWM4L/PMD6/RP86/RE6" pad="2"/>
<connect gate="A" pin="AN31/PWM4H/PMD7/RP87/RE7" pad="3"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="12"/>
<connect gate="A" pin="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" pad="11"/>
<connect gate="A" pin="AN8/PMA6/RP40/RB8" pad="21"/>
<connect gate="A" pin="AN9/PMA7/RP41/RB9" pad="22"/>
<connect gate="A" pin="ASCL1/PMCS2/RP74/RD10" pad="44"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="43"/>
<connect gate="A" pin="AVDD" pad="19"/>
<connect gate="A" pin="AVSS" pad="20"/>
<connect gate="A" pin="C1INC/SDI2/PMA4/RP119/RG7" pad="5"/>
<connect gate="A" pin="C1IND/SCK2/PMA5/RP118/RG6" pad="4"/>
<connect gate="A" pin="C2INC/PMA2/RP121/RG9" pad="8"/>
<connect gate="A" pin="C2IND/SDO2/PMA3/RP120/RG8" pad="6"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="55"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="54"/>
<connect gate="A" pin="D+/RG2" pad="37"/>
<connect gate="A" pin="D-/RG3" pad="36"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="50"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="46"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="39"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="40"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="17"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="48"/>
<connect gate="A" pin="PGEC3/AN1/VREF-/RP33/RB1" pad="15"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="18"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="47"/>
<connect gate="A" pin="PGED3/AN0/VREF+/RP32/RB0" pad="16"/>
<connect gate="A" pin="PMBE/RP67/RD3" pad="51"/>
<connect gate="A" pin="PMCS1/RP75/RD11" pad="45"/>
<connect gate="A" pin="PMRD/RP69/RD5" pad="53"/>
<connect gate="A" pin="PMWR/RP68/RD4" pad="52"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="42"/>
<connect gate="A" pin="SCL2/PMA8/RP101/RF5" pad="32"/>
<connect gate="A" pin="SDA2/PMA9/RP100/RF4" pad="31"/>
<connect gate="A" pin="TCK/AN12/PMA11/RP44/RB12" pad="27"/>
<connect gate="A" pin="TDI/AN13/PMA10/RP45/RB13" pad="28"/>
<connect gate="A" pin="TDO/AN11/PMA12/RP43/RB11" pad="24"/>
<connect gate="A" pin="TMS/AN10/CVREF/PMA13/RP42/RB10" pad="23"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="33"/>
<connect gate="A" pin="VBUS" pad="34"/>
<connect gate="A" pin="VCAP" pad="56"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="58"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="59"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="49"/>
<connect gate="A" pin="VDD" pad="38"/>
<connect gate="A" pin="VDD_2" pad="10"/>
<connect gate="A" pin="VDD_3" pad="26"/>
<connect gate="A" pin="VDD_4" pad="57"/>
<connect gate="A" pin="VSS" pad="41"/>
<connect gate="A" pin="VSS_2" pad="9"/>
<connect gate="A" pin="VSS_3" pad="25"/>
<connect gate="A" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP256MU810-X_BG" prefix="IC">
<description>dsPIC33EP256MU810 XBGA 10X10</description>
<gates>
<gate name="A" symbol="DSPIC33EP256MU810-X_BG"/>
</gates>
<devices>
<device name="" package="XBGA121_10X10MC">
<connects>
<connect gate="A" pin="!MCLR" pad="F1"/>
<connect gate="A" pin="AN10/CVREF/PMA13/RP42/RB10" pad="L5"/>
<connect gate="A" pin="AN11/PMA12/RP43/RB11" pad="J5"/>
<connect gate="A" pin="AN12/PMA11/RP44/RB12" pad="J7"/>
<connect gate="A" pin="AN13/PMA10/RP45/RB13" pad="L7"/>
<connect gate="A" pin="AN14/PMA1/RP46/RB14" pad="K7"/>
<connect gate="A" pin="AN15/PMA0/RP47/RB15" pad="L8"/>
<connect gate="A" pin="AN16/PWM5L/RP49/RC1" pad="D1"/>
<connect gate="A" pin="AN17/PWM5H/RP50/RC2" pad="E4"/>
<connect gate="A" pin="AN18/PWM6L/RP51/RC3" pad="E2"/>
<connect gate="A" pin="AN19/PWM6H/RP52/RC4" pad="E1"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="J2"/>
<connect gate="A" pin="AN20/RP88/RE8" pad="G1"/>
<connect gate="A" pin="AN21/RP89/RE9" pad="G2"/>
<connect gate="A" pin="AN22/RP22/RA6" pad="C5"/>
<connect gate="A" pin="AN23/RP23/RA7" pad="B5"/>
<connect gate="A" pin="AN24/PWM1L/PMD0/RP80/RE0" pad="A4"/>
<connect gate="A" pin="AN25/PWM1H/PMD1/RP81/RE1" pad="B4"/>
<connect gate="A" pin="AN26/PWM2L/PMD2/RP82/RE2" pad="B3"/>
<connect gate="A" pin="AN27/PWM2H/PMD3/RP83/RE3" pad="A2"/>
<connect gate="A" pin="AN28/PWM3L/PMD4/RP84/RE4" pad="A1"/>
<connect gate="A" pin="AN29/PWM3H/PMD5/RP85/RE5" pad="D3"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="J1"/>
<connect gate="A" pin="AN30/PWM4L/PMD6/RP86/RE6" pad="C1"/>
<connect gate="A" pin="AN31/PWM4H/PMD7/RP87/RE7" pad="D2"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="H2"/>
<connect gate="A" pin="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" pad="H1"/>
<connect gate="A" pin="AN8/PMA6/RP40/RB8" pad="K4"/>
<connect gate="A" pin="AN9/PMA7//RP41/RB9" pad="L4"/>
<connect gate="A" pin="ASCL1/PMCS2/RP74/RD10" pad="D11"/>
<connect gate="A" pin="ASCL2/RP18/RA2" pad="H11"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="E10"/>
<connect gate="A" pin="ASDA2/RP19/RA3" pad="G10"/>
<connect gate="A" pin="AVDD" pad="J4"/>
<connect gate="A" pin="AVSS" pad="L3"/>
<connect gate="A" pin="C1INC/SDI2/PMA4/RP119/RG7" pad="F4"/>
<connect gate="A" pin="C1IND/SCK2/PMA5/RP118/RG6" pad="E3"/>
<connect gate="A" pin="C2INC/PMA2/RP121/RG9" pad="F3"/>
<connect gate="A" pin="C2IND/SDO2/PMA3/RP120/RG8" pad="F2"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="C7"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="D7"/>
<connect gate="A" pin="D+/RG2" pad="H10"/>
<connect gate="A" pin="D-/RG3" pad="J11"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="A10"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="D9"/>
<connect gate="A" pin="NO_CONNECT" pad="A8"/>
<connect gate="A" pin="NO_CONNECT_10" pad="E7"/>
<connect gate="A" pin="NO_CONNECT_11" pad="K5"/>
<connect gate="A" pin="NO_CONNECT_12" pad="J9"/>
<connect gate="A" pin="NO_CONNECT_13" pad="J8"/>
<connect gate="A" pin="NO_CONNECT_14" pad="H7"/>
<connect gate="A" pin="NO_CONNECT_15" pad="H5"/>
<connect gate="A" pin="NO_CONNECT_16" pad="H4"/>
<connect gate="A" pin="NO_CONNECT_17" pad="H3"/>
<connect gate="A" pin="NO_CONNECT_18" pad="G8"/>
<connect gate="A" pin="NO_CONNECT_19" pad="G4"/>
<connect gate="A" pin="NO_CONNECT_2" pad="B1"/>
<connect gate="A" pin="NO_CONNECT_20" pad="F7"/>
<connect gate="A" pin="NO_CONNECT_21" pad="F6"/>
<connect gate="A" pin="NO_CONNECT_3" pad="C6"/>
<connect gate="A" pin="NO_CONNECT_4" pad="C9"/>
<connect gate="A" pin="NO_CONNECT_5" pad="D4"/>
<connect gate="A" pin="NO_CONNECT_6" pad="D5"/>
<connect gate="A" pin="NO_CONNECT_7" pad="D6"/>
<connect gate="A" pin="NO_CONNECT_8" pad="D10"/>
<connect gate="A" pin="NO_CONNECT_9" pad="E5"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="F9"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="F11"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="L1"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="B11"/>
<connect gate="A" pin="PGEC3/AN1/RP33/RB1" pad="K1"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="J3"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="C10"/>
<connect gate="A" pin="PGED3/AN0/RP32/RB0" pad="K2"/>
<connect gate="A" pin="PMBE/RP67/RD3" pad="B9"/>
<connect gate="A" pin="PMCS1/RP75/RD11" pad="C11"/>
<connect gate="A" pin="PMRD/RP69/RD5" pad="B8"/>
<connect gate="A" pin="PMWR/RP68/RD4" pad="C8"/>
<connect gate="A" pin="RP104/RF8" pad="J10"/>
<connect gate="A" pin="RP108/RF12" pad="K6"/>
<connect gate="A" pin="RP109/RF13" pad="L6"/>
<connect gate="A" pin="RP112/RG0" pad="A5"/>
<connect gate="A" pin="RP113/RG1" pad="E6"/>
<connect gate="A" pin="RP124/RG12" pad="C3"/>
<connect gate="A" pin="RP125/RG13" pad="A3"/>
<connect gate="A" pin="RP126/RG14" pad="C4"/>
<connect gate="A" pin="RP127/RG15" pad="B2"/>
<connect gate="A" pin="RP30/RA14" pad="E11"/>
<connect gate="A" pin="RP31/RA15" pad="E8"/>
<connect gate="A" pin="RP76/RD12" pad="A9"/>
<connect gate="A" pin="RP77/RD13" pad="D8"/>
<connect gate="A" pin="RP78/RD14" pad="L9"/>
<connect gate="A" pin="RP79/RD15" pad="K9"/>
<connect gate="A" pin="RP98/RF2" pad="K11"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="E9"/>
<connect gate="A" pin="SCL2/PMA8/RP101/RF5" pad="L11"/>
<connect gate="A" pin="SDA2/PMA9/RP100/RF4" pad="L10"/>
<connect gate="A" pin="TCK/RP17/RA1" pad="J6"/>
<connect gate="A" pin="TDI/RP20/RA4" pad="G11"/>
<connect gate="A" pin="TDO/RP21/RA5" pad="G9"/>
<connect gate="A" pin="TMS/RP16/RA0" pad="G3"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="K10"/>
<connect gate="A" pin="VBUS" pad="H8"/>
<connect gate="A" pin="VCAP" pad="B7"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="B6"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="A6"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="A11"/>
<connect gate="A" pin="VDD" pad="F8"/>
<connect gate="A" pin="VDD_2" pad="A7"/>
<connect gate="A" pin="VDD_3" pad="C2"/>
<connect gate="A" pin="VDD_4" pad="K8"/>
<connect gate="A" pin="VDD_5" pad="H6"/>
<connect gate="A" pin="VDD_6" pad="G5"/>
<connect gate="A" pin="VREF+/RA10" pad="K3"/>
<connect gate="A" pin="VREF-/RA9" pad="L2"/>
<connect gate="A" pin="VSS" pad="F10"/>
<connect gate="A" pin="VSS_2" pad="B10"/>
<connect gate="A" pin="VSS_3" pad="F5"/>
<connect gate="A" pin="VSS_4" pad="G7"/>
<connect gate="A" pin="VSS_5" pad="G6"/>
<connect gate="A" pin="VUSB" pad="H9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP256MU810-X_PF" prefix="IC">
<description>dsPIC33EP256MU810-X_PF TQFP 100; 14x14</description>
<gates>
<gate name="A" symbol="DSPIC33EP256MU810-X_PF"/>
</gates>
<devices>
<device name="" package="TQFP100_14X14MC">
<connects>
<connect gate="A" pin="!MCLR" pad="13"/>
<connect gate="A" pin="AN10/CVREF/PMA13/RP42/RB10" pad="34"/>
<connect gate="A" pin="AN11/PMA12/RP43/RB11" pad="35"/>
<connect gate="A" pin="AN12/PMA11/RP44/RB12" pad="41"/>
<connect gate="A" pin="AN13/PMA10/RP45/RB13" pad="42"/>
<connect gate="A" pin="AN14/PMA1/RP46/RB14" pad="43"/>
<connect gate="A" pin="AN15/PMA0/RP47/RB15" pad="44"/>
<connect gate="A" pin="AN16/PWM5L/RP49/RC1" pad="6"/>
<connect gate="A" pin="AN17/PWM5H/RP50/RC2" pad="7"/>
<connect gate="A" pin="AN18/PWM6L/RP51/RC3" pad="8"/>
<connect gate="A" pin="AN19/PWM6H/RP52/RC4" pad="9"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="23"/>
<connect gate="A" pin="AN20/RP88/RE8" pad="18"/>
<connect gate="A" pin="AN21/RP89/RE9" pad="19"/>
<connect gate="A" pin="AN22/RP22/RA6" pad="91"/>
<connect gate="A" pin="AN23/RP23/RA7" pad="92"/>
<connect gate="A" pin="AN24/PWM1L/PMD0/RP80/RE0" pad="93"/>
<connect gate="A" pin="AN25/PWM1H/PMD1/RP81/RE1" pad="94"/>
<connect gate="A" pin="AN26/PWM2L/PMD2/RP82/RE2" pad="98"/>
<connect gate="A" pin="AN27/PWM2H/PMD3/RP83/RE3" pad="99"/>
<connect gate="A" pin="AN28/PWM3L/PMD4/RP84/RE4" pad="100"/>
<connect gate="A" pin="AN29/PWM3H/PMD5/RP85/RE5" pad="3"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="22"/>
<connect gate="A" pin="AN30/PWM4L/PMD6/RP86/RE6" pad="4"/>
<connect gate="A" pin="AN31/PWM4H/PMD7/RP87/RE7" pad="5"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="21"/>
<connect gate="A" pin="AN5/C1INA/VBUSON//VBUSST/RP37/RB5" pad="20"/>
<connect gate="A" pin="AN8/PMA6/RP40/RB8" pad="32"/>
<connect gate="A" pin="AN9/PMA7//RP41/RB9" pad="33"/>
<connect gate="A" pin="ASCL1/PMCS2/RP74/RD10" pad="70"/>
<connect gate="A" pin="ASCL2/RP18/RA2" pad="58"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="69"/>
<connect gate="A" pin="ASDA2/RP19/RA3" pad="59"/>
<connect gate="A" pin="AVDD" pad="30"/>
<connect gate="A" pin="AVSS" pad="31"/>
<connect gate="A" pin="BUSB" pad="55"/>
<connect gate="A" pin="C1INC/SDI2/PMA4/RP119/RG7" pad="11"/>
<connect gate="A" pin="C1IND/SCK2/PMA5/RP118/RG6" pad="10"/>
<connect gate="A" pin="C2INC/PMA2/RP121/RG9" pad="14"/>
<connect gate="A" pin="C2IND/SDO2/PMA3/RP120/RG8" pad="12"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="84"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="83"/>
<connect gate="A" pin="D+/RG2" pad="57"/>
<connect gate="A" pin="D-/RG3" pad="56"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="77"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="72"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="63"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="64"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="26"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="74"/>
<connect gate="A" pin="PGEC3/AN1/RP33/RB1" pad="24"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="27"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="73"/>
<connect gate="A" pin="PGED3/AN0/RP32/RB0" pad="25"/>
<connect gate="A" pin="PMBE/RP67/RD3" pad="78"/>
<connect gate="A" pin="PMCS1/RP75/RD11" pad="71"/>
<connect gate="A" pin="PMRD/RP69/RD5" pad="82"/>
<connect gate="A" pin="PMWR/RP68/RD4" pad="81"/>
<connect gate="A" pin="RP104/RF8" pad="53"/>
<connect gate="A" pin="RP108/RF12" pad="40"/>
<connect gate="A" pin="RP109/RF13" pad="39"/>
<connect gate="A" pin="RP112/RG0" pad="90"/>
<connect gate="A" pin="RP113/RG1" pad="89"/>
<connect gate="A" pin="RP124/RG12" pad="96"/>
<connect gate="A" pin="RP125/RG13" pad="97"/>
<connect gate="A" pin="RP126/RG14" pad="95"/>
<connect gate="A" pin="RP127/RG15" pad="1"/>
<connect gate="A" pin="RP30/RA14" pad="66"/>
<connect gate="A" pin="RP31/RA15" pad="67"/>
<connect gate="A" pin="RP76/RD12" pad="79"/>
<connect gate="A" pin="RP77/RD13" pad="80"/>
<connect gate="A" pin="RP78/RD14" pad="47"/>
<connect gate="A" pin="RP79/RD15" pad="48"/>
<connect gate="A" pin="RP98/RF2" pad="52"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="68"/>
<connect gate="A" pin="SCL2/PMA8/RP101/RF5" pad="50"/>
<connect gate="A" pin="SDA2/PMA9/RP100/RF4" pad="49"/>
<connect gate="A" pin="TCK/RP17/RA1" pad="38"/>
<connect gate="A" pin="TDI/RP20/RA4" pad="60"/>
<connect gate="A" pin="TDO/RP21/RA5" pad="61"/>
<connect gate="A" pin="TMS/RP16/RA0" pad="17"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="51"/>
<connect gate="A" pin="VBUS" pad="54"/>
<connect gate="A" pin="VCAP" pad="85"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="87"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="88"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="76"/>
<connect gate="A" pin="VDD" pad="62"/>
<connect gate="A" pin="VDD_2" pad="2"/>
<connect gate="A" pin="VDD_3" pad="16"/>
<connect gate="A" pin="VDD_4" pad="37"/>
<connect gate="A" pin="VDD_5" pad="46"/>
<connect gate="A" pin="VDD_6" pad="86"/>
<connect gate="A" pin="VREF+/RA10" pad="29"/>
<connect gate="A" pin="VREF-/RA9" pad="28"/>
<connect gate="A" pin="VSS" pad="65"/>
<connect gate="A" pin="VSS_2" pad="15"/>
<connect gate="A" pin="VSS_3" pad="36"/>
<connect gate="A" pin="VSS_4" pad="45"/>
<connect gate="A" pin="VSS_5" pad="75"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP256MU810-X_PT" prefix="IC">
<description>dsPIC33EP256MU810-X_PT, TQFP100 121X12</description>
<gates>
<gate name="A" symbol="DSPIC33EP256MU810-X_PT"/>
</gates>
<devices>
<device name="" package="TQFP100_12X12MC">
<connects>
<connect gate="A" pin="!MCLR" pad="13"/>
<connect gate="A" pin="AN10/CVREF/PMA13/RP42/RB10" pad="34"/>
<connect gate="A" pin="AN11/PMA12/RP43/RB11" pad="35"/>
<connect gate="A" pin="AN12/PMA11/RP44/RB12" pad="41"/>
<connect gate="A" pin="AN13/PMA10/RP45/RB13" pad="42"/>
<connect gate="A" pin="AN14/PMA1/RP46/RB14" pad="43"/>
<connect gate="A" pin="AN15/PMA0/RP47/RB15" pad="44"/>
<connect gate="A" pin="AN16/PWM5L/RP49/RC1" pad="6"/>
<connect gate="A" pin="AN17/PWM5H/RP50/RC2" pad="7"/>
<connect gate="A" pin="AN18/PWM6L/RP51/RC3" pad="8"/>
<connect gate="A" pin="AN19/PWM6H/RP52/RC4" pad="9"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="23"/>
<connect gate="A" pin="AN20/RP88/RE8" pad="18"/>
<connect gate="A" pin="AN21/RP89/RE9" pad="19"/>
<connect gate="A" pin="AN22/RP22/RA6" pad="91"/>
<connect gate="A" pin="AN23/RP23/RA7" pad="92"/>
<connect gate="A" pin="AN24/PWM1L/PMD0/RP80/RE0" pad="93"/>
<connect gate="A" pin="AN25/PWM1H/PMD1/RP81/RE1" pad="94"/>
<connect gate="A" pin="AN26/PWM2L/PMD2/RP82/RE2" pad="98"/>
<connect gate="A" pin="AN27/PWM2H/PMD3/RP83/RE3" pad="99"/>
<connect gate="A" pin="AN28/PWM3L/PMD4/RP84/RE4" pad="100"/>
<connect gate="A" pin="AN29/PWM3H/PMD5/RP85/RE5" pad="3"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="22"/>
<connect gate="A" pin="AN30/PWM4L/PMD6/RP86/RE6" pad="4"/>
<connect gate="A" pin="AN31/PWM4H/PMD7/RP87/RE7" pad="5"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="21"/>
<connect gate="A" pin="AN5/C1INA/VBUSON//VBUSST/RP37/RB5" pad="20"/>
<connect gate="A" pin="AN8/PMA6/RP40/RB8" pad="32"/>
<connect gate="A" pin="AN9/PMA7//RP41/RB9" pad="33"/>
<connect gate="A" pin="ASCL1/PMCS2/RP74/RD10" pad="70"/>
<connect gate="A" pin="ASCL2/RP18/RA2" pad="58"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="69"/>
<connect gate="A" pin="ASDA2/RP19/RA3" pad="59"/>
<connect gate="A" pin="AVDD" pad="30"/>
<connect gate="A" pin="AVSS" pad="31"/>
<connect gate="A" pin="BUSB" pad="55"/>
<connect gate="A" pin="C1INC/SDI2/PMA4/RP119/RG7" pad="11"/>
<connect gate="A" pin="C1IND/SCK2/PMA5/RP118/RG6" pad="10"/>
<connect gate="A" pin="C2INC/PMA2/RP121/RG9" pad="14"/>
<connect gate="A" pin="C2IND/SDO2/PMA3/RP120/RG8" pad="12"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="84"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="83"/>
<connect gate="A" pin="D+/RG2" pad="57"/>
<connect gate="A" pin="D-/RG3" pad="56"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="77"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="72"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="63"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="64"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="26"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="74"/>
<connect gate="A" pin="PGEC3/AN1/RP33/RB1" pad="24"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="27"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="73"/>
<connect gate="A" pin="PGED3/AN0/RP32/RB0" pad="25"/>
<connect gate="A" pin="PMBE/RP67/RD3" pad="78"/>
<connect gate="A" pin="PMCS1/RP75/RD11" pad="71"/>
<connect gate="A" pin="PMRD/RP69/RD5" pad="82"/>
<connect gate="A" pin="PMWR/RP68/RD4" pad="81"/>
<connect gate="A" pin="RP104/RF8" pad="53"/>
<connect gate="A" pin="RP108/RF12" pad="40"/>
<connect gate="A" pin="RP109/RF13" pad="39"/>
<connect gate="A" pin="RP112/RG0" pad="90"/>
<connect gate="A" pin="RP113/RG1" pad="89"/>
<connect gate="A" pin="RP124/RG12" pad="96"/>
<connect gate="A" pin="RP125/RG13" pad="97"/>
<connect gate="A" pin="RP126/RG14" pad="95"/>
<connect gate="A" pin="RP127/RG15" pad="1"/>
<connect gate="A" pin="RP30/RA14" pad="66"/>
<connect gate="A" pin="RP31/RA15" pad="67"/>
<connect gate="A" pin="RP76/RD12" pad="79"/>
<connect gate="A" pin="RP77/RD13" pad="80"/>
<connect gate="A" pin="RP78/RD14" pad="47"/>
<connect gate="A" pin="RP79/RD15" pad="48"/>
<connect gate="A" pin="RP98/RF2" pad="52"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="68"/>
<connect gate="A" pin="SCL2/PMA8/RP101/RF5" pad="50"/>
<connect gate="A" pin="SDA2/PMA9/RP100/RF4" pad="49"/>
<connect gate="A" pin="TCK/RP17/RA1" pad="38"/>
<connect gate="A" pin="TDI/RP20/RA4" pad="60"/>
<connect gate="A" pin="TDO/RP21/RA5" pad="61"/>
<connect gate="A" pin="TMS/RP16/RA0" pad="17"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="51"/>
<connect gate="A" pin="VBUS" pad="54"/>
<connect gate="A" pin="VCAP" pad="85"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="87"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="88"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="76"/>
<connect gate="A" pin="VDD" pad="62"/>
<connect gate="A" pin="VDD_2" pad="2"/>
<connect gate="A" pin="VDD_3" pad="16"/>
<connect gate="A" pin="VDD_4" pad="37"/>
<connect gate="A" pin="VDD_5" pad="46"/>
<connect gate="A" pin="VDD_6" pad="86"/>
<connect gate="A" pin="VREF+/RA10" pad="29"/>
<connect gate="A" pin="VREF-/RA9" pad="28"/>
<connect gate="A" pin="VSS" pad="65"/>
<connect gate="A" pin="VSS_2" pad="15"/>
<connect gate="A" pin="VSS_3" pad="36"/>
<connect gate="A" pin="VSS_4" pad="45"/>
<connect gate="A" pin="VSS_5" pad="75"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP512MU810-X_BG" prefix="IC">
<description>dsPIC33EP512MU810-X_BG XBGA121 10x10</description>
<gates>
<gate name="A" symbol="DSPIC33EP512MU810-X_BG_A"/>
</gates>
<devices>
<device name="" package="XBGA121_10X10MC">
<connects>
<connect gate="A" pin="!MCLR" pad="F1"/>
<connect gate="A" pin="AN10/CVREF/PMA13/RP42/RB10" pad="L5"/>
<connect gate="A" pin="AN11/PMA12/RP43/RB11" pad="J5"/>
<connect gate="A" pin="AN12/PMA11/RP44/RB12" pad="J7"/>
<connect gate="A" pin="AN13/PMA10/RP45/RB13" pad="L7"/>
<connect gate="A" pin="AN14/PMA1/RP46/RB14" pad="K7"/>
<connect gate="A" pin="AN15/PMA0/RP47/RB15" pad="L8"/>
<connect gate="A" pin="AN16/PWM5L/RP49/RC1" pad="D1"/>
<connect gate="A" pin="AN17/PWM5H/RP50/RC2" pad="E4"/>
<connect gate="A" pin="AN18/PWM6L/RP51/RC3" pad="E2"/>
<connect gate="A" pin="AN19/PWM6H/RP52/RC4" pad="E1"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="J2"/>
<connect gate="A" pin="AN20/RP88/RE8" pad="G1"/>
<connect gate="A" pin="AN21/RP89/RE9" pad="G2"/>
<connect gate="A" pin="AN22/RP22/RA6" pad="C5"/>
<connect gate="A" pin="AN23/RP23/RA7" pad="B5"/>
<connect gate="A" pin="AN24/PWM1L/PMD0/RP80/RE0" pad="A4"/>
<connect gate="A" pin="AN25/PWM1H/PMD1/RP81/RE1" pad="B4"/>
<connect gate="A" pin="AN26/PWM2L/PMD2/RP82/RE2" pad="B3"/>
<connect gate="A" pin="AN27/PWM2H/PMD3/RP83/RE3" pad="A2"/>
<connect gate="A" pin="AN28/PWM3L/PMD4/RP84/RE4" pad="A1"/>
<connect gate="A" pin="AN29/PWM3H/PMD5/RP85/RE5" pad="D3"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="J1"/>
<connect gate="A" pin="AN30/PWM4L/PMD6/RP86/RE6" pad="C1"/>
<connect gate="A" pin="AN31/PWM4H/PMD7/RP87/RE7" pad="D2"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="H2"/>
<connect gate="A" pin="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" pad="H1"/>
<connect gate="A" pin="AN8/PMA6/RP40/RB8" pad="K4"/>
<connect gate="A" pin="AN9/PMA7//RP41/RB9" pad="L4"/>
<connect gate="A" pin="ASCL1/PMCS2/RP74/RD10" pad="D11"/>
<connect gate="A" pin="ASCL2/RP18/RA2" pad="H11"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="E10"/>
<connect gate="A" pin="ASDA2/RP19/RA3" pad="G10"/>
<connect gate="A" pin="AVDD" pad="J4"/>
<connect gate="A" pin="AVSS" pad="L3"/>
<connect gate="A" pin="C1INC/SDI2/PMA4/RP119/RG7" pad="F4"/>
<connect gate="A" pin="C1IND/SCK2/PMA5/RP118/RG6" pad="E3"/>
<connect gate="A" pin="C2INC/PMA2/RP121/RG9" pad="F3"/>
<connect gate="A" pin="C2IND/SDO2/PMA3/RP120/RG8" pad="F2"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="C7"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="D7"/>
<connect gate="A" pin="D+/RG2" pad="H10"/>
<connect gate="A" pin="D-/RG3" pad="J11"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="A10"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="D9"/>
<connect gate="A" pin="NO_CONNECT" pad="A8"/>
<connect gate="A" pin="NO_CONNECT_10" pad="E7"/>
<connect gate="A" pin="NO_CONNECT_11" pad="K5"/>
<connect gate="A" pin="NO_CONNECT_12" pad="J9"/>
<connect gate="A" pin="NO_CONNECT_13" pad="J8"/>
<connect gate="A" pin="NO_CONNECT_14" pad="H7"/>
<connect gate="A" pin="NO_CONNECT_15" pad="H5"/>
<connect gate="A" pin="NO_CONNECT_16" pad="H4"/>
<connect gate="A" pin="NO_CONNECT_17" pad="H3"/>
<connect gate="A" pin="NO_CONNECT_18" pad="G8"/>
<connect gate="A" pin="NO_CONNECT_19" pad="G4"/>
<connect gate="A" pin="NO_CONNECT_2" pad="B1"/>
<connect gate="A" pin="NO_CONNECT_20" pad="F7"/>
<connect gate="A" pin="NO_CONNECT_21" pad="F6"/>
<connect gate="A" pin="NO_CONNECT_3" pad="C6"/>
<connect gate="A" pin="NO_CONNECT_4" pad="C9"/>
<connect gate="A" pin="NO_CONNECT_5" pad="D4"/>
<connect gate="A" pin="NO_CONNECT_6" pad="D5"/>
<connect gate="A" pin="NO_CONNECT_7" pad="D6"/>
<connect gate="A" pin="NO_CONNECT_8" pad="D10"/>
<connect gate="A" pin="NO_CONNECT_9" pad="E5"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="F9"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="F11"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="L1"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="B11"/>
<connect gate="A" pin="PGEC3/AN1/RP33/RB1" pad="K1"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="J3"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="C10"/>
<connect gate="A" pin="PGED3/AN0/RP32/RB0" pad="K2"/>
<connect gate="A" pin="PMBE/RP67/RD3" pad="B9"/>
<connect gate="A" pin="PMCS1/RP75/RD11" pad="C11"/>
<connect gate="A" pin="PMRD/RP69/RD5" pad="B8"/>
<connect gate="A" pin="PMWR/RP68/RD4" pad="C8"/>
<connect gate="A" pin="RP104/RF8" pad="J10"/>
<connect gate="A" pin="RP108/RF12" pad="K6"/>
<connect gate="A" pin="RP109/RF13" pad="L6"/>
<connect gate="A" pin="RP112/RG0" pad="A5"/>
<connect gate="A" pin="RP113/RG1" pad="E6"/>
<connect gate="A" pin="RP124/RG12" pad="C3"/>
<connect gate="A" pin="RP125/RG13" pad="A3"/>
<connect gate="A" pin="RP126/RG14" pad="C4"/>
<connect gate="A" pin="RP127/RG15" pad="B2"/>
<connect gate="A" pin="RP30/RA14" pad="E11"/>
<connect gate="A" pin="RP31/RA15" pad="E8"/>
<connect gate="A" pin="RP76/RD12" pad="A9"/>
<connect gate="A" pin="RP77/RD13" pad="D8"/>
<connect gate="A" pin="RP78/RD14" pad="L9"/>
<connect gate="A" pin="RP79/RD15" pad="K9"/>
<connect gate="A" pin="RP98/RF2" pad="K11"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="E9"/>
<connect gate="A" pin="SCL2/PMA8/RP101/RF5" pad="L11"/>
<connect gate="A" pin="SDA2/PMA9/RP100/RF4" pad="L10"/>
<connect gate="A" pin="TCK/RP17/RA1" pad="J6"/>
<connect gate="A" pin="TDI/RP20/RA4" pad="G11"/>
<connect gate="A" pin="TDO/RP21/RA5" pad="G9"/>
<connect gate="A" pin="TMS/RP16/RA0" pad="G3"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="K10"/>
<connect gate="A" pin="VBUS" pad="H8"/>
<connect gate="A" pin="VCAP" pad="B7"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="B6"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="A6"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="A11"/>
<connect gate="A" pin="VDD" pad="F8"/>
<connect gate="A" pin="VDD_2" pad="A7"/>
<connect gate="A" pin="VDD_3" pad="C2"/>
<connect gate="A" pin="VDD_4" pad="K8"/>
<connect gate="A" pin="VDD_5" pad="H6"/>
<connect gate="A" pin="VDD_6" pad="G5"/>
<connect gate="A" pin="VREF+/RA10" pad="K3"/>
<connect gate="A" pin="VREF-/RA9" pad="L2"/>
<connect gate="A" pin="VSS" pad="F10"/>
<connect gate="A" pin="VSS_2" pad="B10"/>
<connect gate="A" pin="VSS_3" pad="F5"/>
<connect gate="A" pin="VSS_4" pad="G7"/>
<connect gate="A" pin="VSS_5" pad="G6"/>
<connect gate="A" pin="VUSB" pad="H9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP512MU810-X_PF" prefix="IC">
<description>dsPIC33EP512MU810-X_PF TQFP100 14x14</description>
<gates>
<gate name="A" symbol="DSPIC33EP512MU810-X_PF"/>
</gates>
<devices>
<device name="" package="TQFP100_14X14MC">
<connects>
<connect gate="A" pin="!MCLR" pad="13"/>
<connect gate="A" pin="AN10/CVREF/PMA13/RP42/RB10" pad="34"/>
<connect gate="A" pin="AN11/PMA12/RP43/RB11" pad="35"/>
<connect gate="A" pin="AN12/PMA11/RP44/RB12" pad="41"/>
<connect gate="A" pin="AN13/PMA10/RP45/RB13" pad="42"/>
<connect gate="A" pin="AN14/PMA1/RP46/RB14" pad="43"/>
<connect gate="A" pin="AN15/PMA0/RP47/RB15" pad="44"/>
<connect gate="A" pin="AN16/PWM5L/RP49/RC1" pad="6"/>
<connect gate="A" pin="AN17/PWM5H/RP50/RC2" pad="7"/>
<connect gate="A" pin="AN18/PWM6L/RP51/RC3" pad="8"/>
<connect gate="A" pin="AN19/PWM6H/RP52/RC4" pad="9"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="23"/>
<connect gate="A" pin="AN20/RP88/RE8" pad="18"/>
<connect gate="A" pin="AN21/RP89/RE9" pad="19"/>
<connect gate="A" pin="AN22/RP22/RA6" pad="91"/>
<connect gate="A" pin="AN23/RP23/RA7" pad="92"/>
<connect gate="A" pin="AN24/PWM1L/PMD0/RP80/RE0" pad="93"/>
<connect gate="A" pin="AN25/PWM1H/PMD1/RP81/RE1" pad="94"/>
<connect gate="A" pin="AN26/PWM2L/PMD2/RP82/RE2" pad="98"/>
<connect gate="A" pin="AN27/PWM2H/PMD3/RP83/RE3" pad="99"/>
<connect gate="A" pin="AN28/PWM3L/PMD4/RP84/RE4" pad="100"/>
<connect gate="A" pin="AN29/PWM3H/PMD5/RP85/RE5" pad="3"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="22"/>
<connect gate="A" pin="AN30/PWM4L/PMD6/RP86/RE6" pad="4"/>
<connect gate="A" pin="AN31/PWM4H/PMD7/RP87/RE7" pad="5"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="21"/>
<connect gate="A" pin="AN5/C1INA/VBUSON//VBUSST/RP37/RB5" pad="20"/>
<connect gate="A" pin="AN8/PMA6/RP40/RB8" pad="32"/>
<connect gate="A" pin="AN9/PMA7//RP41/RB9" pad="33"/>
<connect gate="A" pin="ASCL1/PMCS2/RP74/RD10" pad="70"/>
<connect gate="A" pin="ASCL2/RP18/RA2" pad="58"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="69"/>
<connect gate="A" pin="ASDA2/RP19/RA3" pad="59"/>
<connect gate="A" pin="AVDD" pad="30"/>
<connect gate="A" pin="AVSS" pad="31"/>
<connect gate="A" pin="BUSB" pad="55"/>
<connect gate="A" pin="C1INC/SDI2/PMA4/RP119/RG7" pad="11"/>
<connect gate="A" pin="C1IND/SCK2/PMA5/RP118/RG6" pad="10"/>
<connect gate="A" pin="C2INC/PMA2/RP121/RG9" pad="14"/>
<connect gate="A" pin="C2IND/SDO2/PMA3/RP120/RG8" pad="12"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="84"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="83"/>
<connect gate="A" pin="D+/RG2" pad="57"/>
<connect gate="A" pin="D-/RG3" pad="56"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="77"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="72"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="63"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="64"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="26"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="74"/>
<connect gate="A" pin="PGEC3/AN1/RP33/RB1" pad="24"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="27"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="73"/>
<connect gate="A" pin="PGED3/AN0/RP32/RB0" pad="25"/>
<connect gate="A" pin="PMBE/RP67/RD3" pad="78"/>
<connect gate="A" pin="PMCS1/RP75/RD11" pad="71"/>
<connect gate="A" pin="PMRD/RP69/RD5" pad="82"/>
<connect gate="A" pin="PMWR/RP68/RD4" pad="81"/>
<connect gate="A" pin="RP104/RF8" pad="53"/>
<connect gate="A" pin="RP108/RF12" pad="40"/>
<connect gate="A" pin="RP109/RF13" pad="39"/>
<connect gate="A" pin="RP112/RG0" pad="90"/>
<connect gate="A" pin="RP113/RG1" pad="89"/>
<connect gate="A" pin="RP124/RG12" pad="96"/>
<connect gate="A" pin="RP125/RG13" pad="97"/>
<connect gate="A" pin="RP126/RG14" pad="95"/>
<connect gate="A" pin="RP127/RG15" pad="1"/>
<connect gate="A" pin="RP30/RA14" pad="66"/>
<connect gate="A" pin="RP31/RA15" pad="67"/>
<connect gate="A" pin="RP76/RD12" pad="79"/>
<connect gate="A" pin="RP77/RD13" pad="80"/>
<connect gate="A" pin="RP78/RD14" pad="47"/>
<connect gate="A" pin="RP79/RD15" pad="48"/>
<connect gate="A" pin="RP98/RF2" pad="52"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="68"/>
<connect gate="A" pin="SCL2/PMA8/RP101/RF5" pad="50"/>
<connect gate="A" pin="SDA2/PMA9/RP100/RF4" pad="49"/>
<connect gate="A" pin="TCK/RP17/RA1" pad="38"/>
<connect gate="A" pin="TDI/RP20/RA4" pad="60"/>
<connect gate="A" pin="TDO/RP21/RA5" pad="61"/>
<connect gate="A" pin="TMS/RP16/RA0" pad="17"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="51"/>
<connect gate="A" pin="VBUS" pad="54"/>
<connect gate="A" pin="VCAP" pad="85"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="87"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="88"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="76"/>
<connect gate="A" pin="VDD" pad="62"/>
<connect gate="A" pin="VDD_2" pad="2"/>
<connect gate="A" pin="VDD_3" pad="16"/>
<connect gate="A" pin="VDD_4" pad="37"/>
<connect gate="A" pin="VDD_5" pad="46"/>
<connect gate="A" pin="VDD_6" pad="86"/>
<connect gate="A" pin="VREF+/RA10" pad="29"/>
<connect gate="A" pin="VREF-/RA9" pad="28"/>
<connect gate="A" pin="VSS" pad="65"/>
<connect gate="A" pin="VSS_2" pad="15"/>
<connect gate="A" pin="VSS_3" pad="36"/>
<connect gate="A" pin="VSS_4" pad="45"/>
<connect gate="A" pin="VSS_5" pad="75"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP512MU810-X_PT" prefix="IC">
<description>dsPIC33EP512MU810-X_PT; TQFP 100 12x12</description>
<gates>
<gate name="A" symbol="DSPIC33EP512MU810-X_PT"/>
</gates>
<devices>
<device name="" package="TQFP100_12X12MC">
<connects>
<connect gate="A" pin="!MCLR" pad="13"/>
<connect gate="A" pin="AN10/CVREF/PMA13/RP42/RB10" pad="34"/>
<connect gate="A" pin="AN11/PMA12/RP43/RB11" pad="35"/>
<connect gate="A" pin="AN12/PMA11/RP44/RB12" pad="41"/>
<connect gate="A" pin="AN13/PMA10/RP45/RB13" pad="42"/>
<connect gate="A" pin="AN14/PMA1/RP46/RB14" pad="43"/>
<connect gate="A" pin="AN15/PMA0/RP47/RB15" pad="44"/>
<connect gate="A" pin="AN16/PWM5L/RP49/RC1" pad="6"/>
<connect gate="A" pin="AN17/PWM5H/RP50/RC2" pad="7"/>
<connect gate="A" pin="AN18/PWM6L/RP51/RC3" pad="8"/>
<connect gate="A" pin="AN19/PWM6H/RP52/RC4" pad="9"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="23"/>
<connect gate="A" pin="AN20/RP88/RE8" pad="18"/>
<connect gate="A" pin="AN21/RP89/RE9" pad="19"/>
<connect gate="A" pin="AN22/RP22/RA6" pad="91"/>
<connect gate="A" pin="AN23/RP23/RA7" pad="92"/>
<connect gate="A" pin="AN24/PWM1L/PMD0/RP80/RE0" pad="93"/>
<connect gate="A" pin="AN25/PWM1H/PMD1/RP81/RE1" pad="94"/>
<connect gate="A" pin="AN26/PWM2L/PMD2/RP82/RE2" pad="98"/>
<connect gate="A" pin="AN27/PWM2H/PMD3/RP83/RE3" pad="99"/>
<connect gate="A" pin="AN28/PWM3L/PMD4/RP84/RE4" pad="100"/>
<connect gate="A" pin="AN29/PWM3H/PMD5/RP85/RE5" pad="3"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="22"/>
<connect gate="A" pin="AN30/PWM4L/PMD6/RP86/RE6" pad="4"/>
<connect gate="A" pin="AN31/PWM4H/PMD7/RP87/RE7" pad="5"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="21"/>
<connect gate="A" pin="AN5/C1INA/VBUSON//VBUSST/RP37/RB5" pad="20"/>
<connect gate="A" pin="AN8/PMA6/RP40/RB8" pad="32"/>
<connect gate="A" pin="AN9/PMA7//RP41/RB9" pad="33"/>
<connect gate="A" pin="ASCL1/PMCS2/RP74/RD10" pad="70"/>
<connect gate="A" pin="ASCL2/RP18/RA2" pad="58"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="69"/>
<connect gate="A" pin="ASDA2/RP19/RA3" pad="59"/>
<connect gate="A" pin="AVDD" pad="30"/>
<connect gate="A" pin="AVSS" pad="31"/>
<connect gate="A" pin="BUSB" pad="55"/>
<connect gate="A" pin="C1INC/SDI2/PMA4/RP119/RG7" pad="11"/>
<connect gate="A" pin="C1IND/SCK2/PMA5/RP118/RG6" pad="10"/>
<connect gate="A" pin="C2INC/PMA2/RP121/RG9" pad="14"/>
<connect gate="A" pin="C2IND/SDO2/PMA3/RP120/RG8" pad="12"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="84"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="83"/>
<connect gate="A" pin="D+/RG2" pad="57"/>
<connect gate="A" pin="D-/RG3" pad="56"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="77"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="72"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="63"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="64"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="26"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="74"/>
<connect gate="A" pin="PGEC3/AN1/RP33/RB1" pad="24"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="27"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="73"/>
<connect gate="A" pin="PGED3/AN0/RP32/RB0" pad="25"/>
<connect gate="A" pin="PMBE/RP67/RD3" pad="78"/>
<connect gate="A" pin="PMCS1/RP75/RD11" pad="71"/>
<connect gate="A" pin="PMRD/RP69/RD5" pad="82"/>
<connect gate="A" pin="PMWR/RP68/RD4" pad="81"/>
<connect gate="A" pin="RP104/RF8" pad="53"/>
<connect gate="A" pin="RP108/RF12" pad="40"/>
<connect gate="A" pin="RP109/RF13" pad="39"/>
<connect gate="A" pin="RP112/RG0" pad="90"/>
<connect gate="A" pin="RP113/RG1" pad="89"/>
<connect gate="A" pin="RP124/RG12" pad="96"/>
<connect gate="A" pin="RP125/RG13" pad="97"/>
<connect gate="A" pin="RP126/RG14" pad="95"/>
<connect gate="A" pin="RP127/RG15" pad="1"/>
<connect gate="A" pin="RP30/RA14" pad="66"/>
<connect gate="A" pin="RP31/RA15" pad="67"/>
<connect gate="A" pin="RP76/RD12" pad="79"/>
<connect gate="A" pin="RP77/RD13" pad="80"/>
<connect gate="A" pin="RP78/RD14" pad="47"/>
<connect gate="A" pin="RP79/RD15" pad="48"/>
<connect gate="A" pin="RP98/RF2" pad="52"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="68"/>
<connect gate="A" pin="SCL2/PMA8/RP101/RF5" pad="50"/>
<connect gate="A" pin="SDA2/PMA9/RP100/RF4" pad="49"/>
<connect gate="A" pin="TCK/RP17/RA1" pad="38"/>
<connect gate="A" pin="TDI/RP20/RA4" pad="60"/>
<connect gate="A" pin="TDO/RP21/RA5" pad="61"/>
<connect gate="A" pin="TMS/RP16/RA0" pad="17"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="51"/>
<connect gate="A" pin="VBUS" pad="54"/>
<connect gate="A" pin="VCAP" pad="85"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="87"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="88"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="76"/>
<connect gate="A" pin="VDD" pad="62"/>
<connect gate="A" pin="VDD_2" pad="2"/>
<connect gate="A" pin="VDD_3" pad="16"/>
<connect gate="A" pin="VDD_4" pad="37"/>
<connect gate="A" pin="VDD_5" pad="46"/>
<connect gate="A" pin="VDD_6" pad="86"/>
<connect gate="A" pin="VREF+/RA10" pad="29"/>
<connect gate="A" pin="VREF-/RA9" pad="28"/>
<connect gate="A" pin="VSS" pad="65"/>
<connect gate="A" pin="VSS_2" pad="15"/>
<connect gate="A" pin="VSS_3" pad="36"/>
<connect gate="A" pin="VSS_4" pad="45"/>
<connect gate="A" pin="VSS_5" pad="75"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP512MU814-X_PH" prefix="IC">
<description>dsPIC33EP512MU814 16-bit Microcontrollers and Digital Signal Controllers (up to 512 KB Flash and 52 KB SRAM) with High-SpeedPWM, USB, and Advanced Analog</description>
<gates>
<gate name="A" symbol="DSPIC33EP512MU814-X_PH_A"/>
</gates>
<devices>
<device name="" package="TQFP144_16X16MC">
<connects>
<connect gate="A" pin="!MCLR" pad="19"/>
<connect gate="A" pin="AN10/CVREF/RP42/RB10" pad="49"/>
<connect gate="A" pin="AN11/RP43/RB11" pad="50"/>
<connect gate="A" pin="AN12/RP44/RB12" pad="59"/>
<connect gate="A" pin="AN13/RP45/RB13" pad="60"/>
<connect gate="A" pin="AN14/RP46/RB14" pad="61"/>
<connect gate="A" pin="AN15/RP47/RB15" pad="62"/>
<connect gate="A" pin="AN16/PWM5L/RP49/RC1" pad="10"/>
<connect gate="A" pin="AN17/PWM5H/RP50/RC2" pad="11"/>
<connect gate="A" pin="AN18/PWM6L/RP51/RC3" pad="12"/>
<connect gate="A" pin="AN19/PWM6H/RP52/RC4" pad="13"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="33"/>
<connect gate="A" pin="AN20/RP88/RE8" pad="26"/>
<connect gate="A" pin="AN21/RP89/RE9" pad="27"/>
<connect gate="A" pin="AN22/RP22/RA6" pad="130"/>
<connect gate="A" pin="AN23/RP23/RA7" pad="131"/>
<connect gate="A" pin="AN24/PWM1L/RP80/RE0" pad="136"/>
<connect gate="A" pin="AN25/PWM1H/RP81/RE1" pad="137"/>
<connect gate="A" pin="AN26/PWM2L/RP82/RE2" pad="142"/>
<connect gate="A" pin="AN27/PWM2H/RP83/RE3" pad="143"/>
<connect gate="A" pin="AN28/PWM3L/RP84/RE4" pad="144"/>
<connect gate="A" pin="AN29/PWM3H/RP85/RE5" pad="3"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="32"/>
<connect gate="A" pin="AN30/PWM4L/RP86/RE6" pad="4"/>
<connect gate="A" pin="AN31/PWM4H/RP87/RE7" pad="5"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="31"/>
<connect gate="A" pin="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" pad="30"/>
<connect gate="A" pin="AN8/RP40/RB8" pad="47"/>
<connect gate="A" pin="AN9/RP41/RB9" pad="48"/>
<connect gate="A" pin="ASCL1/RP74/RD10" pad="99"/>
<connect gate="A" pin="ASCL2/RP18/RA2" pad="85"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="98"/>
<connect gate="A" pin="ASDA2/RP19/RA3" pad="86"/>
<connect gate="A" pin="AVDD" pad="41"/>
<connect gate="A" pin="AVSS" pad="42"/>
<connect gate="A" pin="C1INC/SDI2/RP119/RG7" pad="17"/>
<connect gate="A" pin="C1IND/SCK2/RP118/RG6" pad="16"/>
<connect gate="A" pin="C2INC/RP121/RG9" pad="20"/>
<connect gate="A" pin="C2IND/SDO2/RP120/RG8" pad="18"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="122"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="121"/>
<connect gate="A" pin="D+/RG2" pad="80"/>
<connect gate="A" pin="D-/RG3" pad="79"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="110"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="105"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="90"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="91"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="37"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="107"/>
<connect gate="A" pin="PGEC3/AN1/RP33/RB1" pad="34"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="38"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="106"/>
<connect gate="A" pin="PGED3/AN0/RP32/RB0" pad="35"/>
<connect gate="A" pin="PMA0/RJ0" pad="115"/>
<connect gate="A" pin="PMA1/RJ1" pad="116"/>
<connect gate="A" pin="PMA10/RJ10" pad="8"/>
<connect gate="A" pin="PMA11/RJ11" pad="9"/>
<connect gate="A" pin="PMA12/RJ12" pad="14"/>
<connect gate="A" pin="PMA13/RJ13" pad="15"/>
<connect gate="A" pin="PMA2/RJ2" pad="117"/>
<connect gate="A" pin="PMA3/RJ3" pad="118"/>
<connect gate="A" pin="PMA4/RJ4" pad="132"/>
<connect gate="A" pin="PMA5/RJ5" pad="133"/>
<connect gate="A" pin="PMA6/RJ6" pad="134"/>
<connect gate="A" pin="PMA7/RJ7" pad="135"/>
<connect gate="A" pin="PMBE/RK13" pad="55"/>
<connect gate="A" pin="PMCS1/RK11" pad="94"/>
<connect gate="A" pin="PMCS2/RK12" pad="93"/>
<connect gate="A" pin="PMD0/RH0" pad="43"/>
<connect gate="A" pin="PMD1/RH1" pad="44"/>
<connect gate="A" pin="PMD2/RH2" pad="45"/>
<connect gate="A" pin="PMD3/RH3" pad="46"/>
<connect gate="A" pin="PMD4/RH4" pad="65"/>
<connect gate="A" pin="PMD5/RH5" pad="66"/>
<connect gate="A" pin="PMD6/RH6" pad="67"/>
<connect gate="A" pin="PMD7/RH7" pad="68"/>
<connect gate="A" pin="PMRD/RK15" pad="53"/>
<connect gate="A" pin="PMWR/RK14" pad="54"/>
<connect gate="A" pin="PWM7H/PMA9/RJ9" pad="7"/>
<connect gate="A" pin="PWM7L/PMA8/RJ8" pad="6"/>
<connect gate="A" pin="RH10" pad="83"/>
<connect gate="A" pin="RH11" pad="84"/>
<connect gate="A" pin="RH12" pad="101"/>
<connect gate="A" pin="RH13" pad="102"/>
<connect gate="A" pin="RH14" pad="103"/>
<connect gate="A" pin="RH15" pad="104"/>
<connect gate="A" pin="RH8" pad="81"/>
<connect gate="A" pin="RH9" pad="82"/>
<connect gate="A" pin="RJ14" pad="21"/>
<connect gate="A" pin="RJ15" pad="22"/>
<connect gate="A" pin="RK0" pad="28"/>
<connect gate="A" pin="RK1" pad="29"/>
<connect gate="A" pin="RP104/RF8" pad="76"/>
<connect gate="A" pin="RP108/RF12" pad="58"/>
<connect gate="A" pin="RP109/RF13" pad="57"/>
<connect gate="A" pin="RP112/RG0" pad="129"/>
<connect gate="A" pin="RP113/RG1" pad="128"/>
<connect gate="A" pin="RP124/RG12" pad="139"/>
<connect gate="A" pin="RP125/RG13" pad="140"/>
<connect gate="A" pin="RP126/RG14" pad="138"/>
<connect gate="A" pin="RP127/RG15" pad="1"/>
<connect gate="A" pin="RP30/RA14" pad="95"/>
<connect gate="A" pin="RP31/RA15" pad="96"/>
<connect gate="A" pin="RP67/RD3" pad="111"/>
<connect gate="A" pin="RP68/RD4" pad="119"/>
<connect gate="A" pin="RP69/RD5" pad="120"/>
<connect gate="A" pin="RP75/RD11" pad="100"/>
<connect gate="A" pin="RP76/RD12" pad="113"/>
<connect gate="A" pin="RP77/RD13" pad="114"/>
<connect gate="A" pin="RP78/RD14" pad="69"/>
<connect gate="A" pin="RP79/RD15" pad="70"/>
<connect gate="A" pin="RP98/RF2" pad="75"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="97"/>
<connect gate="A" pin="SCL2/RP101/RF5" pad="72"/>
<connect gate="A" pin="SDA2/RP100/RF4" pad="71"/>
<connect gate="A" pin="TCK/RP17/RA1" pad="56"/>
<connect gate="A" pin="TDI/RP20/RA4" pad="87"/>
<connect gate="A" pin="TDO/RP21/RA5" pad="88"/>
<connect gate="A" pin="TMS/RP16/RA0" pad="25"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="74"/>
<connect gate="A" pin="VBUS" pad="77"/>
<connect gate="A" pin="VCAP" pad="123"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="126"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="127"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="109"/>
<connect gate="A" pin="VDD" pad="89"/>
<connect gate="A" pin="VDD_2" pad="2"/>
<connect gate="A" pin="VDD_3" pad="24"/>
<connect gate="A" pin="VDD_4" pad="52"/>
<connect gate="A" pin="VDD_5" pad="64"/>
<connect gate="A" pin="VDD_6" pad="124"/>
<connect gate="A" pin="VDD_7" pad="112"/>
<connect gate="A" pin="VREF+/RA10" pad="40"/>
<connect gate="A" pin="VREF-/RA9" pad="39"/>
<connect gate="A" pin="VSS" pad="73"/>
<connect gate="A" pin="VSS_2" pad="23"/>
<connect gate="A" pin="VSS_3" pad="36"/>
<connect gate="A" pin="VSS_4" pad="51"/>
<connect gate="A" pin="VSS_5" pad="63"/>
<connect gate="A" pin="VSS_6" pad="141"/>
<connect gate="A" pin="VSS_7" pad="125"/>
<connect gate="A" pin="VSS_8" pad="108"/>
<connect gate="A" pin="VSS_9" pad="92"/>
<connect gate="A" pin="VUSB" pad="78"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33EP512MU814-X_PL" prefix="IC">
<description>dsPIC33EP512MU814 16-bit Microcontrollers and Digital Signal Controllers (up to 512 KB Flash and 52 KB SRAM) with High-SpeedPWM, USB, and Advanced Analog</description>
<gates>
<gate name="A" symbol="DSPIC33EP512MU814-X_PL_A"/>
</gates>
<devices>
<device name="" package="LQFP144_20X20MC">
<connects>
<connect gate="A" pin="!MCLR" pad="19"/>
<connect gate="A" pin="AN10/CVREF/RP42/RB10" pad="49"/>
<connect gate="A" pin="AN11/RP43/RB11" pad="50"/>
<connect gate="A" pin="AN12/RP44/RB12" pad="59"/>
<connect gate="A" pin="AN13/RP45/RB13" pad="60"/>
<connect gate="A" pin="AN14/RP46/RB14" pad="61"/>
<connect gate="A" pin="AN15/RP47/RB15" pad="62"/>
<connect gate="A" pin="AN16/PWM5L/RP49/RC1" pad="10"/>
<connect gate="A" pin="AN17/PWM5H/RP50/RC2" pad="11"/>
<connect gate="A" pin="AN18/PWM6L/RP51/RC3" pad="12"/>
<connect gate="A" pin="AN19/PWM6H/RP52/RC4" pad="13"/>
<connect gate="A" pin="AN2/C2INB/VMIO/RP34/RB2" pad="33"/>
<connect gate="A" pin="AN20/RP88/RE8" pad="26"/>
<connect gate="A" pin="AN21/RP89/RE9" pad="27"/>
<connect gate="A" pin="AN22/RP22/RA6" pad="130"/>
<connect gate="A" pin="AN23/RP23/RA7" pad="131"/>
<connect gate="A" pin="AN24/PWM1L/RP80/RE0" pad="136"/>
<connect gate="A" pin="AN25/PWM1H/RP81/RE1" pad="137"/>
<connect gate="A" pin="AN26/PWM2L/RP82/RE2" pad="142"/>
<connect gate="A" pin="AN27/PWM2H/RP83/RE3" pad="143"/>
<connect gate="A" pin="AN28/PWM3L/RP84/RE4" pad="144"/>
<connect gate="A" pin="AN29/PWM3H/RP85/RE5" pad="3"/>
<connect gate="A" pin="AN3/C2INA/VPIO/RP35/RB3" pad="32"/>
<connect gate="A" pin="AN30/PWM4L/RP86/RE6" pad="4"/>
<connect gate="A" pin="AN31/PWM4H/RP87/RE7" pad="5"/>
<connect gate="A" pin="AN4/C1INB/USBOEN/RP36/RB4" pad="31"/>
<connect gate="A" pin="AN5/C1INA/VBUSON/VBUSST/RP37/RB5" pad="30"/>
<connect gate="A" pin="AN8/RP40/RB8" pad="47"/>
<connect gate="A" pin="AN9/RP41/RB9" pad="48"/>
<connect gate="A" pin="ASCL1/RP74/RD10" pad="99"/>
<connect gate="A" pin="ASCL2/RP18/RA2" pad="85"/>
<connect gate="A" pin="ASDA1/DPLN/RP73/RD9" pad="98"/>
<connect gate="A" pin="ASDA2/RP19/RA3" pad="86"/>
<connect gate="A" pin="AVDD" pad="41"/>
<connect gate="A" pin="AVSS" pad="42"/>
<connect gate="A" pin="C1INC/SDI2/RP119/RG7" pad="17"/>
<connect gate="A" pin="C1IND/SCK2/RP118/RG6" pad="16"/>
<connect gate="A" pin="C2INC/RP121/RG9" pad="20"/>
<connect gate="A" pin="C2IND/SDO2/RP120/RG8" pad="18"/>
<connect gate="A" pin="C3INA/VCMPST3/RP71/RD7" pad="122"/>
<connect gate="A" pin="C3INB/RP70/RD6" pad="121"/>
<connect gate="A" pin="D+/RG2" pad="80"/>
<connect gate="A" pin="D-/RG3" pad="79"/>
<connect gate="A" pin="DPH/RP66/RD2" pad="110"/>
<connect gate="A" pin="INT0/DMH/RP64/RD0" pad="105"/>
<connect gate="A" pin="OSC1/RP60/RC12" pad="90"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="91"/>
<connect gate="A" pin="PGEC1/AN6/RP38/RB6" pad="37"/>
<connect gate="A" pin="PGEC2/SOSCO/C3INC/T1CK/RP62/RC14" pad="107"/>
<connect gate="A" pin="PGEC3/AN1/RP33/RB1" pad="34"/>
<connect gate="A" pin="PGED1/AN7/RCV/RP39/RB7" pad="38"/>
<connect gate="A" pin="PGED2/SOSCI/C3IND/RP61/RC13" pad="106"/>
<connect gate="A" pin="PGED3/AN0/RP32/RB0" pad="35"/>
<connect gate="A" pin="PMA0/RJ0" pad="115"/>
<connect gate="A" pin="PMA1/RJ1" pad="116"/>
<connect gate="A" pin="PMA10/RJ10" pad="8"/>
<connect gate="A" pin="PMA11/RJ11" pad="9"/>
<connect gate="A" pin="PMA12/RJ12" pad="14"/>
<connect gate="A" pin="PMA13/RJ13" pad="15"/>
<connect gate="A" pin="PMA2/RJ2" pad="117"/>
<connect gate="A" pin="PMA3/RJ3" pad="118"/>
<connect gate="A" pin="PMA4/RJ4" pad="132"/>
<connect gate="A" pin="PMA5/RJ5" pad="133"/>
<connect gate="A" pin="PMA6/RJ6" pad="134"/>
<connect gate="A" pin="PMA7/RJ7" pad="135"/>
<connect gate="A" pin="PMBE/RK13" pad="55"/>
<connect gate="A" pin="PMCS1/RK11" pad="94"/>
<connect gate="A" pin="PMCS2/RK12" pad="93"/>
<connect gate="A" pin="PMD0/RH0" pad="43"/>
<connect gate="A" pin="PMD1/RH1" pad="44"/>
<connect gate="A" pin="PMD2/RH2" pad="45"/>
<connect gate="A" pin="PMD3/RH3" pad="46"/>
<connect gate="A" pin="PMD4/RH4" pad="65"/>
<connect gate="A" pin="PMD5/RH5" pad="66"/>
<connect gate="A" pin="PMD6/RH6" pad="67"/>
<connect gate="A" pin="PMD7/RH7" pad="68"/>
<connect gate="A" pin="PMRD/RK15" pad="53"/>
<connect gate="A" pin="PMWR/RK14" pad="54"/>
<connect gate="A" pin="PWM7H/PMA9/RJ9" pad="7"/>
<connect gate="A" pin="PWM7L/PMA8/RJ8" pad="6"/>
<connect gate="A" pin="RH10" pad="83"/>
<connect gate="A" pin="RH11" pad="84"/>
<connect gate="A" pin="RH12" pad="101"/>
<connect gate="A" pin="RH13" pad="102"/>
<connect gate="A" pin="RH14" pad="103"/>
<connect gate="A" pin="RH15" pad="104"/>
<connect gate="A" pin="RH8" pad="81"/>
<connect gate="A" pin="RH9" pad="82"/>
<connect gate="A" pin="RJ14" pad="21"/>
<connect gate="A" pin="RJ15" pad="22"/>
<connect gate="A" pin="RK0" pad="28"/>
<connect gate="A" pin="RK1" pad="29"/>
<connect gate="A" pin="RP104/RF8" pad="76"/>
<connect gate="A" pin="RP108/RF12" pad="58"/>
<connect gate="A" pin="RP109/RF13" pad="57"/>
<connect gate="A" pin="RP112/RG0" pad="129"/>
<connect gate="A" pin="RP113/RG1" pad="128"/>
<connect gate="A" pin="RP124/RG12" pad="139"/>
<connect gate="A" pin="RP125/RG13" pad="140"/>
<connect gate="A" pin="RP126/RG14" pad="138"/>
<connect gate="A" pin="RP127/RG15" pad="1"/>
<connect gate="A" pin="RP30/RA14" pad="95"/>
<connect gate="A" pin="RP31/RA15" pad="96"/>
<connect gate="A" pin="RP67/RD3" pad="111"/>
<connect gate="A" pin="RP68/RD4" pad="119"/>
<connect gate="A" pin="RP69/RD5" pad="120"/>
<connect gate="A" pin="RP75/RD11" pad="100"/>
<connect gate="A" pin="RP76/RD12" pad="113"/>
<connect gate="A" pin="RP77/RD13" pad="114"/>
<connect gate="A" pin="RP78/RD14" pad="69"/>
<connect gate="A" pin="RP79/RD15" pad="70"/>
<connect gate="A" pin="RP98/RF2" pad="75"/>
<connect gate="A" pin="RTCC/DMLN/RP72/RD8" pad="97"/>
<connect gate="A" pin="SCL2/RP101/RF5" pad="72"/>
<connect gate="A" pin="SDA2/RP100/RF4" pad="71"/>
<connect gate="A" pin="TCK/RP17/RA1" pad="56"/>
<connect gate="A" pin="TDI/RP20/RA4" pad="87"/>
<connect gate="A" pin="TDO/RP21/RA5" pad="88"/>
<connect gate="A" pin="TMS/RP16/RA0" pad="25"/>
<connect gate="A" pin="USBID/RP99/RF3" pad="74"/>
<connect gate="A" pin="VBUS" pad="77"/>
<connect gate="A" pin="VCAP" pad="123"/>
<connect gate="A" pin="VCMPST1/RP96/RF0" pad="126"/>
<connect gate="A" pin="VCMPST2/RP97/RF1" pad="127"/>
<connect gate="A" pin="VCPCON/RP65/RD1" pad="109"/>
<connect gate="A" pin="VDD" pad="89"/>
<connect gate="A" pin="VDD_2" pad="2"/>
<connect gate="A" pin="VDD_3" pad="24"/>
<connect gate="A" pin="VDD_4" pad="52"/>
<connect gate="A" pin="VDD_5" pad="64"/>
<connect gate="A" pin="VDD_6" pad="124"/>
<connect gate="A" pin="VDD_7" pad="112"/>
<connect gate="A" pin="VREF+/RA10" pad="40"/>
<connect gate="A" pin="VREF-/RA9" pad="39"/>
<connect gate="A" pin="VSS" pad="73"/>
<connect gate="A" pin="VSS_2" pad="23"/>
<connect gate="A" pin="VSS_3" pad="36"/>
<connect gate="A" pin="VSS_4" pad="51"/>
<connect gate="A" pin="VSS_5" pad="63"/>
<connect gate="A" pin="VSS_6" pad="141"/>
<connect gate="A" pin="VSS_7" pad="125"/>
<connect gate="A" pin="VSS_8" pad="108"/>
<connect gate="A" pin="VSS_9" pad="92"/>
<connect gate="A" pin="VUSB" pad="78"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP42XXX" prefix="IC" uservalue="yes">
<description>Dual digital potentiometer with SPI interface</description>
<gates>
<gate name="G$1" symbol="MCP42XX"/>
<gate name="G$2" symbol="VDD-VSS"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="B0" pad="10"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="RS" pad="11"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="12"/>
<connect gate="G$1" pin="SI" pad="3"/>
<connect gate="G$1" pin="SO" pad="13"/>
<connect gate="G$1" pin="W0" pad="9"/>
<connect gate="G$1" pin="W1" pad="6"/>
<connect gate="G$2" pin="VDD" pad="14"/>
<connect gate="G$2" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TSSOP14" package="TSSOP14">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="B0" pad="10"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="RS" pad="11"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="12"/>
<connect gate="G$1" pin="SI" pad="3"/>
<connect gate="G$1" pin="SO" pad="13"/>
<connect gate="G$1" pin="W0" pad="9"/>
<connect gate="G$1" pin="W1" pad="6"/>
<connect gate="G$2" pin="VDD" pad="14"/>
<connect gate="G$2" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC14" package="SOIC-14">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="B0" pad="10"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="RS" pad="11"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="12"/>
<connect gate="G$1" pin="SI" pad="3"/>
<connect gate="G$1" pin="SO" pad="13"/>
<connect gate="G$1" pin="W0" pad="9"/>
<connect gate="G$1" pin="W1" pad="6"/>
<connect gate="G$2" pin="VDD" pad="14"/>
<connect gate="G$2" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18C2*2?" prefix="IC">
<description>High-Performance Microcontrollers with 10-Bit A/D</description>
<gates>
<gate name="G$1" symbol="ABC"/>
<gate name="G$2" symbol="VCC1"/>
<gate name="G$3" symbol="GND1"/>
<gate name="G$4" symbol="GND1"/>
</gates>
<devices>
<device name="SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="CCP1/RC2" pad="13"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="MCLR#/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="SCK/RC3" pad="14"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="T1OSI/RC1" pad="12"/>
<connect gate="G$1" pin="T1OSO/RC0" pad="11"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$2" pin="VCC" pad="20"/>
<connect gate="G$3" pin="GND" pad="8"/>
<connect gate="G$4" pin="GND" pad="19"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="5"/>
</technologies>
</device>
<device name="SO" package="SO_28W">
<connects>
<connect gate="G$1" pin="CCP1/RC2" pad="13"/>
<connect gate="G$1" pin="INT/RB0" pad="21"/>
<connect gate="G$1" pin="MCLR#/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="10"/>
<connect gate="G$1" pin="PGC/RB6" pad="27"/>
<connect gate="G$1" pin="PGD/RB7" pad="28"/>
<connect gate="G$1" pin="PGM/RB3" pad="24"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="SCK/RC3" pad="14"/>
<connect gate="G$1" pin="SDI/RC4" pad="15"/>
<connect gate="G$1" pin="SDO/RC5" pad="16"/>
<connect gate="G$1" pin="T1OSI/RC1" pad="12"/>
<connect gate="G$1" pin="T1OSO/RC0" pad="11"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$2" pin="VCC" pad="20"/>
<connect gate="G$3" pin="GND" pad="8"/>
<connect gate="G$4" pin="GND" pad="19"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="5"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18C4*2?" prefix="IC">
<description>High-Performance Microcontrollers with 10-Bit A/D</description>
<gates>
<gate name="G$1" symbol="ABCDE"/>
<gate name="G$2" symbol="GNDVCC"/>
<gate name="G$3" symbol="GNDVCC"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="CCP1/RC2" pad="17"/>
<connect gate="G$1" pin="CS#/AN7/RE2" pad="10"/>
<connect gate="G$1" pin="INT/RB0" pad="33"/>
<connect gate="G$1" pin="MCLR#/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="13"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="14"/>
<connect gate="G$1" pin="PGC/RB6" pad="39"/>
<connect gate="G$1" pin="PGD/RB7" pad="40"/>
<connect gate="G$1" pin="PGM/RB3" pad="36"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RD#/AN5/RE0" pad="8"/>
<connect gate="G$1" pin="RD0/PSP0" pad="19"/>
<connect gate="G$1" pin="RD1/PSP1" pad="20"/>
<connect gate="G$1" pin="RD2/PSP2" pad="21"/>
<connect gate="G$1" pin="RD3/PSP3" pad="22"/>
<connect gate="G$1" pin="RD4/PSP4" pad="27"/>
<connect gate="G$1" pin="RD5/PSP5" pad="28"/>
<connect gate="G$1" pin="RD6/PSP6" pad="29"/>
<connect gate="G$1" pin="RD7/PSP7" pad="30"/>
<connect gate="G$1" pin="RX/RC7" pad="26"/>
<connect gate="G$1" pin="SCK/RC3" pad="18"/>
<connect gate="G$1" pin="SDI/RC4" pad="23"/>
<connect gate="G$1" pin="SDO/RC5" pad="24"/>
<connect gate="G$1" pin="T1OSI/RC1" pad="16"/>
<connect gate="G$1" pin="T1OSO/RC0" pad="15"/>
<connect gate="G$1" pin="TX/RC6" pad="25"/>
<connect gate="G$1" pin="WR#/AN6/RE1" pad="9"/>
<connect gate="G$2" pin="GND" pad="12"/>
<connect gate="G$2" pin="VCC" pad="11"/>
<connect gate="G$3" pin="GND" pad="31"/>
<connect gate="G$3" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="5"/>
</technologies>
</device>
<device name="L" package="PLCC-44">
<connects>
<connect gate="G$1" pin="CCP1/RC2" pad="19"/>
<connect gate="G$1" pin="CS#/AN7/RE2" pad="11"/>
<connect gate="G$1" pin="INT/RB0" pad="36"/>
<connect gate="G$1" pin="MCLR#/VPP" pad="2"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="14"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="15"/>
<connect gate="G$1" pin="PGC/RB6" pad="43"/>
<connect gate="G$1" pin="PGD/RB7" pad="44"/>
<connect gate="G$1" pin="PGM/RB3" pad="39"/>
<connect gate="G$1" pin="RA0/AN0" pad="3"/>
<connect gate="G$1" pin="RA1/AN1" pad="4"/>
<connect gate="G$1" pin="RA2/AN2" pad="5"/>
<connect gate="G$1" pin="RA3/AN3" pad="6"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="7"/>
<connect gate="G$1" pin="RA5/AN4" pad="8"/>
<connect gate="G$1" pin="RB1" pad="37"/>
<connect gate="G$1" pin="RB2" pad="38"/>
<connect gate="G$1" pin="RB4" pad="41"/>
<connect gate="G$1" pin="RB5" pad="42"/>
<connect gate="G$1" pin="RD#/AN5/RE0" pad="9"/>
<connect gate="G$1" pin="RD0/PSP0" pad="21"/>
<connect gate="G$1" pin="RD1/PSP1" pad="22"/>
<connect gate="G$1" pin="RD2/PSP2" pad="23"/>
<connect gate="G$1" pin="RD3/PSP3" pad="24"/>
<connect gate="G$1" pin="RD4/PSP4" pad="30"/>
<connect gate="G$1" pin="RD5/PSP5" pad="31"/>
<connect gate="G$1" pin="RD6/PSP6" pad="32"/>
<connect gate="G$1" pin="RD7/PSP7" pad="33"/>
<connect gate="G$1" pin="RX/RC7" pad="29"/>
<connect gate="G$1" pin="SCK/RC3" pad="20"/>
<connect gate="G$1" pin="SDI/RC4" pad="25"/>
<connect gate="G$1" pin="SDO/RC5" pad="26"/>
<connect gate="G$1" pin="T1OSI/RC1" pad="18"/>
<connect gate="G$1" pin="T1OSO/RC0" pad="16"/>
<connect gate="G$1" pin="TX/RC6" pad="27"/>
<connect gate="G$1" pin="WR#/AN6/RE1" pad="10"/>
<connect gate="G$2" pin="GND" pad="13"/>
<connect gate="G$2" pin="VCC" pad="12"/>
<connect gate="G$3" pin="GND" pad="34"/>
<connect gate="G$3" pin="VCC" pad="35"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="5"/>
</technologies>
</device>
<device name="PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="CCP1/RC2" pad="36"/>
<connect gate="G$1" pin="CS#/AN7/RE2" pad="27"/>
<connect gate="G$1" pin="INT/RB0" pad="8"/>
<connect gate="G$1" pin="MCLR#/VPP" pad="18"/>
<connect gate="G$1" pin="OSC1/CLKIN" pad="30"/>
<connect gate="G$1" pin="OSC2/CLKOUT" pad="31"/>
<connect gate="G$1" pin="PGC/RB6" pad="16"/>
<connect gate="G$1" pin="PGD/RB7" pad="17"/>
<connect gate="G$1" pin="PGM/RB3" pad="11"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RD#/AN5/RE0" pad="25"/>
<connect gate="G$1" pin="RD0/PSP0" pad="38"/>
<connect gate="G$1" pin="RD1/PSP1" pad="39"/>
<connect gate="G$1" pin="RD2/PSP2" pad="40"/>
<connect gate="G$1" pin="RD3/PSP3" pad="41"/>
<connect gate="G$1" pin="RD4/PSP4" pad="2"/>
<connect gate="G$1" pin="RD5/PSP5" pad="3"/>
<connect gate="G$1" pin="RD6/PSP6" pad="4"/>
<connect gate="G$1" pin="RD7/PSP7" pad="5"/>
<connect gate="G$1" pin="RX/RC7" pad="1"/>
<connect gate="G$1" pin="SCK/RC3" pad="37"/>
<connect gate="G$1" pin="SDI/RC4" pad="42"/>
<connect gate="G$1" pin="SDO/RC5" pad="43"/>
<connect gate="G$1" pin="T1OSI/RC1" pad="35"/>
<connect gate="G$1" pin="T1OSO/RC0" pad="32"/>
<connect gate="G$1" pin="TX/RC6" pad="44"/>
<connect gate="G$1" pin="WR#/AN6/RE1" pad="26"/>
<connect gate="G$2" pin="GND" pad="6"/>
<connect gate="G$2" pin="VCC" pad="7"/>
<connect gate="G$3" pin="GND" pad="29"/>
<connect gate="G$3" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="5"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F0*0?" prefix="IC">
<description>High Performance 8pin Microcontrollers</description>
<gates>
<gate name="G$1" symbol="PIC180X0"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="RB0" pad="7"/>
<connect gate="G$1" pin="RB1" pad="6"/>
<connect gate="G$1" pin="RB2" pad="5"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="3"/>
<connect gate="G$1" pin="RB5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="RB0" pad="7"/>
<connect gate="G$1" pin="RB1" pad="6"/>
<connect gate="G$1" pin="RB2" pad="5"/>
<connect gate="G$1" pin="RB3" pad="4"/>
<connect gate="G$1" pin="RB4" pad="3"/>
<connect gate="G$1" pin="RB5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP2200" prefix="IC" uservalue="yes">
<description>USB 2.0 to UART Protocol Converter with GPIO</description>
<gates>
<gate name="G$1" symbol="MCP2200"/>
</gates>
<devices>
<device name="SOIC20" package="SOIC20">
<connects>
<connect gate="G$1" pin="CTS" pad="13"/>
<connect gate="G$1" pin="D+" pad="19"/>
<connect gate="G$1" pin="D-" pad="18"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="GPIO2" pad="14"/>
<connect gate="G$1" pin="GPIO3" pad="9"/>
<connect gate="G$1" pin="GPIO4" pad="8"/>
<connect gate="G$1" pin="GPIO5" pad="7"/>
<connect gate="G$1" pin="OSC1" pad="2"/>
<connect gate="G$1" pin="OSC2" pad="3"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RTS" pad="11"/>
<connect gate="G$1" pin="RX" pad="12"/>
<connect gate="G$1" pin="RXLED" pad="6"/>
<connect gate="G$1" pin="SSPND" pad="16"/>
<connect gate="G$1" pin="TX" pad="10"/>
<connect gate="G$1" pin="TXLED" pad="5"/>
<connect gate="G$1" pin="USBCFG" pad="15"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VUSB" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="CTS" pad="13"/>
<connect gate="G$1" pin="D+" pad="19"/>
<connect gate="G$1" pin="D-" pad="18"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="GPIO2" pad="14"/>
<connect gate="G$1" pin="GPIO3" pad="9"/>
<connect gate="G$1" pin="GPIO4" pad="8"/>
<connect gate="G$1" pin="GPIO5" pad="7"/>
<connect gate="G$1" pin="OSC1" pad="2"/>
<connect gate="G$1" pin="OSC2" pad="3"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RTS" pad="11"/>
<connect gate="G$1" pin="RX" pad="12"/>
<connect gate="G$1" pin="RXLED" pad="6"/>
<connect gate="G$1" pin="SSPND" pad="16"/>
<connect gate="G$1" pin="TX" pad="10"/>
<connect gate="G$1" pin="TXLED" pad="5"/>
<connect gate="G$1" pin="USBCFG" pad="15"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VUSB" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN20" package="QFN20-5X5">
<connects>
<connect gate="G$1" pin="CTS" pad="P$10"/>
<connect gate="G$1" pin="D+" pad="P$16"/>
<connect gate="G$1" pin="D-" pad="P$15"/>
<connect gate="G$1" pin="GND" pad="P$17"/>
<connect gate="G$1" pin="GPIO2" pad="P$11"/>
<connect gate="G$1" pin="GPIO3" pad="P$6"/>
<connect gate="G$1" pin="GPIO4" pad="P$5"/>
<connect gate="G$1" pin="GPIO5" pad="P$4"/>
<connect gate="G$1" pin="OSC1" pad="P$19"/>
<connect gate="G$1" pin="OSC2" pad="P$20"/>
<connect gate="G$1" pin="RST" pad="P$1"/>
<connect gate="G$1" pin="RTS" pad="P$8"/>
<connect gate="G$1" pin="RX" pad="P$9"/>
<connect gate="G$1" pin="RXLED" pad="P$3"/>
<connect gate="G$1" pin="SSPND" pad="P$13"/>
<connect gate="G$1" pin="TX" pad="P$7"/>
<connect gate="G$1" pin="TXLED" pad="P$2"/>
<connect gate="G$1" pin="USBCFG" pad="P$12"/>
<connect gate="G$1" pin="VDD" pad="P$18"/>
<connect gate="G$1" pin="VUSB" pad="P$14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4725" prefix="IC" uservalue="yes">
<description>12-Bit Digital-to-Analog Converter with EEPROM Memory
in SOT-23-6</description>
<gates>
<gate name="G$1" symbol="MCP4725"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MRF49XA" prefix="IC">
<description>Microchip MRF49XA</description>
<gates>
<gate name="G$1" symbol="MRF49XA"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="!INT!/DIO" pad="16"/>
<connect gate="G$1" pin="!IRO" pad="5"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="CLKOUT" pad="8"/>
<connect gate="G$1" pin="FSK/DATA/!FSEL" pad="6"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="MISO" pad="4"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="RCLKOUT/FCAP/FINT" pad="7"/>
<connect gate="G$1" pin="RFN" pad="13"/>
<connect gate="G$1" pin="RFP" pad="12"/>
<connect gate="G$1" pin="RFXTL/EXTREF" pad="9"/>
<connect gate="G$1" pin="RSSIO" pad="15"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MRF89XA" prefix="IC">
<description>Microchip MRF89XA</description>
<gates>
<gate name="G$1" symbol="MRF89XA"/>
</gates>
<devices>
<device name="-QFN" package="QFN33-5X5">
<connects>
<connect gate="G$1" pin="!CSCON" pad="14"/>
<connect gate="G$1" pin="!CSDAT" pad="15"/>
<connect gate="G$1" pin="AVRS" pad="27"/>
<connect gate="G$1" pin="CLKOUT" pad="19"/>
<connect gate="G$1" pin="DATA" pad="20"/>
<connect gate="G$1" pin="DVRS" pad="28"/>
<connect gate="G$1" pin="GND" pad="33"/>
<connect gate="G$1" pin="IRQ0" pad="21"/>
<connect gate="G$1" pin="IRQ1" pad="22"/>
<connect gate="G$1" pin="MISO" pad="16"/>
<connect gate="G$1" pin="MOSI" pad="17"/>
<connect gate="G$1" pin="NC" pad="32"/>
<connect gate="G$1" pin="OSC1" pad="10"/>
<connect gate="G$1" pin="OSC2" pad="11"/>
<connect gate="G$1" pin="PARS" pad="29"/>
<connect gate="G$1" pin="PLLN" pad="6"/>
<connect gate="G$1" pin="PLLP" pad="7"/>
<connect gate="G$1" pin="PLOCK" pad="23"/>
<connect gate="G$1" pin="RFIO" pad="31"/>
<connect gate="G$1" pin="SCK" pad="18"/>
<connect gate="G$1" pin="TEST0" pad="12"/>
<connect gate="G$1" pin="TEST1" pad="2"/>
<connect gate="G$1" pin="TEST2" pad="24"/>
<connect gate="G$1" pin="TEST3" pad="25"/>
<connect gate="G$1" pin="TEST4" pad="30"/>
<connect gate="G$1" pin="TEST5" pad="1"/>
<connect gate="G$1" pin="TEST6" pad="8"/>
<connect gate="G$1" pin="TEST7" pad="9"/>
<connect gate="G$1" pin="TEST8" pad="13"/>
<connect gate="G$1" pin="VCC" pad="26"/>
<connect gate="G$1" pin="VCORS" pad="3"/>
<connect gate="G$1" pin="VCOTN" pad="4"/>
<connect gate="G$1" pin="VCOTP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MRF89XAM8A" prefix="M">
<description>Microchip MRF89XAM8A 868MHz Module</description>
<gates>
<gate name="G$1" symbol="MRF89XAMXA"/>
</gates>
<devices>
<device name="" package="MRF89XAMXA">
<connects>
<connect gate="G$1" pin="!CSCON" pad="3"/>
<connect gate="G$1" pin="!CSDAT" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="GND@3" pad="11"/>
<connect gate="G$1" pin="IRQ0" pad="4"/>
<connect gate="G$1" pin="IRQ1" pad="9"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MRF89XAM9A" prefix="M">
<description>Microchip MRF89XAM9A 915MHz Module</description>
<gates>
<gate name="G$1" symbol="MRF89XAMXA"/>
</gates>
<devices>
<device name="" package="MRF89XAMXA">
<connects>
<connect gate="G$1" pin="!CSCON" pad="3"/>
<connect gate="G$1" pin="!CSDAT" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="GND@3" pad="11"/>
<connect gate="G$1" pin="IRQ0" pad="4"/>
<connect gate="G$1" pin="IRQ1" pad="9"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FVXXKA301" prefix="IC">
<description>PIC24FVXXKA301 2.0-5.5V 20 pin</description>
<gates>
<gate name="G$1" symbol="PIC24FVXXKA301"/>
</gates>
<devices>
<device name="-P" package="DIL20">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/INT2/SCK1/!SS2!/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/SDI2/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN9/SCL2/!SS1!/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="RA0/CN2/SCK2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="VCAP" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO20W">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/INT2/SCK1/!SS2!/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/SDI2/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN9/SCL2/!SS1!/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="RA0/CN2/SCK2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="VCAP" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/INT2/SCK1/!SS2!/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/SDI2/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN9/SCL2/!SS1!/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="RA0/CN2/SCK2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="VCAP" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FVXXKA302" prefix="IC">
<description>PIC24FVXXKA302 2.0-5.5V 28 pin</description>
<gates>
<gate name="G$1" symbol="PIC24FVXXKA302"/>
</gates>
<devices>
<device name="-SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/INT2/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO28W">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/INT2/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/INT2/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FVXXKA304" prefix="IC">
<description>PIC24FVXXKA304</description>
<gates>
<gate name="G$1" symbol="PIC24FVXXKA304"/>
</gates>
<devices>
<device name="-PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="14"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="11"/>
<connect gate="G$1" pin="AN12/INT2/CN14/RB12" pad="10"/>
<connect gate="G$1" pin="AN4/SDA2/CN6/RB2" pad="23"/>
<connect gate="G$1" pin="AN5/SCL2/CN7/RB3" pad="24"/>
<connect gate="G$1" pin="AN6/CN32/RC0" pad="25"/>
<connect gate="G$1" pin="AN7/CN31/RC1" pad="26"/>
<connect gate="G$1" pin="AN8/CN10/RC2" pad="27"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="15"/>
<connect gate="G$1" pin="CN19/RC9" pad="5"/>
<connect gate="G$1" pin="CN20/RC8" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="29"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="INT0/CN23/RB7" pad="43"/>
<connect gate="G$1" pin="PGEC1/AN3/U2RX/CN5/RB1" pad="22"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="9"/>
<connect gate="G$1" pin="PGEC3/ASCL1/CN24/RB6" pad="42"/>
<connect gate="G$1" pin="PGED1/AN2/U2TX/CN4/RB0" pad="21"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="8"/>
<connect gate="G$1" pin="PGED3/ASDA1/CN27/RB5" pad="41"/>
<connect gate="G$1" pin="RA0/CN2/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="20"/>
<connect gate="G$1" pin="RA10/CN35" pad="12"/>
<connect gate="G$1" pin="RA11/CN36" pad="13"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="30"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="31"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="34"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="18"/>
<connect gate="G$1" pin="RA7/CN9" pad="6"/>
<connect gate="G$1" pin="RA8/CN33" pad="32"/>
<connect gate="G$1" pin="RA9/CN34/!SS2!" pad="35"/>
<connect gate="G$1" pin="SCK2/CN26/RC5" pad="38"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="44"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="1"/>
<connect gate="G$1" pin="SDI2/CN28/RC3" pad="36"/>
<connect gate="G$1" pin="SDO2/CN25/RC4" pad="37"/>
<connect gate="G$1" pin="SOSCI/AN15/!U2RTS!/CN1/RB4" pad="33"/>
<connect gate="G$1" pin="U1RX/CN18/RC6" pad="2"/>
<connect gate="G$1" pin="U1TX/CN17/RC7" pad="3"/>
<connect gate="G$1" pin="VCAP" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="17"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VDD@3" pad="40"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKA301" prefix="IC">
<description>PIC24FXXKA301 2.0-3.6V 20 pin</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKA301"/>
</gates>
<devices>
<device name="-P" package="DIL20">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/SCK1/!SS2!/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/SDI2/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN9/SCL2/!SS1!/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="RA0/CN2/SCK2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO20W">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/SCK1/!SS2!/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/SDI2/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN9/SCL2/!SS1!/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="RA0/CN2/SCK2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/SCK1/!SS2!/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/SDI2/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN9/SCL2/!SS1!/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="RA0/CN2/SCK2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKA302" prefix="IC">
<description>PIC24FXXKA302 2.0-3.6V 28 pin</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKA302"/>
</gates>
<devices>
<device name="-SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO28W">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN2/PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="AN3/PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="AN4/SDA2/U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKA304" prefix="IC">
<description>PIC24FXXKA304</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKA304"/>
</gates>
<devices>
<device name="-PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="14"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="11"/>
<connect gate="G$1" pin="AN12/CN14/RB12" pad="10"/>
<connect gate="G$1" pin="AN4/SDA2/CN6/RB2" pad="23"/>
<connect gate="G$1" pin="AN5/SCL2/CN7/RB3" pad="24"/>
<connect gate="G$1" pin="AN6/CN32/RC0" pad="25"/>
<connect gate="G$1" pin="AN7/CN31/RC1" pad="26"/>
<connect gate="G$1" pin="AN8/CN10/RC2" pad="27"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="15"/>
<connect gate="G$1" pin="CN19/RC9" pad="5"/>
<connect gate="G$1" pin="CN20/RC8" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="29"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="INT0/CN23/RB7" pad="43"/>
<connect gate="G$1" pin="PGEC1/AN3/U2RX/CN5/RB1" pad="22"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="9"/>
<connect gate="G$1" pin="PGEC3/ASCL1/CN24/RB6" pad="42"/>
<connect gate="G$1" pin="PGED1/AN2/U2TX/CN4/RB0" pad="21"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="8"/>
<connect gate="G$1" pin="PGED3/ASDA1/CN27/RB5" pad="41"/>
<connect gate="G$1" pin="RA0/CN2/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="20"/>
<connect gate="G$1" pin="RA10/CN35" pad="12"/>
<connect gate="G$1" pin="RA11/CN36" pad="13"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="30"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="31"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="34"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="18"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="7"/>
<connect gate="G$1" pin="RA7/CN9" pad="6"/>
<connect gate="G$1" pin="RA8/CN33" pad="32"/>
<connect gate="G$1" pin="RA9/CN34/!SS2!" pad="35"/>
<connect gate="G$1" pin="SCK2/CN26/RC5" pad="38"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="44"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="1"/>
<connect gate="G$1" pin="SDI2/CN28/RC3" pad="36"/>
<connect gate="G$1" pin="SDO2/CN25/RC4" pad="37"/>
<connect gate="G$1" pin="SOSCI/AN15/!U2RTS!/CN1/RB4" pad="33"/>
<connect gate="G$1" pin="U1RX/CN18/RC6" pad="2"/>
<connect gate="G$1" pin="U1TX/CN17/RC7" pad="3"/>
<connect gate="G$1" pin="VDD@1" pad="17"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VDD@3" pad="40"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKL100" prefix="IC">
<description>PIC24FXXKL100</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKL100"/>
</gates>
<devices>
<device name="-P" package="DIL14">
<connects>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="INT0/!SS1!/U1RX/CN11/RB15" pad="12"/>
<connect gate="G$1" pin="INT1/SDI1/U1TX/CN12/RB14" pad="11"/>
<connect gate="G$1" pin="PGED3/SOSCI/CN1/RB4" pad="6"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="4"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="5"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="7"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="10"/>
<connect gate="G$1" pin="SCL1/SCK1/!U1CTS!/CN22/RB8" pad="8"/>
<connect gate="G$1" pin="SDA1/SDO1/!U1RTS!/CN21/RB9" pad="9"/>
<connect gate="G$1" pin="VDD" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ST" package="TSSOP14">
<connects>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="INT0/!SS1!/U1RX/CN11/RB15" pad="12"/>
<connect gate="G$1" pin="INT1/SDI1/U1TX/CN12/RB14" pad="11"/>
<connect gate="G$1" pin="PGED3/SOSCI/CN1/RB4" pad="6"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="4"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="5"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="7"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="10"/>
<connect gate="G$1" pin="SCL1/SCK1/!U1CTS!/CN22/RB8" pad="8"/>
<connect gate="G$1" pin="SDA1/SDO1/!U1RTS!/CN21/RB9" pad="9"/>
<connect gate="G$1" pin="VDD" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKL101" prefix="IC">
<description>PIC24FXXKL101</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKL101"/>
</gates>
<devices>
<device name="-P" package="DIL20">
<connects>
<connect gate="G$1" pin="CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="PGEC1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED3/SOSCI/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO20W">
<connects>
<connect gate="G$1" pin="CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="PGEC1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED3/SOSCI/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="PGEC1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED3/SOSCI/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKL200" prefix="IC">
<description>PIC24FXXKL200</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKL200"/>
</gates>
<devices>
<device name="-P" package="DIL14">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/U1TX/CN12/RB14" pad="11"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/CN1/RB4" pad="6"/>
<connect gate="G$1" pin="AN9/INT0/!SS1!/U1RX/CN11/RB15" pad="12"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="4"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="5"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="7"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="10"/>
<connect gate="G$1" pin="SCL1/SCK1/!U1CTS!/CN22/RB8" pad="8"/>
<connect gate="G$1" pin="SDA1/SDO1/!U1RTS!/CN21/RB9" pad="9"/>
<connect gate="G$1" pin="VDD" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ST" package="TSSOP14">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/U1TX/CN12/RB14" pad="11"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/CN1/RB4" pad="6"/>
<connect gate="G$1" pin="AN9/INT0/!SS1!/U1RX/CN11/RB15" pad="12"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="4"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="5"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="7"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="10"/>
<connect gate="G$1" pin="SCL1/SCK1/!U1CTS!/CN22/RB8" pad="8"/>
<connect gate="G$1" pin="SDA1/SDO1/!U1RTS!/CN21/RB9" pad="9"/>
<connect gate="G$1" pin="VDD" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKL201" prefix="IC">
<description>PIC24FXXKL201</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKL201"/>
</gates>
<devices>
<device name="-P" package="DIL20">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN9/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="PGEC1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO20W">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN9/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="PGEC1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN9/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="PGEC1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="RA0/CN2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKL301" prefix="IC">
<description>PIC24FXXKL301</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKL301"/>
</gates>
<devices>
<device name="-P" package="DIL20">
<connects>
<connect gate="G$1" pin="!SS2!/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/SDI2/PGEC2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SCL2/SCK2/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO20W">
<connects>
<connect gate="G$1" pin="!SS2!/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/SDI2/PGEC2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SCL2/SCK2/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="!SS2!/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/SDI2/PGEC2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SCL2/SCK2/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKL302" prefix="IC">
<description>PIC24FXXKL302</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKL302"/>
</gates>
<devices>
<device name="-SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/SDA2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/SDA2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/SDA2" pad="2"/>
<connect gate="G$1" pin="RA1/CN3" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKL401" prefix="IC">
<description>PIC24FXXKL401</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKL401"/>
</gates>
<devices>
<device name="-P" package="DIL20">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/!SS2!/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN9/SCL2/SCK2/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/SDI2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO20W">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/!SS2!/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN9/SCL2/SCK2/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/SDI2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP20">
<connects>
<connect gate="G$1" pin="AN10/INT1/SDI1/CN12/RB14" pad="17"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="16"/>
<connect gate="G$1" pin="AN12/!SS2!/SCK1/CN14/RB12" pad="15"/>
<connect gate="G$1" pin="AN15/PGED3/SOSCI/!U2RTS!/CN1/RB4" pad="9"/>
<connect gate="G$1" pin="AN9/SCL2/SCK2/CN11/RB15" pad="18"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="11"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/SDI2/PGEC2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/SDO2/PGED2/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="7"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="8"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO/PGEC3" pad="10"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="14"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/!SS1!/CN22/RB8" pad="12"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="13"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXKL402" prefix="IC">
<description>PIC24FXXKL402</description>
<gates>
<gate name="G$1" symbol="PIC24FXXKL402"/>
</gates>
<devices>
<device name="-SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO28W">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="AN10/INT1/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/SDO1/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/!SS2!/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN15/SOSCI/!U2RTS!/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="AN9/!SS1!/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="27"/>
<connect gate="G$1" pin="INT0/U1TX/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="PGEC1/U2RX/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/SCK1/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/SDO2/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/U2TX/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/SDI1/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/SCK2/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="RA0/CN2/SDA2/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/CN3/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/AN13" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/AN14" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/!U2CTS!/SOSCO" pad="12"/>
<connect gate="G$1" pin="RA5/!MCLR" pad="1"/>
<connect gate="G$1" pin="RA6/CN8/INT2" pad="20"/>
<connect gate="G$1" pin="RA7/CN9/SDI2" pad="19"/>
<connect gate="G$1" pin="SCL1/!U1CTS!/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="SCL2/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="SDA1/!U1RTS!/CN21/RB9" pad="18"/>
<connect gate="G$1" pin="U1RX/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC7129" prefix="IC" uservalue="yes">
<description>The TC7129 is a 4-1/2 digit Analog-to-Digital Converter
(ADC) that directly drives a multiplexed Liquid Crystal
Display (LCD). Fabricated in high-performance, lowpower
CMOS, the TC7129 ADC is designed specifically
for high-resolution, battery-powered digital multimeter
applications. The traditional dual-slope method
of A/D conversion has been enhanced with a successive
integration technique to produce readings accurate
to better than 0.005% of full-scale and resolution
down to 10 μV per count.
The TC7129 includes features important to multimeter
applications. It detects and indicates low battery condition.
A continuity output drives an annunciator on the
display and can be used with an external driver to sound
an audible alarm. Overrange and underrange outputs,
along with a range-change input, provide the ability to
create auto-ranging instruments. For snapshot readings,
the TC7129 includes a latch-and-hold input to
freeze the present reading. This combination of features
makes the TC7129 the ideal choice for full-featured
multimeter and digital measurement applications.</description>
<gates>
<gate name="G$1" symbol="TC7129"/>
</gates>
<devices>
<device name="TC7129CPL" package="DIL40">
<connects>
<connect gate="G$1" pin="A1G1D1" pad="5"/>
<connect gate="G$1" pin="A2G2D2" pad="8"/>
<connect gate="G$1" pin="A3G3D3" pad="11"/>
<connect gate="G$1" pin="A4D4G4" pad="14"/>
<connect gate="G$1" pin="ANNUN" pad="3"/>
<connect gate="G$1" pin="B1C1CONT" pad="4"/>
<connect gate="G$1" pin="B2C2BAT" pad="7"/>
<connect gate="G$1" pin="B3C3MINUS" pad="10"/>
<connect gate="G$1" pin="B4C4BC5" pad="13"/>
<connect gate="G$1" pin="BP1" pad="18"/>
<connect gate="G$1" pin="BP2" pad="17"/>
<connect gate="G$1" pin="BP3" pad="16"/>
<connect gate="G$1" pin="BUFFER" pad="31"/>
<connect gate="G$1" pin="COMMON" pad="28"/>
<connect gate="G$1" pin="CONTINU" pad="27"/>
<connect gate="G$1" pin="CREF+" pad="29"/>
<connect gate="G$1" pin="CREF-" pad="30"/>
<connect gate="G$1" pin="DGND" pad="36"/>
<connect gate="G$1" pin="DP1" pad="39"/>
<connect gate="G$1" pin="DP2" pad="38"/>
<connect gate="G$1" pin="DP3/UR" pad="21"/>
<connect gate="G$1" pin="DP4/OR" pad="20"/>
<connect gate="G$1" pin="F1E1DP1" pad="6"/>
<connect gate="G$1" pin="F2E2DP2" pad="9"/>
<connect gate="G$1" pin="F3E3DP3" pad="12"/>
<connect gate="G$1" pin="F4E4DP4" pad="15"/>
<connect gate="G$1" pin="INHI" pad="33"/>
<connect gate="G$1" pin="INLO" pad="32"/>
<connect gate="G$1" pin="INTIN" pad="25"/>
<connect gate="G$1" pin="INTOUT" pad="26"/>
<connect gate="G$1" pin="LAT/HOLD" pad="22"/>
<connect gate="G$1" pin="OSC1" pad="1"/>
<connect gate="G$1" pin="OSC2" pad="2"/>
<connect gate="G$1" pin="OSC3" pad="40"/>
<connect gate="G$1" pin="RANGE" pad="37"/>
<connect gate="G$1" pin="REFHI" pad="34"/>
<connect gate="G$1" pin="REFLO" pad="35"/>
<connect gate="G$1" pin="V+" pad="24"/>
<connect gate="G$1" pin="V-" pad="23"/>
<connect gate="G$1" pin="VDISP" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC7129CLW" package="PLCC-44">
<connects>
<connect gate="G$1" pin="A1G1D1" pad="6"/>
<connect gate="G$1" pin="A2G2D2" pad="9"/>
<connect gate="G$1" pin="A3G3D3" pad="13"/>
<connect gate="G$1" pin="A4D4G4" pad="16"/>
<connect gate="G$1" pin="ANNUN" pad="4"/>
<connect gate="G$1" pin="B1C1CONT" pad="5"/>
<connect gate="G$1" pin="B2C2BAT" pad="8"/>
<connect gate="G$1" pin="B3C3MINUS" pad="11"/>
<connect gate="G$1" pin="B4C4BC5" pad="15"/>
<connect gate="G$1" pin="BP1" pad="20"/>
<connect gate="G$1" pin="BP2" pad="19"/>
<connect gate="G$1" pin="BP3" pad="18"/>
<connect gate="G$1" pin="BUFFER" pad="35"/>
<connect gate="G$1" pin="COMMON" pad="31"/>
<connect gate="G$1" pin="CONTINU" pad="30"/>
<connect gate="G$1" pin="CREF+" pad="32"/>
<connect gate="G$1" pin="CREF-" pad="33"/>
<connect gate="G$1" pin="DGND" pad="40"/>
<connect gate="G$1" pin="DP1" pad="43"/>
<connect gate="G$1" pin="DP2" pad="42"/>
<connect gate="G$1" pin="DP3/UR" pad="24"/>
<connect gate="G$1" pin="DP4/OR" pad="22"/>
<connect gate="G$1" pin="F1E1DP1" pad="7"/>
<connect gate="G$1" pin="F2E2DP2" pad="10"/>
<connect gate="G$1" pin="F3E3DP3" pad="14"/>
<connect gate="G$1" pin="F4E4DP4" pad="17"/>
<connect gate="G$1" pin="INHI" pad="37"/>
<connect gate="G$1" pin="INLO" pad="36"/>
<connect gate="G$1" pin="INTIN" pad="28"/>
<connect gate="G$1" pin="INTOUT" pad="29"/>
<connect gate="G$1" pin="LAT/HOLD" pad="25"/>
<connect gate="G$1" pin="OSC1" pad="2"/>
<connect gate="G$1" pin="OSC2" pad="44"/>
<connect gate="G$1" pin="OSC3" pad="3"/>
<connect gate="G$1" pin="RANGE" pad="41"/>
<connect gate="G$1" pin="REFHI" pad="38"/>
<connect gate="G$1" pin="REFLO" pad="39"/>
<connect gate="G$1" pin="V+" pad="27"/>
<connect gate="G$1" pin="V-" pad="26"/>
<connect gate="G$1" pin="VDISP" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC7129CKW" package="PQFP44">
<connects>
<connect gate="G$1" pin="A1G1D1" pad="44"/>
<connect gate="G$1" pin="A2G2D2" pad="3"/>
<connect gate="G$1" pin="A3G3D3" pad="7"/>
<connect gate="G$1" pin="A4D4G4" pad="10"/>
<connect gate="G$1" pin="ANNUN" pad="42"/>
<connect gate="G$1" pin="B1C1CONT" pad="43"/>
<connect gate="G$1" pin="B2C2BAT" pad="2"/>
<connect gate="G$1" pin="B3C3MINUS" pad="5"/>
<connect gate="G$1" pin="B4C4BC5" pad="9"/>
<connect gate="G$1" pin="BP1" pad="14"/>
<connect gate="G$1" pin="BP2" pad="13"/>
<connect gate="G$1" pin="BP3" pad="12"/>
<connect gate="G$1" pin="BUFFER" pad="29"/>
<connect gate="G$1" pin="COMMON" pad="25"/>
<connect gate="G$1" pin="CONTINU" pad="24"/>
<connect gate="G$1" pin="CREF+" pad="26"/>
<connect gate="G$1" pin="CREF-" pad="27"/>
<connect gate="G$1" pin="DGND" pad="34"/>
<connect gate="G$1" pin="DP1" pad="37"/>
<connect gate="G$1" pin="DP2" pad="36"/>
<connect gate="G$1" pin="DP3/UR" pad="18"/>
<connect gate="G$1" pin="DP4/OR" pad="16"/>
<connect gate="G$1" pin="F1E1DP1" pad="1"/>
<connect gate="G$1" pin="F2E2DP2" pad="4"/>
<connect gate="G$1" pin="F3E3DP3" pad="8"/>
<connect gate="G$1" pin="F4E4DP4" pad="11"/>
<connect gate="G$1" pin="INHI" pad="31"/>
<connect gate="G$1" pin="INLO" pad="30"/>
<connect gate="G$1" pin="INTIN" pad="22"/>
<connect gate="G$1" pin="INTOUT" pad="23"/>
<connect gate="G$1" pin="LAT/HOLD" pad="19"/>
<connect gate="G$1" pin="OSC1" pad="40"/>
<connect gate="G$1" pin="OSC2" pad="38"/>
<connect gate="G$1" pin="OSC3" pad="41"/>
<connect gate="G$1" pin="RANGE" pad="35"/>
<connect gate="G$1" pin="REFHI" pad="32"/>
<connect gate="G$1" pin="REFLO" pad="33"/>
<connect gate="G$1" pin="V+" pad="21"/>
<connect gate="G$1" pin="V-" pad="20"/>
<connect gate="G$1" pin="VDISP" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC7660" prefix="IC" uservalue="yes">
<description>The TC7660 is a pin-compatible replacement for the
industry standard 7660 charge pump voltage
converter. It converts a +1.5V to +10V input to a
corresponding -1.5V to -10V output using only two low
cost capacitors, eliminating inductors and their
associated cost, size and electromagnetic interference
(EMI).
The on-board oscillator operates at a nominal
frequency of 10 kHz. Operation below 10 kHz (for
lower supply current applications) is possible by
connecting an external capacitor from OSC to ground.
The TC7660 is available in 8-Pin PDIP, 8-Pin Small
Outline (SOIC) and 8-Pin CERDIP packages in
commercial and extended temperature ranges.</description>
<gates>
<gate name="G$1" symbol="TC7660"/>
</gates>
<devices>
<device name="" package="DIL8">
<connects>
<connect gate="G$1" pin="1/NC" pad="1"/>
<connect gate="G$1" pin="2/CAP+" pad="2"/>
<connect gate="G$1" pin="3/GND" pad="3"/>
<connect gate="G$1" pin="4/CAP-" pad="4"/>
<connect gate="G$1" pin="5/VOUT" pad="5"/>
<connect gate="G$1" pin="6/LO_V" pad="6"/>
<connect gate="G$1" pin="7/OSC" pad="7"/>
<connect gate="G$1" pin="8/V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC8" package="SOIC8">
<connects>
<connect gate="G$1" pin="1/NC" pad="1"/>
<connect gate="G$1" pin="2/CAP+" pad="2"/>
<connect gate="G$1" pin="3/GND" pad="3"/>
<connect gate="G$1" pin="4/CAP-" pad="4"/>
<connect gate="G$1" pin="5/VOUT" pad="5"/>
<connect gate="G$1" pin="6/LO_V" pad="6"/>
<connect gate="G$1" pin="7/OSC" pad="7"/>
<connect gate="G$1" pin="8/V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC7126" prefix="IC" uservalue="yes">
<description>The TC7126A is a 3-1/2 digit CMOS analog-to-digital
converter (ADC) containing all the active components
necessary to construct a 0.05% resolution measurement
system. Seven-segment decoders, digit and
polarity drivers, voltage reference, and clock circuit are
integrated on-chip. The TC7126A directly drives a liquid
crystal display (LCD), and includes a backplane
driver.
A low cost, high resolution indicating meter requires
only a display, four resistors, and four capacitors. The
TC7126A's extremely low power drain and 9V battery
operation make it ideal for portable applications.
The TC7126A reduces linearity error to less than 1
count. Rollover error (the difference in readings for
equal magnitude, but opposite polarity input signals) is
below ±1 count. High-impedance differential inputs
offer 1pA leakage current and a 1012Ω input impedance.
The 15μVP-P noise performance ensures a "rock
solid" reading, and the auto-zero cycle ensures a zero
display reading with a 0V input.
The TC7126A features a precision, low drift internal
voltage reference and is functionally identical to the
TC7126. A low drift external reference is not normally
required with the TC7126A.</description>
<gates>
<gate name="G$1" symbol="TC7126"/>
</gates>
<devices>
<device name="TC7126CPL/ACPL/IPL/AIPL" package="DIL40">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="A3" pad="23"/>
<connect gate="G$1" pin="AB4" pad="19"/>
<connect gate="G$1" pin="ANA_COMM" pad="32"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="BP" pad="21"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3" pad="24"/>
<connect gate="G$1" pin="CAZ" pad="29"/>
<connect gate="G$1" pin="CREF+" pad="34"/>
<connect gate="G$1" pin="CREF-" pad="33"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="14"/>
<connect gate="G$1" pin="E3" pad="18"/>
<connect gate="G$1" pin="F1" pad="6"/>
<connect gate="G$1" pin="F2" pad="13"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="25"/>
<connect gate="G$1" pin="G3" pad="22"/>
<connect gate="G$1" pin="OSC1" pad="40"/>
<connect gate="G$1" pin="OSC2" pad="39"/>
<connect gate="G$1" pin="OSC3" pad="38"/>
<connect gate="G$1" pin="POL(-SIG)" pad="20"/>
<connect gate="G$1" pin="TEST" pad="37"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="26"/>
<connect gate="G$1" pin="VBUFF" pad="28"/>
<connect gate="G$1" pin="VIN+" pad="31"/>
<connect gate="G$1" pin="VIN-" pad="30"/>
<connect gate="G$1" pin="VINT" pad="27"/>
<connect gate="G$1" pin="VREF+" pad="36"/>
<connect gate="G$1" pin="VREF-" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC7126RCPL/ARCPL/RIPL/ARIPL" package="DIL40">
<connects>
<connect gate="G$1" pin="A1" pad="36"/>
<connect gate="G$1" pin="A2" pad="29"/>
<connect gate="G$1" pin="A3" pad="18"/>
<connect gate="G$1" pin="AB4" pad="22"/>
<connect gate="G$1" pin="ANA_COMM" pad="9"/>
<connect gate="G$1" pin="B1" pad="37"/>
<connect gate="G$1" pin="B2" pad="30"/>
<connect gate="G$1" pin="B3" pad="25"/>
<connect gate="G$1" pin="BP" pad="20"/>
<connect gate="G$1" pin="C1" pad="38"/>
<connect gate="G$1" pin="C2" pad="31"/>
<connect gate="G$1" pin="C3" pad="17"/>
<connect gate="G$1" pin="CAZ" pad="12"/>
<connect gate="G$1" pin="CREF+" pad="7"/>
<connect gate="G$1" pin="CREF-" pad="8"/>
<connect gate="G$1" pin="D1" pad="39"/>
<connect gate="G$1" pin="D2" pad="32"/>
<connect gate="G$1" pin="D3" pad="26"/>
<connect gate="G$1" pin="E1" pad="33"/>
<connect gate="G$1" pin="E2" pad="27"/>
<connect gate="G$1" pin="E3" pad="23"/>
<connect gate="G$1" pin="F1" pad="35"/>
<connect gate="G$1" pin="F2" pad="28"/>
<connect gate="G$1" pin="F3" pad="24"/>
<connect gate="G$1" pin="G1" pad="34"/>
<connect gate="G$1" pin="G2" pad="16"/>
<connect gate="G$1" pin="G3" pad="19"/>
<connect gate="G$1" pin="OSC1" pad="1"/>
<connect gate="G$1" pin="OSC2" pad="2"/>
<connect gate="G$1" pin="OSC3" pad="3"/>
<connect gate="G$1" pin="POL(-SIG)" pad="21"/>
<connect gate="G$1" pin="TEST" pad="4"/>
<connect gate="G$1" pin="V+" pad="40"/>
<connect gate="G$1" pin="V-" pad="15"/>
<connect gate="G$1" pin="VBUFF" pad="13"/>
<connect gate="G$1" pin="VIN+" pad="10"/>
<connect gate="G$1" pin="VIN-" pad="11"/>
<connect gate="G$1" pin="VINT" pad="14"/>
<connect gate="G$1" pin="VREF+" pad="5"/>
<connect gate="G$1" pin="VREF-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC7126CLW/ACLW" package="PLCC-44">
<connects>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="14"/>
<connect gate="G$1" pin="A3" pad="26"/>
<connect gate="G$1" pin="AB4" pad="21"/>
<connect gate="G$1" pin="ANA_COMM" pad="36"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="13"/>
<connect gate="G$1" pin="B3" pad="18"/>
<connect gate="G$1" pin="BP" pad="24"/>
<connect gate="G$1" pin="C1" pad="4"/>
<connect gate="G$1" pin="C2" pad="11"/>
<connect gate="G$1" pin="C3" pad="27"/>
<connect gate="G$1" pin="CAZ" pad="32"/>
<connect gate="G$1" pin="CREF+" pad="38"/>
<connect gate="G$1" pin="CREF-" pad="37"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="10"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="E1" pad="9"/>
<connect gate="G$1" pin="E2" pad="16"/>
<connect gate="G$1" pin="E3" pad="20"/>
<connect gate="G$1" pin="F1" pad="7"/>
<connect gate="G$1" pin="F2" pad="15"/>
<connect gate="G$1" pin="F3" pad="19"/>
<connect gate="G$1" pin="G1" pad="8"/>
<connect gate="G$1" pin="G2" pad="28"/>
<connect gate="G$1" pin="G3" pad="25"/>
<connect gate="G$1" pin="OSC1" pad="44"/>
<connect gate="G$1" pin="OSC2" pad="43"/>
<connect gate="G$1" pin="OSC3" pad="42"/>
<connect gate="G$1" pin="POL(-SIG)" pad="22"/>
<connect gate="G$1" pin="TEST" pad="41"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="29"/>
<connect gate="G$1" pin="VBUFF" pad="31"/>
<connect gate="G$1" pin="VIN+" pad="35"/>
<connect gate="G$1" pin="VIN-" pad="33"/>
<connect gate="G$1" pin="VINT" pad="30"/>
<connect gate="G$1" pin="VREF+" pad="40"/>
<connect gate="G$1" pin="VREF-" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC7126CKW/ACKW" package="PQFP44">
<connects>
<connect gate="G$1" pin="A1" pad="12"/>
<connect gate="G$1" pin="A2" pad="19"/>
<connect gate="G$1" pin="A3" pad="30"/>
<connect gate="G$1" pin="AB4" pad="26"/>
<connect gate="G$1" pin="ANA_COMM" pad="40"/>
<connect gate="G$1" pin="B1" pad="11"/>
<connect gate="G$1" pin="B2" pad="18"/>
<connect gate="G$1" pin="B3" pad="23"/>
<connect gate="G$1" pin="BP" pad="28"/>
<connect gate="G$1" pin="C1" pad="10"/>
<connect gate="G$1" pin="C2" pad="17"/>
<connect gate="G$1" pin="C3" pad="31"/>
<connect gate="G$1" pin="CAZ" pad="37"/>
<connect gate="G$1" pin="CREF+" pad="42"/>
<connect gate="G$1" pin="CREF-" pad="41"/>
<connect gate="G$1" pin="D1" pad="9"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="E1" pad="15"/>
<connect gate="G$1" pin="E2" pad="21"/>
<connect gate="G$1" pin="E3" pad="25"/>
<connect gate="G$1" pin="F1" pad="13"/>
<connect gate="G$1" pin="F2" pad="20"/>
<connect gate="G$1" pin="F3" pad="24"/>
<connect gate="G$1" pin="G1" pad="14"/>
<connect gate="G$1" pin="G2" pad="32"/>
<connect gate="G$1" pin="G3" pad="29"/>
<connect gate="G$1" pin="OSC1" pad="7"/>
<connect gate="G$1" pin="OSC2" pad="6"/>
<connect gate="G$1" pin="OSC3" pad="4"/>
<connect gate="G$1" pin="POL(-SIG)" pad="27"/>
<connect gate="G$1" pin="TEST" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="34"/>
<connect gate="G$1" pin="VBUFF" pad="36"/>
<connect gate="G$1" pin="VIN+" pad="39"/>
<connect gate="G$1" pin="VIN-" pad="38"/>
<connect gate="G$1" pin="VINT" pad="35"/>
<connect gate="G$1" pin="VREF+" pad="44"/>
<connect gate="G$1" pin="VREF-" pad="43"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP3304">
<description>The Microchip Technology Inc. MCP3304 13-bit A/D
converters feature full differential inputs and low-power
consumption in a small package that is ideal for battery
powered systems and remote data acquisition
applications. The MCP3302 is programmable to
provide two differential input pairs or four single ended
inputs. The MCP3304 is programmable and provides
four differential input pairs or eight single ended inputs.</description>
<gates>
<gate name="G$1" symbol="MCP3304"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="AGND" pad="14"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="CS_SH" pad="10"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DIN" pad="11"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOIC16">
<connects>
<connect gate="G$1" pin="AGND" pad="14"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="CS_SH" pad="10"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DIN" pad="11"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP3302" prefix="IC" uservalue="yes">
<description>The Microchip Technology Inc. MCP3302 13-bit A/D
converters feature full differential inputs and low-power
consumption in a small package that is ideal for battery
powered systems and remote data acquisition
applications. The MCP3302 is programmable to
provide two differential input pairs or four single ended
inputs. The MCP3304 is programmable and provides
four differential input pairs or eight single ended inputs.</description>
<gates>
<gate name="G$1" symbol="MCP3302"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CLK" pad="11"/>
<connect gate="G$1" pin="CS/SH" pad="8"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="10"/>
<connect gate="G$1" pin="NC5" pad="5"/>
<connect gate="G$1" pin="NC6" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOIC-14">
<connects>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CLK" pad="11"/>
<connect gate="G$1" pin="CS/SH" pad="8"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="10"/>
<connect gate="G$1" pin="NC5" pad="5"/>
<connect gate="G$1" pin="NC6" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MCP3302/B" package="TSSOP14">
<connects>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CLK" pad="11"/>
<connect gate="G$1" pin="CS/SH" pad="8"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="10"/>
<connect gate="G$1" pin="NC5" pad="5"/>
<connect gate="G$1" pin="NC6" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F914/917-IP/T" prefix="IC" uservalue="yes">
<description>40/44-Pin Flash-Based, 8-Bit
CMOS Microcontrollers with
nanoWatt Technology</description>
<gates>
<gate name="G$1" symbol="PIC16F914"/>
</gates>
<devices>
<device name="PIC16F914-I/P" package="DIL40">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1-/SEG12" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/C2-/SEG7" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/C2+/VREF-/COM2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/C1+/VREF+/SEG15" pad="5"/>
<connect gate="G$1" pin="RA4/C1OUT/T0CKI/SEG4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/SS#/SEG5" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO/T1OSO" pad="14"/>
<connect gate="G$1" pin="RA7/OSC1/CLKI/T1OSI" pad="13"/>
<connect gate="G$1" pin="RB0/INT/SEG0" pad="33"/>
<connect gate="G$1" pin="RB1/SEG1" pad="34"/>
<connect gate="G$1" pin="RB2/SEG2" pad="35"/>
<connect gate="G$1" pin="RB3/SEG3" pad="36"/>
<connect gate="G$1" pin="RB4/COM0" pad="37"/>
<connect gate="G$1" pin="RB5/COM1" pad="38"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCK/SEG14" pad="39"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="40"/>
<connect gate="G$1" pin="RC0/VLCD1" pad="15"/>
<connect gate="G$1" pin="RC1/VLCD2" pad="16"/>
<connect gate="G$1" pin="RC2/VLCD3" pad="17"/>
<connect gate="G$1" pin="RC3/SEG6" pad="18"/>
<connect gate="G$1" pin="RC4/T1G#/SDO/SEG11" pad="23"/>
<connect gate="G$1" pin="RC5/T1CKI/CCP1/SEG10" pad="24"/>
<connect gate="G$1" pin="RC6/TX/CK/SCK/SCL/SEG9" pad="25"/>
<connect gate="G$1" pin="RC7/RX/DT/SDI/SDA/SEG8" pad="26"/>
<connect gate="G$1" pin="RD0/COM3" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2/CCP2" pad="21"/>
<connect gate="G$1" pin="RD3/SEG16" pad="22"/>
<connect gate="G$1" pin="RD4/SEG17" pad="27"/>
<connect gate="G$1" pin="RD5/SEG18" pad="28"/>
<connect gate="G$1" pin="RD6/SEG19" pad="29"/>
<connect gate="G$1" pin="RD7/SEG20" pad="30"/>
<connect gate="G$1" pin="RE0/AN5/SEG21" pad="8"/>
<connect gate="G$1" pin="RE1/AN6/SEG22" pad="9"/>
<connect gate="G$1" pin="RE2/AN7/SEG23" pad="10"/>
<connect gate="G$1" pin="RE3/MCRL#/VPP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PIC16F914-I/PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1-/SEG12" pad="19"/>
<connect gate="G$1" pin="RA1/AN1/C2-/SEG7" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/C2+/VREF-/COM2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3/C1+/VREF+/SEG15" pad="22"/>
<connect gate="G$1" pin="RA4/C1OUT/T0CKI/SEG4" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/SS#/SEG5" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO/T1OSO" pad="31"/>
<connect gate="G$1" pin="RA7/OSC1/CLKI/T1OSI" pad="30"/>
<connect gate="G$1" pin="RB0/INT/SEG0" pad="8"/>
<connect gate="G$1" pin="RB1/SEG1" pad="9"/>
<connect gate="G$1" pin="RB2/SEG2" pad="10"/>
<connect gate="G$1" pin="RB3/SEG3" pad="11"/>
<connect gate="G$1" pin="RB4/COM0" pad="14"/>
<connect gate="G$1" pin="RB5/COM1" pad="15"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCK/SEG14" pad="16"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="17"/>
<connect gate="G$1" pin="RC0/VLCD1" pad="32"/>
<connect gate="G$1" pin="RC1/VLCD2" pad="35"/>
<connect gate="G$1" pin="RC2/VLCD3" pad="36"/>
<connect gate="G$1" pin="RC3/SEG6" pad="37"/>
<connect gate="G$1" pin="RC4/T1G#/SDO/SEG11" pad="42"/>
<connect gate="G$1" pin="RC5/T1CKI/CCP1/SEG10" pad="43"/>
<connect gate="G$1" pin="RC6/TX/CK/SCK/SCL/SEG9" pad="44"/>
<connect gate="G$1" pin="RC7/RX/DT/SDI/SDA/SEG8" pad="1"/>
<connect gate="G$1" pin="RD0/COM3" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2/CCP2" pad="40"/>
<connect gate="G$1" pin="RD3/SEG16" pad="41"/>
<connect gate="G$1" pin="RD4/SEG17" pad="2"/>
<connect gate="G$1" pin="RD5/SEG18" pad="3"/>
<connect gate="G$1" pin="RD6/SEG19" pad="4"/>
<connect gate="G$1" pin="RD7/SEG20" pad="5"/>
<connect gate="G$1" pin="RE0/AN5/SEG21" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/SEG22" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/SEG23" pad="27"/>
<connect gate="G$1" pin="RE3/MCRL#/VPP" pad="18"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS1" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F914/917-I/ML" prefix="IC" uservalue="yes">
<description>44-Pin Flash-Based, 8-Bit
CMOS Microcontrollers with
nanoWatt Technology</description>
<gates>
<gate name="G$1" symbol="PIC16F914/917-I/ML"/>
</gates>
<devices>
<device name="914/917-I/ML" package="QFN44ML8X8">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1-/SEG12" pad="19"/>
<connect gate="G$1" pin="RA1/AN1/C2-/SEG7" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/C2+/VREF-/COM2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3/C1+/VREF+/SEG15" pad="22"/>
<connect gate="G$1" pin="RA4/C1OUT/T0CKI/SEG4" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/SS#/SEG5" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO/T1OSO" pad="33"/>
<connect gate="G$1" pin="RA7/OSC1/CLKI/T1OSI" pad="32"/>
<connect gate="G$1" pin="RB0/INT/SEG0" pad="9"/>
<connect gate="G$1" pin="RB1/SEG1" pad="10"/>
<connect gate="G$1" pin="RB2/SEG2" pad="11"/>
<connect gate="G$1" pin="RB3/SEG3" pad="12"/>
<connect gate="G$1" pin="RB4/COM0" pad="14"/>
<connect gate="G$1" pin="RB5/COM1" pad="15"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCK/SEG14" pad="16"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="17"/>
<connect gate="G$1" pin="RC0/VLCD1" pad="34"/>
<connect gate="G$1" pin="RC1/VLCD2" pad="35"/>
<connect gate="G$1" pin="RC2/VLCD3" pad="36"/>
<connect gate="G$1" pin="RC3/SEG6" pad="37"/>
<connect gate="G$1" pin="RC4/T1G#/SDO/SEG11" pad="42"/>
<connect gate="G$1" pin="RC5/T1CKI/CCP1/SEG10" pad="43"/>
<connect gate="G$1" pin="RC6/TX/CK/SCK/SCL/SEG9" pad="44"/>
<connect gate="G$1" pin="RC7/RX/DT/SDI/SDA/SEG8" pad="1"/>
<connect gate="G$1" pin="RD0/COM3" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2/CCP2" pad="40"/>
<connect gate="G$1" pin="RD3/SEG16" pad="41"/>
<connect gate="G$1" pin="RD4/SEG17" pad="2"/>
<connect gate="G$1" pin="RD5/SEG18" pad="3"/>
<connect gate="G$1" pin="RD6/SEG19" pad="4"/>
<connect gate="G$1" pin="RD7/SEG20" pad="5"/>
<connect gate="G$1" pin="RE0/AN5/SEG21" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/SEG22" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/SEG23" pad="27"/>
<connect gate="G$1" pin="RE3/MCRL#/VPP" pad="18"/>
<connect gate="G$1" pin="VDD_28" pad="28"/>
<connect gate="G$1" pin="VDD_7" pad="7"/>
<connect gate="G$1" pin="VDD_8" pad="8"/>
<connect gate="G$1" pin="VSS_30" pad="30"/>
<connect gate="G$1" pin="VSS_31" pad="31"/>
<connect gate="G$1" pin="VSS_6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F913/916" prefix="IC" uservalue="yes">
<description>28-Pin Flash-Based, 8-Bit CMOS Microcontrollers with nanoWatt Technology</description>
<gates>
<gate name="G$1" symbol="PIC16F913/916"/>
</gates>
<devices>
<device name="-I/SO" package="SOIC28W">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1/SEG12" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/C2/SEG7" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/C2/VR/COM2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/C1/VR/COM3/SEG15" pad="5"/>
<connect gate="G$1" pin="RA4/CIOUT/T0CKI/SEG4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/SS/SEG5" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKKO/T1OSO" pad="10"/>
<connect gate="G$1" pin="RA7/OSC1/CLKI/T1OSI" pad="9"/>
<connect gate="G$1" pin="RB0/INT/SEG0" pad="21"/>
<connect gate="G$1" pin="RB1/SEG1/" pad="22"/>
<connect gate="G$1" pin="RB2/SEG2" pad="23"/>
<connect gate="G$1" pin="RB3/SEG3" pad="24"/>
<connect gate="G$1" pin="RB4/COM0" pad="25"/>
<connect gate="G$1" pin="RB5/COM1" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCK/SEG14" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="28"/>
<connect gate="G$1" pin="RC0/VLCD1" pad="11"/>
<connect gate="G$1" pin="RC1/VLCD2" pad="12"/>
<connect gate="G$1" pin="RC2/VLCD3" pad="13"/>
<connect gate="G$1" pin="RC3/SEG6" pad="14"/>
<connect gate="G$1" pin="RC4/T1G/SDO/SEG11" pad="15"/>
<connect gate="G$1" pin="RC5/T1CKI/CCP1/SEG10" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK/SCK/SCL/SEG9" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/SDI/SDA/SEG8/" pad="18"/>
<connect gate="G$1" pin="RE3/MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-I/SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1/SEG12" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/C2/SEG7" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/C2/VR/COM2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/C1/VR/COM3/SEG15" pad="5"/>
<connect gate="G$1" pin="RA4/CIOUT/T0CKI/SEG4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/SS/SEG5" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKKO/T1OSO" pad="10"/>
<connect gate="G$1" pin="RA7/OSC1/CLKI/T1OSI" pad="9"/>
<connect gate="G$1" pin="RB0/INT/SEG0" pad="21"/>
<connect gate="G$1" pin="RB1/SEG1/" pad="22"/>
<connect gate="G$1" pin="RB2/SEG2" pad="23"/>
<connect gate="G$1" pin="RB3/SEG3" pad="24"/>
<connect gate="G$1" pin="RB4/COM0" pad="25"/>
<connect gate="G$1" pin="RB5/COM1" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCK/SEG14" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="28"/>
<connect gate="G$1" pin="RC0/VLCD1" pad="11"/>
<connect gate="G$1" pin="RC1/VLCD2" pad="12"/>
<connect gate="G$1" pin="RC2/VLCD3" pad="13"/>
<connect gate="G$1" pin="RC3/SEG6" pad="14"/>
<connect gate="G$1" pin="RC4/T1G/SDO/SEG11" pad="15"/>
<connect gate="G$1" pin="RC5/T1CKI/CCP1/SEG10" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK/SCK/SCL/SEG9" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/SDI/SDA/SEG8/" pad="18"/>
<connect gate="G$1" pin="RE3/MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-E/ML" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1/SEG12" pad="27"/>
<connect gate="G$1" pin="RA1/AN1/C2/SEG7" pad="28"/>
<connect gate="G$1" pin="RA2/AN2/C2/VR/COM2" pad="1"/>
<connect gate="G$1" pin="RA3/AN3/C1/VR/COM3/SEG15" pad="2"/>
<connect gate="G$1" pin="RA4/CIOUT/T0CKI/SEG4" pad="3"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/SS/SEG5" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2/CLKKO/T1OSO" pad="7"/>
<connect gate="G$1" pin="RA7/OSC1/CLKI/T1OSI" pad="6"/>
<connect gate="G$1" pin="RB0/INT/SEG0" pad="18"/>
<connect gate="G$1" pin="RB1/SEG1/" pad="19"/>
<connect gate="G$1" pin="RB2/SEG2" pad="20"/>
<connect gate="G$1" pin="RB3/SEG3" pad="21"/>
<connect gate="G$1" pin="RB4/COM0" pad="22"/>
<connect gate="G$1" pin="RB5/COM1" pad="23"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCK/SEG14" pad="24"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="25"/>
<connect gate="G$1" pin="RC0/VLCD1" pad="8"/>
<connect gate="G$1" pin="RC1/VLCD2" pad="9"/>
<connect gate="G$1" pin="RC2/VLCD3" pad="10"/>
<connect gate="G$1" pin="RC3/SEG6" pad="11"/>
<connect gate="G$1" pin="RC4/T1G/SDO/SEG11" pad="12"/>
<connect gate="G$1" pin="RC5/T1CKI/CCP1/SEG10" pad="13"/>
<connect gate="G$1" pin="RC6/TX/CK/SCK/SCL/SEG9" pad="14"/>
<connect gate="G$1" pin="RC7/RX/DT/SDI/SDA/SEG8/" pad="15"/>
<connect gate="G$1" pin="RE3/MCLR/VPP" pad="26"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS1" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/SP" package="DIL28-SP">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1/SEG12" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/C2/SEG7" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/C2/VR/COM2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/C1/VR/COM3/SEG15" pad="5"/>
<connect gate="G$1" pin="RA4/CIOUT/T0CKI/SEG4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/C2OUT/SS/SEG5" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKKO/T1OSO" pad="10"/>
<connect gate="G$1" pin="RA7/OSC1/CLKI/T1OSI" pad="9"/>
<connect gate="G$1" pin="RB0/INT/SEG0" pad="21"/>
<connect gate="G$1" pin="RB1/SEG1/" pad="22"/>
<connect gate="G$1" pin="RB2/SEG2" pad="23"/>
<connect gate="G$1" pin="RB3/SEG3" pad="24"/>
<connect gate="G$1" pin="RB4/COM0" pad="25"/>
<connect gate="G$1" pin="RB5/COM1" pad="26"/>
<connect gate="G$1" pin="RB6/ICSPCLK/ICDCK/SEG14" pad="27"/>
<connect gate="G$1" pin="RB7/ICSPDAT/ICDDAT/SEG13" pad="28"/>
<connect gate="G$1" pin="RC0/VLCD1" pad="11"/>
<connect gate="G$1" pin="RC1/VLCD2" pad="12"/>
<connect gate="G$1" pin="RC2/VLCD3" pad="13"/>
<connect gate="G$1" pin="RC3/SEG6" pad="14"/>
<connect gate="G$1" pin="RC4/T1G/SDO/SEG11" pad="15"/>
<connect gate="G$1" pin="RC5/T1CKI/CCP1/SEG10" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK/SCK/SCL/SEG9" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/SDI/SDA/SEG8/" pad="18"/>
<connect gate="G$1" pin="RE3/MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC9400/01/02" prefix="IC" uservalue="yes">
<description>The TC9400/9401/9402 are low-cost Voltage-to-Frequency
(V/F) converters, utilizing low-power CMOS
technology. The converters accept a variable analog
input signal and generate an output pulse train, whose
frequency is linearly proportional to the input voltage.
The devices can also be used as highly accurate
Frequency-to-Voltage (F/V) converters, accepting
virtually any input frequency waveform and providing a
linearly proportional voltage output.
A complete V/F or F/V system only requires the
addition of two capacitors, three resistors, and reference
voltage.</description>
<gates>
<gate name="TC94XX" symbol="TC9400/01/02"/>
</gates>
<devices>
<device name="DIL14" package="DIL14">
<connects>
<connect gate="TC94XX" pin="1/IBIAS" pad="1"/>
<connect gate="TC94XX" pin="10/F2_OUT" pad="10"/>
<connect gate="TC94XX" pin="11/THRE" pad="11"/>
<connect gate="TC94XX" pin="12/AMP_UOT" pad="12"/>
<connect gate="TC94XX" pin="13/NC" pad="13"/>
<connect gate="TC94XX" pin="14/VDD" pad="14"/>
<connect gate="TC94XX" pin="2/ADJ" pad="2"/>
<connect gate="TC94XX" pin="3/I_IN" pad="3"/>
<connect gate="TC94XX" pin="4/VSS" pad="4"/>
<connect gate="TC94XX" pin="5/V_OUT" pad="5"/>
<connect gate="TC94XX" pin="6/GND" pad="6"/>
<connect gate="TC94XX" pin="7/VREF" pad="7"/>
<connect gate="TC94XX" pin="8/PULS" pad="8"/>
<connect gate="TC94XX" pin="9/COMM" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOIC-14">
<connects>
<connect gate="TC94XX" pin="1/IBIAS" pad="1"/>
<connect gate="TC94XX" pin="10/F2_OUT" pad="10"/>
<connect gate="TC94XX" pin="11/THRE" pad="11"/>
<connect gate="TC94XX" pin="12/AMP_UOT" pad="12"/>
<connect gate="TC94XX" pin="13/NC" pad="13"/>
<connect gate="TC94XX" pin="14/VDD" pad="14"/>
<connect gate="TC94XX" pin="2/ADJ" pad="2"/>
<connect gate="TC94XX" pin="3/I_IN" pad="3"/>
<connect gate="TC94XX" pin="4/VSS" pad="4"/>
<connect gate="TC94XX" pin="5/V_OUT" pad="5"/>
<connect gate="TC94XX" pin="6/GND" pad="6"/>
<connect gate="TC94XX" pin="7/VREF" pad="7"/>
<connect gate="TC94XX" pin="8/PULS" pad="8"/>
<connect gate="TC94XX" pin="9/COMM" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCN75" prefix="IC" uservalue="yes">
<description>The TCN75 is a serially programmable temperature
sensor that notifies the host controller when ambient temperature exceeds a user-programmed setpoint. Hysteresis
is also programmable. The INT/CMPTR output is programmable
as either a simple comparator for thermostat operation
or as a temperature event interrupt. Communication
with the TCN75 is accomplished via a two-wire bus that is
compatible with industry standard protocols. This permits
reading the current temperature, programming the setpoint
and hysteresis, and configuring the device.</description>
<gates>
<gate name="TCN75" symbol="TCN75"/>
</gates>
<devices>
<device name="TCN75MPA" package="DIL8">
<connects>
<connect gate="TCN75" pin="A0" pad="7"/>
<connect gate="TCN75" pin="A1" pad="6"/>
<connect gate="TCN75" pin="A2" pad="5"/>
<connect gate="TCN75" pin="GND" pad="4"/>
<connect gate="TCN75" pin="INT/CM" pad="3"/>
<connect gate="TCN75" pin="SCL" pad="2"/>
<connect gate="TCN75" pin="SDA" pad="1"/>
<connect gate="TCN75" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TCN75MOA" package="SOIC8">
<connects>
<connect gate="TCN75" pin="A0" pad="7"/>
<connect gate="TCN75" pin="A1" pad="6"/>
<connect gate="TCN75" pin="A2" pad="5"/>
<connect gate="TCN75" pin="GND" pad="4"/>
<connect gate="TCN75" pin="INT/CM" pad="3"/>
<connect gate="TCN75" pin="SCL" pad="2"/>
<connect gate="TCN75" pin="SDA" pad="1"/>
<connect gate="TCN75" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TCN75MUA" package="MSOP8">
<connects>
<connect gate="TCN75" pin="A0" pad="7"/>
<connect gate="TCN75" pin="A1" pad="6"/>
<connect gate="TCN75" pin="A2" pad="5"/>
<connect gate="TCN75" pin="GND" pad="4"/>
<connect gate="TCN75" pin="INT/CM" pad="3"/>
<connect gate="TCN75" pin="SCL" pad="2"/>
<connect gate="TCN75" pin="SDA" pad="1"/>
<connect gate="TCN75" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PS501-0901" prefix="IC" uservalue="yes">
<description>Single Chip Field Reprogrammable Battery Manager –
Nickel Chemistries</description>
<gates>
<gate name="G$1" symbol="PS501-0901"/>
</gates>
<devices>
<device name="" package="SSOP28">
<connects>
<connect gate="G$1" pin="1/VDDD" pad="1"/>
<connect gate="G$1" pin="10/RSV3" pad="10"/>
<connect gate="G$1" pin="11/VC1" pad="11"/>
<connect gate="G$1" pin="12/VDDA" pad="12"/>
<connect gate="G$1" pin="13/VSSA" pad="13"/>
<connect gate="G$1" pin="14/RSHP" pad="14"/>
<connect gate="G$1" pin="15/RSHN" pad="15"/>
<connect gate="G$1" pin="16/VNTC" pad="16"/>
<connect gate="G$1" pin="17/VREFT" pad="17"/>
<connect gate="G$1" pin="18/ROSC" pad="18"/>
<connect gate="G$1" pin="19/GPIO8" pad="19"/>
<connect gate="G$1" pin="2/GPIO4" pad="2"/>
<connect gate="G$1" pin="20/GPIO9" pad="20"/>
<connect gate="G$1" pin="21/GPIOHV1" pad="21"/>
<connect gate="G$1" pin="22/MCLR" pad="22"/>
<connect gate="G$1" pin="23/HV2" pad="23"/>
<connect gate="G$1" pin="24/GPIO0" pad="24"/>
<connect gate="G$1" pin="25/GPIO1" pad="25"/>
<connect gate="G$1" pin="26/GPIO2" pad="26"/>
<connect gate="G$1" pin="27/GPIO3" pad="27"/>
<connect gate="G$1" pin="28/VSSD" pad="28"/>
<connect gate="G$1" pin="3/GPIO5" pad="3"/>
<connect gate="G$1" pin="4/GPIO6" pad="4"/>
<connect gate="G$1" pin="5/GPIO7" pad="5"/>
<connect gate="G$1" pin="6/SMB-CLK" pad="6"/>
<connect gate="G$1" pin="7/SMB-DTA" pad="7"/>
<connect gate="G$1" pin="8/RSV1" pad="8"/>
<connect gate="G$1" pin="9/RSV2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PS700" prefix="IC" uservalue="yes">
<description>Battery Monitor</description>
<gates>
<gate name="PS700" symbol="PS700"/>
</gates>
<devices>
<device name="" package="TSSOP8">
<connects>
<connect gate="PS700" pin="GND" pad="7"/>
<connect gate="PS700" pin="NTC/IO0" pad="6"/>
<connect gate="PS700" pin="ROSC" pad="5"/>
<connect gate="PS700" pin="SCL" pad="3"/>
<connect gate="PS700" pin="SDA" pad="4"/>
<connect gate="PS700" pin="SR" pad="8"/>
<connect gate="PS700" pin="VC1" pad="2"/>
<connect gate="PS700" pin="VC2/IO1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP23S08" prefix="IC">
<description>&lt;b&gt;8-Bit I/O Expander with SPI Interface&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MCP23S08"/>
</gates>
<devices>
<device name="SO" package="SO-18W">
<connects>
<connect gate="A" pin="A0" pad="5"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="CS#" pad="7"/>
<connect gate="A" pin="GP0" pad="10"/>
<connect gate="A" pin="GP1" pad="11"/>
<connect gate="A" pin="GP2" pad="12"/>
<connect gate="A" pin="GP3" pad="13"/>
<connect gate="A" pin="GP4" pad="14"/>
<connect gate="A" pin="GP5" pad="15"/>
<connect gate="A" pin="GP6" pad="16"/>
<connect gate="A" pin="GP7" pad="17"/>
<connect gate="A" pin="INT" pad="8"/>
<connect gate="A" pin="RESET#" pad="6"/>
<connect gate="A" pin="SCK" pad="1"/>
<connect gate="A" pin="SI" pad="2"/>
<connect gate="A" pin="SO" pad="3"/>
<connect gate="A" pin="VDD" pad="18"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL18">
<connects>
<connect gate="A" pin="A0" pad="5"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="CS#" pad="7"/>
<connect gate="A" pin="GP0" pad="10"/>
<connect gate="A" pin="GP1" pad="11"/>
<connect gate="A" pin="GP2" pad="12"/>
<connect gate="A" pin="GP3" pad="13"/>
<connect gate="A" pin="GP4" pad="14"/>
<connect gate="A" pin="GP5" pad="15"/>
<connect gate="A" pin="GP6" pad="16"/>
<connect gate="A" pin="GP7" pad="17"/>
<connect gate="A" pin="INT" pad="8"/>
<connect gate="A" pin="RESET#" pad="6"/>
<connect gate="A" pin="SCK" pad="1"/>
<connect gate="A" pin="SI" pad="2"/>
<connect gate="A" pin="SO" pad="3"/>
<connect gate="A" pin="VDD" pad="18"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SS" package="SSOP20">
<connects>
<connect gate="A" pin="A0" pad="5"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="CS#" pad="7"/>
<connect gate="A" pin="GP0" pad="12"/>
<connect gate="A" pin="GP1" pad="13"/>
<connect gate="A" pin="GP2" pad="14"/>
<connect gate="A" pin="GP3" pad="15"/>
<connect gate="A" pin="GP4" pad="16"/>
<connect gate="A" pin="GP5" pad="17"/>
<connect gate="A" pin="GP6" pad="18"/>
<connect gate="A" pin="GP7" pad="19"/>
<connect gate="A" pin="INT" pad="8"/>
<connect gate="A" pin="RESET#" pad="6"/>
<connect gate="A" pin="SCK" pad="1"/>
<connect gate="A" pin="SI" pad="2"/>
<connect gate="A" pin="SO" pad="3"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP2551" prefix="IC">
<description>&lt;b&gt;High-Speed CAN Transceiver&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="MCP2551"/>
</gates>
<devices>
<device name="/SN" package="SO08">
<connects>
<connect gate="X" pin="CANH" pad="7"/>
<connect gate="X" pin="CANL" pad="6"/>
<connect gate="X" pin="RS" pad="8"/>
<connect gate="X" pin="RXD" pad="4"/>
<connect gate="X" pin="TXD" pad="1"/>
<connect gate="X" pin="VDD" pad="3"/>
<connect gate="X" pin="VREF" pad="5"/>
<connect gate="X" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/P" package="DIL08">
<connects>
<connect gate="X" pin="CANH" pad="7"/>
<connect gate="X" pin="CANL" pad="6"/>
<connect gate="X" pin="RS" pad="8"/>
<connect gate="X" pin="RXD" pad="4"/>
<connect gate="X" pin="TXD" pad="1"/>
<connect gate="X" pin="VDD" pad="3"/>
<connect gate="X" pin="VREF" pad="5"/>
<connect gate="X" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP23008" prefix="IC">
<description>&lt;b&gt;8-Bit I/O Expander with I2C Interface&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MCP23008"/>
</gates>
<devices>
<device name="SO" package="SO-18W">
<connects>
<connect gate="A" pin="A0" pad="5"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="GP0" pad="10"/>
<connect gate="A" pin="GP1" pad="11"/>
<connect gate="A" pin="GP2" pad="12"/>
<connect gate="A" pin="GP3" pad="13"/>
<connect gate="A" pin="GP4" pad="14"/>
<connect gate="A" pin="GP5" pad="15"/>
<connect gate="A" pin="GP6" pad="16"/>
<connect gate="A" pin="GP7" pad="17"/>
<connect gate="A" pin="INT" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="RESET#" pad="6"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDA" pad="2"/>
<connect gate="A" pin="VDD" pad="18"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL18">
<connects>
<connect gate="A" pin="A0" pad="5"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="GP0" pad="10"/>
<connect gate="A" pin="GP1" pad="11"/>
<connect gate="A" pin="GP2" pad="12"/>
<connect gate="A" pin="GP3" pad="13"/>
<connect gate="A" pin="GP4" pad="14"/>
<connect gate="A" pin="GP5" pad="15"/>
<connect gate="A" pin="GP6" pad="16"/>
<connect gate="A" pin="GP7" pad="17"/>
<connect gate="A" pin="INT" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="RESET#" pad="6"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDA" pad="2"/>
<connect gate="A" pin="VDD" pad="18"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SS" package="SSOP20">
<connects>
<connect gate="A" pin="A0" pad="5"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="GP0" pad="12"/>
<connect gate="A" pin="GP1" pad="13"/>
<connect gate="A" pin="GP2" pad="14"/>
<connect gate="A" pin="GP3" pad="15"/>
<connect gate="A" pin="GP4" pad="16"/>
<connect gate="A" pin="GP5" pad="17"/>
<connect gate="A" pin="GP6" pad="18"/>
<connect gate="A" pin="GP7" pad="19"/>
<connect gate="A" pin="INT" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="RESET#" pad="6"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDA" pad="2"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4455">
<description>&lt;b&gt;PIC18F Flash Microcontroller with USB port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="PIC18F4455/4550"/>
</gates>
<devices>
<device name="SP" package="DIL40">
<connects>
<connect gate="X" pin="CCP1/P1A/RC2" pad="17"/>
<connect gate="X" pin="CK/TX/RC6" pad="25"/>
<connect gate="X" pin="MCLR/VPP/RE3" pad="1"/>
<connect gate="X" pin="OESPP/AN7/RE2" pad="10"/>
<connect gate="X" pin="OSC1/CLKI" pad="13"/>
<connect gate="X" pin="OSC2/CLKO/RA6" pad="14"/>
<connect gate="X" pin="P1B/SPP5/RD5" pad="28"/>
<connect gate="X" pin="P1C/SPP6/RD6" pad="29"/>
<connect gate="X" pin="P1D/SPP7/RD7" pad="30"/>
<connect gate="X" pin="RA0/AN0" pad="2"/>
<connect gate="X" pin="RA1/AN1" pad="3"/>
<connect gate="X" pin="RA2/AN2/VR-/CVR" pad="4"/>
<connect gate="X" pin="RA3/AN3/VR+" pad="5"/>
<connect gate="X" pin="RA4/T0CKI/C1OUT/RCV" pad="6"/>
<connect gate="X" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="7"/>
<connect gate="X" pin="RB0/AN12/INT0/FLT0/SDI/SDA" pad="33"/>
<connect gate="X" pin="RB1/AN10/INT1/SCK/SCL" pad="34"/>
<connect gate="X" pin="RB2/AN8/INT2/VMO" pad="35"/>
<connect gate="X" pin="RB3/AN9/CCP2/VPO" pad="36"/>
<connect gate="X" pin="RB4/KBI0/AN11/CSSPP" pad="37"/>
<connect gate="X" pin="RB5/KBI1/PGM" pad="38"/>
<connect gate="X" pin="RB6/KBI2/PGC" pad="39"/>
<connect gate="X" pin="RB7/KBI3/PGD" pad="40"/>
<connect gate="X" pin="RE0/AN5/CK1SPP" pad="8"/>
<connect gate="X" pin="RE1/AN6/CK2SPP" pad="9"/>
<connect gate="X" pin="SDO/DT/RX/RC7" pad="26"/>
<connect gate="X" pin="SPP0/RD0" pad="19"/>
<connect gate="X" pin="SPP1/RD1" pad="20"/>
<connect gate="X" pin="SPP2/RD2" pad="21"/>
<connect gate="X" pin="SPP3/RD3" pad="22"/>
<connect gate="X" pin="SPP4/RD4" pad="27"/>
<connect gate="X" pin="T13CKI/T1OSO/RC0" pad="15"/>
<connect gate="X" pin="UOE/CCP2/T1OSI/RC1" pad="16"/>
<connect gate="X" pin="VDD" pad="11"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VM/D-/RC4" pad="23"/>
<connect gate="X" pin="VP/D+/RC5" pad="24"/>
<connect gate="X" pin="VSS" pad="12"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VUSB" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TQ-44" package="TQFP44">
<connects>
<connect gate="X" pin="CCP1/P1A/RC2" pad="36"/>
<connect gate="X" pin="CK/TX/RC6" pad="44"/>
<connect gate="X" pin="MCLR/VPP/RE3" pad="18"/>
<connect gate="X" pin="OESPP/AN7/RE2" pad="27"/>
<connect gate="X" pin="OSC1/CLKI" pad="30"/>
<connect gate="X" pin="OSC2/CLKO/RA6" pad="31"/>
<connect gate="X" pin="P1B/SPP5/RD5" pad="3"/>
<connect gate="X" pin="P1C/SPP6/RD6" pad="4"/>
<connect gate="X" pin="P1D/SPP7/RD7" pad="5"/>
<connect gate="X" pin="RA0/AN0" pad="19"/>
<connect gate="X" pin="RA1/AN1" pad="20"/>
<connect gate="X" pin="RA2/AN2/VR-/CVR" pad="21"/>
<connect gate="X" pin="RA3/AN3/VR+" pad="22"/>
<connect gate="X" pin="RA4/T0CKI/C1OUT/RCV" pad="23"/>
<connect gate="X" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="24"/>
<connect gate="X" pin="RB0/AN12/INT0/FLT0/SDI/SDA" pad="8"/>
<connect gate="X" pin="RB1/AN10/INT1/SCK/SCL" pad="9"/>
<connect gate="X" pin="RB2/AN8/INT2/VMO" pad="10"/>
<connect gate="X" pin="RB3/AN9/CCP2/VPO" pad="11"/>
<connect gate="X" pin="RB4/KBI0/AN11/CSSPP" pad="14"/>
<connect gate="X" pin="RB5/KBI1/PGM" pad="15"/>
<connect gate="X" pin="RB6/KBI2/PGC" pad="16"/>
<connect gate="X" pin="RB7/KBI3/PGD" pad="17"/>
<connect gate="X" pin="RE0/AN5/CK1SPP" pad="25"/>
<connect gate="X" pin="RE1/AN6/CK2SPP" pad="26"/>
<connect gate="X" pin="SDO/DT/RX/RC7" pad="1"/>
<connect gate="X" pin="SPP0/RD0" pad="38"/>
<connect gate="X" pin="SPP1/RD1" pad="39"/>
<connect gate="X" pin="SPP2/RD2" pad="40"/>
<connect gate="X" pin="SPP3/RD3" pad="41"/>
<connect gate="X" pin="SPP4/RD4" pad="2"/>
<connect gate="X" pin="T13CKI/T1OSO/RC0" pad="32"/>
<connect gate="X" pin="UOE/CCP2/T1OSI/RC1" pad="35"/>
<connect gate="X" pin="VDD" pad="7"/>
<connect gate="X" pin="VDD@1" pad="28"/>
<connect gate="X" pin="VM/D-/RC4" pad="42"/>
<connect gate="X" pin="VP/D+/RC5" pad="43"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="29"/>
<connect gate="X" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ML" package="QFN44-8X8">
<connects>
<connect gate="X" pin="CCP1/P1A/RC2" pad="36"/>
<connect gate="X" pin="CK/TX/RC6" pad="44"/>
<connect gate="X" pin="MCLR/VPP/RE3" pad="18"/>
<connect gate="X" pin="OESPP/AN7/RE2" pad="27"/>
<connect gate="X" pin="OSC1/CLKI" pad="32"/>
<connect gate="X" pin="OSC2/CLKO/RA6" pad="33"/>
<connect gate="X" pin="P1B/SPP5/RD5" pad="3"/>
<connect gate="X" pin="P1C/SPP6/RD6" pad="4"/>
<connect gate="X" pin="P1D/SPP7/RD7" pad="5"/>
<connect gate="X" pin="RA0/AN0" pad="19"/>
<connect gate="X" pin="RA1/AN1" pad="20"/>
<connect gate="X" pin="RA2/AN2/VR-/CVR" pad="21"/>
<connect gate="X" pin="RA3/AN3/VR+" pad="22"/>
<connect gate="X" pin="RA4/T0CKI/C1OUT/RCV" pad="23"/>
<connect gate="X" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="24"/>
<connect gate="X" pin="RB0/AN12/INT0/FLT0/SDI/SDA" pad="9"/>
<connect gate="X" pin="RB1/AN10/INT1/SCK/SCL" pad="10"/>
<connect gate="X" pin="RB2/AN8/INT2/VMO" pad="11"/>
<connect gate="X" pin="RB3/AN9/CCP2/VPO" pad="12"/>
<connect gate="X" pin="RB4/KBI0/AN11/CSSPP" pad="14"/>
<connect gate="X" pin="RB5/KBI1/PGM" pad="15"/>
<connect gate="X" pin="RB6/KBI2/PGC" pad="16"/>
<connect gate="X" pin="RB7/KBI3/PGD" pad="17"/>
<connect gate="X" pin="RE0/AN5/CK1SPP" pad="25"/>
<connect gate="X" pin="RE1/AN6/CK2SPP" pad="26"/>
<connect gate="X" pin="SDO/DT/RX/RC7" pad="1"/>
<connect gate="X" pin="SPP0/RD0" pad="38"/>
<connect gate="X" pin="SPP1/RD1" pad="39"/>
<connect gate="X" pin="SPP2/RD2" pad="40"/>
<connect gate="X" pin="SPP3/RD3" pad="41"/>
<connect gate="X" pin="SPP4/RD4" pad="2"/>
<connect gate="X" pin="T13CKI/T1OSO/RC0" pad="34"/>
<connect gate="X" pin="UOE/CCP2/T1OSI/RC1" pad="35"/>
<connect gate="X" pin="VDD" pad="8"/>
<connect gate="X" pin="VDD@1" pad="29"/>
<connect gate="X" pin="VM/D-/RC4" pad="42"/>
<connect gate="X" pin="VP/D+/RC5" pad="43"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4550">
<description>&lt;b&gt;PIC18F Flash Microcontroller with USB port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="PIC18F4455/4550"/>
</gates>
<devices>
<device name="SP" package="DIL40">
<connects>
<connect gate="X" pin="CCP1/P1A/RC2" pad="17"/>
<connect gate="X" pin="CK/TX/RC6" pad="25"/>
<connect gate="X" pin="MCLR/VPP/RE3" pad="1"/>
<connect gate="X" pin="OESPP/AN7/RE2" pad="10"/>
<connect gate="X" pin="OSC1/CLKI" pad="13"/>
<connect gate="X" pin="OSC2/CLKO/RA6" pad="14"/>
<connect gate="X" pin="P1B/SPP5/RD5" pad="28"/>
<connect gate="X" pin="P1C/SPP6/RD6" pad="29"/>
<connect gate="X" pin="P1D/SPP7/RD7" pad="30"/>
<connect gate="X" pin="RA0/AN0" pad="2"/>
<connect gate="X" pin="RA1/AN1" pad="3"/>
<connect gate="X" pin="RA2/AN2/VR-/CVR" pad="4"/>
<connect gate="X" pin="RA3/AN3/VR+" pad="5"/>
<connect gate="X" pin="RA4/T0CKI/C1OUT/RCV" pad="6"/>
<connect gate="X" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="7"/>
<connect gate="X" pin="RB0/AN12/INT0/FLT0/SDI/SDA" pad="33"/>
<connect gate="X" pin="RB1/AN10/INT1/SCK/SCL" pad="34"/>
<connect gate="X" pin="RB2/AN8/INT2/VMO" pad="35"/>
<connect gate="X" pin="RB3/AN9/CCP2/VPO" pad="36"/>
<connect gate="X" pin="RB4/KBI0/AN11/CSSPP" pad="37"/>
<connect gate="X" pin="RB5/KBI1/PGM" pad="38"/>
<connect gate="X" pin="RB6/KBI2/PGC" pad="39"/>
<connect gate="X" pin="RB7/KBI3/PGD" pad="40"/>
<connect gate="X" pin="RE0/AN5/CK1SPP" pad="8"/>
<connect gate="X" pin="RE1/AN6/CK2SPP" pad="9"/>
<connect gate="X" pin="SDO/DT/RX/RC7" pad="26"/>
<connect gate="X" pin="SPP0/RD0" pad="19"/>
<connect gate="X" pin="SPP1/RD1" pad="20"/>
<connect gate="X" pin="SPP2/RD2" pad="21"/>
<connect gate="X" pin="SPP3/RD3" pad="22"/>
<connect gate="X" pin="SPP4/RD4" pad="27"/>
<connect gate="X" pin="T13CKI/T1OSO/RC0" pad="15"/>
<connect gate="X" pin="UOE/CCP2/T1OSI/RC1" pad="16"/>
<connect gate="X" pin="VDD" pad="11"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VM/D-/RC4" pad="23"/>
<connect gate="X" pin="VP/D+/RC5" pad="24"/>
<connect gate="X" pin="VSS" pad="12"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VUSB" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TQ-44" package="TQFP44">
<connects>
<connect gate="X" pin="CCP1/P1A/RC2" pad="36"/>
<connect gate="X" pin="CK/TX/RC6" pad="44"/>
<connect gate="X" pin="MCLR/VPP/RE3" pad="18"/>
<connect gate="X" pin="OESPP/AN7/RE2" pad="27"/>
<connect gate="X" pin="OSC1/CLKI" pad="30"/>
<connect gate="X" pin="OSC2/CLKO/RA6" pad="31"/>
<connect gate="X" pin="P1B/SPP5/RD5" pad="3"/>
<connect gate="X" pin="P1C/SPP6/RD6" pad="4"/>
<connect gate="X" pin="P1D/SPP7/RD7" pad="5"/>
<connect gate="X" pin="RA0/AN0" pad="19"/>
<connect gate="X" pin="RA1/AN1" pad="20"/>
<connect gate="X" pin="RA2/AN2/VR-/CVR" pad="21"/>
<connect gate="X" pin="RA3/AN3/VR+" pad="22"/>
<connect gate="X" pin="RA4/T0CKI/C1OUT/RCV" pad="23"/>
<connect gate="X" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="24"/>
<connect gate="X" pin="RB0/AN12/INT0/FLT0/SDI/SDA" pad="8"/>
<connect gate="X" pin="RB1/AN10/INT1/SCK/SCL" pad="9"/>
<connect gate="X" pin="RB2/AN8/INT2/VMO" pad="10"/>
<connect gate="X" pin="RB3/AN9/CCP2/VPO" pad="11"/>
<connect gate="X" pin="RB4/KBI0/AN11/CSSPP" pad="14"/>
<connect gate="X" pin="RB5/KBI1/PGM" pad="15"/>
<connect gate="X" pin="RB6/KBI2/PGC" pad="16"/>
<connect gate="X" pin="RB7/KBI3/PGD" pad="17"/>
<connect gate="X" pin="RE0/AN5/CK1SPP" pad="25"/>
<connect gate="X" pin="RE1/AN6/CK2SPP" pad="26"/>
<connect gate="X" pin="SDO/DT/RX/RC7" pad="1"/>
<connect gate="X" pin="SPP0/RD0" pad="38"/>
<connect gate="X" pin="SPP1/RD1" pad="39"/>
<connect gate="X" pin="SPP2/RD2" pad="40"/>
<connect gate="X" pin="SPP3/RD3" pad="41"/>
<connect gate="X" pin="SPP4/RD4" pad="2"/>
<connect gate="X" pin="T13CKI/T1OSO/RC0" pad="32"/>
<connect gate="X" pin="UOE/CCP2/T1OSI/RC1" pad="35"/>
<connect gate="X" pin="VDD" pad="7"/>
<connect gate="X" pin="VDD@1" pad="28"/>
<connect gate="X" pin="VM/D-/RC4" pad="42"/>
<connect gate="X" pin="VP/D+/RC5" pad="43"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="29"/>
<connect gate="X" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ML" package="QFN44-8X8">
<connects>
<connect gate="X" pin="CCP1/P1A/RC2" pad="36"/>
<connect gate="X" pin="CK/TX/RC6" pad="44"/>
<connect gate="X" pin="MCLR/VPP/RE3" pad="18"/>
<connect gate="X" pin="OESPP/AN7/RE2" pad="27"/>
<connect gate="X" pin="OSC1/CLKI" pad="32"/>
<connect gate="X" pin="OSC2/CLKO/RA6" pad="33"/>
<connect gate="X" pin="P1B/SPP5/RD5" pad="3"/>
<connect gate="X" pin="P1C/SPP6/RD6" pad="4"/>
<connect gate="X" pin="P1D/SPP7/RD7" pad="5"/>
<connect gate="X" pin="RA0/AN0" pad="19"/>
<connect gate="X" pin="RA1/AN1" pad="20"/>
<connect gate="X" pin="RA2/AN2/VR-/CVR" pad="21"/>
<connect gate="X" pin="RA3/AN3/VR+" pad="22"/>
<connect gate="X" pin="RA4/T0CKI/C1OUT/RCV" pad="23"/>
<connect gate="X" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="24"/>
<connect gate="X" pin="RB0/AN12/INT0/FLT0/SDI/SDA" pad="9"/>
<connect gate="X" pin="RB1/AN10/INT1/SCK/SCL" pad="10"/>
<connect gate="X" pin="RB2/AN8/INT2/VMO" pad="11"/>
<connect gate="X" pin="RB3/AN9/CCP2/VPO" pad="12"/>
<connect gate="X" pin="RB4/KBI0/AN11/CSSPP" pad="14"/>
<connect gate="X" pin="RB5/KBI1/PGM" pad="15"/>
<connect gate="X" pin="RB6/KBI2/PGC" pad="16"/>
<connect gate="X" pin="RB7/KBI3/PGD" pad="17"/>
<connect gate="X" pin="RE0/AN5/CK1SPP" pad="25"/>
<connect gate="X" pin="RE1/AN6/CK2SPP" pad="26"/>
<connect gate="X" pin="SDO/DT/RX/RC7" pad="1"/>
<connect gate="X" pin="SPP0/RD0" pad="38"/>
<connect gate="X" pin="SPP1/RD1" pad="39"/>
<connect gate="X" pin="SPP2/RD2" pad="40"/>
<connect gate="X" pin="SPP3/RD3" pad="41"/>
<connect gate="X" pin="SPP4/RD4" pad="2"/>
<connect gate="X" pin="T13CKI/T1OSO/RC0" pad="34"/>
<connect gate="X" pin="UOE/CCP2/T1OSI/RC1" pad="35"/>
<connect gate="X" pin="VDD" pad="8"/>
<connect gate="X" pin="VDD@1" pad="29"/>
<connect gate="X" pin="VM/D-/RC4" pad="42"/>
<connect gate="X" pin="VP/D+/RC5" pad="43"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1276" prefix="IC">
<description>&lt;b&gt;Power Supply Monitor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="RESETS23"/>
</gates>
<devices>
<device name="" package="SOT23B-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="RESET#" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F2011" prefix="IC">
<description>&lt;b&gt;dsPIC Sensor DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F2011/3012"/>
</gates>
<devices>
<device name="/P" package="DIL18">
<connects>
<connect gate="X" pin="AVDD" pad="18"/>
<connect gate="X" pin="AVSS" pad="17"/>
<connect gate="X" pin="CLKI/OSC1" pad="6"/>
<connect gate="X" pin="EMUC1/SOSCO/T1CK/U1ARX/CN0/RC14" pad="9"/>
<connect gate="X" pin="EMUC2/OC1/IC1/INT1/RD0" pad="10"/>
<connect gate="X" pin="EMUD1/SOSCI/T2CK/U1ATX/CN1/RC13" pad="8"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/LVDIN/SS1" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6/U1TX/SDO1/SCL/EMUD/PGD" pad="11"/>
<connect gate="X" pin="RB5/AN5/CN7/U1RX/SDI1/SDA/EMUC/PGC" pad="12"/>
<connect gate="X" pin="RB6/AN6/INT0/SCK1/OCFA" pad="16"/>
<connect gate="X" pin="RB7/AN7/IC2/OC2/EMUD2" pad="15"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="7"/>
<connect gate="X" pin="VDD" pad="14"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SO" package="SO18W">
<connects>
<connect gate="X" pin="AVDD" pad="18"/>
<connect gate="X" pin="AVSS" pad="17"/>
<connect gate="X" pin="CLKI/OSC1" pad="6"/>
<connect gate="X" pin="EMUC1/SOSCO/T1CK/U1ARX/CN0/RC14" pad="9"/>
<connect gate="X" pin="EMUC2/OC1/IC1/INT1/RD0" pad="10"/>
<connect gate="X" pin="EMUD1/SOSCI/T2CK/U1ATX/CN1/RC13" pad="8"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/LVDIN/SS1" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6/U1TX/SDO1/SCL/EMUD/PGD" pad="11"/>
<connect gate="X" pin="RB5/AN5/CN7/U1RX/SDI1/SDA/EMUC/PGC" pad="12"/>
<connect gate="X" pin="RB6/AN6/INT0/SCK1/OCFA" pad="16"/>
<connect gate="X" pin="RB7/AN7/IC2/OC2/EMUD2" pad="15"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="7"/>
<connect gate="X" pin="VDD" pad="14"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN-S28-6X6">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="24"/>
<connect gate="X" pin="CLKI/OSC1" pad="6"/>
<connect gate="X" pin="EMUC1/SOSCO/T1CK/U1ARX/CN0/RC14" pad="9"/>
<connect gate="X" pin="EMUC2/OC1/IC1/INT1/RD0" pad="12"/>
<connect gate="X" pin="EMUD1/SOSCI/T2CK/U1ATX/CN1/RC13" pad="8"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+" pad="27"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-" pad="28"/>
<connect gate="X" pin="RB2/AN2/CN4/LVDIN/SS1" pad="1"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="2"/>
<connect gate="X" pin="RB4/AN4/CN6/U1TX/SDO1/SCL/EMUD/PGD" pad="14"/>
<connect gate="X" pin="RB5/AN5/CN7/U1RX/SDI1/SDA/EMUC/PGC" pad="15"/>
<connect gate="X" pin="RB6/AN6/INT0/SCK1/OCFA" pad="23"/>
<connect gate="X" pin="RB7/AN7/IC2/OC2/EMUD2" pad="22"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="7"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VPP/MCLR" pad="26"/>
<connect gate="X" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F3011" prefix="IC">
<description>&lt;b&gt;dsPIC Motion Controller DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F3011"/>
</gates>
<devices>
<device name="/P" package="DIL40">
<connects>
<connect gate="X" pin="AVDD" pad="40"/>
<connect gate="X" pin="AVSS" pad="39"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="28"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="27"/>
<connect gate="X" pin="FLTA/INT0/RE8" pad="17"/>
<connect gate="X" pin="OSC1/CLKI" pad="13"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="14"/>
<connect gate="X" pin="PGC/EMUC/SDI1/SDA/U1RX/RF2" pad="26"/>
<connect gate="X" pin="PGD/EMUD/SDO1/SCL/U1TX/RF3" pad="25"/>
<connect gate="X" pin="PWM1H/RE1" pad="37"/>
<connect gate="X" pin="PWM1L/RE0" pad="38"/>
<connect gate="X" pin="PWM2H/RE3" pad="35"/>
<connect gate="X" pin="PWM2L/RE2" pad="36"/>
<connect gate="X" pin="PWM3H/RE5" pad="33"/>
<connect gate="X" pin="PWM3L/RE4" pad="34"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7/QEA" pad="6"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8/QEB" pad="7"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="8"/>
<connect gate="X" pin="RB7/AN7" pad="9"/>
<connect gate="X" pin="RB8/AN8" pad="10"/>
<connect gate="X" pin="RC13/CN1/T2CK/U1ATX/SOSCI/EMUD1" pad="15"/>
<connect gate="X" pin="RC14/CN0/T1CK/U1ARX/SOSCO/EMUC1" pad="16"/>
<connect gate="X" pin="RD0/INT1/IC1/OC1/EMUC2" pad="23"/>
<connect gate="X" pin="RD1/INT2/IC2/OC2/EMUD2" pad="18"/>
<connect gate="X" pin="RD2/OC3" pad="22"/>
<connect gate="X" pin="RD3/OC4" pad="19"/>
<connect gate="X" pin="RF0" pad="30"/>
<connect gate="X" pin="RF1" pad="29"/>
<connect gate="X" pin="SCK1/RF6" pad="24"/>
<connect gate="X" pin="VDD" pad="11"/>
<connect gate="X" pin="VDD@1" pad="21"/>
<connect gate="X" pin="VDD@2" pad="32"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="12"/>
<connect gate="X" pin="VSS@1" pad="20"/>
<connect gate="X" pin="VSS@2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/PT" package="TQFP44">
<connects>
<connect gate="X" pin="AVDD" pad="17"/>
<connect gate="X" pin="AVSS" pad="16"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="3"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="2"/>
<connect gate="X" pin="FLTA/INT0/RE8" pad="36"/>
<connect gate="X" pin="OSC1/CLKI" pad="30"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="31"/>
<connect gate="X" pin="PGC/EMUC/SDI1/SDA/U1RX/RF2" pad="1"/>
<connect gate="X" pin="PGD/EMUD/SDO1/SCL/U1TX/RF3" pad="44"/>
<connect gate="X" pin="PWM1H/RE1" pad="14"/>
<connect gate="X" pin="PWM1L/RE0" pad="15"/>
<connect gate="X" pin="PWM2H/RE3" pad="10"/>
<connect gate="X" pin="PWM2L/RE2" pad="11"/>
<connect gate="X" pin="PWM3H/RE5" pad="8"/>
<connect gate="X" pin="PWM3L/RE4" pad="9"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="19"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="20"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1" pad="21"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="22"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7/QEA" pad="23"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8/QEB" pad="24"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="25"/>
<connect gate="X" pin="RB7/AN7" pad="26"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RC13/CN1/T2CK/U1ATX/SOSCI/EMUD1" pad="32"/>
<connect gate="X" pin="RC14/CN0/T1CK/U1ARX/SOSCO/EMUC1" pad="35"/>
<connect gate="X" pin="RD0/INT1/IC1/OC1/EMUC2" pad="42"/>
<connect gate="X" pin="RD1/INT2/IC2/OC2/EMUD2" pad="37"/>
<connect gate="X" pin="RD2/OC3" pad="41"/>
<connect gate="X" pin="RD3/OC4" pad="38"/>
<connect gate="X" pin="RF0" pad="5"/>
<connect gate="X" pin="RF1" pad="4"/>
<connect gate="X" pin="SCK1/RF6" pad="43"/>
<connect gate="X" pin="VDD" pad="7"/>
<connect gate="X" pin="VDD@1" pad="28"/>
<connect gate="X" pin="VDD@2" pad="40"/>
<connect gate="X" pin="VPP/MCLR" pad="18"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="29"/>
<connect gate="X" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN44-8X8">
<connects>
<connect gate="X" pin="AVDD" pad="17"/>
<connect gate="X" pin="AVSS" pad="16"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="3"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="2"/>
<connect gate="X" pin="FLTA/INT0/RE8" pad="36"/>
<connect gate="X" pin="OSC1/CLKI" pad="32"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="33"/>
<connect gate="X" pin="PGC/EMUC/SDI1/SDA/U1RX/RF2" pad="1"/>
<connect gate="X" pin="PGD/EMUD/SDO1/SCL/U1TX/RF3" pad="44"/>
<connect gate="X" pin="PWM1H/RE1" pad="14"/>
<connect gate="X" pin="PWM1L/RE0" pad="15"/>
<connect gate="X" pin="PWM2H/RE3" pad="11"/>
<connect gate="X" pin="PWM2L/RE2" pad="12"/>
<connect gate="X" pin="PWM3H/RE5" pad="9"/>
<connect gate="X" pin="PWM3L/RE4" pad="10"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="19"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="20"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1" pad="21"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="22"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7/QEA" pad="23"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8/QEB" pad="24"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="25"/>
<connect gate="X" pin="RB7/AN7" pad="26"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RC13/CN1/T2CK/U1ATX/SOSCI/EMUD1" pad="34"/>
<connect gate="X" pin="RC14/CN0/T1CK/U1ARX/SOSCO/EMUC1" pad="35"/>
<connect gate="X" pin="RD0/INT1/IC1/OC1/EMUC2" pad="42"/>
<connect gate="X" pin="RD1/INT2/IC2/OC2/EMUD2" pad="37"/>
<connect gate="X" pin="RD2/OC3" pad="41"/>
<connect gate="X" pin="RD3/OC4" pad="38"/>
<connect gate="X" pin="RF0" pad="5"/>
<connect gate="X" pin="RF1" pad="4"/>
<connect gate="X" pin="SCK1/RF6" pad="43"/>
<connect gate="X" pin="VDD" pad="7"/>
<connect gate="X" pin="VDD@1" pad="28"/>
<connect gate="X" pin="VDD@2" pad="40"/>
<connect gate="X" pin="VPP/MCLR" pad="18"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="30"/>
<connect gate="X" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F3012" prefix="IC">
<description>&lt;b&gt;dsPIC Sensor DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F2011/3012"/>
</gates>
<devices>
<device name="/P" package="DIL18">
<connects>
<connect gate="X" pin="AVDD" pad="18"/>
<connect gate="X" pin="AVSS" pad="17"/>
<connect gate="X" pin="CLKI/OSC1" pad="6"/>
<connect gate="X" pin="EMUC1/SOSCO/T1CK/U1ARX/CN0/RC14" pad="9"/>
<connect gate="X" pin="EMUC2/OC1/IC1/INT1/RD0" pad="10"/>
<connect gate="X" pin="EMUD1/SOSCI/T2CK/U1ATX/CN1/RC13" pad="8"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/LVDIN/SS1" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6/U1TX/SDO1/SCL/EMUD/PGD" pad="11"/>
<connect gate="X" pin="RB5/AN5/CN7/U1RX/SDI1/SDA/EMUC/PGC" pad="12"/>
<connect gate="X" pin="RB6/AN6/INT0/SCK1/OCFA" pad="16"/>
<connect gate="X" pin="RB7/AN7/IC2/OC2/EMUD2" pad="15"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="7"/>
<connect gate="X" pin="VDD" pad="14"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SO" package="SO18W">
<connects>
<connect gate="X" pin="AVDD" pad="18"/>
<connect gate="X" pin="AVSS" pad="17"/>
<connect gate="X" pin="CLKI/OSC1" pad="6"/>
<connect gate="X" pin="EMUC1/SOSCO/T1CK/U1ARX/CN0/RC14" pad="9"/>
<connect gate="X" pin="EMUC2/OC1/IC1/INT1/RD0" pad="10"/>
<connect gate="X" pin="EMUD1/SOSCI/T2CK/U1ATX/CN1/RC13" pad="8"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/LVDIN/SS1" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6/U1TX/SDO1/SCL/EMUD/PGD" pad="11"/>
<connect gate="X" pin="RB5/AN5/CN7/U1RX/SDI1/SDA/EMUC/PGC" pad="12"/>
<connect gate="X" pin="RB6/AN6/INT0/SCK1/OCFA" pad="16"/>
<connect gate="X" pin="RB7/AN7/IC2/OC2/EMUD2" pad="15"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="7"/>
<connect gate="X" pin="VDD" pad="14"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN44-8X8">
<connects>
<connect gate="X" pin="AVDD" pad="17"/>
<connect gate="X" pin="AVSS" pad="16"/>
<connect gate="X" pin="CLKI/OSC1" pad="32"/>
<connect gate="X" pin="EMUC1/SOSCO/T1CK/U1ARX/CN0/RC14" pad="35"/>
<connect gate="X" pin="EMUC2/OC1/IC1/INT1/RD0" pad="42"/>
<connect gate="X" pin="EMUD1/SOSCI/T2CK/U1ATX/CN1/RC13" pad="34"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+" pad="19"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-" pad="20"/>
<connect gate="X" pin="RB2/AN2/CN4/LVDIN/SS1" pad="23"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="25"/>
<connect gate="X" pin="RB4/AN4/CN6/U1TX/SDO1/SCL/EMUD/PGD" pad="44"/>
<connect gate="X" pin="RB5/AN5/CN7/U1RX/SDI1/SDA/EMUC/PGC" pad="1"/>
<connect gate="X" pin="RB6/AN6/INT0/SCK1/OCFA" pad="14"/>
<connect gate="X" pin="RB7/AN7/IC2/OC2/EMUD2" pad="12"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="33"/>
<connect gate="X" pin="VDD" pad="4"/>
<connect gate="X" pin="VPP/MCLR" pad="18"/>
<connect gate="X" pin="VSS" pad="30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F3014" prefix="IC">
<description>&lt;b&gt;dsPIC General DSC&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="DSPIC30F3014"/>
</gates>
<devices>
<device name="/P" package="DIL40">
<connects>
<connect gate="A" pin="AVDD" pad="40"/>
<connect gate="A" pin="AVSS" pad="39"/>
<connect gate="A" pin="EMUC2/OC1/RD0" pad="34"/>
<connect gate="A" pin="EMUC3/SCK1/RF6" pad="24"/>
<connect gate="A" pin="EMUD2/OC2/RD1" pad="33"/>
<connect gate="A" pin="EMUD3/U1TX/SDO1/SCL/RF3" pad="25"/>
<connect gate="A" pin="INT1/IC1/RD8" pad="23"/>
<connect gate="A" pin="INT2/IC2/RD9" pad="18"/>
<connect gate="A" pin="MCLR" pad="1"/>
<connect gate="A" pin="OSC1/CLKIN" pad="13"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="14"/>
<connect gate="A" pin="RA11/INT0" pad="17"/>
<connect gate="A" pin="RB0/AN0/CN2" pad="2"/>
<connect gate="A" pin="RB1/AN1/CN3" pad="3"/>
<connect gate="A" pin="RB10/AN10" pad="37"/>
<connect gate="A" pin="RB11/AN11" pad="36"/>
<connect gate="A" pin="RB12/AN12" pad="35"/>
<connect gate="A" pin="RB2/AN2/CN4/SS1/LVDIN" pad="4"/>
<connect gate="A" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="A" pin="RB4/AN4/CN6" pad="6"/>
<connect gate="A" pin="RB5/AN5/CN7" pad="7"/>
<connect gate="A" pin="RB6/AN6/EMUC/PGC/OCFA" pad="8"/>
<connect gate="A" pin="RB7/AN7/EMUD/PGD" pad="9"/>
<connect gate="A" pin="RB8/AN8" pad="10"/>
<connect gate="A" pin="RB9/AN9" pad="38"/>
<connect gate="A" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="15"/>
<connect gate="A" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="16"/>
<connect gate="A" pin="RD2" pad="22"/>
<connect gate="A" pin="RD3" pad="19"/>
<connect gate="A" pin="RF0" pad="30"/>
<connect gate="A" pin="RF1" pad="29"/>
<connect gate="A" pin="U1RX/SDI1/SDA/RF2" pad="26"/>
<connect gate="A" pin="U2RX/CN17/RF4" pad="28"/>
<connect gate="A" pin="U2TX/CN18/RF5" pad="27"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VDD@1" pad="21"/>
<connect gate="A" pin="VDD@2" pad="32"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="VSS@1" pad="20"/>
<connect gate="A" pin="VSS@2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/PT" package="TQFP44">
<connects>
<connect gate="A" pin="AVDD" pad="17"/>
<connect gate="A" pin="AVSS" pad="16"/>
<connect gate="A" pin="EMUC2/OC1/RD0" pad="9"/>
<connect gate="A" pin="EMUC3/SCK1/RF6" pad="43"/>
<connect gate="A" pin="EMUD2/OC2/RD1" pad="8"/>
<connect gate="A" pin="EMUD3/U1TX/SDO1/SCL/RF3" pad="44"/>
<connect gate="A" pin="INT1/IC1/RD8" pad="42"/>
<connect gate="A" pin="INT2/IC2/RD9" pad="37"/>
<connect gate="A" pin="MCLR" pad="18"/>
<connect gate="A" pin="OSC1/CLKIN" pad="30"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="31"/>
<connect gate="A" pin="RA11/INT0" pad="36"/>
<connect gate="A" pin="RB0/AN0/CN2" pad="19"/>
<connect gate="A" pin="RB1/AN1/CN3" pad="20"/>
<connect gate="A" pin="RB10/AN10" pad="14"/>
<connect gate="A" pin="RB11/AN11" pad="11"/>
<connect gate="A" pin="RB12/AN12" pad="10"/>
<connect gate="A" pin="RB2/AN2/CN4/SS1/LVDIN" pad="21"/>
<connect gate="A" pin="RB3/AN3/CN5" pad="22"/>
<connect gate="A" pin="RB4/AN4/CN6" pad="23"/>
<connect gate="A" pin="RB5/AN5/CN7" pad="24"/>
<connect gate="A" pin="RB6/AN6/EMUC/PGC/OCFA" pad="25"/>
<connect gate="A" pin="RB7/AN7/EMUD/PGD" pad="26"/>
<connect gate="A" pin="RB8/AN8" pad="27"/>
<connect gate="A" pin="RB9/AN9" pad="15"/>
<connect gate="A" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="32"/>
<connect gate="A" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="35"/>
<connect gate="A" pin="RD2" pad="41"/>
<connect gate="A" pin="RD3" pad="38"/>
<connect gate="A" pin="RF0" pad="5"/>
<connect gate="A" pin="RF1" pad="4"/>
<connect gate="A" pin="U1RX/SDI1/SDA/RF2" pad="1"/>
<connect gate="A" pin="U2RX/CN17/RF4" pad="3"/>
<connect gate="A" pin="U2TX/CN18/RF5" pad="2"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VDD@1" pad="28"/>
<connect gate="A" pin="VDD@2" pad="40"/>
<connect gate="A" pin="VSS" pad="6"/>
<connect gate="A" pin="VSS@1" pad="29"/>
<connect gate="A" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN44-8X8">
<connects>
<connect gate="A" pin="AVDD" pad="17"/>
<connect gate="A" pin="AVSS" pad="16"/>
<connect gate="A" pin="EMUC2/OC1/RD0" pad="10"/>
<connect gate="A" pin="EMUC3/SCK1/RF6" pad="43"/>
<connect gate="A" pin="EMUD2/OC2/RD1" pad="9"/>
<connect gate="A" pin="EMUD3/U1TX/SDO1/SCL/RF3" pad="44"/>
<connect gate="A" pin="INT1/IC1/RD8" pad="42"/>
<connect gate="A" pin="INT2/IC2/RD9" pad="37"/>
<connect gate="A" pin="MCLR" pad="18"/>
<connect gate="A" pin="OSC1/CLKIN" pad="32"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="33"/>
<connect gate="A" pin="RA11/INT0" pad="36"/>
<connect gate="A" pin="RB0/AN0/CN2" pad="19"/>
<connect gate="A" pin="RB1/AN1/CN3" pad="20"/>
<connect gate="A" pin="RB10/AN10" pad="14"/>
<connect gate="A" pin="RB11/AN11" pad="12"/>
<connect gate="A" pin="RB12/AN12" pad="11"/>
<connect gate="A" pin="RB2/AN2/CN4/SS1/LVDIN" pad="21"/>
<connect gate="A" pin="RB3/AN3/CN5" pad="22"/>
<connect gate="A" pin="RB4/AN4/CN6" pad="23"/>
<connect gate="A" pin="RB5/AN5/CN7" pad="24"/>
<connect gate="A" pin="RB6/AN6/EMUC/PGC/OCFA" pad="25"/>
<connect gate="A" pin="RB7/AN7/EMUD/PGD" pad="26"/>
<connect gate="A" pin="RB8/AN8" pad="27"/>
<connect gate="A" pin="RB9/AN9" pad="15"/>
<connect gate="A" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="34"/>
<connect gate="A" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="35"/>
<connect gate="A" pin="RD2" pad="41"/>
<connect gate="A" pin="RD3" pad="38"/>
<connect gate="A" pin="RF0" pad="5"/>
<connect gate="A" pin="RF1" pad="4"/>
<connect gate="A" pin="U1RX/SDI1/SDA/RF2" pad="1"/>
<connect gate="A" pin="U2RX/CN17/RF4" pad="3"/>
<connect gate="A" pin="U2TX/CN18/RF5" pad="2"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VDD@1" pad="28"/>
<connect gate="A" pin="VDD@2" pad="40"/>
<connect gate="A" pin="VSS" pad="6"/>
<connect gate="A" pin="VSS@1" pad="30"/>
<connect gate="A" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F4011" prefix="IC">
<description>&lt;b&gt;dsPIC Motion Controller DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F4011"/>
</gates>
<devices>
<device name="/P" package="DIL40">
<connects>
<connect gate="X" pin="AVDD" pad="40"/>
<connect gate="X" pin="AVSS" pad="39"/>
<connect gate="X" pin="C1RX/RF0" pad="30"/>
<connect gate="X" pin="C1TX/RF1" pad="29"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="28"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="27"/>
<connect gate="X" pin="FLTA/INT0/RE8" pad="17"/>
<connect gate="X" pin="OSC1/CLKI" pad="13"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="14"/>
<connect gate="X" pin="PGC/EMUC/SDI1/SDA/U1RX/RF2" pad="26"/>
<connect gate="X" pin="PGD/EMUD/SDO1/SCL/U1TX/RF3" pad="25"/>
<connect gate="X" pin="PWM1H/RE1" pad="37"/>
<connect gate="X" pin="PWM1L/RE0" pad="38"/>
<connect gate="X" pin="PWM2H/RE3" pad="35"/>
<connect gate="X" pin="PWM2L/RE2" pad="36"/>
<connect gate="X" pin="PWM3H/RE5" pad="33"/>
<connect gate="X" pin="PWM3L/RE4" pad="34"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7/QEA" pad="6"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8/QEB" pad="7"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="8"/>
<connect gate="X" pin="RB7/AN7" pad="9"/>
<connect gate="X" pin="RB8/AN8" pad="10"/>
<connect gate="X" pin="RC13/CN1/T2CK/U1ATX/SOSCI/EMUD1" pad="15"/>
<connect gate="X" pin="RC14/CN0/T1CK/U1ARX/SOSCO/EMUC1" pad="16"/>
<connect gate="X" pin="RD0/INT1/IC1/OC1/EMUC2" pad="23"/>
<connect gate="X" pin="RD1/INT2/IC2/OC2/EMUD2" pad="18"/>
<connect gate="X" pin="RD2/OC3" pad="22"/>
<connect gate="X" pin="RD3/OC4" pad="19"/>
<connect gate="X" pin="SCK1/RF6" pad="24"/>
<connect gate="X" pin="VDD" pad="11"/>
<connect gate="X" pin="VDD@1" pad="21"/>
<connect gate="X" pin="VDD@2" pad="32"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="12"/>
<connect gate="X" pin="VSS@1" pad="20"/>
<connect gate="X" pin="VSS@2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/PT" package="TQFP44">
<connects>
<connect gate="X" pin="AVDD" pad="17"/>
<connect gate="X" pin="AVSS" pad="16"/>
<connect gate="X" pin="C1RX/RF0" pad="5"/>
<connect gate="X" pin="C1TX/RF1" pad="4"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="3"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="2"/>
<connect gate="X" pin="FLTA/INT0/RE8" pad="36"/>
<connect gate="X" pin="OSC1/CLKI" pad="30"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="31"/>
<connect gate="X" pin="PGC/EMUC/SDI1/SDA/U1RX/RF2" pad="1"/>
<connect gate="X" pin="PGD/EMUD/SDO1/SCL/U1TX/RF3" pad="44"/>
<connect gate="X" pin="PWM1H/RE1" pad="14"/>
<connect gate="X" pin="PWM1L/RE0" pad="15"/>
<connect gate="X" pin="PWM2H/RE3" pad="10"/>
<connect gate="X" pin="PWM2L/RE2" pad="11"/>
<connect gate="X" pin="PWM3H/RE5" pad="8"/>
<connect gate="X" pin="PWM3L/RE4" pad="9"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="19"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="20"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1" pad="21"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="22"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7/QEA" pad="23"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8/QEB" pad="24"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="25"/>
<connect gate="X" pin="RB7/AN7" pad="26"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RC13/CN1/T2CK/U1ATX/SOSCI/EMUD1" pad="32"/>
<connect gate="X" pin="RC14/CN0/T1CK/U1ARX/SOSCO/EMUC1" pad="35"/>
<connect gate="X" pin="RD0/INT1/IC1/OC1/EMUC2" pad="42"/>
<connect gate="X" pin="RD1/INT2/IC2/OC2/EMUD2" pad="37"/>
<connect gate="X" pin="RD2/OC3" pad="41"/>
<connect gate="X" pin="RD3/OC4" pad="38"/>
<connect gate="X" pin="SCK1/RF6" pad="43"/>
<connect gate="X" pin="VDD" pad="7"/>
<connect gate="X" pin="VDD@1" pad="28"/>
<connect gate="X" pin="VDD@2" pad="40"/>
<connect gate="X" pin="VPP/MCLR" pad="18"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="29"/>
<connect gate="X" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN44-8X8">
<connects>
<connect gate="X" pin="AVDD" pad="17"/>
<connect gate="X" pin="AVSS" pad="16"/>
<connect gate="X" pin="C1RX/RF0" pad="5"/>
<connect gate="X" pin="C1TX/RF1" pad="4"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="3"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="2"/>
<connect gate="X" pin="FLTA/INT0/RE8" pad="36"/>
<connect gate="X" pin="OSC1/CLKI" pad="32"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="33"/>
<connect gate="X" pin="PGC/EMUC/SDI1/SDA/U1RX/RF2" pad="1"/>
<connect gate="X" pin="PGD/EMUD/SDO1/SCL/U1TX/RF3" pad="44"/>
<connect gate="X" pin="PWM1H/RE1" pad="14"/>
<connect gate="X" pin="PWM1L/RE0" pad="15"/>
<connect gate="X" pin="PWM2H/RE3" pad="11"/>
<connect gate="X" pin="PWM2L/RE2" pad="12"/>
<connect gate="X" pin="PWM3H/RE5" pad="9"/>
<connect gate="X" pin="PWM3L/RE4" pad="10"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="19"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="20"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1" pad="21"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="22"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7/QEA" pad="23"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8/QEB" pad="24"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="25"/>
<connect gate="X" pin="RB7/AN7" pad="26"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RC13/CN1/T2CK/U1ATX/SOSCI/EMUD1" pad="34"/>
<connect gate="X" pin="RC14/CN0/T1CK/U1ARX/SOSCO/EMUC1" pad="35"/>
<connect gate="X" pin="RD0/INT1/IC1/OC1/EMUC2" pad="42"/>
<connect gate="X" pin="RD1/INT2/IC2/OC2/EMUD2" pad="37"/>
<connect gate="X" pin="RD2/OC3" pad="41"/>
<connect gate="X" pin="RD3/OC4" pad="38"/>
<connect gate="X" pin="SCK1/RF6" pad="43"/>
<connect gate="X" pin="VDD" pad="7"/>
<connect gate="X" pin="VDD@1" pad="28"/>
<connect gate="X" pin="VDD@2" pad="40"/>
<connect gate="X" pin="VPP/MCLR" pad="18"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="30"/>
<connect gate="X" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F4013" prefix="IC">
<description>&lt;b&gt;dsPIC General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="DSPIC30F4013"/>
</gates>
<devices>
<device name="/P" package="DIL40">
<connects>
<connect gate="A" pin="AVDD" pad="40"/>
<connect gate="A" pin="AVSS" pad="39"/>
<connect gate="A" pin="C1RX/RF0" pad="30"/>
<connect gate="A" pin="C1TX/RF1" pad="29"/>
<connect gate="A" pin="EMUC2/OC1/RD0" pad="34"/>
<connect gate="A" pin="EMUC3/SCK1/RF6" pad="24"/>
<connect gate="A" pin="EMUD2/OC2/RD1" pad="33"/>
<connect gate="A" pin="EMUD3/U1TX/SDO1/SCL/RF3" pad="25"/>
<connect gate="A" pin="INT1/IC1/RD8" pad="23"/>
<connect gate="A" pin="INT2/IC2/RD9" pad="18"/>
<connect gate="A" pin="MCLR" pad="1"/>
<connect gate="A" pin="OC3/RD2" pad="22"/>
<connect gate="A" pin="OC4/RD3" pad="19"/>
<connect gate="A" pin="OSC1/CLKIN" pad="13"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="14"/>
<connect gate="A" pin="RA11/INT0" pad="17"/>
<connect gate="A" pin="RB0/AN0/CN2" pad="2"/>
<connect gate="A" pin="RB1/AN1/CN3" pad="3"/>
<connect gate="A" pin="RB10/AN10/CSDI" pad="37"/>
<connect gate="A" pin="RB11/AN11/CSDO" pad="36"/>
<connect gate="A" pin="RB12/AN12/COFS" pad="35"/>
<connect gate="A" pin="RB2/AN2/CN4/SS1/LVDIN" pad="4"/>
<connect gate="A" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="A" pin="RB4/AN4/CN6/IC7" pad="6"/>
<connect gate="A" pin="RB5/AN5/CN7/IC8" pad="7"/>
<connect gate="A" pin="RB6/AN6/EMUC/PGC/OCFA" pad="8"/>
<connect gate="A" pin="RB7/AN7/EMUD/PGD" pad="9"/>
<connect gate="A" pin="RB8/AN8" pad="10"/>
<connect gate="A" pin="RB9/AN9/CSCK" pad="38"/>
<connect gate="A" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="15"/>
<connect gate="A" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="16"/>
<connect gate="A" pin="U1RX/SDI1/SDA/RF2" pad="26"/>
<connect gate="A" pin="U2RX/CN17/RF4" pad="28"/>
<connect gate="A" pin="U2TX/CN18/RF5" pad="27"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VDD@1" pad="21"/>
<connect gate="A" pin="VDD@2" pad="32"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="VSS@1" pad="20"/>
<connect gate="A" pin="VSS@2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/PT" package="TQFP44">
<connects>
<connect gate="A" pin="AVDD" pad="17"/>
<connect gate="A" pin="AVSS" pad="16"/>
<connect gate="A" pin="C1RX/RF0" pad="5"/>
<connect gate="A" pin="C1TX/RF1" pad="4"/>
<connect gate="A" pin="EMUC2/OC1/RD0" pad="9"/>
<connect gate="A" pin="EMUC3/SCK1/RF6" pad="43"/>
<connect gate="A" pin="EMUD2/OC2/RD1" pad="8"/>
<connect gate="A" pin="EMUD3/U1TX/SDO1/SCL/RF3" pad="44"/>
<connect gate="A" pin="INT1/IC1/RD8" pad="42"/>
<connect gate="A" pin="INT2/IC2/RD9" pad="37"/>
<connect gate="A" pin="MCLR" pad="18"/>
<connect gate="A" pin="OC3/RD2" pad="41"/>
<connect gate="A" pin="OC4/RD3" pad="38"/>
<connect gate="A" pin="OSC1/CLKIN" pad="30"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="31"/>
<connect gate="A" pin="RA11/INT0" pad="36"/>
<connect gate="A" pin="RB0/AN0/CN2" pad="19"/>
<connect gate="A" pin="RB1/AN1/CN3" pad="20"/>
<connect gate="A" pin="RB10/AN10/CSDI" pad="14"/>
<connect gate="A" pin="RB11/AN11/CSDO" pad="11"/>
<connect gate="A" pin="RB12/AN12/COFS" pad="10"/>
<connect gate="A" pin="RB2/AN2/CN4/SS1/LVDIN" pad="21"/>
<connect gate="A" pin="RB3/AN3/CN5" pad="22"/>
<connect gate="A" pin="RB4/AN4/CN6/IC7" pad="23"/>
<connect gate="A" pin="RB5/AN5/CN7/IC8" pad="24"/>
<connect gate="A" pin="RB6/AN6/EMUC/PGC/OCFA" pad="25"/>
<connect gate="A" pin="RB7/AN7/EMUD/PGD" pad="26"/>
<connect gate="A" pin="RB8/AN8" pad="27"/>
<connect gate="A" pin="RB9/AN9/CSCK" pad="15"/>
<connect gate="A" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="32"/>
<connect gate="A" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="35"/>
<connect gate="A" pin="U1RX/SDI1/SDA/RF2" pad="1"/>
<connect gate="A" pin="U2RX/CN17/RF4" pad="3"/>
<connect gate="A" pin="U2TX/CN18/RF5" pad="2"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VDD@1" pad="28"/>
<connect gate="A" pin="VDD@2" pad="40"/>
<connect gate="A" pin="VSS" pad="6"/>
<connect gate="A" pin="VSS@1" pad="29"/>
<connect gate="A" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN44-8X8">
<connects>
<connect gate="A" pin="AVDD" pad="17"/>
<connect gate="A" pin="AVSS" pad="16"/>
<connect gate="A" pin="C1RX/RF0" pad="5"/>
<connect gate="A" pin="C1TX/RF1" pad="4"/>
<connect gate="A" pin="EMUC2/OC1/RD0" pad="10"/>
<connect gate="A" pin="EMUC3/SCK1/RF6" pad="43"/>
<connect gate="A" pin="EMUD2/OC2/RD1" pad="9"/>
<connect gate="A" pin="EMUD3/U1TX/SDO1/SCL/RF3" pad="44"/>
<connect gate="A" pin="INT1/IC1/RD8" pad="42"/>
<connect gate="A" pin="INT2/IC2/RD9" pad="37"/>
<connect gate="A" pin="MCLR" pad="18"/>
<connect gate="A" pin="OC3/RD2" pad="41"/>
<connect gate="A" pin="OC4/RD3" pad="38"/>
<connect gate="A" pin="OSC1/CLKIN" pad="32"/>
<connect gate="A" pin="OSC2/CLKO/RC15" pad="33"/>
<connect gate="A" pin="RA11/INT0" pad="36"/>
<connect gate="A" pin="RB0/AN0/CN2" pad="19"/>
<connect gate="A" pin="RB1/AN1/CN3" pad="20"/>
<connect gate="A" pin="RB10/AN10/CSDI" pad="14"/>
<connect gate="A" pin="RB11/AN11/CSDO" pad="12"/>
<connect gate="A" pin="RB12/AN12/COFS" pad="11"/>
<connect gate="A" pin="RB2/AN2/CN4/SS1/LVDIN" pad="21"/>
<connect gate="A" pin="RB3/AN3/CN5" pad="22"/>
<connect gate="A" pin="RB4/AN4/CN6/IC7" pad="23"/>
<connect gate="A" pin="RB5/AN5/CN7/IC8" pad="24"/>
<connect gate="A" pin="RB6/AN6/EMUC/PGC/OCFA" pad="25"/>
<connect gate="A" pin="RB7/AN7/EMUD/PGD" pad="26"/>
<connect gate="A" pin="RB8/AN8" pad="27"/>
<connect gate="A" pin="RB9/AN9/CSCK" pad="15"/>
<connect gate="A" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="34"/>
<connect gate="A" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="35"/>
<connect gate="A" pin="U1RX/SDI1/SDA/RF2" pad="1"/>
<connect gate="A" pin="U2RX/CN17/RF4" pad="3"/>
<connect gate="A" pin="U2TX/CN18/RF5" pad="2"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VDD@1" pad="28"/>
<connect gate="A" pin="VDD@2" pad="40"/>
<connect gate="A" pin="VSS" pad="6"/>
<connect gate="A" pin="VSS@1" pad="30"/>
<connect gate="A" pin="VSS@2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F5011" prefix="IC">
<description>&lt;b&gt;dsPIC General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F5011"/>
</gates>
<devices>
<device name="/PTG" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="C2RX/RG0" pad="61"/>
<connect gate="X" pin="C2TX/RG1" pad="60"/>
<connect gate="X" pin="CLKI/OSC1" pad="39"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="EMUD3/SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="INT0/EMUC3/SCK1/RF6" pad="35"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-" pad="15"/>
<connect gate="X" pin="RB10/AN10" pad="23"/>
<connect gate="X" pin="RB11/AN11" pad="24"/>
<connect gate="X" pin="RB12/AN12" pad="27"/>
<connect gate="X" pin="RB13/AN13" pad="28"/>
<connect gate="X" pin="RB14/AN14" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC/PGC" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD/PGD" pad="18"/>
<connect gate="X" pin="RB8/AN8" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1/EMUC2" pad="46"/>
<connect gate="X" pin="RD1/OC2/EMUD2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2" pad="43"/>
<connect gate="X" pin="SCL/RG2" pad="37"/>
<connect gate="X" pin="SDA/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SOSCI/T4CK/EMUD1/CN1/RC13" pad="47"/>
<connect gate="X" pin="SOSCO/T1CK/EMUC1/CN0/RC14" pad="48"/>
<connect gate="X" pin="T2CK/RC1" pad="2"/>
<connect gate="X" pin="T3CK/RC2" pad="3"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VPP/MCLR" pad="7"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
<connect gate="X" pin="VSS@3" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F5013" prefix="IC">
<description>&lt;b&gt;dsPIC General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F5013"/>
</gates>
<devices>
<device name="/PT" package="TQFP80_12X12">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="26"/>
<connect gate="X" pin="C1RX/RF0" pad="72"/>
<connect gate="X" pin="C1TX/RF1" pad="73"/>
<connect gate="X" pin="C2RX/RG0" pad="75"/>
<connect gate="X" pin="C2TX/RG1" pad="74"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="8"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="10"/>
<connect gate="X" pin="CN13/OC5/RD4" pad="66"/>
<connect gate="X" pin="CN14/OC6/RD5" pad="67"/>
<connect gate="X" pin="CN15/OC7/RD6" pad="68"/>
<connect gate="X" pin="CN16/OC8/RD7" pad="69"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="39"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="40"/>
<connect gate="X" pin="CN19/IC6/RD13" pad="65"/>
<connect gate="X" pin="CN20/IC7/RD14" pad="37"/>
<connect gate="X" pin="CN21/IC8/RD15" pad="38"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="6"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="7"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="78"/>
<connect gate="X" pin="CSDI/RG12" pad="79"/>
<connect gate="X" pin="CSDO/RG13" pad="80"/>
<connect gate="X" pin="EMUC2/OC1/RD0" pad="58"/>
<connect gate="X" pin="EMUC3/SCK1/INT0/RF6" pad="45"/>
<connect gate="X" pin="EMUD2/OC2/RD1" pad="61"/>
<connect gate="X" pin="EMUD3/SDO1/RF8" pad="43"/>
<connect gate="X" pin="IC1/RD8" pad="54"/>
<connect gate="X" pin="IC2/RD9" pad="55"/>
<connect gate="X" pin="IC3/RD10" pad="56"/>
<connect gate="X" pin="IC4/RD11" pad="57"/>
<connect gate="X" pin="IC5/RD12" pad="64"/>
<connect gate="X" pin="MCLR/VPP" pad="9"/>
<connect gate="X" pin="OC3/RD2" pad="62"/>
<connect gate="X" pin="OC4/RD3" pad="63"/>
<connect gate="X" pin="OSC1/CLKI" pad="49"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="X" pin="RA10/VR+" pad="24"/>
<connect gate="X" pin="RA12/INT1" pad="13"/>
<connect gate="X" pin="RA13/INT2" pad="14"/>
<connect gate="X" pin="RA14/INT3" pad="52"/>
<connect gate="X" pin="RA15/INT4" pad="53"/>
<connect gate="X" pin="RA6/CN22" pad="76"/>
<connect gate="X" pin="RA7/CN23" pad="77"/>
<connect gate="X" pin="RA9/VR-" pad="23"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD/PGD" pad="20"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC/PGC" pad="19"/>
<connect gate="X" pin="RB10/AN10" pad="29"/>
<connect gate="X" pin="RB11/AN11" pad="30"/>
<connect gate="X" pin="RB12/AN12" pad="33"/>
<connect gate="X" pin="RB13/AN13" pad="34"/>
<connect gate="X" pin="RB14/AN14" pad="35"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="36"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="18"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="17"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="16"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="15"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="21"/>
<connect gate="X" pin="RB7/AN7" pad="22"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RB9/AN9" pad="28"/>
<connect gate="X" pin="RC1/T2CK" pad="2"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI" pad="59"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK" pad="60"/>
<connect gate="X" pin="RC2/T3CK" pad="3"/>
<connect gate="X" pin="RC3/T4CK" pad="4"/>
<connect gate="X" pin="RC4/T5CK" pad="5"/>
<connect gate="X" pin="SCL/RG2" pad="47"/>
<connect gate="X" pin="SDA/RG3" pad="46"/>
<connect gate="X" pin="SDI1/RF7" pad="44"/>
<connect gate="X" pin="U1RX/RF2" pad="42"/>
<connect gate="X" pin="U1TX/RF3" pad="41"/>
<connect gate="X" pin="VDD" pad="12"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VDD@2" pad="48"/>
<connect gate="X" pin="VDD@3" pad="71"/>
<connect gate="X" pin="VSS" pad="11"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VSS@2" pad="51"/>
<connect gate="X" pin="VSS@3" pad="70"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F5015">
<description>&lt;b&gt;dsPIC Motion Controller DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F5015"/>
</gates>
<devices>
<device name="/PF" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN15/RD6" pad="54"/>
<connect gate="X" pin="EMUC2/OC1/RD0" pad="46"/>
<connect gate="X" pin="EMUD2/OC2/RD1" pad="49"/>
<connect gate="X" pin="FLTA/IC1/INT1/RD8" pad="42"/>
<connect gate="X" pin="FLTB/IC2/INT2/RD9" pad="43"/>
<connect gate="X" pin="IC3/INT3/RD10" pad="44"/>
<connect gate="X" pin="IC4/INT4/RD11" pad="45"/>
<connect gate="X" pin="IC5/CN13/RD4" pad="52"/>
<connect gate="X" pin="IC6/CN14/RD5" pad="53"/>
<connect gate="X" pin="OC3/RD2" pad="50"/>
<connect gate="X" pin="OC4/RD3" pad="51"/>
<connect gate="X" pin="OSC1/CLKI" pad="39"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="40"/>
<connect gate="X" pin="PWM1H/RE1" pad="61"/>
<connect gate="X" pin="PWM1L/RE0" pad="60"/>
<connect gate="X" pin="PWM2H/RE3" pad="63"/>
<connect gate="X" pin="PWM2L/RE2" pad="62"/>
<connect gate="X" pin="PWM3H/RE5" pad="1"/>
<connect gate="X" pin="PWM3L/RE4" pad="64"/>
<connect gate="X" pin="PWM4H/RE7" pad="3"/>
<connect gate="X" pin="PWM4L/RE6" pad="2"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-" pad="15"/>
<connect gate="X" pin="RB10/AN10" pad="23"/>
<connect gate="X" pin="RB11/AN11" pad="24"/>
<connect gate="X" pin="RB12/AN12" pad="27"/>
<connect gate="X" pin="RB13/AN13" pad="28"/>
<connect gate="X" pin="RB14/AN14" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/QEA" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/QEB" pad="11"/>
<connect gate="X" pin="RB6/AN6/EMUC/OCFA/PGC" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD/PGD" pad="18"/>
<connect gate="X" pin="RB8/AN8" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI/T4CK" pad="47"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK" pad="48"/>
<connect gate="X" pin="RF0/C1RX" pad="58"/>
<connect gate="X" pin="RF1/C1TX" pad="59"/>
<connect gate="X" pin="RF2/U1RX/SDI1" pad="34"/>
<connect gate="X" pin="RF3/U1TX/SDO1/EMUD3" pad="33"/>
<connect gate="X" pin="RF4/CN17" pad="31"/>
<connect gate="X" pin="RF5/CN18" pad="32"/>
<connect gate="X" pin="RF6/INT0/SCK1/EMUC3" pad="35"/>
<connect gate="X" pin="SCK2/CN8/RG6" pad="4"/>
<connect gate="X" pin="SCL/RG2" pad="37"/>
<connect gate="X" pin="SDA/RG3" pad="36"/>
<connect gate="X" pin="SDI2/CN9/RG7" pad="5"/>
<connect gate="X" pin="SDO2/CN10/RG8" pad="6"/>
<connect gate="X" pin="SS2/CN11/RG9" pad="8"/>
<connect gate="X" pin="UPDN/CN16/RD7" pad="55"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VPP/MCLR" pad="7"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
<connect gate="X" pin="VSS@3" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F5016" prefix="IC">
<description>&lt;b&gt;dsPIC Motion Controller DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F5016"/>
</gates>
<devices>
<device name="/PF" package="TQFP80_12X12">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="26"/>
<connect gate="X" pin="C1RX/RF0" pad="72"/>
<connect gate="X" pin="C1TX/RF1" pad="73"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="8"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="10"/>
<connect gate="X" pin="CN13/RD4" pad="66"/>
<connect gate="X" pin="CN14/RD5" pad="67"/>
<connect gate="X" pin="CN15/RD6" pad="68"/>
<connect gate="X" pin="CN17/RF4" pad="39"/>
<connect gate="X" pin="CN18/RF5" pad="40"/>
<connect gate="X" pin="CN19/RD13" pad="65"/>
<connect gate="X" pin="CN20/RD14" pad="37"/>
<connect gate="X" pin="CN21/RD15" pad="38"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="6"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="7"/>
<connect gate="X" pin="EMUC2/OC1/RD0" pad="58"/>
<connect gate="X" pin="EMUC3/SCK1/INT0/RF6" pad="45"/>
<connect gate="X" pin="EMUD2/OC2/RD1" pad="61"/>
<connect gate="X" pin="EMUD3/SDO1/RF8" pad="43"/>
<connect gate="X" pin="IC1/RD8" pad="54"/>
<connect gate="X" pin="IC2/RD9" pad="55"/>
<connect gate="X" pin="IC3/RD10" pad="56"/>
<connect gate="X" pin="IC4/RD11" pad="57"/>
<connect gate="X" pin="OC3/RD2" pad="62"/>
<connect gate="X" pin="OC4/RD3" pad="63"/>
<connect gate="X" pin="OSC1/CLKI" pad="49"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="X" pin="RA10/VR+" pad="24"/>
<connect gate="X" pin="RA14/INT3" pad="52"/>
<connect gate="X" pin="RA15/INT4" pad="53"/>
<connect gate="X" pin="RA9/VR-" pad="23"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD/PGD" pad="20"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC/PGC" pad="19"/>
<connect gate="X" pin="RB10/AN10" pad="29"/>
<connect gate="X" pin="RB11/AN11" pad="30"/>
<connect gate="X" pin="RB12/AN12" pad="33"/>
<connect gate="X" pin="RB13/AN13" pad="34"/>
<connect gate="X" pin="RB14/AN14" pad="35"/>
<connect gate="X" pin="RB15/AN15/CN12" pad="36"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1" pad="18"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="17"/>
<connect gate="X" pin="RB4/AN4/CN6/QEA" pad="16"/>
<connect gate="X" pin="RB5/AN5/CN7/QEB" pad="15"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="21"/>
<connect gate="X" pin="RB7/AN7" pad="22"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RB9/AN9" pad="28"/>
<connect gate="X" pin="RC1/T2CK" pad="4"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI" pad="59"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK" pad="60"/>
<connect gate="X" pin="RC3/T4CK" pad="5"/>
<connect gate="X" pin="RD12" pad="64"/>
<connect gate="X" pin="RE0/PWM1L" pad="76"/>
<connect gate="X" pin="RE1/PWM1H" pad="77"/>
<connect gate="X" pin="RE2/PWM2L" pad="78"/>
<connect gate="X" pin="RE3/PWM2H" pad="79"/>
<connect gate="X" pin="RE4/PWM3L" pad="80"/>
<connect gate="X" pin="RE5/PWM3H" pad="1"/>
<connect gate="X" pin="RE6/PWM4L" pad="2"/>
<connect gate="X" pin="RE7/PWM4H" pad="3"/>
<connect gate="X" pin="RE8/INT1/FLTA" pad="13"/>
<connect gate="X" pin="RE9/INT2/FLTB" pad="14"/>
<connect gate="X" pin="RG0" pad="75"/>
<connect gate="X" pin="RG1" pad="74"/>
<connect gate="X" pin="SCL/RG2" pad="47"/>
<connect gate="X" pin="SDA/RG3" pad="46"/>
<connect gate="X" pin="SDI1/RF7" pad="44"/>
<connect gate="X" pin="U1RX/RF2" pad="42"/>
<connect gate="X" pin="U1TX/RF3" pad="41"/>
<connect gate="X" pin="UPDN/CN16/RD7" pad="69"/>
<connect gate="X" pin="VDD" pad="12"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VDD@2" pad="48"/>
<connect gate="X" pin="VDD@3" pad="71"/>
<connect gate="X" pin="VPP/MCLR" pad="9"/>
<connect gate="X" pin="VSS" pad="11"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VSS@2" pad="51"/>
<connect gate="X" pin="VSS@3" pad="70"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F6010" prefix="IC">
<description>&lt;b&gt;dsPIC Motion Controller DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F6010"/>
</gates>
<devices>
<device name="/PF" package="TQFP80_917">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="26"/>
<connect gate="X" pin="C1RX/RF0" pad="72"/>
<connect gate="X" pin="C1TX/RF1" pad="73"/>
<connect gate="X" pin="C2RX/RG0" pad="75"/>
<connect gate="X" pin="C2TX/RG1" pad="74"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="8"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="10"/>
<connect gate="X" pin="CN13/OC5/RD4" pad="66"/>
<connect gate="X" pin="CN14/OC6/RD5" pad="67"/>
<connect gate="X" pin="CN15/OC7/RD6" pad="68"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="39"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="40"/>
<connect gate="X" pin="CN19/IC6/RD13" pad="65"/>
<connect gate="X" pin="CN20/IC7/RD14" pad="37"/>
<connect gate="X" pin="CN21/IC8/RD15" pad="38"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="6"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="7"/>
<connect gate="X" pin="EMUC2/OC1/RD0" pad="58"/>
<connect gate="X" pin="EMUC3/SCK1/INT0/RF6" pad="45"/>
<connect gate="X" pin="EMUD2/OC2/RD1" pad="61"/>
<connect gate="X" pin="EMUD3/SDO1/RF8" pad="43"/>
<connect gate="X" pin="IC1/RD8" pad="54"/>
<connect gate="X" pin="IC2/RD9" pad="55"/>
<connect gate="X" pin="IC3/RD10" pad="56"/>
<connect gate="X" pin="IC4/RD11" pad="57"/>
<connect gate="X" pin="IC5/RD12" pad="64"/>
<connect gate="X" pin="OC3/RD2" pad="62"/>
<connect gate="X" pin="OC4/RD3" pad="63"/>
<connect gate="X" pin="OSC1/CLKI" pad="49"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="X" pin="RA10/VR+" pad="24"/>
<connect gate="X" pin="RA14/INT3" pad="52"/>
<connect gate="X" pin="RA15/INT4" pad="53"/>
<connect gate="X" pin="RA9/VR-" pad="23"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD/PGD" pad="20"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC/PGC" pad="19"/>
<connect gate="X" pin="RB10/AN10" pad="29"/>
<connect gate="X" pin="RB11/AN11" pad="30"/>
<connect gate="X" pin="RB12/AN12" pad="33"/>
<connect gate="X" pin="RB13/AN13" pad="34"/>
<connect gate="X" pin="RB14/AN14" pad="35"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="36"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="18"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="17"/>
<connect gate="X" pin="RB4/AN4/CN6/QEA" pad="16"/>
<connect gate="X" pin="RB5/AN5/CN7/QEB" pad="15"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="21"/>
<connect gate="X" pin="RB7/AN7" pad="22"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RB9/AN9" pad="28"/>
<connect gate="X" pin="RC1/T2CK" pad="4"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI" pad="59"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK" pad="60"/>
<connect gate="X" pin="RC3/T4CK" pad="5"/>
<connect gate="X" pin="RE0/PWM1L" pad="76"/>
<connect gate="X" pin="RE1/PWM1H" pad="77"/>
<connect gate="X" pin="RE2/PWM2L" pad="78"/>
<connect gate="X" pin="RE3/PWM2H" pad="79"/>
<connect gate="X" pin="RE4/PWM3L" pad="80"/>
<connect gate="X" pin="RE5/PWM3H" pad="1"/>
<connect gate="X" pin="RE6/PWM4L" pad="2"/>
<connect gate="X" pin="RE7/PWM4H" pad="3"/>
<connect gate="X" pin="RE8/INT1/FLTA" pad="13"/>
<connect gate="X" pin="RE9/INT2/FLTB" pad="14"/>
<connect gate="X" pin="SCL/RG2" pad="47"/>
<connect gate="X" pin="SDA/RG3" pad="46"/>
<connect gate="X" pin="SDI1/RF7" pad="44"/>
<connect gate="X" pin="U1RX/RF2" pad="42"/>
<connect gate="X" pin="U1TX/RF3" pad="41"/>
<connect gate="X" pin="UPDN/CN16/OC8/RD7" pad="69"/>
<connect gate="X" pin="VDD" pad="12"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VDD@2" pad="48"/>
<connect gate="X" pin="VDD@3" pad="71"/>
<connect gate="X" pin="VPP/MCLR" pad="9"/>
<connect gate="X" pin="VSS" pad="11"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VSS@2" pad="51"/>
<connect gate="X" pin="VSS@3" pad="70"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F6011" prefix="IC">
<description>&lt;b&gt;dsPIC General DSC with CAN port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F6011"/>
</gates>
<devices>
<device name="/PF" package="TQFP64">
<connects>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="C2RX/RG0" pad="61"/>
<connect gate="X" pin="C2TX/RG1" pad="60"/>
<connect gate="X" pin="CLKI/OSC1" pad="39"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="EMUD3/SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="INT0/EMUC3/SCK1/RF6" pad="35"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD/PGD" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC/PGC" pad="15"/>
<connect gate="X" pin="RB10/AN10" pad="23"/>
<connect gate="X" pin="RB11/AN11" pad="24"/>
<connect gate="X" pin="RB12/AN12" pad="27"/>
<connect gate="X" pin="RB13/AN13" pad="28"/>
<connect gate="X" pin="RB14/AN14" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="17"/>
<connect gate="X" pin="RB7/AN7" pad="18"/>
<connect gate="X" pin="RB8/AN8" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1/EMUC2" pad="46"/>
<connect gate="X" pin="RD1/OC2/EMUD2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2" pad="43"/>
<connect gate="X" pin="RG12" pad="63"/>
<connect gate="X" pin="RG13" pad="64"/>
<connect gate="X" pin="RG14" pad="62"/>
<connect gate="X" pin="RG15" pad="1"/>
<connect gate="X" pin="SCL/RG2" pad="37"/>
<connect gate="X" pin="SDA/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SOSCI/T4CK/EMUD1/CN1/RC13" pad="47"/>
<connect gate="X" pin="SOSCO/T1CK/EMUC1/CN0/RC14" pad="48"/>
<connect gate="X" pin="T2CK/RC1" pad="2"/>
<connect gate="X" pin="T3CK/RC2" pad="3"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VPP/MCLR" pad="7"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
<connect gate="X" pin="VSS@3" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F6012" prefix="IC">
<description>&lt;b&gt;dsPIC General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F6012"/>
</gates>
<devices>
<device name="/PF" package="TQFP64">
<connects>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="C2RX/RG0" pad="61"/>
<connect gate="X" pin="C2TX/RG1" pad="60"/>
<connect gate="X" pin="CLKI/OSC1" pad="39"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="EMUD3/SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="INT0/EMUC3/SCK1/RF6" pad="35"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD/PGD" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC/PGC" pad="15"/>
<connect gate="X" pin="RB10/AN10" pad="23"/>
<connect gate="X" pin="RB11/AN11" pad="24"/>
<connect gate="X" pin="RB12/AN12" pad="27"/>
<connect gate="X" pin="RB13/AN13" pad="28"/>
<connect gate="X" pin="RB14/AN14" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="17"/>
<connect gate="X" pin="RB7/AN7" pad="18"/>
<connect gate="X" pin="RB8/AN8" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1/EMUC2" pad="46"/>
<connect gate="X" pin="RD1/OC2/EMUD2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2" pad="43"/>
<connect gate="X" pin="SCL/RG2" pad="37"/>
<connect gate="X" pin="SDA/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SOSCI/T4CK/EMUD1/CN1/RC13" pad="47"/>
<connect gate="X" pin="SOSCO/T1CK/EMUC1/CN0/RC14" pad="48"/>
<connect gate="X" pin="T2CK/RC1" pad="2"/>
<connect gate="X" pin="T3CK/RC2" pad="3"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VPP/MCLR" pad="7"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
<connect gate="X" pin="VSS@3" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F6013" prefix="IC">
<description>&lt;b&gt;dsPIC General DSC with CAN port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F6013"/>
</gates>
<devices>
<device name="/PF" package="TQFP80_917">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="26"/>
<connect gate="X" pin="C1RX/RF0" pad="72"/>
<connect gate="X" pin="C1TX/RF1" pad="73"/>
<connect gate="X" pin="C2RX/RG0" pad="75"/>
<connect gate="X" pin="C2TX/RG1" pad="74"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="8"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="10"/>
<connect gate="X" pin="CN13/OC5/RD4" pad="66"/>
<connect gate="X" pin="CN14/OC6/RD5" pad="67"/>
<connect gate="X" pin="CN15/OC7/RD6" pad="68"/>
<connect gate="X" pin="CN16/OC8/RD7" pad="69"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="39"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="40"/>
<connect gate="X" pin="CN19/IC6/RD13" pad="65"/>
<connect gate="X" pin="CN20/IC7/RD14" pad="37"/>
<connect gate="X" pin="CN21/IC8/RD15" pad="38"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="6"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="7"/>
<connect gate="X" pin="EMUC2/OC1/RD0" pad="58"/>
<connect gate="X" pin="EMUC3/SCK1/INT0/RF6" pad="45"/>
<connect gate="X" pin="EMUD2/OC2/RD1" pad="61"/>
<connect gate="X" pin="EMUD3/SDO1/RF8" pad="43"/>
<connect gate="X" pin="IC1/RD8" pad="54"/>
<connect gate="X" pin="IC2/RD9" pad="55"/>
<connect gate="X" pin="IC3/RD10" pad="56"/>
<connect gate="X" pin="IC4/RD11" pad="57"/>
<connect gate="X" pin="IC5/RD12" pad="64"/>
<connect gate="X" pin="MCLR/VPP" pad="9"/>
<connect gate="X" pin="OC3/RD2" pad="62"/>
<connect gate="X" pin="OC4/RD3" pad="63"/>
<connect gate="X" pin="OSC1/CLKI" pad="49"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="X" pin="RA10/VR+" pad="24"/>
<connect gate="X" pin="RA12/INT1" pad="13"/>
<connect gate="X" pin="RA13/INT2" pad="14"/>
<connect gate="X" pin="RA14/INT3" pad="52"/>
<connect gate="X" pin="RA15/INT4" pad="53"/>
<connect gate="X" pin="RA6/CN22" pad="76"/>
<connect gate="X" pin="RA7/CN23" pad="77"/>
<connect gate="X" pin="RA9/VR-" pad="23"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD/PGD" pad="20"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC/PGC" pad="19"/>
<connect gate="X" pin="RB10/AN10" pad="29"/>
<connect gate="X" pin="RB11/AN11" pad="30"/>
<connect gate="X" pin="RB12/AN12" pad="33"/>
<connect gate="X" pin="RB13/AN13" pad="34"/>
<connect gate="X" pin="RB14/AN14" pad="35"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="36"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="18"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="17"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="16"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="15"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="21"/>
<connect gate="X" pin="RB7/AN7" pad="22"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RB9/AN9" pad="28"/>
<connect gate="X" pin="RC1/T2CK" pad="2"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI" pad="59"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK" pad="60"/>
<connect gate="X" pin="RC2/T3CK" pad="3"/>
<connect gate="X" pin="RC3/T4CK" pad="4"/>
<connect gate="X" pin="RC4/T5CK" pad="5"/>
<connect gate="X" pin="RG12" pad="79"/>
<connect gate="X" pin="RG13" pad="80"/>
<connect gate="X" pin="RG14" pad="78"/>
<connect gate="X" pin="RG15" pad="1"/>
<connect gate="X" pin="SCL/RG2" pad="47"/>
<connect gate="X" pin="SDA/RG3" pad="46"/>
<connect gate="X" pin="SDI1/RF7" pad="44"/>
<connect gate="X" pin="U1RX/RF2" pad="42"/>
<connect gate="X" pin="U1TX/RF3" pad="41"/>
<connect gate="X" pin="VDD" pad="12"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VDD@2" pad="48"/>
<connect gate="X" pin="VDD@3" pad="71"/>
<connect gate="X" pin="VSS" pad="11"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VSS@2" pad="51"/>
<connect gate="X" pin="VSS@3" pad="70"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F6014" prefix="IC">
<description>&lt;b&gt;dsPIC General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F6014"/>
</gates>
<devices>
<device name="/PF" package="TQFP80_917">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="26"/>
<connect gate="X" pin="C1RX/RF0" pad="72"/>
<connect gate="X" pin="C1TX/RF1" pad="73"/>
<connect gate="X" pin="C2RX/RG0" pad="75"/>
<connect gate="X" pin="C2TX/RG1" pad="74"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="8"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="10"/>
<connect gate="X" pin="CN13/OC5/RD4" pad="66"/>
<connect gate="X" pin="CN14/OC6/RD5" pad="67"/>
<connect gate="X" pin="CN15/OC7/RD6" pad="68"/>
<connect gate="X" pin="CN16/OC8/RD7" pad="69"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="39"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="40"/>
<connect gate="X" pin="CN19/IC6/RD13" pad="65"/>
<connect gate="X" pin="CN20/IC7/RD14" pad="37"/>
<connect gate="X" pin="CN21/IC8/RD15" pad="38"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="6"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="7"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="78"/>
<connect gate="X" pin="CSDI/RG12" pad="79"/>
<connect gate="X" pin="CSDO/RG13" pad="80"/>
<connect gate="X" pin="EMUC2/OC1/RD0" pad="58"/>
<connect gate="X" pin="EMUC3/SCK1/INT0/RF6" pad="45"/>
<connect gate="X" pin="EMUD2/OC2/RD1" pad="61"/>
<connect gate="X" pin="EMUD3/SDO1/RF8" pad="43"/>
<connect gate="X" pin="IC1/RD8" pad="54"/>
<connect gate="X" pin="IC2/RD9" pad="55"/>
<connect gate="X" pin="IC3/RD10" pad="56"/>
<connect gate="X" pin="IC4/RD11" pad="57"/>
<connect gate="X" pin="IC5/RD12" pad="64"/>
<connect gate="X" pin="MCLR/VPP" pad="9"/>
<connect gate="X" pin="OC3/RD2" pad="62"/>
<connect gate="X" pin="OC4/RD3" pad="63"/>
<connect gate="X" pin="OSC1/CLKI" pad="49"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="X" pin="RA10/VR+" pad="24"/>
<connect gate="X" pin="RA12/INT1" pad="13"/>
<connect gate="X" pin="RA13/INT2" pad="14"/>
<connect gate="X" pin="RA14/INT3" pad="52"/>
<connect gate="X" pin="RA15/INT4" pad="53"/>
<connect gate="X" pin="RA6/CN22" pad="76"/>
<connect gate="X" pin="RA7/CN23" pad="77"/>
<connect gate="X" pin="RA9/VR-" pad="23"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD/PGD" pad="20"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC/PGC" pad="19"/>
<connect gate="X" pin="RB10/AN10" pad="29"/>
<connect gate="X" pin="RB11/AN11" pad="30"/>
<connect gate="X" pin="RB12/AN12" pad="33"/>
<connect gate="X" pin="RB13/AN13" pad="34"/>
<connect gate="X" pin="RB14/AN14" pad="35"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="36"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="18"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="17"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="16"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="15"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="21"/>
<connect gate="X" pin="RB7/AN7" pad="22"/>
<connect gate="X" pin="RB8/AN8" pad="27"/>
<connect gate="X" pin="RB9/AN9" pad="28"/>
<connect gate="X" pin="RC1/T2CK" pad="2"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI" pad="59"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK" pad="60"/>
<connect gate="X" pin="RC2/T3CK" pad="3"/>
<connect gate="X" pin="RC3/T4CK" pad="4"/>
<connect gate="X" pin="RC4/T5CK" pad="5"/>
<connect gate="X" pin="SCL/RG2" pad="47"/>
<connect gate="X" pin="SDA/RG3" pad="46"/>
<connect gate="X" pin="SDI1/RF7" pad="44"/>
<connect gate="X" pin="U1RX/RF2" pad="42"/>
<connect gate="X" pin="U1TX/RF3" pad="41"/>
<connect gate="X" pin="VDD" pad="12"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VDD@2" pad="48"/>
<connect gate="X" pin="VDD@3" pad="71"/>
<connect gate="X" pin="VSS" pad="11"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VSS@2" pad="51"/>
<connect gate="X" pin="VSS@3" pad="70"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ12GP201" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJ12GP201"/>
</gates>
<devices>
<device name="/SO" package="SO18W">
<connects>
<connect gate="X" pin="INT0/RP7/CN23/RB7" pad="10"/>
<connect gate="X" pin="MCLR#" pad="1"/>
<connect gate="X" pin="PGC1/EMUC1/RP1/AN3/CN5/RB1" pad="5"/>
<connect gate="X" pin="PGD1/EMUD1/RP0/AN2/CN4/RB0" pad="4"/>
<connect gate="X" pin="RA0/CN2/AN0/VREF+/EMUD2/PGD2" pad="2"/>
<connect gate="X" pin="RA1/CN3/AN1/VREF-/EMUC2/PGC2" pad="3"/>
<connect gate="X" pin="RA2/OSCI/CLKI/CN30" pad="6"/>
<connect gate="X" pin="RA3/OSCO/CLKO/CN29" pad="7"/>
<connect gate="X" pin="RA4/CN0/T1CK/SOSCO/EMUC3/PGC3" pad="9"/>
<connect gate="X" pin="RB4/CN1/RP4/SOSCI/EMUD3/PGD3" pad="8"/>
<connect gate="X" pin="RP14/AN7/CN12/RB14" pad="15"/>
<connect gate="X" pin="RP15/AN6/CN11/RB15" pad="16"/>
<connect gate="X" pin="SCL1/RP9/CN21/RB9" pad="12"/>
<connect gate="X" pin="SDA1/RP8/CN22/RB8" pad="11"/>
<connect gate="X" pin="VDD" pad="18"/>
<connect gate="X" pin="VDDCORE" pad="14"/>
<connect gate="X" pin="VSS" pad="13"/>
<connect gate="X" pin="VSS@1" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SP" package="DIL18">
<connects>
<connect gate="X" pin="INT0/RP7/CN23/RB7" pad="10"/>
<connect gate="X" pin="MCLR#" pad="1"/>
<connect gate="X" pin="PGC1/EMUC1/RP1/AN3/CN5/RB1" pad="5"/>
<connect gate="X" pin="PGD1/EMUD1/RP0/AN2/CN4/RB0" pad="4"/>
<connect gate="X" pin="RA0/CN2/AN0/VREF+/EMUD2/PGD2" pad="2"/>
<connect gate="X" pin="RA1/CN3/AN1/VREF-/EMUC2/PGC2" pad="3"/>
<connect gate="X" pin="RA2/OSCI/CLKI/CN30" pad="6"/>
<connect gate="X" pin="RA3/OSCO/CLKO/CN29" pad="7"/>
<connect gate="X" pin="RA4/CN0/T1CK/SOSCO/EMUC3/PGC3" pad="9"/>
<connect gate="X" pin="RB4/CN1/RP4/SOSCI/EMUD3/PGD3" pad="8"/>
<connect gate="X" pin="RP14/AN7/CN12/RB14" pad="15"/>
<connect gate="X" pin="RP15/AN6/CN11/RB15" pad="16"/>
<connect gate="X" pin="SCL1/RP9/CN21/RB9" pad="12"/>
<connect gate="X" pin="SDA1/RP8/CN22/RB8" pad="11"/>
<connect gate="X" pin="VDD" pad="18"/>
<connect gate="X" pin="VDDCORE" pad="14"/>
<connect gate="X" pin="VSS" pad="13"/>
<connect gate="X" pin="VSS@1" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ64GP206" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CoDec port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP206"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RF0" pad="58"/>
<connect gate="X" pin="RF1" pad="59"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ64GP306" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CoDec port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP306"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RF0" pad="58"/>
<connect gate="X" pin="RF1" pad="59"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SCL2/CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ64GP706" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP706"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="C2RX/RG0" pad="61"/>
<connect gate="X" pin="C2TX/RG1" pad="60"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SCL2/CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ64GP708" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP708"/>
</gates>
<devices>
<device name="/PT" package="TQFP80_12X12">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="26"/>
<connect gate="X" pin="C1RX/RF0" pad="72"/>
<connect gate="X" pin="C1TX/RF1" pad="73"/>
<connect gate="X" pin="C2RX/RG0" pad="75"/>
<connect gate="X" pin="C2TX/RG1" pad="74"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="8"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="10"/>
<connect gate="X" pin="CN13/OC5/RD4" pad="66"/>
<connect gate="X" pin="CN14/OC6/RD5" pad="67"/>
<connect gate="X" pin="CN15/OC7/RD6" pad="68"/>
<connect gate="X" pin="CN16/OC8/RD7" pad="69"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="39"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="40"/>
<connect gate="X" pin="CN19/IC6/RD13" pad="65"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="6"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="7"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="78"/>
<connect gate="X" pin="CSDI/RG12" pad="79"/>
<connect gate="X" pin="CSDO/RG13" pad="80"/>
<connect gate="X" pin="IC1/RD8" pad="54"/>
<connect gate="X" pin="IC2/RD9" pad="55"/>
<connect gate="X" pin="IC3/RD10" pad="56"/>
<connect gate="X" pin="IC4/RD11" pad="57"/>
<connect gate="X" pin="IC5/RD12" pad="64"/>
<connect gate="X" pin="MCLR" pad="9"/>
<connect gate="X" pin="OC1/RD0" pad="58"/>
<connect gate="X" pin="OC2/RD1" pad="61"/>
<connect gate="X" pin="OC3/RD2" pad="62"/>
<connect gate="X" pin="OC4/RD3" pad="63"/>
<connect gate="X" pin="OSC1/CLKI/RC12" pad="49"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="X" pin="RA10/VR+" pad="24"/>
<connect gate="X" pin="RA14/INT3/SCL2" pad="52"/>
<connect gate="X" pin="RA15/INT4/SDA2" pad="53"/>
<connect gate="X" pin="RA6/AN22/CN22" pad="76"/>
<connect gate="X" pin="RA7/AN23/CN23" pad="77"/>
<connect gate="X" pin="RA9/VR-" pad="23"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/PGD3" pad="20"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/PGC3" pad="19"/>
<connect gate="X" pin="RB10/AN10" pad="29"/>
<connect gate="X" pin="RB11/AN11" pad="30"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="33"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="34"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="35"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="36"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="18"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="17"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="16"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="15"/>
<connect gate="X" pin="RB6/AN6/EMUC1/PGC1/OCFA" pad="21"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="22"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="27"/>
<connect gate="X" pin="RB9/AN9" pad="28"/>
<connect gate="X" pin="RC1/AN16/T2CK/T7CK" pad="2"/>
<connect gate="X" pin="RC13/CN1/EMUD2/SOSCI" pad="59"/>
<connect gate="X" pin="RC14/CN0/EMUC2/SOSCO/T1CK" pad="60"/>
<connect gate="X" pin="RC2/AN17/T3CK/T6CK" pad="3"/>
<connect gate="X" pin="RC3/AN18/T4CK/T9CK" pad="4"/>
<connect gate="X" pin="RC4/AN19/T5CK/T8CK" pad="5"/>
<connect gate="X" pin="RE8/AN20/INT1/TMS" pad="13"/>
<connect gate="X" pin="RE9/AN21/INT2/TDO" pad="14"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="45"/>
<connect gate="X" pin="SCL1/RG2" pad="47"/>
<connect gate="X" pin="SDA1/RG3" pad="46"/>
<connect gate="X" pin="SDI1/RF7" pad="44"/>
<connect gate="X" pin="SDO1/RF8" pad="43"/>
<connect gate="X" pin="U1CTS/CN20/IC7/RD14" pad="37"/>
<connect gate="X" pin="U1RTS/CN21/IC8/RD15" pad="38"/>
<connect gate="X" pin="U1RX/RF2" pad="42"/>
<connect gate="X" pin="U1TX/RF3" pad="41"/>
<connect gate="X" pin="VDD" pad="12"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VDD@2" pad="48"/>
<connect gate="X" pin="VDD@3" pad="71"/>
<connect gate="X" pin="VDDCORE" pad="70"/>
<connect gate="X" pin="VSS" pad="11"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VSS@2" pad="51"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ64MC506" prefix="IC">
<description>&lt;b&gt;dsPIC33 Motion Controller DSC with CAN port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXMC506"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="PWM1H/RE1" pad="61"/>
<connect gate="X" pin="PWM1L/RE0" pad="60"/>
<connect gate="X" pin="PWM2H/RE3" pad="63"/>
<connect gate="X" pin="PWM2L/RE2" pad="62"/>
<connect gate="X" pin="PWM3H/RE5" pad="1"/>
<connect gate="X" pin="PWM3L/RE4" pad="64"/>
<connect gate="X" pin="PWM4H/RE7" pad="3"/>
<connect gate="X" pin="PWM4L/RE6" pad="2"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/QEA/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/QEB/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16/UPDN" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1/FLTA" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/FLTB/U1CTS" pad="43"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ128GP206" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CoDec port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP206"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RF0" pad="58"/>
<connect gate="X" pin="RF1" pad="59"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ128GP306" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CoDec port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP306"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RF0" pad="58"/>
<connect gate="X" pin="RF1" pad="59"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SCL2/CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ128GP706" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP706"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="C2RX/RG0" pad="61"/>
<connect gate="X" pin="C2TX/RG1" pad="60"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SCL2/CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ128GP708" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP708"/>
</gates>
<devices>
<device name="/PT" package="TQFP80_12X12">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="26"/>
<connect gate="X" pin="C1RX/RF0" pad="72"/>
<connect gate="X" pin="C1TX/RF1" pad="73"/>
<connect gate="X" pin="C2RX/RG0" pad="75"/>
<connect gate="X" pin="C2TX/RG1" pad="74"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="8"/>
<connect gate="X" pin="CN11/SS2/RG9" pad="10"/>
<connect gate="X" pin="CN13/OC5/RD4" pad="66"/>
<connect gate="X" pin="CN14/OC6/RD5" pad="67"/>
<connect gate="X" pin="CN15/OC7/RD6" pad="68"/>
<connect gate="X" pin="CN16/OC8/RD7" pad="69"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="39"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="40"/>
<connect gate="X" pin="CN19/IC6/RD13" pad="65"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="6"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="7"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="78"/>
<connect gate="X" pin="CSDI/RG12" pad="79"/>
<connect gate="X" pin="CSDO/RG13" pad="80"/>
<connect gate="X" pin="IC1/RD8" pad="54"/>
<connect gate="X" pin="IC2/RD9" pad="55"/>
<connect gate="X" pin="IC3/RD10" pad="56"/>
<connect gate="X" pin="IC4/RD11" pad="57"/>
<connect gate="X" pin="IC5/RD12" pad="64"/>
<connect gate="X" pin="MCLR" pad="9"/>
<connect gate="X" pin="OC1/RD0" pad="58"/>
<connect gate="X" pin="OC2/RD1" pad="61"/>
<connect gate="X" pin="OC3/RD2" pad="62"/>
<connect gate="X" pin="OC4/RD3" pad="63"/>
<connect gate="X" pin="OSC1/CLKI/RC12" pad="49"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="X" pin="RA10/VR+" pad="24"/>
<connect gate="X" pin="RA14/INT3/SCL2" pad="52"/>
<connect gate="X" pin="RA15/INT4/SDA2" pad="53"/>
<connect gate="X" pin="RA6/AN22/CN22" pad="76"/>
<connect gate="X" pin="RA7/AN23/CN23" pad="77"/>
<connect gate="X" pin="RA9/VR-" pad="23"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/PGD3" pad="20"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/PGC3" pad="19"/>
<connect gate="X" pin="RB10/AN10" pad="29"/>
<connect gate="X" pin="RB11/AN11" pad="30"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="33"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="34"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="35"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="36"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="18"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="17"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="16"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="15"/>
<connect gate="X" pin="RB6/AN6/EMUC1/PGC1/OCFA" pad="21"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="22"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="27"/>
<connect gate="X" pin="RB9/AN9" pad="28"/>
<connect gate="X" pin="RC1/AN16/T2CK/T7CK" pad="2"/>
<connect gate="X" pin="RC13/CN1/EMUD2/SOSCI" pad="59"/>
<connect gate="X" pin="RC14/CN0/EMUC2/SOSCO/T1CK" pad="60"/>
<connect gate="X" pin="RC2/AN17/T3CK/T6CK" pad="3"/>
<connect gate="X" pin="RC3/AN18/T4CK/T9CK" pad="4"/>
<connect gate="X" pin="RC4/AN19/T5CK/T8CK" pad="5"/>
<connect gate="X" pin="RE8/AN20/INT1/TMS" pad="13"/>
<connect gate="X" pin="RE9/AN21/INT2/TDO" pad="14"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="45"/>
<connect gate="X" pin="SCL1/RG2" pad="47"/>
<connect gate="X" pin="SDA1/RG3" pad="46"/>
<connect gate="X" pin="SDI1/RF7" pad="44"/>
<connect gate="X" pin="SDO1/RF8" pad="43"/>
<connect gate="X" pin="U1CTS/CN20/IC7/RD14" pad="37"/>
<connect gate="X" pin="U1RTS/CN21/IC8/RD15" pad="38"/>
<connect gate="X" pin="U1RX/RF2" pad="42"/>
<connect gate="X" pin="U1TX/RF3" pad="41"/>
<connect gate="X" pin="VDD" pad="12"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VDD@2" pad="48"/>
<connect gate="X" pin="VDD@3" pad="71"/>
<connect gate="X" pin="VDDCORE" pad="70"/>
<connect gate="X" pin="VSS" pad="11"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VSS@2" pad="51"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ128MC506" prefix="IC">
<description>&lt;b&gt;dsPIC33 Motion Controller DSC with CAN port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXMC506"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="PWM1H/RE1" pad="61"/>
<connect gate="X" pin="PWM1L/RE0" pad="60"/>
<connect gate="X" pin="PWM2H/RE3" pad="63"/>
<connect gate="X" pin="PWM2L/RE2" pad="62"/>
<connect gate="X" pin="PWM3H/RE5" pad="1"/>
<connect gate="X" pin="PWM3L/RE4" pad="64"/>
<connect gate="X" pin="PWM4H/RE7" pad="3"/>
<connect gate="X" pin="PWM4L/RE6" pad="2"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/QEA/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/QEB/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16/UPDN" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1/FLTA" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/FLTB/U1CTS" pad="43"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ128MC706" prefix="IC">
<description>&lt;b&gt;dsPIC33 Motion Controller DSC with CAN port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXMC506"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="PWM1H/RE1" pad="61"/>
<connect gate="X" pin="PWM1L/RE0" pad="60"/>
<connect gate="X" pin="PWM2H/RE3" pad="63"/>
<connect gate="X" pin="PWM2L/RE2" pad="62"/>
<connect gate="X" pin="PWM3H/RE5" pad="1"/>
<connect gate="X" pin="PWM3L/RE4" pad="64"/>
<connect gate="X" pin="PWM4H/RE7" pad="3"/>
<connect gate="X" pin="PWM4L/RE6" pad="2"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/QEA/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/QEB/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16/UPDN" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1/FLTA" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/FLTB/U1CTS" pad="43"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ128MC708" prefix="IC">
<description>&lt;b&gt;dsPIC33 Motion Controller DSC with CAN port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXMC708"/>
</gates>
<devices>
<device name="/PT" package="TQFP80_12X12">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="26"/>
<connect gate="X" pin="C1RX/RF0" pad="72"/>
<connect gate="X" pin="C1TX/RF1" pad="73"/>
<connect gate="X" pin="CN13/OC5/RD4" pad="66"/>
<connect gate="X" pin="CN14/OC6/RD5" pad="67"/>
<connect gate="X" pin="CN15/OC7/RD6" pad="68"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="39"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="40"/>
<connect gate="X" pin="CN19/IC6/RD13" pad="65"/>
<connect gate="X" pin="IC1/RD8" pad="54"/>
<connect gate="X" pin="IC2/RD9" pad="55"/>
<connect gate="X" pin="IC3/RD10" pad="56"/>
<connect gate="X" pin="IC4/RD11" pad="57"/>
<connect gate="X" pin="IC5/RD12" pad="64"/>
<connect gate="X" pin="MCLR" pad="9"/>
<connect gate="X" pin="OC1/RD0" pad="58"/>
<connect gate="X" pin="OC2/RD1" pad="61"/>
<connect gate="X" pin="OC3/RD2" pad="62"/>
<connect gate="X" pin="OC4/RD3" pad="63"/>
<connect gate="X" pin="OSC1/CLKI/RC12" pad="49"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="50"/>
<connect gate="X" pin="PWM1H/RE1" pad="77"/>
<connect gate="X" pin="PWM1L/RE0" pad="76"/>
<connect gate="X" pin="PWM2H/RE3" pad="79"/>
<connect gate="X" pin="PWM2L/RE2" pad="78"/>
<connect gate="X" pin="PWM3H/RE5" pad="1"/>
<connect gate="X" pin="PWM3L/RE4" pad="80"/>
<connect gate="X" pin="PWM4H/RE7" pad="3"/>
<connect gate="X" pin="PWM4L/RE6" pad="2"/>
<connect gate="X" pin="RA10/VR+" pad="24"/>
<connect gate="X" pin="RA14/INT3/SCL2" pad="52"/>
<connect gate="X" pin="RA15/INT4/SDA2" pad="53"/>
<connect gate="X" pin="RA9/VR-" pad="23"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/PGD3" pad="20"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/PGC3" pad="19"/>
<connect gate="X" pin="RB10/AN10" pad="29"/>
<connect gate="X" pin="RB11/AN11" pad="30"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="33"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="34"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="35"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="36"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="18"/>
<connect gate="X" pin="RB3/AN3/CN5/INDX" pad="17"/>
<connect gate="X" pin="RB4/AN4/CN6/QEA" pad="16"/>
<connect gate="X" pin="RB5/AN5/CN7/QEB" pad="15"/>
<connect gate="X" pin="RB6/AN6/EMUC1/PGC1/OCFA" pad="21"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="22"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="27"/>
<connect gate="X" pin="RB9/AN9" pad="28"/>
<connect gate="X" pin="RC1/AN16/T2CK/T7CK" pad="4"/>
<connect gate="X" pin="RC13/CN1/EMUD2/SOSCI" pad="59"/>
<connect gate="X" pin="RC14/CN0/EMUC2/SOSCO/T1CK" pad="60"/>
<connect gate="X" pin="RC2/AN17/T3CK/T6CK" pad="5"/>
<connect gate="X" pin="RG0/C2RX" pad="75"/>
<connect gate="X" pin="RG1/C2TX" pad="74"/>
<connect gate="X" pin="RG2/SCL1" pad="47"/>
<connect gate="X" pin="RG3/SDA1" pad="46"/>
<connect gate="X" pin="RG6/CN8/SCK2" pad="6"/>
<connect gate="X" pin="RG7/CN9/SDI2" pad="7"/>
<connect gate="X" pin="RG8/CN10/SDO2" pad="8"/>
<connect gate="X" pin="RG9/CN11/SS2" pad="10"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="45"/>
<connect gate="X" pin="SDI1/RF7" pad="44"/>
<connect gate="X" pin="SDO1/RF8" pad="43"/>
<connect gate="X" pin="TDO/FLTB/INT2/RE9" pad="14"/>
<connect gate="X" pin="TMS/FLTA/INT1/RE8" pad="13"/>
<connect gate="X" pin="U1CTS/CN20/IC7/RD14" pad="37"/>
<connect gate="X" pin="U1RTS/CN21/IC8/RD15" pad="38"/>
<connect gate="X" pin="U1RX/RF2" pad="42"/>
<connect gate="X" pin="U1TX/RF3" pad="41"/>
<connect gate="X" pin="UPDN/CN16/OC8/RD7" pad="69"/>
<connect gate="X" pin="VDD" pad="12"/>
<connect gate="X" pin="VDD@1" pad="32"/>
<connect gate="X" pin="VDD@2" pad="48"/>
<connect gate="X" pin="VDD@3" pad="71"/>
<connect gate="X" pin="VDDCORE" pad="70"/>
<connect gate="X" pin="VSS" pad="11"/>
<connect gate="X" pin="VSS@1" pad="31"/>
<connect gate="X" pin="VSS@2" pad="51"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ256GP506" prefix="IC">
<description>&lt;b&gt;dsPIC33 General DSC with CAN and CoDec ports&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC33FJXXGP506"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="COFS/RG15" pad="1"/>
<connect gate="X" pin="CSCK/RG14" pad="62"/>
<connect gate="X" pin="CSDI/RG12" pad="63"/>
<connect gate="X" pin="CSDO/RG13" pad="64"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SCL2/CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F2010" prefix="IC" uservalue="yes">
<description>&lt;b&gt;dsPIC Motion Controller DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F2010"/>
</gates>
<devices>
<device name="/SOG" package="SO-28W">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="INT0/FLTA/SCK1/OCFA/RE8" pad="16"/>
<connect gate="X" pin="INT2/EMUD2/OC2/IC2/RD1" pad="14"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="PGC/EMUC/RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="PWM1H/RE1" pad="25"/>
<connect gate="X" pin="PWM1L/RE0" pad="26"/>
<connect gate="X" pin="PWM2H/RE3" pad="23"/>
<connect gate="X" pin="PWM2L/RE2" pad="24"/>
<connect gate="X" pin="PWM3H/RE5" pad="21"/>
<connect gate="X" pin="PWM3L/RE4" pad="22"/>
<connect gate="X" pin="RB0/CN2/AN0/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/CN3/AN1/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/CN4/AN2/SS1" pad="4"/>
<connect gate="X" pin="RB3/CN5/AN3/INDX" pad="5"/>
<connect gate="X" pin="RB4/CN6/AN4/QEA/IC7" pad="6"/>
<connect gate="X" pin="RB5/CN7/AN5/QEB/IC8" pad="7"/>
<connect gate="X" pin="RC13/CN1/EMUD1/ATX/T2C" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/ARX/T1C" pad="12"/>
<connect gate="X" pin="RC15/OSC2/CLKO" pad="10"/>
<connect gate="X" pin="RD0/INT1/EMUC2/OC1/IC1" pad="15"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SPG" package="DIL28-3">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="INT0/FLTA/SCK1/OCFA/RE8" pad="16"/>
<connect gate="X" pin="INT2/EMUD2/OC2/IC2/RD1" pad="14"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="PGC/EMUC/RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="PWM1H/RE1" pad="25"/>
<connect gate="X" pin="PWM1L/RE0" pad="26"/>
<connect gate="X" pin="PWM2H/RE3" pad="23"/>
<connect gate="X" pin="PWM2L/RE2" pad="24"/>
<connect gate="X" pin="PWM3H/RE5" pad="21"/>
<connect gate="X" pin="PWM3L/RE4" pad="22"/>
<connect gate="X" pin="RB0/CN2/AN0/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/CN3/AN1/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/CN4/AN2/SS1" pad="4"/>
<connect gate="X" pin="RB3/CN5/AN3/INDX" pad="5"/>
<connect gate="X" pin="RB4/CN6/AN4/QEA/IC7" pad="6"/>
<connect gate="X" pin="RB5/CN7/AN5/QEB/IC8" pad="7"/>
<connect gate="X" pin="RC13/CN1/EMUD1/ATX/T2C" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/ARX/T1C" pad="12"/>
<connect gate="X" pin="RC15/OSC2/CLKO" pad="10"/>
<connect gate="X" pin="RD0/INT1/EMUC2/OC1/IC1" pad="15"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/MMG" package="QFN-S28-6X6">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="24"/>
<connect gate="X" pin="INT0/FLTA/SCK1/OCFA/RE8" pad="13"/>
<connect gate="X" pin="INT2/EMUD2/OC2/IC2/RD1" pad="11"/>
<connect gate="X" pin="OSC1/CLKI" pad="6"/>
<connect gate="X" pin="PGC/EMUC/RX/SDI1/SDA/RF2" pad="15"/>
<connect gate="X" pin="PGD/EMUD/TX/SDO1/SCL/RF3" pad="14"/>
<connect gate="X" pin="PWM1H/RE1" pad="22"/>
<connect gate="X" pin="PWM1L/RE0" pad="23"/>
<connect gate="X" pin="PWM2H/RE3" pad="20"/>
<connect gate="X" pin="PWM2L/RE2" pad="21"/>
<connect gate="X" pin="PWM3H/RE5" pad="18"/>
<connect gate="X" pin="PWM3L/RE4" pad="19"/>
<connect gate="X" pin="RB0/CN2/AN0/EMUD3/VR+" pad="27"/>
<connect gate="X" pin="RB1/CN3/AN1/EMUC3/VR-" pad="28"/>
<connect gate="X" pin="RB2/CN4/AN2/SS1" pad="1"/>
<connect gate="X" pin="RB3/CN5/AN3/INDX" pad="2"/>
<connect gate="X" pin="RB4/CN6/AN4/QEA/IC7" pad="3"/>
<connect gate="X" pin="RB5/CN7/AN5/QEB/IC8" pad="4"/>
<connect gate="X" pin="RC13/CN1/EMUD1/ATX/T2C" pad="8"/>
<connect gate="X" pin="RC14/CN0/EMUC1/ARX/T1C" pad="9"/>
<connect gate="X" pin="RC15/OSC2/CLKO" pad="7"/>
<connect gate="X" pin="RD0/INT1/EMUC2/OC1/IC1" pad="12"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="17"/>
<connect gate="X" pin="VPP/MCLR" pad="26"/>
<connect gate="X" pin="VSS" pad="5"/>
<connect gate="X" pin="VSS@1" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F2012">
<description>&lt;b&gt;dsPIC Sensor DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F2012"/>
</gates>
<devices>
<device name="/SO" package="SO-28W">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="CN17/RF4" pad="22"/>
<connect gate="X" pin="CN18/RF5" pad="21"/>
<connect gate="X" pin="EMUC2/IC1/INT1/RD8" pad="15"/>
<connect gate="X" pin="IC2/INT2/RD9" pad="14"/>
<connect gate="X" pin="MCLR/VPP" pad="1"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="10"/>
<connect gate="X" pin="PGC/EMUC/U1RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/U1TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="6"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="7"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="26"/>
<connect gate="X" pin="RB7/AN7/EMUD2" pad="25"/>
<connect gate="X" pin="RB8/AN8/OC1" pad="24"/>
<connect gate="X" pin="RB9/AN9/OC2" pad="23"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="12"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="16"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SP" package="DIL28-3">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="CN17/RF4" pad="22"/>
<connect gate="X" pin="CN18/RF5" pad="21"/>
<connect gate="X" pin="EMUC2/IC1/INT1/RD8" pad="15"/>
<connect gate="X" pin="IC2/INT2/RD9" pad="14"/>
<connect gate="X" pin="MCLR/VPP" pad="1"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="10"/>
<connect gate="X" pin="PGC/EMUC/U1RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/U1TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="6"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="7"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="26"/>
<connect gate="X" pin="RB7/AN7/EMUD2" pad="25"/>
<connect gate="X" pin="RB8/AN8/OC1" pad="24"/>
<connect gate="X" pin="RB9/AN9/OC2" pad="23"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="12"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="16"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN-S28-6X6">
<connects>
<connect gate="X" pin="AVDD" pad="25"/>
<connect gate="X" pin="AVSS" pad="24"/>
<connect gate="X" pin="CN17/RF4" pad="19"/>
<connect gate="X" pin="CN18/RF5" pad="18"/>
<connect gate="X" pin="EMUC2/IC1/INT1/RD8" pad="12"/>
<connect gate="X" pin="IC2/INT2/RD9" pad="11"/>
<connect gate="X" pin="MCLR/VPP" pad="26"/>
<connect gate="X" pin="OSC1/CLKI" pad="6"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="7"/>
<connect gate="X" pin="PGC/EMUC/U1RX/SDI1/SDA/RF2" pad="15"/>
<connect gate="X" pin="PGD/EMUD/U1TX/SDO1/SCL/RF3" pad="14"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="27"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="28"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="1"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="2"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="3"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="4"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="23"/>
<connect gate="X" pin="RB7/AN7/EMUD2" pad="22"/>
<connect gate="X" pin="RB8/AN8/OC1" pad="21"/>
<connect gate="X" pin="RB9/AN9/OC2" pad="20"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="8"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="9"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="13"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="17"/>
<connect gate="X" pin="VSS" pad="5"/>
<connect gate="X" pin="VSS@1" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F3010" prefix="IC">
<description>&lt;b&gt;dsPIC Motion Controller DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F2010"/>
</gates>
<devices>
<device name="/SO" package="SO-28W">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="INT0/FLTA/SCK1/OCFA/RE8" pad="16"/>
<connect gate="X" pin="INT2/EMUD2/OC2/IC2/RD1" pad="14"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="PGC/EMUC/RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="PWM1H/RE1" pad="25"/>
<connect gate="X" pin="PWM1L/RE0" pad="26"/>
<connect gate="X" pin="PWM2H/RE3" pad="23"/>
<connect gate="X" pin="PWM2L/RE2" pad="24"/>
<connect gate="X" pin="PWM3H/RE5" pad="21"/>
<connect gate="X" pin="PWM3L/RE4" pad="22"/>
<connect gate="X" pin="RB0/CN2/AN0/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/CN3/AN1/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/CN4/AN2/SS1" pad="4"/>
<connect gate="X" pin="RB3/CN5/AN3/INDX" pad="5"/>
<connect gate="X" pin="RB4/CN6/AN4/QEA/IC7" pad="6"/>
<connect gate="X" pin="RB5/CN7/AN5/QEB/IC8" pad="7"/>
<connect gate="X" pin="RC13/CN1/EMUD1/ATX/T2C" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/ARX/T1C" pad="12"/>
<connect gate="X" pin="RC15/OSC2/CLKO" pad="10"/>
<connect gate="X" pin="RD0/INT1/EMUC2/OC1/IC1" pad="15"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SP" package="DIL28-3">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="INT0/FLTA/SCK1/OCFA/RE8" pad="16"/>
<connect gate="X" pin="INT2/EMUD2/OC2/IC2/RD1" pad="14"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="PGC/EMUC/RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="PWM1H/RE1" pad="25"/>
<connect gate="X" pin="PWM1L/RE0" pad="26"/>
<connect gate="X" pin="PWM2H/RE3" pad="23"/>
<connect gate="X" pin="PWM2L/RE2" pad="24"/>
<connect gate="X" pin="PWM3H/RE5" pad="21"/>
<connect gate="X" pin="PWM3L/RE4" pad="22"/>
<connect gate="X" pin="RB0/CN2/AN0/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/CN3/AN1/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/CN4/AN2/SS1" pad="4"/>
<connect gate="X" pin="RB3/CN5/AN3/INDX" pad="5"/>
<connect gate="X" pin="RB4/CN6/AN4/QEA/IC7" pad="6"/>
<connect gate="X" pin="RB5/CN7/AN5/QEB/IC8" pad="7"/>
<connect gate="X" pin="RC13/CN1/EMUD1/ATX/T2C" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/ARX/T1C" pad="12"/>
<connect gate="X" pin="RC15/OSC2/CLKO" pad="10"/>
<connect gate="X" pin="RD0/INT1/EMUC2/OC1/IC1" pad="15"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F3013">
<description>&lt;b&gt;dsPIC Sensor DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F3013"/>
</gates>
<devices>
<device name="/SO" package="SO-28W">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="EMUC2/IC1/INT1/RD8" pad="15"/>
<connect gate="X" pin="IC2/INT2/RD9" pad="14"/>
<connect gate="X" pin="MCLR/VPP" pad="1"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="10"/>
<connect gate="X" pin="PGC/EMUC/U1RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/U1TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="6"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="7"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="26"/>
<connect gate="X" pin="RB7/AN7/EMUD2" pad="25"/>
<connect gate="X" pin="RB8/AN8/OC1" pad="24"/>
<connect gate="X" pin="RB9/AN9/OC2" pad="23"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="12"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="16"/>
<connect gate="X" pin="U2RX/CN17/RF4" pad="22"/>
<connect gate="X" pin="U2TX/CN18/RF5" pad="21"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SP" package="DIL28-3">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="EMUC2/IC1/INT1/RD8" pad="15"/>
<connect gate="X" pin="IC2/INT2/RD9" pad="14"/>
<connect gate="X" pin="MCLR/VPP" pad="1"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="10"/>
<connect gate="X" pin="PGC/EMUC/U1RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/U1TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="4"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="5"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="6"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="7"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="26"/>
<connect gate="X" pin="RB7/AN7/EMUD2" pad="25"/>
<connect gate="X" pin="RB8/AN8/OC1" pad="24"/>
<connect gate="X" pin="RB9/AN9/OC2" pad="23"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="12"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="16"/>
<connect gate="X" pin="U2RX/CN17/RF4" pad="22"/>
<connect gate="X" pin="U2TX/CN18/RF5" pad="21"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN44-8X8">
<connects>
<connect gate="X" pin="AVDD" pad="17"/>
<connect gate="X" pin="AVSS" pad="16"/>
<connect gate="X" pin="EMUC2/IC1/INT1/RD8" pad="42"/>
<connect gate="X" pin="IC2/INT2/RD9" pad="37"/>
<connect gate="X" pin="MCLR/VPP" pad="18"/>
<connect gate="X" pin="OSC1/CLKI" pad="32"/>
<connect gate="X" pin="OSC2/CLKO/RC15" pad="33"/>
<connect gate="X" pin="PGC/EMUC/U1RX/SDI1/SDA/RF2" pad="1"/>
<connect gate="X" pin="PGD/EMUD/U1TX/SDO1/SCL/RF3" pad="44"/>
<connect gate="X" pin="RB0/AN0/CN2/EMUD3/VR+" pad="19"/>
<connect gate="X" pin="RB1/AN1/CN3/EMUC3/VR-" pad="20"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="23"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="25"/>
<connect gate="X" pin="RB4/AN4/CN6" pad="26"/>
<connect gate="X" pin="RB5/AN5/CN7" pad="27"/>
<connect gate="X" pin="RB6/AN6/OCFA" pad="14"/>
<connect gate="X" pin="RB7/AN7/EMUD2" pad="12"/>
<connect gate="X" pin="RB8/AN8/OC1" pad="11"/>
<connect gate="X" pin="RB9/AN9/OC2" pad="10"/>
<connect gate="X" pin="RC13/CN1/EMUD1/SOSCI/T2CK/U1ATX" pad="34"/>
<connect gate="X" pin="RC14/CN0/EMUC1/SOSCO/T1CK/U1ARX" pad="35"/>
<connect gate="X" pin="SCK1/INT0/RF6" pad="43"/>
<connect gate="X" pin="U2RX/CN17/RF4" pad="9"/>
<connect gate="X" pin="U2TX/CN18/RF5" pad="7"/>
<connect gate="X" pin="VDD" pad="4"/>
<connect gate="X" pin="VDD@1" pad="36"/>
<connect gate="X" pin="VSS" pad="2"/>
<connect gate="X" pin="VSS@1" pad="30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F4012" prefix="IC">
<description>&lt;b&gt;dsPIC Motion Controller DSC&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DSPIC30F2010"/>
</gates>
<devices>
<device name="/SO" package="SO-28W">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="INT0/FLTA/SCK1/OCFA/RE8" pad="16"/>
<connect gate="X" pin="INT2/EMUD2/OC2/IC2/RD1" pad="14"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="PGC/EMUC/RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="PWM1H/RE1" pad="25"/>
<connect gate="X" pin="PWM1L/RE0" pad="26"/>
<connect gate="X" pin="PWM2H/RE3" pad="23"/>
<connect gate="X" pin="PWM2L/RE2" pad="24"/>
<connect gate="X" pin="PWM3H/RE5" pad="21"/>
<connect gate="X" pin="PWM3L/RE4" pad="22"/>
<connect gate="X" pin="RB0/CN2/AN0/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/CN3/AN1/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/CN4/AN2/SS1" pad="4"/>
<connect gate="X" pin="RB3/CN5/AN3/INDX" pad="5"/>
<connect gate="X" pin="RB4/CN6/AN4/QEA/IC7" pad="6"/>
<connect gate="X" pin="RB5/CN7/AN5/QEB/IC8" pad="7"/>
<connect gate="X" pin="RC13/CN1/EMUD1/ATX/T2C" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/ARX/T1C" pad="12"/>
<connect gate="X" pin="RC15/OSC2/CLKO" pad="10"/>
<connect gate="X" pin="RD0/INT1/EMUC2/OC1/IC1" pad="15"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SP" package="DIL28-3">
<connects>
<connect gate="X" pin="AVDD" pad="28"/>
<connect gate="X" pin="AVSS" pad="27"/>
<connect gate="X" pin="INT0/FLTA/SCK1/OCFA/RE8" pad="16"/>
<connect gate="X" pin="INT2/EMUD2/OC2/IC2/RD1" pad="14"/>
<connect gate="X" pin="OSC1/CLKI" pad="9"/>
<connect gate="X" pin="PGC/EMUC/RX/SDI1/SDA/RF2" pad="18"/>
<connect gate="X" pin="PGD/EMUD/TX/SDO1/SCL/RF3" pad="17"/>
<connect gate="X" pin="PWM1H/RE1" pad="25"/>
<connect gate="X" pin="PWM1L/RE0" pad="26"/>
<connect gate="X" pin="PWM2H/RE3" pad="23"/>
<connect gate="X" pin="PWM2L/RE2" pad="24"/>
<connect gate="X" pin="PWM3H/RE5" pad="21"/>
<connect gate="X" pin="PWM3L/RE4" pad="22"/>
<connect gate="X" pin="RB0/CN2/AN0/EMUD3/VR+" pad="2"/>
<connect gate="X" pin="RB1/CN3/AN1/EMUC3/VR-" pad="3"/>
<connect gate="X" pin="RB2/CN4/AN2/SS1" pad="4"/>
<connect gate="X" pin="RB3/CN5/AN3/INDX" pad="5"/>
<connect gate="X" pin="RB4/CN6/AN4/QEA/IC7" pad="6"/>
<connect gate="X" pin="RB5/CN7/AN5/QEB/IC8" pad="7"/>
<connect gate="X" pin="RC13/CN1/EMUD1/ATX/T2C" pad="11"/>
<connect gate="X" pin="RC14/CN0/EMUC1/ARX/T1C" pad="12"/>
<connect gate="X" pin="RC15/OSC2/CLKO" pad="10"/>
<connect gate="X" pin="RD0/INT1/EMUC2/OC1/IC1" pad="15"/>
<connect gate="X" pin="VDD" pad="13"/>
<connect gate="X" pin="VDD@1" pad="20"/>
<connect gate="X" pin="VPP/MCLR" pad="1"/>
<connect gate="X" pin="VSS" pad="8"/>
<connect gate="X" pin="VSS@1" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/ML" package="QFN44-8X8">
<connects>
<connect gate="X" pin="AVDD" pad="17"/>
<connect gate="X" pin="AVSS" pad="16"/>
<connect gate="X" pin="INT0/FLTA/SCK1/OCFA/RE8" pad="43"/>
<connect gate="X" pin="INT2/EMUD2/OC2/IC2/RD1" pad="37"/>
<connect gate="X" pin="OSC1/CLKI" pad="32"/>
<connect gate="X" pin="PGC/EMUC/RX/SDI1/SDA/RF2" pad="1"/>
<connect gate="X" pin="PGD/EMUD/TX/SDO1/SCL/RF3" pad="44"/>
<connect gate="X" pin="PWM1H/RE1" pad="14"/>
<connect gate="X" pin="PWM1L/RE0" pad="15"/>
<connect gate="X" pin="PWM2H/RE3" pad="11"/>
<connect gate="X" pin="PWM2L/RE2" pad="12"/>
<connect gate="X" pin="PWM3H/RE5" pad="9"/>
<connect gate="X" pin="PWM3L/RE4" pad="10"/>
<connect gate="X" pin="RB0/CN2/AN0/EMUD3/VR+" pad="19"/>
<connect gate="X" pin="RB1/CN3/AN1/EMUC3/VR-" pad="20"/>
<connect gate="X" pin="RB2/CN4/AN2/SS1" pad="21"/>
<connect gate="X" pin="RB3/CN5/AN3/INDX" pad="22"/>
<connect gate="X" pin="RB4/CN6/AN4/QEA/IC7" pad="23"/>
<connect gate="X" pin="RB5/CN7/AN5/QEB/IC8" pad="24"/>
<connect gate="X" pin="RC13/CN1/EMUD1/ATX/T2C" pad="34"/>
<connect gate="X" pin="RC14/CN0/EMUC1/ARX/T1C" pad="35"/>
<connect gate="X" pin="RC15/OSC2/CLKO" pad="33"/>
<connect gate="X" pin="RD0/INT1/EMUC2/OC1/IC1" pad="42"/>
<connect gate="X" pin="VDD" pad="7"/>
<connect gate="X" pin="VDD@1" pad="28"/>
<connect gate="X" pin="VPP/MCLR" pad="18"/>
<connect gate="X" pin="VSS" pad="6"/>
<connect gate="X" pin="VSS@1" pad="30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1252" prefix="IC">
<description>&lt;b&gt;Positive-Regulated Charge Pump (3.3x5.0)&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="MCP1252/3"/>
</gates>
<devices>
<device name="" package="MSOP-8">
<connects>
<connect gate="X" pin="C+" pad="6"/>
<connect gate="X" pin="C-" pad="5"/>
<connect gate="X" pin="GND" pad="4"/>
<connect gate="X" pin="PGOOD" pad="1"/>
<connect gate="X" pin="SELECT" pad="8"/>
<connect gate="X" pin="SHDN#" pad="7"/>
<connect gate="X" pin="VIN" pad="3"/>
<connect gate="X" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1252-ADJ" prefix="IC">
<description>&lt;b&gt;Positive-Regulated Adjustable Charge Pump&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="MCP1252/3-ADJ"/>
</gates>
<devices>
<device name="" package="MSOP-8">
<connects>
<connect gate="X" pin="C+" pad="6"/>
<connect gate="X" pin="C-" pad="5"/>
<connect gate="X" pin="FB" pad="8"/>
<connect gate="X" pin="GND" pad="4"/>
<connect gate="X" pin="PGOOD" pad="1"/>
<connect gate="X" pin="SHDN#" pad="7"/>
<connect gate="X" pin="VIN" pad="3"/>
<connect gate="X" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1253" prefix="IC">
<description>&lt;b&gt;Positive-Regulated Charge Pump (3.3x5.0)&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="MCP1252/3"/>
</gates>
<devices>
<device name="" package="MSOP-8">
<connects>
<connect gate="X" pin="C+" pad="6"/>
<connect gate="X" pin="C-" pad="5"/>
<connect gate="X" pin="GND" pad="4"/>
<connect gate="X" pin="PGOOD" pad="1"/>
<connect gate="X" pin="SELECT" pad="8"/>
<connect gate="X" pin="SHDN#" pad="7"/>
<connect gate="X" pin="VIN" pad="3"/>
<connect gate="X" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1253-ADJ" prefix="IC">
<description>&lt;b&gt;Positive-Regulated Adjustable Charge Pump&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="MCP1252/3-ADJ"/>
</gates>
<devices>
<device name="" package="MSOP-8">
<connects>
<connect gate="X" pin="C+" pad="6"/>
<connect gate="X" pin="C-" pad="5"/>
<connect gate="X" pin="FB" pad="8"/>
<connect gate="X" pin="GND" pad="4"/>
<connect gate="X" pin="PGOOD" pad="1"/>
<connect gate="X" pin="SHDN#" pad="7"/>
<connect gate="X" pin="VIN" pad="3"/>
<connect gate="X" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP23016" prefix="IC">
<description>&lt;b&gt;16-Bit I/O Expander with I2C Interface&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MCP23016"/>
</gates>
<devices>
<device name="P" package="DIL28-3">
<connects>
<connect gate="A" pin="A0" pad="16"/>
<connect gate="A" pin="A1" pad="17"/>
<connect gate="A" pin="A2" pad="18"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="GP0.0" pad="21"/>
<connect gate="A" pin="GP0.1" pad="22"/>
<connect gate="A" pin="GP0.2" pad="23"/>
<connect gate="A" pin="GP0.3" pad="24"/>
<connect gate="A" pin="GP0.4" pad="25"/>
<connect gate="A" pin="GP0.5" pad="26"/>
<connect gate="A" pin="GP0.6" pad="27"/>
<connect gate="A" pin="GP0.7" pad="28"/>
<connect gate="A" pin="GP1.0" pad="2"/>
<connect gate="A" pin="GP1.1" pad="3"/>
<connect gate="A" pin="GP1.2" pad="4"/>
<connect gate="A" pin="GP1.3" pad="5"/>
<connect gate="A" pin="GP1.4" pad="7"/>
<connect gate="A" pin="GP1.5" pad="11"/>
<connect gate="A" pin="GP1.6" pad="12"/>
<connect gate="A" pin="GP1.7" pad="13"/>
<connect gate="A" pin="INT#" pad="6"/>
<connect gate="A" pin="SCL" pad="14"/>
<connect gate="A" pin="SDA" pad="15"/>
<connect gate="A" pin="TP" pad="10"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VSS" pad="1"/>
<connect gate="A" pin="VSS@1" pad="8"/>
<connect gate="A" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO" package="SO-28W">
<connects>
<connect gate="A" pin="A0" pad="16"/>
<connect gate="A" pin="A1" pad="17"/>
<connect gate="A" pin="A2" pad="18"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="GP0.0" pad="21"/>
<connect gate="A" pin="GP0.1" pad="22"/>
<connect gate="A" pin="GP0.2" pad="23"/>
<connect gate="A" pin="GP0.3" pad="24"/>
<connect gate="A" pin="GP0.4" pad="25"/>
<connect gate="A" pin="GP0.5" pad="26"/>
<connect gate="A" pin="GP0.6" pad="27"/>
<connect gate="A" pin="GP0.7" pad="28"/>
<connect gate="A" pin="GP1.0" pad="2"/>
<connect gate="A" pin="GP1.1" pad="3"/>
<connect gate="A" pin="GP1.2" pad="4"/>
<connect gate="A" pin="GP1.3" pad="5"/>
<connect gate="A" pin="GP1.4" pad="7"/>
<connect gate="A" pin="GP1.5" pad="11"/>
<connect gate="A" pin="GP1.6" pad="12"/>
<connect gate="A" pin="GP1.7" pad="13"/>
<connect gate="A" pin="INT#" pad="6"/>
<connect gate="A" pin="SCL" pad="14"/>
<connect gate="A" pin="SDA" pad="15"/>
<connect gate="A" pin="TP" pad="10"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VSS" pad="1"/>
<connect gate="A" pin="VSS@1" pad="8"/>
<connect gate="A" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="A" pin="A0" pad="16"/>
<connect gate="A" pin="A1" pad="17"/>
<connect gate="A" pin="A2" pad="18"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="GP0.0" pad="21"/>
<connect gate="A" pin="GP0.1" pad="22"/>
<connect gate="A" pin="GP0.2" pad="23"/>
<connect gate="A" pin="GP0.3" pad="24"/>
<connect gate="A" pin="GP0.4" pad="25"/>
<connect gate="A" pin="GP0.5" pad="26"/>
<connect gate="A" pin="GP0.6" pad="27"/>
<connect gate="A" pin="GP0.7" pad="28"/>
<connect gate="A" pin="GP1.0" pad="2"/>
<connect gate="A" pin="GP1.1" pad="3"/>
<connect gate="A" pin="GP1.2" pad="4"/>
<connect gate="A" pin="GP1.3" pad="5"/>
<connect gate="A" pin="GP1.4" pad="7"/>
<connect gate="A" pin="GP1.5" pad="11"/>
<connect gate="A" pin="GP1.6" pad="12"/>
<connect gate="A" pin="GP1.7" pad="13"/>
<connect gate="A" pin="INT#" pad="6"/>
<connect gate="A" pin="SCL" pad="14"/>
<connect gate="A" pin="SDA" pad="15"/>
<connect gate="A" pin="TP" pad="10"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VSS" pad="1"/>
<connect gate="A" pin="VSS@1" pad="8"/>
<connect gate="A" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ML" package="QFN-S28-6X6">
<connects>
<connect gate="A" pin="A0" pad="13"/>
<connect gate="A" pin="A1" pad="14"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="CLK" pad="6"/>
<connect gate="A" pin="GP0.0" pad="18"/>
<connect gate="A" pin="GP0.1" pad="19"/>
<connect gate="A" pin="GP0.2" pad="20"/>
<connect gate="A" pin="GP0.3" pad="21"/>
<connect gate="A" pin="GP0.4" pad="22"/>
<connect gate="A" pin="GP0.5" pad="23"/>
<connect gate="A" pin="GP0.6" pad="24"/>
<connect gate="A" pin="GP0.7" pad="25"/>
<connect gate="A" pin="GP1.0" pad="27"/>
<connect gate="A" pin="GP1.1" pad="28"/>
<connect gate="A" pin="GP1.2" pad="1"/>
<connect gate="A" pin="GP1.3" pad="2"/>
<connect gate="A" pin="GP1.4" pad="4"/>
<connect gate="A" pin="GP1.5" pad="8"/>
<connect gate="A" pin="GP1.6" pad="9"/>
<connect gate="A" pin="GP1.7" pad="10"/>
<connect gate="A" pin="INT#" pad="3"/>
<connect gate="A" pin="SCL" pad="11"/>
<connect gate="A" pin="SDA" pad="12"/>
<connect gate="A" pin="TP" pad="7"/>
<connect gate="A" pin="VDD" pad="17"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="VSS@1" pad="16"/>
<connect gate="A" pin="VSS@2" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2445" prefix="IC">
<description>&lt;b&gt;PIC18F Flash Microcontroller with USB port&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PIC18F2445/2550"/>
</gates>
<devices>
<device name="SO" package="SO-28W">
<connects>
<connect gate="A" pin="CCP1/RC2" pad="13"/>
<connect gate="A" pin="CK/TX/RC6" pad="17"/>
<connect gate="A" pin="CLKIN/OSC1" pad="9"/>
<connect gate="A" pin="RA0/AN0" pad="2"/>
<connect gate="A" pin="RA1/AN1" pad="3"/>
<connect gate="A" pin="RA2/AN2/VR-/CVREF" pad="4"/>
<connect gate="A" pin="RA3/AN3/VR+" pad="5"/>
<connect gate="A" pin="RA4/T0CKI/C1OUT/RCV" pad="6"/>
<connect gate="A" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="7"/>
<connect gate="A" pin="RA6/CLKO/OSC2" pad="10"/>
<connect gate="A" pin="RB0/SDA/SDI/AN12/INT0/FLT0" pad="21"/>
<connect gate="A" pin="RB1/SCL/SCK/AN10/INT1" pad="22"/>
<connect gate="A" pin="RB2/AN8/INT2/VMO" pad="23"/>
<connect gate="A" pin="RB3/AN9/CCP2/VPO" pad="24"/>
<connect gate="A" pin="RB4/AN11/KBI0" pad="25"/>
<connect gate="A" pin="RB5/KBI1/PGM" pad="26"/>
<connect gate="A" pin="RB6/KBI2/PGC" pad="27"/>
<connect gate="A" pin="RB7/KBI3/PGD" pad="28"/>
<connect gate="A" pin="RE3/VPP/MCLR" pad="1"/>
<connect gate="A" pin="SDO/DT/RX/RC7" pad="18"/>
<connect gate="A" pin="T13CKI/T1OSO/RC0" pad="11"/>
<connect gate="A" pin="UOE/CCP2/T1OSI/RC1" pad="12"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VM/D-/RC4" pad="15"/>
<connect gate="A" pin="VP/D+/RC5" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS@1" pad="19"/>
<connect gate="A" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SP" package="DIL28-3">
<connects>
<connect gate="A" pin="CCP1/RC2" pad="13"/>
<connect gate="A" pin="CK/TX/RC6" pad="17"/>
<connect gate="A" pin="CLKIN/OSC1" pad="9"/>
<connect gate="A" pin="RA0/AN0" pad="2"/>
<connect gate="A" pin="RA1/AN1" pad="3"/>
<connect gate="A" pin="RA2/AN2/VR-/CVREF" pad="4"/>
<connect gate="A" pin="RA3/AN3/VR+" pad="5"/>
<connect gate="A" pin="RA4/T0CKI/C1OUT/RCV" pad="6"/>
<connect gate="A" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="7"/>
<connect gate="A" pin="RA6/CLKO/OSC2" pad="10"/>
<connect gate="A" pin="RB0/SDA/SDI/AN12/INT0/FLT0" pad="21"/>
<connect gate="A" pin="RB1/SCL/SCK/AN10/INT1" pad="22"/>
<connect gate="A" pin="RB2/AN8/INT2/VMO" pad="23"/>
<connect gate="A" pin="RB3/AN9/CCP2/VPO" pad="24"/>
<connect gate="A" pin="RB4/AN11/KBI0" pad="25"/>
<connect gate="A" pin="RB5/KBI1/PGM" pad="26"/>
<connect gate="A" pin="RB6/KBI2/PGC" pad="27"/>
<connect gate="A" pin="RB7/KBI3/PGD" pad="28"/>
<connect gate="A" pin="RE3/VPP/MCLR" pad="1"/>
<connect gate="A" pin="SDO/DT/RX/RC7" pad="18"/>
<connect gate="A" pin="T13CKI/T1OSO/RC0" pad="11"/>
<connect gate="A" pin="UOE/CCP2/T1OSI/RC1" pad="12"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VM/D-/RC4" pad="15"/>
<connect gate="A" pin="VP/D+/RC5" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS@1" pad="19"/>
<connect gate="A" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2550" prefix="IC">
<description>&lt;b&gt;PIC18F Flash Microcontroller with USB port&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PIC18F2445/2550"/>
</gates>
<devices>
<device name="SO" package="SO-28W">
<connects>
<connect gate="A" pin="CCP1/RC2" pad="13"/>
<connect gate="A" pin="CK/TX/RC6" pad="17"/>
<connect gate="A" pin="CLKIN/OSC1" pad="9"/>
<connect gate="A" pin="RA0/AN0" pad="2"/>
<connect gate="A" pin="RA1/AN1" pad="3"/>
<connect gate="A" pin="RA2/AN2/VR-/CVREF" pad="4"/>
<connect gate="A" pin="RA3/AN3/VR+" pad="5"/>
<connect gate="A" pin="RA4/T0CKI/C1OUT/RCV" pad="6"/>
<connect gate="A" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="7"/>
<connect gate="A" pin="RA6/CLKO/OSC2" pad="10"/>
<connect gate="A" pin="RB0/SDA/SDI/AN12/INT0/FLT0" pad="21"/>
<connect gate="A" pin="RB1/SCL/SCK/AN10/INT1" pad="22"/>
<connect gate="A" pin="RB2/AN8/INT2/VMO" pad="23"/>
<connect gate="A" pin="RB3/AN9/CCP2/VPO" pad="24"/>
<connect gate="A" pin="RB4/AN11/KBI0" pad="25"/>
<connect gate="A" pin="RB5/KBI1/PGM" pad="26"/>
<connect gate="A" pin="RB6/KBI2/PGC" pad="27"/>
<connect gate="A" pin="RB7/KBI3/PGD" pad="28"/>
<connect gate="A" pin="RE3/VPP/MCLR" pad="1"/>
<connect gate="A" pin="SDO/DT/RX/RC7" pad="18"/>
<connect gate="A" pin="T13CKI/T1OSO/RC0" pad="11"/>
<connect gate="A" pin="UOE/CCP2/T1OSI/RC1" pad="12"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VM/D-/RC4" pad="15"/>
<connect gate="A" pin="VP/D+/RC5" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS@1" pad="19"/>
<connect gate="A" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SP" package="DIL28-3">
<connects>
<connect gate="A" pin="CCP1/RC2" pad="13"/>
<connect gate="A" pin="CK/TX/RC6" pad="17"/>
<connect gate="A" pin="CLKIN/OSC1" pad="9"/>
<connect gate="A" pin="RA0/AN0" pad="2"/>
<connect gate="A" pin="RA1/AN1" pad="3"/>
<connect gate="A" pin="RA2/AN2/VR-/CVREF" pad="4"/>
<connect gate="A" pin="RA3/AN3/VR+" pad="5"/>
<connect gate="A" pin="RA4/T0CKI/C1OUT/RCV" pad="6"/>
<connect gate="A" pin="RA5/AN4/SS/HLVDIN/C2OUT" pad="7"/>
<connect gate="A" pin="RA6/CLKO/OSC2" pad="10"/>
<connect gate="A" pin="RB0/SDA/SDI/AN12/INT0/FLT0" pad="21"/>
<connect gate="A" pin="RB1/SCL/SCK/AN10/INT1" pad="22"/>
<connect gate="A" pin="RB2/AN8/INT2/VMO" pad="23"/>
<connect gate="A" pin="RB3/AN9/CCP2/VPO" pad="24"/>
<connect gate="A" pin="RB4/AN11/KBI0" pad="25"/>
<connect gate="A" pin="RB5/KBI1/PGM" pad="26"/>
<connect gate="A" pin="RB6/KBI2/PGC" pad="27"/>
<connect gate="A" pin="RB7/KBI3/PGD" pad="28"/>
<connect gate="A" pin="RE3/VPP/MCLR" pad="1"/>
<connect gate="A" pin="SDO/DT/RX/RC7" pad="18"/>
<connect gate="A" pin="T13CKI/T1OSO/RC0" pad="11"/>
<connect gate="A" pin="UOE/CCP2/T1OSI/RC1" pad="12"/>
<connect gate="A" pin="VDD" pad="20"/>
<connect gate="A" pin="VM/D-/RC4" pad="15"/>
<connect gate="A" pin="VP/D+/RC5" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS@1" pad="19"/>
<connect gate="A" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F6680" prefix="IC">
<description>&lt;b&gt;PIC18F Flash Microcontroller with CAN port&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="PIC18F6680"/>
</gates>
<devices>
<device name="TQ-64" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN10/C1I+/CVR/RF5" pad="13"/>
<connect gate="X" pin="AN11/C1I-/RF6" pad="12"/>
<connect gate="X" pin="AN5/RF0" pad="18"/>
<connect gate="X" pin="AN6/C2O/RF1" pad="17"/>
<connect gate="X" pin="AN7/C1O/RF2" pad="16"/>
<connect gate="X" pin="AN8/C2I+/RF3" pad="15"/>
<connect gate="X" pin="AN9/C2I-/RF4" pad="14"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CCP2/RE7" pad="59"/>
<connect gate="X" pin="CLKI/OSC1" pad="39"/>
<connect gate="X" pin="CLKO/RA6/OSC2" pad="40"/>
<connect gate="X" pin="CS/RE2" pad="64"/>
<connect gate="X" pin="P1B/RE6" pad="60"/>
<connect gate="X" pin="P1C/RE5" pad="61"/>
<connect gate="X" pin="PSP0/RD0" pad="58"/>
<connect gate="X" pin="PSP1/RD1" pad="55"/>
<connect gate="X" pin="PSP2/RD2" pad="54"/>
<connect gate="X" pin="PSP3/RD3" pad="53"/>
<connect gate="X" pin="PSP4/RD4" pad="52"/>
<connect gate="X" pin="PSP5/RD5" pad="51"/>
<connect gate="X" pin="PSP6/RD6" pad="50"/>
<connect gate="X" pin="PSP7/RD7" pad="49"/>
<connect gate="X" pin="RA0/AN0" pad="24"/>
<connect gate="X" pin="RA1/AN1" pad="23"/>
<connect gate="X" pin="RA2/AN2/VR-" pad="22"/>
<connect gate="X" pin="RA3/AN3/VR+" pad="21"/>
<connect gate="X" pin="RA4/T0CKI" pad="28"/>
<connect gate="X" pin="RA5/AN4/LVDIN" pad="27"/>
<connect gate="X" pin="RB0/INT0" pad="48"/>
<connect gate="X" pin="RB1/INT1" pad="47"/>
<connect gate="X" pin="RB2/INT2" pad="46"/>
<connect gate="X" pin="RB3/INT3" pad="45"/>
<connect gate="X" pin="RB4/KBI0" pad="44"/>
<connect gate="X" pin="RB5/KBI1/PGM" pad="43"/>
<connect gate="X" pin="RB6/KBI2/PGC" pad="42"/>
<connect gate="X" pin="RB7/KBI3/PGD" pad="37"/>
<connect gate="X" pin="RC0/T1O/T13C" pad="30"/>
<connect gate="X" pin="RC1/T1I/CCP2" pad="29"/>
<connect gate="X" pin="RC2/CCP1/P1A" pad="33"/>
<connect gate="X" pin="RC3/SCK/SCL" pad="34"/>
<connect gate="X" pin="RC4/SDI/SDA" pad="35"/>
<connect gate="X" pin="RC5/SDO" pad="36"/>
<connect gate="X" pin="RC6/TX/CK" pad="31"/>
<connect gate="X" pin="RC7/RX/DT" pad="32"/>
<connect gate="X" pin="RD/RE0" pad="2"/>
<connect gate="X" pin="RE3" pad="63"/>
<connect gate="X" pin="RE4" pad="62"/>
<connect gate="X" pin="RG0/CANTX1" pad="3"/>
<connect gate="X" pin="RG1/CANTX2" pad="4"/>
<connect gate="X" pin="RG2/CANRX" pad="5"/>
<connect gate="X" pin="RG3" pad="6"/>
<connect gate="X" pin="RG4/P1D" pad="8"/>
<connect gate="X" pin="RG5/MCLR/VPP" pad="7"/>
<connect gate="X" pin="SS/RF7" pad="11"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
<connect gate="X" pin="VSS@3" pad="56"/>
<connect gate="X" pin="WR/RE1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F8490">
<description>&lt;b&gt;PIC18F Flash Microcontroller with LCD driver&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PIC18F8490"/>
</gates>
<devices>
<device name="TQ-80" package="TQFP80_12X12">
<connects>
<connect gate="A" pin="AVDD" pad="25"/>
<connect gate="A" pin="AVSS" pad="26"/>
<connect gate="A" pin="C1OUT/S20/AN7/RF2" pad="18"/>
<connect gate="A" pin="C2OUT/S19/AN6/RF1" pad="23"/>
<connect gate="A" pin="CK2/TX2/S29/RG1" pad="6"/>
<connect gate="A" pin="COM0" pad="77"/>
<connect gate="A" pin="COM1/RE4" pad="76"/>
<connect gate="A" pin="COM2/RE5" pad="75"/>
<connect gate="A" pin="COM3/RE6" pad="74"/>
<connect gate="A" pin="CVREF/S23/AN10/RF5" pad="15"/>
<connect gate="A" pin="DT2/RX2/S28/RG2" pad="7"/>
<connect gate="A" pin="LCDBIAS1" pad="4"/>
<connect gate="A" pin="LCDBIAS2" pad="3"/>
<connect gate="A" pin="LCDBIAS3" pad="78"/>
<connect gate="A" pin="MCLR/VPP/RG5" pad="9"/>
<connect gate="A" pin="OSC1/CLKI/RA7" pad="49"/>
<connect gate="A" pin="OSC2/CLKO/RA6" pad="50"/>
<connect gate="A" pin="RA0/AN0" pad="30"/>
<connect gate="A" pin="RA1/AN1" pad="29"/>
<connect gate="A" pin="RA2/AN2/VR-/S16" pad="28"/>
<connect gate="A" pin="RA3/AN3/VR+/S17" pad="27"/>
<connect gate="A" pin="RA4/T0CKI/S14" pad="34"/>
<connect gate="A" pin="RA5/AN4/HLVDIN/S15" pad="33"/>
<connect gate="A" pin="RB0/INT0" pad="58"/>
<connect gate="A" pin="RB1/INT1/S8" pad="57"/>
<connect gate="A" pin="RB2/INT2/S9" pad="56"/>
<connect gate="A" pin="RB3/INT3/S10" pad="55"/>
<connect gate="A" pin="RB4/KBI0/S11" pad="54"/>
<connect gate="A" pin="RB5/KBI1" pad="53"/>
<connect gate="A" pin="RB6/KBI2/PGC" pad="52"/>
<connect gate="A" pin="RB7/KBI3/PGD" pad="47"/>
<connect gate="A" pin="RC0/T1OSO/T13CKI" pad="36"/>
<connect gate="A" pin="RC1/T1OSI/CCP2" pad="35"/>
<connect gate="A" pin="RC2/CCP1/S13" pad="43"/>
<connect gate="A" pin="RC3/SCK/SCL" pad="44"/>
<connect gate="A" pin="RC4/SDI/SDA" pad="45"/>
<connect gate="A" pin="RC5/SDO/S12" pad="46"/>
<connect gate="A" pin="RC6/TX1/CK1" pad="37"/>
<connect gate="A" pin="RC7/RX1/DT1" pad="38"/>
<connect gate="A" pin="RD0/S0" pad="72"/>
<connect gate="A" pin="RD1/S1" pad="69"/>
<connect gate="A" pin="RD2/S2" pad="68"/>
<connect gate="A" pin="RD3/S3" pad="67"/>
<connect gate="A" pin="RD4/S4" pad="66"/>
<connect gate="A" pin="RD5/S5" pad="65"/>
<connect gate="A" pin="RD6/S6" pad="64"/>
<connect gate="A" pin="RD7/S7" pad="63"/>
<connect gate="A" pin="S18/AN5/RF0" pad="24"/>
<connect gate="A" pin="S21/AN8/RF3" pad="17"/>
<connect gate="A" pin="S22/AN9/RF4" pad="16"/>
<connect gate="A" pin="S24/AN11/RF6" pad="14"/>
<connect gate="A" pin="S25/SS/RF7" pad="13"/>
<connect gate="A" pin="S26/RG4" pad="10"/>
<connect gate="A" pin="S27/RG3" pad="8"/>
<connect gate="A" pin="S30/RG0" pad="5"/>
<connect gate="A" pin="S31/CCP2/RE7" pad="73"/>
<connect gate="A" pin="S32/RJ0" pad="62"/>
<connect gate="A" pin="S33/RJ1" pad="61"/>
<connect gate="A" pin="S34/RJ2" pad="60"/>
<connect gate="A" pin="S35/RJ3" pad="59"/>
<connect gate="A" pin="S36/RJ7" pad="42"/>
<connect gate="A" pin="S37/RJ6" pad="41"/>
<connect gate="A" pin="S38/RJ5" pad="40"/>
<connect gate="A" pin="S39/RJ4" pad="39"/>
<connect gate="A" pin="S40/RH4" pad="22"/>
<connect gate="A" pin="S41/RH5" pad="21"/>
<connect gate="A" pin="S42/RH6" pad="20"/>
<connect gate="A" pin="S43/RH7" pad="19"/>
<connect gate="A" pin="S44/RH3" pad="2"/>
<connect gate="A" pin="S45/RH2" pad="1"/>
<connect gate="A" pin="S46/RH1" pad="80"/>
<connect gate="A" pin="S47/RH0" pad="79"/>
<connect gate="A" pin="VDD" pad="12"/>
<connect gate="A" pin="VDD@1" pad="32"/>
<connect gate="A" pin="VDD@2" pad="48"/>
<connect gate="A" pin="VDD@3" pad="71"/>
<connect gate="A" pin="VSS" pad="11"/>
<connect gate="A" pin="VSS@1" pad="31"/>
<connect gate="A" pin="VSS@2" pad="51"/>
<connect gate="A" pin="VSS@3" pad="70"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ64GP206" prefix="IC">
<description>&lt;b&gt;PIC24H 16-bit microcontroller&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="PIC24XJXXXGP206"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RF0" pad="58"/>
<connect gate="X" pin="RF1" pad="59"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="RG12" pad="63"/>
<connect gate="X" pin="RG13" pad="64"/>
<connect gate="X" pin="RG14" pad="62"/>
<connect gate="X" pin="RG15" pad="1"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ128GP206" prefix="IC">
<description>&lt;b&gt;PIC24H 16-bit microcontroller&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="PIC24XJXXXGP206"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RF0" pad="58"/>
<connect gate="X" pin="RF1" pad="59"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="RG12" pad="63"/>
<connect gate="X" pin="RG13" pad="64"/>
<connect gate="X" pin="RG14" pad="62"/>
<connect gate="X" pin="RG15" pad="1"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ128GP306" prefix="IC">
<description>&lt;b&gt;PIC24H 16-bit microcontroller&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="PIC24XJXXXGP306"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RF0" pad="58"/>
<connect gate="X" pin="RF1" pad="59"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="RG12" pad="63"/>
<connect gate="X" pin="RG13" pad="64"/>
<connect gate="X" pin="RG14" pad="62"/>
<connect gate="X" pin="RG15" pad="1"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SCL2/CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ128GP506" prefix="IC">
<description>&lt;b&gt;PIC24H 16-bit microcontroller&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="PIC24XJXXXGP506"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="C1RX/RF0" pad="58"/>
<connect gate="X" pin="C1TX/RF1" pad="59"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="RG12" pad="63"/>
<connect gate="X" pin="RG13" pad="64"/>
<connect gate="X" pin="RG14" pad="62"/>
<connect gate="X" pin="RG15" pad="1"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SCL2/CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ256GP206" prefix="IC">
<description>&lt;b&gt;PIC24H 16-bit microcontroller&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="PIC24XJXXXGP206"/>
</gates>
<devices>
<device name="/PT" package="TQFP64_10X10">
<connects>
<connect gate="X" pin="AN16/T2CK/T7CK/RC1" pad="2"/>
<connect gate="X" pin="AN17/T3CK/T6CK/RC2" pad="3"/>
<connect gate="X" pin="AVDD" pad="19"/>
<connect gate="X" pin="AVSS" pad="20"/>
<connect gate="X" pin="CN10/SDO2/RG8" pad="6"/>
<connect gate="X" pin="CN17/U2RX/RF4" pad="31"/>
<connect gate="X" pin="CN18/U2TX/RF5" pad="32"/>
<connect gate="X" pin="CN8/SCK2/RG6" pad="4"/>
<connect gate="X" pin="CN9/SDI2/RG7" pad="5"/>
<connect gate="X" pin="INT0/U1RTS/SCK1/RF6" pad="35"/>
<connect gate="X" pin="MCLR" pad="7"/>
<connect gate="X" pin="PGC2/SOSCO/T1CK/EMUC2/CN0/RC14" pad="48"/>
<connect gate="X" pin="PGD2/SOSCI/T4CK/EMUD2/CN1/RC13" pad="47"/>
<connect gate="X" pin="RB0/AN0/CN2/VR+/PGD3/EMUD3" pad="16"/>
<connect gate="X" pin="RB1/AN1/CN3/VR-/PGC3/EMUC3" pad="15"/>
<connect gate="X" pin="RB10/AN10/TMS" pad="23"/>
<connect gate="X" pin="RB11/AN11/TDO" pad="24"/>
<connect gate="X" pin="RB12/AN12/TCK" pad="27"/>
<connect gate="X" pin="RB13/AN13/TDI" pad="28"/>
<connect gate="X" pin="RB14/AN14/U2RTS" pad="29"/>
<connect gate="X" pin="RB15/AN15/CN12/OCFB" pad="30"/>
<connect gate="X" pin="RB2/AN2/CN4/SS1/LVDIN" pad="14"/>
<connect gate="X" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="X" pin="RB4/AN4/CN6/IC7" pad="12"/>
<connect gate="X" pin="RB5/AN5/CN7/IC8" pad="11"/>
<connect gate="X" pin="RB6/AN6/OCFA/EMUC1/PGC1" pad="17"/>
<connect gate="X" pin="RB7/AN7/EMUD1/PGD1" pad="18"/>
<connect gate="X" pin="RB8/AN8/U2CTS" pad="21"/>
<connect gate="X" pin="RB9/AN9" pad="22"/>
<connect gate="X" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="X" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="X" pin="RD0/OC1" pad="46"/>
<connect gate="X" pin="RD1/OC2" pad="49"/>
<connect gate="X" pin="RD10/IC3/INT3" pad="44"/>
<connect gate="X" pin="RD11/IC4/INT4" pad="45"/>
<connect gate="X" pin="RD2/OC3" pad="50"/>
<connect gate="X" pin="RD3/OC4" pad="51"/>
<connect gate="X" pin="RD4/OC5/IC5/CN13" pad="52"/>
<connect gate="X" pin="RD5/OC6/IC6/CN14" pad="53"/>
<connect gate="X" pin="RD6/OC7/CN15" pad="54"/>
<connect gate="X" pin="RD7/OC8/CN16" pad="55"/>
<connect gate="X" pin="RD8/IC1/INT1" pad="42"/>
<connect gate="X" pin="RD9/IC2/INT2/U1CTS" pad="43"/>
<connect gate="X" pin="RF0" pad="58"/>
<connect gate="X" pin="RF1" pad="59"/>
<connect gate="X" pin="RG0" pad="61"/>
<connect gate="X" pin="RG1" pad="60"/>
<connect gate="X" pin="RG12" pad="63"/>
<connect gate="X" pin="RG13" pad="64"/>
<connect gate="X" pin="RG14" pad="62"/>
<connect gate="X" pin="RG15" pad="1"/>
<connect gate="X" pin="SCL1/RG2" pad="37"/>
<connect gate="X" pin="SDA1/RG3" pad="36"/>
<connect gate="X" pin="SDI1/U1RX/RF2" pad="34"/>
<connect gate="X" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="X" pin="T5CK/CN11/SS2/RG9" pad="8"/>
<connect gate="X" pin="VDD" pad="10"/>
<connect gate="X" pin="VDD@1" pad="26"/>
<connect gate="X" pin="VDD@2" pad="38"/>
<connect gate="X" pin="VDD@3" pad="57"/>
<connect gate="X" pin="VDDC" pad="56"/>
<connect gate="X" pin="VSS" pad="9"/>
<connect gate="X" pin="VSS@1" pad="25"/>
<connect gate="X" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB3750" prefix="IC" uservalue="yes">
<description>The USB375x integrates many features that have historically been discrete devices in a mobile
product. This device provides significant VBUS protection for the entire system, robust USB interface
ESD protection, a USB 2.0 compliant High Speed switch, and USB-IF Battery Charger Detection
(revision 1.1) capabilities that are essential to the latest mobile products.</description>
<gates>
<gate name="USB3750" symbol="USB3750"/>
</gates>
<devices>
<device name="" package="QFN16">
<connects>
<connect gate="USB3750" pin="10/VOUT" pad="10"/>
<connect gate="USB3750" pin="11/VOUT" pad="11"/>
<connect gate="USB3750" pin="2/VBUS" pad="2"/>
<connect gate="USB3750" pin="3/VBUS" pad="3"/>
<connect gate="USB3750" pin="4/VBUS" pad="4"/>
<connect gate="USB3750" pin="9/VOUT" pad="9"/>
<connect gate="USB3750" pin="DM" pad="14"/>
<connect gate="USB3750" pin="DM_1" pad="16"/>
<connect gate="USB3750" pin="DM_2" pad="12"/>
<connect gate="USB3750" pin="DP" pad="15"/>
<connect gate="USB3750" pin="DP_1" pad="1"/>
<connect gate="USB3750" pin="DP_2" pad="13"/>
<connect gate="USB3750" pin="GND" pad="8"/>
<connect gate="USB3750" pin="INT_B" pad="7"/>
<connect gate="USB3750" pin="SCL" pad="6"/>
<connect gate="USB3750" pin="SDA" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB3751" prefix="IC" uservalue="yes">
<description>USB 2.0 Protection IC with
Battery Charger Detection</description>
<gates>
<gate name="USB3751" symbol="USB3751"/>
</gates>
<devices>
<device name="" package="QFN16">
<connects>
<connect gate="USB3751" pin="1/DP1" pad="1"/>
<connect gate="USB3751" pin="10/VOUT" pad="10"/>
<connect gate="USB3751" pin="11/VOUT" pad="11"/>
<connect gate="USB3751" pin="14/DM" pad="14"/>
<connect gate="USB3751" pin="15/DP" pad="15"/>
<connect gate="USB3751" pin="16/DM1" pad="16"/>
<connect gate="USB3751" pin="2/VBUS" pad="2"/>
<connect gate="USB3751" pin="3/VBUS" pad="3"/>
<connect gate="USB3751" pin="4/VBUS" pad="4"/>
<connect gate="USB3751" pin="5/SDA" pad="5"/>
<connect gate="USB3751" pin="6/SCL" pad="6"/>
<connect gate="USB3751" pin="7/INTB" pad="7"/>
<connect gate="USB3751" pin="8/GND" pad="8"/>
<connect gate="USB3751" pin="9/VOUT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB3740" prefix="IC" uservalue="yes">
<description>&lt;B&gt;High Speed Switch for Mobile and
Portable Applications</description>
<gates>
<gate name="USB3740" symbol="USB3740"/>
</gates>
<devices>
<device name="USB3740B-AI9TR" package="QFN10_2,1X1,6">
<connects>
<connect gate="USB3740" pin="1/DM1" pad="1"/>
<connect gate="USB3740" pin="10/DP" pad="10"/>
<connect gate="USB3740" pin="2/DP1" pad="2"/>
<connect gate="USB3740" pin="3/OEN" pad="3"/>
<connect gate="USB3740" pin="4/S" pad="4"/>
<connect gate="USB3740" pin="5/VDD" pad="5"/>
<connect gate="USB3740" pin="6/DP2" pad="6"/>
<connect gate="USB3740" pin="7/DM2" pad="7"/>
<connect gate="USB3740" pin="8/GND" pad="8"/>
<connect gate="USB3740" pin="9/DM" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB3740B-AI2-TR" package="QFN10_1,3X1,8">
<connects>
<connect gate="USB3740" pin="1/DM1" pad="1"/>
<connect gate="USB3740" pin="10/DP" pad="10"/>
<connect gate="USB3740" pin="2/DP1" pad="2"/>
<connect gate="USB3740" pin="3/OEN" pad="3"/>
<connect gate="USB3740" pin="4/S" pad="4"/>
<connect gate="USB3740" pin="5/VDD" pad="5"/>
<connect gate="USB3740" pin="6/DP2" pad="6"/>
<connect gate="USB3740" pin="7/DM2" pad="7"/>
<connect gate="USB3740" pin="8/GND" pad="8"/>
<connect gate="USB3740" pin="9/DM" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
