<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>&lt;H1&gt;NXP Library&lt;/H1&gt;
&lt;author&gt;marco.kuystermans@nxp.com&lt;/author&gt;&lt;p&gt;

&lt;H2&gt;Disclaimer:&lt;/H2&gt;
&lt;i&gt;The information contained in this library is made available for general information and public access only. By using our 
library, you accept this disclaimer in full. If you disagree with any part of this disclaimer, you must not use our library.
Use of this library is permitted on the basis that NXP will not be liable for any loss or damage including without limitation, indirect or consequential loss or 
damage, arising out of or in connection with the use of this library.&lt;/i&gt;

&lt;H2&gt;Information:&lt;/H2&gt;
&lt;ul&gt;&lt;li&gt;Footprints are according to NXP footprint information, see &lt;a href=http://www.nxp.com&gt;NXP website&lt;/a&gt;
&lt;li&gt;SMD Footprints in this library are for reflow soldering only.
&lt;li&gt;&lt;b&gt;Library is generated as a courtesy: Information is NOT guaranteed, use at your own risk&lt;/b&gt;
&lt;li&gt;NXP package numbers (SOT/SOD) numbers used
&lt;/ul&gt;
Please send your comments to the mail address above.</description>
<packages>
<package name="SOT314-2">
<description>&lt;li&gt;&lt;b&gt;SOT314-2&lt;/b&gt;
&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;LQFP64: plastic low profile quad flat package; 64 leads; body 10 x 10 x 1.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-026
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 136E10&lt;/ul&gt;</description>
</package>
<package name="SOT1175-1">
<description>&lt;li&gt;&lt;b&gt;SOT1175-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO7: plastic small outline package; 7 leads; body width 3.9 m
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: ---
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT361-1">
<description>&lt;li&gt;&lt;b&gt;SOT361-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT136-1_ALTERNATIVE">
<description>&lt;li&gt;&lt;b&gt;SOT136-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO28: plastic small outline package; 28 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-013
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 075E06&lt;/ul&gt;
&lt;H3&gt;Please do not use, will be removed&lt;/H3&gt;</description>
</package>
<package name="SOT78A">
<description>&lt;li&gt;&lt;b&gt;SOT78&lt;/b&gt;
&lt;li&gt;JEDEC TO-220AB
&lt;li&gt;JEITA SC-46</description>
</package>
<package name="SOT223">
<description>&lt;li&gt;&lt;b&gt;SOT223&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package with increased heatsink; 4 lead
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-73&lt;/ul&gt;</description>
</package>
<package name="FIDUCIAL0.6-1.2">
<description>FIDUCAL</description>
</package>
<package name="SOD80C">
<description>&lt;li&gt;&lt;b&gt;SOD80C&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Hermetically sealed glass surface-mounted package; 2 connectors
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 100H01
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT457">
<description>&lt;li&gt;&lt;b&gt;SOT457&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSOP6: Plastic surface-mounted package; 6 lead
&lt;li&gt;&lt;u&gt;JEIDA&lt;/u&gt;: SC73
&lt;p&gt;A.K.A. SOT23-6</description>
</package>
<package name="SOT313-2">
<description>&lt;li&gt;&lt;b&gt;SOT313-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;LQFP48: plastic low profile quad flat package; 48 leads; body 7 x 7 x 1.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-026
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 136E05&lt;/ul&gt;
Footprint according to NXP SOT313-2 specification, however the cornerpins are 0.4mm in stead of 0.5mm. Probably an error in the specification.</description>
</package>
<package name="SOT617-1">
<description>&lt;li&gt;&lt;b&gt;SOT617-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN32: plastic thermal enhanced very thin quad flat package; no leads; 32 terminals; body 5 x 5 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOD128">
<description>&lt;li&gt;&lt;b&gt;SOD128&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 2 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT-HVQFN33">
<description>&lt;li&gt;&lt;b&gt;SOTxxx&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN33: plastic thermal enhanced very thin quad flat package; no leads; 33 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: ---
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;
&lt;li&gt;Package according LPC111x datasheet</description>
</package>
<package name="SOT315-1">
<description>&lt;li&gt;&lt;b&gt;SOT315-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;LQFP80: plastic low profile quad flat package; 80 leads; body 12 x 12 x 1.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-026
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 136E15&lt;/ul&gt;</description>
</package>
<package name="SOT407-1">
<description>&lt;li&gt;&lt;b&gt;SOT407-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-026
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 136E20&lt;/ul&gt;</description>
</package>
<package name="HVQFN33-7X7">
<description>&lt;b&gt;HVQFN33 &lt;/b&gt;&lt;p&gt;Plastic thermal enhanced very thin quad flat package; 33 terminals; body 7x7x0.85 mm; &lt;p&gt;
Original Library package</description>
</package>
<package name="SOT926-1">
<description>&lt;li&gt;&lt;b&gt;SOT926-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TFBGA100: plastic thin fine-pitch ball grid array package; 100 balls; body 9 x 9 x 0.7 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT505-1">
<description>&lt;li&gt;&lt;b&gt;SOT505-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT96-1">
<description>&lt;li&gt;&lt;b&gt;SOT96-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO8: plastic small outline package; 8 leads; body width 3.9 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-012
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 076E03&lt;/ul&gt;</description>
</package>
<package name="SOT403-1">
<description>&lt;li&gt;&lt;b&gt;SOT403-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP16: plastic thin shrink small outline package; 16 leads; body width 4.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT109-1">
<description>&lt;li&gt;&lt;b&gt;SOT109-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO16: plastic small outline package; 16 leads; body width 3.9 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-012
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 076E07&lt;/ul&gt;</description>
</package>
<package name="SOT97-1">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT363">
<description>&lt;li&gt;&lt;b&gt;SOT363&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 6 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;:  SC-88&lt;/ul&gt;</description>
</package>
<package name="SOT886">
<description>&lt;li&gt;&lt;b&gt;SOT886&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON6: plastic extremely thin small outline package; no leads; 6 terminals; body 1 x 1.45 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-252
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT891">
<description>&lt;li&gt;&lt;b&gt;SOT891&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON6: plastic extremely thin small outline package; no leads; 6 terminals; body 1 x 1 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT1202">
<description>&lt;li&gt;&lt;b&gt;SOT1202&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON6: extremely thin small outline package; no leads; 6 terminals; body 1.0 x 1.0 x 0.35 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: ---
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT353-1">
<description>&lt;li&gt;&lt;b&gt;SOT353&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 5 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA:  SC-88A&lt;/ul&gt;</description>
</package>
<package name="SOD523">
<description>&lt;li&gt;&lt;b&gt;SOD523&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 2 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-79&lt;/ul&gt;</description>
</package>
<package name="SOT543-1">
<description>&lt;li&gt;&lt;b&gt;SOT543-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TFBGA64: plastic thin fine-pitch ball grid array package; 64 balls; body 6 x 6 x 0.8 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO195
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT669">
<description>&lt;li&gt;&lt;b&gt;SOT669&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single-ended surface-mounted package (LFPAK; Power-SO8); 4 lead
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-235
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT918-1">
<description>&lt;li&gt;&lt;b&gt;SOT918-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TFBGA48: plastic thin fine-pitch ball grid array package; 48 balls; body 5 x 5 x 0.8 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-195
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT137-1_ALTERNATIVE">
<description>&lt;li&gt;&lt;b&gt;SOT137-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO24: plastic small outline package; 28 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-013
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 075E05&lt;/ul&gt;
&lt;H3&gt;Please do not use, will be removed&lt;/H3&gt;</description>
</package>
<package name="SOT1039-1">
<description>&lt;li&gt;&lt;b&gt;SOT1039-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HXQFN16U: plastic thermal enhanced extremely thin quad flat package; no leads;16 terminals; UTLP based; body 3 x 3 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1161-1">
<description>&lt;li&gt;&lt;b&gt;SOT1161-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XQFN16: plastic, extremely thin quad flat package; no leads;16 terminals; body 1.80 x 2.60 x 0.50 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT764">
<description>&lt;li&gt;&lt;b&gt;SOT764&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DHVQFN20: plastic dual in-line compatible thermal enhanced very thin quad flat package; no leads; 20 terminals; body 2.5 x 4.5 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-241
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT486-1">
<description>&lt;li&gt;&lt;b&gt;SOT486-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;LQFP144: plastic low profile quad flat package; 144 leads; body 20 x 20 x 1.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-026
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;:  136E23&lt;/ul&gt;</description>
</package>
<package name="SOT108-1">
<description>&lt;li&gt;&lt;b&gt;SOT108-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO14: plastic small outline package; 14 leads; body width 3.9 mm; body thickness 1.47 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-012
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT162-1">
<description>&lt;li&gt;&lt;b&gt;SOT162-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO16: plastic small outline package; 16 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT163-1">
<description>&lt;li&gt;&lt;b&gt;SOT163-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO20: plastic small outline package; 20 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-013
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 075E04&lt;/ul&gt;</description>
</package>
<package name="SOT136-1">
<description>&lt;li&gt;&lt;b&gt;SOT136-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO28: plastic small outline package; 28 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-013
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 075E06&lt;/ul&gt;</description>
</package>
<package name="SOT176-1">
<description>&lt;li&gt;&lt;b&gt;SOT176-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO8: plastic small outline package; 8 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT109-2">
<description>&lt;li&gt;&lt;b&gt;SOT109-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO16: plastic small outline package; 16 leads; body width 3.9 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-012
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 076E07&lt;/ul&gt;</description>
</package>
<package name="SOT109-3">
<description>&lt;li&gt;&lt;b&gt;SOT109-3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO16: plastic small outline package; 16 leads; body width 3.9 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-012
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 076E07&lt;/ul&gt;</description>
</package>
<package name="SOT137-1">
<description>&lt;li&gt;&lt;b&gt;SOT137-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO24: plastic small outline package; 24 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-013
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 075E05&lt;/ul&gt;</description>
</package>
<package name="SOT287-1">
<description>&lt;li&gt;&lt;b&gt;SOT287-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO32: plastic small outline package; 32 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-119
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT449">
<description>&lt;li&gt;&lt;b&gt;SOT449&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SOJ40: plastic small outline package; 40 leads (J-bent); body width 10.16 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-027
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT865-3">
<description>&lt;li&gt;&lt;b&gt;SOT865-3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN32: plastic thermal enhanced very thin quad flat package; no leads; 32 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT618-1">
<description>&lt;li&gt;&lt;b&gt;SOT618-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN40: plastic thermal enhanced very thin quad flat package; no leads; 40 terminals; body 6 x 6 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1049">
<description>&lt;li&gt;&lt;b&gt;SOT1049&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XQFN10U: plastic extremely thin quad flat package; no leads; 10 terminals; UTLP based; body 2 x 1.55 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-255
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT909">
<description>&lt;li&gt;&lt;b&gt;SOT909&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;HVSON8: plastic thermal enhanced very thin small outline package; no leads;
8 terminals; body 4 x 4 x 0.85 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: MO-229 &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT402-1">
<description>&lt;li&gt;&lt;b&gt;SOT402-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP14: plastic thin shrink small outline package; 14 leads; body width 4.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT616">
<description>&lt;li&gt;&lt;b&gt;SOT616&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN24: plastic thermal enhanced very thin quad flat package; no leads; 24 terminals; body 4 x 4 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT617-3">
<description>&lt;li&gt;&lt;b&gt;SOT617-3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN32: plastic thermal enhanced very thin quad flat package; no leads; 32 terminals; body 5 x 5 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT619-1">
<description>&lt;li&gt;&lt;b&gt;SOT619-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT157">
<description>&lt;li&gt;&lt;b&gt;SOT157&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DBS9P: plastic DIL-bent-SIL power package; 9 leads (lead length 12 mm)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT523">
<description>&lt;li&gt;&lt;b&gt;SOT523&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DBS9P: plastic DIL-bent-SIL power package; 9 leads (lead length 12/11 mm); exposed die pad
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT141">
<description>&lt;li&gt;&lt;b&gt;SOT141&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;PDBS13P: plastic DIL-bent-SIL power package; 13 leads (lead length 12 mm)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT243">
<description>&lt;li&gt;&lt;b&gt;SOT243&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DBS17P: plastic DIL-bent-SIL power package; 17 leads (lead length 12 mm)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT411">
<description>&lt;li&gt;&lt;b&gt;SOT411&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DBS23P: plastic DIL-bent-SIL power package; 23 leads (straight lead length 3.2 mm)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT27">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT38">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT146">
<description>&lt;li&gt;&lt;b&gt;SOT146&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP20: plastic dual in-line package; 20 leads (300 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-001
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-603&lt;/ul&gt;</description>
</package>
<package name="SOT101">
<description>&lt;li&gt;&lt;b&gt;SOT101&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP24: plastic dual in-line package; 24 leads (600 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-015
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 051G02
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-509-24&lt;/ul&gt;</description>
</package>
<package name="SOT222">
<description>&lt;li&gt;&lt;b&gt;SOT222&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP24: plastic dual in-line package; 24 leads (300 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-001
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT117">
<description>&lt;li&gt;&lt;b&gt;SOT117&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP28: plastic dual in-line package; 28 leads (600 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-015
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 051G05
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-510-28&lt;/ul&gt;</description>
</package>
<package name="SOT129">
<description>&lt;li&gt;&lt;b&gt;SOT129&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP40: plastic dual in-line package; 40 leads (600 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-015
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 051G08
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-511-40&lt;/ul&gt;</description>
</package>
<package name="SOT240">
<description>&lt;li&gt;&lt;b&gt;SOT240&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP48: plastic dual in-line package; 48 leads (600 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-011
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT762">
<description>&lt;li&gt;&lt;b&gt;SOT762&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DHVQFN14: plastic dual in-line compatible thermal enhanced very thin quad flat package; no leads; 14 terminals; body 2.5 x 3 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-241
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT763">
<description>&lt;li&gt;&lt;b&gt;SOT763&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DHVQFN16: plastic dual in-line compatible thermal enhanced very thin quad flat package; no leads; 16 terminals; body 2.5 x 3.5 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-241
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT815">
<description>&lt;li&gt;&lt;b&gt;SOT815&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DHVQFN24: plastic dual in-line compatible thermal enhanced very thin quad flat package; no leads; 24 terminals; body 3.5 x 5.5 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT564">
<description>&lt;li&gt;&lt;b&gt;SOT564&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HBCC24: plastic thermal enhanced bottom chip carrier; 24 terminals; body 4 x 4 x 0.65 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-217 
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT360">
<description>&lt;li&gt;&lt;b&gt;SOT360&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP20: plastic thin shrink small outline package; 20 leads; body width 4.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: &lt;/ul&gt;</description>
</package>
<package name="SOT527">
<description>&lt;li&gt;&lt;b&gt;SOT527&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HTSSOP20: plastic thermal enhanced thin shrink small outline package; 20 leads; body width 4.4 mm; exposed die pad
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT487">
<description>&lt;li&gt;&lt;b&gt;SOT487&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP32: plastic thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT549-1">
<description>&lt;li&gt;&lt;b&gt;SOT549-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HTSSOP32: plastic thermal enhanced thin shrink small outline package; 32 leads;body width 6.1 mm; lead pitch 0.65 mm; exposed die pad
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;

MK</description>
</package>
<package name="SOT398">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT1194">
<description>&lt;li&gt;&lt;b&gt;SOT1194&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HUSON4: plastic thermal enhanced ultra thin small outline package; no leads;4 terminals; body 1 x 1 x 0.55 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1115">
<description>!!!!!!Experimental, not tested!!!!!!!!!!!! MK
&lt;li&gt;&lt;b&gt;SOT1115&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON6: extremely thin small outline package; no leads; 6 terminals; body 0.9 x 1.0 x 0.35 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT404">
<description>&lt;li&gt;&lt;b&gt;SOT404&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single-ended surface-mounted package (D2PAK); 3 leads (one lead cropped)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT684">
<description>&lt;li&gt;&lt;b&gt;SOT684&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN56: plastic thermal enhanced very thin quad flat package; no leads;56 terminals; body 8 x 8 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="JENNIC_QFN56">
<description>JENNIC QFN56, NO SOT number. Equals to HVQFN56 (SOT684)  without heatsink. Foutprint based on SOT684.</description>
</package>
<package name="NX3P190/NX3P191">
<description>&lt;li&gt;&lt;b&gt;NX3P190/NX3P191&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;WLCSP4: wafer level chip-size package. 4 bumps; body 0.76 x 0.76 x 0.51 mm. (Backside Coating included)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --  
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT428">
<description>&lt;li&gt;&lt;b&gt;SOT428&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single-ended surface-mounted package (DPAK); 3 leads (one lead cropped)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: TO-252
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-63&lt;/ul&gt;</description>
</package>
<package name="SOT629">
<description>&lt;li&gt;&lt;b&gt;SOT629&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN16: plastic thermal enhanced very thin quad flat package; no leads;
16 terminals; body 4 x 4 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;:  --&lt;/ul&gt;</description>
</package>
<package name="SOT758-1">
<description>&lt;li&gt;&lt;b&gt;SOT758-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN16: plastic thermal enhanced very thin quad flat package; no leads; 16 terminals; body 3 x 3 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT758-3">
<description>&lt;li&gt;&lt;b&gt;SOT758-3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN16: plastic thermal enhanced very thin quad flat package; no leads; 16 terminals; body 3 x 3 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT662">
<description>&lt;li&gt;&lt;b&gt;SOT662&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN20: plastic thermal enhanced very thin quad flat package; no leads; 20 terminals; body 5 x 5 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT788">
<description>&lt;li&gt;&lt;b&gt;SOT788&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN28: plastic thermal enhanced very thin quad flat package; no leads; 28 terminals; body 6 x 6 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT778-1">
<description>&lt;li&gt;&lt;b&gt;SOT778-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 6 x 6 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT778-4">
<description>&lt;li&gt;&lt;b&gt;SOT778-4&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 6 x 6 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT804-1">
<description>&lt;li&gt;&lt;b&gt;SOT804-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN64: plastic thermal enhanced very thin quad flat package; no leads; 64 terminals; body 9 x 9 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT804-2">
<description>&lt;li&gt;&lt;b&gt;SOT804-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN64: plastic thermal enhanced very thin quad flat package; no leads; 64 terminals; body 9 x 9 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT804-3">
<description>&lt;li&gt;&lt;b&gt;SOT804-3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN64: plastic thermal enhanced very thin quad flat package; no leads; 64 terminals; body 9 x 9 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT804-4">
<description>&lt;li&gt;&lt;b&gt;SOT804-4&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN64: plastic thermal enhanced very thin quad flat package; no leads; 64 terminals; body 9 x 9 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT650">
<description>&lt;li&gt;&lt;b&gt;SOT650&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVSON10: plastic thermal enhanced very thin small outline package; no leads; 10 terminals; body 3 x 3 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-229
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;:--&lt;/ul&gt;</description>
</package>
<package name="SOT994">
<description>&lt;li&gt;&lt;b&gt;SOT994&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HWQFN24: plastic thermal enhanced very very thin quad flat package; no leads; 24 terminals; body 4 x 4 x 0.75 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: 
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1031-2">
<description>&lt;li&gt;&lt;b&gt;SOT1031-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HWQFN48R: plastic thermal enhanced very very thin quad flat package; no leads 48 terminals; resin based; body 7 x 7 x 0.7 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1031-1">
<description>&lt;li&gt;&lt;b&gt;SOT1031-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HWQFN48R: plastic thermal enhanced very very thin quad flat package; no leads 48 terminals; resin based; body 7 x 7 x 0.7 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1046">
<description>&lt;li&gt;&lt;b&gt;SOT1046&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HXQFN16U: plastic thermal enhanced extremely thin quad flat package; no leads; 16 terminals; UTLP based; body 2 x 2 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1133-1">
<description>&lt;li&gt;&lt;b&gt;SOT1133-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HXQFN60U: plastic thermal enhanced extremely thin quad flat package; no leads; 60 terminals; UTLP based; body 5 x 5 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1134-1">
<description>&lt;li&gt;&lt;b&gt;SOT1134-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HXQFN60U: plastic thermal enhanced extremely thin quad flat package; no leads; 60 terminals; UTLP based; body 4 x 6 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT102">
<description>&lt;li&gt;&lt;b&gt;SOT102&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP18: plastic dual in-line package; 18 leads (300 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: MS-001
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT248">
<description>&lt;b&gt;Dual In Line&lt;/b&gt; 0.4 inch</description>
</package>
<package name="SOT135">
<description>&lt;li&gt;&lt;b&gt;SOT135&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Ceramic dual in-line package; 28 leads; glass seal
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT337">
<description>&lt;li&gt;&lt;b&gt;SOT337&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP14: plastic shrink small outline package; 14 leads; body width 5.3 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-150
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT338">
<description>&lt;li&gt;&lt;b&gt;SOT338&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP16: plastic shrink small outline package; 16 leads; body width 5.3 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-150
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT369">
<description>&lt;li&gt;&lt;b&gt;SOT369&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP16: plastic shrink small outline package; 16 leads; body width 4.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-152
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT266">
<description>&lt;li&gt;&lt;b&gt;SOT266&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP20: plastic shrink small outline package; 20 leads; body width 4.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-152
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT339">
<description>&lt;li&gt;&lt;b&gt;SOT339&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP20: plastic shrink small outline package; 20 leads; body width 5.3 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-150
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT340">
<description>&lt;li&gt;&lt;b&gt;SOT340&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP24: plastic shrink small outline package; 24 leads; body width 5.3 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-150
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT341">
<description>&lt;li&gt;&lt;b&gt;SOT341&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP28: plastic shrink small outline package; 28 leads; body width 5.3 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-150
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT519">
<description>&lt;li&gt;&lt;b&gt;SOT519&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;:  --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT556">
<description>&lt;li&gt;&lt;b&gt;SOT556&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP24: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-137
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;</description>
</package>
<package name="SOT370">
<description>&lt;li&gt;&lt;b&gt;SOT370&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SSOP48: plastic shrink small outline package; 48 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-118
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: &lt;/ul&gt;</description>
</package>
<package name="SOT549-3">
<description>&lt;li&gt;&lt;b&gt;SOT549-3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HTSSOP32: plastic thermal enhanced thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm; exposed die pad
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT619-2/3">
<description>&lt;li&gt;&lt;b&gt;SOT619-2/3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT619-4/8">
<description>&lt;li&gt;&lt;b&gt;SOT619-4/8&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT619-5/6">
<description>&lt;li&gt;&lt;b&gt;SOT619-5/6&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;

MK</description>
</package>
<package name="SOT619-7">
<description>&lt;li&gt;&lt;b&gt;SOT619-7&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;

MK</description>
</package>
<package name="SOT619-9">
<description>&lt;li&gt;&lt;b&gt;SOT619-9&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;

MK</description>
</package>
<package name="SOT619-11">
<description>&lt;li&gt;&lt;b&gt;SOT619-11&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;

MK</description>
</package>
<package name="SOT758-2">
<description>&lt;li&gt;&lt;b&gt;SOT758-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN16: plastic thermal enhanced very thin quad flat package; no leads; 16 terminals; body 3 x 3 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: -- &lt;/ul&gt;

MK</description>
</package>
<package name="SOT778-2">
<description>&lt;li&gt;&lt;b&gt;SOT778-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 6 x 6 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT778-3">
<description>&lt;li&gt;&lt;b&gt;SOT778-3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 6 x 6 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT778-5">
<description>&lt;li&gt;&lt;b&gt;SOT778-5&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN48: plastic thermal enhanced very thin quad flat package; no leads; 48 terminals; body 6 x 6 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT865-2">
<description>&lt;li&gt;&lt;b&gt;SOT865-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN32: plastic thermal enhanced very thin quad flat package; no leads; 32 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT865-1">
<description>&lt;li&gt;&lt;b&gt;SOT865-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HVQFN32: plastic thermal enhanced very thin quad flat package; no leads; 32 terminals; body 7 x 7 x 0.85 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-220
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1155-2">
<description>&lt;li&gt;&lt;b&gt;SOT1155-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TFBGA48: plastic thin fine-pitch ball grid array package; 48 balls; body 4.5 x 4.5 x 0.7 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1165-1">
<description>&lt;li&gt;&lt;b&gt;SOT1165-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON10: plastic, extremely thin small outline package; no leads; 10 terminals; body 1 x 2.5 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT753">
<description>SOT753 &lt;br&gt;</description>
</package>
<package name="SOT902">
<description>&lt;li&gt;&lt;b&gt;SOT902&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XQFN8U: plastic extremely thin quad flat package; no leads; 8 terminals; UTLP based; body 1.6 x 1.6 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOD323(F)">
<description>&lt;li&gt;&lt;b&gt;SOD323(F)&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 2 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-90&lt;/ul&gt;</description>
</package>
<package name="SOT666">
<description>&lt;b&gt;SOT 666 Reflow soldering foorprint&lt;/b&gt;&lt;p&gt;
Source: Philips - BAS70_1PS7XSB70_SER_8.pdf</description>
</package>
<package name="SOD68">
<description>&lt;li&gt;&lt;b&gt;SOD68&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Hermetically sealed glass package; axial leaded; 2 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: DO-34
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT323">
<description>&lt;li&gt;&lt;b&gt;SOT323&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 3 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-70&lt;/ul&gt;</description>
</package>
<package name="SOT416">
<description>&lt;li&gt;&lt;b&gt;SOT416&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 3 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-75&lt;/ul&gt;</description>
</package>
<package name="SOT54V">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="SOT54A">
</package>
<package name="SOT883(B)">
<description>&lt;li&gt;&lt;b&gt;SOT883(B)&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 3 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-101&lt;/ul&gt;

Remark: SOT883B has the same footprint, package is lower</description>
</package>
<package name="SOT490">
<description>&lt;li&gt;&lt;b&gt;SOT490&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 3 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-89&lt;/ul&gt;</description>
</package>
<package name="SOT1263">
<description>&lt;li&gt;&lt;b&gt;SOT1263&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Microlead ultra small surface-mounted plastic package; 3 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT54">
</package>
<package name="SOT116">
<description>&lt;li&gt;&lt;b&gt;SOT116&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP22: plastic dual in-line package; 22 leads (400 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-010
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 060G07
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-502-22&lt;/ul&gt;</description>
</package>
<package name="SOT111">
<description>&lt;li&gt;&lt;b&gt;SOT111&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DBS9MPF: plastic DIL-bent-SIL medium power package with fin; 9 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT247">
<description>&lt;li&gt;&lt;b&gt;SOT247&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SDIP52: plastic shrink dual in-line package; 52 leads (600 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-020
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT270">
<description>&lt;li&gt;&lt;b&gt;SOT270&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SDIP42: plastic shrink dual in-line package; 42 leads (600 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-020
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT274">
<description>&lt;li&gt;&lt;b&gt;SOT274&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SDIP64: plastic shrink dual in-line package; 64 leads (750 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-021
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT400">
<description>&lt;li&gt;&lt;b&gt;SOT400&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SDIP56: plastic shrink dual in-line package; 56 leads (600 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT110">
<description>&lt;li&gt;&lt;b&gt;SOT110&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SIL9MPF: plastic single in-line medium power package with fin; 9 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1188">
<description>&lt;li&gt;&lt;b&gt;SOT1188&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SIL4: plastic, single in-line package
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT131">
<description>&lt;li&gt;&lt;b&gt;SOT131&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SIL9P: plastic single in-line power package; 9 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT142">
<description>&lt;li&gt;&lt;b&gt;SOT142&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SIL9MP: plastic single in-line medium power package; 9 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT193">
<description>&lt;li&gt;&lt;b&gt;SOT193&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SIL13P: plastic single in-line power package; 13 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT352">
<description>&lt;li&gt;&lt;b&gt;SOT352&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;RBS9MPF: plastic rectangular-bent single in-line medium power package with fin; 9 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT578">
<description>&lt;li&gt;&lt;b&gt;SOT578&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TBS13P: plastic Triple-bent-SIL power package; 13 leads (lead length 7.7 mm)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT143(B)">
<description>&lt;li&gt;&lt;b&gt;SOT143(B)&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 4 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT23">
<description>&lt;li&gt;&lt;b&gt;SOT23&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 3 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: TO-236AB &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT680">
<description>&lt;li&gt;&lt;b&gt;SOT680&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;SO5: plastic small outline package; 5 leads; body width 1.6 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-178 &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="WL-CSP5">
</package>
<package name="SOT1118">
<description>&lt;li&gt;&lt;b&gt;SOT1118&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HUSON6: plastic, thermal enhanced ultra thin small outline package; no leads;6 terminals; body 2 x 2 x 0.65 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT996-2/3">
<description>&lt;li&gt;&lt;b&gt;SOT996-2/3&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON8U: plastic extremely thin small outline package; no leads;8 terminals; UTLP based; body 3 x 2 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: 
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1069-2">
<description>&lt;li&gt;&lt;b&gt;SOT1069&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HWSON8: plastic thermal enhanced very very thin small outline package; no leads;8 terminals; body 2 x 3 x 0.75 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: 
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT78">
<description>&lt;li&gt;&lt;b&gt;SOT78&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single-ended package; heatsink mounted; 1 mounting hole; 3-lead TO-220AB
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: 3-lead TO-220AB
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-46&lt;/ul&gt;</description>
</package>
<package name="SOT186A">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
<package name="SOT1210">
<description>&lt;li&gt;&lt;b&gt;SOT1210&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single ended surface mounted package (LFPAK33); 8 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: ---
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="SOT1134-2">
<description>&lt;li&gt;&lt;b&gt;SOT1134-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;HXQFN60U: plastic thermal enhanced extremely thin quad flat package; no leads; 60 terminals; UTLP based; body 4 x 6 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOD113">
<description>&lt;li&gt;&lt;b&gt;SOD113&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single-ended package; isolated heatsink mounted; 1 mounting hole; 2-lead TO-220 'full pack
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: 2-lead TO-220F
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT357-1">
<description>&lt;li&gt;&lt;b&gt;SOT357-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TQFP64: plastic thin quad flat package; 64 leads; body 10 x 10 x 1.0 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-026
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 137E10 
&lt;li&gt;&lt;u&gt;JEITA:  --&lt;/ul&gt;</description>
</package>
<package name="SOT1089-1">
<description>&lt;li&gt;&lt;b&gt;SOT1089-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON8: plastic, extremely thin small outline package; no leads; 8 terminals; body 1 x 1.35 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1160-1">
<description>&lt;li&gt;&lt;b&gt;SOT1160-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XQFN10: plastic, extremely thin quad flat package; no leads;10 terminals; body 1.40 x 1.80 x 0.50 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- 
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="MO-252">
</package>
<package name="SOT505-2">
<description>&lt;li&gt;&lt;b&gt;SOT505-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOD962">
</package>
<package name="SOD123F">
<description>&lt;li&gt;&lt;b&gt;SOD123F&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 2 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOD1608">
</package>
<package name="SOT1226">
<description>&lt;li&gt;&lt;b&gt;SOT1226&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;X2SON5: plastic thermal enhanced extremely thin small outline package; no leads;
5 terminals; body 0.8 x 0.8 x 0.35 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOD882(T)">
<description>&lt;li&gt;&lt;b&gt;SOD882(T)&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Leadless ultra small plastic package; 2 terminals; body 1.0 x 0.6 x 0.5 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT143R">
<description>&lt;li&gt;&lt;b&gt;SOT143R&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; reverse pinning; 4 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-61AA&lt;/ul&gt;</description>
</package>
<package name="SOD882D">
<description>&lt;li&gt;&lt;b&gt;SOT882D&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Leadless ultra small plastic package; 2 terminals; body 1 x 0.6 x 0.4 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT346">
<description>&lt;li&gt;&lt;b&gt;SOT346&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 3 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: TO-236 &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-59A&lt;/ul&gt;</description>
</package>
<package name="SOD123W">
<description>&lt;li&gt;&lt;b&gt;SOT123W&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 2 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1061">
<description>&lt;li&gt;&lt;b&gt;SOT1061&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;HUSON3: plastic thermal enhanced ultra thin small outline package; no leads;
3 terminals; body 2 x 2 x 0.65 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1220">
<description>&lt;li&gt;&lt;b&gt;SOT1220&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;DFN2020MD-6: plastic thermal enhanced ultra thin small outline package; no leads;
6 terminals; body 2 x 2 x 0.65 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1023">
<description>&lt;li&gt;&lt;b&gt;SOT1023&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic single-ended surface-mounted package (LFPAK); 4 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT873-1">
<description>&lt;li&gt;&lt;b&gt;SOT873-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DFN3333-8: plastic thermal enhanced very thin small outline package; no leads;
8 terminals; body 3.3 x 3.3 x 1.0 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT226">
<description>&lt;li&gt;&lt;b&gt;SOT226&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single-ended package (I2PAK); low-profile 3-lead TO-262
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: TO-262
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT429">
<description>&lt;li&gt;&lt;b&gt;SOT429&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single-ended through-hole package; heatsink mounted; 1 mounting hole; 3-lead TO-247
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: TO-247
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT765">
<description>&lt;li&gt;&lt;b&gt;SOT765&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;VSSOP8: plastic very thin shrink small outline package; 8 leads; body width 2.3 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-187
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1203">
<description>&lt;li&gt;&lt;b&gt;SOT1203&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON8: extremely thin small outline package; no leads;
8 terminals; body 1.35 x 1.0 x 0.35 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT833-1">
<description>&lt;li&gt;&lt;b&gt;SOT833-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON8: plastic extremely thin small outline package; no leads; 8 terminals; body 1 x 1.95 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-252
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1081">
<description>&lt;li&gt;&lt;b&gt;SOT1081-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON10U: plastic extremely thin small outline package; no leads;
10 terminals; UTLP based; body 1 x 1.7 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1122">
<description>&lt;li&gt;&lt;b&gt;SOT1122&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON3: plastic extremely thin small outline package; no leads; 3 terminals; body 1 x 1.45 x 0.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-252
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT617-9">
</package>
<package name="SOT486-1MK">
</package>
<package name="SOT355-1">
<description>&lt;li&gt;&lt;b&gt;SOT355-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP24: plastic thin shrink small outline package; 24 leads; body width 4.4 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1199-1">
<description>&lt;li&gt;&lt;b&gt;SOT1199-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;VFBGA24: plastic very thin fine-pitch ball grid array package;
24 balls; body 3 x 3 x 0.65 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT1176">
<description>&lt;li&gt;&lt;b&gt;SOT1176&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;XSON10: plastic extremely thin small outline package; no leads;
10 terminals; body 1 x 2.5 x 0.5 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
</packages>
<symbols>
<symbol name="LPC1XXX-V7-INTERNAL_LPC115X">
<pin name="NRESET/PIO0_13/EZH13"/>
<pin name="NTRST/PIO1_1/AD3"/>
<pin name="PIO0_0/EZH0/NRTS0"/>
<pin name="PIO0_1/EZH1/RXD0/CT32B0_0"/>
<pin name="PIO0_2/EZH2/TXD0/CT32B0_1"/>
<pin name="PIO0_3/EZH3/NDTR0/CT32B0_2"/>
<pin name="PIO0_4/EZH4/NDSR0/CT32B0_3"/>
<pin name="PIO0_5/EZH5/NDCD0"/>
<pin name="PIO0_6/EZH6/NRI0/CT32B1_0"/>
<pin name="PIO0_7/EZH7/NCTS0/CT32B1_1"/>
<pin name="PIO0_8/EZH8/RXD1/CT32B1_2"/>
<pin name="PIO0_9/EZH9/TXD1/CT32B1_3"/>
<pin name="PIO0_10/EZH10/SCL"/>
<pin name="PIO0_11/EZH11/SDA/CT16B0_0"/>
<pin name="PIO0_12/EZH12/CLKOUT/CT16B0_1"/>
<pin name="PIO0_14/EZH14/SCK"/>
<pin name="PIO0_15/EZH15/SSEL/CT16B1_0"/>
<pin name="PIO0_16/EZH0/MISO/CT16B1_1"/>
<pin name="PIO0_17/EZH1/MOSI"/>
<pin name="PIO0_19/EZH3/C0_IN0/CT32B0_1"/>
<pin name="PIO0_20/EZH4/C0_IN1/CT32B0_2"/>
<pin name="PIO0_21/EZH5/C0_IN2/CT32B0_3"/>
<pin name="PIO0_22/EZH6/C0_IN3"/>
<pin name="PIO0_23/EZH7/C1_IN0/CT32B1_0"/>
<pin name="PIO0_24/EZH8/C1_IN1/CT32B1_1"/>
<pin name="PIO0_25/EZH9/C1_IN2/CT32B1_2/SWDIO"/>
<pin name="PIO0_26/EZH10/C1_IN3/CT32B1_3/SWCLK"/>
<pin name="PIO0_27/EZH11/C0_OUT"/>
<pin name="PIO0_28/EZH12/C1_OUT/CT16B0_0"/>
<pin name="PIO0_29/EZH13/ROSC/CT16B0_1"/>
<pin name="PIO1_3/AD5/WAKEUP"/>
<pin name="PIO1_4/AD6"/>
<pin name="PIO1_5/AD7/CT16B1_0"/>
<pin name="PIO1_6/CT16B1_1"/>
<pin name="PIO2_0/EZH0/CT16B0_0"/>
<pin name="PIO2_1/EZH1/CT16B0_1"/>
<pin name="PIO2_2/EZH2/CT16B1_0"/>
<pin name="PIO2_3/EZH3/CT16B1_1"/>
<pin name="PIO2_4/EZH4/CT32B0_0"/>
<pin name="PIO2_5/EZH5/CT32B0_1"/>
<pin name="PIO2_6/EZH6/CT32B0_2"/>
<pin name="PIO2_7/EZH7/CT32B0_3"/>
<pin name="PIO2_8/EZH8/CT32B1_0"/>
<pin name="PIO2_9/EZH9/CT32B1_1"/>
<pin name="PIO2_10/EZH10/CT32B1_2"/>
<pin name="PIO2_11/EZH11/CT32B1_3"/>
<pin name="PIO2_12/EZH12"/>
<pin name="PIO2_13/EZH13"/>
<pin name="PIO2_14/EZH14"/>
<pin name="PIO2_15/EZH15"/>
<pin name="RTCXIN"/>
<pin name="RTCXOUT"/>
<pin name="SWCLK/PIO0_18/EZH2/CT32B0_0"/>
<pin name="SWDIO/PIO1_2/AD4"/>
<pin name="TDI/PIO0_31/EZH15/AD1"/>
<pin name="TDO/PIO0_30/EZH14/AD0"/>
<pin name="TMS/PIO1_0/AD2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="VREF_CMP"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
</symbol>
<symbol name="STARBUCK_TEA1721">
<pin name="DRN" direction="out"/>
<pin name="FB"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="SRC" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PCF8885">
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="CLK_IN" direction="in" function="clk"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="INT_IN" direction="in" function="dot"/>
<pin name="INT" direction="out" function="dot"/>
<pin name="TEST" direction="in"/>
<pin name="SLEEP" direction="in"/>
<pin name="CLK_OUT" direction="out"/>
<pin name="CPC7" direction="pas"/>
<pin name="CPC6" direction="pas"/>
<pin name="CPC5" direction="pas"/>
<pin name="CPC4" direction="pas"/>
<pin name="CPC3" direction="pas"/>
<pin name="CPC2" direction="pas"/>
<pin name="CPC1" direction="pas"/>
<pin name="CPC0" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD_IRD" direction="pwr"/>
</symbol>
<symbol name="TRIAC">
<pin name="CM" direction="pas"/>
<pin name="LD" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="TRIAC_TRIAC4P">
<pin name="CM@2" direction="pas"/>
<pin name="CM@1" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="LD" direction="pas"/>
</symbol>
<symbol name="DOT">
</symbol>
<symbol name="DIODE">
<description>Diode</description>
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="ESD-PROTECTION_ESD">
<pin name="ESD1" direction="pas"/>
<pin name="ESD2" direction="pas"/>
<pin name="ESD3" direction="pas"/>
<pin name="ESD4" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LPC12XX_48P">
<pin name="!RESET!/PIO0_13/EZH13"/>
<pin name="!TRST!/PIO1_1/AD3"/>
<pin name="PIO0_0/EZH0/!RTS0!"/>
<pin name="PIO0_1/EZH1/RXD0/CT32B0_0"/>
<pin name="PIO0_2/EZH2/TXD0/CT32B0_1"/>
<pin name="PIO0_3/EZH3/!DTR0!/CT32B0_2"/>
<pin name="PIO0_4/EZH4/!DSR0!/CT32B0_3"/>
<pin name="PIO0_5/EZH5/!DCD0!"/>
<pin name="PIO0_6/EZH6/!RI0!/CT32B1_0"/>
<pin name="PIO0_7/EZH7/!CTS0!/CT32B1_1"/>
<pin name="PIO0_8/EZH8/RXD1/CT32B1_2"/>
<pin name="PIO0_9/EZH9/TXD1/CT32B1_3"/>
<pin name="PIO0_10/EZH10/SCL"/>
<pin name="PIO0_11/EZH11/SDA/CT16B0_0"/>
<pin name="PIO0_12/EZH12/CLKOUT/CT16B0_1"/>
<pin name="PIO0_14/EZH14/SCK"/>
<pin name="PIO0_15/EZH15/SSEL/CT16B1_0"/>
<pin name="PIO0_16/EZH0/MISO/CT16B1_1"/>
<pin name="PIO0_17/EZH1/MOSI"/>
<pin name="PIO0_19/EZH3/C0_IN0/CT32B0_1"/>
<pin name="PIO0_20/EZH4/C0_IN1/CT32B0_2"/>
<pin name="PIO0_21/EZH5/C0_IN2/CT32B0_3"/>
<pin name="PIO0_22/EZH6/C0_IN3"/>
<pin name="PIO0_23/EZH7/C1_IN0/CT32B1_0"/>
<pin name="PIO0_24/EZH8/C1_IN1/CT32B1_1"/>
<pin name="PIO0_25/EZH9/C1_IN2/CT32B1_2/SWDIO"/>
<pin name="PIO0_26/EZH10/C1_IN3/CT32B1_3/SWCLK"/>
<pin name="PIO0_27/EZH11/C0_OUT"/>
<pin name="PIO0_28/EZH12/C1_OUT/CT16B0_0"/>
<pin name="PIO0_29/EZH13/ROSC/CT16B0_1"/>
<pin name="PIO1_3/AD5/WAKEUP"/>
<pin name="PIO1_4/AD6"/>
<pin name="PIO1_5/AD7/CT16B1_0"/>
<pin name="PIO1_6/CT16B1_1"/>
<pin name="RTCXIN"/>
<pin name="RTCXOUT"/>
<pin name="SWCLK/PIO0_18/EZH2/CT32B0_0"/>
<pin name="SWDIO/PIO1_2/AD4"/>
<pin name="TDI/PIO0_31/EZH15/AD1"/>
<pin name="TDO/PIO0_30/EZH14/AD0"/>
<pin name="TMS/PIO1_0/AD2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="VREF_CMP"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
</symbol>
<symbol name="CLRC663">
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="GPIO0"/>
<pin name="SIGOUT" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AVDD" direction="out"/>
<pin name="AUX1" direction="out"/>
<pin name="AUX2" direction="out"/>
<pin name="RXP" direction="out"/>
<pin name="RXN" direction="out"/>
<pin name="VMID" direction="out"/>
<pin name="TX2" direction="out"/>
<pin name="TVSS" direction="pwr"/>
<pin name="TX1" direction="out"/>
<pin name="TVDD" direction="pwr"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="PDOWN" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="SCL2"/>
<pin name="SDA2"/>
<pin name="PVDD" direction="pwr"/>
<pin name="IFSEL0" direction="in"/>
<pin name="IFSEL1" direction="in"/>
<pin name="IF0"/>
<pin name="IF1"/>
<pin name="IF2"/>
<pin name="IRQ" direction="out"/>
<pin name="IF3-SDA"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="DIODE_SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="LPC1114FHN33">
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO3_4"/>
<pin name="PIO3_5"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/!RTS!/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LPC1313FBD48">
<pin name="PIO2_6"/>
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_1/DSR"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO3_4"/>
<pin name="PIO2_4"/>
<pin name="PIO2_5"/>
<pin name="PIO3_5"/>
<pin name="PIO0_6/USB_CONNECT/SCK"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_2/DCD"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="PIO2_11/SCK"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="PIO3_0"/>
<pin name="PIO3_1"/>
<pin name="PIO2_3/RI"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO3_3"/>
</symbol>
<symbol name="LPC1313FHN33">
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO3_4"/>
<pin name="PIO3_5"/>
<pin name="PIO0_6/SCK"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LPC1343FHN33">
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO0_6/USB_CONNECT/SCK"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LPC1343FBD48">
<pin name="PIO2_6"/>
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_1/DSR"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO2_4"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO2_5"/>
<pin name="PIO0_6/USB_CONNECT/SCK"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_2/DCD"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="PIO2_11/SCK"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="PIO3_0"/>
<pin name="PIO3_1"/>
<pin name="PIO2_3/RI"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO3_3"/>
</symbol>
<symbol name="LPC175X">
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
<pin name="VDD(3V3)3" direction="pwr"/>
<pin name="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
<pin name="VDD(3V3)2" direction="pwr"/>
<pin name="P2[10]/EINT0/NMI"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VREFP" direction="in"/>
<pin name="RSTOUT" direction="out"/>
<pin name="VREFN" direction="in"/>
<pin name="RTCX1" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="RTCX2" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="P1[31]/SCK1/AD0[5]"/>
<pin name="P1[30]/VBUS/AD0[4]"/>
<pin name="P0[30]/USB_DMIN"/>
<pin name="VSS1" direction="pwr"/>
<pin name="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/MCOA0/USB_PPWR/CAP1[1]"/>
<pin name="P1[20]/MCI0/PWM1[2]/SCK0"/>
<pin name="P1[22]/MCOB0/USB_PWRD/MAT1[0]"/>
<pin name="P1[23]/MCI1/PWM1[4]/MISO0"/>
<pin name="P1[24]/MCI2/PWM1[5]/MOSI0"/>
<pin name="P1[25]/MCOA1/MAT1[1]"/>
<pin name="P1[26]/MCOB1/PWM1[6]/CAP0[0]"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD(REG)(3V3)1" direction="pwr"/>
<pin name="P1[28]/MCOA2/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/MCOB2/PCAP1[1]/MAT0[1]"/>
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="VSS3" direction="pwr"/>
<pin name="P0[22]/RTS1/TD1"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P2[9]/USB_CONNECT/RXD2/ENET_MDIO"/>
<pin name="P2[8]/TD2/TXD2/ENET_MDC"/>
<pin name="P2[7]/RD2/RTS1"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
<pin name="VDDA" direction="pwr"/>
<pin name="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
<pin name="VSS4" direction="pwr"/>
<pin name="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
<pin name="P0[7]/I2STX_CLK/SCK1/MAT2[1]"/>
<pin name="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]"/>
<pin name="P4[28]/RX_MCLK/MAT2[0]/TXD3"/>
<pin name="VSS5" direction="pwr"/>
<pin name="VDD(REG)(3V3)2" direction="pwr"/>
<pin name="P4[29]/TX_MCLK/MAT2[1]/RXD3"/>
<pin name="P1[15]/ENET_REF_CLK"/>
<pin name="P1[9]/ENET_RXD0"/>
<pin name="P1[14]/ENET_RX_ER"/>
<pin name="P1[10]/ENET_RXD1"/>
<pin name="P1[8]/ENET_CRS"/>
<pin name="P1[4]/ENET_TX_EN"/>
<pin name="P1[1]/ENET_TXD1"/>
<pin name="P1[0]/ENET_TXD0"/>
<pin name="VDD(3V3)4" direction="pwr"/>
<pin name="VSS6" direction="pwr"/>
<pin name="TDO/SWO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VDD(3V3)1" direction="pwr"/>
<pin name="P0[29]/USB_DPLUS"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="TCK/SWDCLK"/>
<pin name="P2[1]/PWM1[2]/RXD1"/>
<pin name="P2[0]/PWM1[1]/TXD1"/>
<pin name="P0[9]/I2STX_SDA/MOSI1/MAT2[3]"/>
<pin name="P0[8]/I2STX_WS/MISO1/MAT2[2]"/>
<pin name="P0[2]/TXD0/AD0[7]"/>
<pin name="P0[3]/RXD0/AD0[6]"/>
</symbol>
<symbol name="LPC176X">
<pin name="TDO/SWO"/>
<pin name="TDI"/>
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
<pin name="TCK/SWDCLK"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
<pin name="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]"/>
<pin name="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]"/>
<pin name="VDDA"/>
<pin name="VSSA"/>
<pin name="VREFP"/>
<pin name="NC"/>
<pin name="RSTOUT"/>
<pin name="VREFN"/>
<pin name="RTCX1"/>
<pin name="RESET"/>
<pin name="RTCX2"/>
<pin name="VBAT"/>
<pin name="P1[31]/SCK1/AD0[5]"/>
<pin name="P1[30]/VBUS/AD0[4]"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="P0[28]/SCL0/USB_SCL"/>
<pin name="P0[27]/SDA0/USB_SDA"/>
<pin name="P3[26]/STCLK/MAT0[1]/PWM1[3]"/>
<pin name="P3[25]/MAT0[0]/PWM1[2]"/>
<pin name="VDD(3V3)@1"/>
<pin name="P0[29]/USB_DPLUS"/>
<pin name="P0[30]/USB_DMINUS"/>
<pin name="VSS1"/>
<pin name="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/MCOA0/USB_PPWR/CAP1[1]"/>
<pin name="P1[20]/MCI0/PWM1[2]/SCK0"/>
<pin name="P1[21]/MCABORT/PWM1[3]/SSEL0"/>
<pin name="P1[22]/MCOB0/USB_PWRD/MAT1[0]"/>
<pin name="P1[23]/MCI1/PWM1[4]/MISO0"/>
<pin name="P1[24]/MCI2/PWM1[5]/MOSI0"/>
<pin name="P1[25]/MCOA1/MAT1[1]"/>
<pin name="P1[26]/MCOB1/PWM1[6]/CAP0[0]"/>
<pin name="VSS2"/>
<pin name="VDD(REG)(3V3)@1"/>
<pin name="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]"/>
<pin name="P1[28]/MCOA2/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/MCOB2/PCAP1[1]/MAT0[1]"/>
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P2[13]/EINT3/I2STX_SDA"/>
<pin name="P2[12]/EINT2/I2STX_WS"/>
<pin name="P2[11]/EINT1/I2STX_CLK"/>
<pin name="P2[10]/EINT0/NMI"/>
<pin name="VDD(3V3)@2"/>
<pin name="VSS3"/>
<pin name="P0[22]/RTS1/TD1"/>
<pin name="P0[21]/RI1/RD1"/>
<pin name="P0[20]/DTR1/SCL1"/>
<pin name="P0[19]/DSR1/SDA1"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P2[9]/USB_CONNECT/RXD2/ENET_MDIO"/>
<pin name="P2[8]/TD2/TXD2/ENET_MDC"/>
<pin name="P2[7]/RD2/RTS1"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
<pin name="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
<pin name="VDD(3V3)@3"/>
<pin name="VSS4"/>
<pin name="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
<pin name="P2[1]/PWM1[2]/RXD1"/>
<pin name="P2[0]/PWM1[1]/TXD1"/>
<pin name="P0[9]/I2STX_SDA/MOSI1/MAT2[3]"/>
<pin name="P0[8]/I2STX_WS/MISO1/MAT2[2]"/>
<pin name="P0[7]/I2STX_CLK/SCK1/MAT2[1]"/>
<pin name="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]"/>
<pin name="P0[5]/I2SRX_WS/TD2/CAP2[1]"/>
<pin name="P0[4]/I2SRX_CLK/RD2/CAP2[0]"/>
<pin name="P4[28]/RX_MCLK/MAT2[0]/TXD3"/>
<pin name="VSS6"/>
<pin name="VDD(REG)(3V3)@2"/>
<pin name="P4[29]/TX_MCLK/MAT2[1]/RXD3"/>
<pin name="P1[17]/ENET_MDIO"/>
<pin name="P1[16]/ENET_MDC"/>
<pin name="P1[15]/ENET_REF_CLK"/>
<pin name="P1[14]/ENET_RX_ER"/>
<pin name="P1[10]/ENET_RXD1"/>
<pin name="P1[9]/ENET_RXD0"/>
<pin name="P1[8]/ENET_CRS"/>
<pin name="P1[4]/ENET_TX_EN"/>
<pin name="P1[1]/ENET_TXD1"/>
<pin name="P1[0]/ENET_TXD0"/>
<pin name="VDD(3V3)@4"/>
<pin name="VSS5"/>
<pin name="P0[2]/TXD0/AD0[7]"/>
<pin name="P0[3]/RXD0/AD0[6]"/>
<pin name="RTCK"/>
</symbol>
<symbol name="LPC1768FET">
<pin name="TDO/SWO"/>
<pin name="TDI"/>
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
<pin name="TCK/SWDCLK"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
<pin name="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]"/>
<pin name="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]"/>
<pin name="VDDA"/>
<pin name="VSSA"/>
<pin name="VREFP"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="VREFN"/>
<pin name="RTCX1"/>
<pin name="RESET"/>
<pin name="RTCX2"/>
<pin name="VBAT"/>
<pin name="P1[31]/SCK1/AD0[5]"/>
<pin name="P1[30]/VBUS/AD0[4]"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="P0[28]/SCL0/USB_SCL"/>
<pin name="P0[27]/SDA0/USB_SDA"/>
<pin name="P3[26]/STCLK/MAT0[1]/PWM1[3]"/>
<pin name="P3[25]/MAT0[0]/PWM1[2]"/>
<pin name="VDD(3V3)@1"/>
<pin name="P0[29]/USB_DPLUS"/>
<pin name="P0[30]/USB_DMINUS"/>
<pin name="VSS@1"/>
<pin name="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/MCOA0/USB_PPWR/CAP1[1]"/>
<pin name="P1[20]/MCI0/PWM1[2]/SCK0"/>
<pin name="P1[21]/MCABORT/PWM1[3]/SSEL0"/>
<pin name="P1[22]/MCOB0/USB_PWRD/MAT1[0]"/>
<pin name="P1[23]/MCI1/PWM1[4]/MISO0"/>
<pin name="P1[24]/MCI2/PWM1[5]/MOSI0"/>
<pin name="P1[25]/MCOA1/MAT1[1]"/>
<pin name="P1[26]/MCOB1/PWM1[6]/CAP0[0]"/>
<pin name="VSS@2"/>
<pin name="VDD(REG)(3V3)@1"/>
<pin name="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]"/>
<pin name="P1[28]/MCOA2/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/MCOB2/PCAP1[1]/MAT0[1]"/>
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P2[13]/EINT3/I2STX_SDA"/>
<pin name="P2[12]/EINT2/I2STX_WS"/>
<pin name="P2[11]/EINT1/I2STX_CLK"/>
<pin name="P2[10]/EINT0/NMI"/>
<pin name="VDD(3V3)@2"/>
<pin name="VSS@3"/>
<pin name="P0[22]/RTS1/TD1"/>
<pin name="P0[21]/RI1/RD1"/>
<pin name="P0[20]/DTR1/SCL1"/>
<pin name="P0[19]/DSR1/SDA1"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P2[9]/USB_CONNECT/RXD2/ENET_MDIO"/>
<pin name="P2[8]/TD2/TXD2/ENET_MDC"/>
<pin name="P2[7]/RD2/RTS1"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
<pin name="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
<pin name="VDD(3V3)@3"/>
<pin name="VSS@4"/>
<pin name="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
<pin name="P2[1]/PWM1[2]/RXD1"/>
<pin name="P2[0]/PWM1[1]/TXD1"/>
<pin name="P0[9]/I2STX_SDA/MOSI1/MAT2[3]"/>
<pin name="P0[8]/I2STX_WS/MISO1/MAT2[2]"/>
<pin name="P0[7]/I2STX_CLK/SCK1/MAT2[1]"/>
<pin name="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]"/>
<pin name="P0[5]/I2SRX_WS/TD2/CAP2[1]"/>
<pin name="P0[4]/I2SRX_CLK/RD2/CAP2[0]"/>
<pin name="P4[28]/RX_MCLK/MAT2[0]/TXD3"/>
<pin name="VSS@6"/>
<pin name="VDD(REG)(3V3)@2"/>
<pin name="P4[29]/TX_MCLK/MAT2[1]/RXD3"/>
<pin name="P1[17]/ENET_MDIO"/>
<pin name="P1[16]/ENET_MDC"/>
<pin name="P1[15]/ENET_REF_CLK"/>
<pin name="P1[14]/ENET_RX_ER"/>
<pin name="P1[10]/ENET_RXD1"/>
<pin name="P1[9]/ENET_RXD0"/>
<pin name="P1[8]/ENET_CRS"/>
<pin name="P1[4]/ENET_TX_EN"/>
<pin name="P1[1]/ENET_TXD1"/>
<pin name="P1[0]/ENET_TXD0"/>
<pin name="VDD(3V3)@4"/>
<pin name="VSS@5"/>
<pin name="P0[2]/TXD0/AD0[7]"/>
<pin name="P0[3]/RXD0/AD0[6]"/>
<pin name="RTCK"/>
</symbol>
<symbol name="NX1117">
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="ADJ" direction="pas"/>
<pin name="VOUT1" direction="out"/>
</symbol>
<symbol name="NX1117GND">
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT1" direction="out"/>
</symbol>
<symbol name="MICRO-PHILIPS_EEPROM">
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="PTC"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="VCC" direction="pwr"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="I2CDRIVER">
<pin name="SDAI"/>
<pin name="SCLI"/>
<pin name="EN" direction="in"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="DIR" direction="in"/>
</symbol>
<symbol name="PCA9646">
<pin name="SC1"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="SD2"/>
<pin name="SD1"/>
<pin name="SD0"/>
<pin name="SC3"/>
<pin name="SC2"/>
<pin name="SC0"/>
<pin name="SD3"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="OPAMP+-">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="THERMAL">
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="TEA1795">
<pin name="SSB" direction="in"/>
<pin name="SSA" direction="in"/>
<pin name="DSA" direction="in"/>
<pin name="DSB" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GDA" direction="out"/>
<pin name="GDB" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="CBTL12131">
<pin name="ML_C_3P"/>
<pin name="ML_C_2P"/>
<pin name="ML_C_1P"/>
<pin name="ML_C_0P"/>
<pin name="ML_D_3P"/>
<pin name="ML_D_2P"/>
<pin name="ML_D_1P"/>
<pin name="ML_D_0P"/>
<pin name="ML_A_3P"/>
<pin name="ML_A_2P"/>
<pin name="ML_A_1P"/>
<pin name="ML_A_0P"/>
<pin name="ML_B_3P"/>
<pin name="ML_B_2P"/>
<pin name="ML_B_1P"/>
<pin name="ML_B_0P"/>
<pin name="ML_C_3N"/>
<pin name="ML_C_2N"/>
<pin name="ML_C_1N"/>
<pin name="ML_C_0N"/>
<pin name="ML_D_3N"/>
<pin name="ML_D_2N"/>
<pin name="ML_D_1N"/>
<pin name="ML_D_0N"/>
<pin name="ML_A_3N"/>
<pin name="ML_A_2N"/>
<pin name="ML_A_1N"/>
<pin name="ML_A_0N"/>
<pin name="ML_B_3N"/>
<pin name="ML_B_2N"/>
<pin name="ML_B_1N"/>
<pin name="ML_B_0N"/>
<pin name="AUX_C_P"/>
<pin name="AUX_C_N"/>
<pin name="AUX_D_P"/>
<pin name="AUX_D_N"/>
<pin name="HPD_C" direction="out"/>
<pin name="HPD_D" direction="in"/>
<pin name="LV5" direction="in"/>
<pin name="PL5" direction="in"/>
<pin name="EQ5" direction="in"/>
<pin name="AUX_A_P"/>
<pin name="AUX_A_N"/>
<pin name="AUX_B_P"/>
<pin name="AUX_B_N"/>
<pin name="DDC_A_1"/>
<pin name="DDC_A_0"/>
<pin name="HPD_A" direction="out"/>
<pin name="HPD_B"/>
<pin name="AUX_TERM_SRC" direction="in"/>
<pin name="AUX_TERM_SNK" direction="in"/>
<pin name="AUX_B_P_STATE" direction="out"/>
<pin name="AUX_B_N_STATE" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="PATH_SEL" direction="in"/>
<pin name="DDC_AUX_SEL" direction="in"/>
<pin name="TST_REXT" direction="in"/>
<pin name="HPD_B_FLT" direction="out"/>
</symbol>
<symbol name="N-MOSFET_3S">
<pin name="S@1" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S@2" direction="pas"/>
<pin name="S@3" direction="pas"/>
</symbol>
<symbol name="74AUP1T57">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="CBTL06DP212">
<pin name="IN1_0+" direction="in"/>
<pin name="IN1_0-" direction="in"/>
<pin name="IN1_1+" direction="in"/>
<pin name="IN1_1-" direction="in"/>
<pin name="OUT_0+"/>
<pin name="OUT_0-"/>
<pin name="OUT_1+"/>
<pin name="OUT_1-"/>
<pin name="IN1_2+" direction="in"/>
<pin name="IN1_2-" direction="in"/>
<pin name="IN1_3+" direction="in"/>
<pin name="IN1_3-" direction="in"/>
<pin name="OUT_2+"/>
<pin name="OUT_2-"/>
<pin name="OUT_3+"/>
<pin name="OUT_3-"/>
<pin name="AUX+"/>
<pin name="AUX-"/>
<pin name="HPD_2" direction="in"/>
<pin name="GPU_SEL" direction="in"/>
<pin name="HPD_1" direction="in"/>
<pin name="HPDIN" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="DDC_AUX_SEL" direction="in"/>
<pin name="TST0" direction="in"/>
<pin name="IN2_0+" direction="in"/>
<pin name="IN2_0-" direction="in"/>
<pin name="IN2_1+" direction="in"/>
<pin name="IN2_1-" direction="in"/>
<pin name="IN2_2+" direction="in"/>
<pin name="IN2_2-" direction="in"/>
<pin name="IN2_3+" direction="in"/>
<pin name="IN2_3-" direction="in"/>
<pin name="AUX1+" direction="in"/>
<pin name="AUX1-" direction="in"/>
<pin name="AUX2+" direction="in"/>
<pin name="AUX2-" direction="in"/>
<pin name="DDC_CLK1" direction="in"/>
<pin name="DDC_CLK2" direction="in"/>
<pin name="DDC_DAT1" direction="in"/>
<pin name="DDC_DAT2" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
</symbol>
<symbol name="TEA1713">
<pin name="COMPPFC" direction="pas"/>
<pin name="SNSMAINS" direction="pas"/>
<pin name="SNSAUXPFC" direction="pas"/>
<pin name="SNSCURPFC" direction="pas"/>
<pin name="SNSOUT" direction="out"/>
<pin name="SUPIC" direction="pwr"/>
<pin name="GATEPFC" direction="out"/>
<pin name="SUPREG" direction="pas"/>
<pin name="GATELS" direction="out"/>
<pin name="NC@1" direction="out"/>
<pin name="SUPHV" direction="in"/>
<pin name="GATEHS" direction="out"/>
<pin name="SUPHS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="NC@2" direction="out"/>
<pin name="SNSCURHBC" direction="out"/>
<pin name="CFMIN" direction="pas"/>
<pin name="RFMAX" direction="pas"/>
<pin name="SNSFB" direction="in"/>
<pin name="SSHBC/EN" direction="in"/>
<pin name="RCPROT" direction="pas"/>
<pin name="SNSBOOST" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="SGND" direction="pwr"/>
</symbol>
<symbol name="NX3L2467">
<pin name="1Y0" direction="in"/>
<pin name="1Y1" direction="in"/>
<pin name="2Y0" direction="in"/>
<pin name="2Y1" direction="in"/>
<pin name="3Y0" direction="in"/>
<pin name="3Y1" direction="in"/>
<pin name="4Y0" direction="in"/>
<pin name="4Y1" direction="in"/>
<pin name="1Z" direction="out"/>
<pin name="2Z" direction="out"/>
<pin name="3Z" direction="out"/>
<pin name="4Z" direction="out"/>
<pin name="1S" direction="in"/>
<pin name="2S" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="CBTL02043">
<pin name="A0_P"/>
<pin name="A0_N"/>
<pin name="A1_P"/>
<pin name="A1_N"/>
<pin name="B1_N"/>
<pin name="B1_P"/>
<pin name="B0_N"/>
<pin name="B0_P"/>
<pin name="C1_N"/>
<pin name="C1_P"/>
<pin name="C0_N"/>
<pin name="C0_P"/>
<pin name="SEL" direction="in"/>
<pin name="XSD" direction="in"/>
<pin name="VDD@1"/>
<pin name="VDD@2"/>
<pin name="VDD@3"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
</symbol>
<symbol name="TEA1753">
<pin name="HV"/>
<pin name="HVS"/>
<pin name="PFCTIMER"/>
<pin name="FBDRIVER"/>
<pin name="PFCDRIVER"/>
<pin name="PFCSENSE"/>
<pin name="FBSENSE"/>
<pin name="VOSENSE"/>
<pin name="PFCAUX"/>
<pin name="VINSENSE"/>
<pin name="PFCCOMP"/>
<pin name="LATCH"/>
<pin name="FBAUX"/>
<pin name="FBCTRL"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="TEA1791">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SRSENSE"/>
<pin name="DRIVER" direction="out"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
</symbol>
<symbol name="TEA1738T">
<pin name="PROTECT" direction="in"/>
<pin name="VINSENSE" direction="in"/>
<pin name="DRIVER" direction="out"/>
<pin name="ISENSE" direction="in"/>
<pin name="CTRL" direction="in"/>
<pin name="OPTIMER" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AMP">
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2@2" direction="pwr"/>
<pin name="GND2@1" direction="pwr"/>
</symbol>
<symbol name="PCF8523">
<pin name="OSCO" direction="pas"/>
<pin name="OSCI" direction="pas"/>
<pin name="INT1" direction="out" function="dot"/>
<pin name="VDD" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
</symbol>
<symbol name="PCF8523TS">
<pin name="OSCO" direction="pas"/>
<pin name="OSCI" direction="pas"/>
<pin name="INT1" direction="out" function="dot"/>
<pin name="VDD" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="INT2" direction="out" function="dot"/>
<pin name="CLKOUT" direction="out"/>
</symbol>
<symbol name="TRIAC_TOP_2CM">
<pin name="CM@1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="CM@2" direction="pas"/>
</symbol>
<symbol name="LD680X">
<pin name="IN" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PTN36241B">
<pin name="AIN+" direction="in"/>
<pin name="AIN-" direction="in"/>
<pin name="AOUT+" direction="out"/>
<pin name="AOUT-" direction="out"/>
<pin name="BIN+" direction="in"/>
<pin name="BIN-" direction="in"/>
<pin name="BOUT+" direction="out"/>
<pin name="BOUT-" direction="out"/>
<pin name="COM" direction="in"/>
<pin name="CEN" direction="in"/>
<pin name="AEQ" direction="in"/>
<pin name="SQTH" direction="in"/>
<pin name="BDE/SCL" direction="in"/>
<pin name="ADE/ADD" direction="in"/>
<pin name="BEQ/SDA" direction="in"/>
<pin name="BOS" direction="in"/>
<pin name="AOS" direction="in"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
</symbol>
<symbol name="N-MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="LPC12D27">
<pin name="S0" direction="out"/>
<pin name="S1" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="S3" direction="out"/>
<pin name="S4" direction="out"/>
<pin name="S5" direction="out"/>
<pin name="S6" direction="out"/>
<pin name="S7" direction="out"/>
<pin name="S8" direction="out"/>
<pin name="S9" direction="out"/>
<pin name="S10" direction="out"/>
<pin name="S11" direction="out"/>
<pin name="S12" direction="out"/>
<pin name="S13" direction="out"/>
<pin name="S14" direction="out"/>
<pin name="S15" direction="out"/>
<pin name="S16" direction="out"/>
<pin name="S17" direction="out"/>
<pin name="S18" direction="out"/>
<pin name="S19" direction="out"/>
<pin name="S20" direction="out"/>
<pin name="S21" direction="out"/>
<pin name="S22" direction="out"/>
<pin name="S23" direction="out"/>
<pin name="S24" direction="out"/>
<pin name="S25" direction="out"/>
<pin name="S26" direction="out"/>
<pin name="S27" direction="out"/>
<pin name="S28" direction="out"/>
<pin name="S29" direction="out"/>
<pin name="S30" direction="out"/>
<pin name="S31" direction="out"/>
<pin name="S32" direction="out"/>
<pin name="S33" direction="out"/>
<pin name="S34" direction="out"/>
<pin name="S35" direction="out"/>
<pin name="S36" direction="out"/>
<pin name="S37" direction="out"/>
<pin name="S38" direction="out"/>
<pin name="S39" direction="out"/>
<pin name="BP0" direction="out"/>
<pin name="BP1" direction="out"/>
<pin name="BP2" direction="out"/>
<pin name="BP3" direction="out"/>
<pin name="LCD_SCL"/>
<pin name="LCD_SDA"/>
<pin name="SYNC"/>
<pin name="CLK"/>
<pin name="VDD" direction="pwr"/>
<pin name="VLCD" direction="pwr"/>
<pin name="VSS(LCD)" direction="pwr"/>
<pin name="PIO0_0/!RTS0!"/>
<pin name="PIO0_1/RXD0/CT32B0_CAP0/CT32B0_MAT0"/>
<pin name="PIO0_2/TXD0/CT32B0_CAP1/CT32B0_MAT1"/>
<pin name="PIO0_3/!DTR0!/CT32B0_CAP2/CT32B0_MAT2"/>
<pin name="PIO0_4/CT32B0_CAP3/CT32B0_MAT3"/>
<pin name="PIO0_5/!DCD0!"/>
<pin name="PIO0_6/!RI0!/CT32B1_CAP0/CT32B1_MAT0"/>
<pin name="PIO0_7/!CTS0!/CT32B1_CAP1/CT32B1_MAT1"/>
<pin name="PIO0_8/RXD1/CT32B1_CAP2/CT32B1_MAT2"/>
<pin name="PIO0_9/TXD1/CT32B1_CAP3/CT32B1_MAT3"/>
<pin name="PIO0_10/SCL"/>
<pin name="PIO0_11/SDA/CT16B0_CAP0/CT16B0_MAT0"/>
<pin name="PIO0_12/CLKOUT/CT16B0_CAP1/CT16B0_MAT1"/>
<pin name="!RESET!/PIO0_13"/>
<pin name="PIO0_14/SCK"/>
<pin name="PIO0_15/SSEL/CT16B1_CAP0/CT16B1_MAT0"/>
<pin name="PIO0_16/MISO/CT16B1_CAP1/CT16B1_MAT1"/>
<pin name="PIO0_17/MOSI"/>
<pin name="PIO0_18/SWCLK/CT32B0_CAP0/CT32B0_MAT0"/>
<pin name="PIO0_19/ACMP0_I0/CT32B0_CAP1/CT32B0_MAT1"/>
<pin name="PIO0_20/ACMP0_I1/CT32B0_CAP2/CT32B0_MAT2"/>
<pin name="PIO0_21/ACMP0_I2/CT32B0_CAP3/CT32B0_MAT3"/>
<pin name="PIO0_22/ACMP0_I3"/>
<pin name="PIO0_23/ACMP1_I0/CT32B1_CAP0/CT32B1_MAT0"/>
<pin name="PIO0_24/ACMP1_I1/CT32B1_CAP1/CT32B1_MAT1"/>
<pin name="SWDIO/ACMP1_I2/CT32B1_CAP2/CT32B1_MAT2/PIO0_25"/>
<pin name="SWCLK/ACMP1_I3/CT32B1_CAP3/CT32B1_MAT3/PIO0_26"/>
<pin name="PIO0_27/ACMP0_O"/>
<pin name="PIO0_28/ACMP1_O/CT16B0_CAP0/CT16B0_MAT0"/>
<pin name="PIO0_29/ROSC/CT16B0_CAP1/CT16B0_MAT1"/>
<pin name="R/PIO0_30/AD0"/>
<pin name="R/PIO0_31/AD1"/>
<pin name="R/PIO1_0/AD2"/>
<pin name="R/PIO1_1/AD3"/>
<pin name="PIO1_2/SWDIO/AD4"/>
<pin name="PIO1_3/AD5/WAKEUP"/>
<pin name="PIO1_4/AD6"/>
<pin name="PIO1_5/AD7/CT16B1_CAP0/CT16B1_MAT0"/>
<pin name="PIO1_6/CT16B1_CAP1/CT16B1_MAT1"/>
<pin name="PIO2_0/CT16B0_CAP0/CT16B0_MAT0"/>
<pin name="RTCXI" direction="pas"/>
<pin name="RTCXOUT" direction="pas"/>
<pin name="XTALIN" direction="pas"/>
<pin name="XTALOUT" direction="pas"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="VSS(IO)" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VREF_CMP" direction="pwr"/>
</symbol>
<symbol name="PCA9661">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CE" direction="in" function="dot"/>
<pin name="INT" direction="out" function="dot"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in" function="dot"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="SCL0"/>
<pin name="SDA0"/>
<pin name="TRIG" direction="in"/>
<pin name="VDD(I/O)" direction="pwr"/>
<pin name="VDD(PLL)" direction="pwr"/>
<pin name="VSS(I/O)" direction="pwr"/>
<pin name="VSS(PLL)" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
</symbol>
<symbol name="LPC11U14-48">
<pin name="!RESET!/PIO0_0"/>
<pin name="!TRST!/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/!USB_CONNECT!/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_13/!DTR!/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/!DSR!/CT16B0_MAT1/RXD"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_16/!RI!/CT16B0_CAP0"/>
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="PIO1_20/!DSR!/SCK1"/>
<pin name="PIO1_21/!DCD!/MISO1"/>
<pin name="PIO1_22/!RI!/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="(PIO1_5/CT32B1_CAP1)PIO1_31"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="XTALIN" direction="pas"/>
<pin name="XTALOUT" direction="pas"/>
</symbol>
<symbol name="LPC11U14-33">
<pin name="!RESET!/PIO0_0"/>
<pin name="!TRST!/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/!USB_CONNECT!/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="XTALIN" direction="pas"/>
<pin name="XTALOUT" direction="pas"/>
</symbol>
<symbol name="ESD-PROTECTION-NON_CLAMP">
<pin name="CH2-" direction="pas"/>
<pin name="CH1+" direction="pas"/>
<pin name="CH1-" direction="pas"/>
<pin name="CH2+" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="LPC1110FDX20">
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LPC1112FDH20">
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO0_3"/>
</symbol>
<symbol name="LPC1112FDH28">
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDDA" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO1_5/!RTS!/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="LPC1800_FULL">
<pin name="P0_0"/>
<pin name="P0_1"/>
<pin name="P1_0"/>
<pin name="P1_1"/>
<pin name="P1_2"/>
<pin name="P1_3"/>
<pin name="P1_4"/>
<pin name="P1_5"/>
<pin name="P1_6"/>
<pin name="P1_7"/>
<pin name="P1_8"/>
<pin name="P1_9"/>
<pin name="P1_10"/>
<pin name="P1_11"/>
<pin name="P1_12"/>
<pin name="P1_13"/>
<pin name="P1_14"/>
<pin name="P1_15"/>
<pin name="P1_16"/>
<pin name="P1_17"/>
<pin name="P1_18"/>
<pin name="P1_19"/>
<pin name="P1_20"/>
<pin name="P2_0"/>
<pin name="P2_1"/>
<pin name="P2_2"/>
<pin name="P2_3"/>
<pin name="P2_4"/>
<pin name="P2_5"/>
<pin name="P2_6"/>
<pin name="P2_7"/>
<pin name="P2_8"/>
<pin name="P2_9"/>
<pin name="P2_10"/>
<pin name="P2_11"/>
<pin name="P2_12"/>
<pin name="P2_13"/>
<pin name="P3_0"/>
<pin name="P3_1"/>
<pin name="P3_2"/>
<pin name="P3_3"/>
<pin name="P3_4"/>
<pin name="P3_5"/>
<pin name="P3_6"/>
<pin name="P3_7"/>
<pin name="P3_8"/>
<pin name="P4_0"/>
<pin name="P4_1"/>
<pin name="P4_2"/>
<pin name="P4_3"/>
<pin name="P4_4"/>
<pin name="P4_5"/>
<pin name="P4_6"/>
<pin name="P4_7"/>
<pin name="P4_8"/>
<pin name="P4_9"/>
<pin name="P4_10"/>
<pin name="P5_0"/>
<pin name="P5_1"/>
<pin name="P5_2"/>
<pin name="P5_3"/>
<pin name="P5_4"/>
<pin name="P5_5"/>
<pin name="P5_6"/>
<pin name="P5_7"/>
<pin name="P6_0"/>
<pin name="P6_1"/>
<pin name="P6_2"/>
<pin name="P6_3"/>
<pin name="P6_4"/>
<pin name="P6_5"/>
<pin name="P6_6"/>
<pin name="P6_7"/>
<pin name="P6_8"/>
<pin name="P6_9"/>
<pin name="P6_10"/>
<pin name="P6_11"/>
<pin name="P6_12"/>
<pin name="P7_0"/>
<pin name="P7_1"/>
<pin name="P7_2"/>
<pin name="P7_3"/>
<pin name="P7_4"/>
<pin name="P7_5"/>
<pin name="P7_6"/>
<pin name="P7_7"/>
<pin name="P8_0"/>
<pin name="P8_1"/>
<pin name="P8_2"/>
<pin name="P8_3"/>
<pin name="P8_4"/>
<pin name="P8_5"/>
<pin name="P8_6"/>
<pin name="P8_7"/>
<pin name="P8_8"/>
<pin name="P9_0"/>
<pin name="P9_1"/>
<pin name="P9_2"/>
<pin name="P9_3"/>
<pin name="P9_4"/>
<pin name="P9_5"/>
<pin name="P9_6"/>
<pin name="PA_0"/>
<pin name="PB_0"/>
<pin name="PD_0"/>
<pin name="PC_0"/>
<pin name="PA_1"/>
<pin name="PA_2"/>
<pin name="PA_3"/>
<pin name="PA_4"/>
<pin name="PB_1"/>
<pin name="PB_2"/>
<pin name="PB_3"/>
<pin name="PB_4"/>
<pin name="PB_5"/>
<pin name="PB_6"/>
<pin name="PC_1"/>
<pin name="PC_2"/>
<pin name="PC_3"/>
<pin name="PC_4"/>
<pin name="PC_5"/>
<pin name="PC_6"/>
<pin name="PC_7"/>
<pin name="PC_8"/>
<pin name="PC_9"/>
<pin name="PC_10"/>
<pin name="PC_11"/>
<pin name="PC_12"/>
<pin name="PC_13"/>
<pin name="PC_14"/>
<pin name="PD_1"/>
<pin name="PD_2"/>
<pin name="PD_3"/>
<pin name="PD_4"/>
<pin name="PD_5"/>
<pin name="PD_6"/>
<pin name="PD_7"/>
<pin name="PD_8"/>
<pin name="PD_9"/>
<pin name="PD_10"/>
<pin name="PD_11"/>
<pin name="PD_12"/>
<pin name="PD_13"/>
<pin name="PD_14"/>
<pin name="PD_15"/>
<pin name="PD_16"/>
<pin name="PE_0"/>
<pin name="PF_0"/>
<pin name="PE_1"/>
<pin name="PE_2"/>
<pin name="PE_3"/>
<pin name="PE_4"/>
<pin name="PE_5"/>
<pin name="PE_6"/>
<pin name="PE_7"/>
<pin name="PE_8"/>
<pin name="PE_9"/>
<pin name="PE_10"/>
<pin name="PE_11"/>
<pin name="PE_12"/>
<pin name="PE_13"/>
<pin name="PE_14"/>
<pin name="PE_15"/>
<pin name="PF_1"/>
<pin name="PF_2"/>
<pin name="PF_3"/>
<pin name="PF_4"/>
<pin name="PF_5"/>
<pin name="PF_6"/>
<pin name="PF_7"/>
<pin name="PF_8"/>
<pin name="PF_9"/>
<pin name="PF_10"/>
<pin name="PF_11"/>
</symbol>
<symbol name="+UB">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="-UB">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="N-MOSFET_2S">
<pin name="S@1" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S@2" direction="pas"/>
</symbol>
<symbol name="N-MOSFET_2D">
<pin name="D@2" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D@1" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PCA9509">
<pin name="A1"/>
<pin name="A2"/>
<pin name="EN" direction="in"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="VCC(A)" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC(B)" direction="pwr"/>
</symbol>
<symbol name="BGA7210">
<pin name="GND" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="RF_OUT" direction="out"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="SEROUT" direction="out"/>
<pin name="!SS!" direction="in"/>
<pin name="SER_IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="PUPMXG" direction="in"/>
</symbol>
<symbol name="ZENER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="BUFFER">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="BUFFER_OE">
<pin name="OEN" direction="in" function="dot"/>
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="74125">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
</symbol>
<symbol name="PWRN-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="DIODE2XCC">
<pin name="A1" direction="pas"/>
<pin name="C1C2" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="LPC11AXX">
<pin name="!RESET!/PIO0_0"/>
<pin name="PIO0_14/MISO/AD6/CT32B0_CAP1/CT16B1_MAT1"/>
<pin name="PIO0_1/RXD/CLKOUT/CT32B0_MAT2/SSEL0/CLKIN"/>
<pin name="PIO0_2/SCL/ACMP_O/TCK/SWCLK/CT16B0_CAP0"/>
<pin name="PIO0_3/SDA/ACMP_O/SWDIO/CT16B1_CAP0"/>
<pin name="PIO0_4/R/AOUT/CT16B0_MAT1/MOSI0"/>
<pin name="TCK/SWCLK/PIO0_5/R/CT16B0_MAT2/SCK0"/>
<pin name="TDI/PIO0_6/AD0/CT32B0_MAT3/MISO0"/>
<pin name="TMS/PIO0_7/AD1/CT32B1_CAP0/CT16B0_MAT0"/>
<pin name="TDO/PIO0_8/AD2/CT32B1_MAT0/SCK1"/>
<pin name="!TRST!/PIO0_9/AD3/CT32B1_MAT1/CT16B0_MAT1/!CTS!"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_13/!DTR!/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/!DSR!/CT16B0_MAT1/RXD"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_16/!RI!/CT16B0_CAP0"/>
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="PIO1_20/!DSR!/SCK1"/>
<pin name="PIO1_21/!DCD!/MISO1"/>
<pin name="PIO1_22/!RI!/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="(PIO1_5/CT32B1_CAP1)PIO1_31"/>
<pin name="SWDIO/PIO0_10/AD4/CT32B1_MAT2/CT16B0_MAT2/!RTS!"/>
<pin name="PIO0_15/TXD/AD7/CT32B0_CAP2/SDA"/>
<pin name="PIO0_11/SCK/AD5/CT32B1_MAT3/CT32B0_CAP0"/>
<pin name="PIO0_13/TXD/ACMP_I2/CT32B0_MAT1/SDA"/>
<pin name="PIO0_12/RXD/ACMP_0/CT32B0_MAT0/SCL/CLKIN"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="XTALIN" direction="pas"/>
<pin name="XTALOUT" direction="pas"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="LPC1114">
<pin name="PIO2_6"/>
<pin name="PIO2_0/!DTR!/SSEL1"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_1/!DSR!/SCK1"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO3_4"/>
<pin name="PIO2_4"/>
<pin name="PIO2_5"/>
<pin name="PIO3_5"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_2/!DCD!/MISO1"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="PIO2_11/SCK0"/>
<pin name="R/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="R/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="R/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="R/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="PIO3_0/!DTR!"/>
<pin name="PIO3_1/!DSR!"/>
<pin name="PIO2_3/!RI!/MOSI1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2/!DCD!"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="PIO1_5/!RTS!/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO3_3/!RI!"/>
</symbol>
<symbol name="SL3S4001">
<pin name="RF1P" direction="pas"/>
<pin name="RF1N" direction="pas"/>
<pin name="RF2P" direction="pas"/>
<pin name="RF2N" direction="pas"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VDDB" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PNPRR">
<pin name="INPUT" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNPR">
<pin name="INPUT" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="NPNR">
<pin name="INPUT" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="NPNRR">
<pin name="INPUT" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DIODE_SDD_AKAK">
<pin name="A1" direction="pas"/>
<pin name="K1A2" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="TRANSISTOR-PNP_PNP-DAR">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="SA57000">
<pin name="GND"/>
<pin name="PWROK"/>
<pin name="PWRON"/>
<pin name="VIN"/>
<pin name="VOUT"/>
</symbol>
<symbol name="P-MOSFET_2D">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="N-MOSFET-ESD">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="LM75B">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="OS" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND"/>
</symbol>
<symbol name="DIODE_SHUNT">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="REF" direction="in"/>
</symbol>
<symbol name="DIODE_SDD_AKKA">
<pin name="A1" direction="pas"/>
<pin name="K1K2" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="PCF2123">
<pin name="OSCO" direction="pas"/>
<pin name="OSCI" direction="pas"/>
<pin name="!INT1!" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="SDI" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="CLKOE" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="SCL"/>
<pin name="CE" direction="in"/>
<pin name="TEST" direction="out"/>
</symbol>
<symbol name="P-MOSFER-TR">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="TEA1703">
<pin name="OPTO" direction="out"/>
<pin name="SWDETECT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VSENSE" direction="pas"/>
<pin name="PSENSE" direction="pas"/>
<pin name="NC@1" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="NC@2" direction="in"/>
</symbol>
<symbol name="PCF8537A">
<pin name="S0" direction="out"/>
<pin name="S1" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="S3" direction="out"/>
<pin name="S4" direction="out"/>
<pin name="S5" direction="out"/>
<pin name="S6" direction="out"/>
<pin name="S7" direction="out"/>
<pin name="S8" direction="out"/>
<pin name="S9" direction="out"/>
<pin name="S10" direction="out"/>
<pin name="S11" direction="out"/>
<pin name="S12" direction="out"/>
<pin name="S13" direction="out"/>
<pin name="S14" direction="out"/>
<pin name="S15" direction="out"/>
<pin name="S16" direction="out"/>
<pin name="S17" direction="out"/>
<pin name="S18" direction="out"/>
<pin name="S19" direction="out"/>
<pin name="S20" direction="out"/>
<pin name="S21" direction="out"/>
<pin name="S22" direction="out"/>
<pin name="S23" direction="out"/>
<pin name="S24" direction="out"/>
<pin name="S25" direction="out"/>
<pin name="S26" direction="out"/>
<pin name="S27" direction="out"/>
<pin name="S28" direction="out"/>
<pin name="S29" direction="out"/>
<pin name="S30" direction="out"/>
<pin name="S31" direction="out"/>
<pin name="S32" direction="out"/>
<pin name="S33" direction="out"/>
<pin name="S34" direction="out"/>
<pin name="S35" direction="out"/>
<pin name="S36" direction="out"/>
<pin name="S37" direction="out"/>
<pin name="S38" direction="out"/>
<pin name="S39" direction="out"/>
<pin name="S40" direction="out"/>
<pin name="S41" direction="out"/>
<pin name="S42" direction="out"/>
<pin name="S43" direction="out"/>
<pin name="S44/BP7" direction="out"/>
<pin name="S45/BP6" direction="out"/>
<pin name="BP0" direction="out"/>
<pin name="BP1" direction="out"/>
<pin name="BP2" direction="out"/>
<pin name="BP3" direction="out"/>
<pin name="BP4" direction="out"/>
<pin name="BP5" direction="out"/>
<pin name="VLCD" direction="out"/>
<pin name="VDD2" direction="out"/>
<pin name="VDD1" direction="out"/>
<pin name="VSS" direction="out"/>
<pin name="T3" direction="out"/>
<pin name="T2" direction="out"/>
<pin name="T1" direction="out"/>
<pin name="CLK" direction="out"/>
<pin name="A0" direction="out"/>
<pin name="SCL" direction="out"/>
<pin name="SDA" direction="out"/>
<pin name="!RESET!" direction="out"/>
</symbol>
<symbol name="PCF8537B">
<pin name="S0" direction="out"/>
<pin name="S1" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="S3" direction="out"/>
<pin name="S4" direction="out"/>
<pin name="S5" direction="out"/>
<pin name="S6" direction="out"/>
<pin name="S7" direction="out"/>
<pin name="S8" direction="out"/>
<pin name="S9" direction="out"/>
<pin name="S10" direction="out"/>
<pin name="S11" direction="out"/>
<pin name="S12" direction="out"/>
<pin name="S13" direction="out"/>
<pin name="S14" direction="out"/>
<pin name="S15" direction="out"/>
<pin name="S16" direction="out"/>
<pin name="S17" direction="out"/>
<pin name="S18" direction="out"/>
<pin name="S19" direction="out"/>
<pin name="S20" direction="out"/>
<pin name="S21" direction="out"/>
<pin name="S22" direction="out"/>
<pin name="S23" direction="out"/>
<pin name="S24" direction="out"/>
<pin name="S25" direction="out"/>
<pin name="S26" direction="out"/>
<pin name="S27" direction="out"/>
<pin name="S28" direction="out"/>
<pin name="S29" direction="out"/>
<pin name="S30" direction="out"/>
<pin name="S31" direction="out"/>
<pin name="S32" direction="out"/>
<pin name="S33" direction="out"/>
<pin name="S34" direction="out"/>
<pin name="S35" direction="out"/>
<pin name="S36" direction="out"/>
<pin name="S37" direction="out"/>
<pin name="S38" direction="out"/>
<pin name="S39" direction="out"/>
<pin name="S40" direction="out"/>
<pin name="S41" direction="out"/>
<pin name="S42" direction="out"/>
<pin name="S43" direction="out"/>
<pin name="S44/BP7" direction="out"/>
<pin name="S45/BP6" direction="out"/>
<pin name="BP0" direction="out"/>
<pin name="BP1" direction="out"/>
<pin name="BP2" direction="out"/>
<pin name="BP3" direction="out"/>
<pin name="BP4" direction="out"/>
<pin name="BP5" direction="out"/>
<pin name="VLCD" direction="out"/>
<pin name="VDD2" direction="out"/>
<pin name="VDD1" direction="out"/>
<pin name="VSS" direction="out"/>
<pin name="T3" direction="out"/>
<pin name="T2" direction="out"/>
<pin name="T1" direction="out"/>
<pin name="CLK" direction="out"/>
<pin name="SDIO" direction="out"/>
<pin name="SCL" direction="out"/>
<pin name="!CE!" direction="out"/>
<pin name="!RESET!" direction="out"/>
</symbol>
<symbol name="NX3DV221">
<pin name="VCC" direction="out"/>
<pin name="GND" direction="out"/>
<pin name="!OE!" direction="out"/>
<pin name="S" direction="out"/>
<pin name="D-" direction="out"/>
<pin name="1D-" direction="out"/>
<pin name="2D-" direction="out"/>
<pin name="D+" direction="out"/>
<pin name="1D+" direction="out"/>
<pin name="2D+" direction="out"/>
</symbol>
<symbol name="NTS0102">
<pin name="A2" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="VCC(A)" direction="out"/>
<pin name="VCC(B)" direction="out"/>
<pin name="GND" direction="out"/>
<pin name="OE" direction="out"/>
</symbol>
<symbol name="DIODE_ESD">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="DIODE_ESD_KK">
<pin name="K2" direction="pas"/>
<pin name="K1" direction="pas"/>
</symbol>
<symbol name="DIODE_SDD_KAAK">
<pin name="K1" direction="pas"/>
<pin name="A1A2" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="DIODE_AKAK">
<pin name="A1" direction="pas"/>
<pin name="K1A2" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="DIODE_KAAK">
<pin name="K1" direction="pas"/>
<pin name="A1A2" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="DIODE_AKKA">
<pin name="A1" direction="pas"/>
<pin name="K1K2" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="DIODE_SCHOTTKY_4A_2K">
<pin name="A@1" direction="pas"/>
<pin name="K@1" direction="pas"/>
<pin name="K@2" direction="pas"/>
<pin name="A@2" direction="pas"/>
<pin name="A@3" direction="pas"/>
<pin name="A@4" direction="pas"/>
</symbol>
<symbol name="DIODE_SCHOTTKY_2A_4K">
<pin name="A@1" direction="pas"/>
<pin name="K@1" direction="pas"/>
<pin name="K@2" direction="pas"/>
<pin name="K@4" direction="pas"/>
<pin name="K@3" direction="pas"/>
<pin name="A@2" direction="pas"/>
</symbol>
<symbol name="DIODE_SCHOTTKY_2A_1K">
<pin name="A@1" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="A@2" direction="pas"/>
</symbol>
<symbol name="DIODE_VAR">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="P-MOSFET-TR-2D">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D@1" direction="pas"/>
<pin name="D@2" direction="pas"/>
</symbol>
<symbol name="DLC3">
<pin name="VSSA@1"/>
<pin name="VDDA3V@1"/>
<pin name="TXP"/>
<pin name="TXN"/>
<pin name="TXAMP_TEMP"/>
<pin name="TXAMP_TH0"/>
<pin name="TXAMP_TH1"/>
<pin name="TXAMP_SCL"/>
<pin name="TXAMP_OUT_P"/>
<pin name="TXAMP_SDA"/>
<pin name="TXAMP_OUT_N"/>
<pin name="!RESET!"/>
<pin name="BC_N"/>
<pin name="BC_L"/>
<pin name="PFC_P"/>
<pin name="PFC_N"/>
<pin name="VDD_IO@1"/>
<pin name="OSC32K2"/>
<pin name="OSC32K1"/>
<pin name="VDD_UBAT"/>
<pin name="RTC_BUF"/>
<pin name="VDD_CORE@1"/>
<pin name="GDY4"/>
<pin name="VDD_IO@2"/>
<pin name="VDD_CORE@2"/>
<pin name="VDD_IO@3"/>
<pin name="VDD_IO@4"/>
<pin name="P28"/>
<pin name="P27"/>
<pin name="BOOT"/>
<pin name="GDY3"/>
<pin name="GDY2"/>
<pin name="BC_P"/>
<pin name="BC_IGN"/>
<pin name="GND@1"/>
<pin name="VDD_IO@5"/>
<pin name="GDY1"/>
<pin name="GDY0"/>
<pin name="VDD_CORE@3"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="!SPI_CS!"/>
<pin name="!DISW!"/>
<pin name="!NMI!"/>
<pin name="P26"/>
<pin name="VDD_CORE@4"/>
<pin name="P24"/>
<pin name="P23"/>
<pin name="P22"/>
<pin name="P21"/>
<pin name="P20"/>
<pin name="P19"/>
<pin name="P18"/>
<pin name="VDD_IO@6"/>
<pin name="VDD_CORE@5"/>
<pin name="SIC1"/>
<pin name="SIC0"/>
<pin name="VREF_P_M"/>
<pin name="VREF_N_M"/>
<pin name="VREF_VCM_M"/>
<pin name="RESBN"/>
<pin name="RESBP"/>
<pin name="VSSA@2"/>
<pin name="BC_I_N"/>
<pin name="BC_I_P"/>
<pin name="BC_U_N"/>
<pin name="BC_U_P"/>
<pin name="VDDA3V@2"/>
<pin name="PFC_BUF_N"/>
<pin name="PFC_BUF_P"/>
<pin name="GND@2"/>
<pin name="VDDA3V@3"/>
<pin name="VSSA@3"/>
<pin name="RESAN"/>
<pin name="RESAP"/>
<pin name="PFC_I1_N"/>
<pin name="PFC_I1_P"/>
<pin name="PFC_I0_N"/>
<pin name="PFC_LINEU_N"/>
<pin name="PFC_I0_P"/>
<pin name="PFC_LINEU_P"/>
<pin name="VDDA1V5@1"/>
<pin name="SIC15"/>
<pin name="SIC14"/>
<pin name="VDD_IO@7"/>
<pin name="SIC13"/>
<pin name="SIC12"/>
<pin name="VDD_IO@8"/>
<pin name="VDD_CORE@6"/>
<pin name="P17"/>
<pin name="P16"/>
<pin name="P15"/>
<pin name="P14"/>
<pin name="VDD_IO@9"/>
<pin name="P9"/>
<pin name="P11"/>
<pin name="P5"/>
<pin name="P8"/>
<pin name="P7"/>
<pin name="P6"/>
<pin name="P4"/>
<pin name="VDD_CORE@7"/>
<pin name="VDD_IO@10"/>
<pin name="P3"/>
<pin name="P2"/>
<pin name="P1"/>
<pin name="!TXAMP_EN!"/>
<pin name="GND@4"/>
<pin name="VREF_P_A"/>
<pin name="VREF_N_A"/>
<pin name="VREF_VCM_A"/>
<pin name="RXP"/>
<pin name="REFP"/>
<pin name="REFN"/>
<pin name="RXN"/>
<pin name="VDDA3V@4"/>
<pin name="VSSA@4"/>
<pin name="VDDA1V5@2"/>
<pin name="GND_PLL"/>
<pin name="SYS_XTAL1"/>
<pin name="SYS_XTAL2"/>
<pin name="VDD_PLL"/>
<pin name="VDD_IO@13"/>
<pin name="VPGM"/>
<pin name="VDD_CORE@10"/>
<pin name="VDD_CORE@9"/>
<pin name="TCK"/>
<pin name="TDO"/>
<pin name="VDD_IO@12"/>
<pin name="TDI"/>
<pin name="!TRST!"/>
<pin name="TMS"/>
<pin name="A0/SIC2"/>
<pin name="A1/SIC3"/>
<pin name="VDD_CORE@8"/>
<pin name="A2/SIC4"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="P10"/>
<pin name="P0"/>
<pin name="VDD_IO@11"/>
<pin name="GND@3"/>
</symbol>
<symbol name="TRIAC_TOP">
<pin name="CM" direction="pas"/>
<pin name="LD" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="BUFFER_OPENDRAIN">
<pin name="A" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="2-INPUT-AND">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="2-INPUT-AND-OD">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="2-INPUT-EXCLUSIVE-OR">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="2-INPUT-NAND">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="2-INPUT-NAND-OD">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="2-INPUT-NOR">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="2-INPUT-OR">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="3-INPUT-AND">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="3-INPUT-NAND">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="INVERTER">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="INVERTER-ST">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="INVERTER_OD">
<pin name="A" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="AMP_WITH_BYPASS">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CTRL" direction="in"/>
</symbol>
<symbol name="PCF1252">
<pin name="CT" direction="pas"/>
<pin name="SELECT" direction="in"/>
<pin name="COMIN" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="COMOUT" direction="out"/>
<pin name="RESET" direction="out"/>
<pin name="!POWF!" direction="out"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="ESD-PESD5V0F5UF">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="AMP_WITH_ENABLE">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="TEA1623">
<pin name="REG" direction="out"/>
<pin name="RC" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="DRAIN" direction="pas"/>
<pin name="SOURCE" direction="in"/>
<pin name="AUX" direction="pas"/>
<pin name="GND" direction="in"/>
</symbol>
<symbol name="TEA1731">
<pin name="ISENSE" direction="out"/>
<pin name="PROTECT" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="CTRL" direction="in"/>
<pin name="DRIVER" direction="pas"/>
<pin name="GND" direction="in"/>
</symbol>
<symbol name="BUFFER-ST">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="74LVC1G99">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!OE!" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="PCAL6416A">
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="VDD(I2C)" direction="pwr"/>
<pin name="VDD(P)" direction="pwr"/>
<pin name="VSS"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="ADDR" direction="in"/>
<pin name="!RESET!" direction="in"/>
<pin name="!INT!" direction="out"/>
</symbol>
<symbol name="LPC11U3X-LQFP64">
<pin name="!RESET!/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/!USB_CONNECT!/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="PIO1_0/CT32B1_MAT0"/>
<pin name="VSS" direction="pwr"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="!TRST!/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_21/CT16B1_MAT0"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_1/CT32B1_MAT1"/>
<pin name="PIO1_2/CT32B1_MAT2"/>
<pin name="PIO1_3/CT32B1_MAT3"/>
<pin name="PIO1_4/CT32B1_CAP0"/>
<pin name="PIO1_5/CT32B1_CAP1"/>
<pin name="PIO1_6"/>
<pin name="PIO1_7"/>
<pin name="PIO1_8"/>
<pin name="PIO1_9"/>
<pin name="PIO1_10"/>
<pin name="PIO1_11"/>
<pin name="PIO1_12"/>
<pin name="PIO1_13/!DTR!/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/!DSR!/CT16B0_MAT1/RXD"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_16/!RI!/CT16B0_CAP0"/>
<pin name="PIO1_17/CT16B0_CAP1/RXD"/>
<pin name="PIO1_18/CT16B1_CAP1/TXD"/>
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="PIO1_20/!DSR!/SCK1"/>
<pin name="PIO1_21/!DCD!/MISO1"/>
<pin name="PIO1_22/!RI!/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
</symbol>
<symbol name="LPC11U3X-LQFP48">
<pin name="!RESET!/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/!USB_CONNECT!/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="VSS" direction="pwr"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="!TRST!/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_13/!DTR!/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/!DSR!/CT16B0_MAT1/RXD"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_16/!RI!/CT16B0_CAP0"/>
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="PIO1_20/!DSR!/SCK1"/>
<pin name="PIO1_21/!DCD!/MISO1"/>
<pin name="PIO1_22/!RI!/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO1_31"/>
</symbol>
<symbol name="LPC11U3X-TFBGA48">
<pin name="!RESET!/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/!USB_CONNECT!/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="VSS" direction="pwr"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="!TRST!/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_21/CT16B1_MAT0"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_5/CT32B1_CAP1"/>
<pin name="PIO1_13/!DTR!/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/!DSR!/CT16B0_MAT1/RXD"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_16/!RI!/CT16B0_CAP0"/>
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="PIO1_20/!DSR!/SCK1"/>
<pin name="PIO1_21/!DCD!/MISO1"/>
<pin name="PIO1_22/!RI!/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
</symbol>
<symbol name="LPC11U3X-HVQFN33">
<pin name="!RESET!/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/!USB_CONNECT!/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="VSS" direction="pwr"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="!TRST!/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_21/CT16B1_MAT0"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
</symbol>
<symbol name="IP4294CZ10-TBR">
<pin name="ESD3" direction="pas"/>
<pin name="ESD2" direction="pas"/>
<pin name="ESD1" direction="pas"/>
<pin name="ESD4" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PCAL6408A">
<pin name="P7"/>
<pin name="P6"/>
<pin name="P5"/>
<pin name="P4"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="VDD(I2C)" direction="pwr"/>
<pin name="VDD(P)" direction="pwr"/>
<pin name="VSS"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="ADDR" direction="in"/>
<pin name="!RESET!" direction="in"/>
<pin name="!INT!" direction="out"/>
</symbol>
<symbol name="LPC810M021FN8">
<pin name="!RESET!/PIO0_5"/>
<pin name="PIO0_4/WAKEUP/!TRST!"/>
<pin name="SWCLK/PIO0_3/TCK"/>
<pin name="SWDIO/PIO0_2/TMS"/>
<pin name="PIO0_0/ACMP_I1/TDO"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO0_1/ACMP_I2/CLKIN/TDI"/>
</symbol>
<symbol name="LPC811M001FDH16">
<pin name="!RESET!/PIO0_5"/>
<pin name="PIO0_4/WAKEUP/!TRST!"/>
<pin name="SWCLK/PIO0_3/TCK"/>
<pin name="SWDIO/PIO0_2/TMS"/>
<pin name="PIO0_0/ACMP_I1/TDO"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO0_1/ACMP_I2/CLKIN/TDI"/>
<pin name="PIO0_13"/>
<pin name="PIO0_12"/>
<pin name="PIO0_11"/>
<pin name="PIO0_10"/>
<pin name="PIO0_8/XTALIN"/>
<pin name="PIO0_9/XTALOUT"/>
<pin name="PIO0_7"/>
<pin name="PIO0_6/VDDCMP"/>
</symbol>
<symbol name="LPC812M101FD20">
<pin name="!RESET!/PIO0_5"/>
<pin name="PIO0_4/WAKEUP/!TRST!"/>
<pin name="SWCLK/PIO0_3/TCK"/>
<pin name="SWDIO/PIO0_2/TMS"/>
<pin name="PIO0_0/ACMP_I1/TDO"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO0_1/ACMP_I2/CLKIN/TDI"/>
<pin name="PIO0_13"/>
<pin name="PIO0_12"/>
<pin name="PIO0_11"/>
<pin name="PIO0_10"/>
<pin name="PIO0_8/XTALIN"/>
<pin name="PIO0_9/XTALOUT"/>
<pin name="PIO0_7"/>
<pin name="PIO0_6/VDDCMP"/>
<pin name="PIO0_17"/>
<pin name="PIO0_16"/>
<pin name="PIO0_15"/>
<pin name="PIO0_14"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LPC122XFBD64" prefix="U">
<description>NXP ARM M0 32 bit Microcontroller&lt;p&gt;
&lt;author&gt;AAL Eindhoven MV+ MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1XXX-V7-INTERNAL_LPC115X"/>
</gates>
<devices>
<device name="" package="SOT314-2">
<connects>
<connect gate="G$1" pin="NRESET/PIO0_13/EZH13" pad="40"/>
<connect gate="G$1" pin="NTRST/PIO1_1/AD3" pad="49"/>
<connect gate="G$1" pin="PIO0_0/EZH0/NRTS0" pad="19"/>
<connect gate="G$1" pin="PIO0_1/EZH1/RXD0/CT32B0_0" pad="20"/>
<connect gate="G$1" pin="PIO0_10/EZH10/SCL" pad="37"/>
<connect gate="G$1" pin="PIO0_11/EZH11/SDA/CT16B0_0" pad="38"/>
<connect gate="G$1" pin="PIO0_12/EZH12/CLKOUT/CT16B0_1" pad="39"/>
<connect gate="G$1" pin="PIO0_14/EZH14/SCK" pad="41"/>
<connect gate="G$1" pin="PIO0_15/EZH15/SSEL/CT16B1_0" pad="42"/>
<connect gate="G$1" pin="PIO0_16/EZH0/MISO/CT16B1_1" pad="43"/>
<connect gate="G$1" pin="PIO0_17/EZH1/MOSI" pad="44"/>
<connect gate="G$1" pin="PIO0_19/EZH3/C0_IN0/CT32B0_1" pad="4"/>
<connect gate="G$1" pin="PIO0_2/EZH2/TXD0/CT32B0_1" pad="21"/>
<connect gate="G$1" pin="PIO0_20/EZH4/C0_IN1/CT32B0_2" pad="5"/>
<connect gate="G$1" pin="PIO0_21/EZH5/C0_IN2/CT32B0_3" pad="6"/>
<connect gate="G$1" pin="PIO0_22/EZH6/C0_IN3" pad="7"/>
<connect gate="G$1" pin="PIO0_23/EZH7/C1_IN0/CT32B1_0" pad="8"/>
<connect gate="G$1" pin="PIO0_24/EZH8/C1_IN1/CT32B1_1" pad="9"/>
<connect gate="G$1" pin="PIO0_25/EZH9/C1_IN2/CT32B1_2/SWDIO" pad="10"/>
<connect gate="G$1" pin="PIO0_26/EZH10/C1_IN3/CT32B1_3/SWCLK" pad="11"/>
<connect gate="G$1" pin="PIO0_27/EZH11/C0_OUT" pad="12"/>
<connect gate="G$1" pin="PIO0_28/EZH12/C1_OUT/CT16B0_0" pad="17"/>
<connect gate="G$1" pin="PIO0_29/EZH13/ROSC/CT16B0_1" pad="18"/>
<connect gate="G$1" pin="PIO0_3/EZH3/NDTR0/CT32B0_2" pad="22"/>
<connect gate="G$1" pin="PIO0_4/EZH4/NDSR0/CT32B0_3" pad="23"/>
<connect gate="G$1" pin="PIO0_5/EZH5/NDCD0" pad="24"/>
<connect gate="G$1" pin="PIO0_6/EZH6/NRI0/CT32B1_0" pad="25"/>
<connect gate="G$1" pin="PIO0_7/EZH7/NCTS0/CT32B1_1" pad="26"/>
<connect gate="G$1" pin="PIO0_8/EZH8/RXD1/CT32B1_2" pad="27"/>
<connect gate="G$1" pin="PIO0_9/EZH9/TXD1/CT32B1_3" pad="28"/>
<connect gate="G$1" pin="PIO1_3/AD5/WAKEUP" pad="51"/>
<connect gate="G$1" pin="PIO1_4/AD6" pad="52"/>
<connect gate="G$1" pin="PIO1_5/AD7/CT16B1_0" pad="53"/>
<connect gate="G$1" pin="PIO1_6/CT16B1_1" pad="54"/>
<connect gate="G$1" pin="PIO2_0/EZH0/CT16B0_0" pad="29"/>
<connect gate="G$1" pin="PIO2_1/EZH1/CT16B0_1" pad="30"/>
<connect gate="G$1" pin="PIO2_10/EZH10/CT32B1_2" pad="61"/>
<connect gate="G$1" pin="PIO2_11/EZH11/CT32B1_3" pad="62"/>
<connect gate="G$1" pin="PIO2_12/EZH12" pad="13"/>
<connect gate="G$1" pin="PIO2_13/EZH13" pad="14"/>
<connect gate="G$1" pin="PIO2_14/EZH14" pad="15"/>
<connect gate="G$1" pin="PIO2_15/EZH15" pad="16"/>
<connect gate="G$1" pin="PIO2_2/EZH2/CT16B1_0" pad="31"/>
<connect gate="G$1" pin="PIO2_3/EZH3/CT16B1_1" pad="32"/>
<connect gate="G$1" pin="PIO2_4/EZH4/CT32B0_0" pad="33"/>
<connect gate="G$1" pin="PIO2_5/EZH5/CT32B0_1" pad="34"/>
<connect gate="G$1" pin="PIO2_6/EZH6/CT32B0_2" pad="35"/>
<connect gate="G$1" pin="PIO2_7/EZH7/CT32B0_3" pad="36"/>
<connect gate="G$1" pin="PIO2_8/EZH8/CT32B1_0" pad="59"/>
<connect gate="G$1" pin="PIO2_9/EZH9/CT32B1_1" pad="60"/>
<connect gate="G$1" pin="RTCXIN" pad="57"/>
<connect gate="G$1" pin="RTCXOUT" pad="58"/>
<connect gate="G$1" pin="SWCLK/PIO0_18/EZH2/CT32B0_0" pad="45"/>
<connect gate="G$1" pin="SWDIO/PIO1_2/AD4" pad="50"/>
<connect gate="G$1" pin="TDI/PIO0_31/EZH15/AD1" pad="47"/>
<connect gate="G$1" pin="TDO/PIO0_30/EZH14/AD0" pad="46"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD2" pad="48"/>
<connect gate="G$1" pin="VDD(3V3)" pad="56"/>
<connect gate="G$1" pin="VDD(IO)" pad="63"/>
<connect gate="G$1" pin="VREF_CMP" pad="3"/>
<connect gate="G$1" pin="VSS" pad="55"/>
<connect gate="G$1" pin="VSSIO" pad="64"/>
<connect gate="G$1" pin="XTALIN" pad="1"/>
<connect gate="G$1" pin="XTALOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1721" prefix="U">
<description>&lt;H2&gt;HV start-up flyback controller with integrated MOSFET for 5 W applications&lt;/H2&gt;
The TEA1721 is a small and low cost module Switched Mode Power Supply (SMPS) 
controller IC for low power applications (up to 5 W) and operates directly from the rectified 
universal mains input. The device includes a high voltage power switch (700 V) and has 
been optimized for flyback converter topologies to provide high-efficiency over the entire 
load range with ultra-low power consumption in the no-load condition. It provides a circuit 
for start-up directly from the rectified mains voltage without any external bleeder circuits.
The converter operates as a regulated voltage source from no-load up to the maximum 
output current and operates as current source that delivers the maximum current over a 
broad output voltage range. Using the TEA1721, a low power converter can be built at 
minimum cost and with the minimum number of external components.
The controller regulates the output voltage with primary-side sensing which eliminates the 
need for an additional secondary feedback circuitry and simplifies the design. At higher 
power levels, a frequency and current control mode is used. It operates with Burst mode 
control at low power levels and no-load condition. The burst mode minimizes audible 
noise and provides an energy saver state which reduces the power consumption in 
no-load condition.

&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="STARBUCK_TEA1721"/>
</gates>
<devices>
<device name="" package="SOT1175-1">
<connects>
<connect gate="G$1" pin="DRN" pad="7"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="2"/>
<connect gate="G$1" pin="GND3" pad="3"/>
<connect gate="G$1" pin="SRC" pad="6"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AT">
<attribute name="12NC" value="9352 968 88118"/>
<attribute name="BURST" value="430 Hz"/>
</technology>
<technology name="BT">
<attribute name="12NC" value="9352 968 94118"/>
<attribute name="BURST" value="905 Hz"/>
</technology>
<technology name="DT">
<attribute name="12NC" value="9352 968 89118"/>
<attribute name="BURST" value="1270 Hz"/>
</technology>
<technology name="FT">
<attribute name="12NC" value="9352 968 87118"/>
<attribute name="BURST" value="1750 Hz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8885" prefix="U">
<description>NXP Capacitive 8-channel proximity switch with auto-calibration and very low power consumption&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8885"/>
</gates>
<devices>
<device name="TS" package="SOT361-1">
<connects>
<connect gate="G$1" pin="A0" pad="23"/>
<connect gate="G$1" pin="CLK_IN" pad="28"/>
<connect gate="G$1" pin="CLK_OUT" pad="1"/>
<connect gate="G$1" pin="CPC0" pad="18"/>
<connect gate="G$1" pin="CPC1" pad="17"/>
<connect gate="G$1" pin="CPC2" pad="16"/>
<connect gate="G$1" pin="CPC3" pad="15"/>
<connect gate="G$1" pin="CPC4" pad="14"/>
<connect gate="G$1" pin="CPC5" pad="13"/>
<connect gate="G$1" pin="CPC6" pad="12"/>
<connect gate="G$1" pin="CPC7" pad="11"/>
<connect gate="G$1" pin="IN0" pad="10"/>
<connect gate="G$1" pin="IN1" pad="9"/>
<connect gate="G$1" pin="IN2" pad="8"/>
<connect gate="G$1" pin="IN3" pad="7"/>
<connect gate="G$1" pin="IN4" pad="6"/>
<connect gate="G$1" pin="IN5" pad="5"/>
<connect gate="G$1" pin="IN6" pad="4"/>
<connect gate="G$1" pin="IN7" pad="3"/>
<connect gate="G$1" pin="INT" pad="25"/>
<connect gate="G$1" pin="INT_IN" pad="27"/>
<connect gate="G$1" pin="SCL" pad="20"/>
<connect gate="G$1" pin="SDA" pad="21"/>
<connect gate="G$1" pin="SLEEP" pad="24"/>
<connect gate="G$1" pin="TEST" pad="22"/>
<connect gate="G$1" pin="VDD" pad="26"/>
<connect gate="G$1" pin="VDD_IRD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SOT136-1">
<connects>
<connect gate="G$1" pin="A0" pad="23"/>
<connect gate="G$1" pin="CLK_IN" pad="28"/>
<connect gate="G$1" pin="CLK_OUT" pad="1"/>
<connect gate="G$1" pin="CPC0" pad="18"/>
<connect gate="G$1" pin="CPC1" pad="17"/>
<connect gate="G$1" pin="CPC2" pad="16"/>
<connect gate="G$1" pin="CPC3" pad="15"/>
<connect gate="G$1" pin="CPC4" pad="14"/>
<connect gate="G$1" pin="CPC5" pad="13"/>
<connect gate="G$1" pin="CPC6" pad="12"/>
<connect gate="G$1" pin="CPC7" pad="11"/>
<connect gate="G$1" pin="IN0" pad="10"/>
<connect gate="G$1" pin="IN1" pad="9"/>
<connect gate="G$1" pin="IN2" pad="8"/>
<connect gate="G$1" pin="IN3" pad="7"/>
<connect gate="G$1" pin="IN4" pad="6"/>
<connect gate="G$1" pin="IN5" pad="5"/>
<connect gate="G$1" pin="IN6" pad="4"/>
<connect gate="G$1" pin="IN7" pad="3"/>
<connect gate="G$1" pin="INT" pad="25"/>
<connect gate="G$1" pin="INT_IN" pad="27"/>
<connect gate="G$1" pin="SCL" pad="20"/>
<connect gate="G$1" pin="SDA" pad="21"/>
<connect gate="G$1" pin="SLEEP" pad="24"/>
<connect gate="G$1" pin="TEST" pad="22"/>
<connect gate="G$1" pin="VDD" pad="26"/>
<connect gate="G$1" pin="VDD_IRD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTA316" prefix="T">
<description>Planar passivated high commutation three quadrant triac in a SOT78 plastic package 
intended for use in circuits where high static and dynamic dV/dt and high dI/dt can occur&lt;p&gt;&lt;author&gt;AAL Eindhoven MV+ MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="" package="SOT78A">
<connects>
<connect gate="G$1" pin="CM" pad="T1"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="LD" pad="T2"/>
</connects>
<technologies>
<technology name="-600B">
<attribute name="12NC" value="9340 600 72127"/>
</technology>
<technology name="-600BT">
<attribute name="12NC" value="9340 600 79127"/>
</technology>
<technology name="-600C">
<attribute name="12NC" value="9340 600 74127"/>
</technology>
<technology name="-600D">
<attribute name="12NC" value="9340 600 76127"/>
</technology>
<technology name="-600E">
<attribute name="12NC" value="9340 600 77127"/>
</technology>
<technology name="-600ET">
<attribute name="12NC" value="9340 646 18127"/>
</technology>
<technology name="-800B">
<attribute name="12NC" value="9340 600 73127"/>
</technology>
<technology name="-800C">
<attribute name="12NC" value="9340 600 75127"/>
</technology>
<technology name="-800E">
<attribute name="12NC" value="9340 600 78127"/>
</technology>
<technology name="-800ET">
<attribute name="12NC" value="9340 646 19127"/>
</technology>
</technologies>
</device>
<device name="B" package="SOT404">
<connects>
<connect gate="G$1" pin="CM" pad="1"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="LD" pad="MB"/>
</connects>
<technologies>
<technology name="-600B">
<attribute name="12NC" value="9340 601 04118"/>
</technology>
<technology name="-600C">
<attribute name="12NC" value="9340 601 06118"/>
</technology>
<technology name="-600E">
<attribute name="12NC" value="9340 601 08118"/>
</technology>
<technology name="-800B">
<attribute name="12NC" value="9340 601 05118"/>
</technology>
<technology name="-800C">
<attribute name="12NC" value="9340 601 07118"/>
</technology>
<technology name="-800E">
<attribute name="12NC" value="9340 601 09118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTA316-800E" prefix="T">
<description>Planar passivated high commutation three quadrant triac in a SOT78 plastic package 
intended for use in circuits where high static and dynamic dV/dt and high dI/dt can occur&lt;p&gt;&lt;author&gt;AAL Eindhoven MV+ MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="" package="SOT78A">
<connects>
<connect gate="G$1" pin="CM" pad="T1"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="LD" pad="T2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SAMPLEDESK" value="12NC934060078127"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACT108W" prefix="T">
<description>&lt;H2&gt;AC Thyristor power switch&lt;/H2&gt;AC Thyristor power switch in a SOT223 surface-mountable plastic package with 
self-protective capabilities against low and high energy transients&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="CM" pad="2 4"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="LD" pad="1"/>
</connects>
<technologies>
<technology name="-600D">
<attribute name="12NC" value="9340 644 42135"/>
</technology>
<technology name="-600E">
<attribute name="12NC" value="9340 633 73135"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL_0.6-1.2MM" prefix="X">
<gates>
<gate name="G$1" symbol="DOT"/>
</gates>
<devices>
<device name="" package="FIDUCIAL0.6-1.2">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMLL4148L" prefix="D">
<description>Single high-speed switching diodes, fabricated in planar technology, and encapsulated in small hermetically sealed glass SOD80C Surface-Mounted Device (SMD) packages.
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD80C">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="FARNELL" value="1097176"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PRTR5V0U4AD" prefix="IC">
<description>ESD protection
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="ESD-PROTECTION_ESD"/>
</gates>
<devices>
<device name="" package="SOT457">
<connects>
<connect gate="G$1" pin="ESD1" pad="1"/>
<connect gate="G$1" pin="ESD2" pad="3"/>
<connect gate="G$1" pin="ESD3" pad="4"/>
<connect gate="G$1" pin="ESD4" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="FARNELL" value="1757868"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC122XFBD48" prefix="U">
<description>NXP ARM M0 32 bit Microcontroller&lt;p&gt;
&lt;author&gt;AAL Eindhoven MV+ MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC12XX_48P"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_13/EZH13" pad="28"/>
<connect gate="G$1" pin="!TRST!/PIO1_1/AD3" pad="37"/>
<connect gate="G$1" pin="PIO0_0/EZH0/!RTS0!" pad="15"/>
<connect gate="G$1" pin="PIO0_1/EZH1/RXD0/CT32B0_0" pad="16"/>
<connect gate="G$1" pin="PIO0_10/EZH10/SCL" pad="25"/>
<connect gate="G$1" pin="PIO0_11/EZH11/SDA/CT16B0_0" pad="26"/>
<connect gate="G$1" pin="PIO0_12/EZH12/CLKOUT/CT16B0_1" pad="27"/>
<connect gate="G$1" pin="PIO0_14/EZH14/SCK" pad="29"/>
<connect gate="G$1" pin="PIO0_15/EZH15/SSEL/CT16B1_0" pad="30"/>
<connect gate="G$1" pin="PIO0_16/EZH0/MISO/CT16B1_1" pad="31"/>
<connect gate="G$1" pin="PIO0_17/EZH1/MOSI" pad="32"/>
<connect gate="G$1" pin="PIO0_19/EZH3/C0_IN0/CT32B0_1" pad="4"/>
<connect gate="G$1" pin="PIO0_2/EZH2/TXD0/CT32B0_1" pad="17"/>
<connect gate="G$1" pin="PIO0_20/EZH4/C0_IN1/CT32B0_2" pad="5"/>
<connect gate="G$1" pin="PIO0_21/EZH5/C0_IN2/CT32B0_3" pad="6"/>
<connect gate="G$1" pin="PIO0_22/EZH6/C0_IN3" pad="7"/>
<connect gate="G$1" pin="PIO0_23/EZH7/C1_IN0/CT32B1_0" pad="8"/>
<connect gate="G$1" pin="PIO0_24/EZH8/C1_IN1/CT32B1_1" pad="9"/>
<connect gate="G$1" pin="PIO0_25/EZH9/C1_IN2/CT32B1_2/SWDIO" pad="10"/>
<connect gate="G$1" pin="PIO0_26/EZH10/C1_IN3/CT32B1_3/SWCLK" pad="11"/>
<connect gate="G$1" pin="PIO0_27/EZH11/C0_OUT" pad="12"/>
<connect gate="G$1" pin="PIO0_28/EZH12/C1_OUT/CT16B0_0" pad="13"/>
<connect gate="G$1" pin="PIO0_29/EZH13/ROSC/CT16B0_1" pad="14"/>
<connect gate="G$1" pin="PIO0_3/EZH3/!DTR0!/CT32B0_2" pad="18"/>
<connect gate="G$1" pin="PIO0_4/EZH4/!DSR0!/CT32B0_3" pad="19"/>
<connect gate="G$1" pin="PIO0_5/EZH5/!DCD0!" pad="20"/>
<connect gate="G$1" pin="PIO0_6/EZH6/!RI0!/CT32B1_0" pad="21"/>
<connect gate="G$1" pin="PIO0_7/EZH7/!CTS0!/CT32B1_1" pad="22"/>
<connect gate="G$1" pin="PIO0_8/EZH8/RXD1/CT32B1_2" pad="23"/>
<connect gate="G$1" pin="PIO0_9/EZH9/TXD1/CT32B1_3" pad="24"/>
<connect gate="G$1" pin="PIO1_3/AD5/WAKEUP" pad="39"/>
<connect gate="G$1" pin="PIO1_4/AD6" pad="40"/>
<connect gate="G$1" pin="PIO1_5/AD7/CT16B1_0" pad="41"/>
<connect gate="G$1" pin="PIO1_6/CT16B1_1" pad="42"/>
<connect gate="G$1" pin="RTCXIN" pad="46"/>
<connect gate="G$1" pin="RTCXOUT" pad="45"/>
<connect gate="G$1" pin="SWCLK/PIO0_18/EZH2/CT32B0_0" pad="33"/>
<connect gate="G$1" pin="SWDIO/PIO1_2/AD4" pad="38"/>
<connect gate="G$1" pin="TDI/PIO0_31/EZH15/AD1" pad="35"/>
<connect gate="G$1" pin="TDO/PIO0_30/EZH14/AD0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD2" pad="36"/>
<connect gate="G$1" pin="VDD(3V3)" pad="44"/>
<connect gate="G$1" pin="VDD(IO)" pad="47"/>
<connect gate="G$1" pin="VREF_CMP" pad="3"/>
<connect gate="G$1" pin="VSS" pad="43"/>
<connect gate="G$1" pin="VSSIO" pad="48"/>
<connect gate="G$1" pin="XTALIN" pad="1"/>
<connect gate="G$1" pin="XTALOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CLRC663" prefix="U">
<description>NXP ISO14443 ISO15693 reader IC &lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/bbimages/NXP_logo.gif"&gt;</description>
<gates>
<gate name="G$1" symbol="CLRC663"/>
</gates>
<devices>
<device name="01HN1" package="SOT617-1">
<connects>
<connect gate="G$1" pin="AUX1" pad="10"/>
<connect gate="G$1" pin="AUX2" pad="11"/>
<connect gate="G$1" pin="AVDD" pad="9"/>
<connect gate="G$1" pin="CLKOUT" pad="22"/>
<connect gate="G$1" pin="DVDD" pad="7"/>
<connect gate="G$1" pin="GPIO0" pad="5"/>
<connect gate="G$1" pin="IF0" pad="28"/>
<connect gate="G$1" pin="IF1" pad="29"/>
<connect gate="G$1" pin="IF2" pad="30"/>
<connect gate="G$1" pin="IF3-SDA" pad="31"/>
<connect gate="G$1" pin="IFSEL0" pad="26"/>
<connect gate="G$1" pin="IFSEL1" pad="27"/>
<connect gate="G$1" pin="IRQ" pad="32"/>
<connect gate="G$1" pin="PDOWN" pad="21"/>
<connect gate="G$1" pin="PVDD" pad="25"/>
<connect gate="G$1" pin="RXN" pad="13"/>
<connect gate="G$1" pin="RXP" pad="12"/>
<connect gate="G$1" pin="SCL2" pad="23"/>
<connect gate="G$1" pin="SDA2" pad="24"/>
<connect gate="G$1" pin="SIGOUT" pad="6"/>
<connect gate="G$1" pin="TCK" pad="4"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO" pad="1"/>
<connect gate="G$1" pin="TMS" pad="3"/>
<connect gate="G$1" pin="TVDD" pad="18"/>
<connect gate="G$1" pin="TVSS" pad="16"/>
<connect gate="G$1" pin="TX1" pad="17"/>
<connect gate="G$1" pin="TX2" pad="15"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VMID" pad="14"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTVS3V3P1UP" prefix="D">
<description>NXP TVS Diode
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/bbimages/NXP_logo.gif&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="934064143115"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1111FHN33" prefix="U">
<description>&lt;b&gt;LPC1111 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;Pacjake according to datasheet
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114FHN33"/>
</gates>
<devices>
<device name="" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1112FHN33" prefix="U">
<description>&lt;b&gt;LPC1112 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114FHN33"/>
</gates>
<devices>
<device name="" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1113FHN33" prefix="U">
<description>&lt;b&gt;LPC1113 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114FHN33"/>
</gates>
<devices>
<device name="" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1114FBD48/301/302" prefix="IC">
<description>&lt;b&gt;LPC1114 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1/SWO" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/!DTR!/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO2_1/!DSR!/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK0" pad="31"/>
<connect gate="G$1" pin="PIO2_2/!DCD!/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO2_3/!RI!/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="19"/>
<connect gate="G$1" pin="PIO2_5" pad="20"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0/!DTR!" pad="36"/>
<connect gate="G$1" pin="PIO3_1/!DSR!" pad="37"/>
<connect gate="G$1" pin="PIO3_2/!DCD!" pad="43"/>
<connect gate="G$1" pin="PIO3_3/!RI!" pad="48"/>
<connect gate="G$1" pin="PIO3_4" pad="18"/>
<connect gate="G$1" pin="PIO3_5" pad="21"/>
<connect gate="G$1" pin="R/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="R/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="R/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="R/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="VDD@1" pad="8"/>
<connect gate="G$1" pin="VDD@2" pad="44"/>
<connect gate="G$1" pin="VSS@1" pad="41"/>
<connect gate="G$1" pin="VSS@2" pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1114FHN33" prefix="U">
<description>&lt;b&gt;LPC1114 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114FHN33"/>
</gates>
<devices>
<device name="" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1311FHN33" prefix="U">
<description>&lt;b&gt;LPC1311 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 8 kB Flash, 4 kB SRAM &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
Modified by MK: added second HVQFN33 package according datasheet specification. &lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1313FHN33"/>
</gates>
<devices>
<device name="NXP" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK" pad="15"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="HVQFN33-7X7">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK" pad="15"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1313FBD48" prefix="U">
<description>&lt;b&gt;LPC1313 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 32 kB Flash, 8 kB SRAM &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1313FBD48"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="2"/>
<connect gate="G$1" pin="PIO2_1/DSR" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK" pad="31"/>
<connect gate="G$1" pin="PIO2_2/DCD" pad="26"/>
<connect gate="G$1" pin="PIO2_3/RI" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="19"/>
<connect gate="G$1" pin="PIO2_5" pad="20"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0" pad="36"/>
<connect gate="G$1" pin="PIO3_1" pad="37"/>
<connect gate="G$1" pin="PIO3_2" pad="43"/>
<connect gate="G$1" pin="PIO3_3" pad="48"/>
<connect gate="G$1" pin="PIO3_4" pad="18"/>
<connect gate="G$1" pin="PIO3_5" pad="21"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="VDD(3V3)" pad="44"/>
<connect gate="G$1" pin="VDD(IO)" pad="8"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="VSSIO" pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1313FHN33" prefix="U">
<description>&lt;b&gt;LPC1313 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 32 kB Flash, 8 kB SRAM &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
Modified by MK: added second HVQFN33 package according datasheet specification. &lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1313FHN33"/>
</gates>
<devices>
<device name="" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK" pad="15"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1342FHN33" prefix="U">
<description>&lt;b&gt;LPC1342 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 16 kB Flash, 4 kB SRAM, USB Device &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
Modified by MK: added second HVQFN33 package according datasheet specification. &lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1343FHN33"/>
</gates>
<devices>
<device name="" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK" pad="15"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="USB_DM" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="14"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1343FBD48" prefix="U">
<description>&lt;b&gt;LPC1343 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 32 kB Flash, 8 kB SRAM, USB Device &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1343FBD48"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="2"/>
<connect gate="G$1" pin="PIO2_1/DSR" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK" pad="31"/>
<connect gate="G$1" pin="PIO2_2/DCD" pad="26"/>
<connect gate="G$1" pin="PIO2_3/RI" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="18"/>
<connect gate="G$1" pin="PIO2_5" pad="21"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0" pad="36"/>
<connect gate="G$1" pin="PIO3_1" pad="37"/>
<connect gate="G$1" pin="PIO3_2" pad="43"/>
<connect gate="G$1" pin="PIO3_3" pad="48"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD(3V3)" pad="44"/>
<connect gate="G$1" pin="VDD(IO)" pad="8"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="VSSIO" pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1343FHN33" prefix="U">
<description>&lt;b&gt;LPC1343 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 32 kB Flash, 8 kB SRAM, USB Device &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
Modified by MK: added second HVQFN33 package according datasheet specification. &lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1343FHN33"/>
</gates>
<devices>
<device name="" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK" pad="15"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="USB_DM" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="14"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1751FBD80" prefix="U">
<description>&lt;b&gt;LPC1751 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 32 kB Flash, 8 kB SRAM, USB Device, CAN &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC175X"/>
</gates>
<devices>
<device name="" package="SOT315-1">
<connects>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="37"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="39"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="40"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="47"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="48"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="46"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="45"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="38"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="44"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="22"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="79"/>
<connect gate="G$1" pin="P0[30]/USB_DMIN" pad="23"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="64"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="63"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="62"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="61"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="76"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="71"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="70"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="69"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="25"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="26"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="75"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="27"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="28"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="29"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="30"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="31"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="32"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="35"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="36"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="18"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="17"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="74"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="73"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="72"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="60"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="41"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="59"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="58"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="55"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="54"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="53"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="52"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="51"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="50"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="49"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="65"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="68"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="RSTOUT" pad="11"/>
<connect gate="G$1" pin="RTCX1" pad="13"/>
<connect gate="G$1" pin="RTCX2" pad="15"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="16"/>
<connect gate="G$1" pin="VDD(3V3)1" pad="21"/>
<connect gate="G$1" pin="VDD(3V3)2" pad="42"/>
<connect gate="G$1" pin="VDD(3V3)3" pad="56"/>
<connect gate="G$1" pin="VDD(3V3)4" pad="77"/>
<connect gate="G$1" pin="VDD(REG)(3V3)1" pad="34"/>
<connect gate="G$1" pin="VDD(REG)(3V3)2" pad="67"/>
<connect gate="G$1" pin="VDDA" pad="8"/>
<connect gate="G$1" pin="VREFN" pad="12"/>
<connect gate="G$1" pin="VREFP" pad="10"/>
<connect gate="G$1" pin="VSS1" pad="24"/>
<connect gate="G$1" pin="VSS2" pad="33"/>
<connect gate="G$1" pin="VSS3" pad="43"/>
<connect gate="G$1" pin="VSS4" pad="57"/>
<connect gate="G$1" pin="VSS5" pad="66"/>
<connect gate="G$1" pin="VSS6" pad="78"/>
<connect gate="G$1" pin="VSSA" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1752FBD80" prefix="IC">
<description>&lt;b&gt;LPC1752 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 64 kB Flash, 16 kB SRAM, USB Device, CAN &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC175X"/>
</gates>
<devices>
<device name="" package="SOT315-1">
<connects>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="37"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="39"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="40"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="47"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="48"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="46"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="45"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="38"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="44"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="22"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="79"/>
<connect gate="G$1" pin="P0[30]/USB_DMIN" pad="23"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="64"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="63"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="62"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="61"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="76"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="71"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="70"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="69"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="25"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="26"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="75"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="27"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="28"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="29"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="30"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="31"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="32"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="35"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="36"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="18"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="17"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="74"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="73"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="72"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="60"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="41"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="59"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="58"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="55"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="54"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="53"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="52"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="51"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="50"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="49"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="65"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="68"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="RSTOUT" pad="11"/>
<connect gate="G$1" pin="RTCX1" pad="13"/>
<connect gate="G$1" pin="RTCX2" pad="15"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="16"/>
<connect gate="G$1" pin="VDD(3V3)1" pad="21"/>
<connect gate="G$1" pin="VDD(3V3)2" pad="42"/>
<connect gate="G$1" pin="VDD(3V3)3" pad="56"/>
<connect gate="G$1" pin="VDD(3V3)4" pad="77"/>
<connect gate="G$1" pin="VDD(REG)(3V3)1" pad="34"/>
<connect gate="G$1" pin="VDD(REG)(3V3)2" pad="67"/>
<connect gate="G$1" pin="VDDA" pad="8"/>
<connect gate="G$1" pin="VREFN" pad="12"/>
<connect gate="G$1" pin="VREFP" pad="10"/>
<connect gate="G$1" pin="VSS1" pad="24"/>
<connect gate="G$1" pin="VSS2" pad="33"/>
<connect gate="G$1" pin="VSS3" pad="43"/>
<connect gate="G$1" pin="VSS4" pad="57"/>
<connect gate="G$1" pin="VSS5" pad="66"/>
<connect gate="G$1" pin="VSS6" pad="78"/>
<connect gate="G$1" pin="VSSA" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1754FBD80" prefix="IC">
<description>&lt;b&gt;LPC1754 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 128 kB Flash, 32 kB SRAM, USB Device/Host/OTG, CAN, DAC &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC175X"/>
</gates>
<devices>
<device name="" package="SOT315-1">
<connects>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="37"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="39"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="40"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="47"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="48"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="46"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="45"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="38"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="44"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="22"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="79"/>
<connect gate="G$1" pin="P0[30]/USB_DMIN" pad="23"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="64"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="63"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="62"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="61"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="76"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="71"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="70"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="69"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="25"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="26"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="75"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="27"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="28"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="29"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="30"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="31"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="32"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="35"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="36"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="18"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="17"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="74"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="73"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="72"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="60"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="41"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="59"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="58"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="55"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="54"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="53"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="52"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="51"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="50"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="49"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="65"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="68"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="RSTOUT" pad="11"/>
<connect gate="G$1" pin="RTCX1" pad="13"/>
<connect gate="G$1" pin="RTCX2" pad="15"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="16"/>
<connect gate="G$1" pin="VDD(3V3)1" pad="21"/>
<connect gate="G$1" pin="VDD(3V3)2" pad="42"/>
<connect gate="G$1" pin="VDD(3V3)3" pad="56"/>
<connect gate="G$1" pin="VDD(3V3)4" pad="77"/>
<connect gate="G$1" pin="VDD(REG)(3V3)1" pad="34"/>
<connect gate="G$1" pin="VDD(REG)(3V3)2" pad="67"/>
<connect gate="G$1" pin="VDDA" pad="8"/>
<connect gate="G$1" pin="VREFN" pad="12"/>
<connect gate="G$1" pin="VREFP" pad="10"/>
<connect gate="G$1" pin="VSS1" pad="24"/>
<connect gate="G$1" pin="VSS2" pad="33"/>
<connect gate="G$1" pin="VSS3" pad="43"/>
<connect gate="G$1" pin="VSS4" pad="57"/>
<connect gate="G$1" pin="VSS5" pad="66"/>
<connect gate="G$1" pin="VSS6" pad="78"/>
<connect gate="G$1" pin="VSSA" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1756FBD80" prefix="IC">
<description>&lt;b&gt;LPC1756 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 256 kB Flash, 32 kB SRAM, USB Device/Host/OTG, 2 CAN, DAC &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC175X"/>
</gates>
<devices>
<device name="" package="SOT315-1">
<connects>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="37"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="39"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="40"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="47"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="48"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="46"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="45"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="38"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="44"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="22"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="79"/>
<connect gate="G$1" pin="P0[30]/USB_DMIN" pad="23"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="64"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="63"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="62"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="61"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="76"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="71"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="70"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="69"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="25"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="26"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="75"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="27"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="28"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="29"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="30"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="31"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="32"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="35"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="36"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="18"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="17"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="74"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="73"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="72"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="60"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="41"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="59"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="58"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="55"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="54"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="53"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="52"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="51"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="50"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="49"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="65"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="68"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="RSTOUT" pad="11"/>
<connect gate="G$1" pin="RTCX1" pad="13"/>
<connect gate="G$1" pin="RTCX2" pad="15"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="16"/>
<connect gate="G$1" pin="VDD(3V3)1" pad="21"/>
<connect gate="G$1" pin="VDD(3V3)2" pad="42"/>
<connect gate="G$1" pin="VDD(3V3)3" pad="56"/>
<connect gate="G$1" pin="VDD(3V3)4" pad="77"/>
<connect gate="G$1" pin="VDD(REG)(3V3)1" pad="34"/>
<connect gate="G$1" pin="VDD(REG)(3V3)2" pad="67"/>
<connect gate="G$1" pin="VDDA" pad="8"/>
<connect gate="G$1" pin="VREFN" pad="12"/>
<connect gate="G$1" pin="VREFP" pad="10"/>
<connect gate="G$1" pin="VSS1" pad="24"/>
<connect gate="G$1" pin="VSS2" pad="33"/>
<connect gate="G$1" pin="VSS3" pad="43"/>
<connect gate="G$1" pin="VSS4" pad="57"/>
<connect gate="G$1" pin="VSS5" pad="66"/>
<connect gate="G$1" pin="VSS6" pad="78"/>
<connect gate="G$1" pin="VSSA" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1758FBD80" prefix="IC">
<description>&lt;b&gt;LPC1758 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 512 kB Flash, 64 kB SRAM, USB Device/Host/OTG, 2 CAN, DAC, Ethernet &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC175X"/>
</gates>
<devices>
<device name="" package="SOT315-1">
<connects>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="37"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="39"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="40"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="47"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="48"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="46"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="45"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="38"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="44"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="22"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="79"/>
<connect gate="G$1" pin="P0[30]/USB_DMIN" pad="23"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="64"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="63"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="62"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="61"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="76"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="71"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="70"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="69"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="25"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="26"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="75"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="27"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="28"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="29"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="30"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="31"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="32"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="35"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="36"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="18"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="17"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="74"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="73"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="72"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="60"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="41"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="59"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="58"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="55"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="54"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="53"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="52"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="51"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="50"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="49"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="65"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="68"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="RSTOUT" pad="11"/>
<connect gate="G$1" pin="RTCX1" pad="13"/>
<connect gate="G$1" pin="RTCX2" pad="15"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="16"/>
<connect gate="G$1" pin="VDD(3V3)1" pad="21"/>
<connect gate="G$1" pin="VDD(3V3)2" pad="42"/>
<connect gate="G$1" pin="VDD(3V3)3" pad="56"/>
<connect gate="G$1" pin="VDD(3V3)4" pad="77"/>
<connect gate="G$1" pin="VDD(REG)(3V3)1" pad="34"/>
<connect gate="G$1" pin="VDD(REG)(3V3)2" pad="67"/>
<connect gate="G$1" pin="VDDA" pad="8"/>
<connect gate="G$1" pin="VREFN" pad="12"/>
<connect gate="G$1" pin="VREFP" pad="10"/>
<connect gate="G$1" pin="VSS1" pad="24"/>
<connect gate="G$1" pin="VSS2" pad="33"/>
<connect gate="G$1" pin="VSS3" pad="43"/>
<connect gate="G$1" pin="VSS4" pad="57"/>
<connect gate="G$1" pin="VSS5" pad="66"/>
<connect gate="G$1" pin="VSS6" pad="78"/>
<connect gate="G$1" pin="VSSA" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1764FBD100" prefix="U">
<description>&lt;b&gt;LPC1764 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 128 kB Flash, 32 kB SRAM, USB Device, 2 CAN, Ethernet &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC176X"/>
</gates>
<devices>
<device name="" package="SOT407-1">
<connects>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="46"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="48"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="49"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="62"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="63"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="61"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="60"/>
<connect gate="G$1" pin="P0[19]/DSR1/SDA1" pad="59"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="47"/>
<connect gate="G$1" pin="P0[20]/DTR1/SCL1" pad="58"/>
<connect gate="G$1" pin="P0[21]/RI1/RD1" pad="57"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="56"/>
<connect gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]" pad="9"/>
<connect gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]" pad="8"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[27]/SDA0/USB_SDA" pad="25"/>
<connect gate="G$1" pin="P0[28]/SCL0/USB_SCL" pad="24"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="29"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="98"/>
<connect gate="G$1" pin="P0[30]/USB_DMINUS" pad="30"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="99"/>
<connect gate="G$1" pin="P0[4]/I2SRX_CLK/RD2/CAP2[0]" pad="81"/>
<connect gate="G$1" pin="P0[5]/I2SRX_WS/TD2/CAP2[1]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="79"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="78"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="77"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="76"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="95"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="90"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="89"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="88"/>
<connect gate="G$1" pin="P1[16]/ENET_MDC" pad="87"/>
<connect gate="G$1" pin="P1[17]/ENET_MDIO" pad="86"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="32"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="33"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="94"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="34"/>
<connect gate="G$1" pin="P1[21]/MCABORT/PWM1[3]/SSEL0" pad="35"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="36"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="37"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="38"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="39"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="40"/>
<connect gate="G$1" pin="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]" pad="43"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="44"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="45"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="21"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="20"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="93"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="92"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="91"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="75"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="53"/>
<connect gate="G$1" pin="P2[11]/EINT1/I2STX_CLK" pad="52"/>
<connect gate="G$1" pin="P2[12]/EINT2/I2STX_WS" pad="51"/>
<connect gate="G$1" pin="P2[13]/EINT3/I2STX_SDA" pad="50"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="74"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="73"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="70"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="69"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="68"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="67"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="66"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="65"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="64"/>
<connect gate="G$1" pin="P3[25]/MAT0[0]/PWM1[2]" pad="27"/>
<connect gate="G$1" pin="P3[26]/STCLK/MAT0[1]/PWM1[3]" pad="26"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="82"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="85"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="RSTOUT" pad="14"/>
<connect gate="G$1" pin="RTCK" pad="100"/>
<connect gate="G$1" pin="RTCX1" pad="16"/>
<connect gate="G$1" pin="RTCX2" pad="18"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VDD(3V3)@1" pad="28"/>
<connect gate="G$1" pin="VDD(3V3)@2" pad="54"/>
<connect gate="G$1" pin="VDD(3V3)@3" pad="71"/>
<connect gate="G$1" pin="VDD(3V3)@4" pad="96"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@1" pad="42"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@2" pad="84"/>
<connect gate="G$1" pin="VDDA" pad="10"/>
<connect gate="G$1" pin="VREFN" pad="15"/>
<connect gate="G$1" pin="VREFP" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="31"/>
<connect gate="G$1" pin="VSS2" pad="41"/>
<connect gate="G$1" pin="VSS3" pad="55"/>
<connect gate="G$1" pin="VSS4" pad="72"/>
<connect gate="G$1" pin="VSS5" pad="97"/>
<connect gate="G$1" pin="VSS6" pad="83"/>
<connect gate="G$1" pin="VSSA" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="22"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1765FBD100" prefix="IC">
<description>&lt;b&gt;LPC1765 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 256 kB Flash, 64 kB SRAM, USB Device/Host/OTG, 2 CAN, DAC &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC176X"/>
</gates>
<devices>
<device name="" package="SOT407-1">
<connects>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="46"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="48"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="49"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="62"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="63"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="61"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="60"/>
<connect gate="G$1" pin="P0[19]/DSR1/SDA1" pad="59"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="47"/>
<connect gate="G$1" pin="P0[20]/DTR1/SCL1" pad="58"/>
<connect gate="G$1" pin="P0[21]/RI1/RD1" pad="57"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="56"/>
<connect gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]" pad="9"/>
<connect gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]" pad="8"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[27]/SDA0/USB_SDA" pad="25"/>
<connect gate="G$1" pin="P0[28]/SCL0/USB_SCL" pad="24"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="29"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="98"/>
<connect gate="G$1" pin="P0[30]/USB_DMINUS" pad="30"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="99"/>
<connect gate="G$1" pin="P0[4]/I2SRX_CLK/RD2/CAP2[0]" pad="81"/>
<connect gate="G$1" pin="P0[5]/I2SRX_WS/TD2/CAP2[1]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="79"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="78"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="77"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="76"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="95"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="90"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="89"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="88"/>
<connect gate="G$1" pin="P1[16]/ENET_MDC" pad="87"/>
<connect gate="G$1" pin="P1[17]/ENET_MDIO" pad="86"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="32"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="33"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="94"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="34"/>
<connect gate="G$1" pin="P1[21]/MCABORT/PWM1[3]/SSEL0" pad="35"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="36"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="37"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="38"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="39"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="40"/>
<connect gate="G$1" pin="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]" pad="43"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="44"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="45"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="21"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="20"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="93"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="92"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="91"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="75"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="53"/>
<connect gate="G$1" pin="P2[11]/EINT1/I2STX_CLK" pad="52"/>
<connect gate="G$1" pin="P2[12]/EINT2/I2STX_WS" pad="51"/>
<connect gate="G$1" pin="P2[13]/EINT3/I2STX_SDA" pad="50"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="74"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="73"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="70"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="69"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="68"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="67"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="66"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="65"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="64"/>
<connect gate="G$1" pin="P3[25]/MAT0[0]/PWM1[2]" pad="27"/>
<connect gate="G$1" pin="P3[26]/STCLK/MAT0[1]/PWM1[3]" pad="26"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="82"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="85"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="RSTOUT" pad="14"/>
<connect gate="G$1" pin="RTCK" pad="100"/>
<connect gate="G$1" pin="RTCX1" pad="16"/>
<connect gate="G$1" pin="RTCX2" pad="18"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VDD(3V3)@1" pad="28"/>
<connect gate="G$1" pin="VDD(3V3)@2" pad="54"/>
<connect gate="G$1" pin="VDD(3V3)@3" pad="71"/>
<connect gate="G$1" pin="VDD(3V3)@4" pad="96"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@1" pad="42"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@2" pad="84"/>
<connect gate="G$1" pin="VDDA" pad="10"/>
<connect gate="G$1" pin="VREFN" pad="15"/>
<connect gate="G$1" pin="VREFP" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="31"/>
<connect gate="G$1" pin="VSS2" pad="41"/>
<connect gate="G$1" pin="VSS3" pad="55"/>
<connect gate="G$1" pin="VSS4" pad="72"/>
<connect gate="G$1" pin="VSS5" pad="97"/>
<connect gate="G$1" pin="VSS6" pad="83"/>
<connect gate="G$1" pin="VSSA" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="22"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1766FBD100" prefix="IC">
<description>&lt;b&gt;LPC1766 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 256 kB Flash, 64 kB SRAM, USB Device/Host/OTG, 2 CAN, DAC, Ethernet &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC176X"/>
</gates>
<devices>
<device name="" package="SOT407-1">
<connects>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="46"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="48"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="49"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="62"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="63"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="61"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="60"/>
<connect gate="G$1" pin="P0[19]/DSR1/SDA1" pad="59"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="47"/>
<connect gate="G$1" pin="P0[20]/DTR1/SCL1" pad="58"/>
<connect gate="G$1" pin="P0[21]/RI1/RD1" pad="57"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="56"/>
<connect gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]" pad="9"/>
<connect gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]" pad="8"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[27]/SDA0/USB_SDA" pad="25"/>
<connect gate="G$1" pin="P0[28]/SCL0/USB_SCL" pad="24"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="29"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="98"/>
<connect gate="G$1" pin="P0[30]/USB_DMINUS" pad="30"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="99"/>
<connect gate="G$1" pin="P0[4]/I2SRX_CLK/RD2/CAP2[0]" pad="81"/>
<connect gate="G$1" pin="P0[5]/I2SRX_WS/TD2/CAP2[1]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="79"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="78"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="77"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="76"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="95"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="90"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="89"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="88"/>
<connect gate="G$1" pin="P1[16]/ENET_MDC" pad="87"/>
<connect gate="G$1" pin="P1[17]/ENET_MDIO" pad="86"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="32"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="33"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="94"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="34"/>
<connect gate="G$1" pin="P1[21]/MCABORT/PWM1[3]/SSEL0" pad="35"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="36"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="37"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="38"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="39"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="40"/>
<connect gate="G$1" pin="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]" pad="43"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="44"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="45"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="21"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="20"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="93"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="92"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="91"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="75"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="53"/>
<connect gate="G$1" pin="P2[11]/EINT1/I2STX_CLK" pad="52"/>
<connect gate="G$1" pin="P2[12]/EINT2/I2STX_WS" pad="51"/>
<connect gate="G$1" pin="P2[13]/EINT3/I2STX_SDA" pad="50"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="74"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="73"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="70"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="69"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="68"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="67"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="66"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="65"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="64"/>
<connect gate="G$1" pin="P3[25]/MAT0[0]/PWM1[2]" pad="27"/>
<connect gate="G$1" pin="P3[26]/STCLK/MAT0[1]/PWM1[3]" pad="26"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="82"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="85"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="RSTOUT" pad="14"/>
<connect gate="G$1" pin="RTCK" pad="100"/>
<connect gate="G$1" pin="RTCX1" pad="16"/>
<connect gate="G$1" pin="RTCX2" pad="18"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VDD(3V3)@1" pad="28"/>
<connect gate="G$1" pin="VDD(3V3)@2" pad="54"/>
<connect gate="G$1" pin="VDD(3V3)@3" pad="71"/>
<connect gate="G$1" pin="VDD(3V3)@4" pad="96"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@1" pad="42"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@2" pad="84"/>
<connect gate="G$1" pin="VDDA" pad="10"/>
<connect gate="G$1" pin="VREFN" pad="15"/>
<connect gate="G$1" pin="VREFP" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="31"/>
<connect gate="G$1" pin="VSS2" pad="41"/>
<connect gate="G$1" pin="VSS3" pad="55"/>
<connect gate="G$1" pin="VSS4" pad="72"/>
<connect gate="G$1" pin="VSS5" pad="97"/>
<connect gate="G$1" pin="VSS6" pad="83"/>
<connect gate="G$1" pin="VSSA" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="22"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1768FBD100" prefix="U">
<description>&lt;b&gt;LPC1768 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 512 kB Flash, 64 kB SRAM, USB Device/Host/OTG, 2 CAN, DAC, Ethernet &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC176X"/>
</gates>
<devices>
<device name="" package="SOT407-1">
<connects>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="46"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="48"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="49"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="62"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="63"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="61"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="60"/>
<connect gate="G$1" pin="P0[19]/DSR1/SDA1" pad="59"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="47"/>
<connect gate="G$1" pin="P0[20]/DTR1/SCL1" pad="58"/>
<connect gate="G$1" pin="P0[21]/RI1/RD1" pad="57"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="56"/>
<connect gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]" pad="9"/>
<connect gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]" pad="8"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[27]/SDA0/USB_SDA" pad="25"/>
<connect gate="G$1" pin="P0[28]/SCL0/USB_SCL" pad="24"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="29"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="98"/>
<connect gate="G$1" pin="P0[30]/USB_DMINUS" pad="30"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="99"/>
<connect gate="G$1" pin="P0[4]/I2SRX_CLK/RD2/CAP2[0]" pad="81"/>
<connect gate="G$1" pin="P0[5]/I2SRX_WS/TD2/CAP2[1]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="79"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="78"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="77"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="76"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="95"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="90"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="89"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="88"/>
<connect gate="G$1" pin="P1[16]/ENET_MDC" pad="87"/>
<connect gate="G$1" pin="P1[17]/ENET_MDIO" pad="86"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="32"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="33"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="94"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="34"/>
<connect gate="G$1" pin="P1[21]/MCABORT/PWM1[3]/SSEL0" pad="35"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="36"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="37"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="38"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="39"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="40"/>
<connect gate="G$1" pin="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]" pad="43"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="44"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="45"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="21"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="20"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="93"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="92"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="91"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="75"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="53"/>
<connect gate="G$1" pin="P2[11]/EINT1/I2STX_CLK" pad="52"/>
<connect gate="G$1" pin="P2[12]/EINT2/I2STX_WS" pad="51"/>
<connect gate="G$1" pin="P2[13]/EINT3/I2STX_SDA" pad="50"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="74"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="73"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="70"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="69"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="68"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="67"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="66"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="65"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="64"/>
<connect gate="G$1" pin="P3[25]/MAT0[0]/PWM1[2]" pad="27"/>
<connect gate="G$1" pin="P3[26]/STCLK/MAT0[1]/PWM1[3]" pad="26"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="82"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="85"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="RSTOUT" pad="14"/>
<connect gate="G$1" pin="RTCK" pad="100"/>
<connect gate="G$1" pin="RTCX1" pad="16"/>
<connect gate="G$1" pin="RTCX2" pad="18"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VDD(3V3)@1" pad="28"/>
<connect gate="G$1" pin="VDD(3V3)@2" pad="54"/>
<connect gate="G$1" pin="VDD(3V3)@3" pad="71"/>
<connect gate="G$1" pin="VDD(3V3)@4" pad="96"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@1" pad="42"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@2" pad="84"/>
<connect gate="G$1" pin="VDDA" pad="10"/>
<connect gate="G$1" pin="VREFN" pad="15"/>
<connect gate="G$1" pin="VREFP" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="31"/>
<connect gate="G$1" pin="VSS2" pad="41"/>
<connect gate="G$1" pin="VSS3" pad="55"/>
<connect gate="G$1" pin="VSS4" pad="72"/>
<connect gate="G$1" pin="VSS5" pad="97"/>
<connect gate="G$1" pin="VSS6" pad="83"/>
<connect gate="G$1" pin="VSSA" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="22"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1768FET100" prefix="U">
<description>&lt;b&gt;LPC1768 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 512 kB Flash, 64 kB SRAM, USB Device/Host/OTG, 2 CAN, DAC, Ethernet &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
&lt;author&gt;Package added by AAL Eindhoven MV+ MK&lt;/author&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1768FET"/>
</gates>
<devices>
<device name="" package="SOT926-1">
<connects>
<connect gate="G$1" pin="NC@1" pad="D4"/>
<connect gate="G$1" pin="NC@2" pad="E4"/>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="K8"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="H7"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="K9"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="F10"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="F8"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="F9"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="F6"/>
<connect gate="G$1" pin="P0[19]/DSR1/SDA1" pad="G10"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="J8"/>
<connect gate="G$1" pin="P0[20]/DTR1/SCL1" pad="G9"/>
<connect gate="G$1" pin="P0[21]/RI1/RD1" pad="G8"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="H10"/>
<connect gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]" pad="E5"/>
<connect gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]" pad="D1"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="D2"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="D3"/>
<connect gate="G$1" pin="P0[27]/SDA0/USB_SDA" pad="J2"/>
<connect gate="G$1" pin="P0[28]/SCL0/USB_SCL" pad="J1"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="J3"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="C4"/>
<connect gate="G$1" pin="P0[30]/USB_DMINUS" pad="G4"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="A2"/>
<connect gate="G$1" pin="P0[4]/I2SRX_CLK/RD2/CAP2[0]" pad="A8"/>
<connect gate="G$1" pin="P0[5]/I2SRX_WS/TD2/CAP2[1]" pad="D7"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="B8"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="A9"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="C8"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="A10"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="D5"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="A5"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="D6"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="C6"/>
<connect gate="G$1" pin="P1[16]/ENET_MDC" pad="A6"/>
<connect gate="G$1" pin="P1[17]/ENET_MDIO" pad="B6"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="H4"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="J4"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="B4"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="K4"/>
<connect gate="G$1" pin="P1[21]/MCABORT/PWM1[3]/SSEL0" pad="F5"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="J5"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="K5"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="H5"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="G5"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="K6"/>
<connect gate="G$1" pin="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]" pad="K7"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="J7"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="G6"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="H1"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="F4"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="A4"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="C5"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="B5"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="B9"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="J10"/>
<connect gate="G$1" pin="P2[11]/EINT1/I2STX_CLK" pad="H8"/>
<connect gate="G$1" pin="P2[12]/EINT2/I2STX_WS" pad="K10"/>
<connect gate="G$1" pin="P2[13]/EINT3/I2STX_SDA" pad="J9"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="B10"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="D8"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="E7"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="D9"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="D10"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="E8"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="E9"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/ENET_MDC" pad="E10"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2/ENET_MDIO" pad="F7"/>
<connect gate="G$1" pin="P3[25]/MAT0[0]/PWM1[2]" pad="H3"/>
<connect gate="G$1" pin="P3[26]/STCLK/MAT0[1]/PWM1[3]" pad="K1"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="C7"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="E6"/>
<connect gate="G$1" pin="RESET" pad="F3"/>
<connect gate="G$1" pin="RTCK" pad="B2"/>
<connect gate="G$1" pin="RTCX1" pad="F2"/>
<connect gate="G$1" pin="RTCX2" pad="G1"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="C1"/>
<connect gate="G$1" pin="TDI" pad="C3"/>
<connect gate="G$1" pin="TDO/SWO" pad="A1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="B1"/>
<connect gate="G$1" pin="TRST" pad="C2"/>
<connect gate="G$1" pin="VBAT" pad="G2"/>
<connect gate="G$1" pin="VDD(3V3)@1" pad="A3"/>
<connect gate="G$1" pin="VDD(3V3)@2" pad="C10"/>
<connect gate="G$1" pin="VDD(3V3)@3" pad="H9"/>
<connect gate="G$1" pin="VDD(3V3)@4" pad="K2"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@1" pad="A7"/>
<connect gate="G$1" pin="VDD(REG)(3V3)@2" pad="H6"/>
<connect gate="G$1" pin="VDDA" pad="E2"/>
<connect gate="G$1" pin="VREFN" pad="F1"/>
<connect gate="G$1" pin="VREFP" pad="E3"/>
<connect gate="G$1" pin="VSS@1" pad="B3"/>
<connect gate="G$1" pin="VSS@2" pad="B7"/>
<connect gate="G$1" pin="VSS@3" pad="C9"/>
<connect gate="G$1" pin="VSS@4" pad="G7"/>
<connect gate="G$1" pin="VSS@5" pad="J6"/>
<connect gate="G$1" pin="VSS@6" pad="K3"/>
<connect gate="G$1" pin="VSSA" pad="E1"/>
<connect gate="G$1" pin="XTAL1" pad="H2"/>
<connect gate="G$1" pin="XTAL2" pad="G3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NX1117CADJZ" prefix="U">
<description>The NX1117C/NX1117CE are two series of low-dropout positive voltage regulators with an output current capability of 1 A.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NX1117"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
<connect gate="G$1" pin="VOUT1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NX1117CEADJZ" prefix="U">
<description>The NX1117C/NX1117CE are two series of low-dropout positive voltage regulators with an output current capability of 1 A.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NX1117"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
<connect gate="G$1" pin="VOUT1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NX1117C" prefix="U">
<description>The NX1117C/NX1117CE are two series of low-dropout positive voltage regulators with an output current capability of 1 A.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NX1117GND"/>
</gates>
<devices>
<device name="Z" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
<connect gate="G$1" pin="VOUT1" pad="2"/>
</connects>
<technologies>
<technology name="12">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="15">
<attribute name="12NC" value="9352 914 35115"/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="18">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="19">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="20">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="25">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="285">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="33">
<attribute name="12NC" value="9352 914 42115"/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="50">
<attribute name="12NC" value="9352 914 43115"/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E12">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E15">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E18">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E19">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E20">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E25">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E285">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E33">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
<technology name="E50">
<attribute name="12NC" value=""/>
<attribute name="TOLERANCE" value="1.25%"/>
<attribute name="VOLTAGE" value="5.0V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8594C" prefix="U">
<description>The PCF8594C-2 is a ?oating gate Electrically Erasable Programmable Read Only Memory (EEPROM) with 4 kbits (512 × 8-bit) non-volatile storage.
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="MICRO-PHILIPS_EEPROM"/>
</gates>
<devices>
<device name="C-2T/02" package="SOT96-1">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PTC" pad="7"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SAMPLEDESK" value="12NC935195550118"/>
</technology>
</technologies>
</device>
<device name="C-2P/02" package="SOT97-1">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PTC" pad="7"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9525" prefix="U">
<description>The PCA9525 is a monolithic CMOS integrated circuit for bus buffering in applications including I2C-bus, SMBus, DDC, PMBus, and other systems based on similar principles.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="I2CDRIVER"/>
</gates>
<devices>
<device name="DP" package="SOT505-1">
<connects>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SCLI" pad="3"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="SDAI" pad="6"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="SOT96-1">
<connects>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SCLI" pad="3"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="SDAI" pad="6"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9605" prefix="U">
<description>The PCA9605 is a monolithic CMOS integrated circuit for bus buffering in applications including I2C-bus, SMBus, DDC, PMBus, and other systems based on similar principles.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="I2CDRIVER"/>
</gates>
<devices>
<device name="DP" package="SOT505-1">
<connects>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SCLI" pad="3"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="SDAI" pad="6"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="SOT96-1">
<connects>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SCLI" pad="3"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="SDAI" pad="6"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9646" prefix="U">
<description>The PCA9646 is a monolithic CMOS integrated circuit for 2-wire bus buffering and switching in applications including I2C-bus, SMBus, PMBus, and other systems based on similar principles.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/img/NXP_logo.png&gt;</description>
<gates>
<gate name="G$1" symbol="PCA9646"/>
</gates>
<devices>
<device name="PW" package="SOT403-1">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="RESET" pad="3"/>
<connect gate="G$1" pin="SC0" pad="5"/>
<connect gate="G$1" pin="SC1" pad="7"/>
<connect gate="G$1" pin="SC2" pad="10"/>
<connect gate="G$1" pin="SC3" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SD0" pad="4"/>
<connect gate="G$1" pin="SD1" pad="6"/>
<connect gate="G$1" pin="SD2" pad="9"/>
<connect gate="G$1" pin="SD3" pad="11"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="SOT109-1">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="RESET" pad="3"/>
<connect gate="G$1" pin="SC0" pad="5"/>
<connect gate="G$1" pin="SC1" pad="7"/>
<connect gate="G$1" pin="SC2" pad="10"/>
<connect gate="G$1" pin="SC3" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SD0" pad="4"/>
<connect gate="G$1" pin="SD1" pad="6"/>
<connect gate="G$1" pin="SD2" pad="9"/>
<connect gate="G$1" pin="SD3" pad="11"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC2G06" prefix="U">
<description>&lt;H2&gt;Inverters with open-drain outputs&lt;/H2&gt;The 74LVC2G06 provides two inverting buffers.
The output of this device is an open drain and can be connected to other open-drain 
outputs to implement active-LOW wired-OR or active-HIGH wired-AND functions.
Input can be driven from either 3.3 V or 5 V devices. This feature allows the use of this 
device in a mixed 3.3 V and 5 V environment.
Schmitt trigger action at all inputs makes the circuit tolerant for slower input rise and fall 
time. 
This device is fully specified for partial power-down applications using IOFF. The IOFF
circuitry disables the output, preventing the damaging backflow current through the device 
when it is powered down.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="-1" symbol="BUFFER_OPENDRAIN"/>
<gate name="-2" symbol="BUFFER_OPENDRAIN"/>
</gates>
<devices>
<device name="GW" package="SOT363">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 738 82125"/>
</technology>
</technologies>
</device>
<device name="GV" package="SOT457">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 738 81125"/>
</technology>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 771 68132"/>
</technology>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 824 31132"/>
</technology>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 929 27132"/>
</technology>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 917 99132"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCX2200" prefix="U">
<description>&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="GM" package="SOT886">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VEE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF3" package="SOT891">
<connects>
<connect gate="G$1" pin="+IN" pad="4"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VEE" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GW" package="SOT353-1">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VEE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1795" prefix="U">
<description>The TEA1795T is a member of the new generation of Synchronous Rectifier (SR) controller ICs for switched mode power supplies. Its high level of integration enables the design of a cost-effective power supply with a minimum number of external components.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/bbimages/NXP_logo.gif&gt;</description>
<gates>
<gate name="G$1" symbol="TEA1795"/>
</gates>
<devices>
<device name="T" package="SOT96-1">
<connects>
<connect gate="G$1" pin="DSA" pad="4"/>
<connect gate="G$1" pin="DSB" pad="5"/>
<connect gate="G$1" pin="GDA" pad="3"/>
<connect gate="G$1" pin="GDB" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SSA" pad="1"/>
<connect gate="G$1" pin="SSB" pad="8"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 915 64118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PESD5V0X1UB" prefix="D">
<description>Ultra low capacitance unidirectional ElectroStatic Discharge (ESD) protection diode in a 
SOD523 (SC-79) ultra small and flat lead Surface-Mounted Device (SMD) plastic 
package designed to protect one signal line from the damage caused by ESD and other 
transients.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/img/NXP_logo.png&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_ESD"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CBTL12131" prefix="U">
<description>DisplayPort multiplexer for bidirectional video&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/bbimages/NXP_logo.gif"&gt;</description>
<gates>
<gate name="G$1" symbol="CBTL12131"/>
</gates>
<devices>
<device name="ET" package="SOT543-1">
<connects>
<connect gate="G$1" pin="AUX_A_N" pad="H9"/>
<connect gate="G$1" pin="AUX_A_P" pad="H10"/>
<connect gate="G$1" pin="AUX_B_N" pad="C9"/>
<connect gate="G$1" pin="AUX_B_N_STATE" pad="D2"/>
<connect gate="G$1" pin="AUX_B_P" pad="C10"/>
<connect gate="G$1" pin="AUX_B_P_STATE" pad="D1"/>
<connect gate="G$1" pin="AUX_C_N" pad="H2"/>
<connect gate="G$1" pin="AUX_C_P" pad="H1"/>
<connect gate="G$1" pin="AUX_D_N" pad="C2"/>
<connect gate="G$1" pin="AUX_D_P" pad="C1"/>
<connect gate="G$1" pin="AUX_TERM_SNK" pad="G2"/>
<connect gate="G$1" pin="AUX_TERM_SRC" pad="G1"/>
<connect gate="G$1" pin="DDC_AUX_SEL" pad="D10"/>
<connect gate="G$1" pin="DDC_A_0" pad="G10"/>
<connect gate="G$1" pin="DDC_A_1" pad="G9"/>
<connect gate="G$1" pin="EQ5" pad="E10"/>
<connect gate="G$1" pin="GND@1" pad="B6"/>
<connect gate="G$1" pin="GND@2" pad="J6"/>
<connect gate="G$1" pin="GND@3" pad="F2"/>
<connect gate="G$1" pin="HPD_A" pad="K6"/>
<connect gate="G$1" pin="HPD_B" pad="A6"/>
<connect gate="G$1" pin="HPD_B_FLT" pad="F10"/>
<connect gate="G$1" pin="HPD_C" pad="K5"/>
<connect gate="G$1" pin="HPD_D" pad="A5"/>
<connect gate="G$1" pin="LV5" pad="F9"/>
<connect gate="G$1" pin="ML_A_0N" pad="J7"/>
<connect gate="G$1" pin="ML_A_0P" pad="K7"/>
<connect gate="G$1" pin="ML_A_1N" pad="J8"/>
<connect gate="G$1" pin="ML_A_1P" pad="K8"/>
<connect gate="G$1" pin="ML_A_2N" pad="J9"/>
<connect gate="G$1" pin="ML_A_2P" pad="K9"/>
<connect gate="G$1" pin="ML_A_3N" pad="J10"/>
<connect gate="G$1" pin="ML_A_3P" pad="K10"/>
<connect gate="G$1" pin="ML_B_0N" pad="B7"/>
<connect gate="G$1" pin="ML_B_0P" pad="A7"/>
<connect gate="G$1" pin="ML_B_1N" pad="B8"/>
<connect gate="G$1" pin="ML_B_1P" pad="A8"/>
<connect gate="G$1" pin="ML_B_2N" pad="B9"/>
<connect gate="G$1" pin="ML_B_2P" pad="A9"/>
<connect gate="G$1" pin="ML_B_3N" pad="B10"/>
<connect gate="G$1" pin="ML_B_3P" pad="A10"/>
<connect gate="G$1" pin="ML_C_0N" pad="J1"/>
<connect gate="G$1" pin="ML_C_0P" pad="K1"/>
<connect gate="G$1" pin="ML_C_1N" pad="J2"/>
<connect gate="G$1" pin="ML_C_1P" pad="K2"/>
<connect gate="G$1" pin="ML_C_2N" pad="J3"/>
<connect gate="G$1" pin="ML_C_2P" pad="K3"/>
<connect gate="G$1" pin="ML_C_3N" pad="J4"/>
<connect gate="G$1" pin="ML_C_3P" pad="K4"/>
<connect gate="G$1" pin="ML_D_0N" pad="B1"/>
<connect gate="G$1" pin="ML_D_0P" pad="A1"/>
<connect gate="G$1" pin="ML_D_1N" pad="B2"/>
<connect gate="G$1" pin="ML_D_1P" pad="A2"/>
<connect gate="G$1" pin="ML_D_2N" pad="B3"/>
<connect gate="G$1" pin="ML_D_2P" pad="A3"/>
<connect gate="G$1" pin="ML_D_3N" pad="B4"/>
<connect gate="G$1" pin="ML_D_3P" pad="A4"/>
<connect gate="G$1" pin="PATH_SEL" pad="E1"/>
<connect gate="G$1" pin="PL5" pad="D9"/>
<connect gate="G$1" pin="TST_REXT" pad="F1"/>
<connect gate="G$1" pin="VDD@1" pad="B5"/>
<connect gate="G$1" pin="VDD@2" pad="E2"/>
<connect gate="G$1" pin="VDD@3" pad="E9"/>
<connect gate="G$1" pin="VDD@4" pad="J5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AUP1T57" prefix="U">
<description>&lt;H2&gt;Low-power configurable gate with voltage-level translator&lt;/H2&gt;The 74AUP1T57 provides low-power, low-voltage configurable logic gate functions. The 
output state is determined by eight patterns of 3-bit input. The user can choose the logic 
functions AND, OR, NAND, NOR, XNOR, inverter and buffer. All inputs can be connected 
to VCC or GND.
This device ensures a very low static and dynamic power consumption across the entire 
VCC range from 2.3 V to 3.6 V.
The 74AUP1T57 is designed for logic-level translation applications with input switching 
levels that accept 1.8 V low-voltage CMOS signals, while operating from either a single 
2.5 V or 3.3 V supply voltage.
The wide supply voltage range ensures normal operation as battery voltage drops from 
3.6 V to 2.3 V.
This device is fully specified for partial power-down applications using IOFF. The IOFF
circuitry disables the output, preventing the damaging backflow current through the device 
when it is powered down.
Schmitt trigger inputs make the circuit tolerant to slower input rise and fall times across 
the entire VCC range.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="74AUP1T57"/>
</gates>
<devices>
<device name="GW" package="SOT363">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 804 64125"/>
</technology>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 804 65115"/>
</technology>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 813 64132"/>
</technology>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 928 78132"/>
</technology>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="I2C" value="9352 917 54132"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AUP1G58" prefix="U">
<description>&lt;H2&gt;Low-power configurable multiple function gate&lt;/H2&gt;The 74AUP1G58 provides configurable multiple functions. The output state is determined 
by eight patterns of 3-bit input. The user can choose the logic functions AND, OR, NAND, 
NOR, XOR, inverter and buffer. All inputs can be connected to VCC or GND.
This device ensures a very low static and dynamic power consumption across the entire 
VCC range from 0.8 V to 3.6 V.
This device is fully specified for partial power-down applications using IOFF. 
The IOFF circuitry disables the output, preventing the damaging backflow current through 
the device when it is powered down.
The 74AUP1G58 has Schmitt trigger inputs making it capable of transforming slowly 
changing input signals into sharply defined, jitter-free output signals.
The inputs switch at different points for positive and negative-going signals. The difference 
between the positive voltage VT+ and the negative voltage VT- is defined as the input 
hysteresis voltage VH.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="74AUP1T57"/>
</gates>
<devices>
<device name="GW" package="SOT363">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 799 59125"/>
</technology>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 799 61132"/>
</technology>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 813 29132"/>
</technology>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 928 68132"/>
</technology>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="I2C" value="9352 917 44132"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CBTL06DP212" prefix="U">
<description>High-performance DisplayPort Gen2 2 : 1 multiplexer&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/bbimages/NXP_logo.gif"&gt;</description>
<gates>
<gate name="G$1" symbol="CBTL06DP212"/>
</gates>
<devices>
<device name="" package="SOT918-1">
<connects>
<connect gate="G$1" pin="AUX+" pad="H2"/>
<connect gate="G$1" pin="AUX-" pad="H1"/>
<connect gate="G$1" pin="AUX1+" pad="H9"/>
<connect gate="G$1" pin="AUX1-" pad="J9"/>
<connect gate="G$1" pin="AUX2+" pad="H6"/>
<connect gate="G$1" pin="AUX2-" pad="J6"/>
<connect gate="G$1" pin="DDC_AUX_SEL" pad="C2"/>
<connect gate="G$1" pin="DDC_CLK1" pad="H8"/>
<connect gate="G$1" pin="DDC_CLK2" pad="H5"/>
<connect gate="G$1" pin="DDC_DAT1" pad="J8"/>
<connect gate="G$1" pin="DDC_DAT2" pad="J5"/>
<connect gate="G$1" pin="GND@1" pad="B3"/>
<connect gate="G$1" pin="GND@2" pad="C8"/>
<connect gate="G$1" pin="GND@3" pad="G2"/>
<connect gate="G$1" pin="GND@4" pad="G8"/>
<connect gate="G$1" pin="GND@5" pad="H4"/>
<connect gate="G$1" pin="GND@6" pad="H7"/>
<connect gate="G$1" pin="GPU_SEL" pad="A1"/>
<connect gate="G$1" pin="HPDIN" pad="J1"/>
<connect gate="G$1" pin="HPD_1" pad="J2"/>
<connect gate="G$1" pin="HPD_2" pad="H3"/>
<connect gate="G$1" pin="IN1_0+" pad="B4"/>
<connect gate="G$1" pin="IN1_0-" pad="A4"/>
<connect gate="G$1" pin="IN1_1+" pad="B5"/>
<connect gate="G$1" pin="IN1_1-" pad="A5"/>
<connect gate="G$1" pin="IN1_2+" pad="B6"/>
<connect gate="G$1" pin="IN1_2-" pad="A6"/>
<connect gate="G$1" pin="IN1_3+" pad="A8"/>
<connect gate="G$1" pin="IN1_3-" pad="A9"/>
<connect gate="G$1" pin="IN2_0+" pad="B8"/>
<connect gate="G$1" pin="IN2_0-" pad="B9"/>
<connect gate="G$1" pin="IN2_1+" pad="D8"/>
<connect gate="G$1" pin="IN2_1-" pad="D9"/>
<connect gate="G$1" pin="IN2_2+" pad="E8"/>
<connect gate="G$1" pin="IN2_2-" pad="E9"/>
<connect gate="G$1" pin="IN2_3+" pad="F8"/>
<connect gate="G$1" pin="IN2_3-" pad="F9"/>
<connect gate="G$1" pin="OUT_0+" pad="B2"/>
<connect gate="G$1" pin="OUT_0-" pad="B1"/>
<connect gate="G$1" pin="OUT_1+" pad="D2"/>
<connect gate="G$1" pin="OUT_1-" pad="D1"/>
<connect gate="G$1" pin="OUT_2+" pad="E2"/>
<connect gate="G$1" pin="OUT_2-" pad="E1"/>
<connect gate="G$1" pin="OUT_3+" pad="F2"/>
<connect gate="G$1" pin="OUT_3-" pad="F1"/>
<connect gate="G$1" pin="TST0" pad="B7"/>
<connect gate="G$1" pin="VDD@1" pad="A2"/>
<connect gate="G$1" pin="VDD@2" pad="J4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1713" prefix="U">
<description>Resonant power supply control IC with PFC.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/bbimages/NXP_logo.gif&gt;</description>
<gates>
<gate name="G$1" symbol="TEA1713"/>
</gates>
<devices>
<device name="T" package="SOT137-1">
<connects>
<connect gate="G$1" pin="CFMIN" pad="19"/>
<connect gate="G$1" pin="COMPPFC" pad="1"/>
<connect gate="G$1" pin="GATEHS" pad="13"/>
<connect gate="G$1" pin="GATELS" pad="10"/>
<connect gate="G$1" pin="GATEPFC" pad="7"/>
<connect gate="G$1" pin="HB" pad="15"/>
<connect gate="G$1" pin="NC@1" pad="11"/>
<connect gate="G$1" pin="NC@2" pad="16"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="RCPROT" pad="23"/>
<connect gate="G$1" pin="RFMAX" pad="20"/>
<connect gate="G$1" pin="SGND" pad="18"/>
<connect gate="G$1" pin="SNSAUXPFC" pad="3"/>
<connect gate="G$1" pin="SNSBOOST" pad="24"/>
<connect gate="G$1" pin="SNSCURHBC" pad="17"/>
<connect gate="G$1" pin="SNSCURPFC" pad="4"/>
<connect gate="G$1" pin="SNSFB" pad="21"/>
<connect gate="G$1" pin="SNSMAINS" pad="2"/>
<connect gate="G$1" pin="SNSOUT" pad="5"/>
<connect gate="G$1" pin="SSHBC/EN" pad="22"/>
<connect gate="G$1" pin="SUPHS" pad="14"/>
<connect gate="G$1" pin="SUPHV" pad="12"/>
<connect gate="G$1" pin="SUPIC" pad="6"/>
<connect gate="G$1" pin="SUPREG" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 895 98518"/>
<attribute name="FARNELL" value="1872212"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NX3L2467" prefix="U">
<description>The NX3L2467 is a dual low-ohmic double-pole double-throw analog switch suitable for use as an analog or digital multiplexer/demultiplexer. It consists of four switches, each with two independent input/outputs (nY0 and nY1) and a common input/output (nZ). 
The two digital inputs (1S and 2S) are used to select the switch position. 1S is used in selecting the independent inputs/outputs switched to 1Z and 2Z, and 2S is used in selecting the independent inputs/outputs switched to 3Z and 4Z.
 Schmitt trigger action at the select input (nS) makes the circuit tolerant to slower input rise and fall times across the entire VCC range from 1.4 V to 4.3 V.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NX3L2467"/>
</gates>
<devices>
<device name="PW" package="SOT403-1">
<connects>
<connect gate="G$1" pin="1S" pad="4"/>
<connect gate="G$1" pin="1Y0" pad="3"/>
<connect gate="G$1" pin="1Y1" pad="1"/>
<connect gate="G$1" pin="1Z" pad="2"/>
<connect gate="G$1" pin="2S" pad="12"/>
<connect gate="G$1" pin="2Y0" pad="7"/>
<connect gate="G$1" pin="2Y1" pad="5"/>
<connect gate="G$1" pin="2Z" pad="6"/>
<connect gate="G$1" pin="3Y0" pad="11"/>
<connect gate="G$1" pin="3Y1" pad="9"/>
<connect gate="G$1" pin="3Z" pad="10"/>
<connect gate="G$1" pin="4Y0" pad="15"/>
<connect gate="G$1" pin="4Y1" pad="13"/>
<connect gate="G$1" pin="4Z" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HR" package="SOT1039-1">
<connects>
<connect gate="G$1" pin="1S" pad="2"/>
<connect gate="G$1" pin="1Y0" pad="1"/>
<connect gate="G$1" pin="1Y1" pad="15"/>
<connect gate="G$1" pin="1Z" pad="16"/>
<connect gate="G$1" pin="2S" pad="10"/>
<connect gate="G$1" pin="2Y0" pad="5"/>
<connect gate="G$1" pin="2Y1" pad="3"/>
<connect gate="G$1" pin="2Z" pad="4"/>
<connect gate="G$1" pin="3Y0" pad="9"/>
<connect gate="G$1" pin="3Y1" pad="7"/>
<connect gate="G$1" pin="3Z" pad="8"/>
<connect gate="G$1" pin="4Y0" pad="13"/>
<connect gate="G$1" pin="4Y1" pad="11"/>
<connect gate="G$1" pin="4Z" pad="12"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GU" package="SOT1161-1">
<connects>
<connect gate="G$1" pin="1S" pad="2"/>
<connect gate="G$1" pin="1Y0" pad="1"/>
<connect gate="G$1" pin="1Y1" pad="15"/>
<connect gate="G$1" pin="1Z" pad="16"/>
<connect gate="G$1" pin="2S" pad="10"/>
<connect gate="G$1" pin="2Y0" pad="5"/>
<connect gate="G$1" pin="2Y1" pad="3"/>
<connect gate="G$1" pin="2Z" pad="4"/>
<connect gate="G$1" pin="3Y0" pad="9"/>
<connect gate="G$1" pin="3Y1" pad="7"/>
<connect gate="G$1" pin="3Z" pad="8"/>
<connect gate="G$1" pin="4Y0" pad="13"/>
<connect gate="G$1" pin="4Y1" pad="11"/>
<connect gate="G$1" pin="4Z" pad="12"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CBTL02043A" prefix="U">
<description>CBTL02043A/B is a 2 differential channel, 2-to-1 multiplexer/demultiplexer switch for 
PCI Express Generation 3 (Gen3), or other high-speed serial interface applications. The 
CBTL02043A/B can switch two differential signals to one of two locations. Using a unique 
design technique, NXP has minimized the impedance of the switch such that the 
attenuation observed through the switch is negligible, and also minimized the 
channel-to-channel skew as well as channel-to-channel crosstalk, as required by the 
high-speed serial interface. CBTL02043A/B allows expansion of existing high speed ports 
for extremely low power.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/bbimages/NXP_logo.gif"&gt;</description>
<gates>
<gate name="G$1" symbol="CBTL02043"/>
</gates>
<devices>
<device name="BQ" package="SOT764">
<connects>
<connect gate="G$1" pin="A0_N" pad="4"/>
<connect gate="G$1" pin="A0_P" pad="3"/>
<connect gate="G$1" pin="A1_N" pad="8"/>
<connect gate="G$1" pin="A1_P" pad="7"/>
<connect gate="G$1" pin="B0_N" pad="19"/>
<connect gate="G$1" pin="B0_P" pad="18"/>
<connect gate="G$1" pin="B1_N" pad="16"/>
<connect gate="G$1" pin="B1_P" pad="17"/>
<connect gate="G$1" pin="C0_N" pad="14"/>
<connect gate="G$1" pin="C0_P" pad="15"/>
<connect gate="G$1" pin="C1_N" pad="12"/>
<connect gate="G$1" pin="C1_P" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="20"/>
<connect gate="G$1" pin="GND@3" pad="11"/>
<connect gate="G$1" pin="GND@4" pad="CP"/>
<connect gate="G$1" pin="SEL" pad="9"/>
<connect gate="G$1" pin="VDD@1" pad="1"/>
<connect gate="G$1" pin="VDD@2" pad="6"/>
<connect gate="G$1" pin="VDD@3" pad="10"/>
<connect gate="G$1" pin="XSD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CBTL02043B" prefix="U">
<description>&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/bbimages/NXP_logo.gif"&gt;</description>
<gates>
<gate name="G$1" symbol="CBTL02043"/>
</gates>
<devices>
<device name="BQ" package="SOT764">
<connects>
<connect gate="G$1" pin="A0_N" pad="3"/>
<connect gate="G$1" pin="A0_P" pad="2"/>
<connect gate="G$1" pin="A1_N" pad="7"/>
<connect gate="G$1" pin="A1_P" pad="6"/>
<connect gate="G$1" pin="B0_N" pad="17"/>
<connect gate="G$1" pin="B0_P" pad="18"/>
<connect gate="G$1" pin="B1_N" pad="13"/>
<connect gate="G$1" pin="B1_P" pad="14"/>
<connect gate="G$1" pin="C0_N" pad="5"/>
<connect gate="G$1" pin="C0_P" pad="4"/>
<connect gate="G$1" pin="C1_N" pad="9"/>
<connect gate="G$1" pin="C1_P" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="10"/>
<connect gate="G$1" pin="GND@3" pad="15"/>
<connect gate="G$1" pin="GND@4" pad="CP"/>
<connect gate="G$1" pin="SEL" pad="12"/>
<connect gate="G$1" pin="VDD@1" pad="11"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="20"/>
<connect gate="G$1" pin="XSD" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1753" prefix="U">
<description>The GreenChip III is the third generation of green Switched Mode Power Supply (SMPS) controller ICs. The GreenChip III combines a controller for Power Factor Correction (PFC) and a flyback controller. Its high level of integration allows the design of a cost-effective power supply with a very low number of external components.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/bbimages/NXP_logo.gif&gt;</description>
<gates>
<gate name="G$1" symbol="TEA1753"/>
</gates>
<devices>
<device name="T" package="SOT109-1">
<connects>
<connect gate="G$1" pin="FBAUX" pad="4"/>
<connect gate="G$1" pin="FBCTRL" pad="3"/>
<connect gate="G$1" pin="FBDRIVER" pad="13"/>
<connect gate="G$1" pin="FBSENSE" pad="10"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="HV" pad="16"/>
<connect gate="G$1" pin="HVS" pad="15"/>
<connect gate="G$1" pin="LATCH" pad="5"/>
<connect gate="G$1" pin="PFCAUX" pad="8"/>
<connect gate="G$1" pin="PFCCOMP" pad="6"/>
<connect gate="G$1" pin="PFCDRIVER" pad="12"/>
<connect gate="G$1" pin="PFCSENSE" pad="11"/>
<connect gate="G$1" pin="PFCTIMER" pad="14"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VINSENSE" pad="7"/>
<connect gate="G$1" pin="VOSENSE" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 932 05518"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1791" prefix="U">
<description>The TEA1791AT is a member of the new generation of Synchronous Rectifier (SR) controller ICs for switched mode power supplies. Its high level of integration allows the design of a cost-effective power supply with a very low number of external components.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/bbimages/NXP_logo.gif&gt;</description>
<gates>
<gate name="G$1" symbol="TEA1791"/>
</gates>
<devices>
<device name="AT" package="SOT96-1">
<connects>
<connect gate="G$1" pin="DRIVER" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="5"/>
<connect gate="G$1" pin="NC@3" pad="6"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
<connect gate="G$1" pin="SRSENSE" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 901 57118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1738(L)T" prefix="U">
<description>The TEA1738(T) is a low cost Switched Mode Power Supply (SMPS) controller IC intended for flyback topologies. The TEA1738(T) operates in peak current and frequency control mode. To reduce Electro Magnetic Interference (EMI), frequency jitter has been implemented. Slope compensation is integrated for Continuous Conduction Mode (CCM) operation.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/bbimages/NXP_logo.gif&gt;</description>
<gates>
<gate name="G$1" symbol="TEA1738T"/>
</gates>
<devices>
<device name="" package="SOT96-1">
<connects>
<connect gate="G$1" pin="CTRL" pad="7"/>
<connect gate="G$1" pin="DRIVER" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="ISENSE" pad="4"/>
<connect gate="G$1" pin="OPTIMER" pad="8"/>
<connect gate="G$1" pin="PROTECT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VINSENSE" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 918 76118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BGA2850" prefix="U">
<description>Silicon Monolithic Microwave Integrated Circuit (MMIC) wideband amplifier with internal matching circuit in a 6-pin SOT363 plastic SMD package.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MV+ MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/bbimages/NXP_logo.gif"&gt;</description>
<gates>
<gate name="G$1" symbol="AMP"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G$1" pin="-IN" pad="6"/>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2@1" pad="2"/>
<connect gate="G$1" pin="GND2@2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 900 54115"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8523" prefix="U">
<description>The PCF8523 is a CMOS Real-Time Clock (RTC) and calendar optimized for low power 
consumption. Data is transferred serially via an I2C-bus with a maximum data rate of 
1000 kbit/s. Alarm and timer functions are available with the possibility to generate a 
wake-up signal on an interrupt pin. An offset register allows fine-tuning of the clock. The 
PCF8523 has a backup battery switch-over circuit, which detects power failures and 
automatically switches to the battery supply when a power failure occurs.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8523"/>
</gates>
<devices>
<device name="T" package="SOT96-1">
<connects>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TK" package="SOT909">
<connects>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8523TS">
<description>The PCF8523 is a CMOS Real-Time Clock (RTC) and calendar optimized for low power 
consumption. Data is transferred serially via an I2C-bus with a maximum data rate of 
1000 kbit/s. Alarm and timer functions are available with the possibility to generate a 
wake-up signal on an interrupt pin. An offset register allows fine-tuning of the clock. The 
PCF8523 has a backup battery switch-over circuit, which detects power failures and 
automatically switches to the battery supply when a power failure occurs.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8523TS"/>
</gates>
<devices>
<device name="" package="SOT402-1">
<connects>
<connect gate="G$1" pin="CLKOUT" pad="8"/>
<connect gate="G$1" pin="INT1" pad="13"/>
<connect gate="G$1" pin="INT2" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="11"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="VBAT" pad="4"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACT102H-600D" prefix="T">
<description>&lt;H2&gt;AC Thyristor power switch&lt;/H2&gt;An AC Thyristor power switch with very high noise immunity and over-voltage protection 
configured for negative gate triggering in a SOT96-1 (SO8) small surface-mountable 
plastic package&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TRIAC_TOP"/>
</gates>
<devices>
<device name="" package="SOT96-1">
<connects>
<connect gate="G$1" pin="CM" pad="6 7"/>
<connect gate="G$1" pin="G" pad="5"/>
<connect gate="G$1" pin="LD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9340 645 54118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="Z0109MN0" prefix="T">
<description>&lt;H2&gt;4Q Triac&lt;/H2&gt;
Planar passivated sensitive gate four quadrant triac in a SOT223 (SC-73) 
surface-mountable plastic package intended for applications requiring enhanced immunity 
to noise and direct interfacing to logic level ICs and low power gate drivers.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="CM" pad="2 4"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="LD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9340 650 56135"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD6805" prefix="U">
<description>&lt;H2&gt;Low-dropout regulators, high PSRR, 150 mA&lt;/H2&gt;
The LD6805 series is a small-size Low DropOut regulator (LDO) family with ultra high 
Power Supply Rejection Ratio (PSRR) of 75 dB. The voltage drop is 250 mV at 150 mA 
current rating.
Operating voltages can range from 2.3 V to 5.5 V. The devices are available with fixed 
output voltages between 1.2 V to 3.6 V. 
The LD6805K/xxH devices show a high-ohmic state at the output pin when set to disabled 
mode. The LD6805K/xxP devices contain a pull-down switching transistor to provide a 
low-ohmic output state (auto discharge function) in disabled mode.
The LD6805 series devices are available in a 1 x 1 mm DFN plastic package making them 
ideal for use in portable applications requiring component miniaturization. All devices are 
manufactured in monolithic silicon technology.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LD680X"/>
</gates>
<devices>
<device name="K" package="SOT1194">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTN36241B" prefix="U">
<description>PLEASE CHECK AOUT+ AND AOUT-&lt;p&gt;

PTN36241B is a USB 3.0 (SuperSpeed) re-driver that enhances signal quality by 
performing receive equalization on the deteriorated input signal followed by transmit 
de-emphasis maximizing system link performance. With its superior differential signal 
conditioning and enhancement capability, the device delivers significant flexibility and 
performance scaling for various systems with different PCB trace and cable channel 
conditions and still benefit from optimum power consumption. PTN36241B is a 
dual-channel (channel A and channel B) device that supports data signaling rate of 
5 Gbit/s through each channel. 
PTN36241B is flexibly powered from 3.3 V and is available in HVQFN24 4 mm × 4 mm 
package with 0.5 mm pitch.
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PTN36241B"/>
</gates>
<devices>
<device name="" package="SOT616">
<connects>
<connect gate="G$1" pin="ADE/ADD" pad="3"/>
<connect gate="G$1" pin="AEQ" pad="2"/>
<connect gate="G$1" pin="AIN+" pad="9"/>
<connect gate="G$1" pin="AIN-" pad="8"/>
<connect gate="G$1" pin="AOS" pad="4"/>
<connect gate="G$1" pin="AOUT+" pad="22"/>
<connect gate="G$1" pin="AOUT-" pad="23"/>
<connect gate="G$1" pin="BDE/SCL" pad="16"/>
<connect gate="G$1" pin="BEQ/SDA" pad="17"/>
<connect gate="G$1" pin="BIN+" pad="19"/>
<connect gate="G$1" pin="BIN-" pad="20"/>
<connect gate="G$1" pin="BOS" pad="15"/>
<connect gate="G$1" pin="BOUT+" pad="12"/>
<connect gate="G$1" pin="BOUT-" pad="11"/>
<connect gate="G$1" pin="CEN" pad="5"/>
<connect gate="G$1" pin="COM" pad="14"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="10"/>
<connect gate="G$1" pin="GND@3" pad="18"/>
<connect gate="G$1" pin="GND@4" pad="21"/>
<connect gate="G$1" pin="GND@5" pad="25"/>
<connect gate="G$1" pin="SQTH" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="1"/>
<connect gate="G$1" pin="VDD@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD6806" prefix="U">
<description>&lt;H2&gt;Ultra low-dropout regulator, low noise, 200 mA&lt;/H2&gt;
The LD6806 series is a small-size Low-DropOut regulator (LDO) family with a typical 
voltage drop of 60 mV at 200 mA current rating.
The device is available in three different surface-mounted packages, one 0.4 mm pitch 
CSP, one leadless plastic package SOT886 and one gull wing package SOT753.
The operating voltage ranges from 2.3 V to 5.5 V and the output voltage ranges from 
1.2 V to 3.6 V.
LD6806x/xxH devices show a high-ohmic state at the output pin, while the LD6806x/xxP 
contains a pull-down switching transistor, to provide a low-ohmic output stage when the 
device is disabled. All devices use the same regulator design and are manufactured in 
monolithic silicon technology.
These features make the LD6806 series ideal for use in applications requiring component 
miniaturization, such as mobile phone handsets, cordless telephones and personal digital 
devices.&lt;p&gt;&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LD680X"/>
</gates>
<devices>
<device name="F" package="SOT886">
<connects>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CX4" package="NX3P190/NX3P191">
<connects>
<connect gate="G$1" pin="EN" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="IN" pad="B2"/>
<connect gate="G$1" pin="OUT" pad="B1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TD" package="SOT753">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUK625R0-40C">
<description>&lt;H2&gt;N-channel TrenchMOS intermediate level FET&lt;/H2&gt;Intermediate level gate drive N-channel enhancement mode Field-Effect Transistor (FET) 
in a plastic package using advanced TrenchMOS technology. This product has been 
designed and qualified to the appropriate AEC Q101 standard for use in high performance 
automotive applications.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT428">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC12D27" prefix="U">
<description>&lt;b&gt;LPC12D27&lt;/b&gt;&lt;p&gt;
32-bit ARM Cortex-M0 microcontroller; 128  kB flash and 8 kB SRAM; 40  segment x 4 LCD driver&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/img/NXP_logo.png&gt;</description>
<gates>
<gate name="G$1" symbol="LPC12D27"/>
</gates>
<devices>
<device name="FBD100" package="SOT407-1">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_13" pad="20"/>
<connect gate="G$1" pin="BP0" pad="42"/>
<connect gate="G$1" pin="BP1" pad="44"/>
<connect gate="G$1" pin="BP2" pad="43"/>
<connect gate="G$1" pin="BP3" pad="45"/>
<connect gate="G$1" pin="CLK" pad="38"/>
<connect gate="G$1" pin="LCD_SCL" pad="36"/>
<connect gate="G$1" pin="LCD_SDA" pad="35"/>
<connect gate="G$1" pin="PIO0_0/!RTS0!" pad="6"/>
<connect gate="G$1" pin="PIO0_1/RXD0/CT32B0_CAP0/CT32B0_MAT0" pad="7"/>
<connect gate="G$1" pin="PIO0_10/SCL" pad="17"/>
<connect gate="G$1" pin="PIO0_11/SDA/CT16B0_CAP0/CT16B0_MAT0" pad="18"/>
<connect gate="G$1" pin="PIO0_12/CLKOUT/CT16B0_CAP1/CT16B0_MAT1" pad="19"/>
<connect gate="G$1" pin="PIO0_14/SCK" pad="21"/>
<connect gate="G$1" pin="PIO0_15/SSEL/CT16B1_CAP0/CT16B1_MAT0" pad="22"/>
<connect gate="G$1" pin="PIO0_16/MISO/CT16B1_CAP1/CT16B1_MAT1" pad="23"/>
<connect gate="G$1" pin="PIO0_17/MOSI" pad="24"/>
<connect gate="G$1" pin="PIO0_18/SWCLK/CT32B0_CAP0/CT32B0_MAT0" pad="25"/>
<connect gate="G$1" pin="PIO0_19/ACMP0_I0/CT32B0_CAP1/CT32B0_MAT1" pad="95"/>
<connect gate="G$1" pin="PIO0_2/TXD0/CT32B0_CAP1/CT32B0_MAT1" pad="8"/>
<connect gate="G$1" pin="PIO0_20/ACMP0_I1/CT32B0_CAP2/CT32B0_MAT2" pad="96"/>
<connect gate="G$1" pin="PIO0_21/ACMP0_I2/CT32B0_CAP3/CT32B0_MAT3" pad="97"/>
<connect gate="G$1" pin="PIO0_22/ACMP0_I3" pad="98"/>
<connect gate="G$1" pin="PIO0_23/ACMP1_I0/CT32B1_CAP0/CT32B1_MAT0" pad="99"/>
<connect gate="G$1" pin="PIO0_24/ACMP1_I1/CT32B1_CAP1/CT32B1_MAT1" pad="100"/>
<connect gate="G$1" pin="PIO0_27/ACMP0_O" pad="3"/>
<connect gate="G$1" pin="PIO0_28/ACMP1_O/CT16B0_CAP0/CT16B0_MAT0" pad="4"/>
<connect gate="G$1" pin="PIO0_29/ROSC/CT16B0_CAP1/CT16B0_MAT1" pad="5"/>
<connect gate="G$1" pin="PIO0_3/!DTR0!/CT32B0_CAP2/CT32B0_MAT2" pad="9"/>
<connect gate="G$1" pin="PIO0_4/CT32B0_CAP3/CT32B0_MAT3" pad="10"/>
<connect gate="G$1" pin="PIO0_5/!DCD0!" pad="11"/>
<connect gate="G$1" pin="PIO0_6/!RI0!/CT32B1_CAP0/CT32B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO0_7/!CTS0!/CT32B1_CAP1/CT32B1_MAT1" pad="13"/>
<connect gate="G$1" pin="PIO0_8/RXD1/CT32B1_CAP2/CT32B1_MAT2" pad="14"/>
<connect gate="G$1" pin="PIO0_9/TXD1/CT32B1_CAP3/CT32B1_MAT3" pad="15"/>
<connect gate="G$1" pin="PIO1_2/SWDIO/AD4" pad="81"/>
<connect gate="G$1" pin="PIO1_3/AD5/WAKEUP" pad="82"/>
<connect gate="G$1" pin="PIO1_4/AD6" pad="83"/>
<connect gate="G$1" pin="PIO1_5/AD7/CT16B1_CAP0/CT16B1_MAT0" pad="84"/>
<connect gate="G$1" pin="PIO1_6/CT16B1_CAP1/CT16B1_MAT1" pad="85"/>
<connect gate="G$1" pin="PIO2_0/CT16B0_CAP0/CT16B0_MAT0" pad="16"/>
<connect gate="G$1" pin="R/PIO0_30/AD0" pad="26"/>
<connect gate="G$1" pin="R/PIO0_31/AD1" pad="27"/>
<connect gate="G$1" pin="R/PIO1_0/AD2" pad="28"/>
<connect gate="G$1" pin="R/PIO1_1/AD3" pad="80"/>
<connect gate="G$1" pin="RTCXI" pad="89"/>
<connect gate="G$1" pin="RTCXOUT" pad="88"/>
<connect gate="G$1" pin="S0" pad="46"/>
<connect gate="G$1" pin="S1" pad="47"/>
<connect gate="G$1" pin="S10" pad="56"/>
<connect gate="G$1" pin="S11" pad="57"/>
<connect gate="G$1" pin="S12" pad="58"/>
<connect gate="G$1" pin="S13" pad="59"/>
<connect gate="G$1" pin="S14" pad="60"/>
<connect gate="G$1" pin="S15" pad="61"/>
<connect gate="G$1" pin="S16" pad="62"/>
<connect gate="G$1" pin="S17" pad="63"/>
<connect gate="G$1" pin="S18" pad="64"/>
<connect gate="G$1" pin="S19" pad="65"/>
<connect gate="G$1" pin="S2" pad="48"/>
<connect gate="G$1" pin="S20" pad="66"/>
<connect gate="G$1" pin="S21" pad="67"/>
<connect gate="G$1" pin="S22" pad="68"/>
<connect gate="G$1" pin="S23" pad="69"/>
<connect gate="G$1" pin="S24" pad="70"/>
<connect gate="G$1" pin="S25" pad="71"/>
<connect gate="G$1" pin="S26" pad="72"/>
<connect gate="G$1" pin="S27" pad="73"/>
<connect gate="G$1" pin="S28" pad="74"/>
<connect gate="G$1" pin="S29" pad="75"/>
<connect gate="G$1" pin="S3" pad="49"/>
<connect gate="G$1" pin="S30" pad="76"/>
<connect gate="G$1" pin="S31" pad="77"/>
<connect gate="G$1" pin="S32" pad="78"/>
<connect gate="G$1" pin="S33" pad="79"/>
<connect gate="G$1" pin="S34" pad="29"/>
<connect gate="G$1" pin="S35" pad="30"/>
<connect gate="G$1" pin="S36" pad="31"/>
<connect gate="G$1" pin="S37" pad="32"/>
<connect gate="G$1" pin="S38" pad="33"/>
<connect gate="G$1" pin="S39" pad="34"/>
<connect gate="G$1" pin="S4" pad="50"/>
<connect gate="G$1" pin="S5" pad="51"/>
<connect gate="G$1" pin="S6" pad="52"/>
<connect gate="G$1" pin="S7" pad="53"/>
<connect gate="G$1" pin="S8" pad="54"/>
<connect gate="G$1" pin="S9" pad="55"/>
<connect gate="G$1" pin="SWCLK/ACMP1_I3/CT32B1_CAP3/CT32B1_MAT3/PIO0_26" pad="2"/>
<connect gate="G$1" pin="SWDIO/ACMP1_I2/CT32B1_CAP2/CT32B1_MAT2/PIO0_25" pad="1"/>
<connect gate="G$1" pin="SYNC" pad="37"/>
<connect gate="G$1" pin="VDD" pad="39"/>
<connect gate="G$1" pin="VDD(3V3)" pad="87"/>
<connect gate="G$1" pin="VDD(IO)" pad="90"/>
<connect gate="G$1" pin="VLCD" pad="41"/>
<connect gate="G$1" pin="VREF_CMP" pad="94"/>
<connect gate="G$1" pin="VSS" pad="86"/>
<connect gate="G$1" pin="VSS(IO)" pad="91"/>
<connect gate="G$1" pin="VSS(LCD)" pad="40"/>
<connect gate="G$1" pin="XTALIN" pad="92"/>
<connect gate="G$1" pin="XTALOUT" pad="93"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9661" prefix="U">
<description>The PCA9661 is an advanced single master mode I2C-bus controller. It is a fourth 
generation bus controller designed for data intensive I2C-bus data transfers. 
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/img/NXP_logo.png&gt;</description>
<gates>
<gate name="G$1" symbol="PCA9661"/>
</gates>
<devices>
<device name="B" package="SOT313-2">
<connects>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="9"/>
<connect gate="G$1" pin="A5" pad="10"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="12"/>
<connect gate="G$1" pin="CE" pad="33"/>
<connect gate="G$1" pin="D0" pad="37"/>
<connect gate="G$1" pin="D1" pad="38"/>
<connect gate="G$1" pin="D2" pad="41"/>
<connect gate="G$1" pin="D3" pad="42"/>
<connect gate="G$1" pin="D4" pad="45"/>
<connect gate="G$1" pin="D5" pad="46"/>
<connect gate="G$1" pin="D6" pad="1"/>
<connect gate="G$1" pin="D7" pad="2"/>
<connect gate="G$1" pin="INT" pad="20"/>
<connect gate="G$1" pin="RD" pad="32"/>
<connect gate="G$1" pin="RESET" pad="36"/>
<connect gate="G$1" pin="SCL0" pad="28"/>
<connect gate="G$1" pin="SDA0" pad="27"/>
<connect gate="G$1" pin="TCK" pad="15"/>
<connect gate="G$1" pin="TDI" pad="16"/>
<connect gate="G$1" pin="TDO" pad="17"/>
<connect gate="G$1" pin="TMS" pad="14"/>
<connect gate="G$1" pin="TRIG" pad="34"/>
<connect gate="G$1" pin="TRST" pad="13"/>
<connect gate="G$1" pin="VDD(I/O)" pad="24"/>
<connect gate="G$1" pin="VDD(PLL)" pad="18"/>
<connect gate="G$1" pin="VDD@1" pad="7"/>
<connect gate="G$1" pin="VDD@2" pad="30"/>
<connect gate="G$1" pin="VDD@3" pad="40"/>
<connect gate="G$1" pin="VDD@4" pad="44"/>
<connect gate="G$1" pin="VDD@5" pad="48"/>
<connect gate="G$1" pin="VSS" pad="8 29 35 39 43 47"/>
<connect gate="G$1" pin="VSS(I/O)" pad="23"/>
<connect gate="G$1" pin="VSS(PLL)" pad="19"/>
<connect gate="G$1" pin="WR" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U14" prefix="U">
<description>&lt;h3&gt;NXP Semiconductors&lt;/h3&gt;
&lt;p&gt;&lt;h4&gt;Attention: Pin PIO1_5 is not available in the LQFP48 package, whereas PIO1_31 is not available in the TFBGA48 package!&lt;/h4&gt;&lt;p&gt; 

&lt;a href="http://ics.nxp.com/products/lpc1000/lpc11xx/"&gt;&lt;b&gt;LPC11Uxx&lt;/b&gt; microcontrollers&lt;/a&gt;
&lt;ul&gt;
&lt;li&gt;ARM 32-bit Cortex-M0 Microcontroller with MPU&lt;/li&gt;
&lt;li&gt;CPU clock up to 50MHz&lt;/li&gt;
&lt;li&gt;Up to 32KByte on-chip Flash ROM with In-System Programming (ISP) and In-Application Programming (IAP) via On-Chip Bootloader&lt;/li&gt;
&lt;li&gt;Up to 8KByte SRAM&lt;/li&gt;
&lt;li&gt;Nested Vectored Interrupt Controller&lt;/li&gt;
&lt;li&gt;Up to 2 SPI controllers&lt;/li&gt;
&lt;li&gt;USB 2.0 device controller&lt;/li&gt;
&lt;li&gt;USART with full Modem Interface and RS485 Support and ISO7816-3 support&lt;/li&gt;
&lt;li&gt;Fast Mode I2C-Bus&lt;/li&gt;
&lt;li&gt;4 Timers with 4 capture channels and 13 output channels&lt;/li&gt;
&lt;li&gt;Watchdog (WDT)&lt;/li&gt;
&lt;li&gt;Sytem tick timer&lt;/li&gt;
&lt;li&gt;10-bit ADC with 8 channels&lt;/li&gt;
&lt;li&gt;Power Management Unit (PMU)&lt;/li&gt;
&lt;li&gt;Brownout detection&lt;/li&gt;
&lt;li&gt;12MHz internal RC oscillator&lt;/li&gt;
&lt;li&gt;Serial Wire Debug/Trace port&lt;/li&gt;
&lt;/ul&gt;

Symbol copied from RH, package adapted to NXP spec (MK)</description>
<gates>
<gate name="LPC" symbol="LPC11U14-48"/>
</gates>
<devices>
<device name="FBD" package="SOT313-2">
<connects>
<connect gate="LPC" pin="!RESET!/PIO0_0" pad="3"/>
<connect gate="LPC" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="LPC" pin="(PIO1_5/CT32B1_CAP1)PIO1_31" pad="25"/>
<connect gate="LPC" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="LPC" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="LPC" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="45"/>
<connect gate="LPC" pin="PIO0_18/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="LPC" pin="PIO0_19/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="LPC" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="LPC" pin="PIO0_20/CT16B1_CAP0" pad="9"/>
<connect gate="LPC" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="17"/>
<connect gate="LPC" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="30"/>
<connect gate="LPC" pin="PIO0_23/AD7" pad="42"/>
<connect gate="LPC" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="LPC" pin="PIO0_4/SCL" pad="15"/>
<connect gate="LPC" pin="PIO0_5/SDA" pad="16"/>
<connect gate="LPC" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="22"/>
<connect gate="LPC" pin="PIO0_7/!CTS!" pad="23"/>
<connect gate="LPC" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="LPC" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="LPC" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="36"/>
<connect gate="LPC" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="37"/>
<connect gate="LPC" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="43"/>
<connect gate="LPC" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="48"/>
<connect gate="LPC" pin="PIO1_19/!DTR!/SSEL1" pad="2"/>
<connect gate="LPC" pin="PIO1_20/!DSR!/SCK1" pad="13"/>
<connect gate="LPC" pin="PIO1_21/!DCD!/MISO1" pad="26"/>
<connect gate="LPC" pin="PIO1_22/!RI!/MOSI1" pad="38"/>
<connect gate="LPC" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="18"/>
<connect gate="LPC" pin="PIO1_24/CT32B0_MAT0" pad="21"/>
<connect gate="LPC" pin="PIO1_25/CT32B0_MAT1" pad="1"/>
<connect gate="LPC" pin="PIO1_26/CT32B0_MAT2/RXD" pad="11"/>
<connect gate="LPC" pin="PIO1_27/CT32B0_MAT3/TXD" pad="12"/>
<connect gate="LPC" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="24"/>
<connect gate="LPC" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="31"/>
<connect gate="LPC" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="LPC" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="LPC" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="LPC" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="LPC" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="LPC" pin="USB_DM" pad="19"/>
<connect gate="LPC" pin="USB_DP" pad="20"/>
<connect gate="LPC" pin="VDD@1" pad="44"/>
<connect gate="LPC" pin="VDD@2" pad="8"/>
<connect gate="LPC" pin="VSS@1" pad="41"/>
<connect gate="LPC" pin="VSS@2" pad="5"/>
<connect gate="LPC" pin="XTALIN" pad="6"/>
<connect gate="LPC" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FET" package="SOT1155-2">
<connects>
<connect gate="LPC" pin="!RESET!/PIO0_0" pad="C1"/>
<connect gate="LPC" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="B7"/>
<connect gate="LPC" pin="(PIO1_5/CT32B1_CAP1)PIO1_31" pad="H8"/>
<connect gate="LPC" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="C2"/>
<connect gate="LPC" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="A6"/>
<connect gate="LPC" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="A3"/>
<connect gate="LPC" pin="PIO0_18/RXD/CT32B0_MAT0" pad="B3"/>
<connect gate="LPC" pin="PIO0_19/TXD/CT32B0_MAT1" pad="B2"/>
<connect gate="LPC" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="F1"/>
<connect gate="LPC" pin="PIO0_20/CT16B1_CAP0" pad="F2"/>
<connect gate="LPC" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="G4"/>
<connect gate="LPC" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="E8"/>
<connect gate="LPC" pin="PIO0_23/AD7" pad="A5"/>
<connect gate="LPC" pin="PIO0_3/USB_VBUS" pad="H2"/>
<connect gate="LPC" pin="PIO0_4/SCL" pad="G3"/>
<connect gate="LPC" pin="PIO0_5/SDA" pad="H3"/>
<connect gate="LPC" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="H6"/>
<connect gate="LPC" pin="PIO0_7/!CTS!" pad="G7"/>
<connect gate="LPC" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="F8"/>
<connect gate="LPC" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="F7"/>
<connect gate="LPC" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="B8"/>
<connect gate="LPC" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="A8"/>
<connect gate="LPC" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="A4"/>
<connect gate="LPC" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="A2"/>
<connect gate="LPC" pin="PIO1_19/!DTR!/SSEL1" pad="B1"/>
<connect gate="LPC" pin="PIO1_20/!DSR!/SCK1" pad="H1"/>
<connect gate="LPC" pin="PIO1_21/!DCD!/MISO1" pad="G8"/>
<connect gate="LPC" pin="PIO1_22/!RI!/MOSI1" pad="A7"/>
<connect gate="LPC" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="H4"/>
<connect gate="LPC" pin="PIO1_24/CT32B0_MAT0" pad="G6"/>
<connect gate="LPC" pin="PIO1_25/CT32B0_MAT1" pad="A1"/>
<connect gate="LPC" pin="PIO1_26/CT32B0_MAT2/RXD" pad="G2"/>
<connect gate="LPC" pin="PIO1_27/CT32B0_MAT3/TXD" pad="G1"/>
<connect gate="LPC" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="H7"/>
<connect gate="LPC" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="D7"/>
<connect gate="LPC" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="E7"/>
<connect gate="LPC" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="B6"/>
<connect gate="LPC" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="D8"/>
<connect gate="LPC" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="C8"/>
<connect gate="LPC" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="C7"/>
<connect gate="LPC" pin="USB_DM" pad="G5"/>
<connect gate="LPC" pin="USB_DP" pad="H5"/>
<connect gate="LPC" pin="VDD@1" pad="B4"/>
<connect gate="LPC" pin="VDD@2" pad="E2"/>
<connect gate="LPC" pin="VSS@1" pad="B5"/>
<connect gate="LPC" pin="VSS@2" pad="D2"/>
<connect gate="LPC" pin="XTALIN" pad="D1"/>
<connect gate="LPC" pin="XTALOUT" pad="E1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U14FHN" prefix="U">
<description>&lt;h3&gt;NXP Semiconductors&lt;/h3&gt;
&lt;p&gt;&lt;h4&gt;The LPC11U1x also comes in a LQFP44 and TFBGA48 package with more pins.&lt;/h4&gt;&lt;p&gt; 

&lt;a href="http://ics.nxp.com/products/lpc1000/lpc11xx/"&gt;&lt;b&gt;LPC11Uxx&lt;/b&gt; microcontrollers&lt;/a&gt;
&lt;ul&gt;
&lt;li&gt;ARM 32-bit Cortex-M0 Microcontroller with MPU&lt;/li&gt;
&lt;li&gt;CPU clock up to 50MHz&lt;/li&gt;
&lt;li&gt;Up to 32KByte on-chip Flash ROM with In-System Programming (ISP) and In-Application Programming (IAP) via On-Chip Bootloader&lt;/li&gt;
&lt;li&gt;Up to 8KByte SRAM&lt;/li&gt;
&lt;li&gt;Nested Vectored Interrupt Controller&lt;/li&gt;
&lt;li&gt;Up to 2 SPI controllers&lt;/li&gt;
&lt;li&gt;USB 2.0 device controller&lt;/li&gt;
&lt;li&gt;USART with full Modem Interface and RS485 Support and ISO7816-3 support&lt;/li&gt;
&lt;li&gt;Fast Mode I2C-Bus&lt;/li&gt;
&lt;li&gt;4 Timers with 4 capture channels and 13 output channels&lt;/li&gt;
&lt;li&gt;Watchdog (WDT)&lt;/li&gt;
&lt;li&gt;Sytem tick timer&lt;/li&gt;
&lt;li&gt;10-bit ADC with 8 channels&lt;/li&gt;
&lt;li&gt;Power Management Unit (PMU)&lt;/li&gt;
&lt;li&gt;Brownout detection&lt;/li&gt;
&lt;li&gt;12MHz internal RC oscillator&lt;/li&gt;
&lt;li&gt;Serial Wire Debug/Trace port&lt;/li&gt;
&lt;/ul&gt;

Symbol copied from RH, package adapted to NXP spec (MK)</description>
<gates>
<gate name="G$1" symbol="LPC11U14-33"/>
</gates>
<devices>
<device name="" package="SOT-HVQFN33">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="2"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="3"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="30"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="12"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="20"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="27"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="28"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="1"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="USB_DM" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="14"/>
<connect gate="G$1" pin="VDD@1" pad="6"/>
<connect gate="G$1" pin="VDD@2" pad="29"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PESD1LVDS">
<description>&lt;H2&gt;ESD protection for in-vehicle ultra high-speed interfaces&lt;/H2&gt;
The device is designed to protect in-vehicle ultra high-speed interfaces in automotive 
applications, such as Low-Voltage Differential Signaling (LVDS), High-Definition 
Multimedia Interface (HDMI) and DisplayPort interfaces against ElectroStatic 
Discharge (ESD).&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/img/NXP_logo.png&gt;</description>
<gates>
<gate name="G$1" symbol="ESD-PROTECTION-NON_CLAMP"/>
</gates>
<devices>
<device name="" package="SOT1165-1">
<connects>
<connect gate="G$1" pin="CH1+" pad="2"/>
<connect gate="G$1" pin="CH1-" pad="1"/>
<connect gate="G$1" pin="CH2+" pad="5"/>
<connect gate="G$1" pin="CH2-" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1110FD20">
<description>&lt;b&gt;LPC1110 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1110FDX20"/>
</gates>
<devices>
<device name="" package="SOT163-1">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="18"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="5"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="6"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="11"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="12"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="17"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="10"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="8"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="7"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="9"/>
<connect gate="G$1" pin="VDD(3V3)" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTALIN" pad="14"/>
<connect gate="G$1" pin="XTALOUT" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1111FDH20">
<description>&lt;b&gt;LPC1111 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1110FDX20"/>
</gates>
<devices>
<device name="" package="SOT360">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="18"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="5"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="6"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="11"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="12"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="17"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="10"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="8"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="7"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="9"/>
<connect gate="G$1" pin="VDD(3V3)" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTALIN" pad="14"/>
<connect gate="G$1" pin="XTALOUT" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1112FD20">
<description>&lt;b&gt;LPC1112 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1110FDX20"/>
</gates>
<devices>
<device name="" package="SOT163-1">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="18"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="5"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="6"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="11"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="12"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="17"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="10"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="8"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="7"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="9"/>
<connect gate="G$1" pin="VDD(3V3)" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTALIN" pad="14"/>
<connect gate="G$1" pin="XTALOUT" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1112FDH20">
<description>&lt;b&gt;LPC1112&lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1112FDH20"/>
</gates>
<devices>
<device name="" package="SOT360">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="18"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="19"/>
<connect gate="G$1" pin="PIO0_3" pad="20"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="11"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="12"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="17"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="10"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="8"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="7"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="9"/>
<connect gate="G$1" pin="VDD(3V3)" pad="15"/>
<connect gate="G$1" pin="VDDA" pad="5"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="VSSA" pad="6"/>
<connect gate="G$1" pin="XTALIN" pad="14"/>
<connect gate="G$1" pin="XTALOUT" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1112FDH28">
<description>&lt;b&gt;LPC1112 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1112FDH28"/>
</gates>
<devices>
<device name="" package="SOT361-1">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="24"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="25"/>
<connect gate="G$1" pin="PIO0_3" pad="26"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="27"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="5"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="6"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="28"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="13"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="14"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="15"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="16"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="17"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="18"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="23"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="12"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="10"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="9"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="11"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="XTALIN" pad="20"/>
<connect gate="G$1" pin="XTALOUT" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1114FN28">
<description>&lt;b&gt;LPC1114 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1112FDH28"/>
</gates>
<devices>
<device name="" package="SOT117">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="24"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="25"/>
<connect gate="G$1" pin="PIO0_3" pad="26"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="27"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="5"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="6"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="28"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="13"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="14"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="15"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="16"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="17"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="18"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="23"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="12"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="10"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="9"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="11"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="XTALIN" pad="20"/>
<connect gate="G$1" pin="XTALOUT" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1112FHI33" prefix="U">
<description>&lt;b&gt;LPC1112 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114FHN33"/>
</gates>
<devices>
<device name="" package="SOT617-3">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1114FHI33" prefix="U">
<description>&lt;b&gt;LPC1114 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114FHN33"/>
</gates>
<devices>
<device name="" package="SOT617-3">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_3" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="1"/>
<connect gate="G$1" pin="PIO3_2" pad="28"/>
<connect gate="G$1" pin="PIO3_4" pad="13"/>
<connect gate="G$1" pin="PIO3_5" pad="14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1114FDH28">
<description>&lt;b&gt;LPC1114 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1112FDH28"/>
</gates>
<devices>
<device name="" package="SOT361-1">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="24"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="25"/>
<connect gate="G$1" pin="PIO0_3" pad="26"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="27"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="5"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="6"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="28"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="13"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="14"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="15"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="16"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="17"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="18"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="23"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="12"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="10"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="9"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="11"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="XTALIN" pad="20"/>
<connect gate="G$1" pin="XTALOUT" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC1G32" prefix="V">
<description>&lt;H2&gt;Single 2-input OR gate&lt;/H2&gt; The 74LVC1G32 provides one 2-input OR function.
Inputs can be driven from either 3.3 V or 5 V devices. This feature allows the use of these 
devices as translators in mixed 3.3 V and 5 V applications.
Schmitt trigger action at all inputs makes the circuit tolerant of slower input rise and fall 
time.
This device is fully specified for partial power-down applications using IOFF. 
The IOFF circuitry disables the output, preventing the damaging backflow current through 
the device when it is powered down.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G" symbol="2-INPUT-OR"/>
</gates>
<devices>
<device name="GW" package="SOT353-1">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GV" package="SOT753">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GX" package="SOT1226">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUK98180-100A">
<description>&lt;H2&gt;N-channel TrenchMOS logic level FET&lt;/H2&gt;Logic level N-channel enhancement mode Field-Effect Transistor (FET) in a plastic 
package using TrenchMOS technology. This product has been designed and qualified to 
the appropriate AEC standard for use in automotive critical applications. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="D" pad="2 4"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AUP1G57" prefix="U">
<description>&lt;H2&gt;Low-power configurable gate&lt;/H2&gt;The 74AUP1G57 provides configurable multiple functions. The output state is determined 
by eight patterns of 3-bit input. The user can choose the logic functions AND, OR, NAND, 
NOR, XNOR, inverter, and buffer. All inputs can be connected to VCC or GND.
This device ensures a very low static and dynamic power consumption across the entire 
VCC range from 0.8 V to 3.6 V.
This device is fully specified for partial power-down applications using IOFF. The IOFF
circuitry disables the output, preventing the damaging backflow current through the device 
when it is powered down.
The 74AUP1G57 has Schmitt trigger inputs making it capable of transforming slowly 
changing input signals into sharply defined, jitter-free output signals.
The inputs switch at different points for positive and negative-going signals. The difference 
between the positive voltage VT+ and the negative voltage VT- is defined as the input 
hysteresis voltage VH.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="74AUP1T57"/>
</gates>
<devices>
<device name="GW" package="SOT363">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 799 57125"/>
</technology>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 799 58132"/>
</technology>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 813 28132"/>
</technology>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 928 67132"/>
</technology>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="I2C" value="9352 917 43132"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1723" prefix="U">
<description>Switch mode power supply controller&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src=http://www.nxp.com/bbimages/NXP_logo.gif&gt;</description>
<gates>
<gate name="G$1" symbol="STARBUCK_TEA1721"/>
</gates>
<devices>
<device name="" package="SOT1175-1">
<connects>
<connect gate="G$1" pin="DRN" pad="7"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="2"/>
<connect gate="G$1" pin="GND3" pad="3"/>
<connect gate="G$1" pin="SRC" pad="6"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 968 88118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9509A" prefix="U">
<description>The PCA9509A is a level translating I2C-bus/SMBus repeater with two voltage supplies 
that enables processor low voltage 2-wire serial bus to interface with standard I2C-bus or 
SMBus I/O.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCA9509"/>
</gates>
<devices>
<device name="DP" package="SOT505-1">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC(A)" pad="1"/>
<connect gate="G$1" pin="VCC(B)" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM" package="SOT902">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC(A)" pad="1"/>
<connect gate="G$1" pin="VCC(B)" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9509" prefix="U">
<description>The PCA9509 is a level translating I2C-bus/SMBus repeater with two voltage supplies 
that enables processor low voltage 2-wire serial bus to interface with standard I2C-bus or 
SMBus I/O.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCA9509"/>
</gates>
<devices>
<device name="DP" package="SOT505-1">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC(A)" pad="1"/>
<connect gate="G$1" pin="VCC(B)" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM" package="SOT902">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC(A)" pad="1"/>
<connect gate="G$1" pin="VCC(B)" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SOT96-1">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC(A)" pad="1"/>
<connect gate="G$1" pin="VCC(B)" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BZX84J" prefix="D">
<gates>
<gate name="G$1" symbol="ZENER"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74ABT125" prefix="IC">
<description>&lt;H2&gt;Quad bus BUFFER, 3-state&lt;/H2&gt;The 74ABT125 high-performance BiCMOS device combines low static and dynamic 
power dissipation with high speed and high output drive.
The 74ABT125 device is a quad buffer that is ideal for driving bus lines. The device 
features four Output Enables (1OE, 2OE, 3OE, 4OE), each controlling one of the 3-state 
outputs.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="A" symbol="74125"/>
<gate name="B" symbol="74125"/>
<gate name="C" symbol="74125"/>
<gate name="D" symbol="74125"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="SOT27">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SOT108-1">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DB" package="SOT337">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PW" package="SOT402-1">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BQ" package="SOT762">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG2005CT" prefix="D">
<description>&lt;H2&gt;500 mA low VF dual MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier in 
common cathode configuration with an integrated guard ring for stress protection, 
encapsulated in a SOT23 (TO-236AB) small Surface-Mounted Device (SMD) plastic 
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="FARNELL" value="1972710"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BCX19" prefix="T">
<description>&lt;H2&gt;NPN general purpose transistor&lt;/H2&gt;NPN transistor in a SOT23 plastic package. PNP complement: BCX17.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BCX17" prefix="T">
<description>&lt;H2&gt;PNP general purpose transistors&lt;/H2&gt; PNP transistor in a SOT23 plastic package. 
NPN complement: BCX19.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KTY84" prefix="D">
<description>&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD68">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="K" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1113FBD48/301/302" prefix="IC">
<description>&lt;b&gt;LPC1113 &lt;/b&gt;&lt;p&gt;50 MHz 32-bit ARM Cortex-M0 based microcontroller featuring a high level of integration and very low power consumption. &lt;/p&gt;&lt;p&gt;&lt;H3&gt;On-chip flash program memory&lt;/H3&gt;
The LPC1110/11/12/13/14 contain 32 kB (LPC1114), 24 kB (LPC1113), 16 kB (LPC1112),
8 kB (LPC1111),or 4 kB (LPC1110) of on-chip flash memory.
&lt;h3&gt; On-chip SRAM&lt;/h3&gt;
The LPC1110/11/12/13/14 contain a total of 8 kB, 4 kB, 2 kB, or 1 kB on-chip static RAM
memory.
&lt;p&gt;&lt;author&gt;MK - Datasheet available on www.nxp.com&lt;/author&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1/SWO" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/!DTR!/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO2_1/!DSR!/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK0" pad="31"/>
<connect gate="G$1" pin="PIO2_2/!DCD!/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO2_3/!RI!/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="19"/>
<connect gate="G$1" pin="PIO2_5" pad="20"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0/!DTR!" pad="36"/>
<connect gate="G$1" pin="PIO3_1/!DSR!" pad="37"/>
<connect gate="G$1" pin="PIO3_2/!DCD!" pad="43"/>
<connect gate="G$1" pin="PIO3_3/!RI!" pad="48"/>
<connect gate="G$1" pin="PIO3_4" pad="18"/>
<connect gate="G$1" pin="PIO3_5" pad="21"/>
<connect gate="G$1" pin="R/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="R/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="R/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="R/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="VDD@1" pad="8"/>
<connect gate="G$1" pin="VDD@2" pad="44"/>
<connect gate="G$1" pin="VSS@1" pad="41"/>
<connect gate="G$1" pin="VSS@2" pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SL3S4001" prefix="U">
<description>The UHF EPCglobal Generation 2 standard allows the commercialized provision of mass
adoption of UHF RFID technology for passive smart tags and labels. Main fields of
applications are supply chain management and logistics for worldwide use with special
consideration of European, US and Chinese frequencies to ensure that operating
distances of several meters can be realized.
The UCODE I2C is a product out of the NXP Semiconductors UCODE product family. The
entire UCODE product family offers anti-collision and collision arbitration functionality.
This allows a reader to simultaneously operate multiple labels/tags within its antenna field.
A UCODE I2C based label/ tag requires no external power supply for contactless
operation.
Its contactless interface generates the power supply via the antenna circuit by propagative
energy transmission from the interrogator (reader), while the system clock is generated by
an on-chip oscillator. Data transmitted from the interrogator to the label/tag is
demodulated by the interface, and it also modulates the interrogator's electromagnetic
field for data transmission from the label/tag to the interrogator.
A label/tag can be operated without the need for line of sight or battery, as long as it is
connected to a dedicated antenna for the targeted frequency range. When the label/tag is
within the interrogator's operating range, the high-speed wireless interface allows data
transmission in both directions.
The UCODE I2C also features an I2C interface to read/write data from its build in memory.
In this mode the UCODE I2C needs to be supplied externally. The I2C interface supports
standard and fast I2C modes.
The used EEPROM is based on a field proven non-volatile memory technology. The
EEPROM memory cell is also used in high quality automotive applications.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="SL3S4001"/>
</gates>
<devices>
<device name="" package="SOT902">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RF1N" pad="2"/>
<connect gate="G$1" pin="RF1P" pad="1"/>
<connect gate="G$1" pin="RF2N" pad="6"/>
<connect gate="G$1" pin="RF2P" pad="7"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDDB" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMBT5550" prefix="T">
<description>NPN high-voltage transistor
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMBT5401">
<description>PNP high-voltage transistor&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMBT5551" prefix="T">
<description>&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMST5550" prefix="T">
<description>&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMST5551" prefix="T">
<description>&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMST5401" prefix="T">
<description>&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC847" prefix="T">
<description>&lt;H2&gt;45 V, 100 mA NPN general-purpose transistors&lt;/H2&gt;
NPN general-purpose transistor
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="T" package="SOT416">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="M" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="MB" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="F" package="SOT490">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B">
<attribute name="COMMENT" value="OBSOLETE"/>
</technology>
<technology name="C">
<attribute name="COMMENT" value="OBSOLETE"/>
</technology>
</technologies>
</device>
<device name="MM" package="SOT1263">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B">
<attribute name="COMMENT" value="DEVELOPMENT!"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC857" prefix="T">
<description>PNP general purpose transistors&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="T" package="SOT416">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="M" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="F" package="SOT490">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="A">
<attribute name="COMMENT" value="OBSOLETE"/>
</technology>
<technology name="B">
<attribute name="COMMENT" value="OBSOLETE"/>
</technology>
</technologies>
</device>
<device name="MB" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="MM" package="SOT1263">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC848" prefix="T">
<description>30 V, 100 mA NPN general-purpose transistors
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC846" prefix="T">
<description>65 V, 100 mA NPN general-purpose transistors
&lt;p&gt;&lt;author&gt;AAL Eindhoven  MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="T" package="SOT416">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="MB" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC850" prefix="T">
<description>BC849; BC850
NPN general purpose transistors
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC849" prefix="T">
<description>45 V, 100 mA NPN general-purpose transistors
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC856" prefix="T">
<description>PNP general purpose transistors
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="T" package="SOT416">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC859" prefix="T">
<description>PNP general purpose transistors
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC858" prefix="T">
<description>PNP general purpose transistors
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC860" prefix="T">
<description>PNP general purpose transistors
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC846BS" prefix="T">
<description>Dual 65 V, 100 mA NPN/NPN general-purpose transistor
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="NPN"/>
<gate name="-2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="B" pad="2"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-1" pin="E" pad="1"/>
<connect gate="-2" pin="B" pad="5"/>
<connect gate="-2" pin="C" pad="3"/>
<connect gate="-2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC846DS" prefix="T">
<description>Dual 65 V, 100 mA NPN/NPN general-purpose transistor
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="NPN"/>
<gate name="-2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT457">
<connects>
<connect gate="-1" pin="B" pad="2"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-1" pin="E" pad="1"/>
<connect gate="-2" pin="B" pad="5"/>
<connect gate="-2" pin="C" pad="3"/>
<connect gate="-2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC846S" prefix="T">
<description>Dual 65 V, 100 mA NPN/NPN general-purpose transistor
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="NPN"/>
<gate name="-2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="B" pad="2"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-1" pin="E" pad="1"/>
<connect gate="-2" pin="B" pad="5"/>
<connect gate="-2" pin="C" pad="3"/>
<connect gate="-2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC847BPN" prefix="T">
<description>NPN/PNP general-purpose transistor pair in a very small SOT363 (SC-88) Surface-Mounted Device (SMD) plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-N" symbol="NPN"/>
<gate name="-P" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-N" pin="B" pad="2"/>
<connect gate="-N" pin="C" pad="6"/>
<connect gate="-N" pin="E" pad="1"/>
<connect gate="-P" pin="B" pad="5"/>
<connect gate="-P" pin="C" pad="3"/>
<connect gate="-P" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC847BS" prefix="T">
<description>NPN/NPN general-purpose transistor pair in a very small SOT363 (SC-88) Surface-Mounted Device (SMD) plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="NPN"/>
<gate name="-2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="B" pad="2"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-1" pin="E" pad="1"/>
<connect gate="-2" pin="B" pad="5"/>
<connect gate="-2" pin="C" pad="3"/>
<connect gate="-2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC847BV" prefix="T">
<description>NPN/NPN general-purpose transistor pair in a very small SOT363 (SC-88) Surface-Mounted Device (SMD) plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="NPN"/>
<gate name="-2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="B" pad="2"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-1" pin="E" pad="1"/>
<connect gate="-2" pin="B" pad="5"/>
<connect gate="-2" pin="C" pad="3"/>
<connect gate="-2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="/S500"/>
<technology name="N"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC847DS" prefix="T">
<description>NPN/NPN general-purpose transistor pair in a small SOT457 (SC-74) Surface-Mounted Device (SMD) plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="NPN"/>
<gate name="-2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT457">
<connects>
<connect gate="-1" pin="B" pad="2"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-1" pin="E" pad="1"/>
<connect gate="-2" pin="B" pad="5"/>
<connect gate="-2" pin="C" pad="3"/>
<connect gate="-2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC857BS" prefix="T">
<description>PNP double transistor in an SC-88; SOT363 plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="PNP"/>
<gate name="-2" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="B" pad="2"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-1" pin="E" pad="1"/>
<connect gate="-2" pin="B" pad="5"/>
<connect gate="-2" pin="C" pad="3"/>
<connect gate="-2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC857BV" prefix="T">
<description>PNP double transistor in a SOT666 plastic package. NPN complement: BC847BV.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="PNP"/>
<gate name="-2" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="B" pad="2"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-1" pin="E" pad="1"/>
<connect gate="-2" pin="B" pad="5"/>
<connect gate="-2" pin="C" pad="3"/>
<connect gate="-2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PDTA114" prefix="T">
<description>PNP Resistor-Equipped Transistor (RET) family in small Surface-Mounted Device (SMD)
plastic packages.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNPRR"/>
</gates>
<devices>
<device name="E" package="SOT416">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="M" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="T" package="SOT23">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="U" package="SOT323">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="MB" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PDTA114T" prefix="T">
<description>PNP Resistor-Equipped Transistor (RET) family in small Surface-Mounted Device (SMD)
plastic packages.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNPR"/>
</gates>
<devices>
<device name="E" package="SOT416">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="M" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="T" package="SOT23">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="U" package="SOT323">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="S-A" package="SOT54A">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOT54">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S-V" package="SOT54V">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PDTC114" prefix="T">
<description>NPN Resistor-Equipped Transistor (RET) family in small Surface-Mounted Device (SMD)
plastic packages.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPNRR"/>
</gates>
<devices>
<device name="E" package="SOT416">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="M" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="T" package="SOT23">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="U" package="SOT323">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="MB" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PDTC114T" prefix="T">
<description>&lt;H2&gt;PDTC114T&lt;/H2&gt;
NPN Resistor-Equipped Transistor (RET) family in small Surface-Mounted Device (SMD)
plastic packages.
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPNR"/>
</gates>
<devices>
<device name="E" package="SOT416">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="M" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="T" package="SOT23">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="U" package="SOT323">
<connects>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="Y"/>
</technologies>
</device>
<device name="S-A" package="SOT54A">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOT54">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S-V" package="SOT54V">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="INPUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BSH105" prefix="T">
<description>N-channel enhancement mode MOS transistor</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMGD130UN" prefix="T">
<description>20 V, dual N-channel Trench MOSFET
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="N-MOSFET"/>
<gate name="-2" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="D" pad="6"/>
<connect gate="-1" pin="G" pad="2"/>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="D" pad="3"/>
<connect gate="-2" pin="G" pad="5"/>
<connect gate="-2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS40-07" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT143(B)">
<connects>
<connect gate="-1" pin="A" pad="4"/>
<connect gate="-1" pin="K" pad="1"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="K" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="FARNELL" value="8734364"/>
</technology>
</technologies>
</device>
<device name="V" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="4"/>
<connect gate="-2" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS40-04" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="FARNELL" value="1907602"/>
</technology>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BCV26" prefix="T">
<description>NXP darlington transistor Ic=500mA</description>
<gates>
<gate name="G$1" symbol="TRANSISTOR-PNP_PNP-DAR"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA57000" prefix="IC">
<description>&lt;b&gt;CapFREE 150 mA, low-noise, low-drop regulator&lt;/b&gt; with thermal protection</description>
<gates>
<gate name="G$1" symbol="SA57000"/>
</gates>
<devices>
<device name="D" package="SOT680">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PWROK" pad="4"/>
<connect gate="G$1" pin="PWRON" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="-25"/>
<technology name="-28"/>
<technology name="-29"/>
<technology name="-30"/>
<technology name="-31"/>
<technology name="-33"/>
<technology name="-36"/>
</technologies>
</device>
<device name="UK" package="WL-CSP5">
<connects>
<connect gate="G$1" pin="GND" pad="B2"/>
<connect gate="G$1" pin="PWROK" pad="C3"/>
<connect gate="G$1" pin="PWRON" pad="C1"/>
<connect gate="G$1" pin="VIN" pad="A1"/>
<connect gate="G$1" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="-25"/>
<technology name="-28"/>
<technology name="-29"/>
<technology name="-30"/>
<technology name="-31"/>
<technology name="-33"/>
<technology name="-36"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMDPB80XP" prefix="T">
<description>20 V, dual P-channel Trench MOSFET&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="P-MOSFET_2D"/>
<gate name="-2" symbol="P-MOSFET_2D"/>
</gates>
<devices>
<device name="" package="SOT1118">
<connects>
<connect gate="-1" pin="D" pad="6 7"/>
<connect gate="-1" pin="G" pad="2"/>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="D" pad="3 8"/>
<connect gate="-2" pin="G" pad="5"/>
<connect gate="-2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMZB370UNE" prefix="T">
<description>30 V, single N-channel Trench MOSFET&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-ESD"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PBSS2515MB" prefix="T">
<description>15 V, 0.5 A NPN low VCEsat (BISS) transistor&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM75B" prefix="U">
<description>Digital temperature sensor and thermal watchdog&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LM75B"/>
</gates>
<devices>
<device name="D" package="SOT96-1">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OS" pad="3"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DP" package="SOT505-1">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OS" pad="3"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GD" package="SOT996-2/3">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OS" pad="3"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TP" package="SOT1069-2">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OS" pad="3"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BGA7210">
<description>700 MHz to 3800 MHz high linearity variable gain amplifier</description>
<gates>
<gate name="G$1" symbol="BGA7210"/>
</gates>
<devices>
<device name="" package="SOT617-3">
<connects>
<connect gate="G$1" pin="!SS!" pad="21"/>
<connect gate="G$1" pin="CLK" pad="23"/>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 13 14 18 25 26 27 28 31 32 33"/>
<connect gate="G$1" pin="PUPMXG" pad="24"/>
<connect gate="G$1" pin="RF_IN" pad="29"/>
<connect gate="G$1" pin="RF_OUT" pad="12"/>
<connect gate="G$1" pin="SEROUT" pad="20"/>
<connect gate="G$1" pin="SER_IN" pad="22"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="15"/>
<connect gate="G$1" pin="VDDA" pad="16"/>
<connect gate="G$1" pin="VDDD" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLVH431" prefix="D">
<description>&lt;H2&gt;Low voltage adjustable precision shunt regulators&lt;/H2&gt;
Low voltage three-terminal shunt regulator family with an output voltage range between 
Vref
(1.24 V) and 18 V, to be set by two external resistors.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SHUNT"/>
</gates>
<devices>
<device name="ZR" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="REF" pad="1"/>
</connects>
<technologies>
<technology name="ACDB">
<attribute name="12NC" value="9352 930 25215"/>
<attribute name="FARNELL" value="2143332"/>
<attribute name="MIRRORED" value="NO"/>
<attribute name="TEMPERATURE_RANGE" value="0C to 70C"/>
<attribute name="TOLERANCE" value="1%"/>
</technology>
<technology name="AIDB">
<attribute name="12NC" value="9352 930 26215"/>
<attribute name="FARNELL" value="2143333"/>
<attribute name="MIRRORED" value="NO"/>
<attribute name="TEMPERATURE_RANGE" value="-40C to 85C"/>
<attribute name="TOLERANCE" value="1%"/>
</technology>
<technology name="AQDB">
<attribute name="12NC" value="9352 930 27215"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRRORED" value="NO"/>
<attribute name="TEMPERATURE_RANGE" value="-40C to 125C"/>
<attribute name="TOLERANCE" value="1%"/>
</technology>
<technology name="CDB">
<attribute name="12NC" value="9352 930 22215"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRRORED" value="NO"/>
<attribute name="TEMPERATURE_RANGE" value="0C to 70C"/>
<attribute name="TOLERANCE" value="1.5%"/>
</technology>
<technology name="DQDB">
<attribute name="12NC" value="9352 957 29215"/>
<attribute name="FARNELL" value="2143337"/>
<attribute name="MIRRORED" value="NO"/>
<attribute name="TEMPERATURE_RANGE" value="-40C to 125C"/>
<attribute name="TOLERANCE" value="0.75%"/>
</technology>
<technology name="IDB">
<attribute name="12NC" value="9352 930 23215"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRRORED" value="NO"/>
<attribute name="TEMPERATURE_RANGE" value="-40C to 85C"/>
<attribute name="TOLERANCE" value="1.5%"/>
</technology>
<technology name="QDB">
<attribute name="12NC" value="9352 930 24215"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRRORED" value="NO"/>
<attribute name="TEMPERATURE_RANGE" value="-40C to 125C"/>
<attribute name="TOLERANCE" value="1.5%"/>
</technology>
</technologies>
</device>
<device name="VR" package="SOT753">
<connects>
<connect gate="G$1" pin="A" pad="5"/>
<connect gate="G$1" pin="K" pad="3"/>
<connect gate="G$1" pin="REF" pad="4"/>
</connects>
<technologies>
<technology name="AQDB">
<attribute name="12NC" value="9352 949 17125"/>
<attribute name="FARNELL" value="2143335"/>
<attribute name="MIRORRED" value="NO"/>
<attribute name="TEMPERATURE" value="40C to 125C"/>
<attribute name="TOLERANCE" value="1%"/>
</technology>
<technology name="DQDB">
<attribute name="12NC" value="9352 971 91125"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRORRED" value="NO"/>
<attribute name="TEMPERATURE" value="40C to 125C"/>
<attribute name="TOLERANCE" value="0.75%"/>
</technology>
<technology name="QDB">
<attribute name="12NC" value="9352 949 14125"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRORRED" value="NO"/>
<attribute name="TEMPERATURE" value="40C to 125C"/>
<attribute name="TOLERANCE" value="1.5%"/>
</technology>
</technologies>
</device>
<device name="MQDBZR" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="K" pad="1"/>
<connect gate="G$1" pin="REF" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 930 33215"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRRORED" value="YES"/>
<attribute name="TEMPERATURE_RANGE" value="-40C to 125C"/>
<attribute name="TOLERANCE" value="1.5%"/>
</technology>
<technology name="A">
<attribute name="12NC" value="9352 930 34215"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRRORED" value="YES"/>
<attribute name="TEMPERATURE_RANGE" value="-40C to 125C"/>
<attribute name="TOLERANCE" value="1%"/>
</technology>
<technology name="D">
<attribute name="12NC" value="9352 957 31215"/>
<attribute name="FARNELL" value="-"/>
<attribute name="MIRRORED" value="YES"/>
<attribute name="TEMPERATURE_RANGE" value="-40C to 125C"/>
<attribute name="TOLERANCE" value="0.75%"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NXPS20H100C" prefix="D">
<description>&lt;H2&gt;Dual power Schottky diode&lt;/H2&gt;Dual common cathode power Schottky diode designed for high frequency switched mode 
power supplies in a SOT78 (TO-220AB) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT78">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="K1K2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ISOLATED" value="NO"/>
</technology>
</technologies>
</device>
<device name="X" package="SOT186A">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="K1K2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ISOLATED" value="YES"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF2123" prefix="U">
<description>&lt;H2&gt;SPI Real time clock/calendar&lt;/H2&gt;
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCF2123"/>
</gates>
<devices>
<device name="TS" package="SOT402-1">
<connects>
<connect gate="G$1" pin="!INT1!" pad="5"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="CLKOE" pad="12"/>
<connect gate="G$1" pin="CLKOUT" pad="13"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDI" pad="9"/>
<connect gate="G$1" pin="SDO" pad="8"/>
<connect gate="G$1" pin="TEST" pad="4"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BS" package="SOT758-1">
<connects>
<connect gate="G$1" pin="!INT1!" pad="3"/>
<connect gate="G$1" pin="CE" pad="4"/>
<connect gate="G$1" pin="CLKOE" pad="11"/>
<connect gate="G$1" pin="CLKOUT" pad="12"/>
<connect gate="G$1" pin="OSCI" pad="16"/>
<connect gate="G$1" pin="OSCO" pad="1"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDI" pad="9"/>
<connect gate="G$1" pin="SDO" pad="8"/>
<connect gate="G$1" pin="TEST" pad="2"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PSMN" prefix="T">
<description>&lt;H2&gt;N-channel logic level TrenchMOS(TM) transistor&lt;/H2&gt;
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="MLC" package="SOT1210">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="013-30">
<attribute name="LOGIC_LEVEL" value="13 mOhm"/>
<attribute name="VOLTAGE" value="30V"/>
</technology>
<technology name="2R8-25">
<attribute name="LOGIC_LEVEL" value="2.8 mOhm"/>
<attribute name="VOLTAGE" value="25V"/>
</technology>
<technology name="2R9-30">
<attribute name="LOGIC_LEVEL" value="2.9 mOhm"/>
<attribute name="VOLTAGE" value="30V"/>
</technology>
<technology name="3R0-30">
<attribute name="LOGIC_LEVEL" value="3.0 mOhm"/>
<attribute name="VOLTAGE" value="30V"/>
</technology>
<technology name="3R9-25">
<attribute name="LOGIC_LEVEL" value="3.9 mOhm"/>
<attribute name="VOLTAGE" value="25V"/>
</technology>
<technology name="4R4-30">
<attribute name="LOGIC_LEVEL" value="4.4 mOhm"/>
<attribute name="VOLTAGE" value="30V"/>
</technology>
<technology name="7R0-30">
<attribute name="LOGIC_LEVEL" value="7.0 mOhm"/>
<attribute name="VOLTAGE" value="30V"/>
</technology>
<technology name="9R0-25">
<attribute name="LOGIC_LEVEL" value="9.0 mOhm"/>
<attribute name="VOLTAGE" value="25V"/>
</technology>
<technology name="9R8-30">
<attribute name="LOGIC_LEVEL" value="9.8 mOhm"/>
<attribute name="VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
<device name="YL" package="SOT1023">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="011-30"/>
<technology name="1R2-25"/>
<technology name="1R3-30"/>
<technology name="1R5-30"/>
<technology name="1R7-30"/>
<technology name="3R0-30"/>
<technology name="3R5-30"/>
<technology name="4R0-30"/>
<technology name="5R0-30"/>
<technology name="5R9-30"/>
<technology name="6R0-30"/>
<technology name="9R0-30"/>
<technology name="9R1-30"/>
</technologies>
</device>
<device name="YLC" package="SOT669">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="010-25"/>
<technology name="011-30"/>
<technology name="012-25"/>
<technology name="013-30"/>
<technology name="0R9-25"/>
<technology name="12-25"/>
<technology name="1R0-30"/>
<technology name="1R1-25"/>
<technology name="1R2-25"/>
<technology name="1R2-30"/>
<technology name="1R5-30"/>
<technology name="1R6-40"/>
<technology name="1R7-25"/>
<technology name="1R8-40"/>
<technology name="1R9-25"/>
<technology name="2R2-25"/>
<technology name="2R2-30"/>
<technology name="2R6-30"/>
<technology name="2R9-25"/>
<technology name="3R2-25"/>
<technology name="3R2-30"/>
<technology name="3R7-25"/>
<technology name="3R7-30"/>
<technology name="4R0-25"/>
<technology name="4R1-30"/>
<technology name="4R5-30"/>
<technology name="6R5-25"/>
</technologies>
</device>
<device name="K" package="SOT96-1">
<connects>
<connect gate="G$1" pin="D" pad="5 6 7 8"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="005-30"/>
<technology name="006-20"/>
<technology name="038-100"/>
<technology name="085-150"/>
<technology name="165-200"/>
</technologies>
</device>
<device name="P" package="SOT78">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="003-30"/>
<technology name="004-36"/>
<technology name="005-55"/>
<technology name="005-75"/>
<technology name="008-75"/>
<technology name="009-100"/>
<technology name="015-100"/>
<technology name="030-150"/>
<technology name="035-150"/>
<technology name="057-200"/>
<technology name="070-200"/>
<technology name="5R6-100"/>
</technologies>
</device>
<device name="B" package="SOT404">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="003-30"/>
<technology name="004-36"/>
<technology name="004-60"/>
<technology name="005-55"/>
<technology name="005-75"/>
<technology name="008-75"/>
<technology name="009-100"/>
<technology name="015-100"/>
<technology name="035-150"/>
<technology name="070-200"/>
</technologies>
</device>
<device name="YS" package="SOT669">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="011-80"/>
<technology name="012-100"/>
<technology name="012-60"/>
<technology name="013-80"/>
<technology name="014-40"/>
<technology name="016-100"/>
<technology name="017-60"/>
<technology name="018-80"/>
<technology name="020-100"/>
<technology name="026-80"/>
<technology name="028-100"/>
<technology name="030-60"/>
<technology name="039-100"/>
<technology name="045-80"/>
<technology name="069-100"/>
<technology name="3R3-40"/>
<technology name="4R0-40"/>
<technology name="5R5-60"/>
<technology name="5R8-40"/>
<technology name="8R2-80"/>
<technology name="8R3-40"/>
</technologies>
</device>
<device name="D" package="SOT428">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="005-25"/>
<technology name="010-55"/>
<technology name="025-100"/>
<technology name="063-150"/>
<technology name="130-200"/>
</technologies>
</device>
<device name="PS" package="SOT78">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="012-80"/>
<technology name="013-100"/>
<technology name="015-60"/>
<technology name="016-100"/>
<technology name="017-80"/>
<technology name="027-100"/>
<technology name="034-100"/>
<technology name="1R5-40"/>
<technology name="2R0-60"/>
<technology name="2R2-40"/>
<technology name="2R8-40"/>
<technology name="3R0-60"/>
<technology name="3R3-80"/>
<technology name="3R5-80"/>
<technology name="4R3-100"/>
<technology name="4R3-80"/>
<technology name="4R4-80"/>
<technology name="4R5-40"/>
<technology name="4R6-60"/>
<technology name="5R0-100"/>
<technology name="5R0-80"/>
<technology name="6R5-80"/>
<technology name="7R0-100"/>
</technologies>
</device>
<device name="XS" package="SOT186A">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="013-100"/>
<technology name="016-100"/>
<technology name="027-100"/>
<technology name="4R6-100"/>
<technology name="5R0-100"/>
<technology name="5R6-100"/>
<technology name="7R0-100"/>
<technology name="9R5-100"/>
</technologies>
</device>
<device name="BS" package="SOT404">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="012-80"/>
<technology name="013-100"/>
<technology name="015-60"/>
<technology name="016-100"/>
<technology name="017-80"/>
<technology name="027-100"/>
<technology name="034-100"/>
<technology name="050-80"/>
<technology name="1R1-40"/>
<technology name="1R7-60"/>
<technology name="2R0-60"/>
<technology name="2R2-40"/>
<technology name="2R8-40"/>
<technology name="2R8-80"/>
<technology name="3R0-60"/>
<technology name="3R3-80"/>
<technology name="3R8-100"/>
<technology name="4R3-80"/>
<technology name="4R4-80"/>
<technology name="4R5-40"/>
<technology name="4R6-60"/>
<technology name="5R0-100"/>
<technology name="5R0-80"/>
<technology name="5R6-100"/>
<technology name="6R5-80"/>
<technology name="7R0-100"/>
</technologies>
</device>
<device name="YLB" package="SOT669">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="6R0-25"/>
<technology name="6R0-30"/>
</technologies>
</device>
<device name="LL" package="SOT873-1">
<connects>
<connect gate="G$1" pin="D" pad="5 6 7 8"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="013-30"/>
<technology name="017-30"/>
<technology name="3R5-30"/>
<technology name="3R8-30"/>
<technology name="5R8-30"/>
<technology name="9R0-30"/>
</technologies>
</device>
<device name="LS" package="SOT873-1">
<connects>
<connect gate="G$1" pin="D" pad="5 6 7 8"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="014-60"/>
<technology name="023-80"/>
<technology name="035-100"/>
</technologies>
</device>
<device name="PL" package="SOT78">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="017-30"/>
<technology name="022-30"/>
<technology name="1R1-30"/>
<technology name="1R6-30"/>
<technology name="1R8-30"/>
<technology name="2R0-30"/>
<technology name="2R7-30"/>
<technology name="3R4-30"/>
<technology name="4R3-30"/>
</technologies>
</device>
<device name="BL" package="SOT404">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="017-30"/>
<technology name="022-30"/>
<technology name="1R1-30"/>
<technology name="1R6-30"/>
<technology name="1R8-30"/>
<technology name="2R0-60"/>
<technology name="2R7-30"/>
<technology name="3R4-30"/>
<technology name="4R3-30"/>
</technologies>
</device>
<device name="Y" package="SOT669">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="059-150"/>
<technology name="102-200"/>
</technologies>
</device>
<device name="W" package="SOT429">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="004-55"/>
<technology name="009-100"/>
<technology name="040-200"/>
</technologies>
</device>
<device name="ES" package="SOT226">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="013-100"/>
<technology name="1R5-40"/>
<technology name="3R0-60"/>
<technology name="3R3-80"/>
<technology name="3R5-80"/>
<technology name="4R3-100"/>
<technology name="4R3-80"/>
<technology name="5R0-100"/>
<technology name="7R0-100"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N7002B" prefix="T">
<description>&lt;H2&gt;60 V, single N-channel Trench MOSFET&lt;/H2&gt;N-channel enhancement mode Field-Effect Transistor (FET) in a leadless ultra small 
DFN1006B-3 (SOT883B) Surface-Mounted Device (SMD) plastic package using Trench 
MOSFET technology.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-ESD"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="KM"/>
<technology name="MB"/>
</technologies>
</device>
<device name="KW" package="SOT323">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KT" package="SOT416">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="K" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NX3008NBKMB" prefix="T">
<description>30 V, single N-channel Trench MOSFET
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-ESD"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NX3008PBKMB" prefix="T">
<description>30 V, single P-channel Trench MOSFET
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="P-MOSFER-TR"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMZB670UPE" prefix="T">
<description>20 V, single P-channel Trench MOSFET&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="P-MOSFER-TR"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMZB290UNE" prefix="T">
<description>20 V, single N-channel Trench MOSFET&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-ESD"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMZB290UN" prefix="T">
<description>20 V, single N-channel Trench MOSFET&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BSS84A" prefix="T">
<description>&lt;H2&gt;50 V, 150 mA P-channel Trench MOSFET&lt;/H2&gt;
P-channel enhancement mode Field-Effect Transistor (FET) in a small 
Surface-Mounted Device (SMD) plastic package using Trench MOSFET technology.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="P-MOSFER-TR"/>
</gates>
<devices>
<device name="M" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="K"/>
</technologies>
</device>
<device name="KW" package="SOT323">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KT" package="SOT416">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MB" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="K"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMZB420UN" prefix="T">
<description>30 V, single N-channel Trench MOSFET&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1703" prefix="U">
<description>GreenChip SMPS standby control IC</description>
<gates>
<gate name="G$1" symbol="TEA1703"/>
</gates>
<devices>
<device name="" package="SOT96-1">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="5"/>
<connect gate="G$1" pin="OPTO" pad="3"/>
<connect gate="G$1" pin="PSENSE" pad="7"/>
<connect gate="G$1" pin="SWDETECT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VSENSE" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BYC8X-600P" prefix="D">
<description>Hyperfast power diode</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD113">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8537A" prefix="U">
<description>&lt;H2&gt;Industrial LCD driver for multiplex rates up to 1:8. I2C version.&lt;/H2&gt;
The PCF8537 is a fully featured Liquid Crystal Display (LCD) driver, specifically designed 
for high-contrast Vertical Alignment (VA) LCD with multiplex rates up to 1:8. It generates 
the drive signals for any static or multiplexed LCD containing up to eight backplanes, 
46 segments, and up to 352 elements. The PCF8537 features an internal charge pump 
with internal capacitors for on-chip generation of the LCD driving voltage. To ensure an 
optimal and stable contrast over the full temperature range, the PCF8537 offers a 
programmable temperature compensation of the LCD supply voltage. The PCF8537 can 
be easily connected to a microcontroller by either the two-line I2C-bus (PCF8537AH) or a 
three-line bidirectional SPI-bus (PCF8537BH).
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8537A"/>
</gates>
<devices>
<device name="" package="SOT357-1">
<connects>
<connect gate="G$1" pin="!RESET!" pad="33"/>
<connect gate="G$1" pin="A0" pad="36"/>
<connect gate="G$1" pin="BP0" pad="45"/>
<connect gate="G$1" pin="BP1" pad="46"/>
<connect gate="G$1" pin="BP2" pad="47"/>
<connect gate="G$1" pin="BP3" pad="48"/>
<connect gate="G$1" pin="BP4" pad="49"/>
<connect gate="G$1" pin="BP5" pad="50"/>
<connect gate="G$1" pin="CLK" pad="39"/>
<connect gate="G$1" pin="S0" pad="32"/>
<connect gate="G$1" pin="S1" pad="31"/>
<connect gate="G$1" pin="S10" pad="22"/>
<connect gate="G$1" pin="S11" pad="21"/>
<connect gate="G$1" pin="S12" pad="20"/>
<connect gate="G$1" pin="S13" pad="19"/>
<connect gate="G$1" pin="S14" pad="18"/>
<connect gate="G$1" pin="S15" pad="17"/>
<connect gate="G$1" pin="S16" pad="16"/>
<connect gate="G$1" pin="S17" pad="15"/>
<connect gate="G$1" pin="S18" pad="14"/>
<connect gate="G$1" pin="S19" pad="13"/>
<connect gate="G$1" pin="S2" pad="30"/>
<connect gate="G$1" pin="S20" pad="12"/>
<connect gate="G$1" pin="S21" pad="11"/>
<connect gate="G$1" pin="S22" pad="10"/>
<connect gate="G$1" pin="S23" pad="9"/>
<connect gate="G$1" pin="S24" pad="8"/>
<connect gate="G$1" pin="S25" pad="7"/>
<connect gate="G$1" pin="S26" pad="6"/>
<connect gate="G$1" pin="S27" pad="5"/>
<connect gate="G$1" pin="S28" pad="4"/>
<connect gate="G$1" pin="S29" pad="3"/>
<connect gate="G$1" pin="S3" pad="29"/>
<connect gate="G$1" pin="S30" pad="2"/>
<connect gate="G$1" pin="S31" pad="1"/>
<connect gate="G$1" pin="S32" pad="64"/>
<connect gate="G$1" pin="S33" pad="63"/>
<connect gate="G$1" pin="S34" pad="62"/>
<connect gate="G$1" pin="S35" pad="61"/>
<connect gate="G$1" pin="S36" pad="60"/>
<connect gate="G$1" pin="S37" pad="59"/>
<connect gate="G$1" pin="S38" pad="58"/>
<connect gate="G$1" pin="S39" pad="57"/>
<connect gate="G$1" pin="S4" pad="28"/>
<connect gate="G$1" pin="S40" pad="56"/>
<connect gate="G$1" pin="S41" pad="55"/>
<connect gate="G$1" pin="S42" pad="54"/>
<connect gate="G$1" pin="S43" pad="53"/>
<connect gate="G$1" pin="S44/BP7" pad="52"/>
<connect gate="G$1" pin="S45/BP6" pad="51"/>
<connect gate="G$1" pin="S5" pad="27"/>
<connect gate="G$1" pin="S6" pad="26"/>
<connect gate="G$1" pin="S7" pad="25"/>
<connect gate="G$1" pin="S8" pad="24"/>
<connect gate="G$1" pin="S9" pad="23"/>
<connect gate="G$1" pin="SCL" pad="35"/>
<connect gate="G$1" pin="SDA" pad="34"/>
<connect gate="G$1" pin="T1" pad="37"/>
<connect gate="G$1" pin="T2" pad="38"/>
<connect gate="G$1" pin="T3" pad="40"/>
<connect gate="G$1" pin="VDD1" pad="42"/>
<connect gate="G$1" pin="VDD2" pad="43"/>
<connect gate="G$1" pin="VLCD" pad="44"/>
<connect gate="G$1" pin="VSS" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8537B" prefix="U">
<description>&lt;H2&gt;Industrial LCD driver for multiplex rates up to 1:8. SPI version.&lt;/H2&gt;
The PCF8537 is a fully featured Liquid Crystal Display (LCD) driver, specifically designed 
for high-contrast Vertical Alignment (VA) LCD with multiplex rates up to 1:8. It generates 
the drive signals for any static or multiplexed LCD containing up to eight backplanes, 
46 segments, and up to 352 elements. The PCF8537 features an internal charge pump 
with internal capacitors for on-chip generation of the LCD driving voltage. To ensure an 
optimal and stable contrast over the full temperature range, the PCF8537 offers a 
programmable temperature compensation of the LCD supply voltage. The PCF8537 can 
be easily connected to a microcontroller by either the two-line I2C-bus (PCF8537AH) or a 
three-line bidirectional SPI-bus (PCF8537BH).
&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8537B"/>
</gates>
<devices>
<device name="" package="SOT357-1">
<connects>
<connect gate="G$1" pin="!CE!" pad="34"/>
<connect gate="G$1" pin="!RESET!" pad="33"/>
<connect gate="G$1" pin="BP0" pad="45"/>
<connect gate="G$1" pin="BP1" pad="46"/>
<connect gate="G$1" pin="BP2" pad="47"/>
<connect gate="G$1" pin="BP3" pad="48"/>
<connect gate="G$1" pin="BP4" pad="49"/>
<connect gate="G$1" pin="BP5" pad="50"/>
<connect gate="G$1" pin="CLK" pad="39"/>
<connect gate="G$1" pin="S0" pad="32"/>
<connect gate="G$1" pin="S1" pad="31"/>
<connect gate="G$1" pin="S10" pad="22"/>
<connect gate="G$1" pin="S11" pad="21"/>
<connect gate="G$1" pin="S12" pad="20"/>
<connect gate="G$1" pin="S13" pad="19"/>
<connect gate="G$1" pin="S14" pad="18"/>
<connect gate="G$1" pin="S15" pad="17"/>
<connect gate="G$1" pin="S16" pad="16"/>
<connect gate="G$1" pin="S17" pad="15"/>
<connect gate="G$1" pin="S18" pad="14"/>
<connect gate="G$1" pin="S19" pad="13"/>
<connect gate="G$1" pin="S2" pad="30"/>
<connect gate="G$1" pin="S20" pad="12"/>
<connect gate="G$1" pin="S21" pad="11"/>
<connect gate="G$1" pin="S22" pad="10"/>
<connect gate="G$1" pin="S23" pad="9"/>
<connect gate="G$1" pin="S24" pad="8"/>
<connect gate="G$1" pin="S25" pad="7"/>
<connect gate="G$1" pin="S26" pad="6"/>
<connect gate="G$1" pin="S27" pad="5"/>
<connect gate="G$1" pin="S28" pad="4"/>
<connect gate="G$1" pin="S29" pad="3"/>
<connect gate="G$1" pin="S3" pad="29"/>
<connect gate="G$1" pin="S30" pad="2"/>
<connect gate="G$1" pin="S31" pad="1"/>
<connect gate="G$1" pin="S32" pad="64"/>
<connect gate="G$1" pin="S33" pad="63"/>
<connect gate="G$1" pin="S34" pad="62"/>
<connect gate="G$1" pin="S35" pad="61"/>
<connect gate="G$1" pin="S36" pad="60"/>
<connect gate="G$1" pin="S37" pad="59"/>
<connect gate="G$1" pin="S38" pad="58"/>
<connect gate="G$1" pin="S39" pad="57"/>
<connect gate="G$1" pin="S4" pad="28"/>
<connect gate="G$1" pin="S40" pad="56"/>
<connect gate="G$1" pin="S41" pad="55"/>
<connect gate="G$1" pin="S42" pad="54"/>
<connect gate="G$1" pin="S43" pad="53"/>
<connect gate="G$1" pin="S44/BP7" pad="52"/>
<connect gate="G$1" pin="S45/BP6" pad="51"/>
<connect gate="G$1" pin="S5" pad="27"/>
<connect gate="G$1" pin="S6" pad="26"/>
<connect gate="G$1" pin="S7" pad="25"/>
<connect gate="G$1" pin="S8" pad="24"/>
<connect gate="G$1" pin="S9" pad="23"/>
<connect gate="G$1" pin="SCL" pad="35"/>
<connect gate="G$1" pin="SDIO" pad="36"/>
<connect gate="G$1" pin="T1" pad="37"/>
<connect gate="G$1" pin="T2" pad="38"/>
<connect gate="G$1" pin="T3" pad="40"/>
<connect gate="G$1" pin="VDD1" pad="42"/>
<connect gate="G$1" pin="VDD2" pad="43"/>
<connect gate="G$1" pin="VLCD" pad="44"/>
<connect gate="G$1" pin="VSS" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTA410X" prefix="T">
<description>3Q Hi-Com Triac</description>
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="" package="SOT186A">
<connects>
<connect gate="G$1" pin="CM" pad="1"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="LD" pad="2"/>
</connects>
<technologies>
<technology name="-800CT"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PBSS3515MB" prefix="T">
<description>15 V, 0.5 A PNP low VCEsat (BISS) transistor</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NX3DV221" prefix="U">
<description>High-speed USB 2.0 switch with enable</description>
<gates>
<gate name="G$1" symbol="NX3DV221"/>
</gates>
<devices>
<device name="GM" package="SOT1049">
<connects>
<connect gate="G$1" pin="!OE!" pad="6"/>
<connect gate="G$1" pin="1D+" pad="1"/>
<connect gate="G$1" pin="1D-" pad="2"/>
<connect gate="G$1" pin="2D+" pad="3"/>
<connect gate="G$1" pin="2D-" pad="4"/>
<connect gate="G$1" pin="D+" pad="8"/>
<connect gate="G$1" pin="D-" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="S" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NTS0102" prefix="U">
<description>Dual supply translating transceiver; open drain; auto direction sensing</description>
<gates>
<gate name="G$1" symbol="NTS0102"/>
</gates>
<devices>
<device name="GD" package="SOT996-2/3">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="B1" pad="8"/>
<connect gate="G$1" pin="B2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="6"/>
<connect gate="G$1" pin="VCC(A)" pad="3"/>
<connect gate="G$1" pin="VCC(B)" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF" package="SOT1089-1">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="B1" pad="8"/>
<connect gate="G$1" pin="B2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="6"/>
<connect gate="G$1" pin="VCC(A)" pad="3"/>
<connect gate="G$1" pin="VCC(B)" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GU" package="SOT1160-1">
<connects>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A2" pad="1"/>
<connect gate="G$1" pin="B1" pad="8"/>
<connect gate="G$1" pin="B2" pad="5"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="OE" pad="4"/>
<connect gate="G$1" pin="VCC(A)" pad="2"/>
<connect gate="G$1" pin="VCC(B)" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DP" package="SOT505-2">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="B1" pad="8"/>
<connect gate="G$1" pin="B2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="6"/>
<connect gate="G$1" pin="VCC(A)" pad="3"/>
<connect gate="G$1" pin="VCC(B)" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUK9Y19" prefix="T">
<description>&lt;H2&gt;N-channel TrenchMOS logic level FET&lt;/H2&gt;
Logic level N-channel enhancement mode Field-Effect Transistor (FET) in a plastic 
package using TrenchMOS technology. &lt;p&gt;This product has been designed and qualified to 
the appropriate AEC standard for use in automotive critical applications.&lt;p&gt;
&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
&lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="B" package="SOT669">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="-75"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PESD5V0S1BSF" prefix="D">
<description>&lt;H2&gt;Bidirectional low capacitance ESD protection diode&lt;/H2&gt;
Low capacitance bidirectional ElectroStatic Discharge (ESD) protection diode in a 
SOD962 leadless ultra small Surface-Mounted Device (SMD) package designed to 
protect one signal line from the damage caused by ESD and other transients.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_ESD_KK"/>
</gates>
<devices>
<device name="" package="SOD962">
<connects>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG2005" prefix="D">
<description>&lt;H2&gt;20 V, 0.5 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EPK" package="SOD1608">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AEA" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EL" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
<device name="EB" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ELD" package="SOD882D">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
</technologies>
</device>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ET" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AEV" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACT108">
<description>&lt;H2&gt;AC Thyristor power switch&lt;/H2&gt; AC Thyristor power switch in a SOT54 plastic package with self-protective capabilities 
against low and high energy transients&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="" package="SOT54A">
<connects>
<connect gate="G$1" pin="CM" pad="1"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="LD" pad="3"/>
</connects>
<technologies>
<technology name="-600D"/>
<technology name="-600E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB40" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS76SB40" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS79SB40" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS40" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9340 345 30215"/>
</technology>
</technologies>
</device>
<device name="H" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9340 592 81115"/>
</technology>
</technologies>
</device>
<device name="L" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9340 572 53315"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB44" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB45" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS75SB45" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT416">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS40-05" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB46" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS40-06" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS40-05V" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SDD_AKKA"/>
<gate name="-2" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="A1" pad="1"/>
<connect gate="-1" pin="A2" pad="2"/>
<connect gate="-1" pin="K1K2" pad="6"/>
<connect gate="-2" pin="A1" pad="4"/>
<connect gate="-2" pin="A2" pad="5"/>
<connect gate="-2" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS88SB48" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SDD_AKKA"/>
<gate name="-2" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="A1" pad="1"/>
<connect gate="-1" pin="A2" pad="2"/>
<connect gate="-1" pin="K1K2" pad="6"/>
<connect gate="-2" pin="A1" pad="4"/>
<connect gate="-2" pin="A2" pad="5"/>
<connect gate="-2" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS40XY" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SDD_AKAK"/>
<gate name="-2" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="A1" pad="1"/>
<connect gate="-1" pin="K1A2" pad="6"/>
<connect gate="-1" pin="K2" pad="2"/>
<connect gate="-2" pin="A1" pad="4"/>
<connect gate="-2" pin="K1A2" pad="3"/>
<connect gate="-2" pin="K2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS76SB70" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS79SB70" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70H" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70W" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70L" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diode&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70-04" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70-05" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70-06" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70-07" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT143(B)">
<connects>
<connect gate="-1" pin="A" pad="4"/>
<connect gate="-1" pin="K" pad="1"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="4"/>
<connect gate="-2" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOT363">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="4"/>
<connect gate="-2" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70VV" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt;General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
<gate name="-3" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS70XY" prefix="D">
<description>&lt;H2&gt;General-purpose Schottky diodes&lt;/H2&gt; General-purpose Schottky diodes in small Surface-Mounted Device (SMD) plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SDD_AKAK"/>
<gate name="-2" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="A1" pad="1"/>
<connect gate="-1" pin="K1A2" pad="6"/>
<connect gate="-1" pin="K2" pad="2"/>
<connect gate="-2" pin="A1" pad="4"/>
<connect gate="-2" pin="K1A2" pad="3"/>
<connect gate="-2" pin="K2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS29" prefix="D">
<description>&lt;H2&gt;General purpose controlled avalanche diode&lt;/H2&gt; General purpose switching diodes fabricated in planar 
technology, and encapsulated in small rectangular plastic 
SMD SOT23 packages. The BAS29 consists of a single 
diode. The BAS31 has two diodes in series. The BAS35 
has two diodes with a common anode. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS31" prefix="D">
<description>&lt;H2&gt;General purpose controlled avalanche diode (double)&lt;/H2&gt; General purpose switching diodes fabricated in planar 
technology, and encapsulated in small rectangular plastic 
SMD SOT23 packages. The BAS29 consists of a single 
diode. The BAS31 has two diodes in series. The BAS35 
has two diodes with a common anode. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS35" prefix="D">
<description>&lt;H2&gt;General purpose controlled avalanche diode (double)&lt;/H2&gt; General purpose switching diodes fabricated in planar 
technology, and encapsulated in small rectangular plastic 
SMD SOT23 packages. The BAS29 consists of a single 
diode. The BAS31 has two diodes in series. The BAS35 
has two diodes with a common anode. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_KAAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS19" prefix="D">
<description>&lt;H2&gt;General purpose diode&lt;/H2&gt;The BAS19, BAS20 and BAS21 are general purpose 
diodes fabricated in planar technology, and encapsulated 
in a small SOT23 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS21" prefix="D">
<description>&lt;H2&gt;General purpose diode&lt;/H2&gt;The BAS19, BAS20 and BAS21 are general purpose 
diodes fabricated in planar technology, and encapsulated 
in a small SOT23 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9340 632 68115"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS20" prefix="D">
<description>&lt;H2&gt;General purpose diode&lt;/H2&gt;The BAS19, BAS20 and BAS21 are general purpose 
diodes fabricated in planar technology, and encapsulated 
in a small SOT23 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS321" prefix="D">
<description>&lt;H2&gt;General purpose diode&lt;/H2&gt;The BAS321 is a general purpose diode fabricated in 
planar technology and encapsulated in a plastic SOD323 
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS116H" prefix="D">
<description>&lt;H2&gt;Low leakage switching diode&lt;/H2&gt;Low leakage switching diode, encapsulated in a SOD123F small and flat lead 
Surface-Mounted Device (SMD) plastic package. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS521" prefix="D">
<description>&lt;H2&gt;Single high-voltage switching diode&lt;/H2&gt;Single high-voltage switching diode, fabricated in planar technology, and encapsulated in 
a SOD523 (SC-79) ultra small Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS56" prefix="D">
<description>&lt;H2&gt;High-speed double diode&lt;/H2&gt;Two high-speed switching diodes fabricated in planar technology, and encapsulated in a 
small SOT143B Surface-Mounted Device (SMD) plastic package. The diodes are not 
connected.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE"/>
<gate name="-2" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT143(B)">
<connects>
<connect gate="-1" pin="A" pad="4"/>
<connect gate="-1" pin="K" pad="1"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS17" prefix="D">
<description>&lt;H2&gt;Low-voltage stabistor&lt;/H2&gt;Low-voltage stabilization diode in a small SOT23 plastic 
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS45A" prefix="D">
<description>&lt;H2&gt;Low-leakage diode&lt;/H2&gt;Epitaxial medium-speed switching diode with a low leakage current, encapsulated in a 
small hermetically sealed glass SOD80C Surface-Mounted Device (SMD) package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD68">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="K" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="SOD80C">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS21VD" prefix="D">
<description>&lt;H2&gt;High-voltage switching diodes&lt;/H2&gt;Triple high-voltage switching diodes, encapsulated in a SOT457 (SC-74) small 
Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE"/>
<gate name="-2" symbol="DIODE"/>
<gate name="-3" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT457">
<connects>
<connect gate="-1" pin="A" pad="6"/>
<connect gate="-1" pin="K" pad="1"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="K" pad="2"/>
<connect gate="-3" pin="A" pad="4"/>
<connect gate="-3" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS85">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode with an integrated guard ring for stress protection, 
encapsulated in a small hermetically sealed glass SOD80C Surface-Mounted 
Device SMD package with tin-plated metal discs at each end. It is suitable for 
?automatic placement? and as such it can withstand immersion soldering.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD80C">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS716" prefix="D">
<description>&lt;H2&gt;Low-leakage diode&lt;/H2&gt; Epitaxial medium-speed switching diode with a low 
leakage current in an ultra small SOD523 (SC-79) SMD 
plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS416" prefix="D">
<description>&lt;H2&gt;Low-leakage diode&lt;/H2&gt;Epitaxial, medium-speed switching diode with a low 
leakage current encapsulated in a small SOD323 SMD 
plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS32L" prefix="D">
<description>&lt;H2&gt;High-speed switching diode&lt;/H2&gt; Single high-speed switching diode, fabricated in planar technology, and encapsulated in a 
small hermetically sealed glass SOD80C Surface-Mounted Device (SMD) package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD80C">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS28" prefix="D">
<description>&lt;H2&gt;High-speed double diode&lt;/H2&gt; Two high-speed switching diodes fabricated in planar technology, and encapsulated in a 
small SOT143B Surface-Mounted Device (SMD) plastic package. The diodes are not 
connected.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE"/>
<gate name="-2" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT143(B)">
<connects>
<connect gate="-1" pin="A" pad="4"/>
<connect gate="-1" pin="K" pad="1"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS21J" prefix="D">
<description>&lt;H2&gt;Single high-speed switching diode&lt;/H2&gt;Single high-speed switching diode, encapsulated in a SOD323F (SC-90) very small and
?at lead Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS21AVD" prefix="D">
<description>&lt;H2&gt;High-voltage switching diodes&lt;/H2&gt;Triple high-voltage switching diodes, encapsulated in a SOT457 (SC-74) small 
Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE"/>
<gate name="-2" symbol="DIODE"/>
<gate name="-3" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT457">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS16" prefix="D">
<description>&lt;H2&gt;High-speed switching diode&lt;/H2&gt;High-speed switching diode, encapsulated in small Surface-Mounted Device (SMD)
plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SOT416">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LD" package="SOD882D">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS16V" prefix="D">
<description>&lt;H2&gt;High-speed switching diodes&lt;/H2&gt;High-speed switching diodes, encapsulated in small Surface-Mounted Device (SMD)
plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE"/>
<gate name="-2" symbol="DIODE"/>
<gate name="-3" symbol="DIODE"/>
</gates>
<devices>
<device name="Y" package="SOT363">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS316" prefix="D">
<description>&lt;H2&gt;High-speed switching diode&lt;/H2&gt;High-speed switching diode, encapsulated in small Surface-Mounted Device (SMD)
plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS516" prefix="D">
<description>&lt;H2&gt;High-speed switching diode&lt;/H2&gt;High-speed switching diode, encapsulated in small Surface-Mounted Device (SMD)
plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS116T" prefix="D">
<description>&lt;H2&gt;Single low leakage current switching diode&lt;/H2&gt;Single low leakage current switching diode, encapsulated in an ultra small 
SOT416 (SC-75) Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT416">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS101" prefix="D">
<description>&lt;H2&gt;High-voltage switching diode&lt;/H2&gt;High-voltage switching diode, encapsulated in a SOT23 small Surface-Mounted 
Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS101S" prefix="D">
<description>&lt;H2&gt;High-voltage switching diodes&lt;/H2&gt;High-voltage switching diodes, encapsulated in a SOT23 small Surface-Mounted 
Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS86">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode with an integrated guard ring against static discharges. This 
surface-mounted device is encapsulated in a small hermetically sealed SOD80C glass 
Surface-Mounted Device (SMD) package with tin-plated metal discs at each end. 
It is suitable for ?automatic placement? and as such it can withstand immersion soldering.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD80C">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA277" prefix="D">
<description>&lt;H2&gt;Band-switching diode&lt;/H2&gt;Planar high performance band-switching diode in a small
plastic SOD523 (SC-79) SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA591" prefix="D">
<description>&lt;H2&gt;Band-switching diode&lt;/H2&gt;The BA591 is a planar, high performance band-switching 
diode in the very small SOD323 (SC-76) SMD plastic 
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA891" prefix="D">
<description>&lt;H2&gt;Band-switching diode&lt;/H2&gt;The BA891 is a planar high performance band-switching
diode in the ultra small SOD523 SMD plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT18" prefix="D">
<description>&lt;H2&gt;Silicon planar diode&lt;/H2&gt;Planar high performance band-switching diode in a small rectangular SOT23 SMD plastic
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAP1321" prefix="D">
<description>&lt;H2&gt;Silicon PIN diode
&lt;/H2&gt; Planar PIN diode&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="-02" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-03" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAP1321-04" prefix="D">
<description>&lt;H2&gt;Silicon PIN diode
&lt;/H2&gt; Planar PIN diode&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAP50-05" prefix="D">
<description>&lt;H2&gt;General purpose PIN diode&lt;/H2&gt;Two planar PIN diodes in common cathode configuration.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAP50-04" prefix="D">
<description>&lt;H2&gt;General purpose PIN diode&lt;/H2&gt;Two planar PIN diodes in series configuration.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAP50" prefix="D">
<description>&lt;H2&gt;General purpose PIN diode&lt;/H2&gt;General purpose PIN diode&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="-03" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-02" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LX" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB10" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode 
encapsulated in a SOT323 very small 
plastic SMD package. Single diodes 
and double diodes with different 
pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB14" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diode 
encapsulated in a SOT323 very small 
plastic SMD package. Single diodes 
and double diodes with different 
pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB15" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diode 
encapsulated in a SOT323 very small 
plastic SMD package. Single diodes 
and double diodes with different 
pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="K1K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB16" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diode 
encapsulated in a SOT323 very small 
plastic SMD package. Single diodes 
and double diodes with different 
pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS76SB10" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode encapsulated in a SOD323 
very small plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT721" prefix="D">
<description>&lt;H2&gt;Schottky barrier diodes in small packages&lt;/H2&gt;Planar Schottky barrier diodes with an integrated guard ring for stress protection.
Encapsulated in small Surface-Mounted Device (SMD) plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS76SB21" prefix="D">
<description>&lt;H2&gt;Schottky barrier diodes in small packages&lt;/H2&gt;Planar Schottky barrier diodes with an integrated guard ring for stress protection.
Encapsulated in small Surface-Mounted Device (SMD) plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT721A" prefix="D">
<description>&lt;H2&gt;Schottky barrier diodes in small packages&lt;/H2&gt;Planar Schottky barrier diodes with an integrated guard ring for stress protection.
Encapsulated in small Surface-Mounted Device (SMD) plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT721C" prefix="D">
<description>&lt;H2&gt;Schottky barrier diodes in small packages&lt;/H2&gt;Planar Schottky barrier diodes with an integrated guard ring for stress protection.
Encapsulated in small Surface-Mounted Device (SMD) plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT721S" prefix="D">
<description>&lt;H2&gt;Schottky barrier diodes in small packages&lt;/H2&gt;Planar Schottky barrier diodes with an integrated guard ring for stress protection.
Encapsulated in small Surface-Mounted Device (SMD) plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS79SB10" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode encapsulated in a SC-79 ultra small plastic SMD 
package. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS79SB30" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode encapsulated in a SC-79 ultra small plastic SMD 
package. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS79SB31" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode encapsulated in a SC-79 ultra small plastic SMD 
package. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode encapsulated in small plastic SMD packages. Single diodes and double 
diodes with different pinning are available&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SOT416">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54A" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT23 
small plastic SMD package. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54C" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT23 
small plastic SMD package. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SOT883(B)">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54S" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT23 
small plastic SMD package. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54CV" prefix="D">
<description>&lt;H2&gt;Two Schottky barrier double diodes&lt;/H2&gt; Two planar Schottky barrier double diodes with common cathodes and an integrated 
guard ring for stress protection encapsulated in a SOT666 ultra small and flat lead 
Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SDD_AKKA"/>
<gate name="-2" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="A1" pad="1"/>
<connect gate="-1" pin="A2" pad="2"/>
<connect gate="-1" pin="K1K2" pad="6"/>
<connect gate="-2" pin="A1" pad="5"/>
<connect gate="-2" pin="A2" pad="4"/>
<connect gate="-2" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54VV" prefix="D">
<description>&lt;H2&gt;Schottky barrier triple diode&lt;/H2&gt;Planar Schottky barrier triple diode with an integrated guard ring for stress protection. 
Three electrically isolated Schottky barrier diodes, encapsulated in a SOT666 ultra small 
SMD plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
<gate name="-3" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54XY" prefix="D">
<description>&lt;H2&gt;Schottky barrier quadruple diode in very small SOT363 
package&lt;/H2&gt; Schottky barrier quadruple diode with an integrated guard ring for stress protection. Two 
electrically isolated dual Schottky barrier diodes series, encapsulated in a SOT363 very 
small SMD plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SDD_AKAK"/>
<gate name="-2" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="A1" pad="1"/>
<connect gate="-1" pin="K1A2" pad="6"/>
<connect gate="-1" pin="K2" pad="2"/>
<connect gate="-2" pin="A1" pad="4"/>
<connect gate="-2" pin="K1A2" pad="3"/>
<connect gate="-2" pin="K2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT74" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diode&lt;/H2&gt;Planar Schottky barrier double diode with an integrated guard ring for stress protection. 
Two electrically isolated Schottky barrier diodes, encapsulated in a small SOT143B 
Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT143(B)">
<connects>
<connect gate="-1" pin="A" pad="4"/>
<connect gate="-1" pin="K" pad="1"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOT363">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="4"/>
<connect gate="-2" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="4"/>
<connect gate="-2" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT754" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diodes 
encapsulated in a SOT23 small 
plastic SMD package. Low forward 
voltage selection of the BAT54 series. 
Single diodes and double diodes with 
different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT754A" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT23 small plastic SMD package. Low forward voltage selection of the BAT54 series. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT754C" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT23 small plastic SMD package. Low forward voltage selection of the BAT54 series. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT754S" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT23 small plastic SMD package. Low forward voltage selection of the BAT54 series. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT754L" prefix="D">
<description>&lt;H2&gt;Schottky barrier triple diode&lt;/H2&gt;Three internal (galvanic) isolated silicon epitaxial Schottky 
barrier diodes in a SOT363 small SMD plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
<gate name="-3" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT85">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt; Planar Schottky barrier diode with an integrated protection ring against static 
discharges, encapsulated in a hermetically-sealed subminiature SOD68 
(DO-34) package. The diode is suitable for mounting on a 2 E (5.08 mm) pitch.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD68">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="K" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT854A" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT323 very small SMD plastic package. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT854C" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT323 very small SMD plastic package. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT854S" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT323 very small SMD plastic package. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT854" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt;Planar Schottky barrier diodes encapsulated in a SOT323 very small SMD plastic package. Single diodes and double diodes with different pinning are available.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT86">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt; Planar Schottky barrier diode with an integrated protection ring against static 
discharges, encapsulated in a hermetically-sealed subminiature SOD68 
(DO-34) package. The diode is suitable for mounting on a 2 E (5.08 mm) pitch.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD68">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="K" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RB520CS30L">
<description>&lt;H2&gt;100 mA low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a SOD882 leadless ultra small 
Surface-Mounted Device (SMD) plastic package. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RB520S30">
<description>&lt;H2&gt;200 mA low Vf MEGA Schottky barrier rectifier&lt;/H2&gt;Planar Maximum Ef?ciency General Application (MEGA) Schottky barrier recti?er with an
integrated guard ring for stress protection, encapsulated in a SOD523 (SC-79) ultra small
and ?at lead Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RB521CS30L">
<description>&lt;H2&gt;100 mA low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a SOD882 leadless ultra small 
Surface-Mounted Device (SMD) plastic package. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RB521S30">
<description>&lt;H2&gt;200 mA low Vf MEGA Schottky barrier rectifier&lt;/H2&gt;Planar Maximum Ef?ciency General Application (MEGA) Schottky barrier recti?er with an
integrated guard ring for stress protection, encapsulated in a SOD523 (SC-79) ultra small
and ?at lead Surface-Mounted Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RB751">
<description>&lt;H2&gt;Schottky barrier single diode&lt;/H2&gt;Planar Schottky barrier single diodes with an integrated guard ring for stress protection,
encapsulated in small Surface-Mounted Device (SMD) plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="CS40" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S40" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V40" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB20">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt; Planar Schottky barrier diode with an integrated guard ring for stress protection 
in a SOT323 (SC-70) small SMD plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS74SB23" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode encapsulated in an SC-74
(SOT457) small plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT457">
<connects>
<connect gate="G$1" pin="A" pad="1 3 4 6"/>
<connect gate="G$1" pin="K" pad="2 5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT120A" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diodes&lt;/H2&gt;Planar Schottky barrier double diodes encapsulated in a 
SOT223 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="A1A2" pad="4"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT120C" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diodes&lt;/H2&gt;Planar Schottky barrier double diodes encapsulated in a 
SOT223 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="K1K2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT120S" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diodes&lt;/H2&gt;Planar Schottky barrier double diodes encapsulated in a 
SOT223 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="4"/>
<connect gate="G$1" pin="K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT160A" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diodes&lt;/H2&gt;Planar Schottky barrier double diodes encapsulated in a 
SOT223 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="A1A2" pad="4"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT160C" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diodes&lt;/H2&gt;Planar Schottky barrier double diodes encapsulated in a 
SOT223 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="K1K2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT160S" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diodes&lt;/H2&gt;Planar Schottky barrier double diodes encapsulated in a 
SOT223 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="4"/>
<connect gate="G$1" pin="K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT46W">
<description>&lt;H2&gt;Single Schottky barrier diode&lt;/H2&gt;Single planar Schottky barrier diode with an integrated guard ring for stress protection, 
encapsulated in a Surface-Mounted 
Device (SMD) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="J" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT720" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode with an integrated guard ring for stress protection in a small SOT23 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT760" prefix="D">
<description>&lt;H2&gt;Medium power Schottky barrier single diode&lt;/H2&gt;Planar medium power Schottky barrier single diode with an integrated guard ring for
stress protection, encapsulated in a SOD323 (SC-76) very small Surface-Mounted
Device SMD plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT960" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt; Planar Schottky barrier diode with an integrated guard ring for stress protection in a SOT666 ultra small SMD plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4010" prefix="D">
<description>&lt;H2&gt;40 V, 1 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection.
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EPK" package="SOD1608">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BEA" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="C"/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="C"/>
</technologies>
</device>
<device name="EP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ER" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ET" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BEV" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4015" prefix="D">
<description>&lt;H2&gt;40 V, 1.5 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a leadless ultra small 
SOD1608 (DFN1608D-2) Surface-Mounted Device (SMD) plastic package with visible 
and solderable side pads
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EPK" package="SOD1608">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4020E" prefix="D">
<description>&lt;H2&gt;40 V, 2 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection.
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="PK" package="SOD1608">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="T"/>
</technologies>
</device>
<device name="R" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="T"/>
</technologies>
</device>
<device name="PA" package="SOT1061">
<connects>
<connect gate="G$1" pin="A" pad="1 2"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG1020E" prefix="D">
<description>&lt;H2&gt;10 V, 2 A ultra low VF MEGA Schottky barrier rectifiers&lt;/H2&gt;Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifiers with an 
integrated guard ring for stress protection, encapsulated in small and flat lead plastic SMD 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="A" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG1030E" prefix="D">
<description>&lt;H2&gt;10 V, 3 A ultra low VF MEGA Schottky barrier rectifiers&lt;/H2&gt;Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifiers with an 
integrated guard ring for stress protection, encapsulated in small and flat lead plastic SMD 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="A" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4005" prefix="D">
<description>&lt;H2&gt;40 V 0.5 A Very low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) 
Schottky barrier rectifier with an integrated guard ring for 
stress protection, encapsulated in a SOD323 (SC-76) very 
small SMD plastic packag&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="AEA" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EPK" package="SOD1608">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ET" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AEV" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG2010" prefix="D">
<description>&lt;H2&gt;20V, 1A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EPK" package="SOD1608">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AEB" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BELD" package="SOD882D">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
<device name="ET" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
<device name="ER" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="B"/>
</technologies>
</device>
<device name="AEK" package="SOT346">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="REMARK" value="OBSOLETE"/>
</technology>
</technologies>
</device>
<device name="EA" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="B"/>
</technologies>
</device>
<device name="EV" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
<technology name="B"/>
</technologies>
</device>
<device name="EPA" package="SOT1061">
<connects>
<connect gate="G$1" pin="A" pad="1 2"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG2015" prefix="D">
<description>&lt;H2&gt;20V, 1.5A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EPK" package="SOD1608">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EA" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EV" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG2020" prefix="D">
<description>&lt;H2&gt;20V, 2A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="REMARK" value=""/>
</technology>
<technology name="A">
<attribute name="REMARK" value="OBSOLETE"/>
</technology>
</technologies>
</device>
<device name="AEA" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EPK" package="SOD1608">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EPA" package="SOT1061">
<connects>
<connect gate="G$1" pin="A" pad="1 2"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG2020CPA" prefix="D">
<description>&lt;H2&gt;20V 2A low VF dual MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier in 
common cathode configuration with an integrated guard ring for stress protection, 
encapsulated in a SOT1061 leadless small Surface-Mounted Device (SMD) plastic 
package with medium power capability. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT1061">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG3005" prefix="D">
<description>&lt;H2&gt;30 V, 0.5 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="AEA" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EL" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EB" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ELD" package="SOD882D">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ET" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AEV" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG3005CT" prefix="D">
<description>&lt;H2&gt;30V 500 mA low VF dual MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier in 
common cathode configuration with an integrated guard ring for stress protection, 
encapsulated in a SOT23 (TO-236AB) small Surface-Mounted Device (SMD) plastic 
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG3010" prefix="D">
<description>&lt;H2&gt;30 V, 1A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EB" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="C"/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="C"/>
</technologies>
</device>
<device name="ET" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="B"/>
</technologies>
</device>
<device name="BEA" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BER" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BEV" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG3015" prefix="D">
<description>&lt;H2&gt;20V, 1.5A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EV" package="SOT666">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG3020" prefix="D">
<description>&lt;H2&gt;30 V, 2A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EB" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="C"/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
</technologies>
</device>
<device name="ER" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="B"/>
</technologies>
</device>
<device name="EPA" package="SOT1061">
<connects>
<connect gate="G$1" pin="A" pad="1 2"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG3020CPA" prefix="D">
<description>&lt;H2&gt;30V 2A low VF dual MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier in 
common cathode configuration with an integrated guard ring for stress protection, 
encapsulated in a SOT1061 leadless small Surface-Mounted Device (SMD) plastic 
package with medium power capability. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT1061">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG3030" prefix="D">
<description>&lt;H2&gt;30V, 3A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG3050" prefix="D">
<description>&lt;H2&gt;30V, 5A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a Surface-Mounted Device (SMD) 
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4002" prefix="D">
<description>&lt;H2&gt;40 V 0.2 A Very low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) 
Schottky barrier rectifier with an integrated guard ring for 
stress protection, encapsulated in a SOD323 (SC-76) very 
small SMD plastic packag&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EL" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ELD" package="SOD882D">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EB" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4005CT" prefix="D">
<description>&lt;H2&gt;40 V, 0.5 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a leadless ultra small 
SOD1608 (DFN1608D-2) Surface-Mounted Device (SMD) plastic package with visible 
and solderable side pads
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4010CPA" prefix="D">
<description>&lt;H2&gt;40 V, 1 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a leadless ultra small 
SOD1608 (DFN1608D-2) Surface-Mounted Device (SMD) plastic package with visible 
and solderable side pads
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT1061">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4030E" prefix="D">
<description>&lt;H2&gt;40 V, 3 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection.
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="P" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="T"/>
</technologies>
</device>
<device name="R" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="T"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG4050E" prefix="D">
<description>&lt;H2&gt;40 V, 5 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection.
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="P" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="T"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG6002" prefix="D">
<description>&lt;H2&gt;60V 0.2A very low VF MEGA Schottky barrier recti?ers&lt;/H2&gt;Planar Maximum Ef?ciency General Application (MEGA) Schottky barrier recti?ers with an
integrated guard ring for stress protection, encapsulated in ultra small and ?at lead
Surface-Mounted Device (SMD) plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EB" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG6002TV" prefix="D">
<description>&lt;H2&gt;60V 0.2A very low VF MEGA Schottky barrier recti?ers&lt;/H2&gt;Planar Maximum Ef?ciency General Application (MEGA) Schottky barrier recti?ers with an
integrated guard ring for stress protection, encapsulated in ultra small and ?at lead
Surface-Mounted Device (SMD) plastic packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="4"/>
<connect gate="-2" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG6010" prefix="D">
<description>&lt;H2&gt;60 V, 1 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a leadless ultra small 
SOD1608 (DFN1608D-2) Surface-Mounted Device (SMD) plastic package with visible 
and solderable side pads
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="CEH" package="SOD123F">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CEJ" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ER" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AED" package="SOT457">
<connects>
<connect gate="G$1" pin="A" pad="3 4"/>
<connect gate="G$1" pin="K" pad="1 2 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG6010CPA" prefix="D">
<description>&lt;H2&gt;60 V, 1 A low VF MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier with an 
integrated guard ring for stress protection, encapsulated in a leadless ultra small 
SOD1608 (DFN1608D-2) Surface-Mounted Device (SMD) plastic package with visible 
and solderable side pads
 &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT1061">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG6020" prefix="D">
<description>&lt;H2&gt;60V 2A low VF dual MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier in 
common cathode configuration with an integrated guard ring for stress protection, 
encapsulated in a SOT1061 leadless small Surface-Mounted Device (SMD) plastic 
package with medium power capability. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ER" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EPA" package="SOT1061">
<connects>
<connect gate="G$1" pin="A" pad="1 2"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG6030" prefix="D">
<description>&lt;H2&gt;60V 3A low VF dual MEGA Schottky barrier rectifier&lt;/H2&gt; Planar Maximum Efficiency General Application (MEGA) Schottky barrier rectifier in 
common cathode configuration with an integrated guard ring for stress protection, 
encapsulated in a SOT1061 leadless small Surface-Mounted Device (SMD) plastic 
package with medium power capability. &lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="EP" package="SOD128">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NXPS20H110C" prefix="D">
<description>&lt;H2&gt;Dual power Schottky diode&lt;/H2&gt;Dual common cathode power Schottky diode designed for high frequency switched mode 
power supplies in a SOT78 (TO-220AB) plastic package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT78">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="K1K2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ISOLATED" value="NO"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS10SB82" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;An epitaxial Schottky barrier diode encapsulated in a 
SOD882 leadless ultra small plastic package.
ESD sensitive device, observe handling precautions.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD882(T)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS66SB82">
<description>&lt;H2&gt;15 V, 30 mA low Cd Schottky barrier diode&lt;/H2&gt; Epitaxial low capacitance Schottky barrier diodes encapsulated in very small SMD plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
<gate name="-3" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS88SB82">
<description>&lt;H2&gt;15 V, 30 mA low Cd Schottky barrier diode&lt;/H2&gt; Epitaxial low capacitance Schottky barrier diodes encapsulated in very small SMD plastic 
packages.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
<gate name="-3" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB82" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt; Planar Schottky barrier diodes 
encapsulated in a SOT323 (SC-70) 
very small plastic SMD package. 
Single diodes and double diodes with 
different pinning are available. ESD 
sensitive device, observe handling 
precautions.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB84" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt; Planar Schottky barrier diodes 
encapsulated in a SOT323 (SC-70) 
very small plastic SMD package. 
Single diodes and double diodes with 
different pinning are available. ESD 
sensitive device, observe handling 
precautions.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB85" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt; Planar Schottky barrier diodes 
encapsulated in a SOT323 (SC-70) 
very small plastic SMD package. 
Single diodes and double diodes with 
different pinning are available. ESD 
sensitive device, observe handling 
precautions.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K1K2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS70SB86" prefix="D">
<description>&lt;H2&gt;Schottky barrier (double) diodes&lt;/H2&gt; Planar Schottky barrier diodes 
encapsulated in a SOT323 (SC-70) 
very small plastic SMD package. 
Single diodes and double diodes with 
different pinning are available. ESD 
sensitive device, observe handling 
precautions.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT323">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS76SB17" prefix="D">
<description>&lt;H2&gt;4 V, 30 mA low Cd Schottky barrier diode&lt;/H2&gt;Planar low capacitance Schottky barrier diode encapsulated in a very small SMD plastic
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS79SB17" prefix="D">
<description>&lt;H2&gt;4 V, 30 mA low Cd Schottky barrier diode&lt;/H2&gt;Planar low capacitance Schottky barrier diode encapsulated in a very small SMD plastic
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1PS66SB17" prefix="D">
<description>&lt;H2&gt;4 V, 30 mA low Cd Schottky barrier diode&lt;/H2&gt;Planar low capacitance Schottky barrier diode encapsulated in a very small SMD plastic
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_SCHOTTKY"/>
<gate name="-2" symbol="DIODE_SCHOTTKY"/>
<gate name="-3" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="K" pad="6"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT17" prefix="D">
<description>&lt;H2&gt;Schottky barrier diode&lt;/H2&gt;Planar Schottky barrier diode in a small SOT23 plastic SMD package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMBD353" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diode&lt;/H2&gt; Planar Schottky barrier double diode in a SOT23 small plastic SMD 
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMBD354" prefix="D">
<description>&lt;H2&gt;Schottky barrier double diode&lt;/H2&gt; Planar Schottky barrier double diode in a SOT23 small plastic SMD 
package.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BCX18" prefix="T">
<description>&lt;H2&gt;PNP general purpose transistors&lt;/H2&gt; PNP transistor in a SOT23 plastic package. 
NPN complement: BCX19.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB131" prefix="D">
<description>&lt;H2&gt;VHF variable capacitance diode&lt;/H2&gt;The BB131 is a variable capacitance diode, fabricated in 
planar technology, and encapsulated in the SOD323 (SC-76) very small plastic SMD package&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_VAR"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB135" prefix="D">
<description>&lt;H2&gt;UHF variable capacitance diode&lt;/H2&gt;The BB135 is a variable capacitance diode, fabricated in planar technology, and encapsulated in the SOD323 very small plastic SMD package.The matched type, BB134 has the same specification.e&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_VAR"/>
</gates>
<devices>
<device name="" package="SOD323(F)">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMDPB58UPE" prefix="T">
<description>&lt;H2&gt;20 V dual P-channel Trench MOSFET&lt;/H2&gt; Dual small-signal P-channel enhancement mode Field-Effect Transistor (FET) in a 
leadless medium power DFN2020-6 (SOT1118) Surface-Mounted Device (SMD) plastic 
package using Trench MOSFET technology.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="P-MOSFER-TR"/>
<gate name="-2" symbol="P-MOSFER-TR"/>
</gates>
<devices>
<device name="" package="SOT1118">
<connects>
<connect gate="-1" pin="D" pad="6 7"/>
<connect gate="-1" pin="G" pad="2"/>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="D" pad="3"/>
<connect gate="-2" pin="G" pad="5"/>
<connect gate="-2" pin="S" pad="4 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUK761R3-30E">
<description>&lt;H2&gt;N-channel TrenchMOS standard level FET&lt;/H2&gt;Standard level N-channel MOSFET in a SOT404 package using TrenchMOS technology. 
This product has been designed and qualified to AEC Q101 standard for use in high 
performance automotive applications.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT404">
<connects>
<connect gate="G$1" pin="D" pad="MB"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NPC1100B" prefix="U">
<description>&lt;H2&gt;Low Cost Narrow Band Communication Controller&lt;/H2&gt; The ASIC DLC-3
is a low cost narrow band communication controller MCM (Multi Carrier Modulation) and power line
chip. The integrated ARMÒ CortexTM CPU, memory and common interfaces makes it possible to build
different systems with a minimum of external components. For communication with DLC-3 the most
popular interfaces like Ethernet MII, SPI, several freely configurable serial interfaces and general IO
ports for CPU and DSC are included.
The ASIC includes all components for a power-line communication while Analog Front End and Power
Amplifier are already integrated. With its On-Chip Power-Factor-Correction, Ballast Control and 4 PWM
outputs the LCI is a optimal solution for lighting control units. The freely configurable serial interfaces
makes it easy to build electronic power meters for smart-metering applications.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DLC3"/>
</gates>
<devices>
<device name="" package="SOT486-1">
<connects>
<connect gate="G$1" pin="!DISW!" pad="100"/>
<connect gate="G$1" pin="!NMI!" pad="99"/>
<connect gate="G$1" pin="!RESET!" pad="132"/>
<connect gate="G$1" pin="!SPI_CS!" pad="101"/>
<connect gate="G$1" pin="!TRST!" pad="24"/>
<connect gate="G$1" pin="!TXAMP_EN!" pad="133"/>
<connect gate="G$1" pin="A0/SIC2" pad="26"/>
<connect gate="G$1" pin="A1/SIC3" pad="27"/>
<connect gate="G$1" pin="A2/SIC4" pad="29"/>
<connect gate="G$1" pin="BC_IGN" pad="110"/>
<connect gate="G$1" pin="BC_I_N" pad="79"/>
<connect gate="G$1" pin="BC_I_P" pad="78"/>
<connect gate="G$1" pin="BC_L" pad="130"/>
<connect gate="G$1" pin="BC_N" pad="131"/>
<connect gate="G$1" pin="BC_P" pad="111"/>
<connect gate="G$1" pin="BC_U_N" pad="77"/>
<connect gate="G$1" pin="BC_U_P" pad="76"/>
<connect gate="G$1" pin="BOOT" pad="115"/>
<connect gate="G$1" pin="GDY0" pad="106"/>
<connect gate="G$1" pin="GDY1" pad="107"/>
<connect gate="G$1" pin="GDY2" pad="112"/>
<connect gate="G$1" pin="GDY3" pad="113"/>
<connect gate="G$1" pin="GDY4" pad="121"/>
<connect gate="G$1" pin="GND@1" pad="109"/>
<connect gate="G$1" pin="GND@2" pad="72"/>
<connect gate="G$1" pin="GND@3" pad="36"/>
<connect gate="G$1" pin="GND@4" pad="1"/>
<connect gate="G$1" pin="GND_PLL" pad="12"/>
<connect gate="G$1" pin="OSC32K1" pad="125"/>
<connect gate="G$1" pin="OSC32K2" pad="126"/>
<connect gate="G$1" pin="P0" pad="34"/>
<connect gate="G$1" pin="P1" pad="37"/>
<connect gate="G$1" pin="P10" pad="33"/>
<connect gate="G$1" pin="P11" pad="48"/>
<connect gate="G$1" pin="P14" pad="50"/>
<connect gate="G$1" pin="P15" pad="51"/>
<connect gate="G$1" pin="P16" pad="52"/>
<connect gate="G$1" pin="P17" pad="53"/>
<connect gate="G$1" pin="P18" pad="90"/>
<connect gate="G$1" pin="P19" pad="91"/>
<connect gate="G$1" pin="P2" pad="38"/>
<connect gate="G$1" pin="P20" pad="92"/>
<connect gate="G$1" pin="P21" pad="93"/>
<connect gate="G$1" pin="P22" pad="94"/>
<connect gate="G$1" pin="P23" pad="95"/>
<connect gate="G$1" pin="P24" pad="96"/>
<connect gate="G$1" pin="P26" pad="98"/>
<connect gate="G$1" pin="P27" pad="116"/>
<connect gate="G$1" pin="P28" pad="117"/>
<connect gate="G$1" pin="P29" pad="30"/>
<connect gate="G$1" pin="P3" pad="39"/>
<connect gate="G$1" pin="P30" pad="31"/>
<connect gate="G$1" pin="P31" pad="32"/>
<connect gate="G$1" pin="P4" pad="42"/>
<connect gate="G$1" pin="P5" pad="43"/>
<connect gate="G$1" pin="P6" pad="44"/>
<connect gate="G$1" pin="P7" pad="45"/>
<connect gate="G$1" pin="P8" pad="46"/>
<connect gate="G$1" pin="P9" pad="47"/>
<connect gate="G$1" pin="PFC_BUF_N" pad="74"/>
<connect gate="G$1" pin="PFC_BUF_P" pad="73"/>
<connect gate="G$1" pin="PFC_I0_N" pad="65"/>
<connect gate="G$1" pin="PFC_I0_P" pad="64"/>
<connect gate="G$1" pin="PFC_I1_N" pad="67"/>
<connect gate="G$1" pin="PFC_I1_P" pad="66"/>
<connect gate="G$1" pin="PFC_LINEU_N" pad="63"/>
<connect gate="G$1" pin="PFC_LINEU_P" pad="62"/>
<connect gate="G$1" pin="PFC_N" pad="128"/>
<connect gate="G$1" pin="PFC_P" pad="129"/>
<connect gate="G$1" pin="REFN" pad="7"/>
<connect gate="G$1" pin="REFP" pad="6"/>
<connect gate="G$1" pin="RESAN" pad="69"/>
<connect gate="G$1" pin="RESAP" pad="68"/>
<connect gate="G$1" pin="RESBN" pad="82"/>
<connect gate="G$1" pin="RESBP" pad="81"/>
<connect gate="G$1" pin="RTC_BUF" pad="123"/>
<connect gate="G$1" pin="RXN" pad="8"/>
<connect gate="G$1" pin="RXP" pad="5"/>
<connect gate="G$1" pin="SIC0" pad="86"/>
<connect gate="G$1" pin="SIC1" pad="87"/>
<connect gate="G$1" pin="SIC12" pad="56"/>
<connect gate="G$1" pin="SIC13" pad="57"/>
<connect gate="G$1" pin="SIC14" pad="59"/>
<connect gate="G$1" pin="SIC15" pad="60"/>
<connect gate="G$1" pin="SPI_CLK" pad="104"/>
<connect gate="G$1" pin="SPI_MISO" pad="102"/>
<connect gate="G$1" pin="SPI_MOSI" pad="103"/>
<connect gate="G$1" pin="SYS_XTAL1" pad="13"/>
<connect gate="G$1" pin="SYS_XTAL2" pad="14"/>
<connect gate="G$1" pin="TCK" pad="20"/>
<connect gate="G$1" pin="TDI" pad="23"/>
<connect gate="G$1" pin="TDO" pad="21"/>
<connect gate="G$1" pin="TMS" pad="25"/>
<connect gate="G$1" pin="TXAMP_OUT_N" pad="134"/>
<connect gate="G$1" pin="TXAMP_OUT_P" pad="135"/>
<connect gate="G$1" pin="TXAMP_SCL" pad="137"/>
<connect gate="G$1" pin="TXAMP_SDA" pad="136"/>
<connect gate="G$1" pin="TXAMP_TEMP" pad="140"/>
<connect gate="G$1" pin="TXAMP_TH0" pad="139"/>
<connect gate="G$1" pin="TXAMP_TH1" pad="138"/>
<connect gate="G$1" pin="TXN" pad="141"/>
<connect gate="G$1" pin="TXP" pad="142"/>
<connect gate="G$1" pin="VDDA1V5@1" pad="61"/>
<connect gate="G$1" pin="VDDA1V5@2" pad="11"/>
<connect gate="G$1" pin="VDDA3V@1" pad="143"/>
<connect gate="G$1" pin="VDDA3V@2" pad="75"/>
<connect gate="G$1" pin="VDDA3V@3" pad="70"/>
<connect gate="G$1" pin="VDDA3V@4" pad="9"/>
<connect gate="G$1" pin="VDD_CORE@1" pad="122"/>
<connect gate="G$1" pin="VDD_CORE@10" pad="18"/>
<connect gate="G$1" pin="VDD_CORE@2" pad="118"/>
<connect gate="G$1" pin="VDD_CORE@3" pad="105"/>
<connect gate="G$1" pin="VDD_CORE@4" pad="97"/>
<connect gate="G$1" pin="VDD_CORE@5" pad="88"/>
<connect gate="G$1" pin="VDD_CORE@6" pad="54"/>
<connect gate="G$1" pin="VDD_CORE@7" pad="41"/>
<connect gate="G$1" pin="VDD_CORE@8" pad="28"/>
<connect gate="G$1" pin="VDD_CORE@9" pad="19"/>
<connect gate="G$1" pin="VDD_IO@1" pad="127"/>
<connect gate="G$1" pin="VDD_IO@10" pad="40"/>
<connect gate="G$1" pin="VDD_IO@11" pad="35"/>
<connect gate="G$1" pin="VDD_IO@12" pad="22"/>
<connect gate="G$1" pin="VDD_IO@13" pad="16"/>
<connect gate="G$1" pin="VDD_IO@2" pad="120"/>
<connect gate="G$1" pin="VDD_IO@3" pad="119"/>
<connect gate="G$1" pin="VDD_IO@4" pad="114"/>
<connect gate="G$1" pin="VDD_IO@5" pad="108"/>
<connect gate="G$1" pin="VDD_IO@6" pad="89"/>
<connect gate="G$1" pin="VDD_IO@7" pad="58"/>
<connect gate="G$1" pin="VDD_IO@8" pad="55"/>
<connect gate="G$1" pin="VDD_IO@9" pad="49"/>
<connect gate="G$1" pin="VDD_PLL" pad="15"/>
<connect gate="G$1" pin="VDD_UBAT" pad="124"/>
<connect gate="G$1" pin="VPGM" pad="17"/>
<connect gate="G$1" pin="VREF_N_A" pad="3"/>
<connect gate="G$1" pin="VREF_N_M" pad="84"/>
<connect gate="G$1" pin="VREF_P_A" pad="2"/>
<connect gate="G$1" pin="VREF_P_M" pad="85"/>
<connect gate="G$1" pin="VREF_VCM_A" pad="4"/>
<connect gate="G$1" pin="VREF_VCM_M" pad="83"/>
<connect gate="G$1" pin="VSSA@1" pad="144"/>
<connect gate="G$1" pin="VSSA@2" pad="80"/>
<connect gate="G$1" pin="VSSA@3" pad="71"/>
<connect gate="G$1" pin="VSSA@4" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP" package="SOT486-1MK">
<connects>
<connect gate="G$1" pin="!DISW!" pad="100"/>
<connect gate="G$1" pin="!NMI!" pad="99"/>
<connect gate="G$1" pin="!RESET!" pad="132"/>
<connect gate="G$1" pin="!SPI_CS!" pad="101"/>
<connect gate="G$1" pin="!TRST!" pad="24"/>
<connect gate="G$1" pin="!TXAMP_EN!" pad="133"/>
<connect gate="G$1" pin="A0/SIC2" pad="26"/>
<connect gate="G$1" pin="A1/SIC3" pad="27"/>
<connect gate="G$1" pin="A2/SIC4" pad="29"/>
<connect gate="G$1" pin="BC_IGN" pad="110"/>
<connect gate="G$1" pin="BC_I_N" pad="79"/>
<connect gate="G$1" pin="BC_I_P" pad="78"/>
<connect gate="G$1" pin="BC_L" pad="130"/>
<connect gate="G$1" pin="BC_N" pad="131"/>
<connect gate="G$1" pin="BC_P" pad="111"/>
<connect gate="G$1" pin="BC_U_N" pad="77"/>
<connect gate="G$1" pin="BC_U_P" pad="76"/>
<connect gate="G$1" pin="BOOT" pad="115"/>
<connect gate="G$1" pin="GDY0" pad="106"/>
<connect gate="G$1" pin="GDY1" pad="107"/>
<connect gate="G$1" pin="GDY2" pad="112"/>
<connect gate="G$1" pin="GDY3" pad="113"/>
<connect gate="G$1" pin="GDY4" pad="121"/>
<connect gate="G$1" pin="GND@1" pad="109 MB"/>
<connect gate="G$1" pin="GND@2" pad="72"/>
<connect gate="G$1" pin="GND@3" pad="36"/>
<connect gate="G$1" pin="GND@4" pad="1"/>
<connect gate="G$1" pin="GND_PLL" pad="12"/>
<connect gate="G$1" pin="OSC32K1" pad="125"/>
<connect gate="G$1" pin="OSC32K2" pad="126"/>
<connect gate="G$1" pin="P0" pad="34"/>
<connect gate="G$1" pin="P1" pad="37"/>
<connect gate="G$1" pin="P10" pad="33"/>
<connect gate="G$1" pin="P11" pad="48"/>
<connect gate="G$1" pin="P14" pad="50"/>
<connect gate="G$1" pin="P15" pad="51"/>
<connect gate="G$1" pin="P16" pad="52"/>
<connect gate="G$1" pin="P17" pad="53"/>
<connect gate="G$1" pin="P18" pad="90"/>
<connect gate="G$1" pin="P19" pad="91"/>
<connect gate="G$1" pin="P2" pad="38"/>
<connect gate="G$1" pin="P20" pad="92"/>
<connect gate="G$1" pin="P21" pad="93"/>
<connect gate="G$1" pin="P22" pad="94"/>
<connect gate="G$1" pin="P23" pad="95"/>
<connect gate="G$1" pin="P24" pad="96"/>
<connect gate="G$1" pin="P26" pad="98"/>
<connect gate="G$1" pin="P27" pad="116"/>
<connect gate="G$1" pin="P28" pad="117"/>
<connect gate="G$1" pin="P29" pad="30"/>
<connect gate="G$1" pin="P3" pad="39"/>
<connect gate="G$1" pin="P30" pad="31"/>
<connect gate="G$1" pin="P31" pad="32"/>
<connect gate="G$1" pin="P4" pad="42"/>
<connect gate="G$1" pin="P5" pad="43"/>
<connect gate="G$1" pin="P6" pad="44"/>
<connect gate="G$1" pin="P7" pad="45"/>
<connect gate="G$1" pin="P8" pad="46"/>
<connect gate="G$1" pin="P9" pad="47"/>
<connect gate="G$1" pin="PFC_BUF_N" pad="74"/>
<connect gate="G$1" pin="PFC_BUF_P" pad="73"/>
<connect gate="G$1" pin="PFC_I0_N" pad="65"/>
<connect gate="G$1" pin="PFC_I0_P" pad="64"/>
<connect gate="G$1" pin="PFC_I1_N" pad="67"/>
<connect gate="G$1" pin="PFC_I1_P" pad="66"/>
<connect gate="G$1" pin="PFC_LINEU_N" pad="63"/>
<connect gate="G$1" pin="PFC_LINEU_P" pad="62"/>
<connect gate="G$1" pin="PFC_N" pad="128"/>
<connect gate="G$1" pin="PFC_P" pad="129"/>
<connect gate="G$1" pin="REFN" pad="7"/>
<connect gate="G$1" pin="REFP" pad="6"/>
<connect gate="G$1" pin="RESAN" pad="69"/>
<connect gate="G$1" pin="RESAP" pad="68"/>
<connect gate="G$1" pin="RESBN" pad="82"/>
<connect gate="G$1" pin="RESBP" pad="81"/>
<connect gate="G$1" pin="RTC_BUF" pad="123"/>
<connect gate="G$1" pin="RXN" pad="8"/>
<connect gate="G$1" pin="RXP" pad="5"/>
<connect gate="G$1" pin="SIC0" pad="86"/>
<connect gate="G$1" pin="SIC1" pad="87"/>
<connect gate="G$1" pin="SIC12" pad="56"/>
<connect gate="G$1" pin="SIC13" pad="57"/>
<connect gate="G$1" pin="SIC14" pad="59"/>
<connect gate="G$1" pin="SIC15" pad="60"/>
<connect gate="G$1" pin="SPI_CLK" pad="104"/>
<connect gate="G$1" pin="SPI_MISO" pad="102"/>
<connect gate="G$1" pin="SPI_MOSI" pad="103"/>
<connect gate="G$1" pin="SYS_XTAL1" pad="13"/>
<connect gate="G$1" pin="SYS_XTAL2" pad="14"/>
<connect gate="G$1" pin="TCK" pad="20"/>
<connect gate="G$1" pin="TDI" pad="23"/>
<connect gate="G$1" pin="TDO" pad="21"/>
<connect gate="G$1" pin="TMS" pad="25"/>
<connect gate="G$1" pin="TXAMP_OUT_N" pad="134"/>
<connect gate="G$1" pin="TXAMP_OUT_P" pad="135"/>
<connect gate="G$1" pin="TXAMP_SCL" pad="137"/>
<connect gate="G$1" pin="TXAMP_SDA" pad="136"/>
<connect gate="G$1" pin="TXAMP_TEMP" pad="140"/>
<connect gate="G$1" pin="TXAMP_TH0" pad="139"/>
<connect gate="G$1" pin="TXAMP_TH1" pad="138"/>
<connect gate="G$1" pin="TXN" pad="141"/>
<connect gate="G$1" pin="TXP" pad="142"/>
<connect gate="G$1" pin="VDDA1V5@1" pad="61"/>
<connect gate="G$1" pin="VDDA1V5@2" pad="11"/>
<connect gate="G$1" pin="VDDA3V@1" pad="143"/>
<connect gate="G$1" pin="VDDA3V@2" pad="75"/>
<connect gate="G$1" pin="VDDA3V@3" pad="70"/>
<connect gate="G$1" pin="VDDA3V@4" pad="9"/>
<connect gate="G$1" pin="VDD_CORE@1" pad="122"/>
<connect gate="G$1" pin="VDD_CORE@10" pad="18"/>
<connect gate="G$1" pin="VDD_CORE@2" pad="118"/>
<connect gate="G$1" pin="VDD_CORE@3" pad="105"/>
<connect gate="G$1" pin="VDD_CORE@4" pad="97"/>
<connect gate="G$1" pin="VDD_CORE@5" pad="88"/>
<connect gate="G$1" pin="VDD_CORE@6" pad="54"/>
<connect gate="G$1" pin="VDD_CORE@7" pad="41"/>
<connect gate="G$1" pin="VDD_CORE@8" pad="28"/>
<connect gate="G$1" pin="VDD_CORE@9" pad="19"/>
<connect gate="G$1" pin="VDD_IO@1" pad="127"/>
<connect gate="G$1" pin="VDD_IO@10" pad="40"/>
<connect gate="G$1" pin="VDD_IO@11" pad="35"/>
<connect gate="G$1" pin="VDD_IO@12" pad="22"/>
<connect gate="G$1" pin="VDD_IO@13" pad="16"/>
<connect gate="G$1" pin="VDD_IO@2" pad="120"/>
<connect gate="G$1" pin="VDD_IO@3" pad="119"/>
<connect gate="G$1" pin="VDD_IO@4" pad="114"/>
<connect gate="G$1" pin="VDD_IO@5" pad="108"/>
<connect gate="G$1" pin="VDD_IO@6" pad="89"/>
<connect gate="G$1" pin="VDD_IO@7" pad="58"/>
<connect gate="G$1" pin="VDD_IO@8" pad="55"/>
<connect gate="G$1" pin="VDD_IO@9" pad="49"/>
<connect gate="G$1" pin="VDD_PLL" pad="15"/>
<connect gate="G$1" pin="VDD_UBAT" pad="124"/>
<connect gate="G$1" pin="VPGM" pad="17"/>
<connect gate="G$1" pin="VREF_N_A" pad="3"/>
<connect gate="G$1" pin="VREF_N_M" pad="84"/>
<connect gate="G$1" pin="VREF_P_A" pad="2"/>
<connect gate="G$1" pin="VREF_P_M" pad="85"/>
<connect gate="G$1" pin="VREF_VCM_A" pad="4"/>
<connect gate="G$1" pin="VREF_VCM_M" pad="83"/>
<connect gate="G$1" pin="VSSA@1" pad="144"/>
<connect gate="G$1" pin="VSSA@2" pad="80"/>
<connect gate="G$1" pin="VSSA@3" pad="71"/>
<connect gate="G$1" pin="VSSA@4" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AUP1G07" prefix="U">
<description>&lt;H2&gt;Low-power buffer with open-drain output&lt;/H2&gt;
The 74AUP1G07 provides the single non-inverting buffer with open-drain output. The 
output of the device is an open drain and can be connected to other open-drain outputs to 
implement active-LOW wired-OR or active-HIGH wired-AND functions.
Schmitt-trigger action at all inputs makes the circuit tolerant to slower input rise and fall 
times across the entire VCC range from 0.8 V to 3.6 V.
This device ensures a very low static and dynamic power consumption across the entire 
VCC range from 0.8 V to 3.6 V.
This device is fully specified for partial power-down applications using IOFF. 
The IOFF circuitry disables the output, preventing the damaging backflow current through 
the device when it is powered down.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G" symbol="BUFFER_OPENDRAIN"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="GW" package="SOT353-1">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 790 17125"/>
</technology>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GX" package="SOT1226">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AUP1G86" prefix="U">
<description>&lt;H2&gt;Low-power 2-input EXCLUSIVE-OR gate&lt;/H2&gt;
The 74AUP1G86 provides the single 2-input EXCLUSIVE-OR function.
Schmitt-trigger action at all inputs makes the circuit tolerant to slower input rise and fall 
times across the entire VCC range from 0.8 V to 3.6 V.
This device ensures a very low static and dynamic power consumption across the entire 
VCC range from 0.8 V to 3.6 V.
This device is fully specified for partial power-down applications using IOFF. 
The IOFF circuitry disables the output, preventing the damaging backflow current through 
the device when it is powered down.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G" symbol="2-INPUT-EXCLUSIVE-OR"/>
</gates>
<devices>
<device name="GW" package="SOT353-1">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GX" package="SOT1226">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AUP1G32" prefix="U">
<description>&lt;H2&gt;Low-power 2-input OR-gate&lt;/H2&gt;
The 74AUP1G32 provides the single 2-input OR function.
Schmitt-trigger action at all inputs makes the circuit tolerant to slower input rise and fall 
times across the entire VCC range from 0.8 V to 3.6 V.
This device ensures a very low static and dynamic power consumption across the entire 
VCC range from 0.8 V to 3.6 V.
This device is fully specified for partial power-down applications using IOFF. 
The IOFF circuitry disables the output, preventing the damaging backflow current through 
the device when it is powered down.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G" symbol="2-INPUT-OR"/>
</gates>
<devices>
<device name="GW" package="SOT353-1">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GX" package="SOT1226">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="B" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUMMY_DEV">
<gates>
<gate name="G$1" symbol="2-INPUT-AND"/>
<gate name="G$2" symbol="2-INPUT-AND-OD"/>
<gate name="G$3" symbol="2-INPUT-EXCLUSIVE-OR"/>
<gate name="G$4" symbol="2-INPUT-NAND"/>
<gate name="G$5" symbol="2-INPUT-NAND-OD"/>
<gate name="G$6" symbol="2-INPUT-NOR"/>
<gate name="G$7" symbol="2-INPUT-OR"/>
<gate name="G$8" symbol="3-INPUT-AND"/>
<gate name="G$9" symbol="3-INPUT-NAND"/>
<gate name="G$10" symbol="INVERTER"/>
<gate name="G$11" symbol="INVERTER-ST"/>
<gate name="G$12" symbol="INVERTER_OD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAV99" prefix="D">
<description>&lt;H2&gt;High-speed switching diode&lt;/H2&gt;
High-speed switching diodes, encapsulated in small Surface-Mounted Device (SMD) 
plastic packages.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAV99S" prefix="D">
<description>&lt;H2&gt;High-speed switching diode&lt;/H2&gt;
High-speed switching diodes, encapsulated in small Surface-Mounted Device (SMD) 
plastic packages.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="DIODE_AKAK"/>
<gate name="-2" symbol="DIODE_AKAK"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="-1" pin="A1" pad="1"/>
<connect gate="-1" pin="K1A2" pad="6"/>
<connect gate="-1" pin="K2" pad="2"/>
<connect gate="-2" pin="A1" pad="4"/>
<connect gate="-2" pin="K1A2" pad="3"/>
<connect gate="-2" pin="K2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC1G14" prefix="U">
<description>&lt;H2&gt;Single Schmitt-trigger inverter&lt;/H2&gt;
The 74LVC1G14 provides the inverting buffer function with Schmitt-trigger input. It is 
capable of transforming slowly changing input signals into sharply defined, jitter-free 
output signals.
The input can be driven from either 3.3 V or 5 V devices. This feature allows the use of 
this device in a mixed 3.3 V and 5 V environment. Schmitt-trigger action at the input 
makes the circuit tolerant for slower input rise and fall time.
This device is fully specified for partial power-down applications using IOFF. The IOFF
circuitry disables the output, preventing the damaging backflow current through the device 
when it is powered down.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G" symbol="INVERTER-ST"/>
</gates>
<devices>
<device name="GW" package="SOT353-1">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 685 95125"/>
</technology>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 771 79115"/>
</technology>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 824 12132"/>
</technology>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 917 77132"/>
</technology>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 929 03132"/>
</technology>
</technologies>
</device>
<device name="GX" package="SOT1226">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GV" package="SOT753">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 720 19125"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC125A" prefix="U">
<description>&lt;H2&gt;Quad buffer/line driver with 5 V tolerant input/outputs; 3-state&lt;/H2&gt;The 74LVC125A consists of four non-inverting buffers/line drivers with 3-state outputs 
(nY) that are controlled by the output enable input (nOE). A HIGH at nOE causes the 
outputs to assume a high-impedance OFF-state.
Inputs can be driven from either 3.3 V or 5 V devices. When disabled, up to 5.5 V can be 
applied to the outputs.&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt; &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="P" symbol="PWRN-1"/>
<gate name="-1" symbol="BUFFER_OE"/>
<gate name="-2" symbol="BUFFER_OE"/>
<gate name="-3" symbol="BUFFER_OE"/>
<gate name="-4" symbol="BUFFER_OE"/>
</gates>
<devices>
<device name="D" package="SOT108-1">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="3"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="4"/>
<connect gate="-2" pin="Y" pad="6"/>
<connect gate="-3" pin="A" pad="9"/>
<connect gate="-3" pin="OEN" pad="10"/>
<connect gate="-3" pin="Y" pad="8"/>
<connect gate="-4" pin="A" pad="12"/>
<connect gate="-4" pin="OEN" pad="13"/>
<connect gate="-4" pin="Y" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 317 00118"/>
</technology>
</technologies>
</device>
<device name="DB" package="SOT337">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="3"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="4"/>
<connect gate="-2" pin="Y" pad="6"/>
<connect gate="-3" pin="A" pad="9"/>
<connect gate="-3" pin="OEN" pad="10"/>
<connect gate="-3" pin="Y" pad="8"/>
<connect gate="-4" pin="A" pad="12"/>
<connect gate="-4" pin="OEN" pad="13"/>
<connect gate="-4" pin="Y" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PW" package="SOT402-1">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="3"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="4"/>
<connect gate="-2" pin="Y" pad="6"/>
<connect gate="-3" pin="A" pad="9"/>
<connect gate="-3" pin="OEN" pad="10"/>
<connect gate="-3" pin="Y" pad="8"/>
<connect gate="-4" pin="A" pad="12"/>
<connect gate="-4" pin="OEN" pad="13"/>
<connect gate="-4" pin="Y" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BQ" package="SOT762">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="3"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="4"/>
<connect gate="-2" pin="Y" pad="6"/>
<connect gate="-3" pin="A" pad="9"/>
<connect gate="-3" pin="OEN" pad="10"/>
<connect gate="-3" pin="Y" pad="8"/>
<connect gate="-4" pin="A" pad="12"/>
<connect gate="-4" pin="OEN" pad="13"/>
<connect gate="-4" pin="Y" pad="11"/>
<connect gate="P" pin="GND" pad="7 CP"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BGU7045" prefix="U">
<description>&lt;H2&gt;1 GHz wideband low-noise amplifier with bypass&lt;/H2&gt;
The BGU7045 MMIC is a 3.3 V wideband amplifier with bypass mode. It is designed 
specifically for high linearity, low-noise applications over a frequency range of 40 MHz to 
1 GHz. It is especially suited for Set-Top Box applications.
The LNA is housed in a 6-pin SOT363 plastic SMD package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="AMP_WITH_BYPASS"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G$1" pin="CTRL" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BGU7032" prefix="U">
<description>&lt;H2&gt;1 GHz wideband low-noise amplifier with bypass&lt;/H2&gt;
The BGU7032 MMIC is a wideband amplifier with bypass mode. It is designed specifically 
for high linearity, low-noise applications over a frequency range of 40 MHz to 1 GHz. It is 
especially suited to Set-Top Box applications.
The LNA is housed in a 6-pin SOT363 plastic SMD package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="AMP_WITH_BYPASS"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G$1" pin="CTRL" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SC16C550B">
<gates>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF1252" prefix="U">
<description>&lt;H2&gt;Threshold detector and reset generator&lt;/H2&gt;
The PCF1252-Xs are low-power CMOS voltage threshold
detectors designed especially for supervision of
microcontroller/microprocessor systems for detection of
power-on/off conditions and generation of a system reset
pulse. The PCF1252-X also provides a POWF (power fail)
output which is activated at a precise factory-programmed
trip point. A system RESET output has a built-in delay with
duration determined by an external capacitor (CCT).
A second comparator (comparator 2) has been included to
enable the possibility of a second monitoring point in the
system.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCF1252"/>
</gates>
<devices>
<device name="P" package="SOT97-1">
<connects>
<connect gate="G$1" pin="!POWF!" pad="7"/>
<connect gate="G$1" pin="COMIN" pad="3"/>
<connect gate="G$1" pin="COMOUT" pad="5"/>
<connect gate="G$1" pin="CT" pad="1"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SELECT" pad="2"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="-0"/>
<technology name="-1"/>
<technology name="-2"/>
<technology name="-3"/>
<technology name="-4"/>
<technology name="-5"/>
<technology name="-6"/>
<technology name="-7"/>
<technology name="-8"/>
<technology name="-9"/>
</technologies>
</device>
<device name="T" package="SOT96-1">
<connects>
<connect gate="G$1" pin="!POWF!" pad="7"/>
<connect gate="G$1" pin="COMIN" pad="3"/>
<connect gate="G$1" pin="COMOUT" pad="5"/>
<connect gate="G$1" pin="CT" pad="1"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SELECT" pad="2"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="-0"/>
<technology name="-1"/>
<technology name="-2"/>
<technology name="-3"/>
<technology name="-4"/>
<technology name="-5"/>
<technology name="-6"/>
<technology name="-7"/>
<technology name="-8"/>
<technology name="-9"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC1G125" prefix="U">
<description>&lt;H2&gt;Bus buffer/line driver; 3-state&lt;/H2&gt;
The 74LVC1G125 provides one non-inverting buffer/line driver with 3-state output. 
The 3-state output is controlled by the output enable input (OE). A HIGH-level at pin OE
causes the output to assume a high-impedance OFF-state.
The input can be driven from either 3.3 V or 5 V devices. This feature allows the use of 
this device in a mixed 3.3 V and 5 V environment.
This device is fully specified for partial power-down applications using IOFF. The IOFF
circuitry disables the output, preventing the damaging backflow current through the device 
when it is powered down.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G" symbol="BUFFER_OE"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="GW" package="SOT353-1">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="OEN" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GV" package="SOT753">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="OEN" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="OEN" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="OEN" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="OEN" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="OEN" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GX" package="SOT1226">
<connects>
<connect gate="G" pin="A" pad="2"/>
<connect gate="G" pin="OEN" pad="1"/>
<connect gate="G" pin="Y" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC2G125" prefix="U">
<description>&lt;H2&gt;Dual bus buffer/line driver; 3-state&lt;/H2&gt;
The 74LVC2G125 provides a dual non-inverting buffer/line driver with 3-state output. 
The 3-state output is controlled by the output enable input (pin nOE). A HIGH-level at pin 
nOE causes the output to assume a high-impedance OFF-state. Schmitt trigger action at 
all inputs makes the circuit highly tolerant of slower input rise and fall times.
Inputs can be driven from either 3.3 V or 5 V devices. This feature allows the use of these 
devices as translators in a mixed 3.3 V and 5 V environment.
This device is fully specified for partial power-down applications using IOFF. The IOFF
circuitry disables the output, preventing a damaging backflow current through the device 
when it is powered down. 
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="BUFFER_OE"/>
<gate name="-2" symbol="BUFFER_OE"/>
<gate name="-P" symbol="PWRN"/>
</gates>
<devices>
<device name="DP" package="SOT505-2">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="7"/>
<connect gate="-2" pin="Y" pad="3"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF" package="SOT1089-1">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="7"/>
<connect gate="-2" pin="Y" pad="3"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GD" package="SOT996-2/3">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="7"/>
<connect gate="-2" pin="Y" pad="3"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM" package="SOT902">
<connects>
<connect gate="-1" pin="A" pad="6"/>
<connect gate="-1" pin="OEN" pad="7"/>
<connect gate="-1" pin="Y" pad="2"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="OEN" pad="1"/>
<connect gate="-2" pin="Y" pad="5"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DC" package="SOT765">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="7"/>
<connect gate="-2" pin="Y" pad="3"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GT" package="SOT833-1">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="OEN" pad="1"/>
<connect gate="-1" pin="Y" pad="6"/>
<connect gate="-2" pin="A" pad="5"/>
<connect gate="-2" pin="OEN" pad="7"/>
<connect gate="-2" pin="Y" pad="3"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PESD5V0F5UF" prefix="U">
<description>&lt;H2&gt;Femtofarad unidirectional fivefold ESD protection array&lt;/H2&gt;
Femtofarad capacitance unidirectional ElectroStatic Discharge (ESD) protection diode 
array designed to protect up to five signal lines from the damage caused by ESD and 
other transients. The device is encapsulated in a leadless ultra small 
DFN1410-6 (SOT886) Surface-Mounted Device (SMD) plastic package.
The combination of extremely low capacitance, high ESD maximum rating and ultra small 
package makes the device ideal for high-speed data line protection and antenna 
protection applications.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="ESD-PESD5V0F5UF"/>
</gates>
<devices>
<device name="" package="SOT886">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BGU8007" prefix="U">
<description>&lt;H2&gt;SiGe:C Low Noise Amplifier MMIC for GPS, GLONASS, Galileo 
and Compass&lt;/H2&gt;
The BGU8007 is a Low Noise Amplifier (LNA) for GNSS receiver applications in a plastic 
leadless 6-pin, extremely small SOT886 package. The BGU8007 requires only one 
external matching inductor and one external decoupling capacitor.
The BGU8007 adapts itself to the changing environment resulting from co-habitation of 
different radio systems in modern cellular handsets. It has been designed for low power 
consumption and optimal performance when jamming signals from co-existing cellular 
transmitters are present. At low jamming power levels it delivers 19 dB gain at a noise 
figure of 0.75 dB. During high jamming power levels, resulting for example from a cellular 
transmit burst, it temporarily increases its bias current to improve sensitivity
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="AMP_WITH_ENABLE"/>
</gates>
<devices>
<device name="" package="SOT886">
<connects>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="1 2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1623" prefix="U">
<description>&lt;H2&gt;STARplug switched mode power supply controller IC&lt;/H2&gt;
The TEA1623 is a Switched Mode Power Supply (SMPS) controller IC that operates 
directly from rectified universal mains. It is implemented in the high voltage EZ-HV SOI 
process, combined with a low voltage BiCMOS process.
The device includes a high voltage power switch and a circuit for start-up directly from the 
rectified mains voltage. A dedicated circuit for valley switching is built in, which makes a 
very efficient slim-line electronic power-plug concept possible.
In its most basic version of application, the TEA1623 acts as a voltage source. Here, no 
additional secondary electronics are required. A combined voltage and current source can 
be realized with minimum costs for external components. Implementation of the TEA1623 
renders an efficient and low cost power supply system.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TEA1623"/>
</gates>
<devices>
<device name="P" package="SOT97-1">
<connects>
<connect gate="G$1" pin="AUX" pad="5"/>
<connect gate="G$1" pin="DRAIN" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RC" pad="3"/>
<connect gate="G$1" pin="REG" pad="4"/>
<connect gate="G$1" pin="SOURCE" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PH" package="SOT38">
<connects>
<connect gate="G$1" pin="AUX" pad="11"/>
<connect gate="G$1" pin="DRAIN" pad="14"/>
<connect gate="G$1" pin="GND" pad="4 8"/>
<connect gate="G$1" pin="RC" pad="5"/>
<connect gate="G$1" pin="REG" pad="6"/>
<connect gate="G$1" pin="SOURCE" pad="12"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA1731" prefix="U">
<description>&lt;H2&gt;GreenChip SMPS control IC&lt;/H2&gt;
The TEA1731LTS is a low cost Switched Mode Power Supply (SMPS) controller IC 
intended for flyback topologies. The TEA1731LTS operates in peak current and frequency 
control mode. Frequency jitter has been implemented to reduce ElectroMagnetic 
Interference (EMI). Slope compensation is integrated for Continuous Conduction Mode 
(CCM) operation.
The TEA1731LTS IC features OverPower Protection (OPP). The controller accepts an 
overpower situation for a limited amount of time.
One pin is reserved for protection purposes. OverTemperature Protection (OTP) can be 
implemented with a minimal number of external components.
At low-power levels, the primary peak current is set to 25 % of the maximum peak current. 
The switching frequency is reduced to limit the switching losses. The combination of fixed 
frequency operation at high output power and frequency reduction at low output power 
provides high efficiency over the total load range.
The TEA1731LTS makes the design of low cost, highly efficient and reliable supplies for 
power requirements up to 75 W easier by requiring a minimum number of external 
components.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TEA1731"/>
</gates>
<devices>
<device name="" package="SOT457">
<connects>
<connect gate="G$1" pin="CTRL" pad="4"/>
<connect gate="G$1" pin="DRIVER" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="ISENSE" pad="5"/>
<connect gate="G$1" pin="PROTECT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="LTS">
<attribute name="12NC" value="9352 965 45115"/>
<attribute name="FARNELL" value=""/>
</technology>
<technology name="TS">
<attribute name="12NC" value="9352 965 44115"/>
<attribute name="FARNELL" value="2142714"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS21A" prefix="D">
<description>&lt;H2&gt;High-voltage switching diodes&lt;/H2&gt;
High-voltage switching diodes, encapsulated in a very small Surface-Mounted
Device (SMD) plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_KAAK"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1A2" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAS21S" prefix="D">
<description>&lt;H2&gt;High-voltage switching diodes&lt;/H2&gt;
High-voltage switching diodes, encapsulated in a very small Surface-Mounted
Device (SMD) plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE_AKAK"/>
</gates>
<devices>
<device name="W" package="SOT323">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="K1A2" pad="3"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PNS40010ER" prefix="D">
<description>&lt;H2&gt;400 V, 1 A high power density, standard switching time PN-rectifier&lt;/H2&gt;
High power density, standard switching time PN-rectifier with high-efficiency planar 
technology, encapsulated in a small and flat lead SOD123W Surface-Mounted 
Device (SMD) plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD123W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AUP1G17" prefix="U">
<description>&lt;H2&gt;Low-power Schmitt trigger&lt;/H2&gt;
The 74AUP1G17 provides the single Schmitt trigger buffer. It is capable of transforming 
slowly changing input signals into sharply defined, jitter-free output signals.
This device ensures a very low static and dynamic power consumption across the entire 
VCC range from 0.8 V to 3.6 V.
This device is fully specified for partial Power-down applications using IOFF. 
The IOFF circuitry disables the output, preventing the damaging backflow current through 
the device when it is powered down.
The inputs switch at different points for positive and negative-going signals. The difference 
between the positive voltage VT+ and the negative voltage VT is defined as the input 
hysteresis voltage VH.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-G" symbol="BUFFER-ST"/>
<gate name="-P" symbol="PWRN"/>
</gates>
<devices>
<device name="GW" package="SOT353-1">
<connects>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="Y" pad="4"/>
<connect gate="-P" pin="GND" pad="3"/>
<connect gate="-P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 790 24125"/>
</technology>
</technologies>
</device>
<device name="GM" package="SOT886">
<connects>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="Y" pad="4"/>
<connect gate="-P" pin="GND" pad="3"/>
<connect gate="-P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 790 25115"/>
</technology>
</technologies>
</device>
<device name="GF" package="SOT891">
<connects>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="Y" pad="4"/>
<connect gate="-P" pin="GND" pad="3"/>
<connect gate="-P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 811 12132"/>
</technology>
</technologies>
</device>
<device name="GN" package="SOT1115">
<connects>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="Y" pad="4"/>
<connect gate="-P" pin="GND" pad="3"/>
<connect gate="-P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 917 29132"/>
</technology>
</technologies>
</device>
<device name="GS" package="SOT1202">
<connects>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="Y" pad="4"/>
<connect gate="-P" pin="GND" pad="3"/>
<connect gate="-P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 928 54132"/>
</technology>
</technologies>
</device>
<device name="GX" package="SOT1226">
<connects>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="Y" pad="4"/>
<connect gate="-P" pin="GND" pad="3"/>
<connect gate="-P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="12NC" value="9352 982 28125"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC1G99" prefix="U">
<description>&lt;H2&gt;Ultra-configurable multiple function gate; 3-state&lt;/H2&gt;
The 74LVC1G99 provides a low voltage, ultra-configurable, multiple function gate with 
3-state output. The device can be configured as one of several logic functions including, 
AND, OR, NAND, NOR, XOR, XNOR, inverter, buffer and MUX. No external components 
are required to configure the device as all inputs can be connected directly to VCC or 
GND. The 3-state output is controlled by the output enable input (OE). A HIGH level at OE
causes the output (Y) to assume a high-impedance OFF-state. When OE is LOW, the 
output state is determined by the signals applied to the Schmitt trigger inputs (A, B, C and 
D).
Due to the use of Schmitt trigger inputs the device is tolerant of slowly changing input 
signals, transforming them into sharply defined, jitter free output signals. By eliminating 
leakage current paths to VCC and GND, the inputs and disabled output are also 
over-voltage tolerant, making the device suitable for mixed-voltage applications.
This device is fully specified for partial power-down applications using IOFF. 
The IOFF circuitry disables the output, preventing the damaging backflow current through 
the device when it is powered down.
The 74LVC1G99 is fully specified over the supply range from 1.65 V to 5.5 V.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-G" symbol="74LVC1G99"/>
<gate name="-P" symbol="PWRN"/>
</gates>
<devices>
<device name="DP" package="SOT505-2">
<connects>
<connect gate="-G" pin="!OE!" pad="1"/>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="B" pad="3"/>
<connect gate="-G" pin="C" pad="5"/>
<connect gate="-G" pin="D" pad="6"/>
<connect gate="-G" pin="Y" pad="7"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GT" package="SOT833-1">
<connects>
<connect gate="-G" pin="!OE!" pad="1"/>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="B" pad="3"/>
<connect gate="-G" pin="C" pad="5"/>
<connect gate="-G" pin="D" pad="6"/>
<connect gate="-G" pin="Y" pad="7"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GF" package="SOT1089-1">
<connects>
<connect gate="-G" pin="!OE!" pad="1"/>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="B" pad="3"/>
<connect gate="-G" pin="C" pad="5"/>
<connect gate="-G" pin="D" pad="6"/>
<connect gate="-G" pin="Y" pad="7"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GD" package="SOT996-2/3">
<connects>
<connect gate="-G" pin="!OE!" pad="1"/>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="B" pad="3"/>
<connect gate="-G" pin="C" pad="5"/>
<connect gate="-G" pin="D" pad="6"/>
<connect gate="-G" pin="Y" pad="7"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM" package="SOT902">
<connects>
<connect gate="-G" pin="!OE!" pad="7"/>
<connect gate="-G" pin="A" pad="6"/>
<connect gate="-G" pin="B" pad="5"/>
<connect gate="-G" pin="C" pad="3"/>
<connect gate="-G" pin="D" pad="2"/>
<connect gate="-G" pin="Y" pad="1"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GS" package="SOT1203">
<connects>
<connect gate="-G" pin="!OE!" pad="1"/>
<connect gate="-G" pin="A" pad="2"/>
<connect gate="-G" pin="B" pad="3"/>
<connect gate="-G" pin="C" pad="5"/>
<connect gate="-G" pin="D" pad="6"/>
<connect gate="-G" pin="Y" pad="7"/>
<connect gate="-P" pin="GND" pad="4"/>
<connect gate="-P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD6815TD">
<description>&lt;H2&gt;Low dropout regulator, high PSRR, 150 mA&lt;/H2&gt;
The LD6815 series is a small-size Low DropOut regulator (LDO) family with ultra high 
Power Supply Rejection Ratio (PSRR) of 75 dB. The voltage drop is 250 mV at 150 mA 
current rating.
Operating voltages can range from 2.3 V to 5.5 V. The devices are available with fixed 
output voltages between 1.2 V and 3.6 V. 
The LD6815TD/xxH devices show a high-ohmic state at the output pin when set to 
disabled mode. The LD6815TD/xxP devices contain a pull-down switching transistor to 
provide a low-ohmic output state (auto discharge function) in disabled mode.
The LD6815 series devices are available in SOT753 (TSOP5) plastic package. All devices 
are manufactured in monolithic silicon technology.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LD680X"/>
</gates>
<devices>
<device name="" package="SOT753">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="/12H">
<attribute name="12NC" value="9340 667 69125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="1.2V"/>
</technology>
<technology name="/12P">
<attribute name="12NC" value="9340 667 79125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="1.2V"/>
</technology>
<technology name="/15H">
<attribute name="12NC" value="9340 667 71125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="1.5V"/>
</technology>
<technology name="/15P">
<attribute name="12NC" value="9340 667 81125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="1.5V"/>
</technology>
<technology name="/18H">
<attribute name="12NC" value="9340 667 72125 "/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="1.8V"/>
</technology>
<technology name="/18P">
<attribute name="12NC" value="9340 667 82125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="1.8V"/>
</technology>
<technology name="/21H">
<attribute name="12NC" value="9340 671 26125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="2.1V"/>
</technology>
<technology name="/21P">
<attribute name="12NC" value="9340 669 71125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="2.1V"/>
</technology>
<technology name="/25H">
<attribute name="12NC" value="9340 667 73125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="2.5V"/>
</technology>
<technology name="/25P">
<attribute name="12NC" value="9340 667 83125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="2.5V"/>
</technology>
<technology name="/28H">
<attribute name="12NC" value="9340 667 74125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="2.8V"/>
</technology>
<technology name="/28P">
<attribute name="12NC" value="9340 667 84125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="2.8V"/>
</technology>
<technology name="/29H">
<attribute name="12NC" value="9340 667 75125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="2.9V"/>
</technology>
<technology name="/29P">
<attribute name="12NC" value="9340 667 85125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="2.9V"/>
</technology>
<technology name="/30H">
<attribute name="12NC" value="9340 667 76125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="3.0V"/>
</technology>
<technology name="/30P">
<attribute name="12NC" value="9340 667 86125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="3.0V"/>
</technology>
<technology name="/33H">
<attribute name="12NC" value="9340 667 77125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="3.3V"/>
</technology>
<technology name="/33P">
<attribute name="12NC" value="9340 667 87125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="3.3V"/>
</technology>
<technology name="/36H">
<attribute name="12NC" value="9340 667 78125"/>
<attribute name="IMPEDANCE" value="high"/>
<attribute name="VOLTAGE" value="3.6V"/>
</technology>
<technology name="/36P">
<attribute name="12NC" value="9340 667 88125"/>
<attribute name="IMPEDANCE" value="low"/>
<attribute name="VOLTAGE" value="3.6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCAL6416A">
<description>&lt;H2&gt;Short&lt;/H2&gt;
Description
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCAL6416A"/>
</gates>
<devices>
<device name="HF" package="SOT994">
<connects>
<connect gate="G$1" pin="!INT!" pad="22"/>
<connect gate="G$1" pin="!RESET!" pad="24"/>
<connect gate="G$1" pin="ADDR" pad="18"/>
<connect gate="G$1" pin="P0.0" pad="1"/>
<connect gate="G$1" pin="P0.1" pad="2"/>
<connect gate="G$1" pin="P0.2" pad="3"/>
<connect gate="G$1" pin="P0.3" pad="4"/>
<connect gate="G$1" pin="P0.4" pad="5"/>
<connect gate="G$1" pin="P0.5" pad="6"/>
<connect gate="G$1" pin="P0.6" pad="7"/>
<connect gate="G$1" pin="P0.7" pad="8"/>
<connect gate="G$1" pin="P1.0" pad="10"/>
<connect gate="G$1" pin="P1.1" pad="11"/>
<connect gate="G$1" pin="P1.2" pad="12"/>
<connect gate="G$1" pin="P1.3" pad="13"/>
<connect gate="G$1" pin="P1.4" pad="14"/>
<connect gate="G$1" pin="P1.5" pad="15"/>
<connect gate="G$1" pin="P1.6" pad="16"/>
<connect gate="G$1" pin="P1.7" pad="17"/>
<connect gate="G$1" pin="SCL" pad="19"/>
<connect gate="G$1" pin="SDA" pad="20"/>
<connect gate="G$1" pin="VDD(I2C)" pad="23"/>
<connect gate="G$1" pin="VDD(P)" pad="21"/>
<connect gate="G$1" pin="VSS" pad="9 25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PW" package="SOT355-1">
<connects>
<connect gate="G$1" pin="!INT!" pad="1"/>
<connect gate="G$1" pin="!RESET!" pad="3"/>
<connect gate="G$1" pin="ADDR" pad="21"/>
<connect gate="G$1" pin="P0.0" pad="4"/>
<connect gate="G$1" pin="P0.1" pad="5"/>
<connect gate="G$1" pin="P0.2" pad="6"/>
<connect gate="G$1" pin="P0.3" pad="7"/>
<connect gate="G$1" pin="P0.4" pad="8"/>
<connect gate="G$1" pin="P0.5" pad="9"/>
<connect gate="G$1" pin="P0.6" pad="10"/>
<connect gate="G$1" pin="P0.7" pad="11"/>
<connect gate="G$1" pin="P1.0" pad="13"/>
<connect gate="G$1" pin="P1.1" pad="14"/>
<connect gate="G$1" pin="P1.2" pad="15"/>
<connect gate="G$1" pin="P1.3" pad="16"/>
<connect gate="G$1" pin="P1.4" pad="17"/>
<connect gate="G$1" pin="P1.5" pad="18"/>
<connect gate="G$1" pin="P1.6" pad="19"/>
<connect gate="G$1" pin="P1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD(I2C)" pad="2"/>
<connect gate="G$1" pin="VDD(P)" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EV" package="SOT1199-1">
<connects>
<connect gate="G$1" pin="!INT!" pad="A3"/>
<connect gate="G$1" pin="!RESET!" pad="A2"/>
<connect gate="G$1" pin="ADDR" pad="B5"/>
<connect gate="G$1" pin="P0.0" pad="A1"/>
<connect gate="G$1" pin="P0.1" pad="C3"/>
<connect gate="G$1" pin="P0.2" pad="B1"/>
<connect gate="G$1" pin="P0.3" pad="C1"/>
<connect gate="G$1" pin="P0.4" pad="C2"/>
<connect gate="G$1" pin="P0.5" pad="D1"/>
<connect gate="G$1" pin="P0.6" pad="E1"/>
<connect gate="G$1" pin="P0.7" pad="D2"/>
<connect gate="G$1" pin="P1.0" pad="E3"/>
<connect gate="G$1" pin="P1.1" pad="E4"/>
<connect gate="G$1" pin="P1.2" pad="D3"/>
<connect gate="G$1" pin="P1.3" pad="E5"/>
<connect gate="G$1" pin="P1.4" pad="D4"/>
<connect gate="G$1" pin="P1.5" pad="D5"/>
<connect gate="G$1" pin="P1.6" pad="C5"/>
<connect gate="G$1" pin="P1.7" pad="C4"/>
<connect gate="G$1" pin="SCL" pad="A5"/>
<connect gate="G$1" pin="SDA" pad="A4"/>
<connect gate="G$1" pin="VDD(I2C)" pad="B3"/>
<connect gate="G$1" pin="VDD(P)" pad="B4"/>
<connect gate="G$1" pin="VSS" pad="E2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U34FHN33">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-HVQFN33"/>
</gates>
<devices>
<device name="" package="HVQFN33-7X7">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="2"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="3"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="30"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="20"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="27"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="28"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="1"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="USB_DM" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="14"/>
<connect gate="G$1" pin="VDD" pad="6 29"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name="/311">
<attribute name="FLASH" value="40kB"/>
<attribute name="GPIO" value="26"/>
<attribute name="SRAM" value="8kB"/>
</technology>
<technology name="/421">
<attribute name="FLASH" value="48kB"/>
<attribute name="GPIO" value="26"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U34FBD48" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-LQFP48"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="3"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="45"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="17"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="30"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="42"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="36"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="37"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="43"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="48"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="18"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="21"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="1"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="11"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="12"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="24"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="31"/>
<connect gate="G$1" pin="PIO1_31" pad="25"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD" pad="8 44"/>
<connect gate="G$1" pin="VSS" pad="5 41"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name="/311">
<attribute name="FLASH" value="40kB"/>
<attribute name="GPIO" value="40"/>
<attribute name="SRAM" value="8kB"/>
</technology>
<technology name="/421">
<attribute name="FLASH" value="48kB"/>
<attribute name="GPIO" value="40"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U35FHN33">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-HVQFN33"/>
</gates>
<devices>
<device name="" package="HVQFN33-7X7">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="2"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="3"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="30"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="20"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="27"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="28"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="1"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="USB_DM" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="14"/>
<connect gate="G$1" pin="VDD" pad="6 29"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name="/401">
<attribute name="FLASH" value="64kB"/>
<attribute name="GPIO" value="26"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U35FBD48" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-LQFP48"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="3"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="45"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="17"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="30"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="42"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="36"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="37"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="43"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="48"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="18"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="21"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="1"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="11"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="12"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="24"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="31"/>
<connect gate="G$1" pin="PIO1_31" pad="25"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD" pad="8 44"/>
<connect gate="G$1" pin="VSS" pad="5 41"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name="/401">
<attribute name="FLASH" value="64kB"/>
<attribute name="GPIO" value="40"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U35FHI33">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-HVQFN33"/>
</gates>
<devices>
<device name="" package="HVQFN33-7X7">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="2"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="24"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="3"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="26"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="30"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="31"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="32"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="8"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="20"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="27"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="11"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="15"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="18"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="28"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="1"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="19"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="21"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="23"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="22"/>
<connect gate="G$1" pin="USB_DM" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="14"/>
<connect gate="G$1" pin="VDD" pad="6 29"/>
<connect gate="G$1" pin="VSS" pad="33"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name="/501">
<attribute name="FLASH" value="64kB"/>
<attribute name="GPIO" value="26"/>
<attribute name="SRAM" value="12kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U35FET48" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-TFBGA48"/>
</gates>
<devices>
<device name="" package="SOT1155-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="C1"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="B7"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="C2"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="A6"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="A3"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="B3"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="B2"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="F1"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="F2"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0" pad="G4"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="E8"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="A5"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="H2"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="G3"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="H3"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="H6"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="G7"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="F8"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="F7"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="B8"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="A8"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="A4"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="A2"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="B1"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="H1"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="G8"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="A7"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="H4"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="G6"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="A1"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="G2"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="G1"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="H7"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="D7"/>
<connect gate="G$1" pin="PIO1_5/CT32B1_CAP1" pad="H8"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="E7"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="B6"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="D8"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="C8"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="C7"/>
<connect gate="G$1" pin="USB_DM" pad="G5"/>
<connect gate="G$1" pin="USB_DP" pad="H5"/>
<connect gate="G$1" pin="VDD" pad="B4 E2"/>
<connect gate="G$1" pin="VSS" pad="B5 D2"/>
<connect gate="G$1" pin="XTALIN" pad="D1"/>
<connect gate="G$1" pin="XTALOUT" pad="E1"/>
</connects>
<technologies>
<technology name="/501">
<attribute name="FLASH" value="64kB"/>
<attribute name="GPIO" value="40"/>
<attribute name="SRAM" value="12kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U36FBD48" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-LQFP48"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="3"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="45"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="17"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="30"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="42"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="36"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="37"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="43"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="48"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="18"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="21"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="1"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="11"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="12"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="24"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="31"/>
<connect gate="G$1" pin="PIO1_31" pad="25"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD" pad="8 44"/>
<connect gate="G$1" pin="VSS" pad="5 41"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name="/401">
<attribute name="FLASH" value="96kB"/>
<attribute name="GPIO" value="40"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U37FBD48" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-LQFP48"/>
</gates>
<devices>
<device name="" package="SOT313-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="3"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="45"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="17"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="30"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="42"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="36"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="37"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="43"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="48"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="18"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="21"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="1"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="11"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="12"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="24"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="31"/>
<connect gate="G$1" pin="PIO1_31" pad="25"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD" pad="8 44"/>
<connect gate="G$1" pin="VSS" pad="5 41"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name="/401">
<attribute name="FLASH" value="128kB"/>
<attribute name="GPIO" value="40"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U35FBD64" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-LQFP64"/>
</gates>
<devices>
<device name="" package="SOT314-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="4"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="46"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="5"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="53"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="60"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="61"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="62"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="13"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="11"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0" pad="22"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="40"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="56"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="21"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="29"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="30"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="36"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="37"/>
<connect gate="G$1" pin="PIO1_0/CT32B1_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO1_1/CT32B1_MAT1" pad="17"/>
<connect gate="G$1" pin="PIO1_10" pad="12"/>
<connect gate="G$1" pin="PIO1_11" pad="43"/>
<connect gate="G$1" pin="PIO1_12" pad="59"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="47"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="49"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="57"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="63"/>
<connect gate="G$1" pin="PIO1_17/CT16B0_CAP1/RXD" pad="23"/>
<connect gate="G$1" pin="PIO1_18/CT16B1_CAP1/TXD" pad="28"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="3"/>
<connect gate="G$1" pin="PIO1_2/CT32B1_MAT2" pad="34"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="18"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="35"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="51"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="24"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="14"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="15"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="31"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="41"/>
<connect gate="G$1" pin="PIO1_3/CT32B1_MAT3" pad="50"/>
<connect gate="G$1" pin="PIO1_4/CT32B1_CAP0" pad="16"/>
<connect gate="G$1" pin="PIO1_5/CT32B1_CAP1" pad="32"/>
<connect gate="G$1" pin="PIO1_6" pad="64"/>
<connect gate="G$1" pin="PIO1_7" pad="6"/>
<connect gate="G$1" pin="PIO1_8" pad="39"/>
<connect gate="G$1" pin="PIO1_9" pad="55"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="38"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="52"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="42"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="45"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="44"/>
<connect gate="G$1" pin="USB_DM" pad="25"/>
<connect gate="G$1" pin="USB_DP" pad="26"/>
<connect gate="G$1" pin="VDD" pad="10 33 48 58"/>
<connect gate="G$1" pin="VSS" pad="7 54"/>
<connect gate="G$1" pin="XTALIN" pad="8"/>
<connect gate="G$1" pin="XTALOUT" pad="9"/>
</connects>
<technologies>
<technology name="/401">
<attribute name="FLASH" value="64kB"/>
<attribute name="GPIO" value="54"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U36FBD64" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-LQFP64"/>
</gates>
<devices>
<device name="" package="SOT314-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="4"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="46"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="5"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="53"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="60"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="61"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="62"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="13"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="11"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0" pad="22"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="40"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="56"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="21"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="29"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="30"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="36"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="37"/>
<connect gate="G$1" pin="PIO1_0/CT32B1_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO1_1/CT32B1_MAT1" pad="17"/>
<connect gate="G$1" pin="PIO1_10" pad="12"/>
<connect gate="G$1" pin="PIO1_11" pad="43"/>
<connect gate="G$1" pin="PIO1_12" pad="59"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="47"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="49"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="57"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="63"/>
<connect gate="G$1" pin="PIO1_17/CT16B0_CAP1/RXD" pad="23"/>
<connect gate="G$1" pin="PIO1_18/CT16B1_CAP1/TXD" pad="28"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="3"/>
<connect gate="G$1" pin="PIO1_2/CT32B1_MAT2" pad="34"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="18"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="35"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="51"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="24"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="14"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="15"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="31"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="41"/>
<connect gate="G$1" pin="PIO1_3/CT32B1_MAT3" pad="50"/>
<connect gate="G$1" pin="PIO1_4/CT32B1_CAP0" pad="16"/>
<connect gate="G$1" pin="PIO1_5/CT32B1_CAP1" pad="32"/>
<connect gate="G$1" pin="PIO1_6" pad="64"/>
<connect gate="G$1" pin="PIO1_7" pad="6"/>
<connect gate="G$1" pin="PIO1_8" pad="39"/>
<connect gate="G$1" pin="PIO1_9" pad="55"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="38"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="52"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="42"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="45"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="44"/>
<connect gate="G$1" pin="USB_DM" pad="25"/>
<connect gate="G$1" pin="USB_DP" pad="26"/>
<connect gate="G$1" pin="VDD" pad="10 33 48 58"/>
<connect gate="G$1" pin="VSS" pad="7 54"/>
<connect gate="G$1" pin="XTALIN" pad="8"/>
<connect gate="G$1" pin="XTALOUT" pad="9"/>
</connects>
<technologies>
<technology name="/401">
<attribute name="FLASH" value="96kB"/>
<attribute name="GPIO" value="54"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U37FBD64" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 128  kB flash; up 
to 12  kB SRAM and 4 kB EEPROM; USB device; USART&lt;/H2&gt;
The LPC11U3x are a ARM Cortex-M0 based, low-cost 32-bit MCU family, designed for 
8/16-bit microcontroller applications, offering performance, low power, simple instruction 
set and memory addressing together with reduced code size compared to existing 8/16-bit 
architectures.
The LPC11U3x operate at CPU frequencies of up to 50 MHz.
Equipped with a highly flexible and configurable Full Speed USB 2.0 device controller, the 
LPC11U3x brings unparalleled design flexibility and seamless integration to today’s 
demanding connectivity solutions.
The peripheral complement of the LPC11U3x includes up to 128 kB of flash memory, up 
to 12 kB of SRAM data memory and 4 kB EEPROM, one Fast-mode Plus I
2
C-bus 
interface, one RS-485/EIA-485 USART with support for synchronous mode and smart 
card interface, two SSP interfaces, four general purpose counter/timers, a 10-bit ADC, 
and up to 54 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U3X-LQFP64"/>
</gates>
<devices>
<device name="" package="SOT314-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="4"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="46"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="5"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="53"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="60"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="61"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="62"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="13"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="11"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0" pad="22"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="40"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="56"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="21"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="29"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="30"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="36"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="37"/>
<connect gate="G$1" pin="PIO1_0/CT32B1_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO1_1/CT32B1_MAT1" pad="17"/>
<connect gate="G$1" pin="PIO1_10" pad="12"/>
<connect gate="G$1" pin="PIO1_11" pad="43"/>
<connect gate="G$1" pin="PIO1_12" pad="59"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="47"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="49"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="57"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="63"/>
<connect gate="G$1" pin="PIO1_17/CT16B0_CAP1/RXD" pad="23"/>
<connect gate="G$1" pin="PIO1_18/CT16B1_CAP1/TXD" pad="28"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="3"/>
<connect gate="G$1" pin="PIO1_2/CT32B1_MAT2" pad="34"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="18"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="35"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="51"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="24"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="14"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="15"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="31"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="41"/>
<connect gate="G$1" pin="PIO1_3/CT32B1_MAT3" pad="50"/>
<connect gate="G$1" pin="PIO1_4/CT32B1_CAP0" pad="16"/>
<connect gate="G$1" pin="PIO1_5/CT32B1_CAP1" pad="32"/>
<connect gate="G$1" pin="PIO1_6" pad="64"/>
<connect gate="G$1" pin="PIO1_7" pad="6"/>
<connect gate="G$1" pin="PIO1_8" pad="39"/>
<connect gate="G$1" pin="PIO1_9" pad="55"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="38"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="52"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="42"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="45"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="44"/>
<connect gate="G$1" pin="USB_DM" pad="25"/>
<connect gate="G$1" pin="USB_DP" pad="26"/>
<connect gate="G$1" pin="VDD" pad="10 33 48 58"/>
<connect gate="G$1" pin="VSS" pad="7 54"/>
<connect gate="G$1" pin="XTALIN" pad="8"/>
<connect gate="G$1" pin="XTALOUT" pad="9"/>
</connects>
<technologies>
<technology name="/401">
<attribute name="FLASH" value="128kB"/>
<attribute name="GPIO" value="54"/>
<attribute name="SRAM" value="10kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOPT12-800C0" prefix="T">
<description>&lt;H2&gt;Top Triac&lt;/H2&gt;
Planar passivated Temperature and Overload Protected Triac with high commutation
performance in a SOT78 (TO-220AB) plastic package. This TOPTriac
TM
 conveniently self
protects by turning off in the event of excessive temperature. It is triggered negatively,
which can be continuous DC or pulsed.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="TRIAC_TOP"/>
</gates>
<devices>
<device name="" package="SOT78">
<connects>
<connect gate="G$1" pin="CM" pad="1"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="LD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N7002" prefix="T">
<description>&lt;H2&gt;N-channel TrenchMOS FET&lt;/H2&gt;
N-channel enhancement mode Field-Effect Transistor (FET) in a plastic package using
TrenchMOS technology.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="F"/>
<technology name="P"/>
<technology name="T"/>
</technologies>
</device>
<device name="PW" package="SOT323">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT" package="SOT416">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N7002K" prefix="T">
<description>&lt;H2&gt;N-channel TrenchMOS FET&lt;/H2&gt;
N-channel enhancement mode Field-Effect Transistor (FET) in a plastic package using
TrenchMOS technology.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-ESD"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N7002CK" prefix="T">
<description>&lt;H2&gt;60 V, 0.3 A N-channel Trench MOSFET&lt;/H2&gt;
ESD protected N-channel enhancement mode Field-Effect Transistor (FET) in a
small SOT23 (TO-236AB) Surface-Mounted Device (SMD) plastic package using
Trench MOSFET technology.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-ESD"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N7002P" prefix="T">
<description>&lt;H2&gt;60 V, 320 mA N-channel Trench MOSFET&lt;/H2&gt;
Dual N-channel enhancement mode Field-Effect Transistor (FET) in a very small 
SOT363 (SC-88) Surface-Mounted Device (SMD) plastic package using Trench MOSFET 
technology.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="N-MOSFET"/>
<gate name="-2" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="S" package="SOT363">
<connects>
<connect gate="-1" pin="D" pad="6"/>
<connect gate="-1" pin="G" pad="2"/>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="D" pad="3"/>
<connect gate="-2" pin="G" pad="5"/>
<connect gate="-2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="SOT666">
<connects>
<connect gate="-1" pin="D" pad="6"/>
<connect gate="-1" pin="G" pad="2"/>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="D" pad="3"/>
<connect gate="-2" pin="G" pad="5"/>
<connect gate="-2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N7002BK" prefix="T">
<description>&lt;H2&gt;60 V, 340 mA dual N-channel Trench MOSFET&lt;/H2&gt;
Dual N-channel enhancement mode Field-Effect Transistor (FET) in an ultra small 
SOT666 Surface-Mounted Device (SMD) plastic package using Trench MOSFET 
technology.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="-1" symbol="N-MOSFET"/>
<gate name="-2" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="S" package="SOT363">
<connects>
<connect gate="-1" pin="D" pad="6"/>
<connect gate="-1" pin="G" pad="2"/>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="D" pad="3"/>
<connect gate="-2" pin="G" pad="5"/>
<connect gate="-2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="SOT666">
<connects>
<connect gate="-1" pin="D" pad="6"/>
<connect gate="-1" pin="G" pad="2"/>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="D" pad="3"/>
<connect gate="-2" pin="G" pad="5"/>
<connect gate="-2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BSS84" prefix="T">
<description>&lt;H2&gt;P-channel enhancement mode vertical DMOS transistor&lt;/H2&gt;
P-channel enhancement mode vertical Diffusion Metal-Oxide Semiconductor (DMOS)
transistor in a small Surface-Mounted Device (SMD) plastic package.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="P-MOSFET_2D"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IP4294CZ10-TBR" prefix="U">
<description>&lt;H2&gt;ESD protection for ultra high-speed interfaces&lt;/H2&gt;
The device is designed to protect high-speed interfaces such as SuperSpeed USB, 
High-Definition Multimedia Interface (HDMI), DisplayPort, external Serial Advanced 
Technology Attachment (eSATA) and Low Voltage Differential Signaling (LVDS) interfaces 
against ElectroStatic Discharge (ESD).
The device includes four high-level ESD protection diode structures for ultra high-speed 
signal lines and is encapsulated in leadless ultra small DFN2510A-10 (SOT1176-1) plastic 
package.
All signal lines are protected by a special diode configuration offering ultra low line 
capacitance of only 0.5 pF. These diodes utilize a unique snap-back structure in order to 
provide protection to downstream components from ESD voltages up to 10 kV contact 
exceeding IEC 61000-4-2, level 4.
In order to reduce the capacitance variation versus channel DC voltage, the ground 
diodes between each channel and ground pins 3 and 8 are implemented as Shockley 
diodes.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="IP4294CZ10-TBR"/>
</gates>
<devices>
<device name="" package="SOT1176">
<connects>
<connect gate="G$1" pin="ESD1" pad="1"/>
<connect gate="G$1" pin="ESD2" pad="2"/>
<connect gate="G$1" pin="ESD3" pad="4"/>
<connect gate="G$1" pin="ESD4" pad="5"/>
<connect gate="G$1" pin="GND" pad="3 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCAL6408A" prefix="U">
<description>&lt;H2&gt;Low-voltage translating, 8-bit I2C-bus/SMBus I/O expander 
with interrupt output, reset, and configuration registers&lt;/H2&gt;
The PCAL6408A is an 8-bit general purpose I/O expander that provides remote I/O 
expansion for most microcontroller families via the I2C-bus interface.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="PCAL6408A"/>
</gates>
<devices>
<device name="BS" package="SOT758-1">
<connects>
<connect gate="G$1" pin="!INT!" pad="11"/>
<connect gate="G$1" pin="!RESET!" pad="1"/>
<connect gate="G$1" pin="ADDR" pad="16"/>
<connect gate="G$1" pin="P0" pad="2"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="4"/>
<connect gate="G$1" pin="P3" pad="5"/>
<connect gate="G$1" pin="P4" pad="7"/>
<connect gate="G$1" pin="P5" pad="8"/>
<connect gate="G$1" pin="P6" pad="9"/>
<connect gate="G$1" pin="P7" pad="10"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD(I2C)" pad="15"/>
<connect gate="G$1" pin="VDD(P)" pad="14"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PW" package="SOT403-1">
<connects>
<connect gate="G$1" pin="!INT!" pad="13"/>
<connect gate="G$1" pin="!RESET!" pad="3"/>
<connect gate="G$1" pin="ADDR" pad="2"/>
<connect gate="G$1" pin="P0" pad="4"/>
<connect gate="G$1" pin="P1" pad="5"/>
<connect gate="G$1" pin="P2" pad="6"/>
<connect gate="G$1" pin="P3" pad="7"/>
<connect gate="G$1" pin="P4" pad="9"/>
<connect gate="G$1" pin="P5" pad="10"/>
<connect gate="G$1" pin="P6" pad="11"/>
<connect gate="G$1" pin="P7" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VDD(I2C)" pad="1"/>
<connect gate="G$1" pin="VDD(P)" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HK" package="SOT1161-1">
<connects>
<connect gate="G$1" pin="!INT!" pad="11"/>
<connect gate="G$1" pin="!RESET!" pad="1"/>
<connect gate="G$1" pin="ADDR" pad="16"/>
<connect gate="G$1" pin="P0" pad="2"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="4"/>
<connect gate="G$1" pin="P3" pad="5"/>
<connect gate="G$1" pin="P4" pad="7"/>
<connect gate="G$1" pin="P5" pad="8"/>
<connect gate="G$1" pin="P6" pad="9"/>
<connect gate="G$1" pin="P7" pad="10"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD(I2C)" pad="15"/>
<connect gate="G$1" pin="VDD(P)" pad="14"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC810M021FN8" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0+ microcontroller&lt;/H2&gt;
The LPC81xM are an ARM Cortex-M0+ based, low-cost 32-bit MCU family operating at 
CPU frequencies of up to 30 MHz. The LPC81xM support up to 16 kB of flash memory 
and 4 kB of SRAM.
The peripheral complement of the LPC81xM includes a CRC engine, one I
2
C-bus 
interface, up to three USARTs, up to two SPI interfaces, one multi-rate timer, self wake-up 
timer, and state-configurable timer, one comparator, function-configurable I/O ports 
through a switch matrix, an input pattern match engine, and up to 18 general-purpose I/O 
pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC810M021FN8"/>
</gates>
<devices>
<device name="" package="SOT97-1">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_5" pad="1"/>
<connect gate="G$1" pin="PIO0_0/ACMP_I1/TDO" pad="8"/>
<connect gate="G$1" pin="PIO0_1/ACMP_I2/CLKIN/TDI" pad="5"/>
<connect gate="G$1" pin="PIO0_4/WAKEUP/!TRST!" pad="2"/>
<connect gate="G$1" pin="SWCLK/PIO0_3/TCK" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO0_2/TMS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMP" value="1"/>
<attribute name="FLASH" value="4k"/>
<attribute name="GPIO" value="6"/>
<attribute name="I2C" value="1"/>
<attribute name="SPI" value="1"/>
<attribute name="SRAM" value="1k"/>
<attribute name="USART" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC812M101FDH16" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0+ microcontroller&lt;/H2&gt;
The LPC81xM are an ARM Cortex-M0+ based, low-cost 32-bit MCU family operating at 
CPU frequencies of up to 30 MHz. The LPC81xM support up to 16 kB of flash memory 
and 4 kB of SRAM.
The peripheral complement of the LPC81xM includes a CRC engine, one I
2
C-bus 
interface, up to three USARTs, up to two SPI interfaces, one multi-rate timer, self wake-up 
timer, and state-configurable timer, one comparator, function-configurable I/O ports 
through a switch matrix, an input pattern match engine, and up to 18 general-purpose I/O 
pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC811M001FDH16"/>
</gates>
<devices>
<device name="" package="SOT403-1">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_5" pad="3"/>
<connect gate="G$1" pin="PIO0_0/ACMP_I1/TDO" pad="16"/>
<connect gate="G$1" pin="PIO0_1/ACMP_I2/CLKIN/TDI" pad="9"/>
<connect gate="G$1" pin="PIO0_10" pad="8"/>
<connect gate="G$1" pin="PIO0_11" pad="7"/>
<connect gate="G$1" pin="PIO0_12" pad="2"/>
<connect gate="G$1" pin="PIO0_13" pad="1"/>
<connect gate="G$1" pin="PIO0_4/WAKEUP/!TRST!" pad="4"/>
<connect gate="G$1" pin="PIO0_6/VDDCMP" pad="15"/>
<connect gate="G$1" pin="PIO0_7" pad="14"/>
<connect gate="G$1" pin="PIO0_8/XTALIN" pad="11"/>
<connect gate="G$1" pin="PIO0_9/XTALOUT" pad="10"/>
<connect gate="G$1" pin="SWCLK/PIO0_3/TCK" pad="5"/>
<connect gate="G$1" pin="SWDIO/PIO0_2/TMS" pad="6"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMP" value="1"/>
<attribute name="FLASH" value="16k"/>
<attribute name="GPIO" value="14"/>
<attribute name="I2C" value="1"/>
<attribute name="SPI" value="2"/>
<attribute name="SRAM" value="4k"/>
<attribute name="USART" value="3"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC811M001FDH16" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0+ microcontroller&lt;/H2&gt;
The LPC81xM are an ARM Cortex-M0+ based, low-cost 32-bit MCU family operating at 
CPU frequencies of up to 30 MHz. The LPC81xM support up to 16 kB of flash memory 
and 4 kB of SRAM.
The peripheral complement of the LPC81xM includes a CRC engine, one I
2
C-bus 
interface, up to three USARTs, up to two SPI interfaces, one multi-rate timer, self wake-up 
timer, and state-configurable timer, one comparator, function-configurable I/O ports 
through a switch matrix, an input pattern match engine, and up to 18 general-purpose I/O 
pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC811M001FDH16"/>
</gates>
<devices>
<device name="" package="SOT403-1">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_5" pad="3"/>
<connect gate="G$1" pin="PIO0_0/ACMP_I1/TDO" pad="16"/>
<connect gate="G$1" pin="PIO0_1/ACMP_I2/CLKIN/TDI" pad="9"/>
<connect gate="G$1" pin="PIO0_10" pad="8"/>
<connect gate="G$1" pin="PIO0_11" pad="7"/>
<connect gate="G$1" pin="PIO0_12" pad="2"/>
<connect gate="G$1" pin="PIO0_13" pad="1"/>
<connect gate="G$1" pin="PIO0_4/WAKEUP/!TRST!" pad="4"/>
<connect gate="G$1" pin="PIO0_6/VDDCMP" pad="15"/>
<connect gate="G$1" pin="PIO0_7" pad="14"/>
<connect gate="G$1" pin="PIO0_8/XTALIN" pad="11"/>
<connect gate="G$1" pin="PIO0_9/XTALOUT" pad="10"/>
<connect gate="G$1" pin="SWCLK/PIO0_3/TCK" pad="5"/>
<connect gate="G$1" pin="SWDIO/PIO0_2/TMS" pad="6"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMP" value="1"/>
<attribute name="FLASH" value="8k"/>
<attribute name="GPIO" value="14"/>
<attribute name="I2C" value="1"/>
<attribute name="SPI" value="1"/>
<attribute name="SRAM" value="2k"/>
<attribute name="USART" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC812M101" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0+ microcontroller&lt;/H2&gt;
The LPC81xM are an ARM Cortex-M0+ based, low-cost 32-bit MCU family operating at 
CPU frequencies of up to 30 MHz. The LPC81xM support up to 16 kB of flash memory 
and 4 kB of SRAM.
The peripheral complement of the LPC81xM includes a CRC engine, one I
2
C-bus 
interface, up to three USARTs, up to two SPI interfaces, one multi-rate timer, self wake-up 
timer, and state-configurable timer, one comparator, function-configurable I/O ports 
through a switch matrix, an input pattern match engine, and up to 18 general-purpose I/O 
pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC812M101FD20"/>
</gates>
<devices>
<device name="FD20" package="SOT163-1">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_5" pad="4"/>
<connect gate="G$1" pin="PIO0_0/ACMP_I1/TDO" pad="19"/>
<connect gate="G$1" pin="PIO0_1/ACMP_I2/CLKIN/TDI" pad="12"/>
<connect gate="G$1" pin="PIO0_10" pad="9"/>
<connect gate="G$1" pin="PIO0_11" pad="8"/>
<connect gate="G$1" pin="PIO0_12" pad="3"/>
<connect gate="G$1" pin="PIO0_13" pad="2"/>
<connect gate="G$1" pin="PIO0_14" pad="20"/>
<connect gate="G$1" pin="PIO0_15" pad="11"/>
<connect gate="G$1" pin="PIO0_16" pad="10"/>
<connect gate="G$1" pin="PIO0_17" pad="1"/>
<connect gate="G$1" pin="PIO0_4/WAKEUP/!TRST!" pad="5"/>
<connect gate="G$1" pin="PIO0_6/VDDCMP" pad="18"/>
<connect gate="G$1" pin="PIO0_7" pad="17"/>
<connect gate="G$1" pin="PIO0_8/XTALIN" pad="14"/>
<connect gate="G$1" pin="PIO0_9/XTALOUT" pad="13"/>
<connect gate="G$1" pin="SWCLK/PIO0_3/TCK" pad="6"/>
<connect gate="G$1" pin="SWDIO/PIO0_2/TMS" pad="7"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMP" value="1"/>
<attribute name="FLASH" value="16k"/>
<attribute name="GPIO" value="18"/>
<attribute name="I2C" value="1"/>
<attribute name="SPI" value="1"/>
<attribute name="SRAM" value="4k"/>
<attribute name="USART" value="2"/>
</technology>
</technologies>
</device>
<device name="FDH20" package="SOT360">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_5" pad="4"/>
<connect gate="G$1" pin="PIO0_0/ACMP_I1/TDO" pad="19"/>
<connect gate="G$1" pin="PIO0_1/ACMP_I2/CLKIN/TDI" pad="12"/>
<connect gate="G$1" pin="PIO0_10" pad="9"/>
<connect gate="G$1" pin="PIO0_11" pad="8"/>
<connect gate="G$1" pin="PIO0_12" pad="3"/>
<connect gate="G$1" pin="PIO0_13" pad="2"/>
<connect gate="G$1" pin="PIO0_14" pad="20"/>
<connect gate="G$1" pin="PIO0_15" pad="11"/>
<connect gate="G$1" pin="PIO0_16" pad="10"/>
<connect gate="G$1" pin="PIO0_17" pad="1"/>
<connect gate="G$1" pin="PIO0_4/WAKEUP/!TRST!" pad="5"/>
<connect gate="G$1" pin="PIO0_6/VDDCMP" pad="18"/>
<connect gate="G$1" pin="PIO0_7" pad="17"/>
<connect gate="G$1" pin="PIO0_8/XTALIN" pad="14"/>
<connect gate="G$1" pin="PIO0_9/XTALOUT" pad="13"/>
<connect gate="G$1" pin="SWCLK/PIO0_3/TCK" pad="6"/>
<connect gate="G$1" pin="SWDIO/PIO0_2/TMS" pad="7"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMP" value="1"/>
<attribute name="FLASH" value="16k"/>
<attribute name="GPIO" value="18"/>
<attribute name="I2C" value="1"/>
<attribute name="SPI" value="2"/>
<attribute name="SRAM" value="4k"/>
<attribute name="USART" value="3"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
