<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>&lt;b&gt;ST Microelectronics Devices&lt;/b&gt;&lt;p&gt;
Microcontrollers,  I2C components, linear devices&lt;p&gt;
http://www.st.com&lt;p&gt;
&lt;i&gt;Include st-microelectronics-2.lbr, st-microelectronics-3.lbr.&lt;p&gt;&lt;/i&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO20">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AC</description>
</package>
<package name="SO28">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AB</description>
</package>
<package name="DIL-08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="PSO36">
<description>&lt;b&gt;36 LEADS POWER SMALL OUTLINE PACKAGE&lt;/b&gt;&lt;p&gt;
Source: http://www.st.com/stonline/books/pdf/docs/9426.pdf</description>
</package>
<package name="TSOP44-II">
<description>&lt;b&gt;44 lead Plastic Thin Small Outline Type II&lt;/b&gt;&lt;p&gt;
Source: http://us.st.com/stonline/products/literature/ds/7995.pdf</description>
</package>
<package name="TFBGA48">
<description>&lt;b&gt;TFBGA48 6x8mm - 6x8 Active Ball Array, 0.75mm pitch&lt;/b&gt;&lt;p&gt;
Source: http://us.st.com/stonline/products/literature/ds/7995.pdf</description>
</package>
<package name="TQFP-12X12-80">
<description>&lt;b&gt;TQFP80&lt;/b&gt;&lt;p&gt;
Source: www.st.com/stonline/books/pdf/docs/9202.pdf</description>
</package>
<package name="TQFP-10X10-52">
<description>&lt;b&gt;TQFP52&lt;/b&gt;&lt;p&gt;
Source: www.st.com/stonline/books/pdf/docs/9202.pdf</description>
</package>
<package name="MULTIPOWERSO-30">
<description>&lt;b&gt;MultiPowerSO-30&lt;/b&gt;&lt;p&gt;
Source: http://pdf1.alldatasheet.com/datasheet-pdf/view/84563/STMICROELECTRONICS/VNH3SP30.html</description>
</package>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AB</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO44">
<description>&lt;B&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="TSOP48">
<description>&lt;B&gt;Thin Small Outline Plastic Package&lt;/b&gt;</description>
</package>
<package name="DIL24S">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="SO24W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AA</description>
</package>
<package name="SO28X">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
extra wide body 8.9 mm/JEDEC MO-120AB</description>
</package>
<package name="MULTIWATT-11">
<description>&lt;b&gt;Muliwatt 11 lead&lt;/b&gt;</description>
</package>
<package name="MULTIWATT-15">
<description>&lt;b&gt;Multiwatt 15 lead&lt;/b&gt;</description>
</package>
<package name="PBGA-388">
<description>&lt;b&gt;Plastic Ball Grid Array&lt;/b&gt;</description>
</package>
<package name="POWER-SO10">
<description>&lt;b&gt;Power SO-10&lt;/b&gt;&lt;p&gt;
http://eu.st.com/stonline/ 3732.pdf and 5691.pdf</description>
</package>
<package name="POWERSO-20">
<description>&lt;b&gt;Power Small Outline&lt;/b&gt;</description>
</package>
<package name="POWERSO-36">
<description>&lt;b&gt;Power Small Outline&lt;/b&gt;</description>
</package>
<package name="PQFP144">
<description>&lt;b&gt;Plastic Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PQFP144-28X28">
<description>&lt;b&gt;Plastic Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="SOT323">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="QFPN-28">
<description>&lt;b&gt;QFPN-28&lt;/b&gt; 7x7 x 1.8mm&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/11115/lis3lv02dq.pdf</description>
</package>
<package name="QFN-44-7X7">
<description>&lt;b&gt;QFN-44&lt;/b&gt; (7x7x1.8mm)&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/11020.pdf</description>
</package>
<package name="TSOP32">
<description>&lt;b&gt;Thin Small Outline Package&lt;/b&gt;</description>
</package>
<package name="LCC32">
<description>&lt;b&gt;LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
rectangle</description>
</package>
<package name="DIL32">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="FDIP32">
<description>&lt;b&gt;FDIP32W (F)&lt;/b&gt;&lt;p&gt;
Source: www.st.com</description>
</package>
<package name="SPDIP32">
<description>&lt;b&gt;32-lead shrink plastic DIP (400 ml) package&lt;/b&gt;&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf</description>
</package>
<package name="UFQFPN32">
<description>&lt;b&gt;32-lead ultra thin fine pitch quad flat no-lead package (5 x 5)&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="VFQFPN32">
<description>&lt;b&gt;32-lead very thin fine pitch quad flat no-lead package (5 x 5)&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="LQFP32-7X7">
<description>&lt;b&gt;LQFP-32 package&lt;/b&gt; 7x7 mm case, 0.8 mm lead pitch&lt;/b&gt;&lt;p&gt;
Sourced: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="LQFP44-10X10">
<description>&lt;b&gt;44-pin low profile quad flat package&lt;/b&gt; 10 x 10 mm&lt;p&gt;
Source: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="LQFP48-7X7">
<description>&lt;b&gt;48-pin low profile quad flat package (7 x 7)&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="HSOP8">
<description>&lt;b&gt;HSOP 08&lt;/b&gt; (Exposed pad)&lt;p&gt;
Source: http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00002851.pdf</description>
</package>
<package name="HEPTAW.H">
</package>
<package name="HEPTAWATT">
<description>&lt;b&gt;HEPTAWATT 7&lt;/b&gt;</description>
</package>
<package name="SDIP30">
</package>
<package name="PLCC28">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="S28">
<description>&lt;b&gt;PLCC SOCKET&lt;/b&gt;</description>
</package>
<package name="S-DIL24">
<description>SHRINK DUAL-INLINE-PACKAGE

S-DIL24</description>
</package>
<package name="SIP-9">
</package>
<package name="SO16_NARROW">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
<package name="TQFP64">
<description>&lt;b&gt;64-PIN PLASTIC TQFP&lt;/b&gt; (10x10)&lt;p&gt;
shrink quad flat pack, square&lt;br&gt;
Source: SQFP-S-10X10-64 ipc-smd.lbr</description>
</package>
<package name="HTSSOP28EXP">
<description>HTSSOP28 Exposed Pad</description>
</package>
<package name="PSSO-36TP">
<description>PowerSSO-36 TP package</description>
</package>
</packages>
<symbols>
<symbol name="L297">
<pin name="ENABLE" direction="in"/>
<pin name="SYNC" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="HOME" direction="out"/>
<pin name="A" direction="out"/>
<pin name="INH1" direction="out"/>
<pin name="B" direction="out"/>
<pin name="C" direction="out"/>
<pin name="INH2" direction="out"/>
<pin name="SENS2" direction="out"/>
<pin name="SENS1" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="OSC"/>
<pin name="CW/CCW" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="H/F" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="CNTL" direction="in"/>
<pin name="D" direction="out"/>
</symbol>
<symbol name="L298">
<pin name="SEN_B" direction="in"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="INPUT4" direction="in"/>
<pin name="ENABLE_B" direction="in"/>
<pin name="INPUT3" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="INPUT2" direction="in"/>
<pin name="ENABLE_A" direction="in"/>
<pin name="INPUT1" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="SEN_A" direction="in"/>
</symbol>
<symbol name="L293D">
<pin name="1-2EN" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="2Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="4A" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="3Y" direction="out"/>
<pin name="3A" direction="in"/>
<pin name="3-4EN" direction="in"/>
</symbol>
<symbol name="D-AKAK">
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="D-1">
<pin name="K" direction="pas"/>
</symbol>
<symbol name="REF">
<pin name="REF2" direction="pas"/>
<pin name="REF1" direction="pas"/>
</symbol>
<symbol name="D-2-1">
<pin name="K" direction="pas"/>
</symbol>
<symbol name="C0166BAS">
<pin name="SYSRSTI" direction="in"/>
<pin name="XTALI" direction="in"/>
<pin name="XTALO"/>
<pin name="HCLK" direction="out"/>
<pin name="DEV_CLK" direction="out"/>
<pin name="GCLK2X"/>
<pin name="DCLK"/>
<pin name="SCAN_EN" direction="in"/>
</symbol>
<symbol name="C0166MEM">
<pin name="MA0"/>
<pin name="MA1"/>
<pin name="MA2"/>
<pin name="MA3"/>
<pin name="MA4"/>
<pin name="MA5"/>
<pin name="MA6"/>
<pin name="MA7"/>
<pin name="MA8"/>
<pin name="MA9"/>
<pin name="MA10"/>
<pin name="MA11"/>
<pin name="!RAS0" direction="out"/>
<pin name="!RAS1" direction="out"/>
<pin name="!RAS2" direction="out"/>
<pin name="!RAS3" direction="out"/>
<pin name="!CAS0" direction="out"/>
<pin name="!CAS1" direction="out"/>
<pin name="!CAS2" direction="out"/>
<pin name="!CAS3" direction="out"/>
<pin name="!CAS4" direction="out"/>
<pin name="!CAS5" direction="out"/>
<pin name="!CAS6" direction="out"/>
<pin name="!CAS7" direction="out"/>
<pin name="MD0"/>
<pin name="MD1"/>
<pin name="MD2"/>
<pin name="MD3"/>
<pin name="MD4"/>
<pin name="MD5"/>
<pin name="MD6"/>
<pin name="MD7"/>
<pin name="MD8"/>
<pin name="MD9"/>
<pin name="MD10"/>
<pin name="MD11"/>
<pin name="MD12"/>
<pin name="MD13"/>
<pin name="MD14"/>
<pin name="MD15"/>
<pin name="MD16"/>
<pin name="MD17"/>
<pin name="MD18"/>
<pin name="MD19"/>
<pin name="MD20"/>
<pin name="MD21"/>
<pin name="MD22"/>
<pin name="MD23"/>
<pin name="MD24"/>
<pin name="MD25"/>
<pin name="MD26"/>
<pin name="MD27"/>
<pin name="MD28"/>
<pin name="MD29"/>
<pin name="MD30"/>
<pin name="MD31"/>
<pin name="MD32"/>
<pin name="MD33"/>
<pin name="MD34"/>
<pin name="MD35"/>
<pin name="MD36"/>
<pin name="MD37"/>
<pin name="MD38"/>
<pin name="MD39"/>
<pin name="MD40"/>
<pin name="MD41"/>
<pin name="MD42"/>
<pin name="MD43"/>
<pin name="MD44"/>
<pin name="MD45"/>
<pin name="MD46"/>
<pin name="MD47"/>
<pin name="MD48"/>
<pin name="MD49"/>
<pin name="MD50"/>
<pin name="MD51"/>
<pin name="MD52"/>
<pin name="MD53"/>
<pin name="MD54"/>
<pin name="MD55"/>
<pin name="MD56"/>
<pin name="MD57"/>
<pin name="MD58"/>
<pin name="MD59"/>
<pin name="MD60"/>
<pin name="MD61"/>
<pin name="MD62"/>
<pin name="MD63"/>
<pin name="!MWE"/>
</symbol>
<symbol name="C0166PCI">
<pin name="PCI_CLKI" direction="in"/>
<pin name="PCI_CLKO" direction="out"/>
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
<pin name="!FRAME"/>
<pin name="!TRDY"/>
<pin name="!STOP"/>
<pin name="!DEVSEL"/>
<pin name="PAR"/>
<pin name="!SERR" direction="out"/>
<pin name="!LOCK" direction="in"/>
<pin name="!PCIREQ0" direction="in"/>
<pin name="!PCIREQ1" direction="in"/>
<pin name="!PCIREQ2" direction="in"/>
<pin name="!PCIGNT0" direction="out"/>
<pin name="!PCIGNT1" direction="out"/>
<pin name="!PCIGNT2" direction="out"/>
<pin name="!PCI_INT0" direction="in"/>
<pin name="!PCI_INT1" direction="in"/>
<pin name="!PCI_INT2" direction="in"/>
<pin name="!PCI_INT3" direction="in"/>
<pin name="VDD5@1" direction="pwr"/>
<pin name="VDD5@2" direction="pwr"/>
<pin name="VDD5@3" direction="pwr"/>
<pin name="VDD5@4" direction="pwr"/>
<pin name="CBE0"/>
<pin name="CBE1"/>
<pin name="CBE2"/>
<pin name="CBE3"/>
<pin name="!IRDY"/>
</symbol>
<symbol name="C0166ISA">
<pin name="LA22/!SCS1"/>
<pin name="LA23/!SCS3"/>
<pin name="LA20/!PCS1"/>
<pin name="LA21/!PCS3"/>
<pin name="LA17/DA0" direction="out"/>
<pin name="LA18/DA1" direction="out"/>
<pin name="LA19/DA2" direction="out"/>
<pin name="!RMRTC!/DD15"/>
<pin name="!KBCS!/DD14"/>
<pin name="!RTCRW!/DD13"/>
<pin name="!RTCDS!/DD12"/>
<pin name="SA8/DD0"/>
<pin name="SA9/DD1"/>
<pin name="SA10/DD2"/>
<pin name="SA11/DD3"/>
<pin name="SA12/DD4"/>
<pin name="SA13/DD5"/>
<pin name="SA14/DD6"/>
<pin name="SA15/DD7"/>
<pin name="SA16/DD8"/>
<pin name="SA17/DD9"/>
<pin name="SA18/DD10"/>
<pin name="SA19/DD11"/>
<pin name="SA0"/>
<pin name="SA1"/>
<pin name="SA2"/>
<pin name="SA3"/>
<pin name="SA4"/>
<pin name="SA5"/>
<pin name="SA6"/>
<pin name="SA7"/>
<pin name="SD0"/>
<pin name="SD1"/>
<pin name="SD2"/>
<pin name="SD3"/>
<pin name="SD4"/>
<pin name="SD5"/>
<pin name="SD6"/>
<pin name="SD7"/>
<pin name="SD8"/>
<pin name="SD9"/>
<pin name="SD10"/>
<pin name="SD11"/>
<pin name="SD12"/>
<pin name="SD13"/>
<pin name="SD14"/>
<pin name="SD15"/>
<pin name="IOCHRDY"/>
<pin name="!SYSRSTO" direction="out"/>
<pin name="ISA_CLK" direction="out"/>
<pin name="ISA_CLK2X" direction="out"/>
<pin name="OSC14M" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!BHE"/>
<pin name="!MEMR"/>
<pin name="!SMEMR" direction="out"/>
<pin name="!IOW"/>
<pin name="!MASTER" direction="in"/>
<pin name="!MCS16" direction="in"/>
<pin name="!REF" direction="out"/>
<pin name="AEN" direction="out"/>
<pin name="!ZWS" direction="in"/>
<pin name="!IOCHCK" direction="in"/>
<pin name="!ISAOE" direction="out"/>
<pin name="!RTCAS" direction="out"/>
<pin name="!GPIOCS"/>
<pin name="!MEMW"/>
<pin name="!SMEMW" direction="out"/>
<pin name="!IOR"/>
<pin name="!IOCS16" direction="in"/>
</symbol>
<symbol name="C0166MON">
<pin name="BLUE" direction="out"/>
<pin name="VSYNC" direction="out"/>
<pin name="HSYNC" direction="out"/>
<pin name="VREF_DAC" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="SLC/DDC1"/>
<pin name="SDA/DDC0"/>
<pin name="VCLK" direction="in"/>
<pin name="VIN0" direction="in"/>
<pin name="BLUE_TV" direction="out"/>
<pin name="VCS" direction="out"/>
<pin name="ODD_EVEN" direction="out"/>
<pin name="CVBS" direction="out"/>
<pin name="IREF1_TV" direction="in"/>
<pin name="VREF1_TV" direction="in"/>
<pin name="IREF2_TV" direction="in"/>
<pin name="VREF2_TV" direction="in"/>
<pin name="VSSA_TV" direction="in"/>
<pin name="VDDA_TV" direction="in"/>
<pin name="GREEN" direction="out"/>
<pin name="RED" direction="out"/>
<pin name="GREEN_TV" direction="out"/>
<pin name="RED_TV" direction="out"/>
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="VIN3" direction="in"/>
<pin name="VIN4" direction="in"/>
<pin name="VIN5" direction="in"/>
<pin name="VIN6" direction="in"/>
<pin name="VIN7" direction="in"/>
<pin name="VDD_DAC1" direction="in"/>
<pin name="VDD_DAC2" direction="in"/>
<pin name="VDDGCKPLL" direction="in"/>
<pin name="VDDDCKPLL" direction="in"/>
<pin name="VDDHCKPLL" direction="in"/>
<pin name="VDDDEVPLL" direction="in"/>
<pin name="VSS_DAC1" direction="in"/>
<pin name="VSS_DAC2" direction="in"/>
<pin name="VSS_DLL1" direction="in"/>
<pin name="VSS_DLL2" direction="in"/>
</symbol>
<symbol name="C0166IDE">
<pin name="PIRQ" direction="in"/>
<pin name="SIRQ" direction="in"/>
<pin name="PDRQ" direction="in"/>
<pin name="SDRQ" direction="in"/>
<pin name="!PDACK" direction="out"/>
<pin name="!SDACK" direction="out"/>
<pin name="!PIOR"/>
<pin name="!PIOW" direction="out"/>
<pin name="!SIOR"/>
<pin name="!SIOW" direction="out"/>
<pin name="IRQ_MUX0" direction="in"/>
<pin name="IRQ_MUX1" direction="in"/>
<pin name="IRQ_MUX2" direction="in"/>
<pin name="IRQ_MUX3" direction="in"/>
<pin name="DREA_MUX0" direction="in"/>
<pin name="DREA_MUX1" direction="in"/>
<pin name="DACK_ENC0" direction="out"/>
<pin name="DACK_ENC1" direction="out"/>
<pin name="DACK_ENC2" direction="out"/>
<pin name="TC" direction="out"/>
<pin name="SPKRD" direction="out"/>
</symbol>
<symbol name="VDD">
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="VSS">
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="RESERVED">
<pin name="RESERVED" direction="nc"/>
</symbol>
<symbol name="F168_C">
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="!RSTIN" direction="in"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="!NMI" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="!EA" direction="in"/>
<pin name="!READY" direction="in"/>
<pin name="!!WR_WRL" direction="out"/>
<pin name="VPP/RPD" direction="in"/>
</symbol>
<symbol name="F168_P0">
<pin name="P0L1/AD1"/>
<pin name="P0L2/AD2"/>
<pin name="P0L3/AD3"/>
<pin name="P0L4/AD4"/>
<pin name="P0L5/AD5"/>
<pin name="P0L6/AD6"/>
<pin name="P0L7/AD7"/>
<pin name="P0H0/AD8"/>
<pin name="P0H1/AD9"/>
<pin name="P0H2/AD10"/>
<pin name="P0H3/AD11"/>
<pin name="P0H4/AD12"/>
<pin name="P0H5/AD13"/>
<pin name="P0H6/AD14"/>
<pin name="P0H7/AD15"/>
<pin name="P0L0/AD0"/>
</symbol>
<symbol name="F168_P1">
<pin name="P1L0/A0"/>
<pin name="P1L1/A1"/>
<pin name="P1L2/A2"/>
<pin name="P1L3/A3"/>
<pin name="P1L4/A4"/>
<pin name="P1L5/A5"/>
<pin name="P1L6/A6"/>
<pin name="P1L7/A7"/>
<pin name="P1H0/A8"/>
<pin name="P1H1/A9"/>
<pin name="P1H2/A10"/>
<pin name="P1H3/A11"/>
<pin name="P1H4/A12"/>
<pin name="P1H5/13"/>
<pin name="P1H6/A14"/>
<pin name="P1H7/A15"/>
</symbol>
<symbol name="F168_P2">
<pin name="P2-0/CC0"/>
<pin name="P2-1/CC1"/>
<pin name="P2-2/CC2"/>
<pin name="P2-3/CC3"/>
<pin name="P2-4/CC4"/>
<pin name="P2-5/CC5"/>
<pin name="P2-6/CC6"/>
<pin name="P2-7/CC7"/>
<pin name="P2-8/CC8"/>
<pin name="P2-9/CC9"/>
<pin name="P2-10/CC10"/>
<pin name="P2-11/CC11"/>
<pin name="P2-12/CC12"/>
<pin name="P2-13/CC13"/>
<pin name="P2-14/CC14"/>
<pin name="P2-15/CC15"/>
</symbol>
<symbol name="F168_P3">
<pin name="P3-0/TOIN"/>
<pin name="P3-1/T6OUT"/>
<pin name="P3-2/CAPIN"/>
<pin name="P3-3/T3OUT"/>
<pin name="P3-4/T3EUD"/>
<pin name="P3-5/T4IN"/>
<pin name="P3-6/T3IN"/>
<pin name="P3-7/T2IN"/>
<pin name="P3-8/MRST"/>
<pin name="P3-9/MTSR"/>
<pin name="P3-10/TXD0"/>
<pin name="P3-11/RXD0"/>
<pin name="P3-12/!BHE"/>
<pin name="P3-13/SCLK"/>
<pin name="P3-15/CLKO"/>
</symbol>
<symbol name="F168_P4">
<pin name="P4-0/A16"/>
<pin name="P4-1/A17"/>
<pin name="P4-2/A18"/>
<pin name="P4-3/A19"/>
<pin name="P4-4/A20"/>
<pin name="P4-5/A21"/>
<pin name="P4-6/A22"/>
<pin name="P4-7/A23"/>
</symbol>
<symbol name="F168_P5">
<pin name="P5-0/AN0" direction="in"/>
<pin name="P5-1/AN1" direction="in"/>
<pin name="P5-2/AN2" direction="in"/>
<pin name="P5-3/AN3" direction="in"/>
<pin name="P5-4/AN4" direction="in"/>
<pin name="P5-5/AN5" direction="in"/>
<pin name="P5-6/AN6" direction="in"/>
<pin name="P5-7/AN7" direction="in"/>
<pin name="P5-8/AN8" direction="in"/>
<pin name="P5-9/AN9" direction="in"/>
<pin name="P5-10/AN10" direction="in"/>
<pin name="P5-11/AN11" direction="in"/>
<pin name="P5-12/AN12" direction="in"/>
<pin name="P5-13/AN13" direction="in"/>
<pin name="P5-14/AN14" direction="in"/>
<pin name="P5-15/AN15" direction="in"/>
</symbol>
<symbol name="F168_P6">
<pin name="P6-0/!SC0"/>
<pin name="P6-1/!CS1"/>
<pin name="P6-2/!CS2"/>
<pin name="P6-3/!CS3"/>
<pin name="P6-4/!CS4"/>
<pin name="P6-5/!HOLD"/>
<pin name="!!P6-6HLDA"/>
<pin name="P6-7/!BREQ"/>
</symbol>
<symbol name="F168_P7">
<pin name="!P7-0POUT0"/>
<pin name="P7-1/POUT1"/>
<pin name="P7-2/POUT2"/>
<pin name="P7-3/POUT3"/>
<pin name="P7-4/CC28"/>
<pin name="P7-5/CC29"/>
<pin name="P7-6/CC30"/>
<pin name="P7-7/CC31"/>
</symbol>
<symbol name="F168_P8">
<pin name="P8-0/CC16"/>
<pin name="P8-1/CC17"/>
<pin name="P8-2/CC18"/>
<pin name="P8-3/CC19"/>
<pin name="P8-4/CC20"/>
<pin name="P8-5/CC21"/>
<pin name="P8-6/CC22"/>
<pin name="P8-7/CC23"/>
</symbol>
<symbol name="M29F400">
<pin name="!WE" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="!RB" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="A-1/D15" direction="hiz"/>
<pin name="!BYTE" direction="in"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="ST95P08">
<pin name="!HOLD" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="!S" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="Q" direction="hiz"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="STA013">
<pin name="!RESET" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SCKR" direction="in"/>
<pin name="BIT_EN" direction="in"/>
<pin name="!SRC_INT" direction="in"/>
<pin name="OUT/DATA" direction="out"/>
<pin name="XTI" direction="in"/>
<pin name="XTO" direction="out"/>
<pin name="OCLK"/>
<pin name="!TESTEN" direction="in"/>
<pin name="SCANEN" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SCKT" direction="out"/>
<pin name="LRCKT" direction="out"/>
<pin name="FILT" direction="out"/>
</symbol>
<symbol name="STA013PW">
<pin name="PVDD" direction="pwr"/>
<pin name="PVSS" direction="pwr"/>
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
</symbol>
<symbol name="STA015TS">
<pin name="!RESET" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SCKR" direction="in"/>
<pin name="BIT_EN" direction="in"/>
<pin name="SCK_ADC" direction="in"/>
<pin name="DATA-REQ" direction="out"/>
<pin name="XTI" direction="in"/>
<pin name="XTO" direction="out"/>
<pin name="OCLK"/>
<pin name="!TESTEN" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SCKT" direction="out"/>
<pin name="LRCKT" direction="out"/>
<pin name="FILT" direction="out"/>
<pin name="CRCK_ADC" direction="in"/>
<pin name="SDI_ADC" direction="in"/>
<pin name="GPSO_REQ" direction="out"/>
<pin name="GPSO_SCKL" direction="out"/>
<pin name="GPSO_DATA" direction="out"/>
<pin name="IODATA0"/>
<pin name="IODATA1"/>
<pin name="IODATA2"/>
<pin name="IODATA3"/>
<pin name="IODATA4"/>
<pin name="IODATA5"/>
<pin name="IODATA6"/>
<pin name="IODATA7"/>
<pin name="GPIO_STRB"/>
</symbol>
<symbol name="STA015S">
<pin name="!RESET" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SCKR" direction="in"/>
<pin name="BIT_EN" direction="in"/>
<pin name="SCK_ADC" direction="in"/>
<pin name="DATA-REQ" direction="out"/>
<pin name="XTI" direction="in"/>
<pin name="XTO" direction="out"/>
<pin name="OCLK"/>
<pin name="!TESTEN" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SCKT" direction="out"/>
<pin name="LRCKT" direction="out"/>
<pin name="FILT" direction="out"/>
<pin name="CRCK_ADC" direction="in"/>
<pin name="SDI_ADC" direction="in"/>
</symbol>
<symbol name="STA015PW">
<pin name="PVDD" direction="pwr"/>
<pin name="PVSS" direction="pwr"/>
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
</symbol>
<symbol name="STV5730A">
<pin name="RES" direction="in"/>
<pin name="XTAL_IN" direction="in"/>
<pin name="XTAL_OUT" direction="out"/>
<pin name="CSYNC"/>
<pin name="CLK" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="CSN" direction="in"/>
<pin name="FTR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="MUTE" direction="out"/>
<pin name="LECHAR" direction="in"/>
<pin name="LESCREEN" direction="in"/>
<pin name="YOUT" direction="out"/>
<pin name="CO" direction="out"/>
<pin name="FB" direction="out"/>
<pin name="B" direction="out"/>
<pin name="G" direction="out"/>
<pin name="R" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="VIDEOOUT2" direction="out"/>
<pin name="VIDEOOUT1" direction="out"/>
<pin name="YIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="VIDEO_IN" direction="in"/>
<pin name="BAR" direction="in"/>
</symbol>
<symbol name="VN460SP">
<pin name="IN" direction="in"/>
<pin name="ST" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="L620X">
<pin name="CBOOT2" direction="in"/>
<pin name="OUT2" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="CBOOT1" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
</symbol>
<symbol name="L6203">
<pin name="CBOOT2" direction="in"/>
<pin name="OUT2" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="CBOOT1" direction="in"/>
<pin name="SENSE" direction="in"/>
</symbol>
<symbol name="L6201">
<pin name="CBOOT2" direction="in"/>
<pin name="OUT2" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="CBOOT1" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="L6204">
<pin name="OUT2" direction="out"/>
<pin name="VBOOT" direction="in"/>
<pin name="VS1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="ENABLE1" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="BOOTSTRAP" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="SENSE1" direction="in"/>
<pin name="SENSE2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="ENABLE2" direction="in"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="VS2" direction="pwr"/>
</symbol>
<symbol name="L6115">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
</symbol>
<symbol name="L6122">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="IN3" direction="in"/>
</symbol>
<symbol name="L6205">
<pin name="OUT2A" direction="out"/>
<pin name="VCP" direction="pwr"/>
<pin name="VS_A" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2_A" direction="in"/>
<pin name="EN_A" direction="in"/>
<pin name="IN1_A" direction="in"/>
<pin name="OUT1A" direction="out"/>
<pin name="SENSE_B" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="IN1_B" direction="in"/>
<pin name="IN2_B" direction="in"/>
<pin name="EN_B" direction="in"/>
<pin name="OUT1B" direction="out"/>
<pin name="OUT2B" direction="out"/>
<pin name="VS_B" direction="pwr"/>
<pin name="SENSE_A" direction="in"/>
<pin name="VBOOT" direction="pwr"/>
</symbol>
<symbol name="L6207">
<pin name="OUT2A" direction="out"/>
<pin name="VCP" direction="pwr"/>
<pin name="VS_A" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2_A" direction="in"/>
<pin name="EN_A" direction="in"/>
<pin name="IN1_A" direction="in"/>
<pin name="OUT1A" direction="out"/>
<pin name="SENSE_B" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="IN1_B" direction="in"/>
<pin name="IN2_B" direction="in"/>
<pin name="EN_B" direction="in"/>
<pin name="OUT1B" direction="out"/>
<pin name="OUT2B" direction="out"/>
<pin name="VS_B" direction="pwr"/>
<pin name="SENSE_A" direction="in"/>
<pin name="VBOOT" direction="pwr"/>
<pin name="RCA" direction="in"/>
<pin name="RCB" direction="in"/>
<pin name="VREF_A" direction="in"/>
<pin name="VREF_B" direction="in"/>
</symbol>
<symbol name="TAE3718">
<pin name="REFERENCE" direction="in"/>
<pin name="VSB" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ALARM" direction="oc"/>
<pin name="IN0" direction="in"/>
<pin name="PULSE-TIME" direction="pas"/>
<pin name="IN1" direction="in"/>
<pin name="COMP-IN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="VSA" direction="pwr"/>
<pin name="PHASE" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="TAE3718D">
<pin name="REFERENCE" direction="in"/>
<pin name="VSB" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN0" direction="in"/>
<pin name="PULSE-TIME" direction="pas"/>
<pin name="IN1" direction="in"/>
<pin name="COMP-IN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="VSA" direction="pwr"/>
<pin name="PHASE" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="L9637D">
<pin name="VS" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="K" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="TX" direction="in"/>
<pin name="RX" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="M68AW128M">
<pin name="!LB" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="!E" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!UB" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
<pin name="!W" direction="in"/>
<pin name="!G" direction="in"/>
</symbol>
<symbol name="VCC2-VSS2">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="UPSD325*-52">
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4"/>
<pin name="P3.5"/>
<pin name="P3.6"/>
<pin name="P3.7"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PD1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC7"/>
<pin name="USB+"/>
<pin name="USB-"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VREF" direction="out"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="UPSD325*-80">
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4"/>
<pin name="P3.5"/>
<pin name="P3.6"/>
<pin name="P3.7"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PD1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC7"/>
<pin name="USB+"/>
<pin name="USB-"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VREF" direction="out"/>
<pin name="PD2"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="ALE" direction="out"/>
<pin name="AD0" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="AD3" direction="in"/>
<pin name="AD4" direction="in"/>
<pin name="AD5" direction="in"/>
<pin name="AD6" direction="in"/>
<pin name="AD7" direction="in"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="!WR" direction="out"/>
<pin name="!PSEN" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="NE555">
<pin name="TRE" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="DIS" direction="in"/>
<pin name="TRI" direction="in"/>
<pin name="VCC+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CON" direction="in"/>
<pin name="/RES" direction="in"/>
</symbol>
<symbol name="NE556">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CONT1" direction="in"/>
<pin name="RESET1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="TRES1" direction="in"/>
<pin name="TRIG1" direction="in"/>
<pin name="DIS1" direction="in"/>
<pin name="TRES2" direction="in"/>
<pin name="TRIG2" direction="in"/>
<pin name="DIS2" direction="in"/>
<pin name="RESET2" direction="in"/>
<pin name="CONT2" direction="in"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="VNH3SP30">
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="DIAGA" direction="oc"/>
<pin name="DIAGB" direction="oc"/>
<pin name="PWM" direction="in"/>
<pin name="GNDA" direction="pwr"/>
<pin name="GNDB" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA@1" direction="pas"/>
<pin name="OUTA@2" direction="pas"/>
<pin name="OUTB@1" direction="pas"/>
<pin name="OUTB@2" direction="pas"/>
<pin name="GNDB@1" direction="pwr"/>
<pin name="GNDB@2" direction="pwr"/>
<pin name="GNDA@1" direction="pwr"/>
<pin name="GNDA@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="OUTB@3" direction="pas"/>
<pin name="OUTB@4" direction="pas"/>
<pin name="OUTA@3" direction="pas"/>
<pin name="OUTA@4" direction="pas"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
</symbol>
<symbol name="USB6B1">
<pin name="VCC" direction="pwr"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="IO2@2"/>
<pin name="IO1@2"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="STV5348">
<pin name="VSSD" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSSO" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="TEST" direction="pas"/>
<pin name="RESERVED" direction="pas"/>
<pin name="XTO" direction="out"/>
<pin name="B" direction="out"/>
<pin name="G" direction="out"/>
<pin name="R" direction="out"/>
<pin name="Y" direction="oc"/>
<pin name="ODD/EVEN" direction="out"/>
<pin name="COR" direction="oc"/>
<pin name="BLAN" direction="out"/>
<pin name="L23" direction="out"/>
<pin name="DV" direction="out"/>
<pin name="XTI" direction="in"/>
<pin name="RGBREF" direction="pwr"/>
<pin name="STTV/LFB"/>
<pin name="VCR/TV" direction="in"/>
<pin name="POL" direction="in"/>
<pin name="MA/SL" direction="in"/>
<pin name="CBLK"/>
<pin name="CVBS" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="FFB" direction="in"/>
</symbol>
<symbol name="LIS3LV02DQ">
<pin name="CS" direction="in"/>
<pin name="SCL/SPC" direction="in"/>
<pin name="SDA/SDO/SDI"/>
<pin name="SDO" direction="out"/>
<pin name="RDY/INT"/>
<pin name="VDD_IO" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="CK" direction="in"/>
</symbol>
<symbol name="LIS3L02AQ3">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VOUTY" direction="out"/>
<pin name="PD" direction="in"/>
<pin name="ST" direction="in"/>
<pin name="VOUTX" direction="out"/>
<pin name="VOUTZ" direction="out"/>
<pin name="FS" direction="in"/>
</symbol>
<symbol name="M27C4001">
<pin name="VCC" direction="pwr"/>
<pin name="VPP" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="!G" direction="in"/>
<pin name="!E" direction="in"/>
</symbol>
<symbol name="STM8S105C4-48">
<pin name="NRST"/>
<pin name="PA1/OSC"/>
<pin name="PA2/OSCOUT"/>
<pin name="VSSIO_1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDIO_1" direction="pwr"/>
<pin name="PA3/TIM2_CH3[TIM3_CH1]"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PB7/AIN7"/>
<pin name="PB6/AIN6"/>
<pin name="PB5/AIN5[I2C_SDA]"/>
<pin name="PB4/AIN4[I2C_SCL]"/>
<pin name="PB3/AIN3[TIM1_ETR]"/>
<pin name="PB2/AIN2[TIM1_CH3N]"/>
<pin name="PB1/AIN1[TIM1_CH2N]"/>
<pin name="PB0/AIN0[TIM1_CH1N]"/>
<pin name="PE7/AIN8"/>
<pin name="PE6/AIN9"/>
<pin name="PE5/SPI_NSS"/>
<pin name="PC1/TIM1_CH1/UART2_CK"/>
<pin name="PC2/TIM1_CH2"/>
<pin name="PC3/TIM1_CH3"/>
<pin name="PC4/TIM1_CH4"/>
<pin name="PC5/SPI_SCK"/>
<pin name="VSSIO_2" direction="pwr"/>
<pin name="VDDIO_2" direction="pwr"/>
<pin name="PC6/SPI_MOSI"/>
<pin name="PC7/SPI_MISO"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PE3/TIM1_BKIN"/>
<pin name="PE2/I2C_SDA"/>
<pin name="PE1/I2C_SCL"/>
<pin name="PE0/CLK_CCO"/>
<pin name="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]"/>
<pin name="PD1/SWIM"/>
<pin name="PD2/TIM3_CH1[TIM2_CH3]"/>
<pin name="PD3/TIM2_CH2[ADC_ETR]"/>
<pin name="PD4/TIM2_CH1[BEEP]"/>
<pin name="PD5/UART2_TX"/>
<pin name="PD6/UART2_RX"/>
<pin name="PD7/TLI[TIM1_CH4]"/>
</symbol>
<symbol name="STM8S105C4-44">
<pin name="NRST"/>
<pin name="PA1/OSC"/>
<pin name="PA2/OSCOUT"/>
<pin name="VSSIO_1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDIO_1" direction="pwr"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PB7/AIN7"/>
<pin name="PB6/AIN6"/>
<pin name="PB5/AIN5[I2C_SDA]"/>
<pin name="PB4/AIN4[I2C_SCL]"/>
<pin name="PB3/AIN3[TIM1_ETR]"/>
<pin name="PB2/AIN2[TIM1_CH3N]"/>
<pin name="PB1/AIN1[TIM1_CH2N]"/>
<pin name="PB0/AIN0[TIM1_CH1N]"/>
<pin name="PE6/AIN9"/>
<pin name="PE5/SPI_NSS"/>
<pin name="PC1/TIM1_CH1/UART2_CK"/>
<pin name="PC2/TIM1_CH2"/>
<pin name="PC3/TIM1_CH3"/>
<pin name="PC5/SPI_SCK"/>
<pin name="VSSIO_2" direction="pwr"/>
<pin name="VDDIO_2" direction="pwr"/>
<pin name="PC6/SPI_MOSI"/>
<pin name="PC7/SPI_MISO"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PE2/I2C_SDA"/>
<pin name="PE1/I2C_SCL"/>
<pin name="PE0/CLK_CCO"/>
<pin name="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]"/>
<pin name="PD1/SWIM"/>
<pin name="PD2/TIM3_CH1[TIM2_CH3]"/>
<pin name="PD3/TIM2_CH2[ADC_ETR]"/>
<pin name="PD4/TIM2_CH1[BEEP]"/>
<pin name="PD5/UART2_TX"/>
<pin name="PD6/UART2_RX"/>
<pin name="PD7/TLI[TIM1_CH4]"/>
</symbol>
<symbol name="STM8S105C4-32">
<pin name="NRST"/>
<pin name="PA1/OSC"/>
<pin name="PA2/OSCOUT"/>
<pin name="VSS" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDIO_1" direction="pwr"/>
<pin name="PF4/AIN12"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PB5/AIN5[I2C_SDA]"/>
<pin name="PB4/AIN4[I2C_SCL]"/>
<pin name="PB3/AIN3[TIM1_ETR]"/>
<pin name="PB2/AIN2[TIM1_CH3N]"/>
<pin name="PB1/AIN1[TIM1_CH2N]"/>
<pin name="PB0/AIN0[TIM1_CH1N]"/>
<pin name="PE5/SPI_NSS"/>
<pin name="PC1/TIM1_CH1/UART2_CK"/>
<pin name="PC2/TIM1_CH2"/>
<pin name="PC3/TIM1_CH3"/>
<pin name="PC4/TIM1_CH4"/>
<pin name="PC5/SPI_SCK"/>
<pin name="PC6/SPI_MOSI"/>
<pin name="PC7/SPI_MISO"/>
<pin name="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]"/>
<pin name="PD1/SWIM"/>
<pin name="PD2/TIM3_CH1[TIM2_CH3]"/>
<pin name="PD3/TIM2_CH2[ADC_ETR]"/>
<pin name="PD4/TIM2_CH1[BEEP]"/>
<pin name="PD5/UART2_TX"/>
<pin name="PD6/UART2_RX"/>
<pin name="PD7/TLI[TIM1_CH4]"/>
</symbol>
<symbol name="STM8S105C4-32P">
<pin name="PD3/TIM2_CH2[ADC_ETR]"/>
<pin name="PD4/TIM2_CH1[BEEP]"/>
<pin name="PD5/UART2_TX"/>
<pin name="PD6/UART2_RX"/>
<pin name="PD7/TLI[TIM1_CH4]"/>
<pin name="NRST"/>
<pin name="PA1/OSC"/>
<pin name="PA2/OSCOUT"/>
<pin name="VSS" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDIO_1" direction="pwr"/>
<pin name="PF4/AIN12"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PB5/AIN5[I2C_SDA]"/>
<pin name="PB4/AIN4[I2C_SCL]"/>
<pin name="PB3/AIN3[TIM1_ETR]"/>
<pin name="PB2/AIN2[TIM1_CH3N]"/>
<pin name="PB1/AIN1[TIM1_CH2N]"/>
<pin name="PB0/AIN0[TIM1_CH1N]"/>
<pin name="PE5/SPI_NSS"/>
<pin name="PC1/TIM1_CH1/UART2_CK"/>
<pin name="PC2/TIM1_CH2"/>
<pin name="PC3/TIM1_CH3"/>
<pin name="PC4/TIM1_CH4"/>
<pin name="PC5/SPI_SCK"/>
<pin name="PC6/SPI_MOSI"/>
<pin name="PC7/SPI_MISO"/>
<pin name="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]"/>
<pin name="PD1/SWIM"/>
<pin name="PD2/TIM3_CH1[TIM2_CH3]"/>
</symbol>
<symbol name="L293DD">
<pin name="EN1" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="IN2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="IN3" direction="in"/>
<pin name="OUT4" direction="out"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="OUT3" direction="out"/>
<pin name="IN4" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
</symbol>
<symbol name="L5973D">
<pin name="VREF" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="INH" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="EXPOSEDPAD">
<pin name="EXP" direction="in"/>
</symbol>
<symbol name="L4960">
<pin name="1/IN" direction="in"/>
<pin name="2/FEED.IN" direction="in"/>
<pin name="3/F.COMP"/>
<pin name="4/GND" direction="pwr"/>
<pin name="5/OSC"/>
<pin name="6/SOF.START"/>
<pin name="7/OUT" direction="out"/>
</symbol>
<symbol name="TDA7439DS">
<pin name="1/RIN3" direction="in"/>
<pin name="2/RIN2" direction="in"/>
<pin name="3/RIN1" direction="in"/>
<pin name="4/LIN1" direction="in"/>
<pin name="5/LIN2" direction="in"/>
<pin name="6/LIN3" direction="in"/>
<pin name="7/LIN4" direction="in"/>
<pin name="8/MUXOUTL" direction="out"/>
<pin name="9/MUXOUTR" direction="out"/>
<pin name="10/MINR"/>
<pin name="11/MOUTR" direction="out"/>
<pin name="12/BINR"/>
<pin name="13/BOUTR" direction="out"/>
<pin name="14/BINL"/>
<pin name="15/BOUTL" direction="out"/>
<pin name="16/MOUTL" direction="out"/>
<pin name="17/MINL"/>
<pin name="18/TREL"/>
<pin name="19/TRER"/>
<pin name="20/DGND" direction="pwr"/>
<pin name="21/SCL"/>
<pin name="22/SDA"/>
<pin name="23/CREF"/>
<pin name="24/VS" direction="pwr"/>
<pin name="25/AGND" direction="pwr"/>
<pin name="26/ROUT" direction="out"/>
<pin name="27/LOUT" direction="out"/>
<pin name="28/RIN4" direction="in"/>
</symbol>
<symbol name="TDA7439">
<pin name="1/SDA"/>
<pin name="2/CREF"/>
<pin name="3/VS" direction="pwr"/>
<pin name="4/AGND" direction="pwr"/>
<pin name="5/ROUT" direction="out"/>
<pin name="6/LOUT" direction="out"/>
<pin name="7/RIN4" direction="in"/>
<pin name="8/RIN3" direction="in"/>
<pin name="9/RIN2" direction="in"/>
<pin name="10/RIN1" direction="in"/>
<pin name="11/LIN1" direction="in"/>
<pin name="12/LIN2" direction="in"/>
<pin name="13/LIN3" direction="in"/>
<pin name="14/LIN4" direction="in"/>
<pin name="15/MUXOUTL" direction="out"/>
<pin name="16/INL" direction="in"/>
<pin name="17/MUXOUTR" direction="out"/>
<pin name="18/INR" direction="in"/>
<pin name="19/MINR" direction="in"/>
<pin name="20/MOUTR" direction="out"/>
<pin name="21/BINR" direction="in"/>
<pin name="22/BOUTR" direction="out"/>
<pin name="23/BINL" direction="in"/>
<pin name="24/BOUTL" direction="out"/>
<pin name="25/MOUTL" direction="out"/>
<pin name="26/MINL" direction="in"/>
<pin name="27/TREL"/>
<pin name="28/TRER"/>
<pin name="29/DIGND" direction="pwr"/>
<pin name="30/SCL"/>
</symbol>
<symbol name="L6232B">
<pin name="INUA" direction="in" function="dot"/>
<pin name="INUB" direction="in" function="dot"/>
<pin name="INUC" direction="in" function="dot"/>
<pin name="INLA" direction="in"/>
<pin name="INLB" direction="in"/>
<pin name="INLC" direction="in"/>
<pin name="LIN_VREF" direction="in"/>
<pin name="PWM_VREV" direction="in"/>
<pin name="BRK" direction="in" function="dot"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="BRK_DLY" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="SENSE1" direction="out"/>
<pin name="SENSE2" direction="out"/>
<pin name="GND" direction="sup"/>
<pin name="VS1" direction="pwr"/>
<pin name="VS2" direction="pwr"/>
<pin name="CP" direction="pas"/>
<pin name="CS" direction="pas"/>
</symbol>
<symbol name="TEA6420">
<pin name="L1" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="L2" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="L3" direction="in"/>
<pin name="R3" direction="in"/>
<pin name="L4" direction="in"/>
<pin name="R4" direction="in"/>
<pin name="L5" direction="in"/>
<pin name="R5" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="C" direction="pas"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="ADDR" direction="in"/>
<pin name="ROUT4" direction="out"/>
<pin name="LOUT4" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="LOUT3" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="LOUT2" direction="out"/>
<pin name="ROUT1" direction="out"/>
<pin name="LOUT1" direction="out"/>
</symbol>
<symbol name="L9686">
<pin name="DGND" direction="pwr"/>
<pin name="+V" direction="pwr"/>
<pin name="OUT/REL" direction="out"/>
<pin name="COSC"/>
<pin name="ROSC"/>
<pin name="NC" direction="nc"/>
<pin name="LFD" direction="out"/>
<pin name="STR" direction="in"/>
</symbol>
<symbol name="TDA8137">
<pin name="VIN" direction="in"/>
<pin name="VOUT1" direction="out"/>
<pin name="DISAB" direction="in"/>
<pin name="DELAY" direction="out"/>
<pin name="GND" direction="sup"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="TDA8138A/B">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="DIS/CAPA"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
</symbol>
<symbol name="TDA8138">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="DEL/CAP"/>
<pin name="DIS"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET"/>
<pin name="NC" direction="nc"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
</symbol>
<symbol name="SG2525/3525">
<pin name="INV.IN" direction="in"/>
<pin name="NI.IN" direction="in"/>
<pin name="SYNC"/>
<pin name="OSC.OUT" direction="out"/>
<pin name="CT"/>
<pin name="RT"/>
<pin name="DRSCH"/>
<pin name="SOFT_ST"/>
<pin name="COME"/>
<pin name="SHUT"/>
<pin name="OUT_A" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VC" direction="pwr"/>
<pin name="OUT_B" direction="out"/>
<pin name="+VJ" direction="pwr"/>
<pin name="VREF"/>
</symbol>
<symbol name="STR711F">
<pin name="P0.10/U1.RX/U1.TX/SCDATA"/>
<pin name="P0.11/U1.TX/BOOT.1"/>
<pin name="P0.12/SCCCLK"/>
<pin name="VSS_1"/>
<pin name="P0.13/U2.RX/T2.OCMPA"/>
<pin name="P0.14/U2.TX/T2.ICAPA"/>
<pin name="BOOTEN"/>
<pin name="VSS_2"/>
<pin name="V33_1"/>
<pin name="JTDI"/>
<pin name="JTMS"/>
<pin name="JTCK"/>
<pin name="JTDO"/>
<pin name="NJTRST"/>
<pin name="NU"/>
<pin name="TEST"/>
<pin name="V33IO-PLL_1"/>
<pin name="VSSIO-PLL_1"/>
<pin name="CK"/>
<pin name="P0.15/WAKEUP"/>
<pin name="RTCXTI"/>
<pin name="RTCXTO"/>
<pin name="NSTDBY"/>
<pin name="NRSTIN"/>
<pin name="VSSBKP"/>
<pin name="V18BKP"/>
<pin name="V18_1"/>
<pin name="VSS18_1"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="P1.0/T3.OCMPB/AIN.0"/>
<pin name="P1.1/T3.ICAPA/AIN.1"/>
<pin name="P1.2/T3.OCMPA/AIN.2"/>
<pin name="P1.3/T3.ICAPB/AIN.3"/>
<pin name="P1.4/T1.ICAPA"/>
<pin name="P1.5/T1.ICAPB"/>
<pin name="P1.6/T1.OCMPB"/>
<pin name="V33IO-PLL_2"/>
<pin name="VSSIO-PLL_2"/>
<pin name="P1.7/T1.OCMPA"/>
<pin name="P1.8"/>
<pin name="USBDP+"/>
<pin name="USBDN-"/>
<pin name="VSS_3"/>
<pin name="P1.9"/>
<pin name="P1.10/USBCLK"/>
<pin name="P1.13/HCLK/I0.SCL"/>
<pin name="P1.14/HRXD/I0.SDA"/>
<pin name="P1.15/HTXD"/>
<pin name="VSS_4"/>
<pin name="V33_2"/>
<pin name="P0.0/S0.MISO/U3.TX"/>
<pin name="P0.1/S0.MOSI/U3.RX"/>
<pin name="P0.2/S0.SCLK/I1.SCL"/>
<pin name="P0.3/S0.SSN/I1.SDA"/>
<pin name="P0.4/S1.MISO"/>
<pin name="VSS18_2"/>
<pin name="V18_2"/>
<pin name="VSS_5"/>
<pin name="P0.5/S1.MOSI"/>
<pin name="P0.6/S1.SCLK"/>
<pin name="P0.7/S1.SSN"/>
<pin name="P0.8/U0.RX/U0.TX"/>
<pin name="P0.9/U0.TX/BOOT.0"/>
</symbol>
<symbol name="ST7540">
<pin name="CD_PD"/>
<pin name="REG_DATA"/>
<pin name="GND"/>
<pin name="RXD"/>
<pin name="RXTX"/>
<pin name="TXD"/>
<pin name="BU/THERM"/>
<pin name="CLR/T"/>
<pin name="VDD"/>
<pin name="MCLK"/>
<pin name="RSTO"/>
<pin name="UART/SPI"/>
<pin name="WD"/>
<pin name="PA_IN-"/>
<pin name="TEST2"/>
<pin name="TEST1"/>
<pin name="VDC"/>
<pin name="RX_IN"/>
<pin name="CL"/>
<pin name="VSENCE"/>
<pin name="X2"/>
<pin name="X1"/>
<pin name="SVSS"/>
<pin name="TX_OUT"/>
<pin name="PA_IN+"/>
<pin name="VCC"/>
<pin name="VSS"/>
<pin name="PA_OUT"/>
</symbol>
<symbol name="VNH5050ATR_E">
<pin name="GND_A" direction="pwr"/>
<pin name="DRAIN_LSA" direction="out"/>
<pin name="GND_B" direction="pwr"/>
<pin name="DRAIN_LSB" direction="out"/>
<pin name="SOURCE_HSA" direction="out"/>
<pin name="SOURCE_HSB" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="ENA/DIAGA" direction="oc"/>
<pin name="IN_PWM" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="ENB/DIAGB" direction="oc"/>
<pin name="CS_DIS" direction="out"/>
<pin name="CS" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="L297" prefix="IC">
<description>&lt;b&gt;STEPPER MOTOR CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="L297" symbol="L297"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="L297" pin="A" pad="4"/>
<connect gate="L297" pin="B" pad="6"/>
<connect gate="L297" pin="C" pad="7"/>
<connect gate="L297" pin="CLOCK" pad="18"/>
<connect gate="L297" pin="CNTL" pad="11"/>
<connect gate="L297" pin="CW/CCW" pad="17"/>
<connect gate="L297" pin="D" pad="9"/>
<connect gate="L297" pin="ENABLE" pad="10"/>
<connect gate="L297" pin="GND" pad="2"/>
<connect gate="L297" pin="H/F" pad="19"/>
<connect gate="L297" pin="HOME" pad="3"/>
<connect gate="L297" pin="INH1" pad="5"/>
<connect gate="L297" pin="INH2" pad="8"/>
<connect gate="L297" pin="OSC" pad="16"/>
<connect gate="L297" pin="RESET" pad="20"/>
<connect gate="L297" pin="SENS1" pad="14"/>
<connect gate="L297" pin="SENS2" pad="13"/>
<connect gate="L297" pin="SYNC" pad="1"/>
<connect gate="L297" pin="VCC" pad="12"/>
<connect gate="L297" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L297/1"/>
<attribute name="OC_FARNELL" value="1094209"/>
<attribute name="OC_NEWARK" value="56P8258"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L298" prefix="IC">
<description>&lt;b&gt;DUAL FULL-BRIDGE DRIVER&lt;/b&gt;</description>
<gates>
<gate name="L298" symbol="L298"/>
</gates>
<devices>
<device name="" package="MULTIWATT-15">
<connects>
<connect gate="L298" pin="ENABLE_A" pad="6"/>
<connect gate="L298" pin="ENABLE_B" pad="11"/>
<connect gate="L298" pin="GND" pad="8"/>
<connect gate="L298" pin="INPUT1" pad="5"/>
<connect gate="L298" pin="INPUT2" pad="7"/>
<connect gate="L298" pin="INPUT3" pad="10"/>
<connect gate="L298" pin="INPUT4" pad="12"/>
<connect gate="L298" pin="OUT1" pad="2"/>
<connect gate="L298" pin="OUT2" pad="3"/>
<connect gate="L298" pin="OUT3" pad="13"/>
<connect gate="L298" pin="OUT4" pad="14"/>
<connect gate="L298" pin="SEN_A" pad="1"/>
<connect gate="L298" pin="SEN_B" pad="15"/>
<connect gate="L298" pin="VCC" pad="9"/>
<connect gate="L298" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L298N"/>
<attribute name="OC_FARNELL" value="1589425"/>
<attribute name="OC_NEWARK" value="32M1527"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L293D" prefix="IC">
<description>&lt;b&gt;PUSH-PULL 4 CHANNEL DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L293D"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="1-2EN" pad="1"/>
<connect gate="G$1" pin="1A" pad="2"/>
<connect gate="G$1" pin="1Y" pad="3"/>
<connect gate="G$1" pin="2A" pad="7"/>
<connect gate="G$1" pin="2Y" pad="6"/>
<connect gate="G$1" pin="3-4EN" pad="9"/>
<connect gate="G$1" pin="3A" pad="10"/>
<connect gate="G$1" pin="3Y" pad="11"/>
<connect gate="G$1" pin="4A" pad="15"/>
<connect gate="G$1" pin="4Y" pad="14"/>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="GND4" pad="12"/>
<connect gate="G$1" pin="VCC1" pad="16"/>
<connect gate="G$1" pin="VCC2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L293D"/>
<attribute name="OC_FARNELL" value="9589619"/>
<attribute name="OC_NEWARK" value="56P8249"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DA108S1" prefix="D">
<description>&lt;b&gt;DIODE ARRAY&lt;/b&gt; (ASD)</description>
<gates>
<gate name="_1" symbol="REF"/>
<gate name="-1" symbol="D-1"/>
<gate name="_2" symbol="REF"/>
<gate name="-2" symbol="D-1"/>
<gate name="-3" symbol="D-2-1"/>
<gate name="-4" symbol="D-2-1"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="-1" pin="K" pad="1"/>
<connect gate="-2" pin="K" pad="2"/>
<connect gate="-3" pin="K" pad="3"/>
<connect gate="-4" pin="K" pad="4"/>
<connect gate="_1" pin="REF1" pad="8"/>
<connect gate="_1" pin="REF2" pad="5"/>
<connect gate="_2" pin="REF1" pad="7"/>
<connect gate="_2" pin="REF2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="DA108S1"/>
<attribute name="OC_FARNELL" value="9802215"/>
<attribute name="OC_NEWARK" value="89K0513"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DA112S1" prefix="D">
<description>&lt;b&gt;DIODE ARRAY&lt;/b&gt; (ASD)</description>
<gates>
<gate name="_1" symbol="REF"/>
<gate name="-1" symbol="D-1"/>
<gate name="-2" symbol="D-2-1"/>
<gate name="-3" symbol="D-2-1"/>
<gate name="-4" symbol="D-2-1"/>
<gate name="-5" symbol="D-2-1"/>
<gate name="-6" symbol="D-2-1"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="-1" pin="K" pad="5"/>
<connect gate="-2" pin="K" pad="4"/>
<connect gate="-3" pin="K" pad="3"/>
<connect gate="-4" pin="K" pad="2"/>
<connect gate="-5" pin="K" pad="1"/>
<connect gate="-6" pin="K" pad="7"/>
<connect gate="_1" pin="REF1" pad="8"/>
<connect gate="_1" pin="REF2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="DA112S1"/>
<attribute name="OC_FARNELL" value="9802223"/>
<attribute name="OC_NEWARK" value="89K0514"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STPCC0166B" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="C0166BAS"/>
<gate name="B" symbol="C0166IDE"/>
<gate name="C" symbol="C0166ISA"/>
<gate name="D" symbol="C0166MEM"/>
<gate name="E" symbol="C0166PCI"/>
<gate name="VDD1" symbol="VDD"/>
<gate name="VDD2" symbol="VDD"/>
<gate name="VDD3" symbol="VDD"/>
<gate name="VDD4" symbol="VDD"/>
<gate name="VDD5" symbol="VDD"/>
<gate name="VDD6" symbol="VDD"/>
<gate name="VDD7" symbol="VDD"/>
<gate name="VDD8" symbol="VDD"/>
<gate name="VDD9" symbol="VDD"/>
<gate name="VDD10" symbol="VDD"/>
<gate name="VDD11" symbol="VDD"/>
<gate name="VDD12" symbol="VDD"/>
<gate name="VDD13" symbol="VDD"/>
<gate name="VDD14" symbol="VDD"/>
<gate name="VDD15" symbol="VDD"/>
<gate name="VDD16" symbol="VDD"/>
<gate name="VDD17" symbol="VDD"/>
<gate name="VDD18" symbol="VDD"/>
<gate name="VDD19" symbol="VDD"/>
<gate name="VDD20" symbol="VDD"/>
<gate name="VDD21" symbol="VDD"/>
<gate name="VDD22" symbol="VDD"/>
<gate name="VDD23" symbol="VDD"/>
<gate name="VDD24" symbol="VDD"/>
<gate name="VSS1" symbol="VSS"/>
<gate name="VSS2" symbol="VSS"/>
<gate name="VSS3" symbol="VSS"/>
<gate name="VSS4" symbol="VSS"/>
<gate name="VSS5" symbol="VSS"/>
<gate name="VSS6" symbol="VSS"/>
<gate name="VSS7" symbol="VSS"/>
<gate name="VSS8" symbol="VSS"/>
<gate name="VSS9" symbol="VSS"/>
<gate name="VSS10" symbol="VSS"/>
<gate name="VSS11" symbol="VSS"/>
<gate name="VSS12" symbol="VSS"/>
<gate name="VSS13" symbol="VSS"/>
<gate name="VSS14" symbol="VSS"/>
<gate name="VSS15" symbol="VSS"/>
<gate name="VSS16" symbol="VSS"/>
<gate name="VSS17" symbol="VSS"/>
<gate name="VSS18" symbol="VSS"/>
<gate name="VSS19" symbol="VSS"/>
<gate name="VSS20" symbol="VSS"/>
<gate name="VSS21" symbol="VSS"/>
<gate name="VSS22" symbol="VSS"/>
<gate name="VSS23" symbol="VSS"/>
<gate name="VSS24" symbol="VSS"/>
<gate name="VDD25" symbol="VDD"/>
<gate name="VDD26" symbol="VDD"/>
<gate name="VSS25" symbol="VSS"/>
<gate name="VSS26" symbol="VSS"/>
<gate name="VSS27" symbol="VSS"/>
<gate name="VSS28" symbol="VSS"/>
<gate name="VSS29" symbol="VSS"/>
<gate name="VSS30" symbol="VSS"/>
<gate name="VSS31" symbol="VSS"/>
<gate name="VSS32" symbol="VSS"/>
<gate name="VSS33" symbol="VSS"/>
<gate name="VSS34" symbol="VSS"/>
<gate name="VSS35" symbol="VSS"/>
<gate name="VSS36" symbol="VSS"/>
<gate name="VSS37" symbol="VSS"/>
<gate name="VSS38" symbol="VSS"/>
<gate name="VSS39" symbol="VSS"/>
<gate name="VSS40" symbol="VSS"/>
<gate name="VSS41" symbol="VSS"/>
<gate name="VSS42" symbol="VSS"/>
<gate name="VSS43" symbol="VSS"/>
<gate name="VSS44" symbol="VSS"/>
<gate name="VSS45" symbol="VSS"/>
<gate name="VSS46" symbol="VSS"/>
<gate name="VSS47" symbol="VSS"/>
<gate name="VSS48" symbol="VSS"/>
<gate name="VSS49" symbol="VSS"/>
<gate name="VSS50" symbol="VSS"/>
<gate name="VSS51" symbol="VSS"/>
<gate name="VSS52" symbol="VSS"/>
<gate name="VSS53" symbol="VSS"/>
<gate name="VSS54" symbol="VSS"/>
<gate name="VSS55" symbol="VSS"/>
<gate name="VSS56" symbol="VSS"/>
<gate name="VSS57" symbol="VSS"/>
<gate name="VSS58" symbol="VSS"/>
<gate name="VSS59" symbol="VSS"/>
<gate name="VSS60" symbol="VSS"/>
<gate name="VSS61" symbol="VSS"/>
<gate name="VSS62" symbol="VSS"/>
<gate name="VSS63" symbol="VSS"/>
<gate name="VSS64" symbol="VSS"/>
<gate name="VSS65" symbol="VSS"/>
<gate name="VSS66" symbol="VSS"/>
<gate name="VSS67" symbol="VSS"/>
<gate name="VSS68" symbol="VSS"/>
<gate name="RESERV1" symbol="RESERVED"/>
<gate name="RESERV2" symbol="RESERVED"/>
<gate name="RESERV3" symbol="RESERVED"/>
<gate name="RESERV4" symbol="RESERVED"/>
<gate name="F" symbol="C0166MON"/>
<gate name="VSS69" symbol="VSS"/>
</gates>
<devices>
<device name="" package="PBGA-388">
<connects>
<connect gate="A" pin="DCLK" pad="AF9"/>
<connect gate="A" pin="DEV_CLK" pad="F25"/>
<connect gate="A" pin="GCLK2X" pad="AF15"/>
<connect gate="A" pin="HCLK" pad="G23"/>
<connect gate="A" pin="SCAN_EN" pad="B3"/>
<connect gate="A" pin="SYSRSTI" pad="AF3"/>
<connect gate="A" pin="XTALI" pad="A3"/>
<connect gate="A" pin="XTALO" pad="C4"/>
<connect gate="B" pin="!PDACK" pad="D3"/>
<connect gate="B" pin="!PIOR" pad="E2"/>
<connect gate="B" pin="!PIOW" pad="E4"/>
<connect gate="B" pin="!SDACK" pad="D1"/>
<connect gate="B" pin="!SIOR" pad="E3"/>
<connect gate="B" pin="!SIOW" pad="E1"/>
<connect gate="B" pin="DACK_ENC0" pad="C23"/>
<connect gate="B" pin="DACK_ENC1" pad="A23"/>
<connect gate="B" pin="DACK_ENC2" pad="B22"/>
<connect gate="B" pin="DREA_MUX0" pad="A24"/>
<connect gate="B" pin="DREA_MUX1" pad="B23"/>
<connect gate="B" pin="IRQ_MUX0" pad="E23"/>
<connect gate="B" pin="IRQ_MUX1" pad="D26"/>
<connect gate="B" pin="IRQ_MUX2" pad="E24"/>
<connect gate="B" pin="IRQ_MUX3" pad="C25"/>
<connect gate="B" pin="PDRQ" pad="C1"/>
<connect gate="B" pin="PIRQ" pad="B1"/>
<connect gate="B" pin="SDRQ" pad="D2"/>
<connect gate="B" pin="SIRQ" pad="C2"/>
<connect gate="B" pin="SPKRD" pad="C5"/>
<connect gate="B" pin="TC" pad="D22"/>
<connect gate="C" pin="!BHE" pad="AA2"/>
<connect gate="C" pin="!GPIOCS" pad="AE3"/>
<connect gate="C" pin="!IOCHCK" pad="AD1"/>
<connect gate="C" pin="!IOCS16" pad="AB3"/>
<connect gate="C" pin="!IOR" pad="AA3"/>
<connect gate="C" pin="!IOW" pad="AC2"/>
<connect gate="C" pin="!ISAOE" pad="AF2"/>
<connect gate="C" pin="!KBCS!/DD14" pad="N3"/>
<connect gate="C" pin="!MASTER" pad="AB4"/>
<connect gate="C" pin="!MCS16" pad="AC1"/>
<connect gate="C" pin="!MEMR" pad="Y4"/>
<connect gate="C" pin="!MEMW" pad="AA1"/>
<connect gate="C" pin="!REF" pad="AD2"/>
<connect gate="C" pin="!RMRTC!/DD15" pad="P1"/>
<connect gate="C" pin="!RTCAS" pad="A4"/>
<connect gate="C" pin="!RTCDS!/DD12" pad="P3"/>
<connect gate="C" pin="!RTCRW!/DD13" pad="R2"/>
<connect gate="C" pin="!SMEMR" pad="Y3"/>
<connect gate="C" pin="!SMEMW" pad="AB2"/>
<connect gate="C" pin="!SYSRSTO" pad="AE4"/>
<connect gate="C" pin="!ZWS" pad="AC9"/>
<connect gate="C" pin="AEN" pad="AC3"/>
<connect gate="C" pin="ALE" pad="W3"/>
<connect gate="C" pin="IOCHRDY" pad="Y1"/>
<connect gate="C" pin="ISA_CLK" pad="AD4"/>
<connect gate="C" pin="ISA_CLK2X" pad="AE5"/>
<connect gate="C" pin="LA17/DA0" pad="F2"/>
<connect gate="C" pin="LA18/DA1" pad="G4"/>
<connect gate="C" pin="LA19/DA2" pad="F3"/>
<connect gate="C" pin="LA20/!PCS1" pad="F1"/>
<connect gate="C" pin="LA21/!PCS3" pad="G2"/>
<connect gate="C" pin="LA22/!SCS1" pad="G3"/>
<connect gate="C" pin="LA23/!SCS3" pad="H2"/>
<connect gate="C" pin="OSC14M" pad="AF8"/>
<connect gate="C" pin="SA0" pad="J4"/>
<connect gate="C" pin="SA1" pad="H1"/>
<connect gate="C" pin="SA10/DD2" pad="K3"/>
<connect gate="C" pin="SA11/DD3" pad="L1"/>
<connect gate="C" pin="SA12/DD4" pad="M2"/>
<connect gate="C" pin="SA13/DD5" pad="M1"/>
<connect gate="C" pin="SA14/DD6" pad="L3"/>
<connect gate="C" pin="SA15/DD7" pad="N2"/>
<connect gate="C" pin="SA16/DD8" pad="M4"/>
<connect gate="C" pin="SA17/DD9" pad="N1"/>
<connect gate="C" pin="SA18/DD10" pad="M3"/>
<connect gate="C" pin="SA19/DD11" pad="P4"/>
<connect gate="C" pin="SA2" pad="H3"/>
<connect gate="C" pin="SA3" pad="J2"/>
<connect gate="C" pin="SA4" pad="J1"/>
<connect gate="C" pin="SA5" pad="K2"/>
<connect gate="C" pin="SA6" pad="J3"/>
<connect gate="C" pin="SA7" pad="K1"/>
<connect gate="C" pin="SA8/DD0" pad="K4"/>
<connect gate="C" pin="SA9/DD1" pad="L2"/>
<connect gate="C" pin="SD0" pad="R1"/>
<connect gate="C" pin="SD1" pad="T2"/>
<connect gate="C" pin="SD10" pad="U3"/>
<connect gate="C" pin="SD11" pad="V1"/>
<connect gate="C" pin="SD12" pad="W2"/>
<connect gate="C" pin="SD13" pad="W1"/>
<connect gate="C" pin="SD14" pad="V3"/>
<connect gate="C" pin="SD15" pad="Y2"/>
<connect gate="C" pin="SD2" pad="R3"/>
<connect gate="C" pin="SD3" pad="T1"/>
<connect gate="C" pin="SD4" pad="R4"/>
<connect gate="C" pin="SD5" pad="U2"/>
<connect gate="C" pin="SD6" pad="T3"/>
<connect gate="C" pin="SD7" pad="U1"/>
<connect gate="C" pin="SD8" pad="U4"/>
<connect gate="C" pin="SD9" pad="V2"/>
<connect gate="D" pin="!CAS0" pad="AE21"/>
<connect gate="D" pin="!CAS1" pad="AC20"/>
<connect gate="D" pin="!CAS2" pad="AF21"/>
<connect gate="D" pin="!CAS3" pad="AD20"/>
<connect gate="D" pin="!CAS4" pad="AE22"/>
<connect gate="D" pin="!CAS5" pad="AF22"/>
<connect gate="D" pin="!CAS6" pad="AD21"/>
<connect gate="D" pin="!CAS7" pad="AE23"/>
<connect gate="D" pin="!MWE" pad="AC22"/>
<connect gate="D" pin="!RAS0" pad="AD18"/>
<connect gate="D" pin="!RAS1" pad="AE20"/>
<connect gate="D" pin="!RAS2" pad="AC19"/>
<connect gate="D" pin="!RAS3" pad="AF20"/>
<connect gate="D" pin="MA0" pad="AD15"/>
<connect gate="D" pin="MA1" pad="AF16"/>
<connect gate="D" pin="MA10" pad="AE19"/>
<connect gate="D" pin="MA11" pad="AF19"/>
<connect gate="D" pin="MA2" pad="AC15"/>
<connect gate="D" pin="MA3" pad="AE17"/>
<connect gate="D" pin="MA4" pad="AD16"/>
<connect gate="D" pin="MA5" pad="AF17"/>
<connect gate="D" pin="MA6" pad="AC17"/>
<connect gate="D" pin="MA7" pad="AE18"/>
<connect gate="D" pin="MA8" pad="AD17"/>
<connect gate="D" pin="MA9" pad="AF18"/>
<connect gate="D" pin="MD0" pad="AF23"/>
<connect gate="D" pin="MD1" pad="AE24"/>
<connect gate="D" pin="MD10" pad="Y24"/>
<connect gate="D" pin="MD11" pad="V23"/>
<connect gate="D" pin="MD12" pad="W24"/>
<connect gate="D" pin="MD13" pad="V26"/>
<connect gate="D" pin="MD14" pad="V24"/>
<connect gate="D" pin="MD15" pad="U23"/>
<connect gate="D" pin="MD16" pad="U24"/>
<connect gate="D" pin="MD17" pad="R26"/>
<connect gate="D" pin="MD18" pad="P25"/>
<connect gate="D" pin="MD19" pad="P26"/>
<connect gate="D" pin="MD2" pad="AF24"/>
<connect gate="D" pin="MD20" pad="N25"/>
<connect gate="D" pin="MD21" pad="N26"/>
<connect gate="D" pin="MD22" pad="M25"/>
<connect gate="D" pin="MD23" pad="M26"/>
<connect gate="D" pin="MD24" pad="M24"/>
<connect gate="D" pin="MD25" pad="M23"/>
<connect gate="D" pin="MD26" pad="L24"/>
<connect gate="D" pin="MD27" pad="J25"/>
<connect gate="D" pin="MD28" pad="J26"/>
<connect gate="D" pin="MD29" pad="H26"/>
<connect gate="D" pin="MD3" pad="AD25"/>
<connect gate="D" pin="MD30" pad="G25"/>
<connect gate="D" pin="MD31" pad="G26"/>
<connect gate="D" pin="MD32" pad="AD22"/>
<connect gate="D" pin="MD33" pad="AD23"/>
<connect gate="D" pin="MD34" pad="AE26"/>
<connect gate="D" pin="MD35" pad="AD26"/>
<connect gate="D" pin="MD36" pad="AC24"/>
<connect gate="D" pin="MD37" pad="AB25"/>
<connect gate="D" pin="MD38" pad="AB26"/>
<connect gate="D" pin="MD39" pad="Y23"/>
<connect gate="D" pin="MD4" pad="AC25"/>
<connect gate="D" pin="MD40" pad="AA26"/>
<connect gate="D" pin="MD41" pad="Y26"/>
<connect gate="D" pin="MD42" pad="W25"/>
<connect gate="D" pin="MD43" pad="W26"/>
<connect gate="D" pin="MD44" pad="V25"/>
<connect gate="D" pin="MD45" pad="U25"/>
<connect gate="D" pin="MD46" pad="U26"/>
<connect gate="D" pin="MD47" pad="T25"/>
<connect gate="D" pin="MD48" pad="R25"/>
<connect gate="D" pin="MD49" pad="T24"/>
<connect gate="D" pin="MD5" pad="AC26"/>
<connect gate="D" pin="MD50" pad="R23"/>
<connect gate="D" pin="MD51" pad="R24"/>
<connect gate="D" pin="MD52" pad="N23"/>
<connect gate="D" pin="MD53" pad="P24"/>
<connect gate="D" pin="MD54" pad="N24"/>
<connect gate="D" pin="MD55" pad="L25"/>
<connect gate="D" pin="MD56" pad="L26"/>
<connect gate="D" pin="MD57" pad="K25"/>
<connect gate="D" pin="MD58" pad="K26"/>
<connect gate="D" pin="MD59" pad="K24"/>
<connect gate="D" pin="MD6" pad="AB24"/>
<connect gate="D" pin="MD60" pad="H25"/>
<connect gate="D" pin="MD61" pad="J24"/>
<connect gate="D" pin="MD62" pad="H23"/>
<connect gate="D" pin="MD63" pad="H24"/>
<connect gate="D" pin="MD7" pad="AA25"/>
<connect gate="D" pin="MD8" pad="AA24"/>
<connect gate="D" pin="MD9" pad="Y25"/>
<connect gate="E" pin="!DEVSEL" pad="C8"/>
<connect gate="E" pin="!FRAME" pad="A8"/>
<connect gate="E" pin="!IRDY" pad="D8"/>
<connect gate="E" pin="!LOCK" pad="A6"/>
<connect gate="E" pin="!PCIGNT0" pad="C22"/>
<connect gate="E" pin="!PCIGNT1" pad="B21"/>
<connect gate="E" pin="!PCIGNT2" pad="D20"/>
<connect gate="E" pin="!PCIREQ0" pad="C21"/>
<connect gate="E" pin="!PCIREQ1" pad="A21"/>
<connect gate="E" pin="!PCIREQ2" pad="B20"/>
<connect gate="E" pin="!PCI_INT0" pad="A5"/>
<connect gate="E" pin="!PCI_INT1" pad="C6"/>
<connect gate="E" pin="!PCI_INT2" pad="B4"/>
<connect gate="E" pin="!PCI_INT3" pad="D5"/>
<connect gate="E" pin="!SERR" pad="D7"/>
<connect gate="E" pin="!STOP" pad="A7"/>
<connect gate="E" pin="!TRDY" pad="B7"/>
<connect gate="E" pin="AD0" pad="A20"/>
<connect gate="E" pin="AD1" pad="C20"/>
<connect gate="E" pin="AD10" pad="D17"/>
<connect gate="E" pin="AD11" pad="B16"/>
<connect gate="E" pin="AD12" pad="C17"/>
<connect gate="E" pin="AD13" pad="B15"/>
<connect gate="E" pin="AD14" pad="A15"/>
<connect gate="E" pin="AD15" pad="C16"/>
<connect gate="E" pin="AD16" pad="D15"/>
<connect gate="E" pin="AD17" pad="A14"/>
<connect gate="E" pin="AD18" pad="C15"/>
<connect gate="E" pin="AD19" pad="B13"/>
<connect gate="E" pin="AD2" pad="B19"/>
<connect gate="E" pin="AD20" pad="D13"/>
<connect gate="E" pin="AD21" pad="A13"/>
<connect gate="E" pin="AD22" pad="C14"/>
<connect gate="E" pin="AD23" pad="C13"/>
<connect gate="E" pin="AD24" pad="A12"/>
<connect gate="E" pin="AD25" pad="B11"/>
<connect gate="E" pin="AD26" pad="C12"/>
<connect gate="E" pin="AD27" pad="A11"/>
<connect gate="E" pin="AD28" pad="D12"/>
<connect gate="E" pin="AD29" pad="B10"/>
<connect gate="E" pin="AD3" pad="A19"/>
<connect gate="E" pin="AD30" pad="C11"/>
<connect gate="E" pin="AD31" pad="A10"/>
<connect gate="E" pin="AD4" pad="C19"/>
<connect gate="E" pin="AD5" pad="B18"/>
<connect gate="E" pin="AD6" pad="A18"/>
<connect gate="E" pin="AD7" pad="B17"/>
<connect gate="E" pin="AD8" pad="C18"/>
<connect gate="E" pin="AD9" pad="A17"/>
<connect gate="E" pin="CBE0" pad="D10"/>
<connect gate="E" pin="CBE1" pad="C10"/>
<connect gate="E" pin="CBE2" pad="A9"/>
<connect gate="E" pin="CBE3" pad="B8"/>
<connect gate="E" pin="PAR" pad="B6"/>
<connect gate="E" pin="PCI_CLKI" pad="F24"/>
<connect gate="E" pin="PCI_CLKO" pad="D25"/>
<connect gate="E" pin="VDD5@1" pad="A16"/>
<connect gate="E" pin="VDD5@2" pad="B12"/>
<connect gate="E" pin="VDD5@3" pad="B9"/>
<connect gate="E" pin="VDD5@4" pad="D18"/>
<connect gate="F" pin="BLUE" pad="AF6"/>
<connect gate="F" pin="BLUE_TV" pad="AF11"/>
<connect gate="F" pin="COMP" pad="AF5"/>
<connect gate="F" pin="CVBS" pad="AD11"/>
<connect gate="F" pin="GREEN" pad="AD6"/>
<connect gate="F" pin="GREEN_TV" pad="AC10"/>
<connect gate="F" pin="HSYNC" pad="AC5"/>
<connect gate="F" pin="IREF1_TV" pad="AD8"/>
<connect gate="F" pin="IREF2_TV" pad="AE11"/>
<connect gate="F" pin="ODD_EVEN" pad="AD9"/>
<connect gate="F" pin="RED" pad="AE6"/>
<connect gate="F" pin="RED_TV" pad="AF10"/>
<connect gate="F" pin="RSET" pad="AE8"/>
<connect gate="F" pin="SDA/DDC0" pad="C7"/>
<connect gate="F" pin="SLC/DDC1" pad="B5"/>
<connect gate="F" pin="VCLK" pad="AC12"/>
<connect gate="F" pin="VCS" pad="AE10"/>
<connect gate="F" pin="VDDA_TV" pad="AF12"/>
<connect gate="F" pin="VDDDCKPLL" pad="AF13"/>
<connect gate="F" pin="VDDDEVPLL" pad="G24"/>
<connect gate="F" pin="VDDGCKPLL" pad="AD19"/>
<connect gate="F" pin="VDDHCKPLL" pad="F26"/>
<connect gate="F" pin="VDD_DAC1" pad="AC7"/>
<connect gate="F" pin="VDD_DAC2" pad="AF4"/>
<connect gate="F" pin="VIN0" pad="AE13"/>
<connect gate="F" pin="VIN1" pad="AD14"/>
<connect gate="F" pin="VIN2" pad="AD12"/>
<connect gate="F" pin="VIN3" pad="AE14"/>
<connect gate="F" pin="VIN4" pad="AC14"/>
<connect gate="F" pin="VIN5" pad="AF14"/>
<connect gate="F" pin="VIN6" pad="AD13"/>
<connect gate="F" pin="VIN7" pad="AE15"/>
<connect gate="F" pin="VREF1_TV" pad="AE9"/>
<connect gate="F" pin="VREF2_TV" pad="AD10"/>
<connect gate="F" pin="VREF_DAC" pad="AD7"/>
<connect gate="F" pin="VSSA_TV" pad="AE12"/>
<connect gate="F" pin="VSS_DAC1" pad="AE7"/>
<connect gate="F" pin="VSS_DAC2" pad="AF7"/>
<connect gate="F" pin="VSS_DLL1" pad="E25"/>
<connect gate="F" pin="VSS_DLL2" pad="E26"/>
<connect gate="F" pin="VSYNC" pad="AD5"/>
<connect gate="RESERV1" pin="RESERVED" pad="C26"/>
<connect gate="RESERV2" pin="RESERVED" pad="D24"/>
<connect gate="RESERV3" pin="RESERVED" pad="B24"/>
<connect gate="RESERV4" pin="RESERVED" pad="A25"/>
<connect gate="VDD1" pin="VDD" pad="A22"/>
<connect gate="VDD10" pin="VDD" pad="G1"/>
<connect gate="VDD11" pin="VDD" pad="K23"/>
<connect gate="VDD12" pin="VDD" pad="L4"/>
<connect gate="VDD13" pin="VDD" pad="L23"/>
<connect gate="VDD14" pin="VDD" pad="P2"/>
<connect gate="VDD15" pin="VDD" pad="T4"/>
<connect gate="VDD16" pin="VDD" pad="T23"/>
<connect gate="VDD17" pin="VDD" pad="T26"/>
<connect gate="VDD18" pin="VDD" pad="W4"/>
<connect gate="VDD19" pin="VDD" pad="AA4"/>
<connect gate="VDD2" pin="VDD" pad="B14"/>
<connect gate="VDD20" pin="VDD" pad="AA23"/>
<connect gate="VDD21" pin="VDD" pad="AB1"/>
<connect gate="VDD22" pin="VDD" pad="AB23"/>
<connect gate="VDD23" pin="VDD" pad="AC6"/>
<connect gate="VDD24" pin="VDD" pad="AC11"/>
<connect gate="VDD25" pin="VDD" pad="AC16"/>
<connect gate="VDD26" pin="VDD" pad="AC21"/>
<connect gate="VDD3" pin="VDD" pad="C9"/>
<connect gate="VDD4" pin="VDD" pad="D6"/>
<connect gate="VDD5" pin="VDD" pad="D11"/>
<connect gate="VDD6" pin="VDD" pad="D16"/>
<connect gate="VDD7" pin="VDD" pad="D21"/>
<connect gate="VDD8" pin="VDD" pad="F4"/>
<connect gate="VDD9" pin="VDD" pad="F23"/>
<connect gate="VSS1" pin="VSS" pad="A1"/>
<connect gate="VSS10" pin="VSS" pad="D14"/>
<connect gate="VSS11" pin="VSS" pad="D19"/>
<connect gate="VSS12" pin="VSS" pad="D23"/>
<connect gate="VSS13" pin="VSS" pad="H4"/>
<connect gate="VSS14" pin="VSS" pad="J23"/>
<connect gate="VSS15" pin="VSS" pad="L11"/>
<connect gate="VSS16" pin="VSS" pad="L12"/>
<connect gate="VSS17" pin="VSS" pad="L13"/>
<connect gate="VSS18" pin="VSS" pad="L14"/>
<connect gate="VSS19" pin="VSS" pad="L15"/>
<connect gate="VSS2" pin="VSS" pad="A26"/>
<connect gate="VSS20" pin="VSS" pad="L16"/>
<connect gate="VSS21" pin="VSS" pad="M11"/>
<connect gate="VSS22" pin="VSS" pad="M12"/>
<connect gate="VSS23" pin="VSS" pad="M13"/>
<connect gate="VSS24" pin="VSS" pad="M14"/>
<connect gate="VSS25" pin="VSS" pad="M15"/>
<connect gate="VSS26" pin="VSS" pad="M16"/>
<connect gate="VSS27" pin="VSS" pad="N4"/>
<connect gate="VSS28" pin="VSS" pad="N11"/>
<connect gate="VSS29" pin="VSS" pad="N12"/>
<connect gate="VSS3" pin="VSS" pad="B2"/>
<connect gate="VSS30" pin="VSS" pad="N13"/>
<connect gate="VSS31" pin="VSS" pad="N14"/>
<connect gate="VSS32" pin="VSS" pad="N15"/>
<connect gate="VSS33" pin="VSS" pad="N16"/>
<connect gate="VSS34" pin="VSS" pad="P11"/>
<connect gate="VSS35" pin="VSS" pad="P12"/>
<connect gate="VSS36" pin="VSS" pad="P13"/>
<connect gate="VSS37" pin="VSS" pad="P14"/>
<connect gate="VSS38" pin="VSS" pad="P15"/>
<connect gate="VSS39" pin="VSS" pad="P16"/>
<connect gate="VSS4" pin="VSS" pad="B25"/>
<connect gate="VSS40" pin="VSS" pad="P23"/>
<connect gate="VSS41" pin="VSS" pad="R11"/>
<connect gate="VSS42" pin="VSS" pad="R12"/>
<connect gate="VSS43" pin="VSS" pad="R13"/>
<connect gate="VSS44" pin="VSS" pad="R14"/>
<connect gate="VSS45" pin="VSS" pad="R15"/>
<connect gate="VSS46" pin="VSS" pad="R16"/>
<connect gate="VSS47" pin="VSS" pad="T11"/>
<connect gate="VSS48" pin="VSS" pad="T12"/>
<connect gate="VSS49" pin="VSS" pad="T13"/>
<connect gate="VSS5" pin="VSS" pad="B26"/>
<connect gate="VSS50" pin="VSS" pad="T14"/>
<connect gate="VSS51" pin="VSS" pad="T15"/>
<connect gate="VSS52" pin="VSS" pad="T16"/>
<connect gate="VSS53" pin="VSS" pad="V4"/>
<connect gate="VSS54" pin="VSS" pad="W23"/>
<connect gate="VSS55" pin="VSS" pad="AC4"/>
<connect gate="VSS56" pin="VSS" pad="AC8"/>
<connect gate="VSS57" pin="VSS" pad="AC13"/>
<connect gate="VSS58" pin="VSS" pad="AC18"/>
<connect gate="VSS59" pin="VSS" pad="AC23"/>
<connect gate="VSS6" pin="VSS" pad="C3"/>
<connect gate="VSS60" pin="VSS" pad="AD3"/>
<connect gate="VSS61" pin="VSS" pad="AD24"/>
<connect gate="VSS62" pin="VSS" pad="AE1"/>
<connect gate="VSS63" pin="VSS" pad="AE2"/>
<connect gate="VSS64" pin="VSS" pad="AE16"/>
<connect gate="VSS65" pin="VSS" pad="AE25"/>
<connect gate="VSS66" pin="VSS" pad="AF1"/>
<connect gate="VSS67" pin="VSS" pad="AF25"/>
<connect gate="VSS68" pin="VSS" pad="AF26"/>
<connect gate="VSS69" pin="VSS" pad="A2"/>
<connect gate="VSS7" pin="VSS" pad="C24"/>
<connect gate="VSS8" pin="VSS" pad="D4"/>
<connect gate="VSS9" pin="VSS" pad="D9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STPCC5HEBC"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M6674"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST10F168" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
with CAN 2.0B INTERFACE&lt;p&gt;
Siemens compatible</description>
<gates>
<gate name="_C" symbol="F168_C"/>
<gate name="P0" symbol="F168_P0"/>
<gate name="P1" symbol="F168_P1"/>
<gate name="P2" symbol="F168_P2"/>
<gate name="P4" symbol="F168_P4"/>
<gate name="P5" symbol="F168_P5"/>
<gate name="P6" symbol="F168_P6"/>
<gate name="P7" symbol="F168_P7"/>
<gate name="P8" symbol="F168_P8"/>
<gate name="VDD1" symbol="VDD"/>
<gate name="VDD2" symbol="VDD"/>
<gate name="VDD3" symbol="VDD"/>
<gate name="VDD4" symbol="VDD"/>
<gate name="VDD5" symbol="VDD"/>
<gate name="VDD6" symbol="VDD"/>
<gate name="VDD7" symbol="VDD"/>
<gate name="VDD8" symbol="VDD"/>
<gate name="VDD9" symbol="VDD"/>
<gate name="VDD10" symbol="VDD"/>
<gate name="VSS1" symbol="VSS"/>
<gate name="VSS2" symbol="VSS"/>
<gate name="VSS3" symbol="VSS"/>
<gate name="VSS4" symbol="VSS"/>
<gate name="VSS5" symbol="VSS"/>
<gate name="VSS6" symbol="VSS"/>
<gate name="VSS7" symbol="VSS"/>
<gate name="VSS8" symbol="VSS"/>
<gate name="VSS9" symbol="VSS"/>
<gate name="VSS10" symbol="VSS"/>
<gate name="P3" symbol="F168_P3"/>
</gates>
<devices>
<device name="" package="PQFP144-28X28">
<connects>
<connect gate="P0" pin="P0H0/AD8" pad="108"/>
<connect gate="P0" pin="P0H1/AD9" pad="111"/>
<connect gate="P0" pin="P0H2/AD10" pad="112"/>
<connect gate="P0" pin="P0H3/AD11" pad="113"/>
<connect gate="P0" pin="P0H4/AD12" pad="114"/>
<connect gate="P0" pin="P0H5/AD13" pad="115"/>
<connect gate="P0" pin="P0H6/AD14" pad="116"/>
<connect gate="P0" pin="P0H7/AD15" pad="117"/>
<connect gate="P0" pin="P0L0/AD0" pad="100"/>
<connect gate="P0" pin="P0L1/AD1" pad="101"/>
<connect gate="P0" pin="P0L2/AD2" pad="102"/>
<connect gate="P0" pin="P0L3/AD3" pad="103"/>
<connect gate="P0" pin="P0L4/AD4" pad="104"/>
<connect gate="P0" pin="P0L5/AD5" pad="105"/>
<connect gate="P0" pin="P0L6/AD6" pad="106"/>
<connect gate="P0" pin="P0L7/AD7" pad="107"/>
<connect gate="P1" pin="P1H0/A8" pad="128"/>
<connect gate="P1" pin="P1H1/A9" pad="129"/>
<connect gate="P1" pin="P1H2/A10" pad="130"/>
<connect gate="P1" pin="P1H3/A11" pad="131"/>
<connect gate="P1" pin="P1H4/A12" pad="132"/>
<connect gate="P1" pin="P1H5/13" pad="133"/>
<connect gate="P1" pin="P1H6/A14" pad="134"/>
<connect gate="P1" pin="P1H7/A15" pad="135"/>
<connect gate="P1" pin="P1L0/A0" pad="118"/>
<connect gate="P1" pin="P1L1/A1" pad="119"/>
<connect gate="P1" pin="P1L2/A2" pad="120"/>
<connect gate="P1" pin="P1L3/A3" pad="121"/>
<connect gate="P1" pin="P1L4/A4" pad="122"/>
<connect gate="P1" pin="P1L5/A5" pad="123"/>
<connect gate="P1" pin="P1L6/A6" pad="124"/>
<connect gate="P1" pin="P1L7/A7" pad="125"/>
<connect gate="P2" pin="P2-0/CC0" pad="47"/>
<connect gate="P2" pin="P2-1/CC1" pad="48"/>
<connect gate="P2" pin="P2-10/CC10" pad="59"/>
<connect gate="P2" pin="P2-11/CC11" pad="60"/>
<connect gate="P2" pin="P2-12/CC12" pad="61"/>
<connect gate="P2" pin="P2-13/CC13" pad="62"/>
<connect gate="P2" pin="P2-14/CC14" pad="63"/>
<connect gate="P2" pin="P2-15/CC15" pad="64"/>
<connect gate="P2" pin="P2-2/CC2" pad="49"/>
<connect gate="P2" pin="P2-3/CC3" pad="50"/>
<connect gate="P2" pin="P2-4/CC4" pad="51"/>
<connect gate="P2" pin="P2-5/CC5" pad="52"/>
<connect gate="P2" pin="P2-6/CC6" pad="53"/>
<connect gate="P2" pin="P2-7/CC7" pad="54"/>
<connect gate="P2" pin="P2-8/CC8" pad="57"/>
<connect gate="P2" pin="P2-9/CC9" pad="58"/>
<connect gate="P3" pin="P3-0/TOIN" pad="65"/>
<connect gate="P3" pin="P3-1/T6OUT" pad="66"/>
<connect gate="P3" pin="P3-10/TXD0" pad="77"/>
<connect gate="P3" pin="P3-11/RXD0" pad="78"/>
<connect gate="P3" pin="P3-12/!BHE" pad="79"/>
<connect gate="P3" pin="P3-13/SCLK" pad="80"/>
<connect gate="P3" pin="P3-15/CLKO" pad="81"/>
<connect gate="P3" pin="P3-2/CAPIN" pad="67"/>
<connect gate="P3" pin="P3-3/T3OUT" pad="68"/>
<connect gate="P3" pin="P3-4/T3EUD" pad="69"/>
<connect gate="P3" pin="P3-5/T4IN" pad="70"/>
<connect gate="P3" pin="P3-6/T3IN" pad="73"/>
<connect gate="P3" pin="P3-7/T2IN" pad="74"/>
<connect gate="P3" pin="P3-8/MRST" pad="75"/>
<connect gate="P3" pin="P3-9/MTSR" pad="76"/>
<connect gate="P4" pin="P4-0/A16" pad="85"/>
<connect gate="P4" pin="P4-1/A17" pad="86"/>
<connect gate="P4" pin="P4-2/A18" pad="87"/>
<connect gate="P4" pin="P4-3/A19" pad="88"/>
<connect gate="P4" pin="P4-4/A20" pad="89"/>
<connect gate="P4" pin="P4-5/A21" pad="90"/>
<connect gate="P4" pin="P4-6/A22" pad="91"/>
<connect gate="P4" pin="P4-7/A23" pad="92"/>
<connect gate="P5" pin="P5-0/AN0" pad="27"/>
<connect gate="P5" pin="P5-1/AN1" pad="28"/>
<connect gate="P5" pin="P5-10/AN10" pad="39"/>
<connect gate="P5" pin="P5-11/AN11" pad="40"/>
<connect gate="P5" pin="P5-12/AN12" pad="41"/>
<connect gate="P5" pin="P5-13/AN13" pad="42"/>
<connect gate="P5" pin="P5-14/AN14" pad="43"/>
<connect gate="P5" pin="P5-15/AN15" pad="44"/>
<connect gate="P5" pin="P5-2/AN2" pad="29"/>
<connect gate="P5" pin="P5-3/AN3" pad="30"/>
<connect gate="P5" pin="P5-4/AN4" pad="31"/>
<connect gate="P5" pin="P5-5/AN5" pad="32"/>
<connect gate="P5" pin="P5-6/AN6" pad="33"/>
<connect gate="P5" pin="P5-7/AN7" pad="34"/>
<connect gate="P5" pin="P5-8/AN8" pad="35"/>
<connect gate="P5" pin="P5-9/AN9" pad="36"/>
<connect gate="P6" pin="!!P6-6HLDA" pad="7"/>
<connect gate="P6" pin="P6-0/!SC0" pad="1"/>
<connect gate="P6" pin="P6-1/!CS1" pad="2"/>
<connect gate="P6" pin="P6-2/!CS2" pad="3"/>
<connect gate="P6" pin="P6-3/!CS3" pad="4"/>
<connect gate="P6" pin="P6-4/!CS4" pad="5"/>
<connect gate="P6" pin="P6-5/!HOLD" pad="6"/>
<connect gate="P6" pin="P6-7/!BREQ" pad="8"/>
<connect gate="P7" pin="!P7-0POUT0" pad="19"/>
<connect gate="P7" pin="P7-1/POUT1" pad="20"/>
<connect gate="P7" pin="P7-2/POUT2" pad="21"/>
<connect gate="P7" pin="P7-3/POUT3" pad="22"/>
<connect gate="P7" pin="P7-4/CC28" pad="23"/>
<connect gate="P7" pin="P7-5/CC29" pad="24"/>
<connect gate="P7" pin="P7-6/CC30" pad="25"/>
<connect gate="P7" pin="P7-7/CC31" pad="26"/>
<connect gate="P8" pin="P8-0/CC16" pad="9"/>
<connect gate="P8" pin="P8-1/CC17" pad="10"/>
<connect gate="P8" pin="P8-2/CC18" pad="11"/>
<connect gate="P8" pin="P8-3/CC19" pad="12"/>
<connect gate="P8" pin="P8-4/CC20" pad="13"/>
<connect gate="P8" pin="P8-5/CC21" pad="14"/>
<connect gate="P8" pin="P8-6/CC22" pad="15"/>
<connect gate="P8" pin="P8-7/CC23" pad="16"/>
<connect gate="VDD1" pin="VDD" pad="17"/>
<connect gate="VDD10" pin="VDD" pad="144"/>
<connect gate="VDD2" pin="VDD" pad="46"/>
<connect gate="VDD3" pin="VDD" pad="56"/>
<connect gate="VDD4" pin="VDD" pad="72"/>
<connect gate="VDD5" pin="VDD" pad="82"/>
<connect gate="VDD6" pin="VDD" pad="93"/>
<connect gate="VDD7" pin="VDD" pad="109"/>
<connect gate="VDD8" pin="VDD" pad="126"/>
<connect gate="VDD9" pin="VDD" pad="136"/>
<connect gate="VSS1" pin="VSS" pad="18"/>
<connect gate="VSS10" pin="VSS" pad="143"/>
<connect gate="VSS2" pin="VSS" pad="45"/>
<connect gate="VSS3" pin="VSS" pad="55"/>
<connect gate="VSS4" pin="VSS" pad="71"/>
<connect gate="VSS5" pin="VSS" pad="83"/>
<connect gate="VSS6" pin="VSS" pad="94"/>
<connect gate="VSS7" pin="VSS" pad="110"/>
<connect gate="VSS8" pin="VSS" pad="127"/>
<connect gate="VSS9" pin="VSS" pad="139"/>
<connect gate="_C" pin="!!WR_WRL" pad="96"/>
<connect gate="_C" pin="!EA" pad="99"/>
<connect gate="_C" pin="!NMI" pad="142"/>
<connect gate="_C" pin="!RD" pad="95"/>
<connect gate="_C" pin="!READY" pad="97"/>
<connect gate="_C" pin="!RSTIN" pad="140"/>
<connect gate="_C" pin="!RSTOUT" pad="141"/>
<connect gate="_C" pin="ALE" pad="98"/>
<connect gate="_C" pin="VAGND" pad="38"/>
<connect gate="_C" pin="VAREF" pad="37"/>
<connect gate="_C" pin="VPP/RPD" pad="84"/>
<connect gate="_C" pin="XTAL1" pad="138"/>
<connect gate="_C" pin="XTAL2" pad="137"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ST10F168SQ6/TR"/>
<attribute name="OC_FARNELL" value="1796092"/>
<attribute name="OC_NEWARK" value="37M7384"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M29F400T" prefix="IC">
<description>&lt;b&gt;FLASH MEMORY&lt;/b&gt;&lt;p&gt;
512 KB x 8 or 256 KB x 16, boot block</description>
<gates>
<gate name="G$1" symbol="M29F400"/>
<gate name="P1" symbol="VCC"/>
<gate name="P2" symbol="GND"/>
<gate name="P3" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
</gates>
<devices>
<device name="" package="TSOP48">
<connects>
<connect gate="G$1" pin="!BYTE" pad="47"/>
<connect gate="G$1" pin="!CE" pad="26"/>
<connect gate="G$1" pin="!OE" pad="28"/>
<connect gate="G$1" pin="!RB" pad="15"/>
<connect gate="G$1" pin="!RESET" pad="12"/>
<connect gate="G$1" pin="!WE" pad="11"/>
<connect gate="G$1" pin="A-1/D15" pad="1"/>
<connect gate="G$1" pin="A0" pad="25"/>
<connect gate="G$1" pin="A1" pad="24"/>
<connect gate="G$1" pin="A10" pad="6"/>
<connect gate="G$1" pin="A11" pad="5"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="3"/>
<connect gate="G$1" pin="A14" pad="2"/>
<connect gate="G$1" pin="A15" pad="45"/>
<connect gate="G$1" pin="A16" pad="48"/>
<connect gate="G$1" pin="A17" pad="17"/>
<connect gate="G$1" pin="A2" pad="23"/>
<connect gate="G$1" pin="A3" pad="22"/>
<connect gate="G$1" pin="A4" pad="21"/>
<connect gate="G$1" pin="A5" pad="20"/>
<connect gate="G$1" pin="A6" pad="19"/>
<connect gate="G$1" pin="A7" pad="18"/>
<connect gate="G$1" pin="A8" pad="8"/>
<connect gate="G$1" pin="A9" pad="7"/>
<connect gate="G$1" pin="D0" pad="29"/>
<connect gate="G$1" pin="D1" pad="31"/>
<connect gate="G$1" pin="D10" pad="34"/>
<connect gate="G$1" pin="D11" pad="36"/>
<connect gate="G$1" pin="D12" pad="39"/>
<connect gate="G$1" pin="D13" pad="41"/>
<connect gate="G$1" pin="D14" pad="43"/>
<connect gate="G$1" pin="D2" pad="33"/>
<connect gate="G$1" pin="D3" pad="35"/>
<connect gate="G$1" pin="D4" pad="38"/>
<connect gate="G$1" pin="D5" pad="40"/>
<connect gate="G$1" pin="D6" pad="42"/>
<connect gate="G$1" pin="D7" pad="44"/>
<connect gate="G$1" pin="D8" pad="30"/>
<connect gate="G$1" pin="D9" pad="32"/>
<connect gate="NC1" pin="NC" pad="9"/>
<connect gate="NC2" pin="NC" pad="10"/>
<connect gate="NC3" pin="NC" pad="13"/>
<connect gate="NC4" pin="NC" pad="14"/>
<connect gate="NC5" pin="NC" pad="16"/>
<connect gate="P1" pin="VCC" pad="37"/>
<connect gate="P2" pin="GND" pad="27"/>
<connect gate="P3" pin="GND" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MBM29F400TC-70PFTN-SFLE1"/>
<attribute name="OC_FARNELL" value="1201518"/>
<attribute name="OC_NEWARK" value="89M1908"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M29F400M" prefix="IC">
<description>&lt;b&gt;FLASH MEMORY&lt;/b&gt;&lt;p&gt;
512 KB x 8 or 256 KB x 16, boot block</description>
<gates>
<gate name="G$1" symbol="M29F400"/>
<gate name="NC1" symbol="NC"/>
<gate name="VCC" symbol="VCC"/>
<gate name="GND1" symbol="GND"/>
<gate name="GND2" symbol="GND"/>
</gates>
<devices>
<device name="" package="SO44">
<connects>
<connect gate="G$1" pin="!BYTE" pad="33"/>
<connect gate="G$1" pin="!CE" pad="12"/>
<connect gate="G$1" pin="!OE" pad="14"/>
<connect gate="G$1" pin="!RB" pad="2"/>
<connect gate="G$1" pin="!RESET" pad="44"/>
<connect gate="G$1" pin="!WE" pad="43"/>
<connect gate="G$1" pin="A-1/D15" pad="31"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="40"/>
<connect gate="G$1" pin="A11" pad="39"/>
<connect gate="G$1" pin="A12" pad="38"/>
<connect gate="G$1" pin="A13" pad="37"/>
<connect gate="G$1" pin="A14" pad="36"/>
<connect gate="G$1" pin="A15" pad="35"/>
<connect gate="G$1" pin="A16" pad="34"/>
<connect gate="G$1" pin="A17" pad="3"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="42"/>
<connect gate="G$1" pin="A9" pad="41"/>
<connect gate="G$1" pin="D0" pad="15"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="20"/>
<connect gate="G$1" pin="D11" pad="22"/>
<connect gate="G$1" pin="D12" pad="25"/>
<connect gate="G$1" pin="D13" pad="27"/>
<connect gate="G$1" pin="D14" pad="29"/>
<connect gate="G$1" pin="D2" pad="19"/>
<connect gate="G$1" pin="D3" pad="21"/>
<connect gate="G$1" pin="D4" pad="24"/>
<connect gate="G$1" pin="D5" pad="26"/>
<connect gate="G$1" pin="D6" pad="28"/>
<connect gate="G$1" pin="D7" pad="30"/>
<connect gate="G$1" pin="D8" pad="16"/>
<connect gate="G$1" pin="D9" pad="18"/>
<connect gate="GND1" pin="GND" pad="13"/>
<connect gate="GND2" pin="GND" pad="32"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="VCC" pin="VCC" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="SPANSION LLC"/>
<attribute name="MPN" value="AM29F400BB-90SF"/>
<attribute name="OC_FARNELL" value="1607577"/>
<attribute name="OC_NEWARK" value="58K5516"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST95P08M" prefix="IC">
<description>Serial &lt;b&gt;EEPROM&lt;/b&gt;&lt;p&gt;
SPI bus, 1 K x 8</description>
<gates>
<gate name="G$1" symbol="ST95P08"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!S" pad="1"/>
<connect gate="G$1" pin="!W" pad="3"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="D" pad="5"/>
<connect gate="G$1" pin="Q" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST95P08B" prefix="IC" uservalue="yes">
<description>Serial &lt;b&gt;EEPROM&lt;/b&gt;&lt;p&gt;
SPI bus, 1 K x 8</description>
<gates>
<gate name="G$1" symbol="ST95P08"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL-08">
<connects>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!S" pad="1"/>
<connect gate="G$1" pin="!W" pad="3"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="D" pad="5"/>
<connect gate="G$1" pin="Q" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STA013S" prefix="IC">
<description>&lt;b&gt;MP3 AUDIO DECODER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="STA013"/>
<gate name="B" symbol="STA013PW"/>
</gates>
<devices>
<device name="" package="SO28W">
<connects>
<connect gate="A" pin="!RESET" pad="26"/>
<connect gate="A" pin="!SRC_INT" pad="8"/>
<connect gate="A" pin="!TESTEN" pad="24"/>
<connect gate="A" pin="BIT_EN" pad="7"/>
<connect gate="A" pin="FILT" pad="19"/>
<connect gate="A" pin="LRCKT" pad="11"/>
<connect gate="A" pin="OCLK" pad="12"/>
<connect gate="A" pin="OUT/DATA" pad="28"/>
<connect gate="A" pin="SCANEN" pad="25"/>
<connect gate="A" pin="SCKR" pad="6"/>
<connect gate="A" pin="SCKT" pad="10"/>
<connect gate="A" pin="SCL" pad="4"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="SDI" pad="5"/>
<connect gate="A" pin="SDO" pad="9"/>
<connect gate="A" pin="XTI" pad="21"/>
<connect gate="A" pin="XTO" pad="20"/>
<connect gate="B" pin="PVDD" pad="17"/>
<connect gate="B" pin="PVSS" pad="18"/>
<connect gate="B" pin="VDD_1" pad="1"/>
<connect gate="B" pin="VDD_2" pad="14"/>
<connect gate="B" pin="VDD_3" pad="16"/>
<connect gate="B" pin="VDD_4" pad="23"/>
<connect gate="B" pin="VSS_1" pad="2"/>
<connect gate="B" pin="VSS_2" pad="13"/>
<connect gate="B" pin="VSS_3" pad="15"/>
<connect gate="B" pin="VSS_4" pad="22"/>
<connect gate="B" pin="VSS_5" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STA013$"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="57P0489"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STA013TS" prefix="IC">
<description>&lt;b&gt;MP3 AUDIO DECODER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="STA013"/>
<gate name="B" symbol="STA013PW"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="A" pin="!RESET" pad="25"/>
<connect gate="A" pin="!SRC_INT" pad="40"/>
<connect gate="A" pin="!TESTEN" pad="22"/>
<connect gate="A" pin="BIT_EN" pad="38"/>
<connect gate="A" pin="FILT" pad="12"/>
<connect gate="A" pin="LRCKT" pad="2"/>
<connect gate="A" pin="OCLK" pad="3"/>
<connect gate="A" pin="OUT/DATA" pad="27"/>
<connect gate="A" pin="SCANEN" pad="24"/>
<connect gate="A" pin="SCKR" pad="36"/>
<connect gate="A" pin="SCKT" pad="44"/>
<connect gate="A" pin="SCL" pad="32"/>
<connect gate="A" pin="SDA" pad="31"/>
<connect gate="A" pin="SDI" pad="34"/>
<connect gate="A" pin="SDO" pad="42"/>
<connect gate="A" pin="XTI" pad="15"/>
<connect gate="A" pin="XTO" pad="13"/>
<connect gate="B" pin="PVDD" pad="10"/>
<connect gate="B" pin="PVSS" pad="11"/>
<connect gate="B" pin="VDD_1" pad="29"/>
<connect gate="B" pin="VDD_2" pad="6"/>
<connect gate="B" pin="VDD_3" pad="8"/>
<connect gate="B" pin="VDD_4" pad="21"/>
<connect gate="B" pin="VSS_1" pad="30"/>
<connect gate="B" pin="VSS_2" pad="5"/>
<connect gate="B" pin="VSS_3" pad="7"/>
<connect gate="B" pin="VSS_4" pad="19"/>
<connect gate="B" pin="VSS_5" pad="26"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="28"/>
<connect gate="NC11" pin="NC" pad="33"/>
<connect gate="NC12" pin="NC" pad="35"/>
<connect gate="NC13" pin="NC" pad="37"/>
<connect gate="NC14" pin="NC" pad="39"/>
<connect gate="NC15" pin="NC" pad="41"/>
<connect gate="NC16" pin="NC" pad="43"/>
<connect gate="NC2" pin="NC" pad="4"/>
<connect gate="NC3" pin="NC" pad="9"/>
<connect gate="NC4" pin="NC" pad="14"/>
<connect gate="NC5" pin="NC" pad="16"/>
<connect gate="NC6" pin="NC" pad="17"/>
<connect gate="NC7" pin="NC" pad="18"/>
<connect gate="NC8" pin="NC" pad="20"/>
<connect gate="NC9" pin="NC" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STA013T$"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="57P0492"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STA015" prefix="IC">
<description>&lt;b&gt;MP3 AUDIO DECODER&lt;/b&gt;&lt;p&gt;
with ADPCM capability</description>
<gates>
<gate name="A" symbol="STA015S"/>
<gate name="B" symbol="STA015PW"/>
</gates>
<devices>
<device name="" package="SO28W">
<connects>
<connect gate="A" pin="!RESET" pad="26"/>
<connect gate="A" pin="!TESTEN" pad="24"/>
<connect gate="A" pin="BIT_EN" pad="7"/>
<connect gate="A" pin="CRCK_ADC" pad="27"/>
<connect gate="A" pin="DATA-REQ" pad="28"/>
<connect gate="A" pin="FILT" pad="19"/>
<connect gate="A" pin="LRCKT" pad="11"/>
<connect gate="A" pin="OCLK" pad="12"/>
<connect gate="A" pin="SCKR" pad="6"/>
<connect gate="A" pin="SCKT" pad="10"/>
<connect gate="A" pin="SCK_ADC" pad="8"/>
<connect gate="A" pin="SCL" pad="4"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="SDI" pad="5"/>
<connect gate="A" pin="SDI_ADC" pad="25"/>
<connect gate="A" pin="SDO" pad="9"/>
<connect gate="A" pin="XTI" pad="21"/>
<connect gate="A" pin="XTO" pad="20"/>
<connect gate="B" pin="PVDD" pad="17"/>
<connect gate="B" pin="PVSS" pad="18"/>
<connect gate="B" pin="VDD_1" pad="1"/>
<connect gate="B" pin="VDD_2" pad="14"/>
<connect gate="B" pin="VDD_3" pad="16"/>
<connect gate="B" pin="VDD_4" pad="23"/>
<connect gate="B" pin="VSS_1" pad="2"/>
<connect gate="B" pin="VSS_2" pad="13"/>
<connect gate="B" pin="VSS_3" pad="15"/>
<connect gate="B" pin="VSS_4" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STA015$"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M6100"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STA015TS" prefix="IC">
<description>&lt;b&gt;MP3 AUDIO DECODER&lt;/b&gt;&lt;p&gt;
with ADPCM capability</description>
<gates>
<gate name="A" symbol="STA015TS"/>
<gate name="B" symbol="STA015PW"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="A" pin="!RESET" pad="25"/>
<connect gate="A" pin="!TESTEN" pad="22"/>
<connect gate="A" pin="BIT_EN" pad="38"/>
<connect gate="A" pin="CRCK_ADC" pad="26"/>
<connect gate="A" pin="DATA-REQ" pad="27"/>
<connect gate="A" pin="FILT" pad="12"/>
<connect gate="A" pin="GPIO_STRB" pad="35"/>
<connect gate="A" pin="GPSO_DATA" pad="33"/>
<connect gate="A" pin="GPSO_REQ" pad="4"/>
<connect gate="A" pin="GPSO_SCKL" pad="28"/>
<connect gate="A" pin="IODATA0" pad="20"/>
<connect gate="A" pin="IODATA1" pad="18"/>
<connect gate="A" pin="IODATA2" pad="16"/>
<connect gate="A" pin="IODATA3" pad="14"/>
<connect gate="A" pin="IODATA4" pad="37"/>
<connect gate="A" pin="IODATA5" pad="39"/>
<connect gate="A" pin="IODATA6" pad="41"/>
<connect gate="A" pin="IODATA7" pad="43"/>
<connect gate="A" pin="LRCKT" pad="2"/>
<connect gate="A" pin="OCLK" pad="3"/>
<connect gate="A" pin="SCKR" pad="36"/>
<connect gate="A" pin="SCKT" pad="44"/>
<connect gate="A" pin="SCK_ADC" pad="40"/>
<connect gate="A" pin="SCL" pad="32"/>
<connect gate="A" pin="SDA" pad="31"/>
<connect gate="A" pin="SDI" pad="34"/>
<connect gate="A" pin="SDI_ADC" pad="24"/>
<connect gate="A" pin="SDO" pad="42"/>
<connect gate="A" pin="XTI" pad="15"/>
<connect gate="A" pin="XTO" pad="13"/>
<connect gate="B" pin="PVDD" pad="10"/>
<connect gate="B" pin="PVSS" pad="11"/>
<connect gate="B" pin="VDD_1" pad="29"/>
<connect gate="B" pin="VDD_2" pad="6"/>
<connect gate="B" pin="VDD_3" pad="8"/>
<connect gate="B" pin="VDD_4" pad="21"/>
<connect gate="B" pin="VSS_1" pad="30"/>
<connect gate="B" pin="VSS_2" pad="5"/>
<connect gate="B" pin="VSS_3" pad="7"/>
<connect gate="B" pin="VSS_4" pad="19"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC2" pin="NC" pad="9"/>
<connect gate="NC3" pin="NC" pad="17"/>
<connect gate="NC4" pin="NC" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STA015T$"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M6104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STV5730A" prefix="IC">
<description>Multistandard &lt;b&gt; ON-SCREEN DISPLAY for VCR, PAY-TV&lt;/b&gt;&lt;p&gt;
Satellite receiver</description>
<gates>
<gate name="G$1" symbol="STV5730A"/>
</gates>
<devices>
<device name="" package="SO28W">
<connects>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AVDD" pad="5"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="BAR" pad="19"/>
<connect gate="G$1" pin="CIN" pad="25"/>
<connect gate="G$1" pin="CLK" pad="12"/>
<connect gate="G$1" pin="CO" pad="18"/>
<connect gate="G$1" pin="COUT" pad="24"/>
<connect gate="G$1" pin="CSN" pad="13"/>
<connect gate="G$1" pin="CSYNC" pad="7"/>
<connect gate="G$1" pin="DATA" pad="11"/>
<connect gate="G$1" pin="DGND" pad="20"/>
<connect gate="G$1" pin="DVDD" pad="6"/>
<connect gate="G$1" pin="FB" pad="17"/>
<connect gate="G$1" pin="FTR" pad="4"/>
<connect gate="G$1" pin="G" pad="15"/>
<connect gate="G$1" pin="LECHAR" pad="22"/>
<connect gate="G$1" pin="LESCREEN" pad="23"/>
<connect gate="G$1" pin="MUTE" pad="10"/>
<connect gate="G$1" pin="R" pad="14"/>
<connect gate="G$1" pin="RES" pad="3"/>
<connect gate="G$1" pin="VIDEOOUT1" pad="27"/>
<connect gate="G$1" pin="VIDEOOUT2" pad="26"/>
<connect gate="G$1" pin="VIDEO_IN" pad="2"/>
<connect gate="G$1" pin="XTAL_IN" pad="8"/>
<connect gate="G$1" pin="XTAL_OUT" pad="9"/>
<connect gate="G$1" pin="YIN" pad="28"/>
<connect gate="G$1" pin="YOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VN460SP" prefix="IC">
<description>&lt;b&gt;SINGLE CHANNEL HIGH SIDE SMART POWER SOLID STATE RELAY&lt;/b&gt;&lt;p&gt;
http://eu.st.com/stonline/ 3732.pdf and 5691.pdf</description>
<gates>
<gate name="G$1" symbol="VN460SP"/>
</gates>
<devices>
<device name="" package="POWER-SO10">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="4"/>
<connect gate="G$1" pin="OUT4" pad="5"/>
<connect gate="G$1" pin="ST" pad="8"/>
<connect gate="G$1" pin="VCC" pad="P"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="VN460SP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="57P5296"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L620" prefix="IC">
<description>&lt;b&gt;DMOS FULL BRIDGE DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L620X"/>
</gates>
<devices>
<device name="1" package="SO20">
<connects>
<connect gate="G$1" pin="CBOOT1" pad="12"/>
<connect gate="G$1" pin="CBOOT2" pad="19"/>
<connect gate="G$1" pin="ENABLE" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="14"/>
<connect gate="G$1" pin="GND@4" pad="15"/>
<connect gate="G$1" pin="GND@5" pad="16"/>
<connect gate="G$1" pin="IN1" pad="13"/>
<connect gate="G$1" pin="IN2" pad="18"/>
<connect gate="G$1" pin="OUT1" pad="11"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="VREF" pad="20"/>
<connect gate="G$1" pin="VS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="L6201"/>
<attribute name="OC_FARNELL" value="1271290"/>
<attribute name="OC_NEWARK" value="89K0750"/>
</technology>
</technologies>
</device>
<device name="2" package="DIL18">
<connects>
<connect gate="G$1" pin="CBOOT1" pad="11"/>
<connect gate="G$1" pin="CBOOT2" pad="17"/>
<connect gate="G$1" pin="ENABLE" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="13"/>
<connect gate="G$1" pin="GND@4" pad="14"/>
<connect gate="G$1" pin="GND@5" pad="15"/>
<connect gate="G$1" pin="IN1" pad="12"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="OUT1" pad="10"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="VREF" pad="18"/>
<connect gate="G$1" pin="VS" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L6202"/>
<attribute name="OC_FARNELL" value="1271291"/>
<attribute name="OC_NEWARK" value="26M0513"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6203" prefix="IC">
<description>&lt;b&gt;DMOS FULL BRIDGE DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L6203"/>
</gates>
<devices>
<device name="" package="MULTIWATT-11">
<connects>
<connect gate="G$1" pin="CBOOT1" pad="4"/>
<connect gate="G$1" pin="CBOOT2" pad="8"/>
<connect gate="G$1" pin="ENABLE" pad="11"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="10"/>
<connect gate="G$1" pin="VREF" pad="9"/>
<connect gate="G$1" pin="VS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L6203"/>
<attribute name="OC_FARNELL" value="1467715"/>
<attribute name="OC_NEWARK" value="56P8434"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6201" prefix="IC">
<description>&lt;b&gt;DMOS FULL BRIDGE DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L6201"/>
</gates>
<devices>
<device name="PS" package="POWERSO-20">
<connects>
<connect gate="G$1" pin="CBOOT1" pad="7"/>
<connect gate="G$1" pin="CBOOT2" pad="14"/>
<connect gate="G$1" pin="ENABLE" pad="17"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="11"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="IN1" pad="8"/>
<connect gate="G$1" pin="IN2" pad="13"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="16"/>
<connect gate="G$1" pin="VREF" pad="15"/>
<connect gate="G$1" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="L6201PS"/>
<attribute name="OC_FARNELL" value="1077146"/>
<attribute name="OC_NEWARK" value="89K0751"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6204" prefix="IC">
<description>&lt;b&gt;DUAL DMOS FULL BRIDGE DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L6204"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="BOOTSTRAP" pad="11"/>
<connect gate="G$1" pin="ENABLE1" pad="3"/>
<connect gate="G$1" pin="ENABLE2" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="15"/>
<connect gate="G$1" pin="GND@3" pad="16"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="19"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="18"/>
<connect gate="G$1" pin="OUT3" pad="7"/>
<connect gate="G$1" pin="OUT4" pad="13"/>
<connect gate="G$1" pin="SENSE1" pad="1"/>
<connect gate="G$1" pin="SENSE2" pad="10"/>
<connect gate="G$1" pin="VBOOT" pad="20"/>
<connect gate="G$1" pin="VS1" pad="17"/>
<connect gate="G$1" pin="VS2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="E-L6204"/>
<attribute name="OC_FARNELL" value="1564367"/>
<attribute name="OC_NEWARK" value="56P7372"/>
</technology>
</technologies>
</device>
<device name="D" package="SO28">
<connects>
<connect gate="G$1" pin="BOOTSTRAP" pad="15"/>
<connect gate="G$1" pin="ENABLE1" pad="3"/>
<connect gate="G$1" pin="ENABLE2" pad="12"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="21"/>
<connect gate="G$1" pin="GND@3" pad="22"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="27"/>
<connect gate="G$1" pin="IN3" pad="13"/>
<connect gate="G$1" pin="IN4" pad="16"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="26"/>
<connect gate="G$1" pin="OUT3" pad="9"/>
<connect gate="G$1" pin="OUT4" pad="17"/>
<connect gate="G$1" pin="SENSE1" pad="1"/>
<connect gate="G$1" pin="SENSE2" pad="14"/>
<connect gate="G$1" pin="VBOOT" pad="28"/>
<connect gate="G$1" pin="VS1" pad="23"/>
<connect gate="G$1" pin="VS2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L6204D"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M3485"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6115" prefix="IC">
<description>&lt;b&gt;QUAD 100 V, DMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L6115"/>
</gates>
<devices>
<device name="" package="MULTIWATT-15">
<connects>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="4"/>
<connect gate="G$1" pin="D3" pad="12"/>
<connect gate="G$1" pin="D4" pad="14"/>
<connect gate="G$1" pin="ENABLE" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="S1" pad="1"/>
<connect gate="G$1" pin="S2" pad="3"/>
<connect gate="G$1" pin="S3" pad="13"/>
<connect gate="G$1" pin="S4" pad="15"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6114" prefix="IC">
<description>&lt;b&gt;QUAD 100 V, DMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L6115"/>
<gate name="P2" symbol="GND"/>
<gate name="P1" symbol="GND"/>
<gate name="P3" symbol="GND"/>
<gate name="P4" symbol="GND"/>
<gate name="P5" symbol="GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="D1" pad="5"/>
<connect gate="G$1" pin="D2" pad="7"/>
<connect gate="G$1" pin="D3" pad="14"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="ENABLE" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN1" pad="10"/>
<connect gate="G$1" pin="IN2" pad="11"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="13"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="S2" pad="6"/>
<connect gate="G$1" pin="S3" pad="15"/>
<connect gate="G$1" pin="S4" pad="17"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="P1" pin="GND" pad="2"/>
<connect gate="P2" pin="GND" pad="3"/>
<connect gate="P3" pin="GND" pad="18"/>
<connect gate="P4" pin="GND" pad="19"/>
<connect gate="P5" pin="GND" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6122" prefix="IC">
<description>&lt;b&gt;100 V DMOS SWITCHES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L6122"/>
<gate name="P1" symbol="GND"/>
<gate name="P2" symbol="GND"/>
<gate name="P3" symbol="GND"/>
<gate name="P4" symbol="GND"/>
<gate name="P5" symbol="GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="ENABLE" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN1" pad="11"/>
<connect gate="G$1" pin="IN2" pad="12"/>
<connect gate="G$1" pin="IN3" pad="13"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="S3" pad="6"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="P1" pin="GND" pad="2"/>
<connect gate="P2" pin="GND" pad="3"/>
<connect gate="P3" pin="GND" pad="18"/>
<connect gate="P4" pin="GND" pad="19"/>
<connect gate="P5" pin="GND" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6123" prefix="IC">
<description>&lt;b&gt;100 V DMOS SWITCHES&lt;/b&gt;</description>
<gates>
<gate name="P1" symbol="L6122"/>
</gates>
<devices>
<device name="" package="MULTIWATT-15">
<connects>
<connect gate="P1" pin="D1" pad="15"/>
<connect gate="P1" pin="D2" pad="14"/>
<connect gate="P1" pin="D3" pad="12"/>
<connect gate="P1" pin="ENABLE" pad="7"/>
<connect gate="P1" pin="GND" pad="8"/>
<connect gate="P1" pin="IN1" pad="9"/>
<connect gate="P1" pin="IN2" pad="10"/>
<connect gate="P1" pin="IN3" pad="11"/>
<connect gate="P1" pin="S1" pad="1"/>
<connect gate="P1" pin="S2" pad="3"/>
<connect gate="P1" pin="S3" pad="5"/>
<connect gate="P1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6205" prefix="IC">
<description>&lt;b&gt;DUAL DMOS FULL BRIDGE MOTOR DRIVER&lt;/b&gt;</description>
<gates>
<gate name="P1" symbol="L6205"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="P1" pin="EN_A" pad="20"/>
<connect gate="P1" pin="EN_B" pad="11"/>
<connect gate="P1" pin="GND" pad="5"/>
<connect gate="P1" pin="GND@1" pad="6"/>
<connect gate="P1" pin="GND@2" pad="15"/>
<connect gate="P1" pin="GND@3" pad="16"/>
<connect gate="P1" pin="IN1_A" pad="1"/>
<connect gate="P1" pin="IN1_B" pad="9"/>
<connect gate="P1" pin="IN2_A" pad="2"/>
<connect gate="P1" pin="IN2_B" pad="10"/>
<connect gate="P1" pin="OUT1A" pad="4"/>
<connect gate="P1" pin="OUT1B" pad="7"/>
<connect gate="P1" pin="OUT2A" pad="18"/>
<connect gate="P1" pin="OUT2B" pad="13"/>
<connect gate="P1" pin="SENSE_A" pad="3"/>
<connect gate="P1" pin="SENSE_B" pad="8"/>
<connect gate="P1" pin="VBOOT" pad="12"/>
<connect gate="P1" pin="VCP" pad="19"/>
<connect gate="P1" pin="VS_A" pad="17"/>
<connect gate="P1" pin="VS_B" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="L6205N"/>
<attribute name="OC_FARNELL" value="1564367"/>
<attribute name="OC_NEWARK" value="89K0754"/>
</technology>
</technologies>
</device>
<device name="PD" package="POWERSO-20">
<connects>
<connect gate="P1" pin="EN_A" pad="5"/>
<connect gate="P1" pin="EN_B" pad="16"/>
<connect gate="P1" pin="GND" pad="1"/>
<connect gate="P1" pin="GND@1" pad="10"/>
<connect gate="P1" pin="GND@2" pad="11"/>
<connect gate="P1" pin="GND@3" pad="20"/>
<connect gate="P1" pin="IN1_A" pad="6"/>
<connect gate="P1" pin="IN1_B" pad="14"/>
<connect gate="P1" pin="IN2_A" pad="7"/>
<connect gate="P1" pin="IN2_B" pad="15"/>
<connect gate="P1" pin="OUT1A" pad="9"/>
<connect gate="P1" pin="OUT1B" pad="12"/>
<connect gate="P1" pin="OUT2A" pad="3"/>
<connect gate="P1" pin="OUT2B" pad="18"/>
<connect gate="P1" pin="SENSE_A" pad="8"/>
<connect gate="P1" pin="SENSE_B" pad="13"/>
<connect gate="P1" pin="VBOOT" pad="17"/>
<connect gate="P1" pin="VCP" pad="4"/>
<connect gate="P1" pin="VS_A" pad="2"/>
<connect gate="P1" pin="VS_B" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="L6205PD"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89K0755"/>
</technology>
</technologies>
</device>
<device name="D" package="SO20">
<connects>
<connect gate="P1" pin="EN_A" pad="20"/>
<connect gate="P1" pin="EN_B" pad="11"/>
<connect gate="P1" pin="GND" pad="5"/>
<connect gate="P1" pin="GND@1" pad="6"/>
<connect gate="P1" pin="GND@2" pad="15"/>
<connect gate="P1" pin="GND@3" pad="16"/>
<connect gate="P1" pin="IN1_A" pad="1"/>
<connect gate="P1" pin="IN1_B" pad="9"/>
<connect gate="P1" pin="IN2_A" pad="2"/>
<connect gate="P1" pin="IN2_B" pad="10"/>
<connect gate="P1" pin="OUT1A" pad="4"/>
<connect gate="P1" pin="OUT1B" pad="7"/>
<connect gate="P1" pin="OUT2A" pad="18"/>
<connect gate="P1" pin="OUT2B" pad="13"/>
<connect gate="P1" pin="SENSE_A" pad="3"/>
<connect gate="P1" pin="SENSE_B" pad="8"/>
<connect gate="P1" pin="VBOOT" pad="12"/>
<connect gate="P1" pin="VCP" pad="19"/>
<connect gate="P1" pin="VS_A" pad="17"/>
<connect gate="P1" pin="VS_B" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L6205D"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M3487"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6207" prefix="IC">
<description>&lt;b&gt;DUAL DMOS FULL BRIDGE MOTOR DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L6207"/>
</gates>
<devices>
<device name="PSO36" package="POWERSO-36">
<connects>
<connect gate="G$1" pin="EN_A" pad="8"/>
<connect gate="G$1" pin="EN_B" pad="29"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="36"/>
<connect gate="G$1" pin="IN1_A" pad="10"/>
<connect gate="G$1" pin="IN1_B" pad="26"/>
<connect gate="G$1" pin="IN2_A" pad="11"/>
<connect gate="G$1" pin="IN2_B" pad="27"/>
<connect gate="G$1" pin="OUT1A" pad="15"/>
<connect gate="G$1" pin="OUT1B" pad="22"/>
<connect gate="G$1" pin="OUT2A" pad="5"/>
<connect gate="G$1" pin="OUT2B" pad="32"/>
<connect gate="G$1" pin="RCA" pad="13"/>
<connect gate="G$1" pin="RCB" pad="24"/>
<connect gate="G$1" pin="SENSE_A" pad="12"/>
<connect gate="G$1" pin="SENSE_B" pad="25"/>
<connect gate="G$1" pin="VBOOT" pad="30"/>
<connect gate="G$1" pin="VCP" pad="7"/>
<connect gate="G$1" pin="VREF_A" pad="9"/>
<connect gate="G$1" pin="VREF_B" pad="28"/>
<connect gate="G$1" pin="VS_A" pad="4"/>
<connect gate="G$1" pin="VS_B" pad="33"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="56P8448"/>
</technology>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="G$1" pin="EN_A" pad="23"/>
<connect gate="G$1" pin="EN_B" pad="14"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="19"/>
<connect gate="G$1" pin="IN1_A" pad="1"/>
<connect gate="G$1" pin="IN1_B" pad="12"/>
<connect gate="G$1" pin="IN2_A" pad="2"/>
<connect gate="G$1" pin="IN2_B" pad="11"/>
<connect gate="G$1" pin="OUT1A" pad="5"/>
<connect gate="G$1" pin="OUT1B" pad="8"/>
<connect gate="G$1" pin="OUT2A" pad="21"/>
<connect gate="G$1" pin="OUT2B" pad="16"/>
<connect gate="G$1" pin="RCA" pad="4"/>
<connect gate="G$1" pin="RCB" pad="9"/>
<connect gate="G$1" pin="SENSE_A" pad="3"/>
<connect gate="G$1" pin="SENSE_B" pad="10"/>
<connect gate="G$1" pin="VBOOT" pad="15"/>
<connect gate="G$1" pin="VCP" pad="22"/>
<connect gate="G$1" pin="VREF_A" pad="24"/>
<connect gate="G$1" pin="VREF_B" pad="13"/>
<connect gate="G$1" pin="VS_A" pad="20"/>
<connect gate="G$1" pin="VS_B" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L6207D"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="42M9976"/>
</technology>
</technologies>
</device>
<device name="N" package="DIL24S">
<connects>
<connect gate="G$1" pin="EN_A" pad="23"/>
<connect gate="G$1" pin="EN_B" pad="14"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="19"/>
<connect gate="G$1" pin="IN1_A" pad="1"/>
<connect gate="G$1" pin="IN1_B" pad="12"/>
<connect gate="G$1" pin="IN2_A" pad="2"/>
<connect gate="G$1" pin="IN2_B" pad="11"/>
<connect gate="G$1" pin="OUT1A" pad="5"/>
<connect gate="G$1" pin="OUT1B" pad="8"/>
<connect gate="G$1" pin="OUT2A" pad="21"/>
<connect gate="G$1" pin="OUT2B" pad="16"/>
<connect gate="G$1" pin="RCA" pad="4"/>
<connect gate="G$1" pin="RCB" pad="9"/>
<connect gate="G$1" pin="SENSE_A" pad="3"/>
<connect gate="G$1" pin="SENSE_B" pad="10"/>
<connect gate="G$1" pin="VBOOT" pad="15"/>
<connect gate="G$1" pin="VCP" pad="22"/>
<connect gate="G$1" pin="VREF_A" pad="24"/>
<connect gate="G$1" pin="VREF_B" pad="13"/>
<connect gate="G$1" pin="VS_A" pad="20"/>
<connect gate="G$1" pin="VS_B" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L6207N"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="56P8447"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA3718*" prefix="IC">
<description>&lt;b&gt;STEPPER MOTOR DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TAE3718"/>
</gates>
<devices>
<device name="P" package="MULTIWATT-15">
<connects>
<connect gate="G$1" pin="ALARM" pad="7"/>
<connect gate="G$1" pin="COMP-IN" pad="5"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN0" pad="4"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="OUTA" pad="12"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="PHASE" pad="3"/>
<connect gate="G$1" pin="PULSE-TIME" pad="11"/>
<connect gate="G$1" pin="REFERENCE" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="13"/>
<connect gate="G$1" pin="VSA" pad="10"/>
<connect gate="G$1" pin="VSB" pad="15"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="E-TEA3718SP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M2588"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA3718*D" prefix="IC">
<description>&lt;b&gt;STEPPER MOTOR DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TAE3718D"/>
<gate name="G2" symbol="GND"/>
<gate name="G1" symbol="GND"/>
<gate name="G3" symbol="GND"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="COMP-IN" pad="10"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN0" pad="9"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="15"/>
<connect gate="G$1" pin="OUTB" pad="1"/>
<connect gate="G$1" pin="PHASE" pad="8"/>
<connect gate="G$1" pin="PULSE-TIME" pad="2"/>
<connect gate="G$1" pin="REFERENCE" pad="11"/>
<connect gate="G$1" pin="SENSE" pad="16"/>
<connect gate="G$1" pin="VSA" pad="14"/>
<connect gate="G$1" pin="VSB" pad="3"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G1" pin="GND" pad="5"/>
<connect gate="G2" pin="GND" pad="12"/>
<connect gate="G3" pin="GND" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="E-TEA3718DP"/>
<attribute name="OC_FARNELL" value="1159696"/>
<attribute name="OC_NEWARK" value="91K9593"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="E-TEA3718SDP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="56P7421"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA3718SF" prefix="IC">
<description>&lt;b&gt;STEPPER MOTOR DRIVER&lt;/b&gt;</description>
<gates>
<gate name="." symbol="TAE3718"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
</gates>
<devices>
<device name="P" package="SO20">
<connects>
<connect gate="." pin="ALARM" pad="14"/>
<connect gate="." pin="COMP-IN" pad="12"/>
<connect gate="." pin="GND" pad="5"/>
<connect gate="." pin="IN0" pad="11"/>
<connect gate="." pin="IN1" pad="9"/>
<connect gate="." pin="OUTA" pad="19"/>
<connect gate="." pin="OUTB" pad="1"/>
<connect gate="." pin="PHASE" pad="10"/>
<connect gate="." pin="PULSE-TIME" pad="2"/>
<connect gate="." pin="REFERENCE" pad="13"/>
<connect gate="." pin="SENSE" pad="20"/>
<connect gate="." pin="VSA" pad="18"/>
<connect gate="." pin="VSB" pad="3"/>
<connect gate="." pin="VSS" pad="8"/>
<connect gate="G1" pin="GND" pad="6"/>
<connect gate="G2" pin="GND" pad="15"/>
<connect gate="G3" pin="GND" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="E-TEA3718SFP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="56P7422"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L9637D" prefix="IC">
<description>&lt;b&gt;ISO 9141 INTERFACE&lt;/b&gt;&lt;p&gt;
Source: 1765.pdf</description>
<gates>
<gate name="G$1" symbol="L9637D"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="K" pad="6"/>
<connect gate="G$1" pin="LI" pad="8"/>
<connect gate="G$1" pin="LO" pad="2"/>
<connect gate="G$1" pin="RX" pad="1"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L9637D"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="56P8926"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M68AW128M" prefix="IC">
<description>&lt;b&gt;2 Mbit (128K x16) 3.0V Asynchronous SRAM&lt;/b&gt;&lt;p&gt;
Source: Source: http://us.st.com/stonline/products/literature/ds/7995.pdf</description>
<gates>
<gate name="G$1" symbol="M68AW128M"/>
<gate name="P" symbol="VCC2-VSS2"/>
</gates>
<devices>
<device name="ND" package="TSOP44-II">
<connects>
<connect gate="G$1" pin="!E" pad="6"/>
<connect gate="G$1" pin="!G" pad="41"/>
<connect gate="G$1" pin="!LB" pad="39"/>
<connect gate="G$1" pin="!UB" pad="40"/>
<connect gate="G$1" pin="!W" pad="17"/>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A10" pad="25"/>
<connect gate="G$1" pin="A11" pad="24"/>
<connect gate="G$1" pin="A12" pad="22"/>
<connect gate="G$1" pin="A13" pad="21"/>
<connect gate="G$1" pin="A14" pad="20"/>
<connect gate="G$1" pin="A15" pad="19"/>
<connect gate="G$1" pin="A16" pad="18"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="2"/>
<connect gate="G$1" pin="A4" pad="1"/>
<connect gate="G$1" pin="A5" pad="44"/>
<connect gate="G$1" pin="A6" pad="43"/>
<connect gate="G$1" pin="A7" pad="42"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="D0" pad="7"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="D10" pad="31"/>
<connect gate="G$1" pin="D11" pad="32"/>
<connect gate="G$1" pin="D12" pad="35"/>
<connect gate="G$1" pin="D13" pad="36"/>
<connect gate="G$1" pin="D14" pad="37"/>
<connect gate="G$1" pin="D15" pad="38"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="15"/>
<connect gate="G$1" pin="D7" pad="16"/>
<connect gate="G$1" pin="D8" pad="29"/>
<connect gate="G$1" pin="D9" pad="30"/>
<connect gate="P" pin="VCC@1" pad="11"/>
<connect gate="P" pin="VCC@2" pad="33"/>
<connect gate="P" pin="VSS@1" pad="12"/>
<connect gate="P" pin="VSS@2" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="ZB" package="TFBGA48">
<connects>
<connect gate="G$1" pin="!E" pad="B5"/>
<connect gate="G$1" pin="!G" pad="A2"/>
<connect gate="G$1" pin="!LB" pad="A1"/>
<connect gate="G$1" pin="!UB" pad="B2"/>
<connect gate="G$1" pin="!W" pad="G5"/>
<connect gate="G$1" pin="A0" pad="A3"/>
<connect gate="G$1" pin="A1" pad="A4"/>
<connect gate="G$1" pin="A10" pad="H4"/>
<connect gate="G$1" pin="A11" pad="H5"/>
<connect gate="G$1" pin="A12" pad="G3"/>
<connect gate="G$1" pin="A13" pad="G4"/>
<connect gate="G$1" pin="A14" pad="F3"/>
<connect gate="G$1" pin="A15" pad="F4"/>
<connect gate="G$1" pin="A16" pad="E4"/>
<connect gate="G$1" pin="A2" pad="A5"/>
<connect gate="G$1" pin="A3" pad="B3"/>
<connect gate="G$1" pin="A4" pad="B4"/>
<connect gate="G$1" pin="A5" pad="C3"/>
<connect gate="G$1" pin="A6" pad="C4"/>
<connect gate="G$1" pin="A7" pad="D4"/>
<connect gate="G$1" pin="A8" pad="H2"/>
<connect gate="G$1" pin="A9" pad="H3"/>
<connect gate="G$1" pin="D0" pad="B6"/>
<connect gate="G$1" pin="D1" pad="C5"/>
<connect gate="G$1" pin="D10" pad="C2"/>
<connect gate="G$1" pin="D11" pad="D2"/>
<connect gate="G$1" pin="D12" pad="E2"/>
<connect gate="G$1" pin="D13" pad="F2"/>
<connect gate="G$1" pin="D14" pad="F1"/>
<connect gate="G$1" pin="D15" pad="G1"/>
<connect gate="G$1" pin="D2" pad="C6"/>
<connect gate="G$1" pin="D3" pad="D5"/>
<connect gate="G$1" pin="D4" pad="E5"/>
<connect gate="G$1" pin="D5" pad="F5"/>
<connect gate="G$1" pin="D6" pad="F6"/>
<connect gate="G$1" pin="D7" pad="G6"/>
<connect gate="G$1" pin="D8" pad="B1"/>
<connect gate="G$1" pin="D9" pad="C1"/>
<connect gate="P" pin="VCC@1" pad="D6"/>
<connect gate="P" pin="VCC@2" pad="E1"/>
<connect gate="P" pin="VSS@1" pad="D1"/>
<connect gate="P" pin="VSS@2" pad="E6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M68AW128ML70ZB6"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M5198"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UPSD325*" prefix="IC">
<description>&lt;b&gt;8032 Microcontroller Core&lt;/b&gt; with Flash Programmable System Devices and 256 Kbit SRAM&lt;p&gt;
Sourece: www.st.com/stonline/books/pdf/docs/9202.pdf</description>
<gates>
<gate name="G$1" symbol="UPSD325*-52"/>
</gates>
<devices>
<device name="T6" package="TQFP-10X10-52">
<connects>
<connect gate="G$1" pin="!RESET" pad="44"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="45"/>
<connect gate="G$1" pin="P1.0" pad="34"/>
<connect gate="G$1" pin="P1.1" pad="35"/>
<connect gate="G$1" pin="P1.2" pad="36"/>
<connect gate="G$1" pin="P1.3" pad="37"/>
<connect gate="G$1" pin="P1.4" pad="38"/>
<connect gate="G$1" pin="P1.5" pad="39"/>
<connect gate="G$1" pin="P1.6" pad="40"/>
<connect gate="G$1" pin="P1.7" pad="41"/>
<connect gate="G$1" pin="P3.0" pad="23"/>
<connect gate="G$1" pin="P3.1" pad="24"/>
<connect gate="G$1" pin="P3.2" pad="25"/>
<connect gate="G$1" pin="P3.3" pad="26"/>
<connect gate="G$1" pin="P3.4" pad="27"/>
<connect gate="G$1" pin="P3.5" pad="28"/>
<connect gate="G$1" pin="P3.6" pad="29"/>
<connect gate="G$1" pin="P3.7" pad="30"/>
<connect gate="G$1" pin="P4.0" pad="22"/>
<connect gate="G$1" pin="P4.1" pad="21"/>
<connect gate="G$1" pin="P4.2" pad="20"/>
<connect gate="G$1" pin="P4.3" pad="18"/>
<connect gate="G$1" pin="P4.4" pad="17"/>
<connect gate="G$1" pin="P4.5" pad="16"/>
<connect gate="G$1" pin="P4.6" pad="15"/>
<connect gate="G$1" pin="P4.7" pad="14"/>
<connect gate="G$1" pin="PB0" pad="52"/>
<connect gate="G$1" pin="PB1" pad="51"/>
<connect gate="G$1" pin="PB2" pad="50"/>
<connect gate="G$1" pin="PB3" pad="49"/>
<connect gate="G$1" pin="PB4" pad="48"/>
<connect gate="G$1" pin="PB5" pad="47"/>
<connect gate="G$1" pin="PB6" pad="43"/>
<connect gate="G$1" pin="PB7" pad="42"/>
<connect gate="G$1" pin="PC2" pad="11"/>
<connect gate="G$1" pin="PC3" pad="10"/>
<connect gate="G$1" pin="PC4" pad="6"/>
<connect gate="G$1" pin="PC7" pad="2"/>
<connect gate="G$1" pin="PD1" pad="1"/>
<connect gate="G$1" pin="TCK" pad="12"/>
<connect gate="G$1" pin="TDI" pad="4"/>
<connect gate="G$1" pin="TDO" pad="3"/>
<connect gate="G$1" pin="TMS" pad="13"/>
<connect gate="G$1" pin="USB+" pad="7"/>
<connect gate="G$1" pin="USB-" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="8"/>
<connect gate="G$1" pin="VCC@2" pad="33"/>
<connect gate="G$1" pin="VREF" pad="46"/>
<connect gate="G$1" pin="XTAL1" pad="31"/>
<connect gate="G$1" pin="XTAL2" pad="32"/>
</connects>
<technologies>
<technology name="3B-40">
<attribute name="MF" value=""/>
<attribute name="MPN" value="UPSD3253B-40T6"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="57P4778"/>
</technology>
<technology name="3BV-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="UPSD3253BV-24T6"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M9123"/>
</technology>
<technology name="4A-40">
<attribute name="MF" value=""/>
<attribute name="MPN" value="UPSD3254A-40T6"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="57P4780"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UPSD3254*" prefix="IC">
<description>&lt;b&gt;8032 Microcontroller Core&lt;/b&gt; with Flash Programmable System Devices and 256 Kbit SRAM&lt;p&gt;
Sourece: www.st.com/stonline/books/pdf/docs/9202.pdf</description>
<gates>
<gate name="G$1" symbol="UPSD325*-80"/>
</gates>
<devices>
<device name="U6" package="TQFP-12X12-80">
<connects>
<connect gate="G$1" pin="!PSEN" pad="63"/>
<connect gate="G$1" pin="!RD" pad="65"/>
<connect gate="G$1" pin="!RESET" pad="68"/>
<connect gate="G$1" pin="!WR" pad="62"/>
<connect gate="G$1" pin="A10" pad="55"/>
<connect gate="G$1" pin="A11" pad="57"/>
<connect gate="G$1" pin="A8" pad="51"/>
<connect gate="G$1" pin="A9" pad="53"/>
<connect gate="G$1" pin="AD0" pad="36"/>
<connect gate="G$1" pin="AD1" pad="37"/>
<connect gate="G$1" pin="AD2" pad="38"/>
<connect gate="G$1" pin="AD3" pad="39"/>
<connect gate="G$1" pin="AD4" pad="41"/>
<connect gate="G$1" pin="AD5" pad="43"/>
<connect gate="G$1" pin="AD6" pad="45"/>
<connect gate="G$1" pin="AD7" pad="47"/>
<connect gate="G$1" pin="ALE" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="GND@2" pad="29"/>
<connect gate="G$1" pin="GND@3" pad="69"/>
<connect gate="G$1" pin="P1.0" pad="52"/>
<connect gate="G$1" pin="P1.1" pad="54"/>
<connect gate="G$1" pin="P1.2" pad="56"/>
<connect gate="G$1" pin="P1.3" pad="58"/>
<connect gate="G$1" pin="P1.4" pad="59"/>
<connect gate="G$1" pin="P1.5" pad="60"/>
<connect gate="G$1" pin="P1.6" pad="61"/>
<connect gate="G$1" pin="P1.7" pad="64"/>
<connect gate="G$1" pin="P3.0" pad="75"/>
<connect gate="G$1" pin="P3.1" pad="77"/>
<connect gate="G$1" pin="P3.2" pad="79"/>
<connect gate="G$1" pin="P3.3" pad="2"/>
<connect gate="G$1" pin="P3.4" pad="40"/>
<connect gate="G$1" pin="P3.5" pad="42"/>
<connect gate="G$1" pin="P3.6" pad="44"/>
<connect gate="G$1" pin="P3.7" pad="46"/>
<connect gate="G$1" pin="P4.0" pad="33"/>
<connect gate="G$1" pin="P4.1" pad="31"/>
<connect gate="G$1" pin="P4.2" pad="30"/>
<connect gate="G$1" pin="P4.3" pad="27"/>
<connect gate="G$1" pin="P4.4" pad="25"/>
<connect gate="G$1" pin="P4.5" pad="23"/>
<connect gate="G$1" pin="P4.6" pad="19"/>
<connect gate="G$1" pin="P4.7" pad="18"/>
<connect gate="G$1" pin="PA0" pad="35"/>
<connect gate="G$1" pin="PA1" pad="34"/>
<connect gate="G$1" pin="PA2" pad="32"/>
<connect gate="G$1" pin="PA3" pad="28"/>
<connect gate="G$1" pin="PA4" pad="26"/>
<connect gate="G$1" pin="PA5" pad="24"/>
<connect gate="G$1" pin="PA6" pad="22"/>
<connect gate="G$1" pin="PA7" pad="21"/>
<connect gate="G$1" pin="PB0" pad="80"/>
<connect gate="G$1" pin="PB1" pad="78"/>
<connect gate="G$1" pin="PB2" pad="76"/>
<connect gate="G$1" pin="PB3" pad="74"/>
<connect gate="G$1" pin="PB4" pad="73"/>
<connect gate="G$1" pin="PB5" pad="72"/>
<connect gate="G$1" pin="PB6" pad="67"/>
<connect gate="G$1" pin="PB7" pad="66"/>
<connect gate="G$1" pin="PC2" pad="15"/>
<connect gate="G$1" pin="PC3" pad="14"/>
<connect gate="G$1" pin="PC4" pad="9"/>
<connect gate="G$1" pin="PC7" pad="5"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD2" pad="1"/>
<connect gate="G$1" pin="TCK" pad="16"/>
<connect gate="G$1" pin="TDI" pad="7"/>
<connect gate="G$1" pin="TDO" pad="6"/>
<connect gate="G$1" pin="TMS" pad="20"/>
<connect gate="G$1" pin="USB+" pad="10"/>
<connect gate="G$1" pin="USB-" pad="8"/>
<connect gate="G$1" pin="VCC@1" pad="12"/>
<connect gate="G$1" pin="VCC@2" pad="50"/>
<connect gate="G$1" pin="VREF" pad="70"/>
<connect gate="G$1" pin="XTAL1" pad="48"/>
<connect gate="G$1" pin="XTAL2" pad="49"/>
</connects>
<technologies>
<technology name="A-40">
<attribute name="MF" value=""/>
<attribute name="MPN" value="UPSD3254A-40U6"/>
<attribute name="OC_FARNELL" value="1796098"/>
<attribute name="OC_NEWARK" value="37M9124"/>
</technology>
<technology name="BV-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="UPSD3254BV-24U6"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="57P4782"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE555" prefix="IC">
<description>&lt;b&gt;General purpose bipolar Timer&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="NE555"/>
</gates>
<devices>
<device name="" package="DIL-08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="NE555N"/>
<attribute name="OC_FARNELL" value="1467742"/>
<attribute name="OC_NEWARK" value="89K1486"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE556" prefix="IC">
<description>&lt;b&gt;General Purpose Biopolartimer&lt;/b&gt;&lt;/br&gt;</description>
<gates>
<gate name="G$1" symbol="NE556"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="CONT1" pad="3"/>
<connect gate="G$1" pin="CONT2" pad="11"/>
<connect gate="G$1" pin="DIS1" pad="1"/>
<connect gate="G$1" pin="DIS2" pad="13"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="RESET1" pad="4"/>
<connect gate="G$1" pin="RESET2" pad="10"/>
<connect gate="G$1" pin="TRES1" pad="2"/>
<connect gate="G$1" pin="TRES2" pad="12"/>
<connect gate="G$1" pin="TRIG1" pad="6"/>
<connect gate="G$1" pin="TRIG2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NE556"/>
<attribute name="OC_FARNELL" value="2349784"/>
<attribute name="OC_NEWARK" value="83C0108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNH3SP30" prefix="IC">
<description>&lt;b&gt;FULLY INTEGRATED H-BRIDGE MOTOR DRIVER&lt;/b&gt;&lt;p&gt;
Source: http://pdf1.alldatasheet.com/datasheet-pdf/view/84563/STMICROELECTRONICS/VNH3SP30.html</description>
<gates>
<gate name="G$1" symbol="VNH3SP30"/>
</gates>
<devices>
<device name="" package="MULTIPOWERSO-30">
<connects>
<connect gate="G$1" pin="DIAGA" pad="6"/>
<connect gate="G$1" pin="DIAGB" pad="10"/>
<connect gate="G$1" pin="GNDA" pad="28"/>
<connect gate="G$1" pin="GNDA@1" pad="27"/>
<connect gate="G$1" pin="GNDA@2" pad="26"/>
<connect gate="G$1" pin="GNDB" pad="18"/>
<connect gate="G$1" pin="GNDB@1" pad="19"/>
<connect gate="G$1" pin="GNDB@2" pad="20"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="11"/>
<connect gate="G$1" pin="OUTA" pad="1"/>
<connect gate="G$1" pin="OUTA@1" pad="30"/>
<connect gate="G$1" pin="OUTA@2" pad="25"/>
<connect gate="G$1" pin="OUTA@3" pad="OUTA"/>
<connect gate="G$1" pin="OUTA@4" pad="OUTA@1"/>
<connect gate="G$1" pin="OUTB" pad="15"/>
<connect gate="G$1" pin="OUTB@1" pad="16"/>
<connect gate="G$1" pin="OUTB@2" pad="21"/>
<connect gate="G$1" pin="OUTB@3" pad="OUTB"/>
<connect gate="G$1" pin="OUTB@4" pad="OUTB@1"/>
<connect gate="G$1" pin="PWM" pad="8"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VCC@1" pad="13"/>
<connect gate="G$1" pin="VCC@2" pad="23"/>
<connect gate="G$1" pin="VCC@3" pad="VCC"/>
<connect gate="G$1" pin="VCC@4" pad="VCC@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="VNH3SP30-E"/>
<attribute name="OC_FARNELL" value="1739420"/>
<attribute name="OC_NEWARK" value="33R1486"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB6B1" prefix="IC">
<description>&lt;b&gt;DATA LINES PROTECTION&lt;br&gt;&lt;/b&gt;&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/5605.pdf</description>
<gates>
<gate name="G$1" symbol="USB6B1"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="IO1" pad="2"/>
<connect gate="G$1" pin="IO1@2" pad="7"/>
<connect gate="G$1" pin="IO2" pad="3"/>
<connect gate="G$1" pin="IO2@2" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VCC@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="USB6B1"/>
<attribute name="OC_FARNELL" value="9804358"/>
<attribute name="OC_NEWARK" value="26M4750"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STV5348?*" prefix="IC">
<description>&lt;b&gt;Monochip Teletext And VPS Decoder&lt;/b&gt;&lt;br&gt;
with 8 integrated pages</description>
<gates>
<gate name="G$1" symbol="STV5348"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="BLAN" pad="12"/>
<connect gate="G$1" pin="CBLK" pad="28"/>
<connect gate="G$1" pin="COR" pad="13"/>
<connect gate="G$1" pin="CVBS" pad="1"/>
<connect gate="G$1" pin="DV" pad="19"/>
<connect gate="G$1" pin="FFB" pad="6"/>
<connect gate="G$1" pin="G" pad="9"/>
<connect gate="G$1" pin="L23" pad="18"/>
<connect gate="G$1" pin="MA/SL" pad="2"/>
<connect gate="G$1" pin="ODD/EVEN" pad="14"/>
<connect gate="G$1" pin="POL" pad="4"/>
<connect gate="G$1" pin="R" pad="8"/>
<connect gate="G$1" pin="RESERVED" pad="20"/>
<connect gate="G$1" pin="RGBREF" pad="11"/>
<connect gate="G$1" pin="SCL" pad="16"/>
<connect gate="G$1" pin="SDA" pad="17"/>
<connect gate="G$1" pin="STTV/LFB" pad="5"/>
<connect gate="G$1" pin="TEST" pad="27"/>
<connect gate="G$1" pin="VCR/TV" pad="21"/>
<connect gate="G$1" pin="VDDA" pad="3"/>
<connect gate="G$1" pin="VDDD" pad="22"/>
<connect gate="G$1" pin="VSSA" pad="26"/>
<connect gate="G$1" pin="VSSD" pad="7"/>
<connect gate="G$1" pin="VSSO" pad="25"/>
<connect gate="G$1" pin="XTI" pad="24"/>
<connect gate="G$1" pin="XTO" pad="23"/>
<connect gate="G$1" pin="Y" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="/H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="/T">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="BLAN" pad="12"/>
<connect gate="G$1" pin="CBLK" pad="28"/>
<connect gate="G$1" pin="COR" pad="13"/>
<connect gate="G$1" pin="CVBS" pad="1"/>
<connect gate="G$1" pin="DV" pad="19"/>
<connect gate="G$1" pin="FFB" pad="6"/>
<connect gate="G$1" pin="G" pad="9"/>
<connect gate="G$1" pin="L23" pad="18"/>
<connect gate="G$1" pin="MA/SL" pad="2"/>
<connect gate="G$1" pin="ODD/EVEN" pad="14"/>
<connect gate="G$1" pin="POL" pad="4"/>
<connect gate="G$1" pin="R" pad="8"/>
<connect gate="G$1" pin="RESERVED" pad="20"/>
<connect gate="G$1" pin="RGBREF" pad="11"/>
<connect gate="G$1" pin="SCL" pad="16"/>
<connect gate="G$1" pin="SDA" pad="17"/>
<connect gate="G$1" pin="STTV/LFB" pad="5"/>
<connect gate="G$1" pin="TEST" pad="27"/>
<connect gate="G$1" pin="VCR/TV" pad="21"/>
<connect gate="G$1" pin="VDDA" pad="3"/>
<connect gate="G$1" pin="VDDD" pad="22"/>
<connect gate="G$1" pin="VSSA" pad="26"/>
<connect gate="G$1" pin="VSSD" pad="7"/>
<connect gate="G$1" pin="VSSO" pad="25"/>
<connect gate="G$1" pin="XTI" pad="24"/>
<connect gate="G$1" pin="XTO" pad="23"/>
<connect gate="G$1" pin="Y" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="/T">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS3LV02DQ" prefix="IC">
<description>&lt;b&gt;MEMS INERTIAL SENSOR&lt;/b&gt; 3-Axis - ±2g/±6g Digital Output Low Voltage Linear Accelerometer&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/11115/lis3lv02dq.pdf</description>
<gates>
<gate name="G$1" symbol="LIS3LV02DQ"/>
</gates>
<devices>
<device name="" package="QFPN-28">
<connects>
<connect gate="G$1" pin="CK" pad="16"/>
<connect gate="G$1" pin="CS" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="17"/>
<connect gate="G$1" pin="RDY/INT" pad="6"/>
<connect gate="G$1" pin="SCL/SPC" pad="12"/>
<connect gate="G$1" pin="SDA/SDO/SDI" pad="10"/>
<connect gate="G$1" pin="SDO" pad="9"/>
<connect gate="G$1" pin="VDD@1" pad="3"/>
<connect gate="G$1" pin="VDD@2" pad="19"/>
<connect gate="G$1" pin="VDD_IO" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="LIS3LV02DQ"/>
<attribute name="OC_FARNELL" value="1220909"/>
<attribute name="OC_NEWARK" value="89K0642"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS3L02AQ3" prefix="IC">
<description>&lt;b&gt;3-Axis - ±2g/±6g LINEAR ACCELEROMETER&lt;/b&gt; MEMS INERTIAL SENSOR&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/11020.pdf</description>
<gates>
<gate name="G$1" symbol="LIS3L02AQ3"/>
</gates>
<devices>
<device name="" package="QFN-44-7X7">
<connects>
<connect gate="G$1" pin="FS" pad="16"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PD" pad="14"/>
<connect gate="G$1" pin="ST" pad="7"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VOUTX" pad="8"/>
<connect gate="G$1" pin="VOUTY" pad="6"/>
<connect gate="G$1" pin="VOUTZ" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="LIS3L02AQ3"/>
<attribute name="OC_FARNELL" value="1467821"/>
<attribute name="OC_NEWARK" value="89K0645"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M27C4001" prefix="IC">
<description>&lt;b&gt;4 Mbit (512Kb x 8) UV EPROM and OTP EPROM&lt;/b&gt;&lt;p&gt;
Source: www.st.com .. M27C4001 EPROM 4 MBIT.pdf</description>
<gates>
<gate name="G$1" symbol="M27C4001"/>
</gates>
<devices>
<device name="N" package="TSOP32">
<connects>
<connect gate="G$1" pin="!E" pad="30"/>
<connect gate="G$1" pin="!G" pad="32"/>
<connect gate="G$1" pin="A0" pad="20"/>
<connect gate="G$1" pin="A1" pad="19"/>
<connect gate="G$1" pin="A10" pad="31"/>
<connect gate="G$1" pin="A11" pad="1"/>
<connect gate="G$1" pin="A12" pad="12"/>
<connect gate="G$1" pin="A13" pad="4"/>
<connect gate="G$1" pin="A14" pad="5"/>
<connect gate="G$1" pin="A15" pad="11"/>
<connect gate="G$1" pin="A16" pad="10"/>
<connect gate="G$1" pin="A17" pad="6"/>
<connect gate="G$1" pin="A18" pad="7"/>
<connect gate="G$1" pin="A2" pad="18"/>
<connect gate="G$1" pin="A3" pad="17"/>
<connect gate="G$1" pin="A4" pad="16"/>
<connect gate="G$1" pin="A5" pad="15"/>
<connect gate="G$1" pin="A6" pad="14"/>
<connect gate="G$1" pin="A7" pad="13"/>
<connect gate="G$1" pin="A8" pad="3"/>
<connect gate="G$1" pin="A9" pad="2"/>
<connect gate="G$1" pin="D0" pad="21"/>
<connect gate="G$1" pin="D1" pad="22"/>
<connect gate="G$1" pin="D2" pad="23"/>
<connect gate="G$1" pin="D3" pad="25"/>
<connect gate="G$1" pin="D4" pad="26"/>
<connect gate="G$1" pin="D5" pad="27"/>
<connect gate="G$1" pin="D6" pad="28"/>
<connect gate="G$1" pin="D7" pad="29"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VPP" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="C" package="LCC32">
<connects>
<connect gate="G$1" pin="!E" pad="22"/>
<connect gate="G$1" pin="!G" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="19"/>
<connect gate="G$1" pin="D6" pad="20"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="32"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M27C4001-10C1"/>
<attribute name="OC_FARNELL" value="1094260"/>
<attribute name="OC_NEWARK" value="24M5086"/>
</technology>
</technologies>
</device>
<device name="B" package="DIL32">
<connects>
<connect gate="G$1" pin="!E" pad="22"/>
<connect gate="G$1" pin="!G" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="19"/>
<connect gate="G$1" pin="D6" pad="20"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="32"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M27C4001-10B1"/>
<attribute name="OC_FARNELL" value="3338137"/>
<attribute name="OC_NEWARK" value="56P9200"/>
</technology>
</technologies>
</device>
<device name="F" package="FDIP32">
<connects>
<connect gate="G$1" pin="!E" pad="22"/>
<connect gate="G$1" pin="!G" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="19"/>
<connect gate="G$1" pin="D6" pad="20"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="32"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="M27C4001-15F1"/>
<attribute name="OC_FARNELL" value="1132004"/>
<attribute name="OC_NEWARK" value="24M5087"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM8S105C" prefix="IC">
<description>&lt;b&gt;Access line, 16 MHz STM8S 8-bit MCU&lt;/b&gt; up to 32 Kbytes Flash, integrated EEPROM,10-bit ADC, timers, UART, SPI, I²C&lt;p&gt;
Source: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="STM8S105C4-48"/>
</gates>
<devices>
<device name="" package="LQFP48-7X7">
<connects>
<connect gate="G$1" pin="NRST" pad="1"/>
<connect gate="G$1" pin="PA1/OSC" pad="2"/>
<connect gate="G$1" pin="PA2/OSCOUT" pad="3"/>
<connect gate="G$1" pin="PA3/TIM2_CH3[TIM3_CH1]" pad="9"/>
<connect gate="G$1" pin="PA4" pad="10"/>
<connect gate="G$1" pin="PA5" pad="11"/>
<connect gate="G$1" pin="PA6" pad="12"/>
<connect gate="G$1" pin="PB0/AIN0[TIM1_CH1N]" pad="22"/>
<connect gate="G$1" pin="PB1/AIN1[TIM1_CH2N]" pad="21"/>
<connect gate="G$1" pin="PB2/AIN2[TIM1_CH3N]" pad="20"/>
<connect gate="G$1" pin="PB3/AIN3[TIM1_ETR]" pad="19"/>
<connect gate="G$1" pin="PB4/AIN4[I2C_SCL]" pad="18"/>
<connect gate="G$1" pin="PB5/AIN5[I2C_SDA]" pad="17"/>
<connect gate="G$1" pin="PB6/AIN6" pad="16"/>
<connect gate="G$1" pin="PB7/AIN7" pad="15"/>
<connect gate="G$1" pin="PC1/TIM1_CH1/UART2_CK" pad="26"/>
<connect gate="G$1" pin="PC2/TIM1_CH2" pad="27"/>
<connect gate="G$1" pin="PC3/TIM1_CH3" pad="28"/>
<connect gate="G$1" pin="PC4/TIM1_CH4" pad="29"/>
<connect gate="G$1" pin="PC5/SPI_SCK" pad="30"/>
<connect gate="G$1" pin="PC6/SPI_MOSI" pad="33"/>
<connect gate="G$1" pin="PC7/SPI_MISO" pad="34"/>
<connect gate="G$1" pin="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]" pad="41"/>
<connect gate="G$1" pin="PD1/SWIM" pad="42"/>
<connect gate="G$1" pin="PD2/TIM3_CH1[TIM2_CH3]" pad="43"/>
<connect gate="G$1" pin="PD3/TIM2_CH2[ADC_ETR]" pad="44"/>
<connect gate="G$1" pin="PD4/TIM2_CH1[BEEP]" pad="45"/>
<connect gate="G$1" pin="PD5/UART2_TX" pad="46"/>
<connect gate="G$1" pin="PD6/UART2_RX" pad="47"/>
<connect gate="G$1" pin="PD7/TLI[TIM1_CH4]" pad="48"/>
<connect gate="G$1" pin="PE0/CLK_CCO" pad="40"/>
<connect gate="G$1" pin="PE1/I2C_SCL" pad="39"/>
<connect gate="G$1" pin="PE2/I2C_SDA" pad="38"/>
<connect gate="G$1" pin="PE3/TIM1_BKIN" pad="37"/>
<connect gate="G$1" pin="PE5/SPI_NSS" pad="25"/>
<connect gate="G$1" pin="PE6/AIN9" pad="24"/>
<connect gate="G$1" pin="PE7/AIN8" pad="23"/>
<connect gate="G$1" pin="PG0" pad="35"/>
<connect gate="G$1" pin="PG1" pad="36"/>
<connect gate="G$1" pin="VCAP" pad="6"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="13"/>
<connect gate="G$1" pin="VDDIO_1" pad="8"/>
<connect gate="G$1" pin="VDDIO_2" pad="32"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSSA" pad="14"/>
<connect gate="G$1" pin="VSSIO_1" pad="4"/>
<connect gate="G$1" pin="VSSIO_2" pad="31"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105C4T6"/>
<attribute name="OC_FARNELL" value="1706221"/>
<attribute name="OC_NEWARK" value="09R6031"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105C6T6"/>
<attribute name="OC_FARNELL" value="1706222"/>
<attribute name="OC_NEWARK" value="09R6033"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM8S105S" prefix="IC">
<description>&lt;b&gt;Access line, 16 MHz STM8S 8-bit MCU&lt;/b&gt; up to 32 Kbytes Flash, integrated EEPROM,10-bit ADC, timers, UART, SPI, I²C&lt;p&gt;
Source: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="STM8S105C4-44"/>
</gates>
<devices>
<device name="" package="LQFP44-10X10">
<connects>
<connect gate="G$1" pin="NRST" pad="1"/>
<connect gate="G$1" pin="PA1/OSC" pad="2"/>
<connect gate="G$1" pin="PA2/OSCOUT" pad="3"/>
<connect gate="G$1" pin="PA4" pad="9"/>
<connect gate="G$1" pin="PA5" pad="10"/>
<connect gate="G$1" pin="PA6" pad="11"/>
<connect gate="G$1" pin="PB0/AIN0[TIM1_CH1N]" pad="21"/>
<connect gate="G$1" pin="PB1/AIN1[TIM1_CH2N]" pad="20"/>
<connect gate="G$1" pin="PB2/AIN2[TIM1_CH3N]" pad="19"/>
<connect gate="G$1" pin="PB3/AIN3[TIM1_ETR]" pad="18"/>
<connect gate="G$1" pin="PB4/AIN4[I2C_SCL]" pad="17"/>
<connect gate="G$1" pin="PB5/AIN5[I2C_SDA]" pad="16"/>
<connect gate="G$1" pin="PB6/AIN6" pad="15"/>
<connect gate="G$1" pin="PB7/AIN7" pad="14"/>
<connect gate="G$1" pin="PC1/TIM1_CH1/UART2_CK" pad="24"/>
<connect gate="G$1" pin="PC2/TIM1_CH2" pad="25"/>
<connect gate="G$1" pin="PC3/TIM1_CH3" pad="26"/>
<connect gate="G$1" pin="PC5/SPI_SCK" pad="27"/>
<connect gate="G$1" pin="PC6/SPI_MOSI" pad="30"/>
<connect gate="G$1" pin="PC7/SPI_MISO" pad="31"/>
<connect gate="G$1" pin="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]" pad="37"/>
<connect gate="G$1" pin="PD1/SWIM" pad="38"/>
<connect gate="G$1" pin="PD2/TIM3_CH1[TIM2_CH3]" pad="39"/>
<connect gate="G$1" pin="PD3/TIM2_CH2[ADC_ETR]" pad="40"/>
<connect gate="G$1" pin="PD4/TIM2_CH1[BEEP]" pad="41"/>
<connect gate="G$1" pin="PD5/UART2_TX" pad="42"/>
<connect gate="G$1" pin="PD6/UART2_RX" pad="43"/>
<connect gate="G$1" pin="PD7/TLI[TIM1_CH4]" pad="44"/>
<connect gate="G$1" pin="PE0/CLK_CCO" pad="36"/>
<connect gate="G$1" pin="PE1/I2C_SCL" pad="35"/>
<connect gate="G$1" pin="PE2/I2C_SDA" pad="34"/>
<connect gate="G$1" pin="PE5/SPI_NSS" pad="23"/>
<connect gate="G$1" pin="PE6/AIN9" pad="22"/>
<connect gate="G$1" pin="PG0" pad="32"/>
<connect gate="G$1" pin="PG1" pad="33"/>
<connect gate="G$1" pin="VCAP" pad="6"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="12"/>
<connect gate="G$1" pin="VDDIO_1" pad="8"/>
<connect gate="G$1" pin="VDDIO_2" pad="29"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSSA" pad="13"/>
<connect gate="G$1" pin="VSSIO_1" pad="4"/>
<connect gate="G$1" pin="VSSIO_2" pad="28"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105S4T6C"/>
<attribute name="OC_FARNELL" value="1706227"/>
<attribute name="OC_NEWARK" value="09R6037"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105S6T6C"/>
<attribute name="OC_FARNELL" value="1706228"/>
<attribute name="OC_NEWARK" value="09R6038"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM8S105K" prefix="IC">
<description>&lt;b&gt;Access line, 16 MHz STM8S 8-bit MCU&lt;/b&gt; up to 32 Kbytes Flash, integrated EEPROM,10-bit ADC, timers, UART, SPI, I²C&lt;p&gt;
Source: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="STM8S105C4-32"/>
</gates>
<devices>
<device name="T" package="LQFP32-7X7">
<connects>
<connect gate="G$1" pin="NRST" pad="1"/>
<connect gate="G$1" pin="PA1/OSC" pad="2"/>
<connect gate="G$1" pin="PA2/OSCOUT" pad="3"/>
<connect gate="G$1" pin="PB0/AIN0[TIM1_CH1N]" pad="16"/>
<connect gate="G$1" pin="PB1/AIN1[TIM1_CH2N]" pad="15"/>
<connect gate="G$1" pin="PB2/AIN2[TIM1_CH3N]" pad="14"/>
<connect gate="G$1" pin="PB3/AIN3[TIM1_ETR]" pad="13"/>
<connect gate="G$1" pin="PB4/AIN4[I2C_SCL]" pad="12"/>
<connect gate="G$1" pin="PB5/AIN5[I2C_SDA]" pad="11"/>
<connect gate="G$1" pin="PC1/TIM1_CH1/UART2_CK" pad="18"/>
<connect gate="G$1" pin="PC2/TIM1_CH2" pad="19"/>
<connect gate="G$1" pin="PC3/TIM1_CH3" pad="20"/>
<connect gate="G$1" pin="PC4/TIM1_CH4" pad="21"/>
<connect gate="G$1" pin="PC5/SPI_SCK" pad="22"/>
<connect gate="G$1" pin="PC6/SPI_MOSI" pad="23"/>
<connect gate="G$1" pin="PC7/SPI_MISO" pad="24"/>
<connect gate="G$1" pin="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]" pad="25"/>
<connect gate="G$1" pin="PD1/SWIM" pad="26"/>
<connect gate="G$1" pin="PD2/TIM3_CH1[TIM2_CH3]" pad="27"/>
<connect gate="G$1" pin="PD3/TIM2_CH2[ADC_ETR]" pad="28"/>
<connect gate="G$1" pin="PD4/TIM2_CH1[BEEP]" pad="29"/>
<connect gate="G$1" pin="PD5/UART2_TX" pad="30"/>
<connect gate="G$1" pin="PD6/UART2_RX" pad="31"/>
<connect gate="G$1" pin="PD7/TLI[TIM1_CH4]" pad="32"/>
<connect gate="G$1" pin="PE5/SPI_NSS" pad="17"/>
<connect gate="G$1" pin="PF4/AIN12" pad="8"/>
<connect gate="G$1" pin="VCAP" pad="5"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VDDA" pad="9"/>
<connect gate="G$1" pin="VDDIO_1" pad="7"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="VSSA" pad="10"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105K4T6C"/>
<attribute name="OC_FARNELL" value="1706223"/>
<attribute name="OC_NEWARK" value="09R6034"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105K6T6C"/>
<attribute name="OC_FARNELL" value="1706224"/>
<attribute name="OC_NEWARK" value="09R6035"/>
</technology>
</technologies>
</device>
<device name="" package="UFQFPN32">
<connects>
<connect gate="G$1" pin="NRST" pad="1"/>
<connect gate="G$1" pin="PA1/OSC" pad="2"/>
<connect gate="G$1" pin="PA2/OSCOUT" pad="3"/>
<connect gate="G$1" pin="PB0/AIN0[TIM1_CH1N]" pad="16"/>
<connect gate="G$1" pin="PB1/AIN1[TIM1_CH2N]" pad="15"/>
<connect gate="G$1" pin="PB2/AIN2[TIM1_CH3N]" pad="14"/>
<connect gate="G$1" pin="PB3/AIN3[TIM1_ETR]" pad="13"/>
<connect gate="G$1" pin="PB4/AIN4[I2C_SCL]" pad="12"/>
<connect gate="G$1" pin="PB5/AIN5[I2C_SDA]" pad="11"/>
<connect gate="G$1" pin="PC1/TIM1_CH1/UART2_CK" pad="18"/>
<connect gate="G$1" pin="PC2/TIM1_CH2" pad="19"/>
<connect gate="G$1" pin="PC3/TIM1_CH3" pad="20"/>
<connect gate="G$1" pin="PC4/TIM1_CH4" pad="21"/>
<connect gate="G$1" pin="PC5/SPI_SCK" pad="22"/>
<connect gate="G$1" pin="PC6/SPI_MOSI" pad="23"/>
<connect gate="G$1" pin="PC7/SPI_MISO" pad="24"/>
<connect gate="G$1" pin="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]" pad="25"/>
<connect gate="G$1" pin="PD1/SWIM" pad="26"/>
<connect gate="G$1" pin="PD2/TIM3_CH1[TIM2_CH3]" pad="27"/>
<connect gate="G$1" pin="PD3/TIM2_CH2[ADC_ETR]" pad="28"/>
<connect gate="G$1" pin="PD4/TIM2_CH1[BEEP]" pad="29"/>
<connect gate="G$1" pin="PD5/UART2_TX" pad="30"/>
<connect gate="G$1" pin="PD6/UART2_RX" pad="31"/>
<connect gate="G$1" pin="PD7/TLI[TIM1_CH4]" pad="32"/>
<connect gate="G$1" pin="PE5/SPI_NSS" pad="17"/>
<connect gate="G$1" pin="PF4/AIN12" pad="8"/>
<connect gate="G$1" pin="VCAP" pad="5"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VDDA" pad="9"/>
<connect gate="G$1" pin="VDDIO_1" pad="7"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="VSSA" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105K4U6"/>
<attribute name="OC_FARNELL" value="1706225"/>
<attribute name="OC_NEWARK" value="55R6975"/>
</technology>
</technologies>
</device>
<device name="U" package="VFQFPN32">
<connects>
<connect gate="G$1" pin="NRST" pad="1"/>
<connect gate="G$1" pin="PA1/OSC" pad="2"/>
<connect gate="G$1" pin="PA2/OSCOUT" pad="3"/>
<connect gate="G$1" pin="PB0/AIN0[TIM1_CH1N]" pad="16"/>
<connect gate="G$1" pin="PB1/AIN1[TIM1_CH2N]" pad="15"/>
<connect gate="G$1" pin="PB2/AIN2[TIM1_CH3N]" pad="14"/>
<connect gate="G$1" pin="PB3/AIN3[TIM1_ETR]" pad="13"/>
<connect gate="G$1" pin="PB4/AIN4[I2C_SCL]" pad="12"/>
<connect gate="G$1" pin="PB5/AIN5[I2C_SDA]" pad="11"/>
<connect gate="G$1" pin="PC1/TIM1_CH1/UART2_CK" pad="18"/>
<connect gate="G$1" pin="PC2/TIM1_CH2" pad="19"/>
<connect gate="G$1" pin="PC3/TIM1_CH3" pad="20"/>
<connect gate="G$1" pin="PC4/TIM1_CH4" pad="21"/>
<connect gate="G$1" pin="PC5/SPI_SCK" pad="22"/>
<connect gate="G$1" pin="PC6/SPI_MOSI" pad="23"/>
<connect gate="G$1" pin="PC7/SPI_MISO" pad="24"/>
<connect gate="G$1" pin="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]" pad="25"/>
<connect gate="G$1" pin="PD1/SWIM" pad="26"/>
<connect gate="G$1" pin="PD2/TIM3_CH1[TIM2_CH3]" pad="27"/>
<connect gate="G$1" pin="PD3/TIM2_CH2[ADC_ETR]" pad="28"/>
<connect gate="G$1" pin="PD4/TIM2_CH1[BEEP]" pad="29"/>
<connect gate="G$1" pin="PD5/UART2_TX" pad="30"/>
<connect gate="G$1" pin="PD6/UART2_RX" pad="31"/>
<connect gate="G$1" pin="PD7/TLI[TIM1_CH4]" pad="32"/>
<connect gate="G$1" pin="PE5/SPI_NSS" pad="17"/>
<connect gate="G$1" pin="PF4/AIN12" pad="8"/>
<connect gate="G$1" pin="VCAP" pad="5"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VDDA" pad="9"/>
<connect gate="G$1" pin="VDDIO_1" pad="7"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="VSSA" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105K6U6"/>
<attribute name="OC_FARNELL" value="1706225"/>
<attribute name="OC_NEWARK" value="09R6036"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM8S105K*B" prefix="IC">
<description>&lt;b&gt;Access line, 16 MHz STM8S 8-bit MCU&lt;/b&gt; up to 32 Kbytes Flash, integrated EEPROM,10-bit ADC, timers, UART, SPI, I²C&lt;p&gt;
Source: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="STM8S105C4-32P"/>
</gates>
<devices>
<device name="" package="FDIP32">
<connects>
<connect gate="G$1" pin="NRST" pad="6"/>
<connect gate="G$1" pin="PA1/OSC" pad="7"/>
<connect gate="G$1" pin="PA2/OSCOUT" pad="8"/>
<connect gate="G$1" pin="PB0/AIN0[TIM1_CH1N]" pad="21"/>
<connect gate="G$1" pin="PB1/AIN1[TIM1_CH2N]" pad="20"/>
<connect gate="G$1" pin="PB2/AIN2[TIM1_CH3N]" pad="19"/>
<connect gate="G$1" pin="PB3/AIN3[TIM1_ETR]" pad="18"/>
<connect gate="G$1" pin="PB4/AIN4[I2C_SCL]" pad="17"/>
<connect gate="G$1" pin="PB5/AIN5[I2C_SDA]" pad="16"/>
<connect gate="G$1" pin="PC1/TIM1_CH1/UART2_CK" pad="23"/>
<connect gate="G$1" pin="PC2/TIM1_CH2" pad="24"/>
<connect gate="G$1" pin="PC3/TIM1_CH3" pad="25"/>
<connect gate="G$1" pin="PC4/TIM1_CH4" pad="26"/>
<connect gate="G$1" pin="PC5/SPI_SCK" pad="27"/>
<connect gate="G$1" pin="PC6/SPI_MOSI" pad="28"/>
<connect gate="G$1" pin="PC7/SPI_MISO" pad="29"/>
<connect gate="G$1" pin="PD0/TIM3_CH2[TIM1_BKIN][CLK_CCO]" pad="30"/>
<connect gate="G$1" pin="PD1/SWIM" pad="31"/>
<connect gate="G$1" pin="PD2/TIM3_CH1[TIM2_CH3]" pad="32"/>
<connect gate="G$1" pin="PD3/TIM2_CH2[ADC_ETR]" pad="1"/>
<connect gate="G$1" pin="PD4/TIM2_CH1[BEEP]" pad="2"/>
<connect gate="G$1" pin="PD5/UART2_TX" pad="3"/>
<connect gate="G$1" pin="PD6/UART2_RX" pad="4"/>
<connect gate="G$1" pin="PD7/TLI[TIM1_CH4]" pad="5"/>
<connect gate="G$1" pin="PE5/SPI_NSS" pad="22"/>
<connect gate="G$1" pin="PF4/AIN12" pad="13"/>
<connect gate="G$1" pin="VCAP" pad="10"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDDA" pad="14"/>
<connect gate="G$1" pin="VDDIO_1" pad="12"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSSA" pad="15"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105K4B6"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="55R6973"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value="STM8S105K6B6"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="55R6976"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L293DD" prefix="IC">
<description>&lt;b&gt;PUSH-PULL FOUR CHANNEL DRIVER WITH DIODES&lt;/b&gt;&lt;p&gt;
Source: http://www.st.com/stonline/books/pdf/docs/1330.pdf</description>
<gates>
<gate name="G$1" symbol="L293DD"/>
</gates>
<devices>
<device name="" package="SO20">
<connects>
<connect gate="G$1" pin="EN1" pad="1"/>
<connect gate="G$1" pin="EN2" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="7"/>
<connect gate="G$1" pin="GND@5" pad="14"/>
<connect gate="G$1" pin="GND@6" pad="15"/>
<connect gate="G$1" pin="GND@7" pad="16"/>
<connect gate="G$1" pin="GND@8" pad="17"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="19"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="OUT3" pad="13"/>
<connect gate="G$1" pin="OUT4" pad="18"/>
<connect gate="G$1" pin="VS" pad="10"/>
<connect gate="G$1" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L5973D" prefix="IC">
<description>&lt;b&gt;2.5 A switch step down switching regulator&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00002851.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="L5973D"/>
<gate name="-EXP" symbol="EXPOSEDPAD"/>
</gates>
<devices>
<device name="" package="HSOP8">
<connects>
<connect gate="-EXP" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="COMP" pad="4"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="INH" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SYNC" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="STMICROELECTRONICS"/>
<attribute name="MPN" value="L5973D"/>
<attribute name="OC_FARNELL" value="1077145"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L4960" prefix="IC" uservalue="yes">
<description>2.5A POWER SWITCHING REGULATOR

http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00000075.pdf</description>
<gates>
<gate name="G$1" symbol="L4960"/>
</gates>
<devices>
<device name="" package="HEPTAW.H">
<connects>
<connect gate="G$1" pin="1/IN" pad="1"/>
<connect gate="G$1" pin="2/FEED.IN" pad="2"/>
<connect gate="G$1" pin="3/F.COMP" pad="3"/>
<connect gate="G$1" pin="4/GND" pad="4"/>
<connect gate="G$1" pin="5/OSC" pad="5"/>
<connect gate="G$1" pin="6/SOF.START" pad="6"/>
<connect gate="G$1" pin="7/OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HEPTAWATT" package="HEPTAWATT">
<connects>
<connect gate="G$1" pin="1/IN" pad="1"/>
<connect gate="G$1" pin="2/FEED.IN" pad="2"/>
<connect gate="G$1" pin="3/F.COMP" pad="3"/>
<connect gate="G$1" pin="4/GND" pad="4"/>
<connect gate="G$1" pin="5/OSC" pad="5"/>
<connect gate="G$1" pin="6/SOF.START" pad="6"/>
<connect gate="G$1" pin="7/OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7439DS" prefix="IC" uservalue="yes">
<description>The TDA7439DS is a volume tone (bass, middle
and treble) balance (Left/Right) processor for
quality audio applications in car-radio and Hi-Fi
systems.
Selectable input gain is provided. Control of all
the functions is accomplished by serial bus.
The AC signal setting is obtained by resistor networks
and switches combined with operational
amplifiers.
Thanks to the used BIPOLAR/CMOSTechnology,
Low Distortion, Low Noise and DC stepping are
obtained</description>
<gates>
<gate name="TDA7439DS" symbol="TDA7439DS"/>
</gates>
<devices>
<device name="" package="SO28">
<connects>
<connect gate="TDA7439DS" pin="1/RIN3" pad="1"/>
<connect gate="TDA7439DS" pin="10/MINR" pad="10"/>
<connect gate="TDA7439DS" pin="11/MOUTR" pad="11"/>
<connect gate="TDA7439DS" pin="12/BINR" pad="12"/>
<connect gate="TDA7439DS" pin="13/BOUTR" pad="13"/>
<connect gate="TDA7439DS" pin="14/BINL" pad="14"/>
<connect gate="TDA7439DS" pin="15/BOUTL" pad="15"/>
<connect gate="TDA7439DS" pin="16/MOUTL" pad="16"/>
<connect gate="TDA7439DS" pin="17/MINL" pad="17"/>
<connect gate="TDA7439DS" pin="18/TREL" pad="18"/>
<connect gate="TDA7439DS" pin="19/TRER" pad="19"/>
<connect gate="TDA7439DS" pin="2/RIN2" pad="2"/>
<connect gate="TDA7439DS" pin="20/DGND" pad="20"/>
<connect gate="TDA7439DS" pin="21/SCL" pad="21"/>
<connect gate="TDA7439DS" pin="22/SDA" pad="22"/>
<connect gate="TDA7439DS" pin="23/CREF" pad="23"/>
<connect gate="TDA7439DS" pin="24/VS" pad="24"/>
<connect gate="TDA7439DS" pin="25/AGND" pad="25"/>
<connect gate="TDA7439DS" pin="26/ROUT" pad="26"/>
<connect gate="TDA7439DS" pin="27/LOUT" pad="27"/>
<connect gate="TDA7439DS" pin="28/RIN4" pad="28"/>
<connect gate="TDA7439DS" pin="3/RIN1" pad="3"/>
<connect gate="TDA7439DS" pin="4/LIN1" pad="4"/>
<connect gate="TDA7439DS" pin="5/LIN2" pad="5"/>
<connect gate="TDA7439DS" pin="6/LIN3" pad="6"/>
<connect gate="TDA7439DS" pin="7/LIN4" pad="7"/>
<connect gate="TDA7439DS" pin="8/MUXOUTL" pad="8"/>
<connect gate="TDA7439DS" pin="9/MUXOUTR" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA7439" prefix="IC" uservalue="yes">
<description>The TDA7439 is a volume, tone (bass, mid-range
and treble) and balance (left/right) processor for
high-quality audio applications in car-radio and
Hi-Fi systems. Selectable input gain is provided.
All the functions are controlled by serial bus.
The AC signal setting is obtained by resistor
networks and switches combined with operational
amplifiers.
The TDA7439 employs BIPOLAR/CMOS
technology to provide low distortion, low noise
and DC stepping.</description>
<gates>
<gate name="TDA7439" symbol="TDA7439"/>
</gates>
<devices>
<device name="" package="SDIP30">
<connects>
<connect gate="TDA7439" pin="1/SDA" pad="1"/>
<connect gate="TDA7439" pin="10/RIN1" pad="10"/>
<connect gate="TDA7439" pin="11/LIN1" pad="11"/>
<connect gate="TDA7439" pin="12/LIN2" pad="12"/>
<connect gate="TDA7439" pin="13/LIN3" pad="13"/>
<connect gate="TDA7439" pin="14/LIN4" pad="14"/>
<connect gate="TDA7439" pin="15/MUXOUTL" pad="15"/>
<connect gate="TDA7439" pin="16/INL" pad="16"/>
<connect gate="TDA7439" pin="17/MUXOUTR" pad="17"/>
<connect gate="TDA7439" pin="18/INR" pad="18"/>
<connect gate="TDA7439" pin="19/MINR" pad="19"/>
<connect gate="TDA7439" pin="2/CREF" pad="2"/>
<connect gate="TDA7439" pin="20/MOUTR" pad="20"/>
<connect gate="TDA7439" pin="21/BINR" pad="21"/>
<connect gate="TDA7439" pin="22/BOUTR" pad="22"/>
<connect gate="TDA7439" pin="23/BINL" pad="23"/>
<connect gate="TDA7439" pin="24/BOUTL" pad="24"/>
<connect gate="TDA7439" pin="25/MOUTL" pad="25"/>
<connect gate="TDA7439" pin="26/MINL" pad="26"/>
<connect gate="TDA7439" pin="27/TREL" pad="27"/>
<connect gate="TDA7439" pin="28/TRER" pad="28"/>
<connect gate="TDA7439" pin="29/DIGND" pad="29"/>
<connect gate="TDA7439" pin="3/VS" pad="3"/>
<connect gate="TDA7439" pin="30/SCL" pad="30"/>
<connect gate="TDA7439" pin="4/AGND" pad="4"/>
<connect gate="TDA7439" pin="5/ROUT" pad="5"/>
<connect gate="TDA7439" pin="6/LOUT" pad="6"/>
<connect gate="TDA7439" pin="7/RIN4" pad="7"/>
<connect gate="TDA7439" pin="8/RIN3" pad="8"/>
<connect gate="TDA7439" pin="9/RIN2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6232B" prefix="IC">
<gates>
<gate name="L6232B" symbol="L6232B"/>
</gates>
<devices>
<device name="" package="PLCC28">
<connects>
<connect gate="L6232B" pin="BRK" pad="21"/>
<connect gate="L6232B" pin="BRK_DLY" pad="15"/>
<connect gate="L6232B" pin="COMP" pad="19"/>
<connect gate="L6232B" pin="CP" pad="12"/>
<connect gate="L6232B" pin="CS" pad="10"/>
<connect gate="L6232B" pin="GND" pad="1 2 3 4 26 27 28"/>
<connect gate="L6232B" pin="INLA" pad="8"/>
<connect gate="L6232B" pin="INLB" pad="6"/>
<connect gate="L6232B" pin="INLC" pad="14"/>
<connect gate="L6232B" pin="INUA" pad="23"/>
<connect gate="L6232B" pin="INUB" pad="24"/>
<connect gate="L6232B" pin="INUC" pad="16"/>
<connect gate="L6232B" pin="LIN_VREF" pad="18"/>
<connect gate="L6232B" pin="OUTA" pad="20"/>
<connect gate="L6232B" pin="OUTB" pad="22"/>
<connect gate="L6232B" pin="OUTC" pad="25"/>
<connect gate="L6232B" pin="PWM_VREV" pad="17"/>
<connect gate="L6232B" pin="RC" pad="13"/>
<connect gate="L6232B" pin="SENSE1" pad="5"/>
<connect gate="L6232B" pin="SENSE2" pad="9"/>
<connect gate="L6232B" pin="VS1" pad="7"/>
<connect gate="L6232B" pin="VS2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOCKET" package="S28">
<connects>
<connect gate="L6232B" pin="BRK" pad="21"/>
<connect gate="L6232B" pin="BRK_DLY" pad="15"/>
<connect gate="L6232B" pin="COMP" pad="19"/>
<connect gate="L6232B" pin="CP" pad="12"/>
<connect gate="L6232B" pin="CS" pad="10"/>
<connect gate="L6232B" pin="GND" pad="1 2 3 4 26 27 28"/>
<connect gate="L6232B" pin="INLA" pad="8"/>
<connect gate="L6232B" pin="INLB" pad="6"/>
<connect gate="L6232B" pin="INLC" pad="14"/>
<connect gate="L6232B" pin="INUA" pad="23"/>
<connect gate="L6232B" pin="INUB" pad="24"/>
<connect gate="L6232B" pin="INUC" pad="16"/>
<connect gate="L6232B" pin="LIN_VREF" pad="18"/>
<connect gate="L6232B" pin="OUTA" pad="20"/>
<connect gate="L6232B" pin="OUTB" pad="22"/>
<connect gate="L6232B" pin="OUTC" pad="25"/>
<connect gate="L6232B" pin="PWM_VREV" pad="17"/>
<connect gate="L6232B" pin="RC" pad="13"/>
<connect gate="L6232B" pin="SENSE1" pad="5"/>
<connect gate="L6232B" pin="SENSE2" pad="9"/>
<connect gate="L6232B" pin="VS1" pad="7"/>
<connect gate="L6232B" pin="VS2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA6420" prefix="IC" uservalue="yes">
<description>BUS-CONTROLLED AUDIO MATRIX SWITCH

The TEA6420 switches 5 stereo audio inputs on 4 stereo outputs.
All the switching possibilities are changes through the I²C bus.

Features:
- 5 Stereo Inputs
- 4 Stereo Outputs
- Gain Control 0/2/4/6dB/Mute for each Output
- cascadable (2 different addresses)
- Serial Bus Controlles
- Very low Noise
- Very low Distorsion</description>
<gates>
<gate name="G$1" symbol="TEA6420"/>
</gates>
<devices>
<device name="N" package="S-DIL24">
<connects>
<connect gate="G$1" pin="ADDR" pad="22"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="L1" pad="4"/>
<connect gate="G$1" pin="L2" pad="5"/>
<connect gate="G$1" pin="L3" pad="6"/>
<connect gate="G$1" pin="L4" pad="7"/>
<connect gate="G$1" pin="L5" pad="8"/>
<connect gate="G$1" pin="LOUT1" pad="9"/>
<connect gate="G$1" pin="LOUT2" pad="11"/>
<connect gate="G$1" pin="LOUT3" pad="13"/>
<connect gate="G$1" pin="LOUT4" pad="15"/>
<connect gate="G$1" pin="R1" pad="21"/>
<connect gate="G$1" pin="R2" pad="20"/>
<connect gate="G$1" pin="R3" pad="19"/>
<connect gate="G$1" pin="R4" pad="18"/>
<connect gate="G$1" pin="R5" pad="17"/>
<connect gate="G$1" pin="ROUT1" pad="10"/>
<connect gate="G$1" pin="ROUT2" pad="12"/>
<connect gate="G$1" pin="ROUT3" pad="14"/>
<connect gate="G$1" pin="ROUT4" pad="16"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L9686" prefix="IC" uservalue="yes">
<description>The L9686 is a two frequency oscillator particularly
suitable as relay driver for flashing light control
in automotive applications. The circuit may be
also used for other warning lamps like ”handbrake
on” etc. The lamp failure detection is given by
doubling the flash repetition frequency. The
L9686 is supplied in minidip 8-lead and SO8 plastic
packages.</description>
<gates>
<gate name="G$1" symbol="L9686"/>
</gates>
<devices>
<device name="" package="DIL-08">
<connects>
<connect gate="G$1" pin="+V" pad="2"/>
<connect gate="G$1" pin="COSC" pad="4"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="LFD" pad="7"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT/REL" pad="3"/>
<connect gate="G$1" pin="ROSC" pad="5"/>
<connect gate="G$1" pin="STR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO8" package="SO08">
<connects>
<connect gate="G$1" pin="+V" pad="2"/>
<connect gate="G$1" pin="COSC" pad="4"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="LFD" pad="7"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT/REL" pad="3"/>
<connect gate="G$1" pin="ROSC" pad="5"/>
<connect gate="G$1" pin="STR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8137" prefix="IC" uservalue="yes">
<description>DUAL 5.1V REGULATOR WITH DISABLE AND RESET</description>
<gates>
<gate name="G$1" symbol="TDA8137"/>
</gates>
<devices>
<device name="" package="HEPTAWATT">
<connects>
<connect gate="G$1" pin="DELAY" pad="2"/>
<connect gate="G$1" pin="DISAB" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT1" pad="7"/>
<connect gate="G$1" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8138A/B" prefix="IC" uservalue="yes">
<description>The TDA8138 is a monolithic dual positive voltage
regulator designed to provide fixed precision output
voltages of 5.1V and 12V at currents up to 1A.</description>
<gates>
<gate name="G$1" symbol="TDA8138A/B"/>
</gates>
<devices>
<device name="" package="HEPTAWATT">
<connects>
<connect gate="G$1" pin="DIS/CAPA" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="RESET" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8138" prefix="IC" uservalue="yes">
<description>The TDA8138 is a monolithic dual positive voltage
regulator designed to provide fixed precision output
voltages of 5.1V and 12V at currents up to 1A.</description>
<gates>
<gate name="G$1" symbol="TDA8138"/>
</gates>
<devices>
<device name="" package="SIP-9">
<connects>
<connect gate="G$1" pin="DEL/CAP" pad="P$3"/>
<connect gate="G$1" pin="DIS" pad="P$4"/>
<connect gate="G$1" pin="GND" pad="P$5"/>
<connect gate="G$1" pin="IN1" pad="P$1"/>
<connect gate="G$1" pin="IN2" pad="P$2"/>
<connect gate="G$1" pin="NC" pad="P$7"/>
<connect gate="G$1" pin="OUT1" pad="P$9"/>
<connect gate="G$1" pin="OUT2" pad="P$8"/>
<connect gate="G$1" pin="RESET" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SG2525/3525" prefix="IC" uservalue="yes">
<description>The SG3525A series of pulse width modulator integrated
circuits are designed to offer improved performance
and lowered external parts count when
used in designing all types of switching power supplies.
The on-chip + 5.1 V reference is trimmed to ±
1 % and the input common-mode range of the error
amplifier includes the reference voltage eliminating
external resistors. A sync input to the oscillator allows
multiple units to be slaved or a single unit to be
synchronized to an external system clock. A single
resistor between the CT and the discharge terminals
provide a wide range of dead time ad- justment.
These devices also feature built-in soft-start circuitry
with only an external timing capacitor required. A
shutdown terminal controls both the soft-start circuity
and the output stages, providing instantaneous
turn off through the PWM latch with pulsed shutdown,
as well as soft-start recycle with longer shutdown
commands. These functions are also controlled
by an undervoltage lockout which keeps the outputs
off and the soft-start capacitor discharged for
sub-normal input voltages. This lockout circuitry includes
approximately 500 mV of hysteresis for jitterfree
operation. Another feature of these PWM circuits
is a latch following the comparator. Once a
PWM pulses has been terminated for any reason,
the outputs will remain off for the duration of the period.
The latch is reset with each clock pulse. The
output stages are totem-pole designs capable of
sourcing or sinking in excess of 200 mA. The
SG3525A output stage features NOR logic, giving a
LOW output for an OFF state.</description>
<gates>
<gate name="G$1" symbol="SG2525/3525"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="+VJ" pad="15"/>
<connect gate="G$1" pin="COME" pad="9"/>
<connect gate="G$1" pin="CT" pad="5"/>
<connect gate="G$1" pin="DRSCH" pad="7"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INV.IN" pad="1"/>
<connect gate="G$1" pin="NI.IN" pad="2"/>
<connect gate="G$1" pin="OSC.OUT" pad="4"/>
<connect gate="G$1" pin="OUT_A" pad="11"/>
<connect gate="G$1" pin="OUT_B" pad="14"/>
<connect gate="G$1" pin="RT" pad="6"/>
<connect gate="G$1" pin="SHUT" pad="10"/>
<connect gate="G$1" pin="SOFT_ST" pad="8"/>
<connect gate="G$1" pin="SYNC" pad="3"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VREF" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO16N" package="SO16_NARROW">
<connects>
<connect gate="G$1" pin="+VJ" pad="15"/>
<connect gate="G$1" pin="COME" pad="9"/>
<connect gate="G$1" pin="CT" pad="5"/>
<connect gate="G$1" pin="DRSCH" pad="7"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INV.IN" pad="1"/>
<connect gate="G$1" pin="NI.IN" pad="2"/>
<connect gate="G$1" pin="OSC.OUT" pad="4"/>
<connect gate="G$1" pin="OUT_A" pad="11"/>
<connect gate="G$1" pin="OUT_B" pad="14"/>
<connect gate="G$1" pin="RT" pad="6"/>
<connect gate="G$1" pin="SHUT" pad="10"/>
<connect gate="G$1" pin="SOFT_ST" pad="8"/>
<connect gate="G$1" pin="SYNC" pad="3"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VREF" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STR711F" prefix="IC" uservalue="yes">
<description>The KickStart Kits™ (STR711) are IAR’s
complete, cost-effective solutions for starting
application development and evaluating a full
range of STMicroelectronic’s ARM® core-based
microcontrollers.
They come with all the hardware and software
you need to start developing applications for a full
range of STMicroelectonic’s ARM7TDMI™ and
ARM966E™ core-based microcontrollers. The
kits include the KickStart Development Board with
target microcontroller, the IAR JLink USB-to-
JTAG debugger and IAR Embedded Workbench®
for ARM (EWARM) integrated development
environment with the 32KB KickStart version of
the C/C++ compiler, built in Flash loader and
sample projects for all device peripherals.</description>
<gates>
<gate name="G$1" symbol="STR711F"/>
</gates>
<devices>
<device name="" package="TQFP64">
<connects>
<connect gate="G$1" pin="AVDD" pad="29"/>
<connect gate="G$1" pin="AVSS" pad="30"/>
<connect gate="G$1" pin="BOOTEN" pad="7"/>
<connect gate="G$1" pin="CK" pad="19"/>
<connect gate="G$1" pin="JTCK" pad="12"/>
<connect gate="G$1" pin="JTDI" pad="10"/>
<connect gate="G$1" pin="JTDO" pad="13"/>
<connect gate="G$1" pin="JTMS" pad="11"/>
<connect gate="G$1" pin="NJTRST" pad="14"/>
<connect gate="G$1" pin="NRSTIN" pad="24"/>
<connect gate="G$1" pin="NSTDBY" pad="23"/>
<connect gate="G$1" pin="NU" pad="15"/>
<connect gate="G$1" pin="P0.0/S0.MISO/U3.TX" pad="52"/>
<connect gate="G$1" pin="P0.1/S0.MOSI/U3.RX" pad="53"/>
<connect gate="G$1" pin="P0.10/U1.RX/U1.TX/SCDATA" pad="1"/>
<connect gate="G$1" pin="P0.11/U1.TX/BOOT.1" pad="2"/>
<connect gate="G$1" pin="P0.12/SCCCLK" pad="3"/>
<connect gate="G$1" pin="P0.13/U2.RX/T2.OCMPA" pad="5"/>
<connect gate="G$1" pin="P0.14/U2.TX/T2.ICAPA" pad="6"/>
<connect gate="G$1" pin="P0.15/WAKEUP" pad="20"/>
<connect gate="G$1" pin="P0.2/S0.SCLK/I1.SCL" pad="54"/>
<connect gate="G$1" pin="P0.3/S0.SSN/I1.SDA" pad="55"/>
<connect gate="G$1" pin="P0.4/S1.MISO" pad="56"/>
<connect gate="G$1" pin="P0.5/S1.MOSI" pad="60"/>
<connect gate="G$1" pin="P0.6/S1.SCLK" pad="61"/>
<connect gate="G$1" pin="P0.7/S1.SSN" pad="62"/>
<connect gate="G$1" pin="P0.8/U0.RX/U0.TX" pad="63"/>
<connect gate="G$1" pin="P0.9/U0.TX/BOOT.0" pad="64"/>
<connect gate="G$1" pin="P1.0/T3.OCMPB/AIN.0" pad="31"/>
<connect gate="G$1" pin="P1.1/T3.ICAPA/AIN.1" pad="32"/>
<connect gate="G$1" pin="P1.10/USBCLK" pad="46"/>
<connect gate="G$1" pin="P1.13/HCLK/I0.SCL" pad="47"/>
<connect gate="G$1" pin="P1.14/HRXD/I0.SDA" pad="48"/>
<connect gate="G$1" pin="P1.15/HTXD" pad="49"/>
<connect gate="G$1" pin="P1.2/T3.OCMPA/AIN.2" pad="33"/>
<connect gate="G$1" pin="P1.3/T3.ICAPB/AIN.3" pad="34"/>
<connect gate="G$1" pin="P1.4/T1.ICAPA" pad="35"/>
<connect gate="G$1" pin="P1.5/T1.ICAPB" pad="36"/>
<connect gate="G$1" pin="P1.6/T1.OCMPB" pad="37"/>
<connect gate="G$1" pin="P1.7/T1.OCMPA" pad="40"/>
<connect gate="G$1" pin="P1.8" pad="41"/>
<connect gate="G$1" pin="P1.9" pad="45"/>
<connect gate="G$1" pin="RTCXTI" pad="21"/>
<connect gate="G$1" pin="RTCXTO" pad="22"/>
<connect gate="G$1" pin="TEST" pad="16"/>
<connect gate="G$1" pin="USBDN-" pad="43"/>
<connect gate="G$1" pin="USBDP+" pad="42"/>
<connect gate="G$1" pin="V18BKP" pad="26"/>
<connect gate="G$1" pin="V18_1" pad="27"/>
<connect gate="G$1" pin="V18_2" pad="58"/>
<connect gate="G$1" pin="V33IO-PLL_1" pad="17"/>
<connect gate="G$1" pin="V33IO-PLL_2" pad="38"/>
<connect gate="G$1" pin="V33_1" pad="9"/>
<connect gate="G$1" pin="V33_2" pad="51"/>
<connect gate="G$1" pin="VSS18_1" pad="28"/>
<connect gate="G$1" pin="VSS18_2" pad="57"/>
<connect gate="G$1" pin="VSSBKP" pad="25"/>
<connect gate="G$1" pin="VSSIO-PLL_1" pad="18"/>
<connect gate="G$1" pin="VSSIO-PLL_2" pad="39"/>
<connect gate="G$1" pin="VSS_1" pad="4"/>
<connect gate="G$1" pin="VSS_2" pad="8"/>
<connect gate="G$1" pin="VSS_3" pad="44"/>
<connect gate="G$1" pin="VSS_4" pad="50"/>
<connect gate="G$1" pin="VSS_5" pad="59"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST7540" prefix="IC" uservalue="yes">
<description>The ST7540 is a Half Duplex
synchronous/asynchronous FSK Modem
designed for power line communication network
applications. It operates from a single supply
voltage and integrates a line driver and two linear
regulators for 5V and 3.3V. The device operation
is controlled by means of an internal register,
programmable through the synchronous serial
interface. Additional functions as watchdog, clock
output, output voltage and current control,
preamble detection, time-out and band in use are
included. Realized in Multipower BCD5
technology that allows to integrate DMOS, Bipolar
and CMOS structures in the same chip.</description>
<gates>
<gate name="A" symbol="ST7540"/>
</gates>
<devices>
<device name="" package="HTSSOP28EXP">
<connects>
<connect gate="A" pin="BU/THERM" pad="7"/>
<connect gate="A" pin="CD_PD" pad="1"/>
<connect gate="A" pin="CL" pad="24"/>
<connect gate="A" pin="CLR/T" pad="8"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="MCLK" pad="10"/>
<connect gate="A" pin="PA_IN+" pad="18"/>
<connect gate="A" pin="PA_IN-" pad="14"/>
<connect gate="A" pin="PA_OUT" pad="15"/>
<connect gate="A" pin="REG_DATA" pad="2"/>
<connect gate="A" pin="RSTO" pad="11"/>
<connect gate="A" pin="RXD" pad="4"/>
<connect gate="A" pin="RXTX" pad="5"/>
<connect gate="A" pin="RX_IN" pad="25"/>
<connect gate="A" pin="SVSS" pad="20"/>
<connect gate="A" pin="TEST1" pad="27"/>
<connect gate="A" pin="TEST2" pad="28"/>
<connect gate="A" pin="TXD" pad="6"/>
<connect gate="A" pin="TX_OUT" pad="19"/>
<connect gate="A" pin="UART/SPI" pad="12"/>
<connect gate="A" pin="VCC" pad="17"/>
<connect gate="A" pin="VDC" pad="26"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VSENCE" pad="23"/>
<connect gate="A" pin="VSS" pad="16"/>
<connect gate="A" pin="WD" pad="13"/>
<connect gate="A" pin="X1" pad="21"/>
<connect gate="A" pin="X2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNH5050ATR_E" prefix="IC" uservalue="yes">
<description>The VNH5050A-E is a full bridge motor driver
intended for a wide range of automotive
applications. The device incorporates a dual
monolithic high-side driver and two low-side
switches.</description>
<gates>
<gate name="VNH5050A-E" symbol="VNH5050ATR_E"/>
</gates>
<devices>
<device name="" package="PSSO-36TP">
<connects>
<connect gate="VNH5050A-E" pin="CS" pad="P$19"/>
<connect gate="VNH5050A-E" pin="CS_DIS" pad="P$20"/>
<connect gate="VNH5050A-E" pin="DRAIN_LSA" pad="P$2 P$8"/>
<connect gate="VNH5050A-E" pin="DRAIN_LSB" pad="P$29 P$35"/>
<connect gate="VNH5050A-E" pin="ENA/DIAGA" pad="P$16"/>
<connect gate="VNH5050A-E" pin="ENB/DIAGB" pad="P$21"/>
<connect gate="VNH5050A-E" pin="GND_A" pad="P$1 P$3 P$4 P$5 P$6 P$7"/>
<connect gate="VNH5050A-E" pin="GND_B" pad="P$30 P$31 P$32 P$33 P$34 P$36"/>
<connect gate="VNH5050A-E" pin="INA" pad="P$15"/>
<connect gate="VNH5050A-E" pin="INB" pad="P$22"/>
<connect gate="VNH5050A-E" pin="IN_PWM" pad="P$17"/>
<connect gate="VNH5050A-E" pin="SOURCE_HSA" pad="P$9 P$10 P$11 P$12 P$14"/>
<connect gate="VNH5050A-E" pin="SOURCE_HSB" pad="P$23 P$25 P$26 P$27 P$28"/>
<connect gate="VNH5050A-E" pin="VCC" pad="P$13 P$24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
