<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<description>Hi-fi stereo audio processor; I2C-bus</description>
<packages>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="TDA8425">
<pin name="GND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="IN2R" direction="in"/>
<pin name="IN2L" direction="in"/>
<pin name="IN1R" direction="in"/>
<pin name="IN1L" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="BASS1L"/>
<pin name="BASS2L"/>
<pin name="TREBLEL"/>
<pin name="BASS1R"/>
<pin name="BASS2R"/>
<pin name="TREBLER"/>
<pin name="PSEUD1"/>
<pin name="PSEUD2"/>
<pin name="VCAP"/>
<pin name="SLC"/>
<pin name="SDA"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TDA8425" prefix="U">
<description>The TDA8425 is a monolithic bipolar integrated stereo sound circuit with a loudspeaker channel facility, digitally
controlled via the I2C-bus for application in hi-fi audio and television sound.

Library has been designed by Richard Magdycz.</description>
<gates>
<gate name="G$1" symbol="TDA8425"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="BASS1L" pad="15"/>
<connect gate="G$1" pin="BASS1R" pad="6"/>
<connect gate="G$1" pin="BASS2L" pad="16"/>
<connect gate="G$1" pin="BASS2R" pad="7"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="IN1L" pad="18"/>
<connect gate="G$1" pin="IN1R" pad="20"/>
<connect gate="G$1" pin="IN2L" pad="1"/>
<connect gate="G$1" pin="IN2R" pad="3"/>
<connect gate="G$1" pin="OUTL" pad="13"/>
<connect gate="G$1" pin="OUTR" pad="9"/>
<connect gate="G$1" pin="PSEUD1" pad="19"/>
<connect gate="G$1" pin="PSEUD2" pad="17"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="SLC" pad="12"/>
<connect gate="G$1" pin="TREBLEL" pad="14"/>
<connect gate="G$1" pin="TREBLER" pad="8"/>
<connect gate="G$1" pin="VCAP" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
