<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="HZIP25">
<description>THB8128 vertical</description>
</package>
</packages>
<symbols>
<symbol name="THB8128">
<pin name="OUT-2A" direction="out"/>
<pin name="NFA" direction="pas"/>
<pin name="GNDA" direction="pwr"/>
<pin name="OUT-1A" direction="out"/>
<pin name="VMA" direction="pwr"/>
<pin name="ST/VCC"/>
<pin name="M1" direction="in"/>
<pin name="M2" direction="in"/>
<pin name="M3" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="STEP" direction="in"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="DECAY" direction="pas"/>
<pin name="DOWN" direction="pas"/>
<pin name="MON" direction="pas"/>
<pin name="VREF" direction="pwr"/>
<pin name="SGND" direction="pwr"/>
<pin name="VMB" direction="pwr"/>
<pin name="OUT-2B" direction="out"/>
<pin name="GNDB" direction="pwr"/>
<pin name="NFB" direction="in"/>
<pin name="OUT-1B" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="THB8128">
<gates>
<gate name="G$1" symbol="THB8128"/>
</gates>
<devices>
<device name="VERTICAL" package="HZIP25">
<connects>
<connect gate="G$1" pin="DECAY" pad="16"/>
<connect gate="G$1" pin="DIR" pad="12"/>
<connect gate="G$1" pin="DOWN" pad="17"/>
<connect gate="G$1" pin="ENABLE" pad="10"/>
<connect gate="G$1" pin="GNDA" pad="3"/>
<connect gate="G$1" pin="GNDB" pad="23"/>
<connect gate="G$1" pin="M1" pad="7"/>
<connect gate="G$1" pin="M2" pad="8"/>
<connect gate="G$1" pin="M3" pad="9"/>
<connect gate="G$1" pin="MON" pad="18"/>
<connect gate="G$1" pin="NFA" pad="2"/>
<connect gate="G$1" pin="NFB" pad="24"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="OUT-1A" pad="4"/>
<connect gate="G$1" pin="OUT-1B" pad="25"/>
<connect gate="G$1" pin="OUT-2A" pad="1"/>
<connect gate="G$1" pin="OUT-2B" pad="22"/>
<connect gate="G$1" pin="RESET" pad="11"/>
<connect gate="G$1" pin="SGND" pad="20"/>
<connect gate="G$1" pin="ST/VCC" pad="6"/>
<connect gate="G$1" pin="STEP" pad="13"/>
<connect gate="G$1" pin="VMA" pad="5"/>
<connect gate="G$1" pin="VMB" pad="21"/>
<connect gate="G$1" pin="VREF" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
