<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="SOP-28">
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
<symbols>
<symbol name="WS2803">
<pin name="CKI"/>
<pin name="SDI"/>
<pin name="VCC"/>
<pin name="IREF"/>
<pin name="CKO"/>
<pin name="SDO"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="GND"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="OUT8"/>
<pin name="OUT9"/>
<pin name="OUT10"/>
<pin name="OUT11"/>
<pin name="OUT12"/>
<pin name="OUT13"/>
<pin name="OUT14"/>
<pin name="OUT15"/>
<pin name="OUT16"/>
<pin name="OUT17"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WS2803" prefix="U">
<description>&lt;h3&gt;WS2803&lt;/h3&gt;
18 Channel Constant Current LED Driver with programmable PWM outputs.
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WS2803"/>
</gates>
<devices>
<device name="" package="SOP-28">
<connects>
<connect gate="G$1" pin="CKI" pad="4"/>
<connect gate="G$1" pin="CKO" pad="25"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IREF" pad="3"/>
<connect gate="G$1" pin="NC1" pad="2"/>
<connect gate="G$1" pin="NC2" pad="26"/>
<connect gate="G$1" pin="NC3" pad="27"/>
<connect gate="G$1" pin="OUT0" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT10" pad="16"/>
<connect gate="G$1" pin="OUT11" pad="17"/>
<connect gate="G$1" pin="OUT12" pad="18"/>
<connect gate="G$1" pin="OUT13" pad="19"/>
<connect gate="G$1" pin="OUT14" pad="20"/>
<connect gate="G$1" pin="OUT15" pad="21"/>
<connect gate="G$1" pin="OUT16" pad="22"/>
<connect gate="G$1" pin="OUT17" pad="23"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="OUT3" pad="9"/>
<connect gate="G$1" pin="OUT4" pad="10"/>
<connect gate="G$1" pin="OUT5" pad="11"/>
<connect gate="G$1" pin="OUT6" pad="12"/>
<connect gate="G$1" pin="OUT7" pad="13"/>
<connect gate="G$1" pin="OUT8" pad="14"/>
<connect gate="G$1" pin="OUT9" pad="15"/>
<connect gate="G$1" pin="SDI" pad="5"/>
<connect gate="G$1" pin="SDO" pad="24"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2803-DIP">
<gates>
<gate name="G$1" symbol="WS2803"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="CKI" pad="4"/>
<connect gate="G$1" pin="CKO" pad="27"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IREF" pad="2"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="25"/>
<connect gate="G$1" pin="NC3" pad="24"/>
<connect gate="G$1" pin="OUT0" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT10" pad="16"/>
<connect gate="G$1" pin="OUT11" pad="17"/>
<connect gate="G$1" pin="OUT12" pad="18"/>
<connect gate="G$1" pin="OUT13" pad="19"/>
<connect gate="G$1" pin="OUT14" pad="20"/>
<connect gate="G$1" pin="OUT15" pad="21"/>
<connect gate="G$1" pin="OUT16" pad="22"/>
<connect gate="G$1" pin="OUT17" pad="23"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="OUT3" pad="9"/>
<connect gate="G$1" pin="OUT4" pad="10"/>
<connect gate="G$1" pin="OUT5" pad="11"/>
<connect gate="G$1" pin="OUT6" pad="12"/>
<connect gate="G$1" pin="OUT7" pad="13"/>
<connect gate="G$1" pin="OUT8" pad="14"/>
<connect gate="G$1" pin="OUT9" pad="15"/>
<connect gate="G$1" pin="SDI" pad="5"/>
<connect gate="G$1" pin="SDO" pad="26"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
