<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>&lt;b&gt;Trimble GPS/GNSS Receiver Modules&lt;/b&gt;&lt;p&gt;
SMD GPS/GLONASS/GALILEO/COMPASS Receiver modules,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Based on Trimble datasheets and manuals. For the latest version of documentation, support material and tools visit the website
&lt;a href="http://www.trimble.com/embeddedsystems/"&gt;www.Trimble.com&lt;/a&gt;&lt;br&gt;
If you have suggestions for improvements, please contact the author so that your feedback can be used in next versions of the library. Thank you!&lt;br&gt;
The Library and the Demo-designs are provided "as is", without warranty.&lt;br&gt;
Version: 3.0, Date: 1.Nov. 2011. Check the Trimble website for newer versions of this library.&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;</description>
<packages>
<package name="1919">
<description>&lt;b&gt;Package 1919, 28-pads&lt;/b&gt;&lt;p&gt;
&lt;p&gt;
Size: 19 mm x 19 mm x 2.54 mm&lt;p&gt;
28 SMD edge-castellation pads, 1.27 mm pad-pitch&lt;p&gt;
by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Used for: Condor C1919A, C1919B, C1919C, Copernicus, Copernicus-II, Resolution-SMT, ICM-SMT, Aardvark, Buffalo B1919&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;p&gt;</description>
</package>
<package name="1722">
<description>&lt;b&gt;Package 1722, 28-pads&lt;/b&gt;&lt;p&gt;
&lt;p&gt;
Size: 17 mm x 22 mm x 1.8 mm&lt;p&gt;
28 SMD edge-castellation pads, 1.1 mm pad-pitch&lt;p&gt;
by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Used for: Condor C1216&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;p&gt;</description>
</package>
<package name="1216">
<description>&lt;b&gt;Package 1216, 24-pads&lt;/b&gt;&lt;p&gt;
&lt;p&gt;
Size: 12 mm x 16 mm x 1.8 mm&lt;p&gt;
24 SMD edge-castellation pads, 1.1 mm pad-pitch&lt;p&gt;
by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Used for: Condor C1216&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;p&gt;</description>
</package>
<package name="1011">
<description>&lt;b&gt;Package 1011, 38-pad QFN&lt;/b&gt;&lt;p&gt;
&lt;p&gt;
Size: 10 mm x 11 mm x 2.01 mm&lt;p&gt;
38 SMD pads, 1 mm pad-pitch&lt;p&gt;
by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Used for: Condor C1011&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;p&gt;</description>
</package>
<package name="TRIMBLE-LOGO">
<description>&lt;b&gt;Trimble-Logo&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="FGPMMOPA6E">
</package>
<package name="GPS">
</package>
<package name="M72">
</package>
<package name="QUECTEL_L20">
</package>
<package name="L10">
<description>&lt;h3&gt; Quectel L10&lt;/h3&gt;
&lt;p&gt; A GPS Module by Quectel.</description>
</package>
<package name="M10">
<description>&lt;h3&gt;Quectel M10&lt;/h3&gt;
&lt;p&gt; GSM module by Quectel&lt;/p&gt;</description>
</package>
<package name="SIM908">
</package>
<package name="TC65">
</package>
<package name="MG2639">
</package>
<package name="M95">
</package>
<package name="QUECTEL_L30">
</package>
<package name="QUECTEL_M12">
</package>
</packages>
<symbols>
<symbol name="COPERNICUS">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="LNA_XEN" direction="out"/>
<pin name="RESERVED@6" direction="nc"/>
<pin name="OPEN" direction="in"/>
<pin name="SHORT" direction="in"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@10" direction="nc"/>
<pin name="XRESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="XSTANDBY" direction="in"/>
<pin name="RESERVED@17" direction="nc"/>
<pin name="RESERVED@18" direction="nc"/>
<pin name="PPS" direction="out"/>
<pin name="RXD_B" direction="in"/>
<pin name="RXD_A" direction="in"/>
<pin name="RESERVED@22" direction="nc"/>
<pin name="TXD_A" direction="out"/>
<pin name="TXD_B" direction="out"/>
<pin name="RESERVED@25" direction="nc"/>
<pin name="RESERVED@26" direction="nc"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
</symbol>
<symbol name="C1216">
<pin name="GND@10" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@13" direction="pwr"/>
<pin name="RTCM-IN" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VRTC" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="RESERVED@1" direction="nc"/>
<pin name="XRESET" direction="in"/>
<pin name="1PPS" direction="out"/>
<pin name="RESERVED@4" direction="nc"/>
<pin name="USB-DM"/>
<pin name="USB-DP"/>
<pin name="VDD-USB" direction="in"/>
<pin name="RESERVED@8" direction="nc"/>
<pin name="V28A" direction="out"/>
<pin name="RESERVED@14" direction="nc"/>
<pin name="RESERVED@15" direction="nc"/>
<pin name="RESERVED@16" direction="nc"/>
<pin name="RESERVED@18" direction="nc"/>
<pin name="RESERVED@19" direction="nc"/>
</symbol>
<symbol name="C1722">
<pin name="GND@7" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@14" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VRTC" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="RESERVED@1" direction="nc"/>
<pin name="XRESET" direction="in"/>
<pin name="1PPS" direction="out"/>
<pin name="RESERVED@2" direction="nc"/>
<pin name="USB-DM"/>
<pin name="USB-DP"/>
<pin name="VDD-USB" direction="in"/>
<pin name="RESERVED@5" direction="nc"/>
<pin name="VS-AA" direction="out"/>
<pin name="RESERVED@8" direction="nc"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@12" direction="nc"/>
<pin name="RESERVED@20" direction="nc"/>
<pin name="RESERVED@21" direction="nc"/>
<pin name="GND@17" direction="pwr"/>
<pin name="RESERVED@22" direction="nc"/>
<pin name="RESERVED@23" direction="nc"/>
<pin name="VS-LNA" direction="in"/>
<pin name="RESERVED@27" direction="nc"/>
</symbol>
<symbol name="C1011">
<pin name="GND@16" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RTC_IN" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VRTC" direction="in"/>
<pin name="VCC@15" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="RESERVED@11" direction="nc"/>
<pin name="XRESET" direction="in"/>
<pin name="1PPS" direction="out"/>
<pin name="RESERVED@12" direction="nc"/>
<pin name="RESERVED@13" direction="nc"/>
<pin name="RESERVED@5" direction="nc"/>
<pin name="RESERVED@14" direction="nc"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="RESERVED@20" direction="nc"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="VCC@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="RESERVED@29" direction="nc"/>
<pin name="RESERVED@30" direction="nc"/>
<pin name="RESERVED@31" direction="nc"/>
<pin name="VCC@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="RESERVED@34" direction="nc"/>
<pin name="GND@35" direction="pwr"/>
<pin name="XSTANDBY" direction="in"/>
<pin name="GND@37" direction="pwr"/>
<pin name="RTC_OUT" direction="out"/>
</symbol>
<symbol name="C1919B">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="RESERVED@5" direction="nc"/>
<pin name="VRTC" direction="in"/>
<pin name="XRESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="RTC_CLK"/>
<pin name="PPS" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="RESERVED@7" direction="nc"/>
<pin name="RESERVED@8" direction="nc"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@10" direction="nc"/>
<pin name="RESERVED@16" direction="nc"/>
<pin name="RESERVED@18" direction="nc"/>
<pin name="RESERVED@21" direction="nc"/>
<pin name="RESERVED@22" direction="nc"/>
<pin name="RESERVED@23" direction="nc"/>
<pin name="RESERVED@25" direction="nc"/>
<pin name="RESERVED@26" direction="nc"/>
</symbol>
<symbol name="C1919A">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="RESERVED@5" direction="nc"/>
<pin name="VRTC" direction="in"/>
<pin name="XRESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="PPS" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="RESERVED@7" direction="nc"/>
<pin name="RESERVED@8" direction="nc"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@10" direction="nc"/>
<pin name="RESERVED@16" direction="nc"/>
<pin name="RESERVED@18" direction="nc"/>
<pin name="RESERVED@21" direction="nc"/>
<pin name="RESERVED@22" direction="nc"/>
<pin name="RESERVED@23" direction="nc"/>
<pin name="RESERVED@25" direction="nc"/>
<pin name="RESERVED@26" direction="nc"/>
<pin name="RESERVED@17" direction="nc"/>
</symbol>
<symbol name="COPERNICUS-II">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="LNA_XEN" direction="out"/>
<pin name="VBAT" direction="in"/>
<pin name="OPEN" direction="in"/>
<pin name="SHORT" direction="in"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@10" direction="nc"/>
<pin name="XRESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="XSTANDBY" direction="in"/>
<pin name="RESERVED@17" direction="nc"/>
<pin name="RESERVED@18" direction="nc"/>
<pin name="PPS" direction="out"/>
<pin name="RXD_B" direction="in"/>
<pin name="RXD_A" direction="in"/>
<pin name="RESERVED@22" direction="nc"/>
<pin name="TXD_A" direction="out"/>
<pin name="TXD_B" direction="out"/>
<pin name="RESERVED@25" direction="nc"/>
<pin name="RESERVED@26" direction="nc"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
</symbol>
<symbol name="RESOLUTION-SMT">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="OPEN" direction="in"/>
<pin name="SHORT" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="PPS" direction="out"/>
<pin name="RXD_B" direction="in"/>
<pin name="RXD_A" direction="in"/>
<pin name="TXD_A" direction="out"/>
<pin name="TXD_B" direction="out"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="RESERVED@7" direction="nc"/>
<pin name="RESERVED@23" direction="nc"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="RESERVED@8" direction="nc"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@10" direction="nc"/>
<pin name="RESERVED@11" direction="nc"/>
<pin name="RESERVED@12" direction="nc"/>
<pin name="RESERVED@13" direction="nc"/>
</symbol>
<symbol name="ICM-SMT">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="OPEN" direction="in"/>
<pin name="SHORT" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="PPS" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="RESERVED@7" direction="nc"/>
<pin name="SYSCLK" direction="nc"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="RESERVED@8" direction="nc"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@10" direction="nc"/>
<pin name="RESERVED@11" direction="nc"/>
<pin name="RESERVED@12" direction="nc"/>
<pin name="RESERVED@13" direction="nc"/>
<pin name="RESERVED@21" direction="nc"/>
<pin name="RESERVED@22" direction="nc"/>
</symbol>
<symbol name="TRIMBLE-LOGO">
</symbol>
<symbol name="A1919_AARDVARK">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="RESERVED@5" direction="nc"/>
<pin name="VBACK" direction="in"/>
<pin name="XRESET" direction="in"/>
<pin name="RESERVED@12" direction="nc"/>
<pin name="RESERVED@13" direction="nc"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="PPS" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RESERVED@27" direction="nc"/>
<pin name="GND@28" direction="pwr"/>
<pin name="OPEN" direction="in"/>
<pin name="SHORT" direction="in"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@10" direction="nc"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESERVED@18" direction="nc"/>
<pin name="RESERVED@21" direction="nc"/>
<pin name="RESERVED@22" direction="nc"/>
<pin name="RESERVED@23" direction="nc"/>
<pin name="TACHO" direction="in"/>
<pin name="FWD/REV" direction="in"/>
<pin name="RESERVED@17" direction="nc"/>
</symbol>
<symbol name="B1919_BUFFALO">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_IN" direction="in"/>
<pin name="GND@4" direction="pwr"/>
<pin name="LNA_XEN" direction="out"/>
<pin name="VBAT" direction="in"/>
<pin name="XRESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESERVED@13" direction="nc"/>
<pin name="VDD_USB" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="PPS" direction="out"/>
<pin name="RXD_B" direction="in"/>
<pin name="TXD_B" direction="out"/>
<pin name="RESERVED@27" direction="nc"/>
<pin name="GND@28" direction="pwr"/>
<pin name="OPEN" direction="in"/>
<pin name="SHORT" direction="in"/>
<pin name="RESERVED@9" direction="nc"/>
<pin name="RESERVED@10" direction="nc"/>
<pin name="XSTANDBY" direction="in"/>
<pin name="USB_DM"/>
<pin name="RXD_A" direction="in"/>
<pin name="RESERVED@22" direction="nc"/>
<pin name="TXD_A" direction="out"/>
<pin name="RESERVED@25" direction="nc"/>
<pin name="RESERVED@26" direction="nc"/>
<pin name="USB_DP"/>
</symbol>
<symbol name="FGPMMOPA6">
<pin name="1/VCC" direction="pwr"/>
<pin name="2/ENABLE"/>
<pin name="3/GND" direction="pwr"/>
<pin name="4/VBACKUP"/>
<pin name="5/3D-FIX"/>
<pin name="6/DPLUS"/>
<pin name="7/DMINUS"/>
<pin name="8/GND" direction="pwr"/>
<pin name="9/TXD"/>
<pin name="10/RXD"/>
</symbol>
<symbol name="GPS-FGPMMOPA6C">
<pin name="VCC"/>
<pin name="VBACKUP"/>
<pin name="GND_3"/>
<pin name="GND_8"/>
<pin name="GND_11"/>
<pin name="GND_12"/>
<pin name="GND_13"/>
<pin name="3D-FIX"/>
<pin name="1PPS"/>
<pin name="NC_2"/>
<pin name="NC_7"/>
<pin name="TX"/>
<pin name="RX"/>
</symbol>
<symbol name="M72">
<pin name="1/TXD"/>
<pin name="2/RXD"/>
<pin name="3/RTS"/>
<pin name="4/CTS"/>
<pin name="5/DTR"/>
<pin name="6/RESERVED"/>
<pin name="7/RESERVED"/>
<pin name="8/SIM_GND" direction="pwr"/>
<pin name="9/SIM_PRESENCE"/>
<pin name="10/SIM_DATA"/>
<pin name="11/SIM_VDD" direction="pwr"/>
<pin name="12/SIM_CLK"/>
<pin name="13/SIM_RST"/>
<pin name="14/PWRKEY"/>
<pin name="15/EMERG_OFF"/>
<pin name="16/VDD_EXT" direction="pwr"/>
<pin name="17/VRTC"/>
<pin name="18/DBG_TXD"/>
<pin name="19/DBG_RXD"/>
<pin name="20/DCD"/>
<pin name="21/NETLIGHT"/>
<pin name="22/STATUS"/>
<pin name="23/RI"/>
<pin name="24/VBAT"/>
<pin name="25/VBAT"/>
<pin name="26/GND" direction="pwr"/>
<pin name="27/GND" direction="pwr"/>
<pin name="28/RF_ANT"/>
<pin name="29/GND" direction="pwr"/>
<pin name="30/GND" direction="pwr"/>
</symbol>
<symbol name="QUECTELL20">
<pin name="RES"/>
<pin name="NC"/>
<pin name="TIMEP"/>
<pin name="RES2"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="RES3"/>
<pin name="VCC_RF"/>
<pin name="GND"/>
<pin name="RF_IN"/>
<pin name="GND2"/>
<pin name="GND4"/>
<pin name="VCC"/>
<pin name="V_BCKP"/>
<pin name="RXD1"/>
<pin name="TXD1"/>
<pin name="SCL2"/>
<pin name="SDA2"/>
<pin name="ON_OFF"/>
<pin name="RES4"/>
<pin name="NC6"/>
<pin name="NC5"/>
<pin name="GND3"/>
</symbol>
<symbol name="L10">
<pin name="VDDUSB" direction="pwr"/>
<pin name="RF_IN"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="V_BCKP" direction="pwr"/>
<pin name="RXD1" direction="in"/>
<pin name="TXD1" direction="out"/>
<pin name="VCC_OUT" direction="out"/>
<pin name="SCL2"/>
<pin name="SDA2"/>
<pin name="EXINT0" direction="in"/>
<pin name="AOK" direction="out"/>
<pin name="RESET_N" direction="in"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="VCC_RF" direction="out"/>
<pin name="V_ANT" direction="in"/>
<pin name="AADET_N" direction="in"/>
<pin name="TIMEPULSE" direction="out"/>
<pin name="RESERVED@1" direction="nc"/>
<pin name="RESERVED@2" direction="nc"/>
<pin name="RESERVED@3" direction="nc"/>
<pin name="RESERVED@4" direction="nc"/>
<pin name="RESERVED@5" direction="nc"/>
</symbol>
<symbol name="M10">
<pin name="DISP_DATA"/>
<pin name="DISP_CLK" direction="out"/>
<pin name="DISP_CS" direction="out"/>
<pin name="DISP_D/C" direction="out"/>
<pin name="DISP_RST" direction="out"/>
<pin name="NETLIGHT" direction="out"/>
<pin name="VDD_EXT" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="DBG_RXD" direction="in"/>
<pin name="DBG_TXD" direction="out"/>
<pin name="SIM_PRESENCE" direction="in"/>
<pin name="SIM_VDD" direction="out"/>
<pin name="SIM_DATA"/>
<pin name="SIM_CLK" direction="out"/>
<pin name="SIM_RST" direction="out"/>
<pin name="VRTC"/>
<pin name="EMERG_OFF" direction="in"/>
<pin name="PWRKEY" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="SPK2P" direction="out"/>
<pin name="SPK1N" direction="out"/>
<pin name="SPK1P" direction="out"/>
<pin name="MIC1P" direction="in"/>
<pin name="MIC1N" direction="in"/>
<pin name="MIC2P" direction="in"/>
<pin name="MIC2N" direction="in"/>
<pin name="LIGHT_MOS" direction="out"/>
<pin name="KBR0" direction="out"/>
<pin name="KBR1" direction="out"/>
<pin name="KBR2" direction="out"/>
<pin name="KBR3" direction="out"/>
<pin name="KBR4" direction="out"/>
<pin name="KBC0" direction="in"/>
<pin name="KBC1" direction="in"/>
<pin name="KBC2" direction="in"/>
<pin name="KBC3" direction="in"/>
<pin name="KBC4" direction="in"/>
<pin name="GPIO1_KBC5"/>
<pin name="BUZZER" direction="out"/>
<pin name="TEMP_BAT" direction="in"/>
<pin name="ADC0" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RF_ANT"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="VBAT@1" direction="pwr"/>
<pin name="VBAT@2" direction="pwr"/>
<pin name="VBAT@3" direction="pwr"/>
<pin name="VCHG" direction="in"/>
<pin name="STATUS" direction="out"/>
<pin name="RI" direction="out"/>
<pin name="DCD" direction="out"/>
<pin name="CTS" direction="out"/>
<pin name="RTS" direction="in"/>
<pin name="DTR" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="TXD3" direction="out"/>
<pin name="RXD3" direction="in"/>
<pin name="GPIO0"/>
</symbol>
<symbol name="SIM908">
<pin name="GND"/>
<pin name="GND2"/>
<pin name="PWRKEY"/>
<pin name="NC"/>
<pin name="GND3"/>
<pin name="DISP-CLK"/>
<pin name="DISP-DATA"/>
<pin name="DISP-DC"/>
<pin name="DISP-CS"/>
<pin name="GND4"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="GND5"/>
<pin name="GPS-DGB-TX"/>
<pin name="GPS-DBG-RX"/>
<pin name="SIM-DATA"/>
<pin name="SIM-RST"/>
<pin name="SIM-CLK"/>
<pin name="SIM-VDD"/>
<pin name="SPKN"/>
<pin name="SPKP"/>
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="SPK2P"/>
<pin name="SPK2N"/>
<pin name="MIC2P"/>
<pin name="MIC2N"/>
<pin name="NC5"/>
<pin name="NC6"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GND6"/>
<pin name="NC7"/>
<pin name="NC8"/>
<pin name="GND7"/>
<pin name="GND8"/>
<pin name="VRTC"/>
<pin name="GND9"/>
<pin name="VDD-EXD"/>
<pin name="NC9"/>
<pin name="NC10"/>
<pin name="ADC"/>
<pin name="PWM1"/>
<pin name="PWM2"/>
<pin name="PWM3"/>
<pin name="NETLIGHT"/>
<pin name="STATUS"/>
<pin name="NC11"/>
<pin name="NC12"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND10"/>
<pin name="GND11"/>
<pin name="GSM-ANTINA"/>
<pin name="GND12"/>
<pin name="GND13"/>
<pin name="VBAT"/>
<pin name="VBAT2"/>
<pin name="GND14"/>
<pin name="GND15"/>
<pin name="RTS"/>
<pin name="CTS"/>
<pin name="RXD"/>
<pin name="RI"/>
<pin name="DCD"/>
<pin name="TXD"/>
<pin name="DTR"/>
<pin name="TMP-BAT"/>
<pin name="VCHG"/>
<pin name="GPS-VANT-OUT"/>
<pin name="GPS-VANT-IN"/>
<pin name="GND16"/>
<pin name="GND17"/>
<pin name="GPS-ANTINA"/>
<pin name="GND18"/>
</symbol>
<symbol name="TC65">
<pin name="GND1"/>
<pin name="ADC1"/>
<pin name="ADC2"/>
<pin name="GND2"/>
<pin name="GPIO10"/>
<pin name="GPIO8"/>
<pin name="SPIDI"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="GPIO5"/>
<pin name="I2CCLK"/>
<pin name="VUSBIN"/>
<pin name="DAI5"/>
<pin name="ISENSE"/>
<pin name="DAI6"/>
<pin name="CCCLK"/>
<pin name="CCVCC"/>
<pin name="CCIO"/>
<pin name="CCRST"/>
<pin name="CCIN"/>
<pin name="CCGND"/>
<pin name="DAI4"/>
<pin name="DAI3"/>
<pin name="DAI2"/>
<pin name="DAI1"/>
<pin name="DAI0"/>
<pin name="BATTEMP"/>
<pin name="SYNC"/>
<pin name="RXD1"/>
<pin name="RXD0"/>
<pin name="TXD1"/>
<pin name="TXD0"/>
<pin name="VDDLP"/>
<pin name="VCHARGE"/>
<pin name="CHAGAT"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="GND6"/>
<pin name="GND7"/>
<pin name="BAT5"/>
<pin name="BAT4"/>
<pin name="BAT3"/>
<pin name="BAT2"/>
<pin name="BAT1"/>
<pin name="VEXT"/>
<pin name="RING0"/>
<pin name="DSR0"/>
<pin name="RTS0"/>
<pin name="DTR0"/>
<pin name="RTS1"/>
<pin name="CTS0"/>
<pin name="CTS1"/>
<pin name="DCD0"/>
<pin name="EMRGRST"/>
<pin name="IGT"/>
<pin name="AGND"/>
<pin name="MICN1"/>
<pin name="MICP1"/>
<pin name="MICP2"/>
<pin name="MICN2"/>
<pin name="EPN1"/>
<pin name="EPP1"/>
<pin name="EPP2"/>
<pin name="EPN2"/>
<pin name="VMIC"/>
<pin name="VSENSE"/>
<pin name="USBDN"/>
<pin name="USBDP"/>
<pin name="I2CDAT"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="SPICS"/>
<pin name="GPIO9"/>
<pin name="NC1"/>
<pin name="PWRIND"/>
<pin name="DACOUT"/>
<pin name="GND8"/>
</symbol>
<symbol name="MG2639">
<pin name="RF_ANT"/>
<pin name="RING" direction="out"/>
<pin name="RSSI_LED" direction="out"/>
<pin name="RTS"/>
<pin name="CTS" direction="out"/>
<pin name="DCD" direction="out"/>
<pin name="CARD_RST" direction="out"/>
<pin name="CARD_CLK" direction="out"/>
<pin name="CARD_DATA"/>
<pin name="V_CARD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="SYSRST_N" direction="in"/>
<pin name="SPK_2P" direction="out"/>
<pin name="SPK_1P" direction="out"/>
<pin name="SPK_1N" direction="out"/>
<pin name="MIC_2P" direction="in"/>
<pin name="MIC_1N" direction="in"/>
<pin name="MIC_1P" direction="in"/>
<pin name="PWRKEY_N" direction="in"/>
<pin name="DTR" direction="in"/>
<pin name="DSR" direction="out"/>
<pin name="V_MSM" direction="out"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="VCC">
<pin name="VBAT" direction="pwr"/>
</symbol>
<symbol name="M95">
<pin name="AGND" direction="pas"/>
<pin name="MIC2P" direction="pas"/>
<pin name="MIC2N" direction="pas"/>
<pin name="MIC1P" direction="pas"/>
<pin name="MIC1N" direction="pas"/>
<pin name="VBAT2" direction="pas"/>
<pin name="GND5" direction="pas"/>
<pin name="VBAT1" direction="pas"/>
<pin name="TXD" direction="pas"/>
<pin name="GND4" direction="pas"/>
<pin name="SPK1N" direction="pas"/>
<pin name="SPK1P" direction="pas"/>
<pin name="LOUDSPKN" direction="pas"/>
<pin name="LOUDSPKP" direction="pas"/>
<pin name="PWRKEY" direction="pas"/>
<pin name="EMERG_OFF" direction="pas"/>
<pin name="STATUS" direction="pas"/>
<pin name="NETLIGHT" direction="pas"/>
<pin name="RESERVED3" direction="pas"/>
<pin name="RESERVED4" direction="pas"/>
<pin name="VDD_EXT" direction="pas"/>
<pin name="RESERVED1" direction="pas"/>
<pin name="RESERVED2" direction="pas"/>
<pin name="VRTC" direction="pas"/>
<pin name="DBG_TXD" direction="pas"/>
<pin name="DBG_RXD" direction="pas"/>
<pin name="SIM_VDD" direction="pas"/>
<pin name="SIM_DATA" direction="pas"/>
<pin name="SIM_CLK" direction="pas"/>
<pin name="SIM_RST" direction="pas"/>
<pin name="RESERVED5" direction="pas"/>
<pin name="DTR" direction="pas"/>
<pin name="RXD" direction="pas"/>
<pin name="CTS" direction="pas"/>
<pin name="RTS" direction="pas"/>
<pin name="DCD" direction="pas"/>
<pin name="R1" direction="pas"/>
<pin name="SIM_GND" direction="pas"/>
<pin name="RF_ANT" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="GND1" direction="pas"/>
</symbol>
<symbol name="QUECTEL_L30">
<pin name="1/GND" direction="pwr"/>
<pin name="2/RESET" direction="in"/>
<pin name="3/CFGO/SCK"/>
<pin name="4/CFG1/SCS"/>
<pin name="5/TXD/MISO/SCL"/>
<pin name="6/RXD/MOSI/SDA"/>
<pin name="7/IPPS"/>
<pin name="8/VIO/RTC"/>
<pin name="9/VCC" direction="pwr"/>
<pin name="10/GND" direction="pwr"/>
<pin name="11/GND" direction="pwr"/>
<pin name="12/DR_I2C_CLK"/>
<pin name="13/DR_I2C_DIO"/>
<pin name="14/ON/OFF" direction="out"/>
<pin name="15/WAKEUP"/>
<pin name="16/EITO"/>
<pin name="17/GND" direction="pwr"/>
<pin name="18/GND" direction="pwr"/>
<pin name="19/RFIN" direction="in"/>
<pin name="20/GND" direction="pwr"/>
<pin name="21/GND" direction="pwr"/>
</symbol>
<symbol name="QUECTEL_M12">
<pin name="1/DISP_DATA"/>
<pin name="2/DISP_CLK" direction="out"/>
<pin name="3/DISP_CS" direction="out"/>
<pin name="4/DISP_D/C" direction="out"/>
<pin name="5/DISP_RST" direction="out"/>
<pin name="6/NETLIGHT" direction="out"/>
<pin name="7/VDD_EXT" direction="out"/>
<pin name="8/GND1" direction="pwr"/>
<pin name="9/DBG_RXD" direction="in"/>
<pin name="10/DBG_TXD" direction="out"/>
<pin name="11/SIM_PRESENCE" direction="in"/>
<pin name="12/SIM_VDD" direction="out"/>
<pin name="13/SIM_DATA"/>
<pin name="14/SIM_CLK" direction="out"/>
<pin name="15/SIM_RST" direction="out"/>
<pin name="16/VRTC"/>
<pin name="17/EMERG_OFF" direction="in"/>
<pin name="18/PWRKEY" direction="in"/>
<pin name="19/AGND" direction="out"/>
<pin name="20/SPK2P" direction="out"/>
<pin name="21/SPK1N" direction="out"/>
<pin name="22/SPK1P" direction="out"/>
<pin name="23/MIC1P" direction="in"/>
<pin name="24/MIC1N" direction="in"/>
<pin name="25/MIC2P" direction="in"/>
<pin name="26/MIC2N" direction="in"/>
<pin name="27/LIGHT_MOS" direction="out"/>
<pin name="28/KBR0" direction="out"/>
<pin name="29/KBR1" direction="out"/>
<pin name="30/KBR2" direction="out"/>
<pin name="31/KBR3" direction="out"/>
<pin name="32/KBR4" direction="out"/>
<pin name="33/KBC0" direction="in"/>
<pin name="34/KBC1" direction="in"/>
<pin name="35/KBC2" direction="in"/>
<pin name="36/KBC3" direction="in"/>
<pin name="37/KBC4" direction="in"/>
<pin name="38/GPIO1_KBC5"/>
<pin name="39/BUZZER" direction="out"/>
<pin name="40/TEMP_BAT" direction="in"/>
<pin name="41/ADC0" direction="in"/>
<pin name="42/GND2" direction="pwr"/>
<pin name="43/RF_ANT"/>
<pin name="44/GND3" direction="pwr"/>
<pin name="45/GND4" direction="pwr"/>
<pin name="46/GND5" direction="pwr"/>
<pin name="47/GND6" direction="pwr"/>
<pin name="48/GND7" direction="pwr"/>
<pin name="49/GND8" direction="pwr"/>
<pin name="50/VBAT1" direction="in"/>
<pin name="51/VBAT2" direction="in"/>
<pin name="52/VBAT3" direction="in"/>
<pin name="53/VCHG" direction="in"/>
<pin name="54/STATUS" direction="out"/>
<pin name="55/RI" direction="out"/>
<pin name="56/DCD" direction="out"/>
<pin name="57/CTS" direction="out"/>
<pin name="58/RTS" direction="in"/>
<pin name="59/DTR" direction="in"/>
<pin name="60/TXD" direction="out"/>
<pin name="61/RXD" direction="in"/>
<pin name="62/RESERVED" direction="nc"/>
<pin name="63/RESERVED" direction="nc"/>
<pin name="64/GPIO0"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="COPERNICUS" prefix="M" uservalue="yes">
<description>&lt;b&gt;Copernicus GPS Receiver Module&lt;p&gt;
&lt;font color="red"&gt;!!! OBSOLETE, DO NOT USE FOR NEW DESIGNS !!!&lt;/font&gt;&lt;/b&gt;&lt;p&gt;
SMD GPS Receiver module,  made by
&lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 58048-00, 58048-10 and 58048-20&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="M1" symbol="COPERNICUS"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="M1" pin="GND@1" pad="1"/>
<connect gate="M1" pin="GND@13" pad="13"/>
<connect gate="M1" pin="GND@14" pad="14"/>
<connect gate="M1" pin="GND@15" pad="15"/>
<connect gate="M1" pin="GND@2" pad="2"/>
<connect gate="M1" pin="GND@27" pad="27"/>
<connect gate="M1" pin="GND@28" pad="28"/>
<connect gate="M1" pin="GND@4" pad="4"/>
<connect gate="M1" pin="LNA_XEN" pad="5"/>
<connect gate="M1" pin="OPEN" pad="7"/>
<connect gate="M1" pin="PPS" pad="19"/>
<connect gate="M1" pin="RESERVED@10" pad="10"/>
<connect gate="M1" pin="RESERVED@17" pad="17"/>
<connect gate="M1" pin="RESERVED@18" pad="18"/>
<connect gate="M1" pin="RESERVED@22" pad="22"/>
<connect gate="M1" pin="RESERVED@25" pad="25"/>
<connect gate="M1" pin="RESERVED@26" pad="26"/>
<connect gate="M1" pin="RESERVED@6" pad="6"/>
<connect gate="M1" pin="RESERVED@9" pad="9"/>
<connect gate="M1" pin="RF_IN" pad="3"/>
<connect gate="M1" pin="RXD_A" pad="21"/>
<connect gate="M1" pin="RXD_B" pad="20"/>
<connect gate="M1" pin="SHORT" pad="8"/>
<connect gate="M1" pin="TXD_A" pad="23"/>
<connect gate="M1" pin="TXD_B" pad="24"/>
<connect gate="M1" pin="VCC" pad="12"/>
<connect gate="M1" pin="XRESET" pad="11"/>
<connect gate="M1" pin="XSTANDBY" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C1216_CONDOR" prefix="M" uservalue="yes">
<description>&lt;b&gt;Condor C1216 GPS Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 68676-10&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/condor-gps-module.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="C1216"/>
</gates>
<devices>
<device name="-SMD" package="1216">
<connects>
<connect gate="G$1" pin="1PPS" pad="3"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="RESERVED@1" pad="1"/>
<connect gate="G$1" pin="RESERVED@14" pad="14"/>
<connect gate="G$1" pin="RESERVED@15" pad="15"/>
<connect gate="G$1" pin="RESERVED@16" pad="16"/>
<connect gate="G$1" pin="RESERVED@18" pad="18"/>
<connect gate="G$1" pin="RESERVED@19" pad="19"/>
<connect gate="G$1" pin="RESERVED@4" pad="4"/>
<connect gate="G$1" pin="RESERVED@8" pad="8"/>
<connect gate="G$1" pin="RF_IN" pad="11"/>
<connect gate="G$1" pin="RTCM-IN" pad="17"/>
<connect gate="G$1" pin="RXD" pad="21"/>
<connect gate="G$1" pin="TXD" pad="20"/>
<connect gate="G$1" pin="USB-DM" pad="5"/>
<connect gate="G$1" pin="USB-DP" pad="6"/>
<connect gate="G$1" pin="V28A" pad="9"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VDD-USB" pad="7"/>
<connect gate="G$1" pin="VRTC" pad="22"/>
<connect gate="G$1" pin="XRESET" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C1919A_CONDOR" prefix="M" uservalue="yes">
<description>&lt;b&gt;Condor C1919A GPS Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 67650-10&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/condor-gps-module.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="C1919A"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@16" pad="16"/>
<connect gate="G$1" pin="RESERVED@17" pad="17"/>
<connect gate="G$1" pin="RESERVED@18" pad="18"/>
<connect gate="G$1" pin="RESERVED@21" pad="21"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@23" pad="23"/>
<connect gate="G$1" pin="RESERVED@25" pad="25"/>
<connect gate="G$1" pin="RESERVED@26" pad="26"/>
<connect gate="G$1" pin="RESERVED@5" pad="5"/>
<connect gate="G$1" pin="RESERVED@7" pad="7"/>
<connect gate="G$1" pin="RESERVED@8" pad="8"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RXD" pad="20"/>
<connect gate="G$1" pin="TXD" pad="24"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VRTC" pad="6"/>
<connect gate="G$1" pin="XRESET" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C1919B_CONDOR" prefix="M" uservalue="yes">
<description>&lt;b&gt;Condor C1919B GPS Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 67650-00&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/condor-gps-module.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="C1919B"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@16" pad="16"/>
<connect gate="G$1" pin="RESERVED@18" pad="18"/>
<connect gate="G$1" pin="RESERVED@21" pad="21"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@23" pad="23"/>
<connect gate="G$1" pin="RESERVED@25" pad="25"/>
<connect gate="G$1" pin="RESERVED@26" pad="26"/>
<connect gate="G$1" pin="RESERVED@5" pad="5"/>
<connect gate="G$1" pin="RESERVED@7" pad="7"/>
<connect gate="G$1" pin="RESERVED@8" pad="8"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RTC_CLK" pad="17"/>
<connect gate="G$1" pin="RXD" pad="20"/>
<connect gate="G$1" pin="TXD" pad="24"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VRTC" pad="6"/>
<connect gate="G$1" pin="XRESET" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C1919C_CONDOR" prefix="M" uservalue="yes">
<description>&lt;b&gt;Condor C1919C GPS Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 67650-20&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/condor-gps-module.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="C1919A"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@16" pad="16"/>
<connect gate="G$1" pin="RESERVED@17" pad="17"/>
<connect gate="G$1" pin="RESERVED@18" pad="18"/>
<connect gate="G$1" pin="RESERVED@21" pad="21"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@23" pad="23"/>
<connect gate="G$1" pin="RESERVED@25" pad="25"/>
<connect gate="G$1" pin="RESERVED@26" pad="26"/>
<connect gate="G$1" pin="RESERVED@5" pad="5"/>
<connect gate="G$1" pin="RESERVED@7" pad="7"/>
<connect gate="G$1" pin="RESERVED@8" pad="8"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RXD" pad="20"/>
<connect gate="G$1" pin="TXD" pad="24"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VRTC" pad="6"/>
<connect gate="G$1" pin="XRESET" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C1722_CONDOR" prefix="M" uservalue="yes">
<description>&lt;b&gt;Condor C1722 GPS Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 68675-00&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/condor-gps-module.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="C1722"/>
</gates>
<devices>
<device name="-SMD" package="1722">
<connects>
<connect gate="G$1" pin="1PPS" pad="28"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="RESERVED@1" pad="1"/>
<connect gate="G$1" pin="RESERVED@12" pad="12"/>
<connect gate="G$1" pin="RESERVED@2" pad="2"/>
<connect gate="G$1" pin="RESERVED@20" pad="20"/>
<connect gate="G$1" pin="RESERVED@21" pad="21"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@23" pad="23"/>
<connect gate="G$1" pin="RESERVED@27" pad="27"/>
<connect gate="G$1" pin="RESERVED@5" pad="5"/>
<connect gate="G$1" pin="RESERVED@8" pad="8"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="16"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="3"/>
<connect gate="G$1" pin="USB-DM" pad="25"/>
<connect gate="G$1" pin="USB-DP" pad="26"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VDD-USB" pad="24"/>
<connect gate="G$1" pin="VRTC" pad="11"/>
<connect gate="G$1" pin="VS-AA" pad="19"/>
<connect gate="G$1" pin="VS-LNA" pad="18"/>
<connect gate="G$1" pin="XRESET" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C1011_CONDOR" prefix="M" uservalue="yes">
<description>&lt;b&gt;Condor C1011 GPS Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 68674-00&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/condor-gps-module.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="C1011"/>
</gates>
<devices>
<device name="-SMD" package="1011">
<connects>
<connect gate="G$1" pin="1PPS" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@33" pad="33"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@37" pad="37"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="RESERVED@11" pad="11"/>
<connect gate="G$1" pin="RESERVED@12" pad="12"/>
<connect gate="G$1" pin="RESERVED@13" pad="13"/>
<connect gate="G$1" pin="RESERVED@14" pad="14"/>
<connect gate="G$1" pin="RESERVED@20" pad="20"/>
<connect gate="G$1" pin="RESERVED@29" pad="29"/>
<connect gate="G$1" pin="RESERVED@30" pad="30"/>
<connect gate="G$1" pin="RESERVED@31" pad="31"/>
<connect gate="G$1" pin="RESERVED@34" pad="34"/>
<connect gate="G$1" pin="RESERVED@5" pad="5"/>
<connect gate="G$1" pin="RF_IN" pad="18"/>
<connect gate="G$1" pin="RTC_IN" pad="2"/>
<connect gate="G$1" pin="RTC_OUT" pad="38"/>
<connect gate="G$1" pin="RXD" pad="6"/>
<connect gate="G$1" pin="TXD" pad="10"/>
<connect gate="G$1" pin="VCC@15" pad="15"/>
<connect gate="G$1" pin="VCC@24" pad="24"/>
<connect gate="G$1" pin="VCC@32" pad="32"/>
<connect gate="G$1" pin="VRTC" pad="4"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XSTANDBY" pad="36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COPERNICUS-II" prefix="M" uservalue="yes">
<description>&lt;b&gt;Copernicus-II GPS Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 63530-00 and 63530-10&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/copernicus2.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="COPERNICUS-II"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="LNA_XEN" pad="5"/>
<connect gate="G$1" pin="OPEN" pad="7"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@17" pad="17"/>
<connect gate="G$1" pin="RESERVED@18" pad="18"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@25" pad="25"/>
<connect gate="G$1" pin="RESERVED@26" pad="26"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RXD_A" pad="21"/>
<connect gate="G$1" pin="RXD_B" pad="20"/>
<connect gate="G$1" pin="SHORT" pad="8"/>
<connect gate="G$1" pin="TXD_A" pad="23"/>
<connect gate="G$1" pin="TXD_B" pad="24"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="XRESET" pad="11"/>
<connect gate="G$1" pin="XSTANDBY" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESOLUTION-SMT" prefix="M" uservalue="yes">
<description>&lt;b&gt;Resolution-SMT GPS Timing Receiver Module&lt;/b&gt;&lt;p&gt;
&lt;p&gt;
SMD GPS Timing Receiver module,  made by &lt;a href="http://www.trimble.com/timing/"&gt;Trimble Navigation Ltd, Timing Group&lt;/a&gt;&lt;p&gt;
Partnumber: 66266-00&lt;p&gt;
&lt;a href="http://www.trimble.com/timing/resolution-smt.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="RESOLUTION-SMT"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="OPEN" pad="5"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@11" pad="11"/>
<connect gate="G$1" pin="RESERVED@12" pad="12"/>
<connect gate="G$1" pin="RESERVED@13" pad="13"/>
<connect gate="G$1" pin="RESERVED@23" pad="23"/>
<connect gate="G$1" pin="RESERVED@7" pad="7"/>
<connect gate="G$1" pin="RESERVED@8" pad="8"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RESET" pad="25"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RXD_A" pad="16"/>
<connect gate="G$1" pin="RXD_B" pad="21"/>
<connect gate="G$1" pin="SHORT" pad="6"/>
<connect gate="G$1" pin="TXD_A" pad="17"/>
<connect gate="G$1" pin="TXD_B" pad="22"/>
<connect gate="G$1" pin="VCC" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM-SMT_10MHZ" prefix="M" uservalue="yes">
<description>&lt;b&gt;ICM-SMT GPS Timing Receiver Module 10MHz&lt;/b&gt;&lt;p&gt;
SMD GPS Timing Receiver module,  made by &lt;a href="http://www.trimble.com/timing/"&gt;Trimble Navigation Ltd, Timing Group&lt;/a&gt;&lt;p&gt;
Partnumber: 77766-00&lt;p&gt;
&lt;a href="http://www.trimble.com/timing/ICM_SMT_GPS_Disciplined_Clock.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="ICM-SMT"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="OPEN" pad="5"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@11" pad="11"/>
<connect gate="G$1" pin="RESERVED@12" pad="12"/>
<connect gate="G$1" pin="RESERVED@13" pad="13"/>
<connect gate="G$1" pin="RESERVED@21" pad="21"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@7" pad="7"/>
<connect gate="G$1" pin="RESERVED@8" pad="8"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RESET" pad="25"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RXD" pad="16"/>
<connect gate="G$1" pin="SHORT" pad="6"/>
<connect gate="G$1" pin="SYSCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="17"/>
<connect gate="G$1" pin="VCC" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM-SMT_40MHZ" prefix="M" uservalue="yes">
<description>&lt;b&gt;ICM-SMT GPS Timing Receiver Module 40MHz&lt;/b&gt;&lt;p&gt;
SMD GPS Timing Receiver module,  made by &lt;a href="http://www.trimble.com/timing/"&gt;Trimble Navigation Ltd, Timing Group&lt;/a&gt;&lt;p&gt;
Partnumber: 66650-19&lt;p&gt;
&lt;a href="http://www.trimble.com/timing/ICM_SMT_GPS_Disciplined_Clock.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="ICM-SMT"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="OPEN" pad="5"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@11" pad="11"/>
<connect gate="G$1" pin="RESERVED@12" pad="12"/>
<connect gate="G$1" pin="RESERVED@13" pad="13"/>
<connect gate="G$1" pin="RESERVED@21" pad="21"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@7" pad="7"/>
<connect gate="G$1" pin="RESERVED@8" pad="8"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RESET" pad="25"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RXD" pad="16"/>
<connect gate="G$1" pin="SHORT" pad="6"/>
<connect gate="G$1" pin="SYSCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="17"/>
<connect gate="G$1" pin="VCC" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMBLE-LOGO" prefix="TRIMBLE-LOGO">
<description>&lt;b&gt;Trimble-Logo&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="TRIMBLE-LOGO"/>
</gates>
<devices>
<device name="" package="TRIMBLE-LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A1919_AARDVARK" prefix="M" uservalue="yes">
<description>&lt;b&gt;Aardvark GPS+DR Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS Dead-Reckoning Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 88788-30 and 88788-50&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/aardvark.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="A1919_AARDVARK"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="FWD/REV" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="OPEN" pad="7"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@12" pad="12"/>
<connect gate="G$1" pin="RESERVED@13" pad="13"/>
<connect gate="G$1" pin="RESERVED@17" pad="17"/>
<connect gate="G$1" pin="RESERVED@18" pad="18"/>
<connect gate="G$1" pin="RESERVED@21" pad="21"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@23" pad="23"/>
<connect gate="G$1" pin="RESERVED@27" pad="27"/>
<connect gate="G$1" pin="RESERVED@5" pad="5"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RXD" pad="20"/>
<connect gate="G$1" pin="SHORT" pad="8"/>
<connect gate="G$1" pin="TACHO" pad="25"/>
<connect gate="G$1" pin="TXD" pad="24"/>
<connect gate="G$1" pin="VBACK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="XRESET" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="B1919_BUFFALO" prefix="M" uservalue="yes">
<description>&lt;b&gt;Buffalo B1919 GNSS Receiver Module&lt;/b&gt;&lt;p&gt;
SMD GPS/GLONASS/GALILEO/COMPASS Receiver module,  made by &lt;a href="http://www.trimble.com/embeddedsystems/"&gt;Trimble Navigation Ltd, Embedded Systems Group&lt;/a&gt;&lt;p&gt;
Partnumber: 99777-00&lt;p&gt;
&lt;a href="http://www.trimble.com/embeddedsystems/buffalo.aspx"&gt; Datasheet, User Manual and Tools&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by Trimble Navigation Ltd, Author: &lt;a href="mailto:christian_voit@trimble.com?subject=Trimble Eagle Library"&gt;Christian Voit&lt;/a&gt;&lt;/author&gt;&lt;P&gt;</description>
<gates>
<gate name="G$1" symbol="B1919_BUFFALO"/>
</gates>
<devices>
<device name="-SMD" package="1919">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="LNA_XEN" pad="5"/>
<connect gate="G$1" pin="OPEN" pad="7"/>
<connect gate="G$1" pin="PPS" pad="19"/>
<connect gate="G$1" pin="RESERVED@10" pad="10"/>
<connect gate="G$1" pin="RESERVED@13" pad="13"/>
<connect gate="G$1" pin="RESERVED@22" pad="22"/>
<connect gate="G$1" pin="RESERVED@25" pad="25"/>
<connect gate="G$1" pin="RESERVED@26" pad="26"/>
<connect gate="G$1" pin="RESERVED@27" pad="27"/>
<connect gate="G$1" pin="RESERVED@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="3"/>
<connect gate="G$1" pin="RXD_A" pad="21"/>
<connect gate="G$1" pin="RXD_B" pad="20"/>
<connect gate="G$1" pin="SHORT" pad="8"/>
<connect gate="G$1" pin="TXD_A" pad="23"/>
<connect gate="G$1" pin="TXD_B" pad="24"/>
<connect gate="G$1" pin="USB_DM" pad="18"/>
<connect gate="G$1" pin="USB_DP" pad="17"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VDD_USB" pad="14"/>
<connect gate="G$1" pin="XRESET" pad="11"/>
<connect gate="G$1" pin="XSTANDBY" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FGPMMOPA6E" prefix="IC" uservalue="yes">
<description>66-channel GPS Engine Board</description>
<gates>
<gate name="G$1" symbol="FGPMMOPA6"/>
</gates>
<devices>
<device name="" package="FGPMMOPA6E">
<connects>
<connect gate="G$1" pin="1/VCC" pad="1"/>
<connect gate="G$1" pin="10/RXD" pad="10"/>
<connect gate="G$1" pin="2/ENABLE" pad="2"/>
<connect gate="G$1" pin="3/GND" pad="3"/>
<connect gate="G$1" pin="4/VBACKUP" pad="4"/>
<connect gate="G$1" pin="5/3D-FIX" pad="5"/>
<connect gate="G$1" pin="6/DPLUS" pad="6"/>
<connect gate="G$1" pin="7/DMINUS" pad="7"/>
<connect gate="G$1" pin="8/GND" pad="8"/>
<connect gate="G$1" pin="9/TXD" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS-FGPMMOPA6C" prefix="GPS" uservalue="yes">
<description>The FGPMMOPA6E is a revision of PA6 POT (Patch On Top) GPS Module with an extra embedded
function for external antenna I/O and comes with automatic antenna switching function and short
circuit protection. This POT GPS receiver uses internal patch antenna and will automatically detect
and switch over to external antenna for GPS reception once a connection to external antenna is
made. In addition, the module itself is protected from short circuits to the external antenna. PA6E is
high in position and speed accuracy as well as being high in sensitivity with excellent tracking
capabilities in urban conditions. The GPS chipset inside the module is powered by MediaTek Inc., and
can support up to 66 channels. The module is suitable for every GPS‐related application such as:</description>
<gates>
<gate name="G$1" symbol="GPS-FGPMMOPA6C"/>
</gates>
<devices>
<device name="" package="GPS">
<connects>
<connect gate="G$1" pin="1PPS" pad="P$6"/>
<connect gate="G$1" pin="3D-FIX" pad="P$5"/>
<connect gate="G$1" pin="GND_11" pad="P$11"/>
<connect gate="G$1" pin="GND_12" pad="P$12"/>
<connect gate="G$1" pin="GND_13" pad="P$13"/>
<connect gate="G$1" pin="GND_3" pad="P$3"/>
<connect gate="G$1" pin="GND_8" pad="P$8"/>
<connect gate="G$1" pin="NC_2" pad="P$2"/>
<connect gate="G$1" pin="NC_7" pad="P$7"/>
<connect gate="G$1" pin="RX" pad="P$10"/>
<connect gate="G$1" pin="TX" pad="P$9"/>
<connect gate="G$1" pin="VBACKUP" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUECTEL_M72" prefix="IC" uservalue="yes">
<description>Moduł GSM/GPRS//


http://www.meraprojekt.com.pl/files/quectel/M72_HD_V1.1.pdf</description>
<gates>
<gate name="M72" symbol="M72"/>
</gates>
<devices>
<device name="" package="M72">
<connects>
<connect gate="M72" pin="1/TXD" pad="P$1"/>
<connect gate="M72" pin="10/SIM_DATA" pad="P$10"/>
<connect gate="M72" pin="11/SIM_VDD" pad="P$11"/>
<connect gate="M72" pin="12/SIM_CLK" pad="P$12"/>
<connect gate="M72" pin="13/SIM_RST" pad="P$13"/>
<connect gate="M72" pin="14/PWRKEY" pad="P$14"/>
<connect gate="M72" pin="15/EMERG_OFF" pad="P$15"/>
<connect gate="M72" pin="16/VDD_EXT" pad="P$16"/>
<connect gate="M72" pin="17/VRTC" pad="P$17"/>
<connect gate="M72" pin="18/DBG_TXD" pad="P$18"/>
<connect gate="M72" pin="19/DBG_RXD" pad="P$19"/>
<connect gate="M72" pin="2/RXD" pad="P$2"/>
<connect gate="M72" pin="20/DCD" pad="P$20"/>
<connect gate="M72" pin="21/NETLIGHT" pad="P$21"/>
<connect gate="M72" pin="22/STATUS" pad="P$22"/>
<connect gate="M72" pin="23/RI" pad="P$23"/>
<connect gate="M72" pin="24/VBAT" pad="P$24"/>
<connect gate="M72" pin="25/VBAT" pad="P$25"/>
<connect gate="M72" pin="26/GND" pad="P$26"/>
<connect gate="M72" pin="27/GND" pad="P$27"/>
<connect gate="M72" pin="28/RF_ANT" pad="P$28"/>
<connect gate="M72" pin="29/GND" pad="P$29"/>
<connect gate="M72" pin="3/RTS" pad="P$3"/>
<connect gate="M72" pin="30/GND" pad="P$30"/>
<connect gate="M72" pin="4/CTS" pad="P$4"/>
<connect gate="M72" pin="5/DTR" pad="P$5"/>
<connect gate="M72" pin="6/RESERVED" pad="P$6"/>
<connect gate="M72" pin="7/RESERVED" pad="P$7"/>
<connect gate="M72" pin="8/SIM_GND" pad="P$8"/>
<connect gate="M72" pin="9/SIM_PRESENCE" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUECTEL_L20" uservalue="yes">
<description>Quectel L20 module by Jozsef Kovacs, RobotSzoft Kft</description>
<gates>
<gate name="G$1" symbol="QUECTELL20"/>
</gates>
<devices>
<device name="" package="QUECTEL_L20">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="NC3" pad="NC3"/>
<connect gate="G$1" pin="NC4" pad="NC4"/>
<connect gate="G$1" pin="NC5" pad="NC5"/>
<connect gate="G$1" pin="NC6" pad="NC6"/>
<connect gate="G$1" pin="ON_OFF" pad="ON_OFF"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RES2" pad="RES2"/>
<connect gate="G$1" pin="RES3" pad="RES3"/>
<connect gate="G$1" pin="RES4" pad="RES4"/>
<connect gate="G$1" pin="RF_IN" pad="RF_IN"/>
<connect gate="G$1" pin="RXD1" pad="RXD1"/>
<connect gate="G$1" pin="SCL2" pad="SCL2"/>
<connect gate="G$1" pin="SDA2" pad="SDA2"/>
<connect gate="G$1" pin="TIMEP" pad="TIMEP"/>
<connect gate="G$1" pin="TXD1" pad="TXD1"/>
<connect gate="G$1" pin="VCC" pad="VCC_RF"/>
<connect gate="G$1" pin="VCC_RF" pad="VDD"/>
<connect gate="G$1" pin="V_BCKP" pad="V_BCKP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUECTEL_10" prefix="GPS">
<description>&lt;H3&gt;Quectel L10&lt;/H3&gt;
&lt;p&gt;GPS Module by Quectel&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="L10"/>
</gates>
<devices>
<device name="" package="L10">
<connects>
<connect gate="G$1" pin="AADET_N" pad="20"/>
<connect gate="G$1" pin="AOK" pad="12"/>
<connect gate="G$1" pin="EXINT0" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="13"/>
<connect gate="G$1" pin="GND@3" pad="14"/>
<connect gate="G$1" pin="GND@4" pad="15"/>
<connect gate="G$1" pin="GND@5" pad="17"/>
<connect gate="G$1" pin="RESERVED@1" pad="5"/>
<connect gate="G$1" pin="RESERVED@2" pad="9"/>
<connect gate="G$1" pin="RESERVED@3" pad="21"/>
<connect gate="G$1" pin="RESERVED@4" pad="22"/>
<connect gate="G$1" pin="RESERVED@5" pad="23"/>
<connect gate="G$1" pin="RESET_N" pad="10"/>
<connect gate="G$1" pin="RF_IN" pad="16"/>
<connect gate="G$1" pin="RXD1" pad="4"/>
<connect gate="G$1" pin="SCL2" pad="2"/>
<connect gate="G$1" pin="SDA2" pad="1"/>
<connect gate="G$1" pin="TIMEPULSE" pad="28"/>
<connect gate="G$1" pin="TXD1" pad="3"/>
<connect gate="G$1" pin="USB_DM" pad="25"/>
<connect gate="G$1" pin="USB_DP" pad="26"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VCC_OUT" pad="8"/>
<connect gate="G$1" pin="VCC_RF" pad="18"/>
<connect gate="G$1" pin="VDDUSB" pad="24"/>
<connect gate="G$1" pin="V_ANT" pad="19"/>
<connect gate="G$1" pin="V_BCKP" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUECTEL_M10" prefix="GSM">
<description>&lt;h3&gt;Quectel M10 &lt;/h3&gt;
&lt;p&gt;GSM module by Quectel&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="M10"/>
</gates>
<devices>
<device name="" package="M10">
<connects>
<connect gate="G$1" pin="ADC0" pad="41"/>
<connect gate="G$1" pin="AGND" pad="19"/>
<connect gate="G$1" pin="BUZZER" pad="39"/>
<connect gate="G$1" pin="CTS" pad="57"/>
<connect gate="G$1" pin="DBG_RXD" pad="9"/>
<connect gate="G$1" pin="DBG_TXD" pad="10"/>
<connect gate="G$1" pin="DCD" pad="56"/>
<connect gate="G$1" pin="DISP_CLK" pad="2"/>
<connect gate="G$1" pin="DISP_CS" pad="3"/>
<connect gate="G$1" pin="DISP_D/C" pad="4"/>
<connect gate="G$1" pin="DISP_DATA" pad="1"/>
<connect gate="G$1" pin="DISP_RST" pad="5"/>
<connect gate="G$1" pin="DTR" pad="59"/>
<connect gate="G$1" pin="EMERG_OFF" pad="17"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="42"/>
<connect gate="G$1" pin="GND@3" pad="44"/>
<connect gate="G$1" pin="GND@4" pad="45"/>
<connect gate="G$1" pin="GND@5" pad="46"/>
<connect gate="G$1" pin="GND@6" pad="47"/>
<connect gate="G$1" pin="GND@7" pad="48"/>
<connect gate="G$1" pin="GND@8" pad="49"/>
<connect gate="G$1" pin="GPIO0" pad="64"/>
<connect gate="G$1" pin="GPIO1_KBC5" pad="38"/>
<connect gate="G$1" pin="KBC0" pad="33"/>
<connect gate="G$1" pin="KBC1" pad="34"/>
<connect gate="G$1" pin="KBC2" pad="35"/>
<connect gate="G$1" pin="KBC3" pad="36"/>
<connect gate="G$1" pin="KBC4" pad="37"/>
<connect gate="G$1" pin="KBR0" pad="28"/>
<connect gate="G$1" pin="KBR1" pad="29"/>
<connect gate="G$1" pin="KBR2" pad="30"/>
<connect gate="G$1" pin="KBR3" pad="31"/>
<connect gate="G$1" pin="KBR4" pad="32"/>
<connect gate="G$1" pin="LIGHT_MOS" pad="27"/>
<connect gate="G$1" pin="MIC1N" pad="24"/>
<connect gate="G$1" pin="MIC1P" pad="23"/>
<connect gate="G$1" pin="MIC2N" pad="26"/>
<connect gate="G$1" pin="MIC2P" pad="25"/>
<connect gate="G$1" pin="NETLIGHT" pad="6"/>
<connect gate="G$1" pin="PWRKEY" pad="18"/>
<connect gate="G$1" pin="RF_ANT" pad="43"/>
<connect gate="G$1" pin="RI" pad="55"/>
<connect gate="G$1" pin="RTS" pad="58"/>
<connect gate="G$1" pin="RXD" pad="61"/>
<connect gate="G$1" pin="RXD3" pad="63"/>
<connect gate="G$1" pin="SIM_CLK" pad="14"/>
<connect gate="G$1" pin="SIM_DATA" pad="13"/>
<connect gate="G$1" pin="SIM_PRESENCE" pad="11"/>
<connect gate="G$1" pin="SIM_RST" pad="15"/>
<connect gate="G$1" pin="SIM_VDD" pad="12"/>
<connect gate="G$1" pin="SPK1N" pad="21"/>
<connect gate="G$1" pin="SPK1P" pad="22"/>
<connect gate="G$1" pin="SPK2P" pad="20"/>
<connect gate="G$1" pin="STATUS" pad="54"/>
<connect gate="G$1" pin="TEMP_BAT" pad="40"/>
<connect gate="G$1" pin="TXD" pad="60"/>
<connect gate="G$1" pin="TXD3" pad="62"/>
<connect gate="G$1" pin="VBAT@1" pad="50"/>
<connect gate="G$1" pin="VBAT@2" pad="51"/>
<connect gate="G$1" pin="VBAT@3" pad="52"/>
<connect gate="G$1" pin="VCHG" pad="53"/>
<connect gate="G$1" pin="VDD_EXT" pad="7"/>
<connect gate="G$1" pin="VRTC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIM908">
<description>Combination GSM/GPRS+GPS Module in an SMT package</description>
<gates>
<gate name="G$1" symbol="SIM908"/>
</gates>
<devices>
<device name="" package="SIM908">
<connects>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CTS" pad="CTS"/>
<connect gate="G$1" pin="DCD" pad="DCD"/>
<connect gate="G$1" pin="DISP-CLK" pad="DISP-CLK"/>
<connect gate="G$1" pin="DISP-CS" pad="DISP-CS"/>
<connect gate="G$1" pin="DISP-DATA" pad="DISP-DATA"/>
<connect gate="G$1" pin="DISP-DC" pad="DISP-DC"/>
<connect gate="G$1" pin="DTR" pad="DTR"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND10" pad="GND10"/>
<connect gate="G$1" pin="GND11" pad="GND11"/>
<connect gate="G$1" pin="GND12" pad="GND12"/>
<connect gate="G$1" pin="GND13" pad="GND13"/>
<connect gate="G$1" pin="GND14" pad="GND14"/>
<connect gate="G$1" pin="GND15" pad="GND15"/>
<connect gate="G$1" pin="GND16" pad="GND16"/>
<connect gate="G$1" pin="GND17" pad="GND17"/>
<connect gate="G$1" pin="GND18" pad="GND18"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="GND5" pad="GND5"/>
<connect gate="G$1" pin="GND6" pad="GND6"/>
<connect gate="G$1" pin="GND7" pad="GND7"/>
<connect gate="G$1" pin="GND8" pad="GND8"/>
<connect gate="G$1" pin="GND9" pad="GND9"/>
<connect gate="G$1" pin="GPIO1" pad="GPIO1"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO3" pad="GPIO3"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="GPIO6" pad="GPIO6"/>
<connect gate="G$1" pin="GPS-ANTINA" pad="GPS-ANTINA"/>
<connect gate="G$1" pin="GPS-DBG-RX" pad="GPS-DBG-RXD"/>
<connect gate="G$1" pin="GPS-DGB-TX" pad="GPS-DBG-TXD"/>
<connect gate="G$1" pin="GPS-VANT-IN" pad="GPS-VANT-IN"/>
<connect gate="G$1" pin="GPS-VANT-OUT" pad="GPS-VANT-OUT"/>
<connect gate="G$1" pin="GSM-ANTINA" pad="GSM-ANTINA"/>
<connect gate="G$1" pin="MIC2N" pad="MIC2N"/>
<connect gate="G$1" pin="MIC2P" pad="MIC2P"/>
<connect gate="G$1" pin="MICN" pad="MIC1N"/>
<connect gate="G$1" pin="MICP" pad="MIC1P"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NC10" pad="NC10"/>
<connect gate="G$1" pin="NC11" pad="NC11"/>
<connect gate="G$1" pin="NC12" pad="NC12"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="NC3" pad="NC3"/>
<connect gate="G$1" pin="NC4" pad="NC4"/>
<connect gate="G$1" pin="NC5" pad="NC5"/>
<connect gate="G$1" pin="NC6" pad="NC6"/>
<connect gate="G$1" pin="NC7" pad="NC7"/>
<connect gate="G$1" pin="NC8" pad="NC8"/>
<connect gate="G$1" pin="NC9" pad="NC9"/>
<connect gate="G$1" pin="NETLIGHT" pad="NETLIGHT"/>
<connect gate="G$1" pin="PWM1" pad="PWM1"/>
<connect gate="G$1" pin="PWM2" pad="PWM2"/>
<connect gate="G$1" pin="PWM3" pad="PWM3"/>
<connect gate="G$1" pin="PWRKEY" pad="PWRKEY"/>
<connect gate="G$1" pin="RI" pad="RI"/>
<connect gate="G$1" pin="RTS" pad="RTS"/>
<connect gate="G$1" pin="RXD" pad="RXD"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="SIM-CLK" pad="SIM-CLK"/>
<connect gate="G$1" pin="SIM-DATA" pad="SIM-DATA"/>
<connect gate="G$1" pin="SIM-RST" pad="SIM-RST"/>
<connect gate="G$1" pin="SIM-VDD" pad="SIM-VDD"/>
<connect gate="G$1" pin="SPK2N" pad="SPK2N"/>
<connect gate="G$1" pin="SPK2P" pad="SPK2P"/>
<connect gate="G$1" pin="SPKN" pad="SPK1N"/>
<connect gate="G$1" pin="SPKP" pad="SPK1P"/>
<connect gate="G$1" pin="STATUS" pad="STATUS"/>
<connect gate="G$1" pin="TMP-BAT" pad="TEMP-BAT"/>
<connect gate="G$1" pin="TXD" pad="TXD"/>
<connect gate="G$1" pin="VBAT" pad="VBAT"/>
<connect gate="G$1" pin="VBAT2" pad="VBAT2"/>
<connect gate="G$1" pin="VCHG" pad="VCHG"/>
<connect gate="G$1" pin="VDD-EXD" pad="VDD-EXT"/>
<connect gate="G$1" pin="VRTC" pad="VRTC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC65" prefix="GSM" uservalue="yes">
<description>&lt;b&gt;GSM TC65 Siemens</description>
<gates>
<gate name="G$1" symbol="TC65"/>
</gates>
<devices>
<device name="" package="TC65">
<connects>
<connect gate="G$1" pin="ADC1" pad="P$2"/>
<connect gate="G$1" pin="ADC2" pad="P$3"/>
<connect gate="G$1" pin="AGND" pad="P$57"/>
<connect gate="G$1" pin="BAT1" pad="P$45"/>
<connect gate="G$1" pin="BAT2" pad="P$44"/>
<connect gate="G$1" pin="BAT3" pad="P$43"/>
<connect gate="G$1" pin="BAT4" pad="P$42"/>
<connect gate="G$1" pin="BAT5" pad="P$41"/>
<connect gate="G$1" pin="BATTEMP" pad="P$27"/>
<connect gate="G$1" pin="CCCLK" pad="P$16"/>
<connect gate="G$1" pin="CCGND" pad="P$21"/>
<connect gate="G$1" pin="CCIN" pad="P$20"/>
<connect gate="G$1" pin="CCIO" pad="P$18"/>
<connect gate="G$1" pin="CCRST" pad="P$19"/>
<connect gate="G$1" pin="CCVCC" pad="P$17"/>
<connect gate="G$1" pin="CHAGAT" pad="P$35"/>
<connect gate="G$1" pin="CTS0" pad="P$52"/>
<connect gate="G$1" pin="CTS1" pad="P$53"/>
<connect gate="G$1" pin="DACOUT" pad="P$79"/>
<connect gate="G$1" pin="DAI0" pad="P$26"/>
<connect gate="G$1" pin="DAI1" pad="P$25"/>
<connect gate="G$1" pin="DAI2" pad="P$24"/>
<connect gate="G$1" pin="DAI3" pad="P$23"/>
<connect gate="G$1" pin="DAI4" pad="P$22"/>
<connect gate="G$1" pin="DAI5" pad="P$13"/>
<connect gate="G$1" pin="DAI6" pad="P$15"/>
<connect gate="G$1" pin="DCD0" pad="P$54"/>
<connect gate="G$1" pin="DSR0" pad="P$48"/>
<connect gate="G$1" pin="DTR0" pad="P$50"/>
<connect gate="G$1" pin="EMRGRST" pad="P$55"/>
<connect gate="G$1" pin="EPN1" pad="P$62"/>
<connect gate="G$1" pin="EPN2" pad="P$65"/>
<connect gate="G$1" pin="EPP1" pad="P$63"/>
<connect gate="G$1" pin="EPP2" pad="P$64"/>
<connect gate="G$1" pin="GND1" pad="P$1"/>
<connect gate="G$1" pin="GND2" pad="P$4"/>
<connect gate="G$1" pin="GND3" pad="P$36"/>
<connect gate="G$1" pin="GND4" pad="P$37"/>
<connect gate="G$1" pin="GND5" pad="P$38"/>
<connect gate="G$1" pin="GND6" pad="P$39"/>
<connect gate="G$1" pin="GND7" pad="P$40"/>
<connect gate="G$1" pin="GND8" pad="P$80"/>
<connect gate="G$1" pin="GPIO1" pad="P$71"/>
<connect gate="G$1" pin="GPIO10" pad="P$5"/>
<connect gate="G$1" pin="GPIO2" pad="P$72"/>
<connect gate="G$1" pin="GPIO3" pad="P$73"/>
<connect gate="G$1" pin="GPIO4" pad="P$74"/>
<connect gate="G$1" pin="GPIO5" pad="P$10"/>
<connect gate="G$1" pin="GPIO6" pad="P$9"/>
<connect gate="G$1" pin="GPIO7" pad="P$8"/>
<connect gate="G$1" pin="GPIO8" pad="P$6"/>
<connect gate="G$1" pin="GPIO9" pad="P$76"/>
<connect gate="G$1" pin="I2CCLK" pad="P$11"/>
<connect gate="G$1" pin="I2CDAT" pad="P$70"/>
<connect gate="G$1" pin="IGT" pad="P$56"/>
<connect gate="G$1" pin="ISENSE" pad="P$14"/>
<connect gate="G$1" pin="MICN1" pad="P$58"/>
<connect gate="G$1" pin="MICN2" pad="P$61"/>
<connect gate="G$1" pin="MICP1" pad="P$59"/>
<connect gate="G$1" pin="MICP2" pad="P$60"/>
<connect gate="G$1" pin="NC1" pad="P$77"/>
<connect gate="G$1" pin="PWRIND" pad="P$78"/>
<connect gate="G$1" pin="RING0" pad="P$47"/>
<connect gate="G$1" pin="RTS0" pad="P$49"/>
<connect gate="G$1" pin="RTS1" pad="P$51"/>
<connect gate="G$1" pin="RXD0" pad="P$30"/>
<connect gate="G$1" pin="RXD1" pad="P$29"/>
<connect gate="G$1" pin="SPICS" pad="P$75"/>
<connect gate="G$1" pin="SPIDI" pad="P$7"/>
<connect gate="G$1" pin="SYNC" pad="P$28"/>
<connect gate="G$1" pin="TXD0" pad="P$32"/>
<connect gate="G$1" pin="TXD1" pad="P$31"/>
<connect gate="G$1" pin="USBDN" pad="P$68"/>
<connect gate="G$1" pin="USBDP" pad="P$69"/>
<connect gate="G$1" pin="VCHARGE" pad="P$34"/>
<connect gate="G$1" pin="VDDLP" pad="P$33"/>
<connect gate="G$1" pin="VEXT" pad="P$46"/>
<connect gate="G$1" pin="VMIC" pad="P$66"/>
<connect gate="G$1" pin="VSENSE" pad="P$67"/>
<connect gate="G$1" pin="VUSBIN" pad="P$12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MG2639" prefix="GSM" uservalue="yes">
<description>&lt;b&gt; GSM850/EGSM900/DCS1800/PCS1900 &lt;p&gt; by ZTE Corporation CHINA</description>
<gates>
<gate name="MG2639" symbol="MG2639"/>
<gate name="G$2" symbol="VCC"/>
<gate name="G$3" symbol="GND"/>
</gates>
<devices>
<device name="" package="MG2639">
<connects>
<connect gate="G$2" pin="VBAT" pad="6"/>
<connect gate="G$3" pin="GND" pad="1 3 5 28"/>
<connect gate="MG2639" pin="CARD_CLK" pad="12"/>
<connect gate="MG2639" pin="CARD_DATA" pad="13"/>
<connect gate="MG2639" pin="CARD_RST" pad="11"/>
<connect gate="MG2639" pin="CTS" pad="9"/>
<connect gate="MG2639" pin="DCD" pad="10"/>
<connect gate="MG2639" pin="DSR" pad="26"/>
<connect gate="MG2639" pin="DTR" pad="25"/>
<connect gate="MG2639" pin="MIC_1N" pad="23"/>
<connect gate="MG2639" pin="MIC_1P" pad="22"/>
<connect gate="MG2639" pin="MIC_2P" pad="21"/>
<connect gate="MG2639" pin="PWRKEY_N" pad="24"/>
<connect gate="MG2639" pin="RF_ANT" pad="2"/>
<connect gate="MG2639" pin="RING" pad="4"/>
<connect gate="MG2639" pin="RSSI_LED" pad="7"/>
<connect gate="MG2639" pin="RTS" pad="8"/>
<connect gate="MG2639" pin="RXD" pad="15"/>
<connect gate="MG2639" pin="SPK_1N" pad="20"/>
<connect gate="MG2639" pin="SPK_1P" pad="19"/>
<connect gate="MG2639" pin="SPK_2P" pad="18"/>
<connect gate="MG2639" pin="SYSRST_N" pad="17"/>
<connect gate="MG2639" pin="TXD" pad="16"/>
<connect gate="MG2639" pin="V_CARD" pad="14"/>
<connect gate="MG2639" pin="V_MSM" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUECTEL_M95_HD_V1.0" prefix="IC" uservalue="yes">
<description>Quad-band
GSM/GPRS Module</description>
<gates>
<gate name="M95" symbol="M95"/>
</gates>
<devices>
<device name="" package="M95">
<connects>
<connect gate="M95" pin="AGND" pad="1"/>
<connect gate="M95" pin="CTS" pad="23"/>
<connect gate="M95" pin="DBG_RXD" pad="14"/>
<connect gate="M95" pin="DBG_TXD" pad="15"/>
<connect gate="M95" pin="DCD" pad="25"/>
<connect gate="M95" pin="DTR" pad="20"/>
<connect gate="M95" pin="EMERG_OFF" pad="11"/>
<connect gate="M95" pin="GND1" pad="40"/>
<connect gate="M95" pin="GND2" pad="38"/>
<connect gate="M95" pin="GND3" pad="37"/>
<connect gate="M95" pin="GND4" pad="36"/>
<connect gate="M95" pin="GND5" pad="35"/>
<connect gate="M95" pin="LOUDSPKN" pad="8"/>
<connect gate="M95" pin="LOUDSPKP" pad="9"/>
<connect gate="M95" pin="MIC1N" pad="5"/>
<connect gate="M95" pin="MIC1P" pad="4"/>
<connect gate="M95" pin="MIC2N" pad="3"/>
<connect gate="M95" pin="MIC2P" pad="2"/>
<connect gate="M95" pin="NETLIGHT" pad="13"/>
<connect gate="M95" pin="PWRKEY" pad="10"/>
<connect gate="M95" pin="R1" pad="26"/>
<connect gate="M95" pin="RESERVED1" pad="41"/>
<connect gate="M95" pin="RESERVED2" pad="42"/>
<connect gate="M95" pin="RESERVED3" pad="16"/>
<connect gate="M95" pin="RESERVED4" pad="17"/>
<connect gate="M95" pin="RESERVED5" pad="18"/>
<connect gate="M95" pin="RF_ANT" pad="39"/>
<connect gate="M95" pin="RTS" pad="24"/>
<connect gate="M95" pin="RXD" pad="21"/>
<connect gate="M95" pin="SIM_CLK" pad="30"/>
<connect gate="M95" pin="SIM_DATA" pad="29"/>
<connect gate="M95" pin="SIM_GND" pad="31"/>
<connect gate="M95" pin="SIM_RST" pad="28"/>
<connect gate="M95" pin="SIM_VDD" pad="27"/>
<connect gate="M95" pin="SPK1N" pad="6"/>
<connect gate="M95" pin="SPK1P" pad="7"/>
<connect gate="M95" pin="STATUS" pad="12"/>
<connect gate="M95" pin="TXD" pad="22"/>
<connect gate="M95" pin="VBAT1" pad="34"/>
<connect gate="M95" pin="VBAT2" pad="33"/>
<connect gate="M95" pin="VDD_EXT" pad="19"/>
<connect gate="M95" pin="VRTC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUECTEL_L30" prefix="IC" uservalue="yes">
<gates>
<gate name="L30" symbol="QUECTEL_L30"/>
</gates>
<devices>
<device name="" package="QUECTEL_L30">
<connects>
<connect gate="L30" pin="1/GND" pad="1"/>
<connect gate="L30" pin="10/GND" pad="10"/>
<connect gate="L30" pin="11/GND" pad="11"/>
<connect gate="L30" pin="12/DR_I2C_CLK" pad="12"/>
<connect gate="L30" pin="13/DR_I2C_DIO" pad="13"/>
<connect gate="L30" pin="14/ON/OFF" pad="14"/>
<connect gate="L30" pin="15/WAKEUP" pad="15"/>
<connect gate="L30" pin="16/EITO" pad="16"/>
<connect gate="L30" pin="17/GND" pad="17"/>
<connect gate="L30" pin="18/GND" pad="18"/>
<connect gate="L30" pin="19/RFIN" pad="19"/>
<connect gate="L30" pin="2/RESET" pad="2"/>
<connect gate="L30" pin="20/GND" pad="20"/>
<connect gate="L30" pin="21/GND" pad="21"/>
<connect gate="L30" pin="3/CFGO/SCK" pad="3"/>
<connect gate="L30" pin="4/CFG1/SCS" pad="4"/>
<connect gate="L30" pin="5/TXD/MISO/SCL" pad="5"/>
<connect gate="L30" pin="6/RXD/MOSI/SDA" pad="6"/>
<connect gate="L30" pin="7/IPPS" pad="7"/>
<connect gate="L30" pin="8/VIO/RTC" pad="8"/>
<connect gate="L30" pin="9/VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUECTEL_M12" prefix="IC" uservalue="yes">
<gates>
<gate name="M12" symbol="QUECTEL_M12"/>
</gates>
<devices>
<device name="" package="QUECTEL_M12">
<connects>
<connect gate="M12" pin="1/DISP_DATA" pad="1"/>
<connect gate="M12" pin="10/DBG_TXD" pad="10"/>
<connect gate="M12" pin="11/SIM_PRESENCE" pad="11"/>
<connect gate="M12" pin="12/SIM_VDD" pad="12"/>
<connect gate="M12" pin="13/SIM_DATA" pad="13"/>
<connect gate="M12" pin="14/SIM_CLK" pad="14"/>
<connect gate="M12" pin="15/SIM_RST" pad="15"/>
<connect gate="M12" pin="16/VRTC" pad="16"/>
<connect gate="M12" pin="17/EMERG_OFF" pad="17"/>
<connect gate="M12" pin="18/PWRKEY" pad="18"/>
<connect gate="M12" pin="19/AGND" pad="19"/>
<connect gate="M12" pin="2/DISP_CLK" pad="2"/>
<connect gate="M12" pin="20/SPK2P" pad="20"/>
<connect gate="M12" pin="21/SPK1N" pad="21"/>
<connect gate="M12" pin="22/SPK1P" pad="22"/>
<connect gate="M12" pin="23/MIC1P" pad="23"/>
<connect gate="M12" pin="24/MIC1N" pad="24"/>
<connect gate="M12" pin="25/MIC2P" pad="25"/>
<connect gate="M12" pin="26/MIC2N" pad="26"/>
<connect gate="M12" pin="27/LIGHT_MOS" pad="27"/>
<connect gate="M12" pin="28/KBR0" pad="28"/>
<connect gate="M12" pin="29/KBR1" pad="29"/>
<connect gate="M12" pin="3/DISP_CS" pad="3"/>
<connect gate="M12" pin="30/KBR2" pad="30"/>
<connect gate="M12" pin="31/KBR3" pad="31"/>
<connect gate="M12" pin="32/KBR4" pad="32"/>
<connect gate="M12" pin="33/KBC0" pad="33"/>
<connect gate="M12" pin="34/KBC1" pad="34"/>
<connect gate="M12" pin="35/KBC2" pad="35"/>
<connect gate="M12" pin="36/KBC3" pad="36"/>
<connect gate="M12" pin="37/KBC4" pad="37"/>
<connect gate="M12" pin="38/GPIO1_KBC5" pad="38"/>
<connect gate="M12" pin="39/BUZZER" pad="39"/>
<connect gate="M12" pin="4/DISP_D/C" pad="4"/>
<connect gate="M12" pin="40/TEMP_BAT" pad="40"/>
<connect gate="M12" pin="41/ADC0" pad="41"/>
<connect gate="M12" pin="42/GND2" pad="42"/>
<connect gate="M12" pin="43/RF_ANT" pad="43"/>
<connect gate="M12" pin="44/GND3" pad="44"/>
<connect gate="M12" pin="45/GND4" pad="45"/>
<connect gate="M12" pin="46/GND5" pad="46"/>
<connect gate="M12" pin="47/GND6" pad="47"/>
<connect gate="M12" pin="48/GND7" pad="48"/>
<connect gate="M12" pin="49/GND8" pad="49"/>
<connect gate="M12" pin="5/DISP_RST" pad="5"/>
<connect gate="M12" pin="50/VBAT1" pad="50"/>
<connect gate="M12" pin="51/VBAT2" pad="51"/>
<connect gate="M12" pin="52/VBAT3" pad="52"/>
<connect gate="M12" pin="53/VCHG" pad="53"/>
<connect gate="M12" pin="54/STATUS" pad="54"/>
<connect gate="M12" pin="55/RI" pad="55"/>
<connect gate="M12" pin="56/DCD" pad="56"/>
<connect gate="M12" pin="57/CTS" pad="57"/>
<connect gate="M12" pin="58/RTS" pad="58"/>
<connect gate="M12" pin="59/DTR" pad="59"/>
<connect gate="M12" pin="6/NETLIGHT" pad="6"/>
<connect gate="M12" pin="60/TXD" pad="60"/>
<connect gate="M12" pin="61/RXD" pad="61"/>
<connect gate="M12" pin="62/RESERVED" pad="62"/>
<connect gate="M12" pin="63/RESERVED" pad="63"/>
<connect gate="M12" pin="64/GPIO0" pad="64"/>
<connect gate="M12" pin="7/VDD_EXT" pad="7"/>
<connect gate="M12" pin="8/GND1" pad="8"/>
<connect gate="M12" pin="9/DBG_RXD" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
