<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<description>Current-sense amplifier with voltage output</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
<symbols>
<symbol name="MAX4080">
<pin name="RS-" direction="in"/>
<pin name="RS+" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAX4080" prefix="U">
<description>Undirectional current sense amplifier with voltage output</description>
<gates>
<gate name="G$1" symbol="MAX4080"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="RS+" pad="1"/>
<connect gate="G$1" pin="RS-" pad="8"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
